{"text_format":"1","workbook":"xlsx","n_sheets":38,"sheets":["Eingabe","Commercant","Fournisseur","Indications","Indicazioni","Hinweise","MSE","Kundenstamm","ICS","ICS5000","Keranova","Kerastar","Texte","Musteranlage","Verbindungsleitung","PRIMA PLUS","Absolut","Absolut Thermoset_F","Cheminee","ISOLIT","Technostar120","Verrechnungspartner","Verbindungsleitung TS","Commerciante","Firma","Belegart","Kalkulation","sanschie","Daten","Sortimente","Vokabel","Rabattübersicht","Absolut Thermoset_I","Absolut Thermoset","Lieferanten","Fornitori","Einstellungstabelle","Transportkosten"],"not_rendered":{"charts":0,"images":34,"macros":1,"external_links":0,"defined_names":67,"comments":8,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Eingabe","index":0,"n_rows":60,"n_cols":17,"rows_kept":60,"cut":false,"hidden":false,"merged":[[3,10,3,14],[4,10,4,14],[5,10,5,14],[6,11,6,14],[8,10,8,14],[17,11,17,14],[15,10,15,14],[16,10,16,14],[7,11,7,14],[9,10,9,14],[10,10,10,12],[10,13,10,14],[12,10,12,12],[12,13,12,14]]}
[null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$21","v":"Kunden-Adressdaten"}]
[]
[null,null,null,null,null,null,null,null,null,null,"Ganztec AG"]
[null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,null,null,"Badstrasse 38"]
[null,null,null,null,null,null,null,null,null,null,"5312","Döttingen"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$22","v":"PLZ"},{"$f":"Vokabel!$A$23","v":"Ort"}]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$24","v":"Ansprechpartner"}]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$25","v":"Tel.Nr."},null,null,"E-Mail"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(INDEX(Kundenstamm!$A$3:$L$5000,Kundenstamm!$T$2,1)=\"\",\"\",INDEX(Kundenstamm!$A$3:$L$5000,Kundenstamm!$T$2,1))","v":9999}]
[null,null,null,null,null,null,null,null,null,null,"Fax",null,null,{"$f":"Vokabel!$A$222","v":"Handy"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$27","v":"Objekt"}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$22","v":"PLZ"},{"$f":"Vokabel!$A$23","v":"Ort"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Nettorabatt",0]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$28","v":"Konditionen / Lohn"},null,null,{"$f":"Vokabel!$A$29","v":"   Rabatt 1"},0]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$34","v":"Rabatt 3"},null,0,{"$f":"Vokabel!$A$33","v":"   Rabatt 2"},0]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$30","v":"Stunden"},null,null,{"$f":"Vokabel!$A$35","v":"   CHF per Std."},0]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$31","v":"Kilometer"},null,null,{"$f":"Vokabel!$A$36","v":"   CHF per km"},0]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$32","v":"Pauschale"},null,null,{"$f":"Vokabel!$A$37","v":"   CHF per P."},0]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$38","v":"   MwSt"},7.6999999999999999E-2]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"CD \"&Hinweise!N3","v":"CD Version   20230101"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[0]

{"sheet":"Commercant","index":1,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":true,"merged":[]}
[null,{"$f":"Vokabel!$A$241","v":"INFO:"}]
[null,{"$f":"Vokabel!$A$240","v":"In den Zeilen 5-10 tragen Sie bitte Ihre Firma, und den Zeilen 14-15 den Sachbearbeiter u. Tel.Nr., ein."}]
[]
[null,{"$f":"Vokabel!$A$242","v":"Firmendaten:"}]
[{"$f":"Vokabel!$A$226","v":"1.Zeile"},"Ganztec AG"]
[{"$f":"Vokabel!$A$227","v":"2.Zeile"},"Badstrasse 38"]
[{"$f":"Vokabel!$A$228","v":"3.Zeile"},"5312 Döttingen"]
[{"$f":"Vokabel!$A$229","v":"4.Zeile"},"Tel. 0562680000   Fax. 0562680001"]
[{"$f":"Vokabel!$A$230","v":"5.Zeile"},"Mail:  info@ganztec.ch"]
["Schiedel N° client"]
[]
[]
[null,{"$f":"Vokabel!$A$247","v":"Sachbearbeiter:"},{"$f":"Vokabel!$A$248","v":"Pers.-Nr."},null,{"$f":"Vokabel!$A$249","v":"Frachteinstellungen:"}]
[{"$f":"Vokabel!$A$250","v":"Vorname/Name"},"Herr Mustermann",null,null,63,{"$f":"Vokabel!$A$256","v":"CHF per Tonne"}]
[{"$f":"Vokabel!$A$251","v":"Telefon"},"Tel. 000000",{"$f":"Eingabe!$K$4&\"  \"&Eingabe!$K$16&\" \"&Eingabe!$L$18","v":"Ganztec AG   "}]
[{"$f":"Vokabel!$A$252","v":"Fax"},"Fax. 0000000"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[3,{"$f":"INDEX(Commercant!B46:B48,A44,1)","v":"nichts"}]
["Mailprogramm"]
["Outlook (Express)","Outlook"]
["Lotus Notes","Lotus"]
["keines von Beiden","nichts"]

{"sheet":"Fournisseur","index":2,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":true,"merged":[]}
[]
["Fournisseur"]
[]
[]
["N° client","Adresse 1","Adresse 2","Rue","NP","Lieu","N°. Téléphone","N°. Télécopie","E-Mail","Matchcode"]
[1,"Ganztec AG",null,"Badstrasse 38",5312,"Döttingen","Tel. 0562680000","Fax. 0562680001","info@ganztec.ch",{"$f":"B6&\" \"&E6&\" \"&F6","v":"Ganztec AG 5312 Döttingen"}]
[2,null,null,null,null,null,null,null,null,"  "]
[3,null,null,null,null,null,null,null,null,"  "]
[4,null,null,null,null,null,null,null,null,"  "]
[5,null,null,null,null,null,null,null,null,"  "]
[6,null,null,null,null,null,null,null,null,"  "]
[7,null,null,null,null,null,null,null,null,"  "]
[8,null,null,null,null,null,null,null,null,"  "]
[9,null,null,null,null,null,null,null,null,"  "]
[10,null,null,null,null,null,null,null,null,"  "]
[11,null,null,null,null,null,null,null,null,"  "]
[12,null,null,null,null,null,null,null,null,"  "]
[13,null,null,null,null,null,null,null,null,"  "]
[14,null,null,null,null,null,null,null,null,"  "]
[15,null,null,null,null,null,null,null,null,"  "]
[16,null,null,null,null,null,null,null,null,"  "]
[17,null,null,null,null,null,null,null,null,"  "]
[18,null,null,null,null,null,null,null,null,"  "]
[19,null,null,null,null,null,null,null,null,"  "]
[20,null,null,null,null,null,null,null,null,"  "]
[21,null,null,null,null,null,null,null,null,"  "]
[22,null,null,null,null,null,null,null,null,"  "]
[23,null,null,null,null,null,null,null,null,"  "]
[24,null,null,null,null,null,null,null,null,"  "]
[25,null,null,null,null,null,null,null,null,"  "]
[26,null,null,null,null,null,null,null,null,"  "]
[27,null,null,null,null,null,null,null,null,"  "]
[28,null,null,null,null,null,null,null,null,"  "]
[29,null,null,null,null,null,null,null,null,"  "]
[30,null,null,null,null,null,null,null,null,"  "]

{"sheet":"Indications","index":3,"n_rows":72,"n_cols":14,"rows_kept":72,"cut":false,"hidden":true,"merged":[[26,2,26,3]]}
[]
[]
[null,"Le nouveau logicielle d'offre et commande de Ganztec                                 ",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Daten!$F$161","v":"Version   20230101"}]
[]
[null,"Indications"]
[]
[]
[null,"Installation:","Le programme est installer automatiquement par le setup.exe sur votre PC (c:\\Schiedel-CH\\Kaminprofi\\...)"]
[null,null,"et sur le Desktop"]
[null,null,"En plus du programme un fichier (Kaminprofi_Offerte) est également installé pour stockées les proposition. "]
[]
[null,"Internet Update:","La dernière version du programme est toujours disponible sur internet (http://www.ganztec.ch)"]
[]
[null,"Condition :","Microsoft Windows 2000, NT, XP"]
[null,null,"Microsoft Office (des MS Office 2000 et Programme e-Mail MS Outlook ou Lotus Notes)"]
[null,null,"Les commandes ne peuvent devenir automatiques qu'avec EM Outlook ou Lotus Notes "]
[null,null,"Les réglages mail peuvent être modifiées à tout moment dans le masque \"commerçant\"."]
[]
[null,"Données de base: ","Base de clients: ",null,"L'installation nouvelle d'un client a lieu dans le masque d'entrée. "]
[null,null,null,null,"Vous pouvez enregistrer ce client dans votre base de clients - presser le bouton \"enregistrer client\"! "]
[null,null,null,null,"Le client doit être saisi dans la base de clients, afin que celui-ci puisse être choisi dans le programme. "]
[null,null,null,null,"La base de clients est un élément essentiel du programme. "]
[null,null,null,null,"Avec une mise à jour de programme, la base de clients stockée est importée automatiquement dans le logicielle. "]
[]
[]
[null,null,"Adresse de marchand:",null,"Entrée des données du responsable et d'entreprise.  "]
[null,null,"Textes de preuve et d'assemblage: ",null,"Tous les champs blancs sont des textes de preuve et d'assemblage librement définissables. "]
[]
[null,"Masque d'entrée: ","Projet de construction:",null,"Entrée de l'adresse du chantier."]
[null,null,"Conditions/salaire: ",null,"Entrée de deux remises. La base de calcul pour la deuxième remise est"]
[null,null,null,null,"Brut moins première remise "]
[null,null,null,null,"Les travaux de montage peuvent être introduit à l’heure, par kilomètres ou par un forfait. "]
[null,null,null,null,"(Attention: saisir le texte de montage avant !) "]
[null,null,"Justificatif N°: ",null,"Entrée individuelle d'un numéro de document. "]
[null,null,"Type de justificatif: ",null,"Calcul, offre ou confirmation de commande. "]
[null,null,null,null,"En cliquant sur le logo du produit, le masque d'entrée respectif s'ouvre. "]
[]
[null,"Masques de produit:","Champs de sélection :",null,"Introduisez les données nécessaires dans les champs de sélection."]
[null,null,"Calcul de l' installation:",null,"Après le choix effectué, les articles sont inséré en cliquant sur \"calculation installation\" "]
[null,null,null,null,"dans le tableau calculation."]
[null,null,"Entrée par élément:",null,"La pièce avec le Ø correspondant est inséré sans quantité dans le tableau calculation."]
[]
[null,null,null,"Après chaque calcul enregistrer l'offre ou après l’impression retourner à l'entrée!   "]
[]
[null,"Calcul:","Enregistrer le calcul.",null,"Le calcul (offre) est stocké automatiquement comme petit fichier Excel."]
[null,null,null,null,"Tous les champs peuvent être modifiés dans ce fichier. "]
[]
[null,null,null,"Chemin : C:\\Schiedel-CH\\Kaminprofi\\Kaminprofi_Offerte\\....... Xls"]
[null,null,null,null,"Ce chemin d'accès ne peut pas être rebaptisée, puisque le programme ne fonctionne plus."]
[]
[null,null,"Étendre liste des pièces:",null,"Ici, des articles supplémentaires peuvent être choisis."]
[null,null,"Aperçu d'impression:",null,"L'impression devrait toujours s'effectuer par l'aperçu avant impression, puisqu'une liste de pièces "]
[null,null,null,null,"étendue est ainsi également filtrée sur les articles choisis. "]
[null,null,"Commande:",null,"Génération de commandes automatique au Centre de Client Schiedel de votre choix."]
[]
[null,"Commande:","Ganztec-CC:",null,"Sélection du Centre de Client Ganztec."]
[null,null,"Mode d'expédition:",null,"Pour le mode d'expédition choisir livraison au marchand de matériaux ou livraison chantier."]
[null,null,"Délai de livraison:",null,"Dans ce champ, on peut introduire une date ou d'autres informations (p. ex. semaine. 15) "]
[null,null,null,null,"La commande peut être imprimé, télécopié ou envoyer par courriel. "]
[null,null,"Courriel de commande:",null,"La commande est préparée pour l'envoi au Centre de Client défini, en tant que pièce jointe"]
[]
[null,"Inséré le propre logo d'entreprise:",null,null,"Il existe la possibilité d'insérer son propre logo pour les offres lors de l'enregistrement,"]
[null,null,null,null,"le quelle apparaît alors sur toutes les documents."]
[null,null,"Procédure:",null,"Ouvrez le chemin dans le Explorer - : C:\\Schiedel-CH\\Kaminprofi\\ "]
[null,null,null,null,"le fichier Kalkulation-Muster_F.xls"]
[null,null,null,null,"remplacez ensuite le logo Schiedel par le votre, enregistrer et fermer "]
[null,null,null,null,"Aucune autre modification ne peut être entreprise."]
[]
[null,"Note juridique:",null,null,"Schiedel peut soumettre les offres représentées dans ce logiciel au marchand de matériaux spécialisé "]
[null,null,null,null,"conformément aux conditions de livraison et vente Ganztec en vigueur."]
[null,null,null,null,"Prix départ usine, TVA en sus."]
[null,null,null,null,"Valable des le 1. janvier 2019"]

{"sheet":"Indicazioni","index":4,"n_rows":70,"n_cols":14,"rows_kept":70,"cut":false,"hidden":true,"merged":[]}
[]
[]
[null,"Il nuovo programma di offerta e l'ordine di Ganztec",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Daten!$F$161","v":"Version   20230101"}]
[]
[null,"Note "]
[]
[]
[null,"Installazione:","Il programma viene avviato automaticamente attraverso il File setup.exe sul vostro PC (c:\\Schiedel-CH\\Kaminprofi\\....)"]
[null,null," ed installato sul desktop."]
[null,null,"Con il programma viene inoltre installata una cartella (Kaminprofi_Offerte) per le Offerte memorizzate."]
[]
[null,"Internet-Update:","In Internet trovate sempre la versione più attuale! (http://www.ganztec.ch) "]
[]
[null,"Condizione: ","Microsoft Windows 2000, NT, XP"]
[null,null,"Pacchetto Microsoft Office (MS Office 2000 e programma di posta elettronica di Microsoft Outlook o Lotus Notes)"]
[null,null,"Le Ordinazioni possono essere inviate automaticamente solo con MS Outlook o Lotus Notes."]
[null,null,"Le impostazioni della posta nella maschera \"rivenditori\" possono essere modificate in qualsiasi momento."]
[]
[null,"Banco Dati : ","Dati Clientela: ",null,"Si crea un nuovo cliente attraverso la maschera di inseriment."]
[null,null,null,null,"Si puo' memorizzare un cliente cliccando sul Tasto \"cliente salvare\""]
[null,null,null,null,"Il cliente deve essere memorizzato affinchè possa poi essere selezionato nel file della clientela. Il Banco Dati di Clientela è una parte del programma. "]
[null,null,null,null,"Con un aggiornamento del programma, il File della clientela viene automaticamente importato nel programma. "]
[]
[null,null,"Indirizzo di concessionari ",null,"Inserire i dati della Ditta e addetto responsabile."]
[null,null,"Assemblea testi-line: ",null,"Tutte le caselle bianche sono liberamente definibili di assemblaggio e documento di testo. "]
[]
[null,"Maschera di","Progetti di costruzione:",null,"Immettere l'indirizzo del Cantiere"]
[null," inserimento","Condizioni / salario:",null,"Immettere due riduzioni. La base di calcolo per la seconda "]
[null,null,null,null,"riduzione è data dal prezzo lordo con detrazione del primo sconto."]
[null,null,null,null,"Servizi di installazione possono essere inseriti in ore, chilometraggio o in una somma forfettaria."]
[null,null,null,null," (Nota: Immettere per prima il testo di montaggio/installazione) "]
[null,null,"Numero del documento: ",null,"Entrare un numero di documento. "]
[null,null,"Tipo di documento ",null,"Calcolo, Offerta o conferma d'ordine. "]
[null,null,null,null,"Cliccando sul logo di un prodotto si aprire la corrispondente maschera d'inserimento."]
[]
[null,"Maschera di prodotto:","Selezione campi: ",null,"Inserire i dati necessari per la selezione campi. "]
[null,null,"Il calcolo dei costi di sistema: ",null,"Dopo la selezione,  cliccando su \"sistema di prezzi\" gli articoli vengono generati nella tabella die costi."]
[]
[null,null,"Inserisci i singoli ",null,"Il tipo con il corrispondente diametro viene generato senza quantitativo nella tabella dei costi."]
[]
[null,null,null,"Dopo il calcolo di ogni Offerta memorizzare oppure dopo aver stampato ritornare sulla maschera d'immissione ! "]
[]
[null,"Calcolo dei costi: ","Memorizzazione Calcoli",null,"Il calcolo dei costi (range) è un piccolo file formato Excel che viene salvato automaticamente."]
[null,null,null,null," In questo file, tutti i campi possono essere mutati."]
[]
[null,null,null," C:\\Schiedel-CH\\Kaminprofi\\Kaminprofi_Offerte \\....... .xls "]
[null,null,null,null,"Il nome di questo percorso non può essere cambiato(rinomina), altrimenti il programma non funziona più !! "]
[]
[null,null,"Estensione lista dei Pezzi",null,"Quì, possono essere selezionati ulteriori articoli."]
[null,null,"Stampa",null,"Stampare sempre con il passo \"visione stampa\" in maniera   "]
[null,null,null,null,"che venga filtrata anche una ampia lista di pezzi dell'articolo selezionato"]
[null,null,"Ordinazione:",null,"Generazione automatica di Ordinazione al Centro Schiedel di vostra scelta. "]
[]
[null,"Ordinazione:","Ganztec-CC:",null,"Scelta Centro Ganztec"]
[null,null,"tipo di Spedizione:",null," sceglere il tipo di spedizione \"consegna magazzino del commerciante\" o \"consegna sul cantiere\""]
[null,null,"Data di consegna:",null,"In questo campo, inserire la data di consegna o altre informazioni (ad esempio, numero della Settimana) "]
[null,null,null,null,"Le Ordinazioni possono essere stampate, inviate via fax o per Posta Elettronica. "]
[null,null,"Invio d'ordine via Email: ",null,"L'Ordinazione sarà inviata in allegato via Email al centro clienti definito."]
[]
[null,"Inserimento logo aziendale:",null,null,"E 'possibile, per le offerte memorizzate, di inserire il proprio logo aziendale"]
[null,null,null,null,"che apparirebbe poi in tutte le Offerte di tale Azienda.. "]
[null,null,"Procedura ",null,"Aprire l'Explorer - via C: \\ Schiedel-CH\\Kaminprofi\\.."]
[null,null,null,null,"\\ camino professionale \\ file \"Kalkulation-Muster_I.xls. "]
[null,null,null,null,"Riampiazzare il Logo Aziendale al Posto del Logo Schiedel e poi salvare il documento e chiudere."]
[null,null,null,null,"Non si devono apportare ulteriori modifiche al documento."]
[]
[null,"Avviso legale: ",null,null,"Schiedel può presentare ai concessionari di materiale di costruzione, le Offerte contenute nel presente Programma "]
[null,null,null,null,"in conformità con i termini e le condizioni della Ganztec. "]
[null,null,null,null,"Prezzi franco fabbrica più IVA."]
[null,null,null,null,"Valido dal 1 Gennaio 2019. "]

{"sheet":"Hinweise","index":5,"n_rows":83,"n_cols":14,"rows_kept":83,"cut":false,"hidden":true,"merged":[]}
[]
[]
[null,"Das neue Angebots- und Bestellprogramm von Ganztec                                     ",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Daten!$F$161","v":"Version   20230101"}]
[]
[null,"Hinweise"]
[]
[]
[null,"Installation:","Das Programm wird automatisch durch die setup.exe auf Ihrem PC  (c:\\Schiedel-CH\\Kaminprofi\\....)"]
[null,null,"und auf dem Desktop installiert."]
[null,null,"Zusätzlich zum Programm wird auch ein Ordner (Kaminprofi_Offerte) für gespeicherte Angebote installiert."]
[]
[null,"Internet-Update:","Im Internet steht immer die aktuelle Programmversion zur Verfügung ! (http://www.ganztec.ch)"]
[]
[null,"Voraussetzung:","Microsoft Windows 2000, NT, XP"]
[null,null,"Microsoft Officepaket (ab MS Office 2000 und e-Mail-Programm MS Outlook oder Lotus Notes)"]
[null,null,"Bestellungen können nur mit MS Outlook oder Lotus Notes automatisch gemailt werden."]
[null,null,"Die Mail-Einstellungen können jederzeit in der Maske \"Händler\" geändert werden."]
[]
[null,null,"Achtung: Die Makro-Sicherheitseinstellungen sind auf Mittel oder Niedrig einzustellen!"]
[null,null,"Vorgehensweise bei:"]
[null,null,"Office 2000, XP oder 2003:  Extras  - Makro - Sicherheit - Mittel oder Niedrig auswählen."]
[null,null,"Wenn Sie Mittel auswählen, werden Sie gefragt ob Sie die Makros akzeptieren - mit ja bestätigen !"]
[null,null,"Wenn Sie Niedrig auswählen wird das Programm automatisch mit den Makros gestartet."]
[null,null,"Office 2007 und Office 2010: Schaltfläche Office - Excel Optionen - Vertrauensstellungscenter - "]
[null,null,"                      Einstellungen für das Vertrauensstellungcenter - Einstellungen für Makros - alle Makros aktivieren"]
[null,null,"                      oder alle Makros mit Benachrichtigung deaktivieren auswählen."]
[null,null,"Wenn Sie Makros mit Benachrichtigung deaktivieren auswählen, dann sind bei jedem Neustart die Makros zu aktivieren."]
[]
[null,"Stammdaten:","Kundenstamm:",null,"Neuanlage eines Kunden erfolgt in der Eingabe-Maske."]
[null,null,null,null,"Sie können diesen Kunden in Ihrem Kundenstamm speichern  - Button \"Kunde speichern\" drücken !"]
[null,null,null,null,"Der Kunde muss im Kundenstamm erfasst sein, damit dieser im Programm ausgewählt werden kann."]
[null,null,null,null,"Der Kundenstamm ist ein Bestandteil des Programms. "]
[null,null,null,null,"Bei einem Programmupdate wird der abgespeicherte Kundenstamm automatisch in das"]
[null,null,null,null,"Programm importiert."]
[]
[null,null,"Händleradresse:",null,"Eingabe der Firmen- und Sachbearbeiter-Daten."]
[null,null,"Montage-Belegtexte:",null,"Alle weißen Felder sind frei definierbare Montage- und Belegtexte. "]
[]
[null,"Eingabemaske:","Bauvorhaben:",null,"Eingabe der Baustellen-Anschrift."]
[null,null,"Konditionen/Lohn:",null,"Eingabe von zwei Rabatten. Die Berechnungsgrundlage für den zweiten Rabatt ist "]
[null,null,null,null,"Brutto abzüglich erster Rabatt."]
[null,null,null,null,"Montageleistungen können in Stunden, Kilometer oder in einer Pauschale eingegeben werden."]
[null,null,null,null,"(Achtung: Montagetext vorher eingeben!)"]
[null,null,"Beleg Nr:",null,"Individuelle Eingabe einer Belegnummer."]
[null,null,"Belegart:",null,"Kalkulation, Angebot oder Auftragsbestätigung."]
[null,null,null,null,"Durch klicken auf ein Produkt-Logo öffnet sich die jeweilige Eingabemaske."]
[]
[null,"Produktmasken:","Auswahlfelder:",null,"Geben sie die notwendigen Daten in den Auswahlfeldern ein."]
[null,null,"Kalkulation Anlage:",null,"Nach erfolgter Auswahl werden die Artikel durch klicken auf  \"Kalkulation-Anlage\"  in die Tabelle "]
[null,null,null,null,"Kalkulation generiert."]
[null,null,"Einzelteileingabe:",null,"Der Typ mit dem entsprechenden Ø wird ohne Mengenvorgaben in die Tabelle Kalkulation generiert."]
[]
[null,null,null,"Nach jeder Kalkulation das Angebot speichern oder nach Ausdruck zur Eingabe zurückkehren!"]
[]
[null,"Kalkulation:","Kalkulation speichern:",null,"Die Kalkulation (Angebot) wird als kleine Excel-Datei automatisch gespeichert."]
[null,null,null,null,"In dieser Datei können alle Felder geändert werden."]
[]
[null,null,null,"Pfad: C:\\Schiedel-CH\\Kaminprofi\\Kaminprofi_Offerte\\....... .xls"]
[null,null,null,null,"Dieser Pfad darf nicht umbenannt werden, da sonst das Programm nicht mehr funktioniert."]
[]
[null,null,"Stückliste erweitern:",null,"Hier können zusätzliche Artikel ausgewählt werden."]
[null,null,"Druckansicht:",null,"Der Ausdruck sollte immer über die Druckansicht erfolgen, da damit auch eine erweiterte "]
[null,null,null,null,"Stückliste auf die ausgewählten Artikel gefiltert wird."]
[null,null,"Bestellung:",null,"Automatische Bestellgenerierung an das Schiedel Kunden-Center Ihrer Wahl."]
[]
[null,"Bestellung:","Ganztec-KC:",null,"Auswahl des Lieferanten."]
[null,null,"Versandart:",null,"Die Versandart Zustellung Händlerlager oder Zustellung Baustelle auswählen."]
[null,null,"Liefertermin:",null,"In diesem Feld kann ein Datum oder andere Informationen (z.B. KW 15) eingegeben werden."]
[null,null,null,null,"Die Bestellung kann ausgedruckt, gefaxt oder gemailt werden."]
[null,null,"Bestellung mailen:",null,"Die Bestellung wird an das definierte Kunden-Center als Mail-Anhang vorbereitet."]
[]
[null,"Eigenes Firmenlogo einfügen:",null,null,"Es besteht die Möglichkeit, für Angebote, die gespeichert werden, ein eigenes Logo einzufügen,"]
[null,null,null,null,"das dann bei allen gespeicherten Angeboten erscheint."]
[null,null,"Vorgehensweise:",null,"Öffnen Sie im Explorer - Pfad: C:\\Schiedel-CH\\Kaminprofi\\"]
[null,null,null,null,"die Datei Kalkulation-Muster.xls (Deutsch), die Datei Kalkulation-Muster_F.xls (Francais) "]
[null,null,null,null,"und die Datei Kalkulation-Muster_I.xls (Italiano)."]
[null,null,null,null,"Ersetzen Sie das Logo durch Ihr Eigenes, anschließend speichern und schließen."]
[null,null,null,null,"Es dürfen ansonsten keine weiteren Änderungen vorgenommen werden."]
[]
[null,"Rechtlicher Hinweis:",null,null,"Ganztec kann dem Baustoff-Fachhandel die in dieser Software dargestellten"]
[null,null,null,null,"Angebote gemäß den Geschäfts- und Lieferbedingungen von Ganztec unterbreiten."]
[null,null,null,null,"Preise ab Werk zzgl. MwSt."]
[null,null,null,null,"Gültig ab 1. Januar 2022"]

{"sheet":"MSE","index":6,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"office@egsa.at"]

{"sheet":"Kundenstamm","index":7,"n_rows":7000,"n_cols":38,"rows_kept":4500,"cut":true,"hidden":true,"merged":[[7,22,7,24],[7,25,7,26],[9,22,9,24],[9,25,9,26],[0,22,0,26],[1,22,1,26],[4,23,4,26],[6,22,6,26],[2,22,2,26],[3,23,3,26],[5,22,5,26]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[null,{"$f":"Vokabel!$A$283","v":"Kundenstamm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9999,{"$f":"VLOOKUP(S1,T2:U7000,2,0)","v":1},-1,null,{"$f":"IF(INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,2)=\"\",\"\",INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,2))","v":"Ganztec AG"},null,null,null,null,"Anschrift 1","Anschrift 2","Straße","PLZ","Ort","Ansprechpartner","Tel.Nr.","E-Mail","Handy","Fax","Ku.Nr."]
[{"$f":"Vokabel!$A$213","v":"Ku.Nr."},{"$f":"Vokabel!$A$214","v":"Anschrift 1"},{"$f":"Vokabel!$A$215","v":"Anschrift 2"},{"$f":"Vokabel!$A$216","v":"Strasse"},{"$f":"Vokabel!$A$217","v":"PLZ"},{"$f":"Vokabel!$A$218","v":"Ort"},{"$f":"Vokabel!$A$219","v":"Ansprechpartner"},{"$f":"Vokabel!$A$220","v":"Tel.Nr."},"E-Mail",{"$f":"Vokabel!$A$222","v":"Handy"},"Fax.Nr.",{"$f":"Vokabel!$A$224","v":"Info"},null,null,null,null,null,null,"Kunden-Matchcode",1,{"$f":"U1+1","v":0},1083,{"$f":"IF(INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,3)=\"\",\"\",INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,3))","v":""},null,null,null,null,{"$f":"Eingabe!K4","v":"Ganztec AG"},{"$f":"IF(Eingabe!K5=\"\",\"\",Eingabe!K5)","v":""},{"$f":"IF(Eingabe!K6=\"\",\"\",Eingabe!K6)","v":"Badstrasse 38"},{"$f":"IF(Eingabe!K7=\"\",\"\",Eingabe!K7)","v":"5312"},{"$f":"IF(Eingabe!L7=\"\",\"\",Eingabe!L7)","v":"Döttingen"},{"$f":"IF(Eingabe!K9=\"\",\"\",Eingabe!K9)","v":""},{"$f":"IF(Eingabe!K11=\"\",\"\",Eingabe!K11)","v":""},{"$f":"IF(Eingabe!N11=\"\",\"\",Eingabe!N11)","v":""},{"$f":"IF(Eingabe!N13=\"\",\"\",Eingabe!N13)","v":""},{"$f":"Eingabe!K13","v":0},{"$f":"IF(Eingabe!$Q$13=\"\",\"\",Eingabe!$Q$13)","v":9999}]
[9999,"Ganztec AG",null,"Badstrasse 38","5312","Döttingen",null,"","","","",null,null,null,null,null,null,null,{"$f":"IF(B3=\"\",\"\",B3&\", \"&F3&\",     \"&G3)","v":"Ganztec AG, Döttingen,     "},{"$f":"IF(A3=\"\",\"\",A3)","v":9999},{"$f":"U2+1","v":1},{"$f":"T3","v":9999},{"$f":"IF(INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,4)=\"\",\"\",INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,4))","v":"Badstrasse 38"}]
[10000,"Muster","","Musterstr.","5312","Döttingen","","","",null,null,null,null,null,null,null,null,null,"Muster, Döttingen,     ",10000,2,{"$f":"T4","v":10000},{"$f":"IF(INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,5)=\"\",\"\",INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,5))","v":"5312"},{"$f":"IF(INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,6)=\"\",\"\",INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,6))","v":"Döttingen"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3,"",{"$f":"Vokabel!$A$22","v":"PLZ"},{"$f":"Vokabel!$A$23","v":"Ort"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4,"",{"$f":"IF(INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,7)=\"\",\"\",INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,7))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5,"",{"$f":"Vokabel!$A$24","v":"Ansprechpartner"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6,"",{"$f":"IF(INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,8)=\"\",\"\",INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,8))","v":""},null,null,{"$f":"IF(INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,9)=\"\",\"\",INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,9))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A9=\"\",\"\",A9)","v":""},7,"",{"$f":"Vokabel!$A$25","v":"Tel.Nr."},null,null,"E-Mail"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A10=\"\",\"\",A10)","v":""},8,"",{"$f":"IF(INDEX(Kundenstamm!$A$3:$L$7000,Kundenstamm!$T$2,11)=\"\",\"\",INDEX(Kundenstamm!$A$3:$L$7000,Kundenstamm!$T$2,11))","v":""},null,null,{"$f":"IF(INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,10)=\"\",\"\",INDEX(Kundenstamm!$A$3:$J$7000,Kundenstamm!$T$2,10))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U10+1","v":9},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",10,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",11,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",12,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",13,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",14,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",15,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",16,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",17,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",18,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",19,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",20,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",21,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",22,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",23,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",24,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",25,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",26,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",27,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",28,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",29,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",30,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",31,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",32,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",33,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",34,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",35,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",36,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",37,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",38,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",39,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",40,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",41,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",42,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",43,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",44,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",45,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",46,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",47,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",48,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",49,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",50,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",51,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",52,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",53,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",54,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",55,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",56,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",57,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",58,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",59,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",60,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",61,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",62,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",63,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",64,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B67=\"\",\"\",B67&\", \"&F67&\",     \"&G67)","v":""},"",{"$f":"U66+1","v":65},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",66,{"$f":"T68","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",67,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",68,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",69,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",70,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",71,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A74=\"\",\"\",A74)","v":""},72,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",73,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",74,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",75,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",76,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",77,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",78,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",79,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",80,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",81,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",82,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",83,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",84,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",85,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",86,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",87,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",88,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",89,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",90,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",91,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",92,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",93,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",94,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",95,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",96,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",97,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",98,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",99,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",100,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",101,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",102,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",103,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",104,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",105,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",106,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",107,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",108,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",109,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",110,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",111,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",112,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",113,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",114,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",115,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",116,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",117,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",118,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",119,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",120,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",121,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",122,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",123,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",124,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",125,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",126,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",127,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",128,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B131=\"\",\"\",B131&\", \"&F131&\",     \"&G131)","v":""},"",{"$f":"U130+1","v":129},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",130,{"$f":"T132","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",131,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",132,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",133,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",134,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",135,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A138=\"\",\"\",A138)","v":""},136,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",137,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",138,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",139,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",140,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",141,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",142,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",143,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",144,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",145,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",146,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",147,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",148,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",149,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",150,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",151,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",152,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",153,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",154,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",155,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",156,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",157,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",158,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",159,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",160,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",161,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",162,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",163,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",164,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",165,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",166,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",167,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",168,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",169,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",170,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",171,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",172,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",173,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",174,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",175,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",176,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",177,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",178,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",179,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",180,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",181,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",182,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",183,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",184,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",185,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",186,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",187,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",188,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",189,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",190,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",191,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",192,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B195=\"\",\"\",B195&\", \"&F195&\",     \"&G195)","v":""},"",{"$f":"U194+1","v":193},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",194,{"$f":"T196","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",195,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",196,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",197,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",198,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",199,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A202=\"\",\"\",A202)","v":""},200,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",201,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",202,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",203,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",204,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",205,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",206,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",207,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",208,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",209,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",210,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",211,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",212,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",213,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",214,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",215,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",216,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",217,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",218,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",219,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",220,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",221,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",222,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",223,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",224,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",225,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",226,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",227,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",228,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",229,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",230,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",231,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",232,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",233,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",234,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",235,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",236,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",237,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",238,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",239,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",240,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",241,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",242,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",243,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",244,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",245,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",246,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",247,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",248,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",249,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",250,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",251,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",252,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",253,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",254,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",255,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",256,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B259=\"\",\"\",B259&\", \"&F259&\",     \"&G259)","v":""},"",{"$f":"U258+1","v":257},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",258,{"$f":"T260","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",259,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",260,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",261,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",262,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",263,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A266=\"\",\"\",A266)","v":""},264,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",265,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",266,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",267,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",268,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",269,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",270,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",271,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",272,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",273,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",274,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",275,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",276,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",277,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",278,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",279,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",280,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",281,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",282,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",283,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",284,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",285,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",286,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",287,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",288,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",289,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",290,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",291,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",292,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",293,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",294,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",295,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",296,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",297,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",298,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",299,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",300,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",301,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",302,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",303,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",304,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",305,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",306,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",307,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",308,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",309,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",310,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",311,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",312,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",313,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",314,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",315,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",316,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",317,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",318,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",319,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",320,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B323=\"\",\"\",B323&\", \"&F323&\",     \"&G323)","v":""},"",{"$f":"U322+1","v":321},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",322,{"$f":"T324","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",323,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",324,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",325,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",326,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",327,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A330=\"\",\"\",A330)","v":""},328,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",329,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",330,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",331,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",332,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",333,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",334,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",335,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",336,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",337,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",338,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",339,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",340,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",341,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",342,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",343,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",344,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",345,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",346,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",347,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",348,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",349,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",350,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",351,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",352,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",353,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",354,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",355,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",356,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",357,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",358,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",359,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",360,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",361,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",362,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",363,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",364,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",365,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",366,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",367,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",368,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",369,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",370,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",371,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",372,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",373,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",374,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",375,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",376,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",377,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",378,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",379,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",380,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",381,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",382,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",383,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",384,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B387=\"\",\"\",B387&\", \"&F387&\",     \"&G387)","v":""},"",{"$f":"U386+1","v":385},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",386,{"$f":"T388","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",387,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",388,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",389,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",390,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",391,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A394=\"\",\"\",A394)","v":""},392,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",393,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",394,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",395,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",396,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",397,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",398,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",399,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",400,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",401,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",402,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",403,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",404,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",405,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",406,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",407,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",408,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",409,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",410,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",411,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",412,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",413,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",414,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",415,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",416,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",417,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",418,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",419,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",420,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",421,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",422,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",423,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",424,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",425,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",426,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",427,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",428,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",429,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",430,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",431,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",432,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",433,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",434,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",435,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",436,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",437,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",438,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",439,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",440,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",441,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",442,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",443,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",444,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",445,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",446,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",447,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",448,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B451=\"\",\"\",B451&\", \"&F451&\",     \"&G451)","v":""},"",{"$f":"U450+1","v":449},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",450,{"$f":"T452","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",451,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",452,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",453,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",454,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",455,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A458=\"\",\"\",A458)","v":""},456,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",457,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",458,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",459,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",460,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",461,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",462,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",463,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",464,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",465,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",466,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",467,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",468,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",469,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",470,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",471,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",472,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",473,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",474,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",475,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",476,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",477,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",478,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",479,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",480,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",481,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",482,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",483,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",484,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",485,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",486,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",487,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",488,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",489,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",490,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",491,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",492,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",493,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",494,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",495,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",496,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",497,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",498,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",499,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",500,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",501,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",502,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",503,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",504,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",505,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",506,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",507,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",508,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",509,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",510,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",511,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",512,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B515=\"\",\"\",B515&\", \"&F515&\",     \"&G515)","v":""},"",{"$f":"U514+1","v":513},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",514,{"$f":"T516","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",515,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",516,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",517,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",518,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",519,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A522=\"\",\"\",A522)","v":""},520,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",521,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",522,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",523,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",524,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",525,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",526,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",527,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",528,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",529,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",530,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",531,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",532,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",533,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",534,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",535,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",536,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",537,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",538,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",539,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",540,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",541,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",542,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",543,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",544,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",545,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",546,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",547,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",548,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",549,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",550,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",551,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",552,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",553,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",554,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",555,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",556,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",557,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",558,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",559,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",560,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",561,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",562,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",563,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",564,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",565,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",566,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",567,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",568,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",569,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",570,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",571,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",572,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",573,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",574,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",575,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",576,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B579=\"\",\"\",B579&\", \"&F579&\",     \"&G579)","v":""},"",{"$f":"U578+1","v":577},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",578,{"$f":"T580","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",579,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",580,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",581,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",582,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",583,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A586=\"\",\"\",A586)","v":""},584,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",585,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",586,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",587,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",588,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",589,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",590,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",591,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",592,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",593,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",594,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",595,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",596,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",597,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",598,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",599,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",600,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",601,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",602,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",603,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",604,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",605,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",606,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",607,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",608,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",609,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",610,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",611,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A614=\"\",\"\",A614)","v":""},{"$f":"U613+1","v":612},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",613,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",614,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",615,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",616,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",617,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",618,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",619,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",620,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",621,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",622,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",623,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",624,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",625,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",626,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",627,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",628,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",629,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",630,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",631,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",632,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",633,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",634,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",635,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",636,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",637,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",638,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",639,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",640,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B643=\"\",\"\",B643&\", \"&F643&\",     \"&G643)","v":""},"",641,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",642,{"$f":"T644","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",643,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",644,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",645,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",646,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",647,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",648,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",649,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",650,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",651,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",652,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",653,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",654,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",655,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",656,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",657,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",658,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",659,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",660,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",661,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",662,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",663,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",664,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",665,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",666,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",667,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",668,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",669,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",670,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",671,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",672,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",673,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",674,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",675,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A678=\"\",\"\",A678)","v":""},{"$f":"U677+1","v":676},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",677,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",678,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",679,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",680,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",681,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",682,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",683,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",684,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",685,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",686,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",687,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",688,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",689,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",690,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",691,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",692,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",693,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",694,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",695,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",696,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",697,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",698,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",699,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",700,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",701,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",702,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",703,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",704,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B707=\"\",\"\",B707&\", \"&F707&\",     \"&G707)","v":""},"",705,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",706,{"$f":"T708","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",707,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",708,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",709,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",710,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",711,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",712,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",713,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",714,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",715,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",716,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",717,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",718,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",719,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",720,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",721,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",722,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",723,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",724,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",725,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",726,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",727,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",728,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",729,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",730,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",731,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",732,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",733,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",734,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",735,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",736,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",737,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",738,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",739,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A742=\"\",\"\",A742)","v":""},{"$f":"U741+1","v":740},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",741,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",742,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",743,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",744,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",745,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",746,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",747,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",748,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",749,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",750,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",751,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",752,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",753,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",754,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",755,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",756,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",757,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",758,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",759,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",760,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",761,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",762,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",763,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",764,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",765,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",766,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",767,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",768,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B771=\"\",\"\",B771&\", \"&F771&\",     \"&G771)","v":""},"",769,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",770,{"$f":"T772","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",771,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",772,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",773,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",774,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",775,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",776,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",777,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",778,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",779,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",780,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",781,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",782,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",783,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",784,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",785,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",786,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",787,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",788,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",789,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",790,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",791,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",792,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",793,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",794,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",795,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",796,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",797,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",798,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",799,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",800,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",801,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",802,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",803,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A806=\"\",\"\",A806)","v":""},{"$f":"U805+1","v":804},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",805,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",806,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",807,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",808,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",809,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",810,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",811,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",812,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",813,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",814,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",815,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",816,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",817,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",818,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",819,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",820,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",821,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",822,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",823,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",824,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",825,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",826,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",827,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",828,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",829,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",830,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",831,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",832,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B835=\"\",\"\",B835&\", \"&F835&\",     \"&G835)","v":""},"",833,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",834,{"$f":"T836","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",835,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",836,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",837,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",838,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",839,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",840,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",841,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",842,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",843,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",844,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",845,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",846,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",847,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",848,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",849,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",850,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",851,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",852,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",853,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",854,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",855,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",856,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",857,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",858,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",859,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",860,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",861,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",862,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",863,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",864,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",865,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",866,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",867,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A870=\"\",\"\",A870)","v":""},{"$f":"U869+1","v":868},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",869,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",870,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",871,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",872,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",873,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",874,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",875,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",876,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",877,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",878,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",879,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",880,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",881,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",882,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",883,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",884,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",885,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",886,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",887,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",888,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",889,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",890,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",891,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",892,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",893,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",894,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",895,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",896,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B899=\"\",\"\",B899&\", \"&F899&\",     \"&G899)","v":""},"",897,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",898,{"$f":"T900","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",899,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",900,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",901,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",902,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",903,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",904,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",905,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",906,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",907,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",908,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",909,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",910,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",911,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",912,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",913,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",914,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",915,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",916,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",917,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",918,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",919,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",920,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",921,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",922,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",923,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",924,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",925,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",926,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",927,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",928,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",929,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",930,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",931,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A934=\"\",\"\",A934)","v":""},{"$f":"U933+1","v":932},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",933,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",934,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",935,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",936,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",937,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",938,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",939,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",940,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",941,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",942,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",943,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",944,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",945,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",946,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",947,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",948,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",949,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",950,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",951,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",952,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",953,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",954,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",955,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",956,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",957,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",958,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",959,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",960,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B963=\"\",\"\",B963&\", \"&F963&\",     \"&G963)","v":""},"",961,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",962,{"$f":"T964","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",963,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",964,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",965,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",966,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",967,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",968,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",969,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",970,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",971,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",972,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",973,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",974,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",975,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",976,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",977,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",978,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",979,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",980,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",981,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",982,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",983,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",984,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",985,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",986,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",987,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",988,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",989,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",990,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",991,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",992,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",993,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",994,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",995,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A998=\"\",\"\",A998)","v":""},{"$f":"U997+1","v":996},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",997,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",998,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",999,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1000,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1001,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1002,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1003,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1004,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1005,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1006,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1007,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1008,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1009,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1010,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1011,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1012,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1013,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1014,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1015,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1016,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1017,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1018,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1019,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1020,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1021,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1022,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1023,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1024,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1027=\"\",\"\",B1027&\", \"&F1027&\",     \"&G1027)","v":""},"",1025,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1026,{"$f":"T1028","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1027,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1028,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1029,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1030,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1031,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1032,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1033,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1034,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1035,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1036,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1037,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1038,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1039,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1040,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1041,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1042,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1043,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1044,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1045,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1046,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1047,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1048,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1049,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1050,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1051,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1052,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1053,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1054,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1055,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1056,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1057,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1058,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1059,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1062=\"\",\"\",A1062)","v":""},{"$f":"U1061+1","v":1060},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1061,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1062,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1063,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1064,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1065,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1066,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1067,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1068,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1069,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1070,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1071,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1072,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1073,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1074,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1075,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1076,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1077,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1078,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1079,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1080,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1081,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1082,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1083,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1084,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1085,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1086,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1087,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1088,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1091=\"\",\"\",B1091&\", \"&F1091&\",     \"&G1091)","v":""},"",1089,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1090,{"$f":"T1092","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1091,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1092,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1093,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1094,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1095,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1096,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1097,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1098,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1099,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1100,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1101,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1102,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1103,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1104,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1105,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1106,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1107,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1108,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1109,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1110,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1111,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1112,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1113,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1114,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1115,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1116,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1117,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1118,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1119,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1120,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1121,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1122,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1123,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1126=\"\",\"\",A1126)","v":""},{"$f":"U1125+1","v":1124},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1125,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1126,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1127,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1128,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1129,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1130,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1131,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1132,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1133,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1134,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1135,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1136,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1137,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1138,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1139,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1140,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1141,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1142,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1143,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1144,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1145,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1146,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1147,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1148,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1149,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1150,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1151,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1152,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1155=\"\",\"\",B1155&\", \"&F1155&\",     \"&G1155)","v":""},"",1153,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1154,{"$f":"T1156","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1155,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1156,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1157,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1158,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1159,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1160,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1161,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1162,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1163,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1164,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1165,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1166,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1167,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1168,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1169,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1170,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1171,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1172,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1173,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1174,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1175,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1176,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1177,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1178,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1179,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1180,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1181,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1182,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1183,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1184,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1185,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1186,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1187,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1190=\"\",\"\",A1190)","v":""},{"$f":"U1189+1","v":1188},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1189,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1190,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1191,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1192,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1193,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1194,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1195,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1196,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1197,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1198,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1199,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1200,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1201,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1202,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1203,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1204,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1205,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1206,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1207,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1208,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1209,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1210,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1211,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1212,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1213,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1214,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1215,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1216,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1219=\"\",\"\",B1219&\", \"&F1219&\",     \"&G1219)","v":""},"",1217,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1218,{"$f":"T1220","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1219,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1220,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1221,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1222,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1223,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1224,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1225,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1226,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1227,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1228,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1229,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1230,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1231,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1232,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1233,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1234,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1235,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1236,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1237,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1238,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1239,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1240,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1241,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1242,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1243,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1244,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1245,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1246,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1247,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1248,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1249,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1250,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1251,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1254=\"\",\"\",A1254)","v":""},{"$f":"U1253+1","v":1252},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1253,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1254,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1255,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1256,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1257,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1258,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1259,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1260,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1261,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1262,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1263,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1264,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1265,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1266,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1267,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1268,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1269,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1270,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1271,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1272,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1273,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1274,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1275,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1276,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1277,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1278,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1279,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1280,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1283=\"\",\"\",B1283&\", \"&F1283&\",     \"&G1283)","v":""},"",1281,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1282,{"$f":"T1284","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1283,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1284,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1285,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1286,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1287,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1288,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1289,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1290,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1291,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1292,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1293,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1294,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1295,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1296,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1297,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1298,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1299,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1300,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1301,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1302,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1303,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1304,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1305,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1306,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1307,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1308,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1309,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1310,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1311,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1312,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1313,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1314,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1315,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1318=\"\",\"\",A1318)","v":""},{"$f":"U1317+1","v":1316},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1317,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1318,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1319,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1320,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1321,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1322,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1323,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1324,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1325,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1326,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1327,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1328,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1329,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1330,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1331,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1332,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1333,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1334,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1335,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1336,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1337,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1338,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1339,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1340,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1341,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1342,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1343,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1344,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1347=\"\",\"\",B1347&\", \"&F1347&\",     \"&G1347)","v":""},"",1345,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1346,{"$f":"T1348","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1347,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1348,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1349,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1350,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1351,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1352,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1353,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1354,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1355,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1356,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1357,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1358,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1359,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1360,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1361,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1362,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1363,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1364,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1365,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1366,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1367,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1368,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1369,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1370,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1371,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1372,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1373,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1374,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1375,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1376,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1377,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1378,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1379,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1382=\"\",\"\",A1382)","v":""},{"$f":"U1381+1","v":1380},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1381,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1382,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1383,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1384,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1385,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1386,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1387,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1388,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1389,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1390,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1391,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1392,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1393,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1394,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1395,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1396,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1397,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1398,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1399,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1400,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1401,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1402,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1403,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1404,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1405,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1406,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1407,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1408,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1411=\"\",\"\",B1411&\", \"&F1411&\",     \"&G1411)","v":""},"",1409,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1410,{"$f":"T1412","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1411,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1412,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1413,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1414,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1415,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1416,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1417,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1418,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1419,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1420,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1421,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1422,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1423,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1424,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1425,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1426,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1427,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1428,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1429,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1430,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1431,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1432,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1433,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1434,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1435,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1436,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1437,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1438,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1439,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1440,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1441,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1442,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1443,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1446=\"\",\"\",A1446)","v":""},{"$f":"U1445+1","v":1444},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1445,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1446,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1447,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1448,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1449,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1450,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1451,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1452,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1453,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1454,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1455,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1456,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1457,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1458,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1459,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1460,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1461,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1462,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1463,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1464,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1465,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1466,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1467,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1468,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1469,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1470,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1471,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1472,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1475=\"\",\"\",B1475&\", \"&F1475&\",     \"&G1475)","v":""},"",1473,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1474,{"$f":"T1476","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1475,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1476,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1477,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1478,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1479,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1480,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1481,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1482,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1483,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1484,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1485,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1486,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1487,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1488,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1489,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1490,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1491,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1492,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1493,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1494,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1495,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1496,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1497,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1498,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1499,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1500,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1501,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1502,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1503,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1504,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1505,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1506,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1507,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1510=\"\",\"\",A1510)","v":""},{"$f":"U1509+1","v":1508},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1509,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1510,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1511,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1512,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1513,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1514,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1515,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1516,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1517,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1518,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1519,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1520,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1521,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1522,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1523,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1524,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1525,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1526,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1527,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1528,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1529,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1530,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1531,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1532,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1533,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1534,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1535,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1536,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1539=\"\",\"\",B1539&\", \"&F1539&\",     \"&G1539)","v":""},"",1537,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1538,{"$f":"T1540","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1539,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1540,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1541,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1542,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1543,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1544,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1545,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1546,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1547,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1548,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1549,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1550,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1551,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1552,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1553,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1554,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1555,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1556,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1557,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1558,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1559,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1560,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1561,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1562,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1563,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1564,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1565,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1566,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1567,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1568,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1569,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1570,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1571,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1574=\"\",\"\",A1574)","v":""},{"$f":"U1573+1","v":1572},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1573,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1574,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1575,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1576,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1577,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1578,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1579,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1580,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1581,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1582,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1583,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1584,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1585,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1586,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1587,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1588,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1589,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1590,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1591,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1592,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1593,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1594,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1595,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1596,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1597,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1598,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1599,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1600,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1603=\"\",\"\",B1603&\", \"&F1603&\",     \"&G1603)","v":""},"",1601,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1602,{"$f":"T1604","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1603,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1604,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1605,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1606,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1607,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1608,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1609,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1610,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1611,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1612,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1613,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1614,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1615,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1616,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1617,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1618,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1619,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1620,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1621,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1622,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1623,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1624,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1625,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1626,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1627,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1628,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1629,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1630,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1631,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1632,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1633,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1634,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1635,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1638=\"\",\"\",A1638)","v":""},{"$f":"U1637+1","v":1636},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1637,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1638,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1639,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1640,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1641,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1642,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1643,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1644,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1645,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1646,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1647,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1648,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1649,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1650,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1651,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1652,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1653,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1654,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1655,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1656,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1657,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1658,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1659,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1660,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1661,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1662,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1663,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1664,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1667=\"\",\"\",B1667&\", \"&F1667&\",     \"&G1667)","v":""},"",1665,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1666,{"$f":"T1668","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1667,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1668,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1669,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1670,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1671,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1672,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1673,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1674,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1675,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1676,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1677,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1678,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1679,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1680,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1681,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1682,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1683,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1684,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1685,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1686,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1687,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1688,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1689,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1690,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1691,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1692,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1693,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1694,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1695,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1696,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1697,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1698,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1699,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1702=\"\",\"\",A1702)","v":""},{"$f":"U1701+1","v":1700},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1701,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1702,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1703,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1704,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1705,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1706,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1707,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1708,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1709,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1710,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1711,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1712,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1713,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1714,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1715,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1716,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1717,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1718,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1719,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1720,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1721,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1722,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1723,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1724,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1725,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1726,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1727,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1728,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1731=\"\",\"\",B1731&\", \"&F1731&\",     \"&G1731)","v":""},"",1729,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1730,{"$f":"T1732","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1731,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1732,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1733,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1734,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1735,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1736,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1737,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1738,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1739,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1740,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1741,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1742,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1743,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1744,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1745,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1746,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1747,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1748,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1749,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1750,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1751,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1752,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1753,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1754,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1755,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1756,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1757,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1758,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1759,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1760,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1761,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1762,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1763,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1766=\"\",\"\",A1766)","v":""},{"$f":"U1765+1","v":1764},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1765,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1766,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1767,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1768,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1769,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1770,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1771,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1772,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1773,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1774,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1775,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1776,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1777,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1778,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1779,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1780,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1781,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1782,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1783,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1784,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1785,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1786,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1787,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1788,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1789,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1790,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1791,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1792,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1795=\"\",\"\",B1795&\", \"&F1795&\",     \"&G1795)","v":""},"",1793,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1794,{"$f":"T1796","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1795,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1796,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1797,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1798,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1799,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1800,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1801,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1802,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1803,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1804,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1805,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1806,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1807,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1808,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1809,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1810,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1811,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1812,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1813,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1814,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1815,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1816,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1817,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1818,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1819,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1820,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1821,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1822,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1823,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1824,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1825,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1826,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1827,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1830=\"\",\"\",A1830)","v":""},{"$f":"U1829+1","v":1828},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1829,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1830,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1831,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1832,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1833,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1834,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1835,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1836,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1837,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1838,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1839,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1840,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1841,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1842,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1843,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1844,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1845,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1846,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1847,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1848,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1849,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1850,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1851,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1852,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1853,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1854,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1855,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1856,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1859=\"\",\"\",B1859&\", \"&F1859&\",     \"&G1859)","v":""},"",1857,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1858,{"$f":"T1860","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1859,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1860,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1861,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1862,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1863,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1864,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1865,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1866,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1867,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1868,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1869,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1870,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1871,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1872,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1873,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1874,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1875,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1876,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1877,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1878,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1879,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1880,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1881,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1882,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1883,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1884,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1885,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1886,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1887,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1888,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1889,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1890,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1891,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1894=\"\",\"\",A1894)","v":""},{"$f":"U1893+1","v":1892},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1893,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1894,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1895,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1896,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1897,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1898,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1899,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1900,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1901,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1902,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1903,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1904,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1905,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1906,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1907,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1908,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1909,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1910,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1911,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1912,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1913,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1914,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1915,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1916,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1917,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1918,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1919,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1920,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1923=\"\",\"\",B1923&\", \"&F1923&\",     \"&G1923)","v":""},"",1921,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1922,{"$f":"T1924","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1923,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1924,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1925,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1926,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1927,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1928,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1929,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1930,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1931,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1932,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1933,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1934,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1935,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1936,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1937,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1938,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1939,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1940,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1941,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1942,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1943,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1944,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1945,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1946,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1947,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1948,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1949,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1950,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1951,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1952,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1953,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1954,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1955,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A1958=\"\",\"\",A1958)","v":""},{"$f":"U1957+1","v":1956},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1957,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1958,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1959,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1960,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1961,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1962,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1963,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1964,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1965,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1966,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1967,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1968,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1969,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1970,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1971,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1972,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1973,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1974,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1975,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1976,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1977,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1978,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1979,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1980,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1981,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1982,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1983,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1984,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B1987=\"\",\"\",B1987&\", \"&F1987&\",     \"&G1987)","v":""},"",1985,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1986,{"$f":"T1988","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1987,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1988,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1989,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1990,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1991,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1992,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1993,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1994,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1995,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1996,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1997,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",1998,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2000,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2001,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2004,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2007,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2009,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2010,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2013,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2014,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2018,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2019,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2022,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2025,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2027,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2028,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2031,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2032,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2036,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2037,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2040,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2043,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2045,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2046,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B2051=\"\",\"\",B2051&\", \"&F2051&\",     \"&G2051)","v":""},"",2049,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2050,{"$f":"T2052","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2054,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2055,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2058,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2061,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2063,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2064,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2067,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2068,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2072,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2073,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2076,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2079,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2081,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2082,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2085,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2086,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2090,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2091,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2094,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2097,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2099,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2100,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2103,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2104,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2108,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2109,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2112,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2115,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2117,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2118,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2121,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2123,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2126,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2127,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2130,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2133,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2135,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2136,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2139,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2141,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2144,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2145,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A2150=\"\",\"\",A2150)","v":""},{"$f":"U2149+1","v":2148},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2151,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2153,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2154,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2157,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2159,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2162,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2163,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2166,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2169,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2171,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2172,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2175,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B2179=\"\",\"\",B2179&\", \"&F2179&\",     \"&G2179)","v":""},"",2177,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2180,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2181,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2184,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2187,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2189,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2190,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2193,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2195,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2198,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2199,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2202,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2205,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2207,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2208,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2211,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2213,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2216,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2217,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2220,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2223,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2225,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2226,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2229,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2231,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2234,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2235,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2238,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B2243=\"\",\"\",B2243&\", \"&F2243&\",     \"&G2243)","v":""},"",2241,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2243,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2244,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2247,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2249,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2252,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2253,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2256,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2259,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2261,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2262,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2265,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2267,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2270,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2271,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2274,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2277,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2279,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2280,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2283,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2285,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2288,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2289,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2292,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2293,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2297,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2298,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2301,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2303,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2306,{"$f":"T2308","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2307,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2310,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2311,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2315,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2316,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2319,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2321,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2324,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2325,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2328,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2329,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2333,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2334,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2337,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2339,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2342,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2343,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2346,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2347,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2351,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2352,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2355,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2357,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2360,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2361,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2364,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2365,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B2371=\"\",\"\",B2371&\", \"&F2371&\",     \"&G2371)","v":""},"",2369,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2370,{"$f":"T2372","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2373,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2375,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2378,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2379,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2382,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2383,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2387,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2388,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2391,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2393,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2396,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2397,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2400,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2401,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2405,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2406,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2409,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2411,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2414,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2415,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2418,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2419,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2423,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2424,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2427,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2429,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2432,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B2435=\"\",\"\",B2435&\", \"&F2435&\",     \"&G2435)","v":""},"",2433,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2436,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2437,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2441,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2442,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2445,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2448,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2450,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2451,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2454,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2455,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2459,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2460,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2463,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2466,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A2470=\"\",\"\",A2470)","v":""},{"$f":"U2469+1","v":2468},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2469,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2472,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2473,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2477,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2478,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2481,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2484,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2486,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2487,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2490,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2491,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2495,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2496,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2499,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2502,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2504,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2505,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2508,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2509,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2513,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2514,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2517,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2520,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2522,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2523,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2526,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2527,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2531,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A2534=\"\",\"\",A2534)","v":""},{"$f":"U2533+1","v":2532},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2535,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2538,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2540,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2541,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2544,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2545,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2549,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2550,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2553,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2556,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2558,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2559,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2562,{"$f":"T2564","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2563,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2567,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2568,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2571,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2574,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2576,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2577,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2580,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2581,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2585,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2586,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2589,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2592,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2594,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2595,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2598,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2599,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2603,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2604,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2607,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2610,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2612,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2613,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2616,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2618,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2621,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2622,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B2627=\"\",\"\",B2627&\", \"&F2627&\",     \"&G2627)","v":""},"",2625,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2628,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2630,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2631,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2634,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2636,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2639,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2640,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2643,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2646,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2648,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2649,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2652,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2654,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2657,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2658,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2661,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2664,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2666,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2667,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2670,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2672,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2675,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2676,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2679,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2682,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2684,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2685,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2688,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2690,{"$f":"T2692","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2693,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2694,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2697,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2700,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2702,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2703,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2706,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2708,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2711,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2712,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2715,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2718,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2720,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2721,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A2726=\"\",\"\",A2726)","v":""},{"$f":"U2725+1","v":2724},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2726,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2729,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2730,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2733,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2736,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2738,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2739,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2742,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2744,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2747,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2748,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2751,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2754,{"$f":"T2756","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2756,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2757,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2760,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2762,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2765,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2766,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2769,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2770,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2774,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2775,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2778,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2780,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2783,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2784,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2787,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A2790=\"\",\"\",A2790)","v":""},{"$f":"U2789+1","v":2788},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2792,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2793,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2796,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2798,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2801,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2802,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2805,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2806,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2810,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2811,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2814,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2816,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2819,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2820,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2823,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2824,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2828,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2829,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2832,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2834,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2837,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2838,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2841,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2842,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2846,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2847,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2850,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A2854=\"\",\"\",A2854)","v":""},{"$f":"U2853+1","v":2852},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2855,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2856,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2859,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2860,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2864,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2865,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2868,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2870,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2873,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2874,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2877,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2878,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2882,{"$f":"T2884","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2883,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2886,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2888,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2891,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2892,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2895,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2896,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2900,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2901,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2904,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2906,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2909,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2910,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2913,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2914,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2918,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2919,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2922,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2924,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2927,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2928,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2931,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2932,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2936,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2937,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2940,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2943,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B2947=\"\",\"\",B2947&\", \"&F2947&\",     \"&G2947)","v":""},"",2945,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2946,{"$f":"T2948","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2949,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2950,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2954,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2955,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2958,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2961,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2963,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2964,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2967,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2968,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2972,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2973,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2976,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2979,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2981,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2982,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2985,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2986,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2990,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2991,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2994,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2997,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",2999,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3000,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3003,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3004,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3008,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B3011=\"\",\"\",B3011&\", \"&F3011&\",     \"&G3011)","v":""},"",3009,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3012,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3015,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3017,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3018,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3021,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3022,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3026,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3027,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3030,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3033,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3035,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3036,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3039,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3040,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A3046=\"\",\"\",A3046)","v":""},{"$f":"U3045+1","v":3044},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3045,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3048,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3051,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3053,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3054,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3057,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3058,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3062,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3063,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3066,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3069,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3071,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3072,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3075,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3076,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3080,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3081,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3084,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3087,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3089,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3090,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3093,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3095,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3098,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3099,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3102,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3105,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3107,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A3110=\"\",\"\",A3110)","v":""},{"$f":"U3109+1","v":3108},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3111,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3113,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3116,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3117,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3120,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3123,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3125,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3126,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3129,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3131,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3134,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3135,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3138,{"$f":"T3140","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3141,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3143,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3144,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3147,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3149,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3152,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3153,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3156,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3159,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3161,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3162,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3165,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3167,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3170,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3171,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3174,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3177,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3179,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3180,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3183,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3185,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3188,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3189,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3192,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3195,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3197,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3198,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B3203=\"\",\"\",B3203&\", \"&F3203&\",     \"&G3203)","v":""},"",3201,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3203,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3206,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3207,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3210,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3213,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3215,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3216,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3219,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3221,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3224,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3225,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3228,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3231,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3233,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3234,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3237,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3239,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3242,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3243,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3246,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3249,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3251,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3252,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3255,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3257,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3260,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3261,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3264,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B3267=\"\",\"\",B3267&\", \"&F3267&\",     \"&G3267)","v":""},"",3265,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3269,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3270,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3273,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3275,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3278,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3279,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3282,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3283,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3287,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3288,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3291,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3293,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3296,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3297,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A3302=\"\",\"\",A3302)","v":""},{"$f":"U3301+1","v":3300},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3301,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3305,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3306,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3309,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3311,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3314,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3315,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3318,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3319,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3323,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3324,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3327,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B3331=\"\",\"\",B3331&\", \"&F3331&\",     \"&G3331)","v":""},"",3329,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3332,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3333,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3336,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3337,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3341,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3342,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3345,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3347,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3350,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3351,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3354,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3355,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3359,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3360,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3363,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3365,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3368,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3369,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3372,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3373,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3377,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3378,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3381,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3383,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3386,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3387,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3390,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3391,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3395,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3396,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3399,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3401,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3404,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3405,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3408,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3409,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3413,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3414,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3417,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3420,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3422,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3423,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3426,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3427,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3431,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3432,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3435,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3438,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3440,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3441,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3444,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3445,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3449,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3450,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3453,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3456,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3458,{"$f":"T3460","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3459,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3462,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3463,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3467,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3468,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3471,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3474,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3476,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3477,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3480,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3481,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3485,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3486,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3489,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A3494=\"\",\"\",A3494)","v":""},{"$f":"U3493+1","v":3492},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3494,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3495,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3498,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3499,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3503,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3504,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3507,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3510,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3512,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3513,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3516,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3517,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B3523=\"\",\"\",B3523&\", \"&F3523&\",     \"&G3523)","v":""},"",3521,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3522,{"$f":"T3524","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3525,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3528,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3530,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3531,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3534,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3535,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3539,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3540,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3543,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3546,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3548,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3549,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3552,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3553,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3557,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3558,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3561,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3564,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3566,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3567,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3570,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3571,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3575,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3576,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3579,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3582,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3584,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B3587=\"\",\"\",B3587&\", \"&F3587&\",     \"&G3587)","v":""},"",3585,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3588,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3590,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3593,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3594,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3597,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3600,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3602,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3603,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3606,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3608,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3611,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3612,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3615,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3618,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A3622=\"\",\"\",A3622)","v":""},{"$f":"U3621+1","v":3620},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3621,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3624,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3626,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3629,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3630,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3633,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3636,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3638,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3639,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3642,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3644,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3647,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3648,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3651,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3654,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3656,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3657,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3660,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3662,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3665,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3666,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3669,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3672,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3674,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3675,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3678,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3680,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3683,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A3686=\"\",\"\",A3686)","v":""},{"$f":"U3685+1","v":3684},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3687,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3690,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3692,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3693,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3696,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3698,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3701,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3702,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3705,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3708,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3710,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3711,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3714,{"$f":"T3716","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3716,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3719,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3720,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3723,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3726,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3728,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3729,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3732,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3734,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3737,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3738,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3741,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3742,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3746,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3747,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3750,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3752,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3755,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3756,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3759,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3760,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3764,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3765,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3768,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3770,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3773,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3774,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B3779=\"\",\"\",B3779&\", \"&F3779&\",     \"&G3779)","v":""},"",3777,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3778,{"$f":"T3780","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3782,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3783,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3786,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3788,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3791,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3792,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3795,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3796,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3800,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3801,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3804,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3806,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3809,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3810,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3813,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3814,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3818,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3819,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3822,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3824,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3827,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3828,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3831,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3832,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3836,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3837,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3840,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3842,{"$f":"T3844","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3845,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3846,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3849,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3850,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3854,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3855,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3858,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3860,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3863,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3864,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3867,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3868,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3872,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3873,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A3878=\"\",\"\",A3878)","v":""},{"$f":"U3877+1","v":3876},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3878,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3881,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3882,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3885,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3886,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3890,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3891,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3894,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3896,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3899,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3900,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3903,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3904,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3908,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3909,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3912,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3915,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3917,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3918,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3921,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3922,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3926,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3927,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3930,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3933,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3935,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3936,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3939,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A3942=\"\",\"\",A3942)","v":""},{"$f":"U3941+1","v":3940},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3944,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3945,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3948,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3951,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3953,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3954,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3957,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3958,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3962,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3963,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3966,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B3971=\"\",\"\",B3971&\", \"&F3971&\",     \"&G3971)","v":""},"",3969,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3971,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3972,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3975,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3976,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3980,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3981,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3984,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3987,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3989,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3990,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3993,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3994,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3998,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",3999,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4002,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4005,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4007,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4008,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4011,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4012,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4016,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4017,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4020,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4023,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4025,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4026,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4029,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4030,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4034,{"$f":"T4036","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4035,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4038,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4041,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4043,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4044,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4047,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4048,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4052,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4053,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4056,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4059,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4061,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4062,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4065,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4067,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4070,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4071,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4074,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4077,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4079,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4080,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4083,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4085,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4088,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4089,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4092,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4095,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B4099=\"\",\"\",B4099&\", \"&F4099&\",     \"&G4099)","v":""},"",4097,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4098,{"$f":"T4100","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4101,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4103,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4106,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4107,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4110,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4113,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4115,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4116,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4119,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4121,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4124,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4125,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4128,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4131,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4133,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4134,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4137,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4139,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4142,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4143,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4146,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4149,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4151,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4152,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4155,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4157,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4160,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B4163=\"\",\"\",B4163&\", \"&F4163&\",     \"&G4163)","v":""},"",4161,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4164,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4167,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4169,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4170,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4173,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4175,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4178,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4179,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4182,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4185,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4187,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4188,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4191,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4193,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A4198=\"\",\"\",A4198)","v":""},{"$f":"U4197+1","v":4196},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4197,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4200,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4203,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4205,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4206,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4209,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4211,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4214,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4215,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4218,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4219,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4223,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4224,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4227,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4229,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4232,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4233,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4236,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4237,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4241,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4242,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4245,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4247,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4250,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4251,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4254,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4255,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4259,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A4262=\"\",\"\",A4262)","v":""},{"$f":"U4261+1","v":4260},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4263,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4265,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4268,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4269,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4272,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4273,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4277,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4278,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4281,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4283,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4286,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4287,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4290,{"$f":"T4292","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4291,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4295,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4296,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4299,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4301,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4304,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4305,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4308,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4309,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4313,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4314,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4317,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4319,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4322,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4323,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4326,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4327,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4331,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4332,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4335,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4337,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4340,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4341,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4344,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4345,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4349,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4350,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B4355=\"\",\"\",B4355&\", \"&F4355&\",     \"&G4355)","v":""},"",4353,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4355,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4358,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4359,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4362,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4363,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4367,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4368,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4371,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4373,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4376,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4377,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4380,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4381,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4385,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4386,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4389,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4392,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4394,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4395,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4398,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4399,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4403,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4404,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4407,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4410,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4412,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4413,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4416,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B4419=\"\",\"\",B4419&\", \"&F4419&\",     \"&G4419)","v":""},"",4417,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4421,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4422,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4425,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4428,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4430,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4431,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4434,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4435,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4439,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4440,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4443,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4446,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4448,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4449,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A4454=\"\",\"\",A4454)","v":""},{"$f":"U4453+1","v":4452},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4453,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4457,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4458,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4461,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4464,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4466,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4467,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4470,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4471,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4475,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4476,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4479,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4482,{"$f":"T4484","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4484,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4485,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4488,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4489,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4493,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4494,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4497,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4500,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4502,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4503,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4506,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4507,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4511,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4512,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4515,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4518,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4520,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4521,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4524,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4525,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4529,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4530,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4533,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4536,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4538,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4539,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4542,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4544,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4547,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4548,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4551,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4554,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4556,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4557,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4560,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4562,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4565,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4566,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4569,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4572,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4574,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4575,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4578,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A4582=\"\",\"\",A4582)","v":""},{"$f":"U4581+1","v":4580},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4583,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4584,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4587,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4590,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4592,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4593,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4596,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4598,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4601,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4602,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4605,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4608,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4610,{"$f":"T4612","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4611,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4614,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4616,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4619,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4620,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4623,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4626,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4628,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4629,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4632,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4634,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4637,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4638,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4641,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A4646=\"\",\"\",A4646)","v":""},{"$f":"U4645+1","v":4644},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4646,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4647,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4650,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4652,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4655,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4656,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4659,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4662,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4664,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4665,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4668,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4670,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B4675=\"\",\"\",B4675&\", \"&F4675&\",     \"&G4675)","v":""},"",4673,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4674,{"$f":"T4676","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4677,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4680,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4682,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4683,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4686,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4688,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4691,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4692,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4695,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4698,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4700,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4701,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4704,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4706,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4709,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4710,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4713,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4714,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4718,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4719,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4722,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4724,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4727,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4728,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4731,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4732,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4736,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B4739=\"\",\"\",B4739&\", \"&F4739&\",     \"&G4739)","v":""},"",4737,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4740,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4742,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4745,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4746,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4749,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4750,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4754,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4755,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4758,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4760,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4763,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4764,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4767,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4768,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A4774=\"\",\"\",A4774)","v":""},{"$f":"U4773+1","v":4772},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4773,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4776,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4778,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4781,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4782,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4785,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4786,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4790,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4791,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4794,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4796,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4799,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4800,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4803,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4804,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4808,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4809,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4812,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4814,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4817,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4818,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4821,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4822,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4826,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4827,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4830,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4832,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4835,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A4838=\"\",\"\",A4838)","v":""},{"$f":"U4837+1","v":4836},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4839,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4840,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4844,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4845,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4848,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4850,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4853,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4854,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4857,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4858,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4862,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4863,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4866,{"$f":"T4868","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4869,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4871,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4872,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4875,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4876,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4880,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4881,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4884,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4887,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4889,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4890,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4893,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4894,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4898,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4899,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4902,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4905,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4907,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4908,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4911,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4912,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4916,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4917,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4920,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4923,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4925,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4926,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B4931=\"\",\"\",B4931&\", \"&F4931&\",     \"&G4931)","v":""},"",4929,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4930,{"$f":"T4932","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4934,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4935,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4938,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4941,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4943,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4944,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4947,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4948,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4952,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4953,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4956,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4959,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4961,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4962,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4965,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4966,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4970,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4971,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4974,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4977,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4979,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4980,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4983,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4984,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4988,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4989,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4992,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4995,{"$f":"T4997","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4997,{"$f":"T4999","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",4998,{"$f":"T5000","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5001,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5002,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5006,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5007,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5010,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5013,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5015,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5016,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5019,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5020,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5024,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5025,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U5029+1","v":5028},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5031,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5033,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5034,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5037,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5039,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5042,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5043,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5046,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5049,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5051,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5052,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5055,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5057,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5060,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5061,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5064,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5067,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5069,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5070,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5073,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5075,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5078,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5079,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5082,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5085,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5087,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5088,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5091,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5093,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5096,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5097,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5100,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5103,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5105,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5106,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5109,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5111,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5114,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5115,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5118,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5121,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5123,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5124,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B5129=\"\",\"\",B5129&\", \"&F5129&\",     \"&G5129)","v":""},{"$f":"IF(A5129=\"\",\"\",A5129)","v":""},5127,{"$f":"T5129","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5129,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5132,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5133,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5136,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5139,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5141,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5142,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5145,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5147,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5150,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5151,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5154,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5157,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5159,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5160,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5163,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5165,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5168,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5169,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5172,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5175,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5177,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5178,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5181,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5183,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5186,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5187,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5190,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B5193=\"\",\"\",B5193&\", \"&F5193&\",     \"&G5193)","v":""},{"$f":"IF(A5193=\"\",\"\",A5193)","v":""},5191,{"$f":"T5193","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5195,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5196,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5199,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5201,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5204,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5205,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5208,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5209,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5213,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5214,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5217,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5219,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5222,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5223,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5226,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5227,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5231,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5232,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5235,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5237,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5240,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5241,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5244,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5245,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5249,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5250,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5253,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B5257=\"\",\"\",B5257&\", \"&F5257&\",     \"&G5257)","v":""},{"$f":"IF(A5257=\"\",\"\",A5257)","v":""},5255,{"$f":"T5257","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5258,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5259,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5262,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5263,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5267,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5268,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5271,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5273,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5276,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5277,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5280,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5281,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5285,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5286,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5289,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5291,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5294,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5295,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5298,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5299,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5303,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5304,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5307,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5309,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5312,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5313,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5316,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5317,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5321,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5322,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5325,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5327,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5330,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5331,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5334,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5335,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5339,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5340,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5343,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5345,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U5349+1","v":5348},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5349,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5352,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5353,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5357,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5358,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5361,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5364,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5366,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5367,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5370,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5371,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5375,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5376,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5379,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5382,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5384,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5385,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5388,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5389,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5393,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5394,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5397,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5400,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5402,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5403,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5406,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5407,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5411,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U5413+1","v":5412},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5415,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5418,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5420,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5421,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5424,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5425,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5429,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5430,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5433,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5436,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5438,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5439,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5442,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5443,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B5449=\"\",\"\",B5449&\", \"&F5449&\",     \"&G5449)","v":""},{"$f":"IF(A5449=\"\",\"\",A5449)","v":""},5447,{"$f":"T5449","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5448,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5451,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5454,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5456,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5457,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5460,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5461,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5465,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5466,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5469,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5472,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5474,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5475,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5478,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5479,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5483,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5484,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5487,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5490,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5492,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5493,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5496,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5497,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5501,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5502,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5505,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5508,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5510,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B5513=\"\",\"\",B5513&\", \"&F5513&\",     \"&G5513)","v":""},{"$f":"IF(A5513=\"\",\"\",A5513)","v":""},5511,{"$f":"T5513","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5514,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5516,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5519,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5520,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5523,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5526,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5528,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5529,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5532,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5534,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5537,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5538,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5541,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5544,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5546,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5547,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5550,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5552,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5555,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5556,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5559,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5562,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5564,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5565,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5568,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5570,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5573,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5574,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5577,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5580,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5582,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5583,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5586,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5588,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5591,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5592,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5595,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5598,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5600,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5601,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U5605+1","v":5604},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5606,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5609,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5610,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5613,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5616,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5618,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5619,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5622,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5624,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5627,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5628,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5631,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5634,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5636,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5637,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5640,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5642,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5645,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5646,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5649,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5652,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5654,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5655,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5658,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5660,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5663,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5664,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5667,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5670,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5672,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5673,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5676,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5678,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5681,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5682,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5685,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5686,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5690,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5691,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5694,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5696,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5699,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5700,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B5705=\"\",\"\",B5705&\", \"&F5705&\",     \"&G5705)","v":""},{"$f":"IF(A5705=\"\",\"\",A5705)","v":""},5703,{"$f":"T5705","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5704,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5708,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5709,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5712,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5714,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5717,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5718,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5721,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5722,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5726,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5727,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5730,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U5733+1","v":5732},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5735,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5736,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5739,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5740,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5744,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5745,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5748,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5750,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5753,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5754,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5757,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5758,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5762,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5763,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5766,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5768,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5771,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5772,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5775,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5776,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5780,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5781,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5784,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5786,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5789,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5790,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5793,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5794,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5798,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5799,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5802,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5804,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5807,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5808,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5811,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5812,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5816,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5817,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5820,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5822,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5825,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5826,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5829,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5830,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5834,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5835,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5838,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5841,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5843,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5844,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5847,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5848,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5852,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5853,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5856,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5859,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5861,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5862,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5865,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5866,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5870,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5871,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5874,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5877,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5879,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5880,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5883,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5884,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5888,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5889,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5892,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B5897=\"\",\"\",B5897&\", \"&F5897&\",     \"&G5897)","v":""},{"$f":"IF(A5897=\"\",\"\",A5897)","v":""},5895,{"$f":"T5897","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5897,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5898,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5901,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5902,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5906,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5907,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5910,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5913,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5915,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5916,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5919,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5920,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U5925+1","v":5924},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5925,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5928,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5931,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5933,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5934,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5937,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5938,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5942,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5943,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5946,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5949,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5951,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5952,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5955,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5956,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5960,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5961,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5964,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5967,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5969,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5970,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5973,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5974,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5978,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5979,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5982,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5985,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5987,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U5989+1","v":5988},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5991,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5992,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5996,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5997,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6000,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6003,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6005,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6006,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6009,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6011,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6014,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6015,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6018,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6021,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6025=\"\",\"\",B6025&\", \"&F6025&\",     \"&G6025)","v":""},{"$f":"IF(A6025=\"\",\"\",A6025)","v":""},6023,{"$f":"T6025","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6024,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6027,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6029,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6032,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6033,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6036,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6039,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6041,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6042,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6045,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6047,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6050,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6051,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6054,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6057,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6059,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6060,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6063,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6065,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6068,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6069,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6072,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6075,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6077,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6078,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6081,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6083,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6086,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6089=\"\",\"\",B6089&\", \"&F6089&\",     \"&G6089)","v":""},{"$f":"IF(A6089=\"\",\"\",A6089)","v":""},6087,{"$f":"T6089","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6090,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6093,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6095,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6096,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6099,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6101,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6104,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6105,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6108,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6111,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6113,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6114,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6117,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6119,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6122,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6123,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6126,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6129,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6131,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6132,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6135,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6137,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6140,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6141,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6144,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6147,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6149,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6150,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6153,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6155,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6158,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6159,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6162,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6163,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6167,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6168,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6171,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6173,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6176,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6177,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U6181+1","v":6180},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6181,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6185,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6186,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6189,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6191,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6194,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6195,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6198,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6199,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6203,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6204,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6207,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6209,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6212,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6213,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6216,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6217,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6221,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6222,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6225,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6227,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6230,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6231,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6234,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6235,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6239,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6240,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6243,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6245,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6248,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6249,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6252,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6253,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6257,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6258,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6261,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6263,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6266,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6267,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6270,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6271,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6275,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6276,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6281=\"\",\"\",B6281&\", \"&F6281&\",     \"&G6281)","v":""},{"$f":"IF(A6281=\"\",\"\",A6281)","v":""},6279,{"$f":"T6281","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6281,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6284,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6285,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6288,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6289,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6293,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6294,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6297,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6299,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6302,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6303,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6306,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6307,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6311,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6312,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6315,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6317,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6320,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6321,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6324,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6325,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6329,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6330,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6333,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6336,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6338,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6339,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6342,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6345=\"\",\"\",B6345&\", \"&F6345&\",     \"&G6345)","v":""},{"$f":"IF(A6345=\"\",\"\",A6345)","v":""},6343,{"$f":"T6345","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6347,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6348,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6351,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6354,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6356,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6357,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6360,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6361,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6365,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6366,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6369,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U6373+1","v":6372},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6374,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6375,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6378,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6379,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6383,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6384,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6387,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6390,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6392,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6393,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6396,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6397,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6401,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6402,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6405,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6408,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6410,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6411,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6414,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6415,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6419,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6420,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6423,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6426,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6428,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6429,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6432,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6433,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6437,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6438,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6441,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6444,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6446,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6447,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6450,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6451,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6455,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6456,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6459,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6462,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6464,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6465,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6468,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6469,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6473,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6474,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6477,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6480,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6482,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6483,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6486,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6488,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6491,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6492,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6495,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6498,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6499,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U6501+1","v":6500},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6501,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6502,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6503,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6504,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6505,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6506,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6507,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6508,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6509,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6510,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6511,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6512,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6513,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6514,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6515,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6516,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6517,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6518,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6519,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6520,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6521,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6522,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6523,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6524,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6525,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6526,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6527,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6528,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6529,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6530,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6531,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6532,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6533,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6534,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6537=\"\",\"\",B6537&\", \"&F6537&\",     \"&G6537)","v":""},{"$f":"IF(A6537=\"\",\"\",A6537)","v":""},6535,{"$f":"T6537","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6536,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6537,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6538,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6539,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6540,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6541,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6542,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6543,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6544,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6545,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6546,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6547,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6548,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6549,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6550,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6551,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6552,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6553,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6554,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6555,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6556,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6557,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6558,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6559,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6560,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6561,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6562,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6563,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U6565+1","v":6564},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6565,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6566,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6567,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6568,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6569,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6570,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6571,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6572,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6573,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6574,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6575,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6576,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6577,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6578,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6579,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6580,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6581,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6582,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6583,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6584,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6585,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6586,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6587,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6588,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6589,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6590,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6591,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6592,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6593,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6594,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6595,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6596,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6597,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6598,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6601=\"\",\"\",B6601&\", \"&F6601&\",     \"&G6601)","v":""},{"$f":"IF(A6601=\"\",\"\",A6601)","v":""},6599,{"$f":"T6601","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6600,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6601,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6602,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6603,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6604,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6605,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6606,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6607,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6608,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6609,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6610,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6611,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6612,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6613,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6614,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6615,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6616,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6617,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6618,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6619,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6620,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6621,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6622,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6623,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6624,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6625,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6626,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6627,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U6629+1","v":6628},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6629,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6630,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6631,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6632,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6633,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6634,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6635,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6636,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6637,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6638,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6639,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6640,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6641,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6642,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6643,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6644,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6645,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6646,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6647,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6648,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6649,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6650,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6651,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6652,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6653,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6654,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6655,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6656,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6657,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6658,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6659,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6660,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6661,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6662,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6665=\"\",\"\",B6665&\", \"&F6665&\",     \"&G6665)","v":""},{"$f":"IF(A6665=\"\",\"\",A6665)","v":""},6663,{"$f":"T6665","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6664,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6665,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6666,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6667,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6668,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6669,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6670,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6671,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6672,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6673,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6674,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6675,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6676,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6677,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6678,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6679,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6680,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6681,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6682,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6683,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6684,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6685,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6686,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6687,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6688,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6689,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6690,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6691,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U6693+1","v":6692},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6693,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6694,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6695,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6696,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6697,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6698,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6699,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6700,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6701,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6702,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6703,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6704,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6705,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6706,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6707,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6708,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6709,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6710,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6711,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6712,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6713,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6714,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6715,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6716,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6717,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6718,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6719,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6720,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6721,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6722,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6723,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6724,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6725,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6726,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6729=\"\",\"\",B6729&\", \"&F6729&\",     \"&G6729)","v":""},{"$f":"IF(A6729=\"\",\"\",A6729)","v":""},6727,{"$f":"T6729","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6728,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6729,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6730,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6731,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6732,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6733,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6734,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6735,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6736,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6737,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6738,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6739,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6740,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6741,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6742,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6743,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6744,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6745,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6746,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6747,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6748,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6749,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6750,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6751,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6752,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6753,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6754,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6755,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U6757+1","v":6756},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6757,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6758,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6759,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6760,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6761,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6762,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6763,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6764,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6765,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6766,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6767,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6768,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6769,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6770,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6771,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6772,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6773,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6774,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6775,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6776,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6777,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6778,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6779,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6780,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6781,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6782,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6783,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6784,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6785,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6786,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6787,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6788,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6789,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6790,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6793=\"\",\"\",B6793&\", \"&F6793&\",     \"&G6793)","v":""},{"$f":"IF(A6793=\"\",\"\",A6793)","v":""},6791,{"$f":"T6793","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6792,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6793,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6794,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6795,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6796,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6797,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6798,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6799,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6800,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6801,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6802,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6803,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6804,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6805,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6806,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6807,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6808,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6809,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6810,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6811,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6812,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6813,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6814,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6815,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6816,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6817,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6818,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6819,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U6821+1","v":6820},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6821,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6822,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6823,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6824,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6825,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6826,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6827,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6828,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6829,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6830,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6831,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6832,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6833,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6834,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6835,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6836,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6837,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6838,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6839,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6840,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6841,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6842,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6843,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6844,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6845,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6846,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6847,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6848,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6849,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6850,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6851,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6852,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6853,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6854,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6857=\"\",\"\",B6857&\", \"&F6857&\",     \"&G6857)","v":""},{"$f":"IF(A6857=\"\",\"\",A6857)","v":""},6855,{"$f":"T6857","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6856,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6857,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6858,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6859,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6860,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6861,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6862,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6863,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6864,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6865,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6866,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6867,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6868,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6869,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6870,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6871,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6872,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6873,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6874,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6875,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6876,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6877,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6878,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6879,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6880,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6881,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6882,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6883,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U6885+1","v":6884},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6885,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6886,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6887,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6888,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6889,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6890,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6891,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6892,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6893,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6894,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6895,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6896,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6897,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6898,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6899,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6900,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6901,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6902,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6903,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6904,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6905,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6906,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6907,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6908,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6909,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6910,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6911,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6912,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6913,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6914,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6915,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6916,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6917,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6918,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6921=\"\",\"\",B6921&\", \"&F6921&\",     \"&G6921)","v":""},{"$f":"IF(A6921=\"\",\"\",A6921)","v":""},6919,{"$f":"T6921","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6920,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6921,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6922,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6923,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6924,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6925,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6926,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6927,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6928,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6929,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6930,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6931,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6932,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6933,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6934,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6935,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6936,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6937,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6938,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6939,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6940,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6941,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6942,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6943,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6944,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6945,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6946,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6947,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U6949+1","v":6948},""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6949,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6950,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6951,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6952,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6953,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6954,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6955,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6956,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6957,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6958,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6959,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6960,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6961,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6962,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6963,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6964,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6965,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6966,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6967,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6968,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6969,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6970,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6971,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6972,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6973,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6974,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6975,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6976,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6977,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6978,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6979,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6980,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6981,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6982,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6985=\"\",\"\",B6985&\", \"&F6985&\",     \"&G6985)","v":""},{"$f":"IF(A6985=\"\",\"\",A6985)","v":""},6983,{"$f":"T6985","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6984,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6985,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6986,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6987,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6988,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6989,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6990,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6991,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6992,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6993,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6994,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6995,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6996,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6997,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6998,""]

{"sheet":"ICS","index":8,"n_rows":36,"n_cols":16,"rows_kept":36,"cut":false,"hidden":true,"merged":[[1,5,1,9],[33,5,33,7],[41,5,41,7],[13,12,15,14]]}
[]
[null,null,null,null,null,{"$f":"Daten!AL92","v":"TypICS Matt Ø 180"},null,null,null,null,null,null,null,null,null,{"$f":"M4&\" \"&Daten!V92","v":"ICS Matt 180"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$479","v":"Typ/Lichter Ø mm"},null,null,null,null,null,null,{"$f":"Daten!$H$489","v":"ICS Matt"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$96","v":"Betriebsweise"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$75","v":"Brennstoff"},null,null,null,null,null,null,{"$f":"Vokabel!$A$89","v":"Anpassung der Anlagenhöhe"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$40","v":"Anlagenhöhe in m"},null,null,null,10,null,null,{"$f":"Vokabel!$A$90","v":"tatsächliche Anlagenhöhe "},null,null,{"$f":"VLOOKUP(P2,Sortimente!G:P,10,0)","v":10.305999999999999}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$76","v":"Wand- o. Bodenmontage"},null,null,null,null,null,null,{"$f":"Vokabel!$A$91","v":"Differenz +/-"},null,null,{"$f":"P10-J10","v":0.30599999999999916}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$77","v":"Putztüranschluss"},null,null,null,null,null,null,{"$f":"Vokabel!$A$101","v":"Anpassung durch Eingabe kürzerer Rohrelemente:"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$78","v":"Rauchrohranschluss RA"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$79","v":"RA-Höhe in m"},null,null,null,null,null,null,null,{"$f":"Vokabel!$A$336","v":"Rohr 455 mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$331","v":"RA-Verlängerung (ICS)"},null,null,null,null,null,null,null,{"$f":"Vokabel!$A$337","v":"Rohr 205 mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!A384","v":"Abdeckblende"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$82","v":"Dachdurchführung"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$385","v":"Mündungslösung"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$382","v":"Wandabstand (>50 mm)"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$333","v":"Statische Klemmbänder (2 Stk)"}]
[]
[]
[]
[]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$88","v":"Verbindungsleitung"}]

{"sheet":"ICS5000","index":9,"n_rows":34,"n_cols":16,"rows_kept":34,"cut":false,"hidden":true,"merged":[[1,5,1,9],[41,5,41,7],[13,12,15,14]]}
[]
[null,null,null,null,null,{"$f":"Daten!$AL$230","v":"Typ ICS 5000 Matt Ø 180"},null,null,null,null,null,null,null,null,null,{"$f":"M4&\" \"&Daten!$V$230","v":"ICS5000 180"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Daten!$H$500","v":"ICS5000"}]
[]
[]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$479","v":"Typ/Lichter Ø mm"},null,null,null,null,null,null,{"$f":"Vokabel!$A$89","v":"Anpassung der Anlagenhöhe"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$40","v":"Anlagenhöhe in m"},null,null,null,10,null,null,{"$f":"Vokabel!$A$90","v":"tatsächliche Anlagenhöhe "},null,null,{"$f":"VLOOKUP(P2,Sortimente!G:P,10,0)","v":10.85}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$76","v":"Wand- o. Bodenmontage"},null,null,null,null,null,null,{"$f":"Vokabel!$A$91","v":"Differenz +/-"},null,null,{"$f":"P10-J10","v":0.84999999999999964}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$77","v":"Putztüranschluss"},null,null,null,null,null,null,{"$f":"Vokabel!$A$101","v":"Anpassung durch Eingabe kürzerer Rohrelemente:"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$78","v":"Rauchrohranschluss RA"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$331","v":"RA-Verlängerung (ICS)"},null,null,null,null,null,null,null,{"$f":"Vokabel!$A$336","v":"Rohr 455 mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!A384","v":"Abdeckblende"},null,null,null,null,null,null,null,{"$f":"Vokabel!$A$337","v":"Rohr 205 mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$82","v":"Dachdurchführung"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$385","v":"Mündungslösung"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$382","v":"Wandabstand (>50 mm)"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!A489","v":"Winkel"},null,"15°"]
[]
[null,null,null,null,null,null,null,"30°"]
[]
[null,null,null,null,null,null,null,"45°"]
[]
[null,null,null,null,null,null,null,"90°"]

{"sheet":"Keranova","index":10,"n_rows":28,"n_cols":16,"rows_kept":28,"cut":false,"hidden":true,"merged":[[3,5,3,9],[2,5,2,9],[16,12,17,14]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$117,Daten!$T:$U,2,0)&\" \"&VLOOKUP(Daten!$U$117,Daten!$T:$V,3,0)","v":"Keranova 160"}]
[null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$117,Daten!$T:$AL,19,0)","v":"Typ  KERANOVA 160"}]
[]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$311","v":"Lichter Ø mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$96","v":"Betriebsweise"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$75","v":"Brennstoff"},null,null,null,null,null,null,{"$f":"Vokabel!$A$89","v":"Anpassung der Anlagenhöhe"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$40","v":"Anlagenhöhe in m"},null,null,null,11,null,null,{"$f":"Vokabel!$A$90","v":"tatsächliche Anlagenhöhe "},null,null,{"$f":"VLOOKUP(P2,Sortimente!G:P,10,0)","v":11.305999999999999}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$78","v":"Rauchrohranschluss RA"},null,null,null,null,null,null,{"$f":"Vokabel!$A$97","v":"Differenz +/- "},null,null,{"$f":"P12-J12","v":0.30599999999999916}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$98","v":"(14 cm für Mündung vorsehen!)"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$99","v":"Doppelwandfutter in mm"}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$101","v":"Anpassung durch Eingabe kürzerer Rohrelemente:"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$77","v":"Putztüranschluss"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$100","v":"Putztür"},null,null,null,null,null,null,null,{"$f":"Vokabel!$A$104","v":"Rohr 660 mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$102","v":"Regenhaube"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$54","v":"Kaminaufsätze"},null,{"$f":"Vokabel!$A$63","v":" (ab Ø 16)"}]
[]
[]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$88","v":"Verbindungsleitung"}]

{"sheet":"Kerastar","index":11,"n_rows":33,"n_cols":16,"rows_kept":33,"cut":false,"hidden":true,"merged":[[1,5,1,9]]}
[]
[null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$22,Daten!$T:$AL,19,0)","v":"Typ  KRS 180"},null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$22,Daten!$T:$U,2,0)&\" \"&VLOOKUP(Daten!$U$22,Daten!$T:$V,3,0)","v":"KERASTAR 180"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$311","v":"Lichter Ø mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$75","v":"Brennstoff"},null,null,null,null,null,null,{"$f":"Vokabel!$A$89","v":"Anpassung der Anlagenhöhe"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$40","v":"Anlagenhöhe in m"},null,null,null,10,null,null,{"$f":"Vokabel!$A$90","v":"tatsächliche Anlagenhöhe "},null,null,{"$f":"VLOOKUP(P2,Sortimente!G:P,10,0)","v":10.178000000000001}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$76","v":"Wand- o. Bodenmontage"},null,null,null,null,null,null,{"$f":"Vokabel!$A$91","v":"Differenz +/-"},null,null,{"$f":"P8-J8","v":0.17800000000000082}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$77","v":"Putztüranschluss"},null,null,null,null,null,null,{"$f":"Vokabel!$A$92","v":"Anpassung durch Eingabe "}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$78","v":"Rauchrohranschluss RA"},null,null,null,null,null,null,{"$f":"Vokabel!$A$93","v":"kürzerer Rohrelemente:"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$79","v":"RA-Höhe in m"},null,null,null,null,null,null,null,{"$f":"Vokabel!$A$94","v":"Rohr 330 mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$80","v":"RA-Verlängerung (KRS)"},null,null,null,null,null,null,null,{"$f":"Vokabel!$A$95","v":"Rohr 165 mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$81","v":"Sparrenhalterung"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$82","v":"Dachdurchführung"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$83","v":"Regenhaube"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$84","v":"Mündungslösung"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$85","v":"Wandabstand (>=50 mm)"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$86","v":"Wandhalterung statisch"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$87","v":"(inkl. 2 St. statischer Manschetten)"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$88","v":"Verbindungsleitung"}]

{"sheet":"Texte","index":12,"n_rows":21,"n_cols":4,"rows_kept":21,"cut":false,"hidden":true,"merged":[]}
[null,null,null,{"$f":"Vokabel!$A$225","v":"Variabler Text für Montagearbeiten"}]
[]
[null,{"$f":"Vokabel!$A$226","v":"1.Zeile"}]
[null,{"$f":"Vokabel!$A$227","v":"2.Zeile"}]
[null,{"$f":"Vokabel!$A$228","v":"3.Zeile"}]
[null,{"$f":"Vokabel!$A$229","v":"4.Zeile"}]
[]
[]
[]
[null,null,null,{"$f":"Vokabel!$A$232","v":"Variabler Kopftext für Angebot"}]
[]
[null,{"$f":"Vokabel!$A$226","v":"1.Zeile"},null,{"$f":"IF(Eingabe!K9=0,\"\",IF(Eingabe!K9=\"\",\"\",Vokabel!$A$233&\" \"&Eingabe!K9&\",\"))","v":""}]
[null,{"$f":"Vokabel!$A$227","v":"2.Zeile"},null,{"$f":"Vokabel!$A$234","v":"wir bedanken uns für Ihre Anfrage und bieten Ihnen folgendes an:"}]
[null,null,null,{"$f":"Vokabel!$A$236","v":"Wenn es keine Ansprechperson gibt wird der Kopftext (1.u.2.Zeile) genommen"}]
[null,{"$f":"Vokabel!$A$231","v":"1.u.2.Zeile"},null,{"$f":"Vokabel!$A$235","v":"Wir bedanken uns für Ihre Anfrage und bieten Ihnen folgendes an:"}]
[null,null,null,{"$f":"Vokabel!$A$237","v":"Variabler Schlusstext für Angebot"}]
[]
[null,{"$f":"Vokabel!$A$226","v":"1.Zeile"}]
[null,{"$f":"Vokabel!$A$227","v":"2.Zeile"}]
[null,{"$f":"Vokabel!$A$228","v":"3.Zeile"},null,{"$f":"Vokabel!$A$238","v":"Wir hoffen, dass Ihnen unser Angebot zusagt und freuen uns auf Ihren Auftrag."}]
[null,{"$f":"Vokabel!$A$229","v":"4.Zeile"},null,{"$f":"Vokabel!$A$239","v":"Freundliche Grüsse"}]

{"sheet":"Musteranlage","index":13,"n_rows":138,"n_cols":19,"rows_kept":138,"cut":false,"hidden":true,"merged":[]}
[{"$f":"IF(J1=\"Absolut\",Daten!$U$35,IF(J1=\"Cheminee\",Daten!$U$79,IF(J1=\"ICS\",Daten!$U$92,IF(J1=\"ICS Matt\",Daten!$U$92,IF(J1=\"ICS Kupfer\",Daten!$U$92,IF(J1=\"Keranova\",Daten!$U$117,IF(J1=\"Kerastar\",Daten!$U$22,A2)))))))","v":"ABSOLUT18"},null,null,null,null,null,null,null,null,"Absolut"]
[{"$f":"IF(J1=\"Prima+1,0\",Daten!$U$162,IF(J1=\"Prima Plus\",Daten!$U$139,IF(J1=\"Technostar120\",Daten!$U$10,IF(J1=\"ISOLIT\",Daten!$U$1,IF(J1=\"ICS5000\",Daten!$U$230,\"\")))))","v":""},null,null,null,null,null,null,{"$f":"VLOOKUP(A1,Daten!T:U,2,0)","v":"ABSOLUT"},{"$f":"VLOOKUP(A1,Daten!T:AM,20,0)","v":"Schiedel ABSOLUT, ABS 18"},null,null,{"$f":"VLOOKUP(A1,Daten!$T:$Y,6,0)","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(H2=\"Kerastar\",Vokabel!$A$411&\" \"&Daten!$C$401,IF(H2=\"ADW TecnoStar\",Vokabel!$A$411&\" \"&Daten!$C$401,IF(H2=\"ICS\",Vokabel!$A$411&\" \"&Daten!$C$499,IF($H$2=\"Absolut\",Vokabel!$A$412&\" \"&Daten!$Z$35,IF($H$2=\"Cheminee\",Vokabel!$A$412&\" \"&Daten!$AK$79,IF(H2=\"ISOLIT\",Vokabel!$A$412&\" \"&Daten!$Z$1,IF(H2=\"ICS5000\",Vokabel!$A$411&\" \"&Daten!$M$499,\"\")))))))","v":"Aussenmass: 36/36 cm"},null,null,{"$f":"IF(VLOOKUP(A1,Daten!$T:$AA,8,0)=0,\"\",(VLOOKUP(A1,Daten!$T:$AA,8,0)))","v":"mit integrierter Wärmedämmung"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(VLOOKUP(A1,Daten!$T:$AB,9,0)=0,\"\",(VLOOKUP(A1,Daten!$T:$AB,9,0)))","v":"und keramischem Profil-Innenrohr"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($R$5=\"\",\"\",IF($R$5=1,\"\",\"(inkl. \"&$S$5&\" \"&Vokabel!$A$259&\")\"))","v":""},null,null,null,{"$f":"IF(H2=\"Kerastar\",Daten!$B$461,IF(H2=\"ICS\",Daten!$B$507,IF(H2=\"ICS Kupfer\",Daten!$B$507,IF(H2=\"ICS5000\",Daten!$L$507,\"\"))))","v":""},{"$f":"IF(H2=\"Kerastar\",Daten!$C$461,IF(H2=\"ICS\",Daten!$C$507,IF(H2=\"ICS Kupfer\",Daten!$C$507,IF(H2=\"ICS5000\",Daten!$M$507,\"\"))))","v":""}]
[]
["Nr.","Verkn.",null,null,null,null,null,"Rabatt- fähig","Pos.","Artikelbezeichnung","Baulänge","Artikelnummer","Menge"]
[0,{"$f":"$A$1&Musteranlage!A8","v":"ABSOLUT180"},null,null,null,null,null,{"$f":"IF(L8=\"\",\"\",IF(L8=\"Sonder\",\"J\",VLOOKUP(L8,sanschie!B:K,10,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B8,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B8,Sortimente!D:G,2,0))","v":"P"},null,null,{"$f":"IF(I8=\"\",\"\",VLOOKUP($B8,Sortimente!D:G,4,0))","v":"Absolut 18"},{"$f":"IF(I8=\"\",\"\",IF(VLOOKUP(B8,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B8,Sortimente!D:L,9,0)))","v":""}]
[1,{"$f":"$A$1&Musteranlage!A9","v":"ABSOLUT181"},null,null,null,null,null,{"$f":"IF(L9=\"\",\"\",IF(L9=\"Sonder\",\"J\",VLOOKUP(L9,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B9,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B9,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I9=\"\",\"\",VLOOKUP($B9,Sortimente!D:G,4,0))","v":"103912"},{"$f":"IF(I9=\"\",\"\",IF(VLOOKUP(B9,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B9,Sortimente!D:L,9,0)))","v":23}]
[2,{"$f":"$A$1&Musteranlage!A10","v":"ABSOLUT182"},null,null,null,null,null,{"$f":"IF(L10=\"\",\"\",IF(L10=\"Sonder\",\"J\",VLOOKUP(L10,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B10,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B10,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I10=\"\",\"\",VLOOKUP($B10,Sortimente!D:G,4,0))","v":"103931"},{"$f":"IF(I10=\"\",\"\",IF(VLOOKUP(B10,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B10,Sortimente!D:L,9,0)))","v":""}]
[3,{"$f":"$A$1&Musteranlage!A11","v":"ABSOLUT183"},null,null,null,null,null,{"$f":"IF(L11=\"\",\"\",IF(L11=\"Sonder\",\"J\",VLOOKUP(L11,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B11,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B11,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I11=\"\",\"\",VLOOKUP($B11,Sortimente!D:G,4,0))","v":"103849"},{"$f":"IF(I11=\"\",\"\",IF(VLOOKUP(B11,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B11,Sortimente!D:L,9,0)))","v":""}]
[4,{"$f":"$A$1&Musteranlage!A12","v":"ABSOLUT184"},null,null,null,null,null,{"$f":"IF(L12=\"\",\"\",IF(L12=\"Sonder\",\"J\",VLOOKUP(L12,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B12,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B12,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I12=\"\",\"\",VLOOKUP($B12,Sortimente!D:G,4,0))","v":"103948"},{"$f":"IF(I12=\"\",\"\",IF(VLOOKUP(B12,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B12,Sortimente!D:L,9,0)))","v":5}]
[5,{"$f":"$A$1&Musteranlage!A13","v":"ABSOLUT185"},null,null,null,null,null,{"$f":"IF(L13=\"\",\"\",IF(L13=\"Sonder\",\"J\",VLOOKUP(L13,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B13,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B13,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I13=\"\",\"\",VLOOKUP($B13,Sortimente!D:G,4,0))","v":"103859"},{"$f":"IF(I13=\"\",\"\",IF(VLOOKUP(B13,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B13,Sortimente!D:L,9,0)))","v":1}]
[6,{"$f":"$A$1&Musteranlage!A14","v":"ABSOLUT186"},null,null,null,null,null,{"$f":"IF(L14=\"\",\"\",IF(L14=\"Sonder\",\"J\",VLOOKUP(L14,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B14,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B14,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I14=\"\",\"\",VLOOKUP($B14,Sortimente!D:G,4,0))","v":"103953"},{"$f":"IF(I14=\"\",\"\",IF(VLOOKUP(B14,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B14,Sortimente!D:L,9,0)))","v":""}]
[7,{"$f":"$A$1&Musteranlage!A15","v":"ABSOLUT187"},null,null,null,null,null,{"$f":"IF(L15=\"\",\"\",IF(L15=\"Sonder\",\"J\",VLOOKUP(L15,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B15,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B15,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I15=\"\",\"\",VLOOKUP($B15,Sortimente!D:G,4,0))","v":"103891"},{"$f":"IF(I15=\"\",\"\",IF(VLOOKUP(B15,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B15,Sortimente!D:L,9,0)))","v":1}]
[8,{"$f":"$A$1&Musteranlage!A16","v":"ABSOLUT188"},null,null,null,null,null,{"$f":"IF(L16=\"\",\"\",IF(L16=\"Sonder\",\"J\",VLOOKUP(L16,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B16,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B16,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I16=\"\",\"\",VLOOKUP($B16,Sortimente!D:G,4,0))","v":"103709"},{"$f":"IF(I16=\"\",\"\",IF(VLOOKUP(B16,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B16,Sortimente!D:L,9,0)))","v":""}]
[9,{"$f":"$A$1&Musteranlage!A17","v":"ABSOLUT189"},null,null,null,null,null,{"$f":"IF(L17=\"\",\"\",IF(L17=\"Sonder\",\"J\",VLOOKUP(L17,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B17,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B17,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I17=\"\",\"\",VLOOKUP($B17,Sortimente!D:G,4,0))","v":"103700"},{"$f":"IF(I17=\"\",\"\",IF(VLOOKUP(B17,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B17,Sortimente!D:L,9,0)))","v":""}]
[10,{"$f":"$A$1&Musteranlage!A18","v":"ABSOLUT1810"},null,null,null,null,null,{"$f":"IF(L18=\"\",\"\",IF(L18=\"Sonder\",\"J\",VLOOKUP(L18,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B18,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B18,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I18=\"\",\"\",VLOOKUP($B18,Sortimente!D:G,4,0))","v":"103871"},{"$f":"IF(I18=\"\",\"\",IF(VLOOKUP(B18,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B18,Sortimente!D:L,9,0)))","v":""}]
[11,{"$f":"$A$1&Musteranlage!A19","v":"ABSOLUT1811"},null,null,null,null,null,{"$f":"IF(L19=\"\",\"\",IF(L19=\"Sonder\",\"J\",VLOOKUP(L19,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B19,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B19,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I19=\"\",\"\",VLOOKUP($B19,Sortimente!D:G,4,0))","v":"103983"},{"$f":"IF(I19=\"\",\"\",IF(VLOOKUP(B19,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B19,Sortimente!D:L,9,0)))","v":1}]
[12,{"$f":"$A$1&Musteranlage!A20","v":"ABSOLUT1812"},null,null,null,null,null,{"$f":"IF(L20=\"\",\"\",IF(L20=\"Sonder\",\"J\",VLOOKUP(L20,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B20,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B20,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I20=\"\",\"\",VLOOKUP($B20,Sortimente!D:G,4,0))","v":"103995"},{"$f":"IF(I20=\"\",\"\",IF(VLOOKUP(B20,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B20,Sortimente!D:L,9,0)))","v":""}]
[13,{"$f":"$A$1&Musteranlage!A21","v":"ABSOLUT1813"},null,null,null,null,null,{"$f":"IF(L21=\"\",\"\",IF(L21=\"Sonder\",\"J\",VLOOKUP(L21,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B21,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B21,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I21=\"\",\"\",VLOOKUP($B21,Sortimente!D:G,4,0))","v":"104001"},{"$f":"IF(I21=\"\",\"\",IF(VLOOKUP(B21,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B21,Sortimente!D:L,9,0)))","v":""}]
[14,{"$f":"$A$1&Musteranlage!A22","v":"ABSOLUT1814"},null,null,null,null,null,{"$f":"IF(L22=\"\",\"\",IF(L22=\"Sonder\",\"J\",VLOOKUP(L22,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B22,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B22,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I22=\"\",\"\",VLOOKUP($B22,Sortimente!D:G,4,0))","v":"104007"},{"$f":"IF(I22=\"\",\"\",IF(VLOOKUP(B22,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B22,Sortimente!D:L,9,0)))","v":""}]
[15,{"$f":"$A$1&Musteranlage!A23","v":"ABSOLUT1815"},null,null,null,null,null,{"$f":"IF(L23=\"\",\"\",IF(L23=\"Sonder\",\"J\",VLOOKUP(L23,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B23,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B23,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I23=\"\",\"\",VLOOKUP($B23,Sortimente!D:G,4,0))","v":"104268"},{"$f":"IF(I23=\"\",\"\",IF(VLOOKUP(B23,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B23,Sortimente!D:L,9,0)))","v":""}]
[16,{"$f":"$A$1&Musteranlage!A24","v":"ABSOLUT1816"},null,null,null,null,null,{"$f":"IF(L24=\"\",\"\",IF(L24=\"Sonder\",\"J\",VLOOKUP(L24,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B24,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B24,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I24=\"\",\"\",VLOOKUP($B24,Sortimente!D:G,4,0))","v":"103966"},{"$f":"IF(I24=\"\",\"\",IF(VLOOKUP(B24,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B24,Sortimente!D:L,9,0)))","v":""}]
[17,{"$f":"$A$1&Musteranlage!A25","v":"ABSOLUT1817"},null,null,null,null,null,{"$f":"IF(L25=\"\",\"\",IF(L25=\"Sonder\",\"J\",VLOOKUP(L25,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B25,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B25,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I25=\"\",\"\",VLOOKUP($B25,Sortimente!D:G,4,0))","v":"104274"},{"$f":"IF(I25=\"\",\"\",IF(VLOOKUP(B25,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B25,Sortimente!D:L,9,0)))","v":""}]
[18,{"$f":"$A$1&Musteranlage!A26","v":"ABSOLUT1818"},null,null,null,null,null,{"$f":"IF(L26=\"\",\"\",IF(L26=\"Sonder\",\"J\",VLOOKUP(L26,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B26,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B26,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I26=\"\",\"\",VLOOKUP($B26,Sortimente!D:G,4,0))","v":"104243"},{"$f":"IF(I26=\"\",\"\",IF(VLOOKUP(B26,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B26,Sortimente!D:L,9,0)))","v":""}]
[19,{"$f":"$A$1&Musteranlage!A27","v":"ABSOLUT1819"},null,null,null,null,null,{"$f":"IF(L27=\"\",\"\",IF(L27=\"Sonder\",\"J\",VLOOKUP(L27,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B27,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B27,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I27=\"\",\"\",VLOOKUP($B27,Sortimente!D:G,4,0))","v":"104190"},{"$f":"IF(I27=\"\",\"\",IF(VLOOKUP(B27,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B27,Sortimente!D:L,9,0)))","v":""}]
[20,{"$f":"$A$1&Musteranlage!A28","v":"ABSOLUT1820"},null,null,null,null,null,{"$f":"IF(L28=\"\",\"\",IF(L28=\"Sonder\",\"J\",VLOOKUP(L28,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B28,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B28,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I28=\"\",\"\",VLOOKUP($B28,Sortimente!D:G,4,0))","v":"104144"},{"$f":"IF(I28=\"\",\"\",IF(VLOOKUP(B28,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B28,Sortimente!D:L,9,0)))","v":1}]
[21,{"$f":"$A$1&Musteranlage!A29","v":"ABSOLUT1821"},null,null,null,null,null,{"$f":"IF(L29=\"\",\"\",IF(L29=\"Sonder\",\"J\",VLOOKUP(L29,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B29,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B29,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I29=\"\",\"\",VLOOKUP($B29,Sortimente!D:G,4,0))","v":"104170"},{"$f":"IF(I29=\"\",\"\",IF(VLOOKUP(B29,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B29,Sortimente!D:L,9,0)))","v":""}]
[22,{"$f":"$A$1&Musteranlage!A30","v":"ABSOLUT1822"},null,null,null,null,null,{"$f":"IF(L30=\"\",\"\",IF(L30=\"Sonder\",\"J\",VLOOKUP(L30,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B30,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B30,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I30=\"\",\"\",VLOOKUP($B30,Sortimente!D:G,4,0))","v":"104162"},{"$f":"IF(I30=\"\",\"\",IF(VLOOKUP(B30,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B30,Sortimente!D:L,9,0)))","v":1}]
[23,{"$f":"$A$1&Musteranlage!A31","v":"ABSOLUT1823"},null,null,null,null,null,{"$f":"IF(L31=\"\",\"\",IF(L31=\"Sonder\",\"J\",VLOOKUP(L31,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B31,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B31,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I31=\"\",\"\",VLOOKUP($B31,Sortimente!D:G,4,0))","v":"104175"},{"$f":"IF(I31=\"\",\"\",IF(VLOOKUP(B31,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B31,Sortimente!D:L,9,0)))","v":""}]
[24,{"$f":"$A$1&Musteranlage!A32","v":"ABSOLUT1824"},null,null,null,null,null,{"$f":"IF(L32=\"\",\"\",IF(L32=\"Sonder\",\"J\",VLOOKUP(L32,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B32,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B32,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I32=\"\",\"\",VLOOKUP($B32,Sortimente!D:G,4,0))","v":"140787"},{"$f":"IF(I32=\"\",\"\",IF(VLOOKUP(B32,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B32,Sortimente!D:L,9,0)))","v":""}]
[25,{"$f":"$A$1&Musteranlage!A33","v":"ABSOLUT1825"},null,null,null,null,null,{"$f":"IF(L33=\"\",\"\",IF(L33=\"Sonder\",\"J\",VLOOKUP(L33,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B33,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B33,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I33=\"\",\"\",VLOOKUP($B33,Sortimente!D:G,4,0))","v":"140932"},{"$f":"IF(I33=\"\",\"\",IF(VLOOKUP(B33,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B33,Sortimente!D:L,9,0)))","v":""}]
[26,{"$f":"$A$1&Musteranlage!A34","v":"ABSOLUT1826"},null,null,null,null,null,{"$f":"IF(L34=\"\",\"\",IF(L34=\"Sonder\",\"J\",VLOOKUP(L34,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B34,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B34,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I34=\"\",\"\",VLOOKUP($B34,Sortimente!D:G,4,0))","v":"104206"},{"$f":"IF(I34=\"\",\"\",IF(VLOOKUP(B34,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B34,Sortimente!D:L,9,0)))","v":""}]
[27,{"$f":"$A$1&Musteranlage!A35","v":"ABSOLUT1827"},null,null,null,null,null,{"$f":"IF(L35=\"\",\"\",IF(L35=\"Sonder\",\"J\",VLOOKUP(L35,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B35,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B35,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I35=\"\",\"\",VLOOKUP($B35,Sortimente!D:G,4,0))","v":"103917"},{"$f":"IF(I35=\"\",\"\",IF(VLOOKUP(B35,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B35,Sortimente!D:L,9,0)))","v":1}]
[28,{"$f":"$A$1&Musteranlage!A36","v":"ABSOLUT1828"},null,null,null,null,null,{"$f":"IF(L36=\"\",\"\",IF(L36=\"Sonder\",\"J\",VLOOKUP(L36,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B36,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B36,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I36=\"\",\"\",VLOOKUP($B36,Sortimente!D:G,4,0))","v":"104059"},{"$f":"IF(I36=\"\",\"\",IF(VLOOKUP(B36,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B36,Sortimente!D:L,9,0)))","v":""}]
[29,{"$f":"$A$1&Musteranlage!A37","v":"ABSOLUT1829"},null,null,null,null,null,{"$f":"IF(L37=\"\",\"\",IF(L37=\"Sonder\",\"J\",VLOOKUP(L37,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B37,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B37,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I37=\"\",\"\",VLOOKUP($B37,Sortimente!D:G,4,0))","v":"104083"},{"$f":"IF(I37=\"\",\"\",IF(VLOOKUP(B37,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B37,Sortimente!D:L,9,0)))","v":""}]
[30,{"$f":"$A$1&Musteranlage!A38","v":"ABSOLUT1830"},null,null,null,null,null,{"$f":"IF(L38=\"\",\"\",IF(L38=\"Sonder\",\"J\",VLOOKUP(L38,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B38,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B38,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I38=\"\",\"\",VLOOKUP($B38,Sortimente!D:G,4,0))","v":"103899"},{"$f":"IF(I38=\"\",\"\",IF(VLOOKUP(B38,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B38,Sortimente!D:L,9,0)))","v":""}]
[31,{"$f":"$A$1&Musteranlage!A39","v":"ABSOLUT1831"},null,null,null,null,null,{"$f":"IF(L39=\"\",\"\",IF(L39=\"Sonder\",\"J\",VLOOKUP(L39,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B39,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B39,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I39=\"\",\"\",VLOOKUP($B39,Sortimente!D:G,4,0))","v":"103907"},{"$f":"IF(I39=\"\",\"\",IF(VLOOKUP(B39,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B39,Sortimente!D:L,9,0)))","v":""}]
[32,{"$f":"$A$1&Musteranlage!A40","v":"ABSOLUT1832"},null,null,null,null,null,{"$f":"IF(L40=\"\",\"\",IF(L40=\"Sonder\",\"J\",VLOOKUP(L40,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B40,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B40,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I40=\"\",\"\",VLOOKUP($B40,Sortimente!D:G,4,0))","v":"103474"},{"$f":"IF(I40=\"\",\"\",IF(VLOOKUP(B40,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B40,Sortimente!D:L,9,0)))","v":""}]
[33,{"$f":"$A$1&Musteranlage!A41","v":"ABSOLUT1833"},null,null,null,null,null,{"$f":"IF(L41=\"\",\"\",IF(L41=\"Sonder\",\"J\",VLOOKUP(L41,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B41,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B41,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I41=\"\",\"\",VLOOKUP($B41,Sortimente!D:G,4,0))","v":"104014"},{"$f":"IF(I41=\"\",\"\",IF(VLOOKUP(B41,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B41,Sortimente!D:L,9,0)))","v":""}]
[34,{"$f":"$A$1&Musteranlage!A42","v":"ABSOLUT1834"},null,null,null,null,null,{"$f":"IF(L42=\"\",\"\",IF(L42=\"Sonder\",\"J\",VLOOKUP(L42,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B42,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B42,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I42=\"\",\"\",VLOOKUP($B42,Sortimente!D:G,4,0))","v":"104015"},{"$f":"IF(I42=\"\",\"\",IF(VLOOKUP(B42,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B42,Sortimente!D:L,9,0)))","v":""}]
[35,{"$f":"$A$1&Musteranlage!A43","v":"ABSOLUT1835"},null,null,null,null,null,{"$f":"IF(L43=\"\",\"\",IF(L43=\"Sonder\",\"J\",VLOOKUP(L43,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B43,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B43,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I43=\"\",\"\",VLOOKUP($B43,Sortimente!D:G,4,0))","v":"104016"},{"$f":"IF(I43=\"\",\"\",IF(VLOOKUP(B43,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B43,Sortimente!D:L,9,0)))","v":""}]
[36,{"$f":"$A$1&Musteranlage!A44","v":"ABSOLUT1836"},null,null,null,null,null,{"$f":"IF(L44=\"\",\"\",IF(L44=\"Sonder\",\"J\",VLOOKUP(L44,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B44,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B44,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I44=\"\",\"\",VLOOKUP($B44,Sortimente!D:G,4,0))","v":"104017"},{"$f":"IF(I44=\"\",\"\",IF(VLOOKUP(B44,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B44,Sortimente!D:L,9,0)))","v":""}]
[37,{"$f":"$A$1&Musteranlage!A45","v":"ABSOLUT1837"},null,null,null,null,null,{"$f":"IF(L45=\"\",\"\",IF(L45=\"Sonder\",\"J\",VLOOKUP(L45,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B45,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B45,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I45=\"\",\"\",VLOOKUP($B45,Sortimente!D:G,4,0))","v":"104018"},{"$f":"IF(I45=\"\",\"\",IF(VLOOKUP(B45,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B45,Sortimente!D:L,9,0)))","v":""}]
[38,{"$f":"$A$1&Musteranlage!A46","v":"ABSOLUT1838"},null,null,null,null,null,{"$f":"IF(L46=\"\",\"\",IF(L46=\"Sonder\",\"J\",VLOOKUP(L46,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B46,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B46,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I46=\"\",\"\",VLOOKUP($B46,Sortimente!D:G,4,0))","v":"104032"},{"$f":"IF(I46=\"\",\"\",IF(VLOOKUP(B46,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B46,Sortimente!D:L,9,0)))","v":""}]
[39,{"$f":"$A$1&Musteranlage!A47","v":"ABSOLUT1839"},null,null,null,null,null,{"$f":"IF(L47=\"\",\"\",IF(L47=\"Sonder\",\"J\",VLOOKUP(L47,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B47,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B47,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I47=\"\",\"\",VLOOKUP($B47,Sortimente!D:G,4,0))","v":"104033"},{"$f":"IF(I47=\"\",\"\",IF(VLOOKUP(B47,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B47,Sortimente!D:L,9,0)))","v":""}]
[40,{"$f":"$A$1&Musteranlage!A48","v":"ABSOLUT1840"},null,null,null,null,null,{"$f":"IF(L48=\"\",\"\",IF(L48=\"Sonder\",\"J\",VLOOKUP(L48,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B48,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B48,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I48=\"\",\"\",VLOOKUP($B48,Sortimente!D:G,4,0))","v":"104034"},{"$f":"IF(I48=\"\",\"\",IF(VLOOKUP(B48,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B48,Sortimente!D:L,9,0)))","v":""}]
[41,{"$f":"$A$1&Musteranlage!A49","v":"ABSOLUT1841"},null,null,null,null,null,{"$f":"IF(L49=\"\",\"\",IF(L49=\"Sonder\",\"J\",VLOOKUP(L49,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B49,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B49,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I49=\"\",\"\",VLOOKUP($B49,Sortimente!D:G,4,0))","v":"104035"},{"$f":"IF(I49=\"\",\"\",IF(VLOOKUP(B49,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B49,Sortimente!D:L,9,0)))","v":""}]
[42,{"$f":"$A$1&Musteranlage!A50","v":"ABSOLUT1842"},null,null,null,null,null,{"$f":"IF(L50=\"\",\"\",IF(L50=\"Sonder\",\"J\",VLOOKUP(L50,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B50,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B50,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I50=\"\",\"\",VLOOKUP($B50,Sortimente!D:G,4,0))","v":"104251"},{"$f":"IF(I50=\"\",\"\",IF(VLOOKUP(B50,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B50,Sortimente!D:L,9,0)))","v":""}]
[43,{"$f":"$A$1&Musteranlage!A51","v":"ABSOLUT1843"},null,null,null,null,null,{"$f":"IF(L51=\"\",\"\",IF(L51=\"Sonder\",\"J\",VLOOKUP(L51,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B51,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B51,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I51=\"\",\"\",VLOOKUP($B51,Sortimente!D:G,4,0))","v":"104252"},{"$f":"IF(I51=\"\",\"\",IF(VLOOKUP(B51,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B51,Sortimente!D:L,9,0)))","v":""}]
[44,{"$f":"$A$1&Musteranlage!A52","v":"ABSOLUT1844"},null,null,null,null,null,{"$f":"IF(L52=\"\",\"\",IF(L52=\"Sonder\",\"J\",VLOOKUP(L52,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B52,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B52,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I52=\"\",\"\",VLOOKUP($B52,Sortimente!D:G,4,0))","v":"104253"},{"$f":"IF(I52=\"\",\"\",IF(VLOOKUP(B52,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B52,Sortimente!D:L,9,0)))","v":""}]
[45,{"$f":"$A$1&Musteranlage!A53","v":"ABSOLUT1845"},null,null,null,null,null,{"$f":"IF(L53=\"\",\"\",IF(L53=\"Sonder\",\"J\",VLOOKUP(L53,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B53,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B53,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I53=\"\",\"\",VLOOKUP($B53,Sortimente!D:G,4,0))","v":"103870"},{"$f":"IF(I53=\"\",\"\",IF(VLOOKUP(B53,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B53,Sortimente!D:L,9,0)))","v":1}]
[46,{"$f":"$A$1&Musteranlage!A54","v":"ABSOLUT1846"},null,null,null,null,null,{"$f":"IF(L54=\"\",\"\",IF(L54=\"Sonder\",\"J\",VLOOKUP(L54,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B54,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B54,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I54=\"\",\"\",VLOOKUP($B54,Sortimente!D:G,4,0))","v":"104246"},{"$f":"IF(I54=\"\",\"\",IF(VLOOKUP(B54,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B54,Sortimente!D:L,9,0)))","v":""}]
[47,{"$f":"$A$1&Musteranlage!A55","v":"ABSOLUT1847"},null,null,null,null,null,{"$f":"IF(L55=\"\",\"\",IF(L55=\"Sonder\",\"J\",VLOOKUP(L55,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B55,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B55,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I55=\"\",\"\",VLOOKUP($B55,Sortimente!D:G,4,0))","v":"104245"},{"$f":"IF(I55=\"\",\"\",IF(VLOOKUP(B55,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B55,Sortimente!D:L,9,0)))","v":""}]
[48,{"$f":"$A$1&Musteranlage!A56","v":"ABSOLUT1848"},null,null,null,null,null,{"$f":"IF(L56=\"\",\"\",IF(L56=\"Sonder\",\"J\",VLOOKUP(L56,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B56,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B56,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I56=\"\",\"\",VLOOKUP($B56,Sortimente!D:G,4,0))","v":"104244"},{"$f":"IF(I56=\"\",\"\",IF(VLOOKUP(B56,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B56,Sortimente!D:L,9,0)))","v":""}]
[49,{"$f":"$A$1&Musteranlage!A57","v":"ABSOLUT1849"},null,null,null,null,null,{"$f":"IF(L57=\"\",\"\",IF(L57=\"Sonder\",\"J\",VLOOKUP(L57,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B57,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B57,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I57=\"\",\"\",VLOOKUP($B57,Sortimente!D:G,4,0))","v":"103944"},{"$f":"IF(I57=\"\",\"\",IF(VLOOKUP(B57,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B57,Sortimente!D:L,9,0)))","v":""}]
[50,{"$f":"$A$1&Musteranlage!A58","v":"ABSOLUT1850"},null,null,null,null,null,{"$f":"IF(L58=\"\",\"\",IF(L58=\"Sonder\",\"J\",VLOOKUP(L58,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B58,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B58,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I58=\"\",\"\",VLOOKUP($B58,Sortimente!D:G,4,0))","v":"104256"},{"$f":"IF(I58=\"\",\"\",IF(VLOOKUP(B58,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B58,Sortimente!D:L,9,0)))","v":""}]
[51,{"$f":"$A$1&Musteranlage!A59","v":"ABSOLUT1851"},null,null,null,null,null,{"$f":"IF(L59=\"\",\"\",IF(L59=\"Sonder\",\"J\",VLOOKUP(L59,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B59,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B59,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I59=\"\",\"\",VLOOKUP($B59,Sortimente!D:G,4,0))","v":"104257"},{"$f":"IF(I59=\"\",\"\",IF(VLOOKUP(B59,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B59,Sortimente!D:L,9,0)))","v":""}]
[52,{"$f":"$A$1&Musteranlage!A60","v":"ABSOLUT1852"},null,null,null,null,null,{"$f":"IF(L60=\"\",\"\",IF(L60=\"Sonder\",\"J\",VLOOKUP(L60,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B60,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B60,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I60=\"\",\"\",VLOOKUP($B60,Sortimente!D:G,4,0))","v":"103963"},{"$f":"IF(I60=\"\",\"\",IF(VLOOKUP(B60,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B60,Sortimente!D:L,9,0)))","v":""}]
[53,{"$f":"$A$1&Musteranlage!A61","v":"ABSOLUT1853"},null,null,null,null,null,{"$f":"IF(L61=\"\",\"\",IF(L61=\"Sonder\",\"J\",VLOOKUP(L61,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B61,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B61,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I61=\"\",\"\",VLOOKUP($B61,Sortimente!D:G,4,0))","v":"103941"},{"$f":"IF(I61=\"\",\"\",IF(VLOOKUP(B61,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B61,Sortimente!D:L,9,0)))","v":1}]
[54,{"$f":"$A$1&Musteranlage!A62","v":"ABSOLUT1854"},null,null,null,null,null,{"$f":"IF(L62=\"\",\"\",IF(L62=\"Sonder\",\"J\",VLOOKUP(L62,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B62,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B62,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I62=\"\",\"\",VLOOKUP($B62,Sortimente!D:G,4,0))","v":"104212"},{"$f":"IF(I62=\"\",\"\",IF(VLOOKUP(B62,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B62,Sortimente!D:L,9,0)))","v":""}]
[55,{"$f":"$A$1&Musteranlage!A63","v":"ABSOLUT1855"},null,null,null,null,null,{"$f":"IF(L63=\"\",\"\",IF(L63=\"Sonder\",\"J\",VLOOKUP(L63,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B63,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B63,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I63=\"\",\"\",VLOOKUP($B63,Sortimente!D:G,4,0))","v":"104218"},{"$f":"IF(I63=\"\",\"\",IF(VLOOKUP(B63,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B63,Sortimente!D:L,9,0)))","v":""}]
[56,{"$f":"$A$1&Musteranlage!A64","v":"ABSOLUT1856"},null,null,null,null,null,{"$f":"IF(L64=\"\",\"\",IF(L64=\"Sonder\",\"J\",VLOOKUP(L64,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B64,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B64,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I64=\"\",\"\",VLOOKUP($B64,Sortimente!D:G,4,0))","v":"104224"},{"$f":"IF(I64=\"\",\"\",IF(VLOOKUP(B64,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B64,Sortimente!D:L,9,0)))","v":""}]
[57,{"$f":"$A$1&Musteranlage!A65","v":"ABSOLUT1857"},null,null,null,null,null,{"$f":"IF(L65=\"\",\"\",IF(L65=\"Sonder\",\"J\",VLOOKUP(L65,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B65,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B65,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I65=\"\",\"\",VLOOKUP($B65,Sortimente!D:G,4,0))","v":"104229"},{"$f":"IF(I65=\"\",\"\",IF(VLOOKUP(B65,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B65,Sortimente!D:L,9,0)))","v":""}]
[58,{"$f":"$A$1&Musteranlage!A66","v":"ABSOLUT1858"},null,null,null,null,null,{"$f":"IF(L66=\"\",\"\",IF(L66=\"Sonder\",\"J\",VLOOKUP(L66,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B66,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B66,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I66=\"\",\"\",VLOOKUP($B66,Sortimente!D:G,4,0))","v":"103838"},{"$f":"IF(I66=\"\",\"\",IF(VLOOKUP(B66,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B66,Sortimente!D:L,9,0)))","v":""}]
[59,{"$f":"$A$1&Musteranlage!A67","v":"ABSOLUT1859"},null,null,null,null,null,{"$f":"IF(L67=\"\",\"\",IF(L67=\"Sonder\",\"J\",VLOOKUP(L67,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B67,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B67,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I67=\"\",\"\",VLOOKUP($B67,Sortimente!D:G,4,0))","v":"100265"},{"$f":"IF(I67=\"\",\"\",IF(VLOOKUP(B67,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B67,Sortimente!D:L,9,0)))","v":""}]
[60,{"$f":"$A$1&Musteranlage!A68","v":"ABSOLUT1860"},null,null,null,null,null,{"$f":"IF(L68=\"\",\"\",IF(L68=\"Sonder\",\"J\",VLOOKUP(L68,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B68,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B68,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I68=\"\",\"\",VLOOKUP($B68,Sortimente!D:G,4,0))","v":"100266"},{"$f":"IF(I68=\"\",\"\",IF(VLOOKUP(B68,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B68,Sortimente!D:L,9,0)))","v":""}]
[61,{"$f":"$A$1&Musteranlage!A69","v":"ABSOLUT1861"},null,null,null,null,null,{"$f":"IF(L69=\"\",\"\",IF(L69=\"Sonder\",\"J\",VLOOKUP(L69,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B69,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B69,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I69=\"\",\"\",VLOOKUP($B69,Sortimente!D:G,4,0))","v":"103841"},{"$f":"IF(I69=\"\",\"\",IF(VLOOKUP(B69,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B69,Sortimente!D:L,9,0)))","v":""}]
[62,{"$f":"$A$1&Musteranlage!A70","v":"ABSOLUT1862"},null,null,null,null,null,{"$f":"IF(L70=\"\",\"\",IF(L70=\"Sonder\",\"J\",VLOOKUP(L70,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B70,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B70,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I70=\"\",\"\",VLOOKUP($B70,Sortimente!D:G,4,0))","v":"100264"},{"$f":"IF(I70=\"\",\"\",IF(VLOOKUP(B70,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B70,Sortimente!D:L,9,0)))","v":""}]
[63,{"$f":"$A$1&Musteranlage!A71","v":"ABSOLUT1863"},null,null,null,null,null,{"$f":"IF(L71=\"\",\"\",IF(L71=\"Sonder\",\"J\",VLOOKUP(L71,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B71,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B71,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I71=\"\",\"\",VLOOKUP($B71,Sortimente!D:G,4,0))","v":"103833"},{"$f":"IF(I71=\"\",\"\",IF(VLOOKUP(B71,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B71,Sortimente!D:L,9,0)))","v":""}]
[64,{"$f":"$A$1&Musteranlage!A72","v":"ABSOLUT1864"},null,null,null,null,null,{"$f":"IF(L72=\"\",\"\",IF(L72=\"Sonder\",\"J\",VLOOKUP(L72,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B72,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B72,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I72=\"\",\"\",VLOOKUP($B72,Sortimente!D:G,4,0))","v":"103820"},{"$f":"IF(I72=\"\",\"\",IF(VLOOKUP(B72,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B72,Sortimente!D:L,9,0)))","v":""}]
[65,{"$f":"$A$1&Musteranlage!A73","v":"ABSOLUT1865"},null,null,null,null,null,{"$f":"IF(L73=\"\",\"\",IF(L73=\"Sonder\",\"J\",VLOOKUP(L73,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B73,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B73,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I73=\"\",\"\",VLOOKUP($B73,Sortimente!D:G,4,0))","v":"103821"},{"$f":"IF(I73=\"\",\"\",IF(VLOOKUP(B73,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B73,Sortimente!D:L,9,0)))","v":""}]
[66,{"$f":"$A$1&Musteranlage!A74","v":"ABSOLUT1866"},null,null,null,null,null,{"$f":"IF(L74=\"\",\"\",IF(L74=\"Sonder\",\"J\",VLOOKUP(L74,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B74,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B74,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I74=\"\",\"\",VLOOKUP($B74,Sortimente!D:G,4,0))","v":"103822"},{"$f":"IF(I74=\"\",\"\",IF(VLOOKUP(B74,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B74,Sortimente!D:L,9,0)))","v":""}]
[67,{"$f":"$A$1&Musteranlage!A75","v":"ABSOLUT1867"},null,null,null,null,null,{"$f":"IF(L75=\"\",\"\",IF(L75=\"Sonder\",\"J\",VLOOKUP(L75,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B75,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B75,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I75=\"\",\"\",VLOOKUP($B75,Sortimente!D:G,4,0))","v":"103823"},{"$f":"IF(I75=\"\",\"\",IF(VLOOKUP(B75,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B75,Sortimente!D:L,9,0)))","v":""}]
[68,{"$f":"$A$1&Musteranlage!A76","v":"ABSOLUT1868"},null,null,null,null,null,{"$f":"IF(L76=\"\",\"\",IF(L76=\"Sonder\",\"J\",VLOOKUP(L76,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B76,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B76,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I76=\"\",\"\",VLOOKUP($B76,Sortimente!D:G,4,0))","v":"103824"},{"$f":"IF(I76=\"\",\"\",IF(VLOOKUP(B76,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B76,Sortimente!D:L,9,0)))","v":""}]
[69,{"$f":"$A$1&Musteranlage!A77","v":"ABSOLUT1869"},null,null,null,null,null,{"$f":"IF(L77=\"\",\"\",IF(L77=\"Sonder\",\"J\",VLOOKUP(L77,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B77,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B77,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I77=\"\",\"\",VLOOKUP($B77,Sortimente!D:G,4,0))","v":"103825"},{"$f":"IF(I77=\"\",\"\",IF(VLOOKUP(B77,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B77,Sortimente!D:L,9,0)))","v":""}]
[70,{"$f":"$A$1&Musteranlage!A78","v":"ABSOLUT1870"},null,null,null,null,null,{"$f":"IF(L78=\"\",\"\",IF(L78=\"Sonder\",\"J\",VLOOKUP(L78,sanschie!A:K,11,0)))","v":"J"},{"$f":"IF(ISNA(VLOOKUP($B78,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B78,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I78=\"\",\"\",VLOOKUP($B78,Sortimente!D:G,4,0))","v":"103848"},{"$f":"IF(I78=\"\",\"\",IF(VLOOKUP(B78,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B78,Sortimente!D:L,9,0)))","v":""}]
[71,{"$f":"$A$1&Musteranlage!A79","v":"ABSOLUT1871"},null,null,null,null,null,{"$f":"IF(L79=\"\",\"\",IF(L79=\"Sonder\",\"J\",VLOOKUP(L79,sanschie!A:K,11,0)))","v":"N"},{"$f":"IF(ISNA(VLOOKUP($B79,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B79,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I79=\"\",\"\",VLOOKUP($B79,Sortimente!D:G,4,0))","v":"103846"},{"$f":"IF(I79=\"\",\"\",IF(VLOOKUP(B79,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B79,Sortimente!D:L,9,0)))","v":""}]
[72,{"$f":"$A$1&Musteranlage!A80","v":"ABSOLUT1872"},null,null,null,null,null,{"$f":"IF(L80=\"\",\"\",IF(L80=\"Sonder\",\"J\",VLOOKUP(L80,sanschie!A:K,11,0)))","v":"N"},{"$f":"IF(ISNA(VLOOKUP($B80,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B80,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I80=\"\",\"\",VLOOKUP($B80,Sortimente!D:G,4,0))","v":"103847"},{"$f":"IF(I80=\"\",\"\",IF(VLOOKUP(B80,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B80,Sortimente!D:L,9,0)))","v":""}]
[73,{"$f":"$A$1&Musteranlage!A81","v":"ABSOLUT1873"},null,null,null,null,null,{"$f":"IF(L81=\"\",\"\",IF(L81=\"Sonder\",\"J\",VLOOKUP(L81,sanschie!A:K,11,0)))","v":"N"},{"$f":"IF(ISNA(VLOOKUP($B81,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B81,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I81=\"\",\"\",VLOOKUP($B81,Sortimente!D:G,4,0))","v":"104259"},{"$f":"IF(I81=\"\",\"\",IF(VLOOKUP(B81,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B81,Sortimente!D:L,9,0)))","v":""}]
[74,{"$f":"$A$1&Musteranlage!A82","v":"ABSOLUT1874"},null,null,null,null,null,{"$f":"IF(L82=\"\",\"\",IF(L82=\"Sonder\",\"J\",VLOOKUP(L82,sanschie!A:K,11,0)))","v":"N"},{"$f":"IF(ISNA(VLOOKUP($B82,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B82,Sortimente!D:G,2,0))","v":0},null,null,{"$f":"IF(I82=\"\",\"\",VLOOKUP($B82,Sortimente!D:G,4,0))","v":"104261"},{"$f":"IF(I82=\"\",\"\",IF(VLOOKUP(B82,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B82,Sortimente!D:L,9,0)))","v":2}]
[75,{"$f":"$A$1&Musteranlage!A83","v":"ABSOLUT1875"},null,null,null,null,null,{"$f":"IF(L83=\"\",\"\",IF(L83=\"Sonder\",\"J\",VLOOKUP(L83,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B83,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B83,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I83=\"\",\"\",VLOOKUP($B83,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I83=\"\",\"\",IF(VLOOKUP(B83,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B83,Sortimente!D:L,9,0)))","v":""}]
[76,{"$f":"$A$1&Musteranlage!A84","v":"ABSOLUT1876"},null,null,null,null,null,{"$f":"IF(L84=\"\",\"\",IF(L84=\"Sonder\",\"J\",VLOOKUP(L84,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B84,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B84,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I84=\"\",\"\",VLOOKUP($B84,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I84=\"\",\"\",IF(VLOOKUP(B84,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B84,Sortimente!D:L,9,0)))","v":""}]
[77,{"$f":"$A$1&Musteranlage!A85","v":"ABSOLUT1877"},null,null,null,null,null,{"$f":"IF(L85=\"\",\"\",IF(L85=\"Sonder\",\"J\",VLOOKUP(L85,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B85,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B85,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I85=\"\",\"\",VLOOKUP($B85,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I85=\"\",\"\",IF(VLOOKUP(B85,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B85,Sortimente!D:L,9,0)))","v":""}]
[78,{"$f":"$A$1&Musteranlage!A86","v":"ABSOLUT1878"},null,null,null,null,null,{"$f":"IF(L86=\"\",\"\",IF(L86=\"Sonder\",\"J\",VLOOKUP(L86,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B86,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B86,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I86=\"\",\"\",VLOOKUP($B86,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I86=\"\",\"\",IF(VLOOKUP(B86,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B86,Sortimente!D:L,9,0)))","v":""}]
[79,{"$f":"$A$1&Musteranlage!A87","v":"ABSOLUT1879"},null,null,null,null,null,{"$f":"IF(L87=\"\",\"\",IF(L87=\"Sonder\",\"J\",VLOOKUP(L87,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B87,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B87,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I87=\"\",\"\",VLOOKUP($B87,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I87=\"\",\"\",IF(VLOOKUP(B87,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B87,Sortimente!D:L,9,0)))","v":""}]
[80,{"$f":"$A$1&Musteranlage!A88","v":"ABSOLUT1880"},null,null,null,null,null,{"$f":"IF(L88=\"\",\"\",IF(L88=\"Sonder\",\"J\",VLOOKUP(L88,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B88,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B88,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I88=\"\",\"\",VLOOKUP($B88,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I88=\"\",\"\",IF(VLOOKUP(B88,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B88,Sortimente!D:L,9,0)))","v":""}]
[81,{"$f":"$A$1&Musteranlage!A89","v":"ABSOLUT1881"},null,null,null,null,null,{"$f":"IF(L89=\"\",\"\",IF(L89=\"Sonder\",\"J\",VLOOKUP(L89,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B89,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B89,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I89=\"\",\"\",VLOOKUP($B89,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I89=\"\",\"\",IF(VLOOKUP(B89,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B89,Sortimente!D:L,9,0)))","v":""}]
[82,{"$f":"$A$1&Musteranlage!A90","v":"ABSOLUT1882"},null,null,null,null,null,{"$f":"IF(L90=\"\",\"\",IF(L90=\"Sonder\",\"J\",VLOOKUP(L90,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B90,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B90,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I90=\"\",\"\",VLOOKUP($B90,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I90=\"\",\"\",IF(VLOOKUP(B90,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B90,Sortimente!D:L,9,0)))","v":""}]
[83,{"$f":"$A$1&Musteranlage!A91","v":"ABSOLUT1883"},null,null,null,null,null,{"$f":"IF(L91=\"\",\"\",IF(L91=\"Sonder\",\"J\",VLOOKUP(L91,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B91,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B91,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I91=\"\",\"\",VLOOKUP($B91,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I91=\"\",\"\",IF(VLOOKUP(B91,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B91,Sortimente!D:L,9,0)))","v":""}]
[84,{"$f":"$A$1&Musteranlage!A92","v":"ABSOLUT1884"},null,null,null,null,null,{"$f":"IF(L92=\"\",\"\",IF(L92=\"Sonder\",\"J\",VLOOKUP(L92,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B92,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B92,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I92=\"\",\"\",VLOOKUP($B92,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I92=\"\",\"\",IF(VLOOKUP(B92,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B92,Sortimente!D:L,9,0)))","v":""}]
[85,{"$f":"$A$1&Musteranlage!A93","v":"ABSOLUT1885"},null,null,null,null,null,{"$f":"IF(L93=\"\",\"\",IF(L93=\"Sonder\",\"J\",VLOOKUP(L93,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B93,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B93,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I93=\"\",\"\",VLOOKUP($B93,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I93=\"\",\"\",IF(VLOOKUP(B93,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B93,Sortimente!D:L,9,0)))","v":""}]
[86,{"$f":"$A$1&Musteranlage!A94","v":"ABSOLUT1886"},null,null,null,null,null,{"$f":"IF(L94=\"\",\"\",IF(L94=\"Sonder\",\"J\",VLOOKUP(L94,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B94,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B94,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I94=\"\",\"\",VLOOKUP($B94,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I94=\"\",\"\",IF(VLOOKUP(B94,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B94,Sortimente!D:L,9,0)))","v":""}]
[87,{"$f":"$A$1&Musteranlage!A95","v":"ABSOLUT1887"},null,null,null,null,null,{"$f":"IF(L95=\"\",\"\",IF(L95=\"Sonder\",\"J\",VLOOKUP(L95,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B95,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B95,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I95=\"\",\"\",VLOOKUP($B95,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I95=\"\",\"\",IF(VLOOKUP(B95,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B95,Sortimente!D:L,9,0)))","v":""}]
[88,{"$f":"$A$1&Musteranlage!A96","v":"ABSOLUT1888"},null,null,null,null,null,{"$f":"IF(L96=\"\",\"\",IF(L96=\"Sonder\",\"J\",VLOOKUP(L96,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B96,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B96,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I96=\"\",\"\",VLOOKUP($B96,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I96=\"\",\"\",IF(VLOOKUP(B96,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B96,Sortimente!D:L,9,0)))","v":""}]
[89,{"$f":"$A$1&Musteranlage!A97","v":"ABSOLUT1889"},null,null,null,null,null,{"$f":"IF(L97=\"\",\"\",IF(L97=\"Sonder\",\"J\",VLOOKUP(L97,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B97,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B97,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I97=\"\",\"\",VLOOKUP($B97,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I97=\"\",\"\",IF(VLOOKUP(B97,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B97,Sortimente!D:L,9,0)))","v":""}]
[90,{"$f":"$A$1&Musteranlage!A98","v":"ABSOLUT1890"},null,null,null,null,null,{"$f":"IF(L98=\"\",\"\",IF(L98=\"Sonder\",\"J\",VLOOKUP(L98,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B98,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B98,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I98=\"\",\"\",VLOOKUP($B98,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I98=\"\",\"\",IF(VLOOKUP(B98,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B98,Sortimente!D:L,9,0)))","v":""}]
[91,{"$f":"$A$1&Musteranlage!A99","v":"ABSOLUT1891"},null,null,null,null,null,{"$f":"IF(L99=\"\",\"\",IF(L99=\"Sonder\",\"J\",VLOOKUP(L99,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B99,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B99,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I99=\"\",\"\",VLOOKUP($B99,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I99=\"\",\"\",IF(VLOOKUP(B99,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B99,Sortimente!D:L,9,0)))","v":""}]
[92,{"$f":"$A$1&Musteranlage!A100","v":"ABSOLUT1892"},null,null,null,null,null,{"$f":"IF(L100=\"\",\"\",IF(L100=\"Sonder\",\"J\",VLOOKUP(L100,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B100,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B100,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I100=\"\",\"\",VLOOKUP($B100,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I100=\"\",\"\",IF(VLOOKUP(B100,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B100,Sortimente!D:L,9,0)))","v":""}]
[93,{"$f":"$A$1&Musteranlage!A101","v":"ABSOLUT1893"},null,null,null,null,null,{"$f":"IF(L101=\"\",\"\",IF(L101=\"Sonder\",\"J\",VLOOKUP(L101,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B101,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B101,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I101=\"\",\"\",VLOOKUP($B101,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I101=\"\",\"\",IF(VLOOKUP(B101,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B101,Sortimente!D:L,9,0)))","v":""}]
[94,{"$f":"$A$1&Musteranlage!A102","v":"ABSOLUT1894"},null,null,null,null,null,{"$f":"IF(L102=\"\",\"\",IF(L102=\"Sonder\",\"J\",VLOOKUP(L102,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B102,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B102,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I102=\"\",\"\",VLOOKUP($B102,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I102=\"\",\"\",IF(VLOOKUP(B102,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B102,Sortimente!D:L,9,0)))","v":""}]
[95,{"$f":"$A$1&Musteranlage!A103","v":"ABSOLUT1895"},null,null,null,null,null,{"$f":"IF(L103=\"\",\"\",IF(L103=\"Sonder\",\"J\",VLOOKUP(L103,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B103,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B103,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I103=\"\",\"\",VLOOKUP($B103,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I103=\"\",\"\",IF(VLOOKUP(B103,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B103,Sortimente!D:L,9,0)))","v":""}]
[96,{"$f":"$A$1&Musteranlage!A104","v":"ABSOLUT1896"},null,null,null,null,null,{"$f":"IF(L104=\"\",\"\",IF(L104=\"Sonder\",\"J\",VLOOKUP(L104,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B104,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B104,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I104=\"\",\"\",VLOOKUP($B104,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I104=\"\",\"\",IF(VLOOKUP(B104,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B104,Sortimente!D:L,9,0)))","v":""}]
[97,{"$f":"$A$1&Musteranlage!A105","v":"ABSOLUT1897"},null,null,null,null,null,{"$f":"IF(L105=\"\",\"\",IF(L105=\"Sonder\",\"J\",VLOOKUP(L105,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B105,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B105,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I105=\"\",\"\",VLOOKUP($B105,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I105=\"\",\"\",IF(VLOOKUP(B105,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B105,Sortimente!D:L,9,0)))","v":""}]
[98,{"$f":"$A$1&Musteranlage!A106","v":"ABSOLUT1898"},null,null,null,null,null,{"$f":"IF(L106=\"\",\"\",IF(L106=\"Sonder\",\"J\",VLOOKUP(L106,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B106,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B106,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I106=\"\",\"\",VLOOKUP($B106,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I106=\"\",\"\",IF(VLOOKUP(B106,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B106,Sortimente!D:L,9,0)))","v":""}]
[99,{"$f":"$A$1&Musteranlage!A107","v":"ABSOLUT1899"},null,null,null,null,null,{"$f":"IF(L107=\"\",\"\",IF(L107=\"Sonder\",\"J\",VLOOKUP(L107,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B107,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B107,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I107=\"\",\"\",VLOOKUP($B107,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I107=\"\",\"\",IF(VLOOKUP(B107,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B107,Sortimente!D:L,9,0)))","v":""}]
[100,{"$f":"$A$1&Musteranlage!A108","v":"ABSOLUT18100"},null,null,null,null,null,{"$f":"IF(L108=\"\",\"\",IF(L108=\"Sonder\",\"J\",VLOOKUP(L108,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B108,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B108,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I108=\"\",\"\",VLOOKUP($B108,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I108=\"\",\"\",IF(VLOOKUP(B108,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B108,Sortimente!D:L,9,0)))","v":""}]
[101,{"$f":"$A$1&Musteranlage!A109","v":"ABSOLUT18101"},null,null,null,null,null,{"$f":"IF(L109=\"\",\"\",IF(L109=\"Sonder\",\"J\",VLOOKUP(L109,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B109,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B109,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I109=\"\",\"\",VLOOKUP($B109,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I109=\"\",\"\",IF(VLOOKUP(B109,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B109,Sortimente!D:L,9,0)))","v":""}]
[102,{"$f":"$A$1&Musteranlage!A110","v":"ABSOLUT18102"},null,null,null,null,null,{"$f":"IF(L110=\"\",\"\",IF(L110=\"Sonder\",\"J\",VLOOKUP(L110,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B110,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B110,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I110=\"\",\"\",VLOOKUP($B110,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I110=\"\",\"\",IF(VLOOKUP(B110,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B110,Sortimente!D:L,9,0)))","v":""}]
[103,{"$f":"$A$1&Musteranlage!A111","v":"ABSOLUT18103"},null,null,null,null,null,{"$f":"IF(L111=\"\",\"\",IF(L111=\"Sonder\",\"J\",VLOOKUP(L111,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B111,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B111,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I111=\"\",\"\",VLOOKUP($B111,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I111=\"\",\"\",IF(VLOOKUP(B111,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B111,Sortimente!D:L,9,0)))","v":""}]
[104,{"$f":"$A$1&Musteranlage!A112","v":"ABSOLUT18104"},null,null,null,null,null,{"$f":"IF(L112=\"\",\"\",IF(L112=\"Sonder\",\"J\",VLOOKUP(L112,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B112,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B112,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I112=\"\",\"\",VLOOKUP($B112,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I112=\"\",\"\",IF(VLOOKUP(B112,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B112,Sortimente!D:L,9,0)))","v":""}]
[105,{"$f":"$A$1&Musteranlage!A113","v":"ABSOLUT18105"},null,null,null,null,null,{"$f":"IF(L113=\"\",\"\",IF(L113=\"Sonder\",\"J\",VLOOKUP(L113,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B113,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B113,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I113=\"\",\"\",VLOOKUP($B113,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I113=\"\",\"\",IF(VLOOKUP(B113,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B113,Sortimente!D:L,9,0)))","v":""}]
[106,{"$f":"$A$1&Musteranlage!A114","v":"ABSOLUT18106"},null,null,null,null,null,{"$f":"IF(L114=\"\",\"\",IF(L114=\"Sonder\",\"J\",VLOOKUP(L114,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B114,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B114,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I114=\"\",\"\",VLOOKUP($B114,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I114=\"\",\"\",IF(VLOOKUP(B114,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B114,Sortimente!D:L,9,0)))","v":""}]
[107,{"$f":"$A$1&Musteranlage!A115","v":"ABSOLUT18107"},null,null,null,null,null,{"$f":"IF(L115=\"\",\"\",IF(L115=\"Sonder\",\"J\",VLOOKUP(L115,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B115,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B115,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I115=\"\",\"\",VLOOKUP($B115,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I115=\"\",\"\",IF(VLOOKUP(B115,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B115,Sortimente!D:L,9,0)))","v":""}]
[108,{"$f":"$A$1&Musteranlage!A116","v":"ABSOLUT18108"},null,null,null,null,null,{"$f":"IF(L116=\"\",\"\",IF(L116=\"Sonder\",\"J\",VLOOKUP(L116,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B116,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B116,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I116=\"\",\"\",VLOOKUP($B116,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I116=\"\",\"\",IF(VLOOKUP(B116,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B116,Sortimente!D:L,9,0)))","v":""}]
[109,{"$f":"$A$1&Musteranlage!A117","v":"ABSOLUT18109"},null,null,null,null,null,{"$f":"IF(L117=\"\",\"\",IF(L117=\"Sonder\",\"J\",VLOOKUP(L117,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B117,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B117,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I117=\"\",\"\",VLOOKUP($B117,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I117=\"\",\"\",IF(VLOOKUP(B117,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B117,Sortimente!D:L,9,0)))","v":""}]
[110,{"$f":"$A$1&Musteranlage!A118","v":"ABSOLUT18110"},null,null,null,null,null,{"$f":"IF(L118=\"\",\"\",IF(L118=\"Sonder\",\"J\",VLOOKUP(L118,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B118,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B118,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I118=\"\",\"\",VLOOKUP($B118,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I118=\"\",\"\",IF(VLOOKUP(B118,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B118,Sortimente!D:L,9,0)))","v":""}]
[111,{"$f":"$A$1&Musteranlage!A119","v":"ABSOLUT18111"},null,null,null,null,null,{"$f":"IF(L119=\"\",\"\",IF(L119=\"Sonder\",\"J\",VLOOKUP(L119,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B119,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B119,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I119=\"\",\"\",VLOOKUP($B119,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I119=\"\",\"\",IF(VLOOKUP(B119,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B119,Sortimente!D:L,9,0)))","v":""}]
[112,{"$f":"$A$1&Musteranlage!A120","v":"ABSOLUT18112"},null,null,null,null,null,{"$f":"IF(L120=\"\",\"\",IF(L120=\"Sonder\",\"J\",VLOOKUP(L120,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B120,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B120,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I120=\"\",\"\",VLOOKUP($B120,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I120=\"\",\"\",IF(VLOOKUP(B120,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B120,Sortimente!D:L,9,0)))","v":""}]
[113,{"$f":"$A$1&Musteranlage!A121","v":"ABSOLUT18113"},null,null,null,null,null,{"$f":"IF(L121=\"\",\"\",IF(L121=\"Sonder\",\"J\",VLOOKUP(L121,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B121,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B121,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I121=\"\",\"\",VLOOKUP($B121,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I121=\"\",\"\",IF(VLOOKUP(B121,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B121,Sortimente!D:L,9,0)))","v":""}]
[114,{"$f":"$A$1&Musteranlage!A122","v":"ABSOLUT18114"},null,null,null,null,null,{"$f":"IF(L122=\"\",\"\",IF(L122=\"Sonder\",\"J\",VLOOKUP(L122,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B122,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B122,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I122=\"\",\"\",VLOOKUP($B122,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I122=\"\",\"\",IF(VLOOKUP(B122,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B122,Sortimente!D:L,9,0)))","v":""}]
[115,{"$f":"$A$1&Musteranlage!A123","v":"ABSOLUT18115"},null,null,null,null,null,{"$f":"IF(L123=\"\",\"\",IF(L123=\"Sonder\",\"J\",VLOOKUP(L123,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B123,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B123,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I123=\"\",\"\",VLOOKUP($B123,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I123=\"\",\"\",IF(VLOOKUP(B123,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B123,Sortimente!D:L,9,0)))","v":""}]
[116,{"$f":"$A$1&Musteranlage!A124","v":"ABSOLUT18116"},null,null,null,null,null,{"$f":"IF(L124=\"\",\"\",IF(L124=\"Sonder\",\"J\",VLOOKUP(L124,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B124,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B124,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I124=\"\",\"\",VLOOKUP($B124,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I124=\"\",\"\",IF(VLOOKUP(B124,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B124,Sortimente!D:L,9,0)))","v":""}]
[117,{"$f":"$A$1&Musteranlage!A125","v":"ABSOLUT18117"},null,null,null,null,null,{"$f":"IF(L125=\"\",\"\",IF(L125=\"Sonder\",\"J\",VLOOKUP(L125,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B125,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B125,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I125=\"\",\"\",VLOOKUP($B125,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I125=\"\",\"\",IF(VLOOKUP(B125,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B125,Sortimente!D:L,9,0)))","v":""}]
[118,{"$f":"$A$1&Musteranlage!A126","v":"ABSOLUT18118"},null,null,null,null,null,{"$f":"IF(L126=\"\",\"\",IF(L126=\"Sonder\",\"J\",VLOOKUP(L126,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B126,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B126,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I126=\"\",\"\",VLOOKUP($B126,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I126=\"\",\"\",IF(VLOOKUP(B126,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B126,Sortimente!D:L,9,0)))","v":""}]
[119,{"$f":"$A$1&Musteranlage!A127","v":"ABSOLUT18119"},null,null,null,null,null,{"$f":"IF(L127=\"\",\"\",IF(L127=\"Sonder\",\"J\",VLOOKUP(L127,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B127,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B127,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I127=\"\",\"\",VLOOKUP($B127,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I127=\"\",\"\",IF(VLOOKUP(B127,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B127,Sortimente!D:L,9,0)))","v":""}]
[120,{"$f":"$A$1&Musteranlage!A128","v":"ABSOLUT18120"},null,null,null,null,null,{"$f":"IF(L128=\"\",\"\",IF(L128=\"Sonder\",\"J\",VLOOKUP(L128,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B128,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B128,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I128=\"\",\"\",VLOOKUP($B128,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I128=\"\",\"\",IF(VLOOKUP(B128,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B128,Sortimente!D:L,9,0)))","v":""}]
[121,{"$f":"$A$1&Musteranlage!A129","v":"ABSOLUT18121"},null,null,null,null,null,{"$f":"IF(L129=\"\",\"\",IF(L129=\"Sonder\",\"J\",VLOOKUP(L129,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B129,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B129,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I129=\"\",\"\",VLOOKUP($B129,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I129=\"\",\"\",IF(VLOOKUP(B129,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B129,Sortimente!D:L,9,0)))","v":""}]
[122,{"$f":"$A$1&Musteranlage!A130","v":"ABSOLUT18122"},null,null,null,null,null,{"$f":"IF(L130=\"\",\"\",IF(L130=\"Sonder\",\"J\",VLOOKUP(L130,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B130,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B130,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I130=\"\",\"\",VLOOKUP($B130,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I130=\"\",\"\",IF(VLOOKUP(B130,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B130,Sortimente!D:L,9,0)))","v":""}]
[123,{"$f":"$A$1&Musteranlage!A131","v":"ABSOLUT18123"},null,null,null,null,null,{"$f":"IF(L131=\"\",\"\",IF(L131=\"Sonder\",\"J\",VLOOKUP(L131,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B131,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B131,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I131=\"\",\"\",VLOOKUP($B131,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I131=\"\",\"\",IF(VLOOKUP(B131,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B131,Sortimente!D:L,9,0)))","v":""}]
[124,{"$f":"$A$1&Musteranlage!A132","v":"ABSOLUT18124"},null,null,null,null,null,{"$f":"IF(L132=\"\",\"\",IF(L132=\"Sonder\",\"J\",VLOOKUP(L132,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B132,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B132,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I132=\"\",\"\",VLOOKUP($B132,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I132=\"\",\"\",IF(VLOOKUP(B132,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B132,Sortimente!D:L,9,0)))","v":""}]
[125,{"$f":"$A$1&Musteranlage!A133","v":"ABSOLUT18125"},null,null,null,null,null,{"$f":"IF(L133=\"\",\"\",IF(L133=\"Sonder\",\"J\",VLOOKUP(L133,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B133,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B133,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I133=\"\",\"\",VLOOKUP($B133,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I133=\"\",\"\",IF(VLOOKUP(B133,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B133,Sortimente!D:L,9,0)))","v":""}]
[126,{"$f":"$A$1&Musteranlage!A134","v":"ABSOLUT18126"},null,null,null,null,null,{"$f":"IF(L134=\"\",\"\",IF(L134=\"Sonder\",\"J\",VLOOKUP(L134,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B134,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B134,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I134=\"\",\"\",VLOOKUP($B134,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I134=\"\",\"\",IF(VLOOKUP(B134,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B134,Sortimente!D:L,9,0)))","v":""}]
[127,{"$f":"$A$1&Musteranlage!A135","v":"ABSOLUT18127"},null,null,null,null,null,{"$f":"IF(L135=\"\",\"\",IF(L135=\"Sonder\",\"J\",VLOOKUP(L135,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B135,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B135,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I135=\"\",\"\",VLOOKUP($B135,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I135=\"\",\"\",IF(VLOOKUP(B135,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B135,Sortimente!D:L,9,0)))","v":""}]
[128,{"$f":"$A$1&Musteranlage!A136","v":"ABSOLUT18128"},null,null,null,null,null,{"$f":"IF(L136=\"\",\"\",IF(L136=\"Sonder\",\"J\",VLOOKUP(L136,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B136,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B136,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I136=\"\",\"\",VLOOKUP($B136,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I136=\"\",\"\",IF(VLOOKUP(B136,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B136,Sortimente!D:L,9,0)))","v":""}]
[129,{"$f":"$A$1&Musteranlage!A137","v":"ABSOLUT18129"},null,null,null,null,null,{"$f":"IF(L137=\"\",\"\",IF(L137=\"Sonder\",\"J\",VLOOKUP(L137,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B137,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B137,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I137=\"\",\"\",VLOOKUP($B137,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I137=\"\",\"\",IF(VLOOKUP(B137,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B137,Sortimente!D:L,9,0)))","v":""}]
[130,{"$f":"$A$1&Musteranlage!A138","v":"ABSOLUT18130"},null,null,null,null,null,{"$f":"IF(L138=\"\",\"\",IF(L138=\"Sonder\",\"J\",VLOOKUP(L138,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B138,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B138,Sortimente!D:G,2,0))","v":""},null,null,{"$f":"IF(I138=\"\",\"\",VLOOKUP($B138,Sortimente!D:G,4,0))","v":""},{"$f":"IF(I138=\"\",\"\",IF(VLOOKUP(B138,Sortimente!D:L,9,0)=0,\"\",VLOOKUP(B138,Sortimente!D:L,9,0)))","v":""}]

{"sheet":"Verbindungsleitung","index":14,"n_rows":96,"n_cols":11,"rows_kept":96,"cut":false,"hidden":true,"merged":[]}
[{"$f":"Daten!U170","v":"Nein"}]
[null,null,{"$f":"VLOOKUP(A1,Daten!T:U,2,0)","v":"Nein"},null,{"$f":"IF(E6=\"\",\"\",Vokabel!A265&\" \"&VLOOKUP(A1,Daten!T:AC,5,0)& \" \" &VLOOKUP(A1,Daten!T:AC,3,0))","v":""}]
[null,null,{"$f":"IF(C2=\"Absolut\",Daten!AE35,IF(C2=\"SIH\",Daten!AF79,\"\"))","v":""},{"$f":"IF(C2=\"Kerastar\",\"für \"&Daten!C401,IF(C2=\"ADW TecnoStar\",\"für \"&Daten!C401,IF(C2=\"ICS\",\"für \"&Daten!C401,\"\")))","v":""},{"$f":"IF(VLOOKUP(A1,Daten!$T:$AA,8,0)=0,\"\",(VLOOKUP(A1,Daten!$T:$AA,8,0)))","v":""}]
[null,null,null,null,{"$f":"IF(VLOOKUP(A1,Daten!$T:$AB,9,0)=0,\"\",(VLOOKUP(A1,Daten!$T:$AB,9,0)))","v":""}]
["Nr.","Verkn.","Rabatt- fähig","Pos.",{"$f":"Vokabel!$A$270","v":"Artikelnummer"},{"$f":"Vokabel!$A$271","v":"Artikelbezeichnung"},{"$f":"Vokabel!$A$272&\" mm\"","v":"Baulänge mm"},{"$f":"Vokabel!$A$273","v":"Menge"}]
[0,{"$f":"$A$1&Verbindungsleitung!A6","v":"Nein0"},{"$f":"IF(E6=\"\",\"\",IF(E6=\"Sonder\",\"J\",VLOOKUP(E6,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B6,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B6,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D6=\"\",\"\",VLOOKUP($B6,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E6=\"\",\"\",VLOOKUP(E6,sanschie!B:E,4,0))","v":""},{"$f":"IF(E6=\"\",\"\",IF(VLOOKUP(E6,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E6,sanschie!B:J,9,0)))","v":""},1]
[1,{"$f":"$A$1&Verbindungsleitung!A7","v":"Nein1"},{"$f":"IF(E7=\"\",\"\",IF(E7=\"Sonder\",\"J\",VLOOKUP(E7,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B7,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B7,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D7=\"\",\"\",VLOOKUP($B7,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E7=\"\",\"\",VLOOKUP(E7,sanschie!A:E,5,0))","v":""},{"$f":"IF(E7=\"\",\"\",IF(VLOOKUP(E7,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E7,sanschie!A:J,10,0)))","v":""},null,null,null,{"$f":"Vokabel!$A$267","v":"Achtung:"}]
[2,{"$f":"$A$1&Verbindungsleitung!A8","v":"Nein2"},{"$f":"IF(E8=\"\",\"\",IF(E8=\"Sonder\",\"J\",VLOOKUP(E8,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B8,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B8,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D8=\"\",\"\",VLOOKUP($B8,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E8=\"\",\"\",VLOOKUP(E8,sanschie!A:E,5,0))","v":""},{"$f":"IF(E8=\"\",\"\",IF(VLOOKUP(E8,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E8,sanschie!A:J,10,0)))","v":""},null,null,null,{"$f":"Vokabel!$A$268","v":"Für die Verbindungsleitung werden"}]
[3,{"$f":"$A$1&Verbindungsleitung!A9","v":"Nein3"},{"$f":"IF(E9=\"\",\"\",IF(E9=\"Sonder\",\"J\",VLOOKUP(E9,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B9,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B9,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D9=\"\",\"\",VLOOKUP($B9,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E9=\"\",\"\",VLOOKUP(E9,sanschie!A:E,5,0))","v":""},{"$f":"IF(E9=\"\",\"\",IF(VLOOKUP(E9,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E9,sanschie!A:J,10,0)))","v":""},null,null,null,{"$f":"Vokabel!$A$269","v":"höchstens 14 Artikel übernommen !"}]
[4,{"$f":"$A$1&Verbindungsleitung!A10","v":"Nein4"},{"$f":"IF(E10=\"\",\"\",IF(E10=\"Sonder\",\"J\",VLOOKUP(E10,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B10,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B10,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D10=\"\",\"\",VLOOKUP($B10,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E10=\"\",\"\",VLOOKUP(E10,sanschie!A:E,5,0))","v":""},{"$f":"IF(E10=\"\",\"\",IF(VLOOKUP(E10,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E10,sanschie!A:J,10,0)))","v":""}]
[5,{"$f":"$A$1&Verbindungsleitung!A11","v":"Nein5"},{"$f":"IF(E11=\"\",\"\",IF(E11=\"Sonder\",\"J\",VLOOKUP(E11,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B11,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B11,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D11=\"\",\"\",VLOOKUP($B11,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E11=\"\",\"\",VLOOKUP(E11,sanschie!A:E,5,0))","v":""},{"$f":"IF(E11=\"\",\"\",IF(VLOOKUP(E11,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E11,sanschie!A:J,10,0)))","v":""}]
[6,{"$f":"$A$1&Verbindungsleitung!A12","v":"Nein6"},{"$f":"IF(E12=\"\",\"\",IF(E12=\"Sonder\",\"J\",VLOOKUP(E12,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B12,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B12,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D12=\"\",\"\",VLOOKUP($B12,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E12=\"\",\"\",VLOOKUP(E12,sanschie!A:E,5,0))","v":""},{"$f":"IF(E12=\"\",\"\",IF(VLOOKUP(E12,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E12,sanschie!A:J,10,0)))","v":""}]
[7,{"$f":"$A$1&Verbindungsleitung!A13","v":"Nein7"},{"$f":"IF(E13=\"\",\"\",IF(E13=\"Sonder\",\"J\",VLOOKUP(E13,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B13,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B13,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D13=\"\",\"\",VLOOKUP($B13,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E13=\"\",\"\",VLOOKUP(E13,sanschie!A:E,5,0))","v":""},{"$f":"IF(E13=\"\",\"\",IF(VLOOKUP(E13,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E13,sanschie!A:J,10,0)))","v":""}]
[8,{"$f":"$A$1&Verbindungsleitung!A14","v":"Nein8"},{"$f":"IF(E14=\"\",\"\",IF(E14=\"Sonder\",\"J\",VLOOKUP(E14,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B14,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B14,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D14=\"\",\"\",VLOOKUP($B14,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E14=\"\",\"\",VLOOKUP(E14,sanschie!A:E,5,0))","v":""},{"$f":"IF(E14=\"\",\"\",IF(VLOOKUP(E14,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E14,sanschie!A:J,10,0)))","v":""}]
[9,{"$f":"$A$1&Verbindungsleitung!A15","v":"Nein9"},{"$f":"IF(E15=\"\",\"\",IF(E15=\"Sonder\",\"J\",VLOOKUP(E15,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B15,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B15,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D15=\"\",\"\",VLOOKUP($B15,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E15=\"\",\"\",VLOOKUP(E15,sanschie!A:E,5,0))","v":""},{"$f":"IF(E15=\"\",\"\",IF(VLOOKUP(E15,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E15,sanschie!A:J,10,0)))","v":""}]
[10,{"$f":"$A$1&Verbindungsleitung!A16","v":"Nein10"},{"$f":"IF(E16=\"\",\"\",IF(E16=\"Sonder\",\"J\",VLOOKUP(E16,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B16,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B16,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D16=\"\",\"\",VLOOKUP($B16,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E16=\"\",\"\",VLOOKUP(E16,sanschie!A:E,5,0))","v":""},{"$f":"IF(E16=\"\",\"\",IF(VLOOKUP(E16,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E16,sanschie!A:J,10,0)))","v":""}]
[11,{"$f":"$A$1&Verbindungsleitung!A17","v":"Nein11"},{"$f":"IF(E17=\"\",\"\",IF(E17=\"Sonder\",\"J\",VLOOKUP(E17,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B17,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B17,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D17=\"\",\"\",VLOOKUP($B17,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E17=\"\",\"\",VLOOKUP(E17,sanschie!A:E,5,0))","v":""},{"$f":"IF(E17=\"\",\"\",IF(VLOOKUP(E17,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E17,sanschie!A:J,10,0)))","v":""}]
[12,{"$f":"$A$1&Verbindungsleitung!A18","v":"Nein12"},{"$f":"IF(E18=\"\",\"\",IF(E18=\"Sonder\",\"J\",VLOOKUP(E18,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B18,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B18,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D18=\"\",\"\",VLOOKUP($B18,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E18=\"\",\"\",VLOOKUP(E18,sanschie!A:E,5,0))","v":""},{"$f":"IF(E18=\"\",\"\",IF(VLOOKUP(E18,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E18,sanschie!A:J,10,0)))","v":""}]
[13,{"$f":"$A$1&Verbindungsleitung!A19","v":"Nein13"},{"$f":"IF(E19=\"\",\"\",IF(E19=\"Sonder\",\"J\",VLOOKUP(E19,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B19,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B19,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D19=\"\",\"\",VLOOKUP($B19,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E19=\"\",\"\",VLOOKUP(E19,sanschie!A:E,5,0))","v":""},{"$f":"IF(E19=\"\",\"\",IF(VLOOKUP(E19,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E19,sanschie!A:J,10,0)))","v":""}]
[14,{"$f":"$A$1&Verbindungsleitung!A20","v":"Nein14"},{"$f":"IF(E20=\"\",\"\",IF(E20=\"Sonder\",\"J\",VLOOKUP(E20,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B20,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B20,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D20=\"\",\"\",VLOOKUP($B20,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E20=\"\",\"\",VLOOKUP(E20,sanschie!A:E,5,0))","v":""},{"$f":"IF(E20=\"\",\"\",IF(VLOOKUP(E20,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E20,sanschie!A:J,10,0)))","v":""}]
[15,{"$f":"$A$1&Verbindungsleitung!A21","v":"Nein15"},{"$f":"IF(E21=\"\",\"\",IF(E21=\"Sonder\",\"J\",VLOOKUP(E21,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B21,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B21,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D21=\"\",\"\",VLOOKUP($B21,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E21=\"\",\"\",VLOOKUP(E21,sanschie!A:E,5,0))","v":""},{"$f":"IF(E21=\"\",\"\",IF(VLOOKUP(E21,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E21,sanschie!A:J,10,0)))","v":""}]
[16,{"$f":"$A$1&Verbindungsleitung!A22","v":"Nein16"},{"$f":"IF(E22=\"\",\"\",IF(E22=\"Sonder\",\"J\",VLOOKUP(E22,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B22,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B22,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D22=\"\",\"\",VLOOKUP($B22,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E22=\"\",\"\",VLOOKUP(E22,sanschie!A:E,5,0))","v":""},{"$f":"IF(E22=\"\",\"\",IF(VLOOKUP(E22,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E22,sanschie!A:J,10,0)))","v":""}]
[17,{"$f":"$A$1&Verbindungsleitung!A23","v":"Nein17"},{"$f":"IF(E23=\"\",\"\",IF(E23=\"Sonder\",\"J\",VLOOKUP(E23,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B23,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B23,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D23=\"\",\"\",VLOOKUP($B23,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E23=\"\",\"\",VLOOKUP(E23,sanschie!A:E,5,0))","v":""},{"$f":"IF(E23=\"\",\"\",IF(VLOOKUP(E23,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E23,sanschie!A:J,10,0)))","v":""}]
[18,{"$f":"$A$1&Verbindungsleitung!A24","v":"Nein18"},{"$f":"IF(E24=\"\",\"\",IF(E24=\"Sonder\",\"J\",VLOOKUP(E24,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B24,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B24,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D24=\"\",\"\",VLOOKUP($B24,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E24=\"\",\"\",VLOOKUP(E24,sanschie!A:E,5,0))","v":""},{"$f":"IF(E24=\"\",\"\",IF(VLOOKUP(E24,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E24,sanschie!A:J,10,0)))","v":""}]
[19,{"$f":"$A$1&Verbindungsleitung!A25","v":"Nein19"},{"$f":"IF(E25=\"\",\"\",IF(E25=\"Sonder\",\"J\",VLOOKUP(E25,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B25,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B25,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D25=\"\",\"\",VLOOKUP($B25,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E25=\"\",\"\",VLOOKUP(E25,sanschie!A:E,5,0))","v":""},{"$f":"IF(E25=\"\",\"\",IF(VLOOKUP(E25,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E25,sanschie!A:J,10,0)))","v":""}]
[20,{"$f":"$A$1&Verbindungsleitung!A26","v":"Nein20"},{"$f":"IF(E26=\"\",\"\",IF(E26=\"Sonder\",\"J\",VLOOKUP(E26,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B26,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B26,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D26=\"\",\"\",VLOOKUP($B26,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E26=\"\",\"\",VLOOKUP(E26,sanschie!A:E,5,0))","v":""},{"$f":"IF(E26=\"\",\"\",IF(VLOOKUP(E26,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E26,sanschie!A:J,10,0)))","v":""}]
[21,{"$f":"$A$1&Verbindungsleitung!A27","v":"Nein21"},{"$f":"IF(E27=\"\",\"\",IF(E27=\"Sonder\",\"J\",VLOOKUP(E27,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B27,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B27,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D27=\"\",\"\",VLOOKUP($B27,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E27=\"\",\"\",VLOOKUP(E27,sanschie!A:E,5,0))","v":""},{"$f":"IF(E27=\"\",\"\",IF(VLOOKUP(E27,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E27,sanschie!A:J,10,0)))","v":""}]
[22,{"$f":"$A$1&Verbindungsleitung!A28","v":"Nein22"},{"$f":"IF(E28=\"\",\"\",IF(E28=\"Sonder\",\"J\",VLOOKUP(E28,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B28,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B28,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D28=\"\",\"\",VLOOKUP($B28,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E28=\"\",\"\",VLOOKUP(E28,sanschie!A:E,5,0))","v":""},{"$f":"IF(E28=\"\",\"\",IF(VLOOKUP(E28,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E28,sanschie!A:J,10,0)))","v":""}]
[23,{"$f":"$A$1&Verbindungsleitung!A29","v":"Nein23"},{"$f":"IF(E29=\"\",\"\",IF(E29=\"Sonder\",\"J\",VLOOKUP(E29,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B29,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B29,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D29=\"\",\"\",VLOOKUP($B29,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E29=\"\",\"\",VLOOKUP(E29,sanschie!A:E,5,0))","v":""},{"$f":"IF(E29=\"\",\"\",IF(VLOOKUP(E29,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E29,sanschie!A:J,10,0)))","v":""}]
[24,{"$f":"$A$1&Verbindungsleitung!A30","v":"Nein24"},{"$f":"IF(E30=\"\",\"\",IF(E30=\"Sonder\",\"J\",VLOOKUP(E30,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B30,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B30,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D30=\"\",\"\",VLOOKUP($B30,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E30=\"\",\"\",VLOOKUP(E30,sanschie!A:E,5,0))","v":""},{"$f":"IF(E30=\"\",\"\",IF(VLOOKUP(E30,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E30,sanschie!A:J,10,0)))","v":""}]
[25,{"$f":"$A$1&Verbindungsleitung!A31","v":"Nein25"},{"$f":"IF(E31=\"\",\"\",IF(E31=\"Sonder\",\"J\",VLOOKUP(E31,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B31,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B31,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D31=\"\",\"\",VLOOKUP($B31,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E31=\"\",\"\",VLOOKUP(E31,sanschie!A:E,5,0))","v":""},{"$f":"IF(E31=\"\",\"\",IF(VLOOKUP(E31,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E31,sanschie!A:J,10,0)))","v":""}]
[26,{"$f":"$A$1&Verbindungsleitung!A32","v":"Nein26"},{"$f":"IF(E32=\"\",\"\",IF(E32=\"Sonder\",\"J\",VLOOKUP(E32,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B32,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B32,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D32=\"\",\"\",VLOOKUP($B32,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E32=\"\",\"\",VLOOKUP(E32,sanschie!A:E,5,0))","v":""},{"$f":"IF(E32=\"\",\"\",IF(VLOOKUP(E32,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E32,sanschie!A:J,10,0)))","v":""}]
[27,{"$f":"$A$1&Verbindungsleitung!A33","v":"Nein27"},{"$f":"IF(E33=\"\",\"\",IF(E33=\"Sonder\",\"J\",VLOOKUP(E33,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B33,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B33,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D33=\"\",\"\",VLOOKUP($B33,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E33=\"\",\"\",VLOOKUP(E33,sanschie!A:E,5,0))","v":""},{"$f":"IF(E33=\"\",\"\",IF(VLOOKUP(E33,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E33,sanschie!A:J,10,0)))","v":""}]
[28,{"$f":"$A$1&Verbindungsleitung!A34","v":"Nein28"},{"$f":"IF(E34=\"\",\"\",IF(E34=\"Sonder\",\"J\",VLOOKUP(E34,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B34,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B34,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D34=\"\",\"\",VLOOKUP($B34,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E34=\"\",\"\",VLOOKUP(E34,sanschie!A:E,5,0))","v":""},{"$f":"IF(E34=\"\",\"\",IF(VLOOKUP(E34,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E34,sanschie!A:J,10,0)))","v":""}]
[29,{"$f":"$A$1&Verbindungsleitung!A35","v":"Nein29"},{"$f":"IF(E35=\"\",\"\",IF(E35=\"Sonder\",\"J\",VLOOKUP(E35,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B35,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B35,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D35=\"\",\"\",VLOOKUP($B35,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E35=\"\",\"\",VLOOKUP(E35,sanschie!A:E,5,0))","v":""},{"$f":"IF(E35=\"\",\"\",IF(VLOOKUP(E35,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E35,sanschie!A:J,10,0)))","v":""}]
[30,{"$f":"$A$1&Verbindungsleitung!A36","v":"Nein30"},{"$f":"IF(E36=\"\",\"\",IF(E36=\"Sonder\",\"J\",VLOOKUP(E36,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B36,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B36,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D36=\"\",\"\",VLOOKUP($B36,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E36=\"\",\"\",VLOOKUP(E36,sanschie!A:E,5,0))","v":""},{"$f":"IF(E36=\"\",\"\",IF(VLOOKUP(E36,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E36,sanschie!A:J,10,0)))","v":""}]
[31,{"$f":"$A$1&Verbindungsleitung!A37","v":"Nein31"},{"$f":"IF(E37=\"\",\"\",IF(E37=\"Sonder\",\"J\",VLOOKUP(E37,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B37,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B37,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D37=\"\",\"\",VLOOKUP($B37,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E37=\"\",\"\",VLOOKUP(E37,sanschie!A:E,5,0))","v":""},{"$f":"IF(E37=\"\",\"\",IF(VLOOKUP(E37,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E37,sanschie!A:J,10,0)))","v":""}]
[32,{"$f":"$A$1&Verbindungsleitung!A38","v":"Nein32"},{"$f":"IF(E38=\"\",\"\",IF(E38=\"Sonder\",\"J\",VLOOKUP(E38,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B38,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B38,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D38=\"\",\"\",VLOOKUP($B38,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E38=\"\",\"\",VLOOKUP(E38,sanschie!A:E,5,0))","v":""},{"$f":"IF(E38=\"\",\"\",IF(VLOOKUP(E38,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E38,sanschie!A:J,10,0)))","v":""}]
[33,{"$f":"$A$1&Verbindungsleitung!A39","v":"Nein33"},{"$f":"IF(E39=\"\",\"\",IF(E39=\"Sonder\",\"J\",VLOOKUP(E39,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B39,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B39,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D39=\"\",\"\",VLOOKUP($B39,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E39=\"\",\"\",VLOOKUP(E39,sanschie!A:E,5,0))","v":""},{"$f":"IF(E39=\"\",\"\",IF(VLOOKUP(E39,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E39,sanschie!A:J,10,0)))","v":""}]
[34,{"$f":"$A$1&Verbindungsleitung!A40","v":"Nein34"},{"$f":"IF(E40=\"\",\"\",IF(E40=\"Sonder\",\"J\",VLOOKUP(E40,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B40,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B40,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D40=\"\",\"\",VLOOKUP($B40,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E40=\"\",\"\",VLOOKUP(E40,sanschie!A:E,5,0))","v":""},{"$f":"IF(E40=\"\",\"\",IF(VLOOKUP(E40,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E40,sanschie!A:J,10,0)))","v":""}]
[35,{"$f":"$A$1&Verbindungsleitung!A41","v":"Nein35"},{"$f":"IF(E41=\"\",\"\",IF(E41=\"Sonder\",\"J\",VLOOKUP(E41,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B41,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B41,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D41=\"\",\"\",VLOOKUP($B41,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E41=\"\",\"\",VLOOKUP(E41,sanschie!A:E,5,0))","v":""},{"$f":"IF(E41=\"\",\"\",IF(VLOOKUP(E41,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E41,sanschie!A:J,10,0)))","v":""}]
[36,{"$f":"$A$1&Verbindungsleitung!A42","v":"Nein36"},{"$f":"IF(E42=\"\",\"\",IF(E42=\"Sonder\",\"J\",VLOOKUP(E42,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B42,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B42,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D42=\"\",\"\",VLOOKUP($B42,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E42=\"\",\"\",VLOOKUP(E42,sanschie!A:E,5,0))","v":""},{"$f":"IF(E42=\"\",\"\",IF(VLOOKUP(E42,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E42,sanschie!A:J,10,0)))","v":""}]
[37,{"$f":"$A$1&Verbindungsleitung!A43","v":"Nein37"},{"$f":"IF(E43=\"\",\"\",IF(E43=\"Sonder\",\"J\",VLOOKUP(E43,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B43,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B43,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D43=\"\",\"\",VLOOKUP($B43,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E43=\"\",\"\",VLOOKUP(E43,sanschie!A:E,5,0))","v":""},{"$f":"IF(E43=\"\",\"\",IF(VLOOKUP(E43,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E43,sanschie!A:J,10,0)))","v":""}]
[38,{"$f":"$A$1&Verbindungsleitung!A44","v":"Nein38"},{"$f":"IF(E44=\"\",\"\",IF(E44=\"Sonder\",\"J\",VLOOKUP(E44,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B44,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B44,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D44=\"\",\"\",VLOOKUP($B44,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E44=\"\",\"\",VLOOKUP(E44,sanschie!A:E,5,0))","v":""},{"$f":"IF(E44=\"\",\"\",IF(VLOOKUP(E44,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E44,sanschie!A:J,10,0)))","v":""}]
[39,{"$f":"$A$1&Verbindungsleitung!A45","v":"Nein39"},{"$f":"IF(E45=\"\",\"\",IF(E45=\"Sonder\",\"J\",VLOOKUP(E45,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B45,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B45,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D45=\"\",\"\",VLOOKUP($B45,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E45=\"\",\"\",VLOOKUP(E45,sanschie!A:E,5,0))","v":""},{"$f":"IF(E45=\"\",\"\",IF(VLOOKUP(E45,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E45,sanschie!A:J,10,0)))","v":""}]
[40,{"$f":"$A$1&Verbindungsleitung!A46","v":"Nein40"},{"$f":"IF(E46=\"\",\"\",IF(E46=\"Sonder\",\"J\",VLOOKUP(E46,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B46,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B46,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D46=\"\",\"\",VLOOKUP($B46,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E46=\"\",\"\",VLOOKUP(E46,sanschie!A:E,5,0))","v":""},{"$f":"IF(E46=\"\",\"\",IF(VLOOKUP(E46,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E46,sanschie!A:J,10,0)))","v":""}]
[41,{"$f":"$A$1&Verbindungsleitung!A47","v":"Nein41"},{"$f":"IF(E47=\"\",\"\",IF(E47=\"Sonder\",\"J\",VLOOKUP(E47,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B47,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B47,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D47=\"\",\"\",VLOOKUP($B47,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E47=\"\",\"\",VLOOKUP(E47,sanschie!A:E,5,0))","v":""},{"$f":"IF(E47=\"\",\"\",IF(VLOOKUP(E47,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E47,sanschie!A:J,10,0)))","v":""}]
[42,{"$f":"$A$1&Verbindungsleitung!A48","v":"Nein42"},{"$f":"IF(E48=\"\",\"\",IF(E48=\"Sonder\",\"J\",VLOOKUP(E48,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B48,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B48,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D48=\"\",\"\",VLOOKUP($B48,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E48=\"\",\"\",VLOOKUP(E48,sanschie!A:E,5,0))","v":""},{"$f":"IF(E48=\"\",\"\",IF(VLOOKUP(E48,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E48,sanschie!A:J,10,0)))","v":""}]
[43,{"$f":"$A$1&Verbindungsleitung!A49","v":"Nein43"},{"$f":"IF(E49=\"\",\"\",IF(E49=\"Sonder\",\"J\",VLOOKUP(E49,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B49,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B49,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D49=\"\",\"\",VLOOKUP($B49,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E49=\"\",\"\",VLOOKUP(E49,sanschie!A:E,5,0))","v":""},{"$f":"IF(E49=\"\",\"\",IF(VLOOKUP(E49,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E49,sanschie!A:J,10,0)))","v":""}]
[44,{"$f":"$A$1&Verbindungsleitung!A50","v":"Nein44"},{"$f":"IF(E50=\"\",\"\",IF(E50=\"Sonder\",\"J\",VLOOKUP(E50,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B50,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B50,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D50=\"\",\"\",VLOOKUP($B50,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E50=\"\",\"\",VLOOKUP(E50,sanschie!A:E,5,0))","v":""},{"$f":"IF(E50=\"\",\"\",IF(VLOOKUP(E50,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E50,sanschie!A:J,10,0)))","v":""}]
[45,{"$f":"$A$1&Verbindungsleitung!A51","v":"Nein45"},{"$f":"IF(E51=\"\",\"\",IF(E51=\"Sonder\",\"J\",VLOOKUP(E51,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B51,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B51,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D51=\"\",\"\",VLOOKUP($B51,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E51=\"\",\"\",VLOOKUP(E51,sanschie!A:E,5,0))","v":""},{"$f":"IF(E51=\"\",\"\",IF(VLOOKUP(E51,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E51,sanschie!A:J,10,0)))","v":""}]
[46,{"$f":"$A$1&Verbindungsleitung!A52","v":"Nein46"},{"$f":"IF(E52=\"\",\"\",IF(E52=\"Sonder\",\"J\",VLOOKUP(E52,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B52,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B52,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D52=\"\",\"\",VLOOKUP($B52,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E52=\"\",\"\",VLOOKUP(E52,sanschie!A:E,5,0))","v":""},{"$f":"IF(E52=\"\",\"\",IF(VLOOKUP(E52,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E52,sanschie!A:J,10,0)))","v":""}]
[47,{"$f":"$A$1&Verbindungsleitung!A53","v":"Nein47"},{"$f":"IF(E53=\"\",\"\",IF(E53=\"Sonder\",\"J\",VLOOKUP(E53,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B53,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B53,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D53=\"\",\"\",VLOOKUP($B53,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E53=\"\",\"\",VLOOKUP(E53,sanschie!A:E,5,0))","v":""},{"$f":"IF(E53=\"\",\"\",IF(VLOOKUP(E53,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E53,sanschie!A:J,10,0)))","v":""}]
[48,{"$f":"$A$1&Verbindungsleitung!A54","v":"Nein48"},{"$f":"IF(E54=\"\",\"\",IF(E54=\"Sonder\",\"J\",VLOOKUP(E54,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B54,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B54,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D54=\"\",\"\",VLOOKUP($B54,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E54=\"\",\"\",VLOOKUP(E54,sanschie!A:E,5,0))","v":""},{"$f":"IF(E54=\"\",\"\",IF(VLOOKUP(E54,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E54,sanschie!A:J,10,0)))","v":""}]
[49,{"$f":"$A$1&Verbindungsleitung!A55","v":"Nein49"},{"$f":"IF(E55=\"\",\"\",IF(E55=\"Sonder\",\"J\",VLOOKUP(E55,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B55,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B55,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D55=\"\",\"\",VLOOKUP($B55,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E55=\"\",\"\",VLOOKUP(E55,sanschie!A:E,5,0))","v":""},{"$f":"IF(E55=\"\",\"\",IF(VLOOKUP(E55,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E55,sanschie!A:J,10,0)))","v":""}]
[50,{"$f":"$A$1&Verbindungsleitung!A56","v":"Nein50"},{"$f":"IF(E56=\"\",\"\",IF(E56=\"Sonder\",\"J\",VLOOKUP(E56,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B56,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B56,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D56=\"\",\"\",VLOOKUP($B56,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E56=\"\",\"\",VLOOKUP(E56,sanschie!A:E,5,0))","v":""},{"$f":"IF(E56=\"\",\"\",IF(VLOOKUP(E56,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E56,sanschie!A:J,10,0)))","v":""}]
[51,{"$f":"$A$1&Verbindungsleitung!A57","v":"Nein51"},{"$f":"IF(E57=\"\",\"\",IF(E57=\"Sonder\",\"J\",VLOOKUP(E57,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B57,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B57,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D57=\"\",\"\",VLOOKUP($B57,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E57=\"\",\"\",VLOOKUP(E57,sanschie!A:E,5,0))","v":""},{"$f":"IF(E57=\"\",\"\",IF(VLOOKUP(E57,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E57,sanschie!A:J,10,0)))","v":""}]
[52,{"$f":"$A$1&Verbindungsleitung!A58","v":"Nein52"},{"$f":"IF(E58=\"\",\"\",IF(E58=\"Sonder\",\"J\",VLOOKUP(E58,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B58,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B58,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D58=\"\",\"\",VLOOKUP($B58,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E58=\"\",\"\",VLOOKUP(E58,sanschie!A:E,5,0))","v":""},{"$f":"IF(E58=\"\",\"\",IF(VLOOKUP(E58,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E58,sanschie!A:J,10,0)))","v":""}]
[53,{"$f":"$A$1&Verbindungsleitung!A59","v":"Nein53"},{"$f":"IF(E59=\"\",\"\",IF(E59=\"Sonder\",\"J\",VLOOKUP(E59,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B59,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B59,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D59=\"\",\"\",VLOOKUP($B59,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E59=\"\",\"\",VLOOKUP(E59,sanschie!A:E,5,0))","v":""},{"$f":"IF(E59=\"\",\"\",IF(VLOOKUP(E59,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E59,sanschie!A:J,10,0)))","v":""}]
[54,{"$f":"$A$1&Verbindungsleitung!A60","v":"Nein54"},{"$f":"IF(E60=\"\",\"\",IF(E60=\"Sonder\",\"J\",VLOOKUP(E60,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B60,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B60,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D60=\"\",\"\",VLOOKUP($B60,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E60=\"\",\"\",VLOOKUP(E60,sanschie!A:E,5,0))","v":""},{"$f":"IF(E60=\"\",\"\",IF(VLOOKUP(E60,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E60,sanschie!A:J,10,0)))","v":""}]
[55,{"$f":"$A$1&Verbindungsleitung!A61","v":"Nein55"},{"$f":"IF(E61=\"\",\"\",IF(E61=\"Sonder\",\"J\",VLOOKUP(E61,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B61,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B61,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D61=\"\",\"\",VLOOKUP($B61,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E61=\"\",\"\",VLOOKUP(E61,sanschie!A:E,5,0))","v":""},{"$f":"IF(E61=\"\",\"\",IF(VLOOKUP(E61,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E61,sanschie!A:J,10,0)))","v":""}]
[56,{"$f":"$A$1&Verbindungsleitung!A62","v":"Nein56"},{"$f":"IF(E62=\"\",\"\",IF(E62=\"Sonder\",\"J\",VLOOKUP(E62,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B62,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B62,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D62=\"\",\"\",VLOOKUP($B62,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E62=\"\",\"\",VLOOKUP(E62,sanschie!A:E,5,0))","v":""},{"$f":"IF(E62=\"\",\"\",IF(VLOOKUP(E62,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E62,sanschie!A:J,10,0)))","v":""}]
[57,{"$f":"$A$1&Verbindungsleitung!A63","v":"Nein57"},{"$f":"IF(E63=\"\",\"\",IF(E63=\"Sonder\",\"J\",VLOOKUP(E63,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B63,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B63,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D63=\"\",\"\",VLOOKUP($B63,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E63=\"\",\"\",VLOOKUP(E63,sanschie!A:E,5,0))","v":""},{"$f":"IF(E63=\"\",\"\",IF(VLOOKUP(E63,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E63,sanschie!A:J,10,0)))","v":""}]
[58,{"$f":"$A$1&Verbindungsleitung!A64","v":"Nein58"},{"$f":"IF(E64=\"\",\"\",IF(E64=\"Sonder\",\"J\",VLOOKUP(E64,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B64,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B64,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D64=\"\",\"\",VLOOKUP($B64,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E64=\"\",\"\",VLOOKUP(E64,sanschie!A:E,5,0))","v":""},{"$f":"IF(E64=\"\",\"\",IF(VLOOKUP(E64,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E64,sanschie!A:J,10,0)))","v":""}]
[59,{"$f":"$A$1&Verbindungsleitung!A65","v":"Nein59"},{"$f":"IF(E65=\"\",\"\",IF(E65=\"Sonder\",\"J\",VLOOKUP(E65,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B65,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B65,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D65=\"\",\"\",VLOOKUP($B65,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E65=\"\",\"\",VLOOKUP(E65,sanschie!A:E,5,0))","v":""},{"$f":"IF(E65=\"\",\"\",IF(VLOOKUP(E65,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E65,sanschie!A:J,10,0)))","v":""}]
[60,{"$f":"$A$1&Verbindungsleitung!A66","v":"Nein60"},{"$f":"IF(E66=\"\",\"\",IF(E66=\"Sonder\",\"J\",VLOOKUP(E66,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B66,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B66,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D66=\"\",\"\",VLOOKUP($B66,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E66=\"\",\"\",VLOOKUP(E66,sanschie!A:E,5,0))","v":""},{"$f":"IF(E66=\"\",\"\",IF(VLOOKUP(E66,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E66,sanschie!A:J,10,0)))","v":""}]
[61,{"$f":"$A$1&Verbindungsleitung!A67","v":"Nein61"},{"$f":"IF(E67=\"\",\"\",IF(E67=\"Sonder\",\"J\",VLOOKUP(E67,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B67,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B67,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D67=\"\",\"\",VLOOKUP($B67,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E67=\"\",\"\",VLOOKUP(E67,sanschie!A:E,5,0))","v":""},{"$f":"IF(E67=\"\",\"\",IF(VLOOKUP(E67,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E67,sanschie!A:J,10,0)))","v":""}]
[62,{"$f":"$A$1&Verbindungsleitung!A68","v":"Nein62"},{"$f":"IF(E68=\"\",\"\",IF(E68=\"Sonder\",\"J\",VLOOKUP(E68,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B68,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B68,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D68=\"\",\"\",VLOOKUP($B68,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E68=\"\",\"\",VLOOKUP(E68,sanschie!A:E,5,0))","v":""},{"$f":"IF(E68=\"\",\"\",IF(VLOOKUP(E68,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E68,sanschie!A:J,10,0)))","v":""}]
[63,{"$f":"$A$1&Verbindungsleitung!A69","v":"Nein63"},{"$f":"IF(E69=\"\",\"\",IF(E69=\"Sonder\",\"J\",VLOOKUP(E69,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B69,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B69,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D69=\"\",\"\",VLOOKUP($B69,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E69=\"\",\"\",VLOOKUP(E69,sanschie!A:E,5,0))","v":""},{"$f":"IF(E69=\"\",\"\",IF(VLOOKUP(E69,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E69,sanschie!A:J,10,0)))","v":""}]
[64,{"$f":"$A$1&Verbindungsleitung!A70","v":"Nein64"},{"$f":"IF(E70=\"\",\"\",IF(E70=\"Sonder\",\"J\",VLOOKUP(E70,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B70,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B70,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D70=\"\",\"\",VLOOKUP($B70,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E70=\"\",\"\",VLOOKUP(E70,sanschie!A:E,5,0))","v":""},{"$f":"IF(E70=\"\",\"\",IF(VLOOKUP(E70,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E70,sanschie!A:J,10,0)))","v":""}]
[65,{"$f":"$A$1&Verbindungsleitung!A71","v":"Nein65"},{"$f":"IF(E71=\"\",\"\",IF(E71=\"Sonder\",\"J\",VLOOKUP(E71,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B71,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B71,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D71=\"\",\"\",VLOOKUP($B71,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E71=\"\",\"\",VLOOKUP(E71,sanschie!A:E,5,0))","v":""},{"$f":"IF(E71=\"\",\"\",IF(VLOOKUP(E71,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E71,sanschie!A:J,10,0)))","v":""}]
[66,{"$f":"$A$1&Verbindungsleitung!A72","v":"Nein66"},{"$f":"IF(E72=\"\",\"\",IF(E72=\"Sonder\",\"J\",VLOOKUP(E72,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B72,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B72,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D72=\"\",\"\",VLOOKUP($B72,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E72=\"\",\"\",VLOOKUP(E72,sanschie!A:E,5,0))","v":""},{"$f":"IF(E72=\"\",\"\",IF(VLOOKUP(E72,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E72,sanschie!A:J,10,0)))","v":""}]
[67,{"$f":"$A$1&Verbindungsleitung!A73","v":"Nein67"},{"$f":"IF(E73=\"\",\"\",IF(E73=\"Sonder\",\"J\",VLOOKUP(E73,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B73,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B73,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D73=\"\",\"\",VLOOKUP($B73,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E73=\"\",\"\",VLOOKUP(E73,sanschie!A:E,5,0))","v":""},{"$f":"IF(E73=\"\",\"\",IF(VLOOKUP(E73,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E73,sanschie!A:J,10,0)))","v":""}]
[68,{"$f":"$A$1&Verbindungsleitung!A74","v":"Nein68"},{"$f":"IF(E74=\"\",\"\",IF(E74=\"Sonder\",\"J\",VLOOKUP(E74,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B74,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B74,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D74=\"\",\"\",VLOOKUP($B74,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E74=\"\",\"\",VLOOKUP(E74,sanschie!A:E,5,0))","v":""},{"$f":"IF(E74=\"\",\"\",IF(VLOOKUP(E74,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E74,sanschie!A:J,10,0)))","v":""}]
[69,{"$f":"$A$1&Verbindungsleitung!A75","v":"Nein69"},{"$f":"IF(E75=\"\",\"\",IF(E75=\"Sonder\",\"J\",VLOOKUP(E75,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B75,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B75,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D75=\"\",\"\",VLOOKUP($B75,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E75=\"\",\"\",VLOOKUP(E75,sanschie!A:E,5,0))","v":""},{"$f":"IF(E75=\"\",\"\",IF(VLOOKUP(E75,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E75,sanschie!A:J,10,0)))","v":""}]
[70,{"$f":"$A$1&Verbindungsleitung!A76","v":"Nein70"},{"$f":"IF(E76=\"\",\"\",IF(E76=\"Sonder\",\"J\",VLOOKUP(E76,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B76,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B76,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D76=\"\",\"\",VLOOKUP($B76,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E76=\"\",\"\",VLOOKUP(E76,sanschie!A:E,5,0))","v":""},{"$f":"IF(E76=\"\",\"\",IF(VLOOKUP(E76,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E76,sanschie!A:J,10,0)))","v":""}]
[71,{"$f":"$A$1&Verbindungsleitung!A77","v":"Nein71"},{"$f":"IF(E77=\"\",\"\",IF(E77=\"Sonder\",\"J\",VLOOKUP(E77,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B77,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B77,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D77=\"\",\"\",VLOOKUP($B77,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E77=\"\",\"\",VLOOKUP(E77,sanschie!A:E,5,0))","v":""},{"$f":"IF(E77=\"\",\"\",IF(VLOOKUP(E77,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E77,sanschie!A:J,10,0)))","v":""}]
[72,{"$f":"$A$1&Verbindungsleitung!A78","v":"Nein72"},{"$f":"IF(E78=\"\",\"\",IF(E78=\"Sonder\",\"J\",VLOOKUP(E78,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B78,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B78,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D78=\"\",\"\",VLOOKUP($B78,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E78=\"\",\"\",VLOOKUP(E78,sanschie!A:E,5,0))","v":""},{"$f":"IF(E78=\"\",\"\",IF(VLOOKUP(E78,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E78,sanschie!A:J,10,0)))","v":""}]
[73,{"$f":"$A$1&Verbindungsleitung!A79","v":"Nein73"},{"$f":"IF(E79=\"\",\"\",IF(E79=\"Sonder\",\"J\",VLOOKUP(E79,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B79,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B79,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D79=\"\",\"\",VLOOKUP($B79,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E79=\"\",\"\",VLOOKUP(E79,sanschie!A:E,5,0))","v":""},{"$f":"IF(E79=\"\",\"\",IF(VLOOKUP(E79,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E79,sanschie!A:J,10,0)))","v":""}]
[74,{"$f":"$A$1&Verbindungsleitung!A80","v":"Nein74"},{"$f":"IF(E80=\"\",\"\",IF(E80=\"Sonder\",\"J\",VLOOKUP(E80,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B80,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B80,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D80=\"\",\"\",VLOOKUP($B80,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E80=\"\",\"\",VLOOKUP(E80,sanschie!A:E,5,0))","v":""},{"$f":"IF(E80=\"\",\"\",IF(VLOOKUP(E80,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E80,sanschie!A:J,10,0)))","v":""}]
[75,{"$f":"$A$1&Verbindungsleitung!A81","v":"Nein75"},{"$f":"IF(E81=\"\",\"\",IF(E81=\"Sonder\",\"J\",VLOOKUP(E81,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B81,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B81,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D81=\"\",\"\",VLOOKUP($B81,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E81=\"\",\"\",VLOOKUP(E81,sanschie!A:E,5,0))","v":""},{"$f":"IF(E81=\"\",\"\",IF(VLOOKUP(E81,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E81,sanschie!A:J,10,0)))","v":""}]
[76,{"$f":"$A$1&Verbindungsleitung!A82","v":"Nein76"},{"$f":"IF(E82=\"\",\"\",IF(E82=\"Sonder\",\"J\",VLOOKUP(E82,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B82,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B82,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D82=\"\",\"\",VLOOKUP($B82,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E82=\"\",\"\",VLOOKUP(E82,sanschie!A:E,5,0))","v":""},{"$f":"IF(E82=\"\",\"\",IF(VLOOKUP(E82,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E82,sanschie!A:J,10,0)))","v":""}]
[77,{"$f":"$A$1&Verbindungsleitung!A83","v":"Nein77"},{"$f":"IF(E83=\"\",\"\",IF(E83=\"Sonder\",\"J\",VLOOKUP(E83,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B83,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B83,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D83=\"\",\"\",VLOOKUP($B83,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E83=\"\",\"\",VLOOKUP(E83,sanschie!A:E,5,0))","v":""},{"$f":"IF(E83=\"\",\"\",IF(VLOOKUP(E83,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E83,sanschie!A:J,10,0)))","v":""}]
[78,{"$f":"$A$1&Verbindungsleitung!A84","v":"Nein78"},{"$f":"IF(E84=\"\",\"\",IF(E84=\"Sonder\",\"J\",VLOOKUP(E84,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B84,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B84,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D84=\"\",\"\",VLOOKUP($B84,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E84=\"\",\"\",VLOOKUP(E84,sanschie!A:E,5,0))","v":""},{"$f":"IF(E84=\"\",\"\",IF(VLOOKUP(E84,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E84,sanschie!A:J,10,0)))","v":""}]
[79,{"$f":"$A$1&Verbindungsleitung!A85","v":"Nein79"},{"$f":"IF(E85=\"\",\"\",IF(E85=\"Sonder\",\"J\",VLOOKUP(E85,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B85,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B85,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D85=\"\",\"\",VLOOKUP($B85,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E85=\"\",\"\",VLOOKUP(E85,sanschie!A:E,5,0))","v":""},{"$f":"IF(E85=\"\",\"\",IF(VLOOKUP(E85,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E85,sanschie!A:J,10,0)))","v":""}]
[80,{"$f":"$A$1&Verbindungsleitung!A86","v":"Nein80"},{"$f":"IF(E86=\"\",\"\",IF(E86=\"Sonder\",\"J\",VLOOKUP(E86,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B86,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B86,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D86=\"\",\"\",VLOOKUP($B86,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E86=\"\",\"\",VLOOKUP(E86,sanschie!A:E,5,0))","v":""},{"$f":"IF(E86=\"\",\"\",IF(VLOOKUP(E86,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E86,sanschie!A:J,10,0)))","v":""}]
[81,{"$f":"$A$1&Verbindungsleitung!A87","v":"Nein81"},{"$f":"IF(E87=\"\",\"\",IF(E87=\"Sonder\",\"J\",VLOOKUP(E87,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B87,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B87,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D87=\"\",\"\",VLOOKUP($B87,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E87=\"\",\"\",VLOOKUP(E87,sanschie!A:E,5,0))","v":""},{"$f":"IF(E87=\"\",\"\",IF(VLOOKUP(E87,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E87,sanschie!A:J,10,0)))","v":""}]
[82,{"$f":"$A$1&Verbindungsleitung!A88","v":"Nein82"},{"$f":"IF(E88=\"\",\"\",IF(E88=\"Sonder\",\"J\",VLOOKUP(E88,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B88,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B88,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D88=\"\",\"\",VLOOKUP($B88,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E88=\"\",\"\",VLOOKUP(E88,sanschie!A:E,5,0))","v":""},{"$f":"IF(E88=\"\",\"\",IF(VLOOKUP(E88,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E88,sanschie!A:J,10,0)))","v":""}]
[83,{"$f":"$A$1&Verbindungsleitung!A89","v":"Nein83"},{"$f":"IF(E89=\"\",\"\",IF(E89=\"Sonder\",\"J\",VLOOKUP(E89,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B89,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B89,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D89=\"\",\"\",VLOOKUP($B89,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E89=\"\",\"\",VLOOKUP(E89,sanschie!A:E,5,0))","v":""},{"$f":"IF(E89=\"\",\"\",IF(VLOOKUP(E89,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E89,sanschie!A:J,10,0)))","v":""}]
[84,{"$f":"$A$1&Verbindungsleitung!A90","v":"Nein84"},{"$f":"IF(E90=\"\",\"\",IF(E90=\"Sonder\",\"J\",VLOOKUP(E90,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B90,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B90,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D90=\"\",\"\",VLOOKUP($B90,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E90=\"\",\"\",VLOOKUP(E90,sanschie!A:E,5,0))","v":""},{"$f":"IF(E90=\"\",\"\",IF(VLOOKUP(E90,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E90,sanschie!A:J,10,0)))","v":""}]
[85,{"$f":"$A$1&Verbindungsleitung!A91","v":"Nein85"},{"$f":"IF(E91=\"\",\"\",IF(E91=\"Sonder\",\"J\",VLOOKUP(E91,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B91,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B91,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D91=\"\",\"\",VLOOKUP($B91,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E91=\"\",\"\",VLOOKUP(E91,sanschie!A:E,5,0))","v":""},{"$f":"IF(E91=\"\",\"\",IF(VLOOKUP(E91,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E91,sanschie!A:J,10,0)))","v":""}]
[86,{"$f":"$A$1&Verbindungsleitung!A92","v":"Nein86"},{"$f":"IF(E92=\"\",\"\",IF(E92=\"Sonder\",\"J\",VLOOKUP(E92,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B92,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B92,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D92=\"\",\"\",VLOOKUP($B92,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E92=\"\",\"\",VLOOKUP(E92,sanschie!A:E,5,0))","v":""},{"$f":"IF(E92=\"\",\"\",IF(VLOOKUP(E92,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E92,sanschie!A:J,10,0)))","v":""}]
[87,{"$f":"$A$1&Verbindungsleitung!A93","v":"Nein87"},{"$f":"IF(E93=\"\",\"\",IF(E93=\"Sonder\",\"J\",VLOOKUP(E93,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B93,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B93,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D93=\"\",\"\",VLOOKUP($B93,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E93=\"\",\"\",VLOOKUP(E93,sanschie!A:E,5,0))","v":""},{"$f":"IF(E93=\"\",\"\",IF(VLOOKUP(E93,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E93,sanschie!A:J,10,0)))","v":""}]
[88,{"$f":"$A$1&Verbindungsleitung!A94","v":"Nein88"},{"$f":"IF(E94=\"\",\"\",IF(E94=\"Sonder\",\"J\",VLOOKUP(E94,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B94,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B94,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D94=\"\",\"\",VLOOKUP($B94,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E94=\"\",\"\",VLOOKUP(E94,sanschie!A:E,5,0))","v":""},{"$f":"IF(E94=\"\",\"\",IF(VLOOKUP(E94,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E94,sanschie!A:J,10,0)))","v":""}]
[89,{"$f":"$A$1&Verbindungsleitung!A95","v":"Nein89"},{"$f":"IF(E95=\"\",\"\",IF(E95=\"Sonder\",\"J\",VLOOKUP(E95,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B95,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B95,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D95=\"\",\"\",VLOOKUP($B95,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E95=\"\",\"\",VLOOKUP(E95,sanschie!A:E,5,0))","v":""},{"$f":"IF(E95=\"\",\"\",IF(VLOOKUP(E95,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E95,sanschie!A:J,10,0)))","v":""}]
[90,{"$f":"$A$1&Verbindungsleitung!A96","v":"Nein90"},{"$f":"IF(E96=\"\",\"\",IF(E96=\"Sonder\",\"J\",VLOOKUP(E96,sanschie!A:K,11,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B96,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B96,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D96=\"\",\"\",VLOOKUP($B96,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E96=\"\",\"\",VLOOKUP(E96,sanschie!A:E,5,0))","v":""},{"$f":"IF(E96=\"\",\"\",IF(VLOOKUP(E96,sanschie!A:J,10,0)=0,\"\",VLOOKUP(E96,sanschie!A:J,10,0)))","v":""}]

{"sheet":"PRIMA PLUS","index":15,"n_rows":62,"n_cols":16,"rows_kept":62,"cut":false,"hidden":true,"merged":[[13,12,15,14],[32,5,32,9],[2,5,2,9],[3,5,3,9]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$139,Daten!$T:$U,2,0)&\" \"&VLOOKUP(Daten!$U$139,Daten!$T:$V,3,0)","v":"PRIMA PLUS 180"}]
[null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$139,Daten!$T:$AL,19,0)","v":"Typ  PPL 180 / 0,6"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$311","v":"Lichter Ø mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$96","v":"Betriebsweise"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$75","v":"Brennstoff"},null,null,null,null,null,null,{"$f":"Vokabel!$A$89","v":"Anpassung der Anlagenhöhe"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$40","v":"Anlagenhöhe in m"},null,null,null,10,null,null,{"$f":"Vokabel!$A$90","v":"tatsächliche Anlagenhöhe "},null,null,{"$f":"VLOOKUP(P2,Sortimente!G:P,10,0)","v":10.17}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$97","v":"Differenz +/- "},null,null,{"$f":"P11-J11","v":0.16999999999999993}]
[null,null,null,null,null,{"$f":"Vokabel!$A$78","v":"Rauchrohranschluss RA"},null,null,null,null,null,null,{"$f":"Vokabel!$A$366","v":"(10 cm für Mündung vorsehen!)"}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$101","v":"Anpassung durch Eingabe kürzerer Rohrelemente:"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$66","v":"Putzanschluss"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$100","v":"Putztür"},null,null,null,null,null,null,null,{"$f":"Vokabel!$A$335","v":"Rohr 450 mm"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$334","v":"Rohr 200 mm"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$83","v":"Regenhaube"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$84","v":"Mündungslösung"}]
[]
[]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$88","v":"Verbindungsleitung"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[1]

{"sheet":"Absolut","index":16,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":true,"merged":[[3,5,3,13],[2,5,2,12]]}
[]
[]
[null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$35,Daten!$T:$AL,19,0)","v":"Typ  -  ABSOLUT  Ø  18"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$39","v":"Lichter Ø cm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$40","v":"Anlagenhöhe in m"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$41","v":"Fussausführung"},null,null,null,{"$f":"Vokabel!$A$62","v":"Sockel"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$42","v":"Rauchrohranschluss"},{"$f":"Vokabel!$A$56","v":"(bei kombiniert kleiner Ø)"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$43","v":"Handy-Abdeckplatte"}]
[]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$44","v":"Zubehör"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$45","v":"Anschlussvariante"},null,null,{"$f":"Vokabel!$A$431","v":"2.kl.Zug"},null,{"$f":"Vokabel!$A$430","v":"1.Zug"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$46","v":"Zugregler "},null,null,{"$f":"Vokabel!$A$431","v":"2.kl.Zug"},null,{"$f":"Vokabel!$A$430","v":"1.Zug"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$55","v":"(mit Expl. Kl.)    "}]
[null,null,null,null,null,{"$f":"Vokabel!$A$47","v":"zusätzlicher Rauchrohranschluss "}]
[null,null,null,null,null,{"$f":"Vokabel!$A$61","v":"(bei kombiniert grosser Ø)"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$48","v":"LAS Zuluft-Adapter "},null,{"$f":"Vokabel!$A$57","v":"(für Festbrennstoffzug)"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$49","v":"Revisionstür "},null,{"$f":"Vokabel!$A$58","v":"(für Thermo-Luftzug)"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$50","v":"obere Putztür "},null,{"$f":"Vokabel!$A$59","v":"(bei zweizügigen, für beide Züge)"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$51","v":"Absolut Thermo-Trennstein"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$410","v":"Thermo-Dichtset"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$52","v":"Bewehrungs-Set"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$53","v":"Kaminhalter"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$54","v":"Kaminaufsätze"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$63","v":" (ab Ø 16)"},null,null,null,null,{"$f":"Vokabel!$A$431","v":"2.kl.Zug"},null,{"$f":"Vokabel!$A$430","v":"1.Zug"}]

{"sheet":"Absolut Thermoset_F","index":17,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Cheminee","index":18,"n_rows":29,"n_cols":12,"rows_kept":29,"cut":false,"hidden":true,"merged":[[3,5,3,13],[2,5,2,12]]}
[]
[]
[null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$79,Daten!$T:$AL,19,0)","v":"Typ  CHEMINEE 20"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$39","v":"Lichter Ø cm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$40","v":"Anlagenhöhe in m"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$41","v":"Fussausführung"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$64","v":"Fundamentsockel"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$65","v":"(zweizügig - für beide Züge) "}]
[null,null,null,null,null,{"$f":"Vokabel!$A$66","v":"Putzanschluss"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$65","v":"(zweizügig - für beide Züge) "}]
[null,null,null,null,null,{"$f":"Vokabel!$A$42","v":"Rauchrohranschluss"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$56","v":"(bei kombiniert kleiner Ø)"}]
[null,null,null,null,null,{"$f":"Vokabel!A68","v":"Abdeckplatte (KWD)"}]
[]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$44","v":"Zubehör"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$47","v":"zusätzlicher Rauchrohranschluss "}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$50","v":"obere Putztür "}]
[null,null,null,null,null,{"$f":"Vokabel!$A$59","v":"(bei zweizügigen, für beide Züge)"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$53","v":"Kaminhalter"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$54","v":"Kaminaufsätze"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$63","v":" (ab Ø 16)"},null,null,null,null,{"$f":"Vokabel!$A$431","v":"2.kl.Zug"},{"$f":"Vokabel!$A$430","v":"1.Zug"}]

{"sheet":"ISOLIT","index":19,"n_rows":772,"n_cols":6,"rows_kept":772,"cut":false,"hidden":true,"merged":[[3,5,3,13],[2,5,2,12]]}
[]
[]
[null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$1,Daten!$T:$AL,19,0)","v":"Typ  Schiedel ISOLIT 20/20"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$39","v":"Lichter Ø cm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$40","v":"Anlagenhöhe in m"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$423","v":"Cheminée-Anfänger"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$424","v":"Gasdichte Russtüre"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$425","v":"Elementhöhe 25 cm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$427","v":"Rauchrohranschlusselement"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$426","v":"Bauhöhe 50 cm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!A68","v":"Abdeckplatte (KWD)"}]
[]
[]
[]
[]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$44","v":"Zubehör"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$428","v":"Kaminschleifung"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$429","v":"Schleifungen bis max. 30°"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!$A$54","v":"Kaminaufsätze"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,1]

{"sheet":"Technostar120","index":20,"n_rows":20,"n_cols":16,"rows_kept":20,"cut":false,"hidden":true,"merged":[[3,5,3,9],[2,5,2,9]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$10,Daten!$T:$U,2,0)&VLOOKUP(Daten!$U$10,Daten!$T:$V,3,0)","v":"Technostar12080"}]
[null,null,null,null,null,{"$f":"VLOOKUP(Daten!$U$10,Daten!$T:$AL,19,0)","v":"Typ  TECHNOSTAR120 Ø 80"}]
[]
[]
[null,null,null,null,null,{"$f":"Vokabel!A311","v":"Lichter Ø mm"}]
[]
[null,null,null,null,null,{"$f":"Vokabel!A75","v":"Brennstoff"}]
[]
[]
[null,null,null,null,null,null,null,null,null,9.99]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(P2,Sortimente!G:P,10,0)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"P12-J11","v":-9.99}]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohr 2000 mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohr 500 mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohr 250 mm"]

{"sheet":"Verrechnungspartner","index":21,"n_rows":300,"n_cols":24,"rows_kept":300,"cut":false,"hidden":true,"merged":[[9,22,9,24],[9,25,9,26],[0,22,0,26],[1,22,1,26],[3,22,3,26],[4,23,4,26],[7,22,7,26],[5,23,5,26],[6,22,6,26],[8,22,8,26]]}
[null,"Verrechnungspartner / partenaire de facturation",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10001,{"$f":"VLOOKUP(S1,T2:U300,2,0)","v":1},-1,null,{"$f":"IF(INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,2)=\"A-Händler\",\"\",IF(INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,2)=\"\",\"\",INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,2)))","v":""}]
["Nr.","Adresse 1","Adresse 2","Straße/Rue","PLZ/NP","Ort/Lieu",null,null,null,null,null,null,null,null,null,null,null,null,"Kunden-Matchcode",1,{"$f":"U1+1","v":0},null,{"$f":"IF(INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,2)=\"A-Händler\",\"\",IF(INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,3)=\"\",\"\",INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,3)))","v":""}]
[10001,"A-Händler",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B3=\"\",\"\",B3&\", \"&F3)","v":"A-Händler, "},{"$f":"IF(A3=\"\",\"\",A3)","v":10001},1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B4=\"\",\"\",B4&\", \"&F4)","v":""},{"$f":"IF(A4=\"\",\"\",A4)","v":""},2,null,{"$f":"IF(INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,2)=\"A-Händler\",\"\",IF(INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,4)=\"\",\"\",INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,4)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B5=\"\",\"\",B5&\", \"&F5)","v":""},"",3,null,{"$f":"IF(INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,2)=\"A-Händler\",\"\",IF(INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,5)=\"\",\"\",INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,5)))","v":""},{"$f":"IF(INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,2)=\"A-Händler\",\"\",IF(INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,6)=\"\",\"\",INDEX(Verrechnungspartner!$A$3:$J$300,Verrechnungspartner!$T$2,6)))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B6=\"\",\"\",B6&\", \"&F6)","v":""},"",4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",10]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",11]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",12]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",13]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",14]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",15]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",16]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",17]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",18]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",19]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",20]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",21]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",22]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",23]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",26]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",28]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",29]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",30]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",31]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",34]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",35]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",36]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",37]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",38]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",39]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",40]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",41]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",42]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",43]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",44]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",45]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",46]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",47]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",48]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",49]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",51]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",52]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",53]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",54]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",55]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",56]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",57]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",58]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",59]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",60]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",61]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",62]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",63]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",64]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U66+1","v":65}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A68=\"\",\"\",A68)","v":""},66]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",67]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B70=\"\",\"\",B70&\", \"&F70)","v":""},"",68]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",69]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",70]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",71]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",72]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",73]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",74]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",75]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",76]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",77]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",78]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",79]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",80]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",81]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",82]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",83]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",84]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",85]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",86]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",87]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",88]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",89]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",90]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",91]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",92]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",93]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",94]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",95]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",96]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",97]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",98]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",99]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",100]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",101]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",102]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",103]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",104]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",105]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",106]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",107]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",108]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",109]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",110]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",111]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",112]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",113]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",114]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",115]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",116]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",117]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",118]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",119]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",120]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",121]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",122]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",123]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",124]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",125]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",126]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",127]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",128]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U130+1","v":129}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A132=\"\",\"\",A132)","v":""},130]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",131]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B134=\"\",\"\",B134&\", \"&F134)","v":""},"",132]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",133]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",134]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",135]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",136]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",137]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",138]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",139]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",140]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",141]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",142]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",143]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",144]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",145]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",146]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",147]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",148]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",149]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",150]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",151]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",152]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",153]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",154]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",155]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",156]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",157]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",158]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",159]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",160]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",161]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",162]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",163]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",164]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",165]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",166]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",167]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",168]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",169]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",170]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",171]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",172]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",173]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",174]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",175]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",176]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",177]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",178]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",179]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",180]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",181]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",182]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",183]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",184]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",186]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",187]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",188]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",189]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",190]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",191]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",192]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U194+1","v":193}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A196=\"\",\"\",A196)","v":""},194]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",195]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B198=\"\",\"\",B198&\", \"&F198)","v":""},"",196]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",197]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",198]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",199]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",200]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",201]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",202]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",203]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",204]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",205]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",206]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",207]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",208]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",209]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",210]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",211]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",212]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",213]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",214]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",215]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",216]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",217]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",218]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",219]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",220]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",221]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",222]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",223]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",224]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",225]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",226]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",227]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",228]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",229]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",230]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",231]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",232]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",233]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",234]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",235]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",236]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",237]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",238]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",239]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",240]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",241]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",242]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",243]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",244]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",245]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",246]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",247]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",248]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",249]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",250]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",251]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",252]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",253]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",254]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",255]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",256]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",{"$f":"U258+1","v":257}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF(A260=\"\",\"\",A260)","v":""},258]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",259]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B262=\"\",\"\",B262&\", \"&F262)","v":""},"",260]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",261]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",262]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",263]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",264]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",265]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",266]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",267]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",268]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",269]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",270]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",271]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",272]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",273]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",274]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",275]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",276]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",277]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",278]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",279]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",280]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",281]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",282]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",283]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",284]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",285]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",286]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",287]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",288]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",289]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",290]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",291]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",292]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",293]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",294]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",295]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",296]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",297]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","",298]

{"sheet":"Verbindungsleitung TS","index":22,"n_rows":90,"n_cols":8,"rows_kept":90,"cut":false,"hidden":true,"merged":[]}
[{"$f":"Daten!U203","v":"Nein"}]
[null,null,{"$f":"VLOOKUP(A1,Daten!T:U,2,0)","v":"Nein"},null,{"$f":"IF(E6=\"\",\"\",Vokabel!$A$392&\" \"&VLOOKUP(A1,Daten!T:AC,5,0)& \" \" &VLOOKUP(A1,Daten!T:AC,3,0))","v":""}]
[null,null,{"$f":"IF(C2=\"Absolut\",Daten!AE35,IF(C2=\"SIH\",Daten!AF79,\"\"))","v":""},{"$f":"IF(C2=\"Kerastar\",\"für \"&Daten!C401,IF(C2=\"ADW TecnoStar\",\"für \"&Daten!C401,IF(C2=\"ICS\",\"für \"&Daten!C401,\"\")))","v":""},{"$f":"IF(VLOOKUP(A1,Daten!$T:$AA,8,0)=0,\"\",(VLOOKUP(A1,Daten!$T:$AA,8,0)))","v":""}]
[null,null,null,null,{"$f":"IF(VLOOKUP(A1,Daten!$T:$AB,9,0)=0,\"\",(VLOOKUP(A1,Daten!$T:$AB,9,0)))","v":""}]
["Nr.","Verkn.","Rabatt- fähig","Pos.","Artikelnummer","Artikelbezeichnung","Baulänge","Menge"]
[0,{"$f":"$A$1&'Verbindungsleitung TS'!A6","v":"Nein0"},{"$f":"IF(E6=\"\",\"\",IF(E6=\"Sonder\",\"J\",VLOOKUP(E6,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B6,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B6,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D6=\"\",\"\",VLOOKUP($B6,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E6=\"\",\"\",VLOOKUP(E6,sanschie!B:E,4,0))","v":""},{"$f":"IF(E6=\"\",\"\",IF(VLOOKUP(E6,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E6,sanschie!B:J,9,0)))","v":""},1]
[1,{"$f":"$A$1&'Verbindungsleitung TS'!A7","v":"Nein1"},{"$f":"IF(E7=\"\",\"\",IF(E7=\"Sonder\",\"J\",VLOOKUP(E7,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B7,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B7,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D7=\"\",\"\",VLOOKUP($B7,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E7=\"\",\"\",VLOOKUP(E7,sanschie!B:E,4,0))","v":""},{"$f":"IF(E7=\"\",\"\",IF(VLOOKUP(E7,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E7,sanschie!B:J,9,0)))","v":""}]
[2,{"$f":"$A$1&'Verbindungsleitung TS'!A8","v":"Nein2"},{"$f":"IF(E8=\"\",\"\",IF(E8=\"Sonder\",\"J\",VLOOKUP(E8,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B8,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B8,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D8=\"\",\"\",VLOOKUP($B8,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E8=\"\",\"\",VLOOKUP(E8,sanschie!B:E,4,0))","v":""},{"$f":"IF(E8=\"\",\"\",IF(VLOOKUP(E8,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E8,sanschie!B:J,9,0)))","v":""}]
[3,{"$f":"$A$1&'Verbindungsleitung TS'!A9","v":"Nein3"},{"$f":"IF(E9=\"\",\"\",IF(E9=\"Sonder\",\"J\",VLOOKUP(E9,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B9,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B9,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D9=\"\",\"\",VLOOKUP($B9,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E9=\"\",\"\",VLOOKUP(E9,sanschie!B:E,4,0))","v":""},{"$f":"IF(E9=\"\",\"\",IF(VLOOKUP(E9,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E9,sanschie!B:J,9,0)))","v":""}]
[4,{"$f":"$A$1&'Verbindungsleitung TS'!A10","v":"Nein4"},{"$f":"IF(E10=\"\",\"\",IF(E10=\"Sonder\",\"J\",VLOOKUP(E10,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B10,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B10,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D10=\"\",\"\",VLOOKUP($B10,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E10=\"\",\"\",VLOOKUP(E10,sanschie!B:E,4,0))","v":""},{"$f":"IF(E10=\"\",\"\",IF(VLOOKUP(E10,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E10,sanschie!B:J,9,0)))","v":""}]
[5,{"$f":"$A$1&'Verbindungsleitung TS'!A11","v":"Nein5"},{"$f":"IF(E11=\"\",\"\",IF(E11=\"Sonder\",\"J\",VLOOKUP(E11,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B11,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B11,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D11=\"\",\"\",VLOOKUP($B11,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E11=\"\",\"\",VLOOKUP(E11,sanschie!B:E,4,0))","v":""},{"$f":"IF(E11=\"\",\"\",IF(VLOOKUP(E11,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E11,sanschie!B:J,9,0)))","v":""}]
[6,{"$f":"$A$1&'Verbindungsleitung TS'!A12","v":"Nein6"},{"$f":"IF(E12=\"\",\"\",IF(E12=\"Sonder\",\"J\",VLOOKUP(E12,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B12,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B12,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D12=\"\",\"\",VLOOKUP($B12,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E12=\"\",\"\",VLOOKUP(E12,sanschie!B:E,4,0))","v":""},{"$f":"IF(E12=\"\",\"\",IF(VLOOKUP(E12,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E12,sanschie!B:J,9,0)))","v":""}]
[7,{"$f":"$A$1&'Verbindungsleitung TS'!A13","v":"Nein7"},{"$f":"IF(E13=\"\",\"\",IF(E13=\"Sonder\",\"J\",VLOOKUP(E13,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B13,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B13,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D13=\"\",\"\",VLOOKUP($B13,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E13=\"\",\"\",VLOOKUP(E13,sanschie!B:E,4,0))","v":""},{"$f":"IF(E13=\"\",\"\",IF(VLOOKUP(E13,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E13,sanschie!B:J,9,0)))","v":""}]
[8,{"$f":"$A$1&'Verbindungsleitung TS'!A14","v":"Nein8"},{"$f":"IF(E14=\"\",\"\",IF(E14=\"Sonder\",\"J\",VLOOKUP(E14,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B14,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B14,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D14=\"\",\"\",VLOOKUP($B14,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E14=\"\",\"\",VLOOKUP(E14,sanschie!B:E,4,0))","v":""},{"$f":"IF(E14=\"\",\"\",IF(VLOOKUP(E14,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E14,sanschie!B:J,9,0)))","v":""}]
[9,{"$f":"$A$1&'Verbindungsleitung TS'!A15","v":"Nein9"},{"$f":"IF(E15=\"\",\"\",IF(E15=\"Sonder\",\"J\",VLOOKUP(E15,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B15,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B15,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D15=\"\",\"\",VLOOKUP($B15,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E15=\"\",\"\",VLOOKUP(E15,sanschie!B:E,4,0))","v":""},{"$f":"IF(E15=\"\",\"\",IF(VLOOKUP(E15,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E15,sanschie!B:J,9,0)))","v":""}]
[10,{"$f":"$A$1&'Verbindungsleitung TS'!A16","v":"Nein10"},{"$f":"IF(E16=\"\",\"\",IF(E16=\"Sonder\",\"J\",VLOOKUP(E16,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B16,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B16,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D16=\"\",\"\",VLOOKUP($B16,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E16=\"\",\"\",VLOOKUP(E16,sanschie!B:E,4,0))","v":""},{"$f":"IF(E16=\"\",\"\",IF(VLOOKUP(E16,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E16,sanschie!B:J,9,0)))","v":""}]
[11,{"$f":"$A$1&'Verbindungsleitung TS'!A17","v":"Nein11"},{"$f":"IF(E17=\"\",\"\",IF(E17=\"Sonder\",\"J\",VLOOKUP(E17,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B17,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B17,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D17=\"\",\"\",VLOOKUP($B17,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E17=\"\",\"\",VLOOKUP(E17,sanschie!B:E,4,0))","v":""},{"$f":"IF(E17=\"\",\"\",IF(VLOOKUP(E17,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E17,sanschie!B:J,9,0)))","v":""}]
[12,{"$f":"$A$1&'Verbindungsleitung TS'!A18","v":"Nein12"},{"$f":"IF(E18=\"\",\"\",IF(E18=\"Sonder\",\"J\",VLOOKUP(E18,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B18,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B18,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D18=\"\",\"\",VLOOKUP($B18,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E18=\"\",\"\",VLOOKUP(E18,sanschie!B:E,4,0))","v":""},{"$f":"IF(E18=\"\",\"\",IF(VLOOKUP(E18,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E18,sanschie!B:J,9,0)))","v":""}]
[13,{"$f":"$A$1&'Verbindungsleitung TS'!A19","v":"Nein13"},{"$f":"IF(E19=\"\",\"\",IF(E19=\"Sonder\",\"J\",VLOOKUP(E19,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B19,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B19,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D19=\"\",\"\",VLOOKUP($B19,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E19=\"\",\"\",VLOOKUP(E19,sanschie!B:E,4,0))","v":""},{"$f":"IF(E19=\"\",\"\",IF(VLOOKUP(E19,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E19,sanschie!B:J,9,0)))","v":""}]
[14,{"$f":"$A$1&'Verbindungsleitung TS'!A20","v":"Nein14"},{"$f":"IF(E20=\"\",\"\",IF(E20=\"Sonder\",\"J\",VLOOKUP(E20,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B20,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B20,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D20=\"\",\"\",VLOOKUP($B20,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E20=\"\",\"\",VLOOKUP(E20,sanschie!B:E,4,0))","v":""},{"$f":"IF(E20=\"\",\"\",IF(VLOOKUP(E20,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E20,sanschie!B:J,9,0)))","v":""}]
[15,{"$f":"$A$1&'Verbindungsleitung TS'!A21","v":"Nein15"},{"$f":"IF(E21=\"\",\"\",IF(E21=\"Sonder\",\"J\",VLOOKUP(E21,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B21,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B21,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D21=\"\",\"\",VLOOKUP($B21,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E21=\"\",\"\",VLOOKUP(E21,sanschie!B:E,4,0))","v":""},{"$f":"IF(E21=\"\",\"\",IF(VLOOKUP(E21,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E21,sanschie!B:J,9,0)))","v":""}]
[16,{"$f":"$A$1&'Verbindungsleitung TS'!A22","v":"Nein16"},{"$f":"IF(E22=\"\",\"\",IF(E22=\"Sonder\",\"J\",VLOOKUP(E22,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B22,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B22,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D22=\"\",\"\",VLOOKUP($B22,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E22=\"\",\"\",VLOOKUP(E22,sanschie!B:E,4,0))","v":""},{"$f":"IF(E22=\"\",\"\",IF(VLOOKUP(E22,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E22,sanschie!B:J,9,0)))","v":""}]
[17,{"$f":"$A$1&'Verbindungsleitung TS'!A23","v":"Nein17"},{"$f":"IF(E23=\"\",\"\",IF(E23=\"Sonder\",\"J\",VLOOKUP(E23,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B23,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B23,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D23=\"\",\"\",VLOOKUP($B23,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E23=\"\",\"\",VLOOKUP(E23,sanschie!B:E,4,0))","v":""},{"$f":"IF(E23=\"\",\"\",IF(VLOOKUP(E23,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E23,sanschie!B:J,9,0)))","v":""}]
[18,{"$f":"$A$1&'Verbindungsleitung TS'!A24","v":"Nein18"},{"$f":"IF(E24=\"\",\"\",IF(E24=\"Sonder\",\"J\",VLOOKUP(E24,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B24,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B24,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D24=\"\",\"\",VLOOKUP($B24,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E24=\"\",\"\",VLOOKUP(E24,sanschie!B:E,4,0))","v":""},{"$f":"IF(E24=\"\",\"\",IF(VLOOKUP(E24,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E24,sanschie!B:J,9,0)))","v":""}]
[19,{"$f":"$A$1&'Verbindungsleitung TS'!A25","v":"Nein19"},{"$f":"IF(E25=\"\",\"\",IF(E25=\"Sonder\",\"J\",VLOOKUP(E25,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B25,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B25,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D25=\"\",\"\",VLOOKUP($B25,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E25=\"\",\"\",VLOOKUP(E25,sanschie!B:E,4,0))","v":""},{"$f":"IF(E25=\"\",\"\",IF(VLOOKUP(E25,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E25,sanschie!B:J,9,0)))","v":""}]
[20,{"$f":"$A$1&'Verbindungsleitung TS'!A26","v":"Nein20"},{"$f":"IF(E26=\"\",\"\",IF(E26=\"Sonder\",\"J\",VLOOKUP(E26,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B26,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B26,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D26=\"\",\"\",VLOOKUP($B26,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E26=\"\",\"\",VLOOKUP(E26,sanschie!B:E,4,0))","v":""},{"$f":"IF(E26=\"\",\"\",IF(VLOOKUP(E26,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E26,sanschie!B:J,9,0)))","v":""}]
[21,{"$f":"$A$1&'Verbindungsleitung TS'!A27","v":"Nein21"},{"$f":"IF(E27=\"\",\"\",IF(E27=\"Sonder\",\"J\",VLOOKUP(E27,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B27,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B27,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D27=\"\",\"\",VLOOKUP($B27,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E27=\"\",\"\",VLOOKUP(E27,sanschie!B:E,4,0))","v":""},{"$f":"IF(E27=\"\",\"\",IF(VLOOKUP(E27,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E27,sanschie!B:J,9,0)))","v":""}]
[22,{"$f":"$A$1&'Verbindungsleitung TS'!A28","v":"Nein22"},{"$f":"IF(E28=\"\",\"\",IF(E28=\"Sonder\",\"J\",VLOOKUP(E28,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B28,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B28,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D28=\"\",\"\",VLOOKUP($B28,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E28=\"\",\"\",VLOOKUP(E28,sanschie!B:E,4,0))","v":""},{"$f":"IF(E28=\"\",\"\",IF(VLOOKUP(E28,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E28,sanschie!B:J,9,0)))","v":""}]
[23,{"$f":"$A$1&'Verbindungsleitung TS'!A29","v":"Nein23"},{"$f":"IF(E29=\"\",\"\",IF(E29=\"Sonder\",\"J\",VLOOKUP(E29,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B29,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B29,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D29=\"\",\"\",VLOOKUP($B29,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E29=\"\",\"\",VLOOKUP(E29,sanschie!B:E,4,0))","v":""},{"$f":"IF(E29=\"\",\"\",IF(VLOOKUP(E29,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E29,sanschie!B:J,9,0)))","v":""}]
[24,{"$f":"$A$1&'Verbindungsleitung TS'!A30","v":"Nein24"},{"$f":"IF(E30=\"\",\"\",IF(E30=\"Sonder\",\"J\",VLOOKUP(E30,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B30,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B30,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D30=\"\",\"\",VLOOKUP($B30,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E30=\"\",\"\",VLOOKUP(E30,sanschie!B:E,4,0))","v":""},{"$f":"IF(E30=\"\",\"\",IF(VLOOKUP(E30,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E30,sanschie!B:J,9,0)))","v":""}]
[25,{"$f":"$A$1&'Verbindungsleitung TS'!A31","v":"Nein25"},{"$f":"IF(E31=\"\",\"\",IF(E31=\"Sonder\",\"J\",VLOOKUP(E31,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B31,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B31,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D31=\"\",\"\",VLOOKUP($B31,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E31=\"\",\"\",VLOOKUP(E31,sanschie!B:E,4,0))","v":""},{"$f":"IF(E31=\"\",\"\",IF(VLOOKUP(E31,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E31,sanschie!B:J,9,0)))","v":""}]
[26,{"$f":"$A$1&'Verbindungsleitung TS'!A32","v":"Nein26"},{"$f":"IF(E32=\"\",\"\",IF(E32=\"Sonder\",\"J\",VLOOKUP(E32,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B32,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B32,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D32=\"\",\"\",VLOOKUP($B32,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E32=\"\",\"\",VLOOKUP(E32,sanschie!B:E,4,0))","v":""},{"$f":"IF(E32=\"\",\"\",IF(VLOOKUP(E32,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E32,sanschie!B:J,9,0)))","v":""}]
[27,{"$f":"$A$1&'Verbindungsleitung TS'!A33","v":"Nein27"},{"$f":"IF(E33=\"\",\"\",IF(E33=\"Sonder\",\"J\",VLOOKUP(E33,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B33,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B33,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D33=\"\",\"\",VLOOKUP($B33,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E33=\"\",\"\",VLOOKUP(E33,sanschie!B:E,4,0))","v":""},{"$f":"IF(E33=\"\",\"\",IF(VLOOKUP(E33,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E33,sanschie!B:J,9,0)))","v":""}]
[28,{"$f":"$A$1&'Verbindungsleitung TS'!A34","v":"Nein28"},{"$f":"IF(E34=\"\",\"\",IF(E34=\"Sonder\",\"J\",VLOOKUP(E34,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B34,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B34,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D34=\"\",\"\",VLOOKUP($B34,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E34=\"\",\"\",VLOOKUP(E34,sanschie!B:E,4,0))","v":""},{"$f":"IF(E34=\"\",\"\",IF(VLOOKUP(E34,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E34,sanschie!B:J,9,0)))","v":""}]
[29,{"$f":"$A$1&'Verbindungsleitung TS'!A35","v":"Nein29"},{"$f":"IF(E35=\"\",\"\",IF(E35=\"Sonder\",\"J\",VLOOKUP(E35,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B35,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B35,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D35=\"\",\"\",VLOOKUP($B35,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E35=\"\",\"\",VLOOKUP(E35,sanschie!B:E,4,0))","v":""},{"$f":"IF(E35=\"\",\"\",IF(VLOOKUP(E35,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E35,sanschie!B:J,9,0)))","v":""}]
[30,{"$f":"$A$1&'Verbindungsleitung TS'!A36","v":"Nein30"},{"$f":"IF(E36=\"\",\"\",IF(E36=\"Sonder\",\"J\",VLOOKUP(E36,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B36,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B36,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D36=\"\",\"\",VLOOKUP($B36,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E36=\"\",\"\",VLOOKUP(E36,sanschie!B:E,4,0))","v":""},{"$f":"IF(E36=\"\",\"\",IF(VLOOKUP(E36,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E36,sanschie!B:J,9,0)))","v":""}]
[31,{"$f":"$A$1&'Verbindungsleitung TS'!A37","v":"Nein31"},{"$f":"IF(E37=\"\",\"\",IF(E37=\"Sonder\",\"J\",VLOOKUP(E37,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B37,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B37,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D37=\"\",\"\",VLOOKUP($B37,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E37=\"\",\"\",VLOOKUP(E37,sanschie!B:E,4,0))","v":""},{"$f":"IF(E37=\"\",\"\",IF(VLOOKUP(E37,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E37,sanschie!B:J,9,0)))","v":""}]
[32,{"$f":"$A$1&'Verbindungsleitung TS'!A38","v":"Nein32"},{"$f":"IF(E38=\"\",\"\",IF(E38=\"Sonder\",\"J\",VLOOKUP(E38,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B38,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B38,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D38=\"\",\"\",VLOOKUP($B38,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E38=\"\",\"\",VLOOKUP(E38,sanschie!B:E,4,0))","v":""},{"$f":"IF(E38=\"\",\"\",IF(VLOOKUP(E38,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E38,sanschie!B:J,9,0)))","v":""}]
[33,{"$f":"$A$1&'Verbindungsleitung TS'!A39","v":"Nein33"},{"$f":"IF(E39=\"\",\"\",IF(E39=\"Sonder\",\"J\",VLOOKUP(E39,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B39,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B39,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D39=\"\",\"\",VLOOKUP($B39,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E39=\"\",\"\",VLOOKUP(E39,sanschie!B:E,4,0))","v":""},{"$f":"IF(E39=\"\",\"\",IF(VLOOKUP(E39,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E39,sanschie!B:J,9,0)))","v":""}]
[34,{"$f":"$A$1&'Verbindungsleitung TS'!A40","v":"Nein34"},{"$f":"IF(E40=\"\",\"\",IF(E40=\"Sonder\",\"J\",VLOOKUP(E40,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B40,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B40,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D40=\"\",\"\",VLOOKUP($B40,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E40=\"\",\"\",VLOOKUP(E40,sanschie!B:E,4,0))","v":""},{"$f":"IF(E40=\"\",\"\",IF(VLOOKUP(E40,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E40,sanschie!B:J,9,0)))","v":""}]
[35,{"$f":"$A$1&'Verbindungsleitung TS'!A41","v":"Nein35"},{"$f":"IF(E41=\"\",\"\",IF(E41=\"Sonder\",\"J\",VLOOKUP(E41,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B41,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B41,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D41=\"\",\"\",VLOOKUP($B41,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E41=\"\",\"\",VLOOKUP(E41,sanschie!B:E,4,0))","v":""},{"$f":"IF(E41=\"\",\"\",IF(VLOOKUP(E41,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E41,sanschie!B:J,9,0)))","v":""}]
[36,{"$f":"$A$1&'Verbindungsleitung TS'!A42","v":"Nein36"},{"$f":"IF(E42=\"\",\"\",IF(E42=\"Sonder\",\"J\",VLOOKUP(E42,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B42,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B42,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D42=\"\",\"\",VLOOKUP($B42,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E42=\"\",\"\",VLOOKUP(E42,sanschie!B:E,4,0))","v":""},{"$f":"IF(E42=\"\",\"\",IF(VLOOKUP(E42,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E42,sanschie!B:J,9,0)))","v":""}]
[37,{"$f":"$A$1&'Verbindungsleitung TS'!A43","v":"Nein37"},{"$f":"IF(E43=\"\",\"\",IF(E43=\"Sonder\",\"J\",VLOOKUP(E43,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B43,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B43,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D43=\"\",\"\",VLOOKUP($B43,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E43=\"\",\"\",VLOOKUP(E43,sanschie!B:E,4,0))","v":""},{"$f":"IF(E43=\"\",\"\",IF(VLOOKUP(E43,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E43,sanschie!B:J,9,0)))","v":""}]
[38,{"$f":"$A$1&'Verbindungsleitung TS'!A44","v":"Nein38"},{"$f":"IF(E44=\"\",\"\",IF(E44=\"Sonder\",\"J\",VLOOKUP(E44,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B44,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B44,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D44=\"\",\"\",VLOOKUP($B44,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E44=\"\",\"\",VLOOKUP(E44,sanschie!B:E,4,0))","v":""},{"$f":"IF(E44=\"\",\"\",IF(VLOOKUP(E44,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E44,sanschie!B:J,9,0)))","v":""}]
[39,{"$f":"$A$1&'Verbindungsleitung TS'!A45","v":"Nein39"},{"$f":"IF(E45=\"\",\"\",IF(E45=\"Sonder\",\"J\",VLOOKUP(E45,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B45,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B45,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D45=\"\",\"\",VLOOKUP($B45,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E45=\"\",\"\",VLOOKUP(E45,sanschie!B:E,4,0))","v":""},{"$f":"IF(E45=\"\",\"\",IF(VLOOKUP(E45,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E45,sanschie!B:J,9,0)))","v":""}]
[40,{"$f":"$A$1&'Verbindungsleitung TS'!A46","v":"Nein40"},{"$f":"IF(E46=\"\",\"\",IF(E46=\"Sonder\",\"J\",VLOOKUP(E46,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B46,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B46,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D46=\"\",\"\",VLOOKUP($B46,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E46=\"\",\"\",VLOOKUP(E46,sanschie!B:E,4,0))","v":""},{"$f":"IF(E46=\"\",\"\",IF(VLOOKUP(E46,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E46,sanschie!B:J,9,0)))","v":""}]
[41,{"$f":"$A$1&'Verbindungsleitung TS'!A47","v":"Nein41"},{"$f":"IF(E47=\"\",\"\",IF(E47=\"Sonder\",\"J\",VLOOKUP(E47,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B47,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B47,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D47=\"\",\"\",VLOOKUP($B47,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E47=\"\",\"\",VLOOKUP(E47,sanschie!B:E,4,0))","v":""},{"$f":"IF(E47=\"\",\"\",IF(VLOOKUP(E47,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E47,sanschie!B:J,9,0)))","v":""}]
[42,{"$f":"$A$1&'Verbindungsleitung TS'!A48","v":"Nein42"},{"$f":"IF(E48=\"\",\"\",IF(E48=\"Sonder\",\"J\",VLOOKUP(E48,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B48,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B48,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D48=\"\",\"\",VLOOKUP($B48,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E48=\"\",\"\",VLOOKUP(E48,sanschie!B:E,4,0))","v":""},{"$f":"IF(E48=\"\",\"\",IF(VLOOKUP(E48,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E48,sanschie!B:J,9,0)))","v":""}]
[43,{"$f":"$A$1&'Verbindungsleitung TS'!A49","v":"Nein43"},{"$f":"IF(E49=\"\",\"\",IF(E49=\"Sonder\",\"J\",VLOOKUP(E49,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B49,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B49,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D49=\"\",\"\",VLOOKUP($B49,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E49=\"\",\"\",VLOOKUP(E49,sanschie!B:E,4,0))","v":""},{"$f":"IF(E49=\"\",\"\",IF(VLOOKUP(E49,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E49,sanschie!B:J,9,0)))","v":""}]
[44,{"$f":"$A$1&'Verbindungsleitung TS'!A50","v":"Nein44"},{"$f":"IF(E50=\"\",\"\",IF(E50=\"Sonder\",\"J\",VLOOKUP(E50,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B50,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B50,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D50=\"\",\"\",VLOOKUP($B50,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E50=\"\",\"\",VLOOKUP(E50,sanschie!B:E,4,0))","v":""},{"$f":"IF(E50=\"\",\"\",IF(VLOOKUP(E50,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E50,sanschie!B:J,9,0)))","v":""}]
[45,{"$f":"$A$1&'Verbindungsleitung TS'!A51","v":"Nein45"},{"$f":"IF(E51=\"\",\"\",IF(E51=\"Sonder\",\"J\",VLOOKUP(E51,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B51,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B51,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D51=\"\",\"\",VLOOKUP($B51,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E51=\"\",\"\",VLOOKUP(E51,sanschie!B:E,4,0))","v":""},{"$f":"IF(E51=\"\",\"\",IF(VLOOKUP(E51,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E51,sanschie!B:J,9,0)))","v":""}]
[46,{"$f":"$A$1&'Verbindungsleitung TS'!A52","v":"Nein46"},{"$f":"IF(E52=\"\",\"\",IF(E52=\"Sonder\",\"J\",VLOOKUP(E52,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B52,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B52,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D52=\"\",\"\",VLOOKUP($B52,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E52=\"\",\"\",VLOOKUP(E52,sanschie!B:E,4,0))","v":""},{"$f":"IF(E52=\"\",\"\",IF(VLOOKUP(E52,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E52,sanschie!B:J,9,0)))","v":""}]
[47,{"$f":"$A$1&'Verbindungsleitung TS'!A53","v":"Nein47"},{"$f":"IF(E53=\"\",\"\",IF(E53=\"Sonder\",\"J\",VLOOKUP(E53,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B53,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B53,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D53=\"\",\"\",VLOOKUP($B53,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E53=\"\",\"\",VLOOKUP(E53,sanschie!B:E,4,0))","v":""},{"$f":"IF(E53=\"\",\"\",IF(VLOOKUP(E53,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E53,sanschie!B:J,9,0)))","v":""}]
[48,{"$f":"$A$1&'Verbindungsleitung TS'!A54","v":"Nein48"},{"$f":"IF(E54=\"\",\"\",IF(E54=\"Sonder\",\"J\",VLOOKUP(E54,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B54,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B54,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D54=\"\",\"\",VLOOKUP($B54,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E54=\"\",\"\",VLOOKUP(E54,sanschie!B:E,4,0))","v":""},{"$f":"IF(E54=\"\",\"\",IF(VLOOKUP(E54,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E54,sanschie!B:J,9,0)))","v":""}]
[49,{"$f":"$A$1&'Verbindungsleitung TS'!A55","v":"Nein49"},{"$f":"IF(E55=\"\",\"\",IF(E55=\"Sonder\",\"J\",VLOOKUP(E55,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B55,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B55,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D55=\"\",\"\",VLOOKUP($B55,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E55=\"\",\"\",VLOOKUP(E55,sanschie!B:E,4,0))","v":""},{"$f":"IF(E55=\"\",\"\",IF(VLOOKUP(E55,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E55,sanschie!B:J,9,0)))","v":""}]
[50,{"$f":"$A$1&'Verbindungsleitung TS'!A56","v":"Nein50"},{"$f":"IF(E56=\"\",\"\",IF(E56=\"Sonder\",\"J\",VLOOKUP(E56,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B56,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B56,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D56=\"\",\"\",VLOOKUP($B56,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E56=\"\",\"\",VLOOKUP(E56,sanschie!B:E,4,0))","v":""},{"$f":"IF(E56=\"\",\"\",IF(VLOOKUP(E56,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E56,sanschie!B:J,9,0)))","v":""}]
[51,{"$f":"$A$1&'Verbindungsleitung TS'!A57","v":"Nein51"},{"$f":"IF(E57=\"\",\"\",IF(E57=\"Sonder\",\"J\",VLOOKUP(E57,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B57,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B57,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D57=\"\",\"\",VLOOKUP($B57,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E57=\"\",\"\",VLOOKUP(E57,sanschie!B:E,4,0))","v":""},{"$f":"IF(E57=\"\",\"\",IF(VLOOKUP(E57,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E57,sanschie!B:J,9,0)))","v":""}]
[52,{"$f":"$A$1&'Verbindungsleitung TS'!A58","v":"Nein52"},{"$f":"IF(E58=\"\",\"\",IF(E58=\"Sonder\",\"J\",VLOOKUP(E58,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B58,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B58,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D58=\"\",\"\",VLOOKUP($B58,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E58=\"\",\"\",VLOOKUP(E58,sanschie!B:E,4,0))","v":""},{"$f":"IF(E58=\"\",\"\",IF(VLOOKUP(E58,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E58,sanschie!B:J,9,0)))","v":""}]
[53,{"$f":"$A$1&'Verbindungsleitung TS'!A59","v":"Nein53"},{"$f":"IF(E59=\"\",\"\",IF(E59=\"Sonder\",\"J\",VLOOKUP(E59,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B59,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B59,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D59=\"\",\"\",VLOOKUP($B59,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E59=\"\",\"\",VLOOKUP(E59,sanschie!B:E,4,0))","v":""},{"$f":"IF(E59=\"\",\"\",IF(VLOOKUP(E59,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E59,sanschie!B:J,9,0)))","v":""}]
[54,{"$f":"$A$1&'Verbindungsleitung TS'!A60","v":"Nein54"},{"$f":"IF(E60=\"\",\"\",IF(E60=\"Sonder\",\"J\",VLOOKUP(E60,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B60,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B60,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D60=\"\",\"\",VLOOKUP($B60,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E60=\"\",\"\",VLOOKUP(E60,sanschie!B:E,4,0))","v":""},{"$f":"IF(E60=\"\",\"\",IF(VLOOKUP(E60,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E60,sanschie!B:J,9,0)))","v":""}]
[55,{"$f":"$A$1&'Verbindungsleitung TS'!A61","v":"Nein55"},{"$f":"IF(E61=\"\",\"\",IF(E61=\"Sonder\",\"J\",VLOOKUP(E61,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B61,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B61,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D61=\"\",\"\",VLOOKUP($B61,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E61=\"\",\"\",VLOOKUP(E61,sanschie!B:E,4,0))","v":""},{"$f":"IF(E61=\"\",\"\",IF(VLOOKUP(E61,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E61,sanschie!B:J,9,0)))","v":""}]
[56,{"$f":"$A$1&'Verbindungsleitung TS'!A62","v":"Nein56"},{"$f":"IF(E62=\"\",\"\",IF(E62=\"Sonder\",\"J\",VLOOKUP(E62,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B62,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B62,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D62=\"\",\"\",VLOOKUP($B62,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E62=\"\",\"\",VLOOKUP(E62,sanschie!B:E,4,0))","v":""},{"$f":"IF(E62=\"\",\"\",IF(VLOOKUP(E62,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E62,sanschie!B:J,9,0)))","v":""}]
[57,{"$f":"$A$1&'Verbindungsleitung TS'!A63","v":"Nein57"},{"$f":"IF(E63=\"\",\"\",IF(E63=\"Sonder\",\"J\",VLOOKUP(E63,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B63,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B63,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D63=\"\",\"\",VLOOKUP($B63,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E63=\"\",\"\",VLOOKUP(E63,sanschie!B:E,4,0))","v":""},{"$f":"IF(E63=\"\",\"\",IF(VLOOKUP(E63,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E63,sanschie!B:J,9,0)))","v":""}]
[58,{"$f":"$A$1&'Verbindungsleitung TS'!A64","v":"Nein58"},{"$f":"IF(E64=\"\",\"\",IF(E64=\"Sonder\",\"J\",VLOOKUP(E64,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B64,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B64,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D64=\"\",\"\",VLOOKUP($B64,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E64=\"\",\"\",VLOOKUP(E64,sanschie!B:E,4,0))","v":""},{"$f":"IF(E64=\"\",\"\",IF(VLOOKUP(E64,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E64,sanschie!B:J,9,0)))","v":""}]
[59,{"$f":"$A$1&'Verbindungsleitung TS'!A65","v":"Nein59"},{"$f":"IF(E65=\"\",\"\",IF(E65=\"Sonder\",\"J\",VLOOKUP(E65,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B65,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B65,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D65=\"\",\"\",VLOOKUP($B65,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E65=\"\",\"\",VLOOKUP(E65,sanschie!B:E,4,0))","v":""},{"$f":"IF(E65=\"\",\"\",IF(VLOOKUP(E65,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E65,sanschie!B:J,9,0)))","v":""}]
[60,{"$f":"$A$1&'Verbindungsleitung TS'!A66","v":"Nein60"},{"$f":"IF(E66=\"\",\"\",IF(E66=\"Sonder\",\"J\",VLOOKUP(E66,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B66,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B66,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D66=\"\",\"\",VLOOKUP($B66,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E66=\"\",\"\",VLOOKUP(E66,sanschie!B:E,4,0))","v":""},{"$f":"IF(E66=\"\",\"\",IF(VLOOKUP(E66,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E66,sanschie!B:J,9,0)))","v":""}]
[61,{"$f":"$A$1&'Verbindungsleitung TS'!A67","v":"Nein61"},{"$f":"IF(E67=\"\",\"\",IF(E67=\"Sonder\",\"J\",VLOOKUP(E67,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B67,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B67,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D67=\"\",\"\",VLOOKUP($B67,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E67=\"\",\"\",VLOOKUP(E67,sanschie!B:E,4,0))","v":""},{"$f":"IF(E67=\"\",\"\",IF(VLOOKUP(E67,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E67,sanschie!B:J,9,0)))","v":""}]
[62,{"$f":"$A$1&'Verbindungsleitung TS'!A68","v":"Nein62"},{"$f":"IF(E68=\"\",\"\",IF(E68=\"Sonder\",\"J\",VLOOKUP(E68,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B68,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B68,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D68=\"\",\"\",VLOOKUP($B68,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E68=\"\",\"\",VLOOKUP(E68,sanschie!B:E,4,0))","v":""},{"$f":"IF(E68=\"\",\"\",IF(VLOOKUP(E68,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E68,sanschie!B:J,9,0)))","v":""}]
[63,{"$f":"$A$1&'Verbindungsleitung TS'!A69","v":"Nein63"},{"$f":"IF(E69=\"\",\"\",IF(E69=\"Sonder\",\"J\",VLOOKUP(E69,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B69,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B69,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D69=\"\",\"\",VLOOKUP($B69,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E69=\"\",\"\",VLOOKUP(E69,sanschie!B:E,4,0))","v":""},{"$f":"IF(E69=\"\",\"\",IF(VLOOKUP(E69,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E69,sanschie!B:J,9,0)))","v":""}]
[64,{"$f":"$A$1&'Verbindungsleitung TS'!A70","v":"Nein64"},{"$f":"IF(E70=\"\",\"\",IF(E70=\"Sonder\",\"J\",VLOOKUP(E70,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B70,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B70,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D70=\"\",\"\",VLOOKUP($B70,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E70=\"\",\"\",VLOOKUP(E70,sanschie!B:E,4,0))","v":""},{"$f":"IF(E70=\"\",\"\",IF(VLOOKUP(E70,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E70,sanschie!B:J,9,0)))","v":""}]
[65,{"$f":"$A$1&'Verbindungsleitung TS'!A71","v":"Nein65"},{"$f":"IF(E71=\"\",\"\",IF(E71=\"Sonder\",\"J\",VLOOKUP(E71,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B71,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B71,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D71=\"\",\"\",VLOOKUP($B71,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E71=\"\",\"\",VLOOKUP(E71,sanschie!B:E,4,0))","v":""},{"$f":"IF(E71=\"\",\"\",IF(VLOOKUP(E71,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E71,sanschie!B:J,9,0)))","v":""}]
[66,{"$f":"$A$1&'Verbindungsleitung TS'!A72","v":"Nein66"},{"$f":"IF(E72=\"\",\"\",IF(E72=\"Sonder\",\"J\",VLOOKUP(E72,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B72,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B72,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D72=\"\",\"\",VLOOKUP($B72,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E72=\"\",\"\",VLOOKUP(E72,sanschie!B:E,4,0))","v":""},{"$f":"IF(E72=\"\",\"\",IF(VLOOKUP(E72,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E72,sanschie!B:J,9,0)))","v":""}]
[67,{"$f":"$A$1&'Verbindungsleitung TS'!A73","v":"Nein67"},{"$f":"IF(E73=\"\",\"\",IF(E73=\"Sonder\",\"J\",VLOOKUP(E73,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B73,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B73,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D73=\"\",\"\",VLOOKUP($B73,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E73=\"\",\"\",VLOOKUP(E73,sanschie!B:E,4,0))","v":""},{"$f":"IF(E73=\"\",\"\",IF(VLOOKUP(E73,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E73,sanschie!B:J,9,0)))","v":""}]
[68,{"$f":"$A$1&'Verbindungsleitung TS'!A74","v":"Nein68"},{"$f":"IF(E74=\"\",\"\",IF(E74=\"Sonder\",\"J\",VLOOKUP(E74,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B74,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B74,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D74=\"\",\"\",VLOOKUP($B74,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E74=\"\",\"\",VLOOKUP(E74,sanschie!B:E,4,0))","v":""},{"$f":"IF(E74=\"\",\"\",IF(VLOOKUP(E74,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E74,sanschie!B:J,9,0)))","v":""}]
[69,{"$f":"$A$1&'Verbindungsleitung TS'!A75","v":"Nein69"},{"$f":"IF(E75=\"\",\"\",IF(E75=\"Sonder\",\"J\",VLOOKUP(E75,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B75,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B75,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D75=\"\",\"\",VLOOKUP($B75,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E75=\"\",\"\",VLOOKUP(E75,sanschie!B:E,4,0))","v":""},{"$f":"IF(E75=\"\",\"\",IF(VLOOKUP(E75,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E75,sanschie!B:J,9,0)))","v":""}]
[70,{"$f":"$A$1&'Verbindungsleitung TS'!A76","v":"Nein70"},{"$f":"IF(E76=\"\",\"\",IF(E76=\"Sonder\",\"J\",VLOOKUP(E76,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B76,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B76,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D76=\"\",\"\",VLOOKUP($B76,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E76=\"\",\"\",VLOOKUP(E76,sanschie!B:E,4,0))","v":""},{"$f":"IF(E76=\"\",\"\",IF(VLOOKUP(E76,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E76,sanschie!B:J,9,0)))","v":""}]
[71,{"$f":"$A$1&'Verbindungsleitung TS'!A77","v":"Nein71"},{"$f":"IF(E77=\"\",\"\",IF(E77=\"Sonder\",\"J\",VLOOKUP(E77,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B77,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B77,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D77=\"\",\"\",VLOOKUP($B77,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E77=\"\",\"\",VLOOKUP(E77,sanschie!B:E,4,0))","v":""},{"$f":"IF(E77=\"\",\"\",IF(VLOOKUP(E77,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E77,sanschie!B:J,9,0)))","v":""}]
[72,{"$f":"$A$1&'Verbindungsleitung TS'!A78","v":"Nein72"},{"$f":"IF(E78=\"\",\"\",IF(E78=\"Sonder\",\"J\",VLOOKUP(E78,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B78,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B78,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D78=\"\",\"\",VLOOKUP($B78,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E78=\"\",\"\",VLOOKUP(E78,sanschie!B:E,4,0))","v":""},{"$f":"IF(E78=\"\",\"\",IF(VLOOKUP(E78,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E78,sanschie!B:J,9,0)))","v":""}]
[73,{"$f":"$A$1&'Verbindungsleitung TS'!A79","v":"Nein73"},{"$f":"IF(E79=\"\",\"\",IF(E79=\"Sonder\",\"J\",VLOOKUP(E79,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B79,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B79,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D79=\"\",\"\",VLOOKUP($B79,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E79=\"\",\"\",VLOOKUP(E79,sanschie!B:E,4,0))","v":""},{"$f":"IF(E79=\"\",\"\",IF(VLOOKUP(E79,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E79,sanschie!B:J,9,0)))","v":""}]
[74,{"$f":"$A$1&'Verbindungsleitung TS'!A80","v":"Nein74"},{"$f":"IF(E80=\"\",\"\",IF(E80=\"Sonder\",\"J\",VLOOKUP(E80,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B80,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B80,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D80=\"\",\"\",VLOOKUP($B80,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E80=\"\",\"\",VLOOKUP(E80,sanschie!B:E,4,0))","v":""},{"$f":"IF(E80=\"\",\"\",IF(VLOOKUP(E80,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E80,sanschie!B:J,9,0)))","v":""}]
[75,{"$f":"$A$1&'Verbindungsleitung TS'!A81","v":"Nein75"},{"$f":"IF(E81=\"\",\"\",IF(E81=\"Sonder\",\"J\",VLOOKUP(E81,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B81,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B81,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D81=\"\",\"\",VLOOKUP($B81,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E81=\"\",\"\",VLOOKUP(E81,sanschie!B:E,4,0))","v":""},{"$f":"IF(E81=\"\",\"\",IF(VLOOKUP(E81,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E81,sanschie!B:J,9,0)))","v":""}]
[76,{"$f":"$A$1&'Verbindungsleitung TS'!A82","v":"Nein76"},{"$f":"IF(E82=\"\",\"\",IF(E82=\"Sonder\",\"J\",VLOOKUP(E82,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B82,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B82,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D82=\"\",\"\",VLOOKUP($B82,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E82=\"\",\"\",VLOOKUP(E82,sanschie!B:E,4,0))","v":""},{"$f":"IF(E82=\"\",\"\",IF(VLOOKUP(E82,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E82,sanschie!B:J,9,0)))","v":""}]
[77,{"$f":"$A$1&'Verbindungsleitung TS'!A83","v":"Nein77"},{"$f":"IF(E83=\"\",\"\",IF(E83=\"Sonder\",\"J\",VLOOKUP(E83,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B83,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B83,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D83=\"\",\"\",VLOOKUP($B83,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E83=\"\",\"\",VLOOKUP(E83,sanschie!B:E,4,0))","v":""},{"$f":"IF(E83=\"\",\"\",IF(VLOOKUP(E83,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E83,sanschie!B:J,9,0)))","v":""}]
[78,{"$f":"$A$1&'Verbindungsleitung TS'!A84","v":"Nein78"},{"$f":"IF(E84=\"\",\"\",IF(E84=\"Sonder\",\"J\",VLOOKUP(E84,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B84,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B84,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D84=\"\",\"\",VLOOKUP($B84,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E84=\"\",\"\",VLOOKUP(E84,sanschie!B:E,4,0))","v":""},{"$f":"IF(E84=\"\",\"\",IF(VLOOKUP(E84,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E84,sanschie!B:J,9,0)))","v":""}]
[79,{"$f":"$A$1&'Verbindungsleitung TS'!A85","v":"Nein79"},{"$f":"IF(E85=\"\",\"\",IF(E85=\"Sonder\",\"J\",VLOOKUP(E85,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B85,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B85,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D85=\"\",\"\",VLOOKUP($B85,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E85=\"\",\"\",VLOOKUP(E85,sanschie!B:E,4,0))","v":""},{"$f":"IF(E85=\"\",\"\",IF(VLOOKUP(E85,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E85,sanschie!B:J,9,0)))","v":""}]
[80,{"$f":"$A$1&'Verbindungsleitung TS'!A86","v":"Nein80"},{"$f":"IF(E86=\"\",\"\",IF(E86=\"Sonder\",\"J\",VLOOKUP(E86,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B86,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B86,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D86=\"\",\"\",VLOOKUP($B86,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E86=\"\",\"\",VLOOKUP(E86,sanschie!B:E,4,0))","v":""},{"$f":"IF(E86=\"\",\"\",IF(VLOOKUP(E86,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E86,sanschie!B:J,9,0)))","v":""}]
[81,{"$f":"$A$1&'Verbindungsleitung TS'!A87","v":"Nein81"},{"$f":"IF(E87=\"\",\"\",IF(E87=\"Sonder\",\"J\",VLOOKUP(E87,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B87,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B87,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D87=\"\",\"\",VLOOKUP($B87,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E87=\"\",\"\",VLOOKUP(E87,sanschie!B:E,4,0))","v":""},{"$f":"IF(E87=\"\",\"\",IF(VLOOKUP(E87,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E87,sanschie!B:J,9,0)))","v":""}]
[82,{"$f":"$A$1&'Verbindungsleitung TS'!A88","v":"Nein82"},{"$f":"IF(E88=\"\",\"\",IF(E88=\"Sonder\",\"J\",VLOOKUP(E88,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B88,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B88,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D88=\"\",\"\",VLOOKUP($B88,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E88=\"\",\"\",VLOOKUP(E88,sanschie!B:E,4,0))","v":""},{"$f":"IF(E88=\"\",\"\",IF(VLOOKUP(E88,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E88,sanschie!B:J,9,0)))","v":""}]
[83,{"$f":"$A$1&'Verbindungsleitung TS'!A89","v":"Nein83"},{"$f":"IF(E89=\"\",\"\",IF(E89=\"Sonder\",\"J\",VLOOKUP(E89,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B89,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B89,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D89=\"\",\"\",VLOOKUP($B89,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E89=\"\",\"\",VLOOKUP(E89,sanschie!B:E,4,0))","v":""},{"$f":"IF(E89=\"\",\"\",IF(VLOOKUP(E89,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E89,sanschie!B:J,9,0)))","v":""}]
[84,{"$f":"$A$1&'Verbindungsleitung TS'!A90","v":"Nein84"},{"$f":"IF(E90=\"\",\"\",IF(E90=\"Sonder\",\"J\",VLOOKUP(E90,sanschie!B:K,10,0)))","v":""},{"$f":"IF(ISNA(VLOOKUP($B90,Sortimente!D:G,2,0))=TRUE,\"\",VLOOKUP($B90,Sortimente!D:G,2,0))","v":""},{"$f":"IF(D90=\"\",\"\",VLOOKUP($B90,Sortimente!D:G,4,0))","v":""},{"$f":"IF(E90=\"\",\"\",VLOOKUP(E90,sanschie!B:E,4,0))","v":""},{"$f":"IF(E90=\"\",\"\",IF(VLOOKUP(E90,sanschie!B:J,9,0)=\"\",\"\",VLOOKUP(E90,sanschie!B:J,9,0)))","v":""}]

{"sheet":"Commerciante","index":23,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":true,"merged":[]}
[null,{"$f":"Vokabel!$A$241","v":"INFO:"}]
[null,{"$f":"Vokabel!$A$240","v":"In den Zeilen 5-10 tragen Sie bitte Ihre Firma, und den Zeilen 14-15 den Sachbearbeiter u. Tel.Nr., ein."}]
[]
[null,{"$f":"Vokabel!$A$242","v":"Firmendaten:"}]
[{"$f":"Vokabel!$A$226","v":"1.Zeile"},"Ganztec AG"]
[{"$f":"Vokabel!$A$227","v":"2.Zeile"},"Badstrasse 38"]
[{"$f":"Vokabel!$A$228","v":"3.Zeile"},"5312 Döttingen"]
[{"$f":"Vokabel!$A$229","v":"4.Zeile"},"Tel. 0562680000   Fax. 0562680001",null,null,null,{"$f":"B44","v":"nichts"}]
[{"$f":"Vokabel!$A$230","v":"5.Zeile"},"Mail:  info@ganztec.ch"]
["Ganztec N° client"]
[]
[]
[null,{"$f":"Vokabel!$A$247","v":"Sachbearbeiter:"},{"$f":"Vokabel!$A$248","v":"Pers.-Nr."},null,{"$f":"Vokabel!$A$249","v":"Frachteinstellungen:"}]
[{"$f":"Vokabel!$A$250","v":"Vorname/Name"},"Herr Mustermann",null,null,63,{"$f":"Vokabel!$A$256","v":"CHF per Tonne"}]
[{"$f":"Vokabel!$A$251","v":"Telefon"},"Tel. 000000",{"$f":"Eingabe!$K$4&\"  \"&Eingabe!$K$16&\" \"&Eingabe!$L$18","v":"Ganztec AG   "}]
[{"$f":"Vokabel!$A$252","v":"Fax"},"Fax. 0000000"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[3,{"$f":"INDEX(Commerciante!B46:B48,A44,1)","v":"nichts"}]
["Mailprogramm"]
["Outlook (Express)","Outlook"]
["Lotus Notes","Lotus"]
["keines von Beiden","nichts"]

{"sheet":"Firma","index":24,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":true,"merged":[]}
[null,{"$f":"Vokabel!$A$241","v":"INFO:"}]
[null,{"$f":"Vokabel!$A$240","v":"In den Zeilen 5-10 tragen Sie bitte Ihre Firma, und den Zeilen 14-15 den Sachbearbeiter u. Tel.Nr., ein."}]
[]
[null,{"$f":"Vokabel!$A$242","v":"Firmendaten:"}]
[{"$f":"Vokabel!$A$226","v":"1.Zeile"},"Ganztec AG"]
[{"$f":"Vokabel!$A$227","v":"2.Zeile"},"Badstrasse 38"]
[{"$f":"Vokabel!$A$228","v":"3.Zeile"},"5312 Döttingen"]
[{"$f":"Vokabel!$A$229","v":"4.Zeile"},"Tel. 0562680000   Fax. 0562680001",null,null,null,{"$f":"B44","v":"nichts"}]
[{"$f":"Vokabel!$A$230","v":"5.Zeile"},"Mail:  info@ganztec.ch"]
[{"$f":"Vokabel!$A$466","v":"Schiedel Ku.Nr."}]
[]
[]
[null,{"$f":"Vokabel!$A$247","v":"Sachbearbeiter:"},{"$f":"Vokabel!$A$248","v":"Pers.-Nr."},null,{"$f":"Vokabel!$A$249","v":"Frachteinstellungen:"}]
[{"$f":"Vokabel!$A$250","v":"Vorname/Name"},"Herr Mustermann",null,null,63,{"$f":"Vokabel!$A$256","v":"CHF per Tonne"}]
[{"$f":"Vokabel!$A$251","v":"Telefon"},"Tel. 000000",{"$f":"Eingabe!$K$4&\"  \"&Eingabe!$K$16&\" \"&Eingabe!$L$18","v":"Ganztec AG   "}]
[{"$f":"Vokabel!$A$252","v":"Fax"},"Fax. 0000000"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[3,{"$f":"INDEX(Firma!B46:B48,A44,1)","v":"nichts"}]
["Mailprogramm"]
["Outlook (Express)","Outlook"]
["Lotus Notes","Lotus"]
["keines von Beiden","nichts"]

{"sheet":"Belegart","index":25,"n_rows":6,"n_cols":2,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
[2,{"$f":"INDEX(A4:A8,A1,1)","v":"Angebot"}]
[]
["Belegart:"]
[{"$f":"Vokabel!$A$182","v":"Kalkulation"}]
[{"$f":"Vokabel!$A$183","v":"Angebot"}]
[{"$f":"Vokabel!$A$184","v":"Auftragsbestätigung"}]

{"sheet":"Kalkulation","index":26,"n_rows":228,"n_cols":18,"rows_kept":228,"cut":false,"hidden":true,"merged":[[230,1,230,8],[3,12,4,12],[3,11,4,11]]}
[null,{"$f":"IF(Firma!$B$5=\"\",\"\",Firma!$B$5)","v":"Ganztec AG"},null,0,null,null,null,null,null,null,{"$f":"Firma!$B$10","v":0}]
[null,{"$f":"IF(Firma!$B$6=\"\",\"\",Firma!$B$6)","v":"Badstrasse 38"},null,null,null,null,null,null,null,null,{"$f":"Commercant!$B$10","v":0}]
[null,{"$f":"IF(Firma!$B$7=\"\",\"\",Firma!$B$7)","v":"5312 Döttingen"},null,null,null,null,null,null,null,null,{"$f":"Commerciante!$B$10","v":0}]
[null,{"$f":"IF(Firma!$B$8=\"\",\"\",Firma!$B$8)","v":"Tel. 0562680000   Fax. 0562680001"},null,null,null,null,null,null,null,null,{"$f":"IF(Eingabe!$J$1=1,Kalkulation!$K$1,IF(Eingabe!$J$1=2,Kalkulation!$K$2,IF(Eingabe!$J$1=3,Kalkulation!$K$3,\"\")))","v":0}]
[null,{"$f":"IF(Firma!B9=\"\",\"\",Firma!B9)","v":"Mail:  info@ganztec.ch"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Belegart!B1","v":"Angebot"}]
[null,{"$f":"Eingabe!$K$4","v":"Ganztec AG"},null,null,null,null,{"$f":"IF(J7=\"\",\"\",\"Beleg Nr.:\")","v":""},null,null,{"$f":"IF(Eingabe!M27=\"\",\"\",Eingabe!M27)","v":""}]
[null,{"$f":"Eingabe!$K$5","v":""},null,null,null,null,{"$f":"Vokabel!$A$185","v":"Datum :"},null,null,{"$f":"TODAY()","v":"2023-01-09"}]
[null,{"$f":"Eingabe!$K$6","v":"Badstrasse 38"},null,null,null,null,{"$f":"IF(Firma!$B$14=\"\",\"\",Vokabel!$A$186)","v":"Sachbearbeiter:"},null,null,{"$f":"IF(Firma!$B$14=\"\",\"\",Firma!$B$14)","v":"Herr Mustermann"}]
[null,{"$f":"Eingabe!$K$7&\"  \"&Eingabe!$L$7","v":"5312  Döttingen"},null,null,null,null,{"$f":"IF(Firma!$B$15=\"\",\"\",Vokabel!$A$187)","v":"Tel.Nr.:"},null,null,{"$f":"IF(Firma!$B$15=\"\",\"\",Firma!$B$15)","v":"Tel. 000000"},{"$f":"IF(Firma!$C$14=\"\",Firma!$C$15,Firma!C$14&\" \"&Firma!$C$15)","v":"Ganztec AG   "}]
[null,null,null,null,null,null,{"$f":"IF(Firma!$B$16=\"\",\"\",Vokabel!$A$188)","v":"Fax.Nr.:"},null,null,{"$f":"IF(Firma!$B$16=\"\",\"\",Firma!$B$16)","v":"Fax. 0000000"}]
[null,{"$f":"IF(Eingabe!$N$11=\"\",\"\",Vokabel!$A$223&\":\")","v":""},{"$f":"Eingabe!$N$11","v":0}]
[null,{"$f":"IF(Eingabe!K9=\"\",\"\",Vokabel!$A$180&\"  \"&Eingabe!K9&\" \")","v":""},null,null,null,null,{"$f":"IF(Eingabe!$K$16=\"\",\"\",Vokabel!$A$189)","v":""},null,null,{"$f":"IF(Eingabe!$K$16=\"\",\"\",Eingabe!$K$16)","v":""}]
[null,{"$f":"IF(Eingabe!$K$11=\"\",\"\",\"Tel. \"&Eingabe!$K$11)&IF(Eingabe!$K$13=\"\",\"\",\"  - Fax. \"&Eingabe!$K$13 )&IF(Eingabe!$N$13=\"\",\"\",\" - \"&Vokabel!$A$222&\" \"&Eingabe!$N$13 )","v":""},null,null,null,null,null,null,null,{"$f":"IF(Eingabe!$K$17=\"\",\"\",Eingabe!$K$17)","v":""}]
[null,{"$f":"IF(Belegart!$B$1=\"Auftragsbestätigung\",\"\",IF(Belegart!$B$1=\"Kalkulation\",\"\",Texte!$D$12))","v":""},null,null,null,null,null,null,null,{"$f":"IF(Eingabe!$K$18=\"\",\"\",Eingabe!$K$18&\"  \"&Eingabe!$L$18)","v":""}]
[null,{"$f":"IF(Belegart!$B$1=\"Auftragsbestätigung\",\"\",IF(Belegart!$B$1=\"Kalkulation\",\"\",IF($B$15=\"\",Texte!$D$15,Texte!$D$13)))","v":"Wir bedanken uns für Ihre Anfrage und bieten Ihnen folgendes an:"}]
["ABSOLUT","Schiedel ABSOLUT, ABS 18",null,"Mehrschaliges feuchteunempfindliches Kaminsystem"]
[null,"Aussenmass: 36/36 cm",null,"mit integrierter Wärmedämmung"]
[null,null,null,"und keramischem Profil-Innenrohr"]
[]
[null,{"$f":"IF($A$17=\"ABSOLUT\",\"\",IF($A$17=\"Cheminee\",\"\",IF($A$17=\"ISOLIT\",\"\",IF($A$17=\"Kerastar\",\"\",Vokabel!$A$96))))","v":""},{"$f":"IF($B$21=\"\",\"\",IF($A$17=\"Prima Plus\",Daten!$C$644,IF($A$17=\"Technostar120\",Daten!$C$721,IF($A$17=\"ICS5000\",Daten!$C$721,Daten!$C$564))))","v":""},{"$f":"Vokabel!$A$190","v":"Anlagenhöhe:"},null,{"$f":"IF($A$17=\"Absolut\",Daten!$B$61,IF($A$17=\"Cheminee\",Daten!$B$61,SUBTOTAL(9,E25:E154)/1000))&\" m\"","v":"9 m"},"",null,null,null,{"$f":"IF(A17=\"Absolut\",F21,IF(A17=\"SIH\",F21,IF(A17=\"Absolut Komplett\",F21,\"\")))","v":"9 m"}]
[null,{"$f":"IF($C$22=\"\",\"\",Vokabel!$A$75)","v":""},{"$f":"IF(A17=\"ABSOLUT\",\"\",IF(A17=\"Cheminee\",\"\",IF(A17=\"Keranova\",Daten!$C$582,IF(A17=\"Technostar120\",Daten!$G$705,IF(A17=\"Kerastar\",Daten!$C$390,IF(A17=\"Prima Plus\",Daten!$F$644,IF(A17=\"ICS\",Daten!$F$490,\"\")))))))","v":""},{"$f":"Vokabel!$A$191","v":"Gesamtgewicht:"},null,{"$f":"SUBTOTAL(9,D25:D170)&\" kg\"","v":"749,11 kg"}]
[]
["Nr",{"$f":"Vokabel!$A$192","v":"Artikel-Nr."},{"$f":"Vokabel!$A$194","v":"Bezeichung"},{"$f":"Vokabel!$A$195","v":"Gewicht                                           kg"},{"$f":"Vokabel!$A$196","v":"Bauhöhe  mm"},{"$f":"Vokabel!$A$197","v":"Menge"},"EH","RK",{"$f":"Vokabel!$A$199","v":"Einzelpreis CHF"},{"$f":"Vokabel!$A$200","v":"Gesamtpreis CHF"}]
[0,"103912",{"$f":"IF(B25=\"\",\"\",VLOOKUP(B25,sanschie!A:E,5,0))","v":"ABS Mantelstein EZ 360 x 360mm L330mm"},{"$f":"IF(F25=\"\",\"\",K25*F25)","v":494.73},{"$f":"IF(F25=\"\",\"\",IF(N25=\"\",\"\",N25*F25))","v":0},23,{"$f":"IF(B25=\"\",\"\",VLOOKUP(B25,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B25=\"\",\"\",VLOOKUP(B25,sanschie!A:P,16,0))","v":1},{"$f":"IF(B25=\"\",\"\",IF(H25=\"N\",VLOOKUP(B25,sanschie!$A:$K,7,0),VLOOKUP(B25,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":30},{"$f":"IF(F25=\"\",\"\",(F25*I25))","v":690},{"$f":"IF(B25=\"\",\"\",VLOOKUP(B25,sanschie!$A:$I,9,0))","v":21.51},{"$f":"IF(H25=1,J25,0)","v":690},{"$f":"IF(H25=2,J25,0)","v":0},{"$f":"IF(B25=\"\",\"0\",IF(VLOOKUP(B25,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B25,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B25,sanschie!$A:$K,10,0)))))","v":"0"},null,null,{"$f":"IF(H25=3,J25,0)","v":0},{"$f":"IF(B25=\"\",\"\",IF(H25=\"N\",VLOOKUP(B25,sanschie!$A:$K,7,0),VLOOKUP(B25,sanschie!$A:$K,7,0)))","v":30}]
[0,"103931",{"$f":"IF(B26=\"\",\"\",VLOOKUP(B26,sanschie!A:E,5,0))","v":"ABS Thermo-Trennstein EZ 360 x 360mm L330mm"},"","","",{"$f":"IF(B26=\"\",\"\",VLOOKUP(B26,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B26=\"\",\"\",VLOOKUP(B26,sanschie!A:P,16,0))","v":1},{"$f":"IF(B26=\"\",\"\",IF(H26=\"N\",VLOOKUP(B26,sanschie!$A:$K,7,0),VLOOKUP(B26,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":210},"",{"$f":"IF(B26=\"\",\"\",VLOOKUP(B26,sanschie!$A:$I,9,0))","v":20.7},"",0,{"$f":"IF(B26=\"\",\"0\",IF(VLOOKUP(B26,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B26,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B26,sanschie!$A:$K,10,0)))))","v":"0"},null,null,{"$f":"IF(H26=3,J26,0)","v":0},{"$f":"IF(B26=\"\",\"\",IF(H26=\"N\",VLOOKUP(B26,sanschie!$A:$K,7,0),VLOOKUP(B26,sanschie!$A:$K,7,0)))","v":210}]
[0,"103849",{"$f":"IF(B27=\"\",\"\",VLOOKUP(B27,sanschie!A:E,5,0))","v":"ABS Thermo-Fussplatte EZ 360 x 360mm"},"","","",{"$f":"IF(B27=\"\",\"\",VLOOKUP(B27,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B27=\"\",\"\",VLOOKUP(B27,sanschie!A:P,16,0))","v":1},{"$f":"IF(B27=\"\",\"\",IF(H27=\"N\",VLOOKUP(B27,sanschie!$A:$K,7,0),VLOOKUP(B27,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":124},"",{"$f":"IF(B27=\"\",\"\",VLOOKUP(B27,sanschie!$A:$I,9,0))","v":2.16},"",0,{"$f":"IF(B27=\"\",\"0\",IF(VLOOKUP(B27,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B27,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B27,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B27=\"\",\"\",IF(H27=\"N\",VLOOKUP(B27,sanschie!$A:$K,7,0),VLOOKUP(B27,sanschie!$A:$K,7,0)))","v":124}]
[0,"103948",{"$f":"IF(B28=\"\",\"\",VLOOKUP(B28,sanschie!A:E,5,0))","v":"ABS 180 Profilkeramik-Rohr mit Muffe L1330mm"},61.5,6650,5,{"$f":"IF(B28=\"\",\"\",VLOOKUP(B28,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B28=\"\",\"\",VLOOKUP(B28,sanschie!A:P,16,0))","v":1},{"$f":"IF(B28=\"\",\"\",IF(H28=\"N\",VLOOKUP(B28,sanschie!$A:$K,7,0),VLOOKUP(B28,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":122},610,{"$f":"IF(B28=\"\",\"\",VLOOKUP(B28,sanschie!$A:$I,9,0))","v":12.3},610,0,{"$f":"IF(B28=\"\",\"0\",IF(VLOOKUP(B28,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B28,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B28,sanschie!$A:$K,10,0)))))","v":1330},null,null,0,{"$f":"IF(B28=\"\",\"\",IF(H28=\"N\",VLOOKUP(B28,sanschie!$A:$K,7,0),VLOOKUP(B28,sanschie!$A:$K,7,0)))","v":122}]
[0,"103859",{"$f":"IF(B29=\"\",\"\",VLOOKUP(B29,sanschie!A:E,5,0))","v":"ABS 180 Fertigfuss EZ Ø140- 180 mm  L1070mm"},93,1070,1,{"$f":"IF(B29=\"\",\"\",VLOOKUP(B29,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B29=\"\",\"\",VLOOKUP(B29,sanschie!A:P,16,0))","v":1},{"$f":"IF(B29=\"\",\"\",IF(H29=\"N\",VLOOKUP(B29,sanschie!$A:$K,7,0),VLOOKUP(B29,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":611},611,{"$f":"IF(B29=\"\",\"\",VLOOKUP(B29,sanschie!$A:$I,9,0))","v":93},611,0,{"$f":"IF(B29=\"\",\"0\",IF(VLOOKUP(B29,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B29,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B29,sanschie!$A:$K,10,0)))))","v":1070},null,null,0,{"$f":"IF(B29=\"\",\"\",IF(H29=\"N\",VLOOKUP(B29,sanschie!$A:$K,7,0),VLOOKUP(B29,sanschie!$A:$K,7,0)))","v":611}]
[0,"103953",{"$f":"IF(B30=\"\",\"\",VLOOKUP(B30,sanschie!A:E,5,0))","v":"ABS 180 Profilkeramik-Rohr mit Muffe L660mm"},"","","",{"$f":"IF(B30=\"\",\"\",VLOOKUP(B30,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B30=\"\",\"\",VLOOKUP(B30,sanschie!A:P,16,0))","v":1},{"$f":"IF(B30=\"\",\"\",IF(H30=\"N\",VLOOKUP(B30,sanschie!$A:$K,7,0),VLOOKUP(B30,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":69},"",{"$f":"IF(B30=\"\",\"\",VLOOKUP(B30,sanschie!$A:$I,9,0))","v":5.9},"",0,{"$f":"IF(B30=\"\",\"0\",IF(VLOOKUP(B30,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B30,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B30,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B30=\"\",\"\",IF(H30=\"N\",VLOOKUP(B30,sanschie!$A:$K,7,0),VLOOKUP(B30,sanschie!$A:$K,7,0)))","v":69}]
[0,"103891",{"$f":"IF(B31=\"\",\"\",VLOOKUP(B31,sanschie!A:E,5,0))","v":"ABS 180 Fertigfusspaket "},6.9,0,1,{"$f":"IF(B31=\"\",\"\",VLOOKUP(B31,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B31=\"\",\"\",VLOOKUP(B31,sanschie!A:P,16,0))","v":1},{"$f":"IF(B31=\"\",\"\",IF(H31=\"N\",VLOOKUP(B31,sanschie!$A:$K,7,0),VLOOKUP(B31,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":311},311,{"$f":"IF(B31=\"\",\"\",VLOOKUP(B31,sanschie!$A:$I,9,0))","v":6.9},311,0,{"$f":"IF(B31=\"\",\"0\",IF(VLOOKUP(B31,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B31,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B31,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B31=\"\",\"\",IF(H31=\"N\",VLOOKUP(B31,sanschie!$A:$K,7,0),VLOOKUP(B31,sanschie!$A:$K,7,0)))","v":311}]
[0,"103709",{"$f":"IF(B32=\"\",\"\",VLOOKUP(B32,sanschie!A:E,5,0))","v":"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm"},"","","",{"$f":"IF(B32=\"\",\"\",VLOOKUP(B32,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B32=\"\",\"\",VLOOKUP(B32,sanschie!A:P,16,0))","v":1},{"$f":"IF(B32=\"\",\"\",IF(H32=\"N\",VLOOKUP(B32,sanschie!$A:$K,7,0),VLOOKUP(B32,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":18},"",{"$f":"IF(B32=\"\",\"\",VLOOKUP(B32,sanschie!$A:$I,9,0))","v":4},"",0,{"$f":"IF(B32=\"\",\"0\",IF(VLOOKUP(B32,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B32,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B32,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B32=\"\",\"\",IF(H32=\"N\",VLOOKUP(B32,sanschie!$A:$K,7,0),VLOOKUP(B32,sanschie!$A:$K,7,0)))","v":18}]
[0,"103700",{"$f":"IF(B33=\"\",\"\",VLOOKUP(B33,sanschie!A:E,5,0))","v":"CHZ 180 Keramik Fuss-Scheibe geschlossen"},"","","",{"$f":"IF(B33=\"\",\"\",VLOOKUP(B33,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B33=\"\",\"\",VLOOKUP(B33,sanschie!A:P,16,0))","v":1},{"$f":"IF(B33=\"\",\"\",IF(H33=\"N\",VLOOKUP(B33,sanschie!$A:$K,7,0),VLOOKUP(B33,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":35},"",{"$f":"IF(B33=\"\",\"\",VLOOKUP(B33,sanschie!$A:$I,9,0))","v":2},"",0,{"$f":"IF(B33=\"\",\"0\",IF(VLOOKUP(B33,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B33,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B33,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B33=\"\",\"\",IF(H33=\"N\",VLOOKUP(B33,sanschie!$A:$K,7,0),VLOOKUP(B33,sanschie!$A:$K,7,0)))","v":35}]
[0,"103871",{"$f":"IF(B34=\"\",\"\",VLOOKUP(B34,sanschie!A:E,5,0))","v":"ABS Sockelplatte aus Beton EZ 360 x 360mm"},"","","",{"$f":"IF(B34=\"\",\"\",VLOOKUP(B34,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B34=\"\",\"\",VLOOKUP(B34,sanschie!A:P,16,0))","v":1},{"$f":"IF(B34=\"\",\"\",IF(H34=\"N\",VLOOKUP(B34,sanschie!$A:$K,7,0),VLOOKUP(B34,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":155},"",{"$f":"IF(B34=\"\",\"\",VLOOKUP(B34,sanschie!$A:$I,9,0))","v":25},"",0,{"$f":"IF(B34=\"\",\"0\",IF(VLOOKUP(B34,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B34,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B34,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B34=\"\",\"\",IF(H34=\"N\",VLOOKUP(B34,sanschie!$A:$K,7,0),VLOOKUP(B34,sanschie!$A:$K,7,0)))","v":155}]
[0,"103983",{"$f":"IF(B35=\"\",\"\",VLOOKUP(B35,sanschie!A:E,5,0))","v":"ABS 180 Rauchrohr-Anschlusspaket 90° RA  "},16.100000000000001,1330,1,{"$f":"IF(B35=\"\",\"\",VLOOKUP(B35,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B35=\"\",\"\",VLOOKUP(B35,sanschie!A:P,16,0))","v":1},{"$f":"IF(B35=\"\",\"\",IF(H35=\"N\",VLOOKUP(B35,sanschie!$A:$K,7,0),VLOOKUP(B35,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":386},386,{"$f":"IF(B35=\"\",\"\",VLOOKUP(B35,sanschie!$A:$I,9,0))","v":16.100000000000001},386,0,{"$f":"IF(B35=\"\",\"0\",IF(VLOOKUP(B35,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B35,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B35,sanschie!$A:$K,10,0)))))","v":1330},null,null,0,{"$f":"IF(B35=\"\",\"\",IF(H35=\"N\",VLOOKUP(B35,sanschie!$A:$K,7,0),VLOOKUP(B35,sanschie!$A:$K,7,0)))","v":386}]
[0,"103995",{"$f":"IF(B36=\"\",\"\",VLOOKUP(B36,sanschie!A:E,5,0))","v":"ABS 180 Rauchrohr-Anschlusspaket 45° RA  "},"","","",{"$f":"IF(B36=\"\",\"\",VLOOKUP(B36,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B36=\"\",\"\",VLOOKUP(B36,sanschie!A:P,16,0))","v":1},{"$f":"IF(B36=\"\",\"\",IF(H36=\"N\",VLOOKUP(B36,sanschie!$A:$K,7,0),VLOOKUP(B36,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":404},"",{"$f":"IF(B36=\"\",\"\",VLOOKUP(B36,sanschie!$A:$I,9,0))","v":17.2},"",0,{"$f":"IF(B36=\"\",\"0\",IF(VLOOKUP(B36,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B36,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B36,sanschie!$A:$K,10,0)))))","v":1330},null,null,0,{"$f":"IF(B36=\"\",\"\",IF(H36=\"N\",VLOOKUP(B36,sanschie!$A:$K,7,0),VLOOKUP(B36,sanschie!$A:$K,7,0)))","v":404}]
[0,"104001",{"$f":"IF(B37=\"\",\"\",VLOOKUP(B37,sanschie!A:E,5,0))","v":"ABS 180  Rauchrohranschluss Stutzen-Set 90° Ø180mm"},"","","",{"$f":"IF(B37=\"\",\"\",VLOOKUP(B37,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B37=\"\",\"\",VLOOKUP(B37,sanschie!A:P,16,0))","v":1},{"$f":"IF(B37=\"\",\"\",IF(H37=\"N\",VLOOKUP(B37,sanschie!$A:$K,7,0),VLOOKUP(B37,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":204},"",{"$f":"IF(B37=\"\",\"\",VLOOKUP(B37,sanschie!$A:$I,9,0))","v":4.0999999999999996},"",0,{"$f":"IF(B37=\"\",\"0\",IF(VLOOKUP(B37,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B37,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B37,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B37=\"\",\"\",IF(H37=\"N\",VLOOKUP(B37,sanschie!$A:$K,7,0),VLOOKUP(B37,sanschie!$A:$K,7,0)))","v":204}]
[0,"104007",{"$f":"IF(B38=\"\",\"\",VLOOKUP(B38,sanschie!A:E,5,0))","v":"ABS 180 Rauchrohranschluss Stutzen-Set 45°"},"","","",{"$f":"IF(B38=\"\",\"\",VLOOKUP(B38,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B38=\"\",\"\",VLOOKUP(B38,sanschie!A:P,16,0))","v":1},{"$f":"IF(B38=\"\",\"\",IF(H38=\"N\",VLOOKUP(B38,sanschie!$A:$K,7,0),VLOOKUP(B38,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":204},"",{"$f":"IF(B38=\"\",\"\",VLOOKUP(B38,sanschie!$A:$I,9,0))","v":5.17},"",0,{"$f":"IF(B38=\"\",\"0\",IF(VLOOKUP(B38,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B38,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B38,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B38=\"\",\"\",IF(H38=\"N\",VLOOKUP(B38,sanschie!$A:$K,7,0),VLOOKUP(B38,sanschie!$A:$K,7,0)))","v":204}]
[0,"104268",{"$f":"IF(B39=\"\",\"\",VLOOKUP(B39,sanschie!A:E,5,0))","v":"ABS 180 Steckadapter "},"","","",{"$f":"IF(B39=\"\",\"\",VLOOKUP(B39,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B39=\"\",\"\",VLOOKUP(B39,sanschie!A:P,16,0))","v":1},{"$f":"IF(B39=\"\",\"\",IF(H39=\"N\",VLOOKUP(B39,sanschie!$A:$K,7,0),VLOOKUP(B39,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":173},"",{"$f":"IF(B39=\"\",\"\",VLOOKUP(B39,sanschie!$A:$I,9,0))","v":0.33800000000000002},"",0,{"$f":"IF(B39=\"\",\"0\",IF(VLOOKUP(B39,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B39,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B39,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B39=\"\",\"\",IF(H39=\"N\",VLOOKUP(B39,sanschie!$A:$K,7,0),VLOOKUP(B39,sanschie!$A:$K,7,0)))","v":173}]
[0,"103966",{"$f":"IF(B40=\"\",\"\",VLOOKUP(B40,sanschie!A:E,5,0))","v":"ABS 180 Putztür-Anschlusspaket "},"","","",{"$f":"IF(B40=\"\",\"\",VLOOKUP(B40,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B40=\"\",\"\",VLOOKUP(B40,sanschie!A:P,16,0))","v":1},{"$f":"IF(B40=\"\",\"\",IF(H40=\"N\",VLOOKUP(B40,sanschie!$A:$K,7,0),VLOOKUP(B40,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":448},"",{"$f":"IF(B40=\"\",\"\",VLOOKUP(B40,sanschie!$A:$I,9,0))","v":19.309999999999999},"",0,{"$f":"IF(B40=\"\",\"0\",IF(VLOOKUP(B40,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B40,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B40,sanschie!$A:$K,10,0)))))","v":1330},null,null,0,{"$f":"IF(B40=\"\",\"\",IF(H40=\"N\",VLOOKUP(B40,sanschie!$A:$K,7,0),VLOOKUP(B40,sanschie!$A:$K,7,0)))","v":448}]
[0,"104274",{"$f":"IF(B41=\"\",\"\",VLOOKUP(B41,sanschie!A:E,5,0))","v":"ABS 180 Putztüranschluss Stutzen Set"},"","","",{"$f":"IF(B41=\"\",\"\",VLOOKUP(B41,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B41=\"\",\"\",VLOOKUP(B41,sanschie!A:P,16,0))","v":1},{"$f":"IF(B41=\"\",\"\",IF(H41=\"N\",VLOOKUP(B41,sanschie!$A:$K,7,0),VLOOKUP(B41,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":336},"",{"$f":"IF(B41=\"\",\"\",VLOOKUP(B41,sanschie!$A:$I,9,0))","v":5.0999999999999996},"",0,{"$f":"IF(B41=\"\",\"0\",IF(VLOOKUP(B41,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B41,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B41,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B41=\"\",\"\",IF(H41=\"N\",VLOOKUP(B41,sanschie!$A:$K,7,0),VLOOKUP(B41,sanschie!$A:$K,7,0)))","v":336}]
[0,"104243",{"$f":"IF(B42=\"\",\"\",VLOOKUP(B42,sanschie!A:E,5,0))","v":"ABS Dichtset zu Putztüre Typ 3"},"","","",{"$f":"IF(B42=\"\",\"\",VLOOKUP(B42,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B42=\"\",\"\",VLOOKUP(B42,sanschie!A:P,16,0))","v":1},{"$f":"IF(B42=\"\",\"\",IF(H42=\"N\",VLOOKUP(B42,sanschie!$A:$K,7,0),VLOOKUP(B42,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":27},"",{"$f":"IF(B42=\"\",\"\",VLOOKUP(B42,sanschie!$A:$I,9,0))","v":0.2},"",0,{"$f":"IF(B42=\"\",\"0\",IF(VLOOKUP(B42,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B42,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B42,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B42=\"\",\"\",IF(H42=\"N\",VLOOKUP(B42,sanschie!$A:$K,7,0),VLOOKUP(B42,sanschie!$A:$K,7,0)))","v":27}]
[0,"104190",{"$f":"IF(B43=\"\",\"\",VLOOKUP(B43,sanschie!A:E,5,0))","v":"ABS Thermodichtset EZ 360x360mm und 380x380mm"},"","","",{"$f":"IF(B43=\"\",\"\",VLOOKUP(B43,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B43=\"\",\"\",VLOOKUP(B43,sanschie!A:P,16,0))","v":1},{"$f":"IF(B43=\"\",\"\",IF(H43=\"N\",VLOOKUP(B43,sanschie!$A:$K,7,0),VLOOKUP(B43,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":309},"",{"$f":"IF(B43=\"\",\"\",VLOOKUP(B43,sanschie!$A:$I,9,0))","v":2},"",0,{"$f":"IF(B43=\"\",\"0\",IF(VLOOKUP(B43,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B43,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B43,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B43=\"\",\"\",IF(H43=\"N\",VLOOKUP(B43,sanschie!$A:$K,7,0),VLOOKUP(B43,sanschie!$A:$K,7,0)))","v":309}]
[0,"104144",{"$f":"IF(B44=\"\",\"\",VLOOKUP(B44,sanschie!A:E,5,0))","v":"ABS Handyplatte EZ Faserzement 360 x 360mm"},14.4,0,1,{"$f":"IF(B44=\"\",\"\",VLOOKUP(B44,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B44=\"\",\"\",VLOOKUP(B44,sanschie!A:P,16,0))","v":1},{"$f":"IF(B44=\"\",\"\",IF(H44=\"N\",VLOOKUP(B44,sanschie!$A:$K,7,0),VLOOKUP(B44,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":106},106,{"$f":"IF(B44=\"\",\"\",VLOOKUP(B44,sanschie!$A:$I,9,0))","v":14.4},106,0,{"$f":"IF(B44=\"\",\"0\",IF(VLOOKUP(B44,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B44,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B44,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B44=\"\",\"\",IF(H44=\"N\",VLOOKUP(B44,sanschie!$A:$K,7,0),VLOOKUP(B44,sanschie!$A:$K,7,0)))","v":106}]
[0,"104170",{"$f":"IF(B45=\"\",\"\",VLOOKUP(B45,sanschie!A:E,5,0))","v":"ABS Handyplatte EZ Inox 360 x 360mm  "},"","","",{"$f":"IF(B45=\"\",\"\",VLOOKUP(B45,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B45=\"\",\"\",VLOOKUP(B45,sanschie!A:P,16,0))","v":1},{"$f":"IF(B45=\"\",\"\",IF(H45=\"N\",VLOOKUP(B45,sanschie!$A:$K,7,0),VLOOKUP(B45,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":155},"",{"$f":"IF(B45=\"\",\"\",VLOOKUP(B45,sanschie!$A:$I,9,0))","v":3.4},"",0,{"$f":"IF(B45=\"\",\"0\",IF(VLOOKUP(B45,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B45,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B45,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B45=\"\",\"\",IF(H45=\"N\",VLOOKUP(B45,sanschie!$A:$K,7,0),VLOOKUP(B45,sanschie!$A:$K,7,0)))","v":155}]
[0,"104162",{"$f":"IF(B46=\"\",\"\",VLOOKUP(B46,sanschie!A:E,5,0))","v":"ABS HEB-Set zu Handyplatte aus Faserzement"},0.77,0,1,{"$f":"IF(B46=\"\",\"\",VLOOKUP(B46,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B46=\"\",\"\",VLOOKUP(B46,sanschie!A:P,16,0))","v":1},{"$f":"IF(B46=\"\",\"\",IF(H46=\"N\",VLOOKUP(B46,sanschie!$A:$K,7,0),VLOOKUP(B46,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":34},34,{"$f":"IF(B46=\"\",\"\",VLOOKUP(B46,sanschie!$A:$I,9,0))","v":0.77},34,0,{"$f":"IF(B46=\"\",\"0\",IF(VLOOKUP(B46,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B46,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B46,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B46=\"\",\"\",IF(H46=\"N\",VLOOKUP(B46,sanschie!$A:$K,7,0),VLOOKUP(B46,sanschie!$A:$K,7,0)))","v":34}]
[0,"104175",{"$f":"IF(B47=\"\",\"\",VLOOKUP(B47,sanschie!A:E,5,0))","v":"ABS HEB-Set zu Handyplatte EZ Inox "},"","","",{"$f":"IF(B47=\"\",\"\",VLOOKUP(B47,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B47=\"\",\"\",VLOOKUP(B47,sanschie!A:P,16,0))","v":1},{"$f":"IF(B47=\"\",\"\",IF(H47=\"N\",VLOOKUP(B47,sanschie!$A:$K,7,0),VLOOKUP(B47,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":34},"",{"$f":"IF(B47=\"\",\"\",VLOOKUP(B47,sanschie!$A:$I,9,0))","v":0.77},"",0,{"$f":"IF(B47=\"\",\"0\",IF(VLOOKUP(B47,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B47,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B47,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B47=\"\",\"\",IF(H47=\"N\",VLOOKUP(B47,sanschie!$A:$K,7,0),VLOOKUP(B47,sanschie!$A:$K,7,0)))","v":34}]
[0,"140787",{"$f":"IF(B48=\"\",\"\",VLOOKUP(B48,sanschie!A:E,5,0))","v":"ABS Handyplatte EZ Kupfer 360 x 360mm  "},"","","",{"$f":"IF(B48=\"\",\"\",VLOOKUP(B48,sanschie!A:D,4,0))","v":"Stk"},{"$f":"IF(B48=\"\",\"\",VLOOKUP(B48,sanschie!A:P,16,0))","v":0},{"$f":"IF(B48=\"\",\"\",IF(H48=\"N\",VLOOKUP(B48,sanschie!$A:$K,7,0),VLOOKUP(B48,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":229},"",{"$f":"IF(B48=\"\",\"\",VLOOKUP(B48,sanschie!$A:$I,9,0))","v":3.4},0,0,{"$f":"IF(B48=\"\",\"0\",IF(VLOOKUP(B48,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B48,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B48,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B48=\"\",\"\",IF(H48=\"N\",VLOOKUP(B48,sanschie!$A:$K,7,0),VLOOKUP(B48,sanschie!$A:$K,7,0)))","v":229}]
[0,"140932",{"$f":"IF(B49=\"\",\"\",VLOOKUP(B49,sanschie!A:E,5,0))","v":"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben"},"","","",{"$f":"IF(B49=\"\",\"\",VLOOKUP(B49,sanschie!A:D,4,0))","v":"Stk"},{"$f":"IF(B49=\"\",\"\",VLOOKUP(B49,sanschie!A:P,16,0))","v":0},{"$f":"IF(B49=\"\",\"\",IF(H49=\"N\",VLOOKUP(B49,sanschie!$A:$K,7,0),VLOOKUP(B49,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":75},"",{"$f":"IF(B49=\"\",\"\",VLOOKUP(B49,sanschie!$A:$I,9,0))","v":7.0000000000000007E-2},0,0,{"$f":"IF(B49=\"\",\"0\",IF(VLOOKUP(B49,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B49,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B49,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B49=\"\",\"\",IF(H49=\"N\",VLOOKUP(B49,sanschie!$A:$K,7,0),VLOOKUP(B49,sanschie!$A:$K,7,0)))","v":75}]
[0,"104206",{"$f":"IF(B50=\"\",\"\",VLOOKUP(B50,sanschie!A:E,5,0))","v":"ABS 180 Abströmkonus verkupfert"},"","","",{"$f":"IF(B50=\"\",\"\",VLOOKUP(B50,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B50=\"\",\"\",VLOOKUP(B50,sanschie!A:P,16,0))","v":1},{"$f":"IF(B50=\"\",\"\",IF(H50=\"N\",VLOOKUP(B50,sanschie!$A:$K,7,0),VLOOKUP(B50,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":174},"",{"$f":"IF(B50=\"\",\"\",VLOOKUP(B50,sanschie!$A:$I,9,0))","v":1},"",0,{"$f":"IF(B50=\"\",\"0\",IF(VLOOKUP(B50,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B50,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B50,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B50=\"\",\"\",IF(H50=\"N\",VLOOKUP(B50,sanschie!$A:$K,7,0),VLOOKUP(B50,sanschie!$A:$K,7,0)))","v":174}]
[0,"103917",{"$f":"IF(B51=\"\",\"\",VLOOKUP(B51,sanschie!A:E,5,0))","v":"ABS Anschlussmantelstein EZ 360 x 360mm L330"},21.51,0,1,{"$f":"IF(B51=\"\",\"\",VLOOKUP(B51,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B51=\"\",\"\",VLOOKUP(B51,sanschie!A:P,16,0))","v":1},{"$f":"IF(B51=\"\",\"\",IF(H51=\"N\",VLOOKUP(B51,sanschie!$A:$K,7,0),VLOOKUP(B51,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":80},80,{"$f":"IF(B51=\"\",\"\",VLOOKUP(B51,sanschie!$A:$I,9,0))","v":21.51},80,0,{"$f":"IF(B51=\"\",\"0\",IF(VLOOKUP(B51,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B51,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B51,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B51=\"\",\"\",IF(H51=\"N\",VLOOKUP(B51,sanschie!$A:$K,7,0),VLOOKUP(B51,sanschie!$A:$K,7,0)))","v":80}]
[0,"104059",{"$f":"IF(B52=\"\",\"\",VLOOKUP(B52,sanschie!A:E,5,0))","v":"ABS 180 Schleifung EZ 5° auf Bestellung"},"","","",{"$f":"IF(B52=\"\",\"\",VLOOKUP(B52,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B52=\"\",\"\",VLOOKUP(B52,sanschie!A:P,16,0))","v":1},{"$f":"IF(B52=\"\",\"\",IF(H52=\"N\",VLOOKUP(B52,sanschie!$A:$K,7,0),VLOOKUP(B52,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":1010},"",{"$f":"IF(B52=\"\",\"\",VLOOKUP(B52,sanschie!$A:$I,9,0))","v":25},"",0,{"$f":"IF(B52=\"\",\"0\",IF(VLOOKUP(B52,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B52,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B52,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B52=\"\",\"\",IF(H52=\"N\",VLOOKUP(B52,sanschie!$A:$K,7,0),VLOOKUP(B52,sanschie!$A:$K,7,0)))","v":1010}]
[0,"104083",{"$f":"IF(B53=\"\",\"\",VLOOKUP(B53,sanschie!A:E,5,0))","v":"ABS 180 Abstandhalter offen zu Schleifung"},"","","",{"$f":"IF(B53=\"\",\"\",VLOOKUP(B53,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B53=\"\",\"\",VLOOKUP(B53,sanschie!A:P,16,0))","v":1},{"$f":"IF(B53=\"\",\"\",IF(H53=\"N\",VLOOKUP(B53,sanschie!$A:$K,7,0),VLOOKUP(B53,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":27},"",{"$f":"IF(B53=\"\",\"\",VLOOKUP(B53,sanschie!$A:$I,9,0))","v":0.1},"",0,{"$f":"IF(B53=\"\",\"0\",IF(VLOOKUP(B53,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B53,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B53,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B53=\"\",\"\",IF(H53=\"N\",VLOOKUP(B53,sanschie!$A:$K,7,0),VLOOKUP(B53,sanschie!$A:$K,7,0)))","v":27}]
[0,"103899",{"$f":"IF(B54=\"\",\"\",VLOOKUP(B54,sanschie!A:E,5,0))","v":"ABS 180 Anschlusskonus EZ mit Doppelfutter DN180mm"},"","","",{"$f":"IF(B54=\"\",\"\",VLOOKUP(B54,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B54=\"\",\"\",VLOOKUP(B54,sanschie!A:P,16,0))","v":1},{"$f":"IF(B54=\"\",\"\",IF(H54=\"N\",VLOOKUP(B54,sanschie!$A:$K,7,0),VLOOKUP(B54,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":266},"",{"$f":"IF(B54=\"\",\"\",VLOOKUP(B54,sanschie!$A:$I,9,0))","v":25},"",0,{"$f":"IF(B54=\"\",\"0\",IF(VLOOKUP(B54,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B54,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B54,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B54=\"\",\"\",IF(H54=\"N\",VLOOKUP(B54,sanschie!$A:$K,7,0),VLOOKUP(B54,sanschie!$A:$K,7,0)))","v":266}]
[0,"103907",{"$f":"IF(B55=\"\",\"\",VLOOKUP(B55,sanschie!A:E,5,0))","v":"ABS 180 Adapterring von 180mm auf 180mm L90mm"},"","","",{"$f":"IF(B55=\"\",\"\",VLOOKUP(B55,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B55=\"\",\"\",VLOOKUP(B55,sanschie!A:P,16,0))","v":1},{"$f":"IF(B55=\"\",\"\",IF(H55=\"N\",VLOOKUP(B55,sanschie!$A:$K,7,0),VLOOKUP(B55,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":46},"",{"$f":"IF(B55=\"\",\"\",VLOOKUP(B55,sanschie!$A:$I,9,0))","v":2.5},"",0,{"$f":"IF(B55=\"\",\"0\",IF(VLOOKUP(B55,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B55,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B55,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B55=\"\",\"\",IF(H55=\"N\",VLOOKUP(B55,sanschie!$A:$K,7,0),VLOOKUP(B55,sanschie!$A:$K,7,0)))","v":46}]
[0,"103474",{"$f":"IF(B56=\"\",\"\",VLOOKUP(B56,sanschie!A:E,5,0))","v":"KER 180  Keranova-Fugenglätter"},"","","",{"$f":"IF(B56=\"\",\"\",VLOOKUP(B56,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B56=\"\",\"\",VLOOKUP(B56,sanschie!A:P,16,0))","v":1},{"$f":"IF(B56=\"\",\"\",IF(H56=\"N\",VLOOKUP(B56,sanschie!$A:$K,7,0),VLOOKUP(B56,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":61},"",{"$f":"IF(B56=\"\",\"\",VLOOKUP(B56,sanschie!$A:$I,9,0))","v":0.45200000000000001},"",0,{"$f":"IF(B56=\"\",\"0\",IF(VLOOKUP(B56,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B56,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B56,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B56=\"\",\"\",IF(H56=\"N\",VLOOKUP(B56,sanschie!$A:$K,7,0),VLOOKUP(B56,sanschie!$A:$K,7,0)))","v":61}]
[0,"104014",{"$f":"IF(B57=\"\",\"\",VLOOKUP(B57,sanschie!A:E,5,0))","v":"ABS 180 Doppelfutter zu Rauchrohranschluss Ø100mm"},"","","",{"$f":"IF(B57=\"\",\"\",VLOOKUP(B57,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B57=\"\",\"\",VLOOKUP(B57,sanschie!A:P,16,0))","v":1},{"$f":"IF(B57=\"\",\"\",IF(H57=\"N\",VLOOKUP(B57,sanschie!$A:$K,7,0),VLOOKUP(B57,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":149},"",{"$f":"IF(B57=\"\",\"\",VLOOKUP(B57,sanschie!$A:$I,9,0))","v":1},{"$f":"IF(H57=1,J57,0)","v":""},{"$f":"IF(H57=2,J57,0)","v":0},{"$f":"IF(B57=\"\",\"0\",IF(VLOOKUP(B57,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B57,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B57,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B57=\"\",\"\",IF(H57=\"N\",VLOOKUP(B57,sanschie!$A:$K,7,0),VLOOKUP(B57,sanschie!$A:$K,7,0)))","v":149}]
[0,"104015",{"$f":"IF(B58=\"\",\"\",VLOOKUP(B58,sanschie!A:E,5,0))","v":"ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm"},"","","",{"$f":"IF(B58=\"\",\"\",VLOOKUP(B58,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B58=\"\",\"\",VLOOKUP(B58,sanschie!A:P,16,0))","v":1},{"$f":"IF(B58=\"\",\"\",IF(H58=\"N\",VLOOKUP(B58,sanschie!$A:$K,7,0),VLOOKUP(B58,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":160},"",{"$f":"IF(B58=\"\",\"\",VLOOKUP(B58,sanschie!$A:$I,9,0))","v":1},"",0,{"$f":"IF(B58=\"\",\"0\",IF(VLOOKUP(B58,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B58,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B58,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B58=\"\",\"\",IF(H58=\"N\",VLOOKUP(B58,sanschie!$A:$K,7,0),VLOOKUP(B58,sanschie!$A:$K,7,0)))","v":160}]
[0,"104016",{"$f":"IF(B59=\"\",\"\",VLOOKUP(B59,sanschie!A:E,5,0))","v":"ABS 180 Doppelfutter zu Rauchrohranschluss Ø130mm"},"","","",{"$f":"IF(B59=\"\",\"\",VLOOKUP(B59,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B59=\"\",\"\",VLOOKUP(B59,sanschie!A:P,16,0))","v":1},{"$f":"IF(B59=\"\",\"\",IF(H59=\"N\",VLOOKUP(B59,sanschie!$A:$K,7,0),VLOOKUP(B59,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":173},"",{"$f":"IF(B59=\"\",\"\",VLOOKUP(B59,sanschie!$A:$I,9,0))","v":1},"",0,{"$f":"IF(B59=\"\",\"0\",IF(VLOOKUP(B59,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B59,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B59,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B59=\"\",\"\",IF(H59=\"N\",VLOOKUP(B59,sanschie!$A:$K,7,0),VLOOKUP(B59,sanschie!$A:$K,7,0)))","v":173}]
[0,"104017",{"$f":"IF(B60=\"\",\"\",VLOOKUP(B60,sanschie!A:E,5,0))","v":"ABS 180 Doppelfutter zu Rauchrohranschluss Ø150mm"},"","","",{"$f":"IF(B60=\"\",\"\",VLOOKUP(B60,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B60=\"\",\"\",VLOOKUP(B60,sanschie!A:P,16,0))","v":1},{"$f":"IF(B60=\"\",\"\",IF(H60=\"N\",VLOOKUP(B60,sanschie!$A:$K,7,0),VLOOKUP(B60,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":184},"",{"$f":"IF(B60=\"\",\"\",VLOOKUP(B60,sanschie!$A:$I,9,0))","v":1},"",0,{"$f":"IF(B60=\"\",\"0\",IF(VLOOKUP(B60,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B60,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B60,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B60=\"\",\"\",IF(H60=\"N\",VLOOKUP(B60,sanschie!$A:$K,7,0),VLOOKUP(B60,sanschie!$A:$K,7,0)))","v":184}]
[0,"104018",{"$f":"IF(B61=\"\",\"\",VLOOKUP(B61,sanschie!A:E,5,0))","v":"ABS 180 Doppelfutter zu Rauchrohranschluss Ø180mm"},"","","",{"$f":"IF(B61=\"\",\"\",VLOOKUP(B61,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B61=\"\",\"\",VLOOKUP(B61,sanschie!A:P,16,0))","v":1},{"$f":"IF(B61=\"\",\"\",IF(H61=\"N\",VLOOKUP(B61,sanschie!$A:$K,7,0),VLOOKUP(B61,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":198},"",{"$f":"IF(B61=\"\",\"\",VLOOKUP(B61,sanschie!$A:$I,9,0))","v":1},"",0,{"$f":"IF(B61=\"\",\"0\",IF(VLOOKUP(B61,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B61,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B61,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B61=\"\",\"\",IF(H61=\"N\",VLOOKUP(B61,sanschie!$A:$K,7,0),VLOOKUP(B61,sanschie!$A:$K,7,0)))","v":198}]
[0,"104032",{"$f":"IF(B62=\"\",\"\",VLOOKUP(B62,sanschie!A:E,5,0))","v":"ABS 180 Kondensatfalle zu RA 45° Ø130mm"},"","","",{"$f":"IF(B62=\"\",\"\",VLOOKUP(B62,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B62=\"\",\"\",VLOOKUP(B62,sanschie!A:P,16,0))","v":1},{"$f":"IF(B62=\"\",\"\",IF(H62=\"N\",VLOOKUP(B62,sanschie!$A:$K,7,0),VLOOKUP(B62,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":347},"",{"$f":"IF(B62=\"\",\"\",VLOOKUP(B62,sanschie!$A:$I,9,0))","v":2.2000000000000002},"",0,{"$f":"IF(B62=\"\",\"0\",IF(VLOOKUP(B62,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B62,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B62,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B62=\"\",\"\",IF(H62=\"N\",VLOOKUP(B62,sanschie!$A:$K,7,0),VLOOKUP(B62,sanschie!$A:$K,7,0)))","v":347}]
[0,"104033",{"$f":"IF(B63=\"\",\"\",VLOOKUP(B63,sanschie!A:E,5,0))","v":"ABS 180 Kondensatfalle zu RA 45° Ø150mm"},"","","",{"$f":"IF(B63=\"\",\"\",VLOOKUP(B63,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B63=\"\",\"\",VLOOKUP(B63,sanschie!A:P,16,0))","v":1},{"$f":"IF(B63=\"\",\"\",IF(H63=\"N\",VLOOKUP(B63,sanschie!$A:$K,7,0),VLOOKUP(B63,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":347},"",{"$f":"IF(B63=\"\",\"\",VLOOKUP(B63,sanschie!$A:$I,9,0))","v":2.2000000000000002},"",0,{"$f":"IF(B63=\"\",\"0\",IF(VLOOKUP(B63,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B63,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B63,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B63=\"\",\"\",IF(H63=\"N\",VLOOKUP(B63,sanschie!$A:$K,7,0),VLOOKUP(B63,sanschie!$A:$K,7,0)))","v":347}]
[0,"104034",{"$f":"IF(B64=\"\",\"\",VLOOKUP(B64,sanschie!A:E,5,0))","v":"ABS 180 Kondensatfalle zu RA 45° Ø160mm"},"","","",{"$f":"IF(B64=\"\",\"\",VLOOKUP(B64,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B64=\"\",\"\",VLOOKUP(B64,sanschie!A:P,16,0))","v":1},{"$f":"IF(B64=\"\",\"\",IF(H64=\"N\",VLOOKUP(B64,sanschie!$A:$K,7,0),VLOOKUP(B64,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":347},"",{"$f":"IF(B64=\"\",\"\",VLOOKUP(B64,sanschie!$A:$I,9,0))","v":2.2000000000000002},"",0,{"$f":"IF(B64=\"\",\"0\",IF(VLOOKUP(B64,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B64,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B64,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B64=\"\",\"\",IF(H64=\"N\",VLOOKUP(B64,sanschie!$A:$K,7,0),VLOOKUP(B64,sanschie!$A:$K,7,0)))","v":347}]
[0,"104035",{"$f":"IF(B65=\"\",\"\",VLOOKUP(B65,sanschie!A:E,5,0))","v":"ABS 180 Kondensatfalle zu RA 45° Ø180mm "},"","","",{"$f":"IF(B65=\"\",\"\",VLOOKUP(B65,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B65=\"\",\"\",VLOOKUP(B65,sanschie!A:P,16,0))","v":1},{"$f":"IF(B65=\"\",\"\",IF(H65=\"N\",VLOOKUP(B65,sanschie!$A:$K,7,0),VLOOKUP(B65,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":347},"",{"$f":"IF(B65=\"\",\"\",VLOOKUP(B65,sanschie!$A:$I,9,0))","v":2.2000000000000002},"",0,{"$f":"IF(B65=\"\",\"0\",IF(VLOOKUP(B65,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B65,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B65,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B65=\"\",\"\",IF(H65=\"N\",VLOOKUP(B65,sanschie!$A:$K,7,0),VLOOKUP(B65,sanschie!$A:$K,7,0)))","v":347}]
[0,"104251",{"$f":"IF(B66=\"\",\"\",VLOOKUP(B66,sanschie!A:E,5,0))","v":"ABS Armierungs-Set 2 x 4000mm für Mantelsteine"},"","","",{"$f":"IF(B66=\"\",\"\",VLOOKUP(B66,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B66=\"\",\"\",VLOOKUP(B66,sanschie!A:P,16,0))","v":1},{"$f":"IF(B66=\"\",\"\",IF(H66=\"N\",VLOOKUP(B66,sanschie!$A:$K,7,0),VLOOKUP(B66,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":209},"",{"$f":"IF(B66=\"\",\"\",VLOOKUP(B66,sanschie!$A:$I,9,0))","v":5},"",0,{"$f":"IF(B66=\"\",\"0\",IF(VLOOKUP(B66,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B66,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B66,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B66=\"\",\"\",IF(H66=\"N\",VLOOKUP(B66,sanschie!$A:$K,7,0),VLOOKUP(B66,sanschie!$A:$K,7,0)))","v":209}]
[0,"104252",{"$f":"IF(B67=\"\",\"\",VLOOKUP(B67,sanschie!A:E,5,0))","v":"ABS Armierungs-Set 4 x 4000mm für Mantelsteine"},"","","",{"$f":"IF(B67=\"\",\"\",VLOOKUP(B67,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B67=\"\",\"\",VLOOKUP(B67,sanschie!A:P,16,0))","v":1},{"$f":"IF(B67=\"\",\"\",IF(H67=\"N\",VLOOKUP(B67,sanschie!$A:$K,7,0),VLOOKUP(B67,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":387},"",{"$f":"IF(B67=\"\",\"\",VLOOKUP(B67,sanschie!$A:$I,9,0))","v":10},"",0,{"$f":"IF(B67=\"\",\"0\",IF(VLOOKUP(B67,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B67,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B67,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B67=\"\",\"\",IF(H67=\"N\",VLOOKUP(B67,sanschie!$A:$K,7,0),VLOOKUP(B67,sanschie!$A:$K,7,0)))","v":387}]
[0,"104253",{"$f":"IF(B68=\"\",\"\",VLOOKUP(B68,sanschie!A:E,5,0))","v":"ABS Armierungs-Set 4 x 6000mm für Mantelsteine"},"","","",{"$f":"IF(B68=\"\",\"\",VLOOKUP(B68,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B68=\"\",\"\",VLOOKUP(B68,sanschie!A:P,16,0))","v":1},{"$f":"IF(B68=\"\",\"\",IF(H68=\"N\",VLOOKUP(B68,sanschie!$A:$K,7,0),VLOOKUP(B68,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":566},"",{"$f":"IF(B68=\"\",\"\",VLOOKUP(B68,sanschie!$A:$I,9,0))","v":15},"",0,{"$f":"IF(B68=\"\",\"0\",IF(VLOOKUP(B68,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B68,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B68,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B68=\"\",\"\",IF(H68=\"N\",VLOOKUP(B68,sanschie!$A:$K,7,0),VLOOKUP(B68,sanschie!$A:$K,7,0)))","v":566}]
[0,"103870",{"$f":"IF(B69=\"\",\"\",VLOOKUP(B69,sanschie!A:E,5,0))","v":"ABS Kondensatablauf DN40 zu Fertigfuss"},0.2,0,1,{"$f":"IF(B69=\"\",\"\",VLOOKUP(B69,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B69=\"\",\"\",VLOOKUP(B69,sanschie!A:P,16,0))","v":1},{"$f":"IF(B69=\"\",\"\",IF(H69=\"N\",VLOOKUP(B69,sanschie!$A:$K,7,0),VLOOKUP(B69,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":23},23,{"$f":"IF(B69=\"\",\"\",VLOOKUP(B69,sanschie!$A:$I,9,0))","v":0.2},23,0,{"$f":"IF(B69=\"\",\"0\",IF(VLOOKUP(B69,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B69,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B69,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B69=\"\",\"\",IF(H69=\"N\",VLOOKUP(B69,sanschie!$A:$K,7,0),VLOOKUP(B69,sanschie!$A:$K,7,0)))","v":23}]
[0,"104246",{"$f":"IF(B70=\"\",\"\",VLOOKUP(B70,sanschie!A:E,5,0))","v":"ABS Zugregler 13ZUK180/CH zu Fertigfuss"},"","","",{"$f":"IF(B70=\"\",\"\",VLOOKUP(B70,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B70=\"\",\"\",VLOOKUP(B70,sanschie!A:P,16,0))","v":1},{"$f":"IF(B70=\"\",\"\",IF(H70=\"N\",VLOOKUP(B70,sanschie!$A:$K,7,0),VLOOKUP(B70,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":489},"",{"$f":"IF(B70=\"\",\"\",VLOOKUP(B70,sanschie!$A:$I,9,0))","v":2.5},"",0,{"$f":"IF(B70=\"\",\"0\",IF(VLOOKUP(B70,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B70,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B70,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B70=\"\",\"\",IF(H70=\"N\",VLOOKUP(B70,sanschie!$A:$K,7,0),VLOOKUP(B70,sanschie!$A:$K,7,0)))","v":489}]
[0,"104245",{"$f":"IF(B71=\"\",\"\",VLOOKUP(B71,sanschie!A:E,5,0))","v":"ABS Türblatt gelocht Putztüre Typ3 für Zugregler"},"","","",{"$f":"IF(B71=\"\",\"\",VLOOKUP(B71,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B71=\"\",\"\",VLOOKUP(B71,sanschie!A:P,16,0))","v":1},{"$f":"IF(B71=\"\",\"\",IF(H71=\"N\",VLOOKUP(B71,sanschie!$A:$K,7,0),VLOOKUP(B71,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":82},"",{"$f":"IF(B71=\"\",\"\",VLOOKUP(B71,sanschie!$A:$I,9,0))","v":1.5},"",0,{"$f":"IF(B71=\"\",\"0\",IF(VLOOKUP(B71,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B71,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B71,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B71=\"\",\"\",IF(H71=\"N\",VLOOKUP(B71,sanschie!$A:$K,7,0),VLOOKUP(B71,sanschie!$A:$K,7,0)))","v":82}]
[0,"104244",{"$f":"IF(B72=\"\",\"\",VLOOKUP(B72,sanschie!A:E,5,0))","v":"ABS Türblatt zu Putztüre Typ 3"},"","","",{"$f":"IF(B72=\"\",\"\",VLOOKUP(B72,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B72=\"\",\"\",VLOOKUP(B72,sanschie!A:P,16,0))","v":1},{"$f":"IF(B72=\"\",\"\",IF(H72=\"N\",VLOOKUP(B72,sanschie!$A:$K,7,0),VLOOKUP(B72,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":58},"",{"$f":"IF(B72=\"\",\"\",VLOOKUP(B72,sanschie!$A:$I,9,0))","v":1.5},"",0,{"$f":"IF(B72=\"\",\"0\",IF(VLOOKUP(B72,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B72,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B72,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B72=\"\",\"\",IF(H72=\"N\",VLOOKUP(B72,sanschie!$A:$K,7,0),VLOOKUP(B72,sanschie!$A:$K,7,0)))","v":58}]
[0,"103944",{"$f":"IF(B73=\"\",\"\",VLOOKUP(B73,sanschie!A:E,5,0))","v":"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,"},"","","",{"$f":"IF(B73=\"\",\"\",VLOOKUP(B73,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B73=\"\",\"\",VLOOKUP(B73,sanschie!A:P,16,0))","v":1},{"$f":"IF(B73=\"\",\"\",IF(H73=\"N\",VLOOKUP(B73,sanschie!$A:$K,7,0),VLOOKUP(B73,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":14},"",{"$f":"IF(B73=\"\",\"\",VLOOKUP(B73,sanschie!$A:$I,9,0))","v":0},"",0,{"$f":"IF(B73=\"\",\"0\",IF(VLOOKUP(B73,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B73,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B73,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B73=\"\",\"\",IF(H73=\"N\",VLOOKUP(B73,sanschie!$A:$K,7,0),VLOOKUP(B73,sanschie!$A:$K,7,0)))","v":14}]
[0,"104256",{"$f":"IF(B74=\"\",\"\",VLOOKUP(B74,sanschie!A:E,5,0))","v":"ABS Kaminhalterung Standard"},"","","",{"$f":"IF(B74=\"\",\"\",VLOOKUP(B74,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B74=\"\",\"\",VLOOKUP(B74,sanschie!A:P,16,0))","v":1},{"$f":"IF(B74=\"\",\"\",IF(H74=\"N\",VLOOKUP(B74,sanschie!$A:$K,7,0),VLOOKUP(B74,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":303},"",{"$f":"IF(B74=\"\",\"\",VLOOKUP(B74,sanschie!$A:$I,9,0))","v":16.5},"",0,{"$f":"IF(B74=\"\",\"0\",IF(VLOOKUP(B74,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B74,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B74,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B74=\"\",\"\",IF(H74=\"N\",VLOOKUP(B74,sanschie!$A:$K,7,0),VLOOKUP(B74,sanschie!$A:$K,7,0)))","v":303}]
[0,"104257",{"$f":"IF(B75=\"\",\"\",VLOOKUP(B75,sanschie!A:E,5,0))","v":"ABS Verstärkung zu Kaminhalterung"},"","","",{"$f":"IF(B75=\"\",\"\",VLOOKUP(B75,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B75=\"\",\"\",VLOOKUP(B75,sanschie!A:P,16,0))","v":1},{"$f":"IF(B75=\"\",\"\",IF(H75=\"N\",VLOOKUP(B75,sanschie!$A:$K,7,0),VLOOKUP(B75,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":94},"",{"$f":"IF(B75=\"\",\"\",VLOOKUP(B75,sanschie!$A:$I,9,0))","v":2},"",0,{"$f":"IF(B75=\"\",\"0\",IF(VLOOKUP(B75,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B75,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B75,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B75=\"\",\"\",IF(H75=\"N\",VLOOKUP(B75,sanschie!$A:$K,7,0),VLOOKUP(B75,sanschie!$A:$K,7,0)))","v":94}]
[0,"103963",{"$f":"IF(B76=\"\",\"\",VLOOKUP(B76,sanschie!A:E,5,0))","v":"ABS Rapid-Kartusche zum Kleben der Keramikrohre "},"","","",{"$f":"IF(B76=\"\",\"\",VLOOKUP(B76,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B76=\"\",\"\",VLOOKUP(B76,sanschie!A:P,16,0))","v":1},{"$f":"IF(B76=\"\",\"\",IF(H76=\"N\",VLOOKUP(B76,sanschie!$A:$K,7,0),VLOOKUP(B76,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":19},"",{"$f":"IF(B76=\"\",\"\",VLOOKUP(B76,sanschie!$A:$I,9,0))","v":0.68},"",0,{"$f":"IF(B76=\"\",\"0\",IF(VLOOKUP(B76,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B76,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B76,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B76=\"\",\"\",IF(H76=\"N\",VLOOKUP(B76,sanschie!$A:$K,7,0),VLOOKUP(B76,sanschie!$A:$K,7,0)))","v":19}]
[0,"103941",{"$f":"IF(B77=\"\",\"\",VLOOKUP(B77,sanschie!A:E,5,0))","v":"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg"},10,0,1,{"$f":"IF(B77=\"\",\"\",VLOOKUP(B77,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B77=\"\",\"\",VLOOKUP(B77,sanschie!A:P,16,0))","v":1},{"$f":"IF(B77=\"\",\"\",IF(H77=\"N\",VLOOKUP(B77,sanschie!$A:$K,7,0),VLOOKUP(B77,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":35},35,{"$f":"IF(B77=\"\",\"\",VLOOKUP(B77,sanschie!$A:$I,9,0))","v":10},35,0,{"$f":"IF(B77=\"\",\"0\",IF(VLOOKUP(B77,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B77,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B77,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B77=\"\",\"\",IF(H77=\"N\",VLOOKUP(B77,sanschie!$A:$K,7,0),VLOOKUP(B77,sanschie!$A:$K,7,0)))","v":35}]
[0,"104212",{"$f":"IF(B78=\"\",\"\",VLOOKUP(B78,sanschie!A:E,5,0))","v":"ABS 180 Basten Standard Inox"},"","","",{"$f":"IF(B78=\"\",\"\",VLOOKUP(B78,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B78=\"\",\"\",VLOOKUP(B78,sanschie!A:P,16,0))","v":1},{"$f":"IF(B78=\"\",\"\",IF(H78=\"N\",VLOOKUP(B78,sanschie!$A:$K,7,0),VLOOKUP(B78,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":345},"",{"$f":"IF(B78=\"\",\"\",VLOOKUP(B78,sanschie!$A:$I,9,0))","v":3.4},"",0,{"$f":"IF(B78=\"\",\"0\",IF(VLOOKUP(B78,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B78,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B78,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B78=\"\",\"\",IF(H78=\"N\",VLOOKUP(B78,sanschie!$A:$K,7,0),VLOOKUP(B78,sanschie!$A:$K,7,0)))","v":345}]
[0,"104218",{"$f":"IF(B79=\"\",\"\",VLOOKUP(B79,sanschie!A:E,5,0))","v":"ABS 180 Basten Standard Kupfer"},"","","",{"$f":"IF(B79=\"\",\"\",VLOOKUP(B79,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B79=\"\",\"\",VLOOKUP(B79,sanschie!A:P,16,0))","v":1},{"$f":"IF(B79=\"\",\"\",IF(H79=\"N\",VLOOKUP(B79,sanschie!$A:$K,7,0),VLOOKUP(B79,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":362},"",{"$f":"IF(B79=\"\",\"\",VLOOKUP(B79,sanschie!$A:$I,9,0))","v":4.3},"",0,{"$f":"IF(B79=\"\",\"0\",IF(VLOOKUP(B79,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B79,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B79,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B79=\"\",\"\",IF(H79=\"N\",VLOOKUP(B79,sanschie!$A:$K,7,0),VLOOKUP(B79,sanschie!$A:$K,7,0)))","v":362}]
[0,"104224",{"$f":"IF(B80=\"\",\"\",VLOOKUP(B80,sanschie!A:E,5,0))","v":"ABS 180 Sairlift Inox"},"","","",{"$f":"IF(B80=\"\",\"\",VLOOKUP(B80,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B80=\"\",\"\",VLOOKUP(B80,sanschie!A:P,16,0))","v":1},{"$f":"IF(B80=\"\",\"\",IF(H80=\"N\",VLOOKUP(B80,sanschie!$A:$K,7,0),VLOOKUP(B80,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":400},"",{"$f":"IF(B80=\"\",\"\",VLOOKUP(B80,sanschie!$A:$I,9,0))","v":3.9},"",0,{"$f":"IF(B80=\"\",\"0\",IF(VLOOKUP(B80,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B80,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B80,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B80=\"\",\"\",IF(H80=\"N\",VLOOKUP(B80,sanschie!$A:$K,7,0),VLOOKUP(B80,sanschie!$A:$K,7,0)))","v":400}]
[0,"104229",{"$f":"IF(B81=\"\",\"\",VLOOKUP(B81,sanschie!A:E,5,0))","v":"ABS 180 Sairlift Kupfer"},"","","",{"$f":"IF(B81=\"\",\"\",VLOOKUP(B81,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B81=\"\",\"\",VLOOKUP(B81,sanschie!A:P,16,0))","v":1},{"$f":"IF(B81=\"\",\"\",IF(H81=\"N\",VLOOKUP(B81,sanschie!$A:$K,7,0),VLOOKUP(B81,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":419},"",{"$f":"IF(B81=\"\",\"\",VLOOKUP(B81,sanschie!$A:$I,9,0))","v":3.9},"",0,{"$f":"IF(B81=\"\",\"0\",IF(VLOOKUP(B81,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B81,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B81,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B81=\"\",\"\",IF(H81=\"N\",VLOOKUP(B81,sanschie!$A:$K,7,0),VLOOKUP(B81,sanschie!$A:$K,7,0)))","v":419}]
[0,"103838",{"$f":"IF(B82=\"\",\"\",VLOOKUP(B82,sanschie!A:E,5,0))","v":"ZBH 180 Verschlussbüchse weiss ØA 275mm"},"","","",{"$f":"IF(B82=\"\",\"\",VLOOKUP(B82,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B82=\"\",\"\",VLOOKUP(B82,sanschie!A:P,16,0))","v":1},{"$f":"IF(B82=\"\",\"\",IF(H82=\"N\",VLOOKUP(B82,sanschie!$A:$K,7,0),VLOOKUP(B82,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":123.1},"",{"$f":"IF(B82=\"\",\"\",VLOOKUP(B82,sanschie!$A:$I,9,0))","v":1},"",0,{"$f":"IF(B82=\"\",\"0\",IF(VLOOKUP(B82,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B82,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B82,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B82=\"\",\"\",IF(H82=\"N\",VLOOKUP(B82,sanschie!$A:$K,7,0),VLOOKUP(B82,sanschie!$A:$K,7,0)))","v":123.1}]
[0,"100265",{"$f":"IF(B83=\"\",\"\",VLOOKUP(B83,sanschie!A:E,5,0))","v":"Neutralisationsbox komplett"},"","","",{"$f":"IF(B83=\"\",\"\",VLOOKUP(B83,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B83=\"\",\"\",VLOOKUP(B83,sanschie!A:P,16,0))","v":1},{"$f":"IF(B83=\"\",\"\",IF(H83=\"N\",VLOOKUP(B83,sanschie!$A:$K,7,0),VLOOKUP(B83,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":258.8},"",{"$f":"IF(B83=\"\",\"\",VLOOKUP(B83,sanschie!$A:$I,9,0))","v":11.27},"",0,{"$f":"IF(B83=\"\",\"0\",IF(VLOOKUP(B83,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B83,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B83,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B83=\"\",\"\",IF(H83=\"N\",VLOOKUP(B83,sanschie!$A:$K,7,0),VLOOKUP(B83,sanschie!$A:$K,7,0)))","v":258.8}]
[0,"100266",{"$f":"IF(B84=\"\",\"\",VLOOKUP(B84,sanschie!A:E,5,0))","v":"Nachfüllset zu Neutralisationsbox"},"","","",{"$f":"IF(B84=\"\",\"\",VLOOKUP(B84,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B84=\"\",\"\",VLOOKUP(B84,sanschie!A:P,16,0))","v":1},{"$f":"IF(B84=\"\",\"\",IF(H84=\"N\",VLOOKUP(B84,sanschie!$A:$K,7,0),VLOOKUP(B84,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":67.900000000000006},"",{"$f":"IF(B84=\"\",\"\",VLOOKUP(B84,sanschie!$A:$I,9,0))","v":3.1},"",0,{"$f":"IF(B84=\"\",\"0\",IF(VLOOKUP(B84,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B84,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B84,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B84=\"\",\"\",IF(H84=\"N\",VLOOKUP(B84,sanschie!$A:$K,7,0),VLOOKUP(B84,sanschie!$A:$K,7,0)))","v":67.900000000000006}]
[0,"103841",{"$f":"IF(B85=\"\",\"\",VLOOKUP(B85,sanschie!A:E,5,0))","v":"ZBH Kondensatkanister 20Liter"},"","","",{"$f":"IF(B85=\"\",\"\",VLOOKUP(B85,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B85=\"\",\"\",VLOOKUP(B85,sanschie!A:P,16,0))","v":1},{"$f":"IF(B85=\"\",\"\",IF(H85=\"N\",VLOOKUP(B85,sanschie!$A:$K,7,0),VLOOKUP(B85,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":44.9},"",{"$f":"IF(B85=\"\",\"\",VLOOKUP(B85,sanschie!$A:$I,9,0))","v":1.25},"",0,{"$f":"IF(B85=\"\",\"0\",IF(VLOOKUP(B85,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B85,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B85,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B85=\"\",\"\",IF(H85=\"N\",VLOOKUP(B85,sanschie!$A:$K,7,0),VLOOKUP(B85,sanschie!$A:$K,7,0)))","v":44.9}]
[0,"100264",{"$f":"IF(B86=\"\",\"\",VLOOKUP(B86,sanschie!A:E,5,0))","v":"Kondesatschlauch 36mm L1000mm"},"","","",{"$f":"IF(B86=\"\",\"\",VLOOKUP(B86,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B86=\"\",\"\",VLOOKUP(B86,sanschie!A:P,16,0))","v":1},{"$f":"IF(B86=\"\",\"\",IF(H86=\"N\",VLOOKUP(B86,sanschie!$A:$K,7,0),VLOOKUP(B86,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":7.5},"",{"$f":"IF(B86=\"\",\"\",VLOOKUP(B86,sanschie!$A:$I,9,0))","v":0.36},"",0,{"$f":"IF(B86=\"\",\"0\",IF(VLOOKUP(B86,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B86,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B86,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B86=\"\",\"\",IF(H86=\"N\",VLOOKUP(B86,sanschie!$A:$K,7,0),VLOOKUP(B86,sanschie!$A:$K,7,0)))","v":7.5}]
[0,"103833",{"$f":"IF(B87=\"\",\"\",VLOOKUP(B87,sanschie!A:E,5,0))","v":"ZBH 190 Verschlusszapfen 2Stk. aus Schaumstoff"},"","","",{"$f":"IF(B87=\"\",\"\",VLOOKUP(B87,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B87=\"\",\"\",VLOOKUP(B87,sanschie!A:P,16,0))","v":1},{"$f":"IF(B87=\"\",\"\",IF(H87=\"N\",VLOOKUP(B87,sanschie!$A:$K,7,0),VLOOKUP(B87,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":26.5},"",{"$f":"IF(B87=\"\",\"\",VLOOKUP(B87,sanschie!$A:$I,9,0))","v":0.1},"",0,{"$f":"IF(B87=\"\",\"0\",IF(VLOOKUP(B87,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B87,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B87,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B87=\"\",\"\",IF(H87=\"N\",VLOOKUP(B87,sanschie!$A:$K,7,0),VLOOKUP(B87,sanschie!$A:$K,7,0)))","v":26.5}]
[0,"103820",{"$f":"IF(B88=\"\",\"\",VLOOKUP(B88,sanschie!A:E,5,0))","v":"LBS 150 Ignis Protect 565 x 700 mm"},"","","",{"$f":"IF(B88=\"\",\"\",VLOOKUP(B88,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B88=\"\",\"\",VLOOKUP(B88,sanschie!A:P,16,0))","v":1},{"$f":"IF(B88=\"\",\"\",IF(H88=\"N\",VLOOKUP(B88,sanschie!$A:$K,7,0),VLOOKUP(B88,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":452},"",{"$f":"IF(B88=\"\",\"\",VLOOKUP(B88,sanschie!$A:$I,9,0))","v":6},"",0,{"$f":"IF(B88=\"\",\"0\",IF(VLOOKUP(B88,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B88,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B88,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B88=\"\",\"\",IF(H88=\"N\",VLOOKUP(B88,sanschie!$A:$K,7,0),VLOOKUP(B88,sanschie!$A:$K,7,0)))","v":452}]
[0,"103821",{"$f":"IF(B89=\"\",\"\",VLOOKUP(B89,sanschie!A:E,5,0))","v":"LBS 200 Ignis Protect 565 x 700 mm"},{"$f":"IF(F89=\"\",\"\",K89*F89)","v":""},{"$f":"IF(F89=\"\",\"\",IF(N89=\"\",\"\",N89*F89))","v":""},"",{"$f":"IF(B89=\"\",\"\",VLOOKUP(B89,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B89=\"\",\"\",VLOOKUP(B89,sanschie!A:P,16,0))","v":1},{"$f":"IF(B89=\"\",\"\",IF(H89=\"N\",VLOOKUP(B89,sanschie!$A:$K,7,0),VLOOKUP(B89,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":538},{"$f":"IF(F89=\"\",\"\",(F89*I89))","v":""},{"$f":"IF(B89=\"\",\"\",VLOOKUP(B89,sanschie!$A:$I,9,0))","v":8.4},{"$f":"IF(H89=1,J89,0)","v":""},{"$f":"IF(H89=2,J89,0)","v":0},{"$f":"IF(B89=\"\",\"0\",IF(VLOOKUP(B89,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B89,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B89,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B89=\"\",\"\",IF(H89=\"N\",VLOOKUP(B89,sanschie!$A:$K,7,0),VLOOKUP(B89,sanschie!$A:$K,7,0)))","v":538}]
[0,"103822",{"$f":"IF(B90=\"\",\"\",VLOOKUP(B90,sanschie!A:E,5,0))","v":"LBS 250 Ignis Protect 565 x 700 mm"},"","","",{"$f":"IF(B90=\"\",\"\",VLOOKUP(B90,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B90=\"\",\"\",VLOOKUP(B90,sanschie!A:P,16,0))","v":1},{"$f":"IF(B90=\"\",\"\",IF(H90=\"N\",VLOOKUP(B90,sanschie!$A:$K,7,0),VLOOKUP(B90,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":634},{"$f":"IF(F90=\"\",\"\",(F90*I90))","v":""},{"$f":"IF(B90=\"\",\"\",VLOOKUP(B90,sanschie!$A:$I,9,0))","v":10.5},"",0,{"$f":"IF(B90=\"\",\"0\",IF(VLOOKUP(B90,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B90,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B90,sanschie!$A:$K,10,0)))))","v":"0"},null,null,{"$f":"IF(H90=3,J90,0)","v":0},{"$f":"IF(B90=\"\",\"\",IF(H90=\"N\",VLOOKUP(B90,sanschie!$A:$K,7,0),VLOOKUP(B90,sanschie!$A:$K,7,0)))","v":634}]
[0,"103823",{"$f":"IF(B91=\"\",\"\",VLOOKUP(B91,sanschie!A:E,5,0))","v":"LBS 300 Ignis Protect 565 x 700 mm"},"","","",{"$f":"IF(B91=\"\",\"\",VLOOKUP(B91,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B91=\"\",\"\",VLOOKUP(B91,sanschie!A:P,16,0))","v":1},{"$f":"IF(B91=\"\",\"\",IF(H91=\"N\",VLOOKUP(B91,sanschie!$A:$K,7,0),VLOOKUP(B91,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":695},{"$f":"IF(F91=\"\",\"\",(F91*I91))","v":""},{"$f":"IF(B91=\"\",\"\",VLOOKUP(B91,sanschie!$A:$I,9,0))","v":12.5},"",0,{"$f":"IF(B91=\"\",\"0\",IF(VLOOKUP(B91,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B91,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B91,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B91=\"\",\"\",IF(H91=\"N\",VLOOKUP(B91,sanschie!$A:$K,7,0),VLOOKUP(B91,sanschie!$A:$K,7,0)))","v":695}]
[0,"103824",{"$f":"IF(B92=\"\",\"\",VLOOKUP(B92,sanschie!A:E,5,0))","v":"LBS 350 Ignis Protect 565 x 700 mm"},"","","",{"$f":"IF(B92=\"\",\"\",VLOOKUP(B92,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B92=\"\",\"\",VLOOKUP(B92,sanschie!A:P,16,0))","v":1},{"$f":"IF(B92=\"\",\"\",IF(H92=\"N\",VLOOKUP(B92,sanschie!$A:$K,7,0),VLOOKUP(B92,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":797},{"$f":"IF(F92=\"\",\"\",(F92*I92))","v":""},{"$f":"IF(B92=\"\",\"\",VLOOKUP(B92,sanschie!$A:$I,9,0))","v":13.5},"",0,{"$f":"IF(B92=\"\",\"0\",IF(VLOOKUP(B92,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B92,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B92,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B92=\"\",\"\",IF(H92=\"N\",VLOOKUP(B92,sanschie!$A:$K,7,0),VLOOKUP(B92,sanschie!$A:$K,7,0)))","v":797}]
[0,"103825",{"$f":"IF(B93=\"\",\"\",VLOOKUP(B93,sanschie!A:E,5,0))","v":"LBS 400 Ignis Protect 565 x 700 mm"},"","","",{"$f":"IF(B93=\"\",\"\",VLOOKUP(B93,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B93=\"\",\"\",VLOOKUP(B93,sanschie!A:P,16,0))","v":1},{"$f":"IF(B93=\"\",\"\",IF(H93=\"N\",VLOOKUP(B93,sanschie!$A:$K,7,0),VLOOKUP(B93,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":873},"",{"$f":"IF(B93=\"\",\"\",VLOOKUP(B93,sanschie!$A:$I,9,0))","v":16.7},"",0,{"$f":"IF(B93=\"\",\"0\",IF(VLOOKUP(B93,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B93,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B93,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B93=\"\",\"\",IF(H93=\"N\",VLOOKUP(B93,sanschie!$A:$K,7,0),VLOOKUP(B93,sanschie!$A:$K,7,0)))","v":873}]
[0,"103848",{"$f":"IF(B94=\"\",\"\",VLOOKUP(B94,sanschie!A:E,5,0))","v":"ZBH Kittpistole für Kartuschen"},"","","",{"$f":"IF(B94=\"\",\"\",VLOOKUP(B94,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B94=\"\",\"\",VLOOKUP(B94,sanschie!A:P,16,0))","v":1},{"$f":"IF(B94=\"\",\"\",IF(H94=\"N\",VLOOKUP(B94,sanschie!$A:$K,7,0),VLOOKUP(B94,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":13.8},"",{"$f":"IF(B94=\"\",\"\",VLOOKUP(B94,sanschie!$A:$I,9,0))","v":2.5},"",0,{"$f":"IF(B94=\"\",\"0\",IF(VLOOKUP(B94,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B94,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B94,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B94=\"\",\"\",IF(H94=\"N\",VLOOKUP(B94,sanschie!$A:$K,7,0),VLOOKUP(B94,sanschie!$A:$K,7,0)))","v":13.8}]
[0,"103846",{"$f":"IF(B95=\"\",\"\",VLOOKUP(B95,sanschie!A:E,5,0))","v":"ZBH Diamantblatt für Trennscheibe  Ø115mm"},"","","",{"$f":"IF(B95=\"\",\"\",VLOOKUP(B95,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B95=\"\",\"\",VLOOKUP(B95,sanschie!A:P,16,0))","v":1},{"$f":"IF(B95=\"\",\"\",IF(H95=\"N\",VLOOKUP(B95,sanschie!$A:$K,7,0),VLOOKUP(B95,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":162.19999999999999},"",{"$f":"IF(B95=\"\",\"\",VLOOKUP(B95,sanschie!$A:$I,9,0))","v":0.11},"",0,{"$f":"IF(B95=\"\",\"0\",IF(VLOOKUP(B95,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B95,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B95,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B95=\"\",\"\",IF(H95=\"N\",VLOOKUP(B95,sanschie!$A:$K,7,0),VLOOKUP(B95,sanschie!$A:$K,7,0)))","v":162.19999999999999}]
[0,"103847",{"$f":"IF(B96=\"\",\"\",VLOOKUP(B96,sanschie!A:E,5,0))","v":"ZBH Diamantblatt für Trennscheibe  Ø230mm"},"","","",{"$f":"IF(B96=\"\",\"\",VLOOKUP(B96,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B96=\"\",\"\",VLOOKUP(B96,sanschie!A:P,16,0))","v":1},{"$f":"IF(B96=\"\",\"\",IF(H96=\"N\",VLOOKUP(B96,sanschie!$A:$K,7,0),VLOOKUP(B96,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":322},"",{"$f":"IF(B96=\"\",\"\",VLOOKUP(B96,sanschie!$A:$I,9,0))","v":0.6},"",0,{"$f":"IF(B96=\"\",\"0\",IF(VLOOKUP(B96,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B96,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B96,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B96=\"\",\"\",IF(H96=\"N\",VLOOKUP(B96,sanschie!$A:$K,7,0),VLOOKUP(B96,sanschie!$A:$K,7,0)))","v":322}]
[0,"104259",{"$f":"IF(B97=\"\",\"\",VLOOKUP(B97,sanschie!A:E,5,0))","v":"Euro Paletten"},"","","",{"$f":"IF(B97=\"\",\"\",VLOOKUP(B97,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B97=\"\",\"\",VLOOKUP(B97,sanschie!A:P,16,0))","v":0},{"$f":"IF(B97=\"\",\"\",IF(H97=\"N\",VLOOKUP(B97,sanschie!$A:$K,7,0),VLOOKUP(B97,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":26},"",{"$f":"IF(B97=\"\",\"\",VLOOKUP(B97,sanschie!$A:$I,9,0))","v":15},0,0,{"$f":"IF(B97=\"\",\"0\",IF(VLOOKUP(B97,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B97,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B97,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B97=\"\",\"\",IF(H97=\"N\",VLOOKUP(B97,sanschie!$A:$K,7,0),VLOOKUP(B97,sanschie!$A:$K,7,0)))","v":26}]
[0,"104261",{"$f":"IF(B98=\"\",\"\",VLOOKUP(B98,sanschie!A:E,5,0))","v":"Euro Paletten im Austausch"},30,0,2,{"$f":"IF(B98=\"\",\"\",VLOOKUP(B98,sanschie!A:D,4,0))","v":"STK"},{"$f":"IF(B98=\"\",\"\",VLOOKUP(B98,sanschie!A:P,16,0))","v":0},{"$f":"IF(B98=\"\",\"\",IF(H98=\"N\",VLOOKUP(B98,sanschie!$A:$K,7,0),VLOOKUP(B98,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":0},0,{"$f":"IF(B98=\"\",\"\",VLOOKUP(B98,sanschie!$A:$I,9,0))","v":15},0,0,{"$f":"IF(B98=\"\",\"0\",IF(VLOOKUP(B98,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B98,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B98,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B98=\"\",\"\",IF(H98=\"N\",VLOOKUP(B98,sanschie!$A:$K,7,0),VLOOKUP(B98,sanschie!$A:$K,7,0)))","v":0}]
["","",{"$f":"IF(B99=\"\",\"\",VLOOKUP(B99,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B99=\"\",\"\",VLOOKUP(B99,sanschie!A:D,4,0))","v":""},{"$f":"IF(B99=\"\",\"\",VLOOKUP(B99,sanschie!A:P,16,0))","v":""},{"$f":"IF(B99=\"\",\"\",IF(H99=\"N\",VLOOKUP(B99,sanschie!$A:$K,7,0),VLOOKUP(B99,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B99=\"\",\"\",VLOOKUP(B99,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B99=\"\",\"0\",IF(VLOOKUP(B99,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B99,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B99,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B99=\"\",\"\",IF(H99=\"N\",VLOOKUP(B99,sanschie!$A:$K,7,0),VLOOKUP(B99,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B100=\"\",\"\",VLOOKUP(B100,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B100=\"\",\"\",VLOOKUP(B100,sanschie!A:D,4,0))","v":""},{"$f":"IF(B100=\"\",\"\",VLOOKUP(B100,sanschie!A:P,16,0))","v":""},{"$f":"IF(B100=\"\",\"\",IF(H100=\"N\",VLOOKUP(B100,sanschie!$A:$K,7,0),VLOOKUP(B100,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B100=\"\",\"\",VLOOKUP(B100,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B100=\"\",\"0\",IF(VLOOKUP(B100,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B100,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B100,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B100=\"\",\"\",IF(H100=\"N\",VLOOKUP(B100,sanschie!$A:$K,7,0),VLOOKUP(B100,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B101=\"\",\"\",VLOOKUP(B101,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B101=\"\",\"\",VLOOKUP(B101,sanschie!A:D,4,0))","v":""},{"$f":"IF(B101=\"\",\"\",VLOOKUP(B101,sanschie!A:P,16,0))","v":""},{"$f":"IF(B101=\"\",\"\",IF(H101=\"N\",VLOOKUP(B101,sanschie!$A:$K,7,0),VLOOKUP(B101,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},{"$f":"IF(F101=\"\",\"\",(F101*I101))","v":""},{"$f":"IF(B101=\"\",\"\",VLOOKUP(B101,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B101=\"\",\"0\",IF(VLOOKUP(B101,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B101,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B101,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B101=\"\",\"\",IF(H101=\"N\",VLOOKUP(B101,sanschie!$A:$K,7,0),VLOOKUP(B101,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B102=\"\",\"\",VLOOKUP(B102,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B102=\"\",\"\",VLOOKUP(B102,sanschie!A:D,4,0))","v":""},{"$f":"IF(B102=\"\",\"\",VLOOKUP(B102,sanschie!A:P,16,0))","v":""},{"$f":"IF(B102=\"\",\"\",IF(H102=\"N\",VLOOKUP(B102,sanschie!$A:$K,7,0),VLOOKUP(B102,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B102=\"\",\"\",VLOOKUP(B102,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B102=\"\",\"0\",IF(VLOOKUP(B102,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B102,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B102,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B102=\"\",\"\",IF(H102=\"N\",VLOOKUP(B102,sanschie!$A:$K,7,0),VLOOKUP(B102,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B103=\"\",\"\",VLOOKUP(B103,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B103=\"\",\"\",VLOOKUP(B103,sanschie!A:D,4,0))","v":""},{"$f":"IF(B103=\"\",\"\",VLOOKUP(B103,sanschie!A:P,16,0))","v":""},{"$f":"IF(B103=\"\",\"\",IF(H103=\"N\",VLOOKUP(B103,sanschie!$A:$K,7,0),VLOOKUP(B103,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B103=\"\",\"\",VLOOKUP(B103,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B103=\"\",\"0\",IF(VLOOKUP(B103,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B103,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B103,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B103=\"\",\"\",IF(H103=\"N\",VLOOKUP(B103,sanschie!$A:$K,7,0),VLOOKUP(B103,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B104=\"\",\"\",VLOOKUP(B104,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B104=\"\",\"\",VLOOKUP(B104,sanschie!A:D,4,0))","v":""},{"$f":"IF(B104=\"\",\"\",VLOOKUP(B104,sanschie!A:P,16,0))","v":""},{"$f":"IF(B104=\"\",\"\",IF(H104=\"N\",VLOOKUP(B104,sanschie!$A:$K,7,0),VLOOKUP(B104,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B104=\"\",\"\",VLOOKUP(B104,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B104=\"\",\"0\",IF(VLOOKUP(B104,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B104,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B104,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B104=\"\",\"\",IF(H104=\"N\",VLOOKUP(B104,sanschie!$A:$K,7,0),VLOOKUP(B104,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B105=\"\",\"\",VLOOKUP(B105,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B105=\"\",\"\",VLOOKUP(B105,sanschie!A:D,4,0))","v":""},{"$f":"IF(B105=\"\",\"\",VLOOKUP(B105,sanschie!A:P,16,0))","v":""},{"$f":"IF(B105=\"\",\"\",IF(H105=\"N\",VLOOKUP(B105,sanschie!$A:$K,7,0),VLOOKUP(B105,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B105=\"\",\"\",VLOOKUP(B105,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B105=\"\",\"0\",IF(VLOOKUP(B105,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B105,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B105,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B105=\"\",\"\",IF(H105=\"N\",VLOOKUP(B105,sanschie!$A:$K,7,0),VLOOKUP(B105,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B106=\"\",\"\",VLOOKUP(B106,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B106=\"\",\"\",VLOOKUP(B106,sanschie!A:D,4,0))","v":""},{"$f":"IF(B106=\"\",\"\",VLOOKUP(B106,sanschie!A:P,16,0))","v":""},{"$f":"IF(B106=\"\",\"\",IF(H106=\"N\",VLOOKUP(B106,sanschie!$A:$K,7,0),VLOOKUP(B106,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B106=\"\",\"\",VLOOKUP(B106,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B106=\"\",\"0\",IF(VLOOKUP(B106,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B106,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B106,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B106=\"\",\"\",IF(H106=\"N\",VLOOKUP(B106,sanschie!$A:$K,7,0),VLOOKUP(B106,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B107=\"\",\"\",VLOOKUP(B107,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B107=\"\",\"\",VLOOKUP(B107,sanschie!A:D,4,0))","v":""},{"$f":"IF(B107=\"\",\"\",VLOOKUP(B107,sanschie!A:P,16,0))","v":""},{"$f":"IF(B107=\"\",\"\",IF(H107=\"N\",VLOOKUP(B107,sanschie!$A:$K,7,0),VLOOKUP(B107,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B107=\"\",\"\",VLOOKUP(B107,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B107=\"\",\"0\",IF(VLOOKUP(B107,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B107,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B107,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B107=\"\",\"\",IF(H107=\"N\",VLOOKUP(B107,sanschie!$A:$K,7,0),VLOOKUP(B107,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B108=\"\",\"\",VLOOKUP(B108,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B108=\"\",\"\",VLOOKUP(B108,sanschie!A:D,4,0))","v":""},{"$f":"IF(B108=\"\",\"\",VLOOKUP(B108,sanschie!A:P,16,0))","v":""},{"$f":"IF(B108=\"\",\"\",IF(H108=\"N\",VLOOKUP(B108,sanschie!$A:$K,7,0),VLOOKUP(B108,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B108=\"\",\"\",VLOOKUP(B108,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B108=\"\",\"0\",IF(VLOOKUP(B108,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B108,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B108,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B108=\"\",\"\",IF(H108=\"N\",VLOOKUP(B108,sanschie!$A:$K,7,0),VLOOKUP(B108,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B109=\"\",\"\",VLOOKUP(B109,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B109=\"\",\"\",VLOOKUP(B109,sanschie!A:D,4,0))","v":""},{"$f":"IF(B109=\"\",\"\",VLOOKUP(B109,sanschie!A:P,16,0))","v":""},{"$f":"IF(B109=\"\",\"\",IF(H109=\"N\",VLOOKUP(B109,sanschie!$A:$K,7,0),VLOOKUP(B109,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B109=\"\",\"\",VLOOKUP(B109,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B109=\"\",\"0\",IF(VLOOKUP(B109,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B109,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B109,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B109=\"\",\"\",IF(H109=\"N\",VLOOKUP(B109,sanschie!$A:$K,7,0),VLOOKUP(B109,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B110=\"\",\"\",VLOOKUP(B110,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B110=\"\",\"\",VLOOKUP(B110,sanschie!A:D,4,0))","v":""},{"$f":"IF(B110=\"\",\"\",VLOOKUP(B110,sanschie!A:P,16,0))","v":""},{"$f":"IF(B110=\"\",\"\",IF(H110=\"N\",VLOOKUP(B110,sanschie!$A:$K,7,0),VLOOKUP(B110,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B110=\"\",\"\",VLOOKUP(B110,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B110=\"\",\"0\",IF(VLOOKUP(B110,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B110,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B110,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B110=\"\",\"\",IF(H110=\"N\",VLOOKUP(B110,sanschie!$A:$K,7,0),VLOOKUP(B110,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B111=\"\",\"\",VLOOKUP(B111,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B111=\"\",\"\",VLOOKUP(B111,sanschie!A:D,4,0))","v":""},{"$f":"IF(B111=\"\",\"\",VLOOKUP(B111,sanschie!A:P,16,0))","v":""},{"$f":"IF(B111=\"\",\"\",IF(H111=\"N\",VLOOKUP(B111,sanschie!$A:$K,7,0),VLOOKUP(B111,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B111=\"\",\"\",VLOOKUP(B111,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B111=\"\",\"0\",IF(VLOOKUP(B111,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B111,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B111,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B111=\"\",\"\",IF(H111=\"N\",VLOOKUP(B111,sanschie!$A:$K,7,0),VLOOKUP(B111,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B112=\"\",\"\",VLOOKUP(B112,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B112=\"\",\"\",VLOOKUP(B112,sanschie!A:D,4,0))","v":""},{"$f":"IF(B112=\"\",\"\",VLOOKUP(B112,sanschie!A:P,16,0))","v":""},{"$f":"IF(B112=\"\",\"\",IF(H112=\"N\",VLOOKUP(B112,sanschie!$A:$K,7,0),VLOOKUP(B112,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B112=\"\",\"\",VLOOKUP(B112,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B112=\"\",\"0\",IF(VLOOKUP(B112,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B112,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B112,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B112=\"\",\"\",IF(H112=\"N\",VLOOKUP(B112,sanschie!$A:$K,7,0),VLOOKUP(B112,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B113=\"\",\"\",VLOOKUP(B113,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B113=\"\",\"\",VLOOKUP(B113,sanschie!A:D,4,0))","v":""},{"$f":"IF(B113=\"\",\"\",VLOOKUP(B113,sanschie!A:P,16,0))","v":""},{"$f":"IF(B113=\"\",\"\",IF(H113=\"N\",VLOOKUP(B113,sanschie!$A:$K,7,0),VLOOKUP(B113,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B113=\"\",\"\",VLOOKUP(B113,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B113=\"\",\"0\",IF(VLOOKUP(B113,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B113,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B113,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B113=\"\",\"\",IF(H113=\"N\",VLOOKUP(B113,sanschie!$A:$K,7,0),VLOOKUP(B113,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B114=\"\",\"\",VLOOKUP(B114,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B114=\"\",\"\",VLOOKUP(B114,sanschie!A:D,4,0))","v":""},{"$f":"IF(B114=\"\",\"\",VLOOKUP(B114,sanschie!A:P,16,0))","v":""},{"$f":"IF(B114=\"\",\"\",IF(H114=\"N\",VLOOKUP(B114,sanschie!$A:$K,7,0),VLOOKUP(B114,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B114=\"\",\"\",VLOOKUP(B114,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B114=\"\",\"0\",IF(VLOOKUP(B114,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B114,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B114,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B114=\"\",\"\",IF(H114=\"N\",VLOOKUP(B114,sanschie!$A:$K,7,0),VLOOKUP(B114,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B115=\"\",\"\",VLOOKUP(B115,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B115=\"\",\"\",VLOOKUP(B115,sanschie!A:D,4,0))","v":""},{"$f":"IF(B115=\"\",\"\",VLOOKUP(B115,sanschie!A:P,16,0))","v":""},{"$f":"IF(B115=\"\",\"\",IF(H115=\"N\",VLOOKUP(B115,sanschie!$A:$K,7,0),VLOOKUP(B115,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B115=\"\",\"\",VLOOKUP(B115,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B115=\"\",\"0\",IF(VLOOKUP(B115,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B115,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B115,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B115=\"\",\"\",IF(H115=\"N\",VLOOKUP(B115,sanschie!$A:$K,7,0),VLOOKUP(B115,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B116=\"\",\"\",VLOOKUP(B116,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B116=\"\",\"\",VLOOKUP(B116,sanschie!A:D,4,0))","v":""},{"$f":"IF(B116=\"\",\"\",VLOOKUP(B116,sanschie!A:P,16,0))","v":""},{"$f":"IF(B116=\"\",\"\",IF(H116=\"N\",VLOOKUP(B116,sanschie!$A:$K,7,0),VLOOKUP(B116,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B116=\"\",\"\",VLOOKUP(B116,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B116=\"\",\"0\",IF(VLOOKUP(B116,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B116,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B116,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B116=\"\",\"\",IF(H116=\"N\",VLOOKUP(B116,sanschie!$A:$K,7,0),VLOOKUP(B116,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B117=\"\",\"\",VLOOKUP(B117,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B117=\"\",\"\",VLOOKUP(B117,sanschie!A:D,4,0))","v":""},{"$f":"IF(B117=\"\",\"\",VLOOKUP(B117,sanschie!A:P,16,0))","v":""},{"$f":"IF(B117=\"\",\"\",IF(H117=\"N\",VLOOKUP(B117,sanschie!$A:$K,7,0),VLOOKUP(B117,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B117=\"\",\"\",VLOOKUP(B117,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B117=\"\",\"0\",IF(VLOOKUP(B117,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B117,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B117,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B117=\"\",\"\",IF(H117=\"N\",VLOOKUP(B117,sanschie!$A:$K,7,0),VLOOKUP(B117,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B118=\"\",\"\",VLOOKUP(B118,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B118=\"\",\"\",VLOOKUP(B118,sanschie!A:D,4,0))","v":""},{"$f":"IF(B118=\"\",\"\",VLOOKUP(B118,sanschie!A:P,16,0))","v":""},{"$f":"IF(B118=\"\",\"\",IF(H118=\"N\",VLOOKUP(B118,sanschie!$A:$K,7,0),VLOOKUP(B118,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B118=\"\",\"\",VLOOKUP(B118,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B118=\"\",\"0\",IF(VLOOKUP(B118,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B118,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B118,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B118=\"\",\"\",IF(H118=\"N\",VLOOKUP(B118,sanschie!$A:$K,7,0),VLOOKUP(B118,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B119=\"\",\"\",VLOOKUP(B119,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B119=\"\",\"\",VLOOKUP(B119,sanschie!A:D,4,0))","v":""},{"$f":"IF(B119=\"\",\"\",VLOOKUP(B119,sanschie!A:P,16,0))","v":""},{"$f":"IF(B119=\"\",\"\",IF(H119=\"N\",VLOOKUP(B119,sanschie!$A:$K,7,0),VLOOKUP(B119,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B119=\"\",\"\",VLOOKUP(B119,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B119=\"\",\"0\",IF(VLOOKUP(B119,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B119,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B119,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B119=\"\",\"\",IF(H119=\"N\",VLOOKUP(B119,sanschie!$A:$K,7,0),VLOOKUP(B119,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B120=\"\",\"\",VLOOKUP(B120,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B120=\"\",\"\",VLOOKUP(B120,sanschie!A:D,4,0))","v":""},{"$f":"IF(B120=\"\",\"\",VLOOKUP(B120,sanschie!A:P,16,0))","v":""},{"$f":"IF(B120=\"\",\"\",IF(H120=\"N\",VLOOKUP(B120,sanschie!$A:$K,7,0),VLOOKUP(B120,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B120=\"\",\"\",VLOOKUP(B120,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B120=\"\",\"0\",IF(VLOOKUP(B120,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B120,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B120,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B120=\"\",\"\",IF(H120=\"N\",VLOOKUP(B120,sanschie!$A:$K,7,0),VLOOKUP(B120,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B121=\"\",\"\",VLOOKUP(B121,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B121=\"\",\"\",VLOOKUP(B121,sanschie!A:D,4,0))","v":""},{"$f":"IF(B121=\"\",\"\",VLOOKUP(B121,sanschie!A:P,16,0))","v":""},{"$f":"IF(B121=\"\",\"\",IF(H121=\"N\",VLOOKUP(B121,sanschie!$A:$K,7,0),VLOOKUP(B121,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B121=\"\",\"\",VLOOKUP(B121,sanschie!$A:$I,9,0))","v":""},{"$f":"IF(H121=1,J121,0)","v":0},{"$f":"IF(H121=2,J121,0)","v":0},{"$f":"IF(B121=\"\",\"0\",IF(VLOOKUP(B121,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B121,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B121,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B121=\"\",\"\",IF(H121=\"N\",VLOOKUP(B121,sanschie!$A:$K,7,0),VLOOKUP(B121,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B122=\"\",\"\",VLOOKUP(B122,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B122=\"\",\"\",VLOOKUP(B122,sanschie!A:D,4,0))","v":""},{"$f":"IF(B122=\"\",\"\",VLOOKUP(B122,sanschie!A:P,16,0))","v":""},{"$f":"IF(B122=\"\",\"\",IF(H122=\"N\",VLOOKUP(B122,sanschie!$A:$K,7,0),VLOOKUP(B122,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B122=\"\",\"\",VLOOKUP(B122,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B122=\"\",\"0\",IF(VLOOKUP(B122,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B122,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B122,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B122=\"\",\"\",IF(H122=\"N\",VLOOKUP(B122,sanschie!$A:$K,7,0),VLOOKUP(B122,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B123=\"\",\"\",VLOOKUP(B123,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B123=\"\",\"\",VLOOKUP(B123,sanschie!A:D,4,0))","v":""},{"$f":"IF(B123=\"\",\"\",VLOOKUP(B123,sanschie!A:P,16,0))","v":""},{"$f":"IF(B123=\"\",\"\",IF(H123=\"N\",VLOOKUP(B123,sanschie!$A:$K,7,0),VLOOKUP(B123,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},{"$f":"IF(F123=\"\",\"\",(F123*I123))","v":""},{"$f":"IF(B123=\"\",\"\",VLOOKUP(B123,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B123=\"\",\"0\",IF(VLOOKUP(B123,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B123,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B123,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B123=\"\",\"\",IF(H123=\"N\",VLOOKUP(B123,sanschie!$A:$K,7,0),VLOOKUP(B123,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B124=\"\",\"\",VLOOKUP(B124,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B124=\"\",\"\",VLOOKUP(B124,sanschie!A:D,4,0))","v":""},{"$f":"IF(B124=\"\",\"\",VLOOKUP(B124,sanschie!A:P,16,0))","v":""},{"$f":"IF(B124=\"\",\"\",IF(H124=\"N\",VLOOKUP(B124,sanschie!$A:$K,7,0),VLOOKUP(B124,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B124=\"\",\"\",VLOOKUP(B124,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B124=\"\",\"0\",IF(VLOOKUP(B124,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B124,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B124,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B124=\"\",\"\",IF(H124=\"N\",VLOOKUP(B124,sanschie!$A:$K,7,0),VLOOKUP(B124,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B125=\"\",\"\",VLOOKUP(B125,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B125=\"\",\"\",VLOOKUP(B125,sanschie!A:D,4,0))","v":""},{"$f":"IF(B125=\"\",\"\",VLOOKUP(B125,sanschie!A:P,16,0))","v":""},{"$f":"IF(B125=\"\",\"\",IF(H125=\"N\",VLOOKUP(B125,sanschie!$A:$K,7,0),VLOOKUP(B125,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B125=\"\",\"\",VLOOKUP(B125,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B125=\"\",\"0\",IF(VLOOKUP(B125,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B125,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B125,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B125=\"\",\"\",IF(H125=\"N\",VLOOKUP(B125,sanschie!$A:$K,7,0),VLOOKUP(B125,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B126=\"\",\"\",VLOOKUP(B126,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B126=\"\",\"\",VLOOKUP(B126,sanschie!A:D,4,0))","v":""},{"$f":"IF(B126=\"\",\"\",VLOOKUP(B126,sanschie!A:P,16,0))","v":""},{"$f":"IF(B126=\"\",\"\",IF(H126=\"N\",VLOOKUP(B126,sanschie!$A:$K,7,0),VLOOKUP(B126,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B126=\"\",\"\",VLOOKUP(B126,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B126=\"\",\"0\",IF(VLOOKUP(B126,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B126,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B126,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B126=\"\",\"\",IF(H126=\"N\",VLOOKUP(B126,sanschie!$A:$K,7,0),VLOOKUP(B126,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B127=\"\",\"\",VLOOKUP(B127,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B127=\"\",\"\",VLOOKUP(B127,sanschie!A:D,4,0))","v":""},{"$f":"IF(B127=\"\",\"\",VLOOKUP(B127,sanschie!A:P,16,0))","v":""},{"$f":"IF(B127=\"\",\"\",IF(H127=\"N\",VLOOKUP(B127,sanschie!$A:$K,7,0),VLOOKUP(B127,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B127=\"\",\"\",VLOOKUP(B127,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B127=\"\",\"0\",IF(VLOOKUP(B127,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B127,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B127,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B127=\"\",\"\",IF(H127=\"N\",VLOOKUP(B127,sanschie!$A:$K,7,0),VLOOKUP(B127,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B128=\"\",\"\",VLOOKUP(B128,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B128=\"\",\"\",VLOOKUP(B128,sanschie!A:D,4,0))","v":""},{"$f":"IF(B128=\"\",\"\",VLOOKUP(B128,sanschie!A:P,16,0))","v":""},{"$f":"IF(B128=\"\",\"\",IF(H128=\"N\",VLOOKUP(B128,sanschie!$A:$K,7,0),VLOOKUP(B128,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B128=\"\",\"\",VLOOKUP(B128,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B128=\"\",\"0\",IF(VLOOKUP(B128,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B128,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B128,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B128=\"\",\"\",IF(H128=\"N\",VLOOKUP(B128,sanschie!$A:$K,7,0),VLOOKUP(B128,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B129=\"\",\"\",VLOOKUP(B129,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B129=\"\",\"\",VLOOKUP(B129,sanschie!A:D,4,0))","v":""},{"$f":"IF(B129=\"\",\"\",VLOOKUP(B129,sanschie!A:P,16,0))","v":""},{"$f":"IF(B129=\"\",\"\",IF(H129=\"N\",VLOOKUP(B129,sanschie!$A:$K,7,0),VLOOKUP(B129,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B129=\"\",\"\",VLOOKUP(B129,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B129=\"\",\"0\",IF(VLOOKUP(B129,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B129,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B129,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B129=\"\",\"\",IF(H129=\"N\",VLOOKUP(B129,sanschie!$A:$K,7,0),VLOOKUP(B129,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B130=\"\",\"\",VLOOKUP(B130,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B130=\"\",\"\",VLOOKUP(B130,sanschie!A:D,4,0))","v":""},{"$f":"IF(B130=\"\",\"\",VLOOKUP(B130,sanschie!A:P,16,0))","v":""},{"$f":"IF(B130=\"\",\"\",IF(H130=\"N\",VLOOKUP(B130,sanschie!$A:$K,7,0),VLOOKUP(B130,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B130=\"\",\"\",VLOOKUP(B130,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B130=\"\",\"0\",IF(VLOOKUP(B130,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B130,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B130,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B130=\"\",\"\",IF(H130=\"N\",VLOOKUP(B130,sanschie!$A:$K,7,0),VLOOKUP(B130,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B131=\"\",\"\",VLOOKUP(B131,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B131=\"\",\"\",VLOOKUP(B131,sanschie!A:D,4,0))","v":""},{"$f":"IF(B131=\"\",\"\",VLOOKUP(B131,sanschie!A:P,16,0))","v":""},{"$f":"IF(B131=\"\",\"\",IF(H131=\"N\",VLOOKUP(B131,sanschie!$A:$K,7,0),VLOOKUP(B131,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B131=\"\",\"\",VLOOKUP(B131,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B131=\"\",\"0\",IF(VLOOKUP(B131,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B131,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B131,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B131=\"\",\"\",IF(H131=\"N\",VLOOKUP(B131,sanschie!$A:$K,7,0),VLOOKUP(B131,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B132=\"\",\"\",VLOOKUP(B132,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B132=\"\",\"\",VLOOKUP(B132,sanschie!A:D,4,0))","v":""},{"$f":"IF(B132=\"\",\"\",VLOOKUP(B132,sanschie!A:P,16,0))","v":""},{"$f":"IF(B132=\"\",\"\",IF(H132=\"N\",VLOOKUP(B132,sanschie!$A:$K,7,0),VLOOKUP(B132,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B132=\"\",\"\",VLOOKUP(B132,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B132=\"\",\"0\",IF(VLOOKUP(B132,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B132,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B132,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B132=\"\",\"\",IF(H132=\"N\",VLOOKUP(B132,sanschie!$A:$K,7,0),VLOOKUP(B132,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B133=\"\",\"\",VLOOKUP(B133,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B133=\"\",\"\",VLOOKUP(B133,sanschie!A:D,4,0))","v":""},{"$f":"IF(B133=\"\",\"\",VLOOKUP(B133,sanschie!A:P,16,0))","v":""},{"$f":"IF(B133=\"\",\"\",IF(H133=\"N\",VLOOKUP(B133,sanschie!$A:$K,7,0),VLOOKUP(B133,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B133=\"\",\"\",VLOOKUP(B133,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B133=\"\",\"0\",IF(VLOOKUP(B133,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B133,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B133,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B133=\"\",\"\",IF(H133=\"N\",VLOOKUP(B133,sanschie!$A:$K,7,0),VLOOKUP(B133,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B134=\"\",\"\",VLOOKUP(B134,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B134=\"\",\"\",VLOOKUP(B134,sanschie!A:D,4,0))","v":""},{"$f":"IF(B134=\"\",\"\",VLOOKUP(B134,sanschie!A:P,16,0))","v":""},{"$f":"IF(B134=\"\",\"\",IF(H134=\"N\",VLOOKUP(B134,sanschie!$A:$K,7,0),VLOOKUP(B134,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B134=\"\",\"\",VLOOKUP(B134,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B134=\"\",\"0\",IF(VLOOKUP(B134,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B134,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B134,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B134=\"\",\"\",IF(H134=\"N\",VLOOKUP(B134,sanschie!$A:$K,7,0),VLOOKUP(B134,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B135=\"\",\"\",VLOOKUP(B135,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B135=\"\",\"\",VLOOKUP(B135,sanschie!A:D,4,0))","v":""},{"$f":"IF(B135=\"\",\"\",VLOOKUP(B135,sanschie!A:P,16,0))","v":""},{"$f":"IF(B135=\"\",\"\",IF(H135=\"N\",VLOOKUP(B135,sanschie!$A:$K,7,0),VLOOKUP(B135,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B135=\"\",\"\",VLOOKUP(B135,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B135=\"\",\"0\",IF(VLOOKUP(B135,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B135,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B135,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B135=\"\",\"\",IF(H135=\"N\",VLOOKUP(B135,sanschie!$A:$K,7,0),VLOOKUP(B135,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B136=\"\",\"\",VLOOKUP(B136,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B136=\"\",\"\",VLOOKUP(B136,sanschie!A:D,4,0))","v":""},{"$f":"IF(B136=\"\",\"\",VLOOKUP(B136,sanschie!A:P,16,0))","v":""},{"$f":"IF(B136=\"\",\"\",IF(H136=\"N\",VLOOKUP(B136,sanschie!$A:$K,7,0),VLOOKUP(B136,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B136=\"\",\"\",VLOOKUP(B136,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B136=\"\",\"0\",IF(VLOOKUP(B136,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B136,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B136,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B136=\"\",\"\",IF(H136=\"N\",VLOOKUP(B136,sanschie!$A:$K,7,0),VLOOKUP(B136,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B137=\"\",\"\",VLOOKUP(B137,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B137=\"\",\"\",VLOOKUP(B137,sanschie!A:D,4,0))","v":""},{"$f":"IF(B137=\"\",\"\",VLOOKUP(B137,sanschie!A:P,16,0))","v":""},{"$f":"IF(B137=\"\",\"\",IF(H137=\"N\",VLOOKUP(B137,sanschie!$A:$K,7,0),VLOOKUP(B137,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B137=\"\",\"\",VLOOKUP(B137,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B137=\"\",\"0\",IF(VLOOKUP(B137,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B137,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B137,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B137=\"\",\"\",IF(H137=\"N\",VLOOKUP(B137,sanschie!$A:$K,7,0),VLOOKUP(B137,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B138=\"\",\"\",VLOOKUP(B138,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B138=\"\",\"\",VLOOKUP(B138,sanschie!A:D,4,0))","v":""},{"$f":"IF(B138=\"\",\"\",VLOOKUP(B138,sanschie!A:P,16,0))","v":""},{"$f":"IF(B138=\"\",\"\",IF(H138=\"N\",VLOOKUP(B138,sanschie!$A:$K,7,0),VLOOKUP(B138,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B138=\"\",\"\",VLOOKUP(B138,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B138=\"\",\"0\",IF(VLOOKUP(B138,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B138,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B138,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B138=\"\",\"\",IF(H138=\"N\",VLOOKUP(B138,sanschie!$A:$K,7,0),VLOOKUP(B138,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B139=\"\",\"\",VLOOKUP(B139,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B139=\"\",\"\",VLOOKUP(B139,sanschie!A:D,4,0))","v":""},{"$f":"IF(B139=\"\",\"\",VLOOKUP(B139,sanschie!A:P,16,0))","v":""},{"$f":"IF(B139=\"\",\"\",IF(H139=\"N\",VLOOKUP(B139,sanschie!$A:$K,7,0),VLOOKUP(B139,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B139=\"\",\"\",VLOOKUP(B139,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B139=\"\",\"0\",IF(VLOOKUP(B139,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B139,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B139,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B139=\"\",\"\",IF(H139=\"N\",VLOOKUP(B139,sanschie!$A:$K,7,0),VLOOKUP(B139,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B140=\"\",\"\",VLOOKUP(B140,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B140=\"\",\"\",VLOOKUP(B140,sanschie!A:D,4,0))","v":""},{"$f":"IF(B140=\"\",\"\",VLOOKUP(B140,sanschie!A:P,16,0))","v":""},{"$f":"IF(B140=\"\",\"\",IF(H140=\"N\",VLOOKUP(B140,sanschie!$A:$K,7,0),VLOOKUP(B140,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B140=\"\",\"\",VLOOKUP(B140,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B140=\"\",\"0\",IF(VLOOKUP(B140,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B140,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B140,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B140=\"\",\"\",IF(H140=\"N\",VLOOKUP(B140,sanschie!$A:$K,7,0),VLOOKUP(B140,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B141=\"\",\"\",VLOOKUP(B141,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B141=\"\",\"\",VLOOKUP(B141,sanschie!A:D,4,0))","v":""},{"$f":"IF(B141=\"\",\"\",VLOOKUP(B141,sanschie!A:P,16,0))","v":""},{"$f":"IF(B141=\"\",\"\",IF(H141=\"N\",VLOOKUP(B141,sanschie!$A:$K,7,0),VLOOKUP(B141,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B141=\"\",\"\",VLOOKUP(B141,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B141=\"\",\"0\",IF(VLOOKUP(B141,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B141,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B141,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B141=\"\",\"\",IF(H141=\"N\",VLOOKUP(B141,sanschie!$A:$K,7,0),VLOOKUP(B141,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B142=\"\",\"\",VLOOKUP(B142,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B142=\"\",\"\",VLOOKUP(B142,sanschie!A:D,4,0))","v":""},{"$f":"IF(B142=\"\",\"\",VLOOKUP(B142,sanschie!A:P,16,0))","v":""},{"$f":"IF(B142=\"\",\"\",IF(H142=\"N\",VLOOKUP(B142,sanschie!$A:$K,7,0),VLOOKUP(B142,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B142=\"\",\"\",VLOOKUP(B142,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B142=\"\",\"0\",IF(VLOOKUP(B142,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B142,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B142,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B142=\"\",\"\",IF(H142=\"N\",VLOOKUP(B142,sanschie!$A:$K,7,0),VLOOKUP(B142,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B143=\"\",\"\",VLOOKUP(B143,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B143=\"\",\"\",VLOOKUP(B143,sanschie!A:D,4,0))","v":""},{"$f":"IF(B143=\"\",\"\",VLOOKUP(B143,sanschie!A:P,16,0))","v":""},{"$f":"IF(B143=\"\",\"\",IF(H143=\"N\",VLOOKUP(B143,sanschie!$A:$K,7,0),VLOOKUP(B143,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B143=\"\",\"\",VLOOKUP(B143,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B143=\"\",\"0\",IF(VLOOKUP(B143,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B143,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B143,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B143=\"\",\"\",IF(H143=\"N\",VLOOKUP(B143,sanschie!$A:$K,7,0),VLOOKUP(B143,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B144=\"\",\"\",VLOOKUP(B144,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B144=\"\",\"\",VLOOKUP(B144,sanschie!A:D,4,0))","v":""},{"$f":"IF(B144=\"\",\"\",VLOOKUP(B144,sanschie!A:P,16,0))","v":""},{"$f":"IF(B144=\"\",\"\",IF(H144=\"N\",VLOOKUP(B144,sanschie!$A:$K,7,0),VLOOKUP(B144,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B144=\"\",\"\",VLOOKUP(B144,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B144=\"\",\"0\",IF(VLOOKUP(B144,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B144,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B144,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B144=\"\",\"\",IF(H144=\"N\",VLOOKUP(B144,sanschie!$A:$K,7,0),VLOOKUP(B144,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B145=\"\",\"\",VLOOKUP(B145,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B145=\"\",\"\",VLOOKUP(B145,sanschie!A:D,4,0))","v":""},{"$f":"IF(B145=\"\",\"\",VLOOKUP(B145,sanschie!A:P,16,0))","v":""},{"$f":"IF(B145=\"\",\"\",IF(H145=\"N\",VLOOKUP(B145,sanschie!$A:$K,7,0),VLOOKUP(B145,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B145=\"\",\"\",VLOOKUP(B145,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B145=\"\",\"0\",IF(VLOOKUP(B145,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B145,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B145,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B145=\"\",\"\",IF(H145=\"N\",VLOOKUP(B145,sanschie!$A:$K,7,0),VLOOKUP(B145,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B146=\"\",\"\",VLOOKUP(B146,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B146=\"\",\"\",VLOOKUP(B146,sanschie!A:D,4,0))","v":""},{"$f":"IF(B146=\"\",\"\",VLOOKUP(B146,sanschie!A:P,16,0))","v":""},{"$f":"IF(B146=\"\",\"\",IF(H146=\"N\",VLOOKUP(B146,sanschie!$A:$K,7,0),VLOOKUP(B146,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B146=\"\",\"\",VLOOKUP(B146,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B146=\"\",\"0\",IF(VLOOKUP(B146,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B146,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B146,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B146=\"\",\"\",IF(H146=\"N\",VLOOKUP(B146,sanschie!$A:$K,7,0),VLOOKUP(B146,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B147=\"\",\"\",VLOOKUP(B147,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B147=\"\",\"\",VLOOKUP(B147,sanschie!A:D,4,0))","v":""},{"$f":"IF(B147=\"\",\"\",VLOOKUP(B147,sanschie!A:P,16,0))","v":""},{"$f":"IF(B147=\"\",\"\",IF(H147=\"N\",VLOOKUP(B147,sanschie!$A:$K,7,0),VLOOKUP(B147,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B147=\"\",\"\",VLOOKUP(B147,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B147=\"\",\"0\",IF(VLOOKUP(B147,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B147,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B147,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B147=\"\",\"\",IF(H147=\"N\",VLOOKUP(B147,sanschie!$A:$K,7,0),VLOOKUP(B147,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B148=\"\",\"\",VLOOKUP(B148,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B148=\"\",\"\",VLOOKUP(B148,sanschie!A:D,4,0))","v":""},{"$f":"IF(B148=\"\",\"\",VLOOKUP(B148,sanschie!A:P,16,0))","v":""},{"$f":"IF(B148=\"\",\"\",IF(H148=\"N\",VLOOKUP(B148,sanschie!$A:$K,7,0),VLOOKUP(B148,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B148=\"\",\"\",VLOOKUP(B148,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B148=\"\",\"0\",IF(VLOOKUP(B148,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B148,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B148,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B148=\"\",\"\",IF(H148=\"N\",VLOOKUP(B148,sanschie!$A:$K,7,0),VLOOKUP(B148,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B149=\"\",\"\",VLOOKUP(B149,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B149=\"\",\"\",VLOOKUP(B149,sanschie!A:D,4,0))","v":""},{"$f":"IF(B149=\"\",\"\",VLOOKUP(B149,sanschie!A:P,16,0))","v":""},{"$f":"IF(B149=\"\",\"\",IF(H149=\"N\",VLOOKUP(B149,sanschie!$A:$K,7,0),VLOOKUP(B149,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B149=\"\",\"\",VLOOKUP(B149,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B149=\"\",\"0\",IF(VLOOKUP(B149,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B149,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B149,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B149=\"\",\"\",IF(H149=\"N\",VLOOKUP(B149,sanschie!$A:$K,7,0),VLOOKUP(B149,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B150=\"\",\"\",VLOOKUP(B150,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B150=\"\",\"\",VLOOKUP(B150,sanschie!A:D,4,0))","v":""},{"$f":"IF(B150=\"\",\"\",VLOOKUP(B150,sanschie!A:P,16,0))","v":""},{"$f":"IF(B150=\"\",\"\",IF(H150=\"N\",VLOOKUP(B150,sanschie!$A:$K,7,0),VLOOKUP(B150,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B150=\"\",\"\",VLOOKUP(B150,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B150=\"\",\"0\",IF(VLOOKUP(B150,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B150,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B150,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B150=\"\",\"\",IF(H150=\"N\",VLOOKUP(B150,sanschie!$A:$K,7,0),VLOOKUP(B150,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B151=\"\",\"\",VLOOKUP(B151,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B151=\"\",\"\",VLOOKUP(B151,sanschie!A:D,4,0))","v":""},{"$f":"IF(B151=\"\",\"\",VLOOKUP(B151,sanschie!A:P,16,0))","v":""},{"$f":"IF(B151=\"\",\"\",IF(H151=\"N\",VLOOKUP(B151,sanschie!$A:$K,7,0),VLOOKUP(B151,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B151=\"\",\"\",VLOOKUP(B151,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B151=\"\",\"0\",IF(VLOOKUP(B151,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B151,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B151,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B151=\"\",\"\",IF(H151=\"N\",VLOOKUP(B151,sanschie!$A:$K,7,0),VLOOKUP(B151,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B152=\"\",\"\",VLOOKUP(B152,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B152=\"\",\"\",VLOOKUP(B152,sanschie!A:D,4,0))","v":""},{"$f":"IF(B152=\"\",\"\",VLOOKUP(B152,sanschie!A:P,16,0))","v":""},{"$f":"IF(B152=\"\",\"\",IF(H152=\"N\",VLOOKUP(B152,sanschie!$A:$K,7,0),VLOOKUP(B152,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},{"$f":"IF(F152=\"\",\"\",(F152*I152))","v":""},{"$f":"IF(B152=\"\",\"\",VLOOKUP(B152,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B152=\"\",\"0\",IF(VLOOKUP(B152,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B152,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B152,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B152=\"\",\"\",IF(H152=\"N\",VLOOKUP(B152,sanschie!$A:$K,7,0),VLOOKUP(B152,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B153=\"\",\"\",VLOOKUP(B153,sanschie!A:E,5,0))","v":""},{"$f":"IF(F153=\"\",\"\",K153*F153)","v":""},{"$f":"IF(F153=\"\",\"\",IF(N153=\"\",\"\",N153*F153))","v":""},"",{"$f":"IF(B153=\"\",\"\",VLOOKUP(B153,sanschie!A:D,4,0))","v":""},{"$f":"IF(B153=\"\",\"\",VLOOKUP(B153,sanschie!A:P,16,0))","v":""},{"$f":"IF(B153=\"\",\"\",IF(H153=\"N\",VLOOKUP(B153,sanschie!$A:$K,7,0),VLOOKUP(B153,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B153=\"\",\"\",VLOOKUP(B153,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B153=\"\",\"0\",IF(VLOOKUP(B153,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B153,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B153,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B153=\"\",\"\",IF(H153=\"N\",VLOOKUP(B153,sanschie!$A:$K,7,0),VLOOKUP(B153,sanschie!$A:$K,7,0)))","v":""}]
["","",{"$f":"IF(B154=\"\",\"\",VLOOKUP(B154,sanschie!A:E,5,0))","v":""},"","","",{"$f":"IF(B154=\"\",\"\",VLOOKUP(B154,sanschie!A:D,4,0))","v":""},{"$f":"IF(B154=\"\",\"\",VLOOKUP(B154,sanschie!A:P,16,0))","v":""},{"$f":"IF(B154=\"\",\"\",IF(H154=\"N\",VLOOKUP(B154,sanschie!$A:$K,7,0),VLOOKUP(B154,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},{"$f":"IF(F154=\"\",\"\",(F154*I154))","v":""},{"$f":"IF(B154=\"\",\"\",VLOOKUP(B154,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B154=\"\",\"0\",IF(VLOOKUP(B154,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B154,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B154,sanschie!$A:$K,10,0)))))","v":"0"},null,null,{"$f":"IF(H154=3,J154,0)","v":0},{"$f":"IF(B154=\"\",\"\",IF(H154=\"N\",VLOOKUP(B154,sanschie!$A:$K,7,0),VLOOKUP(B154,sanschie!$A:$K,7,0)))","v":""}]
[null,null,{"$f":"IF(F155=1,Vokabel!$A$391,\"\")","v":""},null,null,{"$f":"IF(F157=0,\"\",1)","v":""},null,null,null,{"$f":"SUM(J25:J154)","v":2886}]
[null,"VL-PPL 0,6 Ø 180",{"$f":"IF(F156=\"\",\"\",IF(A17=\"Technostar\",'Verbindungsleitung TS'!E2,Verbindungsleitung!E2))","v":""},null,null,{"$f":"IF(F157=0,\"\",1)","v":""}]
["",null,{"$f":"IF(B157=\"\",\"\",VLOOKUP(B157,sanschie!A:E,5,0))","v":""},{"$f":"IF(F157=\"\",\"\",K157*F157)","v":""},{"$f":"IF(F157=\"\",\"\",IF(N157=\"\",\"\",N157*F157))","v":""},null,{"$f":"IF(B157=\"\",\"\",VLOOKUP(B157,sanschie!A:D,4,0))","v":""},{"$f":"IF(B157=\"\",\"\",VLOOKUP(B157,sanschie!A:P,16,0))","v":""},{"$f":"IF(B157=\"\",\"\",IF(H157=\"N\",VLOOKUP(B157,sanschie!$A:$K,7,0),VLOOKUP(B157,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},{"$f":"IF(F157=\"\",\"\",(F157*I157))","v":""},{"$f":"IF(B157=\"\",\"\",VLOOKUP(B157,sanschie!$A:$I,9,0))","v":""},{"$f":"IF(H157=1,J157,0)","v":0},{"$f":"IF(H157=2,J157,0)","v":0},{"$f":"IF(B157=\"\",\"0\",IF(VLOOKUP(B157,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B157,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B157,sanschie!$A:$K,10,0)))))","v":"0"},null,null,{"$f":"IF(H157=3,J157,0)","v":0},{"$f":"IF(B157=\"\",\"\",IF(H157=\"N\",VLOOKUP(B157,sanschie!$A:$K,7,0),VLOOKUP(B157,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B158=\"\",\"\",VLOOKUP(B158,sanschie!A:E,5,0))","v":""},{"$f":"IF(F158=\"\",\"\",K158*F158)","v":""},{"$f":"IF(F158=\"\",\"\",IF(N158=\"\",\"\",N158*F158))","v":""},null,{"$f":"IF(B158=\"\",\"\",VLOOKUP(B158,sanschie!A:D,4,0))","v":""},{"$f":"IF(B158=\"\",\"\",VLOOKUP(B158,sanschie!A:P,16,0))","v":""},{"$f":"IF(B158=\"\",\"\",IF(H158=\"N\",VLOOKUP(B158,sanschie!$A:$K,7,0),VLOOKUP(B158,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B158=\"\",\"\",VLOOKUP(B158,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B158=\"\",\"0\",IF(VLOOKUP(B158,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B158,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B158,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B158=\"\",\"\",IF(H158=\"N\",VLOOKUP(B158,sanschie!$A:$K,7,0),VLOOKUP(B158,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B159=\"\",\"\",VLOOKUP(B159,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B159=\"\",\"\",VLOOKUP(B159,sanschie!A:D,4,0))","v":""},{"$f":"IF(B159=\"\",\"\",VLOOKUP(B159,sanschie!A:P,16,0))","v":""},{"$f":"IF(B159=\"\",\"\",IF(H159=\"N\",VLOOKUP(B159,sanschie!$A:$K,7,0),VLOOKUP(B159,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B159=\"\",\"\",VLOOKUP(B159,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B159=\"\",\"0\",IF(VLOOKUP(B159,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B159,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B159,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B159=\"\",\"\",IF(H159=\"N\",VLOOKUP(B159,sanschie!$A:$K,7,0),VLOOKUP(B159,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B160=\"\",\"\",VLOOKUP(B160,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B160=\"\",\"\",VLOOKUP(B160,sanschie!A:D,4,0))","v":""},{"$f":"IF(B160=\"\",\"\",VLOOKUP(B160,sanschie!A:P,16,0))","v":""},{"$f":"IF(B160=\"\",\"\",IF(H160=\"N\",VLOOKUP(B160,sanschie!$A:$K,7,0),VLOOKUP(B160,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B160=\"\",\"\",VLOOKUP(B160,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B160=\"\",\"0\",IF(VLOOKUP(B160,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B160,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B160,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B160=\"\",\"\",IF(H160=\"N\",VLOOKUP(B160,sanschie!$A:$K,7,0),VLOOKUP(B160,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B161=\"\",\"\",VLOOKUP(B161,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B161=\"\",\"\",VLOOKUP(B161,sanschie!A:D,4,0))","v":""},{"$f":"IF(B161=\"\",\"\",VLOOKUP(B161,sanschie!A:P,16,0))","v":""},{"$f":"IF(B161=\"\",\"\",IF(H161=\"N\",VLOOKUP(B161,sanschie!$A:$K,7,0),VLOOKUP(B161,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B161=\"\",\"\",VLOOKUP(B161,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B161=\"\",\"0\",IF(VLOOKUP(B161,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B161,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B161,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B161=\"\",\"\",IF(H161=\"N\",VLOOKUP(B161,sanschie!$A:$K,7,0),VLOOKUP(B161,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B162=\"\",\"\",VLOOKUP(B162,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B162=\"\",\"\",VLOOKUP(B162,sanschie!A:D,4,0))","v":""},{"$f":"IF(B162=\"\",\"\",VLOOKUP(B162,sanschie!A:P,16,0))","v":""},{"$f":"IF(B162=\"\",\"\",IF(H162=\"N\",VLOOKUP(B162,sanschie!$A:$K,7,0),VLOOKUP(B162,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B162=\"\",\"\",VLOOKUP(B162,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B162=\"\",\"0\",IF(VLOOKUP(B162,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B162,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B162,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B162=\"\",\"\",IF(H162=\"N\",VLOOKUP(B162,sanschie!$A:$K,7,0),VLOOKUP(B162,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B163=\"\",\"\",VLOOKUP(B163,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B163=\"\",\"\",VLOOKUP(B163,sanschie!A:D,4,0))","v":""},{"$f":"IF(B163=\"\",\"\",VLOOKUP(B163,sanschie!A:P,16,0))","v":""},{"$f":"IF(B163=\"\",\"\",IF(H163=\"N\",VLOOKUP(B163,sanschie!$A:$K,7,0),VLOOKUP(B163,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B163=\"\",\"\",VLOOKUP(B163,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B163=\"\",\"0\",IF(VLOOKUP(B163,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B163,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B163,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B163=\"\",\"\",IF(H163=\"N\",VLOOKUP(B163,sanschie!$A:$K,7,0),VLOOKUP(B163,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B164=\"\",\"\",VLOOKUP(B164,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B164=\"\",\"\",VLOOKUP(B164,sanschie!A:D,4,0))","v":""},{"$f":"IF(B164=\"\",\"\",VLOOKUP(B164,sanschie!A:P,16,0))","v":""},{"$f":"IF(B164=\"\",\"\",IF(H164=\"N\",VLOOKUP(B164,sanschie!$A:$K,7,0),VLOOKUP(B164,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B164=\"\",\"\",VLOOKUP(B164,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B164=\"\",\"0\",IF(VLOOKUP(B164,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B164,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B164,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B164=\"\",\"\",IF(H164=\"N\",VLOOKUP(B164,sanschie!$A:$K,7,0),VLOOKUP(B164,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B165=\"\",\"\",VLOOKUP(B165,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B165=\"\",\"\",VLOOKUP(B165,sanschie!A:D,4,0))","v":""},{"$f":"IF(B165=\"\",\"\",VLOOKUP(B165,sanschie!A:P,16,0))","v":""},{"$f":"IF(B165=\"\",\"\",IF(H165=\"N\",VLOOKUP(B165,sanschie!$A:$K,7,0),VLOOKUP(B165,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B165=\"\",\"\",VLOOKUP(B165,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B165=\"\",\"0\",IF(VLOOKUP(B165,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B165,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B165,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B165=\"\",\"\",IF(H165=\"N\",VLOOKUP(B165,sanschie!$A:$K,7,0),VLOOKUP(B165,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B166=\"\",\"\",VLOOKUP(B166,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B166=\"\",\"\",VLOOKUP(B166,sanschie!A:D,4,0))","v":""},{"$f":"IF(B166=\"\",\"\",VLOOKUP(B166,sanschie!A:P,16,0))","v":""},{"$f":"IF(B166=\"\",\"\",IF(H166=\"N\",VLOOKUP(B166,sanschie!$A:$K,7,0),VLOOKUP(B166,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B166=\"\",\"\",VLOOKUP(B166,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B166=\"\",\"0\",IF(VLOOKUP(B166,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B166,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B166,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B166=\"\",\"\",IF(H166=\"N\",VLOOKUP(B166,sanschie!$A:$K,7,0),VLOOKUP(B166,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B167=\"\",\"\",VLOOKUP(B167,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B167=\"\",\"\",VLOOKUP(B167,sanschie!A:D,4,0))","v":""},{"$f":"IF(B167=\"\",\"\",VLOOKUP(B167,sanschie!A:P,16,0))","v":""},{"$f":"IF(B167=\"\",\"\",IF(H167=\"N\",VLOOKUP(B167,sanschie!$A:$K,7,0),VLOOKUP(B167,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B167=\"\",\"\",VLOOKUP(B167,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B167=\"\",\"0\",IF(VLOOKUP(B167,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B167,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B167,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B167=\"\",\"\",IF(H167=\"N\",VLOOKUP(B167,sanschie!$A:$K,7,0),VLOOKUP(B167,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B168=\"\",\"\",VLOOKUP(B168,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B168=\"\",\"\",VLOOKUP(B168,sanschie!A:D,4,0))","v":""},{"$f":"IF(B168=\"\",\"\",VLOOKUP(B168,sanschie!A:P,16,0))","v":""},{"$f":"IF(B168=\"\",\"\",IF(H168=\"N\",VLOOKUP(B168,sanschie!$A:$K,7,0),VLOOKUP(B168,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B168=\"\",\"\",VLOOKUP(B168,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B168=\"\",\"0\",IF(VLOOKUP(B168,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B168,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B168,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B168=\"\",\"\",IF(H168=\"N\",VLOOKUP(B168,sanschie!$A:$K,7,0),VLOOKUP(B168,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B169=\"\",\"\",VLOOKUP(B169,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B169=\"\",\"\",VLOOKUP(B169,sanschie!A:D,4,0))","v":""},{"$f":"IF(B169=\"\",\"\",VLOOKUP(B169,sanschie!A:P,16,0))","v":""},{"$f":"IF(B169=\"\",\"\",IF(H169=\"N\",VLOOKUP(B169,sanschie!$A:$K,7,0),VLOOKUP(B169,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B169=\"\",\"\",VLOOKUP(B169,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B169=\"\",\"0\",IF(VLOOKUP(B169,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B169,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B169,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B169=\"\",\"\",IF(H169=\"N\",VLOOKUP(B169,sanschie!$A:$K,7,0),VLOOKUP(B169,sanschie!$A:$K,7,0)))","v":""}]
[" ",null,{"$f":"IF(B170=\"\",\"\",VLOOKUP(B170,sanschie!A:E,5,0))","v":""},"","",null,{"$f":"IF(B170=\"\",\"\",VLOOKUP(B170,sanschie!A:D,4,0))","v":""},{"$f":"IF(B170=\"\",\"\",VLOOKUP(B170,sanschie!A:P,16,0))","v":""},{"$f":"IF(B170=\"\",\"\",IF(H170=\"N\",VLOOKUP(B170,sanschie!$A:$K,7,0),VLOOKUP(B170,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},"",{"$f":"IF(B170=\"\",\"\",VLOOKUP(B170,sanschie!$A:$I,9,0))","v":""},0,0,{"$f":"IF(B170=\"\",\"0\",IF(VLOOKUP(B170,sanschie!$A:$K,10,0)=0,\"0\",IF(VLOOKUP(B170,sanschie!$A:$K,10,0)=\"\",\"0\",(VLOOKUP(B170,sanschie!$A:$K,10,0)))))","v":"0"},null,null,0,{"$f":"IF(B170=\"\",\"\",IF(H170=\"N\",VLOOKUP(B170,sanschie!$A:$K,7,0),VLOOKUP(B170,sanschie!$A:$K,7,0)))","v":""}]
[null,null,{"$f":"IF(F171=1,Vokabel!$A$393,\"\")","v":""},null,null,{"$f":"IF(F156=\"\",\"\",1)","v":""},null,null,null,{"$f":"SUM(J157:J170)","v":0}]
["",{"$f":"IF(Eingabe!$M$23+Eingabe!$M$24+Eingabe!$M$25=0,0,Vokabel!$A$316)","v":0},null,null,null,{"$f":"IF(B172=0,\"\",\"1\")","v":""},null,null,null,null,null,{"$f":"SUM(L25:L171)","v":2886},{"$f":"SUM(M25:M171)","v":0},null,null,null,{"$f":"SUM(Q25:Q171)","v":0}]
[null,{"$f":"IF(Eingabe!$M$23+Eingabe!$M$24+Eingabe!$M$25=0,0,Texte!D3)","v":0},null,null,null,{"$f":"IF(B173=0,\"\",\"1\")","v":""}]
[null,{"$f":"IF(Eingabe!$M$23+Eingabe!$M$24+Eingabe!$M$25=0,0,Texte!D4)","v":0},null,null,null,{"$f":"IF(B174=0,\"\",\"1\")","v":""}]
[null,{"$f":"IF(Eingabe!$M$23+Eingabe!$M$24+Eingabe!$M$25=0,0,Texte!D5)","v":0},null,null,null,{"$f":"IF(B175=0,\"\",\"1\")","v":""}]
[null,{"$f":"IF(Eingabe!$M$23+Eingabe!$M$24+Eingabe!$M$25=0,0,Texte!D6)","v":0},null,null,null,{"$f":"IF(B176=0,\"\",\"1\")","v":""}]
[null,{"$f":"Vokabel!$A$305","v":"Facharbeiterstunden"},null,null,null,{"$f":"IF(Eingabe!M23=\"\",\"\",IF(Eingabe!M23=\"0\",\"\",Eingabe!M23))","v":""},{"$f":"Vokabel!$A$308","v":"STD"},null,{"$f":"Eingabe!O23","v":0},{"$f":"IF(F177=\"\",\"\",(F177*I177))","v":""}]
[null,{"$f":"Vokabel!$A$306","v":"Kilometer"},null,null,null,{"$f":"IF(Eingabe!M24=\"\",\"\",IF(Eingabe!M24=\"0\",\"\",Eingabe!M24))","v":""},"km",null,{"$f":"Eingabe!O24","v":0},{"$f":"IF(F178=\"\",\"\",(F178*I178))","v":""}]
[null,{"$f":"Vokabel!$A$307","v":"Pauschale Montagearbeit"},null,null,null,{"$f":"IF(Eingabe!M25=\"\",\"\",IF(Eingabe!M25=\"0\",\"\",Eingabe!M25))","v":""},{"$f":"Vokabel!$A$309","v":"Pausch"},null,{"$f":"Eingabe!O25","v":0},{"$f":"IF(F179=\"\",\"\",(F179*I179))","v":""},null,{"$f":"SUM(J177:J179)","v":0}]
[null,null,null,null,null,1,null,null,null,null,null,{"$f":"Vokabel!$A$210","v":"Fracht"},{"$f":"Vokabel!$A$209","v":"per Tonne"},null,{"$f":"Vokabel!$A$211","v":"lief.PLZ"},null,{"$f":"Vokabel!$A$212","v":"man. Fracht"}]
[null,null,null,null,null,{"$f":"IF(J187=\"\",Vokabel!$A$201,Vokabel!$A$202)","v":"Summe Bauteile"},null,null,null,{"$f":"SUM(J25:J154,J157:J170)","v":2886},null,null,null,null,{"$f":"IF(Eingabe!$K$18=\"\",Eingabe!$K$7,Eingabe!$K$18)","v":"5312"}]
[null,null,null,null,null,{"$f":"IF(L179=0,\"\",Vokabel!$A$310)","v":""},null,null,null,{"$f":"L179","v":0}]
[null,null,null,null,null,{"$f":"IF(I183=\"\",\"\",IF(Eingabe!$O$21=\"\",\"\",\"-\"&Eingabe!$O$21*100&Vokabel!$A$203))","v":""},null,null,{"$f":"IF(Eingabe!$O$21=0,\"\",IF(Eingabe!$O$21=\"\",\"\",Kalkulation!$L$172))","v":""},{"$f":"IF(Eingabe!$O$21=0,0,IF(Eingabe!$O$21=\"\",0,L183))","v":0},{"$f":"Eingabe!O21*100","v":0},{"$f":"-L172*Eingabe!$O$21","v":0}]
[null,null,null,null,null,{"$f":"IF(I184=\"\",\"\",IF(Eingabe!$O$22=\"\",\"\",\"-\"&Eingabe!$O$22*100&Vokabel!$A$321))","v":""},null,null,{"$f":"IF(Eingabe!$O$22=0,\"\",IF(Eingabe!$O$22=\"\",\"\",Kalkulation!$M$172))","v":""},{"$f":"IF(Eingabe!$O$22=0,0,IF(Eingabe!$O$22=\"\",0,L184))","v":0},{"$f":"Eingabe!O22*100","v":0},{"$f":"-M172*Eingabe!$O$22","v":0}]
[null,null,null,null,null,{"$f":"IF(I185=\"\",\"\",IF(Eingabe!$M$22=\"\",\"\",\"-\"&Eingabe!$M$22*100&Vokabel!$A$490))","v":""},null,null,{"$f":"IF(Eingabe!$M$22=0,\"\",IF(Eingabe!$M$22=\"\",\"\",Kalkulation!$Q$172))","v":""},{"$f":"IF(Eingabe!$M$22=0,0,IF(Eingabe!$M$22=\"\",0,L185))","v":0},{"$f":"Eingabe!M22*100","v":0},{"$f":"-Q172*Eingabe!$M$22","v":0}]
[null,null,null,null,null,{"$f":"IF(Daten!$D$102=2,\"\",IF(Daten!$D$83=1,Vokabel!$A$204,IF(Einstellungstabelle!$B$2=\"N\",\"\",IF(Daten!$D$102=1,Vokabel!$A$205,\"\"))))","v":"Fracht (ab Werk)"},null,null,null,{"$f":"IF(Daten!$D$102=1,Kalkulation!N186,0)","v":197},{"$f":"J186","v":197},null,{"$f":"IF(SUBTOTAL(9,D25:D170)<=1000,0,SUBTOTAL(9,D25:D170)-1000)/1000","v":0},{"$f":"IF(Q181<>0,Q181,IF(Daten!$D$83=1,Firma!E14+Firma!E14*Kalkulation!M186,IF(Einstellungstabelle!$B$2=\"N\",0,IF(Q181=0,Einstellungstabelle!C5,Q181))))","v":197}]
[null,null,null,null,null,{"$f":"IF(J182+J183+J184+J186=0,\"\",Vokabel!$A$206)","v":"Nettobetrag CHF"},null,null,null,{"$f":"IF(J182+J183+J184+J185+J186=0,\"\",SUM(J181:J186))","v":3083},null,{"$f":"SUM(J181:J186)","v":3083}]
[null,{"$f":"VLOOKUP(A17,Daten!$B$147:$C$157,2,0)","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,{"$f":"IF(Eingabe!O27=0,\"\",K188&Vokabel!$A$207)","v":"7,7 % MwSt."},null,null,null,{"$f":"IF(Eingabe!O27=0,\"\",Kalkulation!L187*Eingabe!O27)","v":237.39099999999999},{"$f":"Eingabe!O27*100","v":7.7},{"$f":"Eingabe!O27","v":7.6999999999999999E-2}]
[null,null,null,null,null,{"$f":"IF(Eingabe!O27=0,\"\",Vokabel!$A$208)","v":"Gesamtbetrag  CHF"},null,null,null,{"$f":"IF(Eingabe!O27=0,\"\",Kalkulation!L187+Kalkulation!J188)","v":3320.3910000000001}]
[]
[]
[null,{"$f":"IF(Belegart!$A$1=2,Texte!D18,\"\")","v":0}]
[null,{"$f":"IF(Belegart!$A$1=2,Texte!D19,\"\")","v":0}]
[null,{"$f":"IF(Belegart!$A$1=2,Texte!D20,\"\")","v":"Wir hoffen, dass Ihnen unser Angebot zusagt und freuen uns auf Ihren Auftrag."}]
[null,{"$f":"IF(Belegart!$A$1=2,Texte!$D$21,\"\")","v":"Freundliche Grüsse"}]
[null,{"$f":"IF(Belegart!$A$1=2,J9,\"\")","v":"Herr Mustermann"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"IF(B228=\"\",\"\",VLOOKUP(B228,sanschie!A:E,5,0))","v":""},{"$f":"IF(F228=\"\",\"\",K228*F228)","v":""},{"$f":"IF(F228=\"\",\"\",IF(N228=\"\",\"\",N228*F228))","v":""},null,{"$f":"IF(B228=\"\",\"\",VLOOKUP(B228,sanschie!A:D,4,0))","v":""},{"$f":"IF(B228=\"\",\"\",VLOOKUP(B228,sanschie!A:P,16,0))","v":""},{"$f":"IF(B228=\"\",\"\",IF(H228=\"N\",VLOOKUP(B228,sanschie!$A:$K,7,0),VLOOKUP(B228,sanschie!$A:$K,7,0)*(1-Eingabe!$O$20)))","v":""},{"$f":"IF(F228=\"\",\"\",(F228*I228))","v":""},null,null,null,null,{"$f":"IF(Eingabe!$K$18=\"\",Eingabe!$K$7,Eingabe!$K$18)","v":"5312"}]

{"sheet":"sanschie","index":27,"n_rows":4706,"n_cols":32,"rows_kept":2250,"cut":true,"hidden":true,"merged":[],"bounds":{"rows_first":1000,"rows_last":250,"rows_between":1000,"halvings":1}}
[]
[]
[]
["DPRANR","DPRANR","DASKAT","DPRMEN","DASAB1","WAE",null,"DASOMH","DASGWW","DVA020","DVA026"]
[]
["Artikel-Nr","Artikel-Nr","EAN","Mengeneinheit","Artikelbezeichnung 1","Währung",null,"Palettenmenge","Gewicht","Einbaulänge","Rabattfähig"]
["Kerastar 140","Kerastar 140",null,"Anlage","Kerastar Anlage Ø 140","EUR",null,0,0,null,"J"]
["Kerastar 160","Kerastar 160",null,"Anlage","Kerastar Anlage Ø 160","EUR",null,0,0,null,"J"]
["Kerastar 180","Kerastar 180",null,"Anlage","Kerastar Anlage Ø 180","EUR",null,0,0,null,"J"]
["Kerastar 200","Kerastar 200",null,"Anlage","Kerastar Anlage Ø 200","EUR",null,0,0,null,"J"]
["Kerastar 250","Kerastar 250",null,"Anlage","Kerastar Anlage Ø 250","EUR",null,0,0,null,"J"]
["Kerastar 300","Kerastar 300",null,"Anlage","Kerastar Anlage Ø 300","EUR",null,0,0,null,"J"]
["Kerastar 400","Kerastar 400",null,"Anlage","Kerastar Anlage Ø 400","EUR",null,0,0,null,"J"]
["Keranova 120","Keranova 120",null,"Anlage","Keranova Anlage Ø 120","EUR",null,0,0,null,"J"]
["Keranova 140","Keranova 140",null,"Anlage","Keranova Anlage Ø 140","EUR",null,0,0,null,"J"]
["Keranova 160","Keranova 160",null,"Anlage","Keranova Anlage Ø 160","EUR",null,0,0,null,"J"]
["Keranova 180","Keranova 180",null,"Anlage","Keranova Anlage Ø 180","EUR",null,0,0,null,"J"]
["Keranova 200","Keranova 200",null,"Anlage","Keranova Anlage Ø 200","EUR",null,0,0,null,"J"]
["Keranova 250","Keranova 250",null,"Anlage","Keranova Anlage Ø 250","EUR",null,0,0,null,"J"]
["Technostar12060","Technostar12060",null,"Anlage","Technostar Anlage Ø 60","EUR",null,0,0,null,"J"]
["Technostar12080","Technostar12080",null,"Anlage","Technostar Anlage Ø 80","EUR",null,0,0,null,"J"]
["Technostar120110","Technostar120110",null,"Anlage","Technostar Anlage Ø 110","EUR",null,0,0,null,"J"]
["Technostar120125","Technostar120125",null,"Anlage","Technostar Anlage Ø 125","EUR",null,0,0,null,"J"]
["Technostar120160","Technostar120160",null,"Anlage","Technostar Anlage Ø 160","EUR",null,0,0,null,"J"]
["Technostar120200","Technostar120200",null,"Anlage","Technostar Anlage Ø 200","EUR",null,0,0,null,"J"]
["Technostar120250","Technostar120250",null,"Anlage","Technostar Anlage Ø 250","EUR",null,0,0,null,"J"]
["Absolut 14","Absolut 14",null,"Anlage","Absolut-Kaminanlage Ø 14","EUR",null,0,0,null,"J"]
["Absolut 16","Absolut 16",null,"Anlage","Absolut-Kaminanlage Ø 16","EUR",null,0,0,null,"J"]
["Absolut 18","Absolut 18",null,"Anlage","Absolut-Kaminanlage Ø 18","EUR",null,0,0,null,"J"]
["Absolut 20","Absolut 20",null,"Anlage","Absolut-Kaminanlage Ø 20","EUR",null,0,0,null,"J"]
["Absolut 25","Absolut 25",null,"Anlage","Absolut-Kaminanlage Ø 25","EUR",null,0,0,null,"J"]
["Absolut 30","Absolut 30",null,"Anlage","Absolut-Kaminanlage Ø 30","EUR",null,0,0,null,"J"]
["Absolut 40","Absolut 40",null,"Anlage","Absolut-Kaminanlage Ø 40","EUR",null,0,0,null,"J"]
["Absolut 14TL","Absolut 14TL",null,"Anlage","Absolut-Kaminanlage Ø 14TL","EUR",null,0,0,null,"J"]
["Absolut 16TL","Absolut 16TL",null,"Anlage","Absolut-Kaminanlage Ø 16TL","EUR",null,0,0,null,"J"]
["Absolut 18TL","Absolut 18TL",null,"Anlage","Absolut-Kaminanlage Ø 18TL","EUR",null,0,0,null,"J"]
["Absolut 20TL","Absolut 20TL",null,"Anlage","Absolut-Kaminanlage Ø 20TL","EUR",null,0,0,null,"J"]
["Absolut 25TL","Absolut 25TL",null,"Anlage","Absolut-Kaminanlage Ø 25TL","EUR",null,0,0,null,"J"]
["Absolut 30L","Absolut 30L",null,"Anlage","Absolut-Kaminanlage Ø 30L","EUR",null,0,0,null,"J"]
["Absolut 40L","Absolut 40L",null,"Anlage","Absolut-Kaminanlage Ø 40L","EUR",null,0,0,null,"J"]
["Absolut 1414","Absolut 1414",null,"Anlage","Absolut-Kaminanlage Ø 1414","EUR",null,0,0,null,"J"]
["Absolut 1616","Absolut 1616",null,"Anlage","Absolut-Kaminanlage Ø 1616","EUR",null,0,0,null,"J"]
["Absolut 1818","Absolut 1818",null,"Anlage","Absolut-Kaminanlage Ø 1818","EUR",null,0,0,null,"J"]
["Absolut 2020","Absolut 2020",null,"Anlage","Absolut-Kaminanlage Ø 2020","EUR",null,0,0,null,"J"]
["Absolut 14TL14","Absolut 14TL14",null,"Anlage","Absolut-Kaminanlage Ø 14TL14","EUR",null,0,0,null,"J"]
["Absolut 16TL16","Absolut 16TL16",null,"Anlage","Absolut-Kaminanlage Ø 16TL16","EUR",null,0,0,null,"J"]
["Absolut 18TL18","Absolut 18TL18",null,"Anlage","Absolut-Kaminanlage Ø 18TL18","EUR",null,0,0,null,"J"]
["Absolut 20TL20","Absolut 20TL20",null,"Anlage","Absolut-Kaminanlage Ø 20TL20","EUR",null,0,0,null,"J"]
["Absolut 1614","Absolut 1614",null,"Anlage","Absolut-Kaminanlage Ø 1614","EUR",null,0,0,null,"J"]
["Absolut 1814","Absolut 1814",null,"Anlage","Absolut-Kaminanlage Ø 1814","EUR",null,0,0,null,"J"]
["Absolut 1816","Absolut 1816",null,"Anlage","Absolut-Kaminanlage Ø 1816","EUR",null,0,0,null,"J"]
["Absolut 2014","Absolut 2014",null,"Anlage","Absolut-Kaminanlage Ø 2014","EUR",null,0,0,null,"J"]
["Absolut 2016","Absolut 2016",null,"Anlage","Absolut-Kaminanlage Ø 2016","EUR",null,0,0,null,"J"]
["Absolut 2018","Absolut 2018",null,"Anlage","Absolut-Kaminanlage Ø 2018","EUR",null,0,0,null,"J"]
["Absolut 16TL14","Absolut 16TL14",null,"Anlage","Absolut-Kaminanlage Ø 16TL14","EUR",null,0,0,null,"J"]
["Absolut 18TL14","Absolut 18TL14",null,"Anlage","Absolut-Kaminanlage Ø 18TL14","EUR",null,0,0,null,"J"]
["Absolut 18TL16","Absolut 18TL16",null,"Anlage","Absolut-Kaminanlage Ø 18TL16","EUR",null,0,0,null,"J"]
["Absolut 20TL14","Absolut 20TL14",null,"Anlage","Absolut-Kaminanlage Ø 20TL14","EUR",null,0,0,null,"J"]
["Absolut 20TL16","Absolut 20TL16",null,"Anlage","Absolut-Kaminanlage Ø 20TL16","EUR",null,0,0,null,"J"]
["Absolut 20TL18","Absolut 20TL18",null,"Anlage","Absolut-Kaminanlage Ø 20TL18","EUR",null,0,0,null,"J"]
["CHEMINEE 16","CHEMINEE 16",null,"Anlage","CHEMINEE-Kaminanlage Ø 16","EUR",null,0,0,null,"J"]
["CHEMINEE 18","CHEMINEE 18",null,"Anlage","CHEMINEE-Kaminanlage Ø 18","EUR",null,0,0,null,"J"]
["CHEMINEE 20","CHEMINEE 20",null,"Anlage","CHEMINEE-Kaminanlage Ø 20","EUR",null,0,0,null,"J"]
["CHEMINEE 25","CHEMINEE 25",null,"Anlage","CHEMINEE-Kaminanlage Ø 25","EUR",null,0,0,null,"J"]
["CHEMINEE 30","CHEMINEE 30",null,"Anlage","CHEMINEE-Kaminanlage Ø 30","EUR",null,0,0,null,"J"]
["CHEMINEE 1616","CHEMINEE 1616",null,"Anlage","CHEMINEE-Kaminanlage Ø 1616","EUR",null,0,0,null,"J"]
["CHEMINEE 1818","CHEMINEE 1818",null,"Anlage","CHEMINEE-Kaminanlage Ø 1818","EUR",null,0,0,null,"J"]
["CHEMINEE 2020","CHEMINEE 2020",null,"Anlage","CHEMINEE-Kaminanlage Ø 2020","EUR",null,0,0,null,"J"]
["CHEMINEE 2525","CHEMINEE 2525",null,"Anlage","CHEMINEE-Kaminanlage Ø 2525","EUR",null,0,0,null,"J"]
["CHEMINEE 3030","CHEMINEE 3030",null,"Anlage","CHEMINEE-Kaminanlage Ø 3030","EUR",null,0,0,null,"J"]
["ISOLIT16","ISOLIT16",null,"Anlage","Schiedel ISOLIT 16/16","EUR",null,0,0,null,"J"]
["ISOLIT20","ISOLIT20",null,"Anlage","Schiedel ISOLIT 20/20","EUR",null,0,0,null,"J"]
["ISOLIT25","ISOLIT25",null,"Anlage","Schiedel ISOLIT 25/25","EUR",null,0,0,null,"J"]
["ISOLIT30","ISOLIT30",null,"Anlage","Schiedel ISOLIT 30/30","EUR",null,0,0,null,"J"]
["ICS 80","ICS 80",null,"Anlage","Schiedel ICS 25mm 80","EUR",null,0,0,null,"J"]
["ICS 100","ICS 100",null,"Anlage","Schiedel ICS 25mm 100","EUR",null,0,0,null,"J"]
["ICS 130","ICS 130",null,"Anlage","Schiedel ICS 25mm 130","EUR",null,0,0,null,"J"]
["ICS 150","ICS 150",null,"Anlage","Schiedel ICS 25mm 150","EUR",null,0,0,null,"J"]
["ICS 180","ICS 180",null,"Anlage","Schiedel ICS 25mm 180","EUR",null,0,0,null,"J"]
["ICS 200","ICS 200",null,"Anlage","Schiedel ICS 25mm 200","EUR",null,0,0,null,"J"]
["ICS 250","ICS 250",null,"Anlage","Schiedel ICS 25mm 250","EUR",null,0,0,null,"J"]
["ICS 300","ICS 300",null,"Anlage","Schiedel ICS 25mm 300","EUR",null,0,0,null,"J"]
["ICS 350","ICS 350",null,"Anlage","Schiedel ICS 25mm 350","EUR",null,0,0,null,"J"]
["ICS 400","ICS 400",null,"Anlage","Schiedel ICS 25mm 400","EUR",null,0,0,null,"J"]
["ICS 450","ICS 450",null,"Anlage","Schiedel ICS 25mm 450","EUR",null,0,0,null,"J"]
["ICS 500","ICS 500",null,"Anlage","Schiedel ICS 25mm 500","EUR",null,0,0,null,"J"]
["ICS 550","ICS 550",null,"Anlage","Schiedel ICS 25mm 550","EUR",null,0,0,null,"J"]
["ICS 600","ICS 600",null,"Anlage","Schiedel ICS 25mm 600","EUR",null,0,0,null,"J"]
["ICS 650","ICS 650",null,"Anlage","Schiedel ICS 25mm 650","EUR",null,0,0,null,"J"]
["ICS 700","ICS 700",null,"Anlage","Schiedel ICS 25mm 700","EUR",null,0,0,null,"J"]
["ICS Matt 80","ICS Matt 80",null,"Anlage","Schiedel ICS MATT 25mm 80","EUR",null,0,0,null,"J"]
["ICS MATT 100","ICS MATT 100",null,"Anlage","Schiedel ICS MATT 25mm 100","EUR",null,0,0,null,"J"]
["ICS MATT 130","ICS MATT 130",null,"Anlage","Schiedel ICS MATT 25mm 130","EUR",null,0,0,null,"J"]
["ICS MATT 150","ICS MATT 150",null,"Anlage","Schiedel ICS MATT 25mm 150","EUR",null,0,0,null,"J"]
["ICS MATT 180","ICS MATT 180",null,"Anlage","Schiedel ICS MATT 25mm 180","EUR",null,0,0,null,"J"]
["ICS MATT 200","ICS MATT 200",null,"Anlage","Schiedel ICS MATT 25mm 200","EUR",null,0,0,null,"J"]
["ICS MATT 250","ICS MATT 250",null,"Anlage","Schiedel ICS MATT 25mm 250","EUR",null,0,0,null,"J"]
["ICS MATT 300","ICS MATT 300",null,"Anlage","Schiedel ICS MATT 25mm 300","EUR",null,0,0,null,"J"]
["ICS MATT 350","ICS MATT 350",null,"Anlage","Schiedel ICS MATT 25mm 350","EUR",null,0,0,null,"J"]
["ICS MATT 400","ICS MATT 400",null,"Anlage","Schiedel ICS MATT 25mm 400","EUR",null,0,0,null,"J"]
["ICS MATT 450","ICS MATT 450",null,"Anlage","Schiedel ICS MATT 25mm 450","EUR",null,0,0,null,"J"]
["ICS MATT 500","ICS MATT 500",null,"Anlage","Schiedel ICS MATT 25mm 500","EUR",null,0,0,null,"J"]
["ICS MATT 550","ICS MATT 550",null,"Anlage","Schiedel ICS MATT 25mm 550","EUR",null,0,0,null,"J"]
["ICS MATT 600","ICS MATT 600",null,"Anlage","Schiedel ICS MATT 25mm 600","EUR",null,0,0,null,"J"]
["ICS MATT 650","ICS MATT 650",null,"Anlage","Schiedel ICS MATT 25mm 650","EUR",null,0,0,null,"J"]
["ICS MATT 700","ICS MATT 700",null,"Anlage","Schiedel ICS MATT 25mm 700","EUR",null,0,0,null,"J"]
["ICS Kupfer 80","ICS Kupfer 80",null,"Anlage","Schiedel ICS Kupfer 80","EUR",null,0,0,null,"J"]
["ICS Kupfer 100","ICS Kupfer 100",null,"Anlage","Schiedel ICS Kupfer 100","EUR",null,0,0,null,"J"]
["ICS Kupfer 130","ICS Kupfer 130",null,"Anlage","Schiedel ICS Kupfer 130","EUR",null,0,0,null,"J"]
["ICS Kupfer 150","ICS Kupfer 150",null,"Anlage","Schiedel ICS Kupfer 150","EUR",null,0,0,null,"J"]
["ICS Kupfer 180","ICS Kupfer 180",null,"Anlage","Schiedel ICS Kupfer 180","EUR",null,0,0,null,"J"]
["ICS Kupfer 200","ICS Kupfer 200",null,"Anlage","Schiedel ICS Kupfer 200","EUR",null,0,0,null,"J"]
["ICS Kupfer 250","ICS Kupfer 250",null,"Anlage","Schiedel ICS Kupfer 250","EUR",null,0,0,null,"J"]
["ICS Kupfer 300","ICS Kupfer 300",null,"Anlage","Schiedel ICS Kupfer 300","EUR",null,0,0,null,"J"]
["ICS5000 80","ICS5000 80",null,"Anlage","Schiedel ICS5000 25mm 80","EUR",null,0,0,null,"J"]
["ICS5000 100","ICS5000 100",null,"Anlage","Schiedel ICS5000 25mm 100","EUR",null,0,0,null,"J"]
["ICS5000 130","ICS5000 130",null,"Anlage","Schiedel ICS5000 25mm 130","EUR",null,0,0,null,"J"]
["ICS5000 150","ICS5000 150",null,"Anlage","Schiedel ICS5000 25mm 150","EUR",null,0,0,null,"J"]
["ICS5000 180","ICS5000 180",null,"Anlage","Schiedel ICS5000 25mm 180","EUR",null,0,0,null,"J"]
["ICS5000 200","ICS5000 200",null,"Anlage","Schiedel ICS5000 25mm 200","EUR",null,0,0,null,"J"]
["ICS5000 250","ICS5000 250",null,"Anlage","Schiedel ICS5000 25mm 250","EUR",null,0,0,null,"J"]
["ICS5000 300","ICS5000 300",null,"Anlage","Schiedel ICS5000 25mm 300","EUR",null,0,0,null,"J"]
["ICS5000 350","ICS5000 350",null,"Anlage","Schiedel ICS5000 25mm 350","EUR",null,0,0,null,"J"]
["ICS5000 400","ICS5000 400",null,"Anlage","Schiedel ICS5000 25mm 400","EUR",null,0,0,null,"J"]
["ICS5000 450","ICS5000 450",null,"Anlage","Schiedel ICS5000 25mm 450","EUR",null,0,0,null,"J"]
["ICS5000 500","ICS5000 500",null,"Anlage","Schiedel ICS5000 25mm 500","EUR",null,0,0,null,"J"]
["ICS5000 600","ICS5000 600",null,"Anlage","Schiedel ICS5000 25mm 600","EUR",null,0,0,null,"J"]
["PRIMA PLUS 80","PRIMA PLUS 80",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 80","EUR",null,0,0,null,"J"]
["PRIMA PLUS 100","PRIMA PLUS 100",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 100","EUR",null,0,0,null,"J"]
["PRIMA PLUS 113","PRIMA PLUS 113",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 113","EUR",null,0,0,null,"J"]
["PRIMA PLUS 130","PRIMA PLUS 130",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 130","EUR",null,0,0,null,"J"]
["PRIMA PLUS 150","PRIMA PLUS 150",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 150","EUR",null,0,0,null,"J"]
["PRIMA PLUS 180","PRIMA PLUS 180",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 180","EUR",null,0,0,null,"J"]
["PRIMA PLUS 200","PRIMA PLUS 200",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 200","EUR",null,0,0,null,"J"]
["PRIMA PLUS 230","PRIMA PLUS 230",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 230","EUR",null,0,0,null,"J"]
["PRIMA PLUS 250","PRIMA PLUS 250",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 250","EUR",null,0,0,null,"J"]
["PRIMA PLUS 300","PRIMA PLUS 300",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 300","EUR",null,0,0,null,"J"]
["PRIMA PLUS 350","PRIMA PLUS 350",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 350","EUR",null,0,0,null,"J"]
["PRIMA PLUS 400","PRIMA PLUS 400",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 400","EUR",null,0,0,null,"J"]
["PRIMA PLUS 450","PRIMA PLUS 450",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 450","EUR",null,0,0,null,"J"]
["PRIMA PLUS 500","PRIMA PLUS 500",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 500","EUR",null,0,0,null,"J"]
["PRIMA PLUS 600","PRIMA PLUS 600",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 600","EUR",null,0,0,null,"J"]
["PRIMA PLUS 700","PRIMA PLUS 700",null,"Anlage","Schiedel Prima Plus 0,6mm Ø 700","EUR",null,0,0,null,"J"]
["VL-PPL 0,6 Ø 80","VL-PPL 0,6 Ø 80",null,"Anlage","Schiedel VL-Prima 0,6 mm Ø 80","EUR",null,0,0,null,"J"]
["VL-PPL 0,6 Ø 100","VL-PPL 0,6 Ø 100",null,"Anlage","Schiedel VL-Prima 0,6 mm Ø 100","EUR",null,0,0,null,"J"]
["VL-PPL 0,6 Ø 113","VL-PPL 0,6 Ø 113",null,"Anlage","Schiedel VL-Prima 0,6 mm Ø 113","EUR",null,0,0,null,"J"]
["VL-PPL 0,6 Ø 130","VL-PPL 0,6 Ø 130",null,"Anlage","Schiedel VL-Prima 0,6 mm Ø 130","EUR",null,0,0,null,"J"]
["VL-PPL 0,6 Ø 150","VL-PPL 0,6 Ø 150",null,"Anlage","Schiedel VL-Prima 0,6 mm Ø 150","EUR",null,0,0,null,"J"]
["VL-PPL 0,6 Ø 180","VL-PPL 0,6 Ø 180",null,"Anlage","Schiedel VL-Prima 0,6 mm Ø 180","EUR",null,0,0,null,"J"]
["VL-PPL 0,6 Ø 200","VL-PPL 0,6 Ø 200",null,"Anlage","Schiedel VL-Prima 0,6 mm Ø 200","EUR",null,0,0,null,"J"]
["VL-PPL 0,6 Ø 230","VL-PPL 0,6 Ø 230",null,"Anlage","Schiedel VL-Prima 0,6 mm Ø 230","EUR",null,0,0,null,"J"]
["VL-PPL 0,6 Ø 250","VL-PPL 0,6 Ø 250",null,"Anlage","Schiedel VL-Prima 0,6 mm Ø 250","EUR",null,0,0,null,"J"]
["VL-PPL 0,6 Ø 300","VL-PPL 0,6 Ø 300",null,"Anlage","Schiedel VL-Prima 0,6 mm Ø 300","EUR",null,0,0,null,"J"]
["VL-PPL 1,0 Ø 350","VL-PPL 1,0 Ø 350",null,"Anlage","Schiedel VL-Prima 1,0 mm Ø 350","EUR",null,0,0,null,"J"]
["VL-PPL 1,0 Ø 400","VL-PPL 1,0 Ø 400",null,"Anlage","Schiedel VL-Prima 1,0 mm Ø 400","EUR",null,0,0,null,"J"]
["VL-PPL 1,0 Ø 450","VL-PPL 1,0 Ø 450",null,"Anlage","Schiedel VL-Prima 1,0 mm Ø 450","EUR",null,0,0,null,"J"]
["VL-PPL 1,0 Ø 500","VL-PPL 1,0 Ø 500",null,"Anlage","Schiedel VL-Prima 1,0 mm Ø 500","EUR",null,0,0,null,"J"]
["VL-PPL 1,0 Ø 550","VL-PPL 1,0 Ø 550",null,"Anlage","Schiedel VL-Prima 1,0 mm Ø 550","EUR",null,0,0,null,"J"]
["VL-PPL 1,0 Ø 600","VL-PPL 1,0 Ø 600",null,"Anlage","Schiedel VL-Prima 1,0 mm Ø 600","EUR",null,0,0,null,"J"]
["VL-PPL 1,0 Ø 700","VL-PPL 1,0 Ø 700",null,"Anlage","Schiedel VL-Prima 1,0 mm Ø 700","EUR",null,0,0,null,"J"]
["VL-Technostar12080","VL-Technostar12080",null,"Anlage","Schiedel VL-Technostar120 Ø80","EUR",null,0,0,null,"J"]
["VL-Technostar120110","VL-Technostar120110",null,"Anlage","Schiedel VL-Technostar120 Ø110","EUR",null,0,0,null,"J"]
["VL-Technostar120125","VL-Technostar120125",null,"Anlage","Schiedel VL-Technostar120 Ø125","EUR",null,0,0,null,"J"]
["VL-Technostar120160","VL-Technostar120160",null,"Anlage","Schiedel VL-Technostar120 Ø160","EUR",null,0,0,null,"J"]
["VL-TechnostarLAS80","VL-TechnostarLAS80",null,"Anlage","Schiedel VL-Technostar LAS Ø80","EUR",null,0,0,null,"J"]
["VL-TechnostarLAS110","VL-TechnostarLAS110",null,"Anlage","Schiedel VL-Technostar LAS Ø110","EUR",null,0,0,null,"J"]
["VL-TechnostarLAS125","VL-TechnostarLAS125",null,"Anlage","Schiedel VL-Technostar LAS Ø125","EUR",null,0,0,null,"J"]
["VL-TechnostarLAS160","VL-TechnostarLAS160",null,"Anlage","Schiedel VL-Technostar LAS Ø160","EUR",null,0,0,null,"J"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"INDEX(L192:L193,L190,1)","v":2023}]
[null,null,null,null,null,null,null,null,null,null,null,"Preisbasis"]
[null,null,null,null,null,null,null,null,null,null,null,2023]
[null,null,null,null,null,null,null,null,null,null,null,2022]
[]
[]
[]
[]
[]
[]
[null,null,null,null,{"$f":"Eingabe!$J$1","v":1}]
[null,null,null,null,null,null,"Rundungskurs von Euro auf Franken 1,55"]
[]
["Artikel-Nr","Artikel-Nr","EAN","Mengeneinheit","Artikelbezeichnung 1","Währung","aktueller Preis","Rab.Bez","Gewicht","Einbaulänge","Rabattfähig","Bez. Französisch","Bez. Deutsch","Bez. Italienisch","Rab-GR","Rabatt-KZ","System","Preis?","Preis 2022","Alte Artikelnummer AS400","SAP-Nummer von Schiedel","EAN-Nr.","Preis 2023","Art.Nr. Text","abw","Preis21","ABW","im sorti","neupreis 2023","abw"]
[{"$f":"B204&\"\"","v":"100000"},100000,null,"STK",{"$f":"IF($E$200=2,L204,IF($E$200=3,N204,M204))","v":"TS120 60 Rohr mit Muffe L250mm "},"CHF",{"$f":"IF($L$190=1,W204,S204)","v":17.2},"TECHNOSTAR 120",0.2,250,"J","TS120 60 Tube avec manchon L250mm","TS120 60 Rohr mit Muffe L250mm ","TS120 60 Tubo con manicotto L250mm",121,1,"DN 60",null,15.6,"516025",null,null,17.2,"100000",1.5999999999999996,14.5,2.6999999999999993,"100000",17.2,1.5999999999999996]
["100001",100001,null,"STK","TS120 60 Rohr mit Muffe L500mm ","CHF",17.5,"TECHNOSTAR 120",0.4,500,"J","TS120 60 Tube avec manchon L500mm","TS120 60 Rohr mit Muffe L500mm ","TS120 60 Tubo con manicotto L500mm",121,1,"DN 60",null,15.9,"516050",null,null,17.5,"100001",1.5999999999999996,14.8,2.6999999999999993,"100001",17.5,1.5999999999999996]
["100002",100002,null,"STK","TS120 60 Rohr mit Muffe L1000mm ","CHF",23.6,"TECHNOSTAR 120",0.5,1000,"J","TS120 60 Tube avec manchon L1000mm","TS120 60 Rohr mit Muffe L1000mm ","TS120 60 Tubo con manicotto L1000mm",121,1,"DN 60",null,21.4,"516100",null,null,23.6,"100002",2.2000000000000028,20.3,3.3000000000000007,"100002",23.6,2.2000000000000028]
["100004",100004,null,"STK","TS120 80 Rohr mit Muffe L250mm ","CHF",18.3,"TECHNOSTAR 120",0.4,250,"J","TS120 80 Tube avec manchon L250mm","TS120 80 Rohr mit Muffe L250mm ","TS120 80 Tubo con manicotto L250mm",121,1,"DN 80",null,16.600000000000001,"505051",null,null,18.3,"100004",1.6999999999999993,15.5,2.8000000000000007,"100004",18.3,1.6999999999999993]
["100005",100005,null,"STK","TS120 80 Rohr mit Muffe L500mm ","CHF",20.100000000000001,"TECHNOSTAR 120",0.5,500,"J","TS120 80 Tube avec manchon L500mm","TS120 80 Rohr mit Muffe L500mm ","TS120 80 Tubo con manicotto L500mm",121,1,"DN 80",null,18.2,"505052",null,null,20.100000000000001,"100005",1.9000000000000021,17.100000000000001,3,"100005",20.100000000000001,1.9000000000000021]
["100006",100006,null,"STK","TS120 80 Rohr mit Muffe L1000mm ","CHF",26.9,"TECHNOSTAR 120",0.7,1000,"J","TS120 80 Tube avec manchon L1000mm","TS120 80 Rohr mit Muffe L1000mm ","TS120 80 Tubo con manicotto L1000mm",121,1,"DN 80",null,24.4,"505053",null,null,26.9,"100006",2.5,23.3,3.5999999999999979,"100006",26.9,2.5]
["100007",100007,null,"STK","TS120 80 Rohr mit Muffe L2000mm ","CHF",49.9,"TECHNOSTAR 120",0.9,2000,"J","TS120 80 Tube avec manchon L2000mm","TS120 80 Rohr mit Muffe L2000mm ","TS120 80 Tubo con manicotto L2000mm",121,1,"DN 80",null,45.3,"505054",null,null,49.9,"100007",4.6000000000000014,44.2,5.6999999999999957,"100007",49.9,4.6000000000000014]
["100010",100010,null,"STK","TS120 110 Rohr mit Muffe L250mm","CHF",20.399999999999999,"TECHNOSTAR 120",0.3,250,"J","TS120 110 Tube avec manchon L250mm","TS120 110 Rohr mit Muffe L250mm","TS120 110 Tubo con manicotto L250mm",121,1,"DN110",null,18.5,"505009",null,null,20.399999999999999,"100010",1.8999999999999986,17.399999999999999,3,"100010",20.399999999999999,1.8999999999999986]
["100011",100011,null,"STK","TS120 110 Rohr mit Muffe L500mm ","CHF",30.1,"TECHNOSTAR 120",0.5,500,"J","TS120 110 Tube avec manchon L500mm","TS120 110 Rohr mit Muffe L500mm ","TS120 110 Tubo con manicotto L500mm",121,1,"DN110",null,27.3,"505010",null,null,30.1,"100011",2.8000000000000007,26.2,3.9000000000000021,"100011",30.1,2.8000000000000007]
["100012",100012,null,"STK","TS120 110 Rohr mit Muffe L1000mm ","CHF",49.3,"TECHNOSTAR 120",1,1000,"J","TS120 110 Tube avec manchon L1000mm","TS120 110 Rohr mit Muffe L1000mm ","TS120 110 Tubo con manicotto L1000mm",121,1,"DN110",null,44.8,"505012",null,null,49.3,"100012",4.5,43.7,5.5999999999999943,"100012",49.3,4.5]
["100013",100013,null,"STK","TS120 110 Rohr mit Muffe L2000mm ","CHF",82,"TECHNOSTAR 120",1.9,2000,"J","TS120 110 Tube avec manchon L2000mm","TS120 110 Rohr mit Muffe L2000mm ","TS120 110 Tubo con manicotto L2000mm",121,1,"DN110",null,74.5,"505014",null,null,82,"100013",7.5,73.400000000000006,8.5999999999999943,"100013",82,7.5]
["100014",100014,null,"STK","TS120 125 Rohr mit Muffe L250mm","CHF",27.1,"TECHNOSTAR 120",0.4,250,"J","TS120 125 Tube avec manchon L250mm","TS120 125 Rohr mit Muffe L250mm","TS120 125 Tubo con manicotto L250mm",121,1,"DN 125",null,24.6,"505017",null,null,27.1,"100014",2.5,23.5,3.6000000000000014,"100014",27.1,2.5]
["100015",100015,null,"STK","TS120 125 Rohr mit Muffe L500mm ","CHF",39.5,"TECHNOSTAR 120",0.7,500,"J","TS120 125 Tube avec manchon L500mm","TS120 125 Rohr mit Muffe L500mm ","TS120 125 Tubo con manicotto L500mm",121,1,"DN 125",null,35.9,"505018",null,null,39.5,"100015",3.6000000000000014,34.799999999999997,4.7000000000000028,"100015",39.5,3.6000000000000014]
["100016",100016,null,"STK","TS120 125 Rohr mit Muffe L1000mm ","CHF",64.3,"TECHNOSTAR 120",1.3,1000,"J","TS120 125 Tube avec manchon L1000mm","TS120 125 Rohr mit Muffe L1000mm ","TS120 125 Tubo con manicotto L1000mm",121,1,"DN 125",null,58.4,"505020",null,null,64.3,"100016",5.8999999999999986,57.3,7,"100016",64.3,5.8999999999999986]
["100017",100017,null,"STK","TS120 125 Rohr mit Muffe L2000mm ","CHF",98.2,"TECHNOSTAR 120",2.4500000000000002,2000,"J","TS120 125 Tube avec manchon L2000mm","TS120 125 Rohr mit Muffe L2000mm ","TS120 125 Tubo con manicotto L2000mm",121,1,"DN 125",null,89.2,"505022",null,null,98.2,"100017",9,88.1,10.100000000000009,"100017",98.2,9]
["100018",100018,null,"STK","TS120 160 Rohr mit Muffe L250mm","CHF",41.2,"TECHNOSTAR 120",0.7,250,"J","TS120 160 Tube avec manchon L250mm","TS120 160 Rohr mit Muffe L250mm","TS120 160 Tubo con manicotto L250mm",121,1,"DN 160",null,37.4,"505025",null,null,41.2,"100018",3.8000000000000043,36.299999999999997,4.9000000000000057,"100018",41.2,3.8000000000000043]
["100019",100019,null,"STK","TS120 160 Rohr mit Muffe L500mm ","CHF",60.9,"TECHNOSTAR 120",1.1499999999999999,500,"J","TS120 160 Tube avec manchon L500mm","TS120 160 Rohr mit Muffe L500mm ","TS120 160 Tubo con manicotto L500mm",121,1,"DN 160",null,55.3,"505026",null,null,60.9,"100019",5.6000000000000014,54.2,6.6999999999999957,"100019",60.9,5.6000000000000014]
["100020",100020,null,"STK","TS120 160 Rohr mit Muffe L1000mm ","CHF",100.4,"TECHNOSTAR 120",2.1,1000,"J","TS120 160 Tube avec manchon L1000mm","TS120 160 Rohr mit Muffe L1000mm ","TS120 160 Tubo con manicotto L1000mm",121,1,"DN 160",null,91.2,"505028",null,null,100.4,"100020",9.2000000000000028,90.1,10.300000000000011,"100020",100.4,9.2000000000000028]
["100021",100021,null,"STK","TS120 160 Rohr mit Muffe L2000mm ","CHF",155.9,"TECHNOSTAR 120",4,2000,"J","TS120 160 Tube avec manchon L2000mm","TS120 160 Rohr mit Muffe L2000mm ","TS120 160 Tubo con manicotto L2000mm",121,1,"DN 160",null,141.69999999999999,"505030",null,null,155.9,"100021",14.200000000000017,140.6,15.300000000000011,"100021",155.9,14.200000000000017]
["100023",100023,null,"STK","TS120 200 Rohr mit Muffe L500mm ","CHF",149.6,"TECHNOSTAR 120",1.5,500,"J","TS120 200 Tube avec manchon L500mm","TS120 200 Rohr mit Muffe L500mm ","TS120 200 Tubo con manicotto L500mm",121,1,"DN 200",null,136,"505032",null,null,149.6,"100023",13.599999999999994,134.9,14.699999999999989,"100023",149.6,13.599999999999994]
["100024",100024,null,"STK","TS120 200 Rohr mit Muffe L1000mm ","CHF",203.9,"TECHNOSTAR 120",3.2,1000,"J","TS120 200 Tube avec manchon L1000mm","TS120 200 Rohr mit Muffe L1000mm ","TS120 200 Tubo con manicotto L1000mm",121,1,"DN 200",null,185.3,"505033",null,null,203.9,"100024",18.599999999999994,184.2,19.700000000000017,"100024",203.9,18.599999999999994]
["100025",100025,null,"STK","TS120 200 Rohr mit Muffe L2000mm ","CHF",303.89999999999998,"TECHNOSTAR 120",5.6,2000,"J","TS120 200 Tube avec manchon L2000mm","TS120 200 Rohr mit Muffe L2000mm ","TS120 200 Tubo con manicotto L2000mm",121,1,"DN 200",null,276.2,"505035",null,null,303.89999999999998,"100025",27.699999999999989,275.10000000000002,28.799999999999955,"100025",303.89999999999998,27.699999999999989]
["100026",100026,null,"STK","TS120 250 Rohr mit Muffe L500mm ","CHF",184.8,"TECHNOSTAR 120",1.8,500,"J","TS120 250 Tube avec manchon L500mm","TS120 250 Rohr mit Muffe L500mm ","TS120 250 Tubo con manicotto L500mm",121,1,"DN 250",null,168,"505040",null,null,184.8,"100026",16.800000000000011,166.9,17.900000000000006,"100026",184.8,16.800000000000011]
["100027",100027,null,"STK","TS120 250 Rohr mit Muffe L1000mm ","CHF",255.8,"TECHNOSTAR 120",3.6,1000,"J","TS120 250 Tube avec manchon L1000mm","TS120 250 Rohr mit Muffe L1000mm ","TS120 250 Tubo con manicotto L1000mm",121,1,"DN 250",null,232.5,"505041",null,null,255.8,"100027",23.300000000000011,231.4,24.400000000000006,"100027",255.8,23.300000000000011]
["100028",100028,null,"STK","TS120 250 Rohr mit Muffe L2000mm ","CHF",394,"TECHNOSTAR 120",6.2,2000,"J","TS120 250 Tube avec manchon L 2500mm","TS120 250 Rohr mit Muffe L2000mm ","TS120 250 Tubo con manicotto L 2500mm",121,1,"DN 200",null,358.1,"505043",null,null,394,"100028",35.899999999999977,357,37,"100028",394,35.899999999999977]
["100032",100032,null,"STK","TS120 60 Flex 50/58 Rolle L12500mm","CHF",391.3,"TECHNOSTAR 120",5.7,12500,"J","TS120 50 Tube flexible 50/58 rouleau L12500mm","TS120 60 Flex 50/58 Rolle L12500mm","TS120 50 Tubo flessibile 50/58 ruolo L12500mm",121,1,"DN 60",null,355.7,"516212",null,null,391.3,"100032",35.600000000000023,354.6,36.699999999999989,"100032",391.3,35.600000000000023]
["100033",100033,null,"STK","TS120 60 Flex 50/58 Rolle L25000mm","CHF",786.7,"TECHNOSTAR 120",11.2,25000,"J","TS120 50 Tube flexible 50/58 rouleau L 25000mm","TS120 60 Flex 50/58 Rolle L25000mm","TS120 50 Tubo flessibile 50/58 ruolo L 25000mm",121,1,"DN 250",null,715.1,"516225",null,null,786.7,"100033",71.600000000000023,714,72.700000000000045,"100033",786.7,71.600000000000023]
["100034",100034,null,"STK","TS120 80 Flex 75/83 Rolle L12500mm","CHF",602.6,"TECHNOSTAR 120",5.7,12500,"J","TS120 80 Tube flexible 75/83 rouleau L12500mm","TS120 80 Flex 75/83 Rolle L12500mm","TS120 80 Tubo flessibile 75/83 ruolo L12500mm",121,1,"DN 80",null,547.79999999999995,"505049",null,null,602.6,"100034",54.800000000000068,546.70000000000005,55.899999999999977,"100034",602.6,54.800000000000068]
["100035",100035,null,"STK","TS120 80 Flex 75/83 Rolle L25000mm","CHF",1170.5999999999999,"TECHNOSTAR 120",23,25000,"J","TS120 80 Tube flexible 75/83 rouleau L 25000mm","TS120 80 Flex 75/83 Rolle L25000mm","TS120 80 Tubo flessibile 75/83 ruolo L 25000mm",121,1,"DN 80",null,1064.0999999999999,"505050",null,null,1170.5999999999999,"100035",106.5,1063,107.59999999999991,"100035",1170.5999999999999,106.5]
["100036",100036,null,"STK","TS120 80 Flex 75/83 Rolle L50000mm","CHF",1789.2,"TECHNOSTAR 120",23,50000,"J","TS120 80 Tube flexible 75/83 rouleau L 50000mm","TS120 80 Flex 75/83 Rolle L50000mm","TS120 80 Tubo flessibile 75/83 ruolo L 50000mm",121,1,"DN 80",null,1626.5,"505150",null,null,1789.2,"100036",162.70000000000005,1625.4,163.79999999999995,"100036",1789.2,162.70000000000005]
["100037",100037,null,"STK","TS120 110 Flex 105/113 Rolle L15000mm","CHF",940.5,"TECHNOSTAR 120",9,15000,"J","TS120 110 Tube flexible 105/113 rouleau L 15000mm","TS120 110 Flex 105/113 Rolle L15000mm","TS120 110 Tubo flessibile 105/113 ruolo L 15000mm",121,1,"DN110",null,855,"510007",null,null,940.5,"100037",85.5,853.9,86.600000000000023,"100037",940.5,85.5]
["100038",100038,null,"STK","TS120 110 Flex 105/113 Rolle L25000mm","CHF",1566.6,"TECHNOSTAR 120",15,25000,"J","TS120 110 Tube flexible 105/113 rouleau L 25000mm","TS120 110 Flex 105/113 Rolle L25000mm","TS120 110 Tubo flessibile 105/113 ruolo L 25000mm",121,1,"DN110",null,1424.1,"510016",null,null,1566.6,"100038",142.5,1423,143.59999999999991,"100038",1566.6,142.5]
["100039",100039,null,"STK","TS120 160 Flexrohr verschraubbar L1000mm","CHF",194.5,"TECHNOSTAR 120",2,1000,"J","TS120 160 Tube flexible 155/163  L1000mm vissés","TS120 160 Flexrohr verschraubbar L1000mm","TS120 160 Tubo flessibile 155/163 L1000mm avvitato",121,1,"DN 160",null,176.8,"516116",null,null,194.5,"100039",17.699999999999989,175.7,18.800000000000011,"100039",194.5,17.699999999999989]
["100040",100040,null,"STK","TS120 60 Verbindungskupplung zu Flex mit Muffe","CHF",83.4,"TECHNOSTAR 120",0.2,0,"J","TS120 60 Le cadre avec manchon pour flexible","TS120 60 Verbindungskupplung zu Flex mit Muffe","TS120 60 Giunto con manicotto per flessibile ",121,1,"DN 60",null,75.8,"516007",null,null,83.4,"100040",7.6000000000000085,74.7,8.7000000000000028,"100040",83.4,7.6000000000000085]
["100041",100041,null,"STK","TS120 80 Verbindungskupplung zu Flex mit Muffe","CHF",112.5,"TECHNOSTAR 120",0.2,0,"J","TS120 80 Le cadre avec manchon pour flexible","TS120 80 Verbindungskupplung zu Flex mit Muffe","TS120 80 Giunto con manicotto per flessibile ",121,1,"DN 80",null,102.2,"511060",null,null,112.5,"100041",10.299999999999997,101.1,11.400000000000006,"100041",112.5,10.299999999999997]
["100042",100042,null,"STK","TS120 110 Verbindungskupplung zu Flex mit Muffe","CHF",205.2,"TECHNOSTAR 120",0.5,0,"J","TS120 110 Le cadre avec manchon pour flexible","TS120 110 Verbindungskupplung zu Flex mit Muffe","TS120 110 Giunto con manicotto per flessibile ",121,1,"DN110",null,186.5,"510014",null,null,205.2,"100042",18.699999999999989,185.4,19.799999999999983,"100042",205.2,18.699999999999989]
["100043",100043,null,"STK","TS120 60 Verbindungskupplung zu Flex Steckteil","CHF",83.4,"TECHNOSTAR 120",0.2,0,"J","TS120 60 Le cadre avec d'insertion pour flexible","TS120 60 Verbindungskupplung zu Flex Steckteil","TS120 60 Giunto male per flessibile ",121,1,"DN 60",null,75.8,"516008",null,null,83.4,"100043",7.6000000000000085,74.7,8.7000000000000028,"100043",83.4,7.6000000000000085]
["100044",100044,null,"STK","TS120 80 Verbindungskupplung zu Flex Steckteil","CHF",112.5,"TECHNOSTAR 120",0.2,0,"J","TS120 60 Le cadre avec d'insertion pour flexible","TS120 80 Verbindungskupplung zu Flex Steckteil","TS120 80 Giunto male per flessibile ",121,1,"DN 80",null,102.2,"511061",null,null,112.5,"100044",10.299999999999997,101.1,11.400000000000006,"100044",112.5,10.299999999999997]
["100045",100045,null,"STK","TS120 110 Verbindungskupplung zu Flex Steckteil","CHF",205.2,"TECHNOSTAR 120",0.5,0,"J","TS120 60 Le cadre avec d'insertion pour flexible","TS120 110 Verbindungskupplung zu Flex Steckteil","TS120 110 Giunto male per flessibile ",121,1,"DN110",null,186.5,"510017",null,null,205.2,"100045",18.699999999999989,185.4,19.799999999999983,"100045",205.2,18.699999999999989]
["100046",100046,null,"STK","TS120 60 Schraubkupplung Flex/Flex","CHF",87.6,"TECHNOSTAR 120",0.15,0,"J","TS120 60 Enbrajage flexible/flexible","TS120 60 Schraubkupplung Flex/Flex","TS120 60 Vite flessible/flessibile",121,1,"DN 60",null,79.599999999999994,"516009",null,null,87.6,"100046",8,78.5,9.0999999999999943,"100046",87.6,8]
["100047",100047,null,"STK","TS120 80 Schraubkupplung Flex/Flex","CHF",113.5,"TECHNOSTAR 120",0.15,0,"J","TS120 80 Enbrajage flexible/fflexible","TS120 80 Schraubkupplung Flex/Flex","TS120 80 Vite flessible/fflessibile",121,1,"DN 80",null,103.1,"500091",null,null,113.5,"100047",10.400000000000006,102,11.5,"100047",113.5,10.400000000000006]
["100048",100048,null,"STK","TS120 110 Schraubkupplung Flex/Flex","CHF",227.9,"TECHNOSTAR 120",0.4,0,"J","TS120 110 Enbrajage flexible/flexible","TS120 110 Schraubkupplung Flex/Flex","TS120 110 Vite flessible/flessibile",121,1,"DN110",null,207.1,"510013",null,null,227.9,"100048",20.800000000000011,206,21.900000000000006,"100048",227.9,20.800000000000011]
["100049",100049,null,"STK","TS120 80 Revisionsrohr für Flex","CHF",162,"TECHNOSTAR 120",0.4,259,"J","TS120 80 Tube de révision pour flexible","TS120 80 Revisionsrohr für Flex","TS120 80 Tubo de revisione per flessibile",121,1,"DN 80",null,147.19999999999999,"511062",null,null,162,"100049",14.800000000000011,146.1,15.900000000000006,"100049",162,14.800000000000011]
["100050",100050,null,"STK","TS120 110 Revisionsrohr für Flex","CHF",307.2,"TECHNOSTAR 120",0.6,269,"J","TS120 110 Tube de révision pour flexible","TS120 110 Revisionsrohr für Flex","TS120 110 Tubo de revisione per flessibile",121,1,"DN110",null,279.2,"511012",null,null,307.2,"100050",28,278.10000000000002,29.099999999999966,"100050",307.2,28]
["100051",100051,null,"STK","TS120 160  Revisionsrohr für Flex kurz","CHF",392.2,"TECHNOSTAR 120",0.25,700,"J","TS120 160 Tube de révision pour flexible court","TS120 160  Revisionsrohr für Flex kurz","TS120 160 Tubo de revisione per flessibile breve",121,1,"DN 160",null,356.5,"516118",null,null,392.2,"100051",35.699999999999989,355.4,36.800000000000011,"100051",392.2,35.699999999999989]
["100052",100052,null,"STK","TS120 160 Revisionsrohr 1000mm für Flex","CHF",443.1,"TECHNOSTAR 120",2.5,0,"J","TS120 60 Tube de révision pour flexible L1000mm","TS120 160 Revisionsrohr 1000mm für Flex","TS120 60 Tubo de revisione per flessibile L1000mm",121,1,"DN 160",null,402.8,"516117",null,null,443.1,"100052",40.300000000000011,401.7,41.400000000000034,"100052",443.1,40.300000000000011]
["100053",100053,null,"STK","TS120 160 Aufhängeschelle zu Flex ","CHF",35.200000000000003,"TECHNOSTAR 120",0.15,0,"J","TS120 160 Suspension pour flexible","TS120 160 Aufhängeschelle zu Flex ","TS120 160 Suspensione per flessibile",121,1,"DN 160",null,32,"516119",null,null,35.200000000000003,"100053",3.2000000000000028,30.9,4.3000000000000043,"100053",35.200000000000003,3.2000000000000028]
["100054",100054,null,"STK","TS120 110 Einzugshilfe mit Seil 20Meter","CHF",244.9,"TECHNOSTAR 120",1.8,165,"J","TS120 110 Embout de montage flexible 20M de corde","TS120 110 Einzugshilfe mit Seil 20Meter","TS120 110 Elemento di mont. flessibile  corda 20m",121,1,"DN110",null,222.6,"510015",null,null,244.9,"100054",22.300000000000011,221.5,23.400000000000006,"100054",244.9,22.300000000000011]
["100055",100055,null,"STK","TS120 80 Einzugshilfe mit Seil 20Meter","CHF",184.8,"TECHNOSTAR 120",3,147,"J","TS120 80 Embout de montage flexible 20M de corde","TS120 80 Einzugshilfe mit Seil 20Meter","TS120 80 Elemento di mont. flessibile  corda 20m",121,1,"DN 80",null,168,"511002",null,null,184.8,"100055",16.800000000000011,166.9,17.900000000000006,"100055",184.8,16.800000000000011]
["100058",100058,null,"STK","TS120 60 Revisionsrohr mit Schraubdeckel","CHF",47.8,"TECHNOSTAR 120",0.1,160,"J","TS120 60 Tube de nettoyage ","TS120 60 Revisionsrohr mit Schraubdeckel","TS120 60 Tubo con revisione ",121,1,"DN 60",null,43.4,"516220",null,null,47.8,"100058",4.3999999999999986,42.3,5.5,"100058",47.8,4.3999999999999986]
["100059",100059,null,"STK","TS120 80 Revisionsrohr mit Schraubdeckel","CHF",67.3,"TECHNOSTAR 120",0.4,225,"J","TS120 80 Tube de nettoyage ","TS120 80 Revisionsrohr mit Schraubdeckel","TS120 80 Tubo con revisione ",121,1,"DN 80",null,61.1,"511063",null,null,67.3,"100059",6.1999999999999957,60,7.2999999999999972,"100059",67.3,6.1999999999999957]
["100060",100060,null,"STK","TS120 80  Revisionsrohr  flach  Typ 3","CHF",67.3,"TECHNOSTAR 120",0.2,225,"J","TS120 80 Tube de nettoyage plat type3","TS120 80  Revisionsrohr  flach  Typ 3","TS120 80 Tubo con revisione piatta typ3",121,1,"DN 80",null,61.1,"511065",null,null,67.3,"100060",6.1999999999999957,60,7.2999999999999972,"100060",67.3,6.1999999999999957]
["100061",100061,null,"STK","TS120 110 Revisionsrohr mit Schraubdeckel","CHF",38.299999999999997,"TECHNOSTAR 120",0.3,185,"J","TS120 110 Tube de nettoyage ","TS120 110 Revisionsrohr mit Schraubdeckel","TS120 110 Tubo con revisione ",121,1,"DN110",null,34.799999999999997,"500093",null,null,38.299999999999997,"100061",3.5,33.700000000000003,4.5999999999999943,"100061",38.299999999999997,3.5]
["100062",100062,null,"STK","TS120 125 Revisionsrohr mit Schraubdeckel","CHF",64.8,"TECHNOSTAR 120",0.45,214,"J","TS120 125 Tube de nettoyage ","TS120 125 Revisionsrohr mit Schraubdeckel","TS120 125 Tubo con revisione ",121,1,"DN 125",null,58.9,"500094",null,null,64.8,"100062",5.8999999999999986,57.8,7,"100062",64.8,5.8999999999999986]
["100063",100063,null,"STK","TS120 160 Revisionsrohr mit Schraubdeckel","CHF",130.80000000000001,"TECHNOSTAR 120",0.8,280,"J","TS120 160 Tube de nettoyage ","TS120 160 Revisionsrohr mit Schraubdeckel","TS120 160 Tubo con revisione ",121,1,"DN 160",null,118.9,"500095",null,null,130.80000000000001,"100063",11.900000000000006,117.8,13.000000000000014,"100063",130.80000000000001,11.900000000000006]
["100064",100064,null,"STK","TS120 200 Revisionsrohr mit Schraubdeckel","CHF",284.5,"TECHNOSTAR 120",0.15,340,"J","TS120 200 Tube de nettoyage ","TS120 200 Revisionsrohr mit Schraubdeckel","TS120 200 Tubo con revisione ",121,1,"DN 200",null,258.60000000000002,"500096",null,null,284.5,"100064",25.899999999999977,257.5,27,"100064",284.5,25.899999999999977]
["100065",100065,null,"STK","TS120 250 Revisionsrohr mit Schraubdeckel","CHF",318.5,"TECHNOSTAR 120",1.01,340,"J","TS120 250 Tube de nettoyage ","TS120 250 Revisionsrohr mit Schraubdeckel","TS120 250 Tubo con revisione ",121,1,"DN 250",null,289.5,"500097",null,null,318.5,"100065",29,288.39999999999998,30.100000000000023,"100065",318.5,29]
["100067",100067,null,"STK","TS120 80 Revisionsrohr Eckform ","CHF",67.3,"TECHNOSTAR 120",0.4,0,"J","TS120 80 Tube de nettoyage coin","TS120 80 Revisionsrohr Eckform ","TS120 80 Tubo revisione angolo",121,1,"DN 80",null,61.1,"511064",null,null,67.3,"100067",6.1999999999999957,60,7.2999999999999972,"100067",67.3,6.1999999999999957]
["100074",100074,null,"STK","TS120 80 T-Stück 90°","CHF",67.3,"TECHNOSTAR 120",0.2,225,"J","TS120 80 Té 90°","TS120 80 T-Stück 90°","TS120 80 Pezzo T 90°",121,1,"DN 80",null,61.1,"500140",null,null,67.3,"100074",6.1999999999999957,60,7.2999999999999972,"100074",67.3,6.1999999999999957]
["100075",100075,null,"STK","TS120 110 T-Stück 90°","CHF",139.6,"TECHNOSTAR 120",0.4,250,"J","TS120 110 Té 90°","TS120 110 T-Stück 90°","TS120 110 Pezzo T 90°",121,1,"DN110",null,126.9,"500099",null,null,139.6,"100075",12.699999999999989,125.8,13.799999999999997,"100075",139.6,12.699999999999989]
["100076",100076,null,"STK","TS120 125 T-Stück 90°","CHF",179.9,"TECHNOSTAR 120",0.55000000000000004,250,"J","TS120 125 Té 90°","TS120 125 T-Stück 90°","TS120 125 Pezzo T 90°",121,1,"DN 125",null,163.5,"500100",null,null,179.9,"100076",16.400000000000006,162.4,17.5,"100076",179.9,16.400000000000006]
["100077",100077,null,"STK","TS120 160 T-Stück 90°","CHF",256.10000000000002,"TECHNOSTAR 120",1,280,"J","TS120 160 Té 90°","TS120 160 T-Stück 90°","TS120 160 Pezzo T 90°",121,1,"DN 160",null,232.8,"500101",null,null,256.10000000000002,"100077",23.300000000000011,231.7,24.400000000000034,"100077",256.10000000000002,23.300000000000011]
["100078",100078,null,"STK","TS120 200 T-Stück 90°","CHF",284.5,"TECHNOSTAR 120",1.5,350,"J","TS120 200 Té 90°","TS120 200 T-Stück 90°","TS120 200 Pezzo T 90°",121,1,"DN 200",null,258.60000000000002,"500102",null,null,284.5,"100078",25.899999999999977,257.5,27,"100078",284.5,25.899999999999977]
["100079",100079,null,"STK","TS120 250 T-Stück 90°","CHF",318.5,"TECHNOSTAR 120",1.8,400,"J","TS120 250 Té 90°","TS120 250 T-Stück 90°","TS120 250 Pezzo T 90°",121,1,"DN 250",null,289.5,"500103",null,null,318.5,"100079",29,288.39999999999998,30.100000000000023,"100079",318.5,29]
[{"$f":"B268&\"\"","v":"100080"},100080,null,"STK",{"$f":"IF($E$200=2,L268,IF($E$200=3,N268,M268))","v":"TS120 80  Abzweiger 45°"},"CHF",{"$f":"IF($L$190=1,W268,S268)","v":131.9},"TECHNOSTAR 120",0.25,250,"J","TS120 80 Té 45°","TS120 80  Abzweiger 45°","TS120 80 Pezzo T 45°",121,1,"DN 80",null,119.9,"500150",null,null,131.9,"100080",12,118.8,13.100000000000009,"100080",131.9,12]
["100081",100081,null,"STK","TS120 110 Abzweiger 45°","CHF",164.7,"TECHNOSTAR 120",0.5,300,"J","TS120 110 Té 45°","TS120 110 Abzweiger 45°","TS120 110 Pezzo T 45°",121,1,"DN110",null,149.69999999999999,"500003",null,null,164.7,"100081",15,148.6,16.099999999999994,"100081",164.7,15]
["100082",100082,null,"STK","TS120 125 Abzweiger 45°","CHF",191.9,"TECHNOSTAR 120",0.75,350,"J","TS120 125 Té 45°","TS120 125 Abzweiger 45°","TS120 125 Pezzo T 45°",121,1,"DN 125",null,174.4,"500004",null,null,191.9,"100082",17.5,173.3,18.599999999999994,"100082",191.9,17.5]
["100083",100083,null,"STK","TS120 160 Abzweiger 45°","CHF",291,"TECHNOSTAR 120",1.4,400,"J","TS120 160 Té 45°","TS120 160 Abzweiger 45°","TS120 160 Pezzo T 45°",121,1,"DN 160",null,264.5,"500005",null,null,291,"100083",26.5,263.39999999999998,27.600000000000023,"100083",291,26.5]
["100084",100084,null,"STK","TS120 200 Abzweiger 45°","CHF",341.2,"TECHNOSTAR 120",1.8,470,"J","TS120 200 Té 45°","TS120 200 Abzweiger 45°","TS120 200 Pezzo T 45°",121,1,"DN 200",null,310.10000000000002,"500006",null,null,341.2,"100084",31.099999999999966,309,32.199999999999989,"100084",341.2,31.099999999999966]
["100085",100085,null,"STK","TS120 250 Abzweiger 45°","CHF",397.8,"TECHNOSTAR 120",2.1,535,"J","TS120 250 Té 45°","TS120 250 Abzweiger 45°","TS120 250 Pezzo T 45°",121,1,"DN 250",null,361.6,"500007",null,null,397.8,"100085",36.199999999999989,360.5,37.300000000000011,"100085",397.8,36.199999999999989]
["100088",100088,null,"STK","TS120 60 Bogen 15°","CHF",14.8,"TECHNOSTAR 120",0.05,150,"J","TS120 60 Coude 15°","TS120 60 Bogen 15°","TS120 60 Curva 15°",121,1,"DN 60",null,13.4,"516315",null,null,14.8,"100088",1.4000000000000004,12.3,2.5,"100088",14.8,1.4000000000000004]
["100089",100089,null,"STK","TS120 60 Bogen 30°","CHF",14.8,"TECHNOSTAR 120",0.05,170,"J","TS120 60 Coude 30°","TS120 60 Bogen 30°","TS120 60 Curva 30°",121,1,"DN 60",null,13.4,"516330",null,null,14.8,"100089",1.4000000000000004,12.3,2.5,"100089",14.8,1.4000000000000004]
["100090",100090,null,"STK","TS120 60 Bogen 45°","CHF",14.8,"TECHNOSTAR 120",0.05,170,"J","TS120 60 Coude 45°","TS120 60 Bogen 45°","TS120 60 Curva 45°",121,1,"DN 60",null,13.4,"516345",null,null,14.8,"100090",1.4000000000000004,12.3,2.5,"100090",14.8,1.4000000000000004]
["100091",100091,null,"STK","TS120 60 Bogen 87°","CHF",14.8,"TECHNOSTAR 120",0.08,240,"J","TS120 60 Coude 87°","TS120 60 Bogen 87°","TS120 60 Curva 87°",121,1,"DN 60",null,13.4,"516387",null,null,14.8,"100091",1.4000000000000004,12.3,2.5,"100091",14.8,1.4000000000000004]
["100092",100092,null,"STK","TS120 80 Bogen 15°","CHF",15.7,"TECHNOSTAR 120",0.1,85,"J","TS120 80 Coude 15°","TS120 80 Bogen 15°","TS120 80 Curva 15°",121,1,"DN 80",null,14.2,"500121",null,null,15.7,"100092",1.5,13.1,2.5999999999999996,"100092",15.7,1.5]
["100093",100093,null,"STK","TS120 80 Bogen 30°","CHF",15.7,"TECHNOSTAR 120",0.2,124,"J","TS120 80 Coude 30°","TS120 80 Bogen 30°","TS120 80 Curva 30°",121,1,"DN 80",null,14.2,"500119",null,null,15.7,"100093",1.5,13.1,2.5999999999999996,"100093",15.7,1.5]
["100094",100094,null,"STK","TS120 80 Bogen 45°","CHF",15.7,"TECHNOSTAR 120",0.1,149,"J","TS120 80 Coude 45°","TS120 80 Bogen 45°","TS120 80 Curva 45°",121,1,"DN 80",null,14.2,"500123",null,null,15.7,"100094",1.5,13.1,2.5999999999999996,"100094",15.7,1.5]
["100095",100095,null,"STK","TS120 80 Bogen 87°","CHF",16.3,"TECHNOSTAR 120",0.2,186,"J","TS120 80 Coude 87°","TS120 80 Bogen 87°","TS120 80 Curva 87°",121,1,"DN 80",null,14.8,"500117",null,null,16.3,"100095",1.5,13.7,2.6000000000000014,"100095",16.3,1.5]
["100096",100096,null,"STK","TS120 110 Bogen 15°","CHF",19.5,"TECHNOSTAR 120",0.15,99,"J","TS120 110 Coude 15°","TS120 110 Bogen 15°","TS120 110 Curva 15°",121,1,"DN110",null,17.7,"500009",null,null,19.5,"100096",1.8000000000000007,16.600000000000001,2.8999999999999986,"100096",19.5,1.8000000000000007]
["100097",100097,null,"STK","TS120 110 Bogen 30°","CHF",19.5,"TECHNOSTAR 120",0.4,184,"J","TS120 110 Coude 30°","TS120 110 Bogen 30°","TS120 110 Curva 30°",121,1,"DN110",null,17.7,"500013",null,null,19.5,"100097",1.8000000000000007,16.600000000000001,2.8999999999999986,"100097",19.5,1.8000000000000007]
["100098",100098,null,"STK","TS120 110 Bogen 45°","CHF",20.3,"TECHNOSTAR 120",0.2,201,"J","TS120 110 Coude 45°","TS120 110 Bogen 45°","TS120 110 Curva 45°",121,1,"DN110",null,18.399999999999999,"500019",null,null,20.3,"100098",1.9000000000000021,17.3,3,"100098",20.3,1.9000000000000021]
["100099",100099,null,"STK","TS120 110 Bogen 87°","CHF",21.6,"TECHNOSTAR 120",0.25,266,"J","TS120 110 Coude 87°","TS120 110 Bogen 87°","TS120 110 Curva 87°",121,1,"DN110",null,19.600000000000001,"500024",null,null,21.6,"100099",2,18.5,3.1000000000000014,"100099",21.6,2]
["100100",100100,null,"STK","TS120 125 Bogen 15°","CHF",30,"TECHNOSTAR 120",0.2,106,"J","TS120 125 Coude 15°","TS120 125 Bogen 15°","TS120 125 Curva 15°",121,1,"DN 125",null,27.2,"500010",null,null,30,"100100",2.8000000000000007,26.1,3.8999999999999986,"100100",30,2.8000000000000007]
["100101",100101,null,"STK","TS120 125 Bogen 30°","CHF",30,"TECHNOSTAR 120",0.2,197,"J","TS120 125 Coude 30°","TS120 125 Bogen 30°","TS120 125 Curva 30°",121,1,"DN 125",null,27.2,"500014",null,null,30,"100101",2.8000000000000007,26.1,3.8999999999999986,"100101",30,2.8000000000000007]
["100102",100102,null,"STK","TS120 125 Bogen 45°","CHF",30,"TECHNOSTAR 120",0.25,217,"J","TS120 125 Coude 45°","TS120 125 Bogen 45°","TS120 125 Curva 45°",121,1,"DN 125",null,27.2,"500020",null,null,30,"100102",2.8000000000000007,26.1,3.8999999999999986,"100102",30,2.8000000000000007]
["100103",100103,null,"STK","TS120 125 Bogen 87°","CHF",34.4,"TECHNOSTAR 120",0.3,291,"J","TS120 125 Coude 87°","TS120 125 Bogen 87°","TS120 125 Curva 87°",121,1,"DN 125",null,31.2,"500025",null,null,34.4,"100103",3.1999999999999993,30.1,4.2999999999999972,"100103",34.4,3.1999999999999993]
["100104",100104,null,"STK","TS120 160 Bogen 15°","CHF",41.7,"TECHNOSTAR 120",0.45,121,"J","TS120 160 Coude 15°","TS120 160 Bogen 15°","TS120 160 Curva 15°",121,1,"DN 160",null,37.9,"500011",null,null,41.7,"100104",3.8000000000000043,36.799999999999997,4.9000000000000057,"100104",41.7,3.8000000000000043]
["100105",100105,null,"STK","TS120 160 Bogen 30°","CHF",41.7,"TECHNOSTAR 120",0.5,235,"J","TS120 160 Coude 30°","TS120 160 Bogen 30°","TS120 160 Curva 30°",121,1,"DN 160",null,37.9,"500015",null,null,41.7,"100105",3.8000000000000043,36.799999999999997,4.9000000000000057,"100105",41.7,3.8000000000000043]
["100106",100106,null,"STK","TS120 160 Bogen 45°","CHF",41.7,"TECHNOSTAR 120",0.5,261,"J","TS120 160 Coude 45°","TS120 160 Bogen 45°","TS120 160 Curva 45°",121,1,"DN 160",null,37.9,"500021",null,null,41.7,"100106",3.8000000000000043,36.799999999999997,4.9000000000000057,"100106",41.7,3.8000000000000043]
["100107",100107,null,"STK","TS120 160 Bogen 87°","CHF",47.9,"TECHNOSTAR 120",0.6,355,"J","TS120 160 Coude 87°","TS120 160 Bogen 87°","TS120 160 Curva 87°",121,1,"DN 160",null,43.5,"500026",null,null,47.9,"100107",4.3999999999999986,42.4,5.5,"100107",47.9,4.3999999999999986]
["100108",100108,null,"STK","TS120 200 Bogen 30°","CHF",227.9,"TECHNOSTAR 120",1,390,"J","TS120 200 Coude 30°","TS120 200 Bogen 30°","TS120 200 Curva 30°",121,1,"DN 200",null,207.1,"500016",null,null,227.9,"100108",20.800000000000011,206,21.900000000000006,"100108",227.9,20.800000000000011]
["100109",100109,null,"STK","TS120 200 Bogen 45°","CHF",239.2,"TECHNOSTAR 120",1.2,480,"J","TS120 200 Coude 45°","TS120 200 Bogen 45°","TS120 200 Curva 45°",121,1,"DN 200",null,217.4,"500022",null,null,239.2,"100109",21.799999999999983,216.3,22.899999999999977,"100109",239.2,21.799999999999983]
["100110",100110,null,"STK","TS120 200 Bogen 87°","CHF",284.5,"TECHNOSTAR 120",1,400,"J","TS120 200 Coude 87°","TS120 200 Bogen 87°","TS120 200 Curva 87°",121,1,"DN 200",null,258.60000000000002,"500027",null,null,284.5,"100110",25.899999999999977,257.5,27,"100110",284.5,25.899999999999977]
["100111",100111,null,"STK","TS120 250 Bogen 30°","CHF",250.5,"TECHNOSTAR 120",1,430,"J","TS120 250 Coude 30°","TS120 250 Bogen 30°","TS120 250 Curva 30°",121,1,"DN 250",null,227.7,"500017",null,null,250.5,"100111",22.800000000000011,226.6,23.900000000000006,"100111",250.5,22.800000000000011]
["100112",100112,null,"STK","TS120 250 Bogen 45°","CHF",273.2,"TECHNOSTAR 120",1.2,510,"J","TS120 250 Coude 45°","TS120 250 Bogen 45°","TS120 250 Curva 45°",121,1,"DN 250",null,248.3,"500023",null,null,273.2,"100112",24.899999999999977,247.2,26,"100112",273.2,24.899999999999977]
["100113",100113,null,"STK","TS120 250 Bogen 87°","CHF",329.8,"TECHNOSTAR 120",1.5,475,"J","TS120 250 Coude 87°","TS120 250 Bogen 87°","TS120 250 Curva 87°",121,1,"DN 250",null,299.8,"500028",null,null,329.8,"100113",30,298.7,31.100000000000023,"100113",329.8,30]
["100117",100117,null,"STK","TS120 80 Langbogen 45° ","CHF",16.3,"TECHNOSTAR 120",0.1,260,"J","TS120 80 Coude 45° alonge","TS120 80 Langbogen 45° ","TS120 80 Curva 45° lungo",121,1,"DN 80",null,14.8,"551200",null,null,16.3,"100117",1.5,13.7,2.6000000000000014,"100117",16.3,1.5]
["100118",100118,null,"STK","TS120 80 Langbogen 87° ","CHF",22.8,"TECHNOSTAR 120",0.1,260,"J","TS120 80 Coude 87° alonge","TS120 80 Langbogen 87° ","TS120 80 Curva 87° lungo",121,1,"DN 80",null,20.7,"551201",null,null,22.8,"100118",2.1000000000000014,19.600000000000001,3.1999999999999993,"100118",22.8,2.1000000000000014]
["100119",100119,null,"STK","TS120 110 Langbogen 45° ","CHF",20.3,"TECHNOSTAR 120",0.1,270,"J","TS120 110 Coude 45° alonge","TS120 110 Langbogen 45° ","TS120 110 Curva 45° lungo",121,1,"DN110",null,18.399999999999999,"551210",null,null,20.3,"100119",1.9000000000000021,17.3,3,"100119",20.3,1.9000000000000021]
["100120",100120,null,"STK","TS120 110 Langbogen 87° ","CHF",21.6,"TECHNOSTAR 120",0.1,270,"J","TS120 110 Coude 87° alonge","TS120 110 Langbogen 87° ","TS120 110 Curva 87° lungo",121,1,"DN110",null,19.600000000000001,"551211",null,null,21.6,"100120",2,18.5,3.1000000000000014,"100120",21.6,2]
["100121",100121,null,"STK","TS120 80 Revisionsbogen 87° ","CHF",53.1,"TECHNOSTAR 120",0.4,0,"J","TS120 80 Coude 87° avec nettoyage","TS120 80 Revisionsbogen 87° ","TS120 80 Curva 87° con revisione",121,1,"DN 80",null,48.2,"567025",null,null,53.1,"100121",4.8999999999999986,36.6,16.5,"100121",53.1,4.8999999999999986]
["100122",100122,null,"STK","TS120 110 Revisionsbogen 87° ","CHF",47,"TECHNOSTAR 120",0.3,210,"J","TS120 110 Coude 87° avec nettoyage","TS120 110 Revisionsbogen 87° ","TS120 110 Curva 87° con revisione",121,1,"DN110",null,42.7,"500031",null,null,47,"100122",4.2999999999999972,41.6,5.3999999999999986,"100122",47,4.2999999999999972]
["100123",100123,null,"STK","TS120 125 Revisionsbogen 87° ","CHF",115.5,"TECHNOSTAR 120",0.55000000000000004,222,"J","TS120 125 Coude 87° avec nettoyage","TS120 125 Revisionsbogen 87° ","TS120 125 Curva 87° con revisione",121,1,"DN 125",null,105,"500032",null,null,115.5,"100123",10.5,103.9,11.599999999999994,"100123",115.5,10.5]
["100124",100124,null,"STK","TS120 160 Revisionsbogen 87° ","CHF",246.7,"TECHNOSTAR 120",1,295,"J","TS120 160 Coude 87° avec nettoyage","TS120 160 Revisionsbogen 87° ","TS120 160 Curva 87° con revisione",121,1,"DN 160",null,224.2,"500033",null,null,246.7,"100124",22.5,223.1,23.599999999999994,"100124",246.7,22.5]
["100125",100125,null,"STK","TS120 200 Revisionsbogen 87° ","CHF",467.5,"TECHNOSTAR 120",1.5,310,"J","TS120 200 Coude 87° avec nettoyage","TS120 200 Revisionsbogen 87° ","TS120 200 Curva 87° con revisione",121,1,"DN 200",null,425,"500034",null,null,467.5,"100125",42.5,288.39999999999998,179.10000000000002,"100125",467.5,42.5]
["100126",100126,null,"STK","TS120 250 Revisionsbogen 87° ","CHF",492.8,"TECHNOSTAR 120",1.8,310,"J","TS120 250 Coude 87° avec nettoyage","TS120 250 Revisionsbogen 87° ","TS120 250 Curva 87° con revisione",121,1,"DN 250",null,448,"500035",null,null,492.8,"100126",44.800000000000011,309,183.8,"100126",492.8,44.800000000000011]
["100128",100128,null,"STK","TS120 60 Lang-Revisionsbogen 87° Putz hinten","CHF",53.3,"TECHNOSTAR 120",0.1,110,"J","TS120 60 Coude 87° avec nettoyage alonge","TS120 60 Lang-Revisionsbogen 87° Putz hinten","TS120 60 Curva 87° con revisione lungo",121,1,"DN 60",null,48.4,"516388",null,null,53.3,"100128",4.8999999999999986,47.3,6,"100128",53.3,4.8999999999999986]
["100129",100129,null,"STK","TS120 80 Lang-Revisionsbogen 87° Putz hinten","CHF",53.3,"TECHNOSTAR 120",0.4,130,"J","TS120 80 Coude 87° avec nettoyage alonge","TS120 80 Lang-Revisionsbogen 87° Putz hinten","TS120 80 Curva 87° con revisione lungo",121,1,"DN 80",null,48.4,"551203",null,null,53.3,"100129",4.8999999999999986,47.3,6,"100129",53.3,4.8999999999999986]
["100130",100130,null,"STK","TS120 80 Lang-Revisionsbogen 87° Putz links","CHF",53.3,"TECHNOSTAR 120",0.4,130,"J","TS120 80 Coude 87° avec nettoyage alonge gauche","TS120 80 Lang-Revisionsbogen 87° Putz links","TS120 80 Curva 87° con revisione lungo a sinistra",121,1,"DN 80",null,48.4,"551207",null,null,53.3,"100130",4.8999999999999986,47.3,6,"100130",53.3,4.8999999999999986]
["100131",100131,null,"STK","TS120 80 Lang-Revisionsbogen 87° Putz rechts","CHF",53.3,"TECHNOSTAR 120",0.4,130,"J","TS120 80 Coude 87° avec nettoyage alonge droit","TS120 80 Lang-Revisionsbogen 87° Putz rechts","TS120 80 Curva 87° con revisione lungo destra",121,1,"DN 80",null,48.4,"551205",null,null,53.3,"100131",4.8999999999999986,47.3,6,"100131",53.3,4.8999999999999986]
["100132",100132,null,"STK","TS120 80 Wandfutter hinterlüftet","CHF",15,"TECHNOSTAR 120",0.2,100,"J","TS120 80 Revêtement de paroi","TS120 80 Wandfutter hinterlüftet","TS120 80 Rivestimento a muro",121,1,"DN 80",null,13.6,"511054",null,null,15,"100132",1.4000000000000004,12.5,2.5,"100132",15,1.4000000000000004]
["100133",100133,null,"STK","TS120 110 Wandfutter hinterlüftet","CHF",21.4,"TECHNOSTAR 120",0.4,137,"J","TS120 110 Revêtement de paroi","TS120 110 Wandfutter hinterlüftet","TS120 110 Rivestimento a muro",121,1,"DN110",null,19.399999999999999,"511008",null,null,21.4,"100133",2,18.3,3.0999999999999979,"100133",21.4,2]
["100134",100134,null,"STK","TS120 125 Wandfutter hinterlüftet inox","CHF",138.6,"TECHNOSTAR 120",0.4,149,"J","TS120 125 Revêtement de paroi Inox","TS120 125 Wandfutter hinterlüftet inox","TS120 125 Rivestimento a muro Inox",121,1,"DN 125",null,126,"511009",null,null,138.6,"100134",12.599999999999994,124.9,13.699999999999989,"100134",138.6,12.599999999999994]
["100135",100135,null,"STK","TS120 160 Wandfutter hinterlüftet inox","CHF",154.6,"TECHNOSTAR 120",0.45,149,"J","TS120 160 Revêtement de paroi Inox","TS120 160 Wandfutter hinterlüftet inox","TS120 160 Rivestimento a muro Inox",121,1,"DN 160",null,140.5,"511010",null,null,154.6,"100135",14.099999999999994,139.4,15.199999999999989,"100135",154.6,14.099999999999994]
["100136",100136,null,"STK","TS120 200 Wandfutter hinterlüftet inox","CHF",97.2,"TECHNOSTAR 120",1,0,"J","TS120 200 Revêtement de paroi Inox","TS120 200 Wandfutter hinterlüftet inox","TS120 200 Rivestimento a muro Inox",121,1,"DN 200",null,88.3,"550796",null,null,97.2,"100136",8.9000000000000057,87.2,10,"100136",97.2,8.9000000000000057]
["100137",100137,null,"STK","TS120 250 Wandfutter hinterlüftet inox","CHF",100.6,"TECHNOSTAR 120",1,0,"J","TS120 250 Revêtement de paroi Inox","TS120 250 Wandfutter hinterlüftet inox","TS120 250 Rivestimento a muro Inox",121,1,"DN 250",null,91.4,"553175",null,null,100.6,"100137",9.1999999999999886,90.3,10.299999999999997,"100137",100.6,9.1999999999999886]
["100139",100139,null,"STK","TS120 60 Kaminabstützung komplett mit Bogen 87°","CHF",63.6,"TECHNOSTAR 120",0.2,0,"J","TS120 60 Support de la cheminée complètement","TS120 60 Kaminabstützung komplett mit Bogen 87°","TS120 60 Appoggio completo",121,1,"DN 60",null,57.8,"553118",null,null,63.6,"100139",5.8000000000000043,56.7,6.8999999999999986,"100139",63.6,5.8000000000000043]
["100140",100140,null,"STK","TS120 80 Kaminabstützung komplett mit Bogen 87°","CHF",68.599999999999994,"TECHNOSTAR 120",0.2,0,"J","TS120 80 Support de la cheminée complètement","TS120 80 Kaminabstützung komplett mit Bogen 87°","TS120 80 Appoggio completo",121,1,"DN 80",null,62.3,"511055",null,null,68.599999999999994,"100140",6.2999999999999972,61.2,7.3999999999999915,"100140",68.599999999999994,6.2999999999999972]
["100141",100141,null,"STK","TS120 110 Kaminabstützung komplett mit Bogen 87°","CHF",79.099999999999994,"TECHNOSTAR 120",2,0,"J","TS120 110 Support de la cheminée complètement","TS120 110 Kaminabstützung komplett mit Bogen 87°","TS120 110 Appoggio completo",121,1,"DN110",null,71.900000000000006,"553120",null,null,79.099999999999994,"100141",7.1999999999999886,70.8,8.2999999999999972,"100141",79.099999999999994,7.1999999999999886]
["100142",100142,null,"STK","TS120 125 Kaminabstützung komplett mit Bogen 87° ","CHF",175.6,"TECHNOSTAR 120",2.2999999999999998,0,"J","TS120 125 Support de la cheminée complètement","TS120 125 Kaminabstützung komplett mit Bogen 87° ","TS120 125 Appoggio completo",121,1,"DN 125",null,159.6,"513006",null,null,175.6,"100142",16,158.5,17.099999999999994,"100142",175.6,16]
["100143",100143,null,"STK","TS120 160 Kaminabstützung komplett mit Bogen 87°","CHF",223.2,"TECHNOSTAR 120",2.8,0,"J","TS120 160 Support de la cheminée complètement","TS120 160 Kaminabstützung komplett mit Bogen 87°","TS120 160 Appoggio completo",121,1,"DN 160",null,202.9,"513007",null,null,223.2,"100143",20.299999999999983,201.8,21.399999999999977,"100143",223.2,20.299999999999983]
["100144",100144,null,"STK","TS120 200 Kaminabstützung komplett mit Bogen 87°","CHF",308.2,"TECHNOSTAR 120",3.2,0,"J","TS120 200 Support de la cheminée complètement","TS120 200 Kaminabstützung komplett mit Bogen 87°","TS120 200 Appoggio completo",121,1,"DN 200",null,280.10000000000002,"513008",null,null,308.2,"100144",28.099999999999966,279,29.199999999999989,"100144",308.2,28.099999999999966]
["100145",100145,null,"STK","TS120 250 Kaminabstützung verstellbar ohne Bogen","CHF",500.5,"TECHNOSTAR 120",3.2,0,"J","TS120 250 Support de la cheminée sans Coude 87°","TS120 250 Kaminabstützung verstellbar ohne Bogen","TS120 250 Appoggio senza curva 87°",121,1,"DN 250",null,455,"513009",null,null,500.5,"100145",45.5,343.5,157,"100145",500.5,45.5]
["100147",100147,null,"STK","TS120 60 Abstandhalter für flex und starr","CHF",24.8,"TECHNOSTAR 120",0.05,0,"J","TS120 60 Distanceur pour rigides et flexibles","TS120 60 Abstandhalter für flex und starr","TS120 60 Distanzatori per tubo et flessibile",121,1,"DN 60",null,22.5,"516360",null,null,24.8,"100147",2.3000000000000007,7.1,17.700000000000003,"100147",24.8,2.3000000000000007]
["100148",100148,null,"STK","TS120 80 Abstandhalter für flex und starr","CHF",10.5,"TECHNOSTAR 120",0.3,0,"J","TS120 80 Distanceur pour rigides et flexibles ","TS120 80 Abstandhalter für flex und starr","TS120 80 Distanzatori per tubo et flessibile",121,1,"DN 80",null,9.5,"511089",null,null,10.5,"100148",1,7.7,2.8,"100148",10.5,1]
["100149",100149,null,"STK","TS120 110 Abstandhalter für flex und starr","CHF",11.6,"TECHNOSTAR 120",0.35,0,"J","TS120 110 Distanceur pour rigides et flexibles ","TS120 110 Abstandhalter für flex und starr","TS120 110 Distanzatori per tubo et flessibile",121,1,"DN110",null,10.5,"511091",null,null,11.6,"100149",1.0999999999999996,8.3000000000000007,3.2999999999999989,"100149",11.6,1.0999999999999996]
["100150",100150,null,"STK","TS120 125 Abstandhalter für starr","CHF",15.1,"TECHNOSTAR 120",0.5,0,"J","TS120 125 Distanceur pour rigides ","TS120 125 Abstandhalter für starr","TS120 125 Distanzatori per tubo ",121,1,"DN 125",null,13.7,"553084",null,null,15.1,"100150",1.4000000000000004,12.6,2.5,"100150",15.1,1.4000000000000004]
["100151",100151,null,"STK","TS120 160 Abstandhalter für flex ","CHF",16.5,"TECHNOSTAR 120",0.05,0,"J","TS120 160 Distanceur pour  flexibles ","TS120 160 Abstandhalter für flex ","TS120 160 Distanzatori per flessibile ",121,1,"DN 160",null,15,"516417",null,null,16.5,"100151",1.5,13.9,2.5999999999999996,"100151",16.5,1.5]
[{"$f":"B332&\"\"","v":"100152"},100152,null,"STK",{"$f":"IF($E$200=2,L332,IF($E$200=3,N332,M332))","v":"TS120 160 Abstandhalter für starr"},"CHF",{"$f":"IF($L$190=1,W332,S332)","v":16.100000000000001},"TECHNOSTAR 120",0.05,0,"J","TS120 160 Distanceur pour rigides ","TS120 160 Abstandhalter für starr","TS120 160 Distanzatori per tubo ",121,1,"DN 160",null,14.6,"516416",null,null,16.100000000000001,"100152",1.5000000000000018,13.5,2.6000000000000014,"100152",16.100000000000001,1.5000000000000018]
["100153",100153,null,"STK","TS120 200 Abstandhalter Inox","CHF",55.2,"TECHNOSTAR 120",2.7,0,"J","TS120 200 Distanceur rigides et flexibles Inox","TS120 200 Abstandhalter Inox","TS120 200 Abstandhalter Inox",121,1,"DN 200",null,50.1,"553095",null,null,55.2,"100153",5.1000000000000014,49,6.2000000000000028,"100153",55.2,5.1000000000000014]
["100157",100157,null,"STK","TS120 80 Kesselanschluss Reduktion zentr. 60","CHF",48.3,"TECHNOSTAR 120",0.01,0,"J","TS120 80 Raccordement reduction zentr. 60","TS120 80 Kesselanschluss Reduktion zentr. 60","TS120 80 Raccordo con reduzione zentr. 60",121,1,"DN 80",null,43.9,"500137",null,null,48.3,"100157",4.3999999999999986,42.8,5.5,"100157",48.3,4.3999999999999986]
["100158",100158,null,"STK","TS120 80 Kesselanschluss Reduktion zentr. 70","CHF",109.7,"TECHNOSTAR 120",0.15,0,"J","TS120 80 Raccordement reduction zentr. 70","TS120 80 Kesselanschluss Reduktion zentr. 70","TS120 80 Raccordo con reduzione zentr. 70",121,1,"DN 80",null,99.7,"500132",null,null,109.7,"100158",10,98.6,11.100000000000009,"100158",109.7,10]
["100159",100159,null,"STK","TS120 80 Kesselanschluss Reduktion zentr. 75","CHF",83,"TECHNOSTAR 120",0.15,0,"J","TS120 80 Raccordement reduction zentr. 75","TS120 80 Kesselanschluss Reduktion zentr. 75","TS120 80 Raccordo con reduzione zentr. 75",121,1,"DN 80",null,75.400000000000006,"500131",null,null,83,"100159",7.5999999999999943,74.3,8.7000000000000028,"100159",83,7.5999999999999943]
["100160",100160,null,"STK","TS120 110 Kesselanschluss Reduktion zentr. 80","CHF",56.6,"TECHNOSTAR 120",0.25,0,"J","TS120 110 Raccordement reduction zentr. 80","TS120 110 Kesselanschluss Reduktion zentr. 80","TS120 110 Raccordo con reduzione zentr. 80",121,1,"DN110",null,51.4,"500065",null,null,56.6,"100160",5.2000000000000028,50.3,6.3000000000000043,"100160",56.6,5.2000000000000028]
["100161",100161,null,"STK","TS120 110 Kesselanschluss Reduktion zentr. 100","CHF",100.9,"TECHNOSTAR 120",0.3,0,"J","TS120 110 Raccordement reduction zentr. 100","TS120 110 Kesselanschluss Reduktion zentr. 100","TS120 110 Raccordo con reduzione zentr. 100",121,1,"DN110",null,91.7,"500063",null,null,100.9,"100161",9.2000000000000028,90.6,10.300000000000011,"100161",100.9,9.2000000000000028]
["100162",100162,null,"STK","TS120 125 Kesselanschluss Reduktion zentr. 80","CHF",170.8,"TECHNOSTAR 120",0.25,0,"J","TS120 125 Raccordement reduction zentr. 80","TS120 125 Kesselanschluss Reduktion zentr. 80","TS120 125 Raccordo con reduzione zentr. 80",121,1,"DN 125",null,155.19999999999999,"500067",null,null,170.8,"100162",15.600000000000023,154.1,16.700000000000017,"100162",170.8,15.600000000000023]
["100164",100164,null,"STK","TS120 125 Kesselanschluss Reduktion zentr. 110","CHF",117.3,"TECHNOSTAR 120",0.3,0,"J","TS120 125 Raccordement reduction zentr. 110","TS120 125 Kesselanschluss Reduktion zentr. 110","TS120 125 Raccordo con reduzione zentr. 110",121,1,"DN 125",null,106.6,"500066",null,null,117.3,"100164",10.700000000000003,105.5,11.799999999999997,"100164",117.3,10.700000000000003]
["100167",100167,null,"STK","TS120 160 Kesselanschluss Reduktion zentr. 130","CHF",245.9,"TECHNOSTAR 120",0.5,0,"J","TS120 160 Raccordement reduction zentr. 130","TS120 160 Kesselanschluss Reduktion zentr. 130","TS120 160 Raccordo con reduzione zentr. 130",121,1,"DN 160",null,223.5,"500068",null,null,245.9,"100167",22.400000000000006,222.4,23.5,"100167",245.9,22.400000000000006]
["100168",100168,null,"STK","TS120 160 Kesselanschluss Reduktion zentr. 150","CHF",271,"TECHNOSTAR 120",0.55000000000000004,0,"J","TS120 160 Raccordement reduction zentr. 150","TS120 160 Kesselanschluss Reduktion zentr. 150","TS120 160 Raccordo con reduzione zentr. 150",121,1,"DN 160",null,246.3,"500069",null,null,271,"100168",24.699999999999989,245.2,25.800000000000011,"100168",271,24.699999999999989]
["100169",100169,null,"STK","TS120 200 Kesselanschluss Reduktion zentr. 180","CHF",346.5,"TECHNOSTAR 120",1,0,"J","TS120 200 Raccordement reduction zentr. 180","TS120 200 Kesselanschluss Reduktion zentr. 180","TS120 200 Raccordo con reduzione zentr. 180",121,1,"DN 200",null,315,"500133",null,null,346.5,"100169",31.5,226.6,119.9,"100169",346.5,31.5]
["100170",100170,null,"STK","TS120 250 Kesselanschluss Reduktion zentr. 200","CHF",250.5,"TECHNOSTAR 120",1.2,0,"J","TS120 250 Raccordement reduction zentr. 200","TS120 250 Kesselanschluss Reduktion zentr. 200","TS120 250 Raccordo con reduzione zentr. 200",121,1,"DN 200",null,227.7,"500134",null,null,250.5,"100170",22.800000000000011,226.6,23.900000000000006,"100170",250.5,22.800000000000011]
["100171",100171,null,"STK","TS120 110 Kesselanschluss Reduktion exzentr. 80","CHF",36.1,"TECHNOSTAR 120",0.2,0,"J","TS120 110 Raccordement reduction exzentr. 80","TS120 110 Kesselanschluss Reduktion exzentr. 80","TS120 110 Raccordo con reduzione exzentr. 80",121,1,"DN110",null,32.799999999999997,"511057",null,null,36.1,"100171",3.3000000000000043,31.7,4.4000000000000021,"100171",36.1,3.3000000000000043]
["100172",100172,null,"STK","TS120 125 Kesselanschluss Reduktion exzentr. 80","CHF",146.9,"TECHNOSTAR 120",0.3,0,"J","TS120 125 Raccordement reduction exzentr. 80","TS120 125 Kesselanschluss Reduktion exzentr. 80","TS120 125 Raccordo con reduzione exzentr. 80",121,1,"DN 125",null,133.5,"550680",null,null,146.9,"100172",13.400000000000006,132.4,14.5,"100172",146.9,13.400000000000006]
["100173",100173,null,"STK","TS120 125 Kesselanschluss Reduktion exzentr. 110","CHF",143.5,"TECHNOSTAR 120",0.3,0,"J","TS120 125 Raccordement reduction exzentr. 110","TS120 125 Kesselanschluss Reduktion exzentr. 110","TS120 125 Raccordo con reduzione exzentr. 110",121,1,"DN 125",null,130.4,"550681",null,null,143.5,"100173",13.099999999999994,129.30000000000001,14.199999999999989,"100173",143.5,13.099999999999994]
["100175",100175,null,"STK","TS120 80 Kesselanschluss Erweiterung zentr. 110","CHF",87.5,"TECHNOSTAR 120",0.2,0,"J","TS120 80 Raccordement enlargement zentr.110","TS120 80 Kesselanschluss Erweiterung zentr. 110","TS120 80 Raccordo allargamento zentr. 110",121,1,"DN 80",null,79.5,"511056",null,null,87.5,"100175",8,50.3,37.200000000000003,"100175",87.5,8]
["100176",100176,null,"STK","TS120 125 Kesselanschluss Erweiterung zentr. 130","CHF",122.4,"TECHNOSTAR 120",0.3,0,"J","TS120 125 Raccordement enlargement zentr.130","TS120 125 Kesselanschluss Erweiterung zentr. 130","TS120 125 Raccordo allargamento zentr. 130",121,1,"DN 125",null,111.2,"500061",null,null,122.4,"100176",11.200000000000003,77.099999999999994,45.300000000000011,"100176",122.4,11.200000000000003]
["100177",100177,null,"STK","TS120 110 Kesselanschluss Erweiterung exzentr. 125","CHF",109.4,"TECHNOSTAR 120",0.2,0,"J","TS120 110 Raccordement enlargement exzentr.125","TS120 110 Kesselanschluss Erweiterung exzentr. 125","TS120 110 Raccordo allargamento exzentr. 125",121,1,"DN110",null,99.4,"500043",null,null,109.4,"100177",10,98.3,11.100000000000009,"100177",109.4,10]
["100178",100178,null,"STK","TS120 125 Kesselanschluss Erweiterung exzentr. 160","CHF",158.6,"TECHNOSTAR 120",0.35,0,"J","TS120 125 Raccordement enlargement exzentr.130","TS120 125 Kesselanschluss Erweiterung exzentr. 160","TS120 125 Raccordo allargamento exzentr. 160",121,1,"DN 125",null,144.1,"500044",null,null,158.6,"100178",14.5,143,15.599999999999994,"100178",158.6,14.5]
["100179",100179,null,"STK","TS120 160 Kesselanschluss Erweiterung exzentr. 200","CHF",235,"TECHNOSTAR 120",0.85,0,"J","TS120 160 Raccordement enlargement exzentr.200","TS120 160 Kesselanschluss Erweiterung exzentr. 200","TS120 160 Raccordo allargamento exzentr. 200",121,1,"DN 160",null,213.6,"500045",null,null,235,"100179",21.400000000000006,212.5,22.5,"100179",235,21.400000000000006]
["100180",100180,null,"STK","TS120 200 Kesselanschluss Erweiterung exzentr. 250","CHF",284.5,"TECHNOSTAR 120",1.1000000000000001,165,"J","TS120 200 Raccordement enlargement exzentr.250","TS120 200 Kesselanschluss Erweiterung exzentr. 250","TS120 200 Raccordo allargamento exzentr. 250",121,1,"DN 200",null,258.60000000000002,"500046",null,null,284.5,"100180",25.899999999999977,257.5,27,"100180",284.5,25.899999999999977]
["100181",100181,null,"STK","TS120 250 Kesselanschluss Erweiterung exzentr. 315","CHF",307.2,"TECHNOSTAR 120",1.6,230,"J","TS120 250 Raccordement enlargement exzentr.315","TS120 250 Kesselanschluss Erweiterung exzentr. 315","TS120 250 Raccordo allargamento exzentr. 315",121,1,"DN 250",null,279.2,"500047",null,null,307.2,"100181",28,278.10000000000002,29.099999999999966,"100181",307.2,28]
["100182",100182,null,"STK","TS120 80 Abgasabsperrung 80 für Kaskade","CHF",225.7,"TECHNOSTAR 120",0.25,0,"J","TS120 80 Cascade lambeau 80","TS120 80 Abgasabsperrung 80 für Kaskade","TS120 80 Raccordo di cascade 80",121,1,"DN 80",null,205.1,"561262",null,null,225.7,"100182",20.599999999999994,204,21.699999999999989,"100182",225.7,20.599999999999994]
["100183",100183,null,"STK","TS120 110 Abgasabsperrung 100 für Kaskade","CHF",332.1,"TECHNOSTAR 120",0.25,0,"J","TS120 110 Cascade lambeau 100","TS120 110 Abgasabsperrung 100 für Kaskade","TS120 110 Raccordo di cascade 100",121,1,"DN110",null,301.89999999999998,"561264",null,null,332.1,"100183",30.200000000000045,300.8,31.300000000000011,"100183",332.1,30.200000000000045]
["100184",100184,null,"STK","TS120 110 Abgasabsperrung 80 für Kaskade","CHF",332.1,"TECHNOSTAR 120",0.25,0,"J","TS120 110 Cascade lambeau 80","TS120 110 Abgasabsperrung 80 für Kaskade","TS120 110 Raccordo di cascade 80",121,1,"DN110",null,301.89999999999998,"561263",null,null,332.1,"100184",30.200000000000045,300.8,31.300000000000011,"100184",332.1,30.200000000000045]
["100187",100187,null,"STK","TS120 Temperarturbegrenzer 120° mit montage Nippel","CHF",212.8,"TECHNOSTAR 120",0.2,0,"J","TS120 Limiteur de température 120°& embout montage","TS120 Temperarturbegrenzer 120° mit montage Nippel","TS120 Regulatore di termperatura 120° con tappo",121,1,"ZBH TS120",null,185,"511019",null,null,212.8,"100187",27.800000000000011,184.9,27.900000000000006,"100187",212.8,27.800000000000011]
["100188",100188,null,"STK","TS120 80 Kondensatanblauf senkrecht ","CHF",67.3,"TECHNOSTAR 120",0.1,215,"J","TS120 80 Ecoulement des condensates vertical","TS120 80 Kondensatanblauf senkrecht ","TS120 80 Scarico condensa verticale",121,1,"DN 80",null,61.1,"500136",null,null,67.3,"100188",6.1999999999999957,60,7.2999999999999972,"100188",67.3,6.1999999999999957]
["100189",100189,null,"STK","TS120 110 Kondensatanblauf senkrecht ","CHF",197.5,"TECHNOSTAR 120",0.4,130,"J","TS120 110 Ecoulement des condensates vertical","TS120 110 Kondensatanblauf senkrecht ","TS120 110 Scarico condensa verticale",121,1,"DN110",null,179.5,"500080",null,null,197.5,"100189",18,178.4,19.099999999999994,"100189",197.5,18]
["100190",100190,null,"STK","TS120 125 Kondensatanblauf senkrecht ","CHF",212.9,"TECHNOSTAR 120",0.45,130,"J","TS120 125 Ecoulement des condensates vertical","TS120 125 Kondensatanblauf senkrecht ","TS120 125 Scarico condensa verticale",121,1,"DN 125",null,193.5,"500081",null,null,212.9,"100190",19.400000000000006,192.4,20.5,"100190",212.9,19.400000000000006]
["100191",100191,null,"STK","TS120 160 Kondensatanblauf senkrecht ","CHF",242,"TECHNOSTAR 120",0.6,140,"J","TS120 160 Ecoulement des condensates vertical","TS120 160 Kondensatanblauf senkrecht ","TS120 160 Scarico condensa verticale",121,1,"DN 160",null,220,"500082",null,null,242,"100191",22,218.9,23.099999999999994,"100191",242,22]
["100192",100192,null,"STK","TS120 200 Kondensatanblauf senkrecht ","CHF",278.89999999999998,"TECHNOSTAR 120",1,170,"J","TS120 200 Ecoulement des condensates vertical","TS120 200 Kondensatanblauf senkrecht ","TS120 200 Scarico condensa verticale",121,1,"DN 200",null,253.5,"500083",null,null,278.89999999999998,"100192",25.399999999999977,252.4,26.499999999999972,"100192",278.89999999999998,25.399999999999977]
["100193",100193,null,"STK","TS120 250 Kondensatanblauf senkrecht ","CHF",358.2,"TECHNOSTAR 120",1.1000000000000001,170,"J","TS120 250 Ecoulement des condensates vertical","TS120 250 Kondensatanblauf senkrecht ","TS120 250 Scarico condensa verticale",121,1,"DN 250",null,325.60000000000002,"500084",null,null,358.2,"100193",32.599999999999966,324.5,33.699999999999989,"100193",358.2,32.599999999999966]
["100194",100194,null,"STK","TS120 60 Kondensatablauf waagrecht ","CHF",82.5,"TECHNOSTAR 120",0.15,0,"J","TS120 60 Ecoulement des condensates horizontal","TS120 60 Kondensatablauf waagrecht ","TS120 60 Scarico condensa orizontale",121,1,"DN 60",null,75,"516210",null,null,82.5,"100194",7.5,49.5,33,"100194",82.5,7.5]
["100195",100195,null,"STK","TS120 80 Kondensatablauf waagrecht ","CHF",67.3,"TECHNOSTAR 120",0.2,0,"J","TS120 80 Ecoulement des condensates horizontal","TS120 80 Kondensatablauf waagrecht ","TS120 80 Scarico condensa orizontale",121,1,"DN 80",null,61.1,"500139",null,null,67.3,"100195",6.1999999999999957,60,7.2999999999999972,"100195",67.3,6.1999999999999957]
["100196",100196,null,"STK","TS120 110 Kondensatablauf waagrecht","CHF",116.1,"TECHNOSTAR 120",0.5,0,"J","TS120 110 Ecoulement des condensates horizontal","TS120 110 Kondensatablauf waagrecht","TS120 110 Scarico condensa orizontale",121,1,"DN110",null,105.5,"500086",null,null,116.1,"100196",10.599999999999994,104.4,11.699999999999989,"100196",116.1,10.599999999999994]
["100197",100197,null,"STK","TS120 125 Kondensatablauf waagrecht","CHF",231.3,"TECHNOSTAR 120",0.65,0,"J","TS120 125 Ecoulement des condensates horizontal","TS120 125 Kondensatablauf waagrecht","TS120 125 Scarico condensa orizontale",121,1,"DN 125",null,210.2,"500087",null,null,231.3,"100197",21.100000000000023,209.1,22.200000000000017,"100197",231.3,21.100000000000023]
["100198",100198,null,"STK","TS120 160 Kondensatablauf waagrecht","CHF",317.3,"TECHNOSTAR 120",1.05,0,"J","TS120 160 Ecoulement des condensates horizontal","TS120 160 Kondensatablauf waagrecht","TS120 160 Scarico condensa orizontale",121,1,"DN 160",null,288.39999999999998,"500088",null,null,317.3,"100198",28.900000000000034,287.3,30,"100198",317.3,28.900000000000034]
["100199",100199,null,"STK","TS120 200 Kondensatablauf waagrecht ","CHF",390.5,"TECHNOSTAR 120",1.45,0,"J","TS120 200 Ecoulement des condensates horizontal","TS120 200 Kondensatablauf waagrecht ","TS120 200 Scarico condensa orizontale",121,1,"DN 200",null,355,"500089",null,null,390.5,"100199",35.5,252.4,138.1,"100199",390.5,35.5]
["100200",100200,null,"STK","TS120 250 Kondensatablauf waagrecht ","CHF",423.5,"TECHNOSTAR 120",1.5,0,"J","TS120 250 Ecoulement des condensates horizontal","TS120 250 Kondensatablauf waagrecht ","TS120 250 Scarico condensa orizontale",121,1,"DN 250",null,385,"500090",null,null,423.5,"100200",38.5,324.5,99,"100200",423.5,38.5]
["100201",100201,null,"STK","TS120 60 160 Endmuffe schwarz mit Mündungsrohr","CHF",78.099999999999994,"TECHNOSTAR 120",0.15,117,"J","TS120 60/160 Manchon de final noi avec tube final ","TS120 60 160 Endmuffe schwarz mit Mündungsrohr","TS120 60/160 Manica finale con tubo bocca L500mm",121,1,"DN 60",null,71,"516260",null,null,78.099999999999994,"100201",7.0999999999999943,69.900000000000006,8.1999999999999886,"100201",78.099999999999994,7.0999999999999943]
["100202",100202,null,"STK","TS120 80 160 Endmuffe schwarz mit Mündungsrohr","CHF",78.099999999999994,"TECHNOSTAR 120",0.15,117,"J","TS120 80/160 Manchon de final noi avec tube final","TS120 80 160 Endmuffe schwarz mit Mündungsrohr","TS120 80/160 Manica finale con tubo bocca L500mm",121,1,"DN 80",null,71,"500129",null,null,78.099999999999994,"100202",7.0999999999999943,69.900000000000006,8.1999999999999886,"100202",78.099999999999994,7.0999999999999943]
["100203",100203,null,"STK","TS120 80 200 Endmuffe schwarz mit Mündungsrohr","CHF",119.2,"TECHNOSTAR 120",0.15,117,"J","TS120 80/200 Manchon de final noi avec tube final ","TS120 80 200 Endmuffe schwarz mit Mündungsrohr","TS120 80/200 Manica finale con tubo bocca L500mm",121,1,"DN 80",null,108.3,"500128",null,null,119.2,"100203",10.900000000000006,107.2,12,"100203",119.2,10.900000000000006]
["100204",100204,null,"STK","TS120 80 250 Endmuffe schwarz mit Mündungsrohr","CHF",120.3,"TECHNOSTAR 120",0.15,117,"J","TS120 80/250 Manchon de final noi avec tube final","TS120 80 250 Endmuffe schwarz mit Mündungsrohr","TS120 80/250 Manica finale con tubo bocca L500mm",121,1,"DN 80",null,109.3,"500130",null,null,120.3,"100204",11,108.2,12.099999999999994,"100204",120.3,11]
["100205",100205,null,"STK","TS120 110 200 Endmuffe schwarz mit Mündungsrohr","CHF",124.2,"TECHNOSTAR 120",1.1000000000000001,100,"J","TS120 110/200 Manchon de final noi avec tube final","TS120 110 200 Endmuffe schwarz mit Mündungsrohr","TS120 110/200 Manica finale con tubo bocca L500mm",121,1,"DN110",null,112.9," 500038",null,null,124.2,"100205",11.299999999999997,111.8,12.400000000000006,"100205",124.2,11.299999999999997]
["100206",100206,null,"STK","TS120 110 250 Endmuffe schwarz mit Mündungsrohr","CHF",157.6,"TECHNOSTAR 120",0.3,100,"J","TS120 110/200 Manchon de final noi avec tube final","TS120 110 250 Endmuffe schwarz mit Mündungsrohr","TS120 110/250 Manica finale con tubo bocca L500mm",121,1,"DN110",null,143.19999999999999,"500125",null,null,157.6,"100206",14.400000000000006,142.1,15.5,"100206",157.6,14.400000000000006]
["100207",100207,null,"STK","TS120 125 200 Endmuffe schwarz mit Mündungsrohr","CHF",124.2,"TECHNOSTAR 120",0.15,100,"J","TS120 125/200 Manchon de final noi avec tube final","TS120 125 200 Endmuffe schwarz mit Mündungsrohr","TS120 125/200 Manica finale con tubo bocca L500mm",121,1,"DN 125",null,112.9,"500040",null,null,124.2,"100207",11.299999999999997,111.8,12.400000000000006,"100207",124.2,11.299999999999997]
["100208",100208,null,"STK","TS120 160 250 Endmuffe schwarz mit Mündungsrohr","CHF",157.6,"TECHNOSTAR 120",0.2,100,"J","TS120 160/250 Manchon de final noi avec tube final","TS120 160 250 Endmuffe schwarz mit Mündungsrohr","TS120 160/250 Manica finale con tubo bocca L500mm",121,1,"DN 160",null,143.19999999999999,"500041",null,null,157.6,"100208",14.400000000000006,142.1,15.5,"100208",157.6,14.400000000000006]
["100215",100215,null,"STK","TS120 60 Kaminkopfabedeckung schwarz","CHF",163.30000000000001,"TECHNOSTAR 120",1,0,"J","TS120 60 Recouvrement se souche noir","TS120 60 Kaminkopfabedeckung schwarz","TS120 60 Copertura del tombino PE",121,1,"DN 60",null,148.4,"516470",null,null,163.30000000000001,"100215",14.900000000000006,147.30000000000001,16,"100215",163.30000000000001,14.900000000000006]
["100216",100216,null,"STK","TS120 80 Kaminkopfabedeckung schwarz","CHF",178.4,"TECHNOSTAR 120",1.4,0,"J","TS120 80 Recouvrement se souche noir","TS120 80 Kaminkopfabedeckung schwarz","TS120 80 Copertura del tombino PE",121,1,"DN 80",null,162.1,"552056",null,null,178.4,"100216",16.300000000000011,161,17.400000000000006,"100216",178.4,16.300000000000011]
["100217",100217,null,"STK","TS120 110 Kaminkopfabdeckung schwarz","CHF",237.5,"TECHNOSTAR 120",1.6,0,"J","TS120 110 Recouvrement se souche noir","TS120 110 Kaminkopfabdeckung schwarz","TS120 110 Copertura del tombino PE",121,1,"DN110",null,215.9,"550763",null,null,237.5,"100217",21.599999999999994,214.8,22.699999999999989,"100217",237.5,21.599999999999994]
["100218",100218,null,"STK","TS120 80 Sprengring Flex zu Mündungasabschluss","CHF",35.200000000000003,"TECHNOSTAR 120",0.09,0,"J","TS120 80 Tube de d'embouchure et collier","TS120 80 Sprengring Flex zu Mündungasabschluss","TS120 80 Tubo finale et blomba di flessibile",121,1,"DN 80",null,32,"511066",null,null,35.200000000000003,"100218",3.2000000000000028,30.9,4.3000000000000043,"100218",35.200000000000003,3.2000000000000028]
["100219",100219,null,"STK","TS120 110 Sprengring Flex zu Mündungasabschluss","CHF",69.2,"TECHNOSTAR 120",0.09,0,"J","TS120 110 Tube de d'embouchure et collier","TS120 110 Sprengring Flex zu Mündungasabschluss","TS120110 Tubo finale et blomba di flessibile",121,1,"DN110",null,62.9,"511067",null,null,69.2,"100219",6.3000000000000043,61.8,7.4000000000000057,"100219",69.2,6.3000000000000043]
["100222",100222,null,"STK","TS120 80 Schachtabdeckung für starres Rohr Inox","CHF",262.60000000000002,"TECHNOSTAR 120",2,0,"J","TS120 80 Recouvr. se souche pour tube rigide Inox","TS120 80 Schachtabdeckung für starres Rohr Inox","TS120 80 Copertura del tombino tubo rigido Inox",121,1,"DN 80",null,238.65,"559801",null,null,262.60000000000002,"100222",23.950000000000017,226.6,36.000000000000028,"100222",262.60000000000002,23.950000000000017]
["100223",100223,null,"STK","TS120 80 Schachtabdeckung für flex. Rohr Inox","CHF",358.9,"TECHNOSTAR 120",2,0,"J","TS120 80 Recouvrement se souche flexible Inox","TS120 80 Schachtabdeckung für flex. Rohr Inox","TS120 80 Copertura del tombino tubo fless. Inox",121,1,"DN 80",null,326.27,"559805",null,null,358.9,"100223",32.629999999999995,247.2,111.69999999999999,"100223",358.9,32.629999999999995]
["100224",100224,null,"STK","TS120 110 Schachtabdeckung für starres Rohr Inox","CHF",318.2,"TECHNOSTAR 120",2,0,"J","TS120 110 Recouvr. se souche pour tube rigide Inox","TS120 110 Schachtabdeckung für starres Rohr Inox","TS120 110 Copertura del tombino tubo rigido Inox",121,1,"DN110",null,289.19,"559802",null,null,318.2,"100224",29.009999999999991,247.2,71,"100224",318.2,29.009999999999991]
["100225",100225,null,"STK","TS120 110 Schachtabdeckung für flex. Rohr Inox","CHF",494.2,"TECHNOSTAR 120",2,0,"J","TS120 110 Recouvrement se souche flexible Inox","TS120 110 Schachtabdeckung für flex. Rohr Inox","TS120 110 Copertura del tombino tubo fless. Inox",121,1,"DN110",null,449.22,"559806",null,null,494.2,"100225",44.979999999999961,267.8,226.39999999999998,"100225",494.2,44.979999999999961]
["100226",100226,null,"STK","TS120 125 Schachtabdeckung für starres Rohr Inox","CHF",299.60000000000002,"TECHNOSTAR 120",2,0,"J","TS120 125 Recouvr. se souche pour tube rigide Inox","TS120 125 Schachtabdeckung für starres Rohr Inox","TS120 125 Copertura del tombino tubo rigido Inox",121,1,"DN 125",null,272.36,"559803",null,null,299.60000000000002,"100226",27.240000000000009,329.6,-30,"100226",299.60000000000002,27.240000000000009]
["100228",100228,null,"STK","TS120 160 Schachtabdeckung für starres Rohr Inox","CHF",310.5,"TECHNOSTAR 120",2,0,"J","TS120 160 Recouvr. se souche pour tube rigide Inox","TS120 160 Schachtabdeckung für starres Rohr Inox","TS120 160 Copertura del tombino tubo rigido Inox",121,1,"DN 160",null,282.2,"559804",null,null,310.5,"100228",28.300000000000011,365.7,-55.199999999999989,"100228",310.5,28.300000000000011]
["100230",100230,null,"STK","TS120 80/125 Flachdachkragen Alu D125","CHF",182.1,"TECHNOSTAR 120",0.5,0,"J","TS120 80/125 Solin de toit plat en alu D125","TS120 80/125 Flachdachkragen Alu D125","TS120 80/125 Faldale Aluminio",121,1,"DN 80",null,165.5,"511074",null,null,182.1,"100230",16.599999999999994,164.4,17.699999999999989,"100230",182.1,16.599999999999994]
["100231",100231,null,"STK","TS120 110/160 Flachdachkragen Alu D160","CHF",201.1,"TECHNOSTAR 120",1,0,"J","TS120 110/160 Solin de toit plat en alu D160","TS120 110/160 Flachdachkragen Alu D160","TS120 110/160 Faldale Aluminio",121,1,"DN 110",null,182.8,"511075",null,null,201.1,"100231",18.299999999999983,181.7,19.400000000000006,"100231",201.1,18.299999999999983]
["100233",100233,null,"STK","TS120 80/125 Dachpfanne 5-25° schwarz","CHF",113.1,"TECHNOSTAR 120",3.2,0,"J","TS120 80/125 Solin toit universelle 5-25° noir","TS120 80/125 Dachpfanne 5-25° schwarz","TS120 80/125 Faldale universale 5-25° nero",121,1,"DN 80",null,102.8,"553195",null,null,113.1,"100233",10.299999999999997,101.7,11.399999999999991,"100233",113.1,10.299999999999997]
["100235",100235,null,"STK","TS120 80/125 Dachpfanne 25-45°  schwarz","CHF",113.1,"TECHNOSTAR 120",0.6,0,"J","TS120 80/125 Solin toit universelle 25-45° noir","TS120 80/125 Dachpfanne 25-45°  schwarz","TS120 80/125 Faldale universale 25-45° nero",121,1,"DN 80",null,102.8,"511078",null,null,113.1,"100235",10.299999999999997,101.7,11.399999999999991,"100235",113.1,10.299999999999997]
["100239",100239,null,"STK","TS120 110/160 Dachpfanne 25-45°  schwarz","CHF",199.9,"TECHNOSTAR 120",0.6,0,"J","TS120 110/160 Solin toit universelle 25-45° noir","TS120 110/160 Dachpfanne 25-45°  schwarz","TS120 110/160 Faldale universale 25-45° nero",121,1,"DN 110",null,181.7,"511079",null,null,199.9,"100239",18.200000000000017,180.6,19.300000000000011,"100239",199.9,18.200000000000017]
[{"$f":"B396&\"\"","v":"100240"},100240,null,"STK",{"$f":"IF($E$200=2,L396,IF($E$200=3,N396,M396))","v":"TS120 125/185 Dachpfanne 25-45°  schwarz"},"CHF",{"$f":"IF($L$190=1,W396,S396)","v":295.8},"TECHNOSTAR 120",0.6,0,"J","TS120 125/185 Solin toit universelle 25-45° noir","TS120 125/185 Dachpfanne 25-45°  schwarz","TS120 125/185 Faldale universale 25-45° nero",121,1,"DN 125",null,268.89999999999998,"511080",null,null,295.8,"100240",26.900000000000034,267.8,28,"100240",295.8,26.900000000000034]
["100246",100246,null,"STK","TS120 Schachtabdeckung 320x320mm Inox","CHF",263,"TECHNOSTAR 120",1,0,"J","TS120 Recouvrement 320mm x 320mm Inox pour gain ","TS120 Schachtabdeckung 320x320mm Inox","TS120 Copertura  320x320mm per elemento F90",121,1,"TS ZBH",null,248,"559810",null,null,263,"100246",15,247.2,15.800000000000011,"100246",263,15]
["100247",100247,null,"STK","TS120 Schachtabdeckung 400x400mm Inox","CHF",263,"TECHNOSTAR 120",2,0,"J","TS120 Recouvrement 400mm x 400mm Inox pour gain ","TS120 Schachtabdeckung 400x400mm Inox","TS120 Copertura 400x400mm per elemento F90",121,1,"TS ZBH",null,248,"559812",null,null,263,"100247",15,247.2,15.800000000000011,"100247",263,15]
["100248",100248,null,"STK","TS120 60 Lippendichtung Peroxyd für Muffe","CHF",8.8000000000000007,"TECHNOSTAR 120",0.01,0,"J","TS120 60 joint à lèvre de peroxyd pour manchon","TS120 60 Lippendichtung Peroxyd für Muffe","TS120 60 Guarnizione peroxyd per manicotto",121,1,"DN 60",null,8,"514000",null,null,8.8000000000000007,"100248",0.80000000000000071,4,4.8000000000000007,"100248",8.8000000000000007,0.80000000000000071]
["100249",100249,null,"STK","TS120 80 Lippendichtung Peroxyd für Muffe","CHF",11.3,"TECHNOSTAR 120",1.4999999999999999E-2,0,"J","TS120 80 joint à lèvre de peroxyd pour manchon","TS120 80 Lippendichtung Peroxyd für Muffe","TS120 80 Guarnizione peroxyd per manicotto",121,1,"DN 80",null,10.199999999999999,"514009",null,null,11.3,"100249",1.1000000000000014,9.1,2.2000000000000011,"100249",11.3,1.1000000000000014]
["100250",100250,null,"STK","TS120 110 Lippenndichtung Peroxyd für Muffe","CHF",13,"TECHNOSTAR 120",0.01,0,"J","TS120 110 joint à lèvre de peroxyd pour manchon","TS120 110 Lippenndichtung Peroxyd für Muffe","TS120 110 Guarnizione peroxyd per manicotto",121,1,"DN 110",null,11.8,"514001",null,null,13,"100250",1.1999999999999993,10.7,2.3000000000000007,"100250",13,1.1999999999999993]
["100251",100251,null,"STK","TS120 125 Lippendichtung Peroxyd für Muffe","CHF",14.1,"TECHNOSTAR 120",0.01,0,"J","TS120 125 joint à lèvre de peroxyd pour manchon","TS120 125 Lippendichtung Peroxyd für Muffe","TS120 125 Guarnizione peroxyd per manicotto",121,1,"DN 125",null,12.8,"514002",null,null,14.1,"100251",1.2999999999999989,11.7,2.4000000000000004,"100251",14.1,1.2999999999999989]
["100252",100252,null,"STK","TS120 160 Lippendichtung Peroxyd für Muffe","CHF",19.2,"TECHNOSTAR 120",0.01,0,"J","TS120 160 joint à lèvre de peroxyd pour manchon","TS120 160 Lippendichtung Peroxyd für Muffe","TS120 160 Guarnizione peroxyd per manicotto",121,1,"DN 160",null,17.399999999999999,"514003",null,null,19.2,"100252",1.8000000000000007,16.3,2.8999999999999986,"100252",19.2,1.8000000000000007]
["100256",100256,null,"STK","TS120 Syphon Typ A","CHF",48.3,"TECHNOSTAR 120",0.2,0,"J","TS120 Syphon Typ A","TS120 Syphon Typ A","TS120 Sifone Typ A",121,1,"TS ZBH",null,42,"500106",null,null,48.3,"100256",6.2999999999999972,39.5,8.7999999999999972,"100256",48.3,6.2999999999999972]
["100257",100257,null,"STK","TS120 Syphon Typ B","CHF",61.3,"TECHNOSTAR 120",0.3,0,"J","TS120 Syphon Typ B","TS120 Syphon Typ B","TS120 Sifone Typ B",121,1,"TS ZBH",null,55.7,"500107",null,null,61.3,"100257",5.5999999999999943,35.6,25.699999999999996,"100257",61.3,5.5999999999999943]
["100258",100258,null,"STK","TS120 Verschlussnippel für Messöffnung","CHF",15.4,"TECHNOSTAR 120",0.02,0,"J","TS120 Embout de mesure","TS120 Verschlussnippel für Messöffnung","TS120 Tappo di misura",121,1,"TS ZBH",null,14,"511006",null,null,15.4,"100258",1.4000000000000004,9.5,5.9,"100258",15.4,1.4000000000000004]
["100262",100262,null,"STK","TS120 Schlauchbriede zu Kondensatschlauch","CHF",6.5,"TECHNOSTAR 120",0.03,0,"J","TS120 Bride de tuyau de condensat","TS120 Schlauchbriede zu Kondensatschlauch","TS120 Brida di tubo condensa",121,1,"TS ZBH",null,5.9,"911003",null,null,6.5,"100262",0.59999999999999964,4.8,1.7000000000000002,"100262",6.5,0.59999999999999964]
["100263",100263,null,"STK","TS120 Montagebriede zu Kondensatschlauch","CHF",6.5,"TECHNOSTAR 120",0.02,0,"J","TS120 Bride de motage tuyau de condensat","TS120 Montagebriede zu Kondensatschlauch","TS120 Brida di maontago tubo condensa",121,1,"TS ZBH",null,5.9,"911004",null,null,6.5,"100263",0.59999999999999964,4.8,1.7000000000000002,"100263",6.5,0.59999999999999964]
["100264",100264,null,"STK","Kondesatschlauch 36mm L1000mm","CHF",7.5,"TECHNOSTAR 120",0.36,0,"J","TS120 Tuyau de condensat 36mm L1000mm","Kondesatschlauch 36mm L1000mm","TS120 Tubo condensa 36mm L1000",121,1,"TS ZBH",null,6.5,"911014",null,null,7.5,"100264",1,6.2,1.2999999999999998,"100264",7.5,1]
["100265",100265,null,"STK","Neutralisationsbox komplett","CHF",258.8,"TECHNOSTAR 120",11.27,0,"J","TS120 Boxe de neutralisation complet","Neutralisationsbox komplett","TS120 Bancinella di neutralisazione",121,1,"TS ZBH",null,225,"911025",null,null,258.8,"100265",33.800000000000011,225,33.800000000000011,"100265",258.8,33.800000000000011]
["100266",100266,null,"STK","Nachfüllset zu Neutralisationsbox","CHF",67.900000000000006,"TECHNOSTAR 120",3.1,0,"J","TS120 Set de replacément pour box  neutralisation","Nachfüllset zu Neutralisationsbox","TS120 Set di ricambio bancinella neutralisazione",121,1,"TS ZBH",null,59,"911015",null,null,67.900000000000006,"100266",8.9000000000000057,59,8.9000000000000057,"100266",67.900000000000006,8.9000000000000057]
["100275",100275,null,"STK","TS120 Gleitmittel 250ml","CHF",18.399999999999999,"TECHNOSTAR 120",0.25,0,"J","TS120 Lubrifiant ml","TS120 Gleitmittel 250ml","TS120 Lubrificante 250ml",121,1,"DN 250",null,16.7,"611007",null,null,18.399999999999999,"100275",1.6999999999999993,15.6,2.7999999999999989,"100275",18.399999999999999,1.6999999999999993]
["100280",100280,null,"STK","TS120 60 Rohrhalter fest ohne Gewinderohr","CHF",17.2,"TECHNOSTAR 120",0.45,0,"J","TS120 60 Collier avec plaque de base","TS120 60 Rohrhalter fest ohne Gewinderohr","TS120 60 Fascetta per Tubo con piastra 1/2\" ",121,1,"DN 60",null,13.7,"516450",null,null,17.2,"100280",3.5,12.6,4.5999999999999996,"100280",17.2,3.5]
["100281",100281,null,"STK","TS120 80 Rohrhalter fest ohne Gewinderohr","CHF",19.7,"TECHNOSTAR 120",0.45,0,"J","TS120 80 Collier avec plaque de base","TS120 80 Rohrhalter fest ohne Gewinderohr","TS120 80 Fascetta per Tubo con piastra 1/2\" ",121,1,"DN 80",null,15.7,"512032",null,null,19.7,"100281",4,14.6,5.0999999999999996,"100281",19.7,4]
["100282",100282,null,"STK","TS120 100 Rohrhalter fest ohne Gewinderohr","CHF",20.2,"TECHNOSTAR 120",0.45,0,"J","TS120 100 Collier avec plaque de base","TS120 100 Rohrhalter fest ohne Gewinderohr","TS120 100 Fascetta per Tubo con piastra 1/2\" ",121,1,"DN 60",null,16.100000000000001,"512025",null,null,20.2,"100282",4.0999999999999979,15,5.1999999999999993,"100282",20.2,4.0999999999999979]
["100283",100283,null,"STK","TS120 110 Rohrhalter fest ohne Gewinderohr","CHF",20.2,"TECHNOSTAR 120",0.5,0,"J","TS120 110 Collier avec plaque de base","TS120 110 Rohrhalter fest ohne Gewinderohr","TS120 110 Fascetta per Tubo con piastra 1/2\" ",121,1,"DN 110",null,16.100000000000001,"512026",null,null,20.2,"100283",4.0999999999999979,15,5.1999999999999993,"100283",20.2,4.0999999999999979]
["100284",100284,null,"STK","TS120 125 Rohrhalter fest ohne Gewinderohr","CHF",20.8,"TECHNOSTAR 120",0.55000000000000004,0,"J","TS120 125 Collier avec plaque de base","TS120 125 Rohrhalter fest ohne Gewinderohr","TS120 125 Fascetta per Tubo con piastra 1/2\" ",121,1,"DN 125",null,16.600000000000001,"512027",null,null,20.8,"100284",4.1999999999999993,15.5,5.3000000000000007,"100284",20.8,4.1999999999999993]
["100285",100285,null,"STK","TS120 160 Rohrhalter fest ohne Gewinderohr","CHF",22.9,"TECHNOSTAR 120",0.6,0,"J","TS120 160 Collier avec plaque de base","TS120 160 Rohrhalter fest ohne Gewinderohr","TS120 160 Fascetta per Tubo con piastra 1/2\" ",121,1,"DN 160",null,18.3,"512028",null,null,22.9,"100285",4.5999999999999979,17.2,5.6999999999999993,"100285",22.9,4.5999999999999979]
["100286",100286,null,"STK","TS120 200 Rohrhalter fest ohne Gewinderohr","CHF",28.3,"TECHNOSTAR 120",0.75,0,"J","TS120 200 Collier avec plaque de base","TS120 200 Rohrhalter fest ohne Gewinderohr","TS120 200 Fascetta per Tubo con piastra 1/2\" ",121,1,"DN 200",null,22.6,"512029",null,null,28.3,"100286",5.6999999999999993,21.5,6.8000000000000007,"100286",28.3,5.6999999999999993]
["100287",100287,null,"STK","TS120 250 Rohrhalter fest ohne Gewinderohr","CHF",41.4,"TECHNOSTAR 120",0.85,0,"J","TS120 250 Collier avec plaque de base","TS120 250 Rohrhalter fest ohne Gewinderohr","TS120 250 Fascetta per Tubo con piastra 1/2\" ",121,1,"DN 250",null,33.1,"512030",null,null,41.4,"100287",8.2999999999999972,32,9.3999999999999986,"100287",41.4,8.2999999999999972]
["100288",100288,null,"STK","TS120 60 Rohrhalter gleitend ohne Gewinderohr","CHF",40.799999999999997,"TECHNOSTAR 120",0.45,0,"J","TS120 60 Collier avec plaque de base coulissante","TS120 60 Rohrhalter gleitend ohne Gewinderohr","TS120 60 Fascetta scorrere Tubo con piastra1/2\" ",121,1,"DN 60",null,32.6,"516455",null,null,40.799999999999997,"100288",8.1999999999999957,31.5,9.2999999999999972,"100288",40.799999999999997,8.1999999999999957]
["100289",100289,null,"STK","TS120 80 Rohrhalter gleitend ohne Gewinderohr","CHF",42.4,"TECHNOSTAR 120",0.75,0,"J","TS120 80 Collier avec plaque de base coulissante","TS120 80 Rohrhalter gleitend ohne Gewinderohr","TS120 80 Fascetta scorrere Tubo con piastra1/2\" ",121,1,"DN 80",null,33.9,"512019",null,null,42.4,"100289",8.5,32.799999999999997,9.6000000000000014,"100289",42.4,8.5]
["100290",100290,null,"STK","TS120 100 Rohrhalter gleitend ohne Gewinderohr","CHF",43.5,"TECHNOSTAR 120",0.75,0,"J","TS120 100 Collier avec plaque de base coulissante","TS120 100 Rohrhalter gleitend ohne Gewinderohr","TS120 100 Fascetta scorrere Tubo con piastra1/2\" ",121,1,"DN 60",null,34.799999999999997,"512018",null,null,43.5,"100290",8.7000000000000028,33.700000000000003,9.7999999999999972,"100290",43.5,8.7000000000000028]
["100291",100291,null,"STK","TS120 110 Rohrhalter gleitend ohne Gewinderohr","CHF",43.5,"TECHNOSTAR 120",0.8,0,"J","TS120 110 Collier avec plaque de base coulissante","TS120 110 Rohrhalter gleitend ohne Gewinderohr","TS120 110 Fascetta scorrere Tubo con piastra1/2\" ",121,1,"DN 110",null,34.799999999999997,"512020",null,null,43.5,"100291",8.7000000000000028,33.700000000000003,9.7999999999999972,"100291",43.5,8.7000000000000028]
["100292",100292,null,"STK","TS120 125 Rohrhalter gleitend ohne Gewinderohr","CHF",45,"TECHNOSTAR 120",0.8,0,"J","TS120 125 Collier avec plaque de base coulissante","TS120 125 Rohrhalter gleitend ohne Gewinderohr","TS120 125 Fascetta scorrere Tubo con piastra1/2\" ",121,1,"DN 125",null,36,"512021",null,null,45,"100292",9,34.9,10.100000000000001,"100292",45,9]
["100293",100293,null,"STK","TS120 160 Rohrhalter gleitend ohne Gewinderohr","CHF",46.4,"TECHNOSTAR 120",0.85,0,"J","TS120 160 Collier avec plaque de base coulissante","TS120 160 Rohrhalter gleitend ohne Gewinderohr","TS120 160 Fascetta scorrere Tubo con piastra1/2\" ",121,1,"DN 160",null,37.1,"512022",null,null,46.4,"100293",9.2999999999999972,36,10.399999999999999,"100293",46.4,9.2999999999999972]
["100294",100294,null,"STK","TS120 200 Rohrhalter gleitend ohne Gewinderohr","CHF",56.7,"TECHNOSTAR 120",1.1000000000000001,0,"J","TS120 200 Collier avec plaque de base coulissante","TS120 200 Rohrhalter gleitend ohne Gewinderohr","TS120 200 Fascetta scorrere Tubo con piastra1/2\" ",121,1,"DN 200",null,45.3,"512023",null,null,56.7,"100294",11.400000000000006,44.2,12.5,"100294",56.7,11.400000000000006]
["100295",100295,null,"STK","TS120 250 Rohrhalter gleitend ohne Gewinderohr","CHF",57.7,"TECHNOSTAR 120",1.3,0,"J","TS120 250 Collier avec plaque de base coulissante","TS120 250 Rohrhalter gleitend ohne Gewinderohr","TS120 250 Fascetta scorrere Tubo con piastra1/2\" ",121,1,"DN 250",null,46.1,"512024",null,null,57.7,"100295",11.600000000000001,45,12.700000000000003,"100295",57.7,11.600000000000001]
["100308",100308,null,"STK","TS120 1/2\" Gewinderohr L2000mm","CHF",30.2,"TECHNOSTAR 120",2,0,"J","TS120 tube fileté 1/2\" galvanisé","TS120 1/2\" Gewinderohr L2000mm","TS120 1/2\" Tubo filettato per supporto del tubo ",121,1,"DN 200",null,24.1,"512000",null,null,30.2,"100308",6.0999999999999979,23,7.1999999999999993,"100308",30.2,6.0999999999999979]
["100309",100309,null,"STK","TS120LAS 60/100 Rohr L 250 weiss","CHF",38.700000000000003,"TECHNOSTAR 120 LAS",0.2,250,"J","TS120LAS 60/100 Tuyau L 250 blanc","TS120LAS 60/100 Rohr L 250 weiss","TS120LAS 60/100 Tubo L 250 bianco",122,1,"DN 60",null,35.1,"515001",null,null,38.700000000000003,"100309",3.6000000000000014,34,4.7000000000000028,"100309",38.700000000000003,3.6000000000000014]
["100310",100310,null,"STK","TS120LAS 60/100 Rohr L 500 weiss ","CHF",77.7,"TECHNOSTAR 120 LAS",1.5,500,"J","TS120LAS 60/100 Tuyau L 500 blanc ","TS120LAS 60/100 Rohr L 500 weiss ","TS120LAS 60/100 Tubo L 500 bianco",122,1,"DN 60",null,70.599999999999994,"515002",null,null,77.7,"100310",7.1000000000000085,69.5,8.2000000000000028,"100310",77.7,7.1000000000000085]
["100311",100311,null,"STK","TS120LAS 60/100 Rohr L 1000 weiss ","CHF",99.7,"TECHNOSTAR 120 LAS",3,1000,"J","TS120LAS 60/100 Tuyau L1000 blanc ","TS120LAS 60/100 Rohr L 1000 weiss ","TS120LAS 60/100 Tubo L1000 bianco",122,1,"DN 60",null,90.6,"515003",null,null,99.7,"100311",9.1000000000000085,89.5,10.200000000000003,"100311",99.7,9.1000000000000085]
["100312",100312,null,"STK","TS120LAS 60/100 Rohr L 2000 weiss ","CHF",150,"TECHNOSTAR 120 LAS",5.8,2000,"J","TS120LAS 60/100 Tuyau L 2000 blanc ","TS120LAS 60/100 Rohr L 2000 weiss ","TS120LAS 60/100 Tubo L 2000 bianco",122,1,"DN 60",null,136.30000000000001,"515004",null,null,150,"100312",13.699999999999989,135.19999999999999,14.800000000000011,"100312",150,13.699999999999989]
["100313",100313,null,"STK","TS120LAS 80/125 Rohr L 250 weiss ","CHF",70.599999999999994,"TECHNOSTAR 120 LAS",0.15,250,"J","TS120LAS 80/125 Tuyau L 250 blanc ","TS120LAS 80/125 Rohr L 250 weiss ","TS120LAS 60/100 Tubo L 2000 bianco",122,1,"DN 80",null,64.099999999999994,"500141",null,null,70.599999999999994,"100313",6.5,63,7.5999999999999943,"100313",70.599999999999994,6.5]
["100314",100314,null,"STK","TS120LAS 80/125 Rohr L 500 weiss ","CHF",93.4,"TECHNOSTAR 120 LAS",0.25,500,"J","TS120LAS 80/125 Tuyau L 500 blanc ","TS120LAS 80/125 Rohr L 500 weiss ","TS120LAS 80/125 Tubo L 500 bianco ",122,1,"DN 80",null,84.9,"500142",null,null,93.4,"100314",8.5,83.8,9.6000000000000085,"100314",93.4,8.5]
["100315",100315,null,"STK","TS120LAS 80/125 Rohr L 1000 weiss ","CHF",132.80000000000001,"TECHNOSTAR 120 LAS",0.5,1000,"J","TS120LAS 80/125 Tuyau L1000 blanc ","TS120LAS 80/125 Rohr L 1000 weiss ","TS120LAS 80/125 Tubo L1000 bianco ",122,1,"DN 80",null,120.7,"500143",null,null,132.80000000000001,"100315",12.100000000000009,119.6,13.200000000000017,"100315",132.80000000000001,12.100000000000009]
["100316",100316,null,"STK","TS120LAS 80/125 Rohr L 2000 weiss ","CHF",271.3,"TECHNOSTAR 120 LAS",6.5,2000,"J","TS120LAS 80/125 Tuyau L 2000 blanc ","TS120LAS 80/125 Rohr L 2000 weiss ","TS120LAS 80/125 Tubo L 2000 bianco ",122,1,"DN 80",null,246.6,"554600",null,null,271.3,"100316",24.700000000000017,245.5,25.800000000000011,"100316",271.3,24.700000000000017]
["100318",100318,null,"STK","TS120LAS 110/160 Rohr L 500 weiss","CHF",117.9,"TECHNOSTAR 120 LAS",0.35,500,"J","TS120LAS 110/160 Tuyau L 500 blanc","TS120LAS 110/160 Rohr L 500 weiss","TS120LAS 110/160 Tubo L 500 bianco",122,1,"DN 110",null,107.1,"560911",null,null,117.9,"100318",10.800000000000011,106,11.900000000000006,"100318",117.9,10.800000000000011]
["100319",100319,null,"STK","TS120LAS 110/160 Rohr L 1000 weiss ","CHF",173.8,"TECHNOSTAR 120 LAS",0.75,1000,"J","TS120LAS 110/160 Tuyau L1000 blanc ","TS120LAS 110/160 Rohr L 1000 weiss ","TS120LAS 110/160 Tubo L1000 bianco ",122,1,"DN 110",null,158,"560912",null,null,173.8,"100319",15.800000000000011,156.9,16.900000000000006,"100319",173.8,15.800000000000011]
["100320",100320,null,"STK","TS120LAS 110/160 Rohr L 2000 weiss ","CHF",340.5,"TECHNOSTAR 120 LAS",8.5,2000,"J","TS120LAS 110/160 Tuyau L 2000 blanc ","TS120LAS 110/160 Rohr L 2000 weiss ","TS120LAS 110/160 Tubo L 2000 bianco ",122,1,"DN 110",null,309.5,"560913",null,null,340.5,"100320",31,308.39999999999998,32.100000000000023,"100320",340.5,31]
["100321",100321,null,"STK","TS120LAS 60/100 Bogen 45° weiss ","CHF",52.6,"TECHNOSTAR 120 LAS",0.5,60,"J","TS120LAS 60/100 Coude 45° blanc ","TS120LAS 60/100 Bogen 45° weiss ","TS120LAS 60/100 Curva 45° bianco ",122,1,"DN 60",null,47.8,"515006",null,null,52.6,"100321",4.8000000000000043,46.7,5.8999999999999986,"100321",52.6,4.8000000000000043]
["100322",100322,null,"STK","TS120LAS 60/100 Bogen 87° weiss ","CHF",64.400000000000006,"TECHNOSTAR 120 LAS",0.25,120,"J","TS120LAS 60/100 Coude 87° blanc ","TS120LAS 60/100 Bogen 87° weiss ","TS120LAS 60/100 Curva 87° bianco ",122,1,"DN 60",null,58.5,"515007",null,null,64.400000000000006,"100322",5.9000000000000057,57.4,7.0000000000000071,"100322",64.400000000000006,5.9000000000000057]
["100323",100323,null,"STK","TS120LAS 60/100 Revisions Bogen 87° weiss ","CHF",112.9,"TECHNOSTAR 120 LAS",1.5,115,"J","TS120LAS 60/100 Coude de révision 87° blanc ","TS120LAS 60/100 Revisions Bogen 87° weiss ","TS120LAS 60/100 Curva  87° con revisione bianco ",122,1,"DN 60",null,102.6,"515010",null,null,112.9,"100323",10.300000000000011,101.5,11.400000000000006,"100323",112.9,10.300000000000011]
["100324",100324,null,"STK","TS120LAS 80/125 Bogen 15° weiss ","CHF",92.2,"TECHNOSTAR 120 LAS",0.2,150,"J","TS120LAS 80/125 Coude 15° blanc ","TS120LAS 80/125 Bogen 15° weiss ","TS120LAS 80/125 Curva 15° bianco ",122,1,"DN 80",null,83.8,"500144",null,null,92.2,"100324",8.4000000000000057,82.7,9.5,"100324",92.2,8.4000000000000057]
["100325",100325,null,"STK","TS120LAS 80/125 Bogen 30° weiss ","CHF",93.4,"TECHNOSTAR 120 LAS",0.2,133,"J","TS120LAS 80/125 Coude 30° blanc ","TS120LAS 80/125 Bogen 30° weiss ","TS120LAS 80/125 Curva 30° bianco ",122,1,"DN 80",null,84.9,"500145",null,null,93.4,"100325",8.5,83.8,9.6000000000000085,"100325",93.4,8.5]
["100327",100327,null,"STK","TS120LAS 80/125 Bogen 45° weiss ","CHF",94.6,"TECHNOSTAR 120 LAS",0.2,110,"J","TS120LAS 80/125 Coude 45° blanc ","TS120LAS 80/125 Bogen 45° weiss ","TS120LAS 80/125 Curva 45° bianco ",122,1,"DN 80",null,86,"500146",null,null,94.6,"100327",8.5999999999999943,84.9,9.6999999999999886,"100327",94.6,8.5999999999999943]
["100328",100328,null,"STK","TS120LAS 80/125 Bogen 87° weiss ","CHF",131.5,"TECHNOSTAR 120 LAS",0.2,136,"J","TS120LAS 80/125 Coude 87° blanc ","TS120LAS 80/125 Bogen 87° weiss ","TS120LAS 80/125 Curva 87° bianco ",122,1,"DN 80",null,119.5,"500147",null,null,131.5,"100328",12,118.4,13.099999999999994,"100328",131.5,12]
["100329",100329,null,"STK","TS120LAS 80/125 Revisions Bogen 87° weiss ","CHF",217.6,"TECHNOSTAR 120 LAS",0.2,0,"J","TS120LAS 80/125 Coude de révision 87° blanc ","TS120LAS 80/125 Revisions Bogen 87° weiss ","TS120LAS 80/125 Curva  87° con revisione bianco ",122,1,"DN 80",null,197.8,"560936",null,null,217.6,"100329",19.799999999999983,196.7,20.900000000000006,"100329",217.6,19.799999999999983]
["100331",100331,null,"STK","TS120LAS 110/160 Bogen 15° weiss","CHF",135.30000000000001,"TECHNOSTAR 120 LAS",0.3,145,"J","TS120LAS 110/160 Coude 15° blanc","TS120LAS 110/160 Bogen 15° weiss","TS120LAS 110/160 Curva 15° bianco",122,1,"DN 110",null,123,"560930",null,null,135.30000000000001,"100331",12.300000000000011,121.9,13.400000000000006,"100331",135.30000000000001,12.300000000000011]
["100332",100332,null,"STK","TS120LAS 110/160 Bogen 30° weiss","CHF",135.30000000000001,"TECHNOSTAR 120 LAS",0.3,150,"J","TS120LAS 110/160 Coude 30° blanc","TS120LAS 110/160 Bogen 30° weiss","TS120LAS 110/160 Curva 30° bianco",122,1,"DN 110",null,123,"560931",null,null,135.30000000000001,"100332",12.300000000000011,121.9,13.400000000000006,"100332",135.30000000000001,12.300000000000011]
["100333",100333,null,"STK","TS120LAS 110/160 Bogen 45° weiss","CHF",135.30000000000001,"TECHNOSTAR 120 LAS",0.3,150,"J","TS120LAS 110/160 Coude 45° blanc","TS120LAS 110/160 Bogen 45° weiss","TS120LAS 110/160 Curva 45° bianco",122,1,"DN 110",null,123,"560932",null,null,135.30000000000001,"100333",12.300000000000011,121.9,13.400000000000006,"100333",135.30000000000001,12.300000000000011]
["100334",100334,null,"STK","TS120LAS 110/160 Bogen 87° weiss","CHF",155.6,"TECHNOSTAR 120 LAS",0.5,150,"J","TS120LAS 110/160 Coude 87° blanc","TS120LAS 110/160 Bogen 87° weiss","TS120LAS 110/160 Curva 87° bianco",122,1,"DN 110",null,141.4,"560933",null,null,155.6,"100334",14.199999999999989,140.30000000000001,15.299999999999983,"100334",155.6,14.199999999999989]
["100335",100335,null,"STK","TS120LAS 110/160 Revisions Bogen 87° weiss ","CHF",250.7,"TECHNOSTAR 120 LAS",0.6,150,"J","TS120LAS 110/160 Coude de révision 87° blanc ","TS120LAS 110/160 Revisions Bogen 87° weiss ","TS120LAS 110/160 Curva con revisione 87° bianco ",122,1,"DN 110",null,227.9,"560934",null,null,250.7,"100335",22.799999999999983,226.8,23.899999999999977,"100335",250.7,22.799999999999983]
["100336",100336,null,"STK","TS120LAS 60/100 Kesselanschluss mit Messöffnung","CHF",97.4,"TECHNOSTAR 120 LAS",0.8,150,"J","TS120LAS 60/100 Raccordement chaudière av.mesurée","TS120LAS 60/100 Kesselanschluss mit Messöffnung","TS120LAS 60/100 Collegamento caldaia con misurata",122,1,"DN 60",null,88.5,"515009",null,null,97.4,"100336",8.9000000000000057,57.4,40.000000000000007,"100336",97.4,8.9000000000000057]
["100337",100337,null,"STK","TS120LAS 80/125 Kesselanschluss mit Messöffnung","CHF",109.5,"TECHNOSTAR 120 LAS",0.3,150,"J","TS120LAS 80/125 Raccordement chaudière av.mesurée","TS120LAS 80/125 Kesselanschluss mit Messöffnung","TS120LAS 80/125 Collegamento caldaia con misurata",122,1,"DN 80",null,99.5,"511071",null,null,109.5,"100337",10,98.4,11.099999999999994,"100337",109.5,10]
["100338",100338,null,"STK","TS120LAS 110/160 Kesselanschluss mit Messöffnung","CHF",152.6,"TECHNOSTAR 120 LAS",0.4,150,"J","TS120LAS 110/160 Raccordement chaudière av.mesurée","TS120LAS 110/160 Kesselanschluss mit Messöffnung","TS120LAS 110/160 Collegamento caldaia con misurata",122,1,"DN 110",null,138.69999999999999,"560900",null,null,152.6,"100338",13.900000000000006,137.6,15,"100338",152.6,13.900000000000006]
["100339",100339,null,"STK","TS120LAS 80/125 Reduktion auf 100/60 weiss","CHF",137.19999999999999,"TECHNOSTAR 120 LAS",0.3,70,"J","TS120LAS 80/125 Réduction de la 100/60 blanc","TS120LAS 80/125 Reduktion auf 100/60 weiss","TS120LAS 80/125 Riduzione a 100/60 bianco",122,1,"DN 80",null,124.7,"500171",null,null,137.19999999999999,"100339",12.499999999999986,123.6,13.599999999999994,"100339",137.19999999999999,12.499999999999986]
["100340",100340,null,"STK","TS120LAS 110/160 Reduktion auf 80/125 weiss","CHF",170,"TECHNOSTAR 120 LAS",0.3,150,"J","TS120LAS 110/160 Réduction de la 80/125 blanc","TS120LAS 110/160 Reduktion auf 80/125 weiss","TS120LAS 110/160 Riduzione a  80/125 bianco",122,1,"DN 110",null,154.5,"560920",null,null,170,"100340",15.5,153.4,16.599999999999994,"100340",170,15.5]
["100341",100341,null,"STK","TS120LAS 110/160 Reduktion auf 150/100 weiss","CHF",195.2,"TECHNOSTAR 120 LAS",0.3,150,"J","TS120LAS 110/160 Réduction de la 150/100 blanc","TS120LAS 110/160 Reduktion auf 150/100 weiss","TS120LAS 110/160 Riduzione a  150/100 bianco",122,1,"DN 110",null,177.4,"560950",null,null,195.2,"100341",17.799999999999983,176.3,18.899999999999977,"100341",195.2,17.799999999999983]
[{"$f":"B460&\"\"","v":"100342"},100342,null,"STK",{"$f":"IF($E$200=2,L460,IF($E$200=3,N460,M460))","v":"TS120LAS 60/100 Revisionsrohr gerade weiss"},"CHF",{"$f":"IF($L$190=1,W460,S460)","v":152},"TECHNOSTAR 120 LAS",0.2,220,"J","TS120LAS 60/100 Tuyau de révision blanc","TS120LAS 60/100 Revisionsrohr gerade weiss","TS120LAS 100/60 Tubo di revisione bianco",122,1,"DN 60",null,138.1,"560940",null,null,152,"100342",13.900000000000006,137,15,"100342",152,13.900000000000006]
["100343",100343,null,"STK","TS120LAS 80/125 Revisionsrohr gerade weiss","CHF",217.6,"TECHNOSTAR 120 LAS",0.2,220,"J","TS120LAS 80/125 Tuyau de révision blanc","TS120LAS 80/125 Revisionsrohr gerade weiss","TS120LAS 80/125 Tubo di revisione bianco",122,1,"DN 80",null,197.8,"500149",null,null,217.6,"100343",19.799999999999983,196.7,20.900000000000006,"100343",217.6,19.799999999999983]
["100344",100344,null,"STK","TS120LAS 80/125 Revisionsrohr ecke weiss","CHF",217.6,"TECHNOSTAR 120 LAS",0.2,0,"J","TS120LAS 80/125 Tuyau de révision coin blanc","TS120LAS 80/125 Revisionsrohr ecke weiss","TS120LAS 80/125 Tubo di revisione angolo bianco",122,1,"DN 80",null,197.8,"500148",null,null,217.6,"100344",19.799999999999983,196.7,20.900000000000006,"100344",217.6,19.799999999999983]
["100345",100345,null,"STK","TS120LAS 80/125 Revisionsrohr gerade flach weiss","CHF",217.6,"TECHNOSTAR 120 LAS",0.2,220,"J","TS120LAS 80/125 Tuyau de révision blanc","TS120LAS 80/125 Revisionsrohr gerade flach weiss","TS120LAS 80/125 Tubo di revisione bianco",122,1,"DN 80",null,197.8,"560944",null,null,217.6,"100345",19.799999999999983,196.7,20.900000000000006,"100345",217.6,19.799999999999983]
["100346",100346,null,"STK","TS120LAS 110/160 Revisionsrohr gerade weiss","CHF",220.5,"TECHNOSTAR 120 LAS",0.3,250,"J","TS120LAS 110/160 Tuyau de révision voudrais blanc","TS120LAS 110/160 Revisionsrohr gerade weiss","TS120LAS 80/125 Tubo di revisione sarebbe bianco",122,1,"DN 110",null,200.4,"560935",null,null,220.5,"100346",20.099999999999994,199.3,21.199999999999989,"100346",220.5,20.099999999999994]
["100347",100347,null,"STK","TS120LAS 125/80/80 Kesselanschl. Luft Abgas getr.","CHF",137.80000000000001,"TECHNOSTAR 120 LAS",0.3,0,"J","TS120LAS 125/80/80 Racc. chaudiére  air séparé","TS120LAS 125/80/80 Kesselanschl. Luft Abgas getr.","TS120LAS 125/80/80 Racc. caldaia  airia separata",122,1,"DN 80",null,125.2,"511073",null,null,137.80000000000001,"100347",12.600000000000009,124.1,13.700000000000017,"100347",137.80000000000001,12.600000000000009]
["100353",100353,null,"STK","TS120 125 Abdeckblende weiss ","CHF",59.3,"TECHNOSTAR 120",0.1,0,"J","TS120 125 Cache blanc","TS120 125 Abdeckblende weiss ","TS120 125 Rosetta bianco",121,1,"DN 125",null,53.9,"500160",null,null,59.3,"100353",5.3999999999999986,52.8,6.5,"100353",59.3,5.3999999999999986]
["100354",100354,null,"STK","TS120 160 Abdeckblende weiss","CHF",82.9,"TECHNOSTAR 120",0.1,0,"J","TS120 160 Cache blanc","TS120 160 Abdeckblende weiss","TS120 160 Rosetta bianco",121,1,"DN 160",null,75.3,"500162",null,null,82.9,"100354",7.6000000000000085,74.2,8.7000000000000028,"100354",82.9,7.6000000000000085]
["100355",100355,null,"STK","TS120 125 Abdeckblende DN125 für schrägdach weiss ","CHF",55.5,"TECHNOSTAR 120",0.4,0,"J","TS120 125 Cache  toiture en pente blanc","TS120 125 Abdeckblende DN125 für schrägdach weiss ","TS120 125  Rosetta tetto piovente bianco",121,1,"DN 125",null,50.4,"559899",null,null,55.5,"100355",5.1000000000000014,49.3,6.2000000000000028,"100355",55.5,5.1000000000000014]
["100356",100356,null,"STK","TS120 125 Abdeckblende DN160 für schrägdach weiss ","CHF",65.900000000000006,"TECHNOSTAR 120",0.6,0,"J","TS120 160 Cache toiture en pente blanc","TS120 125 Abdeckblende DN160 für schrägdach weiss ","TS120 160  Rosetta tetto piovente bianco",121,1,"DN 125",null,59.9,"559900",null,null,65.900000000000006,"100356",6.0000000000000071,58.8,7.1000000000000085,"100356",65.900000000000006,6.0000000000000071]
["100357",100357,null,"STK","TS120LAS 80/125 Klemmband Kesselanschluss weiss","CHF",57.9,"TECHNOSTAR 120 LAS",0.05,0,"J","TS120LAS 125 Collier de la raccordement blanc","TS120LAS 80/125 Klemmband Kesselanschluss weiss","TS120LAS 125 Brida di raccordo di caldaia bianco",122,1,"DN 80",null,52.6,"552166",null,null,57.9,"100357",5.2999999999999972,51.5,6.3999999999999986,"100357",57.9,5.2999999999999972]
["100358",100358,null,"STK","TS120LAS 80/125 Kesselanschlussgitter weiss","CHF",82.9,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 80/125 pour air a actionnè indépendants ","TS120LAS 80/125 Kesselanschlussgitter weiss","TS120LAS 80/125 Grill LAS bianco",122,1,"DN 80",null,75.3,"500175",null,null,82.9,"100358",7.6000000000000085,74.2,8.7000000000000028,"100358",82.9,7.6000000000000085]
["100359",100359,null,"STK","TS120LAS 110/160 Kesselanschlussgitter weiss","CHF",90.8,"TECHNOSTAR 120 LAS",0.45,0,"J","TS120LAS 110/160 pour air a actionnè indépendants ","TS120LAS 110/160 Kesselanschlussgitter weiss","TS120LAS 110/160 Grill LAS bianco",122,1,"DN 110",null,82.5,"500176",null,null,90.8,"100359",8.2999999999999972,81.400000000000006,9.3999999999999915,"100359",90.8,8.2999999999999972]
["100360",100360,null,"STK","TS120LAS 60/100 Kondensatablauf waagrecht weiss","CHF",140.6,"TECHNOSTAR 120 LAS",0.2,0,"J","TS120LAS 60/100 Ecoulement condensat horozontal","TS120LAS 60/100 Kondensatablauf waagrecht weiss","TS120LAS 60/100 Scarico condensa orizontale bianco",122,1,"DN 60",null,127.8,"560948",null,null,140.6,"100360",12.799999999999997,126.7,13.899999999999991,"100360",140.6,12.799999999999997]
["100361",100361,null,"STK","TS120LAS 80/125 Kondensatablauf waagrecht weiss","CHF",217.6,"TECHNOSTAR 120 LAS",0.2,0,"J","TS120LAS 80/125 Ecoulement condensat horozontal","TS120LAS 80/125 Kondensatablauf waagrecht weiss","TS120LAS 80/125 Scarico condensa orizontale bianco",122,1,"DN 80",null,197.8,"500151",null,null,217.6,"100361",19.799999999999983,196.7,20.900000000000006,"100361",217.6,19.799999999999983]
["100362",100362,null,"STK","TS120LAS 110/160 Kondensatablauf waagrecht weiss","CHF",324.5,"TECHNOSTAR 120 LAS",0.2,0,"J","TS120LAS 110/160 Ecoulement condensat horozontal","TS120LAS 110/160 Kondensatablauf waagrecht weiss","TS120LAS 110/160 Scarico condensa orizontale bianco",122,1,"DN 110",null,295,"560955",null,null,324.5,"100362",29.5,293.89999999999998,30.600000000000023,"100362",324.5,29.5]
["100363",100363,null,"STK","TS120LAS 80/125 Kondensat. senkr. mit rev.öffnung","CHF",299.10000000000002,"TECHNOSTAR 120 LAS",0.2,220,"J","TS120LAS 80/125 Ecoulement condensat vertical ","TS120LAS 80/125 Kondensat. senkr. mit rev.öffnung","TS120LAS 80/125 Scarico condensa verticale bianco",122,1,"DN 80",null,271.89999999999998,"550159",null,null,299.10000000000002,"100363",27.200000000000045,270.8,28.300000000000011,"100363",299.10000000000002,27.200000000000045]
["100364",100364,null,"STK","TS120LAS 110/160 Kondensat. senkr. mit rev.öffnung","CHF",313.5,"TECHNOSTAR 120 LAS",0.2,250,"J","TS120LAS 110/160 Ecoulement condensat vertical","TS120LAS 110/160 Kondensat. senkr. mit rev.öffnung","TS120LAS 110/160 Scarico condensa verticale bianco",122,1,"DN 110",null,285,"560965",null,null,313.5,"100364",28.5,222.4,91.1,"100364",313.5,28.5]
["100365",100365,null,"STK","TS120LAS 80/125 T-Stück mit Kondensatanblauf senk.","CHF",217.6,"TECHNOSTAR 120 LAS",0.2,220,"J","TS120LAS 80/125 pce T avec ecluvèmet et nettoyage ","TS120LAS 80/125 T-Stück mit Kondensatanblauf senk.","TS120LAS 80/125 pezzo T  scarico cond. et revisone",122,1,"DN 80",null,197.8,"500159",null,null,217.6,"100365",19.799999999999983,196.7,20.900000000000006,"100365",217.6,19.799999999999983]
["100366",100366,null,"STK","TS120LAS 80/125 Schiebestück 305mm weiss","CHF",145.69999999999999,"TECHNOSTAR 120 LAS",2.1,240,"J","TS120LAS 80/125 Elément télescopique 305mm blanc","TS120LAS 80/125 Schiebestück 305mm weiss","TS120LAS 80/125 Elemento telescopico 305mm binco ",122,1,"DN 80",null,132.4,"550380",null,null,145.69999999999999,"100366",13.299999999999983,131.30000000000001,14.399999999999977,"100366",145.69999999999999,13.299999999999983]
["100367",100367,null,"STK","TS120LAS 110/160 Schiebestück 355mm weiss","CHF",167.2,"TECHNOSTAR 120 LAS",4,170,"J","TS120LAS 110/160 Elément télescopique 355mm blanc","TS120LAS 110/160 Schiebestück 355mm weiss","TS120LAS 110/160 Elemento telescopico 355mm binco ",122,1,"DN 110",null,152,"550382",null,null,167.2,"100367",15.199999999999989,150.9,16.299999999999983,"100367",167.2,15.199999999999989]
["100368",100368,null,"STK","TS120LAS 80/125 T-Stück weiss","CHF",217.6,"TECHNOSTAR 120 LAS",0.4,220,"J","TS120LAS 80/125 Piece T blanc","TS120LAS 80/125 T-Stück weiss","TS120LAS 80/125 Pezzo T bianco",122,1,"DN 80",null,197.8,"500170",null,null,217.6,"100368",19.799999999999983,196.7,20.900000000000006,"100368",217.6,19.799999999999983]
["100369",100369,null,"STK","TS120LAS 110/160 T-Stück weiss","CHF",220.5,"TECHNOSTAR 120 LAS",0.4,250,"J","TS120LAS 110/160 Piece T blanc","TS120LAS 110/160 T-Stück weiss","TS120LAS 110/160 Pezzo T bianco",122,1,"DN 110",null,200.4,"560960",null,null,220.5,"100369",20.099999999999994,199.3,21.199999999999989,"100369",220.5,20.099999999999994]
["100370",100370,null,"STK","TS120LAS 80/125 Kaminabstützung für Schacht","CHF",193.9,"TECHNOSTAR 120 LAS",2,0,"J","TS120LAS 80/125 Chemineé soutien blanc","TS120LAS 80/125 Kaminabstützung für Schacht","TS120LAS 80/125 Appoggio bianco",122,1,"DN 80",null,176.2,"513004",null,null,193.9,"100370",17.700000000000017,175.1,18.800000000000011,"100370",193.9,17.700000000000017]
["100371",100371,null,"STK","TS120LAS 110/160 Kaminabstützung für Schacht","CHF",256.2,"TECHNOSTAR 120 LAS",2.15,0,"J","TS120LAS 110/160 Chemineé soutien blanc","TS120LAS 110/160 Kaminabstützung für Schacht","TS120LAS 110/160 Appoggio bianco",122,1,"DN 110",null,232.9,"513005",null,null,256.2,"100371",23.299999999999983,231.8,24.399999999999977,"100371",256.2,23.299999999999983]
["100372",100372,null,"STK","TS120LAS 80/125 Verbindungselement 2 Teilig","CHF",116.9,"TECHNOSTAR 120 LAS",0.3,0,"J","TS120LAS 80/125 élément de raccordement  blanc ","TS120LAS 80/125 Verbindungselement 2 Teilig","TS120LAS 80/125Elemento da congiungere bianco",122,1,"DN 80",null,106.2,"552164",null,null,116.9,"100372",10.700000000000003,105.1,11.800000000000011,"100372",116.9,10.700000000000003]
["100373",100373,null,"STK","TS120  Zuluftgitter 200mm x 200mm weiss","CHF",116.9,"TECHNOSTAR 120",0.3,0,"J","TS120 Grille d'amissin d'air 200mm x 200mm blanc","TS120  Zuluftgitter 200mm x 200mm weiss","TS120 Grill di aria 200mm x 200mm bianco",121,1,"DN 200",null,106.2,"550850",null,null,116.9,"100373",10.700000000000003,105.1,11.800000000000011,"100373",116.9,10.700000000000003]
["100380",100380,null,"STK","TS120LAS 125 LAS Anfängerplatte 400x400 Inox","CHF",198,"TECHNOSTAR 120 LAS",1,0,"J","TS120LAS 125 LAS Cache plafond 400mm x 400mm Inox","TS120LAS 125 LAS Anfängerplatte 400x400 Inox","TS120LAS 125 LAS Partenza verticale 400mm x 400mm ",122,1,"DN 80",null,180,"500165",null,null,198,"100380",18,92.6,105.4,"100380",198,18]
["100382",100382,null,"STK","TS120LAS 80/125 Rohr L 250 Inox ","CHF",80.599999999999994,"TECHNOSTAR 120 LAS",0.15,250,"J","TS120LAS 80/125 Tuyau L 250 Inox ","TS120LAS 80/125 Rohr L 250 Inox ","TS120LAS 80/125 Tubo L 250 Inox",122,1,"DN 80",null,73.2,"500108",null,null,80.599999999999994,"100382",7.3999999999999915,72.099999999999994,8.5,"100382",80.599999999999994,7.3999999999999915]
["100383",100383,null,"STK","TS120LAS 80/125 Rohr L 500 Inox ","CHF",108.2,"TECHNOSTAR 120 LAS",0.25,500,"J","TS120LAS 80/125 Tuyau L 500 Inox ","TS120LAS 80/125 Rohr L 500 Inox ","TS120LAS 80/125 Tubo L 500 Inox",122,1,"DN 80",null,98.3,"500109",null,null,108.2,"100383",9.9000000000000057,97.2,11,"100383",108.2,9.9000000000000057]
["100384",100384,null,"STK","TS120LAS 80/125 Rohr L 1000 Inox ","CHF",180.7,"TECHNOSTAR 120 LAS",0.5,1000,"J","TS120LAS 80/125 Tuyau L1000 Inox ","TS120LAS 80/125 Rohr L 1000 Inox ","TS120LAS 80/125 Tubo L1000 Inox",122,1,"DN 80",null,164.2,"500110",null,null,180.7,"100384",16.5,163.1,17.599999999999994,"100384",180.7,16.5]
["100385",100385,null,"STK","TS120LAS 80/125 Rohr L 2000 Inox ","CHF",302.2,"TECHNOSTAR 120 LAS",5.8,2000,"J","TS120LAS 80/125 Tuyau L 2000 Inox ","TS120LAS 80/125 Rohr L 2000 Inox ","TS120LAS 80/125 Tubo L 2000 Inox",122,1,"DN 80",null,274.7,"554636",null,null,302.2,"100385",27.5,273.60000000000002,28.599999999999966,"100385",302.2,27.5]
["100386",100386,null,"STK","TS120LAS 110/160 Rohr L 250 Inox ","CHF",99.9,"TECHNOSTAR 120 LAS",1.8,250,"J","TS120LAS 110/160 Tuyau L 250 Inox ","TS120LAS 110/160 Rohr L 250 Inox ","TS120LAS 110/160 Tubo L 250 Inox",122,1,"DN 110",null,90.8,"565000",null,null,99.9,"100386",9.1000000000000085,89.7,10.200000000000003,"100386",99.9,9.1000000000000085]
["100387",100387,null,"STK","TS120LAS 110/160 Rohr L 500 Inox ","CHF",144.5,"TECHNOSTAR 120 LAS",2.2999999999999998,500,"J","TS120LAS 110/160 Tuyau L 500 Inox ","TS120LAS 110/160 Rohr L 500 Inox ","TS120LAS 110/160 Tubo L 500 Inox",122,1,"DN 110",null,131.30000000000001,"565500",null,null,144.5,"100387",13.199999999999989,130.19999999999999,14.300000000000011,"100387",144.5,13.199999999999989]
["100388",100388,null,"STK","TS120LAS 110/160 Rohr L 1000 Inox ","CHF",251.1,"TECHNOSTAR 120 LAS",4.5,1000,"J","TS120LAS 110/160 Tuyau L1000 Inox ","TS120LAS 110/160 Rohr L 1000 Inox ","TS120LAS 110/160 Tubo L1000 Inox",122,1,"DN 110",null,228.2,"561000",null,null,251.1,"100388",22.900000000000006,227.1,24,"100388",251.1,22.900000000000006]
["100389",100389,null,"STK","TS120LAS 110/160 Rohr L 2000 Inox ","CHF",352.5,"TECHNOSTAR 120 LAS",7.9,2000,"J","TS120LAS 110/160 Tuyau L 2000 Inox ","TS120LAS 110/160 Rohr L 2000 Inox ","TS120LAS 110/160 Tubo L 2000 Inox",122,1,"DN 110",null,320.39999999999998,"550388",null,null,352.5,"100389",32.100000000000023,319.3,33.199999999999989,"100389",352.5,32.100000000000023]
["100390",100390,null,"STK","TS120LAS 125/185 Rohr L 250 Inox ","CHF",113.5,"TECHNOSTAR 120 LAS",1.5,250,"J","TS120LAS 125/185 Tuyau L 250 Inox ","TS120LAS 125/185 Rohr L 250 Inox ","TS120LAS 125/185 Tubo L 250 Inox",122,1,"DN 125",null,103.1,"550961",null,null,113.5,"100390",10.400000000000006,102,11.5,"100390",113.5,10.400000000000006]
["100391",100391,null,"STK","TS120LAS 125/185 Rohr L 500 Inox ","CHF",147.4,"TECHNOSTAR 120 LAS",3,500,"J","TS120LAS 125/185 Tuyau L 500 Inox ","TS120LAS 125/185 Rohr L 500 Inox ","TS120LAS 125/185 Tubo L 500 Inox",122,1,"DN 125",null,134,"550962",null,null,147.4,"100391",13.400000000000006,132.9,14.5,"100391",147.4,13.400000000000006]
["100392",100392,null,"STK","TS120LAS 125/185 Rohr L 1000 Inox ","CHF",280,"TECHNOSTAR 120 LAS",3.7,1000,"J","TS120LAS 125/185 Tuyau L1000 Inox ","TS120LAS 125/185 Rohr L 1000 Inox ","TS120LAS 125/185 Tubo L1000 Inox",122,1,"DN 125",null,254.5,"550963",null,null,280,"100392",25.5,253.4,26.599999999999994,"100392",280,25.5]
["100399",100399,null,"STK","TS120LAS 80/125 Aussenwandanschluss komplett Inox","CHF",392.4,"TECHNOSTAR 120 LAS",2.4,0,"J","TS120LAS 80/125 Racc.de paroi extrene compl. Inox","TS120LAS 80/125 Aussenwandanschluss komplett Inox","TS120LAS 80/125 Elemento per pareti esterne",122,1,"DN 80",null,356.7,"550949",null,null,392.4,"100399",35.699999999999989,355.6,36.799999999999955,"100399",392.4,35.699999999999989]
["100400",100400,null,"STK","TS120LAS 110/160 Aussenwandanschluss komplett Inox","CHF",541.9,"TECHNOSTAR 120 LAS",2.4,0,"J","TS120LAS 110/160Racc.de paroi extrene compl. Inox","TS120LAS 110/160 Aussenwandanschluss komplett Inox","TS120LAS 110/160 Elemento per pareti esterne",122,1,"DN 110",null,492.6,"550950",null,null,541.9,"100400",49.299999999999955,491.5,50.399999999999977,"100400",541.9,49.299999999999955]
["100401",100401,null,"STK","TS120LAS 125/185 Aussenwandanschluss komplett Inox","CHF",885,"TECHNOSTAR 120 LAS",2.7,0,"J","TS120LAS 125/185 Racc.de paroi extrene compl. Inox","TS120LAS 125/185 Aussenwandanschluss komplett Inox","TS120LAS 125/185 Elemento per pareti esterne",122,1,"DN 125",null,804.5,"550951",null,null,885,"100401",80.5,803.4,81.600000000000023,"100401",885,80.5]
["100405",100405,null,"STK","TS120LAS 125 Verl. Typ 1 zu Aussenwandanschluss","CHF",171.4,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 125 Ralonges type 1 de racc. paroi  Inox","TS120LAS 125 Verl. Typ 1 zu Aussenwandanschluss","TS120LAS 125 Prolunga per perti esterne Typ1",122,1,"DN 80",null,155.80000000000001,"560970",null,null,171.4,"100405",15.599999999999994,154.69999999999999,16.700000000000017,"100405",171.4,15.599999999999994]
["100406",100406,null,"STK","TS120LAS 125 Verl. Typ 2 zu Aussenwandanschluss","CHF",213.9,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 125 Ralonges type 2 de racc. paroi  Inox","TS120LAS 125 Verl. Typ 2 zu Aussenwandanschluss","TS120LAS 125 Prolunga per perti esterne Typ2",122,1,"DN 80",null,194.4,"560971",null,null,213.9,"100406",19.5,193.3,20.599999999999994,"100406",213.9,19.5]
["100407",100407,null,"STK","TS120LAS 125 Verl. Typ 3 zu Aussenwandanschluss","CHF",256.3,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 125 Ralonges type 3 de racc. paroi  Inox","TS120LAS 125 Verl. Typ 3 zu Aussenwandanschluss","TS120LAS 125 Prolunga per perti esterne Typ3",122,1,"DN 80",null,233,"560972",null,null,256.3,"100407",23.300000000000011,231.9,24.400000000000006,"100407",256.3,23.300000000000011]
["100410",100410,null,"STK","TS120LAS 160 Verl. Typ 3 zu Aussenwandanschluss","CHF",256.3,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 160 Ralonges type 3 de racc. paroi  Inox","TS120LAS 160 Verl. Typ 3 zu Aussenwandanschluss","TS120LAS 160 Prolunga per perti esterne Typ3",122,1,"DN 110",null,233,"560975",null,null,256.3,"100410",23.300000000000011,231.9,24.400000000000006,"100410",256.3,23.300000000000011]
["100411",100411,null,"STK","TS120LAS 185 Verl. Typ 1 zu Aussenwandanschluss","CHF",205.2,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 185 Ralonges type 1 de racc. paroi  Inox","TS120LAS 185 Verl. Typ 1 zu Aussenwandanschluss","TS120LAS 185 Prolunga per perti esterne Typ1",122,1,"DN 125",null,186.5,"560976",null,null,205.2,"100411",18.699999999999989,185.4,19.799999999999983,"100411",205.2,18.699999999999989]
["100412",100412,null,"STK","TS120LAS 185 Verl. Typ 2 zu Aussenwandanschluss","CHF",284,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 185 Ralonges type 2 de racc. paroi  Inox","TS120LAS 185 Verl. Typ 2 zu Aussenwandanschluss","TS120LAS 185 Prolunga per perti esterne Typ1",122,1,"DN 125",null,258.10000000000002,"560977",null,null,284,"100412",25.899999999999977,257,27,"100412",284,25.899999999999977]
["100413",100413,null,"STK","TS120LAS 185 Verl. Typ 3 zu Aussenwandanschluss","CHF",340.9,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 185 Ralonges type 3de racc. paroi  Inox","TS120LAS 185 Verl. Typ 3 zu Aussenwandanschluss","TS120LAS 185 Prolunga per perti esterne Typ1",122,1,"DN 125",null,309.89999999999998,"560978",null,null,340.9,"100413",31,308.8,32.099999999999966,"100413",340.9,31]
["100414",100414,null,"STK","TS120LAS 80/125 Revisionsrohr Inox ","CHF",232.1,"TECHNOSTAR 120 LAS",0.2,0,"J","TS120LAS 80/125 Tuyau de révision Inox","TS120LAS 80/125 Revisionsrohr Inox ","TS120LAS 80/125 Tubo di revisione Inox",122,1,"DN 80",null,211,"500116",null,null,232.1,"100414",21.099999999999994,209.9,22.199999999999989,"100414",232.1,21.099999999999994]
["100415",100415,null,"STK","TS120LAS 110/160 Revisionsrohr Inox ","CHF",277.2,"TECHNOSTAR 120 LAS",1.6,0,"J","TS120LAS 110/160 Tuyau de révision Inox","TS120LAS 110/160 Revisionsrohr Inox ","TS120LAS 110/160 Tubo di revisione Inox",122,1,"DN 110",null,252,"550244",null,null,277.2,"100415",25.199999999999989,250.9,26.299999999999983,"100415",277.2,25.199999999999989]
["100416",100416,null,"STK","TS120LAS 125/185 Revisionsrohr Inox ","CHF",335.5,"TECHNOSTAR 120 LAS",2,0,"J","TS120LAS 125/185 Tuyau de révision Inox","TS120LAS 125/185 Revisionsrohr Inox ","TS120LAS 125/185 Tubo di revisione Inox",122,1,"DN 125",null,305,"550246",null,null,335.5,"100416",30.5,303.89999999999998,31.600000000000023,"100416",335.5,30.5]
["100418",100418,null,"STK","TS120LAS 125 Abdeckblende  Inox","CHF",43.1,"TECHNOSTAR 120 LAS",0.3,0,"J","TS120LAS 125 Cache 200mm x 200mm Inox","TS120LAS 125 Abdeckblende  Inox","TS120LAS 125 Chiusura 225mm x 225mm",122,1,"DN 80",null,39.1,"550812",null,null,43.1,"100418",4,38,5.1000000000000014,"100418",43.1,4]
["100419",100419,null,"STK","TS120LAS 160 Abdeckblende  Inox","CHF",58.8,"TECHNOSTAR 120 LAS",0.3,0,"J","TS120LAS 160 Cache 200mm x 200mm Inox","TS120LAS 160 Abdeckblende  Inox","TS120LAS 160 Chiusura 225mm x 225mm",122,1,"DN 110",null,53.4,"550814",null,null,58.8,"100419",5.3999999999999986,52.3,6.5,"100419",58.8,5.3999999999999986]
["100420",100420,null,"STK","TS120LAS 185 Abdeckblende  Inox","CHF",58.8,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 185 Cache 200mm x 200mm Inox","TS120LAS 185 Abdeckblende  Inox","TS120LAS 185 Chiusura 225mm x 225mm",122,1,"DN 125",null,53.4,"550816",null,null,58.8,"100420",5.3999999999999986,52.3,6.5,"100420",58.8,5.3999999999999986]
["100421",100421,null,"STK","TS120LAS 80/125 Dachdurchführung Inox","CHF",328.4,"TECHNOSTAR 120 LAS",3.8,0,"J","TS120LAS 80/125 Passage de troiture Inox","TS120LAS 80/125 Dachdurchführung Inox","TS120LAS 80/125 Pezzo per attraversare tetto Inox",122,1,"DN 80",null,298.5,"554660",null,null,328.4,"100421",29.899999999999977,297.39999999999998,31,"100421",328.4,29.899999999999977]
["100422",100422,null,"STK","TS120LAS 110/160 Dachdurchführung Inox","CHF",426.4,"TECHNOSTAR 120 LAS",5,0,"J","TS120LAS 110/160 Passage de troiture Inox","TS120LAS 110/160 Dachdurchführung Inox","TS120LAS 110/160 Pezzo per attraversare tetto Inox",122,1,"DN 110",null,387.6,"550460",null,null,426.4,"100422",38.799999999999955,386.5,39.899999999999977,"100422",426.4,38.799999999999955]
["100423",100423,null,"STK","TS120LAS 125/185 Dachdurchführung Inox","CHF",477.1,"TECHNOSTAR 120 LAS",5,0,"J","TS120LAS 125/185 Passage de troiture Inox","TS120LAS 125/185 Dachdurchführung Inox","TS120LAS 125/185 Pezzo per attraversare tetto Inox",122,1,"DN 125",null,433.7,"550463",null,null,477.1,"100423",43.400000000000034,432.6,44.5,"100423",477.1,43.400000000000034]
["100427",100427,null,"STK","TS120LAS 80/125 Bogen 15° Inox","CHF",111.5,"TECHNOSTAR 120 LAS",0.2,129,"J","TS120LAS 80/125 Coude 15° Inox","TS120LAS 80/125 Bogen 15° Inox","TS120LAS 80/125 Curva 15° Inox",122,1,"DN 80",null,101.3,"500111",null,null,111.5,"100427",10.200000000000003,100.2,11.299999999999997,"100427",111.5,10.200000000000003]
["100428",100428,null,"STK","TS120LAS 80/125 Bogen 30° Inox","CHF",111.5,"TECHNOSTAR 120 LAS",0.2,133,"J","TS120LAS 80/125 Coude 30° Inox","TS120LAS 80/125 Bogen 30° Inox","TS120LAS 80/125 Curva 30° Inox",122,1,"DN 80",null,101.3,"500112",null,null,111.5,"100428",10.200000000000003,100.2,11.299999999999997,"100428",111.5,10.200000000000003]
["100429",100429,null,"STK","TS120LAS 80/125 Bogen 45° Inox","CHF",111.5,"TECHNOSTAR 120 LAS",0.2,147,"J","TS120LAS 80/125 Coude 45° Inox","TS120LAS 80/125 Bogen 45° Inox","TS120LAS 80/125 Curva 45° Inox",122,1,"DN 80",null,101.3,"500113",null,null,111.5,"100429",10.200000000000003,100.2,11.299999999999997,"100429",111.5,10.200000000000003]
["100430",100430,null,"STK","TS120LAS 80/125 Bogen 87° Inox","CHF",140.1,"TECHNOSTAR 120 LAS",0.2,126,"J","TS120LAS 80/125 Coude 87° Inox","TS120LAS 80/125 Bogen 87° Inox","TS120LAS 80/125 Curva 87° Inox",122,1,"DN 80",null,127.3,"500114",null,null,140.1,"100430",12.799999999999997,126.2,13.899999999999991,"100430",140.1,12.799999999999997]
["100431",100431,null,"STK","TS120LAS 110/160 Bogen 15° Inox","CHF",161.19999999999999,"TECHNOSTAR 120 LAS",1,142,"J","TS120LAS 110/160 Coude 15° Inox","TS120LAS 110/160 Bogen 15° Inox","TS120LAS 110/160 Curva 15° Inox",122,1,"DN 110",null,146.5,"550340",null,null,161.19999999999999,"100431",14.699999999999989,145.4,15.799999999999983,"100431",161.19999999999999,14.699999999999989]
["100432",100432,null,"STK","TS120LAS 110/160 Bogen 30° Inox","CHF",161.19999999999999,"TECHNOSTAR 120 LAS",1,148,"J","TS120LAS 110/160 Coude 30° Inox","TS120LAS 110/160 Bogen 30° Inox","TS120LAS 110/160 Curva 30° Inox",122,1,"DN 110",null,146.5,"550344",null,null,161.19999999999999,"100432",14.699999999999989,145.4,15.799999999999983,"100432",161.19999999999999,14.699999999999989]
[{"$f":"B524&\"\"","v":"100433"},100433,null,"STK",{"$f":"IF($E$200=2,L524,IF($E$200=3,N524,M524))","v":"TS120LAS 110/160 Bogen 45° Inox"},"CHF",{"$f":"IF($L$190=1,W524,S524)","v":173.7},"TECHNOSTAR 120 LAS",1,148,"J","TS120LAS 110/160 Coude 45° Inox","TS120LAS 110/160 Bogen 45° Inox","TS120LAS 110/160 Curva 45° Inox",122,1,"DN 110",null,157.9,"550348",null,null,173.7,"100433",15.799999999999983,156.80000000000001,16.899999999999977,"100433",173.7,15.799999999999983]
["100434",100434,null,"STK","TS120LAS 110/160 Bogen 87° Inox","CHF",207.3,"TECHNOSTAR 120 LAS",1,170,"J","TS120LAS 110/160 Coude 87° Inox","TS120LAS 110/160 Bogen 87° Inox","TS120LAS 110/160 Curva 87° Inox",122,1,"DN 110",null,188.4,"550352",null,null,207.3,"100434",18.900000000000006,187.3,20,"100434",207.3,18.900000000000006]
["100435",100435,null,"STK","TS120LAS 125/185 Bogen 15° Inox","CHF",216.5,"TECHNOSTAR 120 LAS",1.2,155,"J","TS120LAS 125/185 Coude 15° Inox","TS120LAS 125/185 Bogen 15° Inox","TS120LAS 125/185 Curva 15° Inox",122,1,"DN 125",null,196.8,"550360",null,null,216.5,"100435",19.699999999999989,195.7,20.800000000000011,"100435",216.5,19.699999999999989]
["100436",100436,null,"STK","TS120LAS 125/185 Bogen 30° Inox","CHF",216.5,"TECHNOSTAR 120 LAS",2,186,"J","TS120LAS 125/185 Coude 30° Inox","TS120LAS 125/185 Bogen 30° Inox","TS120LAS 125/185 Curva 30° Inox",122,1,"DN 125",null,196.8,"550362",null,null,216.5,"100436",19.699999999999989,195.7,20.800000000000011,"100436",216.5,19.699999999999989]
["100437",100437,null,"STK","TS120LAS 125/185 Bogen 45° Inox","CHF",239.2,"TECHNOSTAR 120 LAS",3.2,188,"J","TS120LAS 110/160 Coude 45° Inox","TS120LAS 125/185 Bogen 45° Inox","TS120LAS 110/160 Curva 45° Inox",122,1,"DN 125",null,217.4,"550364",null,null,239.2,"100437",21.799999999999983,216.3,22.899999999999977,"100437",239.2,21.799999999999983]
["100438",100438,null,"STK","TS120LAS 125/185 Bogen 87° Inox","CHF",261.8,"TECHNOSTAR 120 LAS",6.4,189,"J","TS120LAS 110/160 Coude 87° Inox","TS120LAS 125/185 Bogen 87° Inox","TS120LAS 110/160 Curva 87° Inox",122,1,"DN 125",null,238,"550366",null,null,261.8,"100438",23.800000000000011,236.9,24.900000000000006,"100438",261.8,23.800000000000011]
["100439",100439,null,"STK","TS120LAS 80/125 Zuluftstutzen Inox","CHF",234,"TECHNOSTAR 120 LAS",1.2,0,"J","TS120LAS 80/125 Manchon prise d'air Inox","TS120LAS 80/125 Zuluftstutzen Inox","TS120LAS 80/125 Presa d'aria Inox",122,1,"DN 80",null,212.7,"554664",null,null,234,"100439",21.300000000000011,211.6,22.400000000000006,"100439",234,21.300000000000011]
["100440",100440,null,"STK","TS120LAS 110/160 Zuluftstutzen Inox","CHF",246.9,"TECHNOSTAR 120 LAS",15,0,"J","TS120LAS 110/160 Manchon prise d'air Inox","TS120LAS 110/160 Zuluftstutzen Inox","TS120LAS 110/160 Presa d'aria Inox",122,1,"DN 110",null,224.4,"552206",null,null,246.9,"100440",22.5,223.3,23.599999999999994,"100440",246.9,22.5]
["100441",100441,null,"STK","TS120LAS 125/185 Zuluftstutzen Inox","CHF",358.2,"TECHNOSTAR 120 LAS",18,0,"J","TS120LAS 125/185 Manchon prise d'air Inox","TS120LAS 125/185 Zuluftstutzen Inox","TS120LAS 125/185 Presa d'aria Inox",122,1,"DN 125",null,325.60000000000002,"552207",null,null,358.2,"100441",32.599999999999966,324.5,33.699999999999989,"100441",358.2,32.599999999999966]
["100442",100442,null,"STK","TS120LAS 125 Klemmband Inox","CHF",57.8,"TECHNOSTAR 120 LAS",0.1,0,"J","TS120LAS 125 Collier de serrage Inox","TS120LAS 125 Klemmband Inox","TS120LAS 125 Colare Inox",122,1,"DN 80",null,52.5,"553280",null,null,57.8,"100442",5.2999999999999972,51.4,6.3999999999999986,"100442",57.8,5.2999999999999972]
["100443",100443,null,"STK","TS120LAS 160 Klemmband Inox","CHF",75.3,"TECHNOSTAR 120 LAS",0.2,0,"J","TS120LAS 160 Collier de serrage Inox","TS120LAS 160 Klemmband Inox","TS120LAS 160 Colare Inox",122,1,"DN 110",null,68.400000000000006,"553285",null,null,75.3,"100443",6.8999999999999915,67.3,8,"100443",75.3,6.8999999999999915]
["100445",100445,null,"STK","TS120LAS 80/125 Mündungsabschluss mit Klemmband","CHF",123.7,"TECHNOSTAR 120 LAS",1,145,"J","TS120LAS 80/125 Finition d'embouchure Inox","TS120LAS 80/125 Mündungsabschluss mit Klemmband","TS120LAS 80/125 Termiale con fascetta Inox",122,1,"DN 80",null,112.4,"550969",null,null,123.7,"100445",11.299999999999997,111.3,12.400000000000006,"100445",123.7,11.299999999999997]
["100446",100446,null,"STK","TS120LAS 110/160 Mündungsabschluss mit Klemmband","CHF",136.69999999999999,"TECHNOSTAR 120 LAS",1.2,145,"J","TS120LAS 110/160 Finition d'embouchure Inox","TS120LAS 110/160 Mündungsabschluss mit Klemmband","TS120LAS 110/160 Termiale con fascetta Inox",122,1,"DN 110",null,124.2,"550970",null,null,136.69999999999999,"100446",12.499999999999986,123.1,13.599999999999994,"100446",136.69999999999999,12.499999999999986]
["100447",100447,null,"STK","TS120LAS 125/185 Mündungsabschluss mit Klemmband","CHF",235.9,"TECHNOSTAR 120 LAS",1.4,145,"J","TS120LAS 125/185 Finition d'embouchure Inox","TS120LAS 125/185 Mündungsabschluss mit Klemmband","TS120LAS 125/185 Termiale con fascetta Inox",122,1,"DN 125",null,214.4,"550971",null,null,235.9,"100447",21.5,213.3,22.599999999999994,"100447",235.9,21.5]
["100451",100451,null,"STK","TS120LAS 80 Mündungsrohr Inox","CHF",55.3,"TECHNOSTAR 120 LAS",0.2,250,"J","TS120LAS 80 Tube de finition Inox","TS120LAS 80 Mündungsrohr Inox","TS120LAS 80 Tubo finale Inox",122,1,"DN 80",null,50.2,"553270",null,null,55.3,"100451",5.0999999999999943,49.1,6.1999999999999957,"100451",55.3,5.0999999999999943]
["100452",100452,null,"STK","TS120LAS 110 Mündungsrohr Inox","CHF",62.5,"TECHNOSTAR 120 LAS",0.4,250,"J","TS120LAS 110 Tube de finition Inox","TS120LAS 110 Mündungsrohr Inox","TS120LAS 110 Tubo finale Inox",122,1,"DN110",null,56.8,"553275",null,null,62.5,"100452",5.7000000000000028,55.7,6.7999999999999972,"100452",62.5,5.7000000000000028]
["100453",100453,null,"STK","TS120LAS 125 Mündungsrohr Inox","CHF",69.099999999999994,"TECHNOSTAR 120",0.4,250,"J","TS120LAS 125 Tube de finition Inox","TS120LAS 125 Mündungsrohr Inox","TS120LAS 125 Tubo finale Inox",121,1,"DN 125",null,62.8,0,null,null,69.099999999999994,"100453",6.2999999999999972,61.7,7.3999999999999915,"100453",69.099999999999994,6.2999999999999972]
["100454",100454,null,"STK","TS120LAS 125 Wandhalterung Inox","CHF",79.099999999999994,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 125 Fixation murale Inox","TS120LAS 125 Wandhalterung Inox","TS120LAS 125 Collare al muro Inox",122,1,"DN 80",null,71.900000000000006,"554626",null,null,79.099999999999994,"100454",7.1999999999999886,70.8,8.2999999999999972,"100454",79.099999999999994,7.1999999999999886]
["100455",100455,null,"STK","TS120LAS 125 Verlängerung Typ 1 zu Wandhalterung ","CHF",86.4,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 125 Prolongation type 1 de Fixation Inox","TS120LAS 125 Verlängerung Typ 1 zu Wandhalterung ","TS120LAS 125 Prolunga per Collare muro Typ1 Inox",122,1,"DN 80",null,78.5,"560980",null,null,86.4,"100455",7.9000000000000057,77.400000000000006,9,"100455",86.4,7.9000000000000057]
["100456",100456,null,"STK","TS120LAS 125 Verlängerung Typ 2 zu Wandhalterung ","CHF",128.9,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 125 Prolongation type 2 de Fixation Inox","TS120LAS 125 Verlängerung Typ 2 zu Wandhalterung ","TS120LAS 125 Prolunga per Collare muro Typ2 Inox",122,1,"DN 80",null,117.1,"560982",null,null,128.9,"100456",11.800000000000011,116,12.900000000000006,"100456",128.9,11.800000000000011]
["100457",100457,null,"STK","TS120LAS 125 Verlängerung Typ 3 zu Wandhalterung ","CHF",171.4,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 125 Prolongation type 3 de Fixation Inox","TS120LAS 125 Verlängerung Typ 3 zu Wandhalterung ","TS120LAS 125 Prolunga per Collare muro Typ3 Inox",122,1,"DN 80",null,155.80000000000001,"560985",null,null,171.4,"100457",15.599999999999994,154.69999999999999,16.700000000000017,"100457",171.4,15.599999999999994]
["100458",100458,null,"STK","TS120LAS 160 Wandhalterung Inox","CHF",87.5,"TECHNOSTAR 120 LAS",0.5,0,"J","TS120LAS 160 Fixation murale Inox","TS120LAS 160 Wandhalterung Inox","TS120LAS 160 Collare al muro Inox",122,1,"DN 110",null,79.5,"550484",null,null,87.5,"100458",8,78.400000000000006,9.0999999999999943,"100458",87.5,8]
["100459",100459,null,"STK","TS120LAS 160 Verlängerung Typ 1 zu Wandhalterung ","CHF",103.4,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 160 Prolongation type 1 de Fixation Inox","TS120LAS 160 Verlängerung Typ 1 zu Wandhalterung ","TS120LAS 160 Prolunga per Collare muro Typ1 Inox",122,1,"DN 110",null,94,"560990",null,null,103.4,"100459",9.4000000000000057,92.9,10.5,"100459",103.4,9.4000000000000057]
["100460",100460,null,"STK","TS120LAS 160 Verlängerung Typ 2 zu Wandhalterung ","CHF",145.9,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 160 Prolongation type 2 de Fixation Inox","TS120LAS 160 Verlängerung Typ 2 zu Wandhalterung ","TS120LAS 160 Prolunga per Collare muro Typ2 Inox",122,1,"DN 110",null,132.6,"560994",null,null,145.9,"100460",13.300000000000011,131.5,14.400000000000006,"100460",145.9,13.300000000000011]
["100461",100461,null,"STK","TS120LAS 160 Verlängerung Typ 3 zu Wandhalterung ","CHF",188.4,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 160 Prolongation type 3 de Fixation Inox","TS120LAS 160 Verlängerung Typ 3 zu Wandhalterung ","TS120LAS 160 Prolunga per Collare muro Typ3 Inox",122,1,"DN 110",null,171.2,"560996",null,null,188.4,"100461",17.200000000000017,170.1,18.300000000000011,"100461",188.4,17.200000000000017]
["100466",100466,null,"STK","TS120LAS 60/100  Wandurchführung L500mm","CHF",85.2,"TECHNOSTAR 120",1.5,0,"J","TS120LAS 60/100 Passage de paroi L500mm","TS120LAS 60/100  Wandurchführung L500mm","TS120LAS 60/100 Pezzo attraversato de pareti",121,1,"DN 60",null,77.400000000000006,"515017",null,null,85.2,"100466",7.7999999999999972,76.3,8.9000000000000057,"100466",85.2,7.7999999999999972]
["100467",100467,null,"STK","TS120LAS 80/125  Wandurchführung L500mm","CHF",52.4,"TECHNOSTAR 120 LAS",1.7,0,"J","TS120LAS 80/125 Passage de paroi L500mm","TS120LAS 80/125  Wandurchführung L500mm","TS120LAS 80/125 Pezzo attraversato de pareti",122,1,"DN 80",null,47.6,"555500",null,null,52.4,"100467",4.7999999999999972,46.5,5.8999999999999986,"100467",52.4,4.7999999999999972]
["100468",100468,null,"STK","TS120LAS 110/160 Wandurchführung L500mm","CHF",84.6,"TECHNOSTAR 120 LAS",1.5,0,"J","TS120LAS 110/160 Passage de paroi L500mm","TS120LAS 110/160 Wandurchführung L500mm","TS120LAS 110/160 Pezzo attraversato de pareti",122,1,"DN 110",null,76.900000000000006,"550977",null,null,84.6,"100468",7.6999999999999886,75.8,8.7999999999999972,"100468",84.6,7.6999999999999886]
["100469",100469,null,"STK","TS120LAS 125/185 Wandurchführung L500mm","CHF",170.5,"TECHNOSTAR 120 LAS",1.75,0,"J","TS120LAS 125/185 Passage de paroi L500mm","TS120LAS 125/185 Wandurchführung L500mm","TS120LAS 125/185 Pezzo attraversato de pareti",122,1,"DN 125",null,155,"550978",null,null,170.5,"100469",15.5,133.4,37.099999999999994,"100469",170.5,15.5]
["100476",100476,null,"STK","TS120LAS 60/100  Dachdurchführ. L400mm ü Dach sw","CHF",203.7,"TECHNOSTAR 120 LAS",0.5,0,"J","TS120LAS 60/100 Passage de Troiture PE noir L400 ","TS120LAS 60/100  Dachdurchführ. L400mm ü Dach sw","TS120LAS 60/100 Pz. Attraversare tetto nero L400 ",122,1,"DN 60",null,185.1,"515018",null,null,203.7,"100476",18.599999999999994,184,19.699999999999989,"100476",203.7,18.599999999999994]
["100477",100477,null,"STK","TS120LAS 80/125 Dachdurchführ. L400mm ü Dach sw","CHF",217,"TECHNOSTAR 120",2.4900000000000002,0,"J","TS120LAS 80/125 Passage de Troiture PE noir L400 ","TS120LAS 80/125 Dachdurchführ. L400mm ü Dach sw","TS120LAS 80/125 Pz. Attraversare tetto nero L400 ",121,1,"DN 80",null,197.2,"511092",null,null,217,"100477",19.800000000000011,196.1,20.900000000000006,"100477",217,19.800000000000011]
["100479",100479,null,"STK","TS120LAS 80/125 Dachdurchführ. L1000mm ü Dach sw","CHF",236.1,"TECHNOSTAR 120",2.4900000000000002,0,"J","TS120LAS 80/125 Passage de Troiture PE noir L1000","TS120LAS 80/125 Dachdurchführ. L1000mm ü Dach sw","TS120LAS 80/125 Pz. Attraversare tetto nero L1000",121,1,"DN 80",null,214.6,"511053",null,null,236.1,"100479",21.5,213.5,22.599999999999994,"100479",236.1,21.5]
["100481",100481,null,"STK","TS120LAS 110/160 Dachdurchführ. L1000mm ü Dach sw","CHF",427.3,"TECHNOSTAR 120",1.5,0,"J","TS120LAS 110/160 Passage de Troit. PE noir L1000 ","TS120LAS 110/160 Dachdurchführ. L1000mm ü Dach sw","TS120LAS 110/160 Attraversare tetto nero L1000 ",121,1,"DN 110",null,388.4,"511081",null,null,427.3,"100481",38.900000000000034,387.3,40,"100481",427.3,38.900000000000034]
["100484",100484,null,"STK","TS120LAS 160/185 Dachdurchführ. L1000mm schwarz","CHF",624.4,"TECHNOSTAR 120 LAS",4.9000000000000004,0,"J","TS120LAS 160/185 Passage de Troit. PE noir L1000 ","TS120LAS 160/185 Dachdurchführ. L1000mm schwarz","TS120LAS 160/185 Attraversare tetto nero L1000 ",122,1,"DN 160",null,567.6,"550942",null,null,624.4,"100484",56.799999999999955,566.5,57.899999999999977,"100484",624.4,56.799999999999955]
["100488",100488,null,"STK","TS120 80 Zentrierhalter Typ 100","CHF",53.9,"TECHNOSTAR 120",0.1,0,"J","TS120 80 Collier de centrage Type 100","TS120 80 Zentrierhalter Typ 100","TS120 80 Distanzatori typ 100 Inox",121,1,"DN 80",null,49,"559902",null,null,53.9,"100488",4.8999999999999986,49,4.8999999999999986,"100488",53.9,4.8999999999999986]
["100489",100489,null,"STK","TS120 80 Zentrierhalter Typ 65","CHF",51.3,"TECHNOSTAR 120",0.1,0,"J","TS120 80 Collier de centrage Type  65","TS120 80 Zentrierhalter Typ 65","TS120 80 Distanzatori typ 65 Inox",121,1,"DN 80",null,46.6,"559901",null,null,51.3,"100489",4.6999999999999957,46.6,4.6999999999999957,"100489",51.3,4.6999999999999957]
["100490",100490,null,"STK","TS120 110 Zentrierhalter Typ 100","CHF",55.5,"TECHNOSTAR 120",0.09,0,"J","TS120 110 Collier de centrage Type 100","TS120 110 Zentrierhalter Typ 100","TS120 110 Distanzatori typ 100 Inox",121,1,"DN 110",null,50.4,"513013",null,null,55.5,"100490",5.1000000000000014,50.4,5.1000000000000014,"100490",55.5,5.1000000000000014]
["100491",100491,null,"STK","TS120 110 Zentrierhalter Typ 65","CHF",53.8,"TECHNOSTAR 120",0.05,0,"J","TS120 110 Collier de centrage Type  65","TS120 110 Zentrierhalter Typ 65","TS120 110 Distanzatori typ 65 Inox",121,1,"DN 110",null,48.9,"513012",null,null,53.8,"100491",4.8999999999999986,48.9,4.8999999999999986,"100491",53.8,4.8999999999999986]
["100492",100492,null,"STK","TS120 125 Zentrierhalter Typ 100","CHF",56.1,"TECHNOSTAR 120",0.09,0,"J","TS120 125 Collier de centrage Type 100","TS120 125 Zentrierhalter Typ 100","TS120 125 Distanzatori typ 100 Inox",121,1,"DN 125",null,51,"513015",null,null,56.1,"100492",5.1000000000000014,51,5.1000000000000014,"100492",56.1,5.1000000000000014]
["100493",100493,null,"STK","TS120 125 Zentrierhalter Typ 65","CHF",54.6,"TECHNOSTAR 120",0.05,0,"J","TS120 125 Collier de centrage Type  65","TS120 125 Zentrierhalter Typ 65","TS120 125 Distanzatori typ 65 Inox",121,1,"DN 125",null,49.6,"513014",null,null,54.6,"100493",5,49.6,5,"100493",54.6,5]
["100494",100494,null,"STK","TS120 160 Zentrierhalter Typ 100","CHF",58.8,"TECHNOSTAR 120",0.09,0,"J","TS120 160 Collier de centrage Type 100","TS120 160 Zentrierhalter Typ 100","TS120 160 Distanzatori typ 100 Inox",121,1,"DN 160",null,53.4,"513017",null,null,58.8,"100494",5.3999999999999986,53.4,5.3999999999999986,"100494",58.8,5.3999999999999986]
["100495",100495,null,"STK","TS120 160 Zentrierhalter Typ 65","CHF",57.2,"TECHNOSTAR 120",0.05,0,"J","TS120 160 Collier de centrage Type  65","TS120 160 Zentrierhalter Typ 65","TS120 160 Distanzatori typ 65 Inox",121,1,"DN 160",null,52,"513016",null,null,57.2,"100495",5.2000000000000028,52,5.2000000000000028,"100495",57.2,5.2000000000000028]
["100517",100517,null,"STK","TS120 110 Flanschverbindung komplett","CHF",169.1,"TECHNOSTAR 120",0.45,0,"J","TS120 110 Raccordement à bride ","TS120 110 Flanschverbindung komplett","TS120 110 Manicotto flangiato ",121,1,"DN 110",null,153.69999999999999,"500054",null,null,169.1,"100517",15.400000000000006,153.69999999999999,15.400000000000006,"100517",169.1,15.400000000000006]
["100518",100518,null,"STK","TS120 125 Flanschverbindung komplett","CHF",189.7,"TECHNOSTAR 120",0.55000000000000004,0,"J","TS120 125 Raccordement à bride ","TS120 125 Flanschverbindung komplett","TS120 125 Manicotto flangiato ",121,1,"DN 125",null,172.4,"500055",null,null,189.7,"100518",17.299999999999983,172.4,17.299999999999983,"100518",189.7,17.299999999999983]
["100519",100519,null,"STK","TS120 160 Flanschverbindung komplett","CHF",226,"TECHNOSTAR 120",0.8,0,"J","TS120 160 Raccordement à bride ","TS120 160 Flanschverbindung komplett","TS120 160 Manicotto flangiato ",121,1,"DN 160",null,205.4,"500056",null,null,226,"100519",20.599999999999994,205.4,20.599999999999994,"100519",226,20.599999999999994]
["100532",100532,null,"STK","TS120 Rohrfaltmanchette 150-177mm","CHF",71.5,"TECHNOSTAR 120",0.5,0,"J","TS 120 Tubo di pieghe 150-177 mm","TS120 Rohrfaltmanchette 150-177mm","TS 120 se replie tube de 150-177 mm",121,1,"DN 80",null,65,"511077",null,null,71.5,"100532",6.5,63.9,7.6000000000000014,"100532",71.5,6.5]
["100578",100578,null,"STK","PPL 80 Kaminfuss 45° m.Stütze L195mm","CHF",164,"Schiedel PRIMA PLUS",0.9,0,"J","PPL 80 Pied de Cheminée 45° L 195mm","PPL 80 Kaminfuss 45° m.Stütze L195mm","PPL 80 Piede di camino 45° L 195mm",131,1,"DN 80",null,141.9,"137034708",null,null,164,"100578",22.099999999999994,129,35,"100578",164,22.099999999999994]
["100579",100579,null,"STK","PPL 100 Kaminfuss 45° m.Stütze L200mm","CHF",179,"Schiedel PRIMA PLUS",1,0,"J","PPL 100 Pied de Cheminée 45° L200mm","PPL 100 Kaminfuss 45° m.Stütze L200mm","PPL 100 Piede di camino 45° L200mm",131,1,"DN 100",null,155.1,"137034710",null,null,179,"100579",23.900000000000006,141,38,"100579",179,23.900000000000006]
["100580",100580,null,"STK","PPL 130 Kaminfuss 45° m.Stütze L205mm","CHF",192,"Schiedel PRIMA PLUS",1.2,0,"J","PPL 130 Pied de Cheminée 45° L 205mm","PPL 130 Kaminfuss 45° m.Stütze L205mm","PPL 130 Piede di camino 45° L 205mm",131,1,"DN 130",null,166.1,"137034713",null,null,192,"100580",25.900000000000006,151,41,"100580",192,25.900000000000006]
["100581",100581,null,"STK","PPL 150 Kaminfuss 45° m.Stütze L210mm ","CHF",205,"Schiedel PRIMA PLUS",1.5,0,"J","PPL 150 Pied de Cheminée 45° L 210mm ","PPL 150 Kaminfuss 45° m.Stütze L210mm ","PPL 150 Piede di camino 45° L 210mm ",131,1,"DN 150",null,178.2,"137034715",null,null,205,"100581",26.800000000000011,162,43,"100581",205,26.800000000000011]
["100582",100582,null,"STK","PPL 180 Kaminfuss 45° m.Stütze L215mm ","CHF",219,"Schiedel PRIMA PLUS",1.6,0,"J","PPL 180 Pied de Cheminée 45° L 215mm ","PPL 180 Kaminfuss 45° m.Stütze L215mm ","PPL 180 Piede di camino 45° L 215mm ",131,1,"DN 180",null,190.3,"137034718",null,null,219,"100582",28.699999999999989,173,46,"100582",219,28.699999999999989]
["100583",100583,null,"STK","PPL 200 Kaminfuss 45° m.Stütze L220mm","CHF",233,"Schiedel PRIMA PLUS",2,0,"J","PPL 200 Pied de Cheminée 45° L 220mm","PPL 200 Kaminfuss 45° m.Stütze L220mm","PPL 200 Piede di camino 45° L 220mm",131,1,"DN 200",null,202.4,"137034720",null,null,233,"100583",30.599999999999994,184,49,"100583",233,30.599999999999994]
["100584",100584,null,"STK","PPL 250 Kaminfuss 45° m.Stütze L230mm","CHF",260,"Schiedel PRIMA PLUS",2.4,0,"J","PPL 250 Pied de Cheminée 45° L 230mm","PPL 250 Kaminfuss 45° m.Stütze L230mm","PPL 250 Piede di camino 45° L 230mm",131,1,"DN 250",null,225.5,"137034725",null,null,260,"100584",34.5,205,55,"100584",260,34.5]
["100585",100585,null,"STK","PPL 300 Kaminfuss 45° m.Stütze L240mm","CHF",288,"Schiedel PRIMA PLUS",2.8,0,"J","PPL 300 Pied de Cheminée 45° L 240mm","PPL 300 Kaminfuss 45° m.Stütze L240mm","PPL 300 Piede di camino 45° L 240mm",131,1,"DN 300",null,249.7,"137034730",null,null,288,"100585",38.300000000000011,227,61,"100585",288,38.300000000000011]
["100586",100586,null,"STK","PPL 80 Lang-Bogen 45° L205mm","CHF",97,"Schiedel PRIMA PLUS",0.4,0,"J","PPL 80 Coude alonge 45° L 205mm","PPL 80 Lang-Bogen 45° L205mm","PPL 80 Curva lunga  45° L 205mm",131,1,"DN 80",null,83.6,"137034608",null,null,97,"100586",13.400000000000006,76,21,"100586",97,13.400000000000006]
["100587",100587,null,"STK","PPL 100 Lang-Bogen 45° L201mm","CHF",109,"Schiedel PRIMA PLUS",0.5,0,"J","PPL 100 Coude alonge 45° L 201mm","PPL 100 Lang-Bogen 45° L201mm","PPL 100 Curva lunga  45° L 201mm",131,1,"DN 100",null,94.6,"137034610",null,null,109,"100587",14.400000000000006,86,23,"100587",109,14.400000000000006]
["100588",100588,null,"STK","PPL 130 Lang-Bogen 45°  L215mm","CHF",123,"Schiedel PRIMA PLUS",0.62,0,"J","PPL 130 Coude alonge 45° L 215mm","PPL 130 Lang-Bogen 45°  L215mm","PPL 130 Curva lunga  45° L 215mm",131,1,"DN 130",null,106.7,"137034613",null,null,123,"100588",16.299999999999997,97,26,"100588",123,16.299999999999997]
["100589",100589,null,"STK","PPL 150 Lang-Bogen 45° L220mm","CHF",137,"Schiedel PRIMA PLUS",0.7,0,"J","PPL 150 Coude alonge 45° L 220mm","PPL 150 Lang-Bogen 45° L220mm","PPL 150 Curva lunga  45° L 220mm",131,1,"DN 150",null,118.8,"137034615",null,null,137,"100589",18.200000000000003,108,29,"100589",137,18.200000000000003]
["100590",100590,null,"STK","PPL 180 Lang-Bogen 45° L225mm","CHF",151,"Schiedel PRIMA PLUS",0.8,0,"J","PPL 180 Coude alonge 45° L 225mm","PPL 180 Lang-Bogen 45° L225mm","PPL 180 Curva lunga  45° L 225mm",131,1,"DN 180",null,130.9,"137034618",null,null,151,"100590",20.099999999999994,119,32,"100590",151,20.099999999999994]
["100591",100591,null,"STK","PPL 200 Lang-Bogen 45° L230mm","CHF",171,"Schiedel PRIMA PLUS",1,0,"J","PPL 200 Coude alonge 45° L 230mm","PPL 200 Lang-Bogen 45° L230mm","PPL 200 Curva lunga  45° L 230mm",131,1,"DN 200",null,148.5,"137034620",null,null,171,"100591",22.5,135,36,"100591",171,22.5]
["100592",100592,null,"STK","PPL 250 Lang-Bogen 45° L240mm","CHF",192,"Schiedel PRIMA PLUS",1.1000000000000001,0,"J","PPL 250 Coude alonge 45° L 240mm","PPL 250 Lang-Bogen 45° L240mm","PPL 250 Curva lunga  45° L 240mm",131,1,"DN 250",null,166.1,"137034625",null,null,192,"100592",25.900000000000006,151,41,"100592",192,25.900000000000006]
["100593",100593,null,"STK","PPL 300 Lang-Bogen 45° L250mm","CHF",219,"Schiedel PRIMA PLUS",1.32,0,"J","PPL 300 Coude alonge 45° L250mm","PPL 300 Lang-Bogen 45° L250mm","PPL 300 Curva lunga  45° L250mm",131,1,"DN 300",null,190.3,"137034630",null,null,219,"100593",28.699999999999989,173,46,"100593",219,28.699999999999989]
["100594",100594,null,"STK","PPL 80 Kondensattopf mit Ablauf seitlich","CHF",69,"Schiedel PRIMA PLUS",0.21,70,"J","PPL 80 Pot de condensat latéral","PPL 80 Kondensattopf mit Ablauf seitlich","PPL 80 Bancinella per condensa laterale ",131,1,"DN 80",null,59.4,"265800008","106580","4037494146323",69,"100594",9.6000000000000014,54,15,"100594",69,9.6000000000000014]
["100595",100595,null,"STK","PPL 100 Kondensattopf mit Ablauf seitlich","CHF",75,"Schiedel PRIMA PLUS",0.21,70,"J","PPL 100 Pot de condensat latéral","PPL 100 Kondensattopf mit Ablauf seitlich","PPL 100 Bancinella per condensa laterale ",131,1,"DN 100",null,64.900000000000006,"265800010","106581","4037494146330",75,"100595",10.099999999999994,59,16,"100595",75,10.099999999999994]
[{"$f":"B588&\"\"","v":"100596"},100596,null,"STK",{"$f":"IF($E$200=2,L588,IF($E$200=3,N588,M588))","v":"PPL 130 Kondensattopf mit Ablauf seitlich"},"CHF",{"$f":"IF($L$190=1,W588,S588)","v":81},"Schiedel PRIMA PLUS",0.3,70,"J","PPL 130 Pot de condensat latéral","PPL 130 Kondensattopf mit Ablauf seitlich","PPL 130 Bancinella per condensa laterale ",131,1,"DN 130",null,70.400000000000006,"265800013","106584","4037494146354",81,"100596",10.599999999999994,64,17,"100596",81,10.599999999999994]
["100597",100597,null,"STK","PPL 150 Kondensattopf mit Ablauf seitlich","CHF",90,"Schiedel PRIMA PLUS",0.33,70,"J","PPL 150 Pot de condensat latéral","PPL 150 Kondensattopf mit Ablauf seitlich","PPL 150 Bancinella per condensa laterale ",131,1,"DN 150",null,78.099999999999994,"265800015","106586","4037494146361",90,"100597",11.900000000000006,71,19,"100597",90,11.900000000000006]
["100598",100598,null,"STK","PPL 180 Kondensattopf mit Ablauf seitlich","CHF",97,"Schiedel PRIMA PLUS",0.45,70,"J","PPL 180 Pot de condensat latéral","PPL 180 Kondensattopf mit Ablauf seitlich","PPL 180 Bancinella per condensa laterale ",131,1,"DN 180",null,83.6,"265800018","106588","4037494146378",97,"100598",13.400000000000006,76,21,"100598",97,13.400000000000006]
["100599",100599,null,"STK","PPL 200 Kondensattopf mit Ablauf seitlich","CHF",109,"Schiedel PRIMA PLUS",0.51,70,"J","PPL 200 Pot de condensat latéral","PPL 200 Kondensattopf mit Ablauf seitlich","PPL 200 Bancinella per condensa laterale ",131,1,"DN 200",null,94.6,"265800020","106589","4037494146385",109,"100599",14.400000000000006,86,23,"100599",109,14.400000000000006]
["100600",100600,null,"STK","PPL 250 Kondensattopf mit Ablauf seitlich","CHF",137,"Schiedel PRIMA PLUS",0.62,70,"J","PPL 250 Pot de condensat latéral","PPL 250 Kondensattopf mit Ablauf seitlich","PPL 250 Bancinella per condensa laterale ",131,1,"DN 250",null,118.8,"265800025","106591","4037494146408",137,"100600",18.200000000000003,108,29,"100600",137,18.200000000000003]
["100601",100601,null,"STK","PPL 300 Kondensattopf mit Ablauf seitlich","CHF",179,"Schiedel PRIMA PLUS",0.71,70,"J","PPL 300 Pot de condensat latéral","PPL 300 Kondensattopf mit Ablauf seitlich","PPL 300 Bancinella per condensa laterale ",131,1,"DN 300",null,155.1,"265800030","106592","4037494146415",179,"100601",23.900000000000006,141,38,"100601",179,23.900000000000006]
["100602",100602,null,"STK","PPL 350 Kondensattopf mit Ablauf seitlich","CHF",205,"Schiedel PRIMA PLUS",0.89,70,"J","PPL 350 Pot de condensat latéral","PPL 350 Kondensattopf mit Ablauf seitlich","PPL 350 Bancinella per condensa laterale ",131,1,"DN 350",null,178.2,"265810035",null,null,205,"100602",26.800000000000011,162,43,"100602",205,26.800000000000011]
["100603",100603,null,"STK","PPL 400 Kondensattopf mit Ablauf seitlich","CHF",342,"Schiedel PRIMA PLUS",1.9,70,"J","PPL 400 Pot de condensat latéral","PPL 400 Kondensattopf mit Ablauf seitlich","PPL 400 Bancinella per condensa laterale ",131,1,"DN 400",null,297,"265810040","106875","4037494189801",342,"100603",45,270,72,"100603",342,45]
["100604",100604,null,"STK","PPL 450 Kondensattopf mit Ablauf seitlich","CHF",410,"Schiedel PRIMA PLUS",2.0499999999999998,70,"J","PPL 450 Pot de condensat latéral","PPL 450 Kondensattopf mit Ablauf seitlich","PPL 450 Bancinella per condensa laterale ",131,1,"DN 450",null,356.4,"265810045","106876","4037494146446",410,"100604",53.600000000000023,324,86,"100604",410,53.600000000000023]
["100605",100605,null,"STK","PPL 500 Kondensattopf mit Ablauf seitlich","CHF",547,"Schiedel PRIMA PLUS",2.4300000000000002,70,"J","PPL 500 Pot de condensat latéral","PPL 500 Kondensattopf mit Ablauf seitlich","PPL 500 Bancinella per condensa laterale ",131,1,"DN 500",null,475.2,"265810050","106877","4037494146453",547,"100605",71.800000000000011,432,115,"100605",547,71.800000000000011]
["100606",100606,null,"STK","PPL 600 Kondensattopf mit Ablauf seitlich","CHF",684,"Schiedel PRIMA PLUS",3.3,70,"J","PPL 600 Pot de condensat latéral","PPL 600 Kondensattopf mit Ablauf seitlich","PPL 600 Bancinella per condensa laterale ",131,1,"DN 600",null,594,"265810060","106878","4037494146477",684,"100606",90,540,144,"100606",684,90]
["100607",100607,null,"STK","PPL 700 Kondensattopf mit Ablauf seitlich","CHF",820,"Schiedel PRIMA PLUS",4.29,70,"J","PPL 700 Pot de condensat latéral","PPL 700 Kondensattopf mit Ablauf seitlich","PPL 700 Bancinella per condensa laterale ",131,1,"DN 700",null,712.8,"265810070","106879","4037494146491",820,"100607",107.20000000000005,648,172,"100607",820,107.20000000000005]
["100608",100608,null,"STK","PPL 80-130 Konsolenbleche für Zwischenstütze(Paar)","CHF",137,"Schiedel PRIMA PLUS",2.2000000000000002,0,"J","PPL 80-130Console murale (Pair)pour intermédieaire","PPL 80-130 Konsolenbleche für Zwischenstütze(Paar)","PPL 80-130 Coppia suporti per piastra passante",131,1,"DN 80",null,118.8,"27000001",null,null,137,"100608",18.200000000000003,108,29,"100608",137,18.200000000000003]
["100609",100609,null,"STK","PPL 150 Konsolenbleche für Zwischenstütze (Paar)","CHF",151,"Schiedel PRIMA PLUS",2.39,0,"J","PPL 150 Console murale  (Pair) pour intermédieaire","PPL 150 Konsolenbleche für Zwischenstütze (Paar)","PPL 150 Coppia suporti per piastra passante",131,1,"DN 150",null,130.9,"27000002",null,null,151,"100609",20.099999999999994,119,32,"100609",151,20.099999999999994]
["100610",100610,null,"STK","PPL 180 Konsolenbleche für Zwischenstütze (Paar)","CHF",164,"Schiedel PRIMA PLUS",2.85,0,"J","PPL 180 Console murale  (Pair) pour intermédieaire","PPL 180 Konsolenbleche für Zwischenstütze (Paar)","PPL 180 Coppia suporti per piastra passante",131,1,"DN 180",null,141.9,"27000003",null,null,164,"100610",22.099999999999994,129,35,"100610",164,22.099999999999994]
["100611",100611,null,"STK","PPL 200 Konsolenbleche für Zwischenstütze (Paar)","CHF",179,"Schiedel PRIMA PLUS",3.14,0,"J","PPL 200 Console murale  (Pair) pour intermédieaire","PPL 200 Konsolenbleche für Zwischenstütze (Paar)","PPL 200 Coppia suporti per piastra passante",131,1,"DN 200",null,155.1,"27000004",null,null,179,"100611",23.900000000000006,141,38,"100611",179,23.900000000000006]
["100612",100612,null,"STK","PPL 250 Konsolenbleche für Zwischenstütze (Paar)","CHF",192,"Schiedel PRIMA PLUS",3.54,0,"J","PPL 250 Console murale  (Pair) pour intermédieaire","PPL 250 Konsolenbleche für Zwischenstütze (Paar)","PPL 250 Coppia suporti per piastra passante",131,1,"DN 250",null,166.1,"27000006",null,null,192,"100612",25.900000000000006,151,41,"100612",192,25.900000000000006]
["100613",100613,null,"STK","PPL 300 Konsolenbleche für Zwischenstütze (Paar)","CHF",219,"Schiedel PRIMA PLUS",3.72,0,"J","PPL 300 Console murale  (Pair) pour intermédieaire","PPL 300 Konsolenbleche für Zwischenstütze (Paar)","PPL 300 Coppia suporti per piastra passante",131,1,"DN 300",null,190.3,"27000007",null,null,219,"100613",28.699999999999989,173,46,"100613",219,28.699999999999989]
["100614",100614,null,"STK","PPL 350 Konsolenbleche für Zwischenstütze (Paar)","CHF",246,"Schiedel PRIMA PLUS",4,0,"J","PPL 350 Console murale  (Pair) pour intermédieaire","PPL 350 Konsolenbleche für Zwischenstütze (Paar)","PPL 350 Coppia suporti per piastra passante",131,1,"DN 350",null,213.4,"27000635",null,null,246,"100614",32.599999999999994,194,52,"100614",246,32.599999999999994]
["100615",100615,null,"STK","PPL 400 Konsolenbleche für Zwischenstütze (Paar)","CHF",274,"Schiedel PRIMA PLUS",5.4,0,"J","PPL 400 Console murale  (Pair) pour intermédieaire","PPL 400 Konsolenbleche für Zwischenstütze (Paar)","PPL 400 Coppia suporti per piastra passante",131,1,"DN 400",null,237.6,"27000640",null,null,274,"100615",36.400000000000006,216,58,"100615",274,36.400000000000006]
["100616",100616,null,"STK","PPL 450 Konsolenbleche für Zwischenstütze (Paar)","CHF",342,"Schiedel PRIMA PLUS",7.58,0,"J","PPL 450 Console murale  (Pair) pour intermédieaire","PPL 450 Konsolenbleche für Zwischenstütze (Paar)","PPL 450 Coppia suporti per piastra passante",131,1,"DN 450",null,297,"27000645",null,null,342,"100616",45,270,72,"100616",342,45]
["100617",100617,null,"STK","PPL 500 Konsolenbleche für Zwischenstütze (Paar)","CHF",438,"Schiedel PRIMA PLUS",8.1999999999999993,0,"J","PPL 500 Console murale  (Pair) pour intermédieaire","PPL 500 Konsolenbleche für Zwischenstütze (Paar)","PPL 500 Coppia suporti per piastra passante",131,1,"DN 500",null,380.6,"27000650",null,null,438,"100617",57.399999999999977,346,92,"100617",438,57.399999999999977]
["100618",100618,null,"STK","PPL 600 Konsolenbleche für Zwischenstütze (Paar)","CHF",547,"Schiedel PRIMA PLUS",15.36,0,"J","PPL 600 Console murale  (Pair) pour intermédieaire","PPL 600 Konsolenbleche für Zwischenstütze (Paar)","PPL 600 Coppia suporti per piastra passante",131,1,"DN 600",null,475.2,"27000660",null,null,547,"100618",71.800000000000011,432,115,"100618",547,71.800000000000011]
["100619",100619,null,"STK","PPL 700 Konsolenbleche für Zwischenstütze (Paar)","CHF",684,"Schiedel PRIMA PLUS",20.059999999999999,0,"J","PPL 700 Console murale  (Pair) pour intermédieaire","PPL 700 Konsolenbleche für Zwischenstütze (Paar)","PPL 700 Coppia suporti per piastra passante",131,1,"DN 700",null,594,"27000670",null,null,684,"100619",90,540,144,"100619",684,90]
["100620",100620,null,"STK","PPL 80 Zwischenstütze","CHF",123,"Schiedel PRIMA PLUS",1.3,100,"J","PPL 80 Support intermédieaire","PPL 80 Zwischenstütze","PPL 80 Piastra passante",131,1,"DN 80",null,106.7,"265820308","106073","4037494148228",123,"100620",16.299999999999997,97,26,"100620",123,16.299999999999997]
["100621",100621,null,"STK","PPL 100 Zwischenstütze","CHF",130,"Schiedel PRIMA PLUS",1.36,100,"J","PPL 100 Support intermédieaire","PPL 100 Zwischenstütze","PPL 100 Piastra passante",131,1,"DN 100",null,112.2,"265820310","106074","4037494148235",130,"100621",17.799999999999997,102,28,"100621",130,17.799999999999997]
["100622",100622,null,"STK","PPL 130 Zwischenstütze","CHF",137,"Schiedel PRIMA PLUS",1.45,100,"J","PPL 130 Support intermédieaire","PPL 130 Zwischenstütze","PPL 130 Piastra passante",131,1,"DN 130",null,118.8,"265820313","106077","4037494148259",137,"100622",18.200000000000003,108,29,"100622",137,18.200000000000003]
["100623",100623,null,"STK","PPL 150 Zwischenstütze","CHF",145,"Schiedel PRIMA PLUS",1.68,100,"J","PPL 150 Support intermédieaire","PPL 150 Zwischenstütze","PPL 150 Piastra passante",131,1,"DN 150",null,125.4,"265820315","106079","4037494148266",145,"100623",19.599999999999994,114,31,"100623",145,19.599999999999994]
["100624",100624,null,"STK","PPL 180 Zwischenstütze","CHF",151,"Schiedel PRIMA PLUS",2.0499999999999998,100,"J","PPL 180 Support intermédieaire","PPL 180 Zwischenstütze","PPL 180 Piastra passante",131,1,"DN 180",null,130.9,"265820318","106081","4037494148273",151,"100624",20.099999999999994,119,32,"100624",151,20.099999999999994]
["100625",100625,null,"STK","PPL 200 Zwischenstütze","CHF",164,"Schiedel PRIMA PLUS",2.31,100,"J","PPL 200 Support intermédieaire","PPL 200 Zwischenstütze","PPL 200 Piastra passante",131,1,"DN 200",null,141.9,"265820320","106082","4037494148280",164,"100625",22.099999999999994,129,35,"100625",164,22.099999999999994]
["100626",100626,null,"STK","PPL 250 Zwischenstütze","CHF",192,"Schiedel PRIMA PLUS",3.2,100,"J","PPL 250 Support intermédieaire","PPL 250 Zwischenstütze","PPL 250 Piastra passante",131,1,"DN 250",null,166.1,"265820325","106084","4037494148303",192,"100626",25.900000000000006,151,41,"100626",192,25.900000000000006]
["100627",100627,null,"STK","PPL 300 Zwischenstütze","CHF",219,"Schiedel PRIMA PLUS",3.82,100,"J","PPL 300 Support intermédieaire","PPL 300 Zwischenstütze","PPL 300 Piastra passante",131,1,"DN 300",null,190.3,"265820330","106085","4037494148310",219,"100627",28.699999999999989,173,46,"100627",219,28.699999999999989]
["100628",100628,null,"STK","PPL 350 Zwischenstütze","CHF",274,"Schiedel PRIMA PLUS",4.3099999999999996,100,"J","PPL 350 Support intermédieaire","PPL 350 Zwischenstütze","PPL 350 Piastra passante",131,1,"DN 350",null,237.6,"265821335",null,null,274,"100628",36.400000000000006,216,58,"100628",274,36.400000000000006]
["100629",100629,null,"STK","PPL 400 Zwischenstütze","CHF",315,"Schiedel PRIMA PLUS",6.6,100,"J","PPL 400 Support intermédieaire","PPL 400 Zwischenstütze","PPL 400 Piastra passante",131,1,"DN 400",null,273.89999999999998,"265821340",null,null,315,"100629",41.100000000000023,249,66,"100629",315,41.100000000000023]
["100630",100630,null,"STK","PPL 450 Zwischenstütze","CHF",370,"Schiedel PRIMA PLUS",7.47,100,"J","PPL 450 Support intermédieaire","PPL 450 Zwischenstütze","PPL 450 Piastra passante",131,1,"DN 450",null,321.2,"265821345",null,null,370,"100630",48.800000000000011,292,78,"100630",370,48.800000000000011]
["100631",100631,null,"STK","PPL 500 Zwischenstütze","CHF",424,"Schiedel PRIMA PLUS",8.35,100,"J","PPL 500 Support intermédieaire","PPL 500 Zwischenstütze","PPL 500 Piastra passante",131,1,"DN 500",null,368.5,"265821350",null,null,424,"100631",55.5,335,89,"100631",424,55.5]
["100632",100632,null,"STK","PPL 600 Zwischenstütze","CHF",480,"Schiedel PRIMA PLUS",10.08,100,"J","PPL 600 Support intermédieaire","PPL 600 Zwischenstütze","PPL 600 Piastra passante",131,1,"DN 600",null,416.9,"265821360",null,null,480,"100632",63.100000000000023,379,101,"100632",480,63.100000000000023]
["100633",100633,null,"STK","PPL 700 Zwischenstütze","CHF",547,"Schiedel PRIMA PLUS",11.83,100,"J","PPL 700 Support intermédieaire","PPL 700 Zwischenstütze","PPL 700 Piastra passante",131,1,"DN 700",null,475.2,"265821370",null,null,547,"100633",71.800000000000011,432,115,"100633",547,71.800000000000011]
["100634",100634,null,"STK","PPL 80 Kondensattopf mit Ablauf senkrecht","CHF",49,"Schiedel PRIMA PLUS",0.1,48,"J","PPL 80 Pot de condensation vertical","PPL 80 Kondensattopf mit Ablauf senkrecht","PPL 80 Bancinella per condensa verticale ",131,1,"DN 80",null,41.8,"DS619080",null,null,49,"100634",7.2000000000000028,38,11,"100634",49,7.2000000000000028]
["100635",100635,null,"STK","PPL 100 Kondensattopf mit Ablauf senkrecht","CHF",55,"Schiedel PRIMA PLUS",1.1399999999999999,48,"J","PPL 100 Pot de condensation vertical","PPL 100 Kondensattopf mit Ablauf senkrecht","PPL 100 Bancinella per condensa verticale ",131,1,"DN 100",null,47.3,"DS619100",null,null,55,"100635",7.7000000000000028,43,12,"100635",55,7.7000000000000028]
["100636",100636,null,"STK","PPL 130 Kondensattopf mit Ablauf senkrecht","CHF",62,"Schiedel PRIMA PLUS",0.2,48,"J","PPL 130 Pot de condensation vertical","PPL 130 Kondensattopf mit Ablauf senkrecht","PPL 130 Bancinella per condensa verticale ",131,1,"DN 130",null,53.9,"DS619130",null,null,62,"100636",8.1000000000000014,49,13,"100636",62,8.1000000000000014]
["100637",100637,null,"STK","PPL 150 Kondensattopf mit Ablauf senkrecht","CHF",69,"Schiedel PRIMA PLUS",0.24,48,"J","PPL 150 Pot de condensation vertical","PPL 150 Kondensattopf mit Ablauf senkrecht","PPL 150 Bancinella per condensa verticale ",131,1,"DN 150",null,59.4,"DS619150",null,null,69,"100637",9.6000000000000014,54,15,"100637",69,9.6000000000000014]
["100638",100638,null,"STK","PPL 180 Kondensattopf mit Ablauf senkrecht","CHF",81,"Schiedel PRIMA PLUS",0.32,48,"J","PPL 180 Pot de condensation vertical","PPL 180 Kondensattopf mit Ablauf senkrecht","PPL 180 Bancinella per condensa verticale ",131,1,"DN 180",null,70.400000000000006,"DS619180",null,null,81,"100638",10.599999999999994,64,17,"100638",81,10.599999999999994]
["100639",100639,null,"STK","PPL 200 Kondensattopf mit Ablauf senkrecht","CHF",97,"Schiedel PRIMA PLUS",0.38,48,"J","PPL 200 Pot de condensation vertical","PPL 200 Kondensattopf mit Ablauf senkrecht","PPL 200 Bancinella per condensa verticale ",131,1,"DN 200",null,83.6,"DS619200",null,null,97,"100639",13.400000000000006,76,21,"100639",97,13.400000000000006]
["100640",100640,null,"STK","PPL 250 Kondensattopf mit Ablauf senkrecht","CHF",109,"Schiedel PRIMA PLUS",0.49,48,"J","PPL 250 Pot de condensation vertical","PPL 250 Kondensattopf mit Ablauf senkrecht","PPL 250 Bancinella per condensa verticale ",131,1,"DN 250",null,94.6,"DS619250",null,null,109,"100640",14.400000000000006,86,23,"100640",109,14.400000000000006]
["100642",100642,null,"STK","PPL 350 Kondensattopf mit Ablauf senkrecht","CHF",151,"Schiedel PRIMA PLUS",0.89,48,"J","PPL 350 Pot de condensation vertical","PPL 350 Kondensattopf mit Ablauf senkrecht","PPL 350 Bancinella per condensa verticale ",131,1,"DN 350",null,130.9,"DS619350",null,null,151,"100642",20.099999999999994,119,32,"100642",151,20.099999999999994]
["100643",100643,null,"STK","PPL 400 Kondensattopf mit Ablauf senkrecht","CHF",205,"Schiedel PRIMA PLUS",1.9,48,"J","PPL 400 Pot de condensation vertical","PPL 400 Kondensattopf mit Ablauf senkrecht","PPL 400 Bancinella per condensa verticale ",131,1,"DN 400",null,178.2,"DS619400",null,null,205,"100643",26.800000000000011,162,43,"100643",205,26.800000000000011]
["100644",100644,null,"STK","PPL 450 Kondensattopf mit Ablauf senkrecht","CHF",274,"Schiedel PRIMA PLUS",2.0499999999999998,48,"J","PPL 450 Pot de condensation vertical","PPL 450 Kondensattopf mit Ablauf senkrecht","PPL 450 Bancinella per condensa verticale ",131,1,"DN 450",null,237.6,"DS619450",null,null,274,"100644",36.400000000000006,216,58,"100644",274,36.400000000000006]
["100645",100645,null,"STK","PPL 500 Kondensattopf mit Ablauf senkrecht","CHF",342,"Schiedel PRIMA PLUS",2.4300000000000002,48,"J","PPL 500 Pot de condensation vertical","PPL 500 Kondensattopf mit Ablauf senkrecht","PPL 500 Bancinella per condensa verticale ",131,1,"DN 500",null,297,"DS619500",null,null,342,"100645",45,270,72,"100645",342,45]
["100646",100646,null,"STK","PPL 600 Kondensattopf mit Ablauf senkrecht","CHF",410,"Schiedel PRIMA PLUS",3.3,48,"J","PPL 600 Pot de condensation vertical","PPL 600 Kondensattopf mit Ablauf senkrecht","PPL 600 Bancinella per condensa verticale ",131,1,"DN 600",null,356.4,"DS619600",null,null,410,"100646",53.600000000000023,324,86,"100646",410,53.600000000000023]
["100647",100647,null,"STK","PPL 700 Kondensattopf mit Ablauf senkrecht","CHF",547,"Schiedel PRIMA PLUS",4.29,48,"J","PPL 700 Pot de condensation vertical","PPL 700 Kondensattopf mit Ablauf senkrecht","PPL 700 Bancinella per condensa verticale ",131,1,"DN 700",null,475.2,"DS619700",null,null,547,"100647",71.800000000000011,432,115,"100647",547,71.800000000000011]
["100648",100648,null,"STK","PPL 100 EW-DW Deckenanfängerset komplett L270mm","CHF",410,"Schiedel PRIMA PLUS",3.2,0,"J","PPL 100 set débutant couverture vertical L270mm","PPL 100 EW-DW Deckenanfängerset komplett L270mm","PPL 100 Set di copertura vertical L270mm",131,1,"DN 100",null,356.4,"265800510",null,null,410,"100648",53.600000000000023,324,86,"100648",410,53.600000000000023]
["100649",100649,null,"STK","PPL 130 EW-DW Deckenanfängerset komplett L270mm","CHF",480,"Schiedel PRIMA PLUS",3.8,0,"J","PPL 130 set débutant couverture vertical L270mm","PPL 130 EW-DW Deckenanfängerset komplett L270mm","PPL 130 Set di copertura vertical L270mm",131,1,"DN 130",null,416.9,"265800513","108767","4037494151891",480,"100649",63.100000000000023,379,101,"100649",480,63.100000000000023]
["100650",100650,null,"STK","PPL 150 EW-DW Deckenanfängerset komplett L270mm","CHF",488,"Schiedel PRIMA PLUS",4.5,0,"J","PPL 150 set débutant couverture vertical L270mm","PPL 150 EW-DW Deckenanfängerset komplett L270mm","PPL 150 Set di copertura vertical L270mm",131,1,"DN 150",null,423.5,"265800515","108768","4037494151907",488,"100650",64.5,385,103,"100650",488,64.5]
["100651",100651,null,"STK","PPL 180 EW-DW Deckenanfängerset komplett L270mm","CHF",547,"Schiedel PRIMA PLUS",5,0,"J","PPL 180 set débutant couverture vertical L270mm","PPL 180 EW-DW Deckenanfängerset komplett L270mm","PPL 180 Set di copertura vertical L270mm",131,1,"DN 180",null,475.2,"265800518",null,null,547,"100651",71.800000000000011,432,115,"100651",547,71.800000000000011]
["100652",100652,null,"STK","PPL 200 EW-DW Deckenanfängerset komplett L270mm","CHF",617,"Schiedel PRIMA PLUS",5.7,0,"J","PPL 200 set débutant couverture vertical L270mm","PPL 200 EW-DW Deckenanfängerset komplett L270mm","PPL 200 Set di copertura vertical L270mm",131,1,"DN 200",null,535.70000000000005,"265800520",null,null,617,"100652",81.299999999999955,487,130,"100652",617,81.299999999999955]
["100653",100653,null,"STK","PPL 250 EW-DW Deckenanfängerset komplett L270mm","CHF",684,"Schiedel PRIMA PLUS",6.3,0,"J","PPL 250 set débutant couverture vertical L270mm","PPL 250 EW-DW Deckenanfängerset komplett L270mm","PPL 250 Set di copertura vertical L270mm",131,1,"DN 250",null,594,"265800525",null,null,684,"100653",90,540,144,"100653",684,90]
["100654",100654,null,"STK","PPL 300 EW-DW Deckenanfängerset komplett L270mm","CHF",753,"Schiedel PRIMA PLUS",7,0,"J","PPL 300 set débutant couverture vertical L270mm","PPL 300 EW-DW Deckenanfängerset komplett L270mm","PPL 300 Set di copertura vertical L270mm",131,1,"DN 300",null,654.5,"265800530",null,null,753,"100654",98.5,595,158,"100654",753,98.5]
["100655",100655,null,"STK","PPL 100 EW-DW Deckenanfängerset 45° kompl. L270mm","CHF",547,"Schiedel PRIMA PLUS",3.2,0,"J","PPL 100 set débutant couverture 45° L270mm","PPL 100 EW-DW Deckenanfängerset 45° kompl. L270mm","PPL 100 Set di copertura 45°  L270mm",131,1,"DN 100",null,475.2,"265800610",null,null,547,"100655",71.800000000000011,432,115,"100655",547,71.800000000000011]
["100656",100656,null,"STK","PPL 130 EW-DW Deckenanfängerset 45° kompl. L270mm","CHF",617,"Schiedel PRIMA PLUS",3.8,0,"J","PPL 130 set débutant couverture 45° L270mm","PPL 130 EW-DW Deckenanfängerset 45° kompl. L270mm","PPL 130 Set di copertura 45°  L270mm",131,1,"DN 130",null,535.70000000000005,"265800613","108770","4037494151921",617,"100656",81.299999999999955,487,130,"100656",617,81.299999999999955]
["100657",100657,null,"STK","PPL 150 EW-DW Deckenanfängerset 45° kompl. L270mm","CHF",684,"Schiedel PRIMA PLUS",4.5,0,"J","PPL 150 set débutant couverture 45° L270mm","PPL 150 EW-DW Deckenanfängerset 45° kompl. L270mm","PPL 150 Set di copertura 45°  L270mm",131,1,"DN 150",null,594,"265800615","108771","4037494151938",684,"100657",90,540,144,"100657",684,90]
["100658",100658,null,"STK","PPL 180 EW-DW Deckenanfängerset 45° kompl. L270mm","CHF",753,"Schiedel PRIMA PLUS",5,0,"J","PPL 180 set débutant couverture 45° L270mm","PPL 180 EW-DW Deckenanfängerset 45° kompl. L270mm","PPL 180 Set di copertura 45°  L270mm",131,1,"DN 180",null,654.5,"265800618",null,null,753,"100658",98.5,595,158,"100658",753,98.5]
["100659",100659,null,"STK","PPL 200 EW-DW Deckenanfängerset 45° kompl. L270mm","CHF",820,"Schiedel PRIMA PLUS",5.7,0,"J","PPL 200 set débutant couverture 45° L270mm","PPL 200 EW-DW Deckenanfängerset 45° kompl. L270mm","PPL 200 Set di copertura 45°  L270mm",131,1,"DN 200",null,712.8,"265800620",null,null,820,"100659",107.20000000000005,648,172,"100659",820,107.20000000000005]
["100660",100660,null,"STK","PPL 250 EW-DW Deckenanfängerset 45° kompl. L270mm","CHF",890,"Schiedel PRIMA PLUS",6.3,0,"J","PPL 250 set débutant couverture 45° L270mm","PPL 250 EW-DW Deckenanfängerset 45° kompl. L270mm","PPL 250 Set di copertura 45°  L270mm",131,1,"DN 250",null,773.3,"265800625",null,null,890,"100660",116.70000000000005,703,187,"100660",890,116.70000000000005]
[{"$f":"B652&\"\"","v":"100661"},100661,null,"STK",{"$f":"IF($E$200=2,L652,IF($E$200=3,N652,M652))","v":"PPL 300 EW-DW Deckenanfängerset 45° kompl. L270mm"},"CHF",{"$f":"IF($L$190=1,W652,S652)","v":1026},"Schiedel PRIMA PLUS",7,0,"J","PPL 300 set débutant couverture 45° L270mm","PPL 300 EW-DW Deckenanfängerset 45° kompl. L270mm","PPL 300 Set di copertura 45°  L270mm",131,1,"DN 300",null,892.1,"265800630",null,null,1026,"100661",133.89999999999998,811,215,"100661",1026,133.89999999999998]
["100698",100698,null,"STK","PPL 80 Revisions.-und Anschluss-Basiselement DN80 ","CHF",97,"Schiedel PRIMA PLUS",0.36,283,"J","PPL 80 Elem. base por raccord.et révision DN80 ","PPL 80 Revisions.-und Anschluss-Basiselement DN80 ","PPL 80 Elemento basamento revisione et racc. DN80 ",131,1,"DN 80",null,83.6,"238300508","106030","4037494146705",97,"100698",13.400000000000006,76,21,"100698",97,13.400000000000006]
["100699",100699,null,"STK","PPL 100 Revisions-und Anschluss-Basiselement DN100","CHF",109,"Schiedel PRIMA PLUS",0.46,283,"J","PPL 100 Elem. base por raccord.et révision DN100","PPL 100 Revisions-und Anschluss-Basiselement DN100","PPL 100 Elemento basamento revisione et racc.DN100",131,1,"DN 100",null,94.6,"238300510","106526","4037494146712",109,"100699",14.400000000000006,86,23,"100699",109,14.400000000000006]
["100700",100700,null,"STK","PPL 130 Revisions-und Anschluss-Basiselement DN130","CHF",123,"Schiedel PRIMA PLUS",0.61,283,"J","PPL 130 Elem. base por raccord.et révision DN130","PPL 130 Revisions-und Anschluss-Basiselement DN130","PPL 130 Elemento basamento revisione et racc.DN130",131,1,"DN 130",null,106.7,"238300513","106529","4037494146736",123,"100700",16.299999999999997,97,26,"100700",123,16.299999999999997]
["100701",100701,null,"STK","PPL 150 Revisions-und Anschluss-Basiselement DN150","CHF",137,"Schiedel PRIMA PLUS",0.8,325,"J","PPL 150 Elem. base por raccord.et révision DN150","PPL 150 Revisions-und Anschluss-Basiselement DN150","PPL 150 Revisions-und Anschluss-Basiselement DN150",131,1,"DN 150",null,118.8,"238300515","106531","4037494146743",137,"100701",18.200000000000003,108,29,"100701",137,18.200000000000003]
["100702",100702,null,"STK","PPL 180 Anschluss-Basiselement DN180 L450mm","CHF",151,"Schiedel PRIMA PLUS",1.32,450,"J","PPL 180 Elem. de base raccordement DN180 L 450mm","PPL 180 Anschluss-Basiselement DN180 L450mm","PPL 180 Elemento Basamento raccordo DN180 L 450mm",131,1,"DN 180",null,130.9,"238300518","106533","4037494146750",151,"100702",20.099999999999994,119,32,"100702",151,20.099999999999994]
["100703",100703,null,"STK","PPL 200 Anschluss-Basiselement DN200 L450mm","CHF",164,"Schiedel PRIMA PLUS",1.46,450,"J","PPL 200 Elem. de base raccordement DN200 L 450mm","PPL 200 Anschluss-Basiselement DN200 L450mm","PPL 200 Elemento Basamento raccordo DN200 L 450mm",131,1,"DN 200",null,141.9,"238300520","106534","4037494146767",164,"100703",22.099999999999994,129,35,"100703",164,22.099999999999994]
["100704",100704,null,"STK","PPL 250 Anschluss-Basiselement DN250 L450mm","CHF",219,"Schiedel PRIMA PLUS",2.0299999999999998,450,"J","PPL 250 Elem. de base raccordement DN250 L 450mm","PPL 250 Anschluss-Basiselement DN250 L450mm","PPL 250 Elemento Basamento raccordo DN250 L 450mm",131,1,"DN 250",null,190.3,"238300525","106536","4037494146781",219,"100704",28.699999999999989,173,46,"100704",219,28.699999999999989]
["100705",100705,null,"STK","PPL 300 Anschluss-Basiselement DN300 L450mm","CHF",274,"Schiedel PRIMA PLUS",2.4900000000000002,450,"J","PPL 300 Elem. de base raccordement DN300 L 450mm","PPL 300 Anschluss-Basiselement DN300 L450mm","PPL 300 Elemento Basamento raccordo DN300 L 450mm",131,1,"DN 300",null,237.6,"238300530","106537","4037494146798",274,"100705",36.400000000000006,216,58,"100705",274,36.400000000000006]
["100706",100706,null,"STK","PPL 180 Revisions-Basiselement für Deckel DN150 ","CHF",151,"Schiedel PRIMA PLUS",1.32,450,"J","PPL 180 Elem. de base révision couvercle DN150 ","PPL 180 Revisions-Basiselement für Deckel DN150 ","PPL 180 Elem. basamento revisione chiusura DN150 ",131,1,"DN 180",null,130.9,"238300618","106033","4037494155455",151,"100706",20.099999999999994,119,32,"100706",151,20.099999999999994]
["100707",100707,null,"STK","PPL 200 Revisions-Basiselement für Deckel DN150 ","CHF",179,"Schiedel PRIMA PLUS",1.46,450,"J","PPL 200 Elem. de base révision couvercle DN150 ","PPL 200 Revisions-Basiselement für Deckel DN150 ","PPL 200 Elem. basamento revisione chiusura DN150 ",131,1,"DN 200",null,155.1,"238300620","106034","4037494155462",179,"100707",23.900000000000006,141,38,"100707",179,23.900000000000006]
["100708",100708,null,"STK","PPL 250 Revisions-Basiselement für Deckel DN180 ","CHF",205,"Schiedel PRIMA PLUS",1.88,450,"J","PPL 250 Elem. de base révision couvercle DN180 ","PPL 250 Revisions-Basiselement für Deckel DN180 ","PPL 250 Elem. basamento revisione chiusura DN180 ",131,1,"DN 250",null,178.2,"238300625","106036","4037494155486",205,"100708",26.800000000000011,162,43,"100708",205,26.800000000000011]
["100709",100709,null,"STK","PPL 300 Revisions-Basiselement für Deckel DN180 ","CHF",274,"Schiedel PRIMA PLUS",2.0299999999999998,450,"J","PPL 300 Elem. de base révision couvercle DN180 ","PPL 300 Revisions-Basiselement für Deckel DN180 ","PPL 300 Elem. basamento revisione chiusura DN180 ",131,1,"DN 300",null,237.6,"238300630","106037","4037494155493",274,"100709",36.400000000000006,216,58,"100709",274,36.400000000000006]
["100710",100710,null,"STK","PPL 350 Revisions-Basiselement für Deckel DN300 ","CHF",410,"Schiedel PRIMA PLUS",4.4000000000000004,450,"J","PPL 350 Elem. de base révision couvercle DN300 ","PPL 350 Revisions-Basiselement für Deckel DN300 ","PPL 350 Elem. basamento revisione chiusura DN300 ",131,1,"DN 350",null,356.4,"6135135081",null,null,410,"100710",53.600000000000023,324,86,"100710",410,53.600000000000023]
["100711",100711,null,"STK","PPL 400 Revisions-Basiselement für Deckel DN300 ","CHF",547,"Schiedel PRIMA PLUS",5.0199999999999996,450,"J","PPL 400 Elem. de base révision couvercle DN300 ","PPL 400 Revisions-Basiselement für Deckel DN300 ","PPL 400 Elem. basamento revisione chiusura DN300 ",131,1,"DN 400",null,475.2,"6135140081",null,null,547,"100711",71.800000000000011,432,115,"100711",547,71.800000000000011]
["100712",100712,null,"STK","PPL 450 Revisions-Basiselement für Deckel DN300 ","CHF",684,"Schiedel PRIMA PLUS",6,450,"J","PPL 450 Elem. de base révision couvercle DN300 ","PPL 450 Revisions-Basiselement für Deckel DN300 ","PPL 450 Elem. basamento revisione chiusura DN300 ",131,1,"DN 450",null,594,"6135145081",null,null,684,"100712",90,540,144,"100712",684,90]
["100713",100713,null,"STK","PPL 500 Revisions-Basiselement für Deckel DN300 ","CHF",820,"Schiedel PRIMA PLUS",6.28,450,"J","PPL 500 Elem. de base révision couvercle DN300 ","PPL 500 Revisions-Basiselement für Deckel DN300 ","PPL 500 Elem. basamento revisione chiusura DN300 ",131,1,"DN 500",null,712.8,"6135150081",null,null,820,"100713",107.20000000000005,648,172,"100713",820,107.20000000000005]
["100714",100714,null,"STK","PPL 600 Revisions-Basiselement für Deckel DN300 ","CHF",1026,"Schiedel PRIMA PLUS",7.54,450,"J","PPL 600 Elem. de base révision couvercle DN300 ","PPL 600 Revisions-Basiselement für Deckel DN300 ","PPL 600 Elem. basamento revisione chiusura DN300 ",131,1,"DN 600",null,892.1,"6135160081",null,null,1026,"100714",133.89999999999998,811,215,"100714",1026,133.89999999999998]
["100715",100715,null,"STK","PPL 700 Revisions-Basiselement für Deckel DN300 ","CHF",1300,"Schiedel PRIMA PLUS",8.7899999999999991,450,"J","PPL 700 Elem. de base révision couvercle DN300 ","PPL 700 Revisions-Basiselement für Deckel DN300 ","PPL 700 Elem. basamento revisione chiusura DN300 ",131,1,"DN 700",null,1129.7,"6135170081",null,null,1300,"100715",170.29999999999995,1027,273,"100715",1300,170.29999999999995]
["100716",100716,null,"STK","PPL 130 Anschluss glatt zu Basiselement L120mm","CHF",69,"Schiedel PRIMA PLUS",0.37,0,"J","PPL 130 Raccordement enbout male L120mm","PPL 130 Anschluss glatt zu Basiselement L120mm","PPL 130 Raccordo con maschio L120mm",131,1,"DN 130",null,59.4,"242050013","106559","4037494152966",69,"100716",9.6000000000000014,54,15,"100716",69,9.6000000000000014]
["100717",100717,null,"STK","PPL 150 Anschluss glatt zu Basiselement L120mm","CHF",81,"Schiedel PRIMA PLUS",0.42,0,"J","PPL 150 Raccordement enbout male L120mm","PPL 150 Anschluss glatt zu Basiselement L120mm","PPL 150 Raccordo con maschio L120mm",131,1,"DN 150",null,70.400000000000006,"242050015","106561","4037494152973",81,"100717",10.599999999999994,64,17,"100717",81,10.599999999999994]
["100718",100718,null,"STK","PPL 180 Anschluss glatt zu Basiselement L120mm","CHF",97,"Schiedel PRIMA PLUS",0.54,0,"J","PPL 180 Raccordement enbout male L120mm","PPL 180 Anschluss glatt zu Basiselement L120mm","PPL 180 Raccordo con maschio L120mm",131,1,"DN 180",null,83.6,"242050018","106563","4037494152980",97,"100718",13.400000000000006,76,21,"100718",97,13.400000000000006]
["100719",100719,null,"STK","PPL 200 Anschluss glatt zu Basiselement L120mm","CHF",109,"Schiedel PRIMA PLUS",0.59,0,"J","PPL 200 Raccordement enbout male L120mm","PPL 200 Anschluss glatt zu Basiselement L120mm","PPL 200 Raccordo con maschio L120mm",131,1,"DN 200",null,94.6,"242050020","106564","4037494152997",109,"100719",14.400000000000006,86,23,"100719",109,14.400000000000006]
["100720",100720,null,"STK","PPL 250 Anschluss glatt zu Basiselement L120mm","CHF",164,"Schiedel PRIMA PLUS",0.72,0,"J","PPL 250 Raccordement enbout male L120mm","PPL 250 Anschluss glatt zu Basiselement L120mm","PPL 250 Raccordo con maschio L120mm",131,1,"DN 250",null,141.9,"242050025","106566","4037494153017",164,"100720",22.099999999999994,129,35,"100720",164,22.099999999999994]
["100721",100721,null,"STK","PPL 300 Anschluss glatt zu Basiselement L120mm","CHF",192,"Schiedel PRIMA PLUS",0.85,0,"J","PPL 300 Raccordement enbout male L120mm","PPL 300 Anschluss glatt zu Basiselement L120mm","PPL 300 Raccordo con maschio L120mm",131,1,"DN 300",null,166.1,"242050030","106567","4037494153024",192,"100721",25.900000000000006,151,41,"100721",192,25.900000000000006]
["100723",100723,null,"STK","PPL 130 Anschluss-Doppelfutter zu Basiselement ","CHF",123,"Schiedel PRIMA PLUS",0.67,0,"J","PPL 130 Raccord double manchon pour elém. base ","PPL 130 Anschluss-Doppelfutter zu Basiselement ","PPL 130 Raccordo doppia parete per elem.basamento ",131,1,"DN 130",null,106.7,"242001313","103526","4037494508923",123,"100723",16.299999999999997,97,26,"100723",123,16.299999999999997]
["100724",100724,null,"STK","PPL 150 Anschluss-Doppelfutter zu Basiselement ","CHF",137,"Schiedel PRIMA PLUS",0.77,0,"J","PPL 150 Raccord double manchon pour elém. base ","PPL 150 Anschluss-Doppelfutter zu Basiselement ","PPL 150 Raccordo doppia parete per elem.basamento ",131,1,"DN 150",null,118.8,"242001515","103534","4037494508961",137,"100724",18.200000000000003,108,29,"100724",137,18.200000000000003]
["100725",100725,null,"STK","PPL 180 Anschluss-Doppelfutter zu Basiselement ","CHF",151,"Schiedel PRIMA PLUS",0.96,0,"J","PPL 180 Raccord double manchon pour elém. base ","PPL 180 Anschluss-Doppelfutter zu Basiselement ","PPL 180 Raccordo doppia parete per elem.basamento ",131,1,"DN 180",null,130.9,"242001818","103545","4037494508992",151,"100725",20.099999999999994,119,32,"100725",151,20.099999999999994]
["100726",100726,null,"STK","PPL 200 Anschluss-Doppelfutter zu Basiselement ","CHF",164,"Schiedel PRIMA PLUS",1.06,0,"J","PPL 200 Raccord double manchon pour elém. base ","PPL 200 Anschluss-Doppelfutter zu Basiselement ","PPL 200 Raccordo doppia parete per elem.basamento ",131,1,"DN 200",null,141.9,"242002020","103548","4037494509012",164,"100726",22.099999999999994,129,35,"100726",164,22.099999999999994]
["100727",100727,null,"STK","PPL 250 Anschluss-Doppelfutter zu Basiselement ","CHF",205,"Schiedel PRIMA PLUS",1.31,0,"J","PPL 250 Raccord double manchon pour elém. base ","PPL 250 Anschluss-Doppelfutter zu Basiselement ","PPL 250 Raccordo doppia parete per elem.basamento ",131,1,"DN 250",null,178.2,"242002525","103553","4037494509319",205,"100727",26.800000000000011,162,43,"100727",205,26.800000000000011]
["100728",100728,null,"STK","PPL 300 Anschluss-Doppelfutter zu Basiselement ","CHF",260,"Schiedel PRIMA PLUS",1.5,0,"J","PPL 300 Raccord double manchon pour elém. base ","PPL 300 Anschluss-Doppelfutter zu Basiselement ","PPL 300 Anschluss-Doppelfutter zu Basiselement ",131,1,"DN 300",null,225.5,"242003030","103556","4037494509333",260,"100728",34.5,205,55,"100728",260,34.5]
["100729",100729,null,"STK","PPL 80 Revisionsdeckel für Oel/Gas ","CHF",41,"Schiedel PRIMA PLUS",0.17,0,"J","PPL 80 Couvercle basse température Oel/Gas ","PPL 80 Revisionsdeckel für Oel/Gas ","PPL 80 Chiusura per olio et gas",131,1,"DN 80",null,35.200000000000003,"265820908","105934","5035944365866",41,"100729",5.7999999999999972,32,9,"100729",41,5.7999999999999972]
["100730",100730,null,"STK","PPL 100 Revisionsdeckel für Oel/Gas ","CHF",49,"Schiedel PRIMA PLUS",0.22,0,"J","PPL 100 Couvercle basse température Oel/Gas ","PPL 100 Revisionsdeckel für Oel/Gas ","PPL 100 Chiusura per olio et gas",131,1,"DN 100",null,41.8,"265820910","105935","5035944536112",49,"100730",7.2000000000000028,38,11,"100730",49,7.2000000000000028]
["100731",100731,null,"STK","PPL 130 Revisionsdeckel für Oel/Gas ","CHF",55,"Schiedel PRIMA PLUS",0.32,0,"J","PPL 130 Couvercle basse température Oel/Gas ","PPL 130 Revisionsdeckel für Oel/Gas ","PPL 130 Chiusura per olio et gas",131,1,"DN 130",null,47.3,"265820913","105938","5035944365873",55,"100731",7.7000000000000028,43,12,"100731",55,7.7000000000000028]
["100732",100732,null,"STK","PPL 150 Revisionsdeckel für Oel/Gas ","CHF",69,"Schiedel PRIMA PLUS",0.41,0,"J","PPL 150 Couvercle basse température Oel/Gas ","PPL 150 Revisionsdeckel für Oel/Gas ","PPL 150 Chiusura per olio et gas",131,1,"DN 150",null,59.4,"265820915","105939","5035944365880",69,"100732",9.6000000000000014,54,15,"100732",69,9.6000000000000014]
["100733",100733,null,"STK","PPL 180 Revisionsdeckel für Oel/Gas ","CHF",81,"Schiedel PRIMA PLUS",0.41,0,"J","PPL 180 Couvercle basse température Oel/Gas ","PPL 180 Revisionsdeckel für Oel/Gas ","PPL 180 Chiusura per olio et gas",131,1,"DN 180",null,70.400000000000006,"265820918","106103","5035944536167",81,"100733",10.599999999999994,64,17,"100733",81,10.599999999999994]
["100734",100734,null,"STK","PPL 200 Revisionsdeckel für Oel/Gas ","CHF",97,"Schiedel PRIMA PLUS",0.64,0,"J","PPL 200 Couvercle basse température Oel/Gas ","PPL 200 Revisionsdeckel für Oel/Gas ","PPL 200 Chiusura per olio et gas",131,1,"DN 200",null,83.6,"265820920","105940","5035944365897",97,"100734",13.400000000000006,76,21,"100734",97,13.400000000000006]
["100735",100735,null,"STK","PPL 250 Revisionsdeckel für Oel/Gas ","CHF",137,"Schiedel PRIMA PLUS",0.93,0,"J","PPL 250 Couvercle basse température Oel/Gas ","PPL 250 Revisionsdeckel für Oel/Gas ","PPL 250 Chiusura per olio et gas",131,1,"DN 250",null,118.8,"265820925","105941","5035944541505",137,"100735",18.200000000000003,108,29,"100735",137,18.200000000000003]
["100736",100736,null,"STK","PPL 300 Revisionsdeckel für Oel/Gas ","CHF",179,"Schiedel PRIMA PLUS",1.43,0,"J","PPL 300 Couvercle basse température Oel/Gas ","PPL 300 Revisionsdeckel für Oel/Gas ","PPL 300 Chiusura per olio et gas",131,1,"DN 300",null,155.1,"265820930","105942","4037494152942",179,"100736",23.900000000000006,141,38,"100736",179,23.900000000000006]
["100737",100737,null,"STK","PPL 80 Revisionsdeckel für Festbrennstoffe","CHF",69,"Schiedel PRIMA PLUS",0.15,0,"J","PPL 80 Couvercle pour haute température ","PPL 80 Revisionsdeckel für Festbrennstoffe","PPL 80 Chiusura per combustibilie solidi",131,1,"DN 80",null,59.4,"255160008","106578","4037494431818",69,"100737",9.6000000000000014,54,15,"100737",69,9.6000000000000014]
["100738",100738,null,"STK","PPL 100 Revisionsdeckel für Festbrennstoffe","CHF",75,"Schiedel PRIMA PLUS",0.15,0,"J","PPL 100 Couvercle pour haute température ","PPL 100 Revisionsdeckel für Festbrennstoffe","PPL 100 Chiusura per combustibilie solidi",131,1,"DN 100",null,64.900000000000006,"255160010","106579","4037494431825",75,"100738",10.099999999999994,59,16,"100738",75,10.099999999999994]
["100739",100739,null,"STK","PPL 130 Revisionsdeckel für Festbrennstoffe","CHF",81,"Schiedel PRIMA PLUS",0.2,0,"J","PPL 130 Couvercle pour haute température ","PPL 130 Revisionsdeckel für Festbrennstoffe","PPL 130 Chiusura per combustibilie solidi",131,1,"DN 130",null,70.400000000000006,"255160013","105929","4037494431856",81,"100739",10.599999999999994,64,17,"100739",81,10.599999999999994]
["100740",100740,null,"STK","PPL 150 Revisionsdeckel für Festbrennstoffe","CHF",97,"Schiedel PRIMA PLUS",0.2,0,"J","PPL 150 Couvercle pour haute température ","PPL 150 Revisionsdeckel für Festbrennstoffe","PPL 150 Chiusura per combustibilie solidi",131,1,"DN 150",null,83.6,"255160015","105930","4037494431863",97,"100740",13.400000000000006,76,21,"100740",97,13.400000000000006]
["100741",100741,null,"STK","PPL 180 Revisionsdeckel für Festbrennstoffe","CHF",109,"Schiedel PRIMA PLUS",0.2,0,"J","PPL 180 Couvercle pour haute température ","PPL 180 Revisionsdeckel für Festbrennstoffe","PPL 180 Chiusura per combustibilie solidi",131,1,"DN 180",null,94.6,"255160018","106060","4037494431870",109,"100741",14.400000000000006,86,23,"100741",109,14.400000000000006]
["100742",100742,null,"STK","PPL 200 Revisionsdeckel für Festbrennstoffe","CHF",123,"Schiedel PRIMA PLUS",0.2,0,"J","PPL 200 Couvercle pour haute température ","PPL 200 Revisionsdeckel für Festbrennstoffe","PPL 200 Chiusura per combustibilie solidi",131,1,"DN 200",null,106.7,"255160020","105931","4037494431887",123,"100742",16.299999999999997,97,26,"100742",123,16.299999999999997]
["100743",100743,null,"STK","PPL 250 Revisionsdeckel für Festbrennstoffe","CHF",164,"Schiedel PRIMA PLUS",0.3,0,"J","PPL 250 Couvercle pour haute température ","PPL 250 Revisionsdeckel für Festbrennstoffe","PPL 250 Chiusura per combustibilie solidi",131,1,"DN 250",null,141.9,"255160025","105932","4037494431900",164,"100743",22.099999999999994,129,35,"100743",164,22.099999999999994]
["100744",100744,null,"STK","PPL 300 Revisionsdeckel für Festbrennstoffe","CHF",233,"Schiedel PRIMA PLUS",0.35,0,"J","PPL 300 Couvercle pour haute température ","PPL 300 Revisionsdeckel für Festbrennstoffe","PPL 300 Chiusura per combustibilie solidi",131,1,"DN 300",null,202.4,"255160030","105933","4037494431917",233,"100744",30.599999999999994,184,49,"100744",233,30.599999999999994]
["100745",100745,null,"STK","PPL 80 Verschlussdeckel mit Griff","CHF",55,"Schiedel PRIMA PLUS",0.1,0,"J","PPL 80 Couvercle avec poignée ","PPL 80 Verschlussdeckel mit Griff","PPL 80 Tapo cieco",131,1,"DN 80",null,47.3,"265820808","106594","4037494152096",55,"100745",7.7000000000000028,43,12,"100745",55,7.7000000000000028]
["100746",100746,null,"STK","PPL 100 Verschlussdeckel mit Griff","CHF",62,"Schiedel PRIMA PLUS",0.14000000000000001,0,"J","PPL 100 Couvercle avec poignée ","PPL 100 Verschlussdeckel mit Griff","PPL 100 Tapo cieco",131,1,"DN 100",null,53.9,"265820810","106595","4037494152102",62,"100746",8.1000000000000014,49,13,"100746",62,8.1000000000000014]
["100747",100747,null,"STK","PPL 130 Verschlussdeckel mit Griff","CHF",69,"Schiedel PRIMA PLUS",0.2,0,"J","PPL 130 Couvercle avec poignée ","PPL 130 Verschlussdeckel mit Griff","PPL 130 Tapo cieco",131,1,"DN 130",null,59.4,"265820813","106598","4037494152126",69,"100747",9.6000000000000014,54,15,"100747",69,9.6000000000000014]
["100748",100748,null,"STK","PPL 150 Verschlussdeckel mit Griff","CHF",81,"Schiedel PRIMA PLUS",0.24,0,"J","PPL 150 Couvercle avec poignée ","PPL 150 Verschlussdeckel mit Griff","PPL 150 Tapo cieco",131,1,"DN 150",null,70.400000000000006,"265820815","106600","4037494152133",81,"100748",10.599999999999994,64,17,"100748",81,10.599999999999994]
["100749",100749,null,"STK","PPL 180 Verschlussdeckel mit Griff","CHF",97,"Schiedel PRIMA PLUS",0.32,0,"J","PPL 180 Couvercle avec poignée ","PPL 180 Verschlussdeckel mit Griff","PPL 180 Tapo cieco",131,1,"DN 180",null,83.6,"265820818","106602","4037494152140",97,"100749",13.400000000000006,76,21,"100749",97,13.400000000000006]
["100750",100750,null,"STK","PPL 200 Verschlussdeckel mit Griff","CHF",109,"Schiedel PRIMA PLUS",0.55000000000000004,0,"J","PPL 200 Couvercle avec poignée ","PPL 200 Verschlussdeckel mit Griff","PPL 200 Tapo cieco",131,1,"DN 200",null,94.6,"265820820","106603","4037494152157",109,"100750",14.400000000000006,86,23,"100750",109,14.400000000000006]
["100751",100751,null,"STK","PPL 250 Verschlussdeckel mit Griff","CHF",123,"Schiedel PRIMA PLUS",0.27,0,"J","PPL 250 Couvercle avec poignée ","PPL 250 Verschlussdeckel mit Griff","PPL 250 Tapo cieco",131,1,"DN 250",null,106.7,"265820825","106605","4037494152171",123,"100751",16.299999999999997,97,26,"100751",123,16.299999999999997]
["100752",100752,null,"STK","PPL 300 Verschlussdeckel mit Griff","CHF",137,"Schiedel PRIMA PLUS",0.32,0,"J","PPL 300 Couvercle avec poignée ","PPL 300 Verschlussdeckel mit Griff","PPL 300 Tapo cieco",131,1,"DN 300",null,118.8,"265820830","106606","4037494152188",137,"100752",18.200000000000003,108,29,"100752",137,18.200000000000003]
["100753",100753,null,"STK","PPL 350 Verschlussdeckel mit Griff","CHF",164,"Schiedel PRIMA PLUS",0.89,0,"J","PPL 350 Couvercle avec poignée ","PPL 350 Verschlussdeckel mit Griff","PPL 350 Tapo cieco",131,1,"DN 350",null,141.9,"265820835","106607","4037494492260",164,"100753",22.099999999999994,129,35,"100753",164,22.099999999999994]
["100754",100754,null,"STK","PPL 400 Verschlussdeckel mit Griff","CHF",205,"Schiedel PRIMA PLUS",1.0900000000000001,0,"J","PPL 400 Couvercle avec poignée ","PPL 400 Verschlussdeckel mit Griff","PPL 400 Tapo cieco",131,1,"DN 400",null,178.2,"265820840",null,null,205,"100754",26.800000000000011,162,43,"100754",205,26.800000000000011]
["100755",100755,null,"STK","PPL 450 Verschlussdeckel mit Griff","CHF",274,"Schiedel PRIMA PLUS",2.0499999999999998,0,"J","PPL 450 Couvercle avec poignée ","PPL 450 Verschlussdeckel mit Griff","PPL 450 Tapo cieco",131,1,"DN 450",null,237.6,"265820845",null,null,274,"100755",36.400000000000006,216,58,"100755",274,36.400000000000006]
["100756",100756,null,"STK","PPL 500 Verschlussdeckel mit Griff","CHF",342,"Schiedel PRIMA PLUS",2.4300000000000002,0,"J","PPL 500 Couvercle avec poignée ","PPL 500 Verschlussdeckel mit Griff","PPL 500 Tapo cieco",131,1,"DN 500",null,297,"265820850",null,null,342,"100756",45,270,72,"100756",342,45]
["100757",100757,null,"STK","PPL 600 Verschlussdeckel mit Griff","CHF",410,"Schiedel PRIMA PLUS",3.3,0,"J","PPL 600 Couvercle avec poignée ","PPL 600 Verschlussdeckel mit Griff","PPL 600 Tapo cieco",131,1,"DN 600",null,356.4,"265820860",null,null,410,"100757",53.600000000000023,324,86,"100757",410,53.600000000000023]
["100758",100758,null,"STK","PPL 700 Verschlussdeckel mit Griff","CHF",480,"Schiedel PRIMA PLUS",4.29,0,"J","PPL 700 Couvercle avec poignée ","PPL 700 Verschlussdeckel mit Griff","PPL 700 Tapo cieco",131,1,"DN 700",null,416.9,"265820870",null,null,480,"100758",63.100000000000023,379,101,"100758",480,63.100000000000023]
["100759",100759,null,"STK","PPL 130 Zugbergrenzerset zu Basiselement","CHF",397.3,"Schiedel PRIMA PLUS",1.5,0,"J","PPL 130 Set régulateur de triage","PPL 130 Zugbergrenzerset zu Basiselement","PPL 130  Set regulatore di triaggio per basamento",131,1,"DN 130",null,345.4,"26003013",null,null,397.3,"100759",51.900000000000034,314,83.300000000000011,"100759",397.3,51.900000000000034]
["100760",100760,null,"STK","PPL 150 Zugbergrenzerset zu Basiselement","CHF",409.9,"Schiedel PRIMA PLUS",1.5,0,"J","PPL 150 Set régulateur de triage","PPL 150 Zugbergrenzerset zu Basiselement","PPL 150  Set regulatore di triaggio per basamento",131,1,"DN 150",null,356.4,"26003015",null,null,409.9,"100760",53.5,324,85.899999999999977,"100760",409.9,53.5]
["100761",100761,null,"STK","PPL 180 Zugbergrenzerset zu Basiselement","CHF",423.8,"Schiedel PRIMA PLUS",1.5,0,"J","PPL 180 Set régulateur de triage","PPL 180 Zugbergrenzerset zu Basiselement","PPL 180  Set regulatore di triaggio per basamento",131,1,"DN 180",null,368.5,"26003018",null,null,423.8,"100761",55.300000000000011,335,88.800000000000011,"100761",423.8,55.300000000000011]
[{"$f":"B716&\"\"","v":"100762"},100762,null,"STK",{"$f":"IF($E$200=2,L716,IF($E$200=3,N716,M716))","v":"PPL 200 Zugbergrenzerset zu Basiselement"},"CHF",{"$f":"IF($L$190=1,W716,S716)","v":609.79999999999995},"Schiedel PRIMA PLUS",1.5,0,"J","PPL 200 Set régulateur de triage","PPL 200 Zugbergrenzerset zu Basiselement","PPL 200  Set regulatore di triaggio per basamento",131,1,"DN 200",null,530.20000000000005,"26003020",null,null,609.79999999999995,"100762",79.599999999999909,482,127.79999999999995,"100762",609.79999999999995,79.599999999999909]
["100763",100763,null,"STK","PPL 250 Zugbergrenzerset zu Basiselement","CHF",636.29999999999995,"Schiedel PRIMA PLUS",1.5,0,"J","PPL 250 Set régulateur de triage","PPL 250 Zugbergrenzerset zu Basiselement","PPL 250  Set regulatore di triaggio per basamento",131,1,"DN 250",null,553.29999999999995,"26003025",null,null,636.29999999999995,"100763",83,503,133.29999999999995,"100763",636.29999999999995,83]
["100764",100764,null,"STK","PPL 130 Zugbergrenzer","CHF",304.89999999999998,"Schiedel PRIMA PLUS",0.7,0,"J","PPL 130 régulateur de triage","PPL 130 Zugbergrenzer","PPL 130 Regulatore di triaggio",131,1,"DN 130",null,265.10000000000002,"255300001","101697","4037494266458",304.89999999999998,"100764",39.799999999999955,241,63.899999999999977,"100764",304.89999999999998,39.799999999999955]
["100765",100765,null,"STK","PPL 180 Zugbergrenzer","CHF",464.3,"Schiedel PRIMA PLUS",1.05,0,"J","PPL 180 régulateur de triage","PPL 180 Zugbergrenzer","PPL 180 Regulatore di triaggio",131,1,"DN 180",null,403.7,"255300002","101698","4037494266465",464.3,"100765",60.600000000000023,367,97.300000000000011,"100765",464.3,60.600000000000023]
["100766",100766,null,"STK","PPL 130 Basiselement-Adapter für Zugbegrenzer","CHF",92.4,"Schiedel PRIMA PLUS",0.23300000000000001,0,"J","PPL 130 Adapteur pour régulateur de triage","PPL 130 Basiselement-Adapter für Zugbegrenzer","PPL 130 Raccordo regulatore per elem. basamento ",131,1,"DN 130",null,80.3,"267081313","103660","4037494153055",92.4,"100766",12.100000000000009,73,19.400000000000006,"100766",92.4,12.100000000000009]
["100767",100767,null,"STK","PPL 150 Basiselement-Adapter für Zugbegrenzer","CHF",105,"Schiedel PRIMA PLUS",0.26300000000000001,0,"J","PPL 150 Adapteur pour régulateur de triage","PPL 150 Basiselement-Adapter für Zugbegrenzer","PPL 150 Raccordo regulatore per elem. basamento ",131,1,"DN 150",null,91.3,"267081315","103661","4037494153062",105,"100767",13.700000000000003,83,22,"100767",105,13.700000000000003]
["100768",100768,null,"STK","PPL 180 Basiselement-Adapter für Zugbegrenzer","CHF",119,"Schiedel PRIMA PLUS",0.38200000000000001,0,"J","PPL 180 Adapteur pour régulateur de triage","PPL 180 Basiselement-Adapter für Zugbegrenzer","PPL 180 Raccordo regulatore per elem. basamento ",131,1,"DN 180",null,103.4,"267081318","103662","4037494153079",119,"100768",15.599999999999994,94,25,"100768",119,15.599999999999994]
["100769",100769,null,"STK","PPL 200 Basiselement-Adapter für Zugbegrenzer","CHF",145.5,"Schiedel PRIMA PLUS",0.374,0,"J","PPL 200 Adapteur pour régulateur de triage","PPL 200 Basiselement-Adapter für Zugbegrenzer","PPL 200 Raccordo regulatore per elem. basamento ",131,1,"DN 200",null,126.5,"267081820","103663","4037494153086",145.5,"100769",19,115,30.5,"100769",145.5,19]
["100770",100770,null,"STK","PPL 250 Basiselement-Adapter für Zugbegrenzer","CHF",172.1,"Schiedel PRIMA PLUS",0.53400000000000003,0,"J","PPL 250 Adapteur pour régulateur de triage","PPL 250 Basiselement-Adapter für Zugbegrenzer","PPL 250 Raccordo regulatore per elem. basamento ",131,1,"DN 250",null,149.6,"267081825","103664","4037494153093",172.1,"100770",22.5,136,36.099999999999994,"100770",172.1,22.5]
["100771",100771,null,"STK","PPL 130 Putztüranschluss eckig mit Innentüre ","CHF",192,"Schiedel PRIMA PLUS",3.1219999999999999,325,"J","PPL 130 Porte de révision rectangulaire","PPL 130 Putztüranschluss eckig mit Innentüre ","PPL 130 Elemento per porte d'inspezione",131,1,"DN 130",null,166.1,"235300513","106516","4037494900727",192,"100771",25.900000000000006,151,41,"100771",192,25.900000000000006]
["100772",100772,null,"STK","PPL 150 Putztüranschluss eckig mit Innentüre ","CHF",205,"Schiedel PRIMA PLUS",3.4079999999999999,325,"J","PPL 150 Porte de révision rectangulaire","PPL 150 Putztüranschluss eckig mit Innentüre ","PPL 150 Elemento per porte d'inspezione",131,1,"DN 150",null,178.2,"235300515","106518","4037494900741",205,"100772",26.800000000000011,162,43,"100772",205,26.800000000000011]
["100773",100773,null,"STK","PPL 180 Putztüranschluss eckig mit Innentüre ","CHF",219,"Schiedel PRIMA PLUS",3.806,325,"J","PPL 180 Porte de révision rectangulaire","PPL 180 Putztüranschluss eckig mit Innentüre ","PPL 180 Elemento per porte d'inspezione",131,1,"DN 180",null,190.3,"235300518","106520","4037494900765",219,"100773",28.699999999999989,173,46,"100773",219,28.699999999999989]
["100774",100774,null,"STK","PPL 200 Putztüranschluss eckig mit Innentüre ","CHF",233,"Schiedel PRIMA PLUS",4.0549999999999997,325,"J","PPL 200 Porte de révision rectangulaire","PPL 200 Putztüranschluss eckig mit Innentüre ","PPL 200 Elemento per porte d'inspezione",131,1,"DN 200",null,202.4,"235300520","106521","4037494900772",233,"100774",30.599999999999994,184,49,"100774",233,30.599999999999994]
["100775",100775,null,"STK","PPL 250 Putztüranschluss eckig mit Innentüre ","CHF",246,"Schiedel PRIMA PLUS",4.6840000000000002,325,"J","PPL 250 Porte de révision rectangulaire","PPL 250 Putztüranschluss eckig mit Innentüre ","PPL 250 Elemento per porte d'inspezione",131,1,"DN 250",null,213.4,"235300525","106523","4037494900796",246,"100775",32.599999999999994,194,52,"100775",246,32.599999999999994]
["100776",100776,null,"STK","PPL 300 Putztüranschluss eckig mit Innentüre ","CHF",274,"Schiedel PRIMA PLUS",5.3710000000000004,325,"J","PPL 300 Porte de révision rectangulaire","PPL 300 Putztüranschluss eckig mit Innentüre ","PPL 300 Elemento per porte d'inspezione",131,1,"DN 300",null,237.6,"235300530","106524","4037494900802",274,"100776",36.400000000000006,216,58,"100776",274,36.400000000000006]
["100777",100777,null,"STK","PPL 350 Putztüranschluss eckig mit Innentüre ","CHF",342,"Schiedel PRIMA PLUS",3.4980000000000002,325,"J","PPL 350 Porte de révision rectangulaire","PPL 350 Putztüranschluss eckig mit Innentüre ","PPL 350 Elemento per porte d'inspezione",131,1,"DN 350",null,297,"235300535","106525","4037494900819",342,"100777",45,270,72,"100777",342,45]
["100778",100778,null,"STK","PPL 400 Putztüranschluss eckig mit Innentüre ","CHF",480,"Schiedel PRIMA PLUS",3.8719999999999999,325,"J","PPL 400 Porte de révision rectangulaire","PPL 400 Putztüranschluss eckig mit Innentüre ","PPL 400 Elemento per porte d'inspezione",131,1,"DN 400",null,416.9,"235300540",null,null,480,"100778",63.100000000000023,379,101,"100778",480,63.100000000000023]
["100779",100779,null,"STK","PPL 450 Putztüranschluss eckig mit Innentüre ","CHF",547,"Schiedel PRIMA PLUS",4.3499999999999996,325,"J","PPL 450 Porte de révision rectangulaire","PPL 450 Putztüranschluss eckig mit Innentüre ","PPL 450 Elemento per porte d'inspezione",131,1,"DN 450",null,475.2,"235300545",null,null,547,"100779",71.800000000000011,432,115,"100779",547,71.800000000000011]
["100780",100780,null,"STK","PPL 500 Putztüranschluss eckig mit Innentüre ","CHF",684,"Schiedel PRIMA PLUS",4.8239999999999998,325,"J","PPL 500 Porte de révision rectangulaire","PPL 500 Putztüranschluss eckig mit Innentüre ","PPL 500 Elemento per porte d'inspezione",131,1,"DN 500",null,594,"235300550",null,null,684,"100780",90,540,144,"100780",684,90]
["100781",100781,null,"STK","PPL 600 Putztüranschluss eckig mit Innentüre ","CHF",820,"Schiedel PRIMA PLUS",5.7770000000000001,325,"J","PPL 600 Porte de révision rectangulaire","PPL 600 Putztüranschluss eckig mit Innentüre ","PPL 600 Elemento per porte d'inspezione",131,1,"DN 600",null,712.8,"235300560",null,null,820,"100781",107.20000000000005,648,172,"100781",820,107.20000000000005]
["100782",100782,null,"STK","PPL 700 Putztüranschluss eckig mit Innentüre ","CHF",1095,"Schiedel PRIMA PLUS",6.7329999999999997,325,"J","PPL 700 Porte de révision rectangulaire","PPL 700 Putztüranschluss eckig mit Innentüre ","PPL 700 Elemento per porte d'inspezione",131,1,"DN 700",null,951.5,"235300570",null,null,1095,"100782",143.5,865,230,"100782",1095,143.5]
["100783",100783,null,"STK","PPL Putztüre 150 x 200mm zu Putztüranschluss eckig","CHF",137,"Schiedel PRIMA PLUS",1.8,0,"J","PPL Porte de révision150 x 200mm ","PPL Putztüre 150 x 200mm zu Putztüranschluss eckig","PPL Portina die revisione150 x 200mm",131,1,"PPL ZBH",null,118.8,"4008001","103488","4037494490518",137,"100783",18.200000000000003,108,29,"100783",137,18.200000000000003]
["100784",100784,null,"STK","PPL Verlängerung zu Putztüre eckig  155 x 215mm ","CHF",137,"Schiedel PRIMA PLUS",1.31,0,"J","PPL Verlängerung zu Putztüre eckig  155 x 215mm ","PPL Verlängerung zu Putztüre eckig  155 x 215mm ","PPL enlargem. per portina revisione  155 x 215mm ",131,1,"PPL ZBH",null,118.8,"4008000","103487","5035944624321",137,"100784",18.200000000000003,108,29,"100784",137,18.200000000000003]
["100785",100785,null,"STK","PPL 80-130 Putztüre 150 x 200mm gasdicht","CHF",109,"Schiedel PRIMA PLUS",1.4,0,"J","PPL 80-130 Putztüre 150 x 200mm gasdicht","PPL 80-130 Putztüre 150 x 200mm gasdicht","PPL 80-130 Portina 150 x 200mm ",131,1,"DN 80",null,94.6,"255100504","103574","4037494267769",109,"100785",14.400000000000006,86,23,"100785",109,14.400000000000006]
["100786",100786,null,"STK","PPL 80-130 Montagerahmen L150mm","CHF",81,"Schiedel PRIMA PLUS",0.5,0,"J","PPL 80-130 Montagerahmen L150mm","PPL 80-130 Montagerahmen L150mm","PPL 80-130 Telalio prolungha per portina L150mm",131,1,"DN 80",null,70.400000000000006,"255100604","103579","4037494267783",81,"100786",10.599999999999994,64,17,"100786",81,10.599999999999994]
["100787",100787,null,"STK","PPL 80-130 Montagerahmen L250mm","CHF",97,"Schiedel PRIMA PLUS",0.7,0,"J","PPL 80-130 Montagerahmen L250mm","PPL 80-130 Montagerahmen L250mm","PPL 80-130 Telalio prolungha per portina L250mm",131,1,"DN 80",null,83.6,"255100614","103582","4037494271438",97,"100787",13.400000000000006,76,21,"100787",97,13.400000000000006]
["100788",100788,null,"STK","PPL 150-700 Putztüre 200 x 300mm gasdicht","CHF",179,"Schiedel PRIMA PLUS",2.2799999999999998,0,"J","PPL 150-700 Putztüre 200 x 300mm gasdicht","PPL 150-700 Putztüre 200 x 300mm gasdicht","PPL 150-700 Prtina 200 x 300mm ",131,1,"DN 150",null,155.1,"255100505","103575","4037494267776",179,"100788",23.900000000000006,141,38,"100788",179,23.900000000000006]
["100789",100789,null,"STK","PPL 150-700 Montagerahmen L150mm","CHF",109,"Schiedel PRIMA PLUS",0.7,0,"J","PPL 150-700 Montagerahmen L150mm","PPL 150-700 Montagerahmen L150mm","PPL 150-700 Telalio di monatgio L150mm",131,1,"DN 150",null,94.6,"255100605","103580","4037494267790",109,"100789",14.400000000000006,86,23,"100789",109,14.400000000000006]
["100790",100790,null,"STK","PPL 150-700 Montagerahmen L250mm","CHF",123,"Schiedel PRIMA PLUS",1.2,0,"J","PPL 150-700 Montagerahmen L250mm","PPL 150-700 Montagerahmen L250mm","PPL 150-700 Telalio di monatgio L250mm",131,1,"DN 150",null,106.7,"255100615","103583","4037494267806",123,"100790",16.299999999999997,97,26,"100790",123,16.299999999999997]
["100791",100791,null,"STK","PPL 80-130 Zuluft-Türe 140 x 200mm","CHF",123,"Schiedel PRIMA PLUS",1.4,0,"J","PPL 80-130 Zuluft-Türe 140 x 200mm","PPL 80-130 Zuluft-Türe 140 x 200mm","PPL 80-130 Portina griglia 140 x 200mm",131,1,"DN 80",null,106.7,"255100511","103576","4037494149751",123,"100791",16.299999999999997,97,26,"100791",123,16.299999999999997]
["100792",100792,null,"STK","PPL 150-700 Zuluft-Türe 200 x 300mm","CHF",137,"Schiedel PRIMA PLUS",2.2799999999999998,0,"J","PPL 150-700 Zuluft-Türe 200 x 300mm","PPL 150-700 Zuluft-Türe 200 x 300mm","PPL 150-700 Portina griglia 200 x 300mm",131,1,"DN 150",null,118.8,"255100512","103577","4037494149768",137,"100792",18.200000000000003,108,29,"100792",137,18.200000000000003]
["100794",100794,null,"STK","PPL 80 T-Stück 85° L 283mm","CHF",97,"Schiedel PRIMA PLUS",0.498,283,"J","PPL 80 Pièce Té 85° L 283mm","PPL 80 T-Stück 85° L 283mm","PPL 80 Pezzo T 85° L 283mm",131,1,"DN 80",null,83.6,"231308508",null,null,97,"100794",13.400000000000006,76,21,"100794",97,13.400000000000006]
["100795",100795,null,"STK","PPL 100 T-Stück 85° L 283mm","CHF",109,"Schiedel PRIMA PLUS",0.61799999999999999,283,"J","PPL 100 Pièce Té 85° L 283mm","PPL 100 T-Stück 85° L 283mm","PPL 100 Pezzo T 85° L 283mm",131,1,"DN 100",null,94.6,"231308510",null,null,109,"100795",14.400000000000006,86,23,"100795",109,14.400000000000006]
["100796",100796,null,"STK","PPL 130 T-Stück 85° L 283mm","CHF",123,"Schiedel PRIMA PLUS",0.79400000000000004,283,"J","PPL 130 Pièce Té 85° L 283mm","PPL 130 T-Stück 85° L 283mm","PPL 130 Pezzo T 85° L 283mm",131,1,"DN 130",null,106.7,"231308513",null,null,123,"100796",16.299999999999997,97,26,"100796",123,16.299999999999997]
["100797",100797,null,"STK","PPL 150 T-Stück 85° L325mm","CHF",137,"Schiedel PRIMA PLUS",1.0049999999999999,325,"J","PPL 150 Pièce Té 85° L325mm","PPL 150 T-Stück 85° L325mm","PPL 150 Pezzo T 85° L325mm",131,1,"DN 150",null,118.8,"231308515",null,null,137,"100797",18.200000000000003,108,29,"100797",137,18.200000000000003]
["100798",100798,null,"STK","PPL 180 T-Stück 85° L450mm","CHF",151,"Schiedel PRIMA PLUS",1.534,450,"J","PPL 180 Pièce Té 85° L 450mm","PPL 180 T-Stück 85° L450mm","PPL 180 Pezzo T 85° L 450mm",131,1,"DN 180",null,130.9,"231308518",null,null,151,"100798",20.099999999999994,119,32,"100798",151,20.099999999999994]
["100799",100799,null,"STK","PPL 200 T-Stück 85° L450mm","CHF",179,"Schiedel PRIMA PLUS",1.6970000000000001,450,"J","PPL 200 Pièce Té 85° L 450mm","PPL 200 T-Stück 85° L450mm","PPL 200 Pezzo T 85° L 450mm",131,1,"DN 200",null,155.1,"231308520",null,null,179,"100799",23.900000000000006,141,38,"100799",179,23.900000000000006]
["100800",100800,null,"STK","PPL 250 T-Stück 85° L450mm","CHF",219,"Schiedel PRIMA PLUS",2.09,450,"J","PPL 250 Pièce Té 85° L 450mm","PPL 250 T-Stück 85° L450mm","PPL 250 Pezzo T 85° L 450mm",131,1,"DN 250",null,190.3,"231308525",null,null,219,"100800",28.699999999999989,173,46,"100800",219,28.699999999999989]
["100801",100801,null,"STK","PPL 300 T-Stück 85° L450mm","CHF",300,"Schiedel PRIMA PLUS",2.4750000000000001,450,"J","PPL 300 Pièce Té 85° L 450mm","PPL 300 T-Stück 85° L450mm","PPL 300 Pezzo T 85° L 450mm",131,1,"DN 300",null,260.7,"231308530",null,null,300,"100801",39.300000000000011,237,63,"100801",300,39.300000000000011]
["100802",100802,null,"STK","PPL 80 T-Stück 90° L 283mm","CHF",97,"Schiedel PRIMA PLUS",0.5,283,"J","PPL 80 Pièce Té 90° L 283mm","PPL 80 T-Stück 90° L 283mm","PPL 80 Pezzo T 90° L 283mm",131,1,"DN 80",null,83.6,"231309008","106496","4037494147047",97,"100802",13.400000000000006,76,21,"100802",97,13.400000000000006]
["100803",100803,null,"STK","PPL 100 T-Stück 90° L 283mm","CHF",109,"Schiedel PRIMA PLUS",0.62,283,"J","PPL 100 Pièce Té 90° L 283mm","PPL 100 T-Stück 90° L 283mm","PPL 100 Pezzo T 90° L 283mm",131,1,"DN 100",null,94.6,"231309010","106497","4037494147054",109,"100803",14.400000000000006,86,23,"100803",109,14.400000000000006]
["100804",100804,null,"STK","PPL 130 T-Stück 90° L 283mm","CHF",123,"Schiedel PRIMA PLUS",0.79,283,"J","PPL 130 Pièce Té 90° L 283mm","PPL 130 T-Stück 90° L 283mm","PPL 130 Pezzo T 90° L 283mm",131,1,"DN 130",null,106.7,"231309013","106500","4037494147078",123,"100804",16.299999999999997,97,26,"100804",123,16.299999999999997]
["100805",100805,null,"STK","PPL 150 T-Stück 90° L325mm","CHF",137,"Schiedel PRIMA PLUS",1.01,325,"J","PPL 150 Pièce Té 90° L325mm","PPL 150 T-Stück 90° L325mm","PPL 150 Pezzo T 90° L325mm",131,1,"DN 150",null,118.8,"231309015","106502","4037494147085",137,"100805",18.200000000000003,108,29,"100805",137,18.200000000000003]
["100806",100806,null,"STK","PPL 180 T-Stück 90° L450mm","CHF",151,"Schiedel PRIMA PLUS",1.53,450,"J","PPL 180 Pièce Té 90° L 450mm","PPL 180 T-Stück 90° L450mm","PPL 180 Pezzo T 90° L 450mm",131,1,"DN 180",null,130.9,"231309018","106504","4037494147092",151,"100806",20.099999999999994,119,32,"100806",151,20.099999999999994]
["100807",100807,null,"STK","PPL 200 T-Stück 90° L450mm","CHF",179,"Schiedel PRIMA PLUS",1.7,450,"J","PPL 200 Pièce Té 90° L 450mm","PPL 200 T-Stück 90° L450mm","PPL 200 Pezzo T 90° L 450mm",131,1,"DN 200",null,155.1,"231309020","106505","4037494147108",179,"100807",23.900000000000006,141,38,"100807",179,23.900000000000006]
["100808",100808,null,"STK","PPL 250 T-Stück 90° L450mm","CHF",219,"Schiedel PRIMA PLUS",1.92,450,"J","PPL 250 Pièce Té 90° L 450mm","PPL 250 T-Stück 90° L450mm","PPL 250 Pezzo T 90° L 450mm",131,1,"DN 250",null,190.3,"231309025","106507","4037494147122",219,"100808",28.699999999999989,173,46,"100808",219,28.699999999999989]
["100809",100809,null,"STK","PPL 300 T-Stück 90° L450mm","CHF",300,"Schiedel PRIMA PLUS",2.48,450,"J","PPL 300 Pièce Té 90° L 450mm","PPL 300 T-Stück 90° L450mm","PPL 300 Pezzo T 90° L 450mm",131,1,"DN 300",null,260.7,"231309030","106508","4037494147139",300,"100809",39.300000000000011,237,63,"100809",300,39.300000000000011]
["100810",100810,null,"STK","PPL 350 T-Stück 90° L450mm","CHF",410,"Schiedel PRIMA PLUS",4.74,450,"J","PPL 350 Pièce Té 90° L 450mm","PPL 350 T-Stück 90° L450mm","PPL 350 Pezzo T 90° L 450mm",131,1,"DN 350",null,356.4,"231319035","106838","4037494400289",410,"100810",53.600000000000023,324,86,"100810",410,53.600000000000023]
["100811",100811,null,"STK","PPL 400 T-Stück 90° L530mm","CHF",617,"Schiedel PRIMA PLUS",6.05,530,"J","PPL 400 Pièce Té 90° L 530mm","PPL 400 T-Stück 90° L530mm","PPL 400 Pezzo T 90° L 530mm",131,1,"DN 400",null,535.70000000000005,"231319040","106839","4037494400296",617,"100811",81.299999999999955,487,130,"100811",617,81.299999999999955]
["100812",100812,null,"STK","PPL 450 T-Stück 90° L580mm","CHF",753,"Schiedel PRIMA PLUS",8.99,580,"J","PPL 450 Pièce Té 90° L 580mm","PPL 450 T-Stück 90° L580mm","PPL 450 Pezzo T 90° L 580mm",131,1,"DN 450",null,654.5,"231319045","106840","4037494173541",753,"100812",98.5,595,158,"100812",753,98.5]
["100813",100813,null,"STK","PPL 500 T-Stück 90° L630mm","CHF",958,"Schiedel PRIMA PLUS",10.76,630,"J","PPL 500 Pièce Té 90° L 630mm","PPL 500 T-Stück 90° L630mm","PPL 500 Pezzo T 90° L 630mm",131,1,"DN 500",null,832.7,"231319050","106841","4037494173558",958,"100813",125.29999999999995,757,201,"100813",958,125.29999999999995]
["100814",100814,null,"STK","PPL 600 T-Stück 90° L730mm","CHF",1231,"Schiedel PRIMA PLUS",14.76,730,"J","PPL 600 Pièce Té 90° L 730mm","PPL 600 T-Stück 90° L730mm","PPL 600 Pezzo T 90° L 730mm",131,1,"DN 600",null,1070.3,"231319060","106842","4037494173572",1231,"100814",160.70000000000005,973,258,"100814",1231,160.70000000000005]
["100815",100815,null,"STK","PPL 700 T-Stück 90° L830mm","CHF",1505,"Schiedel PRIMA PLUS",19.37,830,"J","PPL 700 Pièce Té 90° L 830mm","PPL 700 T-Stück 90° L830mm","PPL 700 Pezzo T 90° L 830mm",131,1,"DN 700",null,1307.9000000000001,"231319070","106843","4037494147214",1505,"100815",197.09999999999991,1189,316,"100815",1505,197.09999999999991]
["100816",100816,null,"STK","PPL 80 T-Stück 90° mit Putztüre Festbrennstoff","CHF",151,"Schiedel PRIMA PLUS",0.52,283,"J","PPL 80 Pièce Té 90° av. porte ramonage comb.solid","PPL 80 T-Stück 90° mit Putztüre Festbrennstoff","PPL 80 Pezzo T 90° con revisione per com. solidi",131,1,"DN 80",null,130.9,"238300808",null,null,151,"100816",20.099999999999994,119,32,"100816",151,20.099999999999994]
["100817",100817,null,"STK","PPL 100 T-Stück 90° mit Putztüre Festbrennstoff","CHF",164,"Schiedel PRIMA PLUS",0.67,283,"J","PPL 100 Pièce Té 90° av. porte ramonage comb.solid","PPL 100 T-Stück 90° mit Putztüre Festbrennstoff","PPL 100 Pezzo T 90° con revisione per com. solidi",131,1,"DN 100",null,141.9,"238300810",null,null,164,"100817",22.099999999999994,129,35,"100817",164,22.099999999999994]
["100818",100818,null,"STK","PPL 130 T-Stück 90° mit Putztüre Festbrennstoff","CHF",179,"Schiedel PRIMA PLUS",0.91,283,"J","PPL 130 Pièce Té 90° av. porte ramonage comb.solid","PPL 130 T-Stück 90° mit Putztüre Festbrennstoff","PPL 130 Pezzo T 90° con revisione per com. solidi",131,1,"DN 130",null,155.1,"238300813",null,null,179,"100818",23.900000000000006,141,38,"100818",179,23.900000000000006]
["100819",100819,null,"STK","PPL 150 T-Stück 90° mit Putztüre Festbrennstoff","CHF",192,"Schiedel PRIMA PLUS",1.18,325,"J","PPL 150 Pièce Té 90° av. porte ramonage comb.solid","PPL 150 T-Stück 90° mit Putztüre Festbrennstoff","PPL 150 Pezzo T 90° con revisione per com. solidi",131,1,"DN 150",null,166.1,"238300815",null,null,192,"100819",25.900000000000006,151,41,"100819",192,25.900000000000006]
["100820",100820,null,"STK","PPL 180 T-Stück 90° mit Putztüre Festbrennstoff","CHF",205,"Schiedel PRIMA PLUS",1.82,450,"J","PPL 180 Pièce Té 90° av. porte ramonage comb.solid","PPL 180 T-Stück 90° mit Putztüre Festbrennstoff","PPL 180 Pezzo T 90° con revisione per com. solidi",131,1,"DN 180",null,178.2,"238300818",null,null,205,"100820",26.800000000000011,162,43,"100820",205,26.800000000000011]
["100821",100821,null,"STK","PPL 200 T-Stück 90° mit Putztüre Festbrennstoff","CHF",219,"Schiedel PRIMA PLUS",2.0499999999999998,450,"J","PPL 200 Pièce Té 90° av. porte ramonage comb.solid","PPL 200 T-Stück 90° mit Putztüre Festbrennstoff","PPL 200 Pezzo T 90° con revisione per com. solidi",131,1,"DN 200",null,190.3,"238300820",null,null,219,"100821",28.699999999999989,173,46,"100821",219,28.699999999999989]
["100822",100822,null,"STK","PPL 250 T-Stück 90° mit Putztüre Festbrennstoff","CHF",246,"Schiedel PRIMA PLUS",2.65,450,"J","PPL 250 Pièce Té 90° av. porte ramonage comb.solid","PPL 250 T-Stück 90° mit Putztüre Festbrennstoff","PPL 250 Pezzo T 90° con revisione per com. solidi",131,1,"DN 250",null,213.4,"238300825",null,null,246,"100822",32.599999999999994,194,52,"100822",246,32.599999999999994]
["100823",100823,null,"STK","PPL 300 T-Stück 90° mit Putztüre Festbrennstoff","CHF",274,"Schiedel PRIMA PLUS",3.31,450,"J","PPL 300 Pièce Té 90° av. porte ramonage comb.solid","PPL 300 T-Stück 90° mit Putztüre Festbrennstoff","PPL 300 Pezzo T 90° con revisione per com. solidi",131,1,"DN 300",null,237.6,"238300830",null,null,274,"100823",36.400000000000006,216,58,"100823",274,36.400000000000006]
["100824",100824,null,"STK","PPL 80 T-Stück 45° L283mm","CHF",179,"Schiedel PRIMA PLUS",0.57399999999999995,283,"J","PPL 80 Pièce Té 45° L 283mm","PPL 80 T-Stück 45° L283mm","PPL 80 Pezzo T 45° L 283mm",131,1,"DN 80",null,155.1,"231304508","106478","4037494147221",179,"100824",23.900000000000006,141,38,"100824",179,23.900000000000006]
["100825",100825,null,"STK","PPL 100 T-Stück 45° L283mm","CHF",192,"Schiedel PRIMA PLUS",0.72799999999999998,283,"J","PPL 100 Pièce Té 45° L 283mm","PPL 100 T-Stück 45° L283mm","PPL 100 Pezzo T 45° L 283mm",131,1,"DN 100",null,166.1,"231304510","106479","4037494147238",192,"100825",25.900000000000006,151,41,"100825",192,25.900000000000006]
["100826",100826,null,"STK","PPL 130 T-Stück 45° L325mm","CHF",205,"Schiedel PRIMA PLUS",1.0629999999999999,325,"J","PPL 130 Pièce Té 45° L325mm","PPL 130 T-Stück 45° L325mm","PPL 130 Pezzo T 45° L325mm",131,1,"DN 130",null,178.2,"231304513","106482","4037494147252",205,"100826",26.800000000000011,162,43,"100826",205,26.800000000000011]
[{"$f":"B780&\"\"","v":"100827"},100827,null,"STK",{"$f":"IF($E$200=2,L780,IF($E$200=3,N780,M780))","v":"PPL 150 T-Stück 45° L325mm"},"CHF",{"$f":"IF($L$190=1,W780,S780)","v":246},"Schiedel PRIMA PLUS",1.256,325,"J","PPL 150 Pièce Té 45° L325mm","PPL 150 T-Stück 45° L325mm","PPL 150 Pezzo T 45° L325mm",131,1,"DN 150",null,213.4,"231304515","106484","4037494147269",246,"100827",32.599999999999994,194,52,"100827",246,32.599999999999994]
["100828",100828,null,"STK","PPL 180 T-Stück 45° L450mm","CHF",274,"Schiedel PRIMA PLUS",1.9219999999999999,450,"J","PPL 180 Pièce Té 45° L 450mm","PPL 180 T-Stück 45° L450mm","PPL 180 Pezzo T 45° L 450mm",131,1,"DN 180",null,237.6,"231304518","106486","4037494147276",274,"100828",36.400000000000006,216,58,"100828",274,36.400000000000006]
["100829",100829,null,"STK","PPL 200 T-Stück 45° L450mm","CHF",300,"Schiedel PRIMA PLUS",2.17,450,"J","PPL 200 Pièce Té 45° L 450mm","PPL 200 T-Stück 45° L450mm","PPL 200 Pezzo T 45° L 450mm",131,1,"DN 200",null,260.7,"231304520","106487","4037494147283",300,"100829",39.300000000000011,237,63,"100829",300,39.300000000000011]
["100830",100830,null,"STK","PPL 250 T-Stück 45° L540mm","CHF",370,"Schiedel PRIMA PLUS",3.2320000000000002,540,"J","PPL 250 Pièce Té 45° L 540mm","PPL 250 T-Stück 45° L540mm","PPL 250 Pezzo T 45° L 540mm",131,1,"DN 250",null,321.2,"231304525","106489","4037494147306",370,"100830",48.800000000000011,292,78,"100830",370,48.800000000000011]
["100831",100831,null,"STK","PPL 300 T-Stück 45° L617mm","CHF",480,"Schiedel PRIMA PLUS",4.3659999999999997,617,"J","PPL 300 Pièce Té 45° L 617mm","PPL 300 T-Stück 45° L617mm","PPL 300 Pezzo T 45° L 617mm",131,1,"DN 300",null,416.9,"231304530","106490","4037494147313",480,"100831",63.100000000000023,379,101,"100831",480,63.100000000000023]
["100832",100832,null,"STK","PPL 350 T-Stück 45° L617mm","CHF",753,"Schiedel PRIMA PLUS",8.4700000000000006,617,"J","PPL 350 Pièce Té 45° L 617mm","PPL 350 T-Stück 45° L617mm","PPL 350 Pezzo T 45° L 617mm",131,1,"DN 350",null,654.5,"231314535","106824","4037494400487",753,"100832",98.5,595,158,"100832",753,98.5]
["100833",100833,null,"STK","PPL 400 T-Stück 45° L710mm","CHF",1026,"Schiedel PRIMA PLUS",10.987,710,"J","PPL 400 Pièce Té 45° L 710mm","PPL 400 T-Stück 45° L710mm","PPL 400 Pezzo T 45° L 710mm",131,1,"DN 400",null,892.1,"231314540","106825","4037494400494",1026,"100833",133.89999999999998,811,215,"100833",1026,133.89999999999998]
["100834",100834,null,"STK","PPL 450 T-Stück 45° L780mm","CHF",1300,"Schiedel PRIMA PLUS",12.58,780,"J","PPL 450 Pièce Té 45° L 780mm","PPL 450 T-Stück 45° L780mm","PPL 450 Pezzo T 45° L 780mm",131,1,"DN 450",null,1129.7,"231314545","106826","4037494173596",1300,"100834",170.29999999999995,1027,273,"100834",1300,170.29999999999995]
["100835",100835,null,"STK","PPL 500 T-Stück 45° L850mm","CHF",1574,"Schiedel PRIMA PLUS",15.962999999999999,850,"J","PPL 500 Pièce Té 45° L 850mm","PPL 500 T-Stück 45° L850mm","PPL 500 Pezzo T 45° L 850mm",131,1,"DN 500",null,1368.4,"231314550","106827","4037494173602",1574,"100835",205.59999999999991,1244,330,"100835",1574,205.59999999999991]
["100836",100836,null,"STK","PPL 600 T-Stück 45° L1030mm","CHF",1984,"Schiedel PRIMA PLUS",21.591999999999999,1030,"J","PPL 600 Pièce Té 45° L 1030mm","PPL 600 T-Stück 45° L1030mm","PPL 600 Pezzo T 45° L 1030mm",131,1,"DN 600",null,1724.8,"231314560","106828","4037494173626",1984,"100836",259.20000000000005,1568,416,"100836",1984,259.20000000000005]
["100837",100837,null,"STK","PPL 700 T-Stück 45° L1200mm","CHF",2395,"Schiedel PRIMA PLUS",28.712,1200,"J","PPL 700 Pièce Té 45° L 1200mm","PPL 700 T-Stück 45° L1200mm","PPL 700 Pezzo T 45° L 1200mm",131,1,"DN 700",null,2082.3000000000002,"231314570","106829","4037494147399",2395,"100837",312.69999999999982,1893,502,"100837",2395,312.69999999999982]
["100838",100838,null,"STK","PPL 80 Doppelfutterrohr zu T-Stück L120mm","CHF",62,"Schiedel PRIMA PLUS",0.49,0,"J","PPL 80 double manchon pour pièce Té L120mm","PPL 80 Doppelfutterrohr zu T-Stück L120mm","PPL 80 Doppia parete per pezo T L120mm",131,1,"DN 80",null,53.9,"242030108",null,null,62,"100838",8.1000000000000014,49,13,"100838",62,8.1000000000000014]
["100839",100839,null,"STK","PPL 100 Doppelfutterrohr zu T-Stück L120mm","CHF",69,"Schiedel PRIMA PLUS",0.49,0,"J","PPL 100 double manchon pour pièce Té L120mm","PPL 100 Doppelfutterrohr zu T-Stück L120mm","PPL 100 Doppia parete per pezo T L120mm",131,1,"DN 100",null,59.4,"242030110",null,null,69,"100839",9.6000000000000014,54,15,"100839",69,9.6000000000000014]
["100840",100840,null,"STK","PPL 130 Doppelfutterrohr zu T-Stück L120mm","CHF",75,"Schiedel PRIMA PLUS",0.49,0,"J","PPL 130 double manchon pour pièce Té L120mm","PPL 130 Doppelfutterrohr zu T-Stück L120mm","PPL 130 Doppia parete per pezo T L120mm",131,1,"DN 130",null,64.900000000000006,"242030113","106053","4037494177730",75,"100840",10.099999999999994,59,16,"100840",75,10.099999999999994]
["100841",100841,null,"STK","PPL 150 Doppelfutterrohr zu T-Stück L120mm","CHF",81,"Schiedel PRIMA PLUS",0.49,0,"J","PPL 150 double manchon pour pièce Té L120mm","PPL 150 Doppelfutterrohr zu T-Stück L120mm","PPL 150 Doppia parete per pezo T L120mm",131,1,"DN 150",null,70.400000000000006,"242030115","106054","4037494177747",81,"100841",10.599999999999994,64,17,"100841",81,10.599999999999994]
["100842",100842,null,"STK","PPL 180 Doppelfutterrohr zu T-Stück L120mm","CHF",81,"Schiedel PRIMA PLUS",0.49,0,"J","PPL 180 double manchon pour pièce Té L120mm","PPL 180 Doppelfutterrohr zu T-Stück L120mm","PPL 180 Doppia parete per pezo T L120mm",131,1,"DN 180",null,70.400000000000006,"242030118","106055","4037494177754",81,"100842",10.599999999999994,64,17,"100842",81,10.599999999999994]
["100843",100843,null,"STK","PPL 200 Doppelfutterrohr zu T-Stück L120mm","CHF",90,"Schiedel PRIMA PLUS",0.49,0,"J","PPL 200 double manchon pour pièce Té L120mm","PPL 200 Doppelfutterrohr zu T-Stück L120mm","PPL 200 Doppia parete per pezo T L120mm",131,1,"DN 200",null,78.099999999999994,"242030120","106056","4037494177761",90,"100843",11.900000000000006,71,19,"100843",90,11.900000000000006]
["100844",100844,null,"STK","PPL 250 Doppelfutterrohr zu T-Stück L120mm","CHF",97,"Schiedel PRIMA PLUS",0.49,0,"J","PPL 250 double manchon pour pièce Té L120mm","PPL 250 Doppelfutterrohr zu T-Stück L120mm","PPL 250 Doppia parete per pezo T L120mm",131,1,"DN 250",null,83.6,"242030125","106058","4037494177785",97,"100844",13.400000000000006,76,21,"100844",97,13.400000000000006]
["100845",100845,null,"STK","PPL 300 Doppelfutterrohr zu T-Stück L120mm","CHF",109,"Schiedel PRIMA PLUS",0.49,0,"J","PPL 300 double manchon pour pièce Té L120mm","PPL 300 Doppelfutterrohr zu T-Stück L120mm","PPL 300 Doppia parete per pezo T L120mm",131,1,"DN 300",null,94.6,"242030130","106059","4037494177792",109,"100845",14.400000000000006,86,23,"100845",109,14.400000000000006]
["100846",100846,null,"STK","PPL 80 Längenelement L250mm","CHF",28,"Schiedel PRIMA PLUS",0.3,200,"J","PPL 80 Elément droit L250mm","PPL 80 Längenelement L250mm","PPL 80 Elemento lunghezze L250mm",131,1,"DN 80",null,24.2,"137002508","106193","5035944215697",28,"100846",3.8000000000000007,22,6,"100846",28,3.8000000000000007]
["100847",100847,null,"STK","PPL 100 Längenelement L250mm","CHF",28,"Schiedel PRIMA PLUS",0.38,200,"J","PPL 100 Elément droit L250mm","PPL 100 Längenelement L250mm","PPL 100 Elemento lunghezze L250mm",131,1,"DN 100",null,24.2,"137002510","106194","5035944215703",28,"100847",3.8000000000000007,22,6,"100847",28,3.8000000000000007]
["100848",100848,null,"STK","PPL 130 Längenelement L250mm","CHF",36,"Schiedel PRIMA PLUS",0.49,200,"J","PPL 130 Elément droit L250mm","PPL 130 Längenelement L250mm","PPL 130 Elemento lunghezze L250mm",131,1,"DN 130",null,30.8,"137002513","106197","5035944215734",36,"100848",5.1999999999999993,28,8,"100848",36,5.1999999999999993]
["100849",100849,null,"STK","PPL 150 Längenelement L250mm","CHF",42,"Schiedel PRIMA PLUS",0.56999999999999995,200,"J","PPL 150 Elément droit L250mm","PPL 150 Längenelement L250mm","PPL 150 Elemento lunghezze L250mm",131,1,"DN 150",null,36.299999999999997,"137002515","106199","5035944215758",42,"100849",5.7000000000000028,33,9,"100849",42,5.7000000000000028]
["100850",100850,null,"STK","PPL 180 Längenelement L250mm","CHF",50,"Schiedel PRIMA PLUS",0.68,200,"J","PPL 180 Elément droit L250mm","PPL 180 Längenelement L250mm","PPL 180 Elemento lunghezze L250mm",131,1,"DN 180",null,42.9,"137002518","106201","5035944215772",50,"100850",7.1000000000000014,39,11,"100850",50,7.1000000000000014]
["100851",100851,null,"STK","PPL 200 Längenelement L250mm","CHF",56,"Schiedel PRIMA PLUS",0.76,200,"J","PPL 200 Elément droit L250mm","PPL 200 Längenelement L250mm","PPL 200 Elemento lunghezze L250mm",131,1,"DN 200",null,48.4,"137002520","106202","5035944215789",56,"100851",7.6000000000000014,44,12,"100851",56,7.6000000000000014]
["100852",100852,null,"STK","PPL 250 Längenelement L250mm","CHF",64,"Schiedel PRIMA PLUS",0.95,200,"J","PPL 250 Elément droit L250mm","PPL 250 Längenelement L250mm","PPL 250 Elemento lunghezze L250mm",131,1,"DN 250",null,55,"137002525","106204","5035944215802",64,"100852",9,50,14,"100852",64,9]
["100853",100853,null,"STK","PPL 300 Längenelement L250mm","CHF",70,"Schiedel PRIMA PLUS",1.1399999999999999,200,"J","PPL 300 Elément droit L250mm","PPL 300 Längenelement L250mm","PPL 300 Elemento lunghezze L250mm",131,1,"DN 300",null,60.5,"137002530","106205","5035944215819",70,"100853",9.5,55,15,"100853",70,9.5]
["100854",100854,null,"STK","PPL 350 Längenelement L250mm","CHF",98,"Schiedel PRIMA PLUS",2.21,200,"J","PPL 350 Elément droit L250mm","PPL 350 Längenelement L250mm","PPL 350 Elemento lunghezze L250mm",131,1,"DN 350",null,84.7,"137102535","106630","4037494400784",98,"100854",13.299999999999997,77,21,"100854",98,13.299999999999997]
["100855",100855,null,"STK","PPL 400 Längenelement L250mm","CHF",138,"Schiedel PRIMA PLUS",2.5099999999999998,200,"J","PPL 400 Elément droit L250mm","PPL 400 Längenelement L250mm","PPL 400 Elemento lunghezze L250mm",131,1,"DN 400",null,119.9,"137102540","106631","4037494400791",138,"100855",18.099999999999994,109,29,"100855",138,18.099999999999994]
["100856",100856,null,"STK","PPL 450 Längenelement L250mm","CHF",180,"Schiedel PRIMA PLUS",2.83,200,"J","PPL 450 Elément droit L250mm","PPL 450 Längenelement L250mm","PPL 450 Elemento lunghezze L250mm",131,1,"DN 450",null,156.19999999999999,"137102545","106632","4037494173732",180,"100856",23.800000000000011,142,38,"100856",180,23.800000000000011]
["100857",100857,null,"STK","PPL 500 Längenelement L250mm","CHF",221,"Schiedel PRIMA PLUS",3.14,200,"J","PPL 500 Elément droit L250mm","PPL 500 Längenelement L250mm","PPL 500 Elemento lunghezze L250mm",131,1,"DN 500",null,191.4,"137102550","106633","4037494173749",221,"100857",29.599999999999994,174,47,"100857",221,29.599999999999994]
["100858",100858,null,"STK","PPL 600 Längenelement L250mm","CHF",275,"Schiedel PRIMA PLUS",3.77,200,"J","PPL 600 Elément droit L250mm","PPL 600 Längenelement L250mm","PPL 600 Elemento lunghezze L250mm",131,1,"DN 600",null,238.7,"137102560","106634","4037494173763",275,"100858",36.300000000000011,217,58,"100858",275,36.300000000000011]
["100859",100859,null,"STK","PPL 700 Längenelement L250mm","CHF",371,"Schiedel PRIMA PLUS",4.4000000000000004,200,"J","PPL 700 Elément droit L250mm","PPL 700 Längenelement L250mm","PPL 700 Elemento lunghezze L250mm",131,1,"DN 700",null,322.3,"137102570","106635","4037494173770",371,"100859",48.699999999999989,293,78,"100859",371,48.699999999999989]
["100860",100860,null,"STK","PPL 80 Längenelement L500mm","CHF",42,"Schiedel PRIMA PLUS",0.61,450,"J","PPL 80 Elément droit L500mm","PPL 80 Längenelement L500mm","PPL 80 Elemento lunghezze L500mm",131,1,"DN 80",null,36.299999999999997,"137005008","106207","5035944215529",42,"100860",5.7000000000000028,33,9,"100860",42,5.7000000000000028]
["100861",100861,null,"STK","PPL 100 Längenelement L500mm","CHF",50,"Schiedel PRIMA PLUS",0.76,450,"J","PPL 100 Elément droit L500mm","PPL 100 Längenelement L500mm","PPL 100 Elemento lunghezze L500mm",131,1,"DN 100",null,42.9,"137005010","106208","5035944215536",50,"100861",7.1000000000000014,39,11,"100861",50,7.1000000000000014]
["100862",100862,null,"STK","PPL 130 Längenelement L500mm","CHF",56,"Schiedel PRIMA PLUS",0.99,450,"J","PPL 130 Elément droit L500mm","PPL 130 Längenelement L500mm","PPL 130 Elemento lunghezze L500mm",131,1,"DN 130",null,48.4,"137005013","106211","5035944215567",56,"100862",7.6000000000000014,44,12,"100862",56,7.6000000000000014]
["100863",100863,null,"STK","PPL 150 Längenelement L500mm","CHF",64,"Schiedel PRIMA PLUS",1.1399999999999999,450,"J","PPL 150 Elément droit L500mm","PPL 150 Längenelement L500mm","PPL 150 Elemento lunghezze L500mm",131,1,"DN 150",null,55,"137005015","106213","5035944215581",64,"100863",9,50,14,"100863",64,9]
["100864",100864,null,"STK","PPL 180 Längenelement L500mm","CHF",70,"Schiedel PRIMA PLUS",1.37,450,"J","PPL 180 Elément droit L500mm","PPL 180 Längenelement L500mm","PPL 180 Elemento lunghezze L500mm",131,1,"DN 180",null,60.5,"137005018","106215","5035944215604",70,"100864",9.5,55,15,"100864",70,9.5]
["100865",100865,null,"STK","PPL 200 Längenelement L500mm","CHF",76,"Schiedel PRIMA PLUS",1.52,450,"J","PPL 200 Elément droit L500mm","PPL 200 Längenelement L500mm","PPL 200 Elemento lunghezze L500mm",131,1,"DN 200",null,66,"137005020","106216","5035944215611",76,"100865",10,60,16,"100865",76,10]
["100866",100866,null,"STK","PPL 250 Längenelement L500mm","CHF",83,"Schiedel PRIMA PLUS",1.9,450,"J","PPL 250 Elément droit L500mm","PPL 250 Längenelement L500mm","PPL 250 Elemento lunghezze L500mm",131,1,"DN 250",null,71.5,"137005025","106218","5035944215635",83,"100866",11.5,65,18,"100866",83,11.5]
["100867",100867,null,"STK","PPL 300 Längenelement L500mm","CHF",98,"Schiedel PRIMA PLUS",2.27,450,"J","PPL 300 Elément droit L500mm","PPL 300 Längenelement L500mm","PPL 300 Elemento lunghezze L500mm",131,1,"DN 300",null,84.7,"137005030","106219","5035944215642",98,"100867",13.299999999999997,77,21,"100867",98,13.299999999999997]
["100868",100868,null,"STK","PPL 350 Längenelement L500mm","CHF",152,"Schiedel PRIMA PLUS",4.41,450,"J","PPL 350 Elément droit L500mm","PPL 350 Längenelement L500mm","PPL 350 Elemento lunghezze L500mm",131,1,"DN 350",null,132,"137105035","106644","4037494400685",152,"100868",20,120,32,"100868",152,20]
["100869",100869,null,"STK","PPL 400 Längenelement L500mm","CHF",180,"Schiedel PRIMA PLUS",5.0199999999999996,450,"J","PPL 400 Elément droit L500mm","PPL 400 Längenelement L500mm","PPL 400 Elemento lunghezze L500mm",131,1,"DN 400",null,156.19999999999999,"137105040","106645","4037494400692",180,"100869",23.800000000000011,142,38,"100869",180,23.800000000000011]
["100870",100870,null,"STK","PPL 450 Längenelement L500mm","CHF",221,"Schiedel PRIMA PLUS",5.65,450,"J","PPL 450 Elément droit L500mm","PPL 450 Längenelement L500mm","PPL 450 Elemento lunghezze L500mm",131,1,"DN 450",null,191.4,"137105045","106646","4037494173688",221,"100870",29.599999999999994,174,47,"100870",221,29.599999999999994]
["100871",100871,null,"STK","PPL 500 Längenelement L500mm","CHF",275,"Schiedel PRIMA PLUS",6.28,450,"J","PPL 500 Elément droit L500mm","PPL 500 Längenelement L500mm","PPL 500 Elemento lunghezze L500mm",131,1,"DN 500",null,238.7,"137105050","106647","4037494173695",275,"100871",36.300000000000011,217,58,"100871",275,36.300000000000011]
["100872",100872,null,"STK","PPL 600 Längenelement L500mm","CHF",357,"Schiedel PRIMA PLUS",7.53,450,"J","PPL 600 Elément droit L500mm","PPL 600 Längenelement L500mm","PPL 600 Elemento lunghezze L500mm",131,1,"DN 600",null,310.2,"137105060","106648","4037494173718",357,"100872",46.800000000000011,282,75,"100872",357,46.800000000000011]
["100873",100873,null,"STK","PPL 700 Längenelement L500mm","CHF",439,"Schiedel PRIMA PLUS",8.7899999999999991,450,"J","PPL 700 Elément droit L500mm","PPL 700 Längenelement L500mm","PPL 700 Elemento lunghezze L500mm",131,1,"DN 700",null,381.7,"137105070","106649","4037494173725",439,"100873",57.300000000000011,347,92,"100873",439,57.300000000000011]
["100874",100874,null,"STK","PPL 80 Längenelement L1000mm","CHF",64,"Schiedel PRIMA PLUS",1.22,950,"J","PPL 80 Elément droit L1000mm","PPL 80 Längenelement L1000mm","PPL 80 Elemento lunghezze L1000mm",131,1,"DN 80",null,55,"137010008","106221","5035944215352",64,"100874",9,50,14,"100874",64,9]
["100875",100875,null,"STK","PPL 100 Längenelement L1000mm","CHF",76,"Schiedel PRIMA PLUS",1.52,950,"J","PPL 100 Elément droit L1000mm","PPL 100 Längenelement L1000mm","PPL 100 Elemento lunghezze L1000mm",131,1,"DN 100",null,66,"137010010","106222","5035944215369",76,"100875",10,60,16,"100875",76,10]
["100876",100876,null,"STK","PPL 130 Längenelement L1000mm","CHF",92,"Schiedel PRIMA PLUS",1.98,950,"J","PPL 130 Elément droit L1000mm","PPL 130 Längenelement L1000mm","PPL 130 Elemento lunghezze L1000mm",131,1,"DN 130",null,79.2,"137010013","106225","5035944215390",92,"100876",12.799999999999997,72,20,"100876",92,12.799999999999997]
["100877",100877,null,"STK","PPL 150 Längenelement L1000mm","CHF",104,"Schiedel PRIMA PLUS",2.2799999999999998,950,"J","PPL 150 Elément droit L1000mm","PPL 150 Längenelement L1000mm","PPL 150 Elemento lunghezze L1000mm",131,1,"DN 150",null,90.2,"137010015","106227","5035944215413",104,"100877",13.799999999999997,82,22,"100877",104,13.799999999999997]
["100878",100878,null,"STK","PPL 180 Längenelement L1000mm","CHF",118,"Schiedel PRIMA PLUS",2.73,950,"J","PPL 180 Elément droit L1000mm","PPL 180 Längenelement L1000mm","PPL 180 Elemento lunghezze L1000mm",131,1,"DN 180",null,102.3,"137010018","106229","5035944215437",118,"100878",15.700000000000003,93,25,"100878",118,15.700000000000003]
["100879",100879,null,"STK","PPL 200 Längenelement L1000mm","CHF",131,"Schiedel PRIMA PLUS",3.04,950,"J","PPL 200 Elément droit L1000mm","PPL 200 Längenelement L1000mm","PPL 200 Elemento lunghezze L1000mm",131,1,"DN 200",null,113.3,"137010020","106230","5035944215444",131,"100879",17.700000000000003,103,28,"100879",131,17.700000000000003]
["100880",100880,null,"STK","PPL 250 Längenelement L1000mm","CHF",152,"Schiedel PRIMA PLUS",3.79,950,"J","PPL 250 Elément droit L1000mm","PPL 250 Längenelement L1000mm","PPL 250 Elemento lunghezze L1000mm",131,1,"DN 250",null,132,"137010025","106232","5035944215468",152,"100880",20,120,32,"100880",152,20]
["100881",100881,null,"STK","PPL 300 Längenelement L1000mm","CHF",180,"Schiedel PRIMA PLUS",4.55,950,"J","PPL 300 Elément droit L1000mm","PPL 300 Längenelement L1000mm","PPL 300 Elemento lunghezze L1000mm",131,1,"DN 300",null,156.19999999999999,"137010030","106233","5035944215475",180,"100881",23.800000000000011,142,38,"100881",180,23.800000000000011]
["100882",100882,null,"STK","PPL 350 Längenelement L1000mm","CHF",275,"Schiedel PRIMA PLUS",8.83,950,"J","PPL 350 Elément droit L1000mm","PPL 350 Längenelement L1000mm","PPL 350 Elemento lunghezze L1000mm",131,1,"DN 350",null,238.7,"137110035","106658","4037494400586",275,"100882",36.300000000000011,217,58,"100882",275,36.300000000000011]
["100883",100883,null,"STK","PPL 400 Längenelement L1000mm","CHF",343,"Schiedel PRIMA PLUS",10.039999999999999,950,"J","PPL 400 Elément droit L1000mm","PPL 400 Längenelement L1000mm","PPL 400 Elemento lunghezze L1000mm",131,1,"DN 400",null,298.10000000000002,"137110040","106659","4037494400593",343,"100883",44.899999999999977,271,72,"100883",343,44.899999999999977]
["100884",100884,null,"STK","PPL 450 Längenelement L1000mm","CHF",412,"Schiedel PRIMA PLUS",11.3,950,"J","PPL 450 Elément droit L1000mm","PPL 450 Längenelement L1000mm","PPL 450 Elemento lunghezze L1000mm",131,1,"DN 450",null,357.5,"137110045","106660","4037494173633",412,"100884",54.5,325,87,"100884",412,54.5]
["100885",100885,null,"STK","PPL 500 Längenelement L1000mm","CHF",481,"Schiedel PRIMA PLUS",12.55,950,"J","PPL 500 Elément droit L1000mm","PPL 500 Längenelement L1000mm","PPL 500 Elemento lunghezze L1000mm",131,1,"DN 500",null,418,"137110050","106661","4037494173640",481,"100885",63,380,101,"100885",481,63]
["100886",100886,null,"STK","PPL 600 Längenelement L1000mm","CHF",548,"Schiedel PRIMA PLUS",15.06,950,"J","PPL 600 Elément droit L1000mm","PPL 600 Längenelement L1000mm","PPL 600 Elemento lunghezze L1000mm",131,1,"DN 600",null,476.3,"137110060","106662","4037494173664",548,"100886",71.699999999999989,433,115,"100886",548,71.699999999999989]
["100887",100887,null,"STK","PPL 700 Längenelement L1000mm","CHF",685,"Schiedel PRIMA PLUS",17.579999999999998,950,"J","PPL 700 Elément droit L1000mm","PPL 700 Längenelement L1000mm","PPL 700 Elemento lunghezze L1000mm",131,1,"DN 700",null,595.1,"137110070","106663","4037494173671",685,"100887",89.899999999999977,541,144,"100887",685,89.899999999999977]
["100888",100888,null,"STK","PPL 80 Ablass-Element L200mm","CHF",69,"Schiedel PRIMA PLUS",0.33,200,"J","PPL 80 Elément de montage L200mm","PPL 80 Ablass-Element L200mm","PPL 80 Elemento di montagoi L200mm",131,1,"DN 80",null,59.4,"137002408","106179","4037494147405",69,"100888",9.6000000000000014,54,15,"100888",69,9.6000000000000014]
["100889",100889,null,"STK","PPL 100 Ablass-Element L200mm","CHF",69,"Schiedel PRIMA PLUS",0.41,200,"J","PPL 100 Elément de montage L200mm","PPL 100 Ablass-Element L200mm","PPL 100 Elemento di montagoi L200mm",131,1,"DN 100",null,59.4,"137002410","106180","4037494147412",69,"100889",9.6000000000000014,54,15,"100889",69,9.6000000000000014]
["100890",100890,null,"STK","PPL 130 Ablass-Element L200mm","CHF",75,"Schiedel PRIMA PLUS",0.52,200,"J","PPL 130 Elément de montage L200mm","PPL 130 Ablass-Element L200mm","PPL 130 Elemento di montagoi L200mm",131,1,"DN 130",null,64.900000000000006,"137002413","106183","4037494147436",75,"100890",10.099999999999994,59,16,"100890",75,10.099999999999994]
[{"$f":"B844&\"\"","v":"100891"},100891,null,"STK",{"$f":"IF($E$200=2,L844,IF($E$200=3,N844,M844))","v":"PPL 150 Ablass-Element L200mm"},"CHF",{"$f":"IF($L$190=1,W844,S844)","v":81},"Schiedel PRIMA PLUS",0.6,200,"J","PPL 150 Elément de montage L200mm","PPL 150 Ablass-Element L200mm","PPL 150 Elemento di montagoi L200mm",131,1,"DN 150",null,70.400000000000006,"137002415","106185","4037494147443",81,"100891",10.599999999999994,64,17,"100891",81,10.599999999999994]
["100892",100892,null,"STK","PPL 180 Ablass-Element L200mm","CHF",97,"Schiedel PRIMA PLUS",0.71,200,"J","PPL 180 Elément de montage L200mm","PPL 180 Ablass-Element L200mm","PPL 180 Elemento di montagoi L200mm",131,1,"DN 180",null,83.6,"137002418","106187","4037494147450",97,"100892",13.400000000000006,76,21,"100892",97,13.400000000000006]
["100893",100893,null,"STK","PPL 200 Ablass-Element L200mm","CHF",109,"Schiedel PRIMA PLUS",0.79,200,"J","PPL 200 Elément de montage L200mm","PPL 200 Ablass-Element L200mm","PPL 200 Elemento di montagoi L200mm",131,1,"DN 200",null,94.6,"137002420","106188","4037494147467",109,"100893",14.400000000000006,86,23,"100893",109,14.400000000000006]
["100894",100894,null,"STK","PPL 250 Ablass-Element L200mm","CHF",123,"Schiedel PRIMA PLUS",0.97,200,"J","PPL 250 Elément de montage L200mm","PPL 250 Ablass-Element L200mm","PPL 250 Elemento di montagoi L200mm",131,1,"DN 250",null,106.7,"137002425","106190","4037494147481",123,"100894",16.299999999999997,97,26,"100894",123,16.299999999999997]
["100895",100895,null,"STK","PPL 300 Ablass-Element L200mm","CHF",137,"Schiedel PRIMA PLUS",1.1599999999999999,200,"J","PPL 300 Elément de montage L200mm","PPL 300 Ablass-Element L200mm","PPL 300 Elemento di montagoi L200mm",131,1,"DN 300",null,118.8,"137002430","106191","4037494147498",137,"100895",18.200000000000003,108,29,"100895",137,18.200000000000003]
["100896",100896,null,"STK","PPL 350 Ablass-Element L200mm","CHF",164,"Schiedel PRIMA PLUS",2.25,200,"J","PPL 350 Elément de montage L200mm","PPL 350 Ablass-Element L200mm","PPL 350 Elemento di montagoi L200mm",131,1,"DN 350",null,141.9,"137102435","106616","4037494400883",164,"100896",22.099999999999994,129,35,"100896",164,22.099999999999994]
["100897",100897,null,"STK","PPL 400 Ablass-Element L200mm","CHF",205,"Schiedel PRIMA PLUS",2.5499999999999998,200,"J","PPL 400 Elément de montage L200mm","PPL 400 Ablass-Element L200mm","PPL 400 Elemento di montagoi L200mm",131,1,"DN 400",null,178.2,"137102440","106617","4037494400890",205,"100897",26.800000000000011,162,43,"100897",205,26.800000000000011]
["100898",100898,null,"STK","PPL 450 Ablass-Element L200mm","CHF",260,"Schiedel PRIMA PLUS",2.87,200,"J","PPL 450 Elément de montage L200mm","PPL 450 Ablass-Element L200mm","PPL 450 Elemento di montagoi L200mm",131,1,"DN 450",null,225.5,"137102445","106618","4037494491539",260,"100898",34.5,205,55,"100898",260,34.5]
["100899",100899,null,"STK","PPL 500 Ablass-Element L200mm","CHF",300,"Schiedel PRIMA PLUS",3.18,200,"J","PPL 500 Elément de montage L200mm","PPL 500 Ablass-Element L200mm","PPL 500 Elemento di montagoi L200mm",131,1,"DN 500",null,260.7,"137102450","106619","4037494491546",300,"100899",39.300000000000011,237,63,"100899",300,39.300000000000011]
["100900",100900,null,"STK","PPL 600 Ablass-Element L200mm","CHF",342,"Schiedel PRIMA PLUS",3.81,200,"J","PPL 600 Elément de montage L200mm","PPL 600 Ablass-Element L200mm","PPL 600 Elemento di montagoi L200mm",131,1,"DN 600",null,297,"137102460","106620","4037494491560",342,"100900",45,270,72,"100900",342,45]
["100901",100901,null,"STK","PPL 700 Ablass-Element L200mm","CHF",410,"Schiedel PRIMA PLUS",4.4400000000000004,200,"J","PPL 700 Elément de montage L200mm","PPL 700 Ablass-Element L200mm","PPL 700 Elemento di montagoi L200mm",131,1,"DN 700",null,356.4,"137102470","106621","4037494491577",410,"100901",53.600000000000023,324,86,"100901",410,53.600000000000023]
["100902",100902,null,"STK","PPL 80 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",109,"Schiedel PRIMA PLUS",0.38,0,"J","PPL 80 Elément de mesure 3pc. 3/4\" L150mm","PPL 80 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 80 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 80",null,94.6,"6281108081",null,null,109,"100902",14.400000000000006,86,23,"100902",109,14.400000000000006]
["100903",100903,null,"STK","PPL 100 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",123,"Schiedel PRIMA PLUS",0.44,0,"J","PPL 100 Elément de mesure 3pc. 3/4\" L150mm","PPL 100 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 100 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 100",null,106.7,"6281110081",null,null,123,"100903",16.299999999999997,97,26,"100903",123,16.299999999999997]
["100904",100904,null,"STK","PPL 130 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",137,"Schiedel PRIMA PLUS",0.54,0,"J","PPL 130 Elément de mesure 3pc. 3/4\" L150mm","PPL 130 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 130 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 130",null,118.8,"6281113081",null,null,137,"100904",18.200000000000003,108,29,"100904",137,18.200000000000003]
["100905",100905,null,"STK","PPL 150 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",151,"Schiedel PRIMA PLUS",0.61,0,"J","PPL 150 Elément de mesure 3pc. 3/4\" L150mm","PPL 150 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 150 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 150",null,130.9,"6281115081",null,null,151,"100905",20.099999999999994,119,32,"100905",151,20.099999999999994]
["100906",100906,null,"STK","PPL 180 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",164,"Schiedel PRIMA PLUS",0.71,0,"J","PPL 180 Elément de mesure 3pc. 3/4\" L150mm","PPL 180 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 180 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 180",null,141.9,"6281118081",null,null,164,"100906",22.099999999999994,129,35,"100906",164,22.099999999999994]
["100907",100907,null,"STK","PPL 200 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",179,"Schiedel PRIMA PLUS",0.78,0,"J","PPL 200 Elément de mesure 3pc. 3/4\" L150mm","PPL 200 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 200 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 200",null,155.1,"6281120081",null,null,179,"100907",23.900000000000006,141,38,"100907",179,23.900000000000006]
["100908",100908,null,"STK","PPL 250 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",192,"Schiedel PRIMA PLUS",0.95,0,"J","PPL 250 Elément de mesure 3pc. 3/4\" L150mm","PPL 250 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 250 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 250",null,166.1,"6281125081",null,null,192,"100908",25.900000000000006,151,41,"100908",192,25.900000000000006]
["100909",100909,null,"STK","PPL 300 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",205,"Schiedel PRIMA PLUS",1.1200000000000001,0,"J","PPL 300 Elément de mesure 3pc. 3/4\" L150mm","PPL 300 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 300 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 300",null,178.2,"628113081",null,null,205,"100909",26.800000000000011,162,43,"100909",205,26.800000000000011]
["100910",100910,null,"STK","PPL 350 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",233,"Schiedel PRIMA PLUS",2.56,0,"J","PPL 350 Elément de mesure 3pc. 3/4\" L150mm","PPL 350 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 350 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 350",null,202.4,"6281135081",null,null,233,"100910",30.599999999999994,184,49,"100910",233,30.599999999999994]
["100911",100911,null,"STK","PPL 400 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",274,"Schiedel PRIMA PLUS",2.9,0,"J","PPL 400 Elément de mesure 3pc. 3/4\" L150mm","PPL 400 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 400 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 400",null,237.6,"6281140081",null,null,274,"100911",36.400000000000006,216,58,"100911",274,36.400000000000006]
["100912",100912,null,"STK","PPL 450 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",315,"Schiedel PRIMA PLUS",3.19,0,"J","PPL 450 Elément de mesure 3pc. 3/4\" L150mm","PPL 450 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 450 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 450",null,273.89999999999998,"6281145081",null,null,315,"100912",41.100000000000023,249,66,"100912",315,41.100000000000023]
["100913",100913,null,"STK","PPL 500 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",370,"Schiedel PRIMA PLUS",3.49,0,"J","PPL 500 Elément de mesure 3pc. 3/4\" L150mm","PPL 500 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 500 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 500",null,321.2,"6281150081",null,null,370,"100913",48.800000000000011,292,78,"100913",370,48.800000000000011]
["100914",100914,null,"STK","PPL 600 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",410,"Schiedel PRIMA PLUS",4.07,0,"J","PPL 600 Elément de mesure 3pc. 3/4\" L150mm","PPL 600 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 600 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 600",null,356.4,"6281160081",null,null,410,"100914",53.600000000000023,324,86,"100914",410,53.600000000000023]
["100915",100915,null,"STK","PPL 700 Element mit 3 Messöffnungen 3/4\" L150mm","CHF",452,"Schiedel PRIMA PLUS",4.66,0,"J","PPL 700 Elément de mesure 3pc. 3/4\" L150mm","PPL 700 Element mit 3 Messöffnungen 3/4\" L150mm","PPL 700 Elemento di missura 3pz. 3/4\" L150mm",131,1,"DN 700",null,392.7,"6281170081",null,null,452,"100915",59.300000000000011,357,95,"100915",452,59.300000000000011]
["100916",100916,null,"STK","PPL 80 Abstandhalter","CHF",24.7,"Schiedel PRIMA PLUS",0.15,0,"J","PPL 80 Distanceur","PPL 80 Abstandhalter","PPL 80 Distanzatori",131,1,"DN 80",null,21,"265822208",null,null,24.7,"100916",3.6999999999999993,21,3.6999999999999993,"100916",24.7,3.6999999999999993,24.7,24.65909090909091]
["100917",100917,null,"STK","PPL 100 Abstandhalter","CHF",31,"Schiedel PRIMA PLUS",0.15,0,"J","PPL 100 Distanceur","PPL 100 Abstandhalter","PPL 100 Distanzatori",131,1,"DN 100",null,26.4,"265822210",null,null,31,"100917",4.6000000000000014,24,7,"100917",31,4.6000000000000014]
["100918",100918,null,"STK","PPL 130 Abstandhalter","CHF",32,"Schiedel PRIMA PLUS",0.15,0,"J","PPL 130 Distanceur","PPL 130 Abstandhalter","PPL 130 Distanzatori",131,1,"DN 130",null,27.5,"265822213",null,null,32,"100918",4.5,25,7,"100918",32,4.5]
["100919",100919,null,"STK","PPL 150 Abstandhalter","CHF",35,"Schiedel PRIMA PLUS",0.19,0,"J","PPL 150 Distanceur","PPL 150 Abstandhalter","PPL 150 Distanzatori",131,1,"DN 150",null,29.7,"265822215",null,null,35,"100919",5.3000000000000007,27,8,"100919",35,5.3000000000000007]
["100920",100920,null,"STK","PPL 180 - 200 Abstandhalter","CHF",37,"Schiedel PRIMA PLUS",0.19,0,"J","PPL 180 - 200 Distanceur","PPL 180 - 200 Abstandhalter","PPL 180 - 200 Distanzatori",131,1,"DN 180",null,31.9,"265822220",null,null,37,"100920",5.1000000000000014,29,8,"100920",37,5.1000000000000014]
["100921",100921,null,"STK","PPL 250 Abstandhalter","CHF",40,"Schiedel PRIMA PLUS",0.28999999999999998,0,"J","PPL 250 Distanceur","PPL 250 Abstandhalter","PPL 250 Distanzatori",131,1,"DN 250",null,34.1,"265822225",null,null,40,"100921",5.8999999999999986,31,9,"100921",40,5.8999999999999986]
["100922",100922,null,"STK","PPL 300 Abstandhalter","CHF",42,"Schiedel PRIMA PLUS",0.28999999999999998,0,"J","PPL 300 Distanceur","PPL 300 Abstandhalter","PPL 300 Distanzatori",131,1,"DN 300",null,36.299999999999997,"265822230",null,null,42,"100922",5.7000000000000028,33,9,"100922",42,5.7000000000000028]
["100923",100923,null,"STK","PPL 350 Abstandhalter","CHF",50,"Schiedel PRIMA PLUS",0.54,0,"J","PPL 350 Distanceur","PPL 350 Abstandhalter","PPL 350 Distanzatori",131,1,"DN 350",null,42.9,"265822235","105957","4037494150603",50,"100923",7.1000000000000014,39,11,"100923",50,7.1000000000000014]
["100924",100924,null,"STK","PPL 80 Schiebe-Element 270-415mm","CHF",69,"Schiedel PRIMA PLUS",0.7,0,"J","PPL 80 Elément télescopique 270-415mm","PPL 80 Schiebe-Element 270-415mm","PPL 80 Elemento telescopico 270-415mm",131,1,"DN 80",null,59.4,"137021008",null,null,69,"100924",9.6000000000000014,54,15,"100924",69,9.6000000000000014]
["100925",100925,null,"STK","PPL 100 Schiebe-Element 270-415mm","CHF",81,"Schiedel PRIMA PLUS",0.87,0,"J","PPL 100 Elément télescopique 270-415mm","PPL 100 Schiebe-Element 270-415mm","PPL 100 Elemento telescopico 270-415mm",131,1,"DN 100",null,70.400000000000006,"137021010",null,null,81,"100925",10.599999999999994,64,17,"100925",81,10.599999999999994]
["100926",100926,null,"STK","PPL 130 Schiebe-Element 270-415mm","CHF",97,"Schiedel PRIMA PLUS",1.1200000000000001,0,"J","PPL 130 Elément télescopique 270-415mm","PPL 130 Schiebe-Element 270-415mm","PPL 130 Elemento telescopico 270-415mm",131,1,"DN 130",null,83.6,"137021013",null,null,97,"100926",13.400000000000006,76,21,"100926",97,13.400000000000006]
["100927",100927,null,"STK","PPL 150 Schiebe-Element 270-415mm","CHF",109,"Schiedel PRIMA PLUS",1.28,0,"J","PPL 150 Elément télescopique 270-415mm","PPL 150 Schiebe-Element 270-415mm","PPL 150 Elemento telescopico 270-415mm",131,1,"DN 150",null,94.6,"137021015",null,null,109,"100927",14.400000000000006,86,23,"100927",109,14.400000000000006]
["100928",100928,null,"STK","PPL 180 Schiebe-Element 270-415mm","CHF",123,"Schiedel PRIMA PLUS",1.53,0,"J","PPL 180 Elément télescopique 270-415mm","PPL 180 Schiebe-Element 270-415mm","PPL 180 Elemento telescopico 270-415mm",131,1,"DN 180",null,106.7,"137021018",null,null,123,"100928",16.299999999999997,97,26,"100928",123,16.299999999999997]
["100929",100929,null,"STK","PPL 200 Schiebe-Element 270-415mm","CHF",137,"Schiedel PRIMA PLUS",1.7,0,"J","PPL 200 Elément télescopique 270-415mm","PPL 200 Schiebe-Element 270-415mm","PPL 200 Elemento telescopico 270-415mm",131,1,"DN 200",null,118.8,"137021020",null,null,137,"100929",18.200000000000003,108,29,"100929",137,18.200000000000003]
["100930",100930,null,"STK","PPL 250 Schiebe-Element 270-415mm","CHF",151,"Schiedel PRIMA PLUS",2.11,0,"J","PPL 250 Elément télescopique 270-415mm","PPL 250 Schiebe-Element 270-415mm","PPL 250 Elemento telescopico 270-415mm",131,1,"DN 250",null,130.9,"137021025",null,null,151,"100930",20.099999999999994,119,32,"100930",151,20.099999999999994]
["100931",100931,null,"STK","PPL 300 Schiebe-Element 270-415mm","CHF",164,"Schiedel PRIMA PLUS",2.54,0,"J","PPL 300 Elément télescopique 270-415mm","PPL 300 Schiebe-Element 270-415mm","PPL 300 Elemento telescopico 270-415mm",131,1,"DN 300",null,141.9,"137021030",null,null,164,"100931",22.099999999999994,129,35,"100931",164,22.099999999999994]
["100932",100932,null,"STK","PPL 350 Schiebe-Element 270-415mm","CHF",205,"Schiedel PRIMA PLUS",4.74,0,"J","PPL 350 Elément télescopique 270-415mm","PPL 350 Schiebe-Element 270-415mm","PPL 350 Elemento telescopico 270-415mm",131,1,"DN 350",null,178.2,"137121235","106682","4037494918340",205,"100932",26.800000000000011,162,43,"100932",205,26.800000000000011]
["100933",100933,null,"STK","PPL 400 Schiebe-Element 100-400mm","CHF",233,"Schiedel PRIMA PLUS",5.4,0,"J","PPL 400 Elément télescopique 100-400mm","PPL 400 Schiebe-Element 100-400mm","PPL 400 Elemento telescopico 100-400mm",131,1,"DN 400",null,202.4,"137121240","106683","4037494918357",233,"100933",30.599999999999994,184,49,"100933",233,30.599999999999994]
["100934",100934,null,"STK","PPL 450 Schiebe-Element 100-400mm","CHF",274,"Schiedel PRIMA PLUS",6.07,0,"J","PPL 450 Elément télescopique 100-400mm","PPL 450 Schiebe-Element 100-400mm","PPL 450 Elemento telescopico 100-400mm",131,1,"DN 450",null,237.6,"137121245","106684","4037494918364",274,"100934",36.400000000000006,216,58,"100934",274,36.400000000000006]
["100935",100935,null,"STK","PPL 500 Schiebe-Element 100-400mm","CHF",342,"Schiedel PRIMA PLUS",6.75,0,"J","PPL 500 Elément télescopique 100-400mm","PPL 500 Schiebe-Element 100-400mm","PPL 500 Elemento telescopico 100-400mm",131,1,"DN 500",null,297,"137121250","106685","4037494918371",342,"100935",45,270,72,"100935",342,45]
["100936",100936,null,"STK","PPL 600 Schiebe-Element 100-400mm","CHF",410,"Schiedel PRIMA PLUS",8.09,0,"J","PPL 600 Elément télescopique 100-400mm","PPL 600 Schiebe-Element 100-400mm","PPL 600 Elemento telescopico 100-400mm",131,1,"DN 600",null,356.4,"137121260","106686","4037494918388",410,"100936",53.600000000000023,324,86,"100936",410,53.600000000000023]
["100937",100937,null,"STK","PPL 700 Schiebe-Element 100-400mm","CHF",480,"Schiedel PRIMA PLUS",9.4499999999999993,0,"J","PPL 700 Elément télescopique 100-400mm","PPL 700 Schiebe-Element 100-400mm","PPL 700 Elemento telescopico 100-400mm",131,1,"DN 700",null,416.9,"137121270","106687","4037494918395",480,"100937",63.100000000000023,379,101,"100937",480,63.100000000000023]
["100938",100938,null,"STK","PPL 80 Endrohr mit beidseitiger Muffe L1000mm","CHF",69,"Schiedel PRIMA PLUS",1.2,950,"J","PPL 80 Elément final droit avec 2 manchon L1000mm","PPL 80 Endrohr mit beidseitiger Muffe L1000mm","PPL 80 Elemento finale con 2  femmina L1000mm",131,1,"DN 80",null,59.4,"137010108","106235","4037494147689",69,"100938",9.6000000000000014,54,15,"100938",69,9.6000000000000014]
["100939",100939,null,"STK","PPL 100 Endrohr mit beidseitiger Muffe L1000mm","CHF",81,"Schiedel PRIMA PLUS",1.5,950,"J","PPL 100 Elément final droit avec 2 manchon L1000mm","PPL 100 Endrohr mit beidseitiger Muffe L1000mm","PPL 100 Elemento finale con 2  femmina L1000mm",131,1,"DN 100",null,70.400000000000006,"137010110","106236","4037494147696",81,"100939",10.599999999999994,64,17,"100939",81,10.599999999999994]
["100940",100940,null,"STK","PPL 130 Endrohr mit beidseitiger Muffe L1000mm","CHF",97,"Schiedel PRIMA PLUS",1.9,950,"J","PPL 130 Elément final droit avec 2 manchon L1000mm","PPL 130 Endrohr mit beidseitiger Muffe L1000mm","PPL 130 Elemento finale con 2  femmina L1000mm",131,1,"DN 130",null,83.6,"137010113","106239","4037494147719",97,"100940",13.400000000000006,76,21,"100940",97,13.400000000000006]
["100941",100941,null,"STK","PPL 150 Endrohr mit beidseitiger Muffe L1000mm","CHF",109,"Schiedel PRIMA PLUS",2.2999999999999998,950,"J","PPL 150 Elément final droit avec 2 manchon L1000mm","PPL 150 Endrohr mit beidseitiger Muffe L1000mm","PPL 150 Elemento finale con 2  femmina L1000mm",131,1,"DN 150",null,94.6,"137010115","106241","4037494147726",109,"100941",14.400000000000006,86,23,"100941",109,14.400000000000006]
["100942",100942,null,"STK","PPL 180 Endrohr mit beidseitiger Muffe L1000mm","CHF",123,"Schiedel PRIMA PLUS",2.7,950,"J","PPL 180 Elément final droit avec 2 manchon L1000mm","PPL 180 Endrohr mit beidseitiger Muffe L1000mm","PPL 180 Elemento finale con 2  femmina L1000mm",131,1,"DN 180",null,106.7,"137010118","106243","4037494147733",123,"100942",16.299999999999997,97,26,"100942",123,16.299999999999997]
["100943",100943,null,"STK","PPL 200 Endrohr mit beidseitiger Muffe L1000mm","CHF",137,"Schiedel PRIMA PLUS",3,950,"J","PPL 200 Elément final droit avec 2 manchon L1000mm","PPL 200 Endrohr mit beidseitiger Muffe L1000mm","PPL 200 Elemento finale con 2  femmina L1000mm",131,1,"DN 200",null,118.8,"137010120","106244","4037494147740",137,"100943",18.200000000000003,108,29,"100943",137,18.200000000000003]
["100944",100944,null,"STK","PPL 250 Endrohr mit beidseitiger Muffe L1000mm","CHF",164,"Schiedel PRIMA PLUS",3.8,950,"J","PPL 250 Elément final droit avec 2 manchon L1000mm","PPL 250 Endrohr mit beidseitiger Muffe L1000mm","PPL 250 Elemento finale con 2  femmina L1000mm",131,1,"DN 250",null,141.9,"137010125","106246","4037494147764",164,"100944",22.099999999999994,129,35,"100944",164,22.099999999999994]
["100945",100945,null,"STK","PPL 300 Endrohr mit beidseitiger Muffe L1000mm","CHF",205,"Schiedel PRIMA PLUS",4.5,950,"J","PPL 300 Elément final droit avec 2 manchon L1000mm","PPL 300 Endrohr mit beidseitiger Muffe L1000mm","PPL 300 Elemento finale con 2  femmina L1000mm",131,1,"DN 300",null,178.2,"137010130","106247","4037494147771",205,"100945",26.800000000000011,162,43,"100945",205,26.800000000000011]
["100946",100946,null,"STK","PPL 350 Endrohr mit beidseitiger Muffe L1000mm","CHF",246,"Schiedel PRIMA PLUS",8.83,950,"J","PPL 350 Elément final droit avec 2 manchon L1000mm","PPL 350 Endrohr mit beidseitiger Muffe L1000mm","PPL 350 Elemento finale con 2  femmina L1000mm",131,1,"DN 350",null,213.4,"137110135","106672","4037494426968",246,"100946",32.599999999999994,194,52,"100946",246,32.599999999999994]
["100947",100947,null,"STK","PPL 400 Endrohr mit beidseitiger Muffe L1000mm","CHF",300,"Schiedel PRIMA PLUS",10.039999999999999,950,"J","PPL 400 Elément final droit avec 2 manchon L1000mm","PPL 400 Endrohr mit beidseitiger Muffe L1000mm","PPL 400 Elemento finale con 2  femmina L1000mm",131,1,"DN 400",null,260.7,"137110140",null,null,300,"100947",39.300000000000011,237,63,"100947",300,39.300000000000011]
["100948",100948,null,"STK","PPL 450 Endrohr mit beidseitiger Muffe L1000mm","CHF",370,"Schiedel PRIMA PLUS",11.3,950,"J","PPL 450 Elément final droit avec 2 manchon L1000mm","PPL 450 Endrohr mit beidseitiger Muffe L1000mm","PPL 450 Elemento finale con 2  femmina L1000mm",131,1,"DN 450",null,321.2,"137110145",null,null,370,"100948",48.800000000000011,292,78,"100948",370,48.800000000000011]
["100949",100949,null,"STK","PPL 500 Endrohr mit beidseitiger Muffe L1000mm","CHF",452,"Schiedel PRIMA PLUS",12.55,950,"J","PPL 500 Elément final droit avec 2 manchon L1000mm","PPL 500 Endrohr mit beidseitiger Muffe L1000mm","PPL 500 Elemento finale con 2  femmina L1000mm",131,1,"DN 500",null,392.7,"137110150",null,null,452,"100949",59.300000000000011,357,95,"100949",452,59.300000000000011]
["100950",100950,null,"STK","PPL 600 Endrohr mit beidseitiger Muffe L1000mm","CHF",547,"Schiedel PRIMA PLUS",15.06,950,"J","PPL 600 Elément final droit avec 2 manchon L1000mm","PPL 600 Endrohr mit beidseitiger Muffe L1000mm","PPL 600 Elemento finale con 2  femmina L1000mm",131,1,"DN 600",null,475.2,"137110160",null,null,547,"100950",71.800000000000011,432,115,"100950",547,71.800000000000011]
["100951",100951,null,"STK","PPL 700 Endrohr mit beidseitiger Muffe L1000mm","CHF",643,"Schiedel PRIMA PLUS",17.579999999999998,950,"J","PPL 700 Elément final droit avec 2 manchon L1000mm","PPL 700 Endrohr mit beidseitiger Muffe L1000mm","PPL 700 Elemento finale con 2  femmina L1000mm",131,1,"DN 700",null,558.79999999999995,"137110170",null,null,643,"100951",84.200000000000045,508,135,"100951",643,84.200000000000045]
["100952",100952,null,"STK","PPL 80 Revisions-Basiselement mit Kondensatfalle ","CHF",137,"Schiedel PRIMA PLUS",0.36,283,"J","PPL 80 Elem. de base révision avec décanteur","PPL 80 Revisions-Basiselement mit Kondensatfalle ","PPL 80 Elemento di basamento  condensa senza tapo",131,1,"DN 80",null,118.8,"238300708",null,null,137,"100952",18.200000000000003,108,29,"100952",137,18.200000000000003]
["100953",100953,null,"STK","PPL 100 Revisions-Basiselement mit Kondensatfalle ","CHF",151,"Schiedel PRIMA PLUS",0.46,283,"J","PPL 100 Elem. de base révision avec décanteur","PPL 100 Revisions-Basiselement mit Kondensatfalle ","PPL 100 Elemento di basamento  condensa senza tapo",131,1,"DN 100",null,130.9,"238300710",null,null,151,"100953",20.099999999999994,119,32,"100953",151,20.099999999999994]
["100954",100954,null,"STK","PPL 130 Revisions-Basiselement mit Kondensatfalle ","CHF",164,"Schiedel PRIMA PLUS",0.61,283,"J","PPL 130 Elem. de base révision avec décanteur","PPL 130 Revisions-Basiselement mit Kondensatfalle ","PPL 130 Elemento di basamento  condensa senza tapo",131,1,"DN 130",null,141.9,"238300713",null,null,164,"100954",22.099999999999994,129,35,"100954",164,22.099999999999994]
[{"$f":"B908&\"\"","v":"100955"},100955,null,"STK",{"$f":"IF($E$200=2,L908,IF($E$200=3,N908,M908))","v":"PPL 150 Revisions-Basiselement mit Kondensatfalle "},"CHF",{"$f":"IF($L$190=1,W908,S908)","v":179},"Schiedel PRIMA PLUS",0.8,283,"J","PPL 150 Elem. de base révision avec décanteur","PPL 150 Revisions-Basiselement mit Kondensatfalle ","PPL 150 Elemento di basamento  condensa senza tapo",131,1,"DN 150",null,155.1,"238300715",null,null,179,"100955",23.900000000000006,141,38,"100955",179,23.900000000000006]
["100956",100956,null,"STK","PPL 180 Revisions-Basiselement mit Kondensatfalle ","CHF",205,"Schiedel PRIMA PLUS",1.32,450,"J","PPL 180 Elem. de base révision avec décanteur","PPL 180 Revisions-Basiselement mit Kondensatfalle ","PPL 180 Elemento di basamento  condensa senza tapo",131,1,"DN 180",null,178.2,"238300718",null,null,205,"100956",26.800000000000011,162,43,"100956",205,26.800000000000011]
["100957",100957,null,"STK","PPL 200 Revisions-Basiselement mit Kondensatfalle ","CHF",233,"Schiedel PRIMA PLUS",1.46,450,"J","PPL 200 Elem. de base révision avec décanteur","PPL 200 Revisions-Basiselement mit Kondensatfalle ","PPL 200 Elemento di basamento  condensa senza tapo",131,1,"DN 200",null,202.4,"238300720",null,null,233,"100957",30.599999999999994,184,49,"100957",233,30.599999999999994]
["100958",100958,null,"STK","PPL 250 Revisions-Basiselement mit Kondensatfalle ","CHF",260,"Schiedel PRIMA PLUS",2.0299999999999998,450,"J","PPL 250 Elem. de base révision avec décanteur","PPL 250 Revisions-Basiselement mit Kondensatfalle ","PPL 250 Elemento di basamento  condensa senza tapo",131,1,"DN 250",null,225.5,"238300725",null,null,260,"100958",34.5,205,55,"100958",260,34.5]
["100959",100959,null,"STK","PPL 300 Revisions-Basiselement mit Kondensatfalle ","CHF",288,"Schiedel PRIMA PLUS",2.4900000000000002,450,"J","PPL 300 Elem. de base révision avec décanteur","PPL 300 Revisions-Basiselement mit Kondensatfalle ","PPL 300 Elemento di basamento  condensa senza tapo",131,1,"DN 300",null,249.7,"238300730",null,null,288,"100959",38.300000000000011,227,61,"100959",288,38.300000000000011]
["100960",100960,null,"STK","PPL 80 Kondensatabscheider L150mm","CHF",137,"Schiedel PRIMA PLUS",0.3,0,"J","PPL 80 Décanteur de condensat L150mm","PPL 80 Kondensatabscheider L150mm","PPL 80 Elemento con scarico condensa L150mm",131,1,"DN 80",null,118.8,"137022508","106299","4037494149058",137,"100960",18.200000000000003,108,29,"100960",137,18.200000000000003]
["100961",100961,null,"STK","PPL 100 Kondensatabscheider L150mm","CHF",145,"Schiedel PRIMA PLUS",0.36,0,"J","PPL 100 Décanteur de condensat L150mm","PPL 100 Kondensatabscheider L150mm","PPL 100 Elemento con scarico condensa L150mm",131,1,"DN 100",null,125.4,"137022510","106300","4037494149065",145,"100961",19.599999999999994,114,31,"100961",145,19.599999999999994]
["100962",100962,null,"STK","PPL 130 Kondensatabscheider L150mm","CHF",151,"Schiedel PRIMA PLUS",0.46,0,"J","PPL 130 Décanteur de condensat L150mm","PPL 130 Kondensatabscheider L150mm","PPL 130 Elemento con scarico condensa L150mm",131,1,"DN 130",null,130.9,"137022513","106303","4037494149089",151,"100962",20.099999999999994,119,32,"100962",151,20.099999999999994]
["100963",100963,null,"STK","PPL 150 Kondensatabscheider L150mm","CHF",157,"Schiedel PRIMA PLUS",0.53,0,"J","PPL 150 Décanteur de condensat L150mm","PPL 150 Kondensatabscheider L150mm","PPL 150 Elemento con scarico condensa L150mm",131,1,"DN 150",null,136.4,"137022515","106305","4037494149096",157,"100963",20.599999999999994,124,33,"100963",157,20.599999999999994]
["100964",100964,null,"STK","PPL 180 Kondensatabscheider L150mm","CHF",164,"Schiedel PRIMA PLUS",0.63,0,"J","PPL 180 Décanteur de condensat L150mm","PPL 180 Kondensatabscheider L150mm","PPL 180 Elemento con scarico condensa L150mm",131,1,"DN 180",null,141.9,"137022518","106307","4037494149102",164,"100964",22.099999999999994,129,35,"100964",164,22.099999999999994]
["100965",100965,null,"STK","PPL 200 Kondensatabscheider L150mm","CHF",171,"Schiedel PRIMA PLUS",0.7,0,"J","PPL 200 Décanteur de condensat L150mm","PPL 200 Kondensatabscheider L150mm","PPL 200 Elemento con scarico condensa L150mm",131,1,"DN 200",null,148.5,"137022520","106308","4037494149119",171,"100965",22.5,135,36,"100965",171,22.5]
["100966",100966,null,"STK","PPL 250 Kondensatabscheider L150mm","CHF",179,"Schiedel PRIMA PLUS",0.87,0,"J","PPL 250 Décanteur de condensat L150mm","PPL 250 Kondensatabscheider L150mm","PPL 250 Elemento con scarico condensa L150mm",131,1,"DN 250",null,155.1,"137022525","106310","4037494149133",179,"100966",23.900000000000006,141,38,"100966",179,23.900000000000006]
["100967",100967,null,"STK","PPL 300 Kondensatabscheider L150mm","CHF",205,"Schiedel PRIMA PLUS",1,0,"J","PPL 300 Décanteur de condensat L150mm","PPL 300 Kondensatabscheider L150mm","PPL 300 Elemento con scarico condensa L150mm",131,1,"DN 300",null,178.2,"137022530","106311","4037494149140",205,"100967",26.800000000000011,162,43,"100967",205,26.800000000000011]
["100968",100968,null,"STK","PPL 350 Kondensatabscheider L150mm","CHF",260,"Schiedel PRIMA PLUS",2,0,"J","PPL 350 Décanteur de condensat L150mm","PPL 350 Kondensatabscheider L150mm","PPL 350 Elemento con scarico condensa L150mm",131,1,"DN 350",null,225.5,"137122535","106696","4037494401187",260,"100968",34.5,205,55,"100968",260,34.5]
["100969",100969,null,"STK","PPL 400 Kondensatabscheider L150mm","CHF",315,"Schiedel PRIMA PLUS",2.34,0,"J","PPL 400 Décanteur de condensat L150mm","PPL 400 Kondensatabscheider L150mm","PPL 400 Elemento con scarico condensa L150mm",131,1,"DN 400",null,273.89999999999998,"137122540","106697","4037494401194",315,"100969",41.100000000000023,249,66,"100969",315,41.100000000000023]
["100970",100970,null,"STK","PPL 450 Kondensatabscheider L150mm","CHF",370,"Schiedel PRIMA PLUS",2.63,0,"J","PPL 450 Décanteur de condensat L150mm","PPL 450 Kondensatabscheider L150mm","PPL 450 Elemento con scarico condensa L150mm",131,1,"DN 450",null,321.2,"137122545","106698","4037494173930",370,"100970",48.800000000000011,292,78,"100970",370,48.800000000000011]
["100971",100971,null,"STK","PPL 500 Kondensatabscheider L150mm","CHF",424,"Schiedel PRIMA PLUS",2.93,0,"J","PPL 500 Décanteur de condensat L150mm","PPL 500 Kondensatabscheider L150mm","PPL 500 Elemento con scarico condensa L150mm",131,1,"DN 500",null,368.5,"137122550","106699","4037494173947",424,"100971",55.5,335,89,"100971",424,55.5]
["100972",100972,null,"STK","PPL 600 Kondensatabscheider L150mm","CHF",480,"Schiedel PRIMA PLUS",3.51,0,"J","PPL 600 Décanteur de condensat L150mm","PPL 600 Kondensatabscheider L150mm","PPL 600 Elemento con scarico condensa L150mm",131,1,"DN 600",null,416.9,"137122560","106700","4037494149201",480,"100972",63.100000000000023,379,101,"100972",480,63.100000000000023]
["100973",100973,null,"STK","PPL 700 Kondensatabscheider L150mm","CHF",547,"Schiedel PRIMA PLUS",4.0999999999999996,0,"J","PPL 700 Décanteur de condensat L150mm","PPL 700 Kondensatabscheider L150mm","PPL 700 Elemento con scarico condensa L150mm",131,1,"DN 700",null,475.2,"137122570","106701","4037494149225",547,"100973",71.800000000000011,432,115,"100973",547,71.800000000000011]
["100974",100974,null,"STK","PPL EPDM Stopfen für Messöffnung","CHF",9,"Schiedel PRIMA PLUS",3.0000000000000001E-3,0,"J","PPL EPDM Embout de mesure","PPL EPDM Stopfen für Messöffnung","PPL EPDM Tappo di misura",131,1,"PPL ZBH",null,7.7,"265000002","103598","4037494266502",9,"100974",1.2999999999999998,7,2,"100974",9,1.2999999999999998]
["100975",100975,null,"STK","PPL 80 Klemmband","CHF",13,"Schiedel PRIMA PLUS",0.04,0,"J","PPL 80 Bride de fixation","PPL 80 Klemmband","PPL 80 Fascetta di sicurezza",131,1,"DN 80",null,11,"265822108","105943","4037494148044",13,"100975",2,10,3,"100975",13,2]
["100976",100976,null,"STK","PPL 100 Klemmband","CHF",14,"Schiedel PRIMA PLUS",0.04,0,"J","PPL 100 Bride de fixation","PPL 100 Klemmband","PPL 100 Fascetta di sicurezza",131,1,"DN 100",null,12.1,"265822110","105944","4037494148051",14,"100976",1.9000000000000004,11,3,"100976",14,1.9000000000000004]
["100977",100977,null,"STK","PPL 130 Klemmband","CHF",14,"Schiedel PRIMA PLUS",0.05,0,"J","PPL 130 Bride de fixation","PPL 130 Klemmband","PPL 130 Fascetta di sicurezza",131,1,"DN 130",null,12.1,"265822113","105947","4037494148075",14,"100977",1.9000000000000004,11,3,"100977",14,1.9000000000000004]
["100978",100978,null,"STK","PPL 150 Klemmband","CHF",16,"Schiedel PRIMA PLUS",0.05,0,"J","PPL 150 Bride de fixation","PPL 150 Klemmband","PPL 150 Fascetta di sicurezza",131,1,"DN 150",null,13.2,"265822115","105949","4037494148082",16,"100978",2.8000000000000007,12,4,"100978",16,2.8000000000000007]
["100979",100979,null,"STK","PPL 180 Klemmband","CHF",16,"Schiedel PRIMA PLUS",0.06,0,"J","PPL 180 Bride de fixation","PPL 180 Klemmband","PPL 180 Fascetta di sicurezza",131,1,"DN 180",null,13.2,"265822118","105951","4037494148099",16,"100979",2.8000000000000007,12,4,"100979",16,2.8000000000000007]
["100980",100980,null,"STK","PPL 200 Klemmband","CHF",17,"Schiedel PRIMA PLUS",0.06,0,"J","PPL 200 Bride de fixation","PPL 200 Klemmband","PPL 200 Fascetta di sicurezza",131,1,"DN 200",null,14.3,"265822120","105952","4037494148105",17,"100980",2.6999999999999993,13,4,"100980",17,2.6999999999999993]
["100981",100981,null,"STK","PPL 250 Klemmband","CHF",18,"Schiedel PRIMA PLUS",7.0000000000000007E-2,0,"J","PPL 250 Bride de fixation","PPL 250 Klemmband","PPL 250 Fascetta di sicurezza",131,1,"DN 250",null,15.4,"265822125","105954","4037494148129",18,"100981",2.5999999999999996,14,4,"100981",18,2.5999999999999996]
["100982",100982,null,"STK","PPL 300 Klemmband","CHF",19,"Schiedel PRIMA PLUS",0.8,0,"J","PPL 300 Bride de fixation","PPL 300 Klemmband","PPL 300 Fascetta di sicurezza",131,1,"DN 300",null,16.5,"265822130","105955","4037494148136",19,"100982",2.5,15,4,"100982",19,2.5]
["100983",100983,null,"STK","PPL 350 Klemmband","CHF",21,"Schiedel PRIMA PLUS",0.18,0,"J","PPL 350 Bride de fixation","PPL 350 Klemmband","PPL 350 Fascetta di sicurezza",131,1,"DN 350",null,17.600000000000001,"265822135","105956","4037494493533",21,"100983",3.3999999999999986,16,5,"100983",21,3.3999999999999986]
["100984",100984,null,"STK","PPL 400 Klemmband","CHF",28,"Schiedel PRIMA PLUS",0.32,0,"J","PPL 400 Bride de fixation","PPL 400 Klemmband","PPL 400 Fascetta di sicurezza",131,1,"DN 400",null,24.2,"266002240","101119","4037494177969",28,"100984",3.8000000000000007,22,6,"100984",28,3.8000000000000007]
["100985",100985,null,"STK","PPL 450 Klemmband","CHF",38,"Schiedel PRIMA PLUS",0.35,0,"J","PPL 450 Bride de fixation","PPL 450 Klemmband","PPL 450 Fascetta di sicurezza",131,1,"DN 450",null,33,"266002245","101120","4037494177976",38,"100985",5,30,8,"100985",38,5]
["100986",100986,null,"STK","PPL 500 Klemmband","CHF",50,"Schiedel PRIMA PLUS",0.39,0,"J","PPL 500 Bride de fixation","PPL 500 Klemmband","PPL 500 Fascetta di sicurezza",131,1,"DN 500",null,42.9,"266002250","101121","4037494177983",50,"100986",7.1000000000000014,39,11,"100986",50,7.1000000000000014]
["100987",100987,null,"STK","PPL 600 Klemmband","CHF",64,"Schiedel PRIMA PLUS",0.47,0,"J","PPL 600 Bride de fixation","PPL 600 Klemmband","PPL 600 Fascetta di sicurezza",131,1,"DN 600",null,55,"266002260","101123","4037494178003",64,"100987",9,50,14,"100987",64,9]
["100988",100988,null,"STK","PPL 700 Klemmband","CHF",76,"Schiedel PRIMA PLUS",0.54,0,"J","PPL 700 Bride de fixation","PPL 700 Klemmband","PPL 700 Fascetta di sicurezza",131,1,"DN 700",null,66,"266002270","104478","4037494178010",76,"100988",10,60,16,"100988",76,10]
["100989",100989,null,"STK","PPL 80 Dichtung Viton","CHF",16,"Schiedel PRIMA PLUS",0.03,0,"J","PPL 80 Joint en Viton","PPL 80 Dichtung Viton","PPL 80 Guarnizione Viton",131,1,"DN 80",null,13.2,"270301208","101821","4037494933572",16,"100989",2.8000000000000007,12,4,"100989",16,2.8000000000000007]
["100990",100990,null,"STK","PPL 100 Dichtung Viton","CHF",17,"Schiedel PRIMA PLUS",0.03,0,"J","PPL 100 Joint en Viton","PPL 100 Dichtung Viton","PPL 100 Guarnizione Viton",131,1,"DN 100",null,14.3,"270301210","101822","4037494933589",17,"100990",2.6999999999999993,13,4,"100990",17,2.6999999999999993]
["100991",100991,null,"STK","PPL 130 Dichtung Viton","CHF",19,"Schiedel PRIMA PLUS",0.04,0,"J","PPL 130 Joint en Viton","PPL 130 Dichtung Viton","PPL 130 Guarnizione Viton",131,1,"DN 130",null,16.5,"270301213","101824","4037494933619",19,"100991",2.5,15,4,"100991",19,2.5]
["100992",100992,null,"STK","PPL 150 Dichtung Viton","CHF",21,"Schiedel PRIMA PLUS",0.04,0,"J","PPL 150 Joint en Viton","PPL 150 Dichtung Viton","PPL 150 Guarnizione Viton",131,1,"DN 150",null,17.600000000000001,"270301215","101825","4037494933633",21,"100992",3.3999999999999986,16,5,"100992",21,3.3999999999999986]
["100993",100993,null,"STK","PPL 180 Dichtung Viton","CHF",23,"Schiedel PRIMA PLUS",0.04,0,"J","PPL 180 Joint en Viton","PPL 180 Dichtung Viton","PPL 180 Guarnizione Viton",131,1,"DN 180",null,19.8,"270301218","101826","4037494933657",23,"100993",3.1999999999999993,18,5,"100993",23,3.1999999999999993]
["100994",100994,null,"STK","PPL 200 Dichtung Viton","CHF",25,"Schiedel PRIMA PLUS",0.04,0,"J","PPL 200 Joint en Viton","PPL 200 Dichtung Viton","PPL 200 Guarnizione Viton",131,1,"DN 200",null,20.9,"270301220","101827","4037494933664",25,"100994",4.1000000000000014,19,6,"100994",25,4.1000000000000014]
["100995",100995,null,"STK","PPL 250 Dichtung Viton","CHF",28,"Schiedel PRIMA PLUS",0.04,0,"J","PPL 250 Joint en Viton","PPL 250 Dichtung Viton","PPL 250 Guarnizione Viton",131,1,"DN 250",null,24.2,"270301225","101828","4037494933688",28,"100995",3.8000000000000007,22,6,"100995",28,3.8000000000000007]
["100996",100996,null,"STK","PPL 300 Dichtung Viton","CHF",32,"Schiedel PRIMA PLUS",0.04,0,"J","PPL 300 Joint en Viton","PPL 300 Dichtung Viton","PPL 300 Guarnizione Viton",131,1,"DN 300",null,27.5,"270301230","101829","4037494933695",32,"100996",4.5,25,7,"100996",32,4.5]
["100997",100997,null,"STK","PPL 350 Dichtung Viton","CHF",35,"Schiedel PRIMA PLUS",0.04,0,"J","PPL 350 Joint en Viton","PPL 350 Dichtung Viton","PPL 350 Guarnizione Viton",131,1,"DN 350",null,29.7,"270301235","101284","4037494933701",35,"100997",5.3000000000000007,27,8,"100997",35,5.3000000000000007]
["100998",100998,null,"STK","PPL 400 Dichtung Silikon","CHF",37,"Schiedel PRIMA PLUS",0.05,0,"J","PPL 400 Joint en Silikon","PPL 400 Dichtung Silikon","PPL 400 Guarnizione Silikon",131,1,"DN 400",null,31.9,"270301040","101279","5035944582911",37,"100998",5.1000000000000014,29,8,"100998",37,5.1000000000000014]
["100999",100999,null,"STK","PPL 450 Dichtung Silikon","CHF",40,"Schiedel PRIMA PLUS",0.05,0,"J","PPL 450 Joint en Silikon","PPL 450 Dichtung Silikon","PPL 450 Guarnizione Silikon",131,1,"DN 450",null,34.1,"270301045","101280","5035944588241",40,"100999",5.8999999999999986,31,9,"100999",40,5.8999999999999986]
["101000",101000,null,"STK","PPL 500 Dichtung Silikon","CHF",42,"Schiedel PRIMA PLUS",0.05,0,"J","PPL 500 Joint en Silikon","PPL 500 Dichtung Silikon","PPL 500 Guarnizione Silikon",131,1,"DN 500",null,36.299999999999997,"270301050","101281","5035944660893",42,"101000",5.7000000000000028,33,9,"101000",42,5.7000000000000028]
["101001",101001,null,"STK","PPL 600 Dichtung Silikon","CHF",50,"Schiedel PRIMA PLUS",0.06,0,"J","PPL 600 Joint en Silikon","PPL 600 Dichtung Silikon","PPL 600 Guarnizione Silikon",131,1,"DN 600",null,42.9,"270301060","101282","5035944614308",50,"101001",7.1000000000000014,39,11,"101001",50,7.1000000000000014]
["101002",101002,null,"STK","PPL 700 Dichtung Silikon","CHF",56,"Schiedel PRIMA PLUS",0.06,0,"J","PPL 700 Joint en Silikon","PPL 700 Dichtung Silikon","PPL 700 Guarnizione Silikon",131,1,"DN 700",null,48.4,"270301070","101283","4037494150313",56,"101002",7.6000000000000014,44,12,"101002",56,7.6000000000000014]
["101003",101003,null,"STK","PPL 80 Winkel 15°","CHF",50,"Schiedel PRIMA PLUS",0.22,0,"J","PPL 80 Coude 15°","PPL 80 Winkel 15°","PPL 80 Gomito 15°",131,1,"DN 80",null,42.9,"137031508","106327","4037494150863",50,"101003",7.1000000000000014,39,11,"101003",50,7.1000000000000014]
["101004",101004,null,"STK","PPL 100 Winkel 15°","CHF",56,"Schiedel PRIMA PLUS",0.23,0,"J","PPL 100 Coude 15°","PPL 100 Winkel 15°","PPL 100 Gomito 15°",131,1,"DN 100",null,48.4,"137031510","106328","4037494150870",56,"101004",7.6000000000000014,44,12,"101004",56,7.6000000000000014]
["101005",101005,null,"STK","PPL 130 Winkel 15°","CHF",64,"Schiedel PRIMA PLUS",0.38,0,"J","PPL 130 Coude 15°","PPL 130 Winkel 15°","PPL 130 Gomito 15°",131,1,"DN 130",null,55,"137031513","106331","4037494720509",64,"101005",9,50,14,"101005",64,9]
["101006",101006,null,"STK","PPL 150 Winkel 15°","CHF",70,"Schiedel PRIMA PLUS",0.41599999999999998,0,"J","PPL 150 Coude 15°","PPL 150 Winkel 15°","PPL 150 Gomito 15°",131,1,"DN 150",null,60.5,"137031515","106333","4037494720516",70,"101006",9.5,55,15,"101006",70,9.5]
["101007",101007,null,"STK","PPL 180 Winkel 15°","CHF",76,"Schiedel PRIMA PLUS",0.51,0,"J","PPL 180 Coude 15°","PPL 180 Winkel 15°","PPL 180 Gomito 15°",131,1,"DN 180",null,66,"137031518","106335","4037494719404",76,"101007",10,60,16,"101007",76,10]
["101008",101008,null,"STK","PPL 200 Winkel 15°","CHF",83,"Schiedel PRIMA PLUS",0.57299999999999995,0,"J","PPL 200 Coude 15°","PPL 200 Winkel 15°","PPL 200 Gomito 15°",131,1,"DN 200",null,71.5,"137031520","106336","4037494719411",83,"101008",11.5,65,18,"101008",83,11.5]
["101009",101009,null,"STK","PPL 250 Winkel 15°","CHF",98,"Schiedel PRIMA PLUS",0.74299999999999999,0,"J","PPL 250 Coude 15°","PPL 250 Winkel 15°","PPL 250 Gomito 15°",131,1,"DN 250",null,84.7,"137031525","106338","4037494719428",98,"101009",13.299999999999997,77,21,"101009",98,13.299999999999997]
["101010",101010,null,"STK","PPL 300 Winkel 15°","CHF",111,"Schiedel PRIMA PLUS",0.92100000000000004,0,"J","PPL 300 Coude 15°","PPL 300 Winkel 15°","PPL 300 Gomito 15°",131,1,"DN 300",null,95.7,"137031530","106339","4037494719435",111,"101010",15.299999999999997,87,24,"101010",111,15.299999999999997]
["101011",101011,null,"STK","PPL 350 Winkel 15°","CHF",138,"Schiedel PRIMA PLUS",1.85,0,"J","PPL 350 Coude 15°","PPL 350 Winkel 15°","PPL 350 Gomito 15°",131,1,"DN 350",null,119.9,"137131535","106710","4037494401286",138,"101011",18.099999999999994,109,29,"101011",138,18.099999999999994]
["101012",101012,null,"STK","PPL 400 Winkel 15°","CHF",275,"Schiedel PRIMA PLUS",2.2200000000000002,0,"J","PPL 400 Coude 15°","PPL 400 Winkel 15°","PPL 400 Gomito 15°",131,1,"DN 400",null,238.7,"137131540","106711","4037494401293",275,"101012",36.300000000000011,217,58,"101012",275,36.300000000000011]
["101013",101013,null,"STK","PPL 450 Winkel 15°","CHF",412,"Schiedel PRIMA PLUS",2.72,0,"J","PPL 450 Coude 15°","PPL 450 Winkel 15°","PPL 450 Gomito 15°",131,1,"DN 450",null,357.5,"137131545","106712","4037494150917",412,"101013",54.5,325,87,"101013",412,54.5]
["101014",101014,null,"STK","PPL 500 Winkel 15°","CHF",481,"Schiedel PRIMA PLUS",3.02,0,"J","PPL 500 Coude 15°","PPL 500 Winkel 15°","PPL 500 Gomito 15°",131,1,"DN 500",null,418,"137131550","106713","4037494150924",481,"101014",63,380,101,"101014",481,63]
["101015",101015,null,"STK","PPL 600 Winkel 15°","CHF",618,"Schiedel PRIMA PLUS",3.78,0,"J","PPL 600 Coude 15°","PPL 600 Winkel 15°","PPL 600 Gomito 15°",131,1,"DN 600",null,536.79999999999995,"137131560","106714","4037494150948",618,"101015",81.200000000000045,488,130,"101015",618,81.200000000000045]
["101016",101016,null,"STK","PPL 700 Winkel 15°","CHF",685,"Schiedel PRIMA PLUS",4.76,0,"J","PPL 700 Coude 15°","PPL 700 Winkel 15°","PPL 700 Gomito 15°",131,1,"DN 700",null,595.1,"137131570","106715","4037494150962",685,"101016",89.899999999999977,541,144,"101016",685,89.899999999999977]
["101017",101017,null,"STK","PPL 80 Winkel 30°","CHF",50,"Schiedel PRIMA PLUS",0.27,0,"J","PPL 80 Coude 30°","PPL 80 Winkel 30°","PPL 80 Gomito 30°",131,1,"DN 80",null,42.9,"137033008","106341","4037494150979",50,"101017",7.1000000000000014,39,11,"101017",50,7.1000000000000014]
["101018",101018,null,"STK","PPL 100 Winkel 30°","CHF",56,"Schiedel PRIMA PLUS",0.28999999999999998,0,"J","PPL 100 Coude 30°","PPL 100 Winkel 30°","PPL 100 Gomito 30°",131,1,"DN 100",null,48.4,"137033010","106342","4037494150986",56,"101018",7.6000000000000014,44,12,"101018",56,7.6000000000000014]
[{"$f":"B972&\"\"","v":"101019"},101019,null,"STK",{"$f":"IF($E$200=2,L972,IF($E$200=3,N972,M972))","v":"PPL 130 Winkel 30°"},"CHF",{"$f":"IF($L$190=1,W972,S972)","v":64},"Schiedel PRIMA PLUS",0.43,0,"J","PPL 130 Coude 30°","PPL 130 Winkel 30°","PPL 130 Gomito 30°",131,1,"DN 130",null,55,"137033013","106345","4037494720660",64,"101019",9,50,14,"101019",64,9]
["101020",101020,null,"STK","PPL 150 Winkel 30°","CHF",70,"Schiedel PRIMA PLUS",0.52,0,"J","PPL 150 Coude 30°","PPL 150 Winkel 30°","PPL 150 Gomito 30°",131,1,"DN 150",null,60.5,"137033015","106347","4037494720677",70,"101020",9.5,55,15,"101020",70,9.5]
["101021",101021,null,"STK","PPL 180 Winkel 30°","CHF",76,"Schiedel PRIMA PLUS",0.65,0,"J","PPL 180 Coude 30°","PPL 180 Winkel 30°","PPL 180 Gomito 30°",131,1,"DN 180",null,66,"137033018","106349","4037494719480",76,"101021",10,60,16,"101021",76,10]
["101022",101022,null,"STK","PPL 200 Winkel 30°","CHF",83,"Schiedel PRIMA PLUS",0.66,0,"J","PPL 200 Coude 30°","PPL 200 Winkel 30°","PPL 200 Gomito 30°",131,1,"DN 200",null,71.5,"137033020","106350","4037494719497",83,"101022",11.5,65,18,"101022",83,11.5]
["101023",101023,null,"STK","PPL 250 Winkel 30°","CHF",104,"Schiedel PRIMA PLUS",1.02,0,"J","PPL 250 Coude 30°","PPL 250 Winkel 30°","PPL 250 Gomito 30°",131,1,"DN 250",null,90.2,"137033025","106352","4037494719503",104,"101023",13.799999999999997,82,22,"101023",104,13.799999999999997]
["101024",101024,null,"STK","PPL 300 Winkel 30°","CHF",124,"Schiedel PRIMA PLUS",1.1100000000000001,0,"J","PPL 300 Coude 30°","PPL 300 Winkel 30°","PPL300 Gomito 30°",131,1,"DN 300",null,107.8,"137033030","106353","4037494719510",124,"101024",16.200000000000003,98,26,"101024",124,16.200000000000003]
["101025",101025,null,"STK","PPL 350 Winkel 30°","CHF",165,"Schiedel PRIMA PLUS",2.21,0,"J","PPL 350 Coude 30°","PPL 350 Winkel 30°","PPL 350 Gomito 30°",131,1,"DN 350",null,143,"137133035","106724","4037494401385",165,"101025",22,130,35,"101025",165,22]
["101026",101026,null,"STK","PPL 400 Winkel 30°","CHF",302,"Schiedel PRIMA PLUS",2.72,0,"J","PPL 400 Coude 30°","PPL 400 Winkel 30°","PPL 400 Gomito 30°",131,1,"DN 400",null,261.8,"137133040","106725","4037494401392",302,"101026",40.199999999999989,238,64,"101026",302,40.199999999999989]
["101027",101027,null,"STK","PPL 450 Winkel 30°","CHF",439,"Schiedel PRIMA PLUS",3.4,0,"J","PPL 450 Coude 30°","PPL 450 Winkel 30°","PPL 450 Gomito 30°",131,1,"DN 450",null,381.7,"137133045","106726","4037494151020",439,"101027",57.300000000000011,347,92,"101027",439,57.300000000000011]
["101028",101028,null,"STK","PPL 500 Winkel 30°","CHF",508,"Schiedel PRIMA PLUS",3.91,0,"J","PPL 500 Coude 30°","PPL 500 Winkel 30°","PPL 500 Gomito 30°",131,1,"DN 500",null,441.1,"137133050","106727","4037494151037",508,"101028",66.899999999999977,401,107,"101028",508,66.899999999999977]
["101029",101029,null,"STK","PPL 600 Winkel 30°","CHF",644,"Schiedel PRIMA PLUS",4.99,0,"J","PPL 600 Coude 30°","PPL 600 Winkel 30°","PPL 600 Gomito 30°",131,1,"DN 600",null,559.9,"137133060","106728","4037494151051",644,"101029",84.100000000000023,509,135,"101029",644,84.100000000000023]
["101030",101030,null,"STK","PPL 700 Winkel 30°","CHF",713,"Schiedel PRIMA PLUS",6.35,0,"J","PPL 700 Coude 30°","PPL 700 Winkel 30°","PPL 700 Gomito 30°",131,1,"DN 700",null,619.29999999999995,"137133070","106729","4037494151075",713,"101030",93.700000000000045,563,150,"101030",713,93.700000000000045]
["101031",101031,null,"STK","PPL 80 Winkel 45°","CHF",56,"Schiedel PRIMA PLUS",0.27,0,"J","PPL 80 Coude 45°","PPL 80 Winkel 45°","PPL 80 Gomito 45°",131,1,"DN 80",null,48.4,"137034508","106368","4037494151082",56,"101031",7.6000000000000014,44,12,"101031",56,7.6000000000000014]
["101032",101032,null,"STK","PPL 100 Winkel 45°","CHF",64,"Schiedel PRIMA PLUS",0.35,0,"J","PPL 100 Coude 45°","PPL 100 Winkel 45°","PPL 100 Gomito 45°",131,1,"DN 100",null,55,"137034510","106369","4037494151099",64,"101032",9,50,14,"101032",64,9]
["101033",101033,null,"STK","PPL 130 Winkel 45°","CHF",70,"Schiedel PRIMA PLUS",0.43,0,"J","PPL 130 Coude 45°","PPL 130 Winkel 45°","PPL 130 Gomito 45°",131,1,"DN 130",null,60.5,"137034513","106372","4037494720479",70,"101033",9.5,55,15,"101033",70,9.5]
["101034",101034,null,"STK","PPL 150 Winkel 45°","CHF",76,"Schiedel PRIMA PLUS",0.52,0,"J","PPL 150 Coude 45°","PPL 150 Winkel 45°","PPL 150 Gomito 45°",131,1,"DN 150",null,66,"137034515","106374","4037494716144",76,"101034",10,60,16,"101034",76,10]
["101035",101035,null,"STK","PPL 180 Winkel 45°","CHF",83,"Schiedel PRIMA PLUS",0.65,0,"J","PPL 180 Coude 45°","PPL 180 Winkel 45°","PPL 180 Gomito 45°",131,1,"DN 180",null,71.5,"137034518","106376","4037494719312",83,"101035",11.5,65,18,"101035",83,11.5]
["101036",101036,null,"STK","PPL 200 Winkel 45°","CHF",92,"Schiedel PRIMA PLUS",0.75,0,"J","PPL 200 Coude 45°","PPL 200 Winkel 45°","PPL 200 Gomito 45°",131,1,"DN 200",null,79.2,"137034520","106377","4037494719329",92,"101036",12.799999999999997,72,20,"101036",92,12.799999999999997]
["101037",101037,null,"STK","PPL 250 Winkel 45°","CHF",111,"Schiedel PRIMA PLUS",1.02,0,"J","PPL 250 Coude 45°","PPL 250 Winkel 45°","PPL 250 Gomito 45°",131,1,"DN 250",null,95.7,"137034525","106379","4037494719336",111,"101037",15.299999999999997,87,24,"101037",111,15.299999999999997]
["101038",101038,null,"STK","PPL 300 Winkel 45°","CHF",138,"Schiedel PRIMA PLUS",1.31,0,"J","PPL 300 Coude 45°","PPL 300 Winkel 45°","PPL300 Gomito 45°",131,1,"DN 300",null,119.9,"137034530","106380","4037494719343",138,"101038",18.099999999999994,109,29,"101038",138,18.099999999999994]
["101039",101039,null,"STK","PPL 350 Winkel 45°","CHF",207,"Schiedel PRIMA PLUS",2.94,0,"J","PPL 350 Coude 45°","PPL 350 Winkel 45°","PPL 350 Gomito 45°",131,1,"DN 350",null,179.3,"137134535","106738","4037494401484",207,"101039",27.699999999999989,163,44,"101039",207,27.699999999999989]
["101040",101040,null,"STK","PPL 400 Winkel 45°","CHF",343,"Schiedel PRIMA PLUS",3.53,0,"J","PPL 400 Coude 45°","PPL 400 Winkel 45°","PPL 400 Gomito 45°",131,1,"DN 400",null,298.10000000000002,"137134540","106739","4037494401491",343,"101040",44.899999999999977,271,72,"101040",343,44.899999999999977]
["101041",101041,null,"STK","PPL 450 Winkel 45°","CHF",481,"Schiedel PRIMA PLUS",4.08,0,"J","PPL 450 Coude 45°","PPL 450 Winkel 45°","PPL 450 Gomito 45°",131,1,"DN 450",null,418,"137134545","106740","4037494173954",481,"101041",63,380,101,"101041",481,63]
["101042",101042,null,"STK","PPL 500 Winkel 45°","CHF",548,"Schiedel PRIMA PLUS",4.79,0,"J","PPL 500 Coude 45°","PPL 500 Winkel 45°","PPL 500 Gomito 45°",131,1,"DN 500",null,476.3,"137134550","106741","4037494173961",548,"101042",71.699999999999989,433,115,"101042",548,71.699999999999989]
["101043",101043,null,"STK","PPL 600 Winkel 45°","CHF",685,"Schiedel PRIMA PLUS",6.35,0,"J","PPL 600 Coude 45°","PPL 600 Winkel 45°","PPL 600 Gomito 45°",131,1,"DN 600",null,595.1,"137134560","106742","4037494173985",685,"101043",89.899999999999977,541,144,"101043",685,89.899999999999977]
["101044",101044,null,"STK","PPL 700 Winkel 45°","CHF",754,"Schiedel PRIMA PLUS",8.1199999999999992,0,"J","PPL 700 Coude 45°","PPL 700 Winkel 45°","PPL 700 Gomito 45°",131,1,"DN 700",null,655.6,"137134570","106743","4037494151167",754,"101044",98.399999999999977,596,158,"101044",754,98.399999999999977]
["101045",101045,null,"STK","PPL 80 Winkel 85°","CHF",70,"Schiedel PRIMA PLUS",0.4,0,"J","PPL 80 Coude 85°","PPL 80 Winkel 85°","PPL 80 Gomito 85°",131,1,"DN 80",null,60.5,"137038508","106396","4037494148402",70,"101045",9.5,55,15,"101045",70,9.5]
["101046",101046,null,"STK","PPL 100 Winkel 85°","CHF",76,"Schiedel PRIMA PLUS",0.6,0,"J","PPL 100 Coude 85°","PPL 100 Winkel 85°","PPL 100 Gomito 85°",131,1,"DN 100",null,66,"137038510","106397","4037494148419",76,"101046",10,60,16,"101046",76,10]
["101047",101047,null,"STK","PPL 130 Winkel 85°","CHF",83,"Schiedel PRIMA PLUS",0.57499999999999996,0,"J","PPL 130 Coude 85°","PPL 130 Winkel 85°","PPL 130 Gomito 85°",131,1,"DN 130",null,71.5,"137038513","106400","4037494148433",83,"101047",11.5,65,18,"101047",83,11.5]
["101048",101048,null,"STK","PPL 150 Winkel 85°","CHF",92,"Schiedel PRIMA PLUS",0.69799999999999995,0,"J","PPL 150 Coude 85°","PPL 150 Winkel 85°","PPL 150 Gomito 85°",131,1,"DN 150",null,79.2,"137038515","106402","4037494148440",92,"101048",12.799999999999997,72,20,"101048",92,12.799999999999997]
["101052",101052,null,"STK","PPL 300 Winkel 85°","CHF",193,"Schiedel PRIMA PLUS",2.85,0,"J","PPL 300 Coude 85°","PPL 300 Winkel 85°","PPL300 Gomito 85°",131,1,"DN 300",null,167.2,"137038530","106408","4037494148495",193,"101052",25.800000000000011,152,41,"101052",193,25.800000000000011]
["101057",101057,null,"STK","PPL 600 Winkel 85°","CHF",1164,"Schiedel PRIMA PLUS",10.74,0,"J","PPL 600 Coude 85°","PPL 600 Winkel 85°","PPL 600 Gomito 85°",131,1,"DN 600",null,1012,"137138560","106770","4037494148556",1164,"101057",152,920,244,"101057",1164,152]
["101060",101060,null,"STK","PPL 100 Winkel 90°","CHF",76,"Schiedel PRIMA PLUS",0.45,0,"J","PPL 100 Coude 90°","PPL 100 Winkel 90°","PPL 100 Gomito 90°",131,1,"DN 100",null,66,"137039010","106438","4037494151181",76,"101060",10,60,16,"101060",76,10]
["101062",101062,null,"STK","PPL 150 Winkel 90°","CHF",92,"Schiedel PRIMA PLUS",0.71,0,"J","PPL 150 Coude 90°","PPL 150 Winkel 90°","PPL 150 Gomito 90°",131,1,"DN 150",null,79.2,"137039015","106443","4037494720547",92,"101062",12.799999999999997,72,20,"101062",92,12.799999999999997]
["101067",101067,null,"STK","PPL 350 Winkel 90°","CHF",247,"Schiedel PRIMA PLUS",4.41,0,"J","PPL 350 Coude 90°","PPL 350 Winkel 90°","PPL 350 Gomito 90°",131,1,"DN 350",null,214.5,"137139035","106788","4037494402085",247,"101067",32.5,195,52,"101067",247,32.5]
["101071",101071,null,"STK","PPL 600 Winkel 90°","CHF",1164,"Schiedel PRIMA PLUS",10.74,0,"J","PPL 600 Coude 90°","PPL 600 Winkel 90°","PPL 600 Gomito 90°",131,1,"DN 600",null,1012,"137139060","106792","4037494174043",1164,"101071",152,920,244,"101071",1164,152]
["101072",101072,null,"STK","PPL 700 Winkel 90°","CHF",1369,"Schiedel PRIMA PLUS",13.94,0,"J","PPL 700 Coude 90°","PPL 700 Winkel 90°","PPL 700 Gomito 90°",131,1,"DN 700",null,1190.2,"137139070","106793","4037494151266",1369,"101072",178.79999999999995,1082,287,"101072",1369,178.79999999999995]
["101076",101076,null,"STK","PPL 150 Winkel 85° mit Revisionsöffnung","CHF",219,"Schiedel PRIMA PLUS",1.58,0,"J","PPL 150 Coude 85° d'inspection","PPL 150 Winkel 85° mit Revisionsöffnung","PPL 150 Gomito 85° con revisione",131,1,"DN 150",null,190.3,"137038615","106162","4037494148730",219,"101076",28.699999999999989,173,46,"101076",219,28.699999999999989]
["101080",101080,null,"STK","PPL 300 Winkel 85° mit Revisionsöffnung","CHF",410,"Schiedel PRIMA PLUS",3.97,0,"J","PPL 300 Coude 85° d'inspection","PPL 300 Winkel 85° mit Revisionsöffnung","PPL 300 Gomito 85° con revisione",131,1,"DN 300",null,356.4,"137038630","105997","4037494148785",410,"101080",53.600000000000023,324,86,"101080",410,53.600000000000023]
["101085",101085,null,"STK","PPL 180 Winkel 90° mit Revisionsöffnung","CHF",246,"Schiedel PRIMA PLUS",1.96,0,"J","PPL 180 Coude 90° d'inspection","PPL 180 Winkel 90° mit Revisionsöffnung","PPL 180 Gomito 90° con revisione",131,1,"DN 180",null,213.4,"137039118","106174","4037494148921",246,"101085",32.599999999999994,194,52,"101085",246,32.599999999999994]
["101088",101088,null,"STK","PPL 300 Winkel 90° mit Revisionsöffnung","CHF",410,"Schiedel PRIMA PLUS",3.97,0,"J","PPL 300 Coude 90° d'inspection","PPL 300 Winkel 90° mit Revisionsöffnung","PPL 300 Gomito 90° con revisione",131,1,"DN 300",null,356.4,"137039130","106000","4037494148969",410,"101088",53.600000000000023,324,86,"101088",410,53.600000000000023]
["101091",101091,null,"STK","PPL 180 Winkel 0-45° verstellbar  Trockenbetrieb ","CHF",81,"Schiedel PRIMA PLUS",0.9,0,"J","PPL 180 Coude 0-45° réglable pour fumee seéche","PPL 180 Winkel 0-45° verstellbar  Trockenbetrieb ","PPL 180 Gomito 0-45° regolabile solo per secco",131,1,"DN 180",null,70.400000000000006,"137034418","106363","4037494492192",81,"101091",10.599999999999994,64,17,"101091",81,10.599999999999994]
["101094",101094,null,"STK","PPL 300 Winkel 0-45° verstellbar  Trockenbetrieb ","CHF",123,"Schiedel PRIMA PLUS",1.5,0,"J","PPL 300 Coude 0-45° réglable pour fumee seéche","PPL 300 Winkel 0-45° verstellbar  Trockenbetrieb ","PPL 300 Gomito 0-45° regolabile solo per secco",131,1,"DN 300",null,106.7,"137034430","106367","4037494492239",123,"101094",16.299999999999997,97,26,"101094",123,16.299999999999997]
["101096",101096,null,"STK","PPL 150 Winkel 0-90° verstellbar  Trockenbetrieb  ","CHF",81,"Schiedel PRIMA PLUS",1.7,0,"J","PPL 150 Coude 0-90° réglable pour fumee seéche ","PPL 150 Winkel 0-90° verstellbar  Trockenbetrieb  ","PPL 150 Gomito 0-90° regolabile solo per secco ",131,1,"DN 150",null,70.400000000000006,"137038915","106430","4037494153758",81,"101096",10.599999999999994,64,17,"101096",81,10.599999999999994]
["101099",101099,null,"STK","PPL 250 Winkel 0-90° verstellbar  Trockenbetrieb  ","CHF",123,"Schiedel PRIMA PLUS",2,0,"J","PPL 250 Coude 0-90° réglable pour fumee seéche ","PPL 250 Winkel 0-90° verstellbar  Trockenbetrieb  ","PPL 250 Gomito 0-90° regolabile solo per secco ",131,1,"DN 250",null,106.7,"137038925","106435","4037494153796",123,"101099",16.299999999999997,97,26,"101099",123,16.299999999999997]
["101104",101104,null,"STK","PPL 200 Revisions-Winkel 0-90° verstellbar   ","CHF",246,"Schiedel PRIMA PLUS",3,0,"J","PPL 200 Coude d'inspection 0-90° pour fumee seéche","PPL 200 Revisions-Winkel 0-90° verstellbar   ","PPL 200 Gomito revisione 0-90° regolabile secco",131,1,"DN 200",null,213.4,"137039220","106460","4037494153376",246,"101104",32.599999999999994,194,52,"101104",246,32.599999999999994]
["101108",101108,null,"STK","PPL 100 Kesselanschluss DN + 6mm L150mm","CHF",69,"Schiedel PRIMA PLUS",0.15,0,"J","PPL 100 Raccordement chaudière DN + 6mm L150mm","PPL 100 Kesselanschluss DN + 6mm L150mm","PPL 100 Raccordo di riscaldemento DN + 6mm L150mm",131,1,"DN 100",null,59.4,"265820410","106093","4037494153437",69,"101108",9.6000000000000014,54,15,"101108",69,9.6000000000000014]
["101112",101112,null,"STK","PPL 180 Kesselanschluss DN + 6mm L150mm","CHF",97,"Schiedel PRIMA PLUS",0.22,0,"J","PPL 180 Raccordement chaudière DN + 6mm L150mm","PPL 180 Kesselanschluss DN + 6mm L150mm","PPL 180 Raccordo di riscaldemento DN + 6mm L150mm",131,1,"DN 180",null,83.6,"265820418","106097","4037494153475",97,"101112",13.400000000000006,76,21,"101112",97,13.400000000000006]
["101114",101114,null,"STK","PPL 250 Kesselanschluss DN + 6mm L150mm","CHF",123,"Schiedel PRIMA PLUS",0.42,0,"J","PPL 250 Raccordement chaudière DN + 6mm L150mm","PPL 250 Kesselanschluss DN + 6mm L150mm","PPL 250 Raccordo di riscaldemento DN + 6mm L150mm",131,1,"DN 250",null,106.7,"265820425","106100","4037494153505",123,"101114",16.299999999999997,97,26,"101114",123,16.299999999999997]
["101121",101121,null,"STK","PPL 120 Erweiterung DN130 L150mm","CHF",123,"Schiedel PRIMA PLUS",0.46,0,"J","PPL 120 extension de diamètre DN130 L150mm","PPL 120 Erweiterung DN130 L150mm","PPL 120 Estensione di diametro DN130 L150mm",131,1,"DN 130",null,106.7,"267251213","101792","4037494283080",123,"101121",16.299999999999997,97,26,"101121",123,16.299999999999997]
["101125",101125,null,"STK","PPL 150 Erweiterung DN180 L150mm","CHF",137,"Schiedel PRIMA PLUS",0.67,0,"J","PPL 150 extension de diamètre DN180 L150mm","PPL 150 Erweiterung DN180 L150mm","PPL 150 Estensione di diametro DN180 L150mm",131,1,"DN 150",null,118.8,"267251518","101800","4037494283127",137,"101125",18.200000000000003,108,29,"101125",137,18.200000000000003]
["101127",101127,null,"STK","PPL 160 Erweiterung DN180 L150mm","CHF",137,"Schiedel PRIMA PLUS",0.67,0,"J","PPL 160 extension de diamètre DN180 L150mm","PPL 160 Erweiterung DN180 L150mm","PPL 160 Estensione di diametro DN180 L150mm",131,1,"DN 180",null,118.8,"267251618","101802","4037494283141",137,"101127",18.200000000000003,108,29,"101127",137,18.200000000000003]
["101130",101130,null,"STK","PPL 200 Erweiterung DN250 L150mm","CHF",164,"Schiedel PRIMA PLUS",1.37,0,"J","PPL 200 extension de diamètre DN250 L150mm","PPL 200 Erweiterung DN250 L150mm","PPL 200 Estensione di diametro DN250 L150mm",131,1,"DN 200",null,141.9,"267252025","101808","4037494283189",164,"101130",22.099999999999994,129,35,"101130",164,22.099999999999994]
["101141",101141,null,"STK","PPL 150 Reduktion  DN100 L150mm","CHF",123,"Schiedel PRIMA PLUS",0.1,0,"J","PPL 150 Réduction de diamètre  DN100 L150mm","PPL 150 Reduktion  DN100 L150mm","PPL 150 riduzione di diametro  DN100 L150mm",131,1,"DN 150",null,106.7,"267201510",null,null,123,"101141",16.299999999999997,97,26,"101141",123,16.299999999999997]
["101146",101146,null,"STK","PPL 200 Reduktion  DN150 L150mm","CHF",137,"Schiedel PRIMA PLUS",1.0900000000000001,0,"J","PPL 200 Réduction de diamètre  DN150 L150mm","PPL 200 Reduktion  DN150 L150mm","PPL 200 riduzione di diametro  DN150 L150mm",131,1,"DN 200",null,118.8,"267202015","101768","4037494282908",137,"101146",18.200000000000003,108,29,"101146",137,18.200000000000003]
["101157",101157,null,"STK","PPL 100 Abgasschalldämpfer Schallred. 15DB L580mm","CHF",1138.7,"Schiedel PRIMA PLUS",15,0,"J","PPL 100 Amortisseur du bruit, reducton bruit. 15DB","PPL 100 Abgasschalldämpfer Schallred. 15DB L580mm","PPL 100 Silenzatore passivo 15DB L580mm",131,1,"DN 100",null,990.1,"267300110","103946","4037494154595",1138.7,"101157",148.60000000000002,899,239.70000000000005,"101157",1138.7,148.60000000000002]
["101160",101160,null,"STK","PPL 180 Abgasschalldämpfer Schallred. 15DB L760mm","CHF",1771.2,"Schiedel PRIMA PLUS",18,0,"J","PPL 180 Amortisseur du bruit, reducton bruit. 15DB","PPL 180 Abgasschalldämpfer Schallred. 15DB L760mm","PPL 180 Silenzatore passivo 15DB L760mm",131,1,"DN 180",null,1540.1,"267300218","103950","4037494154632",1771.2,"101160",231.10000000000014,1399,372.20000000000005,"101160",1771.2,231.10000000000014]
["101162",101162,null,"STK","PPL 250 Abgasschalldämpfer Schallred. 15DB L760mm","CHF",2277.1999999999998,"Schiedel PRIMA PLUS",18,0,"J","PPL 250 Amortisseur du bruit, reducton bruit. 15DB","PPL 250 Abgasschalldämpfer Schallred. 15DB L760mm","PPL 250 Silenzatore passivo 15DB L760mm",131,1,"DN 250",null,1980.1,"267300225","103953","4037494154663",2277.1999999999998,"101162",297.09999999999991,1799,478.19999999999982,"101162",2277.1999999999998,297.09999999999991]
["101165",101165,null,"STK","PPL 150 Verlängerung zu Schalldämpfer -10DB ","CHF",569.4,"Schiedel PRIMA PLUS",7,0,"J","PPL 150 Rallongeur d'amortisseur, jusque 10DB ","PPL 150 Verlängerung zu Schalldämpfer -10DB ","PPL 150  Prolunga silenzatore passivo -10DB ",131,1,"DN 150",null,495.1,"267300316","103957","4037494154700",569.4,"101165",74.299999999999955,449,120.39999999999998,"101165",569.4,74.299999999999955]
["101171",101171,null,"STK","PPL 150 Schallabsorber Oel-Gas","CHF",192,"Schiedel PRIMA PLUS",0.8,0,"J","PPL 150 Bride anti-bruit oel et gaz","PPL 150 Schallabsorber Oel-Gas","PPL 150 Fascette antivibranti oel et gaz",131,1,"DN 150",null,166.1,"265000115","101701","4037494266540",192,"101171",25.900000000000006,151,41,"101171",192,25.900000000000006]
["101172",101172,null,"STK","PPL 180 Schallabsorber Oel-Gas","CHF",219,"Schiedel PRIMA PLUS",0.9,0,"J","PPL 180 Bride anti-bruit oel et gaz","PPL 180 Schallabsorber Oel-Gas","PPL 180 Fascette antivibranti oel et gaz",131,1,"DN 180",null,190.3,"265000118","101702","4037494266557",219,"101172",28.699999999999989,173,46,"101172",219,28.699999999999989]
["101176",101176,null,"STK","PPL 100 Schallabsorber Festbrennstoffe","CHF",123,"Schiedel PRIMA PLUS",0.6,0,"J","PPL 100 Bride anti-bruit pour combustibles solides","PPL 100 Schallabsorber Festbrennstoffe","PPL 100 Fascette antivibranti combustibili solidi",131,1,"DN 100",null,106.7,"265000510","101707","4037494279656",123,"101176",16.299999999999997,97,26,"101176",123,16.299999999999997]
["101180",101180,null,"STK","PPL 200 Schallabsorber Festbrennstoffe","CHF",192,"Schiedel PRIMA PLUS",1,0,"J","PPL 200 Bride anti-bruit pour combustibles solides","PPL 200 Schallabsorber Festbrennstoffe","PPL 200 Fascette antivibranti combustibili solidi",131,1,"DN 200",null,166.1,"265000520","101711","4037494279717",192,"101180",25.900000000000006,151,41,"101180",192,25.900000000000006]
["101183",101183,null,"STK","PPL 80 Anschlussrosette ØA 250mm","CHF",35,"Schiedel PRIMA PLUS",1.2,0,"J","PPL 80 Rosace de raccordement ØA 250mm","PPL 80 Anschlussrosette ØA 250mm","PPL 80 Rosetta del muro per tubo singolo ØA 250mm",131,1,"DN 80",null,29.7,"25620008",null,null,35,"101183",5.3000000000000007,27,8,"101183",35,5.3000000000000007]
["101185",101185,null,"STK","PPL 130 Anschlussrosette ØA 300mm ","CHF",49,"Schiedel PRIMA PLUS",1.2,0,"J","PPL 130 Rosace de raccordement ØA 300mm ","PPL 130 Anschlussrosette ØA 300mm ","PPL 130 Rosetta del muro per tubo singolo ØA 300mm",131,1,"DN 130",null,41.8,"25620013",null,null,49,"101185",7.2000000000000028,38,11,"101185",49,7.2000000000000028]
["101193",101193,null,"STK","PPL 80 Rohrschelle  Anschluss 1/2\" Aussengewinde","CHF",26.3,"Zubehör",0.45,0,"J","PPL 80 Collier  embrachement 1/2\" filet ext.","PPL 80 Rohrschelle  Anschluss 1/2\" Aussengewinde","PPL 80 Fascetta di tubo 1/2\" filetto maschio",15,2,"DN 80",null,21,"267000308","103620","4037494283578",26.3,"101193",5.3000000000000007,20,6.3000000000000007,"101193",26.3,5.3000000000000007]
["101197",101197,null,"STK","PPL 150 Rohrschelle Anschluss 1/2\" Aussengewinde","CHF",40,"Zubehör",0.15,0,"J","PPL 150 Collier embrachement 1/2\" filet ext.","PPL 150 Rohrschelle Anschluss 1/2\" Aussengewinde","PPL 150 Fascetta di tubo 1/2\" filetto maschio",15,2,"DN 150",null,32,"267000315","103626","4037494280201",40,"101197",8,31,9,"101197",40,8]
["101200",101200,null,"STK","PPL 200 Rohrschelle Anschluss 1/2\" Aussengewinde","CHF",48.8,"Zubehör",0.18,0,"J","PPL 200 Collier embrachement 1/2\" filet ext.","PPL 200 Rohrschelle Anschluss 1/2\" Aussengewinde","PPL 200 Fascetta di tubo 1/2\" filetto maschio",15,2,"DN 200",null,39,"267000320","103629","4037494280225",48.8,"101200",9.7999999999999972,38,10.799999999999997,"101200",48.8,9.7999999999999972]
["101203",101203,null,"STK","PPL 350 Rohrschelle Anschluss 1/2\" Aussengewinde","CHF",62.5,"Zubehör",0.27,0,"J","PPL 350 Collier embrachement 1/2\" filet ext.","PPL 350 Rohrschelle Anschluss 1/2\" Aussengewinde","PPL 350 Fascetta di tubo 1/2\" filetto maschio",15,2,"DN 350",null,50,"267000335","103632","4037494154816",62.5,"101203",12.5,49,13.5,"101203",62.5,12.5]
["101208",101208,null,"STK","PPL 100 Wandhalter 50mm fix DN 100mm","CHF",55,"Schiedel PRIMA PLUS",0.28000000000000003,0,"J","PPL 100 Fixation murale 50mm fix DN 100mm","PPL 100 Wandhalter 50mm fix DN 100mm","PPL 100 Collare a muro 50mm fix DN 100mm",131,1,"DN 100",null,47.3,"92940100",null,null,55,"101208",7.7000000000000028,43,12,"101208",55,7.7000000000000028]
["101235",101235,null,"STK","PPL 100 Wandhalter 50mm verlängerbar DN100mm","CHF",49,"Schiedel PRIMA PLUS",0.28000000000000003,0,"J","PPL 100 Fixation murale 50mm régl. DN100mm","PPL 100 Wandhalter 50mm verlängerbar DN100mm","PPL 100 Collare a muro 50mm prolunga DN100mm",131,1,"DN 100",null,41.8,"95090100",null,null,49,"101235",7.2000000000000028,38,11,"101235",49,7.2000000000000028]
["101255",101255,null,"PAR","ICS L2 Verlängerung zu Wandhalter 50mm L450mm","CHF",98.4,"Schiedel ICS glänzend",0.95,0,"J","ICS L2 Ralogement pour fixation murale L450mm","ICS L2 Verlängerung zu Wandhalter 50mm L450mm","ICS L2 Prolunga per collare 50mm L450mm",133,1,"ZBH ICS",null,85.49,"267100450","101739","4037494812204",98.4,"101255",12.910000000000011,85.49,12.910000000000011,"101255",98.4,12.910000000000011,98.4,98.423025623025623]
["101256",101256,null,"PAR","ICS L3 Verlängerung zu Wandhalter 50mm L550mm","CHF",112.7,"Schiedel ICS glänzend",1.21,0,"J","ICS L3 Ralogement pour fixation murale L550mm","ICS L3 Verlängerung zu Wandhalter 50mm L550mm","ICS L3 Prolunga per collare 50mm L550mm",133,1,"ZBH ICS",null,97.85,"267100550","101740","4037494812211",112.7,"101256",14.850000000000009,97.85,14.850000000000009,"101256",112.7,14.850000000000009,112.7,112.65286065286065]
["101262",101262,null,"STK","PPL 180 Regenkragen ","CHF",69,"Schiedel PRIMA PLUS",0.35,0,"J","PPL 180 Collerette anti pluie ","PPL 180 Regenkragen ","PPL 180 Scossalina",131,1,"DN 180",null,59.4,"265823018",null,null,69,"101262",9.6000000000000014,54,15,"101262",69,9.6000000000000014]
["101263",101263,null,"STK","PPL 200 Regenkragen ","CHF",75,"Schiedel PRIMA PLUS",0.38,0,"J","PPL 200 Collerette anti pluie ","PPL 200 Regenkragen ","PPL 200 Scossalina",131,1,"DN 200",null,64.900000000000006,"265823020",null,null,75,"101263",10.099999999999994,59,16,"101263",75,10.099999999999994]
["101269",101269,null,"STK","PPL 500 Regenkragen ","CHF",192,"Schiedel PRIMA PLUS",2.34,0,"J","PPL 500 Collerette anti pluie ","PPL 500 Regenkragen ","PPL 500 Scossalina",131,1,"DN 500",null,166.1,"265823050",null,null,192,"101269",25.900000000000006,151,41,"101269",192,25.900000000000006]
["101270",101270,null,"STK","PPL 600 Regenkragen ","CHF",219,"Schiedel PRIMA PLUS",3.07,0,"J","PPL 600 Collerette anti pluie ","PPL 600 Regenkragen ","PPL 600 Scossalina",131,1,"DN 600",null,190.3,"265823060",null,null,219,"101270",28.699999999999989,173,46,"101270",219,28.699999999999989]
["101274",101274,null,"STK","PPL Schachtabdeckung Typ3 450 x 450mm","CHF",151,"Schiedel PRIMA PLUS",1.18,0,"J","PPL Couvre joint carrée Typ3 450 x 450mm","PPL Schachtabdeckung Typ3 450 x 450mm","PPL Copertura del vano tipo3 450 x 450mm",131,1,"PPL ZBH",null,130.9,"354110003","103688","4037494265895",151,"101274",20.099999999999994,119,32,"101274",151,20.099999999999994]
["101278",101278,null,"STK","PPL 130 Mündungskonus zu Schachtabdeckung","CHF",81,"Schiedel PRIMA PLUS",1.1100000000000001,0,"J","PPL 130 Cône de finition pour couvre joint carrée","PPL 130 Mündungskonus zu Schachtabdeckung","PPL 130 Terminale tronco conico",131,1,"DN 130",null,70.400000000000006,"350140013","105981","4037494265932",81,"101278",10.599999999999994,64,17,"101278",81,10.599999999999994]
["101283",101283,null,"STK","PPL 300 Mündungskonus zu Schachtabdeckung","CHF",117,"Schiedel PRIMA PLUS",1.1100000000000001,0,"J","PPL 300 Cône de finition pour couvre joint carrée","PPL 300 Mündungskonus zu Schachtabdeckung","PPL 300 Terminale tronco conico",131,1,"DN 300",null,101.2,"350140030","105989","4037494265994",117,"101283",15.799999999999997,92,25,"101283",117,15.799999999999997]
["101286",101286,null,"STK","PPL 130 Mündungsmanchette L130mm 400 x 400mm","CHF",151,"Schiedel PRIMA PLUS",1.76,0,"J","PPL 130 Tôle de dilatation L130mm 400 x 400mm","PPL 130 Mündungsmanchette L130mm 400 x 400mm","PPL 130Manicotto di sbocco L130mm 400 x 400mm",131,1,"DN 130",null,130.9,"353040213","103677","4037494266793",151,"101286",20.099999999999994,119,32,"101286",151,20.099999999999994]
["101288",101288,null,"STK","PPL 180 Mündungsmanchette L130mm 450 x 450mm","CHF",179,"Schiedel PRIMA PLUS",2.86,0,"J","PPL 180 Tôle de dilatation L130mm 450 x 450mm","PPL 180 Mündungsmanchette L130mm 450 x 450mm","PPL 180Manicotto di sbocco L130mm 450 x 450mm",131,1,"DN 180",null,155.1,"353040218","103681","4037494266816",179,"101288",23.900000000000006,141,38,"101288",179,23.900000000000006]
["101291",101291,null,"STK","PPL 300 Mündungsmanchette L130mm 500 x 500mm","CHF",219,"Schiedel PRIMA PLUS",3,0,"J","PPL 300 Tôle de dilatation L130mm 500 x 500mm","PPL 300 Mündungsmanchette L130mm 500 x 500mm","PPL 300Manicotto di sbocco L130mm 500 x 500mm",131,1,"DN 300",null,190.3,"353040230","103685","4037494266847",219,"101291",28.699999999999989,173,46,"101291",219,28.699999999999989]
["101298",101298,null,"STK","PPL 250 Basten Standard passend zu Münd. Manchette","CHF",326,"Zubehör",3.9,0,"J","PPL 250 Basten Standard juste pour tôle de dilatation","PPL 250 Basten Standard passend zu Münd. Manchette","PPL 250 Terminale Basten per manicotto di sbocco",15,2,"DN 250",null,307,"918225",null,null,326,"101298",19,305,21,"101298",326,19]
["101300",101300,null,"STK","PPL 100 Basten Standard mit Dila zu Dämmrohr 30mm","CHF",360,"Zubehör",3.9,0,"J","PPL 100 Basten Standard avec dila isolation 30mm","PPL 100 Basten Standard mit Dila zu Dämmrohr 30mm","PPL 100 Terminale Basten con dila  p. coppela 30mm",15,2,"DN 100",null,339,"918310",null,null,360,"101300",21,337,23,"101300",360,21]
["101303",101303,null,"STK","PPL 180 Basten Standard mit Dila zu Dämmrohr 30mm","CHF",417,"Zubehör",4.5,0,"J","PPL 180 Basten Standard avec dila  isolation 30mm","PPL 180 Basten Standard mit Dila zu Dämmrohr 30mm","PPL 180 Terminale Basten con dila  p. coppela 30mm",15,2,"DN 180",null,393,"918318",null,null,417,"101303",24,391,26,"101303",417,24]
["101307",101307,null,"STK","PPL 80 Regenhaube ","CHF",81,"Schiedel PRIMA PLUS",0.46,0,"J","PPL 80 Cape pluie ","PPL 80 Regenhaube ","PPL 80 Cappelo prapioggia",131,1,"DN 80",null,70.400000000000006,"25300808",null,null,81,"101307",10.599999999999994,64,17,"101307",81,10.599999999999994]
["101311",101311,null,"STK","PPL 180 Regenhaube ","CHF",123,"Schiedel PRIMA PLUS",1.01,0,"J","PPL 180 Cape pluie ","PPL 180 Regenhaube ","PPL 180 Cappelo prapioggia",131,1,"DN 180",null,106.7,"25300818",null,null,123,"101311",16.299999999999997,97,26,"101311",123,16.299999999999997]
["101312",101312,null,"STK","PPL 200 Regenhaube ","CHF",151,"Schiedel PRIMA PLUS",1.05,0,"J","PPL 200 Cape pluie ","PPL 200 Regenhaube ","PPL 200 Cappelo prapioggia",131,1,"DN 200",null,130.9,"25300820",null,null,151,"101312",20.099999999999994,119,32,"101312",151,20.099999999999994]
["101318",101318,null,"STK","PPL 150 Dämmrohr 20mm Steinwolle L1000mm","CHF",25.3,"Zubehör",1.21,0,"J","PPL 150 Tubo d'isolation 20mm laine de pierre","PPL 150 Dämmrohr 20mm Steinwolle L1000mm","PPL 150 Coppella 20mm di lana di roccia L1000mm",15,2,"DN 150",null,22,"163001215","103495","4037494280317",25.3,"101318",3.3000000000000007,22,3.3000000000000007,"101318",25.3,3.3000000000000007]
["101322",101322,null,"STK","PPL 300 Dämmrohr 25mm Steinwolle L1000mm","CHF",49.5,"Zubehör",2.21,0,"J","PPL 300 Tubo d'isolation 25mm laine de pierre","PPL 300 Dämmrohr 25mm Steinwolle L1000mm","PPL 300 Coppella 25mm di lana di roccia L1000mm",15,2,"DN 300",null,43,"163001230","103501","4037494280355",49.5,"101322",6.5,43,6.5,"101322",49.5,6.5]
["101324",101324,null,"STK","PPL 130 Dämmschale 30mm Alu-Kaschiert L1000mm","CHF",43.8,"Zubehör",1.5,0,"J","PPL 130 Coquille d'isol. 30mm Alu-laine de pierre","PPL 130 Dämmschale 30mm Alu-Kaschiert L1000mm","PPL 130 Coppella 30mm lana di roccia alu L1000mm",15,2,"DN 130",null,37.1,"4009513",null,null,43.8,"101324",6.6999999999999957,36,7.7999999999999972,"101324",43.8,6.6999999999999957]
["101327",101327,null,"STK","PPL 200 Dämmschale 30mm Alu-Kaschiert L1000mm","CHF",56.8,"Zubehör",3,0,"J","PPL 200 Coquille d'isol. 30mm Alu-laine de pierre","PPL 200 Dämmschale 30mm Alu-Kaschiert L1000mm","PPL 200 Coppella 30mm lana di roccia alu L1000mm",15,2,"DN 200",null,48.1,"4009520",null,null,56.8,"101327",8.6999999999999957,47,9.7999999999999972,"101327",56.8,8.6999999999999957]
["101352",101352,null,"STK","CHI 100 Adapter PPL zu Flex","CHF",66,"Schiedel CHIMFLEX",0.22,0,"J","CHI 100 dapteur PPL pour Flex","CHI 100 Adapter PPL zu Flex","CHI 100 Giunto maschio PPL / Flex",132,1,"DN 100",null,57.2,"265930110","106961","4037494149249",66,"101352",8.7999999999999972,52,14,"101352",66,8.7999999999999972]
["101356",101356,null,"STK","CHI 200 Adapter PPL zu Flex","CHF",89,"Schiedel CHIMFLEX",0.44,0,"J","CHI 200 dapteur PPL pour Flex","CHI 200 Adapter PPL zu Flex","CHI 200 Giunto maschio PPL / Flex",132,1,"DN 200",null,77,"265930120","106969","4037494149294",89,"101356",12,70,19,"101356",89,12]
["101360",101360,null,"STK","CHI 130 Adapter Flex zu PPL","CHF",73,"Schiedel CHIMFLEX",0.28999999999999998,0,"J","CHI 130 dapteur Flex pour PPL","CHI 130 Adapter Flex zu PPL","CHI 130 Giunto femina Flex / PPL",132,1,"DN 130",null,62.7,"265930213","106974","4037494149331",73,"101360",10.299999999999997,57,16,"101360",73,10.299999999999997]
["101361",101361,null,"STK","CHI 150 Adapter Flex zu PPL","CHF",76,"Schiedel CHIMFLEX",0.33,0,"J","CHI 150 dapteur Flex pour PPL","CHI 150 Adapter Flex zu PPL","CHI 150 Giunto femina Flex / PPL",132,1,"DN 150",null,66,"265930215","106976","4037494149348",76,"101361",10,60,16,"101361",76,10]
["101367",101367,null,"STK","CHI 130 Adapter Flex zu Flex","CHF",79,"Schiedel CHIMFLEX",1.1000000000000001,0,"J","CHI 130 dapteur Flex pour Flex","CHI 130 Adapter Flex zu Flex","CHI 130 Giunto Flex / Flex",132,1,"DN 130",null,68.2,"265930313","106984","4037494149409",79,"101367",10.799999999999997,62,17,"101367",79,10.799999999999997]
["101368",101368,null,"STK","CHI 150 Adapter Flex zu Flex","CHF",85,"Schiedel CHIMFLEX",1.27,0,"J","CHI 150 dapteur Flex pour Flex","CHI 150 Adapter Flex zu Flex","CHI 150 Giunto Flex / Flex",132,1,"DN 150",null,73.7,"265930315","106986","4037494149416",85,"101368",11.299999999999997,67,18,"101368",85,11.299999999999997]
["101374",101374,null,"STK","CHI 130 CHI Flexrohr 2 lagig Rolle a 12000mm","CHF",1157,"Schiedel CHIMFLEX",18,12000,"J","CHI 130 Tuyau fléxible 2 plis roulau a 12000mm","CHI 130 CHI Flexrohr 2 lagig Rolle a 12000mm","CHI 130 Tubo flessibile 2 veli rotolo a12000mm",132,1,"DN 130",null,1005.4,"D4A12130",null,null,1157,"101374",151.60000000000002,914,243,"101374",1157,151.60000000000002]
["101376",101376,null,"STK","CHI 180 CHI Flexrohr 2 lagig Rolle a 12000mm","CHF",1588,"Schiedel CHIMFLEX",25,12000,"J","CHI 180 Tuyau fléxible 2 plis roulau a 12000mm","CHI 180 CHI Flexrohr 2 lagig Rolle a 12000mm","CHI 180 Tubo flessibile 2 veli rotolo a12000mm",132,1,"DN 180",null,1380.5,"D4A12180",null,null,1588,"101376",207.5,1255,333,"101376",1588,207.5]
["101379",101379,null,"STK","CHI 100 CHI Flexrohr 2 lagig Rolle a 50000mm","CHF",3546,"Schiedel CHIMFLEX",55,50000,"J","CHI 100 Tuyau fléxible 2 plis roulau a 50000mm","CHI 100 CHI Flexrohr 2 lagig Rolle a 50000mm","CHI 100 Tubo flessibile 2 veli rotolo a50000mm",132,1,"DN 100",null,3083.3,"D4A50100",null,null,3546,"101379",462.69999999999982,2803,743,"101379",3546,462.69999999999982]
["101384",101384,null,"STK","CHI 250 CHI Flexrohr 2 lagig Rolle a 5000mm","CHF",1049,"Schiedel CHIMFLEX",20,5000,"J","CHI 250 Tuyau fléxible 2 plis roulau a 5000mm","CHI 250 CHI Flexrohr 2 lagig Rolle a 5000mm","CHI 250 Tubo flessibile 2 veli rotolo a5000mm",132,1,"DN 250",null,911.9,"D4A05250",null,null,1049,"101384",137.10000000000002,829,220,"101384",1049,137.10000000000002]
["101390",101390,null,"STK","CHI 180 Aufhängeschelle zu Flex","CHF",37,"Schiedel CHIMFLEX",0.34,0,"J","CHI 180 Bride pour suspendre le flex","CHI 180 Aufhängeschelle zu Flex","CHI 180 Collare per montagio fessibile",132,1,"DN 180",null,31.9,"D4003180",null,null,37,"101390",5.1000000000000014,29,8,"101390",37,5.1000000000000014]
["101954",101954,null,"STK","ICM 80 Konsolenbleche (Paar)","CHF",131,"Schiedel ICM matt",2.2000000000000002,0,"J","ICM 80 Tôle console murale ( 2 pces. ) ","ICM 80 Konsolenbleche (Paar)","ICM 80 Coppia suporti piastra partenza (Paar)",134,1,"ZBH ICM",null,113.3,"266000608M",null,null,131,"101954",17.700000000000003,103,28,"101954",131,17.700000000000003]
["101956",101956,null,"STK","ICM 130 Konsolenbleche (Paar)","CHF",173,"Schiedel ICM matt",2.85,0,"J","ICM 130 Tôle console murale ( 2 pces. ) ","ICM 130 Konsolenbleche (Paar)","ICM 130 Coppia suporti piastra partenza (Paar)",134,1,"DN 130",null,149.6,"266000613M",null,null,173,"101956",23.400000000000006,136,37,"101956",173,23.400000000000006]
["101959",101959,null,"STK","ICM 200 Konsolenbleche (Paar)","CHF",213,"Schiedel ICM matt",3.54,0,"J","ICM 200 Tôle console murale ( 2 pces. ) ","ICM 200 Konsolenbleche (Paar)","ICM 200 Coppia suporti piastra partenza (Paar)",134,1,"DN 200",null,184.8,"266000620M",null,null,213,"101959",28.199999999999989,168,45,"101959",213,28.199999999999989]
["101965",101965,null,"STK","ICM 500 Konsolenbleche (Paar) ","CHF",679,"Schiedel ICM matt",11.2,0,"J","ICM 500 Tôle console murale ( 2 pces. )  ","ICM 500 Konsolenbleche (Paar) ","ICM 500 Coppia suporti piastra partenza (Paar) ",134,1,"DN 500",null,589.6,"266000650M",null,null,679,"101965",89.399999999999977,536,143,"101965",679,89.399999999999977]
["101967",101967,null,"STK","ICM 700 Konsolenbleche (Paar)","CHF",857,"Schiedel ICM matt",21.48,0,"J","ICM 700 Tôle console murale ( 2 pces. ) ","ICM 700 Konsolenbleche (Paar)","ICM 700 Coppia suporti piastra partenza (Paar)",134,1,"DN 700",null,744.7,"266000670M",null,null,857,"101967",112.29999999999995,677,180,"101967",857,112.29999999999995]
["101975",101975,null,"STK","ICM 570 Wandkonsolen  (Paar) L570mm","CHF",275,"Schiedel ICM matt",5,0,"J","ICM 570 Console réglable ( 2 pces. ) L570mm","ICM 570 Wandkonsolen  (Paar) L570mm","ICM 570 Supporto a muro 2 pezzi L570mm",134,1,"ZBH ICM",null,238.7,0,null,null,275,"101975",36.300000000000011,217,58,"101975",275,36.300000000000011]
["101979",101979,null,"STK","ICM 1004 Wandkonsolen  (Paar) L1004mm","CHF",329,"Schiedel ICM matt",8.4,0,"J","ICM 1004 Console réglable ( 2 pces. ) L1004mm","ICM 1004 Wandkonsolen  (Paar) L1004mm","ICM 1004 Supporto a muro 2 pezzi L1004mm",134,1,"ZBH ICM",null,286,0,null,null,329,"101979",43,260,69,"101979",329,43]
["101983",101983,null,"STK","ICM 80 Verankerungsplatte mit Ablauf senkr.","CHF",165,"Schiedel ICM matt",1.34,95,"J","ICM 80 Plaque de base et écoulement vertical","ICM 80 Verankerungsplatte mit Ablauf senkr.","ICM 80 Piastra base con scadenza verticale",134,1,"DN 80",null,143,"266000408M",null,null,165,"101983",22,130,35,"101983",165,22]
["101984",101984,null,"STK","ICM 100 Verankerungsplatte mit Ablauf senkr.","CHF",207,"Schiedel ICM matt",1.68,95,"J","ICM 100 Plaque de base et écoulement vertical","ICM 100 Verankerungsplatte mit Ablauf senkr.","ICM 100 Piastra base con scadenza verticale",134,1,"DN 100",null,179.3,"266000410M",null,null,207,"101984",27.699999999999989,163,44,"101984",207,27.699999999999989]
["101988",101988,null,"STK","ICM 200 Verankerungsplatte mit Ablauf senkr.","CHF",255,"Schiedel ICM matt",3.37,95,"J","ICM 200 Plaque de base et écoulement vertical","ICM 200 Verankerungsplatte mit Ablauf senkr.","ICM 200 Piastra base con scadenza verticale",134,1,"DN 200",null,221.1,"266000420M","104696","4037494194126",255,"101988",33.900000000000006,201,54,"101988",255,33.900000000000006]
["101993",101993,null,"STK","ICM 450 Verankerungsplatte mit Ablauf senkr.","CHF",795,"Schiedel ICM matt",7.38,95,"J","ICM 450 Plaque de base et écoulement vertical","ICM 450 Verankerungsplatte mit Ablauf senkr.","ICM 450 Piastra base con scadenza verticale",134,1,"DN 450",null,690.8,"266000445M",null,null,795,"101993",104.20000000000005,628,167,"101993",795,104.20000000000005]
["101995",101995,null,"STK","ICM 600 Verankerungsplatte mit Ablauf senkr.","CHF",1341,"Schiedel ICM matt",9.84,95,"J","ICM 600 Plaque de base et écoulement vertical","ICM 600 Verankerungsplatte mit Ablauf senkr.","ICM 600 Piastra base con scadenza verticale",134,1,"DN 600",null,1166,"266000460M",null,null,1341,"101995",175,1060,281,"101995",1341,175]
["101998",101998,null,"STK","ICM 100 Zwischenstütze","CHF",241,"Schiedel ICM matt",2.1,95,"J","ICM 100 Support intermédieaire","ICM 100 Zwischenstütze","ICM 100 Piastra passante",134,1,"DN 100",null,209,"266001010M",null,null,241,"101998",32,190,51,"101998",241,32]
["102003",102003,null,"STK","ICM 250 Zwischenstütze","CHF",343,"Schiedel ICM matt",4.2,95,"J","ICM 250 Support intermédieaire","ICM 250 Zwischenstütze","ICM 250 Piastra passante",134,1,"DN 250",null,298.10000000000002,"266001025M",null,null,343,"102003",44.899999999999977,271,72,"102003",343,44.899999999999977]
["102007",102007,null,"STK","ICM 450 Zwischenstütze","CHF",685,"Schiedel ICM matt",8.6,95,"J","ICM 450 Support intermédieaire","ICM 450 Zwischenstütze","ICM 450 Piastra passante",134,1,"DN 450",null,595.1,"266001045M",null,null,685,"102007",89.899999999999977,541,144,"102007",685,89.899999999999977]
["102011",102011,null,"STK","ICM 80 Verankerungsplatte EW auf DW","CHF",138,"Schiedel ICM matt",2.4,97,"J","ICM 80 Plaque avec male vertical PPL","ICM 80 Verankerungsplatte EW auf DW","ICM 80 Piastra verticale con maschio PPL",134,1,"DN 80",null,119.9,"266000308M",null,null,138,"102011",18.099999999999994,109,29,"102011",138,18.099999999999994]
["102014",102014,null,"STK","ICM 150 Verankerungsplatte EW auf DW","CHF",180,"Schiedel ICM matt",3.8,97,"J","ICM 150 Plaque avec male vertical PPL","ICM 150 Verankerungsplatte EW auf DW","ICM 150 Piastra verticale con maschio PPL",134,1,"DN 150",null,156.19999999999999,"266000315M",null,null,180,"102014",23.800000000000011,142,38,"102014",180,23.800000000000011]
["102016",102016,null,"STK","ICM 200 Verankerungsplatte EW auf DW","CHF",235,"Schiedel ICM matt",4.9000000000000004,97,"J","ICM 200 Plaque avec male vertical PPL","ICM 200 Verankerungsplatte EW auf DW","ICM 200 Piastra verticale con maschio PPL",134,1,"DN 200",null,203.5,"266000320M",null,null,235,"102016",31.5,185,50,"102016",235,31.5]
["102019",102019,null,"STK","ICM 350 Verankerungsplatte EW auf DW","CHF",343,"Schiedel ICM matt",8.1,97,"J","ICM 350 Plaque avec male vertical PPL","ICM 350 Verankerungsplatte EW auf DW","ICM 350 Piastra verticale con maschio PPL",134,1,"DN 350",null,298.10000000000002,"266000335M",null,null,343,"102019",44.899999999999977,271,72,"102019",343,44.899999999999977]
["102025",102025,null,"STK","ICM 80 Kondensatschale mit Ablauf 1/2\"","CHF",104,"Schiedel ICM matt",1.1000000000000001,55,"J","ICM 80 Pot de condensat avec écoulement 1/2\"","ICM 80 Kondensatschale mit Ablauf 1/2\"","ICM 80 Scarico condensa 1/2\"",134,1,"DN 80",null,90.2,"266000508M",null,null,104,"102025",13.799999999999997,82,22,"102025",104,13.799999999999997]
["102027",102027,null,"STK","ICM 130 Kondensatschale mit Ablauf 1/2\"","CHF",131,"Schiedel ICM matt",1.7,55,"J","ICM 130 Pot de condensat avec écoulement 1/2\"","ICM 130 Kondensatschale mit Ablauf 1/2\"","ICM 130 Scarico condensa 1/2\"",134,1,"DN 130",null,113.3,"266000513M",null,null,131,"102027",17.700000000000003,103,28,"102027",131,17.700000000000003]
["102030",102030,null,"STK","ICM 200 Kondensatschale mit Ablauf 1/2\"","CHF",193,"Schiedel ICM matt",2.7,55,"J","ICM 200 Pot de condensat avec écoulement 1/2\"","ICM 200 Kondensatschale mit Ablauf 1/2\"","ICM 200 Scarico condensa 1/2\"",134,1,"DN 200",null,167.2,"266000520M",null,null,193,"102030",25.800000000000011,152,41,"102030",193,25.800000000000011]
["102035",102035,null,"STK","ICM 450 Kondensatschale mit Ablauf 1/2\"","CHF",611,"Schiedel ICM matt",5.3,55,"J","ICM 450 Pot de condensat avec écoulement 1/2\"","ICM 450 Kondensatschale mit Ablauf 1/2\"","ICM 450 Scarico condensa 1/2\"",134,1,"DN 450",null,531.29999999999995,"266000545M",null,null,611,"102035",79.700000000000045,483,128,"102035",611,79.700000000000045]
["102039",102039,null,"STK","ICM 80 Teleskopstütze verstellbar L300 - 500mm","CHF",337,"Schiedel ICM matt",5.8,300,"J","ICM 80 Support téléscopique, régl.L300 - 500mm","ICM 80 Teleskopstütze verstellbar L300 - 500mm","ICM 80 Telescopio di ritenuta L300 - 500mm",134,1,"DN 80",null,292.60000000000002,"266000808M",null,null,337,"102039",44.399999999999977,266,71,"102039",337,44.399999999999977]
["102042",102042,null,"STK","ICM 150 Teleskopstütze verstellbar L300 - 500mm","CHF",384,"Schiedel ICM matt",7.5,300,"J","ICM 150 Support téléscopique, régl.L300 - 500mm","ICM 150 Teleskopstütze verstellbar L300 - 500mm","ICM 150 Telescopio di ritenuta L300 - 500mm",134,1,"DN 150",null,333.3,"266000815M",null,null,384,"102042",50.699999999999989,303,81,"102042",384,50.699999999999989]
["102044",102044,null,"STK","ICM 200 Teleskopstütze verstellbar L300 - 500mm","CHF",426,"Schiedel ICM matt",8.6999999999999993,300,"J","ICM 200 Support téléscopique, régl.L300 - 500mm","ICM 200 Teleskopstütze verstellbar L300 - 500mm","ICM 200 Telescopio di ritenuta L300 - 500mm",134,1,"DN 200",null,369.6,"266000820M",null,null,426,"102044",56.399999999999977,336,90,"102044",426,56.399999999999977]
["102047",102047,null,"STK","ICM 350 Teleskopstütze verstellbar L300 - 500mm","CHF",658,"Schiedel ICM matt",12.5,300,"J","ICM 350 Support téléscopique, régl.L300 - 500mm","ICM 350 Teleskopstütze verstellbar L300 - 500mm","ICM 350 Telescopio di ritenuta L300 - 500mm",134,1,"DN 350",null,572,"266000835M",null,null,658,"102047",86,520,138,"102047",658,86]
["102050",102050,null,"STK","ICM 500 Teleskopstütze verstellbar L300 - 500mm","CHF",1164,"Schiedel ICM matt",32.6,300,"J","ICM 500 Support téléscopique, régl.L300 - 500mm","ICM 500 Teleskopstütze verstellbar L300 - 500mm","ICM 500 Telescopio di ritenuta L300 - 500mm",134,1,"DN 500",null,1012,"266000850M",null,null,1164,"102050",152,920,244,"102050",1164,152]
[{"$f":"B1356&\"\"","v":"102053"},102053,null,"STK",{"$f":"IF($E$200=2,L1356,IF($E$200=3,N1356,M1356))","v":"ICM 130 Fussteil mit Kondensatablauf L1000mm"},"CHF",{"$f":"IF($L$190=1,W1356,S1356)","v":405},"Schiedel ICM matt",4.5,1000,"J","ICM 130 Pied colonne raccourcisable L1000mm","ICM 130 Fussteil mit Kondensatablauf L1000mm","ICM 130 Sezione piedi con scarico condensa L1000mm",134,1,"DN 130",null,352,"266000213M","104689","4037494198377",405,"102053",53,320,85,"102053",405,53]
["102058",102058,null,"STK","ICM 130 Putztüranschluss eckig Unterdruck L455mm","CHF",439,"Schiedel ICM matt",4.5999999999999996,411,"J","ICM 130  Element d'inspéction souspression L455mm","ICM 130 Putztüranschluss eckig Unterdruck L455mm","ICM 130 Elemento inspezione sotto pressione L455mm",134,1,"DN 130",null,381.7,"236900513M","104673","4037494193969",439,"102058",57.300000000000011,347,92,"102058",439,57.300000000000011]
["102062",102062,null,"STK","ICM 250 Putztüranschluss eckig Unterdruck L455mm","CHF",494,"Schiedel ICM matt",6.5,411,"J","ICM 250  Element d'inspéction souspression L455mm","ICM 250 Putztüranschluss eckig Unterdruck L455mm","ICM 250 Elemento inspezione sotto pressione L455mm",134,1,"DN 250",null,429,"236900525M",null,null,494,"102062",65,390,104,"102062",494,65]
["102066",102066,null,"STK","ICM 450 Putztüranschluss eckig Unterdruck L455mm","CHF",821,"Schiedel ICM matt",10.7,411,"J","ICM 450  Element d'inspéction souspression L455mm","ICM 450 Putztüranschluss eckig Unterdruck L455mm","ICM 450 Elemento inspezione sotto pressione L455mm",134,1,"DN 450",null,713.9,"236900545M",null,null,821,"102066",107.10000000000002,649,172,"102066",821,107.10000000000002]
["102067",102067,null,"STK","ICM 500 Putztüranschluss eckig Unterdruck L455mm","CHF",1028,"Schiedel ICM matt",11.4,411,"J","ICM 500  Element d'inspéction souspression L455mm","ICM 500 Putztüranschluss eckig Unterdruck L455mm","ICM 500 Elemento inspezione sotto pressione L455mm",134,1,"DN 500",null,893.2,"236900550M",null,null,1028,"102067",134.79999999999995,812,216,"102067",1028,134.79999999999995]
["102071",102071,null,"STK","ICM 100 Putztüranschluss rund Überdruck L288mm","CHF",337,"Schiedel ICM matt",1.9,288,"J","ICM 100 Element d'inspéction ronde ","ICM 100 Putztüranschluss rund Überdruck L288mm","ICM 100 Elemento di inspezione su pressione",134,1,"DN 100",null,292.60000000000002,"236900010M",null,null,337,"102071",44.399999999999977,266,71,"102071",337,44.399999999999977]
["102076",102076,null,"STK","ICM 250 Putztüranschluss rund Überdruck L455mm","CHF",638,"Schiedel ICM matt",6.8789999999999996,455,"J","ICM 250 Element d'inspéction ronde ","ICM 250 Putztüranschluss rund Überdruck L455mm","ICM 250 Elemento di inspezione su pressione",134,1,"DN 250",null,554.4,"236900025M",null,null,638,"102076",83.600000000000023,504,134,"102076",638,83.600000000000023]
["102079",102079,null,"STK","ICM 400 Putztüranschluss rund Überdruck L705mm","CHF",1301,"Schiedel ICM matt",11.327999999999999,705,"J","ICM 400 Element d'inspéction ronde ","ICM 400 Putztüranschluss rund Überdruck L705mm","ICM 400 Elemento di inspezione su pressione",134,1,"DN 400",null,1130.8,"236900040M",null,null,1301,"102079",170.20000000000005,1028,273,"102079",1301,170.20000000000005]
["102081",102081,null,"STK","ICM 500 Putztüranschluss rund Überdruck L705mm","CHF",1917,"Schiedel ICM matt",13.4,705,"J","ICM 500 Element d'inspéction ronde ","ICM 500 Putztüranschluss rund Überdruck L705mm","ICM 500 Elemento di inspezione su pressione",134,1,"DN 500",null,1666.5,"236900050M",null,null,1917,"102081",250.5,1515,402,"102081",1917,250.5]
["102086",102086,null,"STK","ICM 130 T-Stück 45° L455mm","CHF",343,"Schiedel ICM matt",4.2,455,"J","ICM 130 Pièce Té 45° L455mm","ICM 130 T-Stück 45° L455mm","ICM 130 Pezzo T 45° L455mm",134,1,"DN 130",null,298.10000000000002,"231404513M","104661","4037494194362",343,"102086",44.899999999999977,271,72,"102086",343,44.899999999999977]
["102090",102090,null,"STK","ICM 250 T-Stück 45° L 560mm","CHF",713,"Schiedel ICM matt",8.6999999999999993,560,"J","ICM 250 Pièce Té 45° L 560mm","ICM 250 T-Stück 45° L 560mm","ICM 250 Pezzo T 45° L 560mm",134,1,"DN 250",null,619.29999999999995,"231404525M",null,null,713,"102090",93.700000000000045,563,150,"102090",713,93.700000000000045]
["102094",102094,null,"STK","ICM 450 T-Stück 45° L 885mm","CHF",3408,"Schiedel ICM matt",19.52,885,"J","ICM 450 Pièce Té 45° L 885mm","ICM 450 T-Stück 45° L 885mm","ICM 450 Pezzo T 45° L 885mm",134,1,"DN 450",null,2963.4,"231404545M",null,null,3408,"102094",444.59999999999991,2694,714,"102094",3408,444.59999999999991]
["102097",102097,null,"STK","ICM 700 T-Stück 45° L 1245mm","CHF",5050,"Schiedel ICM matt",48,1245,"J","ICM 700 Pièce Té 45° L 1245mm","ICM 700 T-Stück 45° L 1245mm","ICM 700 Pezzo T 45° L 1245mm",134,1,"DN 700",null,4391.2,"231404570M",null,null,5050,"102097",658.80000000000018,3992,1058,"102097",5050,658.80000000000018]
["102099",102099,null,"STK","ICM 100 T-Stück 90° L288mm","CHF",275,"Schiedel ICM matt",2,288,"J","ICM 100 Pièce Té 90° L288mm","ICM 100 T-Stück 90° L288mm","ICM 100 Pezzo T 90° L288mm",134,1,"DN 100",null,238.7,"231409010M",null,null,275,"102099",36.300000000000011,217,58,"102099",275,36.300000000000011]
["102102",102102,null,"STK","ICM 180 T-Stück 90° L455mm","CHF",377,"Schiedel ICM matt",4.5999999999999996,455,"J","ICM 180 Pièce Té 90° L455mm","ICM 180 T-Stück 90° L455mm","ICM 180 Pezzo T 90° L455mm",134,1,"DN 180",null,327.8,"231409018M","104667","4037494194287",377,"102102",49.199999999999989,298,79,"102102",377,49.199999999999989]
["102108",102108,null,"STK","ICM 450 T-Stück 90° L705mm","CHF",2184,"Schiedel ICM matt",16.7,655,"J","ICM 450 Pièce Té 90° L705mm","ICM 450 T-Stück 90° L705mm","ICM 450 Pezzo T 90° L705mm",134,1,"DN 450",null,1898.6,"231409045M",null,null,2184,"102108",285.40000000000009,1726,458,"102108",2184,285.40000000000009]
["102110",102110,null,"STK","ICM 600 T-Stück 90° L705mm","CHF",3005,"Schiedel ICM matt",27.9,805,"J","ICM 600 Pièce Té 90° L705mm","ICM 600 T-Stück 90° L705mm","ICM 600 Pezzo T 90° L705mm",134,1,"DN 600",null,2612.5,"231409060M",null,null,3005,"102110",392.5,2375,630,"102110",3005,392.5]
["102113",102113,null,"STK","ICM 100 T-Stück 85° L288mm","CHF",275,"Schiedel ICM matt",2,291,"J","ICM 100 Pièce Té 85° L288mm","ICM 100 T-Stück 85° L288mm","ICM 100 Pezzo T 85° L288mm",134,1,"DN 100",null,238.7,"231408510M",null,null,275,"102113",36.300000000000011,217,58,"102113",275,36.300000000000011]
["102118",102118,null,"STK","ICM 250 T-Stück 85° L455mm","CHF",542,"Schiedel ICM matt",6.6,455,"J","ICM 250 Pièce Té 85° L455mm","ICM 250 T-Stück 85° L455mm","ICM 250 Pezzo T 85° L455mm",134,1,"DN 250",null,470.8,"231408525M",null,null,542,"102118",71.199999999999989,428,114,"102118",542,71.199999999999989]
["102122",102122,null,"STK","ICM 450 T-Stück 85° L705mm","CHF",2184,"Schiedel ICM matt",17,655,"J","ICM 450 Pièce Té 85° L705mm","ICM 450 T-Stück 85° L705mm","ICM 450 Pezzo T 85° L705mm",134,1,"DN 450",null,1898.6,"231408545M",null,null,2184,"102122",285.40000000000009,1726,458,"102122",2184,285.40000000000009]
["102125",102125,null,"STK","ICM 700 T-Stück 85° L705mm","CHF",3551,"Schiedel ICM matt",33.799999999999997,905,"J","ICM 700 Pièce Té 85° L705mm","ICM 700 T-Stück 85° L705mm","ICM 700 Pezzo T 85° L705mm",134,1,"DN 700",null,3087.7,"231408570M",null,null,3551,"102125",463.30000000000018,2807,744,"102125",3551,463.30000000000018]
["102127",102127,null,"STK","ICM 150 Inspektions-T-Stück 90° L455mm","CHF",481,"Schiedel ICM matt",4.4000000000000004,455,"J","ICM 150 Pièce Té 90° av. porte de révision L455mm","ICM 150 Inspektions-T-Stück 90° L455mm","ICM 150 Pezzo T 90° con revisione L455mm",134,1,"DN 150",null,418,"236900715M",null,null,481,"102127",63,380,101,"102127",481,63]
["102130",102130,null,"STK","ICM 250 Inspektions-T-Stück 90° L455mm","CHF",685,"Schiedel ICM matt",7.4,455,"J","ICM 250 Pièce Té 90° av. porte de révision L455mm","ICM 250 Inspektions-T-Stück 90° L455mm","ICM 250 Pezzo T 90° con revisione L455mm",134,1,"DN 250",null,595.1,"236900725M",null,null,685,"102130",89.899999999999977,541,144,"102130",685,89.899999999999977]
["102134",102134,null,"STK","ICM 130 Verschlussdeckel","CHF",146,"Schiedel ICM matt",1.7,0,"J","ICM 130 Couvercle avec poignée","ICM 130 Verschlussdeckel","ICM 130 Tapo cieco",134,1,"DN 130",null,126.5,"266002013M",null,null,146,"102134",19.5,115,31,"102134",146,19.5]
["102136",102136,null,"STK","ICM 180 Verschlussdeckel","CHF",173,"Schiedel ICM matt",2.4,0,"J","ICM 180 Couvercle avec poignée","ICM 180 Verschlussdeckel","ICM 180 Tapo cieco",134,1,"DN 180",null,149.6,"266002018M",null,null,173,"102136",23.400000000000006,136,37,"102136",173,23.400000000000006]
["102141",102141,null,"STK","ICM 400 Verschlussdeckel","CHF",329,"Schiedel ICM matt",5.0999999999999996,0,"J","ICM 400 Couvercle avec poignée","ICM 400 Verschlussdeckel","ICM 400 Tapo cieco",134,1,"DN 400",null,286,"266002040M",null,null,329,"102141",43,260,69,"102141",329,43]
["102145",102145,null,"STK","ICM 700 Verschlussdeckel","CHF",815,"Schiedel ICM matt",8.3000000000000007,0,"J","ICM 700 Couvercle avec poignée","ICM 700 Verschlussdeckel","ICM 700 Tapo cieco",134,1,"DN 700",null,708.4,"266002070M",null,null,815,"102145",106.60000000000002,644,171,"102145",815,106.60000000000002]
["102149",102149,null,"STK","ICM 150 Anschluss von EW auf DW in Rauchgasr.","CHF",152,"Schiedel ICM matt",0.80500000000000005,0,"J","ICM 150 Raccord de PPL - ICS","ICM 150 Anschluss von EW auf DW in Rauchgasr.","ICM 150 Raccordo de PPL - ICS",134,1,"DN 150",null,132,"266040015M","104732","4037494194775",152,"102149",20,120,32,"102149",152,20]
["102150",102150,null,"STK","ICM 180 Anschluss von EW auf DW in Rauchgasr.","CHF",165,"Schiedel ICM matt",0.94699999999999995,0,"J","ICM 180 Raccord de PPL - ICS","ICM 180 Anschluss von EW auf DW in Rauchgasr.","ICM 180 Raccordo de PPL - ICS",134,1,"DN 180",null,143,"266040018M","104733","4037494194782",165,"102150",22,130,35,"102150",165,22]
["102154",102154,null,"STK","ICM 350 Anschluss von EW auf DW in Rauchgasr.","CHF",247,"Schiedel ICM matt",1.718,0,"J","ICM 350 Raccord de PPL - ICS","ICM 350 Anschluss von EW auf DW in Rauchgasr.","ICM 350 Raccordo de PPL - ICS",134,1,"DN 350",null,214.5,"266040035M",null,null,247,"102154",32.5,195,52,"102154",247,32.5]
["102159",102159,null,"STK","ICM 700 Anschluss von EW auf DW in Rauchgasr.","CHF",945,"Schiedel ICM matt",4.3739999999999997,0,"J","ICM 700 Raccord de PPL - ICS","ICM 700 Anschluss von EW auf DW in Rauchgasr.","ICM 700 Raccordo de PPL - ICS",134,1,"DN 700",null,821.7,"266040070M",null,null,945,"102159",123.29999999999995,747,198,"102159",945,123.29999999999995]
["102162",102162,null,"STK","ICM 150 Anschluss DW/EW mit Klemmfutter DN130","CHF",165,"Schiedel ICM matt",1.5,0,"J","ICM 150 Raccord PPL - ICS av. manchon double DN130","ICM 150 Anschluss DW/EW mit Klemmfutter DN130","ICM 150 Adattore PPL - ICS con tubo fodera DN130",134,1,"DN 150",null,143,"266021513M","104723","4037494194096",165,"102162",22,130,35,"102162",165,22]
["102164",102164,null,"STK","ICM 180 Anschluss DW/EW mit Klemmfutter DN150","CHF",193,"Schiedel ICM matt",1.7,0,"J","ICM 180 Raccord PPL - ICS av. manchon double DN150","ICM 180 Anschluss DW/EW mit Klemmfutter DN150","ICM 180 Adattore PPL - ICS con tubo fodera DN150",134,1,"DN 180",null,167.2,"266021815M","104726","4037494199947",193,"102164",25.800000000000011,152,41,"102164",193,25.800000000000011]
["102169",102169,null,"STK","ICM 300 Anschluss DW/EW mit Klemmfutter DN300","CHF",261,"Schiedel ICM matt",3.2,0,"J","ICM 300 Raccord PPL - ICS av. manchon double DN300","ICM 300 Anschluss DW/EW mit Klemmfutter DN300","ICM 300 Adattore PPL - ICS con tubo fodera DN300",134,1,"DN 300",null,226.6,"266023030M",null,null,261,"102169",34.400000000000006,206,55,"102169",261,34.400000000000006]
["102173",102173,null,"STK","ICM 150 Anschluss von DW auf EW in Rauchgasr.","CHF",152,"Schiedel ICM matt",0.80500000000000005,0,"J","ICM 150 Raccord de ICS - PPL ","ICM 150 Anschluss von DW auf EW in Rauchgasr.","ICM 150 Adattore ICS - PPL ",134,1,"DN 150",null,132,"266041015M",null,null,152,"102173",20,120,32,"102173",152,20]
["102177",102177,null,"STK","ICM 300 Anschluss von DW auf EW in Rauchgasr.","CHF",221,"Schiedel ICM matt",1.5109999999999999,0,"J","ICM 300 Raccord de ICS - PPL ","ICM 300 Anschluss von DW auf EW in Rauchgasr.","ICM 300 Adattore ICS - PPL ",134,1,"DN 300",null,191.4,"266041030M",null,null,221,"102177",29.599999999999994,174,47,"102177",221,29.599999999999994]
["102178",102178,null,"STK","ICM 350 Anschluss von DW auf EW in Rauchgasr.","CHF",247,"Schiedel ICM matt",1.768,0,"J","ICM 350 Raccord de ICS - PPL ","ICM 350 Anschluss von DW auf EW in Rauchgasr.","ICM 350 Adattore ICS - PPL ",134,1,"DN 350",null,214.5,"266041035M",null,null,247,"102178",32.5,195,52,"102178",247,32.5]
["102182",102182,null,"STK","ICM 600 Anschluss von DW auf EW in Rauchgasr.","CHF",672,"Schiedel ICM matt",3.9710000000000001,0,"J","ICM 600 Raccord de ICS - PPL ","ICM 600 Anschluss von DW auf EW in Rauchgasr.","ICM 600 Adattore ICS - PPL ",134,1,"DN 600",null,584.1,"266041060M",null,null,672,"102182",87.899999999999977,531,141,"102182",672,87.899999999999977]
["102185",102185,null,"STK","ICM 100 Längenelement L195mm","CHF",92,"Schiedel ICM matt",0.90900000000000003,150,"J","ICM 100 Tuyau droit L195mm","ICM 100 Längenelement L195mm","ICM 100 Elemento lunghezze L195mm",134,1,"DN 100",null,79.2,"142002010M",null,null,92,"102185",12.799999999999997,72,20,"102185",92,12.799999999999997]
["102191",102191,null,"STK","ICM 300 Längenelement L195mm","CHF",173,"Schiedel ICM matt",2.31,150,"J","ICM 300 Tuyau droit L195mm","ICM 300 Längenelement L195mm","ICM 300 Elemento lunghezze L195mm",134,1,"DN 300",null,149.6,"142002030M",null,null,173,"102191",23.400000000000006,136,37,"102191",173,23.400000000000006]
["102193",102193,null,"STK","ICM 400 Längenelement L195mm","CHF",399,"Schiedel ICM matt",3.0190000000000001,150,"J","ICM 400 Tuyau droit L195mm","ICM 400 Längenelement L195mm","ICM 400 Elemento lunghezze L195mm",134,1,"DN 400",null,346.5,"142002040M",null,null,399,"102193",52.5,315,84,"102193",399,52.5]
["102196",102196,null,"STK","ICM 600 Längenelement L195mm","CHF",672,"Schiedel ICM matt",6.59,150,"J","ICM 600 Tuyau droit L195mm","ICM 600 Längenelement L195mm","ICM 600 Elemento lunghezze L195mm",134,1,"DN 600",null,584.1,"142002060M",null,null,672,"102196",87.899999999999977,531,141,"102196",672,87.899999999999977]
["102201",102201,null,"STK","ICM 150 Längenelement L250mm","CHF",111,"Schiedel ICM matt",1.5940000000000001,205,"J","ICM 150 Tuyau droit L250mm","ICM 150 Längenelement L250mm","ICM 150 Elemento lunghezze L250mm",134,1,"DN 150",null,95.7,"142002515M","104626","4037494194508",111,"102201",15.299999999999997,87,24,"102201",111,15.299999999999997]
["102205",102205,null,"STK","ICM 300 Längenelement L250mm","CHF",180,"Schiedel ICM matt",2.9209999999999998,205,"J","ICM 300 Tuyau droit L250mm","ICM 300 Längenelement L250mm","ICM 300 Elemento lunghezze L250mm",134,1,"DN 300",null,156.19999999999999,"142002530M",null,null,180,"102205",23.800000000000011,142,38,"102205",180,23.800000000000011]
["102206",102206,null,"STK","ICM 350 Längenelement L250mm","CHF",275,"Schiedel ICM matt",3.3730000000000002,205,"J","ICM 350 Tuyau droit L250mm","ICM 350 Längenelement L250mm","ICM 350 Elemento lunghezze L250mm",134,1,"DN 350",null,238.7,"142002535M",null,null,275,"102206",36.300000000000011,217,58,"102206",275,36.300000000000011]
["102209",102209,null,"STK","ICM 500 Längenelement L250mm","CHF",542,"Schiedel ICM matt",5.0650000000000004,205,"J","ICM 500 Tuyau droit L250mm","ICM 500 Längenelement L250mm","ICM 500 Elemento lunghezze L250mm",134,1,"DN 500",null,470.8,"142002550M",null,null,542,"102209",71.199999999999989,428,114,"102209",542,71.199999999999989]
["102214",102214,null,"STK","ICM 130 Längenelement L500mm","CHF",124,"Schiedel ICM matt",2.8889999999999998,455,"J","ICM 130 Tuyau droit L500mm","ICM 130 Längenelement L500mm","ICM 130 Elemento lunghezze L500mm",134,1,"DN 130",null,107.8,"142005013M","104629","4037494193983",124,"102214",16.200000000000003,98,26,"102214",124,16.200000000000003]
["102217",102217,null,"STK","ICM 200 Längenelement L500mm","CHF",165,"Schiedel ICM matt",4.17,455,"J","ICM 200 Tuyau droit L500mm","ICM 200 Längenelement L500mm","ICM 200 Elemento lunghezze L500mm",134,1,"DN 200",null,143,"142005020M","104632","4037494194461",165,"102217",22,130,35,"102217",165,22]
["102219",102219,null,"STK","ICM 300 Längenelement L500mm","CHF",247,"Schiedel ICM matt",5.9740000000000002,455,"J","ICM 300 Tuyau droit L500mm","ICM 300 Längenelement L500mm","ICM 300 Elemento lunghezze L500mm",134,1,"DN 300",null,214.5,"142005030M",null,null,247,"102219",32.5,195,52,"102219",247,32.5]
["102225",102225,null,"STK","ICM 700 Längenelement L500mm","CHF",952,"Schiedel ICM matt",14.335000000000001,455,"J","ICM 700 Tuyau droit L500mm","ICM 700 Längenelement L500mm","ICM 700 Elemento lunghezze L500mm",134,1,"DN 700",null,827.2,"142005070M",null,null,952,"102225",124.79999999999995,752,200,"102225",952,124.79999999999995]
["102228",102228,null,"STK","ICM 130 Längenelement L1000mm","CHF",207,"Schiedel ICM matt",5.8369999999999997,955,"J","ICM 130 Tuyau droit L1000mm","ICM 130 Längenelement L1000mm","ICM 130 Elemento lunghezze L1000mm",134,1,"DN 130",null,179.3,"142010013M","104633","4037494193976",207,"102228",27.699999999999989,163,44,"102228",207,27.699999999999989]
["102232",102232,null,"STK","ICM 250 Längenelement L1000mm","CHF",357,"Schiedel ICM matt",10.281000000000001,955,"J","ICM 250 Tuyau droit L1000mm","ICM 250 Längenelement L1000mm","ICM 250 Elemento lunghezze L1000mm",134,1,"DN 250",null,310.2,"142010025M",null,null,357,"102232",46.800000000000011,282,75,"102232",357,46.800000000000011]
["102233",102233,null,"STK","ICM 300 Längenelement L1000mm","CHF",399,"Schiedel ICM matt",12.081,955,"J","ICM 300 Tuyau droit L1000mm","ICM 300 Längenelement L1000mm","ICM 300 Elemento lunghezze L1000mm",134,1,"DN 300",null,346.5,"142010030M",null,null,399,"102233",52.5,315,84,"102233",399,52.5]
["102237",102237,null,"STK","ICM 500 Längenelement L1000mm","CHF",815,"Schiedel ICM matt",21.097999999999999,955,"J","ICM 500 Tuyau droit L1000mm","ICM 500 Längenelement L1000mm","ICM 500 Elemento lunghezze L1000mm",134,1,"DN 500",null,708.4,"142010050M",null,null,815,"102237",106.60000000000002,644,171,"102237",815,106.60000000000002]
["102242",102242,null,"STK","ICM 180 Schiebe-Element mit Doppelfutter DN150 ","CHF",357,"Schiedel ICM matt",3.7530000000000001,0,"J","ICM 180 Elément téléscopique avec manchon double","ICM 180 Schiebe-Element mit Doppelfutter DN150 ","ICM 180 Elemento telescopico con tubo fodera DN150",134,1,"DN 180",null,310.2,"266031815M",null,null,357,"102242",46.800000000000011,282,75,"102242",357,46.800000000000011]
[{"$f":"B1548&\"\"","v":"102245"},102245,null,"STK",{"$f":"IF($E$200=2,L1548,IF($E$200=3,N1548,M1548))","v":"ICM 200 Schiebe-Element mit Doppelfutter DN180 "},"CHF",{"$f":"IF($L$190=1,W1548,S1548)","v":439},"Schiedel ICM matt",4.1349999999999998,0,"J","ICM 200 Elément téléscopique avec manchon double","ICM 200 Schiebe-Element mit Doppelfutter DN180 ","ICM 200 Elemento telescopico con tubo fodera DN180",134,1,"DN 200",null,381.7,"266032018M",null,null,439,"102245",57.300000000000011,347,92,"102245",439,57.300000000000011]
["102248",102248,null,"STK","ICM 100 Schiebe-Element L270-375mm","CHF",221,"Schiedel ICM matt",2.54,0,"J","ICM 100 Elément téléscopique L270-375mm","ICM 100 Schiebe-Element L270-375mm","ICM 100 Elemento telescopico  L270-375mm",134,1,"DN 100",null,191.4,"142022710M",null,null,221,"102248",29.599999999999994,174,47,"102248",221,29.599999999999994]
["102251",102251,null,"STK","ICM 180 Schiebe-Element L270-375mm","CHF",261,"Schiedel ICM matt",4.0999999999999996,0,"J","ICM 180 Elément téléscopique L270-375mm","ICM 180 Schiebe-Element L270-375mm","ICM 180 Elemento telescopico  L270-375mm",134,1,"DN 180",null,226.6,"142022718M",null,null,261,"102251",34.400000000000006,206,55,"102251",261,34.400000000000006]
["102256",102256,null,"STK","ICM 400 Schiebe-Element L270-375mm","CHF",679,"Schiedel ICM matt",8.44,0,"J","ICM 400 Elément téléscopique L270-375mm","ICM 400 Schiebe-Element L270-375mm","ICM 400 Elemento telescopico  L270-375mm",134,1,"DN 400",null,589.6,"142022740M",null,null,679,"102256",89.399999999999977,536,143,"102256",679,89.399999999999977]
["102260",102260,null,"STK","ICM 700 Schiebe-Element L270-375mm","CHF",1363,"Schiedel ICM matt",14.25,0,"J","ICM 700 Elément téléscopique L270-375mm","ICM 700 Schiebe-Element L270-375mm","ICM 700 Elemento telescopico  L270-375mm",134,1,"DN 700",null,1184.7,"142022770M",null,null,1363,"102260",178.29999999999995,1077,286,"102260",1363,178.29999999999995]
["102261",102261,null,"STK","ICM 80 Klemmband DN130","CHF",19,"Schiedel ICM matt",0.20100000000000001,0,"J","ICM 80 Bride de fixation entre les tuyaux DN130","ICM 80 Klemmband DN130","ICM 80 Fascetta di sicurezza DN130",134,1,"DN 80",null,16.5,"266002208M",null,null,19,"102261",2.5,15,4,"102261",19,2.5]
["102265",102265,null,"STK","ICM 180 Klemmband DN230","CHF",25,"Schiedel ICM matt",0.29799999999999999,0,"J","ICM 180 Bride de fixation entre les tuyaux DN230","ICM 180 Klemmband DN230","ICM 180 Fascetta di sicurezza DN230",134,1,"DN 180",null,20.9,"266002218M",null,null,25,"102265",4.1000000000000014,19,6,"102265",25,4.1000000000000014]
["102269",102269,null,"STK","ICM 350 Klemmband DN400","CHF",32,"Schiedel ICM matt",0.46100000000000002,0,"J","ICM 350 Bride de fixation entre les tuyaux DN400","ICM 350 Klemmband DN400","ICM 350 Fascetta di sicurezza DN400",134,1,"DN 350",null,27.5,"266002235M",null,null,32,"102269",4.5,25,7,"102269",32,4.5]
["102274",102274,null,"STK","ICM 700 Klemmband DN750","CHF",46,"Schiedel ICM matt",0.8,0,"J","ICM 700 Bride de fixation entre les tuyaux DN750","ICM 700 Klemmband DN750","ICM 700 Fascetta di sicurezza DN750",134,1,"DN 700",null,39.6,"266002270M",null,null,46,"102274",6.3999999999999986,36,10,"102274",46,6.3999999999999986]
["102276",102276,null,"STK","ICM 100 Statisches Klemmband DN150","CHF",35,"Schiedel ICM matt",0.315,0,"J","ICM 100 Bride statique large DN150","ICM 100 Statisches Klemmband DN150","ICM 100 Fascetta di sicurezza statico DN150",134,1,"DN 100",null,29.7,"266002310M",null,null,35,"102276",5.3000000000000007,27,8,"102276",35,5.3000000000000007]
["102279",102279,null,"STK","ICM 180 Statisches Klemmband DN230","CHF",42,"Schiedel ICM matt",0.42499999999999999,0,"J","ICM 180 Bride statique large DN230","ICM 180 Statisches Klemmband DN230","ICM 180 Fascetta di sicurezza statico DN230",134,1,"DN 180",null,36.299999999999997,"266002318M","104719","4037494195055",42,"102279",5.7000000000000028,33,9,"102279",42,5.7000000000000028]
["102284",102284,null,"STK","ICM 400 Statisches Klemmband DN450","CHF",62,"Schiedel ICM matt",0.72799999999999998,0,"J","ICM 400 Bride statique large DN450","ICM 400 Statisches Klemmband DN450","ICM 400 Fascetta di sicurezza statico DN450",134,1,"DN 400",null,53.9,"266002340M",null,null,62,"102284",8.1000000000000014,49,13,"102284",62,8.1000000000000014]
["102287",102287,null,"STK","ICM 600 Statisches Klemmband DN650","CHF",122,"Schiedel ICM matt",1.004,0,"J","ICM 600 Bride statique large DN650","ICM 600 Statisches Klemmband DN650","ICM 600 Fascetta di sicurezza statico DN650",134,1,"DN 600",null,105.6,"266002360M",null,null,122,"102287",16.400000000000006,96,26,"102287",122,16.400000000000006]
["102288",102288,null,"STK","ICM 700 Statisches Klemmband DN750","CHF",183,"Schiedel ICM matt",1.1399999999999999,0,"J","ICM 700 Bride statique large DN750","ICM 700 Statisches Klemmband DN750","ICM 700 Fascetta di sicurezza statico DN750",134,1,"DN 700",null,158.4,"266002370M",null,null,183,"102288",24.599999999999994,144,39,"102288",183,24.599999999999994]
["102292",102292,null,"STK","ICM 150 Wandhalter verstellbar 75 - 300mm DN 200mm","CHF",92,"Schiedel ICM matt",1.66,0,"J","ICM 150 Fixation murale régl. 75 - 300mm DN 200mm","ICM 150 Wandhalter verstellbar 75 - 300mm DN 200mm","ICM 150 Collare a muro regolabile 75-300mm DN200mm",134,1,"DN 150",null,79.2,"95960200M",null,null,92,"102292",12.799999999999997,72,20,"102292",92,12.799999999999997]
["102297",102297,null,"STK","ICM 350 Wandhalter verstellbar 75 - 300mm DN 400mm","CHF",124,"Schiedel ICM matt",2.7509999999999999,0,"J","ICM 350 Fixation murale régl. 75 - 300mm DN 400mm","ICM 350 Wandhalter verstellbar 75 - 300mm DN 400mm","ICM 350 Collare a muro regolabile 75-300mm DN400mm",134,1,"DN 300",null,107.8,"95960400M",null,null,124,"102297",16.200000000000003,98,26,"102297",124,16.200000000000003]
["102300",102300,null,"STK","ICM 500 Wandhalter verstellbar 75 - 300mm DN 550mm","CHF",207,"Schiedel ICM matt",3.41,0,"J","ICM 500 Fixation murale régl. 75 - 300mm DN 550mm","ICM 500 Wandhalter verstellbar 75 - 300mm DN 550mm","ICM 500 Collare a muro regolabile 75-300mm DN550mm",134,1,"DN 300",null,179.3,"95960550M",null,null,207,"102300",27.699999999999989,163,44,"102300",207,27.699999999999989]
["102302",102302,null,"STK","ICM 700 Wandhalter verstellbar 75 - 300mm DN 750mm","CHF",343,"Schiedel ICM matt",4.05,0,"J","ICM 700 Fixation murale régl. 75 - 300mm DN 750mm","ICM 700 Wandhalter verstellbar 75 - 300mm DN 750mm","ICM 700 Collare a muro regolabile 75-300mm DN750mm",134,1,"DN 300",null,298.10000000000002,"95960750M",null,null,343,"102302",44.899999999999977,271,72,"102302",343,44.899999999999977]
["102308",102308,null,"STK","ICM 200 Wandhalter 50mm verlängerbar DN 250mm","CHF",76,"Schiedel ICM matt",0.7,0,"J","ICM 200 Fixation muraler 50mm régl. DN 250mm","ICM 200 Wandhalter 50mm verlängerbar DN 250mm","ICM 200 Collare a muro per prolunga 50mm  DN 250mm",134,1,"DN 200",null,66,"95090250M",null,null,76,"102308",10,60,16,"102308",76,10]
["102311",102311,null,"STK","ICM 350 Wandhalter 50mm verlängerbar DN 400mm ","CHF",138,"Schiedel ICM matt",1.4,0,"J","ICM 350 Fixation muraler 50mm régl. DN 400mm ","ICM 350 Wandhalter 50mm verlängerbar DN 400mm ","ICM 350 Collare a muro per prolunga 50mm  DN 400mm",134,1,"DN 350",null,119.9,"95090400M",null,null,138,"102311",18.099999999999994,109,29,"102311",138,18.099999999999994]
["102315",102315,null,"STK","ICM 600 Wandhalter 50mm verlängerbar DN 650mm  ","CHF",289,"Schiedel ICM matt",3.2,0,"J","ICM 600 Fixation muraler 50mm régl. DN 650mm  ","ICM 600 Wandhalter 50mm verlängerbar DN 650mm  ","ICM 600 Collare a muro per prolunga 50mm  DN 650mm",134,1,"DN 600",null,250.8,"95090650M",null,null,289,"102315",38.199999999999989,228,61,"102315",289,38.199999999999989]
["102316",102316,null,"STK","ICM 700 Wandhalter 50mm verlängerbar DN 750mm ","CHF",357,"Schiedel ICM matt",4,0,"J","ICM 700 Fixation muraler 50mm régl. DN 750mm ","ICM 700 Wandhalter 50mm verlängerbar DN 750mm ","ICM 700 Collare a muro per prolunga 50mm  DN 750mm",134,1,"DN 700",null,310.2,"95090750M",null,null,357,"102316",46.800000000000011,282,75,"102316",357,46.800000000000011]
["102320",102320,null,"PAR","ICM L2 Verlängerung zu Wandhalter 50mm L450mm","CHF",180,"Schiedel ICM matt",0.95,0,"J","ICM L2 Ralogement pour fixation murale L450mm","ICM L2 Verlängerung zu Wandhalter 50mm L450mm","ICM L2 Prolunga per collare 50mm L450mm",134,1,"ZBH ICM",null,156.19999999999999,"267100450M",null,null,180,"102320",23.800000000000011,142,38,"102320",180,23.800000000000011]
["102324",102324,null,"STK","ICM 130 Dachdurführung 0° DN200 L500mm","CHF",193,"Schiedel ICM matt",3.86,0,"J","ICM 130 Garniture de toiture 0° DN200 L500mm","ICM 130 Dachdurführung 0° DN200 L500mm","ICM 130 Faldale piatto 0° DN200 L500mm",134,1,"DN 130",null,167.2,"266320200M",null,null,193,"102324",25.800000000000011,152,41,"102324",193,25.800000000000011]
["102329",102329,null,"STK","ICM 350 Dachdurführung 0° DN450 L500mm","CHF",432,"Schiedel ICM matt",7.72,0,"J","ICM 350 Garniture de toiture 0° DN450 L500mm","ICM 350 Dachdurführung 0° DN450 L500mm","ICM 350 Faldale piatto 0° DN450 L500mm",134,1,"DN 350",null,375.1,"266322450M",null,null,432,"102329",56.899999999999977,341,91,"102329",432,56.899999999999977]
["102331",102331,null,"STK","ICM 450 Dachdurführung 0° DN550 L500mm","CHF",821,"Schiedel ICM matt",9.44,0,"J","ICM 450 Garniture de toiture 0° DN550 L500mm","ICM 450 Dachdurführung 0° DN550 L500mm","ICM 450 Faldale piatto 0° DN550 L500mm",134,1,"DN 450",null,713.9,"266322550M",null,null,821,"102331",107.10000000000002,649,172,"102331",821,107.10000000000002]
["102334",102334,null,"STK","ICM 700 Dachdurführung 0° DN800 L500mm","CHF",1506,"Schiedel ICM matt",14.14,0,"J","ICM 700 Garniture de toiture 0° DN800 L500mm","ICM 700 Dachdurführung 0° DN800 L500mm","ICM 700 Faldale piatto 0° DN800 L500mm",134,1,"DN 700",null,1309,"266322800M",null,null,1506,"102334",197,1190,316,"102334",1506,197]
["102339",102339,null,"STK","ICM 250-300 Dachdurführung 16-25° DN370 ","CHF",562,"Schiedel ICM matt",16.2,0,"J","ICM 250-300 Garniture de toiture 16-25° DN370 ","ICM 250-300 Dachdurführung 16-25° DN370 ","ICM 250-300 Faldale 16-25° DN370 compressa piomba",134,1,"DN 250",null,488.4,"266322370M",null,null,562,"102339",73.600000000000023,444,118,"102339",562,73.600000000000023]
["102343",102343,null,"STK","ICM 450 Dachdurführung 16-25° DN550 mit Bleilappen","CHF",1028,"Schiedel ICM matt",24.99,0,"J","ICM 450 Garniture de toiture 16-25° DN550 ","ICM 450 Dachdurführung 16-25° DN550 mit Bleilappen","ICM 450 Faldale 16-25° DN550 compressa in piomba",134,1,"DN 450",null,893.2,"266323550M",null,null,1028,"102343",134.79999999999995,812,216,"102343",1028,134.79999999999995]
["102344",102344,null,"STK","ICM 500 Dachdurführung 16-25° DN600 mit Bleilappen","CHF",1164,"Schiedel ICM matt",27.09,0,"J","ICM 500 Garniture de toiture 16-25° DN600 ","ICM 500 Dachdurführung 16-25° DN600 mit Bleilappen","ICM 500 Faldale 16-25° DN600 compressa in piomba",134,1,"DN 500",null,1012,"266323600M",null,null,1164,"102344",152,920,244,"102344",1164,152]
["102348",102348,null,"STK","ICM 130 Dachdurführung 26-35° DN200 mit Bleilappen","CHF",494,"Schiedel ICM matt",12.11,0,"J","ICM 130 Garniture de toiture 26-35° DN200 ","ICM 130 Dachdurführung 26-35° DN200 mit Bleilappen","ICM 130 Faldale 26-35° DN200 compressa in piomba",134,1,"DN 130",null,429,"266323200M",null,null,494,"102348",65,390,104,"102348",494,65]
["102352",102352,null,"STK","ICM 300 Dachdurführung 26-35° DN400 mit Bleilappen","CHF",741,"Schiedel ICS glänzend",22.74,0,"J","ICM 300 Garniture de toiture 26-35° DN400 ","ICM 300 Dachdurführung 26-35° DN400 mit Bleilappen","ICM 300 Faldale 26-35° DN400 compressa in piomba",133,1,"DN 300",null,643.5,"266322400M",null,null,741,"102352",97.5,585,156,"102352",741,97.5]
["102357",102357,null,"STK","ICM 600 Dachdurführung 26-35° DN700 mit Bleilappen","CHF",1439,"Schiedel ICM matt",41.05,0,"J","ICM 600 Garniture de toiture 26-35° DN700 ","ICM 600 Dachdurführung 26-35° DN700 mit Bleilappen","ICM 600 Faldale 26-35° DN700 compressa in piomba",134,1,"DN 600",null,1250.7,"266322700M",null,null,1439,"102357",188.29999999999995,1137,302,"102357",1439,188.29999999999995]
["102359",102359,null,"STK","ICM 80-100 Dachdurführung 36-45° DN165  ","CHF",508,"Schiedel ICM matt",12.6,0,"J","ICM 80-100 Garniture de toiture 36-45° DN165  ","ICM 80-100 Dachdurführung 36-45° DN165  ","ICM 80-100 Faldale 36-45° DN165 compressa piomba",134,1,"DN 80",null,441.1,"266324165M",null,null,508,"102359",66.899999999999977,401,107,"102359",508,66.899999999999977]
["102362",102362,null,"STK","ICM 200 Dachdurführung 36-45° DN320 mit Bleilappen","CHF",630,"Schiedel ICM matt",18.510000000000002,0,"J","ICM 200 Garniture de toiture 36-45° DN320 ","ICM 200 Dachdurführung 36-45° DN320 mit Bleilappen","ICM 200 Faldale 36-45° DN320 compressa in piomba",134,1,"DN 200",null,547.79999999999995,"266324320M",null,null,630,"102362",82.200000000000045,498,132,"102362",630,82.200000000000045]
["102367",102367,null,"STK","ICM 450 Dachdurführung 36-45° DN550 mit Bleilappen","CHF",1369,"Schiedel ICM matt",31.59,0,"J","ICM 450 Garniture de toiture 36-45° DN550 ","ICM 450 Dachdurführung 36-45° DN550 mit Bleilappen","ICM 450 Faldale 36-45° DN550 compressa in piomba",134,1,"DN 450",null,1190.2,"266322550M",null,null,1369,"102367",178.79999999999995,1082,287,"102367",1369,178.79999999999995]
["102368",102368,null,"STK","ICM 500 Dachdurführung 36-45° DN600 mit Bleilappen","CHF",1575,"Schiedel ICM matt",34.46,0,"J","ICM 500 Garniture de toiture 36-45° DN600 ","ICM 500 Dachdurführung 36-45° DN600 mit Bleilappen","ICM 500 Faldale 36-45° DN600 compressa in piomba",134,1,"DN 500",null,1369.5,"266322600M",null,null,1575,"102368",205.5,1245,330,"102368",1575,205.5]
["102371",102371,null,"STK","ICM 80 Regenkragen DN130 ","CHF",42,"Schiedel ICM matt",0.28999999999999998,0,"J","ICM 80 Collerette anti pluie  DN130 ","ICM 80 Regenkragen DN130 ","ICM 80 Scossalina DN130 ",134,1,"DN 80",null,36.299999999999997,"265830130M",null,null,42,"102371",5.7000000000000028,33,9,"102371",42,5.7000000000000028]
["102375",102375,null,"STK","ICM 180 Regenkragen DN230","CHF",70,"Schiedel ICM matt",0.39,0,"J","ICM 180 Collerette anti pluie  DN230","ICM 180 Regenkragen DN230","ICM 180 Scossalina DN230",134,1,"DN 180",null,60.5,"265830230M","104683","4037494193693",70,"102375",9.5,55,15,"102375",70,9.5]
["102380",102380,null,"STK","ICM 400 Regenkragen DN450","CHF",124,"Schiedel ICM matt",1.05,0,"J","ICM 400 Collerette anti pluie  DN450","ICM 400 Regenkragen DN450","ICM 400 Scossalina DN450",134,1,"DN 400",null,107.8,"265830450M",null,null,124,"102380",16.200000000000003,98,26,"102380",124,16.200000000000003]
["102383",102383,null,"STK","ICM 600 Regenkragen DN650","CHF",193,"Schiedel ICM matt",1.45,0,"J","ICM 600 Collerette anti pluie  DN650","ICM 600 Regenkragen DN650","ICM 600 Scossalina DN650",134,1,"DN 600",null,167.2,"265830650M",null,null,193,"102383",25.800000000000011,152,41,"102383",193,25.800000000000011]
["102385",102385,null,"STK","ICM 80 Seilabspannring DN130 ","CHF",70,"Schiedel ICM matt",0.436,0,"J","ICM 80 Bride de haubannage DN130 ","ICM 80 Seilabspannring DN130 ","ICM 80 Collare per cavi tiranti DN130 ",134,1,"DN 80",null,60.5,"95900130M",null,null,70,"102385",9.5,55,15,"102385",70,9.5]
["102391",102391,null,"STK","ICM 250 Seilabspannring DN300","CHF",111,"Schiedel ICM matt",0.68,0,"J","ICM 250 Bride de haubannage DN300","ICM 250 Seilabspannring DN300","ICM 250 Collare per cavi tiranti DN300",134,1,"DN 250",null,95.7,"95900300M",null,null,111,"102391",15.299999999999997,87,24,"102391",111,15.299999999999997]
["102394",102394,null,"STK","ICM 400 Seilabspannring DN450","CHF",138,"Schiedel ICM matt",0.5,0,"J","ICM 400 Bride de haubannage DN450","ICM 400 Seilabspannring DN450","ICM 400 Collare per cavi tiranti DN450",134,1,"DN 400",null,119.9,"95900450M",null,null,138,"102394",18.099999999999994,109,29,"102394",138,18.099999999999994]
["102396",102396,null,"STK","ICM 500 Seilabspannring DN550","CHF",193,"Schiedel ICM matt",0.7,0,"J","ICM 500 Bride de haubannage DN550","ICM 500 Seilabspannring DN550","ICM 500 Collare per cavi tiranti DN550",134,1,"DN 500",null,167.2,"95900550M",null,null,193,"102396",25.800000000000011,152,41,"102396",193,25.800000000000011]
["102399",102399,null,"STK","ICM 80 Blende 0-30° DN130 ","CHF",76,"Schiedel ICM matt",1,0,"J","ICM 80 Recouvrement carrée0-30° DN130 ","ICM 80 Blende 0-30° DN130 ","ICM 80 Coperture 0-30° DN130 ",134,1,"DN 80",null,66,"266001408M",null,null,76,"102399",10,60,16,"102399",76,10]
["102403",102403,null,"STK","ICM 180 Blende 0-30° DN230","CHF",93,"Schiedel ICM matt",1.6,0,"J","ICM 180 Recouvrement carrée0-30° DN230","ICM 180 Blende 0-30° DN230","ICM 180 Coperture 0-30° DN230",134,1,"DN 180",null,80.3,"266001418M","104711","4051921059888",93,"102403",12.700000000000003,73,20,"102403",93,12.700000000000003]
["102407",102407,null,"STK","ICM 80 Blende 32-45° DN130 ","CHF",92,"Schiedel ICM matt",1,0,"J","ICM 80 Recouvrement carrée32-45° DN130 ","ICM 80 Blende 32-45° DN130 ","ICM 80 Coperture 32-45° DN130 ",134,1,"DN 80",null,79.2,"266001508M",null,null,92,"102407",12.799999999999997,72,20,"102407",92,12.799999999999997]
["102412",102412,null,"STK","ICM 200 Blende 32-45° DN250","CHF",111,"Schiedel ICM matt",1.8,0,"J","ICM 200 Recouvrement carrée32-45° DN250","ICM 200 Blende 32-45° DN250","ICM 200 Coperture 32-45° DN250",134,1,"DN 200",null,95.7,"266001520M","104716","4037494199220",111,"102412",15.299999999999997,87,24,"102412",111,15.299999999999997]
["102415",102415,null,"STK","ICM 80 Anschlussrosette Øi 130mm ØA 400mm","CHF",70,"Schiedel ICM matt",0.69,0,"J","ICM 80 Rosace de raccordement Øi 130mm ØA 400mm","ICM 80 Anschlussrosette Øi 130mm ØA 400mm","ICM 80 Rosetta di collegamento Øi 130mm ØA 400mm",134,1,"DN 80",null,60.5,"265404408M",null,null,70,"102415",9.5,55,15,"102415",70,9.5]
["102417",102417,null,"STK","ICM 130 Anschlussrosette Øi 180mm ØA 450mm","CHF",75,"Schiedel ICM matt",0.43,0,"J","ICM 130 Rosace de raccordement Øi 180mm ØA 450mm","ICM 130 Anschlussrosette Øi 180mm ØA 450mm","ICM 130 Rosetta di collegamento Øi 180mm ØA 450mm",134,1,"DN 130",null,64.900000000000006,"265404413M",null,null,75,"102417",10.099999999999994,59,16,"102417",75,10.099999999999994]
["102422",102422,null,"STK","ICM 300 Anschlussrosette Øi 350mm ØA 620mm","CHF",90,"Schiedel ICM matt",0.54,0,"J","ICM 300 Rosace de raccordement Øi 350mm ØA 620mm","ICM 300 Anschlussrosette Øi 350mm ØA 620mm","ICM 300 Rosetta di collegamento Øi 350mm ØA 620mm",134,1,"DN 300",null,78.099999999999994,"265404430M",null,null,90,"102422",11.900000000000006,71,19,"102422",90,11.900000000000006]
["102428",102428,null,"STK","ICM 200 Anschlussrosette EW Øi 250mm ØA 420mm","CHF",56,"Schiedel ICM matt",0.52,0,"J","ICM 200 Rosace de raccordement EW Øi250mm ØA 420mm","ICM 200 Anschlussrosette EW Øi 250mm ØA 420mm","ICM 200 Rosetta collegamento EW Øi 250mm ØA 420mm",134,1,"DN 200",null,48.4,"025620025M",null,null,56,"102428",7.6000000000000014,44,12,"102428",56,7.6000000000000014]
["102429",102429,null,"STK","ICM 250 Anschlussrosette EW Øi 300mm ØA 470mm","CHF",62,"Schiedel ICM matt",0.57999999999999996,0,"J","ICM 250 Rosace de raccordement EW Øi300mm ØA 470mm","ICM 250 Anschlussrosette EW Øi 300mm ØA 470mm","ICM 250 Rosetta collegamento EW Øi 300mm ØA 470mm",134,1,"DN 250",null,53.9,"025620030M",null,null,62,"102429",8.1000000000000014,49,13,"102429",62,8.1000000000000014]
["102434",102434,null,"STK","ICM 150 Mündungsabschluss","CHF",165,"Schiedel ICM matt",1.482,295,"J","ICM 150 Cape de finition conique","ICM 150 Mündungsabschluss","ICM 150 Terminale conico",134,1,"DN 150",null,143,"266200015M","104748","4037494194546",165,"102434",22,130,35,"102434",165,22]
["102438",102438,null,"STK","ICM 300 Mündungsabschluss","CHF",275,"Schiedel ICM matt",2.7629999999999999,295,"J","ICM 300 Cape de finition conique","ICM 300 Mündungsabschluss","ICM 300 Terminale conico",134,1,"DN 300",null,238.7,"266200030M",null,null,275,"102438",36.300000000000011,217,58,"102438",275,36.300000000000011]
["102443",102443,null,"STK","ICM 600 Mündungsabschluss","CHF",795,"Schiedel ICM matt",5.1630000000000003,295,"J","ICM 600 Cape de finition conique","ICM 600 Mündungsabschluss","ICM 600 Terminale conico",134,1,"DN 600",null,690.8,"266200060M",null,null,795,"102443",104.20000000000005,628,167,"102443",795,104.20000000000005]
["102446",102446,null,"STK","ICM 130 Basten Standart mit Stulpring Inox matt","CHF",385,"Zubehör",3.9,0,"J","ICM 130 Basten Standart avec dila Inox matt","ICM 130 Basten Standart mit Stulpring Inox matt","ICM 130 Terminale Basten con dila Inox matt",15,2,"DN 130",null,363,"916513",null,null,385,"102446",22,361,24,"102446",385,22]
["102449",102449,null,"STK","ICM 200 Basten Standart mit Stulpring Inox matt","CHF",435,"Zubehör",4.5,0,"J","ICM 200 Basten Standart avec dila Inox matt","ICM 200 Basten Standart mit Stulpring Inox matt","ICM 200 Terminale Basten con dila Inox matt",15,2,"DN 200",null,410,"916520",null,null,435,"102449",25,408,27,"102449",435,25]
["102452",102452,null,"STK","ICM 80 Element mit Messöffnung1/2\" L205mm","CHF",193,"Schiedel ICM matt",1.0289999999999999,0,"J","ICM 80 Element avec manchon de mésure 1/2\" L205mm","ICM 80 Element mit Messöffnung1/2\" L205mm","ICM 80 Elemento di missura 1/2\" L205mm",134,1,"DN 80",null,167.2,"266002508M",null,null,193,"102452",25.800000000000011,152,41,"102452",193,25.800000000000011]
["102454",102454,null,"STK","ICM 130 Element mit Messöffnung1/2\" L205mm","CHF",221,"Schiedel ICM matt",1.49,0,"J","ICM 130 Element avec manchon de mésure 1/2\" L205mm","ICM 130 Element mit Messöffnung1/2\" L205mm","ICM 130 Elemento di missura 1/2\" L205mm",134,1,"DN 130",null,191.4,"266002513M",null,null,221,"102454",29.599999999999994,174,47,"102454",221,29.599999999999994]
["102457",102457,null,"STK","ICM 200 Element mit Messöffnung1/2\" L205mm","CHF",261,"Schiedel ICM matt",2.137,0,"J","ICM 200 Element avec manchon de mésure 1/2\" L205mm","ICM 200 Element mit Messöffnung1/2\" L205mm","ICM 200 Elemento di missura 1/2\" L205mm",134,1,"DN 200",null,226.6,"266002520M",null,null,261,"102457",34.400000000000006,206,55,"102457",261,34.400000000000006]
["102462",102462,null,"STK","ICM 450 Element mit Messöffnung1/2\" L205mm","CHF",618,"Schiedel ICM matt",4.6879999999999997,0,"J","ICM 450 Element avec manchon de mésure 1/2\" L205mm","ICM 450 Element mit Messöffnung1/2\" L205mm","ICM 450 Elemento di missura 1/2\" L205mm",134,1,"DN 450",null,536.79999999999995,"266002545M",null,null,618,"102462",81.200000000000045,488,130,"102462",618,81.200000000000045]
["102466",102466,null,"STK","ICM 80 Element mit Kondensatablauf 1/2\" L205mm","CHF",193,"Schiedel ICM matt",1.03,0,"J","ICM 80 Element avec écoulement cond. 1/2\" L205mm","ICM 80 Element mit Kondensatablauf 1/2\" L205mm","ICM 80 Elemento con scarico condensa 1/2\" L205mm",134,1,"DN 80",null,167.2,"266002808M",null,null,193,"102466",25.800000000000011,152,41,"102466",193,25.800000000000011]
["102469",102469,null,"STK","ICM 150 Element mit Kondensatablauf 1/2\" L205mm","CHF",235,"Schiedel ICM matt",1.675,0,"J","ICM 150 Element avec écoulement cond. 1/2\" L205mm","ICM 150 Element mit Kondensatablauf 1/2\" L205mm","ICM 150 Elemento con scarico condensa 1/2\" L205mm",134,1,"DN 150",null,203.5,"266002815M",null,null,235,"102469",31.5,185,50,"102469",235,31.5]
["102471",102471,null,"STK","ICM 200 Element mit Kondensatablauf 1/2\" L205mm","CHF",261,"Schiedel ICM matt",2.137,0,"J","ICM 200 Element avec écoulement cond. 1/2\" L205mm","ICM 200 Element mit Kondensatablauf 1/2\" L205mm","ICM 200 Elemento con scarico condensa 1/2\" L205mm",134,1,"DN 200",null,226.6,"266002820M",null,null,261,"102471",34.400000000000006,206,55,"102471",261,34.400000000000006]
["102477",102477,null,"STK","ICM 500 Element mit Kondensatablauf 1/2\" L205mm","CHF",891,"Schiedel ICM matt",5.165,0,"J","ICM 500 Element avec écoulement cond. 1/2\" L205mm","ICM 500 Element mit Kondensatablauf 1/2\" L205mm","ICM 500 Elemento con scarico condensa 1/2\" L205mm",134,1,"DN 500",null,774.4,"266002850M",null,null,891,"102477",116.60000000000002,704,187,"102477",891,116.60000000000002]
["102480",102480,null,"STK","ICM 80 Winkel 15° ","CHF",165,"Schiedel ICM matt",0.73899999999999999,0,"J","ICM 80 Coude 15° ","ICM 80 Winkel 15° ","ICM 80 Gomito 15° ",134,1,"DN 80",null,143,"142031508M",null,null,165,"102480",22,130,35,"102480",165,22]
["102482",102482,null,"STK","ICM 130 Winkel 15° ","CHF",186,"Schiedel ICM matt",1.0840000000000001,0,"J","ICM 130 Coude 15° ","ICM 130 Winkel 15° ","ICM 130 Gomito 15° ",134,1,"DN 130",null,161.69999999999999,"142031513M","104641","4051921053114",186,"102482",24.300000000000011,147,39,"102482",186,24.300000000000011]
["102485",102485,null,"STK","ICM 200 Winkel 15° ","CHF",228,"Schiedel ICM matt",1.5660000000000001,0,"J","ICM 200 Coude 15° ","ICM 200 Winkel 15° ","ICM 200 Gomito 15° ",134,1,"DN 200",null,198,"142031520M","104644","4037494933053",228,"102485",30,180,48,"102485",228,30]
["102489",102489,null,"STK","ICM 100 Winkel 30°","CHF",180,"Schiedel ICM matt",0.877,0,"J","ICM 100 Coude 30°","ICM 100 Winkel 30°","ICM 100 Gomito 30°",134,1,"DN 100",null,156.19999999999999,"142033010M",null,null,180,"102489",23.800000000000011,142,38,"102489",180,23.800000000000011]
["102493",102493,null,"STK","ICM 200 Winkel 30°","CHF",235,"Schiedel ICM matt",1.98,0,"J","ICM 200 Coude 30°","ICM 200 Winkel 30°","ICM 200 Gomito 30°",134,1,"DN 200",null,203.5,"142033020M","104648","4037494194621",235,"102493",31.5,185,50,"102493",235,31.5]
["102498",102498,null,"STK","ICM 450 Winkel 30°","CHF",685,"Schiedel ICM matt",6.7149999999999999,0,"J","ICM 450 Coude 30°","ICM 450 Winkel 30°","ICM 450 Gomito 30°",134,1,"DN 450",null,595.1,"142033045M",null,null,685,"102498",89.899999999999977,541,144,"102498",685,89.899999999999977]
["102501",102501,null,"STK","ICM 700 Winkel 30°","CHF",1233,"Schiedel ICM matt",11.978,0,"J","ICM 700 Coude 30°","ICM 700 Winkel 30°","ICM 700 Gomito 30°",134,1,"DN 700",null,1071.4000000000001,"142033070M",null,null,1233,"102501",161.59999999999991,974,259,"102501",1233,161.59999999999991]
["102503",102503,null,"STK","ICM 100 Winkel 45°","CHF",180,"Schiedel ICM matt",1.109,0,"J","ICM 100 Coude 45°","ICM 100 Winkel 45°","ICM 100 Gomito 45°",134,1,"DN 100",null,156.19999999999999,"142034510M",null,null,180,"102503",23.800000000000011,142,38,"102503",180,23.800000000000011]
["102508",102508,null,"STK","ICM 250 Winkel 45°","CHF",261,"Schiedel ICM matt",2.819,0,"J","ICM 250 Coude 45°","ICM 250 Winkel 45°","ICM 250 Gomito 45°",134,1,"DN 250",null,226.6,"142034525M",null,null,261,"102508",34.400000000000006,206,55,"102508",261,34.400000000000006]
["102512",102512,null,"STK","ICM 450 Winkel 45°","CHF",685,"Schiedel ICM matt",7.8760000000000003,0,"J","ICM 450 Coude 45°","ICM 450 Winkel 45°","ICM 450 Gomito 45°",134,1,"DN 450",null,595.1,"142034545M",null,null,685,"102512",89.899999999999977,541,144,"102512",685,89.899999999999977]
["102513",102513,null,"STK","ICM 500 Winkel 45°","CHF",849,"Schiedel ICM matt",9.1259999999999994,0,"J","ICM 500 Coude 45°","ICM 500 Winkel 45°","ICM 500 Gomito 45°",134,1,"DN 500",null,738.1,"142034550M",null,null,849,"102513",110.89999999999998,671,178,"102513",849,110.89999999999998]
["102517",102517,null,"STK","ICM 100 Winkel 85°","CHF",200,"Schiedel ICM matt",1.5,0,"J","ICM 100 Coude 85°","ICM 100 Winkel 85°","ICM 100 Gomito 85°",134,1,"DN 100",null,173.8,"142038510M",null,null,200,"102517",26.199999999999989,158,42,"102517",200,26.199999999999989]
["102521",102521,null,"STK","ICM 200 Winkel 85°","CHF",302,"Schiedel ICM matt",3.39,0,"J","ICM 200 Coude 85°","ICM 200 Winkel 85°","ICM 200 Gomito 85°",134,1,"DN 200",null,261.8,"142038520M",null,null,302,"102521",40.199999999999989,238,64,"102521",302,40.199999999999989]
["102524",102524,null,"STK","ICM 350 Winkel 85°","CHF",548,"Schiedel ICM matt",7.33,0,"J","ICM 350 Coude 85°","ICM 350 Winkel 85°","ICM 350 Gomito 85°",134,1,"DN 350",null,476.3,"142038535M",null,null,548,"102524",71.699999999999989,433,115,"102524",548,71.699999999999989]
["102526",102526,null,"STK","ICM 450 Winkel 85°","CHF",1028,"Schiedel ICM matt",11.615,0,"J","ICM 450 Coude 85°","ICM 450 Winkel 85°","ICM 450 Gomito 85°",134,1,"DN 450",null,893.2,"142038545M",null,null,1028,"102526",134.79999999999995,812,216,"102526",1028,134.79999999999995]
["102532",102532,null,"STK","ICM 130 Inspektions-Winkel 85°","CHF",481,"Schiedel ICM matt",2.68,0,"J","ICM 130 Coude avec inspection 85°","ICM 130 Inspektions-Winkel 85°","ICM 130 Gmoito con revisione 85°",134,1,"DN 130",null,418,"142038713M",null,null,481,"102532",63,380,101,"102532",481,63]
["102535",102535,null,"STK","ICM 200 Inspektions-Winkel 85°","CHF",603,"Schiedel ICM matt",3.98,0,"J","ICM 200 Coude avec inspection 85°","ICM 200 Inspektions-Winkel 85°","ICM 200 Gmoito con revisione 85°",134,1,"DN 200",null,523.6,"142038720M",null,null,603,"102535",79.399999999999977,476,127,"102535",603,79.399999999999977]
["102537",102537,null,"STK","ICM 300 Inspektions-Winkel 85°","CHF",685,"Schiedel ICM matt",6.74,0,"J","ICM 300 Coude avec inspection 85°","ICM 300 Inspektions-Winkel 85°","ICM 300 Gmoito con revisione 85°",134,1,"DN 300",null,595.1,"142038730M",null,null,685,"102537",89.899999999999977,541,144,"102537",685,89.899999999999977]
["102540",102540,null,"STK","ICM 450 Inspektions-Winkel 85°","CHF",1357,"Schiedel ICM matt",12.78,0,"J","ICM 450 Coude avec inspection 85°","ICM 450 Inspektions-Winkel 85°","ICM 450 Gmoito con revisione 85°",134,1,"DN 450",null,1179.2,"142038745M",null,null,1357,"102540",177.79999999999995,1072,285,"102540",1357,177.79999999999995]
["102545",102545,null,"STK","ICM 100 Winkel 90°","CHF",200,"Schiedel ICM matt",1.5,0,"J","ICM 100 Coude 90°","ICM 100 Winkel 90°","ICM 100 Gomito 90°",134,1,"DN 100",null,173.8,"142039010M",null,null,200,"102545",26.199999999999989,158,42,"102545",200,26.199999999999989]
["102549",102549,null,"STK","ICM 200 Winkel 90°","CHF",302,"Schiedel ICM matt",3.39,0,"J","ICM 200 Coude 90°","ICM 200 Winkel 90°","ICM 200 Gomito 90°",134,1,"DN 200",null,261.8,"142039020M","104656","4037494197516",302,"102549",40.199999999999989,238,64,"102549",302,40.199999999999989]
["102552",102552,null,"STK","ICM 350 Winkel 90°","CHF",548,"Schiedel ICM matt",7.33,0,"J","ICM 350 Coude 90°","ICM 350 Winkel 90°","ICM 350 Gomito 90°",134,1,"DN 350",null,476.3,"142039035M",null,null,548,"102552",71.699999999999989,433,115,"102552",548,71.699999999999989]
["102554",102554,null,"STK","ICM 450 Winkel 90°","CHF",1028,"Schiedel ICM matt",11.61,0,"J","ICM 450 Coude 90°","ICM 450 Winkel 90°","ICM 450 Gomito 90°",134,1,"DN 450",null,893.2,"142039045M",null,null,1028,"102554",134.79999999999995,812,216,"102554",1028,134.79999999999995]
["102560",102560,null,"STK","ICM 130 Inspektions-Winkel 90°","CHF",481,"Schiedel ICM matt",2.68,0,"J","ICM 130 Coude avec inspection 90°","ICM 130 Inspektions-Winkel 90°","ICM 130 Gmoito con revisione 90°",134,1,"DN 130",null,418,"142039213M",null,null,481,"102560",63,380,101,"102560",481,63]
["102563",102563,null,"STK","ICM 200 Inspektions-Winkel 90°","CHF",603,"Schiedel ICM matt",3.98,0,"J","ICM 200 Coude avec inspection 90°","ICM 200 Inspektions-Winkel 90°","ICM 200 Gmoito con revisione 90°",134,1,"DN 200",null,523.6,"142039220M",null,null,603,"102563",79.399999999999977,476,127,"102563",603,79.399999999999977]
["102565",102565,null,"STK","ICM 300 Inspektions-Winkel 90°","CHF",685,"Schiedel ICM matt",6.74,0,"J","ICM 300 Coude avec inspection 90°","ICM 300 Inspektions-Winkel 90°","ICM 300 Gmoito con revisione 90°",134,1,"DN 300",null,595.1,"142039230M",null,null,685,"102565",89.899999999999977,541,144,"102565",685,89.899999999999977]
[{"$f":"B1868&\"\"","v":"102568"},102568,null,"STK",{"$f":"IF($E$200=2,L1868,IF($E$200=3,N1868,M1868))","v":"ICM 450 Inspektions-Winkel 90°"},"CHF",{"$f":"IF($L$190=1,W1868,S1868)","v":1357},"Schiedel ICM matt",13.164,0,"J","ICM 450 Coude avec inspection 90°","ICM 450 Inspektions-Winkel 90°","ICM 450 Gmoito con revisione 90°",134,1,"DN 450",null,1179.2,"142039245M",null,null,1357,"102568",177.79999999999995,1072,285,"102568",1357,177.79999999999995]
["102574",102574,null,"STK","ICK 80 Konsolenbleche (Paar)","CHF",171,"Schiedel ICK verkupfert",2.2000000000000002,0,"J","ICK 80 Tôle console murale ( 2 pces. ) ","ICK 80 Konsolenbleche (Paar)","ICK 80 Coppia suporti piastra partenza (Paar)",135,1,"DN 80",null,148.5,"266000608K",null,null,171,"102574",22.5,135,36,"102574",171,22.5]
["102578",102578,null,"STK","ICK 180 Konsolenbleche (Paar)","CHF",260,"Schiedel ICK verkupfert",3.32,0,"J","ICK 180 Tôle console murale ( 2 pces. ) ","ICK 180 Konsolenbleche (Paar)","ICK 180 Coppia suporti piastra partenza (Paar)",135,1,"DN 180",null,225.5,"266000618K",null,null,260,"102578",34.5,205,55,"102578",260,34.5]
["102583",102583,null,"PAR","ICK 750 Wandkonsolen (Paar) L500mm verstärkt","CHF",403,"Schiedel ICK verkupfert",6,0,"J","ICK 750 Console réglable ( 2 pces. ) L500mm renforcée","ICK 750 Wandkonsolen (Paar) L500mm verstärkt","ICK 750 Supporto a muro 2 pezzi L500mm rinforzato",135,1,"ZBH ICK",null,349.8,"95120750K",null,null,403,"102583",53.199999999999989,318,85,"102583",403,53.199999999999989]
["102586",102586,null,"PAR","ICK 999 Wandkonsolen (Paar) L1304mm","CHF",695,"Schiedel ICK verkupfert",9,0,"J","ICK 999 Console réglable ( 2 pces. ) L1304mm","ICK 999 Wandkonsolen (Paar) L1304mm","ICK 999 Supporto a muro 2 pezzi L1304mm",135,1,"ZBH ICK",null,603.9,"95120999K",null,null,695,"102586",91.100000000000023,549,146,"102586",695,91.100000000000023]
["102588",102588,null,"STK","ICK 100 Verankerungsplatte mit Ablauf senkr.","CHF",269,"Schiedel ICK verkupfert",1.68,95,"J","ICK 100 Plaque de base et écoulement vertical","ICK 100 Verankerungsplatte mit Ablauf senkr.","ICK 100 Piastra base con scadenza verticale",135,1,"DN 100",null,233.2,"266000410K",null,null,269,"102588",35.800000000000011,212,57,"102588",269,35.800000000000011]
["102591",102591,null,"STK","ICK 180 Verankerungsplatte mit Ablauf senkr.","CHF",322,"Schiedel ICK verkupfert",3.03,95,"J","ICK 180 Plaque de base et écoulement vertical","ICK 180 Verankerungsplatte mit Ablauf senkr.","ICK 180 Piastra base con scadenza verticale",135,1,"DN 180",null,279.39999999999998,"266000418K",null,null,322,"102591",42.600000000000023,254,68,"102591",322,42.600000000000023]
["102597",102597,null,"STK","ICK 130 Zwischenstütze","CHF",322,"Schiedel ICK verkupfert",2.5,95,"J","ICK 130 Support intermédieaire","ICK 130 Zwischenstütze","ICK 130 Piastra passante",135,1,"DN 130",null,279.39999999999998,"266001013K",null,null,322,"102597",42.600000000000023,254,68,"102597",322,42.600000000000023]
["102598",102598,null,"STK","ICK 150 Zwischenstütze","CHF",340,"Schiedel ICK verkupfert",2.8,95,"J","ICK 150 Support intermédieaire","ICK 150 Zwischenstütze","ICK 150 Piastra passante",135,1,"DN 150",null,294.8,"266001015K",null,null,340,"102598",45.199999999999989,268,72,"102598",340,45.199999999999989]
["102602",102602,null,"STK","ICK 300 Zwischenstütze","CHF",517,"Schiedel ICK verkupfert",5,95,"J","ICK 300 Support intermédieaire","ICK 300 Zwischenstütze","ICK 300 Piastra passante",135,1,"DN 300",null,448.8,"266001030K",null,null,517,"102602",68.199999999999989,408,109,"102602",517,68.199999999999989]
["102606",102606,null,"STK","ICK 150 Verankerungsplatte EW auf DW","CHF",233,"Schiedel ICK verkupfert",3.8,97,"J","ICK 150 Plaque avec male vertical PPL","ICK 150 Verankerungsplatte EW auf DW","ICK 150 Piastra verticale con maschio PPL",135,1,"DN 150",null,202.4,"266000315K",null,null,233,"102606",30.599999999999994,184,49,"102606",233,30.599999999999994]
["102610",102610,null,"STK","ICK 300 Verankerungsplatte EW auf DW","CHF",394,"Schiedel ICK verkupfert",7,97,"J","ICK 300 Plaque avec male vertical PPL","ICK 300 Verankerungsplatte EW auf DW","ICK 300 Piastra verticale con maschio PPL",135,1,"DN 300",null,342.1,"266000330K",null,null,394,"102610",51.899999999999977,311,83,"102610",394,51.899999999999977]
["102611",102611,null,"STK","ICK 80 Kondensatschale mit Ablauf 1/2\"","CHF",136,"Schiedel ICK verkupfert",1.1000000000000001,55,"J","ICK 80 Pot de condensat avec écoulement 1/2\"","ICK 80 Kondensatschale mit Ablauf 1/2\"","ICK 80 Scarico condensa 1/2\"",135,1,"DN 80",null,117.7,"266000508K",null,null,136,"102611",18.299999999999997,107,29,"102611",136,18.299999999999997]
["102617",102617,null,"STK","ICK 250 Kondensatschale mit Ablauf 1/2\"","CHF",279,"Schiedel ICK verkupfert",3.4,55,"J","ICK 250 Pot de condensat avec écoulement 1/2\"","ICK 250 Kondensatschale mit Ablauf 1/2\"","ICK 250 Scarico condensa 1/2\"",135,1,"DN 250",null,242,"266000525K",null,null,279,"102617",37,220,59,"102617",279,37]
["102620",102620,null,"STK","ICK 100 Teleskopstütze verstellbar L300 - 500mm","CHF",456,"Schiedel ICK verkupfert",6.2,300,"J","ICK 100 Support téléscopique, régl. L300 - 500mm","ICK 100 Teleskopstütze verstellbar L300 - 500mm","ICK 100 Telescopio di ritenuta L300 - 500mm",135,1,"DN 100",null,396,"266000810K",null,null,456,"102620",60,360,96,"102620",456,60]
["102622",102622,null,"STK","ICK 150 Teleskopstütze verstellbar L300 - 500mm","CHF",500,"Schiedel ICK verkupfert",7.5,300,"J","ICK 150 Support téléscopique, régl. L300 - 500mm","ICK 150 Teleskopstütze verstellbar L300 - 500mm","ICK 150 Telescopio di ritenuta L300 - 500mm",135,1,"DN 150",null,434.5,"266000815K",null,null,500,"102622",65.5,395,105,"102622",500,65.5]
["102625",102625,null,"STK","ICK 250 Teleskopstütze verstellbar L300 - 500mm","CHF",624,"Schiedel ICK verkupfert",9.9,300,"J","ICK 250 Support téléscopique, régl. L300 - 500mm","ICK 250 Teleskopstütze verstellbar L300 - 500mm","ICK 250 Telescopio di ritenuta L300 - 500mm",135,1,"DN 250",null,542.29999999999995,"266000825K",null,null,624,"102625",81.700000000000045,493,131,"102625",624,81.700000000000045]
["102630",102630,null,"STK","ICK 200 Fussteil mit Kondensatablauf L1000mm","CHF",642,"Schiedel ICK verkupfert",6.5,1000,"J","ICK 200 Pied colonne raccourcisable L1000mm","ICK 200 Fussteil mit Kondensatablauf L1000mm","ICK 200 Sezione piedi con scarico condensa L1000mm",135,1,"DN 200",null,557.70000000000005,"266000220K",null,null,642,"102630",84.299999999999955,507,135,"102630",642,84.299999999999955]
[{"$f":"B1932&\"\"","v":"102634"},102634,null,"STK",{"$f":"IF($E$200=2,L1932,IF($E$200=3,N1932,M1932))","v":"ICK 180 Putztüranschluss eckig Unterdruck L455mm"},"CHF",{"$f":"IF($L$190=1,W1932,S1932)","v":606},"Schiedel ICK verkupfert",5.3,411,"J","ICK 180  Element d'inspéction souspression L455mm","ICK 180 Putztüranschluss eckig Unterdruck L455mm","ICK 180 Elemento inspezione sotto pressione L455mm",135,1,"DN 180",null,526.9,"236900518K",null,null,606,"102634",79.100000000000023,479,127,"102634",606,79.100000000000023]
["102638",102638,null,"STK","ICK 80 Putztüranschluss rund Überdruck L288mm","CHF",384,"Schiedel ICK verkupfert",1.6,288,"J","ICK 80 Element d'inspéction surpression L288mm","ICK 80 Putztüranschluss rund Überdruck L288mm","ICK 80 Elemento di inspezione su pressione L288mm",135,1,"DN 80",null,333.3,"236900008K",null,null,384,"102638",50.699999999999989,303,81,"102638",384,50.699999999999989]
["102639",102639,null,"STK","ICK 100 Putztüranschluss rund Überdruck L288mm","CHF",438,"Schiedel ICK verkupfert",1.9,288,"J","ICK 100 Element d'inspéction surpression L288mm","ICK 100 Putztüranschluss rund Überdruck L288mm","ICK 100 Elemento di inspezione su pressione L288mm",135,1,"DN 100",null,380.6,"236900010K",null,null,438,"102639",57.399999999999977,346,92,"102639",438,57.399999999999977]
["102645",102645,null,"STK","ICK 300 Putztüranschluss rund Überdruck L485mm","CHF",1007,"Schiedel ICK verkupfert",7.73,485,"J","ICK 300 Element d'inspéction souspression L485mm","ICK 300 Putztüranschluss rund Überdruck L485mm","ICK 300 Elemento di inspezione su pressione L485mm",135,1,"DN 300",null,875.6,"236900030K",null,null,1007,"102645",131.39999999999998,796,211,"102645",1007,131.39999999999998]
["102646",102646,null,"STK","ICK 80 T-Stück 45° L 330mm","CHF",340,"Schiedel ICK verkupfert",1.9,330,"J","ICK 80 Pièce Té 45° L 330mm","ICK 80 T-Stück 45° L 330mm","ICK 80 Pezzo T 45° L 330mm",135,1,"DN 80",null,294.8,"231404508K",null,null,340,"102646",45.199999999999989,268,72,"102646",340,45.199999999999989]
["102652",102652,null,"STK","ICK 250 T-Stück 45° L 560mm","CHF",926,"Schiedel ICK verkupfert",8.6999999999999993,560,"J","ICK 250 Pièce Té 45° L 560mm","ICK 250 T-Stück 45° L 560mm","ICK 250 Pezzo T 45° L 560mm",135,1,"DN 250",null,805.2,"231404525K",null,null,926,"102652",120.79999999999995,732,194,"102652",926,120.79999999999995]
["102654",102654,null,"STK","ICK 80 T-Stück 90° L288mm","CHF",314,"Schiedel ICK verkupfert",1.7,288,"J","ICM 80 Pièce Té 90° L288mm","ICK 80 T-Stück 90° L288mm","ICM 80 Pezzo T 90° L288mm",135,1,"DN 80",null,272.8,"231409008K",null,null,314,"102654",41.199999999999989,248,66,"102654",314,41.199999999999989]
["102657",102657,null,"STK","ICK 150 T-Stück 90° L455mm","CHF",447,"Schiedel ICK verkupfert",3.9,455,"J","ICM 150 Pièce Té 90° L455mm","ICK 150 T-Stück 90° L455mm","ICM 150 Pezzo T 90° L455mm",135,1,"DN 150",null,388.3,"231409015K",null,null,447,"102657",58.699999999999989,353,94,"102657",447,58.699999999999989]
["102661",102661,null,"STK","ICK 300 T-Stück 90° L485mm","CHF",883,"Schiedel ICK verkupfert",7.9,480,"J","ICM 300 Pièce Té 90° L485mm","ICK 300 T-Stück 90° L485mm","ICM 300 Pezzo T 90° L485mm",135,1,"DN 300",null,767.8,"231409030K",null,null,883,"102661",115.20000000000005,698,185,"102661",883,115.20000000000005]
["102666",102666,null,"STK","ICK 180 Verschlussdeckel","CHF",226,"Schiedel ICK verkupfert",2.4,0,"J","ICK 180 Couvercle avec poignée ","ICK 180 Verschlussdeckel","ICK 180 Tapo cieco",135,1,"DN 180",null,195.8,"266002018K",null,null,226,"102666",30.199999999999989,178,48,"102666",226,30.199999999999989]
["102669",102669,null,"STK","ICK 300 Verschlussdeckel","CHF",322,"Schiedel ICK verkupfert",4.0999999999999996,0,"J","ICK 300 Couvercle avec poignée ","ICK 300 Verschlussdeckel","ICK 300 Tapo cieco",135,1,"DN 300",null,279.39999999999998,"266002030K",null,null,322,"102669",42.600000000000023,254,68,"102669",322,42.600000000000023]
["102671",102671,null,"STK","ICK 100 Anschluss von EW auf DW in Rauchgasr.","CHF",161,"Schiedel ICK verkupfert",0.56799999999999995,0,"J","ICK 100 Raccord de PPL - ICS ","ICK 100 Anschluss von EW auf DW in Rauchgasr.","ICK 100 Raccordo de PPL - ICS ",135,1,"DN 100",null,139.69999999999999,"266040010K",null,null,161,"102671",21.300000000000011,127,34,"102671",161,21.300000000000011]
["102674",102674,null,"STK","ICK 180 Anschluss von EW auf DW in Rauchgasr.","CHF",214,"Schiedel ICK verkupfert",0.94699999999999995,0,"J","ICK 180 Raccord de PPL - ICS","ICK 180 Anschluss von EW auf DW in Rauchgasr.","ICK 180 Raccordo de PPL - ICS",135,1,"DN 180",null,185.9,"266040018K",null,null,214,"102674",28.099999999999994,169,45,"102674",214,28.099999999999994]
["102680",102680,null,"STK","ICK 150 Anschluss DW/EW mit Klemmfutter DN130","CHF",214,"Schiedel ICK verkupfert",1.5,0,"J","ICK 150 Raccord PPL - ICS av. manchon double DN130","ICK 150 Anschluss DW/EW mit Klemmfutter DN130","ICK 150 Adattore PPL - ICS con tubo fodera DN130",135,1,"DN 150",null,185.9,"266021513K",null,null,214,"102680",28.099999999999994,169,45,"102680",214,28.099999999999994]
["102682",102682,null,"STK","ICK 180 Anschluss DW/EW mit Klemmfutter DN150","CHF",251,"Schiedel ICK verkupfert",1.7,0,"J","ICK 180 Raccord PPL - ICS av. manchon double DN150","ICK 180 Anschluss DW/EW mit Klemmfutter DN150","ICK 180 Adattore PPL - ICS con tubo fodera DN150",135,1,"DN 180",null,217.8,"266021815K",null,null,251,"102682",33.199999999999989,198,53,"102682",251,33.199999999999989]
["102685",102685,null,"STK","ICK 200 Anschluss DW/EW mit Klemmfutter DN200","CHF",304,"Schiedel ICK verkupfert",2.2000000000000002,0,"J","ICK 200 Raccord PPL - ICS av. manchon double DN200","ICK 200 Anschluss DW/EW mit Klemmfutter DN200","ICK 200 Adattore PPL - ICS con tubo fodera DN200",135,1,"DN 200",null,264,"266022020K",null,null,304,"102685",40,240,64,"102685",304,40]
["102689",102689,null,"STK","ICK 100 Anschluss von DW auf EW in Rauchgasr.","CHF",161,"Schiedel ICK verkupfert",0.56799999999999995,0,"J","ICK 100 Raccord de ICS - PPL ","ICK 100 Anschluss von DW auf EW in Rauchgasr.","ICK 100 Adattore ICS - PPL ",135,1,"DN 100",null,139.69999999999999,"266041010K",null,null,161,"102689",21.300000000000011,127,34,"102689",161,21.300000000000011]
["102693",102693,null,"STK","ICK 200 Anschluss von DW auf EW in Rauchgasr.","CHF",233,"Schiedel ICK verkupfert",1.042,0,"J","ICK 200 Raccord de ICS - PPL ","ICK 200 Anschluss von DW auf EW in Rauchgasr.","ICK 200 Adattore ICS - PPL ",135,1,"DN 200",null,202.4,"266041020K",null,null,233,"102693",30.599999999999994,184,49,"102693",233,30.599999999999994]
["102694",102694,null,"STK","ICK 250 Anschluss von DW auf EW in Rauchgasr.","CHF",251,"Schiedel ICK verkupfert",1.2789999999999999,0,"J","ICK 250 Raccord de ICS - PPL ","ICK 250 Anschluss von DW auf EW in Rauchgasr.","ICK 250 Adattore ICS - PPL ",135,1,"DN 250",null,217.8,"266041025K",null,null,251,"102694",33.199999999999989,198,53,"102694",251,33.199999999999989]
[{"$f":"B1996&\"\"","v":"102698"},102698,null,"STK",{"$f":"IF($E$200=2,L1996,IF($E$200=3,N1996,M1996))","v":"ICK 130 Längenelement L195mm"},"CHF",{"$f":"IF($L$190=1,W1996,S1996)","v":126},"Schiedel ICK verkupfert",1.1200000000000001,150,"J","ICK 130 Elément droit L195mm","ICK 130 Längenelement L195mm","ICK 130 Elemento lunghezze L195mm",135,1,"DN 130",null,108.9,"142002013K",null,null,126,"102698",17.099999999999994,99,27,"102698",126,17.099999999999994]
["102703",102703,null,"STK","ICK 300 Längenelement L195mm","CHF",226,"Schiedel ICK verkupfert",2.31,150,"J","ICK 300 Elément droit L195mm","ICK 300 Längenelement L195mm","ICK 300 Elemento lunghezze L195mm",135,1,"DN 300",null,195.8,"142002030K",null,null,226,"102703",30.199999999999989,178,48,"102703",226,30.199999999999989]
["102705",102705,null,"STK","ICK 100 Längenelement L250mm","CHF",136,"Schiedel ICK verkupfert",1.1479999999999999,205,"J","ICK 100 Elément droit L250mm","ICK 100 Längenelement L250mm","ICK 100 Elemento lunghezze L250mm",135,1,"DN 100",null,117.7,"142002510K",null,null,136,"102705",18.299999999999997,107,29,"102705",136,18.299999999999997]
["102708",102708,null,"STK","ICK 180 Längenelement L250mm","CHF",161,"Schiedel ICK verkupfert",1.861,205,"J","ICK 180 Elément droit L250mm","ICK 180 Längenelement L250mm","ICK 180 Elemento lunghezze L250mm",135,1,"DN 180",null,139.69999999999999,"142002518K",null,null,161,"102708",21.300000000000011,127,34,"102708",161,21.300000000000011]
["102713",102713,null,"STK","ICK 100 Längenelement L500mm","CHF",145,"Schiedel ICK verkupfert",2.3410000000000002,455,"J","ICK 100 Elément droit L500mm","ICK 100 Längenelement L500mm","ICK 100 Elemento lunghezze L500mm",135,1,"DN 100",null,125.4,"142005010K",null,null,145,"102713",19.599999999999994,114,31,"102713",145,19.599999999999994]
["102717",102717,null,"STK","ICK 200 Längenelement L500mm","CHF",214,"Schiedel ICK verkupfert",4.17,455,"J","ICK 200 Elément droit L500mm","ICK 200 Längenelement L500mm","ICK 200 Elemento lunghezze L500mm",135,1,"DN 200",null,185.9,"142005020K",null,null,214,"102717",28.099999999999994,169,45,"102717",214,28.099999999999994]
["102721",102721,null,"STK","ICK 100 Längenelement L1000mm","CHF",233,"Schiedel ICK verkupfert",4.7290000000000001,955,"J","ICK 100 Elément droit L1000mm","ICK 100 Längenelement L1000mm","ICK 100 Elemento lunghezze L1000mm",135,1,"DN 100",null,202.4,"142010010K",null,null,233,"102721",30.599999999999994,184,49,"102721",233,30.599999999999994]
["102724",102724,null,"STK","ICK 180 Längenelement L1000mm","CHF",357,"Schiedel ICK verkupfert",7.6879999999999997,955,"J","ICK 180 Elément droit L1000mm","ICK 180 Längenelement L1000mm","ICK 180 Elemento lunghezze L1000mm",135,1,"DN 180",null,310.2,"142010018K",null,null,357,"102724",46.800000000000011,282,75,"102724",357,46.800000000000011]
["102726",102726,null,"STK","ICK 250 Längenelement L1000mm","CHF",463,"Schiedel ICK verkupfert",10.281000000000001,955,"J","ICK 250 Elément droit L1000mm","ICK 250 Längenelement L1000mm","ICK 250 Elemento lunghezze L1000mm",135,1,"DN 250",null,402.6,"142010025K",null,null,463,"102726",60.399999999999977,366,97,"102726",463,60.399999999999977]
["102729",102729,null,"STK","ICK 100 Schiebe-Element L270-375mm","CHF",286,"Schiedel ICK verkupfert",2.54,0,"J","ICK 100 Elément télescopique L270-375mm","ICK 100 Schiebe-Element L270-375mm","ICK 100 Elemento telescopico  L270-375mm",135,1,"DN 100",null,248.6,"142022710K",null,null,286,"102729",37.400000000000006,226,60,"102729",286,37.400000000000006]
["102735",102735,null,"STK","ICK 300 Schiebe-Element L270-375mm","CHF",482,"Schiedel ICK verkupfert",6.42,0,"J","ICK 300 Elément télescopique L270-375mm","ICK 300 Schiebe-Element L270-375mm","ICK 300 Elemento telescopico  L270-375mm",135,1,"DN 300",null,419.1,"142022730K",null,null,482,"102735",62.899999999999977,381,101,"102735",482,62.899999999999977]
["102737",102737,null,"STK","ICK 100 Klemmband DN150","CHF",27,"Schiedel ICK verkupfert",0.221,0,"J","ICK 100 Bride de fixation entre les tuyaux DN150","ICK 100 Klemmband DN150","ICK 100 Fascetta di sicurezza DN150",135,1,"DN 100",null,23.1,"266002210K",null,null,27,"102737",3.8999999999999986,21,6,"102737",27,3.8999999999999986]
["102740",102740,null,"STK","ICK 180 Klemmband DN230","CHF",33,"Schiedel ICK verkupfert",0.29799999999999999,0,"J","ICK 180 Bride de fixation entre les tuyaux DN230","ICK 180 Klemmband DN230","ICK 180 Fascetta di sicurezza DN230",135,1,"DN 180",null,28.6,"266002218K",null,null,33,"102740",4.3999999999999986,26,7,"102740",33,4.3999999999999986]
["102744",102744,null,"STK","ICK 80 Statisches Klemmband DN 130","CHF",41,"Schiedel ICK verkupfert",0.28699999999999998,0,"J","ICK 80 Bride statique large DN 130","ICK 80 Statisches Klemmband DN 130","ICK 80 Fascetta di sicurezza statico DN 130",135,1,"DN 80",null,35.200000000000003,"266002308K",null,null,41,"102744",5.7999999999999972,32,9,"102744",41,5.7999999999999972]
["102749",102749,null,"STK","ICK 200 Statisches Klemmband DN 250","CHF",60,"Schiedel ICK verkupfert",0.45300000000000001,0,"J","ICK 200 Bride statique large DN 250","ICK 200 Statisches Klemmband DN 250","ICK 200 Fascetta di sicurezza statico DN 250",135,1,"DN 200",null,51.7,"266002320K",null,null,60,"102749",8.2999999999999972,47,13,"102749",60,8.2999999999999972]
["102752",102752,null,"STK","ICK 80 Wandhalter 50mm fix DN 130mm ","CHF",55,"Schiedel ICK verkupfert",0.44,0,"J","ICK 80 Fixation murale 50mm fix DN 130mm ","ICK 80 Wandhalter 50mm fix DN 130mm ","ICK 80 Collare a muro 50mm  fix DN 130mm ",135,1,"DN 80",null,47.3,"92940130K",null,null,55,"102752",7.7000000000000028,43,12,"102752",55,7.7000000000000028]
["102754",102754,null,"STK","ICK 130 Wandhalter 50mm fix DN 180mm ","CHF",73,"Schiedel ICK verkupfert",0.53,0,"J","ICK 130 Fixation murale 50mm fix DN 180mm ","ICK 130 Wandhalter 50mm fix DN 180mm ","ICK 130 Collare a muro 50mm  fix DN 180mm ",135,1,"DN 130",null,62.7,"92940180K",null,null,73,"102754",10.299999999999997,57,16,"102754",73,10.299999999999997]
["102757",102757,null,"STK","ICK 200 Wandhalter 50mm fix DN 250mm","CHF",100,"Schiedel ICK verkupfert",0.7,0,"J","ICK 200 Fixation murale 50mm fix DN 250mm","ICK 200 Wandhalter 50mm fix DN 250mm","ICK 200 Collare a muro 50mm  fix DN 250mm",135,1,"DN 200",null,86.9,"92940250K",null,null,100,"102757",13.099999999999994,79,21,"102757",100,13.099999999999994]
["102760",102760,null,"STK","ICK 80 Wandhalter verstellbar 75 - 300mm DN 130mm","CHF",92,"Schiedel ICK verkupfert",1.1200000000000001,0,"J","ICK 80 Fixation murale régl. 75 - 300mm DN 130mm","ICK 80 Wandhalter verstellbar 75 - 300mm DN 130mm","ICK 80 Collare a muro regolabile 75-300mm DN130mm",135,1,"DN 80",null,79.2,"95960130K",null,null,92,"102760",12.799999999999997,72,20,"102760",92,12.799999999999997]
["102763",102763,null,"STK","ICK 150 Wandhalter verstellbar 75 - 300mm DN 200mm","CHF",118,"Schiedel ICK verkupfert",1.66,0,"J","ICK 150 Fixation murale régl. 75 - 300mm DN 200mm","ICK 150 Wandhalter verstellbar 75 - 300mm DN 200mm","ICK 150 Collare a muro regolabile 75-300mm DN200mm",135,1,"DN 150",null,102.3,"95960200K",null,null,118,"102763",15.700000000000003,93,25,"102763",118,15.700000000000003]
["102768",102768,null,"STK","ICK 80 Wandhalter 50mm verlängerbar DN 130mm ","CHF",55,"Schiedel ICK verkupfert",0.5,0,"J","ICK 80 Fixation murale 50mm régl. DN 130mm ","ICK 80 Wandhalter 50mm verlängerbar DN 130mm ","ICK 80 Collare a muro 50mm prolunga DN 130mm ",135,1,"DN 80",null,47.3,"95090130K",null,null,55,"102768",7.7000000000000028,43,12,"102768",55,7.7000000000000028]
["102772",102772,null,"STK","ICK 180 Wandhalter 50mm verlängerbar DN 230mm ","CHF",92,"Schiedel ICK verkupfert",0.7,0,"J","ICK 180 Fixation murale 50mm régl. DN 230mm ","ICK 180 Wandhalter 50mm verlängerbar DN 230mm ","ICK 180 Collare a muro 50mm prolunga DN 230mm ",135,1,"DN 180",null,79.2,"95090230K",null,null,92,"102772",12.799999999999997,72,20,"102772",92,12.799999999999997]
["102776",102776,null,"PAR","ICK W1 Verlängerung zu Wandhalter 50mm L 130mm","CHF",73,"Schiedel ICK verkupfert",0.13,0,"J","ICK W1 Ralogement pour fixation murale L130mm","ICK W1 Verlängerung zu Wandhalter 50mm L 130mm","ICK W1 Prolunga per collare 50mm L130mm",135,1,"DN 130",null,62.7,"267100130K",null,null,73,"102776",10.299999999999997,57,16,"102776",73,10.299999999999997]
["102777",102777,null,"PAR","ICK W2 Verlängerung zu Wandhalter 50mm L 176mm","CHF",108,"Schiedel ICK verkupfert",0.17,0,"J","ICK W2 Ralogement pour fixation murale L176mm","ICK W2 Verlängerung zu Wandhalter 50mm L 176mm","ICK W2 Prolunga per collare 50mm L176mm",135,1,"ZBH ICK",null,93.5,"267100176K",null,null,108,"102777",14.5,85,23,"102777",108,14.5]
["102781",102781,null,"PAR","ICK L4 Verlängerung zu Wandhalter 50mm L 750mm","CHF",322,"Schiedel ICK verkupfert",1.52,0,"J","ICK L4 Ralogement pour fixation murale L750mm","ICK L4 Verlängerung zu Wandhalter 50mm L 750mm","ICK L4 Prolunga per collare 50mm L750mm",135,1,"ZBH ICK",null,279.39999999999998,"267100750K",null,null,322,"102781",42.600000000000023,254,68,"102781",322,42.600000000000023]
["102786",102786,null,"STK","ICK 250-300 Dachdurführung 0° DN370 L500mm","CHF",375,"Schiedel ICK verkupfert",6.9,0,"J","ICK 250-300 Garniture de toiture 0° DN370 L500mm","ICK 250-300 Dachdurführung 0° DN370 L500mm","ICK 250-300 Faldale piatto 0° DN370 L500mm",135,1,"DN 250",null,325.60000000000002,"266320370K",null,null,375,"102786",49.399999999999977,296,79,"102786",375,49.399999999999977]
["102788",102788,null,"STK","ICK 130 Dachdurführung 16-25° DN200 mit Bleilappen","CHF",500,"Schiedel ICK verkupfert",11.25,0,"J","ICK 130 Garniture de toiture 16-25° DN200 ","ICK 130 Dachdurführung 16-25° DN200 mit Bleilappen","ICK 130 Faldale 16-25° DN200 compressa in piomba",135,1,"DN 130",null,434.5,"266322200K",null,null,500,"102788",65.5,395,105,"102788",500,65.5]
["102791",102791,null,"STK","ICK 250-300 Dachdurführung 16-25° DN370 ","CHF",730,"Schiedel ICK verkupfert",19.61,0,"J","ICK 250-300 Garniture de toiture 16-25° DN370 ","ICK 250-300 Dachdurführung 16-25° DN370 ","ICK 250-300 Faldale 16-25° DN370 compressa piomba",135,1,"DN 250",null,634.70000000000005,"266322370K",null,null,730,"102791",95.299999999999955,577,153,"102791",730,95.299999999999955]
["102796",102796,null,"STK","ICK 250-300 Dachdurführung 26-35° DN370 ","CHF",856,"Schiedel ICK verkupfert",21.26,0,"J","ICK 250-300 Garniture de toiture 26-35° DN370 ","ICK 250-300 Dachdurführung 26-35° DN370 ","ICK 250-300 Faldale 26-35° DN370 compressa piomba",135,1,"DN 250",null,743.6,"266323370K",null,null,856,"102796",112.39999999999998,676,180,"102796",856,112.39999999999998]
["102800",102800,null,"STK","ICK 200 Dachdurführung 36-45° DN320 mit Bleilappen","CHF",819,"Schiedel ICK verkupfert",18.510000000000002,0,"J","ICK 200 Garniture de toiture 36-45° DN320 ","ICK 200 Dachdurführung 36-45° DN320 mit Bleilappen","ICK 200 Faldale 36-45° DN320 compressa in piomba",135,1,"DN 200",null,711.7,"266324320K",null,null,819,"102800",107.29999999999995,647,172,"102800",819,107.29999999999995]
["102805",102805,null,"STK","ICK 150 Regenkragen DN200","CHF",81,"Schiedel ICK verkupfert",0.38,0,"J","ICK 150 Collerette anti pluie  DN200","ICK 150 Regenkragen DN200","ICK 150 Scossalina DN200",135,1,"DN 150",null,70.400000000000006,"265830200K",null,null,81,"102805",10.599999999999994,64,17,"102805",81,10.599999999999994]
["102808",102808,null,"STK","ICK 250 Regenkragen DN300","CHF",108,"Schiedel ICK verkupfert",0.51,0,"J","ICK 250 Collerette anti pluie  DN300","ICK 250 Regenkragen DN300","ICK 250 Scossalina DN300",135,1,"DN 250",null,93.5,"265830300K",null,null,108,"102808",14.5,85,23,"102808",108,14.5]
["102810",102810,null,"STK","ICK 80 Seilabspannring DN130 ","CHF",92,"Schiedel ICK verkupfert",0.436,0,"J","ICK 80 Bride de haubannage DN130 ","ICK 80 Seilabspannring DN130 ","ICK 80 Collare per cavi tiranti DN130 ",135,1,"DN 80",null,79.2,"95900130K",null,null,92,"102810",12.799999999999997,72,20,"102810",92,12.799999999999997]
["102813",102813,null,"STK","ICK 150 Seilabspannring DN200","CHF",118,"Schiedel ICK verkupfert",0.53900000000000003,0,"J","ICK 150 Bride de haubannage DN200","ICK 150 Seilabspannring DN200","ICK 150 Collare per cavi tiranti DN200",135,1,"DN 150",null,102.3,"95900200K",null,null,118,"102813",15.700000000000003,93,25,"102813",118,15.700000000000003]
["102819",102819,null,"STK","ICK 100 Blende 0-30° DN150","CHF",104,"Schiedel ICK verkupfert",1.1000000000000001,0,"J","ICK 100 Recouvrement carrée 0-30° DN150","ICK 100 Blende 0-30° DN150","ICK 100 Coperture 0-30° DN150",135,1,"DN 100",null,90.2,"266001410K",null,null,104,"102819",13.799999999999997,82,22,"102819",104,13.799999999999997]
["102821",102821,null,"STK","ICK 150 Blende 0-30° DN200","CHF",114,"Schiedel ICK verkupfert",1.4,0,"J","ICK 150 Recouvrement carrée 0-30° DN200","ICK 150 Blende 0-30° DN200","ICK 150 Coperture 0-30° DN200",135,1,"DN 150",null,99,"266001415K",null,null,114,"102821",15,90,24,"102821",114,15]
["102824",102824,null,"STK","ICK 250 Blende 0-30° DN300","CHF",145,"Schiedel ICK verkupfert",2,0,"J","ICK 250 Recouvrement carrée 0-30° DN300","ICK 250 Blende 0-30° DN300","ICK 250 Coperture 0-30° DN300",135,1,"DN 250",null,125.4,"266001425K",null,null,145,"102824",19.599999999999994,114,31,"102824",145,19.599999999999994]
["102829",102829,null,"STK","ICK 150 Blende 32-45° DN200","CHF",131,"Schiedel ICK verkupfert",1.4,0,"J","ICK 150 Recouvrement carrée 32-45° DN200","ICK 150 Blende 32-45° DN200","ICK 150 Coperture 32-45° DN200",135,1,"DN 150",null,113.3,"266001515K",null,null,131,"102829",17.700000000000003,103,28,"102829",131,17.700000000000003]
["102833",102833,null,"STK","ICK 300 Blende 32-45° DN350","CHF",180,"Schiedel ICK verkupfert",2.2000000000000002,0,"J","ICK 300 Recouvrement carrée 32-45° DN350","ICK 300 Blende 32-45° DN350","ICK 300 Coperture 32-45° DN350",135,1,"DN 300",null,156.19999999999999,"266001530K",null,null,180,"102833",23.800000000000011,142,38,"102833",180,23.800000000000011]
["102836",102836,null,"STK","ICK 130 Anschlussrosette Øi 180mm ØA 450mm","CHF",99,"Schiedel ICK verkupfert",0.43,0,"J","ICK 130 Rosace de raccordement Øi 180mm ØA 450mm","ICK 130 Anschlussrosette Øi 180mm ØA 450mm","ICK 130 Rosetta di collegamento Øi 180mm ØA 450mm",135,1,"DN 130",null,85.8,"265404413K",null,null,99,"102836",13.200000000000003,78,21,"102836",99,13.200000000000003]
["102838",102838,null,"STK","ICK 180 Anschlussrosette Øi 230mm ØA 500mm","CHF",105,"Schiedel ICK verkupfert",0.47,0,"J","ICK 180 Rosace de raccordement Øi 230mm ØA 500mm","ICK 180 Anschlussrosette Øi 230mm ØA 500mm","ICK 180 Rosetta di collegamento Øi 230mm ØA 500mm",135,1,"DN 180",null,91.3,"265404418K",null,null,105,"102838",13.700000000000003,83,22,"102838",105,13.700000000000003]
["102841",102841,null,"STK","ICK 300 Anschlussrosette Øi 350mm ØA 620mm","CHF",117,"Schiedel ICK verkupfert",0.54,0,"J","ICK 300 Rosace de raccordement Øi 350mm ØA 620mm","ICK 300 Anschlussrosette Øi 350mm ØA 620mm","ICK 300 Rosetta di collegamento Øi 350mm ØA 620mm",135,1,"DN 300",null,101.2,"265404430K",null,null,117,"102841",15.799999999999997,92,25,"102841",117,15.799999999999997]
["102845",102845,null,"STK","ICK 150 Mündungsabschluss","CHF",214,"Schiedel ICK verkupfert",1.482,295,"J","ICK 150 Cape de finition conique","ICK 150 Mündungsabschluss","ICK 150 Terminale conico",135,1,"DN 150",null,185.9,"266200015K",null,null,214,"102845",28.099999999999994,169,45,"102845",214,28.099999999999994]
["102847",102847,null,"STK","ICK 200 Mündungsabschluss","CHF",251,"Schiedel ICK verkupfert",1.9119999999999999,295,"J","ICK 200 Cape de finition conique","ICK 200 Mündungsabschluss","ICK 200 Terminale conico",135,1,"DN 200",null,217.8,"266200020K",null,null,251,"102847",33.199999999999989,198,53,"102847",251,33.199999999999989]
["102852",102852,null,"STK","ICK 150 Basten Standart mit Stulpring Kupfer","CHF",446,"Zubehör",4.0999999999999996,0,"J","ICK 150 Basten Standart avec dila, cuivre","ICK 150 Basten Standart mit Stulpring Kupfer","ICK 150 Terminale Basten con dila Kupfer",15,2,"DN 150",null,420,"916715",null,null,446,"102852",26,418,28,"102852",446,26]
["102856",102856,null,"STK","ICK 300 Basten Standart mit Stulpring Kupfer","CHF",536,"Zubehör",4.5,0,"J","ICK 300 Basten Standart avec dila, cuivre","ICK 300 Basten Standart mit Stulpring Kupfer","ICK 300 Terminale Basten con dila Kupfer",15,2,"DN 300",null,505,"916730",null,null,536,"102856",31,503,33,"102856",536,31]
["102860",102860,null,"STK","ICK 150 Element mit Messöffnung L205mm","CHF",304,"Schiedel ICK verkupfert",1.675,0,"J","ICK 150 Element avec manchon de mésure 1/2\" L205mm","ICK 150 Element mit Messöffnung L205mm","ICK 150 Elemento di missura  L205mm",135,1,"DN 150",null,264,"266002515K",null,null,304,"102860",40,240,64,"102860",304,40]
["102861",102861,null,"STK","ICK 180 Element mit Messöffnung L205mm","CHF",322,"Schiedel ICK verkupfert",1.952,0,"J","ICK 180 Element avec manchon de mésure 1/2\" L205mm","ICK 180 Element mit Messöffnung L205mm","ICK 180 Elemento di missura  L205mm",135,1,"DN 180",null,279.39999999999998,"266002518K",null,null,322,"102861",42.600000000000023,254,68,"102861",322,42.600000000000023]
["102865",102865,null,"STK","ICK 80 Element mit Kondensatablauf L205mm","CHF",251,"Schiedel ICK verkupfert",1.03,0,"J","ICK 80 Element décanteur de condensatf L205mm","ICK 80 Element mit Kondensatablauf L205mm","ICK 80 Element mit Kondensatablauf L205mm",135,1,"DN 80",null,217.8,"266002808K",null,null,251,"102865",33.199999999999989,198,53,"102865",251,33.199999999999989]
["102870",102870,null,"STK","ICK 200 Element mit Kondensatablauf L205mm","CHF",340,"Schiedel ICK verkupfert",2.137,0,"J","ICK 200 Element décanteur de condensatf L205mm","ICK 200 Element mit Kondensatablauf L205mm","ICK 200 Elemento con scarico condensa L205mm",135,1,"DN 200",null,294.8,"266002820K",null,null,340,"102870",45.199999999999989,268,72,"102870",340,45.199999999999989]
["102873",102873,null,"STK","ICK 80 Winkel 15°","CHF",214,"Schiedel ICK verkupfert",0.73899999999999999,0,"J","ICK 80 Coude 15°","ICK 80 Winkel 15°","ICK 80 Gomito 15°",135,1,"DN 80",null,185.9,"142031508K",null,null,214,"102873",28.099999999999994,169,45,"102873",214,28.099999999999994]
["102875",102875,null,"STK","ICK 130 Winkel 15°","CHF",242,"Schiedel ICK verkupfert",1.0840000000000001,0,"J","ICK 130 Coude 15°","ICK 130 Winkel 15°","ICK 130 Gomito 15°",135,1,"DN 130",null,210.1,"142031513K",null,null,242,"102875",31.900000000000006,191,51,"102875",242,31.900000000000006]
["102880",102880,null,"STK","ICK 300 Winkel 15°","CHF",340,"Schiedel ICK verkupfert",2.2469999999999999,0,"J","ICK 300 Coude 15°","ICK 300 Winkel 15°","ICK 300 Gomito 15°",135,1,"DN 300",null,294.8,"142031530K",null,null,340,"102880",45.199999999999989,268,72,"102880",340,45.199999999999989]
["102884",102884,null,"STK","ICK 150 Winkel 30°","CHF",286,"Schiedel ICK verkupfert",1.2230000000000001,0,"J","ICK 150 Coude 30°","ICK 150 Winkel 30°","ICK 150 Gomito 30°",135,1,"DN 150",null,248.6,"142033015K",null,null,286,"102884",37.400000000000006,226,60,"102884",286,37.400000000000006]
["102888",102888,null,"STK","ICK 300 Winkel 30°","CHF",536,"Schiedel ICK verkupfert",2.839,0,"J","ICK 300 Coude 30°","ICK 300 Winkel 30°","ICK 300 Gomito 30°",135,1,"DN 300",null,465.3,"142033030K",null,null,536,"102888",70.699999999999989,423,113,"102888",536,70.699999999999989]
["102889",102889,null,"STK","ICK 80 Winkel 45°","CHF",214,"Schiedel ICK verkupfert",0.93400000000000005,0,"J","ICK 80 Coude 45°","ICK 80 Winkel 45°","ICK 80 Gomito 45°",135,1,"DN 80",null,185.9,"142034508K",null,null,214,"102889",28.099999999999994,169,45,"102889",214,28.099999999999994]
["102893",102893,null,"STK","ICK 180 Winkel 45°","CHF",286,"Schiedel ICK verkupfert",1.8049999999999999,0,"J","ICK 180 Coude 45°","ICK 180 Winkel 45°","ICK 180 Gomito 45°",135,1,"DN 180",null,248.6,"142034518K",null,null,286,"102893",37.400000000000006,226,60,"102893",286,37.400000000000006]
["102896",102896,null,"STK","ICK 300 Winkel 45°","CHF",394,"Schiedel ICK verkupfert",3.8250000000000002,0,"J","ICK 300 Coude 45°","ICK 300 Winkel 45°","ICK 300 Gomito 45°",135,1,"DN 300",null,342.1,"142034530K",null,null,394,"102896",51.899999999999977,311,83,"102896",394,51.899999999999977]
["102902",102902,null,"STK","ICK 200 Winkel 90°","CHF",394,"Schiedel ICK verkupfert",3.39,0,"J","ICK 200 Coude 90°","ICK 200 Winkel 90°","ICK 200 Gomito 90°",135,1,"DN 200",null,342.1,"142039020K",null,null,394,"102902",51.899999999999977,311,83,"102902",394,51.899999999999977]
["102904",102904,null,"STK","ICK 300 Winkel 90°","CHF",536,"Schiedel ICK verkupfert",5.84,0,"J","ICK 300 Coude 90°","ICK 300 Winkel 90°","ICK 300 Gomito 90°",135,1,"DN 300",null,465.3,"142039030K",null,null,536,"102904",70.699999999999989,423,113,"102904",536,70.699999999999989]
["102907",102907,null,"STK","ICK 130 Inspektionswinkel 90°","CHF",624,"Schiedel ICK verkupfert",2.68,0,"J","ICK 130 Coude avec inspection 90°","ICK 130 Inspektionswinkel 90°","ICK 130 Gmoito con revisione 90°",135,1,"DN 130",null,542.29999999999995,"142039213K",null,null,624,"102907",81.700000000000045,493,131,"102907",624,81.700000000000045]
["102912",102912,null,"STK","ICK 300 Inspektionswinkel 90°","CHF",891,"Schiedel ICK verkupfert",6.74,0,"J","ICK 300 Coude avec inspection 90°","ICK 300 Inspektionswinkel 90°","ICK 300 Gmoito con revisione 90°",135,1,"DN 300",null,774.4,"142039230K",null,null,891,"102912",116.60000000000002,704,187,"102912",891,116.60000000000002]
["102916",102916,null,"STK","ICM5000 150  Verankerungsplatte mit Ablauf senkr.","CHF",185,"Schiedel ICM5000",2.5,95,"J","ICM5000 150 Plaque de base et écoulement vertical","ICM5000 150  Verankerungsplatte mit Ablauf senkr.","ICM5000 150  Piastra base con scadenza verticale",136,1,"DN 150",null,160.6,0,null,null,185,"102916",24.400000000000006,146,39,"102916",185,24.400000000000006]
["102917",102917,null,"STK","ICM5000 180  Verankerungsplatte mit Ablauf senkr.","CHF",195,"Schiedel ICM5000",3.1,95,"J","ICM5000 180 Plaque de base et écoulement vertical","ICM5000 180  Verankerungsplatte mit Ablauf senkr.","ICM5000 180  Piastra base con scadenza verticale",136,1,"DN 180",null,169.4,0,null,null,195,"102917",25.599999999999994,154,41,"102917",195,25.599999999999994]
["102920",102920,null,"STK","ICM5000 300  Verankerungsplatte mit Ablauf senkr.","CHF",318,"Schiedel ICM5000",5,95,"J","ICM5000 300 Plaque de base et écoulement vertical","ICM5000 300  Verankerungsplatte mit Ablauf senkr.","ICM5000 300  Piastra base con scadenza verticale",136,1,"DN 300",null,276.10000000000002,0,null,null,318,"102920",41.899999999999977,251,67,"102920",318,41.899999999999977]
["102925",102925,null,"STK","ICM5000 600  Verankerungsplatte mit Ablauf senkr.","CHF",698,"Schiedel ICM5000",10,95,"J","ICM5000 600 Plaque de base et écoulement vertical","ICM5000 600  Verankerungsplatte mit Ablauf senkr.","ICM5000 600  Piastra base con scadenza verticale",136,1,"DN 600",null,606.1,0,null,null,698,"102925",91.899999999999977,551,147,"102925",698,91.899999999999977]
["102928",102928,null,"STK","ICM5000 130  Verankerungsplatte mit Ablauf waagr.","CHF",162,"Schiedel ICM5000",3.2,97,"J","ICM5000 130 Plaque de base, écoulement horizontal","ICM5000 130  Verankerungsplatte mit Ablauf waagr.","ICM5000 130  Piastra base con scadenza horizontale",136,1,"DN 130",null,140.80000000000001,0,null,null,162,"102928",21.199999999999989,128,34,"102928",162,21.199999999999989]
["102930",102930,null,"STK","ICM5000 180  Verankerungsplatte mit Ablauf waagr.","CHF",183,"Schiedel ICM5000",4.5,97,"J","ICM5000 180 Plaque de base, écoulement horizontal","ICM5000 180  Verankerungsplatte mit Ablauf waagr.","ICM5000 180  Piastra base con scadenza horizontale",136,1,"DN 180",null,158.4,0,null,null,183,"102930",24.599999999999994,144,39,"102930",183,24.599999999999994]
["102935",102935,null,"STK","ICM5000 400  Verankerungsplatte mit Ablauf waagr.","CHF",529,"Schiedel ICM5000",10.5,97,"J","ICM5000 400 Plaque de base, écoulement horizontal","ICM5000 400  Verankerungsplatte mit Ablauf waagr.","ICM5000 400  Piastra base con scadenza horizontale",136,1,"DN 400",null,459.8,0,null,null,529,"102935",69.199999999999989,418,111,"102935",529,69.199999999999989]
["102939",102939,null,"STK","ICM5000 80 Zwischenstütze","CHF",149,"Schiedel ICM5000",1.7,188,"J","ICM5000 80 Support intermédieaire","ICM5000 80 Zwischenstütze","ICM5000 80 Piastra passante",136,1,"DN 80",null,128.69999999999999,0,null,null,149,"102939",20.300000000000011,117,32,"102939",149,20.300000000000011]
["102943",102943,null,"STK","ICM5000 180 Zwischenstütze","CHF",195,"Schiedel ICM5000",3.8,278,"J","ICM5000 180 Support intermédieaire","ICM5000 180 Zwischenstütze","ICM5000 180 Piastra passante",136,1,"DN 180",null,169.4,0,null,null,195,"102943",25.599999999999994,154,41,"102943",195,25.599999999999994]
["102944",102944,null,"STK","ICM5000 200 Zwischenstütze","CHF",229,"Schiedel ICM5000",4.2,285,"J","ICM5000 200 Support intermédieaire","ICM5000 200 Zwischenstütze","ICM5000 200 Piastra passante",136,1,"DN 200",null,199.1,0,null,null,229,"102944",29.900000000000006,181,48,"102944",229,29.900000000000006]
["102948",102948,null,"STK","ICM5000 400 Zwischenstütze","CHF",417,"Schiedel ICM5000",8.1999999999999993,485,"J","ICM5000 400 Support intermédieaire","ICM5000 400 Zwischenstütze","ICM5000 400 Piastra passante",136,1,"DN 400",null,361.9,0,null,null,417,"102948",55.100000000000023,329,88,"102948",417,55.100000000000023]
["102953",102953,null,"STK","ICM5000 100 Kondensattopf","CHF",113,"Schiedel ICM5000",1.4,null,"J","ICM5000 100 Pot de condensat avec écoulement 1/2\"","ICM5000 100 Kondensattopf","ICM5000 100 Bancinella per condensa verticale ",136,1,"DN 100",null,97.9,0,null,null,113,"102953",15.099999999999994,89,24,"102953",113,15.099999999999994]
["102956",102956,null,"STK","ICM5000 180 Kondensattopf","CHF",122,"Schiedel ICM5000",2.4,null,"J","ICM5000 180 Pot de condensat avec écoulement 1/2\"","ICM5000 180 Kondensattopf","ICM5000 180 Bancinella per condensa verticale ",136,1,"DN 180",null,105.6,0,null,null,122,"102956",16.400000000000006,96,26,"102956",122,16.400000000000006]
["102959",102959,null,"STK","ICM5000 300 Kondensattopf","CHF",170,"Schiedel ICM5000",4,null,"J","ICM5000 300 Pot de condensat avec écoulement 1/2\"","ICM5000 300 Kondensattopf","ICM5000 300 Bancinella per condensa verticale ",136,1,"DN 300",null,147.4,0,null,null,170,"102959",22.599999999999994,134,36,"102959",170,22.599999999999994]
["102962",102962,null,"STK","ICM5000 450 Kondensattopf","CHF",434,"Schiedel ICM5000",5.5,null,"J","ICM5000 450 Pot de condensat avec écoulement 1/2\"","ICM5000 450 Kondensattopf","ICM5000 450 Bancinella per condensa verticale ",136,1,"DN 450",null,377.3,0,null,null,434,"102962",56.699999999999989,343,91,"102962",434,56.699999999999989]
["102967",102967,null,"STK","ICM5000 130 Putztüranschluss rund Überdruck","CHF",280,"Schiedel ICM5000",2.8,455,"J","ICM5000 130 Element d'inspéction ronde ","ICM5000 130 Putztüranschluss rund Überdruck","ICM5000 130 Elemento di inspezione su pressione",136,1,"DN 130",null,243.1,0,null,null,280,"102967",36.900000000000006,221,59,"102967",280,36.900000000000006]
["102971",102971,null,"STK","ICM5000 250 Putztüranschluss rund Überdruck","CHF",513,"Schiedel ICM5000",6.9,455,"J","ICM5000 250 Element d'inspéction ronde ","ICM5000 250 Putztüranschluss rund Überdruck","ICM5000 250 Elemento di inspezione su pressione",136,1,"DN 250",null,445.5,0,null,null,513,"102971",67.5,405,108,"102971",513,67.5]
["102972",102972,null,"STK","ICM5000 300 Putztüranschluss rund Überdruck","CHF",600,"Schiedel ICM5000",7.7,480,"J","ICM5000 300 Element d'inspéction ronde ","ICM5000 300 Putztüranschluss rund Überdruck","ICM5000 300 Elemento di inspezione su pressione",136,1,"DN 300",null,521.4,0,null,null,600,"102972",78.600000000000023,474,126,"102972",600,78.600000000000023]
["102976",102976,null,"STK","ICM5000 500 Putztüranschluss rund Überdruck","CHF",2085,"Schiedel ICM5000",13.5,705,"J","ICM5000 500 Element d'inspéction ronde ","ICM5000 500 Putztüranschluss rund Überdruck","ICM5000 500 Elemento di inspezione su pressione",136,1,"DN 500",null,1812.8,0,null,null,2085,"102976",272.20000000000005,1648,437,"102976",2085,272.20000000000005]
["102979",102979,null,"STK","ICM5000 100 T-Stück 45°","CHF",572,"Schiedel ICM5000",2.5,355,"J","ICM5000 100 Pièce Té 45° L 355mm","ICM5000 100 T-Stück 45°","ICM5000 100 Pezzo T 45° L 355mm",136,1,"DN 100",null,497.2,0,null,null,572,"102979",74.800000000000011,452,120,"102979",572,74.800000000000011]
["102985",102985,null,"STK","ICM5000 300 T-Stück 45°","CHF",1077,"Schiedel ICM5000",11.5,623,"J","ICM5000 300 Pièce Té 45° L 623mm","ICM5000 300 T-Stück 45°","ICM5000 300 Pezzo T 45° L 623mm",136,1,"DN 300",null,936.1,0,null,null,1077,"102985",140.89999999999998,851,226,"102985",1077,140.89999999999998]
["102987",102987,null,"STK","ICM5000 400 T-Stück 45°","CHF",1898,"Schiedel ICM5000",20,815,"J","ICM5000 400 Pièce Té 45° L 815mm","ICM5000 400 T-Stück 45°","ICM5000 400 Pezzo T 45° L 815mm",136,1,"DN 400",null,1650,0,null,null,1898,"102987",248,1500,398,"102987",1898,248]
["102990",102990,null,"STK","ICM5000 600 T-Stück 45°","CHF",2851,"Schiedel ICM5000",37,1100,"J","ICM5000 600 Pièce Té 45° L 1100mm","ICM5000 600 T-Stück 45°","ICM5000 600 Pezzo T 45° L 1100mm",136,1,"DN 600",null,2478.3000000000002,0,null,null,2851,"102990",372.69999999999982,2253,598,"102990",2851,372.69999999999982]
["102995",102995,null,"STK","ICM5000 180 T-Stück 90°","CHF",294,"Schiedel ICM5000",4.7,455,"J","ICM5000 180 Pièce Té 90° L455mm","ICM5000 180 T-Stück 90°","ICM5000 180 Pezzo T 90° L455mm",136,1,"DN 180",null,255.2,0,null,null,294,"102995",38.800000000000011,232,62,"102995",294,38.800000000000011]
["102999",102999,null,"STK","ICM5000 350 T-Stück 90°","CHF",694,"Schiedel ICM5000",11,530,"J","ICM5000 350 Pièce Té 90° L535mm","ICM5000 350 T-Stück 90°","ICM5000 350 Pezzo T 90° L535mm",136,1,"DN 350",null,602.79999999999995,0,null,null,694,"102999",91.200000000000045,548,146,"102999",694,91.200000000000045]
["103000",103000,null,"STK","ICM5000 400 T-Stück 90°","CHF",1085,"Schiedel ICM5000",14,605,"J","ICM5000 400 Pièce Té 90° L705mm","ICM5000 400 T-Stück 90°","ICM5000 400 Pezzo T 90° L705mm",136,1,"DN 400",null,942.7,0,null,null,1085,"103000",142.29999999999995,857,228,"103000",1085,142.29999999999995]
["103003",103003,null,"STK","ICM5000 600 T-Stück 90°","CHF",2412,"Schiedel ICM5000",24,805,"J","ICM5000 600 Pièce Té 90° L705mm","ICM5000 600 T-Stück 90°","ICM5000 600 Pezzo T 90° L705mm",136,1,"DN 600",null,2096.6,0,null,null,2412,"103003",315.40000000000009,1906,506,"103003",2412,315.40000000000009]
["103008",103008,null,"STK","ICM5000 180 Verschlussdeckel","CHF",127,"Schiedel ICM5000",2.4,0,"J","ICM5000 180 Couvercle avec poignée","ICM5000 180 Verschlussdeckel","ICM5000 180 Tapo cieco",136,1,"DN 180",null,110,0,null,null,127,"103008",17,100,27,"103008",127,17]
["103011",103011,null,"STK","ICM5000 300 Verschlussdeckel","CHF",173,"Schiedel ICM5000",4.0999999999999996,0,"J","ICM5000 300 Couvercle avec poignée","ICM5000 300 Verschlussdeckel","ICM5000 300 Tapo cieco",136,1,"DN 300",null,149.6,0,null,null,173,"103011",23.400000000000006,136,37,"103011",173,23.400000000000006]
["103013",103013,null,"STK","ICM5000 400 Verschlussdeckel","CHF",250,"Schiedel ICM5000",5.0999999999999996,0,"J","ICM5000 400 Couvercle avec poignée","ICM5000 400 Verschlussdeckel","ICM5000 400 Tapo cieco",136,1,"DN 400",null,216.7,0,null,null,250,"103013",33.300000000000011,197,53,"103013",250,33.300000000000011]
[{"$f":"B2316&\"\"","v":"103019"},103019,null,"STK",{"$f":"IF($E$200=2,L2316,IF($E$200=3,N2316,M2316))","v":"ICM5000 130 Anschluss von EW auf DW in Rauchgasr."},"CHF",{"$f":"IF($L$190=1,W2316,S2316)","v":271},"Schiedel ICM5000",0.8,0,"J","ICM5000 130 Raccord de PPL - ICS","ICM5000 130 Anschluss von EW auf DW in Rauchgasr.","ICM5000 130 Raccordo de PPL - ICS",136,1,"DN 130",null,235.4,0,null,null,271,"103019",35.599999999999994,214,57,"103019",271,35.599999999999994]
["103022",103022,null,"STK","ICM5000 200 Anschluss von EW auf DW in Rauchgasr.","CHF",328,"Schiedel ICM5000",1.8,0,"J","ICM5000 200 Raccord de PPL - ICS","ICM5000 200 Anschluss von EW auf DW in Rauchgasr.","ICM5000 200 Raccordo de PPL - ICS",136,1,"DN 200",null,284.89999999999998,0,null,null,328,"103022",43.100000000000023,259,69,"103022",328,43.100000000000023]
["103026",103026,null,"STK","ICM5000 400 Anschluss von EW auf DW in Rauchgasr.","CHF",488,"Schiedel ICM5000",3.6,0,"J","ICM5000 400 Raccord de PPL - ICS","ICM5000 400 Anschluss von EW auf DW in Rauchgasr.","ICM5000 400 Raccordo de PPL - ICS",136,1,"DN 400",null,423.5,0,null,null,488,"103026",64.5,385,103,"103026",488,64.5]
["103027",103027,null,"STK","ICM5000 450 Anschluss von EW auf DW in Rauchgasr.","CHF",532,"Schiedel ICM5000",4.2,0,"J","ICM5000 450 Raccord de PPL - ICS","ICM5000 450 Anschluss von EW auf DW in Rauchgasr.","ICM5000 450 Raccordo de PPL - ICS",136,1,"DN 450",null,462,0,null,null,532,"103027",70,420,112,"103027",532,70]
["103031",103031,null,"STK","ICM5000 100 Erweiterung um 1Ø in Rauchgasrichtung","CHF",100,"Schiedel ICM5000",1.4,0,"J","ICM5000 100 Extension en 1 diamètre des combustion","ICM5000 100 Erweiterung um 1Ø in Rauchgasrichtung","ICM5000 100 Estensione 1 diametro direzione  fumi",136,1,"DN 100",null,86.9,0,null,null,100,"103031",13.099999999999994,79,21,"103031",100,13.099999999999994]
["103036",103036,null,"STK","ICM5000 250 Erweiterung um 1Ø in Rauchgasrichtung","CHF",131,"Schiedel ICM5000",3.1,0,"J","ICM5000 250 Extension en 1 diamètre des combustion","ICM5000 250 Erweiterung um 1Ø in Rauchgasrichtung","ICM5000 250 Estensione 1 diametro direzione  fumi",136,1,"DN 250",null,113.3,0,null,null,131,"103036",17.700000000000003,103,28,"103036",131,17.700000000000003]
["103039",103039,null,"STK","ICM5000 400 Erweiterung um 1Ø in Rauchgasrichtung","CHF",200,"Schiedel ICM5000",4.5999999999999996,0,"J","ICM5000 400 Extension en 1 diamètre des combustion","ICM5000 400 Erweiterung um 1Ø in Rauchgasrichtung","ICM5000 400 Estensione 1 diametro direzione  fumi",136,1,"DN 400",null,173.8,0,null,null,200,"103039",26.199999999999989,158,42,"103039",200,26.199999999999989]
["103042",103042,null,"STK","ICM5000 100 Flansch zum Anschweissen im Auftrag","CHF",100,"Schiedel ICM5000",0.6,0,"J","ICM5000 100 Rebord pour Raccord à souder en ordre","ICM5000 100 Flansch zum Anschweissen im Auftrag","ICM5000 100 Flangia da saldare al fine",136,1,"DN 100",null,86.9,0,null,null,100,"103042",13.099999999999994,79,21,"103042",100,13.099999999999994]
["103045",103045,null,"STK","ICM5000 180 Flansch zum Anschweissen im Auftrag","CHF",126,"Schiedel ICM5000",1.6,0,"J","ICM5000 180 Rebord pour Raccord à souder en ordre","ICM5000 180 Flansch zum Anschweissen im Auftrag","ICM5000 180 Flangia da saldare al fine",136,1,"DN 180",null,108.9,0,null,null,126,"103045",17.099999999999994,99,27,"103045",126,17.099999999999994]
["103050",103050,null,"STK","ICM5000 400 Flansch zum Anschweissen im Auftrag","CHF",200,"Schiedel ICM5000",3.6,0,"J","ICM5000 400 Rebord pour Raccord à souder en ordre","ICM5000 400 Flansch zum Anschweissen im Auftrag","ICM5000 400 Flangia da saldare al fine",136,1,"DN 400",null,173.8,0,null,null,200,"103050",26.199999999999989,158,42,"103050",200,26.199999999999989]
["103054",103054,null,"STK","ICM5000 80 Längenelement  L195mm","CHF",87,"Schiedel ICM5000",0.8,155,"J","ICM5000 80 Tuyau droit L195mm","ICM5000 80 Längenelement  L195mm","ICM5000 80 Elemento lunghezze  L195mm",136,1,"DN 80",null,74.8,0,null,null,87,"103054",12.200000000000003,68,19,"103054",87,12.200000000000003]
["103055",103055,null,"STK","ICM5000 100 Längenelement L195mm","CHF",74,"Schiedel ICM5000",1,155,"J","ICM5000 100 Tuyau droit L195mm","ICM5000 100 Längenelement L195mm","ICM5000 100 Elemento lunghezze L195mm",136,1,"DN 100",null,63.8,0,null,null,74,"103055",10.200000000000003,58,16,"103055",74,10.200000000000003]
["103059",103059,null,"STK","ICM5000 200 Längenelement L195mm","CHF",102,"Schiedel ICM5000",1.7,155,"J","ICM5000 200 Tuyau droit L195mm","ICM5000 200 Längenelement L195mm","ICM5000 200 Elemento lunghezze L195mm",136,1,"DN 200",null,88,0,null,null,102,"103059",14,80,22,"103059",102,14]
["103063",103063,null,"STK","ICM5000 400 Längenelement L195mm","CHF",290,"Schiedel ICM5000",3,155,"J","ICM5000 400 Tuyau droit L195mm","ICM5000 400 Längenelement L195mm","ICM5000 400 Elemento lunghezze L195mm",136,1,"DN 400",null,251.9,0,null,null,290,"103063",38.099999999999994,229,61,"103063",290,38.099999999999994]
["103068",103068,null,"STK","ICM5000 100 Längenelement L250mm","CHF",79,"Schiedel ICM5000",1.2,205,"J","ICM5000 100 Tuyau droit L250mm","ICM5000 100 Längenelement L250mm","ICM5000 100 Elemento lunghezze L250mm",136,1,"DN 100",null,68.2,0,null,null,79,"103068",10.799999999999997,62,17,"103068",79,10.799999999999997]
["103070",103070,null,"STK","ICM5000 150 Längenelement L250mm","CHF",95,"Schiedel ICM5000",1.7,205,"J","ICM5000 150 Tuyau droit L250mm","ICM5000 150 Längenelement L250mm","ICM5000 150 Elemento lunghezze L250mm",136,1,"DN 150",null,82.5,0,null,null,95,"103070",12.5,75,20,"103070",95,12.5]
["103073",103073,null,"STK","ICM5000 250 Längenelement L250mm","CHF",126,"Schiedel ICM5000",2.5,205,"J","ICM5000 250 Tuyau droit L250mm","ICM5000 250 Längenelement L250mm","ICM5000 250 Elemento lunghezze L250mm",136,1,"DN 250",null,108.9,0,null,null,126,"103073",17.099999999999994,99,27,"103073",126,17.099999999999994]
["103078",103078,null,"STK","ICM5000 500 Längenelement L250mm","CHF",327,"Schiedel ICM5000",5.3,205,"J","ICM5000 500 Tuyau droit L250mm","ICM5000 500 Längenelement L250mm","ICM5000 500 Elemento lunghezze L250mm",136,1,"DN 500",null,283.8,0,null,null,327,"103078",43.199999999999989,258,69,"103078",327,43.199999999999989]
["103079",103079,null,"STK","ICM5000 600 Längenelement L250mm","CHF",360,"Schiedel ICM5000",6.2,205,"J","ICM5000 600 Tuyau droit L250mm","ICM5000 600 Längenelement L250mm","ICM5000 600 Elemento lunghezze L250mm",136,1,"DN 600",null,312.39999999999998,0,null,null,360,"103079",47.600000000000023,284,76,"103079",360,47.600000000000023]
["103082",103082,null,"STK","ICM5000 130 Längenelement L500mm","CHF",117,"Schiedel ICM5000",3,455,"J","ICM5000 130 Tuyau droit L500mm","ICM5000 130 Längenelement L500mm","ICM5000 130 Elemento lunghezze L500mm",136,1,"DN 130",null,101.2,0,null,null,117,"103082",15.799999999999997,92,25,"103082",117,15.799999999999997]
["103086",103086,null,"STK","ICM5000 250 Längenelement L500mm","CHF",173,"Schiedel ICM5000",5,455,"J","ICM5000 250 Tuyau droit L500mm","ICM5000 250 Längenelement L500mm","ICM5000 250 Elemento lunghezze L500mm",136,1,"DN 250",null,149.6,0,null,null,173,"103086",23.400000000000006,136,37,"103086",173,23.400000000000006]
["103091",103091,null,"STK","ICM5000 500 Längenelement L500mm","CHF",442,"Schiedel ICM5000",11,455,"J","ICM5000 500 Tuyau droit L500mm","ICM5000 500 Längenelement L500mm","ICM5000 500 Elemento lunghezze L500mm",136,1,"DN 500",null,383.9,0,null,null,442,"103091",58.100000000000023,349,93,"103091",442,58.100000000000023]
["103094",103094,null,"STK","ICM5000 100 Längenelement L1000mm","CHF",149,"Schiedel ICM5000",2.5,955,"J","ICM5000 100 Tuyau droit L1000mm","ICM5000 100 Längenelement L1000mm","ICM5000 100 Elemento lunghezze L1000mm",136,1,"DN 100",null,128.69999999999999,0,null,null,149,"103094",20.300000000000011,117,32,"103094",149,20.300000000000011]
["103096",103096,null,"STK","ICM5000 150 Längenelement L1000mm","CHF",179,"Schiedel ICM5000",3.3,955,"J","ICM5000 150 Tuyau droit L1000mm","ICM5000 150 Längenelement L1000mm","ICM5000 150 Elemento lunghezze L1000mm",136,1,"DN 150",null,155.1,0,null,null,179,"103096",23.900000000000006,141,38,"103096",179,23.900000000000006]
["103102",103102,null,"STK","ICM5000 400 Längenelement L1000mm","CHF",514,"Schiedel ICM5000",8,955,"J","ICM5000 400 Tuyau droit L1000mm","ICM5000 400 Längenelement L1000mm","ICM5000 400 Elemento lunghezze L1000mm",136,1,"DN 400",null,446.6,0,null,null,514,"103102",67.399999999999977,406,108,"103102",514,67.399999999999977]
["103105",103105,null,"STK","ICM5000 600 Längenelement L1000mm","CHF",656,"Schiedel ICM5000",13,955,"J","ICM5000 600 Tuyau droit L1000mm","ICM5000 600 Längenelement L1000mm","ICM5000 600 Elemento lunghezze L1000mm",136,1,"DN 600",null,569.79999999999995,0,null,null,656,"103105",86.200000000000045,518,138,"103105",656,86.200000000000045]
["103107",103107,null,"STK","ICM5000 100 Schiebeelement L375 - 585mm","CHF",200,"Schiedel ICM5000",2.6,0,"J","ICM5000 100 Tuyau téléscopique L270-375mm","ICM5000 100 Schiebeelement L375 - 585mm","ICM5000 100 Elemento telescopico L375 - 585mm",136,1,"DN 100",null,173.8,0,null,null,200,"103107",26.199999999999989,158,42,"103107",200,26.199999999999989]
["103110",103110,null,"STK","ICM5000 180 Schiebeelement L375 - 585mm","CHF",255,"Schiedel ICM5000",4.0999999999999996,0,"J","ICM5000 180 Tuyau téléscopique L270-375mm","ICM5000 180 Schiebeelement L375 - 585mm","ICM5000 180 Elemento telescopico L375 - 585mm",136,1,"DN 180",null,221.1,0,null,null,255,"103110",33.900000000000006,201,54,"103110",255,33.900000000000006]
["103114",103114,null,"STK","ICM5000 350 Schiebeelement L375 - 585mm","CHF",338,"Schiedel ICM5000",7.5,0,"J","ICM5000 350 Tuyau téléscopique L270-375mm","ICM5000 350 Schiebeelement L375 - 585mm","ICM5000 350 Elemento telescopico L375 - 585mm",136,1,"DN 350",null,293.7,0,null,null,338,"103114",44.300000000000011,267,71,"103114",338,44.300000000000011]
["103118",103118,null,"STK","ICM5000 600 Schiebeelement L375 - 585mm","CHF",734,"Schiedel ICM5000",12.5,0,"J","ICM5000 600 Tuyau téléscopique L270-375mm","ICM5000 600 Schiebeelement L375 - 585mm","ICM5000 600 Elemento telescopico L375 - 585mm",136,1,"DN 600",null,638,0,null,null,734,"103118",96,580,154,"103118",734,96]
["103123",103123,null,"STK","ICM5000 180 Dichtring Silikon inkl. Gleitmittel","CHF",17,"Schiedel ICM5000",0.03,0,"J","ICM5000 180 Joint en silicone","ICM5000 180 Dichtring Silikon inkl. Gleitmittel","ICM5000 180 Guarnizione silicone",136,1,"DN 180",null,14.3,0,null,null,17,"103123",2.6999999999999993,13,4,"103123",17,2.6999999999999993]
["103125",103125,null,"STK","ICM5000 250 Dichtring Silikon inkl. Gleitmittel","CHF",18,"Schiedel ICM5000",0.04,0,"J","ICM5000 250 Joint en silicone","ICM5000 250 Dichtring Silikon inkl. Gleitmittel","ICM5000 250 Guarnizione silicone",136,1,"DN 250",null,15.4,0,null,null,18,"103125",2.5999999999999996,14,4,"103125",18,2.5999999999999996]
["103128",103128,null,"STK","ICM5000 400 Dichtring Silikon inkl. Gleitmittel","CHF",21,"Schiedel ICM5000",0.05,0,"J","ICM5000 400 Joint en silicone","ICM5000 400 Dichtring Silikon inkl. Gleitmittel","ICM5000 400 Guarnizione silicone",136,1,"DN 400",null,17.600000000000001,0,null,null,21,"103128",3.3999999999999986,16,5,"103128",21,3.3999999999999986]
["103133",103133,null,"STK","ICM5000 100 Dichtmanchette für Aussenmantel","CHF",42,"Schiedel ICM5000",0.04,0,"J","ICM5000 100 Manchon de Joint pour gaine externe","ICM5000 100 Dichtmanchette für Aussenmantel","ICM5000 100 Manicotto di tenuta per guaina esterna",136,1,"DN 100",null,36.299999999999997,0,null,null,42,"103133",5.7000000000000028,33,9,"103133",42,5.7000000000000028]
["103137",103137,null,"STK","ICM5000 200 Dichtmanchette für Aussenmantel","CHF",69,"Schiedel ICM5000",0.13,0,"J","ICM5000 200 Manchon de Joint pour gaine externe","ICM5000 200 Dichtmanchette für Aussenmantel","ICM5000 200 Manicotto di tenuta per guaina esterna",136,1,"DN 200",null,59.4,0,null,null,69,"103137",9.6000000000000014,54,15,"103137",69,9.6000000000000014]
["103138",103138,null,"STK","ICM5000 250 Dichtmanchette für Aussenmantel","CHF",76,"Schiedel ICM5000",0.19,0,"J","ICM5000 250 Manchon de Joint pour gaine externe","ICM5000 250 Dichtmanchette für Aussenmantel","ICM5000 250 Manicotto di tenuta per guaina esterna",136,1,"DN 250",null,66,0,null,null,76,"103138",10,60,16,"103138",76,10]
["103142",103142,null,"STK","ICM5000 450 Dichtmanchette für Aussenmantel","CHF",109,"Schiedel ICM5000",0.6,0,"J","ICM5000 450 Manchon de Joint pour gaine externe","ICM5000 450 Dichtmanchette für Aussenmantel","ICM5000 450 Manicotto di tenuta per guaina esterna",136,1,"DN 450",null,94.6,0,null,null,109,"103142",14.400000000000006,86,23,"103142",109,14.400000000000006]
["103146",103146,null,"STK","ICM5000 100 Klemmband bei jedem Bauteil inkl. ","CHF",16,"Schiedel ICM5000",0.2,0,"J","ICM5000 100 Bride de fixation  les tuyaux DN150","ICM5000 100 Klemmband bei jedem Bauteil inkl. ","ICM5000 100 Fascetta di sicurezza",136,1,"DN 100",null,13.2,0,null,null,16,"103146",2.8000000000000007,12,4,"103146",16,2.8000000000000007]
["103151",103151,null,"STK","ICM5000 250 Klemmband bei jedem Bauteil inkl. ","CHF",19,"Schiedel ICM5000",0.32,0,"J","ICM5000 250 Bride de fixation  les tuyaux DN300","ICM5000 250 Klemmband bei jedem Bauteil inkl. ","ICM5000 250 Fascetta di sicurezza",136,1,"DN 250",null,16.5,0,null,null,19,"103151",2.5,15,4,"103151",19,2.5]
["103154",103154,null,"STK","ICM5000 400 Klemmband bei jedem Bauteil inkl. ","CHF",21,"Schiedel ICM5000",0.51,0,"J","ICM5000 400 Bride de fixation  les tuyaux DN450","ICM5000 400 Klemmband bei jedem Bauteil inkl. ","ICM5000 400 Fascetta di sicurezza",136,1,"DN 400",null,17.600000000000001,0,null,null,21,"103154",3.3999999999999986,16,5,"103154",21,3.3999999999999986]
["103157",103157,null,"STK","ICM5000 600 Klemmband bei jedem Bauteil inkl. ","CHF",26,"Schiedel ICM5000",0.71,0,"J","ICM5000 600 Bride de fixation  les tuyaux DN650","ICM5000 600 Klemmband bei jedem Bauteil inkl. ","ICM5000 600 Fascetta di sicurezza",136,1,"DN 600",null,22,0,null,null,26,"103157",4,20,6,"103157",26,4]
["103173",103173,null,"STK","ICM5000 130 Mündungsabschluss horizontal","CHF",202,"Schiedel ICM5000",2,0,"J","ICM5000 130 Cape de finition horizontal","ICM5000 130 Mündungsabschluss horizontal","ICM5000 130 Terminale horizontale",136,1,"DN 130",null,174.9,0,null,null,202,"103173",27.099999999999994,159,43,"103173",202,27.099999999999994]
["103175",103175,null,"STK","ICM5000 180 Mündungsabschluss horizontal","CHF",237,"Schiedel ICM5000",2.8,0,"J","ICM5000 180 Cape de finition horizontal","ICM5000 180 Mündungsabschluss horizontal","ICM5000 180 Terminale horizontale",136,1,"DN 180",null,205.7,0,null,null,237,"103175",31.300000000000011,187,50,"103175",237,31.300000000000011]
["103178",103178,null,"STK","ICM5000 300 Mündungsabschluss horizontal","CHF",380,"Schiedel ICM5000",5.5,0,"J","ICM5000 300 Cape de finition horizontal","ICM5000 300 Mündungsabschluss horizontal","ICM5000 300 Terminale horizontale",136,1,"DN 300",null,330,0,null,null,380,"103178",50,300,80,"103178",380,50]
["103182",103182,null,"STK","ICM5000 500 Mündungsabschluss horizontal","CHF",415,"Schiedel ICM5000",12.5,0,"J","ICM5000 500 Cape de finition horizontal","ICM5000 500 Mündungsabschluss horizontal","ICM5000 500 Terminale horizontale",136,1,"DN 500",null,360.8,0,null,null,415,"103182",54.199999999999989,328,87,"103182",415,54.199999999999989]
["103187",103187,null,"STK","ICM5000 150 Element mit Kondensatablauf 1/2\"","CHF",185,"Schiedel ICM5000",1.3,0,"J","ICM5000 150 Element avec écoulement cond.  L205mm","ICM5000 150 Element mit Kondensatablauf 1/2\"","ICM5000 150 Elemento con scarico condensa 1/2\"",136,1,"DN 150",null,160.6,0,null,null,185,"103187",24.400000000000006,146,39,"103187",185,24.400000000000006]
["103190",103190,null,"STK","ICM5000 250 Element mit Kondensatablauf 1/2\"","CHF",227,"Schiedel ICM5000",2,0,"J","ICM5000 250 Element avec écoulement cond.  L205mm","ICM5000 250 Element mit Kondensatablauf 1/2\"","ICM5000 250 Elemento con scarico condensa 1/2\"",136,1,"DN 250",null,196.9,0,null,null,227,"103190",30.099999999999994,179,48,"103190",227,30.099999999999994]
["103192",103192,null,"STK","ICM5000 350 Element mit Kondensatablauf 1/2\"","CHF",271,"Schiedel ICM5000",2.7,0,"J","ICM5000 350 Element avec écoulement cond.  L205mm","ICM5000 350 Element mit Kondensatablauf 1/2\"","ICM5000 350 Elemento con scarico condensa 1/2\"",136,1,"DN 350",null,235.4,0,null,null,271,"103192",35.599999999999994,214,57,"103192",271,35.599999999999994]
["103198",103198,null,"STK","ICM5000 100 Winkel 15°","CHF",123,"Schiedel ICM5000",0.9,0,"J","ICM5000 100 Coude 15° ","ICM5000 100 Winkel 15°","ICM5000 100 Gomito 15°",136,1,"DN 100",null,106.7,0,null,null,123,"103198",16.299999999999997,97,26,"103198",123,16.299999999999997]
["103201",103201,null,"STK","ICM5000 180 Winkel 15°","CHF",162,"Schiedel ICM5000",1.5,0,"J","ICM5000 180 Coude 15° ","ICM5000 180 Winkel 15°","ICM5000 180 Gomito 15°",136,1,"DN 180",null,140.80000000000001,0,null,null,162,"103201",21.199999999999989,128,34,"103201",162,21.199999999999989]
["103203",103203,null,"STK","ICM5000 250 Winkel 15°","CHF",207,"Schiedel ICM5000",1.9,0,"J","ICM5000 250 Coude 15° ","ICM5000 250 Winkel 15°","ICM5000 250 Gomito 15°",136,1,"DN 250",null,179.3,0,null,null,207,"103203",27.699999999999989,163,44,"103203",207,27.699999999999989]
["103206",103206,null,"STK","ICM5000 100 Winkel 30°","CHF",121,"Schiedel ICM5000",0.9,0,"J","ICM5000 100 Coude 30°","ICM5000 100 Winkel 30°","ICM5000 100 Gomito 30°",136,1,"DN 100",null,104.5,0,null,null,121,"103206",16.5,95,26,"103206",121,16.5]
["103211",103211,null,"STK","ICM5000 250 Winkel 30°","CHF",212,"Schiedel ICM5000",2.5,0,"J","ICM5000 250 Coude 30°","ICM5000 250 Winkel 30°","ICM5000 250 Gomito 30°",136,1,"DN 250",null,183.7,0,null,null,212,"103211",28.300000000000011,167,45,"103211",212,28.300000000000011]
["103215",103215,null,"STK","ICM5000 450 Winkel 30°","CHF",533,"Schiedel ICM5000",6.8,0,"J","ICM5000 450 Coude 30°","ICM5000 450 Winkel 30°","ICM5000 450 Gomito 30°",136,1,"DN 450",null,463.1,0,null,null,533,"103215",69.899999999999977,421,112,"103215",533,69.899999999999977]
["103220",103220,null,"STK","ICM5000 130 Winkel 45°","CHF",119,"Schiedel ICM5000",1.4,0,"J","ICM5000 130 Coude 45°","ICM5000 130 Winkel 45°","ICM5000 130 Gomito 45°",136,1,"DN 130",null,103.4,0,null,null,119,"103220",15.599999999999994,94,25,"103220",119,15.599999999999994]
["103223",103223,null,"STK","ICM5000 200 Winkel 45°","CHF",167,"Schiedel ICM5000",2.2000000000000002,0,"J","ICM5000 200 Coude 45°","ICM5000 200 Winkel 45°","ICM5000 200 Gomito 45°",136,1,"DN 200",null,145.19999999999999,0,null,null,167,"103223",21.800000000000011,132,35,"103223",167,21.800000000000011]
[{"$f":"B2508&\"\"","v":"103225"},103225,null,"STK",{"$f":"IF($E$200=2,L2508,IF($E$200=3,N2508,M2508))","v":"ICM5000 300 Winkel 45°"},"CHF",{"$f":"IF($L$190=1,W2508,S2508)","v":245},"Schiedel ICM5000",3.8,0,"J","ICM5000 300 Coude 45°","ICM5000 300 Winkel 45°","ICM5000 300 Gomito 45°",136,1,"DN 300",null,212.3,0,null,null,245,"103225",32.699999999999989,193,52,"103225",245,32.699999999999989]
["103230",103230,null,"STK","ICM5000 600 Winkel 45°","CHF",737,"Schiedel ICM5000",12,0,"J","ICM5000 600 Coude 45°","ICM5000 600 Winkel 45°","ICM5000 600 Gomito 45°",136,1,"DN 600",null,640.20000000000005,0,null,null,737,"103230",96.799999999999955,582,155,"103230",737,96.799999999999955]
["103234",103234,null,"STK","ICM5000 150 Winkel 90°","CHF",167,"Schiedel ICM5000",2.4,0,"J","ICM5000 150 Coude 90°","ICM5000 150 Winkel 90°","ICM5000 150 Gomito 90°",136,1,"DN 150",null,145.19999999999999,0,null,null,167,"103234",21.800000000000011,132,35,"103234",167,21.800000000000011]
["103235",103235,null,"STK","ICM5000 180 Winkel 90°","CHF",183,"Schiedel ICM5000",3.1,0,"J","ICM5000 180 Coude 90°","ICM5000 180 Winkel 90°","ICM5000 180 Gomito 90°",136,1,"DN 180",null,158.4,0,null,null,183,"103235",24.599999999999994,144,39,"103235",183,24.599999999999994]
["103239",103239,null,"STK","ICM5000 350 Winkel 90°","CHF",500,"Schiedel ICM5000",7.4,0,"J","ICM5000 350 Coude 90°","ICM5000 350 Winkel 90°","ICM5000 350 Gomito 90°",136,1,"DN 350",null,434.5,0,null,null,500,"103239",65.5,395,105,"103239",500,65.5]
["103243",103243,null,"STK","ICM5000 600 Winkel 90°","CHF",849,"Schiedel ICM5000",18,0,"J","ICM5000 600 Coude 90°","ICM5000 600 Winkel 90°","ICM5000 600 Gomito 90°",136,1,"DN 600",null,738.1,0,null,null,849,"103243",110.89999999999998,671,178,"103243",849,110.89999999999998]
["103249",103249,null,"STK","KRS 250 Fussteil Bodenmontage mit Ablauf L350mm","CHF",322,"Schiedel KERASTAR",15,330,"J","KRS 250 Elément de base avec écoulement L350mm","KRS 250 Fussteil Bodenmontage mit Ablauf L350mm","KRS 250 Elemento Poggiapiedi con scarico L350mm",137,1,"DN 250",null,280,"265700825","105697","4037494277522",322,"103249",42,280,42,"103249",322,42]
["103252",103252,null,"STK","KRS Fusssteher-Set 4Stk. verstellbar L325-540mm","CHF",527,"Schiedel KERASTAR",1.5,0,"J","KRS Pieds réglable pour plaque de base ","KRS Fusssteher-Set 4Stk. verstellbar L325-540mm","KRS Piede stayer set modificabili 4 pz L325-540 mm",137,1,"ZBH Kerastar",null,458,"265400300","101493","4037494283844",527,"103252",69,458,69,"103252",527,69]
["103255",103255,null,"STK","KRS 180 Fussteil für Wohnraum verstelb. L186-286mm","CHF",236,"Schiedel KERASTAR",7,186,"J","KRS 180 Elément de base réglable, habitation ","KRS 180 Fussteil für Wohnraum verstelb. L186-286mm","KRS 180 Elemento di base regolabile senza scarico",137,1,"DN 180",null,205,"265701118","105705","4037494135761",236,"103255",31,205,31,"103255",236,31]
["103258",103258,null,"STK","KRS 140 Grundplatte verstärkt mit Ablauf","CHF",187,"Schiedel KERASTAR",5.8,44,"J","KRS 140 Plaque de base et écoulement","KRS 140 Grundplatte verstärkt mit Ablauf","KRS 140 Piastra base rinforzato  con scadenza",137,1,"DN 140",null,162,"265701714",null,null,187,"103258",25,162,25,"103258",187,25]
["103260",103260,null,"STK","KRS 180 Grundplatte verstärkt mit Ablauf","CHF",213,"Schiedel KERASTAR",7.6,44,"J","KRS 180 Plaque de base et écoulement","KRS 180 Grundplatte verstärkt mit Ablauf","KRS 180 Piastra base rinforzato  con scadenza",137,1,"DN 180",null,185,"265701718",null,null,213,"103260",28,185,28,"103260",213,28]
["103263",103263,null,"STK","KRS 300 Grundplatte verstärkt mit Ablauf","CHF",559,"Schiedel KERASTAR",12,44,"J","KRS 300 Plaque de base et écoulement","KRS 300 Grundplatte verstärkt mit Ablauf","KRS 300 Piastra base rinforzato  con scadenza",137,1,"DN 300",null,486,"265701730",null,null,559,"103263",73,486,73,"103263",559,73]
["103268",103268,null,"STK","KRS 200 Grundplatte mit Russtopf.","CHF",339,"Schiedel KERASTAR",8.4,44,"J","KRS 200 Plaque de base avec pot à suie.","KRS 200 Grundplatte mit Russtopf.","KRS 200 Piastra base e bentola fuliggine.",137,1,"DN 200",null,294,"265702620",null,null,339,"103268",45,294,45,"103268",339,45]
["103273",103273,null,"STK","KRS 200  Revisionselement trocken- Betrieb L665mm","CHF",547,"Schiedel KERASTAR",23,665,"J","KRS 200  Elément porte d'inspection L665mm","KRS 200  Revisionselement trocken- Betrieb L665mm","KRS 200  Elemento con inspezione per com. Solidi",137,1,"DN 200",null,475,"236715020","105673","4037494277614",547,"103273",72,475,72,"103273",547,72]
["103276",103276,null,"STK","KRS 400  Revisionselement trocken- Betrieb L665mm","CHF",1413,"Schiedel KERASTAR",40,665,"J","KRS 400  Elément porte d'inspection L665mm","KRS 400  Revisionselement trocken- Betrieb L665mm","KRS 400  Elemento con inspezione per com. Solidi",137,1,"DN 400",null,1228,"236715040",null,null,1413,"103276",185,1228,185,"103276",1413,185]
["103285",103285,null,"STK","KRS 160  T-Stück 90 ° L665mm ","CHF",329,"Schiedel KERASTAR",17,665,"J","KRS 160 Pièce Té 90 ° L665mm ","KRS 160  T-Stück 90 ° L665mm ","KRS 160 Pezzo T 90 ° L665mm ",137,1,"DN 160",null,286,"230706616","105654","4037494277645",329,"103285",43,286,43,"103285",329,43]
["103291",103291,null,"STK","KRS 140  Anschlussrosette zu T-Stk. Øi 145mm ","CHF",57,"Schiedel KERASTAR",0.8,0,"J","KRS 140 Rosace de raccordement pour pc.-T-Øi 145mm","KRS 140  Anschlussrosette zu T-Stk. Øi 145mm ","KRS 140  Rosetta collegamento per pz. T Øi 145mm",137,1,"DN 140",null,49,"265701314",null,null,57,"103291",8,49,8,"103291",57,8]
["103294",103294,null,"STK","KRS 200  Anschlussrosette zu T-Stk. Øi 205mm","CHF",61,"Schiedel KERASTAR",1,0,"J","KRS 200 Rosace de raccordement pour pc.-T-Øi 205mm","KRS 200  Anschlussrosette zu T-Stk. Øi 205mm","KRS 200  Rosetta collegamento per pz. T Øi 205mm",137,1,"DN 200",null,53,"265701320",null,null,61,"103294",8,53,8,"103294",61,8]
["103296",103296,null,"STK","KRS 300  Anschlussrosette zu T-Stk. Øi 305mm","CHF",213,"Schiedel KERASTAR",1.8,0,"J","KRS 300 Rosace de raccordement pour pc.-T-Øi 305mm","KRS 300  Anschlussrosette zu T-Stk. Øi 305mm","KRS 300  Rosetta collegamento per pz. T Øi 305mm",137,1,"DN 300",null,185,"265701330",null,null,213,"103296",28,185,28,"103296",213,28]
["103299",103299,null,"STK","KRS 160  T-Stück 45 ° L665mm ","CHF",473,"Schiedel KERASTAR",20.5,665,"J","KRS 160  Pièce Té 45 ° L665mm ","KRS 160  T-Stück 45 ° L665mm ","KRS 160  Pezzo T 45 ° L665mm ",137,1,"DN 160",null,411,"230716616","105659","4037494277690",473,"103299",62,411,62,"103299",473,62]
["103303",103303,null,"STK","KRS 140  Längenelement L665mm ","CHF",165,"Schiedel KERASTAR",13,665,"J","KRS 140  Elément droit L665mm ","KRS 140  Längenelement L665mm ","KRS 140  Elemento lunghezze L665mm ",137,1,"DN 140",null,143,"133006614","105579","4037494277737",165,"103303",22,143,22,"103303",165,22]
["103307",103307,null,"STK","KRS 250  Längenelement L665mm ","CHF",227,"Schiedel KERASTAR",19,665,"J","KRS 250  Elément droit L665mm ","KRS 250  Längenelement L665mm ","KRS 250  Elemento lunghezze L665mm ",137,1,"DN 250",null,197,"133006625","105583","4037494277775",227,"103307",30,197,30,"103307",227,30]
["103312",103312,null,"STK","KRS 180  Längenelement L330mm ","CHF",133,"Schiedel KERASTAR",9,331,"J","KRS 180  Elément droit L330mm ","KRS 180  Längenelement L330mm ","KRS 180  Elemento lunghezze L330mm ",137,1,"DN 180",null,115,"133003318","105576","4037494277805",133,"103312",18,115,18,"103312",133,18]
["103315",103315,null,"STK","KRS 300  Längenelement L330mm ","CHF",339,"Schiedel KERASTAR",13,331,"J","KRS 300  Elément droit L330mm ","KRS 300  Längenelement L330mm ","KRS 300  Elemento lunghezze L330mm ",137,1,"DN 300",null,294,"133003330",null,null,339,"103315",45,294,45,"103315",339,45]
["103317",103317,null,"STK","KRS 140  Längenelement L165mm ","CHF",81,"Schiedel KERASTAR",3.5,165,"J","KRS 140  Elément droit L165mm ","KRS 140  Längenelement L165mm ","KRS 140  Elemento lunghezze L165mm ",137,1,"DN 140",null,70,"133001614","105569","4037494277836",81,"103317",11,70,11,"103317",81,11]
["103320",103320,null,"STK","KRS 200  Längenelement L165mm ","CHF",91,"Schiedel KERASTAR",5,165,"J","KRS 200  Elément droit L165mm ","KRS 200  Längenelement L165mm ","KRS 200  Elemento lunghezze L165mm ",137,1,"DN 200",null,79,"133001620","105572","4037494277867",91,"103320",12,79,12,"103320",91,12]
["103326",103326,null,"STK","KRS 180  Mündungsabschluss L207mm","CHF",110,"Schiedel KERASTAR",3.1,207,"J","KRS 180  Cape de finition conique L207mm","KRS 180  Mündungsabschluss L207mm","KRS 180  Terminale conico L207mm",137,1,"DN 180",null,95,"265700018",null,null,110,"103326",15,95,15,"103326",110,15]
["103327",103327,null,"STK","KRS 200  Mündungsabschluss L207mm","CHF",122,"Schiedel KERASTAR",4.5,207,"J","KRS 200  Cape de finition conique L207mm","KRS 200  Mündungsabschluss L207mm","KRS 200  Terminale conico L207mm",137,1,"DN 200",null,106,"265700020",null,null,122,"103327",16,106,16,"103327",122,16]
["103331",103331,null,"STK","KRS 140  Winkel 15 ° ","CHF",199,"Schiedel KERASTAR",4.9000000000000004,0,"J","KRS 140  Coude 15 ° ","KRS 140  Winkel 15 ° ","KRS 140  Gomito 15 ° ",137,1,"DN 140",null,173,"133031514","105584","4037494278130",199,"103331",26,173,26,"103331",199,26]
["103335",103335,null,"STK","KRS 250  Winkel 15 ° ","CHF",325,"Schiedel KERASTAR",12.6,0,"J","KRS 250  Coude 15 ° ","KRS 250  Winkel 15 ° ","KRS 250  Gomito 15 ° ",137,1,"DN 250",null,282,"133031525","105588","4037494278178",325,"103335",43,282,43,"103335",325,43]
["103338",103338,null,"STK","KRS 140  Winkel 30 ° ","CHF",217,"Schiedel KERASTAR",6.5,0,"J","KRS 140  Coude 30 ° ","KRS 140  Winkel 30 ° ","KRS 140  Gomito 30 ° ",137,1,"DN 140",null,188,"133033014","105589","4037494278185",217,"103338",29,188,29,"103338",217,29]
["103340",103340,null,"STK","KRS 180  Winkel 30 ° ","CHF",247,"Schiedel KERASTAR",8.6,0,"J","KRS 180  Coude 30 ° ","KRS 180  Winkel 30 ° ","KRS 180  Gomito 30 ° ",137,1,"DN 180",null,214,"133033018","105591","4037494278208",247,"103340",33,214,33,"103340",247,33]
["103346",103346,null,"STK","KRS 160  Winkel 45 ° ","CHF",229,"Schiedel KERASTAR",7.5,0,"J","KRS 160  Coude 45 ° ","KRS 160  Winkel 45 ° ","KRS 160  Gomito 45 ° ",137,1,"DN 160",null,199,"133034516","105595","4037494278246",229,"103346",30,199,30,"103346",229,30]
["103349",103349,null,"STK","KRS 250  Winkel 45 ° ","CHF",351,"Schiedel KERASTAR",12.4,0,"J","KRS 250  Coude 45 ° ","KRS 250  Winkel 45 ° ","KRS 250  Gomito 45 ° ",137,1,"DN 250",null,305,"133034525","105598","4037494278277",351,"103349",46,305,46,"103349",351,46]
["103351",103351,null,"STK","KRS 400  Winkel 45 ° ","CHF",906,"Schiedel KERASTAR",18,0,"J","KRS 400  Coude 45 ° ","KRS 400  Winkel 45 ° ","KRS 400  Gomito 45 ° ",137,1,"DN 400",null,787,"133034540",null,null,906,"103351",119,787,119,"103351",906,119]
["103354",103354,null,"STK","KRS 180 Anschlussrosette Øi 314mm ØA 484mm","CHF",34,"Schiedel KERASTAR",0.63,0,"J","KRS 180 Rosage de raccordement Øi 314mm ØA 484mm","KRS 180 Anschlussrosette Øi 314mm ØA 484mm","KRS 180 Rosetta di collegamento Øi 314mm ØA 484mm",137,1,"DN 180",null,29,"265404732",null,null,34,"103354",5,29,5,"103354",34,5]
["103359",103359,null,"STK","KRS 140 Abdeckros.16-21° Dachneigung ","CHF",32,"Schiedel KERASTAR",0.42,0,"J","KRS 140 Rosace récouvrement.16-21° pente du toit ","KRS 140 Abdeckros.16-21° Dachneigung ","KRS 140 Copertina rosa 16-21 ° passo",137,1,"DN 140",null,27,"265702514",null,null,32,"103359",5,27,5,"103359",32,5]
["103363",103363,null,"STK","KRS 250 Abdeckros.16-21° Dachneigung  ","CHF",50,"Schiedel KERASTAR",0.52,0,"J","KRS 250 Rosace récouvrement.16-21° pente du toit  ","KRS 250 Abdeckros.16-21° Dachneigung  ","KRS 250 Copertina rosa 16-21 ° passo ",137,1,"DN 250",null,43,"265702525",null,null,50,"103363",7,43,7,"103363",50,7]
["103382",103382,null,"STK","KRS Wand-Konsole Typ 820mm (Paar)","CHF",206,"Schiedel KERASTAR",2.76,0,"J","KRS Console murale Typ 820mm (Paire)","KRS Wand-Konsole Typ 820mm (Paar)","KRS Suporto a muro per piastra di base tipo 820mm",137,1,"ZBH Kerastar",null,179,"265400282",null,null,206,"103382",27,179,27,"103382",206,27]
["103383",103383,null,"STK","KRS Wand-Konsole Typ 1004mm (Paar)","CHF",279,"Schiedel KERASTAR",3.26,0,"J","KRS Console murale Typ 1004mm (Paire)","KRS Wand-Konsole Typ 1004mm (Paar)","KRS Suporto a muro per piastra di base tipo 1004mm",137,1,"ZBH Kerastar",null,242,"265400295",null,null,279,"103383",37,242,37,"103383",279,37]
["103392",103392,null,"STK","KRS 160 Seilabspannring","CHF",26,"Schiedel KERASTAR",0.68,0,"J","KRS 160 Bride de haubanage","KRS 160 Seilabspannring","KRS 160 Collare per cavi tiranti",137,1,"DN 160",null,22,"265700716","105689","4037494278406",26,"103392",4,22,4,"103392",26,4]
["103393",103393,null,"STK","KRS 180 Seilabspannring","CHF",28,"Schiedel KERASTAR",0.73,0,"J","KRS 180 Bride de haubanage","KRS 180 Seilabspannring","KRS 180 Collare per cavi tiranti",137,1,"DN 180",null,24,"265700718","105690","4037494278413",28,"103393",4,24,4,"103393",28,4]
["103399",103399,null,"STK","KRS 200 Statisches Klemmband","CHF",30,"Schiedel KERASTAR",1.833,0,"J","KRS 200 Bride du fixation statique","KRS 200 Statisches Klemmband","KRS 200 Fascetta di sicurezza statico",137,1,"DN 200",null,26,"265702420",null,null,30,"103399",4,26,4,"103399",30,4]
["103400",103400,null,"STK","KRS 250 Statisches Klemmband","CHF",35,"Schiedel KERASTAR",2.0979999999999999,0,"J","KRS 250 Bride du fixation statique","KRS 250 Statisches Klemmband","KRS 250 Fascetta di sicurezza statico",137,1,"DN 250",null,30,"265702425",null,null,35,"103400",5,30,5,"103400",35,5]
["103404",103404,null,"STK","KRS 160 Wandhalt.statisch 50mm","CHF",91,"Schiedel KERASTAR",2.2000000000000002,0,"J","KRS 160 Fixation murale statique 50mm","KRS 160 Wandhalt.statisch 50mm","KRS 160 Collare a muro 50mm statico 50mm",137,1,"DN 160",null,79,"265701516",null,null,91,"103404",12,79,12,"103404",91,12]
["103414",103414,null,"STK","KRS 140 Sparrenhalter ","CHF",88,"Schiedel KERASTAR",1.38,0,"J","KRS 140 Fixation aux chevrons","KRS 140 Sparrenhalter ","KRS 140 Fissaggio delle travi",137,1,"DN 140",null,76,"265700914","105698","4037494277980",88,"103414",12,76,12,"103414",88,12]
["103419",103419,null,"STK","KRS 450 Sparrenhalter ","CHF",98,"Schiedel KERASTAR",1.8,0,"J","KRS 450 Fixation aux chevrons","KRS 450 Sparrenhalter ","KRS 450 Fissaggio delle travi",137,1,"DN 300",null,85,"265700930",null,null,98,"103419",13,85,13,"103419",98,13]
["103422",103422,null,"STK","KRS 160  Wandhalter 50 Light ","CHF",55,"Schiedel KERASTAR",0.89,0,"J","KRS 160  Fixation murale 50 mm légère ","KRS 160  Wandhalter 50 Light ","KRS 160  Collare a muro 50mm leggermente",137,1,"DN 160",null,47,"265700316",null,null,55,"103422",8,47,8,"103422",55,8]
["103424",103424,null,"STK","KRS 200  Wandhalter 50 Light ","CHF",56,"Schiedel KERASTAR",0.98,0,"J","KRS 200  Fixation murale 50 mm légère ","KRS 200  Wandhalter 50 Light ","KRS 200  Collare a muro 50mm leggermente",137,1,"DN 200",null,48,"265700320",null,null,56,"103424",8,48,8,"103424",56,8]
["103427",103427,null,"STK","KRS 160  Wandhalterung 50mm ","CHF",37,"Schiedel KERASTAR",0.95,0,"J","KRS 160  Fixation murale 50mm ","KRS 160  Wandhalterung 50mm ","KRS 160  Collare a muro 50mm ",137,1,"DN 160",null,32,"265706016","101560","4037494816882",37,"103427",5,32,5,"103427",37,5]
["103433",103433,null,"STK","KRS 160 Basten Standard mit Stulpring Inox","CHF",375,"Schiedel KERASTAR",4.0999999999999996,0,"J","KRS 160  Chapeau Basten standart avec dila Inox","KRS 160 Basten Standard mit Stulpring Inox","KRS 160 Terminale Basten con dila Inox",137,1,"DN 160",null,353,"917015",null,null,375,"103433",22,351,24,"103433",375,22]
["103435",103435,null,"STK","KRS 200 Basten Standard mit Stulpring Inox","CHF",410,"Schiedel KERASTAR",4.8,0,"J","KRS 200  Chapeau Basten standart avec dila Inox","KRS 200 Basten Standard mit Stulpring Inox","KRS 200 Terminale Basten con dila Inox",137,1,"DN 200",null,386,"917020",null,null,410,"103435",24,384,26,"103435",410,24]
["103438",103438,null,"STK","KRS 140 Basten Regulator mit Stulpring Inox","CHF",470,"Schiedel KERASTAR",4.2,0,"J","KRS 140 Chapeau Basten Regulator avec dila Inox","KRS 140 Basten Regulator mit Stulpring Inox","KRS 140 Terminale regulator Basten con dila Inox",137,1,"DN 140",null,443,"917213",null,null,470,"103438",27,441,29,"103438",470,27]
["103442",103442,null,"STK","KRS 250 Basten Regulator mit Stulpring Inox","CHF",578,"Schiedel KERASTAR",5.5,0,"J","KRS 250 Chapeau Basten Regulator avec dila Inox","KRS 250 Basten Regulator mit Stulpring Inox","KRS 250 Terminale regulator Basten con dila Inox",137,1,"DN 250",null,545,"917225",null,null,578,"103442",33,543,35,"103442",578,33]
["103447",103447,null,"STK","KER 160 Kondensattopf komplett L132mm","CHF",115,"Schiedel KERANOVA",3.75,0,"J","KER 160 Collecteur de condensat L132 mm","KER 160 Kondensattopf komplett L132mm","KER 160 Bancinella per condensa L132mm",113,1,"DN 160",null,100,"KKTU16","105450","4037494262382",115,"103447",15,98,17,"103447",115,15]
["103448",103448,null,"STK","KER 180 Kondensattopf komplett L145mm","CHF",124,"Schiedel KERANOVA",4.6500000000000004,0,"J","KER 180 Collecteur de condensat L145 mm","KER 180 Kondensattopf komplett L145mm","KER 180 Bancinella per condensa L145mm",113,1,"DN 180",null,107,"KKTU18","105451","4037494262399",124,"103448",17,105,19,"103448",124,17]
["103454",103454,null,"STK","KER 120 Keranova-Rohr komplett L1330mm ","CHF",133.4,"Schiedel KERANOVA",6.38,1330,"J","KER 120 Conduit KERANOVA complet L1330mm ","KER 120 Keranova-Rohr komplett L1330mm ","KER 120 Condoto keranova completto L1330mm ",113,1,"DN 120",null,116,"KRR12133","105453","4037494056738",133.4,"103454",17.400000000000006,116,17.400000000000006,"103454",133.4,17.400000000000006,133.4,133.4]
["103457",103457,null,"STK","KER 180 Keranova-Rohr komplett L1330mm ","CHF",164.5,"Schiedel KERANOVA",12.77,1330,"J","KER 180 Conduit KERANOVA complet L1330mm ","KER 180 Keranova-Rohr komplett L1330mm ","KER 180 Condoto keranova completto L1330mm ",113,1,"DN 180",null,143,"KRR18133","105459","4037494056769",164.5,"103457",21.5,143,21.5,"103457",164.5,21.5,164.5,164.45]
["103459",103459,null,"STK","KER 120 Keranova-Rohr komplett L660mm ","CHF",92,"Schiedel KERANOVA",4.34,665,"J","KER 120 Conduit KERANOVA complet L660mm ","KER 120 Keranova-Rohr komplett L660mm ","KER 120 Condoto keranova completto L660mm ",113,1,"DN 120",null,80,"KRR1266","105454","4037494056783",92,"103459",12,80,12,"103459",92,12,92,92]
["103462",103462,null,"STK","KER 180 Keranova-Rohr komplett L660mm ","CHF",113,"Schiedel KERANOVA",6.5,665,"J","KER 180 Conduit KERANOVA complet L660mm ","KER 180 Keranova-Rohr komplett L660mm ","KER 180 Condoto keranova completto L660mm ",113,1,"DN 180",null,98,"KRR1866","105460","4037494056813",113,"103462",15,97,16,"103462",113,15]
["103467",103467,null,"STK","KER 160 Verbindungsmanchette inkl. Abstandhalter","CHF",43,"Schiedel KERANOVA",0.35,0,"J","KER 160 Manchon de raccordement incl.distanceurs","KER 160 Verbindungsmanchette inkl. Abstandhalter","KER 160 Manicotto di collegamento",113,1,"DN 160",null,37,"KAH16",null,null,43,"103467",6,37,6,"103467",43,6]
["103471",103471,null,"STK","KER 120  Keranova-Fugenglätter","CHF",52,"Schiedel KERANOVA",0.41,0,"J","KER 120  Keranova-Lissoir pour joints","KER 120  Keranova-Fugenglätter","KER 120  Ferro per per lisciatura dei giunti",113,1,"DN 120",null,45,"KFG12","105447","4037494044612",52,"103471",7,45,7,"103471",52,7]
["103475",103475,null,"STK","KER 200  Keranova-Fugenglätter","CHF",72,"Schiedel KERANOVA",0.47799999999999998,0,"J","KER 200  Keranova-Lissoir pour joints","KER 200  Keranova-Fugenglätter","KER 200  Ferro per per lisciatura dei giunti",113,1,"DN 200",null,62,"KFG20","101442","4037494044650",72,"103475",10,62,10,"103475",72,10]
["103476",103476,null,"STK","KER 250 Keranova-Fugenglätter","CHF",79,"Schiedel KERANOVA",0.47799999999999998,0,"J","KER 250  Keranova-Lissoir pour joints","KER 250 Keranova-Fugenglätter","KER 250  Ferro per per lisciatura dei giunti",113,1,"DN 250",null,68,"KFG25","101443","4037494044667",79,"103476",11,68,11,"103476",79,11]
["103482",103482,null,"STK","KER 120 T-Stück 90° L330mm Stutzen L90mm","CHF",212,"Schiedel KERANOVA",2.4500000000000002,330,"J","KER 120 Pièce Té 90° L330mm raccord L90mm","KER 120 T-Stück 90° L330mm Stutzen L90mm","KER 120 Pezzo T 90° L330mm raccordo L90mm",113,1,"DN 120",null,184,"KT12","108649","4037494063644",212,"103482",28,184,28,"103482",212,28,212,212.02030456852793]
["103483",103483,null,"STK","KER 140 T-Stück 90° L330mm Stutzen L90mm","CHF",223.5,"Schiedel KERANOVA",2.48,330,"J","KER 140 Pièce Té 90° L330mm raccord L90mm","KER 140 T-Stück 90° L330mm Stutzen L90mm","KER 140 Pezzo T 90° L330mm raccordo L90mm",113,1,"DN 140",null,194,"KT14","108650","4037494063651",223.5,"103483",29.5,194,29.5,"103483",223.5,29.5,223.5,223.54314720812184]
["103490",103490,null,"STK","KER 180 Revisionsdeckel zu T-Stück Festbrennstoffe","CHF",61,"Schiedel KERANOVA",1.335,0,"J","KER 180 Couvercle révision pour piece T ","KER 180 Revisionsdeckel zu T-Stück Festbrennstoffe","KER 180 Tapo per pezzo T per combustibile solidi",113,1,"DN 180",null,53,"25500618",null,null,61,"103490",8,53,8,"103490",61,8]
["103492",103492,null,"STK","KER 120 Universalstutzen 0°","CHF",79,"Schiedel KERANOVA",1.7,0,"J","KER 120 Manchon universel RA et PA 0°","KER 120 Universalstutzen 0°","KER 120 Raccordo universale0°",113,1,"DN 120",null,68,"KSTU12","105476","4037494262153",79,"103492",11,68,11,"103492",79,11]
["103495",103495,null,"STK","KER 180 Universalstutzen 0°","CHF",98,"Schiedel KERANOVA",3.3,0,"J","KER 180  Manchon universel RA et PA 0°","KER 180 Universalstutzen 0°","KER 180 Raccordo universale0°",113,1,"DN 180",null,85,"KSTU18","105482","4037494262184",98,"103495",13,83,15,"103495",98,13]
["103500",103500,null,"STK","KER 140 Universalstutzen 45°","CHF",112,"Schiedel KERANOVA",2.1,0,"J","KER 140  Manchon universel RA et PA 45°","KER 140 Universalstutzen 45°","KER 140 Raccordo universale45°",113,1,"DN 140",null,97,"KSTU1445","105479","4037494265574",112,"103500",15,97,15,"103500",112,15]
["103506",103506,null,"STK","KER 120 Revisionsdeckel für Oel/Gas","CHF",92,"Schiedel KERANOVA",0.41,0,"J","KER 120 Couvercle de révision pour oel et mazout","KER 120 Revisionsdeckel für Oel/Gas","KER 120 Chiusura di revisione per oel/gaz",113,1,"DN 120",null,80,"RVP120","100547","4037494011713",92,"103506",12,80,12,"103506",92,12]
["103509",103509,null,"STK","KER 180 Revisionsdeckel für Oel/Gas","CHF",109,"Schiedel KERANOVA",0.5,0,"J","KER 180 Couvercle de révision pour oel et mazout","KER 180 Revisionsdeckel für Oel/Gas","KER 180 Chiusura di revisione per oel/gaz",113,1,"DN 180",null,94,"RVP180","100550","4037494011751",109,"103509",15,94,15,"103509",109,15]
["103511",103511,null,"STK","KER 120 Revisionsdeckel für Festbrennstoff","CHF",53,"Schiedel KERANOVA",0.8,0,"J","KER 120 Couvercle de révision combustibles solides","KER 120 Revisionsdeckel für Festbrennstoff","KER 120 Chiusura di revisione combustibile solidi",113,1,"DN 120",null,46,"RVPF120","105492","4037494262320",53,"103511",7,46,7,"103511",53,7]
["103514",103514,null,"STK","KER 180 Revisionsdeckel für Festbrennstoff","CHF",61,"Schiedel KERANOVA",1.335,0,"J","KER 180 Couvercle de révision combustibles solides","KER 180 Revisionsdeckel für Festbrennstoff","KER 180 Chiusura di revisione combustibile solidi",113,1,"DN 180",null,53,"RVPF180","105495","4037494085226",61,"103514",8,53,8,"103514",61,8]
["103520",103520,null,"STK","KER 180 Anreisschablone Universal","CHF",120,"Schiedel KERANOVA",1.06,0,"J","KER 180 Gabarit de tracage universel","KER 180 Anreisschablone Universal","KER 180 Dima di tracciamento",113,1,"DN 180",null,104,"KASU18","105436","4037494262559",120,"103520",16,104,16,"103520",120,16]
["103522",103522,null,"STK","KER 250 Anreisschablone Universal","CHF",124,"Schiedel KERANOVA",1.24,0,"J","KER 250 Gabarit de tracage universel","KER 250 Anreisschablone Universal","KER 250 Dima di tracciamento",113,1,"DN 250",null,107,"KASU25","105440","4037494267073",124,"103522",17,107,17,"103522",124,17]
["103525",103525,null,"STK","KER 160 Bogen verstellbar 0-30° L660mm","CHF",395,"Schiedel KERANOVA",5.5,660,"J","KER 160 Coude réglable 0-30° L660mm","KER 160 Bogen verstellbar 0-30° L660mm","KER 160 Gomito regolabile 0-30° L660mm",113,1,"DN 160",null,343,"KVB16",null,null,395,"103525",52,343,52,"103525",395,52]
["103529",103529,null,"STK","KER 120 Statische-Manchette für Muffenverbindungen","CHF",38,"Schiedel KERANOVA",0.2,0,"J","KER 120 Manchette statique","KER 120 Statische-Manchette für Muffenverbindungen","KER 120 Brida statica per raccordoa manicotto",113,1,"DN 120",null,33,"KSM12","105470","4037494262474",38,"103529",5,33,5,"103529",38,5]
["103533",103533,null,"STK","KER 200 Statische-Manchette für Muffenverbindungen","CHF",49,"Schiedel KERANOVA",0.4,0,"J","KER 200 Manchette statique","KER 200 Statische-Manchette für Muffenverbindungen","KER 200 Brida statica per raccordoa manicotto",113,1,"DN 200",null,42,"KSM20","105474","4037494262511",49,"103533",7,42,7,"103533",49,7]
["103535",103535,null,"STK","KER 120 Statische-Abstützung für Bogen-Verstellbar","CHF",76,"Schiedel KERANOVA",0.2,0,"J","KER 120 Support statique pour coude réglable","KER 120 Statische-Abstützung für Bogen-Verstellbar","KER 120 Suporto statico per curva di spostamento",113,1,"DN 120",null,66,"KSA12","105464","4037494263464",76,"103535",10,66,10,"103535",76,10]
["103539",103539,null,"STK","KER 200 Statische-Abstützung für Bogen-Verstellbar","CHF",92,"Schiedel KERANOVA",0.2,0,"J","KER 200 Support statique pour coude réglable","KER 200 Statische-Abstützung für Bogen-Verstellbar","KER 200 Suporto statico per curva di spostamento",113,1,"DN 200",null,80,"KSA20","105468","4037494263501",92,"103539",12,80,12,"103539",92,12]
["103544",103544,null,"STK","KER 200 Universal-Kachelofenzargenset 200 x 200mm","CHF",212,"Schiedel KERANOVA",4.4000000000000004,0,"J","KER 200 et pour poêle en catelles 200 x 200mm","KER 200 Universal-Kachelofenzargenset 200 x 200mm","KER 200 Kit per telaio di stufe in maiolica 200 x 200mm",113,1,"DN 200",null,184,"KOZS2020","100472","4037494136263",212,"103544",28,184,28,"103544",212,28]
["103547",103547,null,"STK","KER 180 Zugbegrenzer mit Explosionsklappe","CHF",357,"Schiedel KERANOVA",1.05,0,"J","KER 180 Clapet d'éxplosion avec limiteur de tirage","KER 180 Zugbegrenzer mit Explosionsklappe","KER 180 Regolatore di tiragio combustibile",113,1,"ZBH Keranova",null,310,"ZBE18",null,null,357,"103547",47,310,47,"103547",357,47]
["103550",103550,null,"STK","KER 130 Adapter für Zugbegrenzer für DN160mm","CHF",48,"Schiedel KERANOVA",0.1,0,"J","KER 130 Baque d'adaption p. clapet d'éxpl. DN160mm","KER 130 Adapter für Zugbegrenzer für DN160mm","KER 130 Adattore per regolatore DN160mm",113,1,"ZBH Keranova",null,41,"AZB1316",null,null,48,"103550",7,41,7,"103550",48,7]
["103557",103557,null,"STK","KER 140 Adapter für Doppelfutter 130mm","CHF",65,"Schiedel KERANOVA",0.2,0,"J","KER 140 adapteur pour manchon doubler 130mm","KER 140 Adapter für Doppelfutter 130mm","KER 140 Adattore per doppia parete 130mm",113,1,"ZBH Keranova",null,56,"KAD1413","105421","4037494510100",65,"103557",9,56,9,"103557",65,9]
["103561",103561,null,"STK","KER 180 Adapter für Doppelfutter 150mm","CHF",78,"Schiedel KERANOVA",0.32,0,"J","KER 180 adapteur pour manchon doubler 150mm","KER 180 Adapter für Doppelfutter 150mm","KER 180 Adattore per doppia parete 150mm",113,1,"ZBH Keranova",null,67,"KAD1815","105425","4037494510148",78,"103561",11,67,11,"103561",78,11]
["103565",103565,null,"STK","KER 250 Adapter für Doppelfutter 250mm","CHF",91,"Schiedel KERANOVA",0.44,0,"J","KER 250 adapteur pour manchon doubler 250mm","KER 250 Adapter für Doppelfutter 250mm","KER 250 Adattore per doppia parete 250mm",113,1,"ZBH Keranova",null,79,"KAD2525","105429","4037494510179",91,"103565",12,79,12,"103565",91,12]
["103568",103568,null,"STK","KER 130 Doppelfutter 130mm","CHF",72,"Schiedel KERANOVA",0.18,0,"J","KER 130 Manchon double avec bajonette 130mm","KER 130 Doppelfutter 130mm","KER 130 Doppia parete 130mm",113,1,"ZBH Keranova",null,62,"DDWFV1313",null,null,72,"103568",10,62,10,"103568",72,10]
["103570",103570,null,"STK","KER 180 Doppelfutter 180mm","CHF",80,"Schiedel KERANOVA",0.18,0,"J","KER 180 Manchon double avec bajonette 180mm","KER 180 Doppelfutter 180mm","KER 180 Doppia parete 180mm",113,1,"ZBH Keranova",null,69,"DDWFV1818",null,null,80,"103570",11,69,11,"103570",80,11]
["103573",103573,null,"STK","KER 120 Abdeckblende 250 x 250mm","CHF",23,"Schiedel KERANOVA",0.2,0,"J","KER 120 Recouvrement carrée 250 x 250mm","KER 120 Abdeckblende 250 x 250mm","KER 120 Coperture 250 x 250mm",113,1,"ZBH Keranova",null,20,"ASBL13","101831","4037494262443",23,"103573",3,20,3,"103573",23,3]
["103579",103579,null,"STK","KER 180-200 Anschlussblende mit Gummi-Einlage","CHF",135,"Schiedel KERANOVA",1.75,0,"J","KER 180-200 Recouvrement carrée","KER 180-200 Anschlussblende mit Gummi-Einlage","KER 180-200 Coperture",113,1,"ZBH Keranova",null,117,"ASBAM1820","103248","4037494136041",135,"103579",18,117,18,"103579",135,18]
["103595",103595,null,"STK","KER Schieberahmen zu PTS1 145 x 275 mm L90mm","CHF",23,"Schiedel KERANOVA",0.26,0,"J","KER Cadre coulissant pour PTS1 145 x 275 mm L90mm","KER Schieberahmen zu PTS1 145 x 275 mm L90mm","KER Telaio adattamento PTS1 145 x 275 mm L90mm",113,1,"ZBH Keranova",null,20,"SRPTS1",null,null,23,"103595",3,20,3,"103595",23,3]
["103601",103601,null,"STK","KER 130 Mauerschelle","CHF",18,"Schiedel KERANOVA",0.52,0,"J","KER 130 Collier pour fixation au mur","KER 130 Mauerschelle","KER 130 Fascetta per parete",113,1,"DN 120",null,15,"265500205","103611","4037494266106",18,"103601",3,15,3,"103601",18,3]
["103606",103606,null,"STK","KER 250 Mauerschelle","CHF",33,"Schiedel KERANOVA",0.7,0,"J","KER 250 Collier pour fixation au mur","KER 250 Mauerschelle","KER 250 Fascetta per parete",113,1,"DN 250",null,28,"265500210","103616","4037494266151",33,"103606",5,28,5,"103606",33,5]
["103611",103611,null,"STK","KER 180 Mündungskonus","CHF",86,"Schiedel KERANOVA",0.57899999999999996,0,"J","KER 180 Cône de finition","KER 180 Mündungskonus","KER 180 Cono per sbocco",113,1,"DN 180",null,74,"MDKS18","105491","4037494063736",86,"103611",12,74,12,"103611",86,12]
["103614",103614,null,"STK","KER Rotempo Fugendichtmasse Kartusche a 310ml","CHF",40,"Schiedel KERANOVA",0.44,0,"J","KER Rotempo masse de join a 310ml ","KER Rotempo Fugendichtmasse Kartusche a 310ml","KER Rotempo mastice cartuccia di a 310ml",113,1,"ZBH Keranova",null,34,"FMR","100555","4037494012857",40,"103614",6,34,6,"103614",40,6]
["103618",103618,null,"STK","KER 80-200 Ablasswinde leicht ","CHF",1677,"Schiedel KERANOVA",15,0,"N","KER 80-200 Treuil légér 15 kg","KER 80-200 Ablasswinde leicht ","KER 80-200 Martinetto leggero",113,1,"ZBH Keranova",null,1458,"PALGL",null,null,1677,"103618",219,1458,219,"103618",1677,219]
["103622",103622,null,"STK","KER 120-250 Versetzzange ","CHF",1683,"Schiedel KERANOVA",11,0,"J","KER 120-250 Pince à poser réglable ","KER 120-250 Versetzzange ","KER 120-250 Pinza regolabile",113,1,"ZBH Keranova",null,1463,"411000",null,null,1683,"103622",220,1463,220,"103622",1683,220]
["103627",103627,null,"STK","ISOLIT 250 Einzügerelement 25","CHF",60,"ISOLIT",55,250,"J","ISOLIT 250 Elément simple 25","ISOLIT 250 Einzügerelement 25","ISOLIT 250 Elemento semplice 25",114,1,"DN 250",null,52,"300003",null,null,60,"103627",8,52,8,"103627",60,8]
["103638",103638,null,"STK","ISOLIT 200 Anfängerelement 20","CHF",149,"ISOLIT",40,250,"J","ISOLIT 200 Départ de cheminée 20","ISOLIT 200 Anfängerelement 20","ISOLIT 200 Elemento iniziale 20",114,1,"DN 200",null,129,"301001",null,null,149,"103638",20,129,20,"103638",149,20]
["103644",103644,null,"STK","ISOLIT 250 Rauchrohranschlusselement RA 25/25/90°","CHF",345,"ISOLIT",100,500,"J","ISOLIT 250 Raccord de conduit de fumée 25/25/ 90°","ISOLIT 250 Rauchrohranschlusselement RA 25/25/90°","ISOLIT 250 Elemento con raccordo 25/25/90°",114,1,"DN 250",null,300,"304019",null,null,345,"103644",45,300,45,"103644",345,45]
["103649",103649,null,"STK","ISOLIT 250 Russtürelement gasdicht RE 25","CHF",616,"ISOLIT",50,250,"J","ISOLIT 250 Porte de ramonage étanche 25","ISOLIT 250 Russtürelement gasdicht RE 25","ISOLIT 250 Elemento con portina ermetica ai gas 25",114,1,"DN 250",null,535,"307002",null,null,616,"103649",81,535,81,"103649",616,81]
["103663",103663,null,"STK","ISOLIT 200 Schleifung einzügig 20","CHF",807,"ISOLIT",90,0,"J","ISOLIT 200 déviation simple 20","ISOLIT 200 Schleifung einzügig 20","ISOLIT 200 Deviazione semplice 20",114,1,"DN 200",null,701,"315057",null,null,807,"103663",106,513,294,"103663",807,106]
["103664",103664,null,"STK","ISOLIT 250 Schleifung einzügig 25","CHF",914,"ISOLIT",110,0,"J","ISOLIT 250 déviation simple 25","ISOLIT 250 Schleifung einzügig 25","ISOLIT 250 Deviazione semplice 25",114,1,"DN 250",null,794,"315058",null,null,914,"103664",120,586,328,"103664",914,120]
["103672",103672,null,"STK","ISOLIT 300 Kombi-Mündungs-Manchette Inox 30","CHF",351,"ISOLIT",2.2999999999999998,0,"J","ISOLIT 300 Manchette combinée Inox 30","ISOLIT 300 Kombi-Mündungs-Manchette Inox 30","ISOLIT 300 Manicotto di sbocco 30",114,1,"DN 300",null,305,"913230",null,null,351,"103672",46,303,48,"103672",351,46]
["103677",103677,null,"STK","ISOLIT 160 Basten Standard Kupfer eckig  160mm","CHF",345,"ISOLIT",4.5999999999999996,0,"J","ISOLIT 160 Basten Standard cuivre carrée 160mm","ISOLIT 160 Basten Standard Kupfer eckig  160mm","ISOLIT 160 Basten standard rame rettangolare 160mm",114,1,"DN 160",null,325,"916100",null,null,345,"103677",20,323,22,"103677",345,20]
["103680",103680,null,"STK","ISOLIT 300 Basten Standard Kupfer eckig  300mm","CHF",545,"ISOLIT",8.6999999999999993,0,"J","ISOLIT 300 Basten Standard cuivre carrée 300mm","ISOLIT 300 Basten Standard Kupfer eckig  300mm","ISOLIT 300 Basten standard rame rettangolare 300mm",114,1,"DN 300",null,514,"916130",null,null,545,"103680",31,512,33,"103680",545,31]
["103682",103682,null,"STK","ISOLIT 200 Sairlift Inox eckig  200mm","CHF",398,"ISOLIT",4.3,0,"J","ISOLIT 200 Sairlift Inox carrée 200mm","ISOLIT 200 Sairlift Inox eckig  200mm","ISOLIT 200 Sairlift inox rettangolare 200mm",114,1,"DN 200",null,375,"908020",null,null,398,"103682",23,375,23,"103682",398,23]
["103687",103687,null,"STK","ISOLIT 200 Sairlift Kupfer eckig  200mm","CHF",413,"ISOLIT",4.5,0,"J","ISOLIT 250 Sairlift cuivre carrée 250mm","ISOLIT 200 Sairlift Kupfer eckig  200mm","ISOLIT 250 Sairlift rame rettangolare 250mm",114,1,"DN 200",null,389,"908520",null,null,413,"103687",24,389,24,"103687",413,24]
["103695",103695,null,"STK","CHZ 200 Anschlusskonus mit Doppelfutter DN200mm","CHF",281,"Schiedel CHEMINEE ZUG",50,0,"J","CHZ 200 Cône de racc., avec manchon double ","CHZ 200 Anschlusskonus mit Doppelfutter DN200mm","CHZ 200 Cono di raccordo et doppia parete DN200mm",112,1,"DN 200",null,244,"201002",null,null,281,"103695",37,244,37,"103695",281,37]
["103701",103701,null,"STK","CHZ 200 Keramik Fuss-Scheibe geschlossen","CHF",45,"Schiedel CHEMINEE ZUG",4,0,"J","CHZ 200 Disque de socle fermée","CHZ 200 Keramik Fuss-Scheibe geschlossen","CHZ 200 Disco di base ceramica senza foro",112,1,"DN 200",null,39,"201025",null,null,45,"103701",6,37,8,"103701",45,6]
["103706",103706,null,"STK","CHZ 180 Schnellbau-Fundament Set ","CHF",58,"Schiedel CHEMINEE ZUG",0,0,"J","CHZ 180 Fondation à montage rapide","CHZ 180 Schnellbau-Fundament Set ","CHZ 180 Set basamento per montaggio",112,1,"DN 180",null,50,"201031",null,null,58,"103706",8,50,8,"103706",58,8]
["103708",103708,null,"STK","CHZ 250 Schnellbau-Fundament Set ","CHF",121,"Schiedel CHEMINEE ZUG",0,0,"J","CHZ 250 Fondation à montage rapide","CHZ 250 Schnellbau-Fundament Set ","CHZ 250 Set basamento per montaggio",112,1,"DN 250",null,105,"201033",null,null,121,"103708",16,105,16,"103708",121,16]
["103711",103711,null,"STK","CHZ 250 Füllstein zu Schnellbaufundament L330mm","CHF",28,"Schiedel CHEMINEE ZUG",8,0,"J","CHZ 250 Fondation rapide, socle en supl. L330mm","CHZ 250 Füllstein zu Schnellbaufundament L330mm","CHZ 250  Basamento supplementare L330mm",112,1,"DN 250",null,24,"201016",null,null,28,"103711",4,24,4,"103711",28,4]
["103720",103720,null,"STK","CHZ Mantelstein EZ 360 x 360mm L330mm Ø180-200mm","CHF",23,"Schiedel CHEMINEE ZUG",25,0,"J","CHZ Elément manteau EZ 360 x 360mm L330mm Ø180-200mm","CHZ Mantelstein EZ 360 x 360mm L330mm Ø180-200mm","CHZ Mantello EZ 360 x 360mm L330mm Ø180-200mm",112,1,"DN 200",null,20,"200000",null,null,23,"103720",3,20,3,"103720",23,3]
["103722",103722,null,"STK","CHZ Mantelstein EZ  480 x 480mm L330mm Ø250mm","CHF",28,"Schiedel CHEMINEE ZUG",47,0,"J","CHZ Elément manteau EZ  480 x 480mm L330mm Ø250mm","CHZ Mantelstein EZ  480 x 480mm L330mm Ø250mm","CHZ Mantello EZ  480 x 480mm L330mm Ø250mm",112,1,"DN 250",null,24,"200002",null,null,28,"103722",4,24,4,"103722",28,4]
["103726",103726,null,"STK","CHZ Mantelstein rund ØA 550mm Øi 390mm L330mm","CHF",33,"Schiedel CHEMINEE ZUG",44,0,"J","CHZ Elément manteau ronde ØA 550mm Øi 390mm L330mm","CHZ Mantelstein rund ØA 550mm Øi 390mm L330mm","CHZ Mantello rotondo ØA 550mm Øi 390mm L330mm",112,1,"ZBH CHZ",null,28,"4011955",null,null,33,"103726",5,28,5,"103726",33,5]
["103735",103735,null,"STK","CHZ 180 Keramikrohr ØA 210mm  L330mm","CHF",23,"Schiedel CHEMINEE ZUG",6.4,330,"J","CHZ 180 Conduit réfractaire ØA 210mm  L330mm","CHZ 180 Keramikrohr ØA 210mm  L330mm","CHZ 180 Condotto refrattario ØA 210mm  L330mm",112,1,"DN 180",null,20,"205010",null,null,23,"103735",3,18,5,"103735",23,3]
["103744",103744,null,"STK","CHZ 160 Isoliermatte 2Stk. pro Rohr L330mm","CHF",13,"Schiedel CHEMINEE ZUG",1,0,"J","CHZ 160 Matelas isolant 2 pce. par conduit L330mm","CHZ 160 Isoliermatte 2Stk. pro Rohr L330mm","CHZ 160 Matera isolante 2 pz. per condotto L330mm",112,1,"DN 160",null,11,"210005",null,null,13,"103744",2,11,2,"103744",13,2]
["103747",103747,null,"STK","CHZ 250 Isoliermatte 2Stk. pro Rohr L330mm","CHF",15,"Schiedel CHEMINEE ZUG",1.4,0,"J","CHZ 250 Matelas isolant 2 pce. par conduit L330mm","CHZ 250 Isoliermatte 2Stk. pro Rohr L330mm","CHZ 250 Matera isolante 2 pz. per condotto L330mm",112,1,"DN 250",null,13,"210008",null,null,15,"103747",2,13,2,"103747",15,2]
["103748",103748,null,"STK","CHZ 300 Isoliermatte 2Stk. pro Rohr L330mm","CHF",18,"Schiedel CHEMINEE ZUG",1.6,0,"J","CHZ 300 Matelas isolant 2 pce. par conduit L330mm","CHZ 300 Isoliermatte 2Stk. pro Rohr L330mm","CHZ 300 Matera isolante 2 pz. per condotto L330mm",112,1,"DN 300",null,15,"210009",null,null,18,"103748",3,15,3,"103748",18,3]
["103754",103754,null,"STK","CHZ 300 Keramik T-Stück 90° für RA L660mm","CHF",348,"Schiedel CHEMINEE ZUG",42,665,"J","CHZ 300 Raccord de conduit de fumée 90° RA L660mm","CHZ 300 Keramik T-Stück 90° für RA L660mm","CHZ 300 Elemento con raccordo RA 90° L660mm",112,1,"DN 300",null,302,"204034",null,null,348,"103754",46,300,48,"103754",348,46]
["103757",103757,null,"STK","CHZ 250 Frontplattenset zu RA 90° aus Steinwolle","CHF",44,"Schiedel CHEMINEE ZUG",3,0,"J","CHZ 250 Panneau frontal pour RA 90°","CHZ 250 Frontplattenset zu RA 90° aus Steinwolle","CHZ 250 Lastra frontale per RA 90° ",112,1,"DN 250",null,38,"162010302","100383","4037494102459",44,"103757",6,38,6,"103757",44,6]
["103759",103759,null,"STK","CHZ 160 Keramik T-Stück 45° für RA L660mm","CHF",183,"Schiedel CHEMINEE ZUG",18,665,"J","CHZ 160 Raccord de conduit de fumée 45° L660mm","CHZ 160 Keramik T-Stück 45° für RA L660mm","CHZ 160 Elemento con raccordo RA 45° L660mm",112,1,"DN 160",null,159,"204216",null,null,183,"103759",24,157,26,"103759",183,24]
["103764",103764,null,"STK","CHZ 160 Keramik-Putztüranschluss PA L660mm","CHF",112,"Schiedel CHEMINEE ZUG",17,665,"J","CHZ 160 El. de racc. p. porte ramonage PA L660mm","CHZ 160 Keramik-Putztüranschluss PA L660mm","CHZ 160 Elemento PA per portina pulizia PA L660mm",112,1,"DN 160",null,97,"207026",null,null,112,"103764",15,95,17,"103764",112,15]
["103768",103768,null,"STK","CHZ 300 Keramik-Putztüranschluss PA L660mm","CHF",167,"Schiedel CHEMINEE ZUG",48.4,665,"J","CHZ 300 El. de racc. p. porte ramonage PA L660mm","CHZ 300 Keramik-Putztüranschluss PA L660mm","CHZ 300 Elemento PA per portina pulizia PA L660mm",112,1,"DN 300",null,145,"207007",null,null,167,"103768",22,143,24,"103768",167,22]
["103772",103772,null,"STK","CHZ 250 Kaminschleifung 0-35° EZ komplett ","CHF",1445,"Schiedel CHEMINEE ZUG",70,0,"J","CHZ 250 Déviation 0-35° EZ complet, 2 angles","CHZ 250 Kaminschleifung 0-35° EZ komplett ","CHZ 250 Deviazione 0-35° EZ completo",112,1,"DN 250",null,1256,"215045",null,null,1445,"103772",189,571,874,"103772",1445,189]
["103773",103773,null,"STK","CHZ 300 Kaminschleifung 0-35° EZ komplett ","CHF",1973,"Schiedel CHEMINEE ZUG",80,0,"J","CHZ 300 Déviation 0-35° EZ complet, 2 angles","CHZ 300 Kaminschleifung 0-35° EZ komplett ","CHZ 300 Deviazione 0-35° EZ completo",112,1,"DN 300",null,1715,"215046",null,null,1973,"103773",258,670,1303,"103773",1973,258]
["103779",103779,null,"STK","CHZ 160 Abdeckplatte Beton 520 x 520mm Loch ?160mm","CHF",135,"Schiedel CHEMINEE ZUG",26,0,"J","CHZ 160 Plaque de réc., bet 520 x 520mm trou 160mm","CHZ 160 Abdeckplatte Beton 520 x 520mm Loch ?160mm","CHZ 160 Lastra copertura 520x520 foro quadr. 160mm",112,1,"DN 160",null,117,"811000",null,null,135,"103779",18,117,18,"103779",135,18]
["103786",103786,null,"STK","CHZ Abdeckplatte Beton 600 x 600mm ohne Loch","CHF",158,"Schiedel CHEMINEE ZUG",46,0,"J","CHZ Plaque de réc., bet. 600 x 600mm sans trou","CHZ Abdeckplatte Beton 600 x 600mm ohne Loch","CHZ Lastra copertura  600 x 600mm senza foro",112,1,"DN 200",null,137,"811010",null,null,158,"103786",21,137,21,"103786",158,21]
["103789",103789,null,"STK","CHZ Postament 80 x 80mm  L250mm","CHF",33,"Schiedel CHEMINEE ZUG",3.6,0,"J","CHZ Piédestaux 80 x 80mm  L250mm","CHZ Postament 80 x 80mm  L250mm","CHZ Piedistallo 80 x 80mm  L250mm",112,1,"ZBH CHZ",null,28,"811171",null,null,33,"103789",5,28,5,"103789",33,5]
["103801",103801,null,"STK","CHZ 120 Doppelfutter lose L150mm","CHF",97,"Schiedel CHEMINEE ZUG",0.5,0,"J","CHZ 120 Doublemanchon lâche L150mm","CHZ 120 Doppelfutter lose L150mm","CHZ 120 Manicoto doppio parete L150mm",112,1,"ZBH CHZ",null,84,"912002",null,null,97,"103801",13,84,13,"103801",97,13]
["103808",103808,null,"STK","CHZ 160 Mündungsmanchette mit Tablett 320 x 320mm","CHF",145,"Schiedel CHEMINEE ZUG",0.75,0,"J","CHZ 160 Manschette combinée, ronde ","CHZ 160 Mündungsmanchette mit Tablett 320 x 320mm","CHZ 160 Manicotti di sbocco 320 x 320mm",112,1,"DN 160",null,126,"913010",null,null,145,"103808",19,124,21,"103808",145,19]
["103812",103812,null,"STK","CHZ 300 Mündungsmanchette mit Tablett 470 x 470mm","CHF",243,"Schiedel CHEMINEE ZUG",1.4,0,"J","CHZ 300 Manschette combinée, ronde ","CHZ 300 Mündungsmanchette mit Tablett 470 x 470mm","CHZ 300 Manicotti di sbocco 470 x 470mm",112,1,"DN 300",null,211,"913015",null,null,243,"103812",32,209,34,"103812",243,32]
["103820",103820,null,"STK","LBS 150 Ignis Protect 565 x 700 mm","CHF",452,"ganztec-LEICHTBAUSCHACHT",6,0,"J","LBS 150 Ignis Protect 565 x 700 mm","LBS 150 Ignis Protect 565 x 700 mm","LBS 150 Ignis Protect 565 x 700 mm",141,1,0,null,361,"271000150","101841","4037494157466",452,"103820",91,359,93,"103820",452,91]
["103821",103821,null,"STK","LBS 200 Ignis Protect 565 x 700 mm","CHF",538,"ganztec-LEICHTBAUSCHACHT",8.4,0,"J","LBS 200 Ignis Protect 565 x 700 mm","LBS 200 Ignis Protect 565 x 700 mm","LBS 200 Ignis Protect 565 x 700 mm",141,1,0,null,430,"271000200","101842","4037494157473",538,"103821",108,428,110,"103821",538,108]
["103825",103825,null,"STK","LBS 400 Ignis Protect 565 x 700 mm","CHF",873,"ganztec-LEICHTBAUSCHACHT",16.7,0,"J","LBS 400 Ignis Protect 565 x 700 mm","LBS 400 Ignis Protect 565 x 700 mm","LBS 400 Ignis Protect 565 x 700 mm",141,1,0,null,698,"271000400","101846","4037494157534",873,"103825",175,696,177,"103825",873,175]
["103828",103828,null,"STK","LBS 320 Leichtbauschacht i 320mm A 410mm L1000mm","CHF",189,"ganztec-LEICHTBAUSCHACHT",43.3,0,"J","LBS Gaine d'inst. légère □i 320mm □E 410mm L1000mm","LBS 320 Leichtbauschacht i 320mm A 410mm L1000mm","LBS 320 Elemento installatione leggermente  ",141,1,0,null,151,"LBS10035",null,null,189,"103828",38,149,40,"103828",189,38]
["103836",103836,null,"STK","ZBH 150 Verschlussbüchse weiss ØA 275mm","CHF",115,"ganztec-LEICHTBAUSCHACHT",1,0,"J","ZBH 150 Couvercle pour raccords, blanc ØA 275mm","ZBH 150 Verschlussbüchse weiss ØA 275mm","ZBH 150 Coperchio per raccordo biancoØA 275mm",141,1,"ZBH ABS",null,100,"913415",null,null,115,"103836",15,100,15,"103836",115,15]
["103838",103838,null,"STK","ZBH 180 Verschlussbüchse weiss ØA 275mm","CHF",123.1,"ganztec-LEICHTBAUSCHACHT",1,0,"J","ZBH 180 Couvercle pour raccords, blanc ØA 275mm","ZBH 180 Verschlussbüchse weiss ØA 275mm","ZBH 180 Coperchio per raccordo biancoØA 275mm",141,1,"ZBH ABS",null,107,"913418",null,null,123.1,"103838",16.099999999999994,107,16.099999999999994,"103838",123.1,16.099999999999994]
["103841",103841,null,"STK","ZBH Kondensatkanister 20Liter","CHF",44.9,"ganztec-LEICHTBAUSCHACHT",1.25,0,"J","ZBH Récipiant de condensat, 20 litre","ZBH Kondensatkanister 20Liter","ZBH Bomboletta per condensa  20 litero",141,1,"ZBH ABS",null,39,"911012",null,null,44.9,"103841",5.8999999999999986,39,5.8999999999999986,"103841",44.9,5.8999999999999986]
["103847",103847,null,"STK","ZBH Diamantblatt für Trennscheibe  Ø230mm","CHF",322,"ganztec-LEICHTBAUSCHACHT",0.6,0,"N","ZBH Disque diamant Ø230mm","ZBH Diamantblatt für Trennscheibe  Ø230mm","ZBHDisque diamanteper della lama  Ø230mm",141,1,"ZBH ABS",null,280,"800301",null,null,322,"103847",42,280,42,"103847",322,42]
["103851",103851,null,"STK","ABS Thermo-Fussplatte EZ 480 x 480mm","CHF",149,"Schiedel ABSOLUT",4.3,0,"J","ABS Plaque de base thermo EZ 480 x 480mm","ABS Thermo-Fussplatte EZ 480 x 480mm","ABS Lastra die base thermo EZ 480 x 480mm",111,1,0,null,129,"100514848","100102","4037494824467",149,"103851",20,129,20,"103851",149,20]
["103852",103852,null,"STK","ABS Thermo-Fussplatte EZTL 360 x 500mm","CHF",160,"Schiedel ABSOLUT",3.1,0,"J","ABS Plaque de base thermo EZTL 360 x 560mm","ABS Thermo-Fussplatte EZTL 360 x 500mm","ABS Lastra die base thermo EZTL 360 x 560mm",111,1,0,null,139,"100513650","100095","4037494806746",160,"103852",21,139,21,"103852",160,21]
["103856",103856,null,"STK","ABS Thermo-Fussplatte DZTL 360 x 850mm","CHF",234,"Schiedel ABSOLUT",4.3,0,"J","ABS Plaque de base thermo DZTL 360 x 850mm","ABS Thermo-Fussplatte DZTL 360 x 850mm","ABS Lastra die base thermo DZTL 360 x 850mm",111,1,0,null,203,"100513683","100097","4037494806760",234,"103856",31,203,31,"103856",234,31]
["103861",103861,null,"STK","ABS 250 Grundpaket","CHF",736,"Schiedel ABSOLUT",30,1000,"J","ABS 250 Paquet de base pour pied préfabriqué","ABS 250 Grundpaket","ABS 250 Kit per Basamento prefabbricado",111,1,"DN 250",null,640,"204011025","100133","4037494183403",736,"103861",96,638,98,"103861",736,96]
["103864",103864,null,"STK","ABS 180 Fertigfuss EZTL 120-180mm  L1070mm ","CHF",734,"Schiedel ABSOLUT",118,1070,"J","ABS Pied préfabriqué EZTL Ø120-180mm L1070mm","ABS 180 Fertigfuss EZTL 120-180mm  L1070mm ","ABS Basamento perfabbric. EZTL Ø120-180mm L1070mm",111,1,"DN 180",null,638,"200010018","102056","4037494187210",734,"103864",96,638,96,"103864",734,96]
["103866",103866,null,"STK","ABS 180 Fertigfuss DZ 2 x Ø120-180mm L1070mm","CHF",1472,"Schiedel ABSOLUT",172,1070,"J","ABS Pied préfabriqué DZ 2 x Ø120-180mm L1070mm","ABS 180 Fertigfuss DZ 2 x Ø120-180mm L1070mm","ABS Basamento perfabbric. DZ 2xØ120-180mm L1070mm",111,1,"DN 180",null,1280,"200001818","102054","4037494187197",1472,"103866",192,1280,192,"103866",1472,192]
["103874",103874,null,"STK","ABS Sockelplatte aus Beton EZ 550 x 550mm","CHF",197,"Schiedel ABSOLUT",48.7,0,"J","ABS Plaque de socle en beton EZ 550 x 550mm","ABS Sockelplatte aus Beton EZ 550 x 550mm","ABS Piastra di base cemento EZ 550 x 550mm",111,1,0,null,171,"210005555","100160","4037494109328",197,"103874",26,171,26,"103874",197,26]
["103879",103879,null,"STK","ABS Sockelplatte aus Beton EZTL 550 x 710mm","CHF",151,"Schiedel ABSOLUT",61.2,0,"J","ABS Plaque de socle en beton EZTL 550 x 710mm","ABS Sockelplatte aus Beton EZTL 550 x 710mm","ABS Piastra di base cemento EZTL 550 x 710mm",111,1,0,null,131,"210015571","100161","4037494109342",151,"103879",20,131,20,"103879",151,20]
["103891",103891,null,"STK","ABS 180 Fertigfusspaket ","CHF",311,"Schiedel ABSOLUT",6.9,0,"J","ABS 180 Paquet de pied préfabriqué","ABS 180 Fertigfusspaket ","ABS 180 Kit per basamanto prefabbricado",111,1,"DN 180",null,270,"203040018","100120","4037494153833",311,"103891",41,268,43,"103891",311,41]
["103892",103892,null,"STK","ABS 200 Fertigfusspaket ","CHF",311,"Schiedel ABSOLUT",6.1,0,"J","ABS 200 Paquet de pied préfabriqué","ABS 200 Fertigfusspaket ","ABS 200 Kit per basamanto prefabbricado",111,1,"DN 200",null,270,"203040020","100121","4037494153840",311,"103892",41,268,43,"103892",311,41]
["103901",103901,null,"STK","ABS 250 Anschlusskonus EZ mit Doppelfutter DN250mm","CHF",365,"Schiedel ABSOLUT",66,0,"J","ABS 250 Cône de racc.EZ avec doublemanchon DN250mm","ABS 250 Anschlusskonus EZ mit Doppelfutter DN250mm","ABS 250 cono raccordo EZ et doppia parete DN250mm",111,1,"DN 250",null,317,"1866025",null,null,365,"103901",48,317,48,"103901",365,48]
["103906",103906,null,"STK","ABS 180 Adapterring von 180mm auf 160mm L90mm","CHF",41,"Schiedel ABSOLUT",2,0,"J","ABS 180 Bague d'adapt. de 180mm au 160mm L90mm","ABS 180 Adapterring von 180mm auf 160mm L90mm","ABS 180 Anello di adattamento 180mm su 160mm L90mm",111,1,"DN 180",null,35,"260101816","102217","4037494092880",41,"103906",6,33,8,"103906",41,6]
["103910",103910,null,"STK","ABS 250 Adapterring von 250mm auf 250mm L90mm","CHF",79,"Schiedel ABSOLUT",2.8,0,"J","ABS 250 Bague d'adapt. de 250mm au 250mm L90mm","ABS 250 Adapterring von 250mm auf 250mm L90mm","ABS 250 Anello di adattamento 250mm su 250mm L90mm",111,1,"DN 250",null,68,"260102525",null,null,79,"103910",11,66,13,"103910",79,11]
["103913",103913,null,"STK","ABS Mantelstein EZ 380 x 380mm L330mm","CHF",33,"Schiedel ABSOLUT",22.61,0,"J","ABS Manteau composite EZ 380 x 380mm L330mm","ABS Mantelstein EZ 380 x 380mm L330mm","ABS Mantello composito EZ 380 x 380mm L330mm",111,1,0,null,28,"1873838","100027","4037494068960",33,"103913",5,28,5,"103913",33,5]
["103916",103916,null,"STK","ABS Mantelstein EZ 670 x 670mm L330mm","CHF",186,"Schiedel ABSOLUT",66.5,0,"J","ABS Manteau composite EZ 670 x 670mm L330mm","ABS Mantelstein EZ 670 x 670mm L330mm","ABS Mantello composito EZ 670 x 670mm L330mm",111,1,0,null,161,"1876767","100035","4049723001303",186,"103916",25,161,25,"103916",186,25]
["103921",103921,null,"STK","ABS Mantelstein EZTL 380 x 540mm L330mm","CHF",44,"Schiedel ABSOLUT",32.979999999999997,0,"J","ABS Manteau composite EZTL 380 x 540mm L330mm","ABS Mantelstein EZTL 380 x 540mm L330mm","ABS Mantello composito EZTL 380 x 540mm L330mm",111,1,0,null,38,"1873854","100028","4037494141465",44,"103921",6,38,6,"103921",44,6]
["103925",103925,null,"STK","ABS Mantelstein DZ 360 x 650mm L330mm","CHF",51,"Schiedel ABSOLUT",36.43,0,"J","ABS Manteau composite DZ 360 x 650mm L330mm","ABS Mantelstein DZ 360 x 650mm L330mm","ABS Mantello composito DZ 360 x 650mm L330mm",111,1,0,null,44,"1873665","100025","4037494055076",51,"103925",7,44,7,"103925",51,7]
["103926",103926,null,"STK","ABS Mantelstein DZ 380 x 710mm L330mm","CHF",56,"Schiedel ABSOLUT",40.54,0,"J","ABS Manteau composite DZ 380 x 710mm L330mm","ABS Mantelstein DZ 380 x 710mm L330mm","ABS Mantello composito DZ 380 x 710mm L330mm",111,1,0,null,48,"1873871","100029","4037494068984",56,"103926",8,48,8,"103926",56,8]
["103930",103930,null,"STK","ABS Mantelstein DZTL 380 x 880mm 2 x 200mm L330mm ","CHF",60,"Schiedel ABSOLUT",45,0,"J","ABS Manteau comp. DZTL 380 x 880mm 2x200mm L330mm ","ABS Mantelstein DZTL 380 x 880mm 2 x 200mm L330mm ","ABS Mantello composito DZTL 380 x 880mm 2 x 200mm L330mm ",111,1,0,null,52,"1883888",null,null,60,"103930",8,52,8,"103930",60,8]
["103934",103934,null,"STK","ABS Thermo-Trennstein EZ TL 360 x 500mm L330mm","CHF",222,"Schiedel ABSOLUT",29.3,0,"J","ABS Elément de séparation EZ TL 360 x 500mm L330mm","ABS Thermo-Trennstein EZ TL 360 x 500mm L330mm","ABS Thermo-Trennstein EZ TL 360 x 500mm L330mm",111,1,0,null,193,"100503650","100085","4037494297698",222,"103934",29,193,29,"103934",222,29]
["103940",103940,null,"STK","ABS Thermo-Trennstein DZTL 380 x 880mm L330mm","CHF",370,"Schiedel ABSOLUT",40,0,"J","ABS Elément de séparation DZTL 380 x 880mm L330mm","ABS Thermo-Trennstein DZTL 380 x 880mm L330mm","ABS Thermo-Trennstein DZTL 380 x 880mm L330mm",111,1,0,null,321,"100503888",null,null,370,"103940",49,321,49,"103940",370,49]
["103943",103943,null,"STK","ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","CHF",14,"Schiedel ABSOLUT",0,0,"J","ABS Set de distanceurs pour 2 conduit Ø140,","ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","ABS set di distanzatori per 2pz tubo ceramica Ø140",111,1,0,null,12,"7196020","108246","4037494065907",14,"103943",2,12,2,"103943",14,2]
["103947",103947,null,"STK","ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","CHF",113,"Schiedel ABSOLUT",10.7,1330,"J","ABS 160 Conduit profilé L1330mm","ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","ABS 160 Condotto profilato L1330mm",111,1,"DN 160",null,98,"2080016","100039","4037494057414",113,"103947",15,96,17,"103947",113,15]
["103957",103957,null,"STK","ABS 400 Profilkeramik-Rohr mit Muffe L660mm","CHF",158,"Schiedel ABSOLUT",20.5,665,"J","ABS 400 Conduit profilé L660mm","ABS 400 Profilkeramik-Rohr mit Muffe L660mm","ABS 400 Condotto profilato L660mm",111,1,"DN 400",null,137,"2090040","100049","4049723002058",158,"103957",21,135,23,"103957",158,21]
["103965",103965,null,"STK","ABS 160 Putztür-Anschlusspaket ","CHF",428,"Schiedel ABSOLUT",17.64,1330,"J","ABS 160 Paquet de raccordement PA","ABS 160 Putztür-Anschlusspaket ","ABS 160 Kit per raccordo PA",111,1,"DN 160",null,372,"235110016","100166","4037494183427",428,"103965",56,370,58,"103965",428,56]
[{"$f":"B3084&\"\"","v":"103966"},103966,null,"STK",{"$f":"IF($E$200=2,L3084,IF($E$200=3,N3084,M3084))","v":"ABS 180 Putztür-Anschlusspaket "},"CHF",{"$f":"IF($L$190=1,W3084,S3084)","v":448},"Schiedel ABSOLUT",19.309999999999999,1330,"J","ABS 180 Paquet de raccordement PA","ABS 180 Putztür-Anschlusspaket ","ABS 180 Kit per raccordo PA",111,1,"DN 180",null,389,"235110018","100167","4037494183434",448,"103966",59,387,61,"103966",448,59]
["103970",103970,null,"STK","ABS 400 Putztür-Anschlusspaket ","CHF",731,"Schiedel ABSOLUT",21,665,"J","ABS 400 Paquet de raccordement PA","ABS 400 Putztür-Anschlusspaket ","ABS 400 Kit per raccordo PA",111,1,"DN 400",null,635,"235110040",null,null,731,"103970",96,633,98,"103970",731,96]
["103985",103985,null,"STK","ABS 250 Rauchrohr-Anschlusspaket 90° RA  ","CHF",490,"Schiedel ABSOLUT",16.55,665,"J","ABS 250 Paquet de raccordement 90° RA  ","ABS 250 Rauchrohr-Anschlusspaket 90° RA  ","ABS 250 Kit per raccordo  90° RA  ",111,1,"DN 250",null,426,"2110025","100055","4037494173442",490,"103985",64,424,66,"103985",490,64]
["103993",103993,null,"STK","ABS 140 Rauchrohr-Anschlusspaket 45° RA  ","CHF",355,"Schiedel ABSOLUT",13.15,1330,"J","ABS 140 Paquet de raccordement RA 45° RA  ","ABS 140 Rauchrohr-Anschlusspaket 45° RA  ","ABS 140 Kit per raccordo  45° RA  ",111,1,"DN 140",null,321,"2114514","100056","4037494074008",355,"103993",34,349,6,"103993",355,34]
["103995",103995,null,"STK","ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","CHF",404,"Schiedel ABSOLUT",17.2,1330,"J","ABS 180 Paquet de raccordement RA 45° RA  ","ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","ABS 180 Kit per raccordo  45° RA  ",111,1,"DN 180",null,351,"2114518","100058","4037494074022",404,"103995",53,349,55,"103995",404,53]
["104002",104002,null,"STK","ABS 200 Rauchrohranschluss Stutzen-Set 90° Ø200mm","CHF",212,"Schiedel ABSOLUT",4.7,0,"J","ABS Set de manchon RA 90° Ø200/200mm","ABS 200 Rauchrohranschluss Stutzen-Set 90° Ø200mm","ABS Rauchrohranschluss Stutzen-Set 90° Ø200/200mm",111,1,"DN 200",null,184,"2192020","100071","4037494136225",212,"104002",28,182,30,"104002",212,28]
["104006",104006,null,"STK","ABS 160 Rauchrohranschluss Stutzen-Set 45°","CHF",199,"Schiedel ABSOLUT",5.09,0,"J","ABS Set de manchon RA 45° Ø160mm","ABS 160 Rauchrohranschluss Stutzen-Set 45°","ABS Rauchrohranschluss Stutzen-Set 45° Ø160mm",111,1,"DN 160",null,173,"2194516","100074","4037494136195",199,"104006",26,171,28,"104006",199,26]
["104010",104010,null,"STK","ABS 160 Doppelfutter zu Rauchrohranschluss Ø80mm","CHF",124,"Schiedel ABSOLUT",1,0,"J","ABS Manchon double pour raccordement RA Ø160/80mm","ABS 160 Doppelfutter zu Rauchrohranschluss Ø80mm","ABS Doppelfutter zu Rauchrohranschluss Ø160/80mm",111,1,"DN 160",null,107,"9141608",null,null,124,"104010",17,107,17,"104010",124,17]
["104011",104011,null,"STK","ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","CHF",136,"Schiedel ABSOLUT",1,0,"J","ABS Manchon double pour raccordement RA Ø160/100mm","ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","ABS Doppelfutter zu Rauchrohranschluss Ø160/100mm",111,1,"DN 160",null,118,"9141610",null,null,136,"104011",18,118,18,"104011",136,18]
["104015",104015,null,"STK","ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm","CHF",160,"Schiedel ABSOLUT",1,0,"J","ABS Manchon double pour raccordement RA Ø180/120mm","ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm","ABS Doppelfutter zu Rauchrohranschluss Ø180/120mm",111,1,"DN 180",null,139,"9141812",null,null,160,"104015",21,139,21,"104015",160,21]
["104019",104019,null,"STK","ABS 200 Doppelfutter zu Rauchrohranschluss Ø100mm","CHF",160,"Schiedel ABSOLUT",1,0,"J","ABS Manchon double pour raccordement RA Ø200/100mm","ABS 200 Doppelfutter zu Rauchrohranschluss Ø100mm","ABS Doppelfutter zu Rauchrohranschluss Ø200/100mm",111,1,"DN 200",null,139,"9142010",null,null,160,"104019",21,139,21,"104019",160,21]
["104024",104024,null,"STK","ABS 200 Doppelfutter zu Rauchrohranschluss Ø200mm","CHF",222,"Schiedel ABSOLUT",1,0,"J","ABS Manchon double pour raccordement RA Ø200/200mm","ABS 200 Doppelfutter zu Rauchrohranschluss Ø200mm","ABS Doppelfutter zu Rauchrohranschluss Ø200/200mm",111,1,"DN 200",null,193,"9142020",null,null,222,"104024",29,193,29,"104024",222,29]
["104026",104026,null,"STK","ABS 250 Doppelfutter zu Rauchrohranschluss Ø200mm","CHF",222,"Schiedel ABSOLUT",1.2,0,"J","ABS Manchon double pour raccordement RA Ø250/200mm","ABS 250 Doppelfutter zu Rauchrohranschluss Ø200mm","ABS Doppelfutter zu Rauchrohranschluss Ø250/200mm",111,1,"DN 250",null,193,"9142520",null,null,222,"104026",29,193,29,"104026",222,29]
["104029",104029,null,"STK","ABS 160 Kondensatfalle zu RA 45° Ø130mm ","CHF",322,"Schiedel ABSOLUT",2.2000000000000002,0,"J","ABS collecteur de condensat p. RA 45° Ø160/130mm","ABS 160 Kondensatfalle zu RA 45° Ø130mm ","ABS Adattore per RA 45° per condensa Ø160/130mm ",111,1,"DN 160",null,280,"21751613",null,null,322,"104029",42,280,42,"104029",322,42]
["104034",104034,null,"STK","ABS 180 Kondensatfalle zu RA 45° Ø160mm","CHF",347,"Schiedel ABSOLUT",2.2000000000000002,0,"J","ABS collecteur de condensat p. RA 45° Ø180/160mm","ABS 180 Kondensatfalle zu RA 45° Ø160mm","ABS Adattore per RA 45° per condensa Ø180/160mm",111,1,"DN 180",null,301,"21751816",null,null,347,"104034",46,301,46,"104034",347,46]
["104038",104038,null,"STK","ABS 200 Kondensatfalle zu RA 45° Ø160mm","CHF",365,"Schiedel ABSOLUT",2.2000000000000002,0,"J","ABS collecteur de condensat p. RA 45° Ø200/160mm","ABS 200 Kondensatfalle zu RA 45° Ø160mm","ABS Adattore per RA 45° per condensa Ø200/160mm",111,1,"DN 200",null,317,"21752016",null,null,365,"104038",48,317,48,"104038",365,48]
["104039",104039,null,"STK","ABS 200 Kondensatfalle zu RA 45° Ø180mm ","CHF",365,"Schiedel ABSOLUT",2.2000000000000002,0,"J","ABS collecteur de condensat p. RA 45° Ø200/180mm","ABS 200 Kondensatfalle zu RA 45° Ø180mm ","ABS Adattore per RA 45° per condensa Ø200/180mm ",111,1,"DN 200",null,317,"21752018",null,null,365,"104039",48,317,48,"104039",365,48]
["104043",104043,null,"STK","ABS 250 Kondensatfalle zu RA 45° Ø250mm","CHF",426,"Schiedel ABSOLUT",2.5,0,"J","ABS collecteur de condensat p. RA 45° Ø250/250mm","ABS 250 Kondensatfalle zu RA 45° Ø250mm","ABS Adattore per RA 45° per condensa Ø250/250mm",111,1,"DN 250",null,370,"21752525",null,null,426,"104043",56,370,56,"104043",426,56]
[{"$f":"B3148&\"\"","v":"104066"},104066,null,"STK",{"$f":"IF($E$200=2,L3148,IF($E$200=3,N3148,M3148))","v":"ABS 200 Schleifung EZ 5° auf Bestellung"},"CHF",{"$f":"IF($L$190=1,W3148,S3148)","v":1134},"Schiedel ABSOLUT",25,0,"J","ABS 200 Déviation EZ 5° sur commande, 2 angles","ABS 200 Schleifung EZ 5° auf Bestellung","ABS 200 Deviazione EZ 5° su ordinazione",111,1,"DN 200",null,986,"1860020",null,null,1134,"104066",148,748,386,"104066",1134,148]
["104084",104084,null,"STK","ABS 200 Abstandhalter offen zu Schleifung","CHF",38,"Schiedel ABSOLUT",0.1,0,"J","ABS 200 Distanceurs  ouvrir pour deviation","ABS 200 Abstandhalter offen zu Schleifung","ABS 200 Distanzatori aprire per deviazione",111,1,"DN 200",null,33,"256000520","900000388","4037494102565",38,"104084",5,33,5,"104084",38,5]
["104144",104144,null,"STK","ABS Handyplatte EZ Faserzement 360 x 360mm","CHF",106,"Schiedel ABSOLUT",14.4,0,"J","ABS Plaque Handy EZ en fibrocementt 360 x 360mm","ABS Handyplatte EZ Faserzement 360 x 360mm","ABS Lastra Handy EZ fibrocemento 360 x 360mm",111,1,0,null,92,"373636",null,null,106,"104144",14,92,14,"104144",106,14]
["104147",104147,null,"STK","ABS Handyplatte EZ Faserzement 550 x 550mm","CHF",156,"Schiedel ABSOLUT",22,0,"J","ABS Plaque Handy EZ en fibrocement 550 x 550mm","ABS Handyplatte EZ Faserzement 550 x 550mm","ABS Lastra Handy EZ fibrocemento 550 x 550mm",111,1,0,null,135,"38225555",null,null,156,"104147",21,135,21,"104147",156,21]
["104152",104152,null,"STK","ABS Handyplatte DZ Faserzement 380 x 710mm  ","CHF",180,"Schiedel ABSOLUT",21.6,0,"J","ABS Plaque Handy DZ en fibrocement 380 x 710mm  ","ABS Handyplatte DZ Faserzement 380 x 710mm  ","ABS Lastra Handy DZ fibrocemento 380 x 710mm  ",111,1,0,null,156,"373871",null,null,180,"104152",24,156,24,"104152",180,24]
["104153",104153,null,"STK","ABS Handyplatte DZTL Faserzement 380 x 880mm","CHF",211,"Schiedel ABSOLUT",24.6,0,"J","ABS Plaque Handy DZTL en fibrocement 380 x 880mm","ABS Handyplatte DZTL Faserzement 380 x 880mm","ABS Lastra Handy DZTL fibrocemento 380 x 880mm",111,1,0,null,183,"373888",null,null,211,"104153",28,183,28,"104153",211,28]
["104164",104164,null,"STK","ABS Abdeckung zu Handyplatte EZTL 120 x 280mm","CHF",51,"Schiedel ABSOLUT",0.5,0,"J","ABS  Recouvrement p. plaque Handy EZTL 120 x 280mm","ABS Abdeckung zu Handyplatte EZTL 120 x 280mm","ABS Copertura per lastra Handy EZTL 120 x 280mm",111,1,0,null,44,"354251228",null,null,51,"104164",7,44,7,"104164",51,7]
["104169",104169,null,"STK","ABS Zulufthaube zu Faserzementpl. DZTL 140- 200mm","CHF",106,"Schiedel ABSOLUT",0.7,0,"J","ABS Hotte d'entrée d'air pour Handy fibrocement ","ABS Zulufthaube zu Faserzementpl. DZTL 140- 200mm","ABS perlufthaube per fibrocementopl. DZTL 140- 200mm",111,1,0,null,92,"354230002","100225","4037494143421",106,"104169",14,92,14,"104169",106,14]
["104174",104174,null,"STK","ABS Handyplatte EZ Inox 670 x 670mm ","CHF",241,"Schiedel ABSOLUT",5.0999999999999996,0,"J","ABS Plaque Handy EZ Inox 670 x 670mm ","ABS Handyplatte EZ Inox 670 x 670mm ","ABS Lastra Handy EZ Inox 670 x 670mm ",111,1,0,null,209,"38606767",null,null,241,"104174",32,209,32,"104174",241,32]
["104177",104177,null,"STK","ABS Handyplatte EZTL Inox 380 x 540mm  ","CHF",217,"Schiedel ABSOLUT",4.3,0,"J","ABS Plaque Handy EZTL Inox 380 x 540mm  ","ABS Handyplatte EZTL Inox 380 x 540mm  ","ABS Lastra Handy EZTL Inox 380 x 540mm  ",111,1,0,null,188,"38673854",null,null,217,"104177",29,188,29,"104177",217,29]
["104179",104179,null,"STK","ABS Handyplatte EZTL Inox 550 x 710mm ","CHF",255,"Schiedel ABSOLUT",5.78,0,"J","ABS Plaque Handy EZTL Inox 550 x 710mm ","ABS Handyplatte EZTL Inox 550 x 710mm ","ABS Lastra Handy EZTL Inox 550 x 710mm ",111,1,0,null,221,"38675571",null,null,255,"104179",34,221,34,"104179",255,34]
["104185",104185,null,"STK","ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","CHF",51,"Schiedel ABSOLUT",1,0,"J","ABS HEB-Set de fixation pour plaque Handy TL Inox","ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","ABS HEB-Set lastra Handy TL inox con viti lunghe",111,1,0,null,44,"356500002","102321","4049723000627",51,"104185",7,44,7,"104185",51,7]
["104188",104188,null,"STK","ABS Handyplatte EZTL Kupfer 480 x 620mm","CHF",358,"Schiedel ABSOLUT",5,0,"J","ABS Plaque Handy EZTL cuivre 480 x 620mm","ABS Handyplatte EZTL Kupfer 480 x 620mm","ABS Lastra Handy EZTL Kupfer 480 x 620mm",111,1,0,null,311,"038674862K",null,null,358,"104188",47,311,47,"104188",358,47]
["104190",104190,null,"STK","ABS Thermodichtset EZ 360x360mm und 380x380mm","CHF",309,"Schiedel ABSOLUT",2,0,"J","ABS Set d'etachéité Thermo ","ABS Thermodichtset EZ 360x360mm und 380x380mm","ABS Set hermetico thermo EZ 360x360mm und 380x380mm",111,1,"DN 80",null,268,"270300901",null,null,309,"104190",41,268,41,"104190",309,41]
["104193",104193,null,"STK","ABS Thermodichtset DZTL 360x830mm und 380x880mm","CHF",309,"Schiedel ABSOLUT",2,0,"J","ABS Set d'etachéité Thermo ","ABS Thermodichtset DZTL 360x830mm und 380x880mm","ABS Set hermetico thermo DZTL 360x830mm und 380x880mm",111,1,"DN 80",null,268,"270300923",null,null,309,"104193",41,268,41,"104193",309,41]
["104204",104204,null,"STK","ABS 140 Abströmkonus verkupfert","CHF",161,"Schiedel ABSOLUT",0.70599999999999996,0,"J","ABS 140 Cône de finition cuivrée avec grille d'air","ABS 140 Abströmkonus verkupfert","ABS 140 Cono per sbocco verkupfert",111,1,"DN 140",null,140,0,null,null,161,"104204",21,140,21,"104204",161,21]
["104208",104208,null,"STK","ABS 250 Abströmkonus verkupfert","CHF",258,"Schiedel ABSOLUT",1.06,0,"J","ABS 250 Cône de finition cuivrée","ABS 250 Abströmkonus verkupfert","ABS 250 Cono per sbocco verkupfert",111,1,"DN 250",null,224,0,null,null,258,"104208",34,224,34,"104208",258,34]
["104213",104213,null,"STK","ABS 200 Basten Standard Inox","CHF",361,"Schiedel ABSOLUT",4.7,0,"J","ABS 200 Basten Standard Inox","ABS 200 Basten Standard Inox","ABS 200 Cono per sbocco rame",111,1,"DN 200",null,340,"916070",null,null,361,"104213",21,338,23,"104213",361,21]
["104216",104216,null,"STK","ABS 400 Basten Standard Inox","CHF",596,"Schiedel ABSOLUT",7.5,0,"J","ABS 400 Basten Standard Inox","ABS 400 Basten Standard Inox","ABS 400 Cono per sbocco rame",111,1,"DN 400",null,562,"916095",null,null,596,"104216",34,560,36,"104216",596,34]
["104218",104218,null,"STK","ABS 180 Basten Standard Kupfer","CHF",362,"Schiedel ABSOLUT",4.3,0,"J","ABS 180 Basten Standard cuivre","ABS 180 Basten Standard Kupfer","ABS 180 Basten Standard rame",111,1,"DN 180",null,341,"916160",null,null,362,"104218",21,339,23,"104218",362,21]
["104223",104223,null,"STK","ABS 160 Sairlift Inox","CHF",374,"Schiedel ABSOLUT",3.9,0,"J","ABS 160 Sairlift Inox","ABS 160 Sairlift Inox","ABS 160 Sairlift inox",111,1,"DN 160",null,325,"909116",null,null,374,"104223",49,325,49,"104223",374,49]
["104227",104227,null,"STK","ABS 300 Sairlift Inox","CHF",610,"Schiedel ABSOLUT",7.1,0,"J","ABS 300 Sairlift Inox","ABS 300 Sairlift Inox","ABS 300 Sairlift inox",111,1,"DN 300",null,530,"909130",null,null,610,"104227",80,530,80,"104227",610,80]
["104228",104228,null,"STK","ABS 160 Sairlift Kupfer","CHF",397,"Schiedel ABSOLUT",4.0999999999999996,0,"J","ABS 160 Sairlift cuivre","ABS 160 Sairlift Kupfer","ABS 160 Sairlift rame",111,1,"DN 160",null,345,"909216",null,null,397,"104228",52,345,52,"104228",397,52]
["104232",104232,null,"STK","ABS 300 Sairlift Kupfer","CHF",633,"Schiedel ABSOLUT",6,0,"J","ABS 300 Sairlift cuivre","ABS 300 Sairlift Kupfer","ABS 300 Sairlift rame",111,1,"DN 300",null,550,"909230",null,null,633,"104232",83,550,83,"104232",633,83]
["104243",104243,null,"STK","ABS Dichtset zu Putztüre Typ 3","CHF",27,"Schiedel ABSOLUT",0.2,0,"J","ABS Set d'étanchéité pour porte ramonage Typ 3","ABS Dichtset zu Putztüre Typ 3","ABS Set hermetico per portina tipo 3",111,1,"ZBH ABS",null,23,"270301002","100216","4037494181737",27,"104243",4,23,4,"104243",27,4]
["104251",104251,null,"STK","ABS Armierungs-Set 2 x 4000mm für Mantelsteine","CHF",209,"Schiedel ABSOLUT",5,0,"J","ABS Set d'armature 2 x 4000mm, incl. mortier 5 kg","ABS Armierungs-Set 2 x 4000mm für Mantelsteine","ABS Set d'armatura 2 x 4000mm per Mantello",111,1,"ZBH ABS",null,181,"6447503",null,null,209,"104251",28,181,28,"104251",209,28]
["104256",104256,null,"STK","ABS Kaminhalterung Standard","CHF",303,"Schiedel ABSOLUT",16.5,0,"J","ABS Système de fixation entre ou sur les chevrons","ABS Kaminhalterung Standard","ABS Kaminhalterung Standard",111,1,"ZBH ABS",null,263,"354520003","100514","4037494175088",303,"104256",40,263,40,"104256",303,40]
["104261",104261,null,"STK","Euro Paletten im Austausch","CHF",0,null,15,0,"N","Palettes échanchable","Euro Paletten im Austausch","Palette di scambio",null,null,0,null,0,"710004",null,null,null,"104261",0,0,0,"104261",null,0]
["104268",104268,null,"STK","ABS 180 Steckadapter ","CHF",173,"Schiedel ABSOLUT",0.33800000000000002,0,"J","ABS 200 Adapteur emboîtable, pour mazout et gaz ","ABS 180 Steckadapter ","ABS 220 Adattore a innestro",111,1,"DN 180",null,150,"STA180","100017","4037494055045",173,"104268",23,150,23,"104268",173,23]
["104270",104270,null,"STK","ABS 220 Steckadapter ","CHF",198,"Schiedel ABSOLUT",0.34599999999999997,0,"J","ABS 250 Adapteur emboîtable, pour mazout et gaz ","ABS 220 Steckadapter ","ABS 140 Set per pocchetta PA",111,1,"DN 250",null,172,"STA220","100553","4037494012819",198,"104270",26,172,26,"104270",198,26]
["104273",104273,null,"STK","ABS 160 Putztüranschluss Stutzen Set","CHF",325,"Schiedel ABSOLUT",4.9000000000000004,0,"J","ABS 180 Set de manchon PA","ABS 160 Putztüranschluss Stutzen Set","ABS 200 Set per pocchetta PA",111,1,"DN 160",null,282,"241401016","100186","4037494183472",325,"104273",43,280,45,"104273",325,43]
["104474",104474,null,"STK","Kombi-Mündungs-Manchette 18/58","CHF",168,"Schiedel CHEMINEE ZUG",1.3,0,"J","Manchette combinée 18/58","Kombi-Mündungs-Manchette 18/58","Manicotto di sbocco 18/58",112,1,"DN 180",null,146,"913118",null,null,168,"104474",22,144,24,"104474",168,22]
["104490",104490,null,"STK","TS120 Kesselanschluss DN60/80","CHF",52.5,"TECHNOSTAR 120",0.02,0,"J","TS120 Raccordement DN60/80","TS120 Kesselanschluss DN60/80","TS 120 Raccordo DN60/80",121,1,"DN 80",null,47.7,"511068",null,null,52.5,"104490",4.7999999999999972,46.6,5.8999999999999986,"104490",52.5,4.7999999999999972]
["104547",104547,null,"STK","KRS Regenkragen        20","CHF",63,"Schiedel KERASTAR",1.05,0,"J","KRS 200 Collerette anti-plue","KRS Regenkragen        20","KRS 200 Scossalina",137,1,"DN 200",null,54,"265700420",null,null,63,"104547",9,54,9,"104547",63,9]
["104577",104577,null,"STK","Zugreglerpaket PT12/18 EXE","CHF",390,"Schiedel CHEMINEE ZUG",3,0,"J","Paquet de Régulateur PT 12/18","Zugreglerpaket PT12/18 EXE","Set die Regolatori PT12/18",112,1,0,null,339,"030950",null,null,390,"104577",51,339,51,"104577",390,51]
["104657",104657,null,"STK","KRS 300 Wandhalt.statisch 50mm","CHF",141,"Schiedel KERASTAR",2.5,0,"J","KRS 300 Fixation murale statique 50mm","KRS 300 Wandhalt.statisch 50mm","KRS 300 Collare a muro 50mm statico 50mm",137,1,"DN 300",null,122,0,null,null,141,"104657",19,122,19,"104657",141,19]
["104660",104660,null,"STK","KRS 400  Wandhalterung 50mm ","CHF",96,"Schiedel KERASTAR",4.4000000000000004,0,"J","KRS 400  Fixation murale 50mm ","KRS 400  Wandhalterung 50mm ","KRS 400  Collare a muro 50mm ",137,1,"DN 400",null,83,0,null,null,96,"104660",13,83,13,"104660",96,13]
["104662",104662,null,"STK","KRS Regenkragen        16","CHF",61,"Schiedel KERASTAR",0.9,0,"J","KRS 160 Collerette anti-plue","KRS Regenkragen        16","KRS 160 Scossalina        ",137,1,"DN 160",null,53,0,null,null,61,"104662",8,53,8,"104662",61,8]
["104665",104665,null,"STK","KRS Regenkragen        30","CHF",110,"Schiedel KERASTAR",1.2,0,"J","KRS 300 Collerette anti-plue","KRS Regenkragen        30","KRS 300 Scossalina",137,1,"DN 300",null,95,0,null,null,110,"104665",15,95,15,"104665",110,15]
["104669",104669,null,"STK","ICM 300 Element mit Empa Messstutzen","CHF",932,"Schiedel ICM matt",3.0489999999999999,0,"J","ICM 300 Elément avec manchon de mesure EMPA","ICM 300 Element mit Empa Messstutzen","ICM 300 Elemento di misura EMPA",136,1,"DN 300",null,809.6,null,null,null,932,"104669",122.39999999999998,736,196,"104669",932,122.39999999999998]
["140677",140677,null,"STK","ICM5000 150 Abluftregenhut Typ AT Inox ","CHF",513.6,"Zubehör",4,0,"J","échappement capuchon de pluie Ø150","ICM5000 150 Abluftregenhut Typ AT Inox ","scarico parapioggia Ø150",136,2,"DN 150",null,446.6,null,null,null,513.6,"140677",67,406,107.60000000000002,"140677",513.6,67]
["140733",140733,null,"STK",{"$f":"IF($E$200=2,L3291,IF($E$200=3,N3291,M3291))","v":"LBS 350 Leichtbauschacht i 350mm A 440mm L1000mm"},"CHF",207,"ganztec-LEICHTBAUSCHACHT",45,0,"J","LBS Gaine d'inst. légère □i 350mm □E 440mm L1000mm","LBS 350 Leichtbauschacht i 350mm A 440mm L1000mm","LBS 350 Elemento installatione leggermente  ",141,1,0,null,165,null,null,null,207,"140733",42,163,44,"140733",207,42]
["140740",140740,null,"STK","ICM5000 300 Element mit Empa Messstutzen","CHF",754,"Schiedel ICM5000",3,0,"J","Elément de mesure EMPA Ø300","ICM5000 300 Element mit Empa Messstutzen","Elemento di misura EMPA Ø300",136,1,"DN 300",null,655.6,null,null,null,754,"140740",98.399999999999977,596,158,"140740",754,98.399999999999977]
["140743",140743,null,"STK","ICM5000 150 Element mit Empa Messstutzen","CHF",590,"Schiedel ICM5000",3,0,"J","Elément de mesure EMPA Ø150","ICM5000 150 Element mit Empa Messstutzen","Elemento di misura EMPA Ø150",136,1,"DN 300",null,512.6,null,null,null,590,"140743",77.399999999999977,466,124,"140743",590,77.399999999999977]
["140746",140746,null,"STK","PPL 180 Empa Messtutzen L450mm","CHF",343,"Schiedel PRIMA PLUS",1.05,0,"J","PPL 180 elément de mesure EMPA L250mm","PPL 180 Empa Messtutzen L450mm","PPL 180 elmento di missura EMPA L450mm",131,1,"DN 180",null,298.10000000000002,null,null,null,343,"140746",44.899999999999977,271,72,"140746",343,44.899999999999977]
["140752",140752,null,"STK","ICM5000 300 Abluftregenhut Typ AT Inox ","CHF",1075.3,"Zubehör",5,0,"J","échappement capuchon de pluie Ø300","ICM5000 300 Abluftregenhut Typ AT Inox ","scarico parapioggia Ø300",136,2,"DN 300",null,935,null,null,null,1075.3,"140752",140.29999999999995,850,225.29999999999995,"140752",1075.3,140.29999999999995]
["140753",140753,null,"STK",{"$f":"IF($E$200=2,L3306,IF($E$200=3,N3306,M3306))","v":"LBS 200 Leichtbauschacht i 200mm A 290mm L1000mm"},"CHF",129,"ganztec-LEICHTBAUSCHACHT",25,0,"J","LBS Gaine d'inst. légère □i 200mm □E 290mm L1000mm","LBS 200 Leichtbauschacht i 200mm A 290mm L1000mm","LBS 200 Elemento installatione leggermente  ",141,1,0,null,103,null,null,null,129,"140753",26,101,28,"140753",129,26]
["140757",140757,null,"STK","ICM5000 100 Anschluss von DW auf EW in Rauchgasr.","CHF",240,"Schiedel ICM5000",0.6,0,"J","ICM5000 100 Raccord de ICS - PPL","ICM5000 100 Anschluss von DW auf EW in Rauchgasr.","ICM5000 100 Raccordo de ICS - PPL",136,1,"DN 100",null,207.9,null,null,null,240,"140757",32.099999999999994,189,51,"140757",240,32.099999999999994]
["140761",140761,null,"STK","ICM5000 200 Anschluss von DW auf EW in Rauchgasr.","CHF",328,"Schiedel ICM5000",1.8,0,"J","ICM5000 200 Raccord de ICS - PPL","ICM5000 200 Anschluss von DW auf EW in Rauchgasr.","ICM5000 200 Raccordo de ICS - PPL",136,1,"DN 200",null,284.89999999999998,null,null,null,328,"140761",43.100000000000023,259,69,"140761",328,43.100000000000023]
["140764",140764,null,"STK","ICM5000 350 Anschluss von DW auf EW in Rauchgasr.","CHF",414,"Schiedel ICM5000",3,0,"J","ICM5000 350 Raccord de ICS - PPL","ICM5000 350 Anschluss von DW auf EW in Rauchgasr.","ICM5000 350 Raccordo de ICS - PPL",136,1,"DN 350",null,359.7,null,null,null,414,"140764",54.300000000000011,327,87,"140764",414,54.300000000000011]
["140766",140766,null,"STK","ICM5000 450 Anschluss von DW auf EW in Rauchgasr.","CHF",532,"Schiedel ICM5000",4.2,0,"J","ICM5000 450 Raccord de ICS - PPL","ICM5000 450 Anschluss von DW auf EW in Rauchgasr.","ICM5000 450 Raccordo de ICS - PPL",136,1,"DN 450",null,462,null,null,null,532,"140766",70,420,112,"140766",532,70]
["140823",140823,null,"STK","PPL 180 Basten Standard Kupfer zu Münd. Manchette","CHF",342,"Zubehör",3.9,0,"J","PPL 180 Basten Standard pour tôle de dilatation","PPL 180 Basten Standard Kupfer zu Münd. Manchette","PPL 180 Terminale Basten per manicotto di sbocco",131,2,"DN 180",null,322,null,null,null,342,"140823",20,320,22,"140823",342,20]
["140842",140842,null,"STK","ICM 180 Verschlussdeckel mit Zugbegrenzer ","CHF",383.3,"Schiedel ICM matt",3,0,"J","ICM 180 Fermeture avec  régulateur ","ICM 180 Verschlussdeckel mit Zugbegrenzer ","ICM 180 Coperchio con regulatore ",136,1,"DN 180",null,333.3,null,null,null,383.3,"140842",50,303,80.300000000000011,"140842",383.3,50]
["140844",140844,null,"STK","ICM 250 Verschlussdeckel mit Zugbegrenzer ","CHF",617.4,"Schiedel ICM matt",4,0,"J","ICM 250 Fermeture avec  régulateur ","ICM 250 Verschlussdeckel mit Zugbegrenzer ","ICM 250 Coperchio con regulatore ",136,1,"DN 250",null,536.79999999999995,null,null,null,617.4,"140844",80.600000000000023,488,129.39999999999998,"140844",617.4,80.600000000000023]
["140849",140849,null,"STK","KRS 140 Deckenanschluss-Element","CHF",479,"Schiedel KERASTAR",5.8,0,"J","KRS 140 Elément de connexion de plafond","KRS 140 Deckenanschluss-Element","KRS 140 Soffitto elemento di collegamento",137,1,"DN 140",null,416,null,null,null,479,"140849",63,416,63,"140849",479,63]
["140854",140854,null,"STK","KRS 140 Ofenaufsatz-Element","CHF",178,"Schiedel KERASTAR",5.8,0,"J","KRS 140 Poêle élément supérieur","KRS 140 Ofenaufsatz-Element","KRS 140 Stufa elemento superiore",137,1,"DN 140",null,154,null,null,null,178,"140854",24,154,24,"140854",178,24]
["140858",140858,null,"STK","KRS 250 Ofenaufsatz-Element","CHF",233,"Schiedel KERASTAR",5.8,0,"J","KRS 250 Poêle élément supérieur","KRS 250 Ofenaufsatz-Element","KRS 250 Stufa elemento superiore",137,1,"DN 250",null,202,null,null,null,233,"140858",31,202,31,"140858",233,31]
["140892",140892,null,"STK","PPL 300 Basten Stand. Kupfer mit Dila Isol 30mm","CHF",536,"Zubehör",3.9,0,"J","PPL300 Basten Standard couivre avec dilatation","PPL 300 Basten Stand. Kupfer mit Dila Isol 30mm","PPL 300 Terminale Basten rame con Dila Isol 30mm",15,2,null,null,505,null,null,null,536,"140892",31,503,33,"140892",536,31]
[null,null,null,"Stk",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,"Stk",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,"Stk",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,"Stk",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,"Stk",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
["100008",100008,null,"STK","TS120 80 Rohr mit Muffe mit Messöffnung L100mm","CHF",28.6,"TECHNOSTAR 120",0.4,0,"J","TS120 80 Tube avec manchon avec messure L100mm","TS120 80 Rohr mit Muffe mit Messöffnung L100mm","TS120 80 Tubo con manicotto con missura L100mm",121,1,"DN 80",null,26,"569200",null,null,28.6,"100008",2.6000000000000014,20,8.6000000000000014,{"$error":"#N/A"},28.6,2.6000000000000014]
["100022",100022,null,"STK","TS120 200 Rohr mit Muffe L250mm","CHF",95.2,"TECHNOSTAR 120",1,0,"J","TS120 200 Tube avec manchon L250mm","TS120 200 Rohr mit Muffe L250mm","TS120 200 Tubo con manicotto L250mm",121,1,"DN 200",null,86.5,"550409",null,null,95.2,"100022",8.7000000000000028,85.4,9.7999999999999972,{"$error":"#N/A"},95.2,8.7000000000000028]
["100031",100031,null,"STK","TS120 315 Rohr mit Muffe L2000mm ","CHF",519.6,"TECHNOSTAR 120",7.2,0,"J","TS120 315 Tube avec manchon L3150mm","TS120 315 Rohr mit Muffe L2000mm ","TS120 315 Tubo con manicotto L3150mm",121,1,"DN 315",null,472.3,"553030",null,null,519.6,"100031",47.300000000000011,471.2,48.400000000000034,{"$error":"#N/A"},519.6,47.300000000000011]
["100070",100070,null,"STK","TS120 80 Schraubteil mit Muffe zu Grundkörper","CHF",21.2,"TECHNOSTAR 120",0.05,0,"J","TS120 80 Manchon pour T  visser","TS120 80 Schraubteil mit Muffe zu Grundkörper","TS120 80 Pezzo female per Pezzo T",121,1,"DN 80",null,19.2,"567012",null,null,21.2,"100070",2,18.100000000000001,3.0999999999999979,{"$error":"#N/A"},21.2,2]
["100071",100071,null,"STK","TS120 80 Kondensatablauf zu T-Stück","CHF",21.9,"TECHNOSTAR 120",0.05,0,"J","TS120 80 D'évacuation des condensats pour T visser","TS120 80 Kondensatablauf zu T-Stück","TS120 80 Scarico condensa per pezzo T",121,1,"DN 80",null,19.899999999999999,"567016",null,null,21.9,"100071",2,18.8,3.0999999999999979,{"$error":"#N/A"},21.9,2]
["100087",100087,null,"STK","TS120 160 Abzweiger 45° mit Abgang 110 L500mm","CHF",291,"TECHNOSTAR 120",1,0,"J","TS120 160 Té 45° avec départ 110 L500mm","TS120 160 Abzweiger 45° mit Abgang 110 L500mm","TS120 160 Pezzo T 45° iniziano 110 L500mm",121,1,"DN 160",null,264.5,"500012",null,null,291,"100087",26.5,263.39999999999998,27.600000000000023,{"$error":"#N/A"},291,26.5]
["100127",100127,null,"STK","TS120 315 Revisionsbogen 87° ","CHF",500.5,"TECHNOSTAR 120",1.2,0,"J","TS120 315 Coude 87° avec nettoyage","TS120 315 Revisionsbogen 87° ","TS120 315 Curva 87° con revisione",121,1,"DN 315",null,455,"553080",null,null,500.5,"100127",45.5,427.5,73,{"$error":"#N/A"},500.5,45.5]
["100155",100155,null,"STK","TS120 315 Abstandhalter Inox","CHF",103.6,"TECHNOSTAR 120",0.7,0,"J","TS120 315 Distanceur rigides et flexibles Inox","TS120 315 Abstandhalter Inox","TS120 315 Abstandhalter Inox",121,1,"DN 315",null,94.1,"5530100",null,null,103.6,"100155",9.5,93,10.599999999999994,{"$error":"#N/A"},103.6,9.5]
["100156",100156,null,"STK","TS120 60 Kesselanschluss Reduktion zentr. 50","CHF",52.5,"TECHNOSTAR 120",0.15,0,"J","TS120 60 Raccordement reduction zentr. 50","TS120 60 Kesselanschluss Reduktion zentr. 50","TS120 60 Raccordo con reduzione zentr. 50",121,1,"DN 60",null,47.7,"516110",null,null,52.5,"100156",4.7999999999999972,46.6,5.8999999999999986,{"$error":"#N/A"},52.5,4.7999999999999972]
[{"$f":"B3408&\"\"","v":"100186"},100186,null,"STK",{"$f":"IF($E$200=2,L3408,IF($E$200=3,N3408,M3408))","v":"TS120 Muffenbriede 110/103 Inox"},"CHF",{"$f":"IF($L$190=1,W3408,S3408)","v":40.1},"TECHNOSTAR 120",0.2,0,"J","TS120 103/110 Manchon Bride","TS120 Muffenbriede 110/103 Inox","TS120 103/110 Brida mascio Inox",121,1,"DN110",null,36.4,"511059",null,null,40.1,"100186",3.7000000000000028,35.299999999999997,4.8000000000000043,{"$error":"#N/A"},40.1,3.7000000000000028]
["100211",100211,null,"STK","TS120 80 Mündungsrohr schwarz L980mm","CHF",37.799999999999997,"TECHNOSTAR 120",0.3,0,"J","TS120 80 Tube de final L980mm","TS120 80 Mündungsrohr schwarz L980mm","TS120 60 Tubo bocca L400mm",121,1,"DN 80",null,34.299999999999997,0,null,null,37.799999999999997,"100211",3.5,33.200000000000003,4.5999999999999943,{"$error":"#N/A"},37.799999999999997,3.5]
["100213",100213,null,"STK","TS120 125 Mündungsrohr schwarz L400mm","CHF",23.4,"TECHNOSTAR 120",0.7,0,"J","TS120 125 Tube de final L400mm","TS120 125 Mündungsrohr schwarz L400mm","TS120 60 Tubo bocca L400mm",121,1,"DN 125",null,21.2,"552068",null,null,23.4,"100213",2.1999999999999993,20.100000000000001,3.2999999999999972,{"$error":"#N/A"},23.4,2.1999999999999993]
["100221",100221,null,"STK","TS120 110 Haube zu Kaminkopfabedeckung schwarz","CHF",34.700000000000003,"TECHNOSTAR 120",0.01,0,"J","TS120 110 Capot pour Recouvrement  souche noir","TS120 110 Haube zu Kaminkopfabedeckung schwarz","TS120 110 Cappuccio per copertura del tombino PE",121,1,"DN110",null,31.5,0,null,null,34.700000000000003,"100221",3.2000000000000028,25.8,8.9000000000000021,{"$error":"#N/A"},34.700000000000003,3.2000000000000028]
["100236",100236,null,"STK","TS120 80/125 Dachpfanne 25-45°  rot","CHF",93.5,"TECHNOSTAR 120",3.2,0,"J","TS120 80/125 Solin toit universelle 25-45° rouge","TS120 80/125 Dachpfanne 25-45°  rot","TS120 80/125 Faldale universale 25-45° rosso",121,1,"DN 80",null,85,"554850",null,null,93.5,"100236",8.5,83.9,9.5999999999999943,{"$error":"#N/A"},93.5,8.5]
["100242",100242,null,"STK","TS120 80/125 Dachpfanne 35-55°  schwarz","CHF",113.1,"TECHNOSTAR 120",3.2,0,"J","TS120 80/125 Solin toit universelle 35-55° noir","TS120 80/125 Dachpfanne 35-55°  schwarz","TS120 80/125 Faldale universale 5-25° nero",121,1,"DN 80",null,102.8,"553200",null,null,113.1,"100242",10.299999999999997,101.7,11.399999999999991,{"$error":"#N/A"},113.1,10.299999999999997]
["100253",100253,null,"STK","TS120 200 Lippendichtung Peroxyd für Muffe","CHF",41,"TECHNOSTAR 120",0.2,0,"J","TS120 200 joint à lèvre de peroxyd pour manchon","TS120 200 Lippendichtung Peroxyd für Muffe","TS120 200 Guarnizione peroxyd per manicotto",121,1,"DN 200",null,37.200000000000003,0,null,null,41,"100253",3.7999999999999972,36.1,4.8999999999999986,{"$error":"#N/A"},41,3.7999999999999972]
["100254",100254,null,"STK","TS120 Dichtung zu Revisions-Deckel 110-160 ","CHF",14.9,"TECHNOSTAR 120",0.01,0,"J","TS120 110-160 joint pour couvrir révision","TS120 Dichtung zu Revisions-Deckel 110-160 ","TS120 110-160 Guarnizione per Giusura",121,1,"DN 110",null,13.5,0,null,null,14.9,"100254",1.4000000000000004,12.4,2.5,{"$error":"#N/A"},14.9,1.4000000000000004]
["100269",100269,null,"STK","TS120 Neutrabox Lippendichtung zu Behälter","CHF",16.100000000000001,"TECHNOSTAR 120",0.05,0,"J",null,"TS120 Neutrabox Lippendichtung zu Behälter",null,121,1,"TS ZBH",null,14,"911018",null,null,16.100000000000001,"100269",2.1000000000000014,14,2.1000000000000014,{"$error":"#N/A"},16.100000000000001,2.1000000000000014]
["100270",100270,null,"STK","TS120 Neutrabox Filtermatte zu Behälter","CHF",8.1,"TECHNOSTAR 120",1E-3,0,"J",null,"TS120 Neutrabox Filtermatte zu Behälter",null,121,1,"TS ZBH",null,7,"911019",null,null,8.1,"100270",1.0999999999999996,7,1.0999999999999996,{"$error":"#N/A"},8.1,1.0999999999999996]
["100277",100277,null,"STK","TS120 60 Reduktion auf 40mm zum schweissen","CHF",21.2,"TECHNOSTAR 120",0.05,0,"J",null,"TS120 60 Reduktion auf 40mm zum schweissen",null,121,1,"DN 60",null,19.2,"516006",null,null,21.2,"100277",2,18.100000000000001,3.0999999999999979,{"$error":"#N/A"},21.2,2]
["100279",100279,null,"STK","TS120 160 Ablaufdeckel 40mm ","CHF",46.6,"TECHNOSTAR 120",1.9,0,"J",null,"TS120 160 Ablaufdeckel 40mm ",null,121,1,"DN 160",null,42.3,"500001",null,null,46.6,"100279",4.3000000000000043,41.2,5.3999999999999986,{"$error":"#N/A"},46.6,4.3000000000000043]
["100298",100298,null,"STK","TS120 100 Rohrschelle verzinkt 1/2\" ","CHF",15.8,"TECHNOSTAR 120",0.4,0,"J","TS120 100 Collier  galvanisé 1/2\"","TS120 100 Rohrschelle verzinkt 1/2\" ","TS120 100 Feacetta per Tubo 1/2\" galvanizzato",121,1,"DN 60",null,12.6,"512006",null,null,15.8,"100298",3.2000000000000011,11.5,4.3000000000000007,{"$error":"#N/A"},15.8,3.2000000000000011]
["100302",100302,null,"STK","TS120 160 Rohrschelle Inox 1/2\"","CHF",305,"TECHNOSTAR 120",0.16,0,"J","TS120 160 Collier  Inox 1/2\"","TS120 160 Rohrschelle Inox 1/2\"","TS120 160 Feacetta per Tubo 1/2\" Inox",121,1,"DN 160",null,265,"267000316","103627","4037494814802",305,"100302",40,256.5,48.5,{"$error":"#N/A"},305,40]
["100307",100307,null,"STK","TS120 1/2\" Grundplatte für Rohrhalter gleitend","CHF",35.9,"TECHNOSTAR 120",0.3,0,"J","TS120 Plaque base coulissante 1/2\" galvanisé","TS120 1/2\" Grundplatte für Rohrhalter gleitend","TS120 1/2\" Pisatra di base scorrevole galvanizzato",121,1,"TS ZBH",null,28.7,"512003",null,null,35.9,"100307",7.1999999999999993,27.6,8.2999999999999972,{"$error":"#N/A"},35.9,7.1999999999999993]
["100348",100348,null,"STK","TS120LAS 80/125 Rotex weiss","CHF",142.9,"TECHNOSTAR 120 LAS",0.3,0,"J","TS120LAS 80/125 Raccordement chaudière ROTEX blanc","TS120LAS 80/125 Rotex weiss","TS120LAS 80/125 Raccordo di caldaia ROTEX bianco",122,1,"DN 80",null,129.9,"511072",null,null,142.9,"100348",13,128.80000000000001,14.099999999999994,{"$error":"#N/A"},142.9,13]
["100350",100350,null,"STK","TS120LAS 80/125/50 Kesselanschl. Luft Abgas getr. ","CHF",142.9,"TECHNOSTAR 120 LAS",0.3,0,"J","TS120LAS 125/80/80 Racc. chaudiére  air séparé","TS120LAS 80/125/50 Kesselanschl. Luft Abgas getr. ","TS120LAS 125/80/80 Racc. di caldaia  aira separat",122,1,"DN 80",null,129.9,"568012",null,null,142.9,"100350",13,128.80000000000001,14.099999999999994,{"$error":"#N/A"},142.9,13]
["100374",100374,null,"STK","TS120LAS 80/125 KAS mit Helmholz. Raumluftunab.","CHF",115,"TECHNOSTAR 120 LAS",0.5,0,"J","TS120LAS 80/125  Racc.avec Helmholz.ouvrir fumée","TS120LAS 80/125 KAS mit Helmholz. Raumluftunab.","TS120LAS 80/125 Racc.con Helmholz aprire c.fumaria",122,1,"DN 80",null,104.5,"552026",null,null,115,"100374",10.5,103.4,11.599999999999994,{"$error":"#N/A"},115,10.5]
["140774",140774,null,"Stk","ABS 200 Grundplatte mit Abkantung zu ICM250","CHF",333,null,0,"150","J","ABS 200 Plaque de base  avec la bordure ICM250","ABS 200 Grundplatte mit Abkantung zu ICM250","ABS 200 Piastra di base con bordo a ICM250",null,null,"200",null,289.43,null,null,null,333,"140774",null,289.43,43.569999999999993,{"$error":"#N/A"},333,43.569999999999993]
["140777",140777,null,"Stk","ABS 180 TL  Grundplatte mit Abkantung zu ICM250","CHF",400,null,7,"150","J","ABS 180 TL Plaque de base  avec la bordure ICM250","ABS 180 TL  Grundplatte mit Abkantung zu ICM250","ABS 180 TL Piastra di base con bordo a ICM250",null,null,"180",null,347.11,null,null,null,400,"140777",null,347.11,52.889999999999986,{"$error":"#N/A"},400,52.889999999999986]
["140848",140848,null,"Stk","TS120  Schlüssel zum offnen des Rev. Deckel 80-125","CHF",21.7,"TECHNOSTAR 120",1E-4,0,"J","TS 120 clé pour ouvrir le couvercle 80-125 Rev.","TS120  Schlüssel zum offnen des Rev. Deckel 80-125","TS 120 chiave per aprire il coperchio 80-125 Rev.",121,null,null,null,19.7,null,null,null,21.7,"140848",null,18.600000000000001,3.0999999999999979,{"$error":"#N/A"},21.7,2]
["140951",140951,null,"Stk","TS120 125 350 Endmuffe schwarz mit Mündungsrohr","CHF",215.4,"TECHNOSTAR 120",1.3,"117","J","TS120 125 350 Endmuffe schwarz mit Mündungsrohr","TS120 125 350 Endmuffe schwarz mit Mündungsrohr","TS120 125 350 Endmuffe schwarz mit Mündungsrohr",121,null,"110",null,195.8,null,null,null,215.4,"140951",null,194.7,20.700000000000017,{"$error":"#N/A"},215.4,19.599999999999994]
["140874",140874,null,"Stk","ABS Handyplatte DZ  Kupfer 380 x 710mm  ","CHF",470,"Schiedel ABSOLUT",3.4,null,"J","ABS Plaque Handy DZ cuivre 380 x 710mm  ","ABS Handyplatte DZ  Kupfer 380 x 710mm  ","ABS Lastra Handy DZ rame 380 x 710mm  ",111,null,null,null,408,null,null,null,470,"140874",null,408,62,{"$error":"#N/A"},470,62]
["140879",140879,null,"Stk","ABSTL 200 Grundplatte  zu ICK 200","CHF",479,null,0,"150","J","ABSTL 200 Plaque de base  avec la bordure  ICK 200","ABSTL 200 Grundplatte  zu ICK 200","ABSTL 200 Piastra di base con bordo a ICK 200",null,null,"200",null,416.12,null,null,null,479,"140879",null,416.12,62.879999999999995,{"$error":"#N/A"},479,62.879999999999995]
["140866",140866,null,"Stk","PPL 130 Kaminfuss 85° ","CHF",123,"Schiedel PRIMA PLUS",1.2,"205","J","PPL 130 Pied de Cheminée 85° ","PPL 130 Kaminfuss 85° ","PPL 130 Piede di camino 85°",131,null,"130",null,106.7,null,null,null,123,"140866",null,97,26,{"$error":"#N/A"},123,16.299999999999997]
["140869",140869,null,"Stk","PPL 200 Kaminfuss 85° ","CHF",179,"Schiedel PRIMA PLUS",2,"220","J","PPL 200 Pied de Cheminée 85° ","PPL 200 Kaminfuss 85° ","PPL 200 Piede di camino 85°",131,null,"200",null,155.1,null,null,null,179,"140869",null,141,38,{"$error":"#N/A"},179,23.900000000000006]
["140871",140871,null,"Stk","PPL 300 Kaminfuss 45° m.Stütze L240mm","CHF",260,"Schiedel PRIMA PLUS",2.8,"240","J","PPL 300 Pied de Cheminée 85°","PPL 300 Kaminfuss 45° m.Stütze L240mm","PPL 300 Piede di camino 85° ",131,null,"300",null,225.5,null,null,null,260,"140871",null,205,55,{"$error":"#N/A"},260,34.5]
["140931",140931,null,"Stk","CFS 130/200 Putztüranschluss rund  L450mm","CHF",385,"Schiedel CLV",4,"400","J","CFS 130/200 Putztüranschluss rund  L450mm","CFS 130/200 Putztüranschluss rund  L450mm","CFS 130/200 Putztüranschluss rund  L450mm",138,null,"130",null,334.4,null,null,null,385,"140931",null,304,81,{"$error":"#N/A"},385,50.600000000000023]
[{"$f":"B3504&\"\"","v":"140898"},140898,null,"Stk",{"$f":"IF($E$200=2,L3504,IF($E$200=3,N3504,M3504))","v":"ICM 150 Abgasschalldämpfer  L1000mm"},"CHF",{"$f":"IF($L$190=1,W3504,S3504)","v":1110.7},"Zubehör",30,"1000","J","ICM 150 Amortisseur du bruit L1000mm","ICM 150 Abgasschalldämpfer  L1000mm","ICM 150 Silenzatore L1000mm",15,null,"150",null,965.8,null,null,null,1110.7,"140898",null,878,232.70000000000005,{"$error":"#N/A"},1110.7,144.90000000000009]
["140902",140902,null,"Stk","ICM 300 Abgasschalldämpfer  L1000mm","CHF",2183.4,"Zubehör",50,"1000","J","ICM 300  Amortisseur du bruit L1000mm","ICM 300 Abgasschalldämpfer  L1000mm","ICM 300 Silenzatore L1000mm",15,null,"300",null,1898.6,null,null,null,2183.4,"140902",null,1726,457.40000000000009,{"$error":"#N/A"},2183.4,284.80000000000018]
["140907",140907,null,"Stk","ICM 600 Abgasschalldämpfer  L1000mm","CHF",4469.3,"Schiedel ICM5000",75,"1000","J","ICM 500  Amortisseur du bruit L1000mm","ICM 600 Abgasschalldämpfer  L1000mm","ICM 500 Silenzatore L1000mm",136,null,"600",null,3886.3,null,null,null,4469.3,"140907",null,3533,936.30000000000018,{"$error":"#N/A"},4469.3,583]
["140932",140932,null,"Stk","ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben","CHF",75,null,7.0000000000000007E-2,0,"J","ABS HEB-Set de fixation pour plaque Handy cuivre","ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben","ABS HEB-Set lastra Handy TL rame con viti lunghe",null,null,null,null,65,null,null,null,75,"140932",null,44,31,{"$error":"#N/A"},75,10]
["140961",140961,null,"Stk","ABS Kachelofen Zuluftanschluss Ø180 auf 335x100mm","CHF",313,null,1,"200","J","ABS Kachelofen Zuluftanschluss Ø180 auf 335x100mm","ABS Kachelofen Zuluftanschluss Ø180 auf 335x100mm","ABS Kachelofen Zuluftanschluss Ø180 auf 335x100mm",null,null,"180",null,272,null,null,null,313,"140961",null,272,41,{"$error":"#N/A"},313,41]
["140882",140882,null,"Stk","CHI 300 Adapter Flex zu Flex","CHF",124,"Schiedel CHIMFLEX",0.7,"150","J","CHI 300 Adapteur Flex / Flex","CHI 300 Adapter Flex zu Flex","CHI 300 Giunto maschio Flex / Flex",132,null,"300",null,107.8,null,null,null,124,"140882",null,98,26,{"$error":"#N/A"},124,16.200000000000003]
["140956",140956,null,"Stk","TS120LAS 60/100 Grundbausatz DN60  im Schacht ","CHF",520.9,"TECHNOSTAR 120 LAS",15,700,"J","TS120LAS 60/100 kit de base DN60 dans l'arbre","TS120LAS 60/100 Grundbausatz DN60  im Schacht ","TS120LAS 60/100 Kit di base DN60 di nel pozzo","122",null,60,null,473.5,null,null,null,520.9,"140956",null,472.4,48.5,{"$error":"#N/A"},520.9,47.399999999999977]
["140958",140958,null,"Stk","TS120LAS 80/125 Grundbausatz 80/125 Inox  Fassade","CHF",991.1,"TECHNOSTAR 120 LAS",25,1000,"J","TS120LAS 80/125 kit de base 80/125 Inox  façade","TS120LAS 80/125 Grundbausatz 80/125 Inox  Fassade","TS120LAS 80/125 kit base 80/125 Inox sulla facciat","122",null,80,null,901,null,null,null,991.1,"140958",null,899.9,91.200000000000045,{"$error":"#N/A"},991.1,90.100000000000023]
[{"$f":"B3531&\"\"","v":"104656"},104656,null,"Stk","TS120 75 Lippendichtung Silikon für Muffe","CHF",{"$f":"IF($L$190=1,W3531,S3531)","v":11},"TECHNOSTAR 120",1.4999999999999999E-2,null,"J",null,"TS120 75 Lippendichtung Silikon für Muffe",null,null,null,null,null,10,null,null,null,11,"104656",null,4.9000000000000004,6.1,{"$error":"#N/A"},11,1]
["104675",104675,null,"Stk","Kundendienst ","CHF",178,null,0,null,"J",null,"Kundendienst ",null,null,null,null,null,154.5,null,null,null,178,"104675",null,154.5,23.5,{"$error":"#N/A"},178,23.5]
["104687",104687,null,"Stk","ISOLIT 200 Basten Standard Kupfer eckig ","CHF",375,"ISOLIT",5.0999999999999996,null,"J",null,"ISOLIT 200 Basten Standard Kupfer eckig ",null,null,null,null,null,353,null,null,null,375,"104687",null,351,24,{"$error":"#N/A"},375,22]
["104704",104704,null,"Stk","TS120 80 Dichtung zu Regenhaube Kaminkopf","CHF",13.8,"TECHNOSTAR 120",0.02,null,"J","TS120 80 Joint torique bleu","TS120 80 Dichtung zu Regenhaube Kaminkopf","TS120 80 Guarnizione per pezzo T",null,null,null,null,12.5,null,null,null,13.8,"104704",null,11.4,2.4000000000000004,{"$error":"#N/A"},13.8,1.3000000000000007]
["140717",140717,null,"Stk","Ausstellungs-Mantelsteinständer  ABS36/50","CHF",575,"Zubehör",20,null,"J",null,"Ausstellungs-Mantelsteinständer  ABS36/50",null,null,null,null,null,500,null,null,null,575,"140717",null,500,75,{"$error":"#N/A"},575,75]
["140861",140861,null,"Stk","ICM5000 80 Erweiterung auf DN130 Rauchgasrichtung","CHF",190,"Schiedel ICM5000",1.2,null,"J","ICM5000 80 Extension en 1 diamètre des combustion","ICM5000 80 Erweiterung auf DN130 Rauchgasrichtung","ICM5000 80 Estensione 1 diametro direzione  fumi",null,null,null,null,165,null,null,null,190,"140861",null,150,40,{"$error":"#N/A"},190,25]
["140883",140883,null,"Stk","ICM5000 350 Deflektor Regenhut Typ AT Inox Matt","CHF",1246.0999999999999,"Zubehör",7,null,"J",null,"ICM5000 350 Deflektor Regenhut Typ AT Inox Matt",null,null,null,null,null,1083.5,null,null,null,1246.0999999999999,"140883",null,985,261.09999999999991,{"$error":"#N/A"},1246.0999999999999,162.59999999999991]
["140886",140886,null,"Stk","ICM5000 500 Deflektor Regenhut Typ AT Inox Matt","CHF",2087.3000000000002,"Zubehör",17,null,"J",null,"ICM5000 500 Deflektor Regenhut Typ AT Inox Matt",null,null,null,null,null,1815,null,null,null,2087.3000000000002,"140886",null,1650,437.30000000000018,{"$error":"#N/A"},2087.3000000000002,272.30000000000018]
["140913",140913,null,"Stk","CFS 130/200 T-Stück 90°","CHF",157,"Schiedel CLV",3.5,null,"J","CFS 130/200 Pièce T 90°","CFS 130/200 T-Stück 90°",null,null,null,null,null,136.4,null,null,null,157,"140913",null,124,33,{"$error":"#N/A"},157,20.599999999999994]
["140917",140917,null,"Stk","CFS 130/200 Winkel 15°","CHF",87,"Schiedel CLV",0.9,null,"J","CFS 130/200 Coude 15°","CFS 130/200 Winkel 15°",null,null,null,null,null,74.8,null,null,null,87,"140917",null,68,19,{"$error":"#N/A"},87,12.200000000000003]
["140921",140921,null,"Stk","CFS 130/200 Zwischenstütze","CHF",133,"Schiedel CLV",5,null,"J","CFS 130/200 Support intermédiaire","CFS 130/200 Zwischenstütze",null,null,null,null,null,115.5,null,null,null,133,"140921",null,105,28,{"$error":"#N/A"},133,17.5]
["140922",140922,null,"Stk","CFS 130/200 Schiebelement L375-585mm","CHF",173,"Schiedel CLV",3,null,"J","CFS 130/200 Conduit télescopique ","CFS 130/200 Schiebelement L375-585mm",null,null,null,null,null,149.6,null,null,null,173,"140922",null,136,37,{"$error":"#N/A"},173,23.400000000000006]
["140926",140926,null,"Stk","CFS 130/200 Inspektions-Winkel 87°","CHF",260,"Schiedel CLV",2,null,"J","CFS 130/200 Coude d'inspection 85°  ","CFS 130/200 Inspektions-Winkel 87°",null,null,null,null,null,225.5,null,null,null,260,"140926",null,205,55,{"$error":"#N/A"},260,34.5]
["140965",140965,null,"Stk","TS120 110 Abgasabsperrung 110 für Kaskade","CHF",332.1,"TECHNOSTAR 120",0.35,null,"J",null,"TS120 110 Abgasabsperrung 110 für Kaskade",null,null,null,null,null,301.89999999999998,null,null,null,332.1,"140965",null,300.76,31.340000000000032,{"$error":"#N/A"},332.1,30.200000000000045]
["140967",140967,null,"Stk","ICM5000 600 Deflektor Regenhut Typ AT Inox Matt","CHF",1872.2,"Zubehör",17,null,"J",null,"ICM5000 600 Deflektor Regenhut Typ AT Inox Matt",null,null,null,null,null,1628,null,null,null,1872.2,"140967",null,1480,392.20000000000005,{"$error":"#N/A"},1872.2,244.20000000000005]
["140970",140970,null,"Stk","ICM5000-50 200 T-Stück 45°","CHF",868,"Schiedel ICM5000",8,null,"J","ICM5000 200 Pièce Té 45° L 530mm","ICM5000-50 200 T-Stück 45°","ICM5000 200 Pezzo T 45° L 530mm",null,null,null,null,754.6,null,null,null,868,"140970",null,686,182,{"$error":"#N/A"},868,113.39999999999998]
["140975",140975,null,"Stk","ICM5000-50 200 Längenelement L195mm","CHF",146,"Schiedel ICM5000",2,null,"J","ICM5000 200 Tuyau droit L195mm","ICM5000-50 200 Längenelement L195mm","ICM5000 200 Elemento lunghezze L195mm",null,null,null,null,126.5,null,null,null,146,"140975",null,115,31,{"$error":"#N/A"},146,19.5]
["140979",140979,null,"Stk","ICM5000-50 200 Winkel 30°","CHF",243,"Schiedel ICM5000",2.2999999999999998,null,"J","ICM5000 200 Coude 30°","ICM5000-50 200 Winkel 30°","ICM5000 200 Gomito 30°",null,null,null,null,211.2,null,null,null,243,"140979",null,192,51,{"$error":"#N/A"},243,31.800000000000011]
[{"$f":"B3595&\"\"","v":"140983"},140983,null,"Stk","ICM5000-50 200 Anschl. DW auf EW inkl. Flansch","CHF",{"$f":"IF($L$190=1,W3595,S3595)","v":365},"Schiedel ICM5000",3.5,null,"J","ICM5000 200 Raccord de PPL - ICS","ICM5000-50 200 Anschl. DW auf EW inkl. Flansch","ICM5000 200 Raccordo de PPL - ICS",null,null,null,null,316.8,null,null,null,365,"140983",null,288,77,{"$error":"#N/A"},365,48.199999999999989]
["140986",140986,null,"Stk","ICM5000-50 250 Anschluss EW auf DW inkl. Flansch","CHF",299,"Schiedel ICM5000",3,null,"J","ICM5000 250 Raccord de PPL - ICS","ICM5000-50 250 Anschluss EW auf DW inkl. Flansch","ICM5000 250 Raccordo de PPL - ICS",null,null,null,null,259.60000000000002,null,null,null,299,"140986",null,236,63,{"$error":"#N/A"},299,39.399999999999977]
["140988",140988,null,"Stk","ICM5000-50 250 Erweiterung  1Ø in Rauchgasrichtung","CHF",269,"Schiedel ICM5000",3.1,null,"J","ICM5000 250 Extension en 1 diamètre des combustion","ICM5000-50 250 Erweiterung  1Ø in Rauchgasrichtung","ICM5000 250 Estensione 1 diametro direzione  fumi",null,null,null,null,233.2,null,null,null,269,"140988",null,212,57,{"$error":"#N/A"},269,35.800000000000011]
["140991",140991,null,"Stk","ICM5000-50 250 Längenelement L250mm","CHF",164,"Schiedel ICM5000",3,null,"J","ICM5000 250 Tuyau droit L250mm","ICM5000-50 250 Längenelement L250mm","ICM5000 250 Elemento lunghezze L250mm",null,null,null,null,141.9,null,null,null,164,"140991",null,129,35,{"$error":"#N/A"},164,22.099999999999994]
["140997",140997,null,"Stk","ICM5000-50 250 Winkel 30°","CHF",275,"Schiedel ICM5000",3.5,null,"J","ICM5000 250 Coude 30°","ICM5000-50 250 Winkel 30°","ICM5000 250 Gomito 30°",null,null,null,null,238.7,null,null,null,275,"140997",null,217,58,{"$error":"#N/A"},275,36.300000000000011]
["140999",140999,null,"Stk","ICM5000-50 250 Winkel 90°","CHF",298,"Schiedel ICM5000",5,null,"J","ICM5000 250 Coude 90°","ICM5000-50 250 Winkel 90°","ICM5000 250 Gomito 90°",null,null,null,null,258.5,null,null,null,298,"140999",null,235,63,{"$error":"#N/A"},298,39.5]
["141003",141003,null,"Stk","ICM5000-50 spez Übergang s50 auf s25","CHF",515,"Schiedel ICM5000",0,null,"J","ICM Pèce speciale","ICM5000-50 spez Übergang s50 auf s25","ICM Pezzo speziale",null,null,null,null,447.7,null,null,null,515,"141003",null,407,108,{"$error":"#N/A"},515,67.300000000000011]
["141010",141010,null,"Stk","ICM5000-50 400 Anschl. DW auf EW in Rauchgasr s1mm","CHF",324,"Schiedel ICM5000",5,null,"J","ICM5000 400 Raccord de PPL - ICS","ICM5000-50 400 Anschl. DW auf EW in Rauchgasr s1mm","ICM5000 400 Raccordo de PPL - ICS",null,null,null,null,281.60000000000002,null,null,null,324,"141010",null,256,68,{"$error":"#N/A"},324,42.399999999999977]
["141014",141014,null,"Stk","ICM5000-50 400 Putztüranschluss rund","CHF",1449,"Schiedel ICM5000",11.5,null,"J","ICM5000 400 Element d'inspéction ronde ","ICM5000-50 400 Putztüranschluss rund","ICM5000 400 Elemento di inspezione su pressione",null,null,null,null,1259.5,null,null,null,1449,"141014",null,1145,304,{"$error":"#N/A"},1449,189.5]
["141017",141017,null,"Stk","ICM5000-50 400 Längenelement L195mm","CHF",293,"Schiedel ICM5000",4,null,"J","ICM5000 400 Tuyau droit L195mm","ICM5000-50 400 Längenelement L195mm","ICM5000 400 Elemento lunghezze L195mm",null,null,null,null,254.1,null,null,null,293,"141017",null,231,62,{"$error":"#N/A"},293,38.900000000000006]
["141019",141019,null,"Stk","ICM5000-50 400 Längenelement L500mm","CHF",405,"Schiedel ICM5000",9,null,"J","ICM5000 400 Tuyau droit L500mm","ICM5000-50 400 Längenelement L500mm","ICM5000 400 Elemento lunghezze L500mm",null,null,null,null,352,null,null,null,405,"141019",null,320,85,{"$error":"#N/A"},405,53]
["141022",141022,null,"Stk","ICM5000-50 400 Element mit Empa Messstutzen","CHF",1301,"Schiedel ICM5000",8,null,"J","ICM 400 Elément avec manchon de mesure EMPA","ICM5000-50 400 Element mit Empa Messstutzen","ICM 400 Elemento di misura EMPA",null,null,null,null,1130.8,null,null,null,1301,"141022",null,1028,273,{"$error":"#N/A"},1301,170.20000000000005]
["141026",141026,null,"Stk","ICM5000-50 400 Zwischenstütze","CHF",319,"Schiedel ICM5000",8.1999999999999993,null,"J","ICM5000 400 Support intermédieaire","ICM5000-50 400 Zwischenstütze","ICM5000 400 Piastra passante",null,null,null,null,277.2,null,null,null,319,"141026",null,252,67,{"$error":"#N/A"},319,41.800000000000011]
["141028",141028,null,"Stk","TS120LAS 125 Rev-Deckel mit Knauf RAL","CHF",29.6,"TECHNOSTAR 120 LAS",0,null,"J",null,"TS120LAS 125 Rev-Deckel mit Knauf RAL",null,null,null,null,null,26.9,null,null,null,29.6,"141028",null,25.8,3.8000000000000007,{"$error":"#N/A"},29.6,2.7000000000000028]
["141040",141040,null,"Stk","ABS 200 Grundplatte mit Abkantung zu ICM200","CHF",342,null,7,null,"J",null,"ABS 200 Grundplatte mit Abkantung zu ICM200",null,null,null,null,null,297,null,null,null,342,"141040",null,297,45,{"$error":"#N/A"},342,45]
["141044",141044,null,"Stk","ICM 100 Anschluss mit Klemmfutter DN80","CHF",138,"Schiedel ICM matt",1.2,null,"J","ICM 100 Raccord PPL - ICS av. manchon double DN80","ICM 100 Anschluss mit Klemmfutter DN80","ICM 100 Adattore PPL - ICS con tubo fodera DN80",null,null,null,null,119.9,null,null,null,138,"141044",null,109,29,{"$error":"#N/A"},138,18.099999999999994]
["141048",141048,null,"Stk","LBS 320 Grundplatte 410mm x 410mm zu LBS320","CHF",39,"ganztec-LEICHTBAUSCHACHT",4,null,"J","LBS 320 Plaque de Base pour Gaine d'inst. 410mm ","LBS 320 Grundplatte 410mm x 410mm zu LBS320","LBS 320 Piastra di Base per Inst. leggera. 410x410",null,null,null,null,31,null,null,null,39,"141048",null,29,10,{"$error":"#N/A"},39,8]
["141049",141049,null,"Stk","CFS 100/150 T-Stück 87°","CHF",145,"Schiedel CLV",2.5,null,"J","CFS 100/150 Pièce T 87°","CFS 100/150 T-Stück 87°",null,null,null,null,null,125.4,null,null,null,145,"141049",null,114,31,{"$error":"#N/A"},145,19.599999999999994]
["141053",141053,null,"Stk","CFS 100/150 Rohrelement L250mm","CHF",41,"Schiedel CLV",1.1000000000000001,null,"J",null,"CFS 100/150 Rohrelement L250mm",null,null,null,null,null,35.200000000000003,null,null,null,41,"141053",null,32,9,{"$error":"#N/A"},41,5.7999999999999972]
["141058",141058,null,"Stk","CFS 100/150 Zwischenstütze","CHF",128,"Schiedel CLV",4.5999999999999996,null,"J",null,"CFS 100/150 Zwischenstütze",null,null,null,null,null,111.1,null,null,null,128,"141058",null,101,27,{"$error":"#N/A"},128,16.900000000000006]
["141061",141061,null,"Stk","CFS 100/150 Kondensattopf","CHF",79,"Schiedel CLV",0.4,null,"J",null,"CFS 100/150 Kondensattopf",null,null,null,null,null,68.2,null,null,null,79,"141061",null,62,17,{"$error":"#N/A"},79,10.799999999999997]
["141063",141063,null,"Stk","CFS 100/150 Inspektions-Winkel 87°","CHF",259,"Schiedel CLV",1.8,null,"J",null,"CFS 100/150 Inspektions-Winkel 87°",null,null,null,null,null,224.4,null,null,null,259,"141063",null,204,55,{"$error":"#N/A"},259,34.599999999999994]
["141068",141068,null,"Stk","Closeline / Rohr exklusiv CNS gebürstet","CHF",416,"Schiedel ICM matt",0,null,"J",null,"Closeline / Rohr exklusiv CNS gebürstet",null,null,null,null,null,361,null,null,null,416,"141068",null,361,55,{"$error":"#N/A"},416,55]
["141073",141073,null,"Stk","ICM5000 450 Element mit Empa Messstutzen","CHF",1422,"Schiedel ICM5000",3.0489999999999999,null,"J","ICM 400 Elément avec manchon de mesure EMPA","ICM5000 450 Element mit Empa Messstutzen","ICM 400 Elemento di misura EMPA",null,null,null,null,1236,null,null,null,1422,"141073",null,1236,186,{"$error":"#N/A"},1422,186]
["100376",100376,null,"STK","TS120LAS 80/125 KAS ohne Helmholz.Raumluftabhängig","CHF",170.4,"TECHNOSTAR 120 LAS",0.8,0,"J","TS120LAS 80/125  Racc. sans Helmholz.ouvrir fumée","TS120LAS 80/125 KAS ohne Helmholz.Raumluftabhängig","TS120LAS 80/125 Racc.sen.Helmholz aprire c.fumaria",122,1,"DN 80",null,154.79999999999998,"552073",null,null,170.4,"100376",15.600000000000023,null,null,null,170.4,15.600000000000023,170.4,170.35406698564591]
["100377",100377,null,"STK","TS120LAS 80/125 KAS ohne Helmholz. Raumluftunab.","CHF",171.5,"TECHNOSTAR 120 LAS",0.5,0,"J","TS120LAS 80/125  Racc. sans Helmholz.ambiant fumée","TS120LAS 80/125 KAS ohne Helmholz. Raumluftunab.","TS120LAS 80/125 Racc.sen.Helmholz aprire c.fumaria",122,1,"DN 80",null,155.9,"552072",null,null,171.5,"100377",15.599999999999994,null,null,null,171.5,15.599999999999994]
["100393",100393,null,"STK","TS120LAS 160/225 Rohr L 500 Inox ","CHF",169,"TECHNOSTAR 120 LAS",4.0999999999999996,0,"J","TS120LAS 160/225 Tuyau L 500 Inox ","TS120LAS 160/225 Rohr L 500 Inox ","TS120LAS 160/225 Tubo L 500 Inox",122,1,"DN 160",null,153.6,"550964",null,null,169,"100393",15.400000000000006,null,null,null,169,15.400000000000006]
["100396",100396,null,"STK","TS120LAS 200/300 Rohr L 1000 Inox ","CHF",369.5,"TECHNOSTAR 120 LAS",6.4,0,"J","TS120LAS 200/300 Tuyau L1000 Inox ","TS120LAS 200/300 Rohr L 1000 Inox ","TS120LAS 200/300 Tubo L1000 Inox",122,1,"DN 200",null,335.9,"550967",null,null,369.5,"100396",33.600000000000023,null,null,null,369.5,33.600000000000023]
["100408",100408,null,"STK","TS120LAS 160 Verl. Typ 1 zu Aussenwandanschluss","CHF",171.4,"TECHNOSTAR 120 LAS",0.4,0,"J","TS120LAS 160 Ralonges type 1 de racc. paroi  Inox","TS120LAS 160 Verl. Typ 1 zu Aussenwandanschluss","TS120LAS 160 Prolunga per perti esterne Typ1",122,1,"DN 110",null,155.80000000000001,"560973",null,null,171.4,"100408",15.599999999999994,null,null,null,171.4,15.599999999999994]
["100417",100417,null,"STK","TS120LAS 110 Abdeckblende  Inox","CHF",40.4,"TECHNOSTAR 120 LAS",0.3,0,"J","TS120LAS 110 Cache 200mm x 200mm Inox","TS120LAS 110 Abdeckblende  Inox","TS120LAS 110 Chiusura 225mm x 225mm",122,1,"DN110",null,36.700000000000003,"550810",null,null,40.4,"100417",3.6999999999999957,null,null,null,40.4,3.6999999999999957]
["100426",100426,null,"STK","TS120LAS 250/350 Dachdurchführung Inox","CHF",758.2,"TECHNOSTAR 120 LAS",5.5,0,"J","TS120LAS 250/350 Passage de troiture Inox","TS120LAS 250/350 Dachdurchführung Inox","TS120LAS 250/350 Pezzo per attraversare tetto Inox",122,1,"DN 250",null,689.2,"553230",null,null,758.2,"100426",69,null,null,null,758.2,69]
["100462",100462,null,"STK","TS120LAS 185 Wandhalterung Inox","CHF",137.19999999999999,"TECHNOSTAR 120 LAS",0.6,0,"J","TS120LAS 185 Fixation murale Inox","TS120LAS 185 Wandhalterung Inox","TS120LAS 185 Collare al muro Inox",122,1,"DN 125",null,124.7,"550485",null,null,137.19999999999999,"100462",12.499999999999986,null,null,null,137.19999999999999,12.499999999999986]
["100470",100470,null,"STK","TS120LAS 160/225 Wandurchführung L500mm","CHF",122.6,"TECHNOSTAR 120 LAS",2.1,0,"J","TS120LAS 160/225 Passage de paroi L500mm","TS120LAS 160/225 Wandurchführung L500mm","TS120LAS 160/225 Pezzo attraversato de pareti",122,1,"DN 160",null,111.4,"550979",null,null,122.6,"100470",11.199999999999989,null,null,null,122.6,11.199999999999989]
["100471",100471,null,"STK","TS120LAS 200/250 Wandurchführung L500mm","CHF",136.1,"TECHNOSTAR 120 LAS",2.5,0,"J","TS120LAS 200/300 Passage de paroi L500mm","TS120LAS 200/250 Wandurchführung L500mm","TS120LAS 200/250 Pezzo attraversato de pareti",122,1,"DN 200",null,123.7,"550980",null,null,136.1,"100471",12.399999999999991,null,null,null,136.1,12.399999999999991]
["100474",100474,null,"STK","TS120LAS 110/160 80/125 Red.ztr.Wandurchführung ","CHF",155.4,"TECHNOSTAR 120 LAS",0.3,0,"J","TS120LAS 110/160 80/125 redu. ztr.passage de paroi","TS120LAS 110/160 80/125 Red.ztr.Wandurchführung ","TS120 LAS 110/160 80/12 Reduzione attraversato muro",122,1,"DN 110",null,141.19999999999999,"553115",null,null,155.4,"100474",14.200000000000017,null,null,null,155.4,14.200000000000017,155.4,155.38945888966967]
["100483",100483,null,"STK","TS120LAS 125/185 Dachdurchführ.L1000mm ü Dach sw","CHF",482.8,"TECHNOSTAR 120",1.6,0,"J","TS120LAS 125/185 Passage de Troit. PE noir L1000 ","TS120LAS 125/185 Dachdurchführ.L1000mm ü Dach sw","TS120LAS 125/185 Attraversare tetto nero L1000 ",121,1,"DN 125",null,438.9,"511082",null,null,482.8,"100483",43.900000000000034,null,null,null,482.8,43.900000000000034]
["100487",100487,null,"STK","TS120LAS 80/125 Rohr L250mm geschlitzt weiss","CHF",85.2,"TECHNOSTAR 120",0.15,0,"J","TS120LAS 80/125 Tube fendu L250mm blanc","TS120LAS 80/125 Rohr L250mm geschlitzt weiss","TS120LAS 80/125 Tubo scanalato L 250 bianco",121,1,"DN 80",null,77.400000000000006,"598094",null,null,85.2,"100487",7.7999999999999972,null,null,null,85.2,7.7999999999999972]
["100497",100497,null,"STK","TS120 200 Zentrierhalter Typ 65","CHF",68.8,"TECHNOSTAR 120",0.3,0,"J","TS120 200 Collier de centrage Type  65","TS120 200 Zentrierhalter Typ 65","TS120 80 Distanzatori typ 65 Inox",121,1,"DN 200",null,62.5,"513018",null,null,68.8,"100497",6.2999999999999972,null,null,null,68.8,6.2999999999999972]
["100502",100502,null,"STK","TS120 122 Bride Bridex zu Abstandhalter","CHF",18.7,"TECHNOSTAR 120",0.1,0,"J","TS120 122 Bride Bridex pour collier centrage","TS120 122 Bride Bridex zu Abstandhalter","TS120 122 Sposa Bridex per distanzatori",121,1,"DN 110",null,17,"513050",null,null,18.7,"100502",1.6999999999999993,null,null,null,18.7,1.6999999999999993]
["100506",100506,null,"STK","TS120 160 Bride Bridex zu Abstandhalter","CHF",21.6,"TECHNOSTAR 120",0.01,0,"J","TS120 160 Bride Bridex pour collier centrage","TS120 160 Bride Bridex zu Abstandhalter","TS120 160 Sposa Bridex per distanzatori",121,1,"DN 160",null,19.600000000000001,"513003",null,null,21.6,"100506",2,null,null,null,21.6,2]
["100510",100510,null,"STK","TS120 Bügel Typ 100 zu Abstandhalter","CHF",8.1,"TECHNOSTAR 120",0.02,0,"J","TS120 étrier Ttype 100  pour collier centrage","TS120 Bügel Typ 100 zu Abstandhalter","TS120 Staffa Typ 100 per distanzatori",121,1,"TS ZBH",null,7,"513021",null,null,8.1,"100510",1.0999999999999996,null,null,null,8.1,1.0999999999999996]
["100511",100511,null,"STK","TS120 110 Flanschteil m Nut ","CHF",21.6,"TECHNOSTAR 120",0.45,0,"J",null,"TS120 110 Flanschteil m Nut ",null,121,1,"DN 110",null,19.600000000000001,"500048",null,null,21.6,"100511",2,null,null,null,21.6,2]
["100515",100515,null,"STK","TS120 125 Flanschteil ohne Nut ","CHF",28.4,"TECHNOSTAR 120",0.45,0,"J",null,"TS120 125 Flanschteil ohne Nut ",null,121,1,"DN 125",null,25.8,"500052",null,null,28.4,"100515",2.5999999999999979,null,null,null,28.4,2.5999999999999979]
["100523",100523,null,"STK","TS120 125/110 Spannbriede zu Flanschverbindung","CHF",45.4,"TECHNOSTAR 120",0.1,0,"J",null,"TS120 125/110 Spannbriede zu Flanschverbindung",null,121,1,"DN 110",null,41.2,"513010",null,null,45.4,"100523",4.1999999999999957,null,null,null,45.4,4.1999999999999957]
["100526",100526,null,"STK","TS120 250 Flanschverbindung geschraubt","CHF",241.7,"TECHNOSTAR 120",0.6,0,"J","TS120 250 Raccordement à bride ","TS120 250 Flanschverbindung geschraubt","TS120 250 Manicotto flangiato ",121,1,"DN 250",null,219.7,"500059",null,null,241.7,"100526",22,null,null,null,241.7,22]
["100529",100529,null,"STK","TS120 160 Kesselanschluss für GB312","CHF",325.2,"TECHNOSTAR 120",0.6,0,"J","TS120 160 Raccordement pour GB312","TS120 160 Kesselanschluss für GB312","TS120 160 Raccordemento per GB312",121,1,"DN 160",null,295.60000000000002,"562232",null,null,325.2,"100529",29.599999999999966,null,null,null,325.2,29.599999999999966]
["100533",100533,null,"STK","TS120LAS 80/125  Trennstück auf 2x80mm","CHF",421.7,"TECHNOSTAR 120",0.5,0,"J","TS120LAS 80/125 Separateur to 2 x 80mm","TS120LAS 80/125  Trennstück auf 2x80mm","TS120LAS 80/125 Separatore to 2 x 80mm",121,1,"DN 80",null,383.3,"510008",null,null,421.7,"100533",38.399999999999977,null,null,null,421.7,38.399999999999977]
["100538",100538,null,"STK","TS120 80 Rohrset 5x2000mm","CHF",244.4,"TECHNOSTAR 120",7,0,"J","TS120 80 Set du tube  5x2000mm ","TS120 80 Rohrset 5x2000mm","TS120 80 Set tubo  5x2000mm ",121,1,"DN 80",null,222.1,"554596",null,null,244.4,"100538",22.300000000000011,null,null,null,244.4,22.300000000000011]
["100542",100542,null,"STK","TS120 80 Bausatz GA onhne Kesselnaschluss","CHF",358.2,"TECHNOSTAR 120",8,0,"J","TS120 80 Set GA sans raccordement","TS120 80 Bausatz GA onhne Kesselnaschluss","TS120 80 Set GA senza raccordemento",121,1,"DN 80",null,325.60000000000002,"554032",null,null,358.2,"100542",32.599999999999966,null,null,null,358.2,32.599999999999966]
["100543",100543,null,"STK","TS120 80/110 Bausatz GA ohne Kesselnaschluss","CHF",651.70000000000005,"TECHNOSTAR 120",12,0,"J","TS120 80/110 Set GA sans raccordement","TS120 80/110 Bausatz GA ohne Kesselnaschluss","TS120 80/110 Set GA senza raccordemento",121,1,"DN 80",null,592.4,"554527",null,null,651.70000000000005,"100543",59.300000000000068,null,null,null,651.70000000000005,59.300000000000068]
["100547",100547,null,"STK","TS120LAS 110/160 Bausatz GA-K ohne Kesselan. ","CHF",826.9,"TECHNOSTAR 120",7.7,0,"J","TS120LAS 110/160 Set GAF-K sans raccordement ","TS120LAS 110/160 Bausatz GA-K ohne Kesselan. ","TS120LAS 110/160 Set GAF-K senza raccordemento ",121,1,"DN 110",null,751.7,"554494",null,null,826.9,"100547",75.199999999999932,null,null,null,826.9,75.199999999999932]
["100560",100560,null,"STK","TS120 80/110 Grundbausatz PP1.1DV51722 80/110","CHF",355.9,"TECHNOSTAR 120",20,0,"J","TS120 80/110 Set de base  PP1.180/110 DV51722 ","TS120 80/110 Grundbausatz PP1.1DV51722 80/110","TS120 80/110 Set di base  PP1.180/110 DV51722 ",121,1,"DN 80",null,323.5,"568082",null,null,355.9,"100560",32.399999999999977,null,null,null,355.9,32.399999999999977]
["100568",100568,null,"STK","TS120 80 Grundbausatz PP1 DN80 DV51721","CHF",461.2,"TECHNOSTAR 120",20,0,"J","TS120 80 Set de base PP1 DN80 DV51721","TS120 80 Grundbausatz PP1 DN80 DV51721","TS120 80 Set di base PP1 DN80 DV51721",121,1,"DN 80",null,419.2,"568080",null,null,461.2,"100568",42,null,null,null,461.2,42]
["100570",100570,null,"STK","TS120 80 Grundbausatz PP2 DV51725","CHF",494.2,"TECHNOSTAR 120",20,0,"J","TS120 80 Set de base PP2 DV51725","TS120 80 Grundbausatz PP2 DV51725","TS120 80 Set di base PP2 DV51725",121,1,"DN 80",null,449.2,"568085",null,null,494.2,"100570",45,null,null,null,494.2,45]
["100574",100574,null,"STK","TS120 80 Bausatz ÜB-Flex 12500mm","CHF",852,"TECHNOSTAR 120",11,0,"J","TS120 80 Set de ÜB-Flex 12500mm","TS120 80 Bausatz ÜB-Flex 12500mm","TS120 80 Set  ÜB-Flex 12500mm",121,1,"DN 80",null,774.5,"554036",null,null,852,"100574",77.5,null,null,null,852,77.5]
["100662",100662,null,"STK","PPL 100 Einlegering F60 zu Deckenanfängerset","CHF",123,"Schiedel PRIMA PLUS",0.05,0,"J","PPL 100 Anneau d'insertion à F60 plafond ","PPL 100 Einlegering F60 zu Deckenanfängerset","PPL 150 anello di inserimento F60 ",131,1,"DN 100",null,106.7,"265800410",null,null,123,"100662",16.299999999999997,null,null,null,123,16.299999999999997]
["100665",100665,null,"STK","PPL 180 Einlegering F60 zu Deckenanfängerset","CHF",123,"Schiedel PRIMA PLUS",0.08,0,"J","PPL 180 Anneau d'insertion à F60 plafond ","PPL 180 Einlegering F60 zu Deckenanfängerset","PPL 150 anello di inserimento F60 ",131,1,"DN 180",null,106.7,"265800418",null,null,123,"100665",16.299999999999997,null,null,null,123,16.299999999999997]
["100666",100666,null,"STK","PPL 200 Einlegering F60 zu Deckenanfängerset","CHF",151,"Schiedel PRIMA PLUS",0.09,0,"J","PPL 200 Anneau d'insertion à F60 plafond ","PPL 200 Einlegering F60 zu Deckenanfängerset","PPL 150 anello di inserimento F60 ",131,1,"DN 200",null,130.9,"265800420",null,null,151,"100666",20.099999999999994,null,null,null,151,20.099999999999994]
["100670",100670,null,"STK","PPL 130 Doppelfutter zu Deckenanfängerset","CHF",216,"Schiedel PRIMA PLUS",0.4,0,"J","PPL 130 Manchon double pour set débutant ","PPL 130 Doppelfutter zu Deckenanfängerset","PPL 130 Parete doppia per set di copertura ",131,1,"DN 130",null,187,"265800313",null,null,216,"100670",29,null,null,null,216,29]
["100675",100675,null,"STK","PPL 300 Doppelfutter zu Deckenanfängerset","CHF",355,"Schiedel PRIMA PLUS",1.4,0,"J","PPL 300 Manchon double pour set débutant ","PPL 300 Doppelfutter zu Deckenanfängerset","PPL 300 Parete doppia per set di copertura ",131,1,"DN 300",null,308,"265800330",null,null,355,"100675",47,null,null,null,355,47]
["100678",100678,null,"STK","PPL 150 Einlegehülse zu Deckenanfängerset","CHF",81,"Schiedel PRIMA PLUS",1.2,0,"J","PPL 150 insert disk 0 ° à Starter plafond fixé ","PPL 150 Einlegehülse zu Deckenanfängerset","PPL 150  insert disk da 0 ° a soffitto Starter Set ",131,1,"DN 150",null,70.400000000000006,"265800115",null,null,81,"100678",10.599999999999994,null,null,null,81,10.599999999999994]
["100680",100680,null,"STK","PPL 200 Einlegehülse zu Deckenanfängerset","CHF",97,"Schiedel PRIMA PLUS",1.5,0,"J","PPL 200 insert disk 0 ° à Starter plafond fixé ","PPL 200 Einlegehülse zu Deckenanfängerset","PPL 200  insert disk da 0 ° a soffitto Starter Set ",131,1,"DN 200",null,83.6,"265800120",null,null,97,"100680",13.400000000000006,null,null,null,97,13.400000000000006]
["100686",100686,null,"STK","PPL 180 Einlegehülse 45° zu Deckenanfängerset","CHF",179,"Schiedel PRIMA PLUS",1.7,0,"J","PPL 180 insert disk 45 ° à Starter plafond fixé ","PPL 180 Einlegehülse 45° zu Deckenanfängerset","PPL 180  insert disk da 45° soffitto Starter Set ",131,1,"DN 180",null,155.1,"265800218",null,null,179,"100686",23.900000000000006,null,null,null,179,23.900000000000006]
["100689",100689,null,"STK","PPL 300 Einlegehülse 45° zu Deckenanfängerset","CHF",233,"Schiedel PRIMA PLUS",2.1,0,"J","PPL 300 insert disk 45 ° à Starter plafond fixé ","PPL 300 Einlegehülse 45° zu Deckenanfängerset","PPL 300  insert disk da 45° soffitto Starter Set ",131,1,"DN 300",null,202.4,"265800230",null,null,233,"100689",30.599999999999994,null,null,null,233,30.599999999999994]
["100693",100693,null,"STK","PPL 150 Dämmschale zu Deckenanfängerset L1000mm","CHF",53.3,"Schiedel PRIMA PLUS",1.5,0,"J","PPL 150 Coquille d'isollation pour plafond L1000mm","PPL 150 Dämmschale zu Deckenanfängerset L1000mm","PPL 150 Coppella per soffito starter set L1000mm",131,1,"DN 150",null,45.1,0,null,null,53.3,"100693",8.1999999999999957,null,null,null,53.3,8.1999999999999957]
["100694",100694,null,"STK","PPL 180 Dämmschale zu Deckenanfängerset L1000mm","CHF",58.5,"Schiedel PRIMA PLUS",1.6,0,"J","PPL 180 Coquille d'isollation pour plafond L1000mm","PPL 180 Dämmschale zu Deckenanfängerset L1000mm","PPL 180 Coppella per soffito starter set L1000mm",131,1,"DN 180",null,49.5,0,null,null,58.5,"100694",9,null,null,null,58.5,9]
["100722",100722,null,"STK","PPL 100 Anschluss-Doppelfutter zu Basiselement ","CHF",109,"Schiedel PRIMA PLUS",0.49,0,"J","PPL 100 Raccord double manchon pour elém. base ","PPL 100 Anschluss-Doppelfutter zu Basiselement ","PPL 100 Raccordo doppia parete per elem.basamento ",131,1,"DN 100",null,94.6,"242001010","103510","4037494508817",109,"100722",14.400000000000006,null,null,null,109,14.400000000000006]
["101132",101132,null,"STK","PPL 300 Erweiterung DN350 L150mm","CHF",192,"Schiedel PRIMA PLUS",1.7,0,"J","PPL 300 extension de diamètre DN350 L150mm","PPL 300 Erweiterung DN350 L150mm","PPL 300 Estensione di diametro DN350 L150mm",131,1,"DN 300",null,166.1,"267253035","101812","4037494498613",192,"101132",25.900000000000006,null,null,null,192,25.900000000000006]
["101135",101135,null,"STK","PPL 450 Erweiterung DN500 L150mm","CHF",342,"Schiedel PRIMA PLUS",3,0,"J","PPL 450 extension de diamètre DN500 L150mm","PPL 450 Erweiterung DN500 L150mm","PPL 450 Estensione di diametro DN500 L150mm",131,1,"DN 450",null,297,"267254550",null,null,342,"101135",45,null,null,null,342,45]
["101140",101140,null,"STK","PPL 150 Reduktion  DN80 L150mm","CHF",109,"Schiedel PRIMA PLUS",0.1,0,"J","PPL 150 Réduction de diamètre  DN80 L150mm","PPL 150 Reduktion  DN80 L150mm","PPL 150 riduzione di diametro  DN80 L150mm",131,1,"DN 150",null,94.6,"267201508",null,null,109,"101140",14.400000000000006,null,null,null,109,14.400000000000006]
["101151",101151,null,"STK","PPL 400 Reduktion  DN350 L150mm","CHF",205,"Schiedel PRIMA PLUS",1.9,0,"J","PPL 400 Réduction de diamètre  DN350 L150mm","PPL 400 Reduktion  DN350 L150mm","PPL 400 riduzione di diametro  DN350 L150mm",131,1,"DN 400",null,178.2,"267204035",null,null,205,"101151",26.800000000000011,null,null,null,205,26.800000000000011]
["101189",101189,null,"STK","PPL 230 Anschlussrosette ØA 400mm","CHF",75,"Schiedel PRIMA PLUS",1,0,"J","PPL 230 Rosace de raccordement ØA 400mm","PPL 230 Anschlussrosette ØA 400mm","PPL 230 Rosetta del muro per tubo singolo ØA 400mm",131,1,"DN 180",null,64.900000000000006,"025620023",null,null,75,"101189",10.099999999999994,null,null,null,75,10.099999999999994]
["101230",101230,null,"STK","PPL 600 Wandhalter verstellbar 75 - 300mm DN600mm","CHF",300,"Schiedel PRIMA PLUS",5,0,"J","PPL 600 Fixation murale régl. 75 - 300mm DN600mm","PPL 600 Wandhalter verstellbar 75 - 300mm DN600mm","PPL 600 Collare a muro regolabile 75-300mm DN600mm",131,1,"DN 600",null,260.7,"95960600",null,null,300,"101230",39.300000000000011,null,null,null,300,39.300000000000011]
["101232",101232,null,"STK","PPL 700 Wandhalter verstellbar 75 - 300mm DN700mm","CHF",356,"Schiedel PRIMA PLUS",6,0,"J","PPL 700 Fixation murale régl. 75 - 300mm DN700mm","PPL 700 Wandhalter verstellbar 75 - 300mm DN700mm","PPL 700 Collare a muro regolabile 75-300mm DN700mm",131,1,"DN 700",null,309.10000000000002,"95960700",null,null,356,"101232",46.899999999999977,null,null,null,356,46.899999999999977]
["101332",101332,null,"STK","PPL 450 Dämmschale 30mm Alu-Kaschiert L1000mm","CHF",127.6,"Zubehör",0,0,"J","PPL 450 Coquille d'isol. 30mm Alu-laine de pierre","PPL 450 Dämmschale 30mm Alu-Kaschiert L1000mm","PPL 450 Coppella 30mm lana di roccia alu L1000mm",15,2,"DN 450",null,108.1,0,null,null,127.6,"101332",19.5,null,null,null,127.6,19.5]
["101336",101336,null,"STK","PPL 100 Dämmschale 50mm Alu-Kaschiert L1000mm","CHF",55.6,"Zubehör",1.7,0,"J","PPL 100 Coquille d'isol. 50mm Alu-laine de pierre","PPL 100 Dämmschale 50mm Alu-Kaschiert L1000mm","PPL 100 Coppella 50mm lana di roccia alu L1000mm",15,2,"DN 100",null,47.1,"4009610",null,null,55.6,"101336",8.5,null,null,null,55.6,8.5]
["101341",101341,null,"STK","PPL 250 Dämmschale 50mm Alu-Kaschiert L1000mm","CHF",89.8,"Zubehör",3.5,0,"J","PPL 250 Coquille d'isol. 50mm Alu-laine de pierre","PPL 250 Dämmschale 50mm Alu-Kaschiert L1000mm","PPL 250 Coppella 50mm lana di roccia alu L1000mm",15,2,"DN 250",null,76.099999999999994,"4009625",null,null,89.8,"101341",13.700000000000003,null,null,null,89.8,13.700000000000003]
["101343",101343,null,"STK","PPL 350 Dämmschale 50mm Alu-Kaschiert L1000mm","CHF",111.1,"Zubehör",5,0,"J","PPL 350 Coquille d'isol. 50mm Alu-laine de pierre","PPL 350 Dämmschale 50mm Alu-Kaschiert L1000mm","PPL 350 Coppella 50mm lana di roccia alu L1000mm",15,2,"DN 350",null,94.1,"4009635",null,null,111.1,"101343",17,null,null,null,111.1,17]
["101346",101346,null,"STK","PPL 500 Dämmschale 50mm Alu-Kaschiert L1000mm","CHF",190.1,"Zubehör",0,0,"J","PPL 500 Coquille d'isol. 50mm Alu-laine de pierre","PPL 500 Dämmschale 50mm Alu-Kaschiert L1000mm","PPL 500 Coppella 50mm lana di roccia alu L1000mm",15,2,"DN 500",null,161.1,0,null,null,190.1,"101346",29,null,null,null,190.1,29]
["101393",101393,null,"STK","CHI 300 Aufhängeschelle zu Flex","CHF",54,"Schiedel CHIMFLEX",2,0,"J","CHI 300 Bride pour suspendre le flex","CHI 300 Aufhängeschelle zu Flex","CHI 300 Collare per montagio fessibile",132,1,"DN 300",null,46.2,"D4003300",null,null,54,"101393",7.7999999999999972,null,null,null,54,7.7999999999999972]
[{"$f":"B3869&\"\"","v":"102430"},102430,null,"STK",{"$f":"IF($E$200=2,L3869,IF($E$200=3,N3869,M3869))","v":"ICM 300 Anschlussrosette EW Øi 350mm ØA 520mm"},"CHF",{"$f":"IF($L$190=1,W3869,S3869)","v":70},"Schiedel ICM matt",1.2,0,"J","ICM 300 Rosace de raccordement EW Øi350mm ØA 520mm","ICM 300 Anschlussrosette EW Øi 350mm ØA 520mm","ICM 300 Rosetta collegamento EW Øi 350mm ØA 520mm",134,1,"DN 300",null,60.5,"025620035M",null,null,70,"102430",9.5,null,null,null,70,9.5]
["103158",103158,null,"STK","ICM5000 80 Mündungsabschluss","CHF",89,"Schiedel ICM5000",1.6,0,"J","ICM5000 80 Cape de finition conique","ICM5000 80 Mündungsabschluss","ICM5000 80 Terminale conico",136,1,"DN 80",null,77,0,null,null,89,"103158",12,null,null,null,89,12]
["103162",103162,null,"STK","ICM5000 180 Mündungsabschluss","CHF",111,"Schiedel ICM5000",3,0,"J","ICM5000 180 Cape de finition conique","ICM5000 180 Mündungsabschluss","ICM5000 180 Terminale conico",136,1,"DN 180",null,95.7,0,null,null,111,"103162",15.299999999999997,null,null,null,111,15.299999999999997]
["103167",103167,null,"STK","ICM5000 400 Mündungsabschluss","CHF",255,"Schiedel ICM5000",6.5,0,"J","ICM5000 400 Cape de finition conique","ICM5000 400 Mündungsabschluss","ICM5000 400 Terminale conico",136,1,"DN 400",null,221.1,0,null,null,255,"103167",33.900000000000006,null,null,null,255,33.900000000000006]
["103170",103170,null,"STK","ICM5000 600 Mündungsabschluss","CHF",450,"Schiedel ICM5000",9,0,"J","ICM5000 600 Cape de finition conique","ICM5000 600 Mündungsabschluss","ICM5000 600 Terminale conico",136,1,"DN 600",null,390.5,0,null,null,450,"103170",59.5,null,null,null,450,59.5]
["103269",103269,null,"STK","KRS 250 Grundplatte mit Russtopf","CHF",342,"Schiedel KERASTAR",10.5,0,"J","KRS 250 Plaque de base avec pot à suie","KRS 250 Grundplatte mit Russtopf","KRS 250 Piastra base e bentola fuliggine",137,1,"DN 250",null,297,"265702625",null,null,342,"103269",45,null,null,null,342,45]
["103282",103282,null,"STK","KRS 300  Revisionselement kond.  Betrieb L665mm ","CHF",1108,"Schiedel KERASTAR",25,0,"J","KRS 300  Elément porte d'inspection L665mm ","KRS 300  Revisionselement kond.  Betrieb L665mm ","KRS 300  Elemento con inspezione per com. liquido",137,1,"DN 300",null,963,0,null,null,1108,"103282",145,null,null,null,1108,145]
["103365",103365,null,"STK","KRS 160 Abdeckros.22-26° Dachneigung  ","CHF",35,"Schiedel KERASTAR",0.44,0,"J","KRS 160 Rosace récouvrement.22-26° pente du toit  ","KRS 160 Abdeckros.22-26° Dachneigung  ","KRS 160 Copertina rosa 22-26°  passo ",137,1,"DN 160",null,30,"265702516",null,null,35,"103365",5,null,null,null,35,5]
["103367",103367,null,"STK","KRS 200 Abdeckros.22-26° Dachneigung   ","CHF",57,"Schiedel KERASTAR",0.48,0,"J","KRS 200 Rosace récouvrement.22-26° pente du toit   ","KRS 200 Abdeckros.22-26° Dachneigung   ","KRS 200 Copertina rosa 22-26°  passo  ",137,1,"DN 200",null,49,"265702520",null,null,57,"103367",8,null,null,null,57,8]
["103370",103370,null,"STK","KRS 160 Abdeckros.27-31° Dachneigung  ","CHF",35,"Schiedel KERASTAR",0.44,0,"J","KRS 160 Rosace récouvrement.27-31° pente du toit  ","KRS 160 Abdeckros.27-31° Dachneigung  ","KRS 160 Copertina rosa 27-31°  passo ",137,1,"DN 160",null,30,0,null,null,35,"103370",5,null,null,null,35,5]
["103374",103374,null,"STK","KRS 140 Abdeckros.36-38° Dachneigung  ","CHF",32,"Schiedel KERASTAR",0.42,0,"J","KRS 140 Rosace récouvrement.36-38° pente du toit  ","KRS 140 Abdeckros.36-38° Dachneigung  ","KRS 140 Copertina rosa 36-38°  passo ",137,1,"DN 140",null,27,0,null,null,32,"103374",5,null,null,null,32,5]
["103378",103378,null,"STK","KRS 250 Abdeckros.36-38° Dachneigung  ","CHF",50,"Schiedel KERASTAR",0.52,0,"J","KRS 250 Rosace récouvrement.36-38° pente du toit  ","KRS 250 Abdeckros.36-38° Dachneigung  ","KRS 250 Copertina rosa 36-38°  passo ",137,1,"DN 250",null,43,0,null,null,50,"103378",7,null,null,null,50,7]
["103409",103409,null,"STK","KRS 550 Wandhalt.statisch 50mm","CHF",166,"Schiedel KERASTAR",3.5,0,"J","KRS 550 Fixation murale statique 50mm","KRS 550 Wandhalt.statisch 50mm","KRS 550 Collare a muro 50mm statico 50mm",137,1,"DN 400",null,144,0,null,null,166,"103409",22,null,null,null,166,22]
["103411",103411,null,"STK","KRS L2 ZBE Verläng.f.Wandhalt. 452mm","CHF",101.4,"Schiedel KERASTAR",0.95,0,"J","KRS L2 ZBE Rallonge pour fixation murale 452mm","KRS L2 ZBE Verläng.f.Wandhalt. 452mm","KRS L2 ZBE Verläng.f.Wandhalt. 452mm",137,1,"ZBH Kerastar",null,88,0,null,null,101.4,"103411",13.400000000000006,null,null,null,101.4,13.400000000000006,101.4,101.44444444444444]
["103487",103487,null,"STK","KER 250 T-Stück 90° L330mm Stutzen L90mm","CHF",302.89999999999998,"Schiedel KERASTAR",4,0,"J","KER 250 Pièce Té 90° L330mm raccord L90mm","KER 250 T-Stück 90° L330mm Stutzen L90mm","KER 250 Pezzo T 90° L330mm raccordo L90mm",137,1,"DN 250",null,263,"KT25",null,null,302.89999999999998,"103487",39.899999999999977,null,null,null,302.89999999999998,39.899999999999977,302.89999999999998,302.88114754098359]
["103554",103554,null,"STK","KER 100 Adapter für Doppelfutter 100mm","CHF",18,"Schiedel KERANOVA",0.16,0,"J","KER 100 adapteur pour manchon doubler 100mm","KER 100 Adapter für Doppelfutter 100mm","KER 100 Adattore per doppia parete 100mm",113,1,"ZBH Keranova",null,15,"KAD1010",null,null,18,"103554",3,null,null,null,18,3]
["103582",103582,null,"STK","KER 160 Zentrierhalter Typ 65","CHF",27,"Schiedel KERANOVA",0.8,0,"J","KER 160 Distanceurs Typ 65","KER 160 Zentrierhalter Typ 65","KER 160 Distanzatori tipo 65",113,1,"DN 160",null,23,"KSAB1665",null,null,27,"103582",4,null,null,null,27,4]
["103583",103583,null,"STK","KER 180 Zentrierhalter Typ 65","CHF",29,"Schiedel KERANOVA",0.8,0,"J","KER 180 Distanceurs Typ 65","KER 180 Zentrierhalter Typ 65","KER 180 Distanzatori tipo 65",113,1,"DN 180",null,25,"KSAB1865",null,null,29,"103583",4,null,null,null,29,4]
["103587",103587,null,"STK","KER 160 Zentrierhalter Typ 100","CHF",27,"Schiedel KERANOVA",0.8,0,"J","KER 160 Distanceurs Typ 100","KER 160 Zentrierhalter Typ 100","KER 160 Distanzatori tipo 100",113,1,"DN 160",null,23,"KSAB16100",null,null,27,"103587",4,null,null,null,27,4]
["103591",103591,null,"STK","KER 175 Briede Bridex für KER Abstandhalter Ø160","CHF",12,"Schiedel KERANOVA",0.01,0,"J",null,"KER 175 Briede Bridex für KER Abstandhalter Ø160",null,113,1,"ZBH Keranova",null,10,"513210",null,null,12,"103591",2,null,null,null,12,2]
["103600",103600,null,"STK","KER 120 Mauerschelle","CHF",18,"Schiedel KERANOVA",0.5,0,"J","KER 120 Collier pour fixation au mur","KER 120 Mauerschelle","KER 120 Fascetta per parete",113,1,"DN 120",null,15,"265500204","103610","4037494131435",18,"103600",3,null,null,null,18,3]
["103623",103623,null,"STK","KER 300-400 Versetzzange ","CHF",1683,"Schiedel KERANOVA",6.6,0,"J","KER 300-400 Pince à poser réglable  ","KER 300-400 Versetzzange ","KER 300-400 Pinza regolabile",113,1,"ZBH Keranova",null,1463,"411001",null,null,1683,"103623",220,null,null,null,1683,220]
["103630",103630,null,"STK","ISOLIT 200 Doppelelzügerelement 20/20","CHF",133,"ISOLIT",72.5,0,"J","ISOLIT 200 Elément double 20","ISOLIT 200 Doppelelzügerelement 20/20","ISOLIT 200 Elemento doppia 20",114,1,"DN 200",null,115,"300006",null,null,133,"103630",18,null,null,null,133,18]
["103633",103633,null,"STK","ISOLIT 160 Isolation zu Anfänger 16","CHF",12,"ISOLIT",0.4,0,"J","ISOLIT 160 Isolation pour les débutants 16","ISOLIT 160 Isolation zu Anfänger 16","ISOLIT 160 Isolamento per principianti 16",114,1,"DN 160",null,10,"301004",null,null,12,"103633",2,null,null,null,12,2]
["103635",103635,null,"STK","ISOLIT 250 Isolation zu Anfänger 25","CHF",14,"ISOLIT",0.8,0,"J","ISOLIT 250 Isolation pour les débutants 25","ISOLIT 250 Isolation zu Anfänger 25","ISOLIT 250 Isolamento per principianti 25",114,1,"DN 250",null,12,"301006",null,null,14,"103635",2,null,null,null,14,2]
["103645",103645,null,"STK","ISOLIT 300 Rauchrohranschlusselement RA 30/20/90°","CHF",375,"ISOLIT",120,0,"J","ISOLIT 300 Raccord de conduit de fumée 30/20/ 90°","ISOLIT 300 Rauchrohranschlusselement RA 30/20/90°","ISOLIT 300 Elemento con raccordo 30/20/90°",114,1,"DN 300",null,326,"304021",null,null,375,"103645",49,null,null,null,375,49]
["103655",103655,null,"STK","ISOLIT Russtüre 18/21 Steg","CHF",38,"ISOLIT",0.8,0,"J","ISOLIT Pont pour porte de ramonage 18/21","ISOLIT Russtüre 18/21 Steg","ISOLIT Ponte per portina 18/21",114,1,"ZBH ISOLIT",null,33,"312007",null,null,38,"103655",5,null,null,null,38,5]
["103665",103665,null,"STK","ISOLIT 200 Schleifung doppelzügig 20/20","CHF",1613,"ISOLIT",170,0,"J","ISOLIT 200 déviation double 20","ISOLIT 200 Schleifung doppelzügig 20/20","ISOLIT 200 Deviazione doppia 20",114,1,"DN 200",null,1402,"315059",null,null,1613,"103665",211,null,null,null,1613,211]
["103668",103668,null,"STK","ISOLIT  Abdeckplatte Beton 600 x 920mm ohne Loch","CHF",403,"ISOLIT",60,0,"J","ISOLIT Couverture complète sans trou 600 x 920 ","ISOLIT  Abdeckplatte Beton 600 x 920mm ohne Loch","Isolit Copertura piena 600 x 920mm senza foro",114,1,"DN 200",null,350,"811005",null,null,403,"103668",53,null,null,null,403,53]
["103690",103690,null,"STK","CHZ 200 Anschlusskonus ohne Doppelfutter ","CHF",107.5,"Schiedel CHEMINEE ZUG",30,0,"J","CHZ 200 Cône de racc., sans manchon double ","CHZ 200 Anschlusskonus ohne Doppelfutter ","CHZ 200 Cono di raccordo senza doppia parete",112,1,"DN 200",null,93,"201000",null,null,107.5,"103690",14.5,null,null,null,107.5,14.5,107.5,107.46666666666667]
["103712",103712,null,"STK","CHZ 120-160 Füllstein zu Schnellbaufund. L170mm","CHF",36,"Schiedel CHEMINEE ZUG",5,0,"J","CHZ 120-160 Fondation rapide, socle en supl. L170mm","CHZ 120-160 Füllstein zu Schnellbaufund. L170mm","CHZ 120-160 Basamento supplementare L170mm",112,1,"ZBH CHZ",null,31,"101062",null,null,36,"103712",5,null,null,null,36,5]
["103724",103724,null,"STK","CHZ Mantelstein EZ  600 x 600mm L330mm Ø350mm","CHF",88,"Schiedel CHEMINEE ZUG",64,0,"J","CHZ Elément manteau EZ  600 x 600mm L330mm Ø350mm","CHZ Mantelstein EZ  600 x 600mm L330mm Ø350mm","CHZ Mantello EZ  600 x 600mm L330mm Ø350mm",112,1,"DN 350",null,76,"200005",null,null,88,"103724",12,null,null,null,88,12]
["103731",103731,null,"STK","CHZ Mantelstein DZ 600 x 1140mm L330mm 2xØ350mm","CHF",160,"Schiedel CHEMINEE ZUG",90,0,"J","CHZ Elément manteau DZ 600 x 1140mm L330mm 2xØ350mm","CHZ Mantelstein DZ 600 x 1140mm L330mm 2xØ350mm","CHZ Mantello DZ 600 x 1140mm L330mm 2xØ350mm",112,1,"DZ DN350",null,139,"100030",null,null,160,"103731",21,null,null,null,160,21]
["103737",103737,null,"STK","CHZ 220 Keramikrohr ØA 260mm  L330mm","CHF",34,"Schiedel CHEMINEE ZUG",10.6,0,"J","CHZ 220 Conduit réfractaire ØA 260mm  L330mm","CHZ 220 Keramikrohr ØA 260mm  L330mm","CHZ 220 Condotto refrattario ØA 260mm  L330mm",112,1,"DN 220",null,29,"105016",null,null,34,"103737",5,null,null,null,34,5]
["103743",103743,null,"STK","CHZ 500 Keramikrohr ØA 600mm  L330mm","CHF",157,"Schiedel CHEMINEE ZUG",45.3,0,"J","CHZ 500 Conduit réfractaire ØA 600mm  L330mm","CHZ 500 Keramikrohr ØA 600mm  L330mm","CHZ 500 Condotto refrattario ØA 600mm  L330mm",112,1,"DN 500",null,136,"105024",null,null,157,"103743",21,null,null,null,157,21]
["103783",103783,null,"STK","CHZ 300 Abdeckplatte Beton 780 x 780mm Loch Ø300mm","CHF",239,"Schiedel CHEMINEE ZUG",67,0,"J","CHZ 300 Plaque de réc., bet 780 x 780mm trou 300mm","CHZ 300 Abdeckplatte Beton 780 x 780mm Loch Ø300mm","CHZ 300 Lastra copertura 780 x 780mm foro Ø300mm",112,1,"DN 300",null,207,"811225",null,null,239,"103783",32,null,null,null,239,32]
["103794",103794,null,"STK","CHZ 130 Langdoppelfutter lose L200mm","CHF",241,"Schiedel CHEMINEE ZUG",1,0,"J","CHZ 130 Doublemanchon long, lâche L200mm","CHZ 130 Langdoppelfutter lose L200mm","CHZ 130 Manicoto doppio parete lungo L200mm",112,1,"ZBH CHZ",null,209,"912000",null,null,241,"103794",32,null,null,null,241,32]
["103797",103797,null,"STK","CHZ 200 Langdoppelfutter lose L200mm","CHF",142,"Schiedel CHEMINEE ZUG",1.2,0,"J","CHZ 200 Doublemanchon long, lâche L200mm","CHZ 200 Langdoppelfutter lose L200mm","CHZ 200 Manicoto doppio parete lungo L200mm",112,1,"ZBH CHZ",null,123,"912005",null,null,142,"103797",19,null,null,null,142,19]
["103799",103799,null,"STK","CHZ 300 Langdoppelfutter lose L200mm","CHF",227,"Schiedel CHEMINEE ZUG",2,0,"J","CHZ 300 Doublemanchon long, lâche L200mm","CHZ 300 Langdoppelfutter lose L200mm","CHZ 300 Manicoto doppio parete lungo L200mm",112,1,"ZBH CHZ",null,197,"912007",null,null,227,"103799",30,null,null,null,227,30]
["103814",103814,null,"STK","CHZ 350 Sairlift Inox komplett","CHF",636,"Schiedel CHEMINEE ZUG",8.9,0,"J","CHZ 350 Sairlift Inox complet, ronde","CHZ 350 Sairlift Inox komplett","CHZ 350 Sairlift inox kompletto",112,1,"DN 350",null,553,"909135",null,null,636,"103814",83,null,null,null,636,83]
["103871",103871,null,"STK","ABS Sockelplatte aus Beton EZ 360 x 360mm","CHF",155,"Schiedel ABSOLUT",25,0,"J","ABS Plaque de socle en beton EZ 360 x 360mm","ABS Sockelplatte aus Beton EZ 360 x 360mm","ABS Piastra di base cemento EZ 360 x 360mm",111,1,0,null,134,"1543636",null,null,155,"103871",21,null,null,null,155,21]
["103872",103872,null,"STK","ABS Sockelplatte aus Beton EZ 380 x 380mm","CHF",160,"Schiedel ABSOLUT",25,0,"J","ABS Plaque de socle en beton EZ 380 x 380mm","ABS Sockelplatte aus Beton EZ 380 x 380mm","ABS Piastra di base cemento EZ 380 x 380mm",111,1,0,null,139,"1543838",null,null,160,"103872",21,null,null,null,160,21]
["103882",103882,null,"STK","ABS 140 Grundpaket","CHF",451,"Schiedel ABSOLUT",13.5,0,"J","ABS Paquet de base 14","ABS 140 Grundpaket","ABS Kit di base 14",111,1,"DN 140",null,392,"204010014","100129","4037494153857",451,"103882",59,null,null,null,451,59]
["103893",103893,null,"STK","ABS 250 Fertigfusspaket ","CHF",311,"Schiedel ABSOLUT",16.5,0,"J","ABS 250 Paquet de pied préfabriqué","ABS 250 Fertigfusspaket ","ABS 250 Kit per basamanto prefabbricado",111,1,"DN 250",null,270,"203040025","102065","4037494173459",311,"103893",41,null,null,null,311,41]
["103908",103908,null,"STK","ABS 180 Adapterring von 180mm auf 200mm L90mm","CHF",53,"Schiedel ABSOLUT",2.5,0,"J","ABS 180 Bague d'adapt. de 180mm au 200mm L90mm","ABS 180 Adapterring von 180mm auf 200mm L90mm","ABS 180 Anello di adattamento 180mm su 200mm L90mm",111,1,"DN 180",null,46,"260101820","102219","4037494102480",53,"103908",7,null,null,null,53,7]
["103945",103945,null,"STK","ABS 120 Profilkeramik-Rohr mit Muffe L1330mm","CHF",98,"Schiedel ABSOLUT",7.8,0,"J","ABS 120 Conduit profilé L1330mm","ABS 120 Profilkeramik-Rohr mit Muffe L1330mm","ABS 120 Condotto profilato L1330mm",111,1,"DN 120",null,85,"2080012","100037","4037494057407",98,"103945",13,null,null,null,98,13]
["103952",103952,null,"STK","ABS 160 Profilkeramik-Rohr mit Muffe L660mm","CHF",61,"Schiedel ABSOLUT",5.4,0,"J","ABS 160 Conduit profilé L660mm","ABS 160 Profilkeramik-Rohr mit Muffe L660mm","ABS 160 Condotto profilato L660mm",111,1,"DN 160",null,53,"2090016","100044","4037494057452",61,"103952",8,null,null,null,61,8]
["103958",103958,null,"STK","ABS 120 Profilkeramik-Rohr mit Muffe L330mm","CHF",33,"Schiedel ABSOLUT",2,0,"J","ABS 120 Conduit profilé L330mm","ABS 120 Profilkeramik-Rohr mit Muffe L330mm","ABS 120 Condotto profilato L330mm",111,1,"DN 120",null,28,"2093312",null,null,33,"103958",5,null,null,null,33,5]
["103960",103960,null,"STK","ABS 160 Profilkeramik-Rohr mit Muffe L330mm","CHF",35,"Schiedel ABSOLUT",3,0,"J","ABS 160 Conduit profilé L330mm","ABS 160 Profilkeramik-Rohr mit Muffe L330mm","ABS 160 Condotto profilato L330mm",111,1,"DN 160",null,30,"2093316",null,null,35,"103960",5,null,null,null,35,5]
["103971",103971,null,"STK","ABS 120 PA Formstück L330mm","CHF",126,"Schiedel ABSOLUT",3,0,"J","ABS 120 PA Piece L330mm","ABS 120 PA Formstück L330mm","ABS 120 PA adattamento PA L330mm",111,1,"DN 120",null,109,"235603312","102121","4037494127230",126,"103971",17,null,null,null,126,17]
["103976",103976,null,"STK","ABS 250 PA Formstück L330mm","CHF",328,"Schiedel ABSOLUT",8,0,"J","ABS 250 PA Piece L330mm","ABS 250 PA Formstück L330mm","ABS 250 PA adattamento PA L330mm",111,1,"DN 250",null,285,0,null,null,328,"103976",43,null,null,null,328,43]
["103980",103980,null,"STK","ABS 120 Rauchrohr-Anschlusspaket 90° RA  ","CHF",343,"Schiedel ABSOLUT",11.5,0,"J","ABS 120 Paquet de raccordement 90° RA  ","ABS 120 Rauchrohr-Anschlusspaket 90° RA  ","ABS 120 Kit per raccordo  90° RA  ",111,1,"DN 120",null,298,"2110012","100050","4037494057476",343,"103980",45,null,null,null,343,45]
["103990",103990,null,"STK","ABS 300 Teilesack zu RA-Paket","CHF",255,"Schiedel ABSOLUT",12,0,"J","ABS 300 Sac avec des pieces pour RA-paquet ","ABS 300 Teilesack zu RA-Paket","ABS 300 Set di componenti per kit RA",111,1,"DN 300",null,221,"582030",null,null,255,"103990",34,null,null,null,255,34]
["103992",103992,null,"STK","ABS 120 Rauchrohr-Anschlusspaket 45° RA  ","CHF",343,"Schiedel ABSOLUT",12.5,0,"J","ABS 120 Paquet de raccordement RA 45° RA  ","ABS 120 Rauchrohr-Anschlusspaket 45° RA  ","ABS 120 Kit per raccordo  45° RA  ",111,1,"DN 120",null,298,"2114512",null,null,343,"103992",45,null,null,null,343,45]
["104048",104048,null,"STK","ABS 140 Schleifung EZ 20° auf Bestellung","CHF",1010,"Schiedel ABSOLUT",71,0,"J","ABS 140 Déviation EZ 20° sur commande, 2 angles","ABS 140 Schleifung EZ 20° auf Bestellung","ABS 140 Deviazione EZ 20° su ordinazione",111,1,"DN 140",null,878,0,null,null,1010,"104048",132,null,null,null,1010,132]
[{"$f":"B4061&\"\"","v":"104051"},104051,null,"STK",{"$f":"IF($E$200=2,L4061,IF($E$200=3,N4061,M4061))","v":"ABS 140 Schleifung EZ 35° auf Bestellung"},"CHF",{"$f":"IF($L$190=1,W4061,S4061)","v":1010},"Schiedel ABSOLUT",71,0,"J","ABS 140 Déviation EZ 35° sur commande, 2 angles","ABS 140 Schleifung EZ 35° auf Bestellung","ABS 140 Deviazione EZ 35° su ordinazione",111,1,"DN 140",null,878,0,null,null,1010,"104051",132,null,null,null,1010,132]
["104054",104054,null,"STK","ABS 160 Schleifung EZ 15° auf Bestellung","CHF",1010,"Schiedel ABSOLUT",75,0,"J","ABS 160 Déviation EZ 15° sur commande, 2 angles","ABS 160 Schleifung EZ 15° auf Bestellung","ABS 160 Deviazione EZ 15° su ordinazione",111,1,"DN 160",null,878,0,null,null,1010,"104054",132,null,null,null,1010,132]
["104057",104057,null,"STK","ABS 160 Schleifung EZ 30° auf Bestellung","CHF",1010,"Schiedel ABSOLUT",75,0,"J","ABS 160 Déviation EZ 30° sur commande, 2 angles","ABS 160 Schleifung EZ 30° auf Bestellung","ABS 160 Deviazione EZ 30° su ordinazione",111,1,"DN 160",null,878,0,null,null,1010,"104057",132,null,null,null,1010,132]
["104062",104062,null,"STK","ABS 180 Schleifung EZ 20° auf Bestellung","CHF",1010,"Schiedel ABSOLUT",80,0,"J","ABS 180 Déviation EZ 20° sur commande, 2 angles","ABS 180 Schleifung EZ 20° auf Bestellung","ABS 180 Deviazione EZ 20° su ordinazione",111,1,"DN 180",null,878,0,null,null,1010,"104062",132,null,null,null,1010,132]
["104067",104067,null,"STK","ABS 200 Schleifung EZ 10° auf Bestellung","CHF",1134,"Schiedel ABSOLUT",90,0,"J","ABS 200 Déviation EZ 10° sur commande, 2 angles","ABS 200 Schleifung EZ 10° auf Bestellung","ABS 200 Deviazione EZ 10° su ordinazione",111,1,"DN 200",null,986,0,null,null,1134,"104067",148,null,null,null,1134,148]
["104072",104072,null,"STK","ABS 200 Schleifung EZ 35° auf Bestellung","CHF",1134,"Schiedel ABSOLUT",90,0,"J","ABS 200 Déviation EZ 35° sur commande, 2 angles","ABS 200 Schleifung EZ 35° auf Bestellung","ABS 200 Deviazione EZ 35° su ordinazione",111,1,"DN 200",null,986,0,null,null,1134,"104072",148,null,null,null,1134,148]
["104075",104075,null,"STK","ABS 250 Schleifung EZ 15° auf Bestellung","CHF",1445,"Schiedel ABSOLUT",150,0,"J","ABS 250 Déviation EZ 15° sur commande, 2 angles","ABS 250 Schleifung EZ 15° auf Bestellung","ABS 250 Deviazione EZ 15° su ordinazione",111,1,"DN 250",null,1256,0,null,null,1445,"104075",189,null,null,null,1445,189]
["104077",104077,null,"STK","ABS 250 Schleifung EZ 25° auf Bestellung","CHF",1445,"Schiedel ABSOLUT",150,0,"J","ABS 250 Déviation EZ 25° sur commande, 2 angles","ABS 250 Schleifung EZ 25° auf Bestellung","ABS 250 Deviazione EZ 25° su ordinazione",111,1,"DN 250",null,1256,0,null,null,1445,"104077",189,null,null,null,1445,189]
["104086",104086,null,"STK","ABS 300 Abstandhalter offen zu Schleifung","CHF",51,"Schiedel ABSOLUT",0.2,0,"J","ABS 300 Distanceurs  ouvrir pour deviation","ABS 300 Abstandhalter offen zu Schleifung","ABS 300 Distanzatori aprire per deviazione",111,1,"DN 300",null,44,0,null,null,51,"104086",7,null,null,null,51,7]
["104092",104092,null,"STK","ABS 250 Abstandhalter geschlossen zu Schleifung","CHF",51,"Schiedel ABSOLUT",0.1,0,"J","ABS 250 Distanceurs  ferme pour deviation","ABS 250 Abstandhalter geschlossen zu Schleifung","ABS 250 Distanzatori ciuso per deviazione",111,1,"DN 250",null,44,"256000425","900000383","4049723001037",51,"104092",7,null,null,null,51,7]
["104093",104093,null,"STK","ABS 300 Abstandhalter geschlossen zu Schleifung","CHF",57,"Schiedel ABSOLUT",0.25,0,"J","ABS 300 Distanceurs  ferme pour deviation","ABS 300 Abstandhalter geschlossen zu Schleifung","ABS 300 Distanzatori ciuso per deviazione",111,1,"DN 300",null,49,0,null,null,57,"104093",8,null,null,null,57,8]
["104097",104097,null,"STK","ABS 180 Inox Rohrwinkel 5° zu Schleifung ","CHF",76,"Schiedel ABSOLUT",0.1,0,"J","ABS 180 Coude inox 5° pour déviation absolut","ABS 180 Inox Rohrwinkel 5° zu Schleifung ","ABS 180 Gomito inox 5° per deviazione absolut",111,1,"DN 180",null,66,"257000518",null,null,76,"104097",10,null,null,null,76,10]
["104101",104101,null,"STK","ABS 400 Inox Rohrwinkel 5° zu Schleifung ","CHF",186,"Schiedel ABSOLUT",0.1,0,"J","ABS 400 Coude inox 5° pour déviation absolut","ABS 400 Inox Rohrwinkel 5° zu Schleifung ","ABS 400 Gomito inox 5° per deviazione absolut",111,1,"DN 400",null,161,0,null,null,186,"104101",25,null,null,null,186,25]
["104105",104105,null,"STK","ABS 200 Inox Rohrwinkel 10° zu Schleifung ","CHF",82,"Schiedel ABSOLUT",0.1,0,"J","ABS 200 Coude inox 10° pour déviation absolut","ABS 200 Inox Rohrwinkel 10° zu Schleifung ","ABS 200 Gomito inox 10° per deviazione absolut",111,1,"DN 200",null,71,"257001020",null,null,82,"104105",11,null,null,null,82,11]
["104106",104106,null,"STK","ABS 250 Inox Rohrwinkel 10° zu Schleifung ","CHF",94,"Schiedel ABSOLUT",0.1,0,"J","ABS 250 Coude inox 10° pour déviation absolut","ABS 250 Inox Rohrwinkel 10° zu Schleifung ","ABS 250 Gomito inox 10° per deviazione absolut",111,1,"DN 250",null,81,"257001025",null,null,94,"104106",13,null,null,null,94,13]
["104112",104112,null,"STK","ABS 200 Inox Rohrwinkel 15° zu Schleifung ","CHF",82,"Schiedel ABSOLUT",0.1,0,"J","ABS 200 Coude inox 15° pour déviation absolut","ABS 200 Inox Rohrwinkel 15° zu Schleifung ","ABS 200 Gomito inox 15° per deviazione absolut",111,1,"DN 200",null,71,"257001520",null,null,82,"104112",11,null,null,null,82,11]
["104115",104115,null,"STK","ABS 400 Inox Rohrwinkel 15° zu Schleifung ","CHF",186,"Schiedel ABSOLUT",0.15,0,"J","ABS 400 Coude inox 15° pour déviation absolut","ABS 400 Inox Rohrwinkel 15° zu Schleifung ","ABS 400 Gomito inox 15° per deviazione absolut",111,1,"DN 400",null,161,0,null,null,186,"104115",25,null,null,null,186,25]
["104117",104117,null,"STK","ABS 160 Inox Rohrwinkel 20° zu Schleifung ","CHF",69,"Schiedel ABSOLUT",0.1,0,"J","ABS 160 Coude inox 20° pour déviation absolut","ABS 160 Inox Rohrwinkel 20° zu Schleifung ","ABS 160 Gomito inox 20° per deviazione absolut",111,1,"DN 160",null,60,"257002016",null,null,69,"104117",9,null,null,null,69,9]
["104120",104120,null,"STK","ABS 250 Inox Rohrwinkel 20° zu Schleifung ","CHF",94,"Schiedel ABSOLUT",0.1,0,"J","ABS 250 Coude inox 20° pour déviation absolut","ABS 250 Inox Rohrwinkel 20° zu Schleifung ","ABS 250 Gomito inox 20° per deviazione absolut",111,1,"DN 250",null,81,"257002025",null,null,94,"104120",13,null,null,null,94,13]
["104125",104125,null,"STK","ABS 180 Inox Rohrwinkel 25° zu Schleifung ","CHF",76,"Schiedel ABSOLUT",0.1,0,"J","ABS 180 Coude inox 25° pour déviation absolut","ABS 180 Inox Rohrwinkel 25° zu Schleifung ","ABS 180 Gomito inox 25° per deviazione absolut",111,1,"DN 180",null,66,"257002518",null,null,76,"104125",10,null,null,null,76,10]
["104129",104129,null,"STK","ABS 400 Inox Rohrwinkel 25° zu Schleifung ","CHF",186,"Schiedel ABSOLUT",0.15,0,"J","ABS 400 Coude inox 25° pour déviation absolut","ABS 400 Inox Rohrwinkel 25° zu Schleifung ","ABS 400 Gomito inox 25° per deviazione absolut",111,1,"DN 400",null,161,0,null,null,186,"104129",25,null,null,null,186,25]
["104133",104133,null,"STK","ABS 200 Inox Rohrwinkel 30° zu Schleifung ","CHF",82,"Schiedel ABSOLUT",0.1,0,"J","ABS 200 Coude inox 30° pour déviation absolut","ABS 200 Inox Rohrwinkel 30° zu Schleifung ","ABS 200 Gomito inox 30° per deviazione absolut",111,1,"DN 200",null,71,"257003020",null,null,82,"104133",11,null,null,null,82,11]
["104134",104134,null,"STK","ABS 250 Inox Rohrwinkel 30° zu Schleifung ","CHF",94,"Schiedel ABSOLUT",0.1,0,"J","ABS 250 Coude inox 30° pour déviation absolut","ABS 250 Inox Rohrwinkel 30° zu Schleifung ","ABS 250 Gomito inox 30° per deviazione absolut",111,1,"DN 250",null,81,"257003025",null,null,94,"104134",13,null,null,null,94,13]
["104140",104140,null,"STK","ABS 200 Inox Rohrwinkel 35° zu Schleifung ","CHF",82,"Schiedel ABSOLUT",0.1,0,"J","ABS 200 Coude inox 35° pour déviation absolut","ABS 200 Inox Rohrwinkel 35° zu Schleifung ","ABS 200 Gomito inox 35° per deviazione absolut",111,1,"DN 200",null,71,0,null,null,82,"104140",11,null,null,null,82,11]
["104141",104141,null,"STK","ABS 250 Inox Rohrwinkel 35° zu Schleifung ","CHF",94,"Schiedel ABSOLUT",0.1,0,"J","ABS 250 Coude inox 35° pour déviation absolut","ABS 250 Inox Rohrwinkel 35° zu Schleifung ","ABS 250 Gomito inox 35° per deviazione absolut",111,1,"DN 250",null,81,0,null,null,94,"104141",13,null,null,null,94,13]
["104157",104157,null,"STK","ABS Handyplatte DZTL Faserzement 360 x 830mm ","CHF",221,"Schiedel ABSOLUT",39,0,"J","ABS Plaque Handy DZTL en fibrocement 360 x 830mm ","ABS Handyplatte DZTL Faserzement 360 x 830mm ","ABS Lastra Handy DZTL fibrocemento 360 x 830mm ",111,1,0,null,221,"393683",null,null,221,"104157",0,null,null,null,221,0,221,221]
["104158",104158,null,"STK","ABS Handyplatte EZ Faserzement 380 x 380mm","CHF",153,"Schiedel ABSOLUT",25.7,0,"J","ABS Plaque Handy EZ en fibrocement 380 x 380mm","ABS Handyplatte EZ Faserzement 380 x 380mm","ABS Lastra Handy EZ fibrocemento 380 x 380mm",111,1,0,null,153,"393838",null,null,153,"104158",0,null,null,null,153,0,153,153]
["104168",104168,null,"STK","ABS Zulufthaube zu Faserzementplatte EZTL 250mm","CHF",79,"Schiedel ABSOLUT",0.7,0,"J","ABS Hotte d'entrée d'air pour Handy fibrocement","ABS Zulufthaube zu Faserzementplatte EZTL 250mm","ABS perlufthaube per fibrocementoplatte EZTL 250mm",111,1,0,null,68,"354230025","100226","4037494824559",79,"104168",11,null,null,null,79,11]
["104200",104200,null,"STK","ABS 200 Abströmkonus Inox","CHF",99,"Schiedel ABSOLUT",0.57899999999999996,0,"J","ABS 200 Cône de finition Inox","ABS 200 Abströmkonus Inox","ABS 200 Cono per sbocco inox",111,1,"DN 200",null,86,0,null,null,99,"104200",13,null,null,null,99,13]
["104236",104236,null,"STK","ABS LAS Anschlussrohr Inox Ø100mm L500mm","CHF",73,"Schiedel ABSOLUT",2.5,0,"J","ABS LAS Conduit de raccordement Inox Ø100mm L500mm","ABS LAS Anschlussrohr Inox Ø100mm L500mm","ABS LAS Anschlussrohr Inox Ø100mm L500mm",111,1,"ZBH ABS",null,63,"255040100",null,null,73,"104236",10,null,null,null,73,10]
["104240",104240,null,"STK","ABS Putztüre zu Rauchzugklappe","CHF",241,"Schiedel ABSOLUT",2.5,0,"J","ABS 200 porte de ramonage ","ABS Putztüre zu Rauchzugklappe","ABS Portina per Regolatore ",111,1,"ZBH ABS",null,209,"255100019",null,null,241,"104240",32,null,null,null,241,32]
["104242",104242,null,"STK","ABS Putztüre Typ 3 mit Wechselband ","CHF",167,"Schiedel ABSOLUT",2.5,0,"J","ABS porte de ramonage Typ 3 avec bandes chanchable","ABS Putztüre Typ 3 mit Wechselband ","ABS Porta tipo 3 con fasce intercambiabili",111,1,"ZBH ABS",null,145,"255100028","102199","4037494183182",167,"104242",22,null,null,null,167,22]
["104254",104254,null,"STK","ABS Armierungs-Vergussmörtel Kessel weiss 17kg ","CHF",82,"Schiedel ABSOLUT",17,0,"J","ABS Mortier blanc de remplissage d'armature 17 kg ","ABS Armierungs-Vergussmörtel Kessel weiss 17kg ","ABS Malta per set d'armatura seccio bianco 17kg ",111,1,"ZBH ABS",null,71,"1754020","102609","4037494013021",82,"104254",11,null,null,null,82,11]
["104265",104265,null,"STK","Zement Normo 5 Sack a 50kg.","CHF",202,"Zubehör",0,0,"J","ABS 140 Adapteur emboîtable, pour mazout et gaz ","Zement Normo 5 Sack a 50kg.","ABS 160 Adattore a innestro",15,2,0,null,175,"700008",null,null,202,"104265",27,null,null,null,202,27]
["104278",104278,null,"STK","TS120 80 160 Endmuffe schwarz ","CHF",105.6,"TECHNOSTAR 120",0.15,0,"J","TS120 80/160 Manchon de final noi avec tube final","TS120 80 160 Endmuffe schwarz ","TS120 80/160 Manica finale con tubo bocca L500mm",121,1,"DN 80",null,96,0,null,null,105.6,"104278",9.5999999999999943,null,null,null,105.6,9.5999999999999943]
["104281",104281,null,"STK","TS120 110 200 Endmuffe schwarz ","CHF",134.19999999999999,"TECHNOSTAR 120",1.1000000000000001,0,"J","TS120 110/200 Manchon de final noi avec tube final","TS120 110 200 Endmuffe schwarz ","TS120 110/200 Manica finale con tubo bocca L500mm",121,1,"DN 110",null,122,0,null,null,134.19999999999999,"104281",12.199999999999989,null,null,null,134.19999999999999,12.199999999999989]
["104285",104285,null,"STK","ICKA Grundplatte m. Ablauf D080","CHF",189.9,"Schiedel ICK verkupfert",2.14,0,"J",null,"ICKA Grundplatte m. Ablauf D080","ICKA 100 Piastra base con scadenza verticale",135,1,0,null,165,"DF81C7080",null,null,189.9,"104285",24.900000000000006,null,null,null,189.9,24.900000000000006,189.9,189.91176470588235]
[{"$f":"B4189&\"\"","v":"104289"},104289,null,"STK",{"$f":"IF($E$200=2,L4189,IF($E$200=3,N4189,M4189))","v":"ICKA Grundplatte m. Ablauf D200"},"CHF",{"$f":"IF($L$190=1,W4189,S4189)","v":347.6},"Schiedel ICK verkupfert",4.67,0,"J",null,"ICKA Grundplatte m. Ablauf D200","ICKA Konsoleblech 470mm zu D080",135,1,0,null,302,"DF81C7200",null,null,347.6,"104289",45.600000000000023,null,null,null,347.6,45.600000000000023,347.6,347.59607843137258]
["104290",104290,null,"STK","ICKA Konsoleblech 470mm zu D080","CHF",186.5,"Schiedel ICK verkupfert",4.24,0,"J",null,"ICKA Konsoleblech 470mm zu D080","ICKA Konsoleblech 470mm zu D100",135,1,0,null,162,"DF81D2080",null,null,186.5,"104290",24.5,null,null,null,186.5,24.5,186.5,186.45882352941177]
["104296",104296,null,"STK","ICKA Grundpl. mit Stutzen D130","CHF",232.5,"Schiedel ICK verkupfert",3.42,0,"J",null,"ICKA Grundpl. mit Stutzen D130",null,135,1,0,null,202,"DF81D6130",null,null,232.5,"104296",30.5,null,null,null,232.5,30.5,232.5,232.49803921568628]
["104299",104299,null,"STK","ICKA Grundpl. mit Stutzen D200","CHF",307.3,"Schiedel ICK verkupfert",5.15,0,"J",null,"ICKA Grundpl. mit Stutzen D200",null,135,1,0,null,267,"DF81D6200",null,null,307.3,"104299",40.300000000000011,null,null,null,307.3,40.300000000000011,307.3,307.31176470588235]
["104301",104301,null,"STK","ICKA Revisiondeckel rund D100","CHF",142.69999999999999,"Schiedel ICK verkupfert",0.59,0,"J",null,"ICKA Revisiondeckel rund D100",null,135,1,0,null,124,"DF8125100",null,null,142.69999999999999,"104301",18.699999999999989,null,null,null,142.69999999999999,18.699999999999989,142.69999999999999,142.72156862745098]
["104304",104304,null,"STK","ICKA Revisiondeckel rund D180","CHF",199.1,"Schiedel ICK verkupfert",1.1200000000000001,0,"J",null,"ICKA Revisiondeckel rund D180",null,135,1,0,null,173,"DF8125180",null,null,199.1,"104304",26.099999999999994,null,null,null,199.1,26.099999999999994,199.1,199.11960784313726]
["104309",104309,null,"STK","ICKA Kondensattopf D150","CHF",163.4,"Schiedel ICK verkupfert",0.9,0,"J","ICKA Pot de condensat D180","ICKA Kondensattopf D150","ICKA Bancinella per condensa D180",135,1,0,null,142,"DF8129150",null,null,163.4,"104309",21.400000000000006,null,null,null,163.4,21.400000000000006,163.4,163.43921568627451]
["104313",104313,null,"STK","ICKA Klemmband D100","CHF",17.3,"Schiedel ICK verkupfert",0.2,0,"J",null,"ICKA Klemmband D100",null,135,1,0,null,15,"DF8183100",null,null,17.3,"104313",2.3000000000000007,null,null,null,17.3,2.3000000000000007,17.3,17.264705882352942]
["104317",104317,null,"STK","ICKA Inspektionsbogen 90° D150","CHF",455.8,"Schiedel ICK verkupfert",3.81,0,"J",null,"ICKA Inspektionsbogen 90° D150",null,135,1,0,null,396,"DH81A2150",null,null,455.8,"104317",59.800000000000011,null,null,null,455.8,59.800000000000011,455.8,455.78823529411767]
["104320",104320,null,"STK","ICKA Rohr 250mm& Kond. Abl.D080","CHF",260.10000000000002,"Schiedel ICK verkupfert",1.76,0,"J",null,"ICKA Rohr 250mm& Kond. Abl.D080",null,135,1,"DN 250",null,226,"DH81A5080",null,null,260.10000000000002,"104320",34.100000000000023,null,null,null,260.10000000000002,34.100000000000023,260.10000000000002,260.12156862745098]
["104322",104322,null,"STK","ICKA Rohr 250mm& Kond. Abl.D130","CHF",303.89999999999998,"Schiedel ICK verkupfert",2.04,0,"J",null,"ICKA Rohr 250mm& Kond. Abl.D130",null,135,1,"DN 250",null,264,"DH81A5130",null,null,303.89999999999998,"104322",39.899999999999977,null,null,null,303.89999999999998,39.899999999999977,303.89999999999998,303.85882352941178]
["104325",104325,null,"STK","ICKA Rohr 250mm& Kond. Abl.D200","CHF",367.2,"Schiedel ICK verkupfert",2.64,0,"J",null,"ICKA Rohr 250mm& Kond. Abl.D200",null,135,1,"DN 250",null,319,"DH81A5200",null,null,367.2,"104325",48.199999999999989,null,null,null,367.2,48.199999999999989,367.2,367.16274509803924]
["104331",104331,null,"STK","ICKA Zwischenstütze D130","CHF",287.7,"Schiedel ICK verkupfert",4.16,0,"J",null,"ICKA Zwischenstütze D130","ICKA Piastra passante D150",135,1,0,null,250,"DH81D3130",null,null,287.7,"104331",37.699999999999989,null,null,null,287.7,37.699999999999989,287.7,287.74509803921569]
["104333",104333,null,"STK","ICKA Zwischenstütze D200","CHF",364.9,"Schiedel ICK verkupfert",6.11,0,"J",null,"ICKA Zwischenstütze D200",null,135,1,0,null,317,"DH81D3200",null,null,364.9,"104333",47.899999999999977,null,null,null,364.9,47.899999999999977,364.9,364.8607843137255]
["104336",104336,null,"STK","ICKA Rohr 950mm D150","CHF",345.3,"Schiedel ICK verkupfert",7.13,0,"J",null,"ICKA Rohr 950mm D150",null,135,1,0,null,300,"DH8101150",null,null,345.3,"104336",45.300000000000011,null,null,null,345.3,45.300000000000011,345.3,345.29411764705884]
["104340",104340,null,"STK","ICKA Rohr 450mm D080","CHF",139.30000000000001,"Schiedel ICK verkupfert",2.25,0,"J",null,"ICKA Rohr 450mm D080",null,135,1,"DN 80",null,121,"DH8102080",null,null,139.30000000000001,"104340",18.300000000000011,null,null,null,139.30000000000001,18.300000000000011,139.30000000000001,139.2686274509804]
["104345",104345,null,"STK","ICKA Rohr 200mm D150","CHF",155.4,"Schiedel ICK verkupfert",1.97,0,"J",null,"ICKA Rohr 200mm D150",null,135,1,"DN 200",null,135,"DH8103150",null,null,155.4,"104345",20.400000000000006,null,null,null,155.4,20.400000000000006,155.4,155.38235294117646]
["104348",104348,null,"STK","ICKA Rohr 150mm D100","CHF",116.2,"Schiedel ICK verkupfert",1.17,0,"J",null,"ICKA Rohr 150mm D100",null,135,1,"DN 150",null,101,"DH8104100",null,null,116.2,"104348",15.200000000000003,null,null,null,116.2,15.200000000000003,116.2,116.24901960784314]
["104350",104350,null,"STK","ICKA Rohr 150mm D150","CHF",141.6,"Schiedel ICK verkupfert",1.61,0,"J",null,"ICKA Rohr 150mm D150",null,135,1,"DN 150",null,123,"DH8104150",null,null,141.6,"104350",18.599999999999994,null,null,null,141.6,18.599999999999994,141.6,141.57058823529411]
[{"$f":"B4253&\"\"","v":"104353"},104353,null,"STK",{"$f":"IF($E$200=2,L4253,IF($E$200=3,N4253,M4253))","v":"ICKA Schieberohr 270-375mm D080"},"CHF",{"$f":"IF($L$190=1,W4253,S4253)","v":226.7},"Schiedel ICK verkupfert",2.5499999999999998,0,"J",null,"ICKA Schieberohr 270-375mm D080",null,135,1,0,null,197,"DH8109080",null,null,226.7,"104353",29.699999999999989,null,null,null,226.7,29.699999999999989,226.7,226.74313725490197]
["104359",104359,null,"STK","ICKA Bogen 90° D080","CHF",224.4,"Schiedel ICK verkupfert",1.5,0,"J",null,"ICKA Bogen 90° D080",null,135,1,0,null,195,"DH8115080",null,null,224.4,"104359",29.400000000000006,null,null,null,224.4,29.400000000000006,224.4,224.44117647058823]
["104361",104361,null,"STK","ICKA Bogen 90° D130","CHF",264.7,"Schiedel ICK verkupfert",2.29,0,"J",null,"ICKA Bogen 90° D130",null,135,1,0,null,230,"DH8115130",null,null,264.7,"104361",34.699999999999989,null,null,null,264.7,34.699999999999989,264.7,264.72549019607845]
["104364",104364,null,"STK","ICKA Bogen 90° D200","CHF",353.4,"Schiedel ICK verkupfert",3.83,0,"J",null,"ICKA Bogen 90° D200",null,135,1,0,null,307,"DH8115200",null,null,353.4,"104364",46.399999999999977,null,null,null,353.4,46.399999999999977,353.4,353.35098039215688]
["104368",104368,null,"STK","ICKA Bogen 45° D150","CHF",199.1,"Schiedel ICK verkupfert",1.92,0,"J",null,"ICKA Bogen 45° D150",null,135,1,0,null,173,"DH8117150",null,null,199.1,"104368",26.099999999999994,null,null,null,199.1,26.099999999999994,199.1,199.11960784313726]
["104372",104372,null,"STK","ICKA Bogen 15° D100","CHF",153.1,"Schiedel ICK verkupfert",1.1200000000000001,0,"J",null,"ICKA Bogen 15° D100",null,135,1,0,null,133,"DH8118100",null,null,153.1,"104372",20.099999999999994,null,null,null,153.1,20.099999999999994,153.1,153.08039215686276]
["104373",104373,null,"STK","ICKA Bogen 15° D130","CHF",169.2,"Schiedel ICK verkupfert",1.61,0,"J",null,"ICKA Bogen 15° D130",null,135,1,0,null,147,"DH8118130",null,null,169.2,"104373",22.199999999999989,null,null,null,169.2,22.199999999999989,169.2,169.19411764705882]
["104377",104377,null,"STK","ICKA Bogen 30° D080","CHF",141.6,"Schiedel ICK verkupfert",1.02,0,"J",null,"ICKA Bogen 30° D080",null,135,1,0,null,123,"DH8119080",null,null,141.6,"104377",18.599999999999994,null,null,null,141.6,18.599999999999994,141.6,141.57058823529411]
["104382",104382,null,"STK","ICKA Bogen 30° D200","CHF",210.6,"Schiedel ICK verkupfert",2.2200000000000002,0,"J",null,"ICKA Bogen 30° D200",null,135,1,0,null,183,"DH8119200",null,null,210.6,"104382",27.599999999999994,null,null,null,210.6,27.599999999999994,210.6,210.62941176470588]
["104384",104384,null,"STK","ICKA Tstück 90° D150","CHF",481.1,"Schiedel ICK verkupfert",4.3499999999999996,0,"J",null,"ICKA Tstück 90° D150",null,135,1,0,null,418,"DH8120150",null,null,481.1,"104384",63.100000000000023,null,null,null,481.1,63.100000000000023,481.1,481.10980392156864]
["104387",104387,null,"STK","ICKA Abzweiger 45° D100","CHF",310.8,"Schiedel ICK verkupfert",3.18,0,"J",null,"ICKA Abzweiger 45° D100",null,135,1,0,null,270,"DH8121100",null,null,310.8,"104387",40.800000000000011,null,null,null,310.8,40.800000000000011,310.8,310.76470588235293]
["104392",104392,null,"STK","ICKA Regenhaube D080","CHF",193.4,"Schiedel ICK verkupfert",1.08,0,"J",null,"ICKA Regenhaube D080",null,135,1,0,null,168,"DH8137080",null,null,193.4,"104392",25.400000000000006,null,null,null,193.4,25.400000000000006,193.4,193.36470588235295]
["104396",104396,null,"STK","ICKA Regenhaube D250","CHF",332.6,"Schiedel ICK verkupfert",0,0,"J",null,"ICKA Regenhaube D250",null,135,1,0,null,289,"DH8137250",null,null,332.6,"104396",43.600000000000023,null,null,null,332.6,43.600000000000023,332.6,332.63333333333333]
["104400",104400,null,"STK","ICKA Abströhmkonus D150","CHF",232.5,"Schiedel ICK verkupfert",1.81,0,"J",null,"ICKA Abströhmkonus D150",null,135,1,0,null,202,"DH8138150",null,null,232.5,"104400",30.5,null,null,null,232.5,30.5,232.5,232.49803921568628]
["104403",104403,null,"STK","ICKA Rohr 250mm& Messöffn. D080","CHF",254.4,"Schiedel ICK verkupfert",1.34,0,"J",null,"ICKA Rohr 250mm& Messöffn. D080",null,135,1,"DN 250",null,221,"DH8195080",null,null,254.4,"104403",33.400000000000006,null,null,null,254.4,33.400000000000006,254.4,254.36666666666667]
["104405",104405,null,"STK","ICKA Rohr 250mm& Messöffn. D130","CHF",290,"Schiedel ICK verkupfert",1.81,0,"J",null,"ICKA Rohr 250mm& Messöffn. D130",null,135,1,"DN 250",null,252,"DH8195130",null,null,290,"104405",38,null,null,null,290,38,290,290.04705882352943]
["104408",104408,null,"STK","ICKA Rohr 250mm& Messöffn. D200","CHF",349.9,"Schiedel ICK verkupfert",2.5099999999999998,0,"J",null,"ICKA Rohr 250mm& Messöffn. D200",null,135,1,"DN 250",null,304,"DH8195200",null,null,349.9,"104408",45.899999999999977,null,null,null,349.9,45.899999999999977,349.9,349.89803921568625]
["104414",104414,null,"STK","ICKA Dachdurchführ. 5-45° D300","CHF",239.4,"Schiedel ICK verkupfert",10.24,0,"J","ICKA Bride de haubanage DN130","ICKA Dachdurchführ. 5-45° D300","ICKA Collare per cavi tiranti DN130",135,1,0,null,208,"98460300",null,null,239.4,"104414",31.400000000000006,null,null,null,239.4,31.400000000000006,239.4,239.40392156862745]
["104416",104416,null,"STK","ICKA Seilabspannring D150","CHF",48.3,"Schiedel ICK verkupfert",1.03,0,"J","ICKA Bride de haubanage DN180","ICKA Seilabspannring D150","ICKA Collare per cavi tiranti DN180",135,1,0,null,42,"98900150",null,null,48.3,"104416",6.2999999999999972,null,null,null,48.3,6.2999999999999972,48.3,48.341176470588238]
["104419",104419,null,"STK","ICKA Seilabspannring D250","CHF",58.7,"Schiedel ICK verkupfert",1.43,0,"J","ICKA Bride de haubanage DN300","ICKA Seilabspannring D250","ICKA Collare per cavi tiranti DN300",135,1,0,null,51,"98900250",null,null,58.7,"104419",7.7000000000000028,null,null,null,58.7,7.7000000000000028,58.7,58.7]
["104424",104424,null,"STK","ICKA W.halter verst 75-300 D250","CHF",151.9,"Schiedel ICK verkupfert",3.9420000000000002,0,"J",null,"ICKA W.halter verst 75-300 D250",null,135,1,0,null,132,"98960300",null,null,151.9,"104424",19.900000000000006,null,null,null,151.9,19.900000000000006,151.9,151.92941176470589]
["104428",104428,null,"STK","ICKA Wandhalter 50mm DN80","CHF",67.900000000000006,"Schiedel ICK verkupfert",1.1000000000000001,0,"J","ICKA Fixation murale 50mm DN100","ICKA Wandhalter 50mm DN80","ICKA Collare a muro  50mm DN100",135,1,0,null,59,"98940130",null,null,67.900000000000006,"104428",8.9000000000000057,null,null,null,67.900000000000006,8.9000000000000057,67.900000000000006,67.907843137254901]
["104431",104431,null,"STK","ICKA Wandhalter 50mm DN200","CHF",88.6,"Schiedel ICK verkupfert",1.548,0,"J","ICKA Fixation murale 50mm DN180","ICKA Wandhalter 50mm DN200","ICKA Collare a muro  50mm DN180",135,1,0,null,77,"98940200",null,null,88.6,"104431",11.599999999999994,null,null,null,88.6,11.599999999999994,88.6,88.625490196078431]
["104433",104433,null,"STK","ICKA Wandhalter 50mm D200","CHF",93.2,"Schiedel ICK verkupfert",1.871,0,"J","ICKA Fixation murale 50mm DN230","ICKA Wandhalter 50mm D200","ICKA Collare a muro  50mm DN230",135,1,0,null,81,"98940250",null,null,93.2,"104433",12.200000000000003,null,null,null,93.2,12.200000000000003,93.2,93.229411764705887]
["104436",104436,null,"STK","ICKA Wandhalter 50mm D300","CHF",110.5,"Schiedel ICK verkupfert",2.7440000000000002,0,"J","ICKA Fixation murale 50mm DN400","ICKA Wandhalter 50mm D300","ICKA Collare a muro  50mm DN400",135,1,0,null,96,"98940355",null,null,110.5,"104436",14.5,null,null,null,110.5,14.5,110.5,110.49411764705883]
["104439",104439,null,"STK","ICKA W.halter verst 75-300 D300","CHF",160,"Schiedel ICK verkupfert",4.5540000000000003,0,"J",null,"ICKA W.halter verst 75-300 D300",null,135,1,0,null,139,"98960355",null,null,160,"104439",21,null,null,null,160,21,160,159.98627450980393]
["104442",104442,null,"STK","ICKA Putztüranschluss rund D 13","CHF",534.1,"Schiedel ICK verkupfert",0,0,"J",null,"ICKA Putztüranschluss rund D 13",null,135,1,0,null,464,"DH8113130",null,null,534.1,"104442",70.100000000000023,null,null,null,534.1,70.100000000000023,534.1,534.05490196078426]
["104447",104447,null,"STK","ICKA Dachdurchf 36-45° 300","CHF",348.7,"Schiedel ICK verkupfert",15,0,"J",null,"ICKA Dachdurchf 36-45° 300",null,135,1,"DN 300",null,303,"028600430",null,null,348.7,"104447",45.699999999999989,null,null,null,348.7,45.699999999999989,348.7,348.74705882352941]
["104451",104451,null,"STK","ICKA Winkel 85Gr 150","CHF",290,"Schiedel ICK verkupfert",2.2999999999999998,0,"J","ICKA Coude 85Gr 180","ICKA Winkel 85Gr 150","ICKA Gomito 85Gr 180",135,1,"DN 150",null,252,"142038515K",null,null,290,"104451",38,null,null,null,290,38,290,290.04705882352943]
["104455",104455,null,"STK","ICKA Winkel 85Gr 300","CHF",512.20000000000005,"Schiedel ICK verkupfert",5.8,0,"J","ICKA Coude avec inspection 85Gr 080","ICKA Winkel 85Gr 300","ICKA Gmoito con revisione 85Gr 080",135,1,"DN 300",null,445,"142038530K",null,null,512.20000000000005,"104455",67.200000000000045,null,null,null,512.20000000000005,67.200000000000045,512.20000000000005,512.18627450980398]
["104456",104456,null,"STK","ICKA Insp.Winkel 85Gr 080","CHF",368.3,"Schiedel ICK verkupfert",1.3,0,"J","ICKA Coude avec inspection 85Gr 100","ICKA Insp.Winkel 85Gr 080","ICKA Gmoito con revisione 85Gr 100",135,1,0,null,320,"142038708K",null,null,368.3,"104456",48.300000000000011,null,null,null,368.3,48.300000000000011,368.3,368.31372549019608]
["104460",104460,null,"STK","ICKA Insp.Winkel 85Gr 200","CHF",531.79999999999995,"Schiedel ICK verkupfert",3.3,0,"J","ICKA Coude avec inspection 85Gr 250","ICKA Insp.Winkel 85Gr 200","ICKA Gmoito con revisione 85Gr 250",135,1,"DN 200",null,462,"142038720K",null,null,531.79999999999995,"104460",69.799999999999955,null,null,null,531.79999999999995,69.799999999999955,531.79999999999995,531.75294117647059]
["104465",104465,null,"STK","ICKA T-Stück 85Gr 150","CHF",481.1,"Schiedel ICK verkupfert",3.9,0,"J","ICKA 180 Pièce Té 85° L455mm","ICKA T-Stück 85Gr 150","ICKA 180 Pezzo T 85° L455mm",135,1,"DN 150",null,418,"231408515K",null,null,481.1,"104465",63.100000000000023,null,null,null,481.1,63.100000000000023,481.1,481.10980392156864]
["104468",104468,null,"STK","ICKA T-Stück 85Gr 250","CHF",672.2,"Schiedel ICK verkupfert",6.6,0,"J","ICKA 300 Pièce Té 85° L485mm","ICKA T-Stück 85Gr 250","ICKA 300 Pezzo T 85° L485mm",135,1,"DN 250",null,584,"231408525K",null,null,672.2,"104468",88.200000000000045,null,null,null,672.2,88.200000000000045,672.2,672.17254901960791]
["104470",104470,null,"STK","ICKA Inspekt.-T-Stück 90Gr 150","CHF",587,"Schiedel ICK verkupfert",4.4000000000000004,0,"J","ICKA 180 Pièce Té 90° av. porte de révision ","ICKA Inspekt.-T-Stück 90Gr 150","ICKA 180 Pezzo T 90° con revisione ",135,1,"DN 150",null,510,"236900715K",null,null,587,"104470",77,null,null,null,587,77]
["104480",104480,null,"STK","CHZ Abströmkonus 30","CHF",186,"Schiedel CHEMINEE ZUG",1.2,0,"J",null,"CHZ Abströmkonus 30",null,112,1,"DN 300",null,161,"110004",null,null,186,"104480",25,null,null,null,186,25]
["104484",104484,null,"STK","Manchette hinterlüftet  16","CHF",558.5,"TECHNOSTAR 120",1.9,0,"J",null,"Manchette hinterlüftet  16",null,121,1,0,null,507.7,"413002",null,null,558.5,"104484",50.800000000000011,null,null,null,558.5,50.800000000000011]
["104488",104488,null,"STK","Kesselanschluss LAD 2xDN80","CHF",274.39999999999998,"TECHNOSTAR 120",3,0,"J",null,"Kesselanschluss LAD 2xDN80",null,121,1,0,null,249.4,"510009",null,null,274.39999999999998,"104488",24.999999999999972,null,null,null,274.39999999999998,24.999999999999972]
["104492",104492,null,"STK","TS Grundplatte 3/4 Zoll Mant.R","CHF",10,"TECHNOSTAR 120",0.3,0,"J",null,"TS Grundplatte 3/4 Zoll Mant.R",null,121,1,0,null,8.1,"512004",null,null,10,"104492",1.9000000000000004,null,null,null,10,1.9000000000000004]
["104494",104494,null,"STK","TS160 Rohrschelle 90","CHF",8,"TECHNOSTAR 120",0.4,0,"J",null,"TS160 Rohrschelle 90",null,121,1,0,null,6.8,"612000",null,null,8,"104494",1.2000000000000002,null,null,null,8,1.2000000000000002]
["104497",104497,null,"STK","TS160 Bride Bridex 145 Flex125","CHF",15,"TECHNOSTAR 120",0.01,0,"J",null,"TS160 Bride Bridex 145 Flex125",null,121,1,"DN 160",null,12.5,"613002",null,null,15,"104497",2.5,null,null,null,15,2.5]
["104503",104503,null,"STK","TS160 Kesselan.bride 130/140","CHF",27,"TECHNOSTAR 120",0.25,0,"J",null,"TS160 Kesselan.bride 130/140",null,121,1,0,null,23,"613009",null,null,27,"104503",4,null,null,null,27,4]
["104505",104505,null,"STK","TS160 Kesselan.bride 170/180","CHF",30,"TECHNOSTAR 120",0.25,0,"J",null,"TS160 Kesselan.bride 170/180",null,121,1,"DN 80",null,25.5,"613013",null,null,30,"104505",4.5,null,null,null,30,4.5]
["104508",104508,null,"STK","TS160 Kesselan.bride 200/210","CHF",30,"TECHNOSTAR 120",0.3,0,"J",null,"TS160 Kesselan.bride 200/210",null,121,1,0,null,25.5,"613016",null,null,30,"104508",4.5,null,null,null,30,4.5]
["104513",104513,null,"STK","Abdeckplatte  68/68 30/30","CHF",221,"ISOLIT",41,0,"J",null,"Abdeckplatte  68/68 30/30",null,114,1,0,null,192,"811017",null,null,221,"104513",29,null,null,null,221,29]
["104517",104517,null,"STK","Abdeckplatte  95/95 30/30","CHF",310.5,"ISOLIT",98,0,"J",null,"Abdeckplatte  95/95 30/30",null,114,1,0,null,269,"811037",null,null,310.5,"104517",41.5,null,null,null,310.5,41.5,310.5,310.52348993288592]
["104518",104518,null,"STK","Neutrabox PH-Indikator-Papier","CHF",26,"TECHNOSTAR 120",0,0,"J",null,"Neutrabox PH-Indikator-Papier",null,121,1,0,null,22,"911016",null,null,26,"104518",4,null,null,null,26,4]
["104521",104521,null,"STK","TS160 Rohrhalterung gleit. 90","CHF",59,"TECHNOSTAR 120",0.7,0,"J",null,"TS160 Rohrhalterung gleit. 90",null,121,1,0,null,51,"612002",null,null,59,"104521",8,null,null,null,59,8]
["104526",104526,null,"STK","TS Abdeckplatte 80-110 34/34","CHF",236.4,"TECHNOSTAR 120",2.1,0,"J",null,"TS Abdeckplatte 80-110 34/34",null,121,1,"DN 80",null,214.9,"511099",null,null,236.4,"104526",21.5,null,null,null,236.4,21.5]
["104529",104529,null,"STK","ABS Fertigf.M 12-18/L/20 (L+R)","CHF",1472.3,"Schiedel ABSOLUT",228,0,"J",null,"ABS Fertigf.M 12-18/L/20 (L+R)",null,111,1,0,null,1280,"200151820",null,null,1472.3,"104529",192.29999999999995,null,null,null,1472.3,192.29999999999995,1472.3,1472.3004694835681]
["104531",104531,null,"STK","ABS Fertigfußpaket 12","CHF",980,"Schiedel ABSOLUT",7.02,0,"J",null,"ABS Fertigfußpaket 12",null,111,1,0,null,852,"203040012","100117","4037494195659",980,"104531",128,null,null,null,980,128]
["104537",104537,null,"STK","LAS Reduktion 125/110 80/70","CHF",79.400000000000006,"TECHNOSTAR 120",0.1,0,"J",null,"LAS Reduktion 125/110 80/70",null,121,1,0,null,72.099999999999994,"500172",null,null,79.400000000000006,"104537",7.3000000000000114,null,null,null,79.400000000000006,7.3000000000000114]
["104541",104541,null,"STK","Verschlussbüchse  25 CNS","CHF",136.9,"Schiedel ABSOLUT",1,0,"J",null,"Verschlussbüchse  25 CNS",null,111,1,0,null,119,"913325",null,null,136.9,"104541",17.900000000000006,null,null,null,136.9,17.900000000000006,136.9,136.87793427230048]
["104546",104546,null,"STK","TNS Anschlussrosette 200/370","CHF",60,"Schiedel KERASTAR",0.45,0,"J",null,"TNS Anschlussrosette 200/370","TNS  Rosetta di collegamento  200/370",137,1,0,null,52,"265404720","100954","4037494279540",60,"104546",8,null,null,null,60,8]
["104548",104548,null,"STK","KRS Wandhalterung 60   20","CHF",74,"Schiedel KERASTAR",1.23,0,"J","KRS Fixation murale 60mm DN200mm","KRS Wandhalterung 60   20","KRS Collare a muro 60mm DN200mm",137,1,0,null,64,"265701420",null,null,74,"104548",10,null,null,null,74,10]
["104552",104552,null,"STK","ICS Regenhaube 08","CHF",189.6,"Schiedel ICS glänzend",1.19,0,"J",null,"ICS Regenhaube 08",null,133,1,"ZBH ICS",null,164.8,"DF2137080","104534","5035944642288",189.6,"104552",24.799999999999983,null,null,null,189.6,24.799999999999983,189.6,189.59502818326351]
["104557",104557,null,"STK","CHI Flexrohr Rolle 15m D100","CHF",1327.5,"Schiedel CHIMFLEX",17.25,0,"J",null,"CHI Flexrohr Rolle 15m D100",null,132,1,0,null,1153.9000000000001,"D4A15100",null,null,1327.5,"104557",173.59999999999991,null,null,null,1327.5,173.59999999999991,1327.5,1327.5103338632753]
["104561",104561,null,"STK","CHI Flexrohr Rolle 30m D100","CHF",1687,"Schiedel CHIMFLEX",34.5,0,"J",null,"CHI Flexrohr Rolle 30m D100",null,132,1,0,null,1466.3,"D4A30100",null,null,1687,"104561",220.70000000000005,null,null,null,1687,220.70000000000005]
["104563",104563,null,"STK","CHI Befestigungsplatte D100","CHF",40,"Schiedel CHIMFLEX",2.75,0,"J",null,"CHI Befestigungsplatte D100",null,132,1,0,null,34.1,"D4002100",null,null,40,"104563",5.8999999999999986,null,null,null,40,5.8999999999999986]
["104567",104567,null,"STK","CHI Befestigungsplatte D200","CHF",41,"Schiedel CHIMFLEX",2.75,0,"J",null,"CHI Befestigungsplatte D200",null,132,1,0,null,35.200000000000003,"D4002200",null,null,41,"104567",5.7999999999999972,null,null,null,41,5.7999999999999972]
["104568",104568,null,"STK","Wandhalter 50mm D405","CHF",97,"Schiedel PRIMA PLUS",2.875,0,"J","KRS Fixation murale 60mm DN200mm","Wandhalter 50mm D405","KRS Collare a muro  60mm DN200mm",131,1,0,null,83.6,"92940405",null,null,97,"104568",13.400000000000006,null,null,null,97,13.400000000000006]
["104569",104569,null,"STK","ICS Uniflash-Dachabdeckung","CHF",241,"Schiedel ICS glänzend",1.1000000000000001,0,"J",null,"ICS Uniflash-Dachabdeckung",null,133,1,"ZBH ICS",null,209.09,"94540002",null,null,241,"104569",31.909999999999997,null,null,null,241,31.909999999999997,241,241.03158388003749]
["104570",104570,null,"STK","ICS Statisches Klemmband D280","CHF",123.5,"Schiedel ICS glänzend",2.15,0,"J","ICKA  Bride du fixation DN280","ICS Statisches Klemmband D280","ICS Fascetta di sicurezza statico D280",133,1,"ZBH ICS",null,107.12,"95840280",null,null,123.5,"104570",16.379999999999995,null,null,null,123.5,16.379999999999995,123.5,123.48416119962512]
["104571",104571,null,"STK","Wandhalter verstelb.75-300 280","CHF",123,"Schiedel PRIMA PLUS",1.81,0,"J",null,"Wandhalter verstelb.75-300 280",null,131,1,0,null,106.7,"95960280",null,null,123,"104571",16.299999999999997,null,null,null,123,16.299999999999997]
["104572",104572,null,"STK","ICS Uniflash-Dachabdeckung","CHF",130.6,"Schiedel ICS glänzend",0.76800000000000002,0,"J",null,"ICS Uniflash-Dachabdeckung",null,133,1,"ZBH ICS",null,113.3,"94540001",null,null,130.6,"104572",17.299999999999997,null,null,null,130.6,17.299999999999997,130.6,130.60824742268039]
["104573",104573,null,"STK","ICK Abdeckblende 0 - 30° D180","CHF",133.1,"Schiedel ICK verkupfert",0,0,"J","ICK Recouvrement carrée 0 - 30° D180","ICK Abdeckblende 0 - 30° D180","ICK Coperture 0 - 30° D180",135,1,0,null,115.5,"98050230",null,null,133.1,"104573",17.599999999999994,null,null,null,133.1,17.599999999999994,133.1,133.14432989690721]
["104574",104574,null,"STK","ICK Abdeckblende 32 - 45° D180","CHF",133.1,"Schiedel ICK verkupfert",0,0,"J","ICK Recouvrement carrée 32 - 45° D180","ICK Abdeckblende 32 - 45° D180","ICK Coperture 32 - 45° D180",135,1,0,null,115.5,"98060230",null,null,133.1,"104574",17.599999999999994,null,null,null,133.1,17.599999999999994,133.1,133.14432989690721]
["104575",104575,null,"STK","Abdeckplatte  78/78 30/30 F","CHF",295,"ISOLIT",67,0,"J",null,"Abdeckplatte  78/78 30/30 F",null,114,1,0,null,256,"811224",null,null,295,"104575",39,null,null,null,295,39]
["104576",104576,null,"STK","Kaminhalterung First","CHF",290.5,"Schiedel ABSOLUT",16.5,0,"J",null,"Kaminhalterung First",null,111,1,0,null,252,"035050015",null,null,290.5,"104576",38.5,null,null,null,290.5,38.5,290.5,290.49671977507029]
["104578",104578,null,"STK","PPL Bogen 0-30 Gr.vari.0,6/130","CHF",69,"Schiedel PRIMA PLUS",0,0,"J",null,"PPL Bogen 0-30 Gr.vari.0,6/130",null,131,1,0,null,59.4,"137032913",null,null,69,"104578",9.6000000000000014,null,null,null,69,9.6000000000000014]
["104579",104579,null,"STK","PPL Bogen 0-30 Gr.vari.0,6/200","CHF",97,"Schiedel PRIMA PLUS",0,0,"J",null,"PPL Bogen 0-30 Gr.vari.0,6/200",null,131,1,0,null,83.6,"137032920","105994","4037494148648",97,"104579",13.400000000000006,null,null,null,97,13.400000000000006]
["104580",104580,null,"STK","PPL Bogen 0-30 Gr.vari.0,6/250","CHF",109,"Schiedel PRIMA PLUS",0,0,"J",null,"PPL Bogen 0-30 Gr.vari.0,6/250",null,131,1,0,null,94.6,"137032925","105995","4037494148662",109,"104580",14.400000000000006,null,null,null,109,14.400000000000006]
["104581",104581,null,"STK","PPL Bogen 0-30 Gr.vari.0,6/300","CHF",123,"Schiedel PRIMA PLUS",0,0,"J",null,"PPL Bogen 0-30 Gr.vari.0,6/300",null,131,1,0,null,106.7,"137032930",null,null,123,"104581",16.299999999999997,null,null,null,123,16.299999999999997]
["104582",104582,null,"STK","PPL Rev.Deckel Festbrennst 080","CHF",54.9,"Schiedel PRIMA PLUS",0.17,0,"J",null,"PPL Rev.Deckel Festbrennst 080",null,131,1,0,null,47.3,"255150608","103585","4037494135488",54.9,"104582",7.6000000000000014,null,null,null,54.9,7.6000000000000014,54.9,54.944444444444443]
["104583",104583,null,"STK","PPL Rev.Deckel Festbrennst 100","CHF",69,"Schiedel PRIMA PLUS",0.19,0,"J",null,"PPL Rev.Deckel Festbrennst 100",null,131,1,0,null,59.4,"255150610","103586","4037494125779",69,"104583",9.6000000000000014,null,null,null,69,9.6000000000000014,69,69]
["104584",104584,null,"STK","PPL Rev.Deckel Festbrennst 130","CHF",81.8,"Schiedel PRIMA PLUS",0.2,0,"J",null,"PPL Rev.Deckel Festbrennst 130",null,131,1,0,null,70.400000000000006,"255150613","103589","4037494125793",81.8,"104584",11.399999999999991,null,null,null,81.8,11.399999999999991,81.8,81.777777777777786]
["104585",104585,null,"STK","PPL Rev.Deckel Festbrennst 180","CHF",97.1,"Schiedel PRIMA PLUS",0.3,0,"J",null,"PPL Rev.Deckel Festbrennst 180",null,131,1,0,null,83.6,"255150618","103593","4037494125816",97.1,"104585",13.5,null,null,null,97.1,13.5,97.1,97.111111111111114]
["104586",104586,null,"STK","PPL Rev.Deckel Festbrennst 200","CHF",109.9,"Schiedel PRIMA PLUS",0.35,0,"J",null,"PPL Rev.Deckel Festbrennst 200",null,131,1,0,null,94.6,"255150620","103594","4037494125823",109.9,"104586",15.300000000000011,null,null,null,109.9,15.300000000000011,109.9,109.88888888888889]
["104587",104587,null,"STK","PPL Rev.Deckel Festbrennst 250","CHF",123.9,"Schiedel PRIMA PLUS",0.4,0,"J",null,"PPL Rev.Deckel Festbrennst 250",null,131,1,0,null,106.7,"255150625","103596","4037494125830",123.9,"104587",17.200000000000003,null,null,null,123.9,17.200000000000003,123.9,123.94444444444446]
["104588",104588,null,"STK","PPL Reduktion  D250/200","CHF",148.19999999999999,"Schiedel PRIMA PLUS",1.32,0,"J",null,"PPL Reduktion  D250/200",null,131,1,0,null,127.6,"267202530",null,null,148.19999999999999,"104588",20.599999999999994,null,null,null,148.19999999999999,20.599999999999994,148.19999999999999,148.22222222222223]
["104589",104589,null,"STK","PPL Einlagering F60 isol25 230","CHF",41,"Schiedel PRIMA PLUS",0,0,"J",null,"PPL Einlagering F60 isol25 230",null,131,1,0,null,35.200000000000003,"265800423",null,null,41,"104589",5.7999999999999972,null,null,null,41,5.7999999999999972]
["104592",104592,null,"STK","TS120LAS 80/125 Mündungsschalldämpfer DN80 CNS","CHF",1631.9,"TECHNOSTAR 120",15,0,"J","TS120LAS 80/125 Amortisseur de finition inox","TS120LAS 80/125 Mündungsschalldämpfer DN80 CNS","TS120LAS 80/125 Silenzatori finale inox",121,1,"DN 80",null,1419,"26740080",null,null,1631.9,"104592",212.90000000000009,null,null,null,1631.9,212.90000000000009]
["104593",104593,null,"STK","Handypl.CNS 36x50/8,5cm o.Bef","CHF",173.9,"Schiedel ABSOLUT",4.5,0,"J",null,"Handypl.CNS 36x50/8,5cm o.Bef",null,111,1,0,null,151,"038613650","108222","4037494143858",173.9,"104593",22.900000000000006,null,null,null,173.9,22.900000000000006,173.9,173.94607843137254]
["104594",104594,null,"STK","Handypl.CNS 38x54/8,5cm o.Bef","CHF",178.6,"Schiedel ABSOLUT",4.3,0,"J",null,"Handypl.CNS 38x54/8,5cm o.Bef",null,111,1,0,null,155,"038613854","108224","4037494143872",178.6,"104594",23.599999999999994,null,null,null,178.6,23.599999999999994,178.6,178.55392156862746]
["104596",104596,null,"STK","Verl Typ 136 zu Halter 80-180","CHF",57,"Schiedel PRIMA PLUS",0.26,0,"J",null,"Verl Typ 136 zu Halter 80-180",null,131,1,0,null,49.3,"95080136",null,null,57,"104596",7.7000000000000028,null,null,null,57,7.7000000000000028]
["104598",104598,null,"STK","Verl.Wandkonsole 160 CNS Typ1","CHF",170.2,"TECHNOSTAR 120",0.4,0,"J",null,"Verl.Wandkonsole 160 CNS Typ1",null,121,1,0,null,154.69999999999999,"560870",null,null,170.2,"104598",15.5,null,null,null,170.2,15.5,170.2,170.21774691358024]
["104599",104599,null,"STK","Verl.Wandkonsole 160 CNS Typ2","CHF",213.9,"TECHNOSTAR 120",0.5,0,"J",null,"Verl.Wandkonsole 160 CNS Typ2",null,121,1,0,null,194.4,"560871",null,null,213.9,"104599",19.5,null,null,null,213.9,19.5]
["104600",104600,null,"STK","TS Stulpstütze mit Schiene 125","CHF",42.7,"TECHNOSTAR 120",2,0,"J",null,"TS Stulpstütze mit Schiene 125",null,121,1,"DN 125",null,38.799999999999997,"560110",null,null,42.7,"104600",3.9000000000000057,null,null,null,42.7,3.9000000000000057]
["104601",104601,null,"STK","Basten Stand.ICS Stulpr.080CNS","CHF",378,"Schiedel ICS glänzend",3.9,0,"J",null,"Basten Stand.ICS Stulpr.080CNS",null,133,1,0,null,356,"916508",null,null,378,"104601",22,null,null,null,378,22]
["104602",104602,null,"STK","ZBE Körperschallabsorb.Gas 080","CHF",96,"Schiedel PRIMA PLUS",0.6,0,"J","Basten Stand.ICS av. Dila 080CNS","ZBE Körperschallabsorb.Gas 080","Basten Stand  ICS con dila 80 inox",131,1,0,null,83,"265000080",null,null,96,"104602",13,null,null,null,96,13]
["104603",104603,null,"STK","ICM/PPL An.Klemmfutter 150/160","CHF",129.9,"Schiedel ICS glänzend",1.6,0,"J",null,"ICM/PPL An.Klemmfutter 150/160",null,133,1,"DN 150",null,122.35,"266021516M","104725","4037494193891",129.9,"104603",7.5500000000000114,null,null,null,129.9,7.5500000000000114,129.9,129.91095505617977]
["104605",104605,null,"STK","Wandh. verst.75-300 355 Kupfer","CHF",179,"Schiedel PRIMA PLUS",4.8,0,"J",null,"Wandh. verst.75-300 355 Kupfer",null,131,1,0,null,155.1,"95960355K",null,null,179,"104605",23.900000000000006,null,null,null,179,23.900000000000006]
["104606",104606,null,"STK","Wandh. verst.75-300 355 Matt","CHF",137,"Schiedel PRIMA PLUS",4.8,0,"J",null,"Wandh. verst.75-300 355 Matt",null,131,1,0,null,118.8,"95960355M",null,null,137,"104606",18.200000000000003,null,null,null,137,18.200000000000003]
["104607",104607,null,"STK","KRS Dep.Plaf. Holzbau DN180","CHF",785,"Schiedel KERASTAR",16,0,"J",null,"KRS Dep.Plaf. Holzbau DN180",null,137,1,0,null,682,"2020180053",null,null,785,"104607",103,null,null,null,785,103]
["104608",104608,null,"STK","KRS Dep.Plaf. Betonbau DN180","CHF",785,"Schiedel KERASTAR",16,0,"J",null,"KRS Dep.Plaf. Betonbau DN180",null,137,1,0,null,682,"2030180053",null,null,785,"104608",103,null,null,null,785,103]
["104609",104609,null,"STK","ICS Fussteil m.Bodenablauf 300","CHF",552.29999999999995,"Schiedel ICS glänzend",12,0,"J",null,"ICS Fussteil m.Bodenablauf 300",null,133,1,"DN 300",null,520.15,"266000230","100999","4037494496527",552.29999999999995,"104609",32.149999999999977,null,null,null,552.29999999999995,32.149999999999977,552.29999999999995,552.29410112359551]
["104610",104610,null,"STK","PPL 200 Kesselanschluss 220mm","CHF",123,"Schiedel PRIMA PLUS",0,0,"J",null,"PPL 200 Kesselanschluss 220mm",null,131,1,"DN 200",null,106.7,"265820422",null,null,123,"104610",16.299999999999997,null,null,null,123,16.299999999999997]
["104611",104611,null,"STK","ABS LAS-Zuluftadapter 2xDN125","CHF",235,"Schiedel ABSOLUT",2.5,0,"J",null,"ABS LAS-Zuluftadapter 2xDN125",null,111,1,0,null,204,"255040212",null,null,235,"104611",31,null,null,null,235,31]
["104612",104612,null,"STK","Handypl.CNS 55x71/8,5cm o.Bef","CHF",187.6,"Schiedel ABSOLUT",5.78,0,"J",null,"Handypl.CNS 55x71/8,5cm o.Bef",null,111,1,0,null,163,"038615571","108226","4049723002157",187.6,"104612",24.599999999999994,null,null,null,187.6,24.599999999999994,187.6,187.61730205278593]
["104613",104613,null,"STK","KRS PA-Formstück rund 40","CHF",1413,"Schiedel KERASTAR",35,0,"J",null,"KRS PA-Formstück rund 40",null,137,1,0,null,1228,"236715040",null,null,1413,"104613",185,null,null,null,1413,185]
["104614",104614,null,"STK","KRS Dachdurchführung 0° 500","CHF",213.3,"Schiedel ICS glänzend",1.8,0,"J",null,"KRS Dachdurchführung 0° 500",null,133,1,0,null,185.4,"266320500","101232","4037494176207",213.3,"104614",27.900000000000006,null,null,null,213.3,27.900000000000006,213.3,213.33078175895767]
["104615",104615,null,"STK","KRS PA- rund 20 überdruck","CHF",547,"Schiedel KERASTAR",20,0,"J",null,"KRS PA- rund 20 überdruck",null,137,1,0,null,475,"236716020",null,null,547,"104615",72,null,null,null,547,72]
["104616",104616,null,"STK","PPL Klemmband 160","CHF",14,"Schiedel PRIMA PLUS",0.1,0,"J",null,"PPL Klemmband 160",null,131,1,0,null,12.1,"265822116","105950","4037494493526",14,"104616",1.9000000000000004,null,null,null,14,1.9000000000000004]
["104617",104617,null,"STK","PPL Adapter zu Flex D160/160","CHF",92,"Schiedel PRIMA PLUS",0.33,0,"J","PPL Bride du fixation 160","PPL Adapter zu Flex D160/160","PPL Fascetta di sicurezza DN160",131,1,0,null,79.2,"265930116","106967","4049723009347",92,"104617",12.799999999999997,null,null,null,92,12.799999999999997]
["104618",104618,null,"STK","ICS Schiebeelem.390-475 mm 100","CHF",248.9,"Schiedel ICS glänzend",1.9,0,"J",null,"ICS Schiebeelem.390-475 mm 100",null,133,1,"DN 100",null,214.24,"266031008",null,null,248.9,"104618",34.659999999999997,null,null,null,248.9,34.659999999999997,248.9,248.86464646464646]
["104619",104619,null,"STK","ICS Schiebeelem.390-475 mm 100","CHF",256,"Schiedel ICS glänzend",2.2000000000000002,0,"J",null,"ICS Schiebeelem.390-475 mm 100",null,133,1,"DN 100",null,220.42,"266031010",null,null,256,"104619",35.580000000000013,null,null,null,256,35.580000000000013,256,256.04343434343434]
["104620",104620,null,"STK","ICS Inspekt.-T-Stück 90Gr 100","CHF",335,"Schiedel ICS glänzend",3.9,0,"J",null,"ICS Inspekt.-T-Stück 90Gr 100",null,133,1,"DN 100",null,288.39999999999998,"236900710",null,null,335,"104620",46.600000000000023,null,null,null,335,46.600000000000023,335,335.01010101010098]
["104621",104621,null,"STK","TS120 Abgasklappe MUK 080","CHF",818.7,"TECHNOSTAR 120",2,0,"J","TS120 80 Porte MUK","TS120 Abgasklappe MUK 080","TS120 80 Portina MUK",121,1,"DN 80",null,711.9,"516708",null,null,818.7,"104621",106.80000000000007,null,null,null,818.7,106.80000000000007]
["104624",104624,null,"STK","ZBE Dichtring Silikon 45","CHF",28,"Schiedel PRIMA PLUS",0.03,0,"J","Basten Stand.Dila 250mm.180 cuivre","ZBE Dichtring Silikon 45","Basten Stand  ICS con dila 250mm 180 rame",131,1,0,null,24,"270301245",null,null,28,"104624",4,null,null,null,28,4]
["104625",104625,null,"STK","TS120 80 Schalldämpfer AGP DN80 PP L330mm","CHF",1070.9000000000001,"TECHNOSTAR 120",15,0,"J","TS120 80 Amortisseur AGP PP L330mm","TS120 80 Schalldämpfer AGP DN80 PP L330mm","TS120 80 Silenzatori AGP PP L330mm",121,1,"DN 80",null,931.2,"26740180",null,null,1070.9000000000001,"104625",139.70000000000005,null,null,null,1070.9000000000001,139.70000000000005]
["104626",104626,null,"STK","TS120 110 Schalldämpfer AGP DN110 L330mm","CHF",1092.5,"TECHNOSTAR 120",15,0,"J","TS120 110 Amortisseur AGP PP L330mm","TS120 110 Schalldämpfer AGP DN110 L330mm","TS120 110 Silenzatori AGP PP L330mm",121,1,"DN 110",null,950,"26740182",null,null,1092.5,"104626",142.5,null,null,null,1092.5,142.5]
[{"$f":"B4509&\"\"","v":"104627"},104627,null,"STK",{"$f":"IF($E$200=2,L4509,IF($E$200=3,N4509,M4509))","v":"TS120 110 Schalldämpfer AGP DN110 L550mm"},"CHF",{"$f":"IF($L$190=1,W4509,S4509)","v":1177.5999999999999},"TECHNOSTAR 120",20,0,"J","TS120 110 Amortisseur AGP PP L550mm","TS120 110 Schalldämpfer AGP DN110 L550mm","TS120 110 Silenzatori AGP PP L550mm",121,1,"DN 110",null,1024,"26740184",null,null,1177.5999999999999,"104627",153.59999999999991,null,null,null,1177.5999999999999,153.59999999999991]
["104628",104628,null,"STK","PPL Rohrelement 1000 1,0/500","CHF",474,"Schiedel PRIMA PLUS",7.5,0,"J",null,"PPL Rohrelement 1000 1,0/500",null,131,1,0,null,411.4,"137010050",null,null,474,"104628",62.600000000000023,null,null,null,474,62.600000000000023]
["104629",104629,null,"STK","PPL Rohrelement 500 1,0/500","CHF",274,"Schiedel PRIMA PLUS",3.6,0,"J",null,"PPL Rohrelement 500 1,0/500",null,131,1,0,null,237.6,"137005050",null,null,274,"104629",36.400000000000006,null,null,null,274,36.400000000000006]
["104630",104630,null,"STK","PPL Bogen 15 Gr.1,0/400","CHF",274,"Schiedel PRIMA PLUS",1.5,0,"J",null,"PPL Bogen 15 Gr.1,0/400",null,131,1,0,null,237.6,"137031540",null,null,274,"104630",36.400000000000006,null,null,null,274,36.400000000000006]
["104631",104631,null,"STK","PPL Klemmband 400","CHF",28,"Schiedel PRIMA PLUS",0.3,0,"J",null,"PPL Klemmband 400",null,131,1,0,null,24.2,"265822140",null,null,28,"104631",3.8000000000000007,null,null,null,28,3.8000000000000007]
["104635",104635,null,"STK","PPL 220 Schallabsorber Festbrennstoffe","CHF",135.4,"Schiedel PRIMA PLUS",2.5,0,"J",null,"PPL 220 Schallabsorber Festbrennstoffe",null,131,1,0,null,117.7,"265000522",null,null,135.4,"104635",17.700000000000003,null,null,null,135.4,17.700000000000003,135.4,135.39924812030074]
["104636",104636,null,"STK","TS120 80 300 Endmuffe schwarz mit Mündungsrohr","CHF",184.8,"TECHNOSTAR 120",0.19,0,"J","TS120 80/300 Manchon de final noir avec tube final","TS120 80 300 Endmuffe schwarz mit Mündungsrohr","TS120 80/300 Manica finale nero con tubo bocca L500mm",121,1,"DN 80",null,168,0,null,null,184.8,"104636",16.800000000000011,null,null,null,184.8,16.800000000000011]
["104637",104637,null,"STK","TS120 80 300 Endmuffe schwarz ","CHF",184.8,"TECHNOSTAR 120",0.17,0,"J","TS120 80/300 Manchon de final noir ","TS120 80 300 Endmuffe schwarz ","TS120 80/300 Manica finale",121,1,"DN 80",null,168,0,null,null,184.8,"104637",16.800000000000011,null,null,null,184.8,16.800000000000011]
["104638",104638,null,"STK","TS120 80 350 Endmuffe schwarz ","CHF",215.4,"TECHNOSTAR 120",0.19,0,"J","TS120 80/350 Manchon de final noir ","TS120 80 350 Endmuffe schwarz ","TS120 80/350 Manica finale",121,1,"DN 80",null,195.8,0,null,null,215.4,"104638",19.599999999999994,null,null,null,215.4,19.599999999999994]
["104639",104639,null,"STK","TS120 80 350 Endmuffe schwarz mit Mündungsrohr","CHF",215.4,"TECHNOSTAR 120",0.21,0,"J","TS120 80/350 Manchon de final noir avec tube final","TS120 80 350 Endmuffe schwarz mit Mündungsrohr","TS120 80/350 Manica finale nero con tubo bocca L500mm",121,1,"DN 80",null,195.8,0,null,null,215.4,"104639",19.599999999999994,null,null,null,215.4,19.599999999999994]
["104641",104641,null,"STK","TS120 110 350 Endmuffe schwarz ","CHF",215.4,"TECHNOSTAR 120",0.7,0,"J","TS120 110/350 Manchon de final noir ","TS120 110 350 Endmuffe schwarz ","TS120 110/350 Manica finale",121,1,"DN 110",null,195.8,0,null,null,215.4,"104641",19.599999999999994,null,null,null,215.4,19.599999999999994]
["104642",104642,null,"STK","TS120 110 300 Endmuffe schwarz mit Mündungsrohr","CHF",184.8,"TECHNOSTAR 120",1.1000000000000001,0,"J","TS120 110/300 Manchon de final noir avec tube final","TS120 110 300 Endmuffe schwarz mit Mündungsrohr","TS120 110/300 Manica finale nero con tubo bocca L500mm",121,1,"DN 110",null,168,0,null,null,184.8,"104642",16.800000000000011,null,null,null,184.8,16.800000000000011]
["104643",104643,null,"STK","TS120 110 350 Endmuffe schwarz mit Mündungsrohr","CHF",215.4,"TECHNOSTAR 120",1.3,0,"J","TS120 110/350 Manchon de final noir avec tube final","TS120 110 350 Endmuffe schwarz mit Mündungsrohr","TS120 110/350 Manica finale nero con tubo bocca L500mm",121,1,"DN 110",null,195.8,0,null,null,215.4,"104643",19.599999999999994,null,null,null,215.4,19.599999999999994]
["104647",104647,null,"STK","ABS 120 RA Formstück L330mm","CHF",96,"Schiedel ABSOLUT",3,0,"J",null,"ABS 120 RA Formstück L330mm",null,111,1,"DN 120",null,83,"235603312","102121","4037494127230",96,"104647",13,null,null,null,96,13]
["104648",104648,null,"STK","ABS 140 RA Formstück L330mm","CHF",110,"Schiedel ABSOLUT",3.5,0,"J",null,"ABS 140 RA Formstück L330mm",null,111,1,"DN 140",null,95,"235603314","102122","4037494137390",110,"104648",15,null,null,null,110,15]
["104649",104649,null,"STK","ABS 160 RA Formstück L330mm","CHF",120,"Schiedel ABSOLUT",4,0,"J",null,"ABS 160 RA Formstück L330mm",null,111,1,"DN 160",null,104,"235603316","102123","4037494142233",120,"104649",16,null,null,null,120,16]
["104650",104650,null,"STK","ABS 180 RA Formstück L330mm","CHF",134,"Schiedel ABSOLUT",4.5,0,"J",null,"ABS 180 RA Formstück L330mm",null,111,1,"DN 180",null,116,"235603318","102124","4037494119044",134,"104650",18,null,null,null,134,18]
["104651",104651,null,"STK","ABS 200 RA Formstück L330mm","CHF",167,"Schiedel ABSOLUT",6,0,"J",null,"ABS 200 RA Formstück L330mm",null,111,1,"DN 200",null,147,"235603320","102125","4037494168097",167,"104651",20,null,null,null,167,20]
["104652",104652,null,"STK","TS120 160 Kesselanschluss Erweiterung zentr. 180","CHF",302.5,"TECHNOSTAR 120",0.85,0,"J","TS120 160/180 Raccordement enlagissement","TS120 160 Kesselanschluss Erweiterung zentr. 180","TS120 160/180 Raccordo enlargemento",121,1,"DN 160",null,275,0,null,null,302.5,"104652",27.5,null,null,null,302.5,27.5]
["104653",104653,null,"STK","TS120 160 Kesselanschluss Erweiterung zentr. 200","CHF",330,"TECHNOSTAR 120",0.85,0,"J","TS120 160/180 Raccordement enlagissement","TS120 160 Kesselanschluss Erweiterung zentr. 200","TS120 160/200 Raccordo enlargemento",121,1,"DN 160",null,300,0,null,null,330,"104653",30,null,null,null,330,30]
["104654",104654,null,"STK","TS120LAS 80/125 Schalldämpfer weiss","CHF",1381.4,"TECHNOSTAR 120",15,0,"J","TS120LAS 80/125 Amortisseur blanc","TS120LAS 80/125 Schalldämpfer weiss","TS120LAS 80/125 Silenzatori binaco",121,1,"DN 80",null,1201.2,"26740060",null,null,1381.4,"104654",180.20000000000005,null,null,null,1381.4,180.20000000000005]
["100317",100317,null,"STK","TS120LAS 110/160 Rohr L 250 weiss ","CHF",97.8,"TECHNOSTAR 120 LAS",0.25,250,"J","TS120LAS 110/160 Tuyau L 250 blanc ","TS120LAS 110/160 Rohr L 250 weiss ","TS120LAS 110/160 Tubo L 250 bianco ",122,1,"DN 110",null,88.9,0,null,null,97.8,"100317",8.8999999999999915,null,null,null,97.8,8.8999999999999915]
["101209",101209,null,"STK","ICS 80 Wandhalter 50mm fix DN 130mm ","CHF",41.2,"Schiedel ICS glänzend",0.44,0,"J","ICS 80 Fixation murale 50mm fix DN 130mm ","ICS 80 Wandhalter 50mm fix DN 130mm ","ICS 80 Collare a muro 50mm fix DN 130mm ",133,1,"ZBH ICS",null,41.2,"92940130",null,null,41.2,"101209",0,null,null,null,41.2,0,41.2,41.2]
["101210",101210,null,"STK","ICS 100 Wandhalter 50mm fix DN 150mm ","CHF",44.3,"Schiedel ICS glänzend",0.48,0,"J","ICS 100 Fixation murale 50mm fix DN 150mm ","ICS 100 Wandhalter 50mm fix DN 150mm ","ICS 100 Collare a muro 50mm fix DN 150mm ",133,1,"ZBH ICS",null,44.29,"92940150",null,null,44.3,"101210",9.9999999999980105E-3,null,null,null,44.3,9.9999999999980105E-3,44.3,44.29]
["101211",101211,null,"STK","ICS 130 Wandhalter 50mm fix DN 180mm ","CHF",48.4,"Schiedel ICS glänzend",0.53,0,"J","ICS 130 Fixation murale 50mm fix DN 180mm ","ICS 130 Wandhalter 50mm fix DN 180mm ","ICS 130 Collare a muro 50mm fix DN 180mm ",133,1,"ZBH ICS",null,48.41,"92940180",null,null,48.4,"101211",-9.9999999999980105E-3,null,null,null,48.4,-9.9999999999980105E-3,48.4,48.41]
["101212",101212,null,"STK","ICS 150 Wandhalter 50mm fix DN 200mm ","CHF",53.6,"Schiedel ICS glänzend",0.57999999999999996,0,"J","ICS 150 Fixation murale 50mm fix DN 200mm ","ICS 150 Wandhalter 50mm fix DN 200mm ","ICS 150 Collare a muro 50mm fix DN 200mm ",133,1,"ZBH ICS",null,53.56,"92940200",null,null,53.6,"101212",3.9999999999999147E-2,null,null,null,53.6,3.9999999999999147E-2,53.6,53.56]
["101213",101213,null,"STK","ICS 180 Wandhalter 50mm fix DN 230mm ","CHF",55.6,"Schiedel ICS glänzend",0.64,0,"J","ICS 180 Fixation murale 50mm fix DN 230mm ","ICS 180 Wandhalter 50mm fix DN 230mm ","ICS 180 Collare a muro 50mm fix DN 230mm ",133,1,"ZBH ICS",null,55.62,"92940230",null,null,55.6,"101213",-1.9999999999996021E-2,null,null,null,55.6,-1.9999999999996021E-2,55.6,55.62]
["101214",101214,null,"STK","ICS 200 Wandhalter 50mm fix DN 250mm","CHF",56.7,"Schiedel ICS glänzend",0.7,0,"J","ICS 200 Fixation murale 50mm fix DN 250mm","ICS 200 Wandhalter 50mm fix DN 250mm","ICS 200 Collare a muro 50mm fix DN 250mm",133,1,"ZBH ICS",null,56.65,"92940250",null,null,56.7,"101214",5.0000000000004263E-2,null,null,null,56.7,5.0000000000004263E-2,56.7,56.65]
["101215",101215,null,"STK","ICS 250 Wandhalter 50mm fix DN 300mm ","CHF",60.8,"Schiedel ICS glänzend",0.79,0,"J","ICS 250 Fixation murale 50mm fix DN 300mm ","ICS 250 Wandhalter 50mm fix DN 300mm ","ICS 250 Collare a muro 50mm fix DN 300mm ",133,1,"ZBH ICS",null,60.77,"92940300",null,null,60.8,"101215",2.9999999999994031E-2,null,null,null,60.8,2.9999999999994031E-2,60.8,60.77]
["101216",101216,null,"STK","ICS 300 Wandhalter 50mm fix DN 350mm ","CHF",67,"Schiedel ICS glänzend",0.95,0,"J","ICS 300 Fixation murale 50mm fix DN 350mm ","ICS 300 Wandhalter 50mm fix DN 350mm ","ICS 300 Collare a muro 50mm fix DN 350mm ",133,1,"ZBH ICS",null,66.95,"92940355",null,null,67,"101216",4.9999999999997158E-2,null,null,null,67,4.9999999999997158E-2,67,66.95]
["101218",101218,null,"STK","ICS 80 Wandhalter verstellbar 75 - 300mm DN130mm","CHF",70,"Schiedel ICS glänzend",1.1200000000000001,0,"J","ICS 80 Fixation murale régl. 75 - 300mm DN130mm","ICS 80 Wandhalter verstellbar 75 - 300mm DN130mm","ICS 80 Collare a muro regolabile 75-300mm DN130mm",133,1,"ZBH ICS",null,70.040000000000006,"95960130",null,null,70,"101218",-4.0000000000006253E-2,null,null,null,70,-4.0000000000006253E-2,70,70.040000000000006]
["101220",101220,null,"STK","ICS 130 Wandhalter verstellbar 75 - 300mm DN180mm","CHF",74.2,"Schiedel ICS glänzend",1.51,0,"J","ICS 130 Fixation murale régl. 75 - 300mm DN180mm","ICS 130 Wandhalter verstellbar 75 - 300mm DN180mm","ICS 130 Collare a muro regolabile 75-300mm DN180mm",133,1,"ZBH ICS",null,74.16,"95960180",null,null,74.2,"101220",4.0000000000006253E-2,null,null,null,74.2,4.0000000000006253E-2,74.2,74.16]
["101221",101221,null,"STK","ICS 150 Wandhalter verstellbar 75 - 300mm DN200mm","CHF",75.2,"Schiedel ICS glänzend",1.66,0,"J","ICS 150 Fixation murale régl. 75 - 300mm DN200mm","ICS 150 Wandhalter verstellbar 75 - 300mm DN200mm","ICS 150 Collare a muro regolabile 75-300mm DN200mm",133,1,"ZBH ICS",null,75.19,"95960200",null,null,75.2,"101221",1.0000000000005116E-2,null,null,null,75.2,1.0000000000005116E-2,75.2,75.19]
["101222",101222,null,"STK","ICS 180 Wandhalter verstellbar 75 - 300mm DN230mm","CHF",84.5,"Schiedel ICS glänzend",1.89,0,"J","ICS 180 Fixation murale régl. 75 - 300mm DN230mm","ICS 180 Wandhalter verstellbar 75 - 300mm DN230mm","ICS 180 Collare a muro regolabile 75-300mm DN230mm",133,1,"ZBH ICS",null,84.46,"95960230",null,null,84.5,"101222",4.0000000000006253E-2,null,null,null,84.5,4.0000000000006253E-2,84.5,84.46]
["101223",101223,null,"STK","ICS 200 Wandhalter verstellbar 75 - 300mm DN250mm","CHF",81.400000000000006,"Schiedel ICS glänzend",2.0299999999999998,0,"J","ICS 200 Fixation murale régl. 75 - 300mm DN250mm","ICS 200 Wandhalter verstellbar 75 - 300mm DN250mm","ICS 200 Collare a muro regolabile 75-300mm DN250mm",133,1,"ZBH ICS",null,81.37,"95960250",null,null,81.400000000000006,"101223",3.0000000000001137E-2,null,null,null,81.400000000000006,3.0000000000001137E-2,81.400000000000006,81.37]
["101224",101224,null,"STK","ICS 250 Wandhalter verstellbar 75 - 300mm DN300mm","CHF",91.7,"Schiedel ICS glänzend",2.2789999999999999,0,"J","ICS 250 Fixation murale régl. 75 - 300mm DN300mm","ICS 250 Wandhalter verstellbar 75 - 300mm DN300mm","ICS 250 Collare a muro regolabile 75-300mm DN300mm",133,1,"ZBH ICS",null,91.67,"95960300",null,null,91.7,"101224",3.0000000000001137E-2,null,null,null,91.7,3.0000000000001137E-2,91.7,91.67]
["101225",101225,null,"STK","ICS 300 Wandhalter verstellbar 75 - 300mm DN350mm","CHF",96.8,"Schiedel ICS glänzend",2.5150000000000001,0,"J","ICS 300 Fixation murale régl. 75 - 300mm DN350mm","ICS 300 Wandhalter verstellbar 75 - 300mm DN350mm","ICS 300 Collare a muro regolabile 75-300mm DN350mm",133,1,"ZBH ICS",null,96.82,"95960350",null,null,96.8,"101225",-1.9999999999996021E-2,null,null,null,96.8,-1.9999999999996021E-2,96.8,96.82]
["101226",101226,null,"STK","ICS 350 Wandhalter verstellbar 75 - 300mm DN400mm","CHF",144.19999999999999,"Schiedel ICS glänzend",2.7509999999999999,0,"J","ICS 350 Fixation murale régl. 75 - 300mm DN400mm","ICS 350 Wandhalter verstellbar 75 - 300mm DN400mm","ICS 350 Collare a muro regolabile 75-300mm DN400mm",133,1,"ZBH ICS",null,144.19999999999999,"95960400",null,null,144.19999999999999,"101226",0,null,null,null,144.19999999999999,0,144.19999999999999,144.19999999999999]
["101227",101227,null,"STK","ICS 400 Wandhalter verstellbar 75 - 300mm DN450mm","CHF",181.3,"Schiedel ICS glänzend",2.9870000000000001,0,"J","ICS 400 Fixation murale régl. 75 - 300mm DN450mm","ICS 400 Wandhalter verstellbar 75 - 300mm DN450mm","ICS 400 Collare a muro regolabile 75-300mm DN450mm",133,1,"ZBH ICS",null,181.28,"95960450",null,null,181.3,"101227",2.0000000000010232E-2,null,null,null,181.3,2.0000000000010232E-2,181.3,181.28]
["101228",101228,null,"STK","ICS 450 Wandhalter verstellbar 75 - 300mm DN500mm","CHF",206,"Schiedel ICS glänzend",3.2229999999999999,0,"J","ICS 450 Fixation murale régl. 75 - 300mm DN500mm","ICS 450 Wandhalter verstellbar 75 - 300mm DN500mm","ICS 450 Collare a muro regolabile 75-300mm DN500mm",133,1,"ZBH ICS",null,206,"95960500",null,null,206,"101228",0,null,null,null,206,0,206,206]
["101229",101229,null,"STK","ICS 500 Wandhalter verstellbar 75 - 300mm DN550mm","CHF",226.6,"Schiedel ICS glänzend",3.41,0,"J","ICS 500 Fixation murale régl. 75 - 300mm DN550mm","ICS 500 Wandhalter verstellbar 75 - 300mm DN550mm","ICS 500 Collare a muro regolabile 75-300mm DN550mm",133,1,"ZBH ICS",null,226.6,"95960550",null,null,226.6,"101229",0,null,null,null,226.6,0,226.6,226.6]
["101231",101231,null,"STK","ICS 600 Wandhalter verstellbar 75 - 300mm DN650mm","CHF",247.2,"Schiedel ICS glänzend",3.6960000000000002,0,"J","ICS 600 Fixation murale régl. 75 - 300mm DN650mm","ICS 600 Wandhalter verstellbar 75 - 300mm DN650mm","ICS 600 Collare a muro regolabile 75-300mm DN650mm",133,1,"ZBH ICS",null,247.2,"95960650",null,null,247.2,"101231",0,null,null,null,247.2,0,247.2,247.2]
["101233",101233,null,"STK","ICS 700 Wandhalter verstellbar 75 - 300mm DN750mm","CHF",309,"Schiedel ICS glänzend",4.05,0,"J","ICS 700 Fixation murale régl. 75 - 300mm DN750mm","ICS 700 Wandhalter verstellbar 75 - 300mm DN750mm","ICS 700 Collare a muro regolabile 75-300mm DN750mm",133,1,"ZBH ICS",null,309,"95960750",null,null,309,"101233",0,null,null,null,309,0,309,309]
["101236",101236,null,"STK","ICS 80 Wandhalter 50mm verlängerbar DN130mm ","CHF",41.2,"Schiedel ICS glänzend",0.5,0,"J","ICS 80 Fixation murale 50mm régl. DN130mm ","ICS 80 Wandhalter 50mm verlängerbar DN130mm ","ICS 80 Collare a muro 50mm prolunga DN130mm ",133,1,"ZBH ICS",null,41.2,"95090130",null,null,41.2,"101236",0,null,null,null,41.2,0,41.2,41.2]
["101237",101237,null,"STK","ICS 100 Wandhalter 50mm verlängerbar DN150mm ","CHF",44.3,"Schiedel ICS glänzend",0.5,0,"J","ICS 100 Fixation murale 50mm régl. DN150mm ","ICS 100 Wandhalter 50mm verlängerbar DN150mm ","ICS 100 Collare a muro 50mm prolunga DN150mm ",133,1,"ZBH ICS",null,44.29,"95090150",null,null,44.3,"101237",9.9999999999980105E-3,null,null,null,44.3,9.9999999999980105E-3,44.3,44.29]
["101238",101238,null,"STK","ICS 130 Wandhalter 50mm verlängerbar DN180mm ","CHF",48.4,"Schiedel ICS glänzend",0.6,0,"J","ICS 130 Fixation murale 50mm régl. DN180mm ","ICS 130 Wandhalter 50mm verlängerbar DN180mm ","ICS 130 Collare a muro 50mm prolunga DN180mm ",133,1,"ZBH ICS",null,48.41,"95090180",null,null,48.4,"101238",-9.9999999999980105E-3,null,null,null,48.4,-9.9999999999980105E-3,48.4,48.41]
["101239",101239,null,"STK","ICS 150 Wandhalter 50mm verlängerbar DN200mm ","CHF",53.6,"Schiedel ICS glänzend",0.6,0,"J","ICS 150 Fixation murale 50mm régl. DN200mm ","ICS 150 Wandhalter 50mm verlängerbar DN200mm ","ICS 150 Collare a muro 50mm prolunga DN200mm ",133,1,"ZBH ICS",null,53.56,"95090200",null,null,53.6,"101239",3.9999999999999147E-2,null,null,null,53.6,3.9999999999999147E-2,53.6,53.56]
["101240",101240,null,"STK","ICS 180 Wandhalter 50mm verlängerbar DN230mm ","CHF",55.6,"Schiedel ICS glänzend",0.7,0,"J","ICS 180 Fixation murale 50mm régl. DN230mm ","ICS 180 Wandhalter 50mm verlängerbar DN230mm ","ICS 180 Collare a muro 50mm prolunga DN230mm ",133,1,"ZBH ICS",null,55.62,"95090230",null,null,55.6,"101240",-1.9999999999996021E-2,null,null,null,55.6,-1.9999999999996021E-2,55.6,55.62]
["101241",101241,null,"STK","ICS 200 Wandhalter 50mm verlängerbar DN250mm","CHF",56.7,"Schiedel ICS glänzend",0.7,0,"J","ICS 200 Fixation murale 50mm régl. DN250mm","ICS 200 Wandhalter 50mm verlängerbar DN250mm","ICS 200 Collare a muro 50mm prolunga DN250mm",133,1,"ZBH ICS",null,56.65,"95090250",null,null,56.7,"101241",5.0000000000004263E-2,null,null,null,56.7,5.0000000000004263E-2,56.7,56.65]
["101242",101242,null,"STK","ICS 250 Wandhalter 50mm verlängerbar DN300mm ","CHF",60.8,"Schiedel ICS glänzend",0.8,0,"J","ICS 250 Fixation murale 50mm régl. DN300mm ","ICS 250 Wandhalter 50mm verlängerbar DN300mm ","ICS 250 Collare a muro 50mm prolunga DN300mm ",133,1,"ZBH ICS",null,60.77,"95090300",null,null,60.8,"101242",2.9999999999994031E-2,null,null,null,60.8,2.9999999999994031E-2,60.8,60.77]
["101243",101243,null,"STK","ICS 300 Wandhalter 50mm verlängerbar DN350mm ","CHF",63.9,"Schiedel ICS glänzend",0.9,0,"J","ICS 300 Fixation murale 50mm régl. DN350mm ","ICS 300 Wandhalter 50mm verlängerbar DN350mm ","ICS 300 Collare a muro 50mm prolunga DN350mm ",133,1,"ZBH ICS",null,63.86,"95090350",null,null,63.9,"101243",3.9999999999999147E-2,null,null,null,63.9,3.9999999999999147E-2,63.9,63.86]
["101244",101244,null,"STK","ICS 350 Wandhalter 50mm verlängerbar DN400mm ","CHF",121.5,"Schiedel ICS glänzend",1.4,0,"J","ICS 350 Fixation murale 50mm régl. DN400mm ","ICS 350 Wandhalter 50mm verlängerbar DN400mm ","ICS 350 Collare a muro 50mm prolunga DN400mm ",133,1,"ZBH ICS",null,121.54,"95090400",null,null,121.5,"101244",-4.0000000000006253E-2,null,null,null,121.5,-4.0000000000006253E-2,121.5,121.54]
["101245",101245,null,"STK","ICS 400 Wandhalter 50mm verlängerbar DN450mm ","CHF",152.4,"Schiedel ICS glänzend",1.6,0,"J","ICS 400 Fixation murale 50mm régl. DN450mm ","ICS 400 Wandhalter 50mm verlängerbar DN450mm ","ICS 400 Collare a muro 50mm prolunga DN450mm ",133,1,"ZBH ICS",null,152.44,"95090450",null,null,152.4,"101245",-3.9999999999992042E-2,null,null,null,152.4,-3.9999999999992042E-2,152.4,152.44]
["101246",101246,null,"STK","ICS 450 Wandhalter 50mm verlängerbar DN500mm ","CHF",177.2,"Schiedel ICS glänzend",2,0,"J","ICS 450 Fixation murale 50mm régl. DN500mm ","ICS 450 Wandhalter 50mm verlängerbar DN500mm ","ICS 450 Collare a muro 50mm prolunga DN500mm ",133,1,"ZBH ICS",null,177.16,"95090500",null,null,177.2,"101246",3.9999999999992042E-2,null,null,null,177.2,3.9999999999992042E-2,177.2,177.16]
["101247",101247,null,"STK","ICS 500 Wandhalter 50mm verlängerbar DN550mm ","CHF",208.1,"Schiedel ICS glänzend",2.1,0,"J","ICS 500 Fixation murale 50mm régl. DN550mm ","ICS 500 Wandhalter 50mm verlängerbar DN550mm ","ICS 500 Collare a muro 50mm prolunga DN550mm ",133,1,"ZBH ICS",null,208.06,"95090550",null,null,208.1,"101247",3.9999999999992042E-2,null,null,null,208.1,3.9999999999992042E-2,208.1,208.06]
["101249",101249,null,"STK","ICS 600 Wandhalter 50mm verlängerbar DN650mm  ","CHF",244.1,"Schiedel ICS glänzend",3.2,0,"J","ICS 600 Fixation murale 50mm régl. DN650mm  ","ICS 600 Wandhalter 50mm verlängerbar DN650mm  ","ICS 600 Collare a muro 50mm prolunga DN650mm  ",133,1,"ZBH ICS",null,244.11,"95090650",null,null,244.1,"101249",-1.0000000000019327E-2,null,null,null,244.1,-1.0000000000019327E-2,244.1,244.11]
["101251",101251,null,"STK","ICS 700 Wandhalter 50mm verlängerbar DN 750mm ","CHF",325.5,"Schiedel ICS glänzend",4,0,"J","ICS 700 Fixation murale 50mm régl. DN 750mm ","ICS 700 Wandhalter 50mm verlängerbar DN 750mm ","ICS 700 Collare a muro 50mm prolunga DN 750mm ",133,1,"ZBH ICS",null,325.48,"95090750",null,null,325.5,"101251",1.999999999998181E-2,null,null,null,325.5,1.999999999998181E-2,325.5,325.48]
["101252",101252,null,"PAR","ICS W1 Verlängerung zu Wandhalter 50mm L130mm","CHF",45.3,"Schiedel ICS glänzend",0.13,0,"J","ICS W1 Ralogement pour fixation murale L130mm","ICS W1 Verlängerung zu Wandhalter 50mm L130mm","ICS W1 Prolunga per collare 50mm L130mm",133,1,"ZBH ICS",null,45.32,"267100130","101735","4037494812167",45.3,"101252",-2.0000000000003126E-2,null,null,null,45.3,-2.0000000000003126E-2,45.3,45.32]
["101253",101253,null,"PAR","ICS W2 Verlängerung zu Wandhalter 50mm L176mm","CHF",49.4,"Schiedel ICS glänzend",0.17,0,"J","ICS W2 Ralogement pour fixation murale L176mm","ICS W2 Verlängerung zu Wandhalter 50mm L176mm","ICS W2 Prolunga per collare 50mm L176mm",133,1,"ZBH ICS",null,49.44,"267100176","101736","4037494812174",49.4,"101253",-3.9999999999999147E-2,null,null,null,49.4,-3.9999999999999147E-2,49.4,49.44]
["101319",101319,null,"STK","PPL 180 Dämmrohr 20mm Steinwolle L1000mm","CHF",31.1,"Zubehör",1.21,0,"J","PPL 180 Tubo d'isolation 20mm laine de pierre","PPL 180 Dämmrohr 20mm Steinwolle L1000mm","PPL 180 Coppella 20mm di lana di roccia L1000mm",15,2,"DN 180",null,27,"163001218","103497","4037494280324",31.1,"101319",4.1000000000000014,null,null,null,31.1,4.1000000000000014]
["101914",101914,null,"STK","ICS 150 Inspektions-Winkel 85°","CHF",348.1,"Schiedel ICS glänzend",3.05,0,"J","ICS 150 Coude avec inspection 85°","ICS 150 Inspektions-Winkel 85°","ICS 150 Gmoito con revisione 85°",133,1,"DN 150",null,348.14,"142038715","100786","4037494177143",348.1,"101914",-3.999999999996362E-2,null,null,null,348.1,-3.999999999996362E-2,348.1,348.14]
["101915",101915,null,"STK","ICS 180 Inspektions-Winkel 85°","CHF",380.1,"Schiedel ICS glänzend",3.68,0,"J","ICS 180 Coude avec inspection 85°","ICS 180 Inspektions-Winkel 85°","ICS 180 Gmoito con revisione 85°",133,1,"DN 180",null,380.07,"142038718","100787","4037494177167",380.1,"101915",3.0000000000029559E-2,null,null,null,380.1,3.0000000000029559E-2,380.1,380.07]
["101916",101916,null,"STK","ICS 200 Inspektions-Winkel 85°","CHF",421.3,"Schiedel ICS glänzend",3.98,0,"J","ICS 200 Coude avec inspection 85°","ICS 200 Inspektions-Winkel 85°","ICS 200 Gmoito con revisione 85°",133,1,"DN 200",null,421.27,"142038720","100788","4037494177181",421.3,"101916",3.0000000000029559E-2,null,null,null,421.3,3.0000000000029559E-2,421.3,421.27]
["101917",101917,null,"STK","ICS 250 Inspektions-Winkel 85°","CHF",429.5,"Schiedel ICS glänzend",5.12,0,"J","ICS 250 Coude avec inspection 85°","ICS 250 Inspektions-Winkel 85°","ICS 250 Gmoito con revisione 85°",133,1,"DN 250",null,429.51,"142038725","100789","4037494177204",429.5,"101917",-9.9999999999909051E-3,null,null,null,429.5,-9.9999999999909051E-3,429.5,429.51]
[{"$f":"B4573&\"\"","v":"101918"},101918,null,"STK",{"$f":"IF($E$200=2,L4573,IF($E$200=3,N4573,M4573))","v":"ICS 300 Inspektions-Winkel 85°"},"CHF",{"$f":"IF($L$190=1,W4573,S4573)","v":535.6},"Schiedel ICS glänzend",6.74,0,"J","ICS 300 Coude avec inspection 85°","ICS 300 Inspektions-Winkel 85°","ICS 300 Gmoito con revisione 85°",133,1,"DN 300",null,535.6,"142038730","100790","4037494177228",535.6,"101918",0,null,null,null,535.6,0,535.6,535.6]
["101919",101919,null,"STK","ICS 350 Inspektions-Winkel 85°","CHF",607.70000000000005,"Schiedel ICS glänzend",8.18,0,"J","ICS 350 Coude avec inspection 85°","ICS 350 Inspektions-Winkel 85°","ICS 350 Gmoito con revisione 85°",133,1,"DN 350",null,607.70000000000005,"142038735","100791","4037494177242",607.70000000000005,"101919",0,null,null,null,607.70000000000005,0,607.70000000000005,607.70000000000005]
["101920",101920,null,"STK","ICS 400 Inspektions-Winkel 85°","CHF",1163.9000000000001,"Schiedel ICS glänzend",10.199999999999999,0,"J","ICS 400 Coude avec inspection 85°","ICS 400 Inspektions-Winkel 85°","ICS 400 Gmoito con revisione 85°",133,1,"DN 400",null,1163.9000000000001,"142038740","100792","4037494177259",1163.9000000000001,"101920",0,null,null,null,1163.9000000000001,0,1163.9000000000001,1163.9000000000001]
["101921",101921,null,"STK","ICS 450 Inspektions-Winkel 85°","CHF",1380.2,"Schiedel ICS glänzend",12.78,0,"J","ICS 450 Coude avec inspection 85°","ICS 450 Inspektions-Winkel 85°","ICS 450 Gmoito con revisione 85°",133,1,"DN 450",null,1380.2,"142038745","100793","4037494177266",1380.2,"101921",0,null,null,null,1380.2,0,1380.2,1380.2]
["101922",101922,null,"STK","ICS 500 Inspektions-Winkel 85°","CHF",1452.3,"Schiedel ICS glänzend",14.94,0,"J","ICS 500 Coude avec inspection 85°","ICS 500 Inspektions-Winkel 85°","ICS 500 Gmoito con revisione 85°",133,1,"DN 500",null,1452.3,"142038750","100794","4037494177273",1452.3,"101922",0,null,null,null,1452.3,0,1452.3,1452.3]
["101923",101923,null,"STK","ICS 600 Inspektions-Winkel 85°","CHF",1620.2,"Schiedel ICS glänzend",19.5,0,"J","ICS 600 Coude avec inspection 85°","ICS 600 Inspektions-Winkel 85°","ICS 600 Gmoito con revisione 85°",133,1,"DN 600",null,1620.19,"142038760","100795","4037494177297",1620.2,"101923",9.9999999999909051E-3,null,null,null,1620.2,9.9999999999909051E-3,1620.2,1620.19]
["101924",101924,null,"STK","ICS 700 Inspektions-Winkel 85°","CHF",1745.9,"Schiedel ICS glänzend",24.9,0,"J","ICS 700 Coude avec inspection 85°","ICS 700 Inspektions-Winkel 85°","ICS 700 Gmoito con revisione 85°",133,1,"DN 700",null,1745.85,"142038770","100796","4037494177303",1745.9,"101924",5.0000000000181899E-2,null,null,null,1745.9,5.0000000000181899E-2,1745.9,1745.85]
["101925",101925,null,"STK","ICS 80 Winkel 90°","CHF",129.80000000000001,"Schiedel ICS glänzend",1.2,0,"J","ICS 80 Coude 90°","ICS 80 Winkel 90°","ICS 80 Gomito 90°",133,1,"DN 80",null,129.78,"142039008","100810","4037494165331",129.80000000000001,"101925",2.0000000000010232E-2,null,null,null,129.80000000000001,2.0000000000010232E-2,129.80000000000001,129.78]
["101926",101926,null,"STK","ICS 100 Winkel 90°","CHF",137,"Schiedel ICS glänzend",1.5,0,"J","ICS 100 Coude 90°","ICS 100 Winkel 90°","ICS 100 Gomito 90°",133,1,"DN 100",null,136.99,"142039010","100811","4037494165348",137,"101926",9.9999999999909051E-3,null,null,null,137,9.9999999999909051E-3,137,136.99]
["101927",101927,null,"STK","ICS 130 Winkel 90°","CHF",146.30000000000001,"Schiedel ICS glänzend",2,0,"J","ICS 130 Coude 90°","ICS 130 Winkel 90°","ICS 130 Gomito 90°",133,1,"DN 130",null,146.26,"142039013","100812","4037494165355",146.30000000000001,"101927",4.0000000000020464E-2,null,null,null,146.30000000000001,4.0000000000020464E-2,146.30000000000001,146.26]
["101928",101928,null,"STK","ICS 150 Winkel 90°","CHF",163.80000000000001,"Schiedel ICS glänzend",2.38,0,"J","ICS 150 Coude 90°","ICS 150 Winkel 90°","ICS 150 Gomito 90°",133,1,"DN 150",null,163.77000000000001,"142039015","100813","4037494165362",163.80000000000001,"101928",3.0000000000001137E-2,null,null,null,163.80000000000001,3.0000000000001137E-2,163.80000000000001,163.77000000000001]
["101929",101929,null,"STK","ICS 180 Winkel 90°","CHF",178.2,"Schiedel ICS glänzend",3.07,0,"J","ICS 180 Coude 90°","ICS 180 Winkel 90°","ICS 180 Gomito 90°",133,1,"DN 180",null,178.19,"142039018","100814","4037494165379",178.2,"101929",9.9999999999909051E-3,null,null,null,178.2,9.9999999999909051E-3,178.2,178.19]
["101930",101930,null,"STK","ICS 200 Winkel 90°","CHF",207,"Schiedel ICS glänzend",3.39,0,"J","ICS 200 Coude 90°","ICS 200 Winkel 90°","ICS 200 Gomito 90°",133,1,"DN 200",null,207.03,"142039030","100817","4037494165409",207,"101930",-3.0000000000001137E-2,null,null,null,207,-3.0000000000001137E-2,207,207.03]
["101931",101931,null,"STK","ICS 250 Winkel 90°","CHF",234.8,"Schiedel ICS glänzend",4.55,0,"J","ICS 250 Coude 90°","ICS 250 Winkel 90°","ICS 250 Gomito 90°",133,1,"DN 250",null,234.84,"142039025","100816","4037494165393",234.8,"101931",-3.9999999999992042E-2,null,null,null,234.8,-3.9999999999992042E-2,234.8,234.84]
["101932",101932,null,"STK","ICS 300 Winkel 90°","CHF",288.39999999999998,"Schiedel ICS glänzend",5.84,0,"J","ICS 300 Coude 90°","ICS 300 Winkel 90°","ICS 300 Gomito 90°",133,1,"DN 300",null,288.39999999999998,"142039030","100817","4037494165409",288.39999999999998,"101932",0,null,null,null,288.39999999999998,0,288.39999999999998,288.39999999999998]
["101933",101933,null,"STK","ICS 350 Winkel 90°","CHF",542.79999999999995,"Schiedel ICS glänzend",7.33,0,"J","ICS 350 Coude 90°","ICS 350 Winkel 90°","ICS 350 Gomito 90°",133,1,"DN 350",null,542.80999999999995,"142039035","100818","4037494165416",542.79999999999995,"101933",-9.9999999999909051E-3,null,null,null,542.79999999999995,-9.9999999999909051E-3,542.79999999999995,542.80999999999995]
["101934",101934,null,"STK","ICS 400 Winkel 90°","CHF",584,"Schiedel ICS glänzend",9.8000000000000007,0,"J","ICS 400 Coude 90°","ICS 400 Winkel 90°","ICS 400 Gomito 90°",133,1,"DN 400",null,584.01,"142039040","100819","4037494165423",584,"101934",-9.9999999999909051E-3,null,null,null,584,-9.9999999999909051E-3,584,584.01]
["101935",101935,null,"STK","ICS 450 Winkel 90°","CHF",733.4,"Schiedel ICS glänzend",11.61,0,"J","ICS 450 Coude 90°","ICS 450 Winkel 90°","ICS 450 Gomito 90°",133,1,"DN 450",null,733.36,"142039045","100820","4037494165430",733.4,"101935",3.999999999996362E-2,null,null,null,733.4,3.999999999996362E-2,733.4,733.36]
["101936",101936,null,"STK","ICS 500 Winkel 90°","CHF",783.8,"Schiedel ICS glänzend",13.6,0,"J","ICS 500 Coude 90°","ICS 500 Winkel 90°","ICS 500 Gomito 90°",133,1,"DN 500",null,783.83,"142039050","100821","4037494165447",783.8,"101936",-3.0000000000086402E-2,null,null,null,783.8,-3.0000000000086402E-2,783.8,783.83]
["101937",101937,null,"STK","ICS 600 Winkel 90°","CHF",939.4,"Schiedel ICS glänzend",18,0,"J","ICS 600 Coude 90°","ICS 600 Winkel 90°","ICS 600 Gomito 90°",133,1,"DN 600",null,939.36,"142039060","100822","4037494165461",939.4,"101937",3.999999999996362E-2,null,null,null,939.4,3.999999999996362E-2,939.4,939.36]
["101938",101938,null,"STK","ICS 700 Winkel 90°","CHF",1064,"Schiedel ICS glänzend",22.89,0,"J","ICS 700 Coude 90°","ICS 700 Winkel 90°","ICS 700 Gomito 90°",133,1,"DN 700",null,1063.99,"142039070","100823","4037494165478",1064,"101938",9.9999999999909051E-3,null,null,null,1064,9.9999999999909051E-3,1064,1063.99]
["101939",101939,null,"STK","ICS 80 Inspektions-Winkel 90°","CHF",325.5,"Schiedel ICS glänzend",1.61,0,"J","ICS 80 Coude avec 'inspection 90°","ICS 80 Inspektions-Winkel 90°","ICS 80 Gmoito con revisione 90°",133,1,"DN 80",null,325.48,"142039208","100824","4037494177310",325.5,"101939",1.999999999998181E-2,null,null,null,325.5,1.999999999998181E-2,325.5,325.48]
["101940",101940,null,"STK","ICS 100 Inspektions-Winkel 90°","CHF",328.6,"Schiedel ICS glänzend",2.02,0,"J","ICS 100 Coude avec 'inspection 90°","ICS 100 Inspektions-Winkel 90°","ICS 100 Gmoito con revisione 90°",133,1,"DN 100",null,328.57,"142039210","100825","4037494177334",328.6,"101940",3.0000000000029559E-2,null,null,null,328.6,3.0000000000029559E-2,328.6,328.57]
["101941",101941,null,"STK","ICS 130 Inspektions-Winkel 90°","CHF",353.3,"Schiedel ICS glänzend",2.68,0,"J","ICS 130 Coude avec 'inspection 90°","ICS 130 Inspektions-Winkel 90°","ICS 130 Gmoito con revisione 90°",133,1,"DN 130",null,353.29,"142039213","100826","4037494177358",353.3,"101941",9.9999999999909051E-3,null,null,null,353.3,9.9999999999909051E-3,353.3,353.29]
["101942",101942,null,"STK","ICS 150 Inspektions-Winkel 90°","CHF",383.2,"Schiedel ICS glänzend",3.05,0,"J","ICS 150 Coude avec 'inspection 90°","ICS 150 Inspektions-Winkel 90°","ICS 150 Gmoito con revisione 90°",133,1,"DN 150",null,383.16,"142039215","100827","4037494177372",383.2,"101942",3.999999999996362E-2,null,null,null,383.2,3.999999999996362E-2,383.2,383.16]
["101943",101943,null,"STK","ICS 180 Inspektions-Winkel 90°","CHF",309,"Schiedel ICS glänzend",3.68,0,"J","ICS 180 Coude avec 'inspection 90°","ICS 180 Inspektions-Winkel 90°","ICS 180 Gmoito con revisione 90°",133,1,"DN 180",null,268,"142039218","100828","4037494177396",309,"101943",41,null,null,null,309,41]
["101944",101944,null,"STK","ICS 200 Inspektions-Winkel 90°","CHF",420.2,"Schiedel ICS glänzend",3.98,0,"J","ICS 200 Coude avec 'inspection 90°","ICS 200 Inspektions-Winkel 90°","ICS 200 Gmoito con revisione 90°",133,1,"DN 200",null,420.24,"142039220","100829","4037494177419",420.2,"101944",-4.0000000000020464E-2,null,null,null,420.2,-4.0000000000020464E-2,420.2,420.24]
["101945",101945,null,"STK","ICS 250 Inspektions-Winkel 90°","CHF",445,"Schiedel ICS glänzend",5.12,0,"J","ICS 250 Coude avec 'inspection 90°","ICS 250 Inspektions-Winkel 90°","ICS 250 Gmoito con revisione 90°",133,1,"DN 250",null,444.96,"142039225","100830","4037494177433",445,"101945",4.0000000000020464E-2,null,null,null,445,4.0000000000020464E-2,445,444.96]
["101946",101946,null,"STK","ICS 300 Inspektions-Winkel 90°","CHF",451.1,"Schiedel ICS glänzend",6.74,0,"J","ICS 300 Coude avec 'inspection 90°","ICS 300 Inspektions-Winkel 90°","ICS 300 Gmoito con revisione 90°",133,1,"DN 300",null,451.14,"142039230","100831","4037494177457",451.1,"101946",-3.999999999996362E-2,null,null,null,451.1,-3.999999999996362E-2,451.1,451.14]
["101947",101947,null,"STK","ICS 350 Inspektions-Winkel 90°","CHF",683,"Schiedel ICS glänzend",8.18,0,"J","ICS 350 Coude avec 'inspection 90°","ICS 350 Inspektions-Winkel 90°","ICS 350 Gmoito con revisione 90°",133,1,"DN 350",null,593.28,"142039235","100832","4037494177471",683,"101947",89.720000000000027,null,null,null,683,89.720000000000027]
["101948",101948,null,"STK","ICS 400 Inspektions-Winkel 90°","CHF",1012.5,"Schiedel ICS glänzend",10.3,0,"J","ICS 400 Coude avec 'inspection 90°","ICS 400 Inspektions-Winkel 90°","ICS 400 Gmoito con revisione 90°",133,1,"DN 400",null,1012.49,"142039240","100833","4037494177488",1012.5,"101948",9.9999999999909051E-3,null,null,null,1012.5,9.9999999999909051E-3,1012.5,1012.49]
["101949",101949,null,"STK","ICS 450 Inspektions-Winkel 90°","CHF",1082.5,"Schiedel ICS glänzend",13.164,0,"J","ICS 450 Coude avec 'inspection 90°","ICS 450 Inspektions-Winkel 90°","ICS 450 Gmoito con revisione 90°",133,1,"DN 450",null,1082.53,"142039245","100834","4037494177495",1082.5,"101949",-2.9999999999972715E-2,null,null,null,1082.5,-2.9999999999972715E-2,1082.5,1082.53]
["101950",101950,null,"STK","ICS 500 Inspektions-Winkel 90°","CHF",1143.3,"Schiedel ICS glänzend",15.371,0,"J","ICS 500 Coude avec 'inspection 90°","ICS 500 Inspektions-Winkel 90°","ICS 500 Gmoito con revisione 90°",133,1,"DN 500",null,1143.3,"142039250","100835","4037494177501",1143.3,"101950",0,null,null,null,1143.3,0,1143.3,1143.3]
["101951",101951,null,"STK","ICS 600 Inspektions-Winkel 90°","CHF",1312.2,"Schiedel ICS glänzend",20.262,0,"J","ICS 600 Coude avec 'inspection 90°","ICS 600 Inspektions-Winkel 90°","ICS 600 Gmoito con revisione 90°",133,1,"DN 600",null,1312.22,"142039260","100836","4037494177525",1312.2,"101951",-1.999999999998181E-2,null,null,null,1312.2,-1.999999999998181E-2,1312.2,1312.22]
["101952",101952,null,"STK","ICS 700 Inspektions-Winkel 90°","CHF",1449.2,"Schiedel ICS glänzend",25.789000000000001,0,"J","ICS 700 Coude avec 'inspection 90°","ICS 700 Inspektions-Winkel 90°","ICS 700 Gmoito con revisione 90°",133,1,"DN 700",null,1449.21,"142039270","100837","4037494177532",1449.2,"101952",-9.9999999999909051E-3,null,null,null,1449.2,-9.9999999999909051E-3,1449.2,1449.21]
["101968",101968,null,"PAR","ICM 700 Wandkonsolen (Paar) L500mm","CHF",181.5,"Schiedel ICM matt",5,0,"J","ICM 700 Console réglable ( 2 pces. ) L500mm","ICM 700 Wandkonsolen (Paar) L500mm","ICM 700 Wandkonsolen (Paar) L500mm",134,1,"DN 700",null,181.5,"95120700M",null,null,181.5,"101968",0,null,null,null,181.5,0,181.5,181.5]
["101969",101969,null,"PAR","ICM 750 Wandkonsolen (Paar) L500mm verstärkt","CHF",247.5,"Schiedel ICM matt",6,0,"J","ICM 750 Console réglable ( 2 pces. ) L500mm renforcée","ICM 750 Wandkonsolen (Paar) L500mm verstärkt","ICM 750 Supporto a muro 2 pezzi L500mm rinforzato",134,1,"ZBH ICM",null,247.5,"95120750M",null,null,247.5,"101969",0,null,null,null,247.5,0,247.5,247.5]
["101970",101970,null,"PAR","ICM 800 Wandkonsolen (Paar) L600mm","CHF",253,"Schiedel ICM matt",7,0,"J","ICM 800 Console réglable ( 2 pces. ) L600mm","ICM 800 Wandkonsolen (Paar) L600mm","ICM 800 Supporto a muro 2 pezzi L600mm",134,1,"ZBH ICM",null,253,"95120800M",null,null,253,"101970",0,null,null,null,253,0,253,253]
["101971",101971,null,"PAR","ICM 900 Wandkonsolen (Paar) L900mm","CHF",297,"Schiedel ICM matt",8,0,"J","ICM 900 Console réglable ( 2 pces. ) L900mm","ICM 900 Wandkonsolen (Paar) L900mm","ICM 900 Supporto a muro 2 pezzi L900mm",134,1,"ZBH ICM",null,297,"95120900M",null,null,297,"101971",0,null,null,null,297,0,297,297]
["101972",101972,null,"PAR","ICM 999 Wandkonsolen (Paar) L1304mm","CHF",429,"Schiedel ICM matt",9,0,"J","ICM 999 Console réglable ( 2 pces. ) L1304mm","ICM 999 Wandkonsolen (Paar) L1304mm","ICM 999 Supporto a muro 2 pezzi L1304mm",134,1,"ZBH ICM",null,429,"95120999M",null,null,429,"101972",0,null,null,null,429,0,429,429]
["102423",102423,null,"STK","ICM 80 Anschlussrosette EW Øi 130mm ØA 300mm ","CHF",42,"Schiedel ICM matt",0.3,0,"J","ICM 80 Rosace de raccordement EW Øi 130mm ØA 300mm","ICM 80 Anschlussrosette EW Øi 130mm ØA 300mm ","ICM 80 Rosetta collegamento EW Øi 130mm ØA 300mm",134,1,"DN 80",null,36.299999999999997,"025620013M",null,null,42,"102423",5.7000000000000028,null,null,null,42,5.7000000000000028]
["102424",102424,null,"STK","ICM 100 Anschlussrosette EW Øi 150mm ØA 320mm","CHF",46,"Schiedel ICM matt",0.36,0,"J","ICM 100 Rosace de raccordement EW Øi150mm ØA 320mm","ICM 100 Anschlussrosette EW Øi 150mm ØA 320mm","ICM 100 Rosetta collegamento EW Øi 150mm ØA 320mm",134,1,"DN 100",null,39.6,"025620015M",null,null,46,"102424",6.3999999999999986,null,null,null,46,6.3999999999999986]
["103831",103831,null,"STK","ZBH 160 Verschlusszapfen 2Stk. aus Schaumstoff","CHF",21.9,"ganztec-LEICHTBAUSCHACHT",0.1,0,"J","ZBH 160 Bouchons de fermeture prod. mousse 2 pces","ZBH 160 Verschlusszapfen 2Stk. aus Schaumstoff","ZBH 160 Tappi 2 pz. di schiuma",141,1,"ZBH ABS",null,19,"913815",null,null,21.9,"103831",2.8999999999999986,null,null,null,21.9,2.8999999999999986]
["104604",104604,null,"STK","TS120 Rev.rohr für Flex 60","CHF",145.1,"TECHNOSTAR 120",0.4,180,"J","TS120 60 Tuyau de revision pour flex","TS120 Rev.rohr für Flex 60","TS120 60 revisione per flessibile",121,1,"DN 60",null,131.9,"516012",null,null,145.1,"104604",13.199999999999989,null,null,null,145.1,13.199999999999989]
["104705",104705,null,"Stk","TS120 Messnippel weiss DN20 zu LAS","CHF",15.4,"TECHNOSTAR 120 LAS",0.02,0,"J","TS120 80 Joint torique bleu","TS120 Messnippel weiss DN20 zu LAS","TS120 80 Guarnizione per pezzo T",122,null,null,null,14,null,null,null,15.4,"104705",null,null,null,null,15.4,1.4000000000000004]
["104706",104706,null,"Stk","TS120 Rändelschraube Kunststoff zu LAS Messöffnung","CHF",2.9,"TECHNOSTAR 120 LAS",0.02,0,"J","TS120 80 Joint torique bleu","TS120 Rändelschraube Kunststoff zu LAS Messöffnung","TS120 80 Guarnizione per pezzo T",122,null,null,null,2.6,null,null,null,2.9,"104706",null,null,null,null,2.9,0.29999999999999982,2.9,2.8602358633202298]
["104707",104707,null,"Stk","TS120 14mm O Ring zu Rändelschraube LAS Messöffn.","CHF",6.6,"TECHNOSTAR 120 LAS",0.02,0,"J","TS120 80 Joint torique bleu","TS120 14mm O Ring zu Rändelschraube LAS Messöffn.","TS120 80 Guarnizione per pezzo T",122,null,null,null,6,null,null,null,6.6,"104707",null,null,null,null,6.6,0.59999999999999964]
["140682",140682,null,"Stk","TS120 160 Kesselanschluss auf 153mm","CHF",398.9,"TECHNOSTAR 120",1.25,"100","J","TS120 160 Raccordement 153","TS120 160 Kesselanschluss auf 153mm","TS120 160 Raccordo 153",121,null,"160",null,362.6,null,null,null,398.9,"140682",null,null,null,null,398.9,36.299999999999955]
["140681",140681,null,"Stk","TS120 125 Kesselanschluss auf 153mm","CHF",293.10000000000002,"TECHNOSTAR 120",1.0900000000000001,"100","J","TS120 125 Raccordement 153","TS120 125 Kesselanschluss auf 153mm","TS120 125 Raccordo 153",121,null,"125",null,266.39999999999998,null,null,null,293.10000000000002,"140681",null,null,null,null,293.10000000000002,26.700000000000045]
["140680",140680,null,"Stk","TS120 110 Kesselanschluss auf 153mm","CHF",301.10000000000002,"TECHNOSTAR 120",0.89,"100","J","TS120 160 Tube avec manchon L500mm","TS120 110 Kesselanschluss auf 153mm","TS120 160 Tubo con manicotto L500mm",121,null,"110",null,273.69,null,null,null,301.10000000000002,"140680",null,null,null,null,301.10000000000002,27.410000000000025]
["140683",140683,null,"Stk","TS120 200 Kesselanschluss auf 153mm","CHF",473.1,"TECHNOSTAR 120",1.67,"100","J","TS120 200 Raccordement 153","TS120 200 Kesselanschluss auf 153mm","TS120 200 Raccordo 153",121,null,"200",null,430.05,null,null,null,473.1,"140683",null,null,null,null,473.1,43.050000000000011]
["140684",140684,null,"Stk","TS120 110 Kesselanschluss auf 183mm","CHF",356.9,"TECHNOSTAR 120",1.44,"100","J","TS120 110 Raccordement 183","TS120 110 Kesselanschluss auf 183mm","TS120 110 Raccordo 183",121,null,"110",null,324.42,null,null,null,356.9,"140684",null,null,null,null,356.9,32.479999999999961]
["140685",140685,null,"Stk","TS120 125 Kesselanschluss auf183mm","CHF",372.3,"TECHNOSTAR 120",1.58,"100","J","TS120 125 Raccordement 183","TS120 125 Kesselanschluss auf183mm","TS120 125 Raccordo 183",121,null,"125",null,338.37,null,null,null,372.3,"140685",null,null,null,null,372.3,33.930000000000007]
["140686",140686,null,"Stk","TS120 160 Kesselanschluss auf 183mm","CHF",391.8,"TECHNOSTAR 120",1.59,"100","J","TS120 160 Raccordement 183","TS120 160 Kesselanschluss auf 183mm","TS120 160 Raccordo 183",121,null,"160",null,356.16,null,null,null,391.8,"140686",null,null,null,null,391.8,35.639999999999986]
["140687",140687,null,"Stk","TS120 200 Kesselanschluss auf 183mm","CHF",480,"TECHNOSTAR 120",1.76,"100","J","TS120 200 Raccordement 183","TS120 200 Kesselanschluss auf 183mm","TS120 200 Raccordo 183",121,null,"200",null,436.34,null,null,null,480,"140687",null,null,null,null,480,43.660000000000025]
["140688",140688,null,"Stk","TS120 160 Kesselanschluss auf 203mm","CHF",429,"TECHNOSTAR 120",1.93,"100","J","TS120 160 Raccordement 203","TS120 160 Kesselanschluss auf 203mm","TS120 160 Raccordo 203",121,null,"160",null,389.91,null,null,null,429,"140688",null,null,null,null,429,39.089999999999975]
["140689",140689,null,"Stk","TS120 200 Kesselanschluss auf 203mm","CHF",408.6,"TECHNOSTAR 120",1.8,"100","J","TS120 200 Raccordement 203","TS120 200 Kesselanschluss auf 203mm","TS120 200 Raccordo 203",121,null,"200",null,371.44,null,null,null,408.6,"140689",null,null,null,null,408.6,37.160000000000025]
["140690",140690,null,"Stk","TS120 250 Kesselanschluss auf 203mm","CHF",566.4,"TECHNOSTAR 120",2.4,"100","J","TS120 250 Raccordement 203","TS120 250 Kesselanschluss auf 203mm","TS120 250 Raccordo 203",121,null,"250",null,514.82000000000005,null,null,null,566.4,"140690",null,null,null,null,566.4,51.579999999999927]
["140691",140691,null,"Stk","TS120 160 Kesselanschluss auf 253mm","CHF",491.5,"TECHNOSTAR 120",2.02,"100","J","TS120 160 Raccordement 253","TS120 160 Kesselanschluss auf 253mm","TS120 160 Raccordo 253",121,null,"160",null,446.78,null,null,null,491.5,"140691",null,null,null,null,491.5,44.720000000000027]
["140692",140692,null,"Stk","TS120 200 Kesselanschluss auf 253mm","CHF",481,"TECHNOSTAR 120",2.5499999999999998,"100","J","TS120 200 Raccordement 253","TS120 200 Kesselanschluss auf 253mm","TS120 200 Raccordo 253",121,null,"200",null,437.23,null,null,null,481,"140692",null,null,null,null,481,43.769999999999982]
["104679",104679,null,"Stk","ISOLIT 160 Basten Standard Inox eckig ","CHF",323,"ISOLIT",3.6,"300","J","ISOLIT 160 Cape Basten Standard Inox ","ISOLIT 160 Basten Standard Inox eckig ","ISOLIT 160 Basten Standard Inox ",114,null,"160",null,304,null,null,null,323,"104679",null,null,null,null,323,19]
["140693",140693,null,"Stk","TS120 250 Kesselanschluss auf 253mm","CHF",507.3,"TECHNOSTAR 120",2.95,"100","J","TS120 250 Raccordement 253","TS120 250 Kesselanschluss auf 253mm","TS120 250 Raccordo 253",121,null,"250",null,461.17,null,null,null,507.3,"140693",null,null,null,null,507.3,46.129999999999995]
["140694",140694,null,"Stk","TS120 315 Kesselanschluss auf 253mm","CHF",556.6,"TECHNOSTAR 120",3.36,"100","J","TS120 315 Raccordement 253","TS120 315 Kesselanschluss auf 253mm","TS120 315 Raccordo 253",121,null,"315",null,505.94,null,null,null,556.6,"140694",null,null,null,null,556.6,50.660000000000025]
["140695",140695,null,"Stk","TS120 250 Kesselanschluss auf 303mm","CHF",590,"TECHNOSTAR 120",3.12,"100","J","TS120 250 Raccordement 303","TS120 250 Kesselanschluss auf 303mm","TS120 250 Raccordo 303",121,null,"250",null,536.28,null,null,null,590,"140695",null,null,null,null,590,53.720000000000027]
[{"$f":"B4637&\"\"","v":"140696"},140696,null,"Stk",{"$f":"IF($E$200=2,L4637,IF($E$200=3,N4637,M4637))","v":"TS120 315 Kesselanschluss auf 303mm"},"CHF",{"$f":"IF($L$190=1,W4637,S4637)","v":674},"TECHNOSTAR 120",5.25,"100","J","TS120 315 Raccordement 303","TS120 315 Kesselanschluss auf 303mm","TS120 315 Raccordo 303",121,null,"315",null,612.72,null,null,null,674,"140696",null,null,null,null,674,61.279999999999973]
["140698",140698,null,"Stk","TS120 125 Flexrohr verschraubbar L1000mm","CHF",139.5,"TECHNOSTAR 120",1.7,"1000","J","TS120 125 Tube flexible   L1000mm vissés","TS120 125 Flexrohr verschraubbar L1000mm","TS120 125 Tubo flessibile  L1000mm avitato",121,null,"125",null,126.8,null,null,null,139.5,"140698",null,null,null,null,139.5,12.700000000000003]
["140699",140699,null,"Stk","TS120 125  Revisionsrohr für Flex ","CHF",325.8,"TECHNOSTAR 120",0.25,"322","J","TS120 160 Tube de révision pour flexible court","TS120 125  Revisionsrohr für Flex ","TS120 160 Tubo de revisione per flessibile breve",121,null,"125",null,296.10000000000002,null,null,null,325.8,"140699",null,null,null,null,325.8,29.699999999999989]
["140700",140700,null,"Stk","TS120 125 Abstandhalter für flex ","CHF",38.700000000000003,"TECHNOSTAR 120",0.05,0,"J","TS120 125 Distanceur pour  flexibles ","TS120 125 Abstandhalter für flex ","TS120 125 Distanzatori per flessibile ",121,null,"125",null,35.1,null,null,null,38.700000000000003,"140700",null,null,null,null,38.700000000000003,3.6000000000000014]
["140701",140701,null,"Stk","TS120 125 Aufhängeschelle zu Flex ","CHF",43.3,"TECHNOSTAR 120",0.15,0,"J","TS120 160 Suspension pour flexible","TS120 125 Aufhängeschelle zu Flex ","TS120 160 Suspensione per flessibile",121,null,"125",null,39.299999999999997,null,null,null,43.3,"140701",null,null,null,null,43.3,4]
["140702",140702,null,"Stk","TS120 125 Kaminkopfabdeckung schwarz","CHF",363.8,"TECHNOSTAR 120",1,"400","J","TS120 160 Recouvrement se souche flexible Inox","TS120 125 Kaminkopfabdeckung schwarz","TS120 160 Copertura del tombino tubo fless. Inox",121,null,"125",null,330.7,null,null,null,363.8,"140702",null,null,null,null,363.8,33.100000000000023]
["140703",140703,null,"Stk","LBS Sparrenhalter zu Leichtbauschacht 14 bis 20","CHF",143,"ganztec-LEICHTBAUSCHACHT",28.8,"0","J","LBS Gaine d'inst. légère ?i 230mm ?E 320mm L1000mm","LBS Sparrenhalter zu Leichtbauschacht 14 bis 20","LBS 230 Elemento installatione leggermente  ",141,null,"0",null,114,null,null,null,143,"140703",null,null,null,null,143,29]
["140704",140704,null,"Stk","LBS Sparrenhalter zu Leichtbauschacht 22 bis 32","CHF",143,"ganztec-LEICHTBAUSCHACHT",2,"0","J","LBS Gaine d'inst. légère ?i 230mm ?E 320mm L1000mm","LBS Sparrenhalter zu Leichtbauschacht 22 bis 32","LBS 230 Elemento installatione leggermente  ",141,null,"0",null,114,null,null,null,143,"140704",null,null,null,null,143,29]
["140705",140705,null,"Stk","LBS Sparrenhalter zu Leichtbauschacht 35 bis 40","CHF",143,"ganztec-LEICHTBAUSCHACHT",2,"0","J","LBS Gaine d'inst. légère ?i 230mm ?E 320mm L1000mm","LBS Sparrenhalter zu Leichtbauschacht 35 bis 40","LBS 230 Elemento installatione leggermente  ",141,null,"0",null,114,null,null,null,143,"140705",null,null,null,null,143,29]
["140709",140709,null,"Stk","ABS 300 Schleifung EZ 5° auf Bestellung","CHF",1973,"Schiedel ABSOLUT",230,"0","J","ABS 250 Déviation EZ 5° sur commande, 2 angles","ABS 300 Schleifung EZ 5° auf Bestellung","ABS 250 Deviazione EZ 5° su ordinazione",111,null,"300",null,1715,null,null,null,1973,"140709",null,null,null,null,1973,258]
["140710",140710,null,"Stk","ABS 300 Schleifung EZ 10° auf Bestellung","CHF",1973,"Schiedel ABSOLUT",230,"0","J","ABS 250 Déviation EZ 5° sur commande, 2 angles","ABS 300 Schleifung EZ 10° auf Bestellung","ABS 250 Deviazione EZ 5° su ordinazione",111,null,"300",null,1715,null,null,null,1973,"140710",null,null,null,null,1973,258]
["140711",140711,null,"Stk","ABS 300 Schleifung EZ 15° auf Bestellung","CHF",1973,"Schiedel ABSOLUT",230,"0","J","ABS 250 Déviation EZ 5° sur commande, 2 angles","ABS 300 Schleifung EZ 15° auf Bestellung","ABS 250 Deviazione EZ 5° su ordinazione",111,null,"300",null,1715,null,null,null,1973,"140711",null,null,null,null,1973,258]
["140712",140712,null,"Stk","ABS 300 Schleifung EZ 20° auf Bestellung","CHF",1973,"Schiedel ABSOLUT",230,"0","J","ABS 250 Déviation EZ 5° sur commande, 2 angles","ABS 300 Schleifung EZ 20° auf Bestellung","ABS 250 Deviazione EZ 5° su ordinazione",111,null,"300",null,1715,null,null,null,1973,"140712",null,null,null,null,1973,258]
["140713",140713,null,"Stk","ABS 300 Schleifung EZ 25° auf Bestellung","CHF",1973,"Schiedel ABSOLUT",230,"0","J","ABS 250 Déviation EZ 5° sur commande, 2 angles","ABS 300 Schleifung EZ 25° auf Bestellung","ABS 250 Deviazione EZ 5° su ordinazione",111,null,"300",null,1715,null,null,null,1973,"140713",null,null,null,null,1973,258]
["140714",140714,null,"Stk","ABS 300 Schleifung EZ 30° auf Bestellung","CHF",1973,"Schiedel ABSOLUT",230,"0","J","ABS 250 Déviation EZ 5° sur commande, 2 angles","ABS 300 Schleifung EZ 30° auf Bestellung","ABS 250 Deviazione EZ 5° su ordinazione",111,null,"300",null,1715,null,null,null,1973,"140714",null,null,null,null,1973,258]
["140715",140715,null,"Stk","ABS 300 Schleifung EZ 35° auf Bestellung","CHF",1973,"Schiedel ABSOLUT",230,"0","J","ABS 250 Déviation EZ 5° sur commande, 2 angles","ABS 300 Schleifung EZ 35° auf Bestellung","ABS 250 Deviazione EZ 5° su ordinazione",111,null,"300",null,1715,null,null,null,1973,"140715",null,null,null,null,1973,258]
["140716",140716,null,"Stk","Verschlussdeckel Messing 3/4\" ","CHF",9,"Schiedel ICM matt",0.2,"25","J","PPL EPDM Embout de mesure","Verschlussdeckel Messing 3/4\" ","PPL EPDM Tappo di misura",134,null,"36",null,7.7,null,null,null,9,"140716",null,null,null,null,9,1.2999999999999998]
["140718",140718,null,"Stk","ABS Gewindestangen M20 zu Kaminhalterung","CHF",82,"Schiedel ABSOLUT",4.0999999999999996,"0","J","ABS Set de renforcement du système de fixation","ABS Gewindestangen M20 zu Kaminhalterung","ABS Rinforzato per fisaggio della canna fumaria",111,null,null,null,71,null,null,null,82,"140718",null,null,null,null,82,11]
["140726",140726,null,"Stk","ICM5000 200 Element mit Empa Messstutzen","CHF",685,"Schiedel ICM5000",2.6,"450","J","ICM5000 200 Elément avec manchon de mesure EMPA","ICM5000 200 Element mit Empa Messstutzen","ICM5000 200 Elemento di misura EMPA",136,null,"200",null,595.1,null,null,null,685,"140726",null,null,null,null,685,89.899999999999977]
["140727",140727,null,"Stk","ABS Schleifung DZTL  0 - 35° 120 bis 200 ","CHF",1947,"Schiedel ABSOLUT",120,"0","J","ABS 120-200 Déviation DZ  0 - 35° 120 - 200,","ABS Schleifung DZTL  0 - 35° 120 bis 200 ","ABS Deviazione DZ 0 - 35° 120 - 200 su ordinazione",111,null,"0",null,1693,null,null,null,1947,"140727",null,null,null,null,1947,254]
["140728",140728,null,"Stk","ABS Schleifung EZTL  0 - 35° 120 bis 200 ","CHF",1673,"Schiedel ABSOLUT",80,"0","J","ABS 120-200 Déviation DZ  0 - 35° 120 - 200,","ABS Schleifung EZTL  0 - 35° 120 bis 200 ","ABS Deviazione DZ 0 - 35° 120 - 200 su ordinazione",111,null,"0",null,1454,null,null,null,1673,"140728",null,null,null,null,1673,219]
["140729",140729,null,"Stk","ABS Schleifung EZTL  0 - 35° 250","CHF",1513,"Schiedel ABSOLUT",100,"0","J","ABS 120-200 Déviation DZ  0 - 35° 120 - 200,","ABS Schleifung EZTL  0 - 35° 250","ABS Deviazione DZ 0 - 35° 120 - 200 su ordinazione",111,null,"0",null,1315,null,null,null,1513,"140729",null,null,null,null,1513,198]
["140730",140730,null,"Stk","ABS Schleifung EZTL  0 - 35° 300","CHF",2104,"Schiedel ABSOLUT",140,"0","J","ABS 120-200 Déviation DZ  0 - 35° 120 - 200,","ABS Schleifung EZTL  0 - 35° 300","ABS Deviazione DZ 0 - 35° 120 - 200 su ordinazione",111,null,"300",null,1829,null,null,null,2104,"140730",null,null,null,null,2104,275]
["140731",140731,null,"Stk","ABS Schleifung EZTL  0 - 35° 400","CHF",3073,"Schiedel ABSOLUT",160,"0","J","ABS 120-200 Déviation DZ  0 - 35° 120 - 200,","ABS Schleifung EZTL  0 - 35° 400","ABS Deviazione DZ 0 - 35° 120 - 200 su ordinazione",111,null,"400",null,2672,null,null,null,3073,"140731",null,null,null,null,3073,401]
["140738",140738,null,"Stk","ICM5000 200 Anschluss von DW auf EW in Rauchgasr.","CHF",328,"Schiedel ICM5000",2.4,"150","J","ICM5000 200 Anschluss von DW auf EW in Rauchgasr.","ICM5000 200 Anschluss von DW auf EW in Rauchgasr.","ICM5000 200 Anschluss von DW auf EW in Rauchgasr.",136,null,"200",null,284.89999999999998,null,null,null,328,"140738",null,null,null,null,328,43.100000000000023]
["140739",140739,null,"Stk","ICM5000 300 Anschluss von DW auf EW inkl. Flansch","CHF",395,"Schiedel ICM5000",2.8,"150","J","ICM5000 300 Anschluss von DW auf EW inkl. Flansch","ICM5000 300 Anschluss von DW auf EW inkl. Flansch","ICM5000 300 Anschluss von DW auf EW inkl. Flansch",136,null,"300",null,343.2,null,null,null,395,"140739",null,null,null,null,395,51.800000000000011]
["104693",104693,null,"Stk","ABS 250 Basten Standard Inox Stutzen rund  ","CHF",400,"Schiedel ABSOLUT",5.5,"300","J","ABS 250 Cap Basten Standard Inox Stutzen rund  ","ABS 250 Basten Standard Inox Stutzen rund  ","ABS 250 Basten Standard Inox Stutzen rund  ",111,null,"250",null,377,null,null,null,400,"104693",null,null,null,null,400,23]
["140770",140770,null,"Stk","ICM5000 180 Element mit Empa Messstutzen","CHF",658,"Schiedel ICM5000",2.6,"450","J","ICM5000 180 Elément avec manchon de mesure EMPA","ICM5000 180 Element mit Empa Messstutzen","ICM5000 180 Elemento di misura EMPA",136,null,"180",null,572,null,null,null,658,"140770",null,null,null,null,658,86]
["140785",140785,null,"Stk","ICM 400 Element mit Empa Messstutzen","CHF",1301,"Schiedel ICM matt",3.0489999999999999,"450","J","ICM 400 Elément avec manchon de mesure EMPA","ICM 400 Element mit Empa Messstutzen","ICM 400 Elemento di misura EMPA",134,null,"400",null,1130.8,null,null,null,1301,"140785",null,null,null,null,1301,170.20000000000005]
["140773",140773,null,"Stk","ZBH Glasfaserschnur gedreht/umstrickt 6mm","CHF",5.8,"Zubehör",0.1,1000,"J","TS120 Bande de fibre de céramique 35mm L1000","ZBH Glasfaserschnur gedreht/umstrickt 6mm","TS120 nastro in fibra di ceramica 35mm L1000",15,null,"6",null,5,null,null,null,5.8,"140773",null,null,null,null,5.8,0.79999999999999982]
["140776",140776,null,"Stk","ABS 180 Grundplatte mit Abkantung zu ICM250","CHF",341,"Schiedel ABSOLUT",0,"150","J","ABS 180 Plaque de base  avec la bordure ICM250","ABS 180 Grundplatte mit Abkantung zu ICM250","ABS 180 Piastra di base con bordo a ICM250",111,null,"180",null,296,null,null,null,341,"140776",null,null,null,null,341,45]
["140787",140787,null,"Stk","ABS Handyplatte EZ Kupfer 360 x 360mm  ","CHF",229,"Schiedel ABSOLUT",3.4,"0","J","ABS Plaque Handy EZ Inox 360 x 360mm  ","ABS Handyplatte EZ Kupfer 360 x 360mm  ","ABS Lastra Handy EZ Inox 360 x 360mm  ",111,null,"0",null,199,null,null,null,229,"140787",null,null,null,null,229,30]
["140788",140788,null,"Stk","ABS Handyplatte EZ Kupfer 380 x 380mm ","CHF",241,"Schiedel ABSOLUT",3.6,"0","J","ABS Plaque Handy EZ Inox 380 x 380mm  ","ABS Handyplatte EZ Kupfer 380 x 380mm ","ABS Lastra Handy EZ Inox 380 x 380mm  ",111,null,"0",null,209,null,null,null,241,"140788",null,null,null,null,241,32]
["140789",140789,null,"Stk","ABS Handyplatte EZ Kupfer 480 x 480mm","CHF",260,"Schiedel ABSOLUT",4.5,"0","J","ABS Plaque Handy EZ Inox 480 x 480mm","ABS Handyplatte EZ Kupfer 480 x 480mm","ABS Lastra Handy EZ Inox 480 x 480mm",111,null,"0",null,226,null,null,null,260,"140789",null,null,null,null,260,34]
["140790",140790,null,"Stk","ABS Handyplatte EZ Kupfer 550 x 550mm  ","CHF",279,"Schiedel ABSOLUT",4.8,"0","J","ABS Plaque Handy EZ Inox 550 x 550mm  ","ABS Handyplatte EZ Kupfer 550 x 550mm  ","ABS Lastra Handy EZ Inox 550 x 550mm  ",111,null,"0",null,242,null,null,null,279,"140790",null,null,null,null,279,37]
["140791",140791,null,"Stk","ABS Handyplatte EZ Kupfer 670 x 670mm ","CHF",303,"Schiedel ABSOLUT",5.0999999999999996,"0","J","ABS Plaque Handy EZ Inox 670 x 670mm ","ABS Handyplatte EZ Kupfer 670 x 670mm ","ABS Lastra Handy EZ Inox 670 x 670mm ",111,null,"0",null,263,null,null,null,303,"140791",null,null,null,null,303,40]
["140793",140793,null,"Stk","CHZ 160 Keramik Rauchrohrstutzen 90° für RA  lose","CHF",75,"Schiedel CHEMINEE ZUG",18,100,"J","CHZ 160 Raccord de conduit de fumée 90° RA en vrac","CHZ 160 Keramik Rauchrohrstutzen 90° für RA  lose","CHZ 160 Elemento con raccordo RA 90° sciolto",112,null,"160",null,65,null,null,null,75,"140793",null,null,null,null,75,10]
["140794",140794,null,"Stk","CHZ 180 Keramik Rauchrohrstutzen 90° für RA  lose","CHF",82,"Schiedel CHEMINEE ZUG",18,100,"J","CHZ 180 Raccord de conduit de fumée 90° RA en vrac","CHZ 180 Keramik Rauchrohrstutzen 90° für RA  lose","CHZ 180 Elemento con raccordo RA 90° sciolto",112,null,"180",null,71,null,null,null,82,"140794",null,null,null,null,82,11]
["140795",140795,null,"Stk","CHZ 200 Keramik Rauchrohrstutzen 90° für RA  lose","CHF",89,"Schiedel CHEMINEE ZUG",18,100,"J","CHZ 200 Raccord de conduit de fumée 90° RA en vrac","CHZ 200 Keramik Rauchrohrstutzen 90° für RA  lose","CHZ 200 Elemento con raccordo RA 90° sciolto",112,null,"200",null,77,null,null,null,89,"140795",null,null,null,null,89,12]
["140796",140796,null,"Stk","CHZ 160 Keramik Rauchrohrstutzen 45° für RA  lose","CHF",75,"Schiedel CHEMINEE ZUG",18,100,"J","CHZ 160 Raccord de conduit de fumée 90° RA en vrac","CHZ 160 Keramik Rauchrohrstutzen 45° für RA  lose","CHZ 160 Elemento con raccordo RA 90° sciolto",112,null,"160",null,65,null,null,null,75,"140796",null,null,null,null,75,10]
["140797",140797,null,"Stk","CHZ 180 Keramik Rauchrohrstutzen 45° für RA  lose","CHF",82,"Schiedel CHEMINEE ZUG",18,100,"J","CHZ 180 Raccord de conduit de fumée 45° RA en vrac","CHZ 180 Keramik Rauchrohrstutzen 45° für RA  lose","CHZ 180 Elemento con raccordo RA 45° sciolto",112,null,"180",null,71,null,null,null,82,"140797",null,null,null,null,82,11]
["140798",140798,null,"Stk","CHZ 200 Keramik Rauchrohrstutzen 45° für RA  lose","CHF",89,"Schiedel CHEMINEE ZUG",18,100,"J","CHZ 200 Raccord de conduit de fumée 45° RA en vrac","CHZ 200 Keramik Rauchrohrstutzen 45° für RA  lose","CHZ 200 Elemento con raccordo RA 45° sciolto",112,null,"200",null,77,null,null,null,89,"140798",null,null,null,null,89,12]
["140801",140801,null,"Stk","PPL 250 Längenelement L500mm","CHF",123,"Schiedel PRIMA PLUS",1.9,"165","J","PPL 250 Elément droit L500mm","PPL 250 Längenelement L500mm","PPL 250 Elemento lunghezza L500mm",131,null,"250",null,106.7,null,null,null,123,"140801",null,null,null,null,123,16.299999999999997]
["140802",140802,null,"Stk","CHI 160 CHI Flexrohr 2 lagig Rolle a 12000mm","CHF",1630,"Schiedel CHIMFLEX",21,"0","J","CHI 160 Tuyau fléxible 2 plis rouleau a 12000mm","CHI 160 CHI Flexrohr 2 lagig Rolle a 12000mm","CHI 160 Tubo flessibile 2 veli rotolo a12000mm",132,null,"160",null,1416.8,null,null,null,1630,"140802",null,null,null,null,1630,213.20000000000005]
["140803",140803,null,"Stk","CHI 160 Adapter von Flex zu PPL ","CHF",92,"Schiedel CHIMFLEX",0.33,"150","J","CHI 160 Adapteur PPL pour Flex","CHI 160 Adapter von Flex zu PPL ","CHI 160 Giunto femminale Flex/ PPL",132,null,"160",null,79.2,null,null,null,92,"140803",null,null,null,null,92,12.799999999999997]
["140804",140804,null,"Stk","PPL 160 Kesselanschluss DN + 6mm L150mm","CHF",97,"Schiedel PRIMA PLUS",0.19,150,"J","PPL 160 Raccordement chaudière DN + 6mm L150mm","PPL 160 Kesselanschluss DN + 6mm L150mm","PPL 160 Raccordo di riscaldemento DN + 6mm L150mm",131,null,"160",null,83.6,null,null,null,97,"140804",null,null,null,null,97,13.400000000000006]
["140792",140792,null,"Stk","TS120LAS Schieber schwarz zu Deckel von Rev. Bogen","CHF",7.7,"TECHNOSTAR 120 LAS",1E-4,0,"J","TS120LAS Schieber schwarz zu Deckel von Rev. Bogen","TS120LAS Schieber schwarz zu Deckel von Rev. Bogen","TS120LAS Schieber schwarz zu Deckel von Rev. Bogen",122,null,"0",null,7,null,null,null,7.7,"140792",null,null,null,null,7.7,0.70000000000000018]
["140805",140805,null,"Stk","ICM 400 Winkel 15°","CHF",371,"Schiedel ICM matt",5.0039999999999996,"0","J","ICM 350 Coude 15°","ICM 400 Winkel 15°","ICM 350 Gomito 15°",134,null,"350",null,322.3,null,null,null,371,"140805",null,null,null,null,371,48.699999999999989]
["140806",140806,null,"Stk","ICM 400 Winkel 15°","CHF",520,"Schiedel ICM matt",7.6310000000000002,"0","J","ICM 400 Coude 30°","ICM 400 Winkel 15°","ICM 400 Gomito 30°",134,null,"400",null,452.1,null,null,null,520,"140806",null,null,null,null,520,67.899999999999977]
["140807",140807,null,"Stk","ICM 450 Winkel 15°","CHF",658,"Schiedel ICM matt",7.6310000000000002,"0","J","ICM 450 Coude 30°","ICM 450 Winkel 15°","ICM 450 Gomito 30°",134,null,"450",null,572,null,null,null,658,"140807",null,null,null,null,658,86]
["140808",140808,null,"Stk","ICM 500 Winkel 15°","CHF",821,"Schiedel ICM matt",7.6310000000000002,"0","J","ICM 500 Coude 30°","ICM 500 Winkel 15°","ICM 500 Gomito 15°",134,null,"500",null,713.9,null,null,null,821,"140808",null,null,null,null,821,107.10000000000002]
["140809",140809,null,"Stk","ICM 600 Winkel 15°","CHF",986,"Schiedel ICM matt",7.6310000000000002,"0","J","ICM 500 Coude 30°","ICM 600 Winkel 15°","ICM 500 Gomito 15°",134,null,"600",null,856.9,null,null,null,986,"140809",null,null,null,null,986,129.10000000000002]
["140810",140810,null,"Stk","ICM 500 Element mit Empa Messstutzen","CHF",1760,"Schiedel ICM matt",7,500,"J","ICM 500 Elément avec manchon de mesure EMPA","ICM 500 Element mit Empa Messstutzen","ICM 500 Elemento di misura EMPA",134,null,"500",null,1530.1,null,null,null,1760,"140810",null,null,null,null,1760,229.90000000000009]
["140811",140811,null,"Stk","PPL 400 Erweiterung DN500 L150mm","CHF",274,"Schiedel PRIMA PLUS",2,150,"J","PPL 400 extension de diamètre DN450 L150mm","PPL 400 Erweiterung DN500 L150mm","PPL 400 Estensione di diametro DN450 L150mm",131,null,"400",null,237.6,null,null,null,274,"140811",null,null,null,null,274,36.400000000000006]
["140813",140813,null,"Stk","LBS 150 Leichtbauschacht NWi150mm NWA240mm L1000mm","CHF",113,"ganztec-LEICHTBAUSCHACHT",25,"1000","J","LBS Gaine d'inst. légère i 150mm E 240mm L1000mm","LBS 150 Leichtbauschacht NWi150mm NWA240mm L1000mm","LBS 150 Elemento installatione leggermente  ",141,null,"150",null,90,null,null,null,113,"140813",null,null,null,null,113,23]
["140816",140816,null,"Stk","TS120 60 Haube zu Kaminkopfabdeckung schwarz","CHF",23.9,"TECHNOSTAR 120",0.01,"20","J","TS120 80 Capot pour Recouvrement  souche noir","TS120 60 Haube zu Kaminkopfabdeckung schwarz","TS120 80 Cappuccio per copertura del tombino PE",121,null,"60",null,21.7,null,null,null,23.9,"140816",null,null,null,null,23.9,2.1999999999999993]
["140817",140817,null,"Stk","TS120 60 Dichtung zu Regenhaube Kaminkopf","CHF",12.6,"TECHNOSTAR 120",0.02,"5","J","TS120 80 Joint torique bleu","TS120 60 Dichtung zu Regenhaube Kaminkopf","TS120 80 Guarnizione per pezzo T",121,null,"60",null,11.4,null,null,null,12.6,"140817",null,null,null,null,12.6,1.1999999999999993]
["140818",140818,null,"Stk","LBS 450 Leichtbauschacht NWi450mm NWA540mm L1000mm","CHF",259,"ganztec-LEICHTBAUSCHACHT",43.3,"1000","J","LBS Gaine d'inst. légère i 450mm ext.540mm L1000mm","LBS 450 Leichtbauschacht NWi450mm NWA540mm L1000mm","LBS i 450 Elemento instal. leggermente ext 540mm",141,null,"450",null,207,null,null,null,259,"140818",null,null,null,null,259,52]
["140819",140819,null,"Stk","PPL 100 Basten Standard Kupfer zu Münd. Manchette","CHF",284,"Zubehör",3.9,"300","J","PPL 100 Basten Standard pour tôle de dilatation","PPL 100 Basten Standard Kupfer zu Münd. Manchette","PPL 100 Terminale Basten per manicotto di sbocco",15,null,"100",null,267,null,null,null,284,"140819",null,null,null,null,284,17]
["140822",140822,null,"Stk","PPL 150 Basten Standard Kupfer zu Münd. Manchette","CHF",326,"Zubehör",3.9,"300","J","PPL 150 Basten Standard pour tôle de dilatation","PPL 150 Basten Standard Kupfer zu Münd. Manchette","PPL 150 Terminale Basten per manicotto di sbocco",15,null,"150",null,307,null,null,null,326,"140822",null,null,null,null,326,19]
["140824",140824,null,"Stk","PPL 200 Basten Standard Kupfer zu Münd. Manchette","CHF",355,"Zubehör",3.9,"300","J","PPL 200 Basten Standard pour tôle de dilatation","PPL 200 Basten Standard Kupfer zu Münd. Manchette","PPL 200 Terminale Basten per manicotto di sbocco",15,null,"200",null,334,null,null,null,355,"140824",null,null,null,null,355,21]
["140825",140825,null,"Stk","PPL 250 Basten Standard Kupfer zu Münd. Manchette","CHF",374,"Zubehör",3.9,"300","J","PPL 250 Basten Standard pour tôle de dilatation","PPL 250 Basten Standard Kupfer zu Münd. Manchette","PPL 250 Terminale Basten per manicotto di sbocco",15,null,"250",null,352,null,null,null,374,"140825",null,null,null,null,374,22]
["140826",140826,null,"Stk","PPL 300 Basten Standard Kupfer zu Münd. Manchette","CHF",405,"Zubehör",3.9,"300","J","PPL 300 Basten Standard pour tôle de dilatation","PPL 300 Basten Standard Kupfer zu Münd. Manchette","PPL 300 Terminale Basten per manicotto di sbocco",15,null,"300",null,382,null,null,null,405,"140826",null,null,null,null,405,23]
["140828",140828,null,"Stk","TS120LAS 80/125 Dichtung125mm Revisionsbogendeckel","CHF",18.3,"TECHNOSTAR 120 LAS",0.01,0,"J","TS120LAS 80/125 Joint 125mm pur Cap de révision","TS120LAS 80/125 Dichtung125mm Revisionsbogendeckel","TS120LAS 80/125 125mm Guarnizione per Copertura",122,null,"80",null,16.600000000000001,null,null,null,18.3,"140828",null,null,null,null,18.3,1.6999999999999993]
[{"$f":"B4701&\"\"","v":"140831"},140831,null,"Stk",{"$f":"IF($E$200=2,L4701,IF($E$200=3,N4701,M4701))","v":"TS120 60 Sprengring UV zu Flex "},"CHF",{"$f":"IF($L$190=1,W4701,S4701)","v":38.5},"TECHNOSTAR 120",0.01,"10","J","TS120 60 Tube de d'embouchure et collier","TS120 60 Sprengring UV zu Flex ","TS120 60 Tubo finale et blomba di flessibile",121,null,"60",null,35,null,null,null,38.5,"140831",null,null,null,null,38.5,3.5]
["140820",140820,null,"Stk","PPL 130 Basten Standard Kupfer zu Münd. Manchette","CHF",305,"Zubehör",4.2,"300","J","PPL 130 Basten Standard cuivre tôle de dilatation","PPL 130 Basten Standard Kupfer zu Münd. Manchette","PPL 130 Terminale Basten rame manicotto di sbocco",15,null,"130",null,287,null,null,null,305,"140820",null,null,null,null,305,18]
["140830",140830,null,"Stk","TS120LAS 110/160 Verschlussblech RLA Betrieb weiss","CHF",52.8,"TECHNOSTAR 120 LAS",0.3,null,"J","TS120LAS 110/160 Plaque fermeture ILA blanc","TS120LAS 110/160 Verschlussblech RLA Betrieb weiss","TS120LAS 110/160 Piastra OFCST bianco",122,null,"110",null,48,null,null,null,52.8,"140830",null,null,null,null,52.8,4.7999999999999972]
["140829",140829,null,"Stk","TS120LAS 110/160 Abgasset Raumluftunabhängig GB162","CHF",139.1,"TECHNOSTAR 120 LAS",0.6,null,"J","TS120LAS 110/160 Set Echapment ensebl. pour GB162","TS120LAS 110/160 Abgasset Raumluftunabhängig GB162","TS120LAS 110/160 Set scarico insieme per GB162",122,null,"110",null,126.4,null,null,null,139.1,"140829",null,null,null,null,139.1,12.699999999999989]
["140821",140821,null,"Stk","TS120 160 Kesselanschluss Reduktion exzentr. 125","CHF",176.9,"TECHNOSTAR 120",0.3,"100","J","TS120 160 Raccordement reduction exzentr. 125","TS120 160 Kesselanschluss Reduktion exzentr. 125","TS120 160 Raccordement reduction exzentr. 125",121,null,"160",null,160.80000000000001,null,null,null,176.9,"140821",null,null,null,null,176.9,16.099999999999994]
["140833",140833,null,"Stk","TS120 125 250 Endmuffe schwarz mit Mündungsrohr","CHF",156.30000000000001,"TECHNOSTAR 120",0.16,"170","J","TS120 125/250 Manchon de final noi avec tube final","TS120 125 250 Endmuffe schwarz mit Mündungsrohr","TS120 125/250 Manica finale con tubo bocca L500mm",121,null,"125",null,142.1,null,null,null,156.30000000000001,"140833",null,null,null,null,156.30000000000001,14.200000000000017,156.30000000000001,156.32289083761717]

{"sheet":"Daten","index":28,"n_rows":807,"n_cols":123,"rows_kept":807,"cut":false,"hidden":true,"merged":[[116,0,116,1]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"INDEX(Daten!$T$3:$T$8,T1,1)","v":"ISOLIT20"},{"$f":"INDEX(V3:V6,T1,1)","v":"20"},null,null,null,{"$f":"INDEX(Daten!$Z$3:$Z$8,$T$1,1)","v":"44/44 cm"},null,null,null,null,null,null,null,null,null,null,null,null,"Frachtermittlung"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Verkn.","System","Ø",null,"Bezeichnung","System: Text1","Außenmaß","System: Text2","System: Text3","System: Text4",null,null,null,null,null,null,null,null,"Typ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kerastar 140","Gesamthöhe",null,"m",{"$f":"ROUND(BV3/1000,2)","v":1.68},null,{"$f":"ROUND(BX3/1000,2)","v":1.85},null,{"$f":"ROUND(BZ3/1000,2)","v":2.0099999999999998},null,{"$f":"ROUND(CB3/1000,2)","v":2.1800000000000002},null,{"$f":"ROUND(CD3/1000,2)","v":2.35},null,{"$f":"ROUND(CF3/1000,2)","v":2.5099999999999998},null,{"$f":"ROUND(CH3/1000,2)","v":2.68},null,{"$f":"ROUND(CJ3/1000,2)","v":2.85},null,{"$f":"ROUND(CL3/1000,2)","v":3.01},null,null,null,null,null,null,null,null,null,null,null,null,"ICS 080","Gesamthöhe",null,"m",{"$f":"ROUND(DC3/1000,2)","v":0.51},null,{"$f":"ROUND(DE3/1000,2)","v":0.71},null,{"$f":"ROUND(DG3/1000,2)","v":0.96},null,{"$f":"ROUND(DI3/1000,2)","v":1.17},null,{"$f":"ROUND(DK3/1000,2)","v":1.46},null,{"$f":"ROUND(DM3/1000,2)","v":1.67},null,{"$f":"ROUND(DO3/1000,2)","v":1.92}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U3&V3","v":"ISOLIT16"},"ISOLIT","16",null,"Schiedel ISOLIT ",{"$f":"Vokabel!$A$421","v":"ISOLIT Monoblock Feststoffkaminsystem"},"40/40 cm",{"$f":"Vokabel!$A$422","v":"mit eingebetteten Luftkammern in den Wandungen"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  Schiedel ISOLIT \" &V3&\"/\"&V3","v":"Typ  Schiedel ISOLIT 16/16"},{"$f":"X3&\" \"&V3&\"/\"&V3","v":"Schiedel ISOLIT  16/16"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",{"$f":"BV8+BV10+BV11+BV12+BV13+BV14","v":1682},null,{"$f":"BX8+BX10+BX11+BX12+BX13+BX14","v":1848},null,{"$f":"BZ8+BZ10+BZ11+BZ12+BZ13+BZ14","v":2013},null,{"$f":"CB8+CB10+CB11+CB12+CB13+CB14","v":2179},null,{"$f":"CD8+CD10+CD11+CD12+CD13+CD14","v":2348},null,{"$f":"CF8+CF10+CF11+CF12+CF13+CF14","v":2514},null,{"$f":"CH8+CH10+CH11+CH12+CH13+CH14","v":2679},null,{"$f":"CJ8+CJ10+CJ11+CJ12+CJ13+CJ14","v":2845},null,{"$f":"CL8+CL10+CL11+CL12+CL13+CL14","v":3014},null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC7+DC9+DC11+DC12+DC13+DC10","v":509},null,{"$f":"DE7+DE9+DE11+DE12+DE13+DE10","v":714},null,{"$f":"DG7+DG9+DG11+DG12+DG13+DG10","v":964},null,{"$f":"DI7+DI9+DI11+DI12+DI13+DI10","v":1169},null,{"$f":"DK7+DK9+DK11+DK12+DK13+DK10","v":1464},null,{"$f":"DM7+DM9+DM11+DM12+DM13+DM10","v":1669},null,{"$f":"DO7+DO9+DO11+DO12+DO13+DO10","v":1919}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U4&V4","v":"ISOLIT20"},"ISOLIT","20",null,"Schiedel ISOLIT ",{"$f":"Vokabel!$A$421","v":"ISOLIT Monoblock Feststoffkaminsystem"},"44/44 cm",{"$f":"Vokabel!$A$422","v":"mit eingebetteten Luftkammern in den Wandungen"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  Schiedel ISOLIT \" &V4&\"/\"&V4","v":"Typ  Schiedel ISOLIT 20/20"},{"$f":"X4&\" \"&V4&\"/\"&V4","v":"Schiedel ISOLIT  20/20"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m",{"$f":"ROUND(BV5/1000,2)","v":1.33},null,{"$f":"ROUND(BX5/1000,2)","v":1.5},null,{"$f":"ROUND(BZ5/1000,2)","v":1.66},null,{"$f":"ROUND(CB5/1000,2)","v":1.83},null,{"$f":"ROUND(CD5/1000,2)","v":2},null,{"$f":"ROUND(CF5/1000,2)","v":2.16},null,{"$f":"ROUND(CH5/1000,2)","v":2.33},null,{"$f":"ROUND(CJ5/1000,2)","v":2.4900000000000002},null,{"$f":"ROUND(CL5/1000,2)","v":2.66},null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U5&V5","v":"ISOLIT25"},"ISOLIT","25",null,"Schiedel ISOLIT ",{"$f":"Vokabel!$A$421","v":"ISOLIT Monoblock Feststoffkaminsystem"},"49/49 cm",{"$f":"Vokabel!$A$422","v":"mit eingebetteten Luftkammern in den Wandungen"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  Schiedel ISOLIT \" &V5&\"/\"&V5","v":"Typ  Schiedel ISOLIT 25/25"},{"$f":"X5&\" \"&V5&\"/\"&V5","v":"Schiedel ISOLIT  25/25"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe ",null,null,"mm",{"$f":"IF($F$390=\"90°\",BV11+BV10+BV9+BV12+BV13+BV14,BV14+BV13+BV12+BV11+BV10+BU9)","v":1329.5},null,{"$f":"IF($F$390=\"90°\",BX11+BX10+BX9+BX12+BX13+BX14,BX14+BX13+BX12+BX11+BX10+BW9)","v":1495.5},null,{"$f":"IF($F$390=\"90°\",BZ11+BZ10+BZ9+BZ12+BZ13+BZ14,BZ14+BZ13+BZ12+BZ11+BZ10+BY9)","v":1660.5},null,{"$f":"IF($F$390=\"90°\",CB11+CB10+CB9+CB12+CB13+CB14,CB14+CB13+CB12+CB11+CB10+CA9)","v":1826.5},null,{"$f":"IF($F$390=\"90°\",CD11+CD10+CD9+CD12+CD13+CD14,CD14+CD13+CD12+CD11+CD10+CC9)","v":1995.5},null,{"$f":"IF($F$390=\"90°\",CF11+CF10+CF9+CF12+CF13+CF14,CF14+CF13+CF12+CF11+CF10+CE9)","v":2161.5},null,{"$f":"IF($F$390=\"90°\",CH11+CH10+CH9+CH12+CH13+CH14,CH14+CH13+CH12+CH11+CH10+CG9)","v":2326.5},null,{"$f":"IF($F$390=\"90°\",CJ11+CJ10+CJ9+CJ12+CJ13+CJ14,CJ14+CJ13+CJ12+CJ11+CJ10+CI9)","v":2492.5},null,{"$f":"IF($F$390=\"90°\",CL11+CL10+CL9+CL12+CL13+CL14,CL14+CL13+CL12+CL11+CL10+CK9)","v":2661.5},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408508",126]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U6&V6","v":"ISOLIT30"},"ISOLIT","30",null,"Schiedel ISOLIT ",{"$f":"Vokabel!$A$421","v":"ISOLIT Monoblock Feststoffkaminsystem"},"54/54 cm",{"$f":"Vokabel!$A$422","v":"mit eingebetteten Luftkammern in den Wandungen"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  Schiedel ISOLIT \" &V6&\"/\"&V6","v":"Typ  Schiedel ISOLIT 30/30"},{"$f":"X6&\" \"&V6&\"/\"&V6","v":"Schiedel ISOLIT  30/30"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom UK.Sockel/OK WK bis mitte Anschluss)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409008",126]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404508",218,null,{"$f":"IF($C$515=\"90°\",$DA6,IF($D$515=\"85°\",$DA5,$DA7))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA6,IF($D$515=\"85°\",$DA5,$DA7))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA6,IF($D$515=\"85°\",$DA5,$DA7))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA6,IF($D$515=\"85°\",$DA5,$DA7))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA6,IF($D$515=\"85°\",$DA5,$DA7))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA6,IF($D$515=\"85°\",$DA5,$DA7))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA6,IF($D$515=\"85°\",$DA5,$DA7))","v":126}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund","eckig"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA",null,"45°",313.5,313.5,108,313.5,108,313.5,108,313.5,108,313.5,108,313.5,108,313.5,108,313.5,108,313.5,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",288,288,null,{"$f":"IF($B$490=2,$CZ9,$DA9)","v":288},null,{"$f":"IF($B$490=2,$CZ9,$DA9)","v":288},null,{"$f":"IF($B$490=2,$CZ9,$DA9)","v":288},null,{"$f":"IF($B$490=2,$CZ9,$DA9)","v":288},null,{"$f":"IF($B$490=2,$CZ9,$DA9)","v":288},null,{"$f":"IF($B$490=2,$CZ9,$DA9)","v":288},null,{"$f":"IF($B$490=2,$CZ9,$DA9)","v":288}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"INDEX(Daten!$T$11:$T$17,T10,1)","v":"Technostar12080"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel","Boden und Wandmontage gleiche Höhe",95,null,{"$f":"$DA10","v":95},null,{"$f":"$DA10","v":95},null,{"$f":"$DA10","v":95},null,{"$f":"$DA10","v":95},null,{"$f":"$DA10","v":95},null,{"$f":"$DA10","v":95},null,{"$f":"$DA10","v":95}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U11&V11","v":"Technostar12060"},"Technostar120",60,null,"TECHNOSTAR120 Ø",{"$f":"Vokabel!$A$171","v":"PP-Kunststoff-Abgasleitungssystem"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  TECHNOSTAR120 Ø \" &V11","v":"Typ  TECHNOSTAR120 Ø 60"},{"$f":"\"TECHNOSTAR 120 Ø \" &V11&\" mm\"","v":"TECHNOSTAR 120 Ø 60 mm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,null,null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010008",955,0,{"$f":"$DA$11*DB11","v":0},0,{"$f":"$DA$11*DD11","v":0},0,{"$f":"$DA$11*DF11","v":0},0,{"$f":"$DA$11*DH11","v":0},1,{"$f":"$DA$11*DJ11","v":955},1,{"$f":"$DA$11*DL11","v":955},1,{"$f":"$DA$11*DN11","v":955}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Technostar12080","Technostar120",80,null,"TECHNOSTAR120 Ø",{"$f":"Vokabel!$A$171","v":"PP-Kunststoff-Abgasleitungssystem"},null,null,null,null,null,null,null,null,null,null,null,null,"Typ  TECHNOSTAR120 Ø 80","TECHNOSTAR 120 Ø 80 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133001614,166,0,{"$f":"BT12*BU12","v":0},1,{"$f":"BT12*BW12","v":166},0,{"$f":"BT12*BY12","v":0},1,{"$f":"$BT$12*CA12","v":166},0,{"$f":"$BT$12*CC12","v":0},1,{"$f":"$BT$12*CE12","v":166},0,{"$f":"$BT$12*CG12","v":0},1,{"$f":"$BT$12*CI12","v":166},0,{"$f":"$BT$12*CK12","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005008",455,0,{"$f":"$DA$12*DB12","v":0},0,{"$f":"$DA$12*DD12","v":0},1,{"$f":"$DA$12*DF12","v":455},1,{"$f":"$DA$12*DH12","v":455},0,{"$f":"$DA$12*DJ12","v":0},0,{"$f":"$DA$12*DL12","v":0},1,{"$f":"$DA$12*DN12","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Technostar120110","Technostar120",110,null,"TECHNOSTAR120 Ø",{"$f":"Vokabel!$A$171","v":"PP-Kunststoff-Abgasleitungssystem"},null,null,null,null,null,null,null,null,null,null,null,null,"Typ  TECHNOSTAR120 Ø 110","TECHNOSTAR 120 Ø 110 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133006614,666,0,{"$f":"BT13*BU13","v":0},0,{"$f":"BT13*BW13","v":0},0,{"$f":"BT13*BY13","v":0},0,{"$f":"$BT$13*CA13","v":0},1,{"$f":"$BT$13*CC13","v":666},1,{"$f":"$BT$13*CE13","v":666},1,{"$f":"$BT$13*CG13","v":666},1,{"$f":"$BT$13*CI13","v":666},2,{"$f":"$BT$13*CK13","v":1332},null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002508",205,0,{"$f":"$DA$13*DB13","v":0},1,{"$f":"$DA$13*DD13","v":205},0,{"$f":"$DA$13*DF13","v":0},1,{"$f":"$DA$13*DH13","v":205},0,{"$f":"$DA$13*DJ13","v":0},1,{"$f":"$DA$13*DL13","v":205},0,{"$f":"$DA$13*DN13","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Technostar120125","Technostar120",125,null,"TECHNOSTAR120 Ø",{"$f":"Vokabel!$A$171","v":"PP-Kunststoff-Abgasleitungssystem"},null,null,null,null,null,null,null,null,null,null,null,null,"Typ  TECHNOSTAR120 Ø 125","TECHNOSTAR 120 Ø 125 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133003314,331,0,{"$f":"BT14*BU14","v":0},0,{"$f":"BT14*BW14","v":0},1,{"$f":"BT14*BY14","v":331},1,{"$f":"$BT$14*CA14","v":331},0,{"$f":"$BT$14*CC14","v":0},null,{"$f":"$BT$14*CE14","v":0},1,{"$f":"$BT$14*CG14","v":331},1,{"$f":"$BT$14*CI14","v":331},0,{"$f":"$BT$14*CK14","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Technostar120160","Technostar120",160,null,"TECHNOSTAR120 Ø",{"$f":"Vokabel!$A$171","v":"PP-Kunststoff-Abgasleitungssystem"},null,null,null,null,null,null,null,null,null,null,null,null,"Typ  TECHNOSTAR120 Ø 160","TECHNOSTAR 120 Ø 160 mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Technostar120200","Technostar120",200,null,"TECHNOSTAR120 Ø",{"$f":"Vokabel!$A$171","v":"PP-Kunststoff-Abgasleitungssystem"},null,null,null,null,null,null,null,null,null,null,null,null,"Typ  TECHNOSTAR120 Ø 200","TECHNOSTAR 120 Ø 200 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 100","Gesamthöhe",null,"m",{"$f":"ROUND(DC17/1000,2)","v":0.51},null,{"$f":"ROUND(DE17/1000,2)","v":0.71},null,{"$f":"ROUND(DG17/1000,2)","v":0.96},null,{"$f":"ROUND(DI17/1000,2)","v":1.17},null,{"$f":"ROUND(DK17/1000,2)","v":1.46},null,{"$f":"ROUND(DM17/1000,2)","v":1.67},null,{"$f":"ROUND(DO17/1000,2)","v":1.92}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Technostar120250","Technostar120",250,null,"TECHNOSTAR120 Ø",{"$f":"Vokabel!$A$171","v":"PP-Kunststoff-Abgasleitungssystem"},null,null,null,null,null,null,null,null,null,null,null,null,"Typ  TECHNOSTAR120 Ø 250","TECHNOSTAR 120 Ø 250 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kerastar 160","Gesamthöhe",null,"m",{"$f":"ROUND(BV18/1000,2)","v":1.68},null,{"$f":"ROUND(BX18/1000,2)","v":1.85},null,{"$f":"ROUND(BZ18/1000,2)","v":2.0099999999999998},null,{"$f":"ROUND(CB18/1000,2)","v":2.1800000000000002},null,{"$f":"ROUND(CD18/1000,2)","v":2.35},null,{"$f":"ROUND(CF18/1000,2)","v":2.5099999999999998},null,{"$f":"ROUND(CH18/1000,2)","v":2.68},null,{"$f":"ROUND(CJ18/1000,2)","v":2.85},null,{"$f":"ROUND(CL18/1000,2)","v":3.01},null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC21+DC23+DC25+DC26+DC27+DC24","v":509},null,{"$f":"DE21+DE23+DE25+DE26+DE27+DE24","v":714},null,{"$f":"DG21+DG23+DG25+DG26+DG27+DG24","v":964},null,{"$f":"DI21+DI23+DI25+DI26+DI27+DI24","v":1169},null,{"$f":"DK21+DK23+DK25+DK26+DK27+DK24","v":1464},null,{"$f":"DM21+DM23+DM25+DM26+DM27+DM24","v":1669},null,{"$f":"DO21+DO23+DO25+DO26+DO27+DO24","v":1919}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",{"$f":"BV23+BV25+BV26+BV27+BV28+BV29","v":1682},null,{"$f":"BX23+BX25+BX26+BX27+BX28+BX29","v":1848},null,{"$f":"BZ23+BZ25+BZ26+BZ27+BZ28+BZ29","v":2013},null,{"$f":"CB23+CB25+CB26+CB27+CB28+CB29","v":2179},null,{"$f":"CD23+CD25+CD26+CD27+CD28+CD29","v":2348},null,{"$f":"CF23+CF25+CF26+CF27+CF28+CF29","v":2514},null,{"$f":"CH23+CH25+CH26+CH27+CH28+CH29","v":2679},null,{"$f":"CJ23+CJ25+CJ26+CJ27+CJ28+CJ29","v":2845},null,{"$f":"CL23+CL25+CL26+CL27+CL28+CL29","v":3014},null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m",{"$f":"ROUND(BV20/1000,2)","v":1.33},null,{"$f":"ROUND(BX20/1000,2)","v":1.5},null,{"$f":"ROUND(BZ20/1000,2)","v":1.66},null,{"$f":"ROUND(CB20/1000,2)","v":1.83},null,{"$f":"ROUND(CD20/1000,2)","v":2},null,{"$f":"ROUND(CF20/1000,2)","v":2.16},null,{"$f":"ROUND(CH20/1000,2)","v":2.33},null,{"$f":"ROUND(CJ20/1000,2)","v":2.4900000000000002},null,{"$f":"ROUND(CL20/1000,2)","v":2.66},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408510",126]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe ",null,null,"mm",{"$f":"IF($F$390=\"90°\",BV26+BV25+BV24+BV27+BV28+BV29,BV29+BV28+BV27+BV26+BV25+BU24)","v":1329.5},null,{"$f":"IF($F$390=\"90°\",BX26+BX25+BX24+BX27+BX28+BX29,BX29+BX28+BX27+BX26+BX25+BW24)","v":1495.5},null,{"$f":"IF($F$390=\"90°\",BZ26+BZ25+BZ24+BZ27+BZ28+BZ29,BZ29+BZ28+BZ27+BZ26+BZ25+BY24)","v":1660.5},null,{"$f":"IF($F$390=\"90°\",CB26+CB25+CB24+CB27+CB28+CB29,CB29+CB28+CB27+CB26+CB25+CA24)","v":1826.5},null,{"$f":"IF($F$390=\"90°\",CD26+CD25+CD24+CD27+CD28+CD29,CD29+CD28+CD27+CD26+CD25+CC24)","v":1995.5},null,{"$f":"IF($F$390=\"90°\",CF26+CF25+CF24+CF27+CF28+CF29,CF29+CF28+CF27+CF26+CF25+CE24)","v":2161.5},null,{"$f":"IF($F$390=\"90°\",CH26+CH25+CH24+CH27+CH28+CH29,CH29+CH28+CH27+CH26+CH25+CG24)","v":2326.5},null,{"$f":"IF($F$390=\"90°\",CJ26+CJ25+CJ24+CJ27+CJ28+CJ29,CJ29+CJ28+CJ27+CJ26+CJ25+CI24)","v":2492.5},null,{"$f":"IF($F$390=\"90°\",CL26+CL25+CL24+CL27+CL28+CL29,CL29+CL28+CL27+CL26+CL25+CK24)","v":2661.5},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409010",126]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom UK.Sockel/OK WK bis mitte Anschluss)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404510",246,null,{"$f":"IF($C$515=\"90°\",$DA20,IF($D$515=\"85°\",$DA19,$DA21))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA20,IF($D$515=\"85°\",$DA19,$DA21))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA20,IF($D$515=\"85°\",$DA19,$DA21))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA20,IF($D$515=\"85°\",$DA19,$DA21))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA20,IF($D$515=\"85°\",$DA19,$DA21))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA20,IF($D$515=\"85°\",$DA19,$DA21))","v":126},null,{"$f":"IF($C$515=\"90°\",$DA20,IF($D$515=\"85°\",$DA19,$DA21))","v":126}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"INDEX(Daten!$T$23:$T$29,T22,1)","v":"KERASTAR180"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund","eckig"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U23&V23","v":"KERASTAR140"},"KERASTAR",140,null,"Schiedel KERASTAR Ø",{"$f":"Vokabel!$A$164","v":"Dreischaliges Edelstahl-Kaminsystem mit"},null,{"$f":"Vokabel!$A$172","v":"keramischem Profil-Innenrohr in Elementbauweise"},{"$f":"Vokabel!$A$178","v":"und keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  KRS \" &V23","v":"Typ  KRS 140"},{"$f":"X23&\" \"& V23&\" mm\"","v":"Schiedel KERASTAR Ø 140 mm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",288,288,null,{"$f":"IF($B$490=2,$CZ23,$DA23)","v":288},null,{"$f":"IF($B$490=2,$CZ23,$DA23)","v":288},null,{"$f":"IF($B$490=2,$CZ23,$DA23)","v":288},null,{"$f":"IF($B$490=2,$CZ23,$DA23)","v":288},null,{"$f":"IF($B$490=2,$CZ23,$DA23)","v":288},null,{"$f":"IF($B$490=2,$CZ23,$DA23)","v":288},null,{"$f":"IF($B$490=2,$CZ23,$DA23)","v":288}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR160","KERASTAR",160,null,"Schiedel KERASTAR Ø",{"$f":"Vokabel!$A$164","v":"Dreischaliges Edelstahl-Kaminsystem mit"},null,{"$f":"Vokabel!$A$172","v":"keramischem Profil-Innenrohr in Elementbauweise"},{"$f":"Vokabel!$A$178","v":"und keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,"Typ  KRS 160","Schiedel KERASTAR Ø 160 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA",null,"45°",116,313.5,116,313.5,116,313.5,116,313.5,116,313.5,116,313.5,116,313.5,116,313.5,116,313.5,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,95,null,{"$f":"$DA24","v":95},null,{"$f":"$DA24","v":95},null,{"$f":"$DA24","v":95},null,{"$f":"$DA24","v":95},null,{"$f":"$DA24","v":95},null,{"$f":"$DA24","v":95},null,{"$f":"$DA24","v":95}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180","KERASTAR",180,null,"Schiedel KERASTAR Ø",{"$f":"Vokabel!$A$164","v":"Dreischaliges Edelstahl-Kaminsystem mit"},null,{"$f":"Vokabel!$A$172","v":"keramischem Profil-Innenrohr in Elementbauweise"},{"$f":"Vokabel!$A$178","v":"und keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,"Typ  KRS 180","Schiedel KERASTAR Ø 180 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010010",955,0,{"$f":"$DA$11*DB25","v":0},0,{"$f":"$DA$11*DD25","v":0},0,{"$f":"$DA$11*DF25","v":0},0,{"$f":"$DA$11*DH25","v":0},1,{"$f":"$DA$11*DJ25","v":955},1,{"$f":"$DA$11*DL25","v":955},1,{"$f":"$DA$11*DN25","v":955}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR200","KERASTAR",200,null,"Schiedel KERASTAR Ø",{"$f":"Vokabel!$A$164","v":"Dreischaliges Edelstahl-Kaminsystem mit"},null,{"$f":"Vokabel!$A$172","v":"keramischem Profil-Innenrohr in Elementbauweise"},{"$f":"Vokabel!$A$178","v":"und keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,"Typ  KRS 200","Schiedel KERASTAR Ø 200 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,null,null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005010",455,0,{"$f":"$DA$12*DB26","v":0},0,{"$f":"$DA$12*DD26","v":0},1,{"$f":"$DA$12*DF26","v":455},1,{"$f":"$DA$12*DH26","v":455},0,{"$f":"$DA$12*DJ26","v":0},0,{"$f":"$DA$12*DL26","v":0},1,{"$f":"$DA$12*DN26","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR250","KERASTAR",250,null,"Schiedel KERASTAR Ø",{"$f":"Vokabel!$A$164","v":"Dreischaliges Edelstahl-Kaminsystem mit"},null,{"$f":"Vokabel!$A$172","v":"keramischem Profil-Innenrohr in Elementbauweise"},{"$f":"Vokabel!$A$178","v":"und keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,"Typ  KRS 250","Schiedel KERASTAR Ø 250 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133001616,166,0,{"$f":"BT27*BU27","v":0},1,{"$f":"BT27*BW27","v":166},0,{"$f":"BT27*BY27","v":0},1,{"$f":"BT27*CA27","v":166},0,{"$f":"BT27*CC27","v":0},1,{"$f":"$BT$27*CE27","v":166},0,{"$f":"$BT$27*CG27","v":0},1,{"$f":"$BT$27*CI27","v":166},0,{"$f":"$BT$27*CK27","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002510",205,0,{"$f":"$DA$13*DB27","v":0},1,{"$f":"$DA$13*DD27","v":205},0,{"$f":"$DA$13*DF27","v":0},1,{"$f":"$DA$13*DH27","v":205},0,{"$f":"$DA$13*DJ27","v":0},1,{"$f":"$DA$13*DL27","v":205},0,{"$f":"$DA$13*DN27","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR300","KERASTAR",300,null,"Schiedel KERASTAR Ø",{"$f":"Vokabel!$A$164","v":"Dreischaliges Edelstahl-Kaminsystem mit"},null,{"$f":"Vokabel!$A$172","v":"keramischem Profil-Innenrohr in Elementbauweise"},{"$f":"Vokabel!$A$178","v":"und keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,"Typ  KRS 300","Schiedel KERASTAR Ø 300 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133006616,666,0,{"$f":"BT28*BU28","v":0},0,{"$f":"BT28*BW28","v":0},0,{"$f":"BT28*BY28","v":0},0,{"$f":"BT28*CA28","v":0},1,{"$f":"BT28*CC28","v":666},1,{"$f":"$BT$28*CE28","v":666},1,{"$f":"$BT$28*CG28","v":666},1,{"$f":"$BT$28*CI28","v":666},2,{"$f":"$BT$28*CK28","v":1332}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR400","KERASTAR",400,null,"Schiedel KERASTAR Ø",{"$f":"Vokabel!$A$164","v":"Dreischaliges Edelstahl-Kaminsystem mit"},null,{"$f":"Vokabel!$A$172","v":"keramischem Profil-Innenrohr in Elementbauweise"},{"$f":"Vokabel!$A$178","v":"und keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,"Typ  KRS 400","Schiedel KERASTAR Ø 400 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133003316,331,0,{"$f":"BT29*BU29","v":0},0,{"$f":"BT29*BW29","v":0},1,{"$f":"BT29*BY29","v":331},1,{"$f":"BT29*CA29","v":331},0,{"$f":"BT29*CC29","v":0},null,{"$f":"$BT$29*CE29","v":0},1,{"$f":"$BT$29*CG29","v":331},1,{"$f":"$BT$29*CI29","v":331},0,{"$f":"$BT$29*CK29","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 130","Gesamthöhe",null,"m",{"$f":"ROUND(DC31/1000,2)","v":0.76},null,{"$f":"ROUND(DE31/1000,2)","v":0.96},null,{"$f":"ROUND(DG31/1000,2)","v":1.21},null,{"$f":"ROUND(DI31/1000,2)","v":1.42},null,{"$f":"ROUND(DK31/1000,2)","v":1.71},null,{"$f":"ROUND(DM31/1000,2)","v":1.92},null,{"$f":"ROUND(DO31/1000,2)","v":2.17}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC35+DC37+DC39+DC40+DC41+DC38","v":759},null,{"$f":"DE35+DE37+DE39+DE40+DE41+DE38","v":964},null,{"$f":"DG35+DG37+DG39+DG40+DG41+DG38","v":1214},null,{"$f":"DI35+DI37+DI39+DI40+DI41+DI38","v":1419},null,{"$f":"DK35+DK37+DK39+DK40+DK41+DK38","v":1714},null,{"$f":"DM35+DM37+DM39+DM40+DM41+DM38","v":1919},null,{"$f":"DO35+DO37+DO39+DO40+DO41+DO38","v":2169}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kerastar 180","Gesamthöhe",null,"m",{"$f":"ROUND(BV33/1000,2)","v":1.68},null,{"$f":"ROUND(BX33/1000,2)","v":1.85},null,{"$f":"ROUND(BZ33/1000,2)","v":2.0099999999999998},null,{"$f":"ROUND(CB33/1000,2)","v":2.1800000000000002},null,{"$f":"ROUND(CD33/1000,2)","v":2.35},null,{"$f":"ROUND(CF33/1000,2)","v":2.5099999999999998},null,{"$f":"ROUND(CH33/1000,2)","v":2.68},null,{"$f":"ROUND(CJ33/1000,2)","v":2.85},null,{"$f":"ROUND(CL33/1000,2)","v":3.01},null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",{"$f":"BV38+BV40+BV41+BV42+BV43+BV44","v":1682},null,{"$f":"BX38+BX40+BX41+BX42+BX43+BX44","v":1848},null,{"$f":"BZ38+BZ40+BZ41+BZ42+BZ43+BZ44","v":2013},null,{"$f":"CB38+CB40+CB41+CB42+CB43+CB44","v":2179},null,{"$f":"CD38+CD40+CD41+CD42+CD43+CD44","v":2348},null,{"$f":"CF38+CF40+CF41+CF42+CF43+CF44","v":2514},null,{"$f":"CH38+CH40+CH41+CH42+CH43+CH44","v":2679},null,{"$f":"CJ38+CJ40+CJ41+CJ42+CJ43+CJ44","v":2845},null,{"$f":"CL38+CL40+CL41+CL42+CL43+CL44","v":3014},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408513",240]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m",{"$f":"ROUND(BV35/1000,2)","v":1.33},null,{"$f":"ROUND(BX35/1000,2)","v":1.5},null,{"$f":"ROUND(BZ35/1000,2)","v":1.66},null,{"$f":"ROUND(CB35/1000,2)","v":1.83},null,{"$f":"ROUND(CD35/1000,2)","v":2},null,{"$f":"ROUND(CF35/1000,2)","v":2.16},null,{"$f":"ROUND(CH35/1000,2)","v":2.33},null,{"$f":"ROUND(CJ35/1000,2)","v":2.4900000000000002},null,{"$f":"ROUND(CL35/1000,2)","v":2.66},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409013",209]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"INDEX(Daten!$T$37:$T$75,T35,1)","v":"ABSOLUT18"},{"$f":"INDEX(Daten!V37:V75,$T$35,1)","v":18},{"$f":"INDEX(Daten!W37:W75,$T$35,1)","v":"Ja"},null,null,{"$f":"INDEX(Daten!Z37:Z75,$T$35,1)","v":"36/36 cm"},null,null,{"$f":"INDEX(Daten!AC37:AC75,$T$35,1)","v":"J"},{"$f":"INDEX(Daten!AD37:AD75,$T$35,1)","v":18},{"$f":"INDEX(Daten!AE37:AE75,$T$35,1)","v":0},{"$f":"INDEX(Daten!AF37:AF75,$T$35,1)","v":" "},{"$f":"INDEX(Daten!AG37:AG75,$T$35,1)","v":0},{"$f":"INDEX(Daten!AH37:AH75,$T$35,1)","v":0},{"$f":"INDEX(Daten!AI37:AI75,$T$35,1)","v":0},{"$f":"INDEX(Daten!AJ37:AJ75,$T$35,1)","v":-0.58250000000000002},null,null,null,{"$f":"INDEX(Daten!AN37:AN75,$T$35,1)","v":0},{"$f":"INDEX(Daten!AO37:AO75,$T$35,1)","v":18},{"$f":"INDEX(Daten!AP37:AP75,$T$35,1)","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe ",null,null,"mm",{"$f":"IF($F$390=\"90°\",BV41+BV40+BV39+BV42+BV43+BV44,BV44+BV43+BV42+BV41+BV40+BU39)","v":1329.5},null,{"$f":"IF($F$390=\"90°\",BX41+BX40+BX39+BX42+BX43+BX44,BX44+BX43+BX42+BX41+BX40+BW39)","v":1495.5},null,{"$f":"IF($F$390=\"90°\",BZ41+BZ40+BZ39+BZ42+BZ43+BZ44,BZ44+BZ43+BZ42+BZ41+BZ40+BY39)","v":1660.5},null,{"$f":"IF($F$390=\"90°\",CB41+CB40+CB39+CB42+CB43+CB44,CB44+CB43+CB42+CB41+CB40+CA39)","v":1826.5},null,{"$f":"IF($F$390=\"90°\",CD41+CD40+CD39+CD42+CD43+CD44,CD44+CD43+CD42+CD41+CD40+CC39)","v":1995.5},null,{"$f":"IF($F$390=\"90°\",CF41+CF40+CF39+CF42+CF43+CF44,CF44+CF43+CF42+CF41+CF40+CE39)","v":2161.5},null,{"$f":"IF($F$390=\"90°\",CH41+CH40+CH39+CH42+CH43+CH44,CH44+CH43+CH42+CH41+CH40+CG39)","v":2326.5},null,{"$f":"IF($F$390=\"90°\",CJ41+CJ40+CJ39+CJ42+CJ43+CJ44,CJ44+CJ43+CJ42+CJ41+CJ40+CI39)","v":2492.5},null,{"$f":"IF($F$390=\"90°\",CL41+CL40+CL39+CL42+CL43+CL44,CL44+CL43+CL42+CL41+CL40+CK39)","v":2661.5},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404513",328,null,{"$f":"IF($C$515=\"90°\",$DA34,IF($D$515=\"85°\",$DA33,$DA35))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA34,IF($D$515=\"85°\",$DA33,$DA35))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA34,IF($D$515=\"85°\",$DA33,$DA35))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA34,IF($D$515=\"85°\",$DA33,$DA35))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA34,IF($D$515=\"85°\",$DA33,$DA35))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA34,IF($D$515=\"85°\",$DA33,$DA35))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA34,IF($D$515=\"85°\",$DA33,$DA35))","v":209}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Verkn.","System","Ø","Thermo","Bezeichnung","System: Text1","Außenmaß","System: Text2","System: Text3","Fertigfuß","Ø 1.Zug","Ø 2.Zug","Lüftung","RA45°","RA g.Z",null,"FM Kartuschen","Summe FM","Typ","Sortiment und Typ","Doppelfutterrohr kl. Zug","Doppelfutterrohr gr. Zug","Abdeckplatte nur Stahl",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom UK.Sockel/OK WK bis mitte Anschluss)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund","eckig"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U37&V37","v":"ABSOLUT14"},"ABSOLUT",14,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/36 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",14,null," ",null,null,null,{"$f":"IF($B$183=\"Deckenanschlusskonus\",$B$61/4,($B$61-11.33)/4)","v":-0.58250000000000002},{"$f":"ROUNDUP(IF(AJ37<0,0,AJ37),0)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V37","v":"Typ  -  ABSOLUT  Ø  14"},{"$f":"X37&\" \"& V37","v":"Schiedel ABSOLUT, ABS 14"},null,14,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",288,455,null,{"$f":"IF($B$490=2,$CZ37,$DA37)","v":455},null,{"$f":"IF($B$490=2,$CZ37,$DA37)","v":455},null,{"$f":"IF($B$490=2,$CZ37,$DA37)","v":455},null,{"$f":"IF($B$490=2,$CZ37,$DA37)","v":455},null,{"$f":"IF($B$490=2,$CZ37,$DA37)","v":455},null,{"$f":"IF($B$490=2,$CZ37,$DA37)","v":455},null,{"$f":"IF($B$490=2,$CZ37,$DA37)","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT16","ABSOLUT",16,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/36 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",16,null," ",null,null,null,{"$f":"IF($B$183=\"Deckenanschlusskonus\",$B$61/4,($B$61-11.33)/4)","v":-0.58250000000000002},0,"Typ  -  ABSOLUT  Ø  16","Schiedel ABSOLUT, ABS 16",null,16,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,{"$f":"IF($A$56=3,1045,95)","v":95},null,{"$f":"$DA38","v":95},null,{"$f":"$DA38","v":95},null,{"$f":"$DA38","v":95},null,{"$f":"$DA38","v":95},null,{"$f":"$DA38","v":95},null,{"$f":"$DA38","v":95},null,{"$f":"$DA38","v":95}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT18","ABSOLUT",18,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/36 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",18,null," ",null,null,null,{"$f":"IF($B$183=\"Deckenanschlusskonus\",$B$61/4,($B$61-11.33)/4)","v":-0.58250000000000002},0,"Typ  -  ABSOLUT  Ø  18","Schiedel ABSOLUT, ABS 18",null,18,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA",null,"45°",124,313.5,124,313.5,124,313.5,124,313.5,124,313.5,124,313.5,124,313.5,124,313.5,124,313.5,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010013",955,0,{"$f":"$DA$11*DB39","v":0},0,{"$f":"$DA$11*DD39","v":0},0,{"$f":"$DA$11*DF39","v":0},0,{"$f":"$DA$11*DH39","v":0},1,{"$f":"$DA$11*DJ39","v":955},1,{"$f":"$DA$11*DL39","v":955},1,{"$f":"$DA$11*DN39","v":955}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT20","ABSOLUT",20,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"38/38 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",20,null," ",null,null,null,{"$f":"IF($B$183=\"Deckenanschlusskonus\",$B$61/4,($B$61-11.33)/4)","v":-0.58250000000000002},0,"Typ  -  ABSOLUT  Ø  20","Schiedel ABSOLUT, ABS 20",null,20,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005013",455,0,{"$f":"$DA$12*DB40","v":0},0,{"$f":"$DA$12*DD40","v":0},1,{"$f":"$DA$12*DF40","v":455},1,{"$f":"$DA$12*DH40","v":455},0,{"$f":"$DA$12*DJ40","v":0},0,{"$f":"$DA$12*DL40","v":0},1,{"$f":"$DA$12*DN40","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT25","ABSOLUT",25,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"48/48 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",25,null," ",null,null,null,{"$f":"IF($B$183=\"Deckenanschlusskonus\",$B$61/4,($B$61-11.33)/2)","v":-1.165},0,"Typ  -  ABSOLUT  Ø  25","Schiedel ABSOLUT, ABS 25",null,25,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,null,null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002513",205,0,{"$f":"$DA$13*DB41","v":0},1,{"$f":"$DA$13*DD41","v":205},0,{"$f":"$DA$13*DF41","v":0},1,{"$f":"$DA$13*DH41","v":205},0,{"$f":"$DA$13*DJ41","v":0},1,{"$f":"$DA$13*DL41","v":205},0,{"$f":"$DA$13*DN41","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT30","ABSOLUT",30,"Nein","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"55/55 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"N",30,null," ",null,null,null,{"$f":"IF($B$183=\"Deckenanschlusskonus\",$B$61/4,($B$61-11.33)/1.66)","v":-1.4036144578313254},0,"Typ  -  ABSOLUT  Ø  30","Schiedel ABSOLUT, ABS 30",null,30,"Ja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133001618,166,0,{"$f":"BT42*BU42","v":0},1,{"$f":"BT42*BW42","v":166},0,{"$f":"BT42*BY42","v":0},1,{"$f":"BT42*CA42","v":166},0,{"$f":"BT42*CC42","v":0},1,{"$f":"$BT$42*CE42","v":166},0,{"$f":"$BT$42*CG42","v":0},1,{"$f":"$BT$42*CI42","v":166},0,{"$f":"$BT$42*CK42","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT40","ABSOLUT",40,"Nein","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"67/67 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"N",40,null," ",null,null,null,{"$f":"IF($B$183=\"Deckenanschlusskonus\",$B$61/4,($B$61-11.33)/1.33)","v":-1.7518796992481203},0,"Typ  -  ABSOLUT  Ø  40","Schiedel ABSOLUT, ABS 40",null,40,"Ja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133006618,666,0,{"$f":"BT43*BU43","v":0},0,{"$f":"BT43*BW43","v":0},0,{"$f":"BT43*BY43","v":0},0,{"$f":"BT43*CA43","v":0},1,{"$f":"BT43*CC43","v":666},1,{"$f":"$BT$43*CE43","v":666},1,{"$f":"$BT$43*CG43","v":666},1,{"$f":"$BT$43*CI43","v":666},2,{"$f":"$BT$43*CK43","v":1332}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133003318,331,0,{"$f":"BT44*BU44","v":0},0,{"$f":"BT44*BW44","v":0},1,{"$f":"BT44*BY44","v":331},1,{"$f":"BT44*CA44","v":331},0,{"$f":"BT44*CC44","v":0},0,{"$f":"$BT$44*CE44","v":0},1,{"$f":"$BT$44*CG44","v":331},1,{"$f":"$BT$44*CI44","v":331},0,{"$f":"$BT$44*CK44","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"ICS 150","Gesamthöhe",null,"m",{"$f":"ROUND(DC45/1000,2)","v":0.76},null,{"$f":"ROUND(DE45/1000,2)","v":0.96},null,{"$f":"ROUND(DG45/1000,2)","v":1.21},null,{"$f":"ROUND(DI45/1000,2)","v":1.42},null,{"$f":"ROUND(DK45/1000,2)","v":1.71},null,{"$f":"ROUND(DM45/1000,2)","v":1.92},null,{"$f":"ROUND(DO45/1000,2)","v":2.17}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U45&V45","v":"ABSOLUT14TL"},"ABSOLUT","14TL","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/50 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",14,null,"Ja",null,null,null,{"$f":"($B$61-11.33)/4","v":-0.58250000000000002},{"$f":"ROUNDUP(IF(AJ45<0,0,AJ45),0)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V45","v":"Typ  -  ABSOLUT  Ø  14TL"},{"$f":"X45&\" \"& V45","v":"Schiedel ABSOLUT, ABS 14TL"},null,14,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC49+DC51+DC53+DC54+DC55+DC52","v":759},null,{"$f":"DE49+DE51+DE53+DE54+DE55+DE52","v":964},null,{"$f":"DG49+DG51+DG53+DG54+DG55+DG52","v":1214},null,{"$f":"DI49+DI51+DI53+DI54+DI55+DI52","v":1419},null,{"$f":"DK49+DK51+DK53+DK54+DK55+DK52","v":1714},null,{"$f":"DM49+DM51+DM53+DM54+DM55+DM52","v":1919},null,{"$f":"DO49+DO51+DO53+DO54+DO55+DO52","v":2169}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT16TL","ABSOLUT","16TL","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/50 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",16,null,"Ja",null,null,null,{"$f":"($B$61-11.33)/4","v":-0.58250000000000002},0,"Typ  -  ABSOLUT  Ø  16TL","Schiedel ABSOLUT, ABS 16TL",null,16,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT18TL","ABSOLUT","18TL","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/50 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",18,null,"Ja",null,null,null,{"$f":"($B$61-11.33)/4","v":-0.58250000000000002},0,"Typ  -  ABSOLUT  Ø  18TL","Schiedel ABSOLUT, ABS 18TL",null,18,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kerastar 200","Gesamthöhe",null,"m",{"$f":"ROUND(BV48/1000,2)","v":1.68},null,{"$f":"ROUND(BX48/1000,2)","v":1.85},null,{"$f":"ROUND(BZ48/1000,2)","v":2.0099999999999998},null,{"$f":"ROUND(CB48/1000,2)","v":2.1800000000000002},null,{"$f":"ROUND(CD48/1000,2)","v":2.35},null,{"$f":"ROUND(CF48/1000,2)","v":2.5099999999999998},null,{"$f":"ROUND(CH48/1000,2)","v":2.68},null,{"$f":"ROUND(CJ48/1000,2)","v":2.85},null,{"$f":"ROUND(CL48/1000,2)","v":3.01},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408515",240]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT20TL","ABSOLUT","20TL","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"38/54 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",20,null,"Ja",null,null,null,{"$f":"($B$61-11.33)/4","v":-0.58250000000000002},0,"Typ  -  ABSOLUT  Ø  20TL","Schiedel ABSOLUT, ABS 20TL",null,20,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",{"$f":"BV53+BV55+BV56+BV57+BV58+BV59","v":1682},null,{"$f":"BX53+BX55+BX56+BX57+BX58+BX59","v":1848},null,{"$f":"BZ53+BZ55+BZ56+BZ57+BZ58+BZ59","v":2013},null,{"$f":"CB53+CB55+CB56+CB57+CB58+CB59","v":2179},null,{"$f":"CD53+CD55+CD56+CD57+CD58+CD59","v":2348},null,{"$f":"CF53+CF55+CF56+CF57+CF58+CF59","v":2514},null,{"$f":"CH53+CH55+CH56+CH57+CH58+CH59","v":2679},null,{"$f":"CJ53+CJ55+CJ56+CJ57+CJ58+CJ59","v":2845},null,{"$f":"CL53+CL55+CL56+CL57+CL58+CL59","v":3014},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409015",209]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT25TL","ABSOLUT","25TL","Nein","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"48/62 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"N",25,null,"Ja",null,null,null,{"$f":"($B$61-11.33)/2","v":-1.165},0,"Typ  -  ABSOLUT  Ø  25TL","Schiedel ABSOLUT, ABS 25TL",null,25,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m",{"$f":"ROUND(BV50/1000,2)","v":1.33},null,{"$f":"ROUND(BX50/1000,2)","v":1.5},null,{"$f":"ROUND(BZ50/1000,2)","v":1.66},null,{"$f":"ROUND(CB50/1000,2)","v":1.83},null,{"$f":"ROUND(CD50/1000,2)","v":2},null,{"$f":"ROUND(CF50/1000,2)","v":2.16},null,{"$f":"ROUND(CH50/1000,2)","v":2.33},null,{"$f":"ROUND(CJ50/1000,2)","v":2.4900000000000002},null,{"$f":"ROUND(CL50/1000,2)","v":2.66},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404515",329,null,{"$f":"IF($C$515=\"90°\",$DA48,IF($D$515=\"85°\",$DA47,$DA49))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA48,IF($D$515=\"85°\",$DA47,$DA49))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA48,IF($D$515=\"85°\",$DA47,$DA49))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA48,IF($D$515=\"85°\",$DA47,$DA49))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA48,IF($D$515=\"85°\",$DA47,$DA49))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA48,IF($D$515=\"85°\",$DA47,$DA49))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA48,IF($D$515=\"85°\",$DA47,$DA49))","v":209}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT30L","ABSOLUT","30L","Nein","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"55/71 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"N",30,null,"Ja",null,null,null,{"$f":"($B$61-11.33)/1.66","v":-1.4036144578313254},0,"Typ  -  ABSOLUT  Ø  30L","Schiedel ABSOLUT, ABS 30L",null,30,"Ja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe ",null,null,"mm",{"$f":"IF($F$390=\"90°\",BV56+BV55+BV54+BV57+BV58+BV59,BV59+BV58+BV57+BV56+BV55+BU54)","v":1329.5},null,{"$f":"IF($F$390=\"90°\",BX56+BX55+BX54+BX57+BX58+BX59,BX59+BX58+BX57+BX56+BX55+BW54)","v":1495.5},null,{"$f":"IF($F$390=\"90°\",BZ56+BZ55+BZ54+BZ57+BZ58+BZ59,BZ59+BZ58+BZ57+BZ56+BZ55+BY54)","v":1660.5},null,{"$f":"IF($F$390=\"90°\",CB56+CB55+CB54+CB57+CB58+CB59,CB59+CB58+CB57+CB56+CB55+CA54)","v":1826.5},null,{"$f":"IF($F$390=\"90°\",CD56+CD55+CD54+CD57+CD58+CD59,CD59+CD58+CD57+CD56+CD55+CC54)","v":1995.5},null,{"$f":"IF($F$390=\"90°\",CF56+CF55+CF54+CF57+CF58+CF59,CF59+CF58+CF57+CF56+CF55+CE54)","v":2161.5},null,{"$f":"IF($F$390=\"90°\",CH56+CH55+CH54+CH57+CH58+CH59,CH59+CH58+CH57+CH56+CH55+CG54)","v":2326.5},null,{"$f":"IF($F$390=\"90°\",CJ56+CJ55+CJ54+CJ57+CJ58+CJ59,CJ59+CJ58+CJ57+CJ56+CJ55+CI54)","v":2492.5},null,{"$f":"IF($F$390=\"90°\",CL56+CL55+CL54+CL57+CL58+CL59,CL59+CL58+CL57+CL56+CL55+CK54)","v":2661.5},null,null,null,null,null,null,null,null,null,null,null,null,null,"rund","eckig"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT40L","ABSOLUT","40L","Nein","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"67/86 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"N",40,null,"Ja",null,null,null,{"$f":"($B$61-11.33)/1.33","v":-1.7518796992481203},0,"Typ  -  ABSOLUT  Ø  40L","Schiedel ABSOLUT, ABS 40L",null,40,"Ja",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom UK.Sockel/OK WK bis mitte Anschluss)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",305,455,null,{"$f":"IF($B$490=2,$CZ51,$DA51)","v":455},null,{"$f":"IF($B$490=2,$CZ51,$DA51)","v":455},null,{"$f":"IF($B$490=2,$CZ51,$DA51)","v":455},null,{"$f":"IF($B$490=2,$CZ51,$DA51)","v":455},null,{"$f":"IF($B$490=2,$CZ51,$DA51)","v":455},null,{"$f":"IF($B$490=2,$CZ51,$DA51)","v":455},null,{"$f":"IF($B$490=2,$CZ51,$DA51)","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,{"$f":"IF($A$56=3,1045,95)","v":95},null,{"$f":"$DA52","v":95},null,{"$f":"$DA52","v":95},null,{"$f":"$DA52","v":95},null,{"$f":"$DA52","v":95},null,{"$f":"$DA52","v":95},null,{"$f":"$DA52","v":95},null,{"$f":"$DA52","v":95}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U53&V53","v":"ABSOLUT1614"},"ABSOLUT",1614,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/65 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",16,14," ",null,16,{"$f":"IF($B$61>11.33,1,IF($B$61>14.33,2,IF($B$61>18.33,3,0)))","v":0},{"$f":"IF($B$61>11.33,1,IF($B$61>14.33,2,IF($B$61>18.33,3,0)))","v":0},{"$f":"SUM(AI53:AJ53)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V53","v":"Typ  -  ABSOLUT  Ø  1614"},{"$f":"X53&\" \"& V53","v":"Schiedel ABSOLUT, ABS 1614"},14,16,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010015",955,0,{"$f":"$DA$11*DB53","v":0},0,{"$f":"$DA$11*DD53","v":0},0,{"$f":"$DA$11*DF53","v":0},0,{"$f":"$DA$11*DH53","v":0},1,{"$f":"$DA$11*DJ53","v":955},1,{"$f":"$DA$11*DL53","v":955},1,{"$f":"$DA$11*DN53","v":955}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT1814","ABSOLUT",1814,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/65 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",18,14," ",null,18,{"$f":"IF($B$61>11.33,1,IF($B$61>14.33,2,IF($B$61>18.33,3,0)))","v":0},0,0,"Typ  -  ABSOLUT  Ø  1814","Schiedel ABSOLUT, ABS 1814",14,18,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA",null,"45°",130,313.5,130,313.5,130,313.5,130,313.5,130,313.5,130,313.5,130,313.5,130,313.5,130,313.5,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005015",455,0,{"$f":"$DA$12*DB54","v":0},0,{"$f":"$DA$12*DD54","v":0},1,{"$f":"$DA$12*DF54","v":455},1,{"$f":"$DA$12*DH54","v":455},0,{"$f":"$DA$12*DJ54","v":0},0,{"$f":"$DA$12*DL54","v":0},1,{"$f":"$DA$12*DN54","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT1816","ABSOLUT",1816,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/65 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",18,16," ",null,18,0,0,0,"Typ  -  ABSOLUT  Ø  1816","Schiedel ABSOLUT, ABS 1816",16,18,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002515",205,0,{"$f":"$DA$13*DB55","v":0},1,{"$f":"$DA$13*DD55","v":205},0,{"$f":"$DA$13*DF55","v":0},1,{"$f":"$DA$13*DH55","v":205},0,{"$f":"$DA$13*DJ55","v":0},1,{"$f":"$DA$13*DL55","v":205},0,{"$f":"$DA$13*DN55","v":0}]
[null,null,null,null,{"$f":"IF($U$1=\"DrehFix100\",\"Doppelwandfutter Ø 130\",IF($U$1=\"DrehFix130\",\"Doppelwandfutter Ø 180\",\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT2014","ABSOLUT",2014,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"38/71 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",20,14,null,null,20,0,0,0,"Typ  -  ABSOLUT  Ø  2014","Schiedel ABSOLUT, ABS 2014",14,20,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,null,null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT2016","ABSOLUT",2016,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"38/71 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",20,16,null,null,20,0,0,0,"Typ  -  ABSOLUT  Ø  2016","Schiedel ABSOLUT, ABS 2016",16,20,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133001620,166,0,{"$f":"BT57*BU57","v":0},1,{"$f":"BT57*BW57","v":166},0,{"$f":"BT57*BY57","v":0},1,{"$f":"BT57*CA57","v":166},0,{"$f":"BT57*CC57","v":0},1,{"$f":"$BT$57*CE57","v":166},0,{"$f":"$BT$57*CG57","v":0},1,{"$f":"$BT$57*CI57","v":166},0,{"$f":"$BT$57*CK57","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT2018","ABSOLUT",2018,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"38/71 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",20,18,null,null,20,0,0,0,"Typ  -  ABSOLUT  Ø  2018","Schiedel ABSOLUT, ABS 2018",18,20,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133006620,666,0,{"$f":"BT58*BU58","v":0},0,{"$f":"BT58*BW58","v":0},0,{"$f":"BT58*BY58","v":0},0,{"$f":"BT58*CA58","v":0},1,{"$f":"BT58*CC58","v":666},1,{"$f":"$BT$58*CE58","v":666},1,{"$f":"$BT$58*CG58","v":666},1,{"$f":"$BT$58*CI58","v":666},2,{"$f":"$BT$58*CK58","v":1332},null,null,null,null,null,null,null,null,null,null,null,null,"ICS 180","Gesamthöhe",null,"m",{"$f":"ROUND(DC59/1000,2)","v":0.76},null,{"$f":"ROUND(DE59/1000,2)","v":0.96},null,{"$f":"ROUND(DG59/1000,2)","v":1.21},null,{"$f":"ROUND(DI59/1000,2)","v":1.42},null,{"$f":"ROUND(DK59/1000,2)","v":1.71},null,{"$f":"ROUND(DM59/1000,2)","v":1.92},null,{"$f":"ROUND(DO59/1000,2)","v":2.17}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133003320,331,0,{"$f":"BT59*BU59","v":0},0,{"$f":"BT59*BW59","v":0},1,{"$f":"BT59*BY59","v":331},1,{"$f":"BT59*CA59","v":331},0,{"$f":"BT59*CC59","v":0},0,{"$f":"$BT$59*CE59","v":0},1,{"$f":"$BT$59*CG59","v":331},1,{"$f":"$BT$59*CI59","v":331},0,{"$f":"$BT$59*CK59","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC63+DC65+DC67+DC68+DC69+DC66","v":759},null,{"$f":"DE63+DE65+DE67+DE68+DE69+DE66","v":964},null,{"$f":"DG63+DG65+DG67+DG68+DG69+DG66","v":1214},null,{"$f":"DI63+DI65+DI67+DI68+DI69+DI66","v":1419},null,{"$f":"DK63+DK65+DK67+DK68+DK69+DK66","v":1714},null,{"$f":"DM63+DM65+DM67+DM68+DM69+DM66","v":1919},null,{"$f":"DO63+DO65+DO67+DO68+DO69+DO66","v":2169}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U60&V60","v":"ABSOLUT16TL14"},"ABSOLUT","16TL14","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/83 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",16,14,"Ja",null,16,{"$f":"IF($B$61>11.33,1,IF($B$61>14.33,2,IF($B$61>18.33,3,0)))","v":0},0,{"$f":"SUM(AI60:AJ60)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V60","v":"Typ  -  ABSOLUT  Ø  16TL14"},{"$f":"X60&\" \"& V60","v":"Schiedel ABSOLUT, ABS 16TL14"},14,16,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[16,{"$f":"INDEX(Daten!$A$63:$A$111,A61,1)","v":9},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT18TL14","ABSOLUT","18TL14","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/83 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",18,14,"Ja",null,18,0,0,0,"Typ  -  ABSOLUT  Ø  18TL14","Schiedel ABSOLUT, ABS 18TL14",14,18,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408518",240]
["Anlagenhöhe",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT18TL16","ABSOLUT","18TL16","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/83 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",18,16,"Ja",null,18,0,0,0,"Typ  -  ABSOLUT  Ø  18TL16","Schiedel ABSOLUT, ABS 18TL16",16,18,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kerastar 250","Gesamthöhe",null,"m",{"$f":"ROUND(BV63/1000,2)","v":1.68},null,{"$f":"ROUND(BX63/1000,2)","v":1.85},null,{"$f":"ROUND(BZ63/1000,2)","v":2.0099999999999998},null,{"$f":"ROUND(CB63/1000,2)","v":2.1800000000000002},null,{"$f":"ROUND(CD63/1000,2)","v":2.35},null,{"$f":"ROUND(CF63/1000,2)","v":2.5099999999999998},null,{"$f":"ROUND(CH63/1000,2)","v":2.68},null,{"$f":"ROUND(CJ63/1000,2)","v":2.85},null,{"$f":"ROUND(CL63/1000,2)","v":3.01},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409018",209]
[4,null,null,null,{"$f":"IF(U117=\"Keranova140\",\"Steckadapter\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT20TL14","ABSOLUT","20TL14","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"38/88 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",20,14,"Ja",null,20,0,0,0,"Typ  -  ABSOLUT  Ø  20TL14","Schiedel ABSOLUT, ABS 20TL14",14,20,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",{"$f":"BV68+BV70+BV71+BV72+BV73+BV74","v":1682},null,{"$f":"BX68+BX70+BX71+BX72+BX73+BX74","v":1848},null,{"$f":"BZ68+BZ70+BZ71+BZ72+BZ73+BZ74","v":2013},null,{"$f":"CB68+CB70+CB71+CB72+CB73+CB74","v":2179},null,{"$f":"CD68+CD70+CD71+CD72+CD73+CD74","v":2348},null,{"$f":"CF68+CF70+CF71+CF72+CF73+CF74","v":2514},null,{"$f":"CH68+CH70+CH71+CH72+CH73+CH74","v":2679},null,{"$f":"CJ68+CJ70+CJ71+CJ72+CJ73+CJ74","v":2845},null,{"$f":"CL68+CL70+CL71+CL72+CL73+CL74","v":3014},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404518",358,null,{"$f":"IF($C$515=\"90°\",$DA62,IF($D$515=\"85°\",$DA61,$DA63))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA62,IF($D$515=\"85°\",$DA61,$DA63))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA62,IF($D$515=\"85°\",$DA61,$DA63))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA62,IF($D$515=\"85°\",$DA61,$DA63))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA62,IF($D$515=\"85°\",$DA61,$DA63))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA62,IF($D$515=\"85°\",$DA61,$DA63))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA62,IF($D$515=\"85°\",$DA61,$DA63))","v":209}]
[4.33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT20TL16","ABSOLUT","20TL16","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"38/88 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",20,16,"Ja",null,null,0,0,0,"Typ  -  ABSOLUT  Ø  20TL16","Schiedel ABSOLUT, ABS 20TL16",16,20,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m",{"$f":"ROUND(BV65/1000,2)","v":1.33},null,{"$f":"ROUND(BX65/1000,2)","v":1.5},null,{"$f":"ROUND(BZ65/1000,2)","v":1.66},null,{"$f":"ROUND(CB65/1000,2)","v":1.83},null,{"$f":"ROUND(CD65/1000,2)","v":2},null,{"$f":"ROUND(CF65/1000,2)","v":2.16},null,{"$f":"ROUND(CH65/1000,2)","v":2.33},null,{"$f":"ROUND(CJ65/1000,2)","v":2.4900000000000002},null,{"$f":"ROUND(CL65/1000,2)","v":2.66},null,null,null,null,null,null,null,null,null,null,null,null,null,"rund","eckig"]
[4.66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUT20TL18","ABSOLUT","20TL18","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"38/88 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",20,18,"Ja",null,null,0,0,0,"Typ  -  ABSOLUT  Ø  20TL18","Schiedel ABSOLUT, ABS 20TL18",18,20,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe ",null,null,"mm",{"$f":"IF($F$390=\"90°\",BV71+BV70+BV69+BV72+BV73+BV74,BV74+BV73+BV72+BV71+BV70+BU69)","v":1329.5},null,{"$f":"IF($F$390=\"90°\",BX71+BX70+BX69+BX72+BX73+BX74,BX74+BX73+BX72+BX71+BX70+BW69)","v":1495.5},null,{"$f":"IF($F$390=\"90°\",BZ71+BZ70+BZ69+BZ72+BZ73+BZ74,BZ74+BZ73+BZ72+BZ71+BZ70+BY69)","v":1660.5},null,{"$f":"IF($F$390=\"90°\",CB71+CB70+CB69+CB72+CB73+CB74,CB74+CB73+CB72+CB71+CB70+CA69)","v":1826.5},null,{"$f":"IF($F$390=\"90°\",CD71+CD70+CD69+CD72+CD73+CD74,CD74+CD73+CD72+CD71+CD70+CC69)","v":1995.5},null,{"$f":"IF($F$390=\"90°\",CF71+CF70+CF69+CF72+CF73+CF74,CF74+CF73+CF72+CF71+CF70+CE69)","v":2161.5},null,{"$f":"IF($F$390=\"90°\",CH71+CH70+CH69+CH72+CH73+CH74,CH74+CH73+CH72+CH71+CH70+CG69)","v":2326.5},null,{"$f":"IF($F$390=\"90°\",CJ71+CJ70+CJ69+CJ72+CJ73+CJ74,CJ74+CJ73+CJ72+CJ71+CJ70+CI69)","v":2492.5},null,{"$f":"IF($F$390=\"90°\",CL71+CL70+CL69+CL72+CL73+CL74,CL74+CL73+CL72+CL71+CL70+CK69)","v":2661.5},null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",305,455,null,{"$f":"IF($B$490=2,$CZ65,$DA65)","v":455},null,{"$f":"IF($B$490=2,$CZ65,$DA65)","v":455},null,{"$f":"IF($B$490=2,$CZ65,$DA65)","v":455},null,{"$f":"IF($B$490=2,$CZ65,$DA65)","v":455},null,{"$f":"IF($B$490=2,$CZ65,$DA65)","v":455},null,{"$f":"IF($B$490=2,$CZ65,$DA65)","v":455},null,{"$f":"IF($B$490=2,$CZ65,$DA65)","v":455}]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom UK.Sockel/OK WK bis mitte Anschluss)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,{"$f":"IF($A$56=3,1045,95)","v":95},null,{"$f":"$DA66","v":95},null,{"$f":"$DA66","v":95},null,{"$f":"$DA66","v":95},null,{"$f":"$DA66","v":95},null,{"$f":"$DA66","v":95},null,{"$f":"$DA66","v":95},null,{"$f":"$DA66","v":95}]
[5.33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U67&V67","v":"ABSOLUT1414"},"ABSOLUT",1414,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/65 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",14,14," ",null,null,{"$f":"IF($B$61>11.33,1,IF($B$61>14.33,2,IF($B$61>18.33,3,0)))","v":0},0,{"$f":"SUM(AI67:AJ67)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V67","v":"Typ  -  ABSOLUT  Ø  1414"},{"$f":"X67&\" \"& V67","v":"Schiedel ABSOLUT, ABS 1414"},14,14,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010018",955,0,{"$f":"$DA$11*DB67","v":0},0,{"$f":"$DA$11*DD67","v":0},0,{"$f":"$DA$11*DF67","v":0},0,{"$f":"$DA$11*DH67","v":0},1,{"$f":"$DA$11*DJ67","v":955},1,{"$f":"$DA$11*DL67","v":955},1,{"$f":"$DA$11*DN67","v":955}]
[5.66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U68&V68","v":"ABSOLUT1616"},"ABSOLUT",1616,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/65 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",16,16," ",null,null,0,0,{"$f":"SUM(AI68:AJ68)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V68","v":"Typ  -  ABSOLUT  Ø  1616"},{"$f":"X68&\" \"& V68","v":"Schiedel ABSOLUT, ABS 1616"},16,16,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005018",455,0,{"$f":"$DA$12*DB68","v":0},0,{"$f":"$DA$12*DD68","v":0},1,{"$f":"$DA$12*DF68","v":455},1,{"$f":"$DA$12*DH68","v":455},0,{"$f":"$DA$12*DJ68","v":0},0,{"$f":"$DA$12*DL68","v":0},1,{"$f":"$DA$12*DN68","v":455}]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U69&V69","v":"ABSOLUT1818"},"ABSOLUT",1818,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/65 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",18,18," ",null,null,0,0,{"$f":"SUM(AI69:AJ69)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V69","v":"Typ  -  ABSOLUT  Ø  1818"},{"$f":"X69&\" \"& V69","v":"Schiedel ABSOLUT, ABS 1818"},18,18,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA",null,"45°",147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002518",205,0,{"$f":"$DA$13*DB69","v":0},1,{"$f":"$DA$13*DD69","v":205},0,{"$f":"$DA$13*DF69","v":0},1,{"$f":"$DA$13*DH69","v":205},0,{"$f":"$DA$13*DJ69","v":0},1,{"$f":"$DA$13*DL69","v":205},0,{"$f":"$DA$13*DN69","v":0}]
[6.33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U70&V70","v":"ABSOLUT2020"},"ABSOLUT",2020,"Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"38/71 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",20,20," ",null,null,0,0,{"$f":"SUM(AI70:AJ70)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V70","v":"Typ  -  ABSOLUT  Ø  2020"},{"$f":"X70&\" \"& V70","v":"Schiedel ABSOLUT, ABS 2020"},20,20,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666]
[6.66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,null,null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"}]
[7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U72&V72","v":"ABSOLUT14TL14"},"ABSOLUT","14TL14","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/83 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",14,14,"Ja",null,null,{"$f":"IF($B$61>11.33,1,IF($B$61>14.33,2,IF($B$61>18.33,3,0)))","v":0},0,{"$f":"SUM(AI72:AJ72)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V72","v":"Typ  -  ABSOLUT  Ø  14TL14"},{"$f":"X72&\" \"& V72","v":"Schiedel ABSOLUT, ABS 14TL14"},14,14,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133001625,166,0,{"$f":"BT72*BU72","v":0},1,{"$f":"BT72*BW72","v":166},0,{"$f":"BT72*BY72","v":0},1,{"$f":"BT72*CA72","v":166},0,{"$f":"BT72*CC72","v":0},1,{"$f":"$BT$72*CE72","v":166},0,{"$f":"$BT$72*CG72","v":0},1,{"$f":"$BT$72*CI72","v":166},0,{"$f":"$BT$72*CK72","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"ICS 200","Gesamthöhe",null,"m",{"$f":"ROUND(DC73/1000,2)","v":0.76},null,{"$f":"ROUND(DE73/1000,2)","v":0.96},null,{"$f":"ROUND(DG73/1000,2)","v":1.21},null,{"$f":"ROUND(DI73/1000,2)","v":1.42},null,{"$f":"ROUND(DK73/1000,2)","v":1.71},null,{"$f":"ROUND(DM73/1000,2)","v":1.92},null,{"$f":"ROUND(DO73/1000,2)","v":2.17}]
[7.33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U73&V73","v":"ABSOLUT16TL16"},"ABSOLUT","16TL16","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/83 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",16,16,"Ja",null,null,0,0,{"$f":"SUM(AI73:AJ73)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V73","v":"Typ  -  ABSOLUT  Ø  16TL16"},{"$f":"X73&\" \"& V73","v":"Schiedel ABSOLUT, ABS 16TL16"},16,16,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133006625,666,0,{"$f":"BT73*BU73","v":0},0,{"$f":"BT73*BW73","v":0},0,{"$f":"BT73*BY73","v":0},0,{"$f":"BT73*CA73","v":0},1,{"$f":"BT73*CC73","v":666},1,{"$f":"$BT$73*CE73","v":666},1,{"$f":"$BT$73*CG73","v":666},1,{"$f":"$BT$73*CI73","v":666},2,{"$f":"$BT$73*CK73","v":1332},null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC77+DC79+DC81+DC82+DC83+DC80","v":759},null,{"$f":"DE77+DE79+DE81+DE82+DE83+DE80","v":964},null,{"$f":"DG77+DG79+DG81+DG82+DG83+DG80","v":1214},null,{"$f":"DI77+DI79+DI81+DI82+DI83+DI80","v":1419},null,{"$f":"DK77+DK79+DK81+DK82+DK83+DK80","v":1714},null,{"$f":"DM77+DM79+DM81+DM82+DM83+DM80","v":1919},null,{"$f":"DO77+DO79+DO81+DO82+DO83+DO80","v":2169}]
[7.66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U74&V74","v":"ABSOLUT18TL18"},"ABSOLUT","18TL18","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"36/83 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",18,18,"Ja",null,null,0,0,{"$f":"SUM(AI74:AJ74)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V74","v":"Typ  -  ABSOLUT  Ø  18TL18"},{"$f":"X74&\" \"& V74","v":"Schiedel ABSOLUT, ABS 18TL18"},18,18,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133003325,331,0,{"$f":"BT74*BU74","v":0},0,{"$f":"BT74*BW74","v":0},1,{"$f":"BT74*BY74","v":331},1,{"$f":"BT74*CA74","v":331},0,{"$f":"BT74*CC74","v":0},0,{"$f":"$BT$74*CE74","v":0},1,{"$f":"$BT$74*CG74","v":331},1,{"$f":"$BT$74*CI74","v":331},0,{"$f":"$BT$74*CK74","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U75&V75","v":"ABSOLUT20TL20"},"ABSOLUT","20TL20","Ja","Schiedel ABSOLUT, ABS",{"$f":"Vokabel!$A$166","v":"Mehrschaliges feuchteunempfindliches Kaminsystem"},"38/88 cm",{"$f":"Vokabel!$A$174","v":"mit integrierter Wärmedämmung"},{"$f":"Vokabel!$A$179","v":"und keramischem Profil-Innenrohr"},"J",20,20,"Ja",null,null,0,0,{"$f":"SUM(AI75:AJ75)","v":0},{"$f":"\"Typ  -  ABSOLUT  Ø  \" &V75","v":"Typ  -  ABSOLUT  Ø  20TL20"},{"$f":"X75&\" \"& V75","v":"Schiedel ABSOLUT, ABS 20TL20"},20,20,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408520",240]
[8.33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409020",209]
[8.66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kerastar 300","Gesamthöhe",null,"m",{"$f":"ROUND(BV78/1000,2)","v":1.68},null,{"$f":"ROUND(BX78/1000,2)","v":1.85},null,{"$f":"ROUND(BZ78/1000,2)","v":2.0099999999999998},null,{"$f":"ROUND(CB78/1000,2)","v":2.1800000000000002},null,{"$f":"ROUND(CD78/1000,2)","v":2.35},null,{"$f":"ROUND(CF78/1000,2)","v":2.5099999999999998},null,{"$f":"ROUND(CH78/1000,2)","v":2.68},null,{"$f":"ROUND(CJ78/1000,2)","v":2.85},null,{"$f":"ROUND(CL78/1000,2)","v":3.01},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404520",378,null,{"$f":"IF($C$515=\"90°\",$DA76,IF($D$515=\"85°\",$DA75,$DA77))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA76,IF($D$515=\"85°\",$DA75,$DA77))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA76,IF($D$515=\"85°\",$DA75,$DA77))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA76,IF($D$515=\"85°\",$DA75,$DA77))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA76,IF($D$515=\"85°\",$DA75,$DA77))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA76,IF($D$515=\"85°\",$DA75,$DA77))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA76,IF($D$515=\"85°\",$DA75,$DA77))","v":209}]
[9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",{"$f":"BV83+BV85+BV86+BV87+BV88+BV89","v":1682},null,{"$f":"BX83+BX85+BX86+BX87+BX88+BX89","v":1848},null,{"$f":"BZ83+BZ85+BZ86+BZ87+BZ88+BZ89","v":2013},null,{"$f":"CB83+CB85+CB86+CB87+CB88+CB89","v":2179},null,{"$f":"CD83+CD85+CD86+CD87+CD88+CD89","v":2348},null,{"$f":"CF83+CF85+CF86+CF87+CF88+CF89","v":2514},null,{"$f":"CH83+CH85+CH86+CH87+CH88+CH89","v":2679},null,{"$f":"CJ83+CJ85+CJ86+CJ87+CJ88+CJ89","v":2845},null,{"$f":"CL83+CL85+CL86+CL87+CL88+CL89","v":3014},null,null,null,null,null,null,null,null,null,null,null,null,null,"rund","eckig"]
[9.33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"INDEX(Daten!$T$81:$T$89,T79,1)","v":"CHEMINEE20"},{"$f":"INDEX(Daten!V81:V89,$T$79,1)","v":20},null,{"$f":"INDEX(Daten!X81:X89,$T$79,1)","v":"Schiedel CHEMINEE"},{"$f":"INDEX(Daten!Y81:Y89,$T$79,1)","v":"Dreischaliges Kaminsystem"},{"$f":"INDEX(Daten!Z81:Z89,$T$79,1)","v":"Ja"},{"$f":"INDEX(Daten!AA81:AA89,$T$79,1)","v":"mit Hinterlüftung und Schamotte-Innenrohr"},{"$f":"INDEX(Daten!AB81:AB89,$T$79,1)","v":0},{"$f":"INDEX(Daten!AC81:AC89,$T$79,1)","v":"N"},{"$f":"INDEX(Daten!AD81:AD89,$T$79,1)","v":0},{"$f":"INDEX(Daten!AE81:AE89,$T$79,1)","v":20},{"$f":"INDEX(Daten!AF81:AF89,$T$79,1)","v":0},{"$f":"INDEX(Daten!AG81:AG89,$T$79,1)","v":" "},{"$f":"INDEX(Daten!AH81:AH89,$T$79,1)","v":0},{"$f":"INDEX(Daten!AI81:AI89,$T$79,1)","v":0},{"$f":"INDEX(Daten!AJ81:AJ89,$T$79,1)","v":"Ja"},{"$f":"INDEX(Daten!AK81:AK89,$T$79,1)","v":"36/36 cm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m",{"$f":"ROUND(BV80/1000,2)","v":1.33},null,{"$f":"ROUND(BX80/1000,2)","v":1.5},null,{"$f":"ROUND(BZ80/1000,2)","v":1.66},null,{"$f":"ROUND(CB80/1000,2)","v":1.83},null,{"$f":"ROUND(CD80/1000,2)","v":2},null,{"$f":"ROUND(CF80/1000,2)","v":2.16},null,{"$f":"ROUND(CH80/1000,2)","v":2.33},null,{"$f":"ROUND(CJ80/1000,2)","v":2.4900000000000002},null,{"$f":"ROUND(CL80/1000,2)","v":2.66},null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",405,455,null,{"$f":"IF($B$490=2,$CZ79,$DA79)","v":455},null,{"$f":"IF($B$490=2,$CZ79,$DA79)","v":455},null,{"$f":"IF($B$490=2,$CZ79,$DA79)","v":455},null,{"$f":"IF($B$490=2,$CZ79,$DA79)","v":455},null,{"$f":"IF($B$490=2,$CZ79,$DA79)","v":455},null,{"$f":"IF($B$490=2,$CZ79,$DA79)","v":455},null,{"$f":"IF($B$490=2,$CZ79,$DA79)","v":455}]
[9.66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Verkn.","System","Ø",null,"Bezeichnung","System: Text1","Deckenanschl-k.","System: Text2","System: Text3","Fertigfuß 1","Fertigfuß 2","Ø 1.Zug","Ø 2.Zug","Lüftung","RA45°","RA g.Z","FBK","Außenmaß",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe ",null,null,"mm",{"$f":"IF($F$390=\"90°\",BV86+BV85+BV84+BV87+BV88+BV89,BV89+BV88+BV87+BV86+BV85+BU84)","v":1329.5},null,{"$f":"IF($F$390=\"90°\",BX86+BX85+BX84+BX87+BX88+BX89,BX89+BX88+BX87+BX86+BX85+BW84)","v":1495.5},null,{"$f":"IF($F$390=\"90°\",BZ86+BZ85+BZ84+BZ87+BZ88+BZ89,BZ89+BZ88+BZ87+BZ86+BZ85+BY84)","v":1660.5},null,{"$f":"IF($F$390=\"90°\",CB86+CB85+CB84+CB87+CB88+CB89,CB89+CB88+CB87+CB86+CB85+CA84)","v":1826.5},null,{"$f":"IF($F$390=\"90°\",CD86+CD85+CD84+CD87+CD88+CD89,CD89+CD88+CD87+CD86+CD85+CC84)","v":1995.5},null,{"$f":"IF($F$390=\"90°\",CF86+CF85+CF84+CF87+CF88+CF89,CF89+CF88+CF87+CF86+CF85+CE84)","v":2161.5},null,{"$f":"IF($F$390=\"90°\",CH86+CH85+CH84+CH87+CH88+CH89,CH89+CH88+CH87+CH86+CH85+CG84)","v":2326.5},null,{"$f":"IF($F$390=\"90°\",CJ86+CJ85+CJ84+CJ87+CJ88+CJ89,CJ89+CJ88+CJ87+CJ86+CJ85+CI84)","v":2492.5},null,{"$f":"IF($F$390=\"90°\",CL86+CL85+CL84+CL87+CL88+CL89,CL89+CL88+CL87+CL86+CL85+CK84)","v":2661.5},null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,{"$f":"IF($A$56=3,1045,95)","v":95},null,{"$f":"$DA80","v":95},null,{"$f":"$DA80","v":95},null,{"$f":"$DA80","v":95},null,{"$f":"$DA80","v":95},null,{"$f":"$DA80","v":95},null,{"$f":"$DA80","v":95},null,{"$f":"$DA80","v":95}]
[10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U81&V81","v":"CHEMINEE16"},"CHEMINEE",16,null,"Schiedel CHEMINEE",{"$f":"Vokabel!$A$167","v":"Dreischaliges Kaminsystem"},"Ja",{"$f":"Vokabel!$A$175","v":"mit Hinterlüftung und Schamotte-Innenrohr"},null,"N",null,16,null," ",null,null,"Ja","32/32 cm",{"$f":"\"Typ  CHEMINEE \" &V81","v":"Typ  CHEMINEE 16"},{"$f":"X81&\" \"& V81","v":"Schiedel CHEMINEE 16"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom UK.Sockel/OK WK bis mitte Anschluss)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010020",955,0,{"$f":"$DA$11*DB81","v":0},0,{"$f":"$DA$11*DD81","v":0},0,{"$f":"$DA$11*DF81","v":0},0,{"$f":"$DA$11*DH81","v":0},1,{"$f":"$DA$11*DJ81","v":955},1,{"$f":"$DA$11*DL81","v":955},1,{"$f":"$DA$11*DN81","v":955}]
[10.33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U82&V82","v":"CHEMINEE18"},"CHEMINEE",18,null,"Schiedel CHEMINEE",{"$f":"Vokabel!$A$167","v":"Dreischaliges Kaminsystem"},"Ja",{"$f":"Vokabel!$A$175","v":"mit Hinterlüftung und Schamotte-Innenrohr"},null,"N",null,18,null," ",null,null,"Ja","36/36 cm",{"$f":"\"Typ  CHEMINEE \" &V82","v":"Typ  CHEMINEE 18"},{"$f":"X82&\" \"& V82","v":"Schiedel CHEMINEE 18"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005020",455,0,{"$f":"$DA$12*DB82","v":0},0,{"$f":"$DA$12*DD82","v":0},1,{"$f":"$DA$12*DF82","v":455},1,{"$f":"$DA$12*DH82","v":455},0,{"$f":"$DA$12*DJ82","v":0},0,{"$f":"$DA$12*DL82","v":0},1,{"$f":"$DA$12*DN82","v":455}]
[10.66,null,null,2,{"$f":"INDEX(Daten!D85:D86,D83,1)","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U83&V83","v":"CHEMINEE20"},"CHEMINEE",20,null,"Schiedel CHEMINEE",{"$f":"Vokabel!$A$167","v":"Dreischaliges Kaminsystem"},"Ja",{"$f":"Vokabel!$A$175","v":"mit Hinterlüftung und Schamotte-Innenrohr"},null,"N",null,20,null," ",null,null,"Ja","36/36 cm",{"$f":"\"Typ  CHEMINEE \" &V83","v":"Typ  CHEMINEE 20"},{"$f":"X83&\" \"& V83","v":"Schiedel CHEMINEE 20"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002520",205,0,{"$f":"$DA$13*DB83","v":0},1,{"$f":"$DA$13*DD83","v":205},0,{"$f":"$DA$13*DF83","v":0},1,{"$f":"$DA$13*DH83","v":205},0,{"$f":"$DA$13*DJ83","v":0},1,{"$f":"$DA$13*DL83","v":205},0,{"$f":"$DA$13*DN83","v":0}]
[11,null,null,"Fracht nach Tonne",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U84&V84","v":"CHEMINEE25"},"CHEMINEE",25,null,"Schiedel CHEMINEE",{"$f":"Vokabel!$A$167","v":"Dreischaliges Kaminsystem"},"Ja",{"$f":"Vokabel!$A$175","v":"mit Hinterlüftung und Schamotte-Innenrohr"},null,"N",null,25,null," ",null,null,"Nein","48/48 cm",{"$f":"\"Typ  CHEMINEE \" &V84","v":"Typ  CHEMINEE 25"},{"$f":"X84&\" \"& V84","v":"Schiedel CHEMINEE 25"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA",null,"45°",147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5]
[11.33,null,null,{"$f":"$E$85","v":"Ja"},{"$f":"Vokabel!$A$4","v":"Ja"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U85&V85","v":"CHEMINEE30"},"CHEMINEE",30,null,"Schiedel CHEMINEE",{"$f":"Vokabel!$A$167","v":"Dreischaliges Kaminsystem"},"Ja",{"$f":"Vokabel!$A$175","v":"mit Hinterlüftung und Schamotte-Innenrohr"},null,"N",null,30,null," ",null,null,"Nein","55/55 cm",{"$f":"\"Typ  CHEMINEE \" &V85","v":"Typ  CHEMINEE 30"},{"$f":"X85&\" \"& V85","v":"Schiedel CHEMINEE 30"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666]
[11.66,null,null,{"$f":"$E$86","v":"Nein"},{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,null,null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,null,null,null,null,null,null,null,null,null,null,null,"ICS 250","Gesamthöhe",null,"m",{"$f":"ROUND(DC87/1000,2)","v":0.76},null,{"$f":"ROUND(DE87/1000,2)","v":0.96},null,{"$f":"ROUND(DG87/1000,2)","v":1.21},null,{"$f":"ROUND(DI87/1000,2)","v":1.42},null,{"$f":"ROUND(DK87/1000,2)","v":1.71},null,{"$f":"ROUND(DM87/1000,2)","v":1.92},null,{"$f":"ROUND(DO87/1000,2)","v":2.17}]
[12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U87&V87","v":"CHEMINEE2020"},"CHEMINEE",2020,null,"Schiedel CHEMINEE",{"$f":"Vokabel!$A$167","v":"Dreischaliges Kaminsystem"},"Nein",{"$f":"Vokabel!$A$175","v":"mit Hinterlüftung und Schamotte-Innenrohr"},null,"N",null,20,20," ",null,null,"Nein","36/67 cm",{"$f":"\"Typ  CHEMINEE \" &V87","v":"Typ  CHEMINEE 2020"},{"$f":"X87&\" \"& V87","v":"Schiedel CHEMINEE 2020"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133001625,166,0,{"$f":"BT87*BU87","v":0},1,{"$f":"BT87*BW87","v":166},0,{"$f":"BT87*BY87","v":0},1,{"$f":"BT87*CA87","v":166},0,{"$f":"BT87*CC87","v":0},1,{"$f":"$BT$72*CE87","v":166},0,{"$f":"$BT$72*CG87","v":0},1,{"$f":"$BT$72*CI87","v":166},0,{"$f":"$BT$72*CK87","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC91+DC93+DC95+DC96+DC97+DC94","v":759},null,{"$f":"DE91+DE93+DE95+DE96+DE97+DE94","v":964},null,{"$f":"DG91+DG93+DG95+DG96+DG97+DG94","v":1214},null,{"$f":"DI91+DI93+DI95+DI96+DI97+DI94","v":1419},null,{"$f":"DK91+DK93+DK95+DK96+DK97+DK94","v":1714},null,{"$f":"DM91+DM93+DM95+DM96+DM97+DM94","v":1919},null,{"$f":"DO91+DO93+DO95+DO96+DO97+DO94","v":2169}]
[12.33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U88&V88","v":"CHEMINEE2525"},"CHEMINEE",2525,null,"Schiedel CHEMINEE",{"$f":"Vokabel!$A$167","v":"Dreischaliges Kaminsystem"},"Nein",{"$f":"Vokabel!$A$175","v":"mit Hinterlüftung und Schamotte-Innenrohr"},null,"N",null,25,25," ",null,null,"Nein","48/90 cm",{"$f":"\"Typ  CHEMINEE \" &V88","v":"Typ  CHEMINEE 2525"},{"$f":"X88&\" \"& V88","v":"Schiedel CHEMINEE 2525"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133006625,666,0,{"$f":"BT88*BU88","v":0},0,{"$f":"BT88*BW88","v":0},0,{"$f":"BT88*BY88","v":0},0,{"$f":"BT88*CA88","v":0},1,{"$f":"BT88*CC88","v":666},1,{"$f":"$BT$73*CE88","v":666},1,{"$f":"$BT$73*CG88","v":666},1,{"$f":"$BT$73*CI88","v":666},2,{"$f":"$BT$73*CK88","v":1332},null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[12.66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U89&V89","v":"CHEMINEE3030"},"CHEMINEE",3030,null,"Schiedel CHEMINEE",{"$f":"Vokabel!$A$167","v":"Dreischaliges Kaminsystem"},"Nein",{"$f":"Vokabel!$A$175","v":"mit Hinterlüftung und Schamotte-Innenrohr"},null,"N",null,30,30," ",null,null,"Nein","55/104 cm",{"$f":"\"Typ  CHEMINEE \" &V89","v":"Typ  CHEMINEE 3030"},{"$f":"X89&\" \"& V89","v":"Schiedel CHEMINEE 3030"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133003325,331,0,{"$f":"BT89*BU89","v":0},0,{"$f":"BT89*BW89","v":0},1,{"$f":"BT89*BY89","v":331},1,{"$f":"BT89*CA89","v":331},0,{"$f":"BT89*CC89","v":0},0,{"$f":"$BT$74*CE89","v":0},1,{"$f":"$BT$74*CG89","v":331},1,{"$f":"$BT$74*CI89","v":331},0,{"$f":"$BT$74*CK89","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408525",235]
[13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409025",209]
[13.33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ICS!$M$4","v":"ICS Matt"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404525",413,null,{"$f":"IF($C$515=\"90°\",$DA90,IF($D$515=\"85°\",$DA89,$DA91))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA90,IF($D$515=\"85°\",$DA89,$DA91))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA90,IF($D$515=\"85°\",$DA89,$DA91))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA90,IF($D$515=\"85°\",$DA89,$DA91))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA90,IF($D$515=\"85°\",$DA89,$DA91))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA90,IF($D$515=\"85°\",$DA89,$DA91))","v":209},null,{"$f":"IF($C$515=\"90°\",$DA90,IF($D$515=\"85°\",$DA89,$DA91))","v":209}]
[13.66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(T93:T107,$T$92,1)","v":"ICS Matt 180"},5,{"$f":"INDEX(T93:T107,$T$92,1)","v":"ICS Matt 180"},{"$f":"INDEX(V93:V107,$T$92,1)","v":180},null,{"$f":"INDEX(X93:X107,$T$92,1)","v":"Schiedel ICS Matt Ø"},{"$f":"INDEX(Y93:Y107,$T$92,1)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V$92,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V$92,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V$92)))","v":"TypICS Matt Ø 180"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kerastar 400","Gesamthöhe",null,"m",{"$f":"ROUND(BV93/1000,2)","v":1.68},null,{"$f":"ROUND(BX93/1000,2)","v":1.85},null,{"$f":"ROUND(BZ93/1000,2)","v":2.0099999999999998},null,{"$f":"ROUND(CB93/1000,2)","v":2.1800000000000002},null,{"$f":"ROUND(CD93/1000,2)","v":2.35},null,{"$f":"ROUND(CF93/1000,2)","v":2.5099999999999998},null,{"$f":"ROUND(CH93/1000,2)","v":2.68},null,{"$f":"ROUND(CJ93/1000,2)","v":2.85},null,{"$f":"ROUND(CL93/1000,2)","v":3.01},null,null,null,null,null,null,null,null,null,null,null,null,null,"rund","eckig"]
[14,null,null,3,{"$f":"INDEX(Daten!E95:E100,D93,1)","v":110},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",Vokabel!$A$476&\" \"&V93,IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V93,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V93)))","v":"ICS Matt 80"},{"$f":"U93&\" \"&V93","v":"ICS Matt 80"},{"$f":"IF(ICS!$M$4=\"ICS\",\"ICS\",IF(ICS!$M$4=\"ICS Matt\",\"ICS Matt\",IF(ICS!$M$4=\"ICS Kupfer\",\"ICS Kupfer\")))","v":"ICS Matt"},80,null,{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel ICS Ø\",IF(ICS!$M$4=\"ICS Matt\",\"Schiedel ICS Matt Ø\",IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&Vokabel!A476&\" Ø\")))","v":"Schiedel ICS Matt Ø"},{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V93,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V93,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V93)))","v":"TypICS Matt Ø 80"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V93,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V93,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V93)))","v":"Schiedel ICS Matt Ø 80"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",{"$f":"BV98+BV100+BV101+BV102+BV103+BV104","v":1682},null,{"$f":"BX98+BX100+BX101+BX102+BX103+BX104","v":1848},null,{"$f":"BZ98+BZ100+BZ101+BZ102+BZ103+BZ104","v":2013},null,{"$f":"CB98+CB100+CB101+CB102+CB103+CB104","v":2179},null,{"$f":"CD98+CD100+CD101+CD102+CD103+CD104","v":2348},null,{"$f":"CF98+CF100+CF101+CF102+CF103+CF104","v":2514},null,{"$f":"CH98+CH100+CH101+CH102+CH103+CH104","v":2679},null,{"$f":"CJ98+CJ100+CJ101+CJ102+CJ103+CJ104","v":2845},null,{"$f":"CL98+CL100+CL101+CL102+CL103+CL104","v":3014},null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",455,455,null,{"$f":"IF($B$490=2,$CZ93,$DA93)","v":455},null,{"$f":"IF($B$490=2,$CZ93,$DA93)","v":455},null,{"$f":"IF($B$490=2,$CZ93,$DA93)","v":455},null,{"$f":"IF($B$490=2,$CZ93,$DA93)","v":455},null,{"$f":"IF($B$490=2,$CZ93,$DA93)","v":455},null,{"$f":"IF($B$490=2,$CZ93,$DA93)","v":455},null,{"$f":"IF($B$490=2,$CZ93,$DA93)","v":455}]
[14.33,null,null,"Frachttabelle",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",Vokabel!$A$476&\" \"&V94,IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V94,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V94)))","v":"ICS Matt 100"},{"$f":"U94&\" \"&V94","v":"ICS Matt 100"},{"$f":"$U$93","v":"ICS Matt"},100,null,{"$f":"$X$93","v":"Schiedel ICS Matt Ø"},{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V94,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V94,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V94)))","v":"TypICS Matt Ø 100"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V94,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V94,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V94)))","v":"Schiedel ICS Matt Ø 100"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m",{"$f":"ROUND(BV95/1000,2)","v":1.33},null,{"$f":"ROUND(BX95/1000,2)","v":1.5},null,{"$f":"ROUND(BZ95/1000,2)","v":1.66},null,{"$f":"ROUND(CB95/1000,2)","v":1.83},null,{"$f":"ROUND(CD95/1000,2)","v":2},null,{"$f":"ROUND(CF95/1000,2)","v":2.16},null,{"$f":"ROUND(CH95/1000,2)","v":2.33},null,{"$f":"ROUND(CJ95/1000,2)","v":2.4900000000000002},null,{"$f":"ROUND(CL95/1000,2)","v":2.66},null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,{"$f":"IF($A$56=3,1045,95)","v":95},null,{"$f":"$DA94","v":95},null,{"$f":"$DA94","v":95},null,{"$f":"$DA94","v":95},null,{"$f":"$DA94","v":95},null,{"$f":"$DA94","v":95},null,{"$f":"$DA94","v":95},null,{"$f":"$DA94","v":95}]
[14.66,null,1,{"$f":"E95","v":"Nein"},{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",Vokabel!$A$476&\" \"&V95,IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V95,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V95)))","v":"ICS Matt 130"},"ICS Matt 130","ICS Matt",130,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V95,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V95,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V95)))","v":"TypICS Matt Ø 130"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V95,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V95,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V95)))","v":"Schiedel ICS Matt Ø 130"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe ",null,null,"mm",{"$f":"IF($F$390=\"90°\",BV101+BV100+BV99+BV102+BV103+BV104,BV104+BV103+BV102+BV101+BV100+BU99)","v":1329.5},null,{"$f":"IF($F$390=\"90°\",BX101+BX100+BX99+BX102+BX103+BX104,BX104+BX103+BX102+BX101+BX100+BW99)","v":1495.5},null,{"$f":"IF($F$390=\"90°\",BZ101+BZ100+BZ99+BZ102+BZ103+BZ104,BZ104+BZ103+BZ102+BZ101+BZ100+BY99)","v":1660.5},null,{"$f":"IF($F$390=\"90°\",CB101+CB100+CB99+CB102+CB103+CB104,CB104+CB103+CB102+CB101+CB100+CA99)","v":1826.5},null,{"$f":"IF($F$390=\"90°\",CD101+CD100+CD99+CD102+CD103+CD104,CD104+CD103+CD102+CD101+CD100+CC99)","v":1995.5},null,{"$f":"IF($F$390=\"90°\",CF101+CF100+CF99+CF102+CF103+CF104,CF104+CF103+CF102+CF101+CF100+CE99)","v":2161.5},null,{"$f":"IF($F$390=\"90°\",CH101+CH100+CH99+CH102+CH103+CH104,CH104+CH103+CH102+CH101+CH100+CG99)","v":2326.5},null,{"$f":"IF($F$390=\"90°\",CJ101+CJ100+CJ99+CJ102+CJ103+CJ104,CJ104+CJ103+CJ102+CJ101+CJ100+CI99)","v":2492.5},null,{"$f":"IF($F$390=\"90°\",CL101+CL100+CL99+CL102+CL103+CL104,CL104+CL103+CL102+CL101+CL100+CK99)","v":2661.5},null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010025",955,0,{"$f":"$DA$11*DB95","v":0},0,{"$f":"$DA$11*DD95","v":0},0,{"$f":"$DA$11*DF95","v":0},0,{"$f":"$DA$11*DH95","v":0},1,{"$f":"$DA$11*DJ95","v":955},1,{"$f":"$DA$11*DL95","v":955},1,{"$f":"$DA$11*DN95","v":955}]
[15,null,2,"0 bis 400 kg             --  140 EUR",140,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",Vokabel!$A$476&\" \"&V96,IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V96,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V96)))","v":"ICS Matt 150"},"ICS Matt 150","ICS Matt",150,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V96,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V96,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V96)))","v":"TypICS Matt Ø 150"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V96,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V96,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V96)))","v":"Schiedel ICS Matt Ø 150"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom UK.Sockel/OK WK bis mitte Anschluss)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005025",455,0,{"$f":"$DA$12*DB96","v":0},0,{"$f":"$DA$12*DD96","v":0},1,{"$f":"$DA$12*DF96","v":455},1,{"$f":"$DA$12*DH96","v":455},0,{"$f":"$DA$12*DJ96","v":0},0,{"$f":"$DA$12*DL96","v":0},1,{"$f":"$DA$12*DN96","v":455}]
[15.33,null,3,"401 bis 2.500 kg      --  110 EUR",110,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",Vokabel!$A$476&\" \"&V97,IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V97,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V97)))","v":"ICS Matt 180"},"ICS Matt 180","ICS Matt",180,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V97,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V97,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V97)))","v":"TypICS Matt Ø 180"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V97,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V97,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V97)))","v":"Schiedel ICS Matt Ø 180"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002525",205,0,{"$f":"$DA$13*DB97","v":0},1,{"$f":"$DA$13*DD97","v":205},0,{"$f":"$DA$13*DF97","v":0},1,{"$f":"$DA$13*DH97","v":205},0,{"$f":"$DA$13*DJ97","v":0},1,{"$f":"$DA$13*DL97","v":205},0,{"$f":"$DA$13*DN97","v":0}]
[15.66,null,4,"2.501 bis 5.000 kg  --  160 EUR",160,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",Vokabel!$A$476&\" \"&V98,IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V98,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V98)))","v":"ICS Matt 200"},"ICS Matt 200","ICS Matt",200,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V98,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V98,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V98)))","v":"TypICS Matt Ø 200"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V98,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V98,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V98)))","v":"Schiedel ICS Matt Ø 200"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666]
[16,null,5,"über 5.000 kg          --  250 EUR",250,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",Vokabel!$A$476&\" \"&V99,IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V99,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V99)))","v":"ICS Matt 250"},"ICS Matt 250","ICS Matt",250,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V99,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V99,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V99)))","v":"TypICS Matt Ø 250"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V99,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V99,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V99)))","v":"Schiedel ICS Matt Ø 250"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA",null,"45°",147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5,147,313.5]
[16.329999999999998,null,6,"per Kommission       --   65 EUR",65,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",Vokabel!$A$476&\" \"&V100,IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V100,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V100)))","v":"ICS Matt 300"},"ICS Matt 300","ICS Matt",300,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V100,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V100,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V100)))","v":"TypICS Matt Ø 300"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V100,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V100,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V100)))","v":"Schiedel ICS Matt Ø 300"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",null,null,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,666,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 300","Gesamthöhe",null,"m",{"$f":"ROUND(DC101/1000,2)","v":0.77},null,{"$f":"ROUND(DE101/1000,2)","v":0.98},null,{"$f":"ROUND(DG101/1000,2)","v":1.23},null,{"$f":"ROUND(DI101/1000,2)","v":1.43},null,{"$f":"ROUND(DK101/1000,2)","v":1.73},null,{"$f":"ROUND(DM101/1000,2)","v":1.93},null,{"$f":"ROUND(DO101/1000,2)","v":2.1800000000000002}]
[16.66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",\"\",IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V101,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V101)))","v":"ICS Matt 350"},{"$f":"IF(T91=\"ICS Kupfer\",\"\",U101&\" \"&V101)","v":"ICS Matt 350"},"ICS Matt",350,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V101,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V101,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V101)))","v":"TypICS Matt Ø 350"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V101,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V101,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V101)))","v":"Schiedel ICS Matt Ø 350"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,null,null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,{"$f":"IF($B$401=2,\"44\",\"350\")","v":"350"},null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC105+DC107+DC109+DC110+DC111+DC108","v":772},null,{"$f":"DE105+DE107+DE109+DE110+DE111+DE108","v":977},null,{"$f":"DG105+DG107+DG109+DG110+DG111+DG108","v":1227},null,{"$f":"DI105+DI107+DI109+DI110+DI111+DI108","v":1432},null,{"$f":"DK105+DK107+DK109+DK110+DK111+DK108","v":1727},null,{"$f":"DM105+DM107+DM109+DM110+DM111+DM108","v":1932},null,{"$f":"DO105+DO107+DO109+DO110+DO111+DO108","v":2182}]
[17,null,null,1,{"$f":"INDEX(Daten!D104:D105,D102,1)","v":"Ja"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",\"\",IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V102,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V102)))","v":"ICS Matt 400"},{"$f":"IF(T91=\"ICS Kupfer\",\"\",U102&\" \"&V102)","v":"ICS Matt 400"},"ICS Matt",400,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V102,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V102,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V102)))","v":"TypICS Matt Ø 400"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V102,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V102,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V102)))","v":"Schiedel ICS Matt Ø 400"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133001625,166,0,{"$f":"BT102*BU102","v":0},1,{"$f":"BT102*BW102","v":166},0,{"$f":"BT102*BY102","v":0},1,{"$f":"BT102*CA102","v":166},0,{"$f":"BT102*CC102","v":0},1,{"$f":"$BT$72*CE102","v":166},0,{"$f":"$BT$72*CG102","v":0},1,{"$f":"$BT$72*CI102","v":166},0,{"$f":"$BT$72*CK102","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[17.329999999999998,null,null,"Fracht",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",\"\",IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V103,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V103)))","v":"ICS Matt 450"},{"$f":"IF(T91=\"ICS Kupfer\",\"\",U103&\" \"&V103)","v":"ICS Matt 450"},"ICS Matt",450,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V103,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V103,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V103)))","v":"TypICS Matt Ø 450"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V103,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V103,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V103)))","v":"Schiedel ICS Matt Ø 450"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133006625,666,0,{"$f":"BT103*BU103","v":0},0,{"$f":"BT103*BW103","v":0},0,{"$f":"BT103*BY103","v":0},0,{"$f":"BT103*CA103","v":0},1,{"$f":"BT103*CC103","v":666},1,{"$f":"$BT$73*CE103","v":666},1,{"$f":"$BT$73*CG103","v":666},1,{"$f":"$BT$73*CI103","v":666},2,{"$f":"$BT$73*CK103","v":1332},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408530",246]
[17.66,null,null,{"$f":"$E$104","v":"Ja"},{"$f":"Vokabel!$A$4","v":"Ja"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",\"\",IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V104,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V104)))","v":"ICS Matt 500"},{"$f":"IF(T91=\"ICS Kupfer\",\"\",U104&\" \"&V104)","v":"ICS Matt 500"},"ICS Matt",500,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V104,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V104,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V104)))","v":"TypICS Matt Ø 500"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V104,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V104,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V104)))","v":"Schiedel ICS Matt Ø 500"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133003325,331,0,{"$f":"BT104*BU104","v":0},0,{"$f":"BT104*BW104","v":0},1,{"$f":"BT104*BY104","v":331},1,{"$f":"BT104*CA104","v":331},0,{"$f":"BT104*CC104","v":0},0,{"$f":"$BT$74*CE104","v":0},1,{"$f":"$BT$74*CG104","v":331},1,{"$f":"$BT$74*CI104","v":331},0,{"$f":"$BT$74*CK104","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409030",222]
[18,null,null,{"$f":"$E$105","v":"Nein"},{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",\"\",IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V105,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V105)))","v":"ICS Matt 550"},{"$f":"IF(T91=\"ICS Kupfer\",\"\",U105&\" \"&V105)","v":"ICS Matt 550"},"ICS Matt",550,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V105,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V105,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V105)))","v":"TypICS Matt Ø 550"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V105,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V105,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V105)))","v":"Schiedel ICS Matt Ø 550"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404530",472,null,{"$f":"IF($C$515=\"90°\",$DA104,IF($D$515=\"85°\",$DA103,$DA105))","v":222},null,{"$f":"IF($C$515=\"90°\",$DA104,IF($D$515=\"85°\",$DA103,$DA105))","v":222},null,{"$f":"IF($C$515=\"90°\",$DA104,IF($D$515=\"85°\",$DA103,$DA105))","v":222},null,{"$f":"IF($C$515=\"90°\",$DA104,IF($D$515=\"85°\",$DA103,$DA105))","v":222},null,{"$f":"IF($C$515=\"90°\",$DA104,IF($D$515=\"85°\",$DA103,$DA105))","v":222},null,{"$f":"IF($C$515=\"90°\",$DA104,IF($D$515=\"85°\",$DA103,$DA105))","v":222},null,{"$f":"IF($C$515=\"90°\",$DA104,IF($D$515=\"85°\",$DA103,$DA105))","v":222}]
[18.329999999999998,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",\"\",IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V106,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V106)))","v":"ICS Matt 600"},{"$f":"IF(T91=\"ICS Kupfer\",\"\",U106&\" \"&V106)","v":"ICS Matt 600"},"ICS Matt",600,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V106,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V106,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V106)))","v":"TypICS Matt Ø 600"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V106,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V106,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V106)))","v":"Schiedel ICS Matt Ø 600"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund","eckig"]
[18.66,null,null,"Typ","Kg","Fracht",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($T$91=\"ICS Kupfer\",\"\",IF($T$91=\"ICS\",Vokabel!$A$481&\" \"&V107,IF($T$91=\"ICS Matt\",Vokabel!$A$480&\" \"&V107)))","v":"ICS Matt 700"},{"$f":"IF(T91=\"ICS Kupfer\",\"\",U107&\" \"&V107)","v":"ICS Matt 700"},"ICS Matt",700,null,"Schiedel ICS Matt Ø",{"$f":"IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$169,Vokabel!$A$168)","v":"Doppelwandiges Edelstahl-Kaminsystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ICS!$M$4=\"ICS\",Vokabel!$A$478&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V107,IF(ICS!$M$4=\"ICS Matt\",Vokabel!$A$478&Vokabel!$A$480&\" Ø \"&$V107,IF(ICS!$M$4=\"ICS Kupfer\",Vokabel!$A$478&\" \"&Vokabel!$A$476&\" Ø \" &$V107)))","v":"TypICS Matt Ø 700"},{"$f":"IF(ICS!$M$4=\"ICS\",\"Schiedel \"&\" ICS \"&Vokabel!$A$473&\" Ø \" &$V107,IF(ICS!$M$4=\"ICS Matt\",\"Schiedel \"&Vokabel!$A$480&\" Ø \"&$V107,IF(ICS!$M$4=\"ICS Kupfer\",\"Schiedel \"&\" \"&Vokabel!$A$476&\" Ø \" &$V107)))","v":"Schiedel ICS Matt Ø 700"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",455,455,null,{"$f":"IF($B$490=2,$CZ107,$DA107)","v":455},null,{"$f":"IF($B$490=2,$CZ107,$DA107)","v":455},null,{"$f":"IF($B$490=2,$CZ107,$DA107)","v":455},null,{"$f":"IF($B$490=2,$CZ107,$DA107)","v":455},null,{"$f":"IF($B$490=2,$CZ107,$DA107)","v":455},null,{"$f":"IF($B$490=2,$CZ107,$DA107)","v":455},null,{"$f":"IF($B$490=2,$CZ107,$DA107)","v":455}]
[19,null,null,{"$f":"Kalkulation!$B$17","v":"Schiedel ABSOLUT, ABS 18"},{"$f":"SUBTOTAL(9,Kalkulation!D25:D171)","v":749.11},100,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,95,null,{"$f":"$DA108","v":95},null,{"$f":"$DA108","v":95},null,{"$f":"$DA108","v":95},null,{"$f":"$DA108","v":95},null,{"$f":"$DA108","v":95},null,{"$f":"$DA108","v":95},null,{"$f":"$DA108","v":95}]
[19.329999999999998,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010030",955,0,{"$f":"$DA$11*DB109","v":0},0,{"$f":"$DA$11*DD109","v":0},0,{"$f":"$DA$11*DF109","v":0},0,{"$f":"$DA$11*DH109","v":0},1,{"$f":"$DA$11*DJ109","v":955},1,{"$f":"$DA$11*DL109","v":955},1,{"$f":"$DA$11*DN109","v":955}]
[19.66,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005030",455,0,{"$f":"$DA$12*DB110","v":0},0,{"$f":"$DA$12*DD110","v":0},1,{"$f":"$DA$12*DF110","v":455},1,{"$f":"$DA$12*DH110","v":455},0,{"$f":"$DA$12*DJ110","v":0},0,{"$f":"$DA$12*DL110","v":0},1,{"$f":"$DA$12*DN110","v":455}]
[20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhen mitte Anschluss",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002530",205,0,{"$f":"$DA$13*DB111","v":0},1,{"$f":"$DA$13*DD111","v":205},0,{"$f":"$DA$13*DF111","v":0},1,{"$f":"$DA$13*DH111","v":205},0,{"$f":"$DA$13*DJ111","v":0},1,{"$f":"$DA$13*DL111","v":205},0,{"$f":"$DA$13*DN111","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BS112","v":1.66},{"$f":"INDEX($BR$114:$BR$123,$BR$113,1)","v":1.66}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"Daten!U22","v":"KERASTAR180"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$BV$4,IF($BS$113=\"KERASTAR160\",$BV$19,IF($BS$113=\"KERASTAR180\",$BV$34,IF($BS$113=\"KERASTAR200\",$BV$49,IF($BS$113=\"KERASTAR250\",$BV$64,IF($BS$113=\"KERASTAR300\",$BV$79,IF($BS$113=\"KERASTAR400\",$BV$94,\"\")))))))","v":1.33},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 350","Gesamthöhe",null,"m",{"$f":"ROUND(DC115/1000,2)","v":0.8},null,{"$f":"ROUND(DE115/1000,2)","v":1},null,{"$f":"ROUND(DG115/1000,2)","v":1.25},null,{"$f":"ROUND(DI115/1000,2)","v":1.46},null,{"$f":"ROUND(DK115/1000,2)","v":1.75},null,{"$f":"ROUND(DM115/1000,2)","v":1.96},null,{"$f":"ROUND(DO115/1000,2)","v":2.21}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$BX$4,IF($BS$113=\"KERASTAR160\",$BX$19,IF($BS$113=\"KERASTAR180\",$BX$34,IF($BS$113=\"KERASTAR200\",$BX$49,IF($BS$113=\"KERASTAR250\",$BX$64,IF($BS$113=\"KERASTAR300\",$BX$79,IF($BS$113=\"KERASTAR400\",$BX$94,\"\")))))))","v":1.5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC119+DC121+DC123+DC124+DC125+DC122","v":797},null,{"$f":"DE119+DE121+DE123+DE124+DE125+DE122","v":1002},null,{"$f":"DG119+DG121+DG123+DG124+DG125+DG122","v":1252},null,{"$f":"DI119+DI121+DI123+DI124+DI125+DI122","v":1457},null,{"$f":"DK119+DK121+DK123+DK124+DK125+DK122","v":1752},null,{"$f":"DM119+DM121+DM123+DM124+DM125+DM122","v":1957},null,{"$f":"DO119+DO121+DO123+DO124+DO125+DO122","v":2207}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$BZ$4,IF($BS$113=\"KERASTAR160\",$BZ$19,IF($BS$113=\"KERASTAR180\",$BZ$34,IF($BS$113=\"KERASTAR200\",$BZ$49,IF($BS$113=\"KERASTAR250\",$BZ$64,IF($BS$113=\"KERASTAR300\",$BZ$79,IF($BS$113=\"KERASTAR400\",$BZ$94,\"\")))))))","v":1.66},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"INDEX(Daten!$T$118:$T$123,T117,1)","v":"Keranova160"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CB$4,IF($BS$113=\"KERASTAR160\",$CB$19,IF($BS$113=\"KERASTAR180\",$CB$34,IF($BS$113=\"KERASTAR200\",$CB$49,IF($BS$113=\"KERASTAR250\",$CB$64,IF($BS$113=\"KERASTAR300\",$CB$79,IF($BS$113=\"KERASTAR400\",$CB$94,\"\")))))))","v":1.83},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408535",270]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U118&V118","v":"Keranova120"},"Keranova",120,null,"Schiedel KERANOVA  Ø",{"$f":"Vokabel!$A$165","v":"Einwandiges Kamin-Sanierungssystem"},null,{"$f":"Vokabel!$A$173","v":"aus Profilkeramik mit keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  KERANOVA \" &V118","v":"Typ  KERANOVA 120"},{"$f":"X118&\" \"& V118&\" mm\"","v":"Schiedel KERANOVA  Ø 120 mm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CD$4,IF($BS$113=\"KERASTAR160\",$CD$19,IF($BS$113=\"KERASTAR180\",$CD$34,IF($BS$113=\"KERASTAR200\",$CD$49,IF($BS$113=\"KERASTAR250\",$CD$64,IF($BS$113=\"KERASTAR300\",$CD$79,IF($BS$113=\"KERASTAR400\",$CD$94,\"\")))))))","v":2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409035",247]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Keranova140","Keranova",140,null,"Schiedel KERANOVA  Ø",{"$f":"Vokabel!$A$165","v":"Einwandiges Kamin-Sanierungssystem"},null,{"$f":"Vokabel!$A$173","v":"aus Profilkeramik mit keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  KERANOVA 140","Schiedel KERANOVA  Ø 140 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CF$4,IF($BS$113=\"KERASTAR160\",$CF$19,IF($BS$113=\"KERASTAR180\",$CF$34,IF($BS$113=\"KERASTAR200\",$CF$49,IF($BS$113=\"KERASTAR250\",$CF$64,IF($BS$113=\"KERASTAR300\",$CF$79,IF($BS$113=\"KERASTAR400\",$CF$94,\"\")))))))","v":2.16},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404535",530,null,{"$f":"IF($C$515=\"90°\",$DA118,IF($D$515=\"85°\",$DA117,$DA119))","v":247},null,{"$f":"IF($C$515=\"90°\",$DA118,IF($D$515=\"85°\",$DA117,$DA119))","v":247},null,{"$f":"IF($C$515=\"90°\",$DA118,IF($D$515=\"85°\",$DA117,$DA119))","v":247},null,{"$f":"IF($C$515=\"90°\",$DA118,IF($D$515=\"85°\",$DA117,$DA119))","v":247},null,{"$f":"IF($C$515=\"90°\",$DA118,IF($D$515=\"85°\",$DA117,$DA119))","v":247},null,{"$f":"IF($C$515=\"90°\",$DA118,IF($D$515=\"85°\",$DA117,$DA119))","v":247},null,{"$f":"IF($C$515=\"90°\",$DA118,IF($D$515=\"85°\",$DA117,$DA119))","v":247}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Keranova160","Keranova",160,null,"Schiedel KERANOVA  Ø",{"$f":"Vokabel!$A$165","v":"Einwandiges Kamin-Sanierungssystem"},null,{"$f":"Vokabel!$A$173","v":"aus Profilkeramik mit keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  KERANOVA 160","Schiedel KERANOVA  Ø 160 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CH$4,IF($BS$113=\"KERASTAR160\",$CH$19,IF($BS$113=\"KERASTAR180\",$CH$34,IF($BS$113=\"KERASTAR200\",$CH$49,IF($BS$113=\"KERASTAR250\",$CH$64,IF($BS$113=\"KERASTAR300\",$CH$79,IF($BS$113=\"KERASTAR400\",$CH$94,\"\")))))))","v":2.33},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund","eckig"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Keranova180","Keranova",180,null,"Schiedel KERANOVA  Ø",{"$f":"Vokabel!$A$165","v":"Einwandiges Kamin-Sanierungssystem"},null,{"$f":"Vokabel!$A$173","v":"aus Profilkeramik mit keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  KERANOVA 180","Schiedel KERANOVA  Ø 180 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CJ$4,IF($BS$113=\"KERASTAR160\",$CJ$19,IF($BS$113=\"KERASTAR180\",$CJ$34,IF($BS$113=\"KERASTAR200\",$CJ$49,IF($BS$113=\"KERASTAR250\",$CJ$64,IF($BS$113=\"KERASTAR300\",$CJ$79,IF($BS$113=\"KERASTAR400\",$CJ$94,\"\")))))))","v":2.4900000000000002},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",535,455,null,{"$f":"IF($B$490=2,$CZ121,$DA121)","v":455},null,{"$f":"IF($B$490=2,$CZ121,$DA121)","v":455},null,{"$f":"IF($B$490=2,$CZ121,$DA121)","v":455},null,{"$f":"IF($B$490=2,$CZ121,$DA121)","v":455},null,{"$f":"IF($B$490=2,$CZ121,$DA121)","v":455},null,{"$f":"IF($B$490=2,$CZ121,$DA121)","v":455},null,{"$f":"IF($B$490=2,$CZ121,$DA121)","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Keranova200","Keranova",200,null,"Schiedel KERANOVA  Ø",{"$f":"Vokabel!$A$165","v":"Einwandiges Kamin-Sanierungssystem"},null,{"$f":"Vokabel!$A$173","v":"aus Profilkeramik mit keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  KERANOVA 200","Schiedel KERANOVA  Ø 200 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CL$4,IF($BS$113=\"KERASTAR160\",$CL$19,IF($BS$113=\"KERASTAR180\",$CL$34,IF($BS$113=\"KERASTAR200\",$CL$49,IF($BS$113=\"KERASTAR250\",$CL$64,IF($BS$113=\"KERASTAR300\",$CL$79,IF($BS$113=\"KERASTAR400\",$CL$94,\"\")))))))","v":2.66},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,95,null,{"$f":"$DA122","v":95},null,{"$f":"$DA122","v":95},null,{"$f":"$DA122","v":95},null,{"$f":"$DA122","v":95},null,{"$f":"$DA122","v":95},null,{"$f":"$DA122","v":95},null,{"$f":"$DA122","v":95}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Keranova250","Keranova",250,null,"Schiedel KERANOVA  Ø",{"$f":"Vokabel!$A$165","v":"Einwandiges Kamin-Sanierungssystem"},null,{"$f":"Vokabel!$A$173","v":"aus Profilkeramik mit keramischer Steckverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  KERANOVA 250","Schiedel KERANOVA  Ø 250 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$151","v":"noch nicht bekannt"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010035",955,0,{"$f":"$DA123*DB123","v":0},0,{"$f":"$DA123*DD123","v":0},0,{"$f":"$DA123*DF123","v":0},0,{"$f":"$DA123*DH123","v":0},1,{"$f":"$DA123*DJ123","v":955},1,{"$f":"$DA123*DL123","v":955},1,{"$f":"$DA123*DN123","v":955}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005035",455,0,{"$f":"$DA124*DB124","v":0},0,{"$f":"$DA124*DD124","v":0},1,{"$f":"$DA124*DF124","v":455},1,{"$f":"$DA124*DH124","v":455},0,{"$f":"$DA124*DJ124","v":0},0,{"$f":"$DA124*DL124","v":0},1,{"$f":"$DA124*DN124","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhen Gesamt",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002535",205,0,{"$f":"$DA125*DB125","v":0},1,{"$f":"$DA125*DD125","v":205},0,{"$f":"$DA125*DF125","v":0},1,{"$f":"$DA125*DH125","v":205},0,{"$f":"$DA125*DJ125","v":0},1,{"$f":"$DA125*DL125","v":205},0,{"$f":"$DA125*DN125","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BS126","v":1.68},{"$f":"INDEX(BR128:BR137,BR127,1)","v":1.68}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"Daten!U22","v":"KERASTAR180"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$BV$2,IF($BS$113=\"KERASTAR160\",$BV$17,IF($BS$113=\"KERASTAR180\",$BV$32,IF($BS$113=\"KERASTAR200\",$BV$47,IF($BS$113=\"KERASTAR250\",$BV$62,IF($BS$113=\"KERASTAR300\",$BV$77,IF($BS$113=\"KERASTAR400\",$BV$92,\"\")))))))","v":1.68},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 400","Gesamthöhe",null,"m",{"$f":"ROUND(DC129/1000,2)","v":0.83},null,{"$f":"ROUND(DE129/1000,2)","v":1.04},null,{"$f":"ROUND(DG129/1000,2)","v":1.29},null,{"$f":"ROUND(DI129/1000,2)","v":1.49},null,{"$f":"ROUND(DK129/1000,2)","v":1.79},null,{"$f":"ROUND(DM129/1000,2)","v":1.99},null,{"$f":"ROUND(DO129/1000,2)","v":2.2400000000000002}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$BX$2,IF($BS$113=\"KERASTAR160\",$BX$17,IF($BS$113=\"KERASTAR180\",$BX$32,IF($BS$113=\"KERASTAR200\",$BX$47,IF($BS$113=\"KERASTAR250\",$BX$62,IF($BS$113=\"KERASTAR300\",$BX$77,IF($BS$113=\"KERASTAR400\",$BX$92,\"\")))))))","v":1.85},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC133+DC135+DC137+DC138+DC139+DC136","v":830},null,{"$f":"DE133+DE135+DE137+DE138+DE139+DE136","v":1035},null,{"$f":"DG133+DG135+DG137+DG138+DG139+DG136","v":1285},null,{"$f":"DI133+DI135+DI137+DI138+DI139+DI136","v":1490},null,{"$f":"DK133+DK135+DK137+DK138+DK139+DK136","v":1785},null,{"$f":"DM133+DM135+DM137+DM138+DM139+DM136","v":1990},null,{"$f":"DO133+DO135+DO137+DO138+DO139+DO136","v":2240}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$BZ$2,IF($BS$113=\"KERASTAR160\",$BZ$17,IF($BS$113=\"KERASTAR180\",$BZ$32,IF($BS$113=\"KERASTAR200\",$BZ$47,IF($BS$113=\"KERASTAR250\",$BZ$62,IF($BS$113=\"KERASTAR300\",$BZ$77,IF($BS$113=\"KERASTAR400\",$BZ$92,\"\")))))))","v":2.0099999999999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CB$2,IF($BS$113=\"KERASTAR160\",$CB$17,IF($BS$113=\"KERASTAR180\",$CB$32,IF($BS$113=\"KERASTAR200\",$CB$47,IF($BS$113=\"KERASTAR250\",$CB$62,IF($BS$113=\"KERASTAR300\",$CB$77,IF($BS$113=\"KERASTAR400\",$CB$92,\"\")))))))","v":2.1800000000000002},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408540",305]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CD$2,IF($BS$113=\"KERASTAR160\",$CD$17,IF($BS$113=\"KERASTAR180\",$CD$32,IF($BS$113=\"KERASTAR200\",$CD$47,IF($BS$113=\"KERASTAR250\",$CD$62,IF($BS$113=\"KERASTAR300\",$CD$77,IF($BS$113=\"KERASTAR400\",$CD$92,\"\")))))))","v":2.35},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409040",280]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CF$2,IF($BS$113=\"KERASTAR160\",$CF$17,IF($BS$113=\"KERASTAR180\",$CF$32,IF($BS$113=\"KERASTAR200\",$CF$47,IF($BS$113=\"KERASTAR250\",$CF$62,IF($BS$113=\"KERASTAR300\",$CF$77,IF($BS$113=\"KERASTAR400\",$CF$92,\"\")))))))","v":2.5099999999999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404540",615,null,{"$f":"IF($C$515=\"90°\",$DA132,IF($D$515=\"85°\",$DA131,$DA133))","v":280},null,{"$f":"IF($C$515=\"90°\",$DA132,IF($D$515=\"85°\",$DA131,$DA133))","v":280},null,{"$f":"IF($C$515=\"90°\",$DA132,IF($D$515=\"85°\",$DA131,$DA133))","v":280},null,{"$f":"IF($C$515=\"90°\",$DA132,IF($D$515=\"85°\",$DA131,$DA133))","v":280},null,{"$f":"IF($C$515=\"90°\",$DA132,IF($D$515=\"85°\",$DA131,$DA133))","v":280},null,{"$f":"IF($C$515=\"90°\",$DA132,IF($D$515=\"85°\",$DA131,$DA133))","v":280},null,{"$f":"IF($C$515=\"90°\",$DA132,IF($D$515=\"85°\",$DA131,$DA133))","v":280}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CH$2,IF($BS$113=\"KERASTAR160\",$CH$17,IF($BS$113=\"KERASTAR180\",$CH$32,IF($BS$113=\"KERASTAR200\",$CH$47,IF($BS$113=\"KERASTAR250\",$CH$62,IF($BS$113=\"KERASTAR300\",$CH$77,IF($BS$113=\"KERASTAR400\",$CH$92,\"\")))))))","v":2.68},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund gibt es nicht 705","eckig"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CJ$2,IF($BS$113=\"KERASTAR160\",$CJ$17,IF($BS$113=\"KERASTAR180\",$CJ$32,IF($BS$113=\"KERASTAR200\",$CJ$47,IF($BS$113=\"KERASTAR250\",$CJ$62,IF($BS$113=\"KERASTAR300\",$CJ$77,IF($BS$113=\"KERASTAR400\",$CJ$92,\"\")))))))","v":2.85},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",455,455,null,{"$f":"IF($B$490=2,$CZ135,$DA135)","v":455},null,{"$f":"IF($B$490=2,$CZ135,$DA135)","v":455},null,{"$f":"IF($B$490=2,$CZ135,$DA135)","v":455},null,{"$f":"IF($B$490=2,$CZ135,$DA135)","v":455},null,{"$f":"IF($B$490=2,$CZ135,$DA135)","v":455},null,{"$f":"IF($B$490=2,$CZ135,$DA135)","v":455},null,{"$f":"IF($B$490=2,$CZ135,$DA135)","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($BS$113=\"KERASTAR140\",$CL$2,IF($BS$113=\"KERASTAR160\",$CL$17,IF($BS$113=\"KERASTAR180\",$CL$32,IF($BS$113=\"KERASTAR200\",$CL$47,IF($BS$113=\"KERASTAR250\",$CL$62,IF($BS$113=\"KERASTAR300\",$CL$77,IF($BS$113=\"KERASTAR400\",$CL$92,\"\")))))))","v":3.01},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,95,null,{"$f":"$DA136","v":95},null,{"$f":"$DA136","v":95},null,{"$f":"$DA136","v":95},null,{"$f":"$DA136","v":95},null,{"$f":"$DA136","v":95},null,{"$f":"$DA136","v":95},null,{"$f":"$DA136","v":95}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010040",955,0,{"$f":"$DA137*DB137","v":0},0,{"$f":"$DA137*DD137","v":0},0,{"$f":"$DA137*DF137","v":0},0,{"$f":"$DA137*DH137","v":0},1,{"$f":"$DA137*DJ137","v":955},1,{"$f":"$DA137*DL137","v":955},1,{"$f":"$DA137*DN137","v":955}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RA-Verlängerung",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005040",455,0,{"$f":"$DA138*DB138","v":0},0,{"$f":"$DA138*DD138","v":0},1,{"$f":"$DA138*DF138","v":455},1,{"$f":"$DA138*DH138","v":455},0,{"$f":"$DA138*DJ138","v":0},0,{"$f":"$DA138*DL138","v":0},1,{"$f":"$DA138*DN138","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"INDEX(Daten!T140:T154,$T$139,1)","v":"PRIMA PLUS 180"},{"$f":"INDEX(Daten!V140:V154,$T$139,1)","v":180},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrbedarf bei Anschlußhöhe",null,"manuelle Nachjustierung (beim Rohr 331 oder 666)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002540",205,0,{"$f":"$DA139*DB139","v":0},1,{"$f":"$DA139*DD139","v":205},0,{"$f":"$DA139*DF139","v":0},1,{"$f":"$DA139*DH139","v":205},0,{"$f":"$DA139*DJ139","v":0},1,{"$f":"$DA139*DL139","v":205},0,{"$f":"$DA139*DN139","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U140&\" \"&V140","v":"PRIMA PLUS 80"},"PRIMA PLUS",80,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  PPL \" &V140&\" / 0,6\"","v":"Typ  PPL 80 / 0,6"},{"$f":"X140&\" \"& V140&\" / 0,6 mm\"","v":"Schiedel PRIMA PLUS Ø 80 / 0,6 mm"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 100","PRIMA PLUS",100,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  PPL 100 / 0,6","Schiedel PRIMA PLUS Ø 100 / 0,6 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A-NR."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 130","PRIMA PLUS",130,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  PPL 130 / 0,6","Schiedel PRIMA PLUS Ø 130 / 0,6 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"$BS$113","v":"KERASTAR180"},{"$f":"IF(BR142=\"KERASTAR140\",133001614,IF(BR142=\"KERASTAR160\",133001616,IF(BR142=\"KERASTAR180\",133001618,IF(BR142=\"KERASTAR200\",133001620,IF(BR142=\"KERASTAR250\",133001625,\"\")))))","v":133001618},{"$f":"$BR$114","v":1.33},{"$f":"$BU$12","v":0},null,null,{"$f":"IF($BR$113=10,0,VLOOKUP($BR$112,BT142:BU150,2,0))","v":0},{"$f":"IF($C$461=\"166 mm\",1,0)","v":0},{"$f":"Kerastar!$P$18","v":0},null,{"$f":"BS142","v":133001618},{"$f":"SUM(BX142:BZ142)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 450","Gesamthöhe",null,"m",{"$f":"ROUND(DC143/1000,2)","v":0.86},null,{"$f":"ROUND(DE143/1000,2)","v":1.07},null,{"$f":"ROUND(DG143/1000,2)","v":1.32},null,{"$f":"ROUND(DI143/1000,2)","v":1.52},null,{"$f":"ROUND(DK143/1000,2)","v":1.82},null,{"$f":"ROUND(DM143/1000,2)","v":2.02},null,{"$f":"ROUND(DO143/1000,2)","v":2.27}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 150","PRIMA PLUS",150,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  PPL 150 / 0,6","Schiedel PRIMA PLUS Ø 150 / 0,6 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",{"$f":"$BS$142","v":133001618},{"$f":"$BR$115","v":1.5},{"$f":"$BW$12","v":1},null,"Meter",null,{"$f":"BY142*166/1000","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC147+DC149+DC151+DC152+DC153+DC150","v":860},null,{"$f":"DE147+DE149+DE151+DE152+DE153+DE150","v":1065},null,{"$f":"DG147+DG149+DG151+DG152+DG153+DG150","v":1315},null,{"$f":"DI147+DI149+DI151+DI152+DI153+DI150","v":1520},null,{"$f":"DK147+DK149+DK151+DK152+DK153+DK150","v":1815},null,{"$f":"DM147+DM149+DM151+DM152+DM153+DM150","v":2020},null,{"$f":"DO147+DO149+DO151+DO152+DO153+DO150","v":2270}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 180","PRIMA PLUS",180,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  PPL 180 / 0,6","Schiedel PRIMA PLUS Ø 180 / 0,6 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133001618,{"$f":"$BR$116","v":1.66},{"$f":"$BY$12","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[null,"Preislistengültigkeit!",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 200","PRIMA PLUS",200,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  PPL 200 / 0,6","Schiedel PRIMA PLUS Ø 200 / 0,6 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133001618,{"$f":"$BR$117","v":1.83},{"$f":"$CA$12","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408545",332]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 250","PRIMA PLUS",250,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  PPL 250 / 0,6","Schiedel PRIMA PLUS Ø 250 / 0,6 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133001618,{"$f":"$BR$118","v":2},{"$f":"$CC$12","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409045",310]
[null,"ABSOLUT",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 300","PRIMA PLUS",300,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  PPL 300 / 0,6","Schiedel PRIMA PLUS Ø 300 / 0,6 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133001618,{"$f":"$BR$119","v":2.16},{"$f":"$CE$12","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404545",675,null,{"$f":"IF($C$515=\"90°\",$DA146,IF($D$515=\"85°\",$DA145,$DA147))","v":310},null,{"$f":"IF($C$515=\"90°\",$DA146,IF($D$515=\"85°\",$DA145,$DA147))","v":310},null,{"$f":"IF($C$515=\"90°\",$DA146,IF($D$515=\"85°\",$DA145,$DA147))","v":310},null,{"$f":"IF($C$515=\"90°\",$DA146,IF($D$515=\"85°\",$DA145,$DA147))","v":310},null,{"$f":"IF($C$515=\"90°\",$DA146,IF($D$515=\"85°\",$DA145,$DA147))","v":310},null,{"$f":"IF($C$515=\"90°\",$DA146,IF($D$515=\"85°\",$DA145,$DA147))","v":310},null,{"$f":"IF($C$515=\"90°\",$DA146,IF($D$515=\"85°\",$DA145,$DA147))","v":310}]
[null,"CHEMINEE",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 350","PRIMA PLUS",350,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  PPL 350 / 0,6","Schiedel PRIMA PLUS Ø 350 / 0,6 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133001618,{"$f":"$BR$120","v":2.33},{"$f":"$CG$12","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund gibt es nicht 705","eckig"]
[null,"KERASTAR",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 400","PRIMA PLUS",400,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,"Typ  PPL 400 / 0,6","Schiedel PRIMA PLUS Ø 400 / 0,6 mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133001618,{"$f":"$BR$121","v":2.4900000000000002},{"$f":"$CI$12","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",455,455,null,{"$f":"IF($B$490=2,$CZ149,$DA149)","v":455},null,{"$f":"IF($B$490=2,$CZ149,$DA149)","v":455},null,{"$f":"IF($B$490=2,$CZ149,$DA149)","v":455},null,{"$f":"IF($B$490=2,$CZ149,$DA149)","v":455},null,{"$f":"IF($B$490=2,$CZ149,$DA149)","v":455},null,{"$f":"IF($B$490=2,$CZ149,$DA149)","v":455},null,{"$f":"IF($B$490=2,$CZ149,$DA149)","v":455}]
[null,"Keranova",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 450","PRIMA PLUS",450,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  PPL \" &V150&\" / 1,0\"","v":"Typ  PPL 450 / 1,0"},{"$f":"X150&\" \"& V150&\" / 1,0 mm\"","v":"Schiedel PRIMA PLUS Ø 450 / 1,0 mm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133001618,{"$f":"$BR$122","v":2.66},{"$f":"$CK$12","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,95,null,{"$f":"$DA150","v":95},null,{"$f":"$DA150","v":95},null,{"$f":"$DA150","v":95},null,{"$f":"$DA150","v":95},null,{"$f":"$DA150","v":95},null,{"$f":"$DA150","v":95},null,{"$f":"$DA150","v":95}]
[null,"ICS",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMA PLUS 500","PRIMA PLUS",500,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  PPL \" &V151&\" / 1,0\"","v":"Typ  PPL 500 / 1,0"},{"$f":"X151&\" \"& V151&\" / 1,0 mm\"","v":"Schiedel PRIMA PLUS Ø 500 / 1,0 mm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",{"$f":"IF(BR151=\"KERASTAR140\",133003314,IF(BR151=\"KERASTAR160\",133003316,IF(BR151=\"KERASTAR180\",133003318,IF(BR151=\"KERASTAR200\",133003320,IF(BR151=\"KERASTAR250\",133003325,\"\")))))","v":133003318},{"$f":"$BR$114","v":1.33},{"$f":"$BU$14","v":0},null,null,{"$f":"IF($BR$113=10,1,VLOOKUP($BR$112,BT151:BU159,2,0))","v":1},{"$f":"IF($C$461=\"331 mm\",1,0)","v":0},{"$f":"Kerastar!$P$16","v":0},null,{"$f":"BS151","v":133003318},{"$f":"SUM(BX151:BZ151)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010045",955,0,{"$f":"$DA151*DB151","v":0},0,{"$f":"$DA151*DD151","v":0},0,{"$f":"$DA151*DF151","v":0},0,{"$f":"$DA151*DH151","v":0},1,{"$f":"$DA151*DJ151","v":955},1,{"$f":"$DA151*DL151","v":955},1,{"$f":"$DA151*DN151","v":955}]
[null,"ICS Kupfer",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U152&\" \"&V152","v":"PRIMA PLUS 600"},"PRIMA PLUS",600,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  PPL \" &V152&\" / 1,0\"","v":"Typ  PPL 600 / 1,0"},{"$f":"X152&\" \"& V152&\" / 1,0 mm\"","v":"Schiedel PRIMA PLUS Ø 600 / 1,0 mm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",{"$f":"$BS$151","v":133003318},{"$f":"$BR$115","v":1.5},{"$f":"$BW$14","v":0},null,"Meter",null,{"$f":"BY151*331/1000","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005045",455,0,{"$f":"$DA152*DB152","v":0},0,{"$f":"$DA152*DD152","v":0},1,{"$f":"$DA152*DF152","v":455},1,{"$f":"$DA152*DH152","v":455},0,{"$f":"$DA152*DJ152","v":0},0,{"$f":"$DA152*DL152","v":0},1,{"$f":"$DA152*DN152","v":455}]
[null,"ICS Matt",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U153&\" \"&V153","v":"PRIMA PLUS 700"},"PRIMA PLUS",700,null,"Schiedel PRIMA PLUS Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  PPL \" &V153&\" / 1,0\"","v":"Typ  PPL 700 / 1,0"},{"$f":"X153&\" \"& V153&\" / 1,0 mm\"","v":"Schiedel PRIMA PLUS Ø 700 / 1,0 mm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133003318,{"$f":"$BR$116","v":1.66},{"$f":"$BY$14","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002545",205,0,{"$f":"$DA153*DB153","v":0},1,{"$f":"$DA153*DD153","v":205},0,{"$f":"$DA153*DF153","v":0},1,{"$f":"$DA153*DH153","v":205},0,{"$f":"$DA153*DJ153","v":0},1,{"$f":"$DA153*DL153","v":205},0,{"$f":"$DA153*DN153","v":0}]
[null,"ISOLIT",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133003318,{"$f":"$BR$117","v":1.83},{"$f":"$CA$14","v":1}]
[null,"Prima Plus",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133003318,{"$f":"$BR$118","v":2},{"$f":"$CC$14","v":0}]
[null,"Technostar120",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133003318,{"$f":"$BR$119","v":2.16},{"$f":"$CE$14","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 500","Gesamthöhe",null,"m",{"$f":"ROUND(DC157/1000,2)","v":0.88},null,{"$f":"ROUND(DE157/1000,2)","v":1.0900000000000001},null,{"$f":"ROUND(DG157/1000,2)","v":1.34},null,{"$f":"ROUND(DI157/1000,2)","v":1.54},null,{"$f":"ROUND(DK157/1000,2)","v":1.84},null,{"$f":"ROUND(DM157/1000,2)","v":2.04},null,{"$f":"ROUND(DO157/1000,2)","v":2.29}]
[null,"ICS5000",{"$f":"Vokabel!$A$257","v":"Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133003318,{"$f":"$BR$120","v":2.33},{"$f":"$CG$14","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC161+DC163+DC165+DC166+DC167+DC164","v":880},null,{"$f":"DE161+DE163+DE165+DE166+DE167+DE164","v":1085},null,{"$f":"DG161+DG163+DG165+DG166+DG167+DG164","v":1335},null,{"$f":"DI161+DI163+DI165+DI166+DI167+DI164","v":1540},null,{"$f":"DK161+DK163+DK165+DK166+DK167+DK164","v":1835},null,{"$f":"DM161+DM163+DM165+DM166+DM167+DM164","v":2040},null,{"$f":"DO161+DO163+DO165+DO166+DO167+DO164","v":2290}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133003318,{"$f":"$BR$121","v":2.4900000000000002},{"$f":"$CI$14","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133003318,{"$f":"$BR$122","v":2.66},{"$f":"$CK$14","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408550",357]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",{"$f":"IF(BR160=\"KERASTAR140\",133006614,IF(BR160=\"KERASTAR160\",133006616,IF(BR160=\"KERASTAR180\",133006618,IF(BR160=\"KERASTAR200\",133006620,IF(BR160=\"KERASTAR250\",133006625,\"\")))))","v":133006618},{"$f":"$BR$114","v":1.33},{"$f":"$BU$13","v":0},null,null,{"$f":"IF($BR$113=10,0,VLOOKUP($BR$112,BT160:BU168,2,0))","v":0},{"$f":"IF($C$461=\"666 mm\",1,0)","v":0},null,null,{"$f":"BS160","v":133006618},{"$f":"SUM(BX160:BZ160)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409050",330]
[null,1,{"$f":"INDEX(A163:A165,B161,1)","v":1},null,{"$f":"Eingabe!J1","v":1},{"$f":"INDEX(E163:E165,E161,1)","v":"Version   20230101"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",{"$f":"$BS$160","v":133006618},{"$f":"$BR$115","v":1.5},{"$f":"$BW$13","v":0},null,"Meter",{"$f":"IF(BY160<>0,BY160*666/1000,0)","v":0},{"$f":"BY160*666/1000","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404550",735,null,{"$f":"IF($C$515=\"90°\",$DA160,IF($D$515=\"85°\",$DA159,$DA161))","v":330},null,{"$f":"IF($C$515=\"90°\",$DA160,IF($D$515=\"85°\",$DA159,$DA161))","v":330},null,{"$f":"IF($C$515=\"90°\",$DA160,IF($D$515=\"85°\",$DA159,$DA161))","v":330},null,{"$f":"IF($C$515=\"90°\",$DA160,IF($D$515=\"85°\",$DA159,$DA161))","v":330},null,{"$f":"IF($C$515=\"90°\",$DA160,IF($D$515=\"85°\",$DA159,$DA161))","v":330},null,{"$f":"IF($C$515=\"90°\",$DA160,IF($D$515=\"85°\",$DA159,$DA161))","v":330},null,{"$f":"IF($C$515=\"90°\",$DA160,IF($D$515=\"85°\",$DA159,$DA161))","v":330}]
[null,"Sprache",null,null,"Versionseingabe:",null,20230101,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"INDEX(Daten!T163:T166,T162,1)","v":"Prima+1,0250"},{"$f":"INDEX(Daten!V163:V166,$T$162,1)","v":250},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133006618,{"$f":"$BR$116","v":1.66},{"$f":"$BY$13","v":0},null,"Sum.Meter",null,{"$f":"SUM(BY143,BY152,BY161)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund gibt es nicht 705","eckig"]
[1,"Deutsch",null,"D",{"$f":"F163&\"   \"&$G$162","v":"Version   20230101"},"Version",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U163&V163","v":"Prima+1,0150"},"Prima+1,0",150,null,"Schiedel Prima+1,0 mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  PRIMA+1,0 mm Ø \" &V163","v":"Typ  PRIMA+1,0 mm Ø 150"},{"$f":"X163&\" \"& V163","v":"Schiedel Prima+1,0 mm Ø 150"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133006618,{"$f":"$BR$117","v":1.83},{"$f":"$CA$13","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",455,455,null,{"$f":"IF($B$490=2,$CZ163,$DA163)","v":455},null,{"$f":"IF($B$490=2,$CZ163,$DA163)","v":455},null,{"$f":"IF($B$490=2,$CZ163,$DA163)","v":455},null,{"$f":"IF($B$490=2,$CZ163,$DA163)","v":455},null,{"$f":"IF($B$490=2,$CZ163,$DA163)","v":455},null,{"$f":"IF($B$490=2,$CZ163,$DA163)","v":455},null,{"$f":"IF($B$490=2,$CZ163,$DA163)","v":455}]
[2,"Französisch",null,"FR",{"$f":"F164&\"   \"&$G$162","v":"Version   20230101"},"Version",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U164&V164","v":"Prima+1,0180"},"Prima+1,0",180,null,"Schiedel Prima+1,0 mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  PRIMA+1,0 mm Ø \" &V164","v":"Typ  PRIMA+1,0 mm Ø 180"},{"$f":"X164&\" \"& V164","v":"Schiedel Prima+1,0 mm Ø 180"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133006618,{"$f":"$BR$118","v":2},{"$f":"$CC$13","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,95,null,{"$f":"$DA164","v":95},null,{"$f":"$DA164","v":95},null,{"$f":"$DA164","v":95},null,{"$f":"$DA164","v":95},null,{"$f":"$DA164","v":95},null,{"$f":"$DA164","v":95},null,{"$f":"$DA164","v":95}]
[3,"Italienisch",null,"ITA",{"$f":"F165&\"   \"&$G$162","v":"Versione   20230101"},"Versione",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U165&V165","v":"Prima+1,0200"},"Prima+1,0",200,null,"Schiedel Prima+1,0 mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  PRIMA+1,0 mm Ø \" &V165","v":"Typ  PRIMA+1,0 mm Ø 200"},{"$f":"X165&\" \"& V165","v":"Schiedel Prima+1,0 mm Ø 200"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133006618,{"$f":"$BR$119","v":2.16},{"$f":"$CE$13","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010050",955,0,{"$f":"$DA165*DB165","v":0},0,{"$f":"$DA165*DD165","v":0},0,{"$f":"$DA165*DF165","v":0},0,{"$f":"$DA165*DH165","v":0},1,{"$f":"$DA165*DJ165","v":955},1,{"$f":"$DA165*DL165","v":955},1,{"$f":"$DA165*DN165","v":955}]
[4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U166&V166","v":"Prima+1,0250"},"Prima+1,0",250,null,"Schiedel Prima+1,0 mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,{"$f":"\"Typ  PRIMA+1,0 mm Ø \" &V166","v":"Typ  PRIMA+1,0 mm Ø 250"},{"$f":"X166&\" \"& V166","v":"Schiedel Prima+1,0 mm Ø 250"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133006618,{"$f":"$BR$120","v":2.33},{"$f":"$CG$13","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005050",455,0,{"$f":"$DA166*DB166","v":0},0,{"$f":"$DA166*DD166","v":0},1,{"$f":"$DA166*DF166","v":455},1,{"$f":"$DA166*DH166","v":455},0,{"$f":"$DA166*DJ166","v":0},0,{"$f":"$DA166*DL166","v":0},1,{"$f":"$DA166*DN166","v":455}]
[5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133006618,{"$f":"$BR$121","v":2.4900000000000002},{"$f":"$CI$13","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002550",205,0,{"$f":"$DA167*DB167","v":0},1,{"$f":"$DA167*DD167","v":205},0,{"$f":"$DA167*DF167","v":0},1,{"$f":"$DA167*DH167","v":205},0,{"$f":"$DA167*DJ167","v":0},1,{"$f":"$DA167*DL167","v":205},0,{"$f":"$DA167*DN167","v":0}]
[6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KERASTAR180",133006618,{"$f":"$BR$122","v":2.66},{"$f":"$CK$13","v":2}]
[7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"INDEX(T171:T185,$T$170,1)","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 550","Gesamthöhe",null,"m",{"$f":"ROUND(DC171/1000,2)","v":0.95},null,{"$f":"ROUND(DE171/1000,2)","v":1.1599999999999999},null,{"$f":"ROUND(DG171/1000,2)","v":1.41},null,{"$f":"ROUND(DI171/1000,2)","v":1.61},null,{"$f":"ROUND(DK171/1000,2)","v":1.91},null,{"$f":"ROUND(DM171/1000,2)","v":2.11},null,{"$f":"ROUND(DO171/1000,2)","v":2.36}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U171","v":"Nein"},{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC175+DC177+DC179+DC180+DC181+DC178","v":950},null,{"$f":"DE175+DE177+DE179+DE180+DE181+DE178","v":1155},null,{"$f":"DG175+DG177+DG179+DG180+DG181+DG178","v":1405},null,{"$f":"DI175+DI177+DI179+DI180+DI181+DI178","v":1610},null,{"$f":"DK175+DK177+DK179+DK180+DK181+DK178","v":1905},null,{"$f":"DM175+DM177+DM179+DM180+DM181+DM178","v":2110},null,{"$f":"DO175+DO177+DO179+DO180+DO181+DO178","v":2360}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U172&\" \"&\"Ø \"&V172","v":"VL-PPL 0,6 Ø 80"},"VL-PPL 0,6",80,null,"Schiedel PRIMA PLUS 0,6mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 0,6 Ø 100","VL-PPL 0,6",100,null,"Schiedel PRIMA PLUS 0,6mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408555",427]
[null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 0,6 Ø 130","VL-PPL 0,6",130,null,"Schiedel PRIMA PLUS 0,6mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409055",400]
[null,"Sockel bei Absolut",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 0,6 Ø 150","VL-PPL 0,6",150,null,"Schiedel PRIMA PLUS 0,6mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404555",835,null,{"$f":"IF($C$515=\"90°\",$DA174,IF($D$515=\"85°\",$DA173,$DA175))","v":400},null,{"$f":"IF($C$515=\"90°\",$DA174,IF($D$515=\"85°\",$DA173,$DA175))","v":400},null,{"$f":"IF($C$515=\"90°\",$DA174,IF($D$515=\"85°\",$DA173,$DA175))","v":400},null,{"$f":"IF($C$515=\"90°\",$DA174,IF($D$515=\"85°\",$DA173,$DA175))","v":400},null,{"$f":"IF($C$515=\"90°\",$DA174,IF($D$515=\"85°\",$DA173,$DA175))","v":400},null,{"$f":"IF($C$515=\"90°\",$DA174,IF($D$515=\"85°\",$DA173,$DA175))","v":400},null,{"$f":"IF($C$515=\"90°\",$DA174,IF($D$515=\"85°\",$DA173,$DA175))","v":400}]
[1,{"$f":"IF($C$181=3,\"\",Vokabel!$A$5)","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 0,6 Ø 180","VL-PPL 0,6",180,null,"Schiedel PRIMA PLUS 0,6mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund gibt es nicht 705","eckig"]
[2,{"$f":"IF($C$181=3,\"\",Vokabel!$A$4)","v":"Ja"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 0,6 Ø 200","VL-PPL 0,6",200,null,"Schiedel PRIMA PLUS 0,6mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",455,455,null,{"$f":"IF($B$490=2,$CZ177,$DA177)","v":455},null,{"$f":"IF($B$490=2,$CZ177,$DA177)","v":455},null,{"$f":"IF($B$490=2,$CZ177,$DA177)","v":455},null,{"$f":"IF($B$490=2,$CZ177,$DA177)","v":455},null,{"$f":"IF($B$490=2,$CZ177,$DA177)","v":455},null,{"$f":"IF($B$490=2,$CZ177,$DA177)","v":455},null,{"$f":"IF($B$490=2,$CZ177,$DA177)","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 0,6 Ø 250","VL-PPL 0,6",250,null,"Schiedel PRIMA PLUS 0,6mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,95,null,{"$f":"$DA178","v":95},null,{"$f":"$DA178","v":95},null,{"$f":"$DA178","v":95},null,{"$f":"$DA178","v":95},null,{"$f":"$DA178","v":95},null,{"$f":"$DA178","v":95},null,{"$f":"$DA178","v":95}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 0,6 Ø 300","VL-PPL 0,6",300,null,"Schiedel PRIMA PLUS 0,6mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010055",955,0,{"$f":"$DA179*DB179","v":0},0,{"$f":"$DA179*DD179","v":0},0,{"$f":"$DA179*DF179","v":0},0,{"$f":"$DA179*DH179","v":0},1,{"$f":"$DA179*DJ179","v":955},1,{"$f":"$DA179*DL179","v":955},1,{"$f":"$DA179*DN179","v":955}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 1,0 Ø 350","VL-PPL 1,0",350,null,"Schiedel PRIMA PLUS 1mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005055",455,0,{"$f":"$DA180*DB180","v":0},0,{"$f":"$DA180*DD180","v":0},1,{"$f":"$DA180*DF180","v":455},1,{"$f":"$DA180*DH180","v":455},0,{"$f":"$DA180*DJ180","v":0},0,{"$f":"$DA180*DL180","v":0},1,{"$f":"$DA180*DN180","v":455}]
[null,null,{"$f":"IF(V35=14,\"\",$B$183)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 1,0 Ø 400","VL-PPL 1,0",400,null,"Schiedel PRIMA PLUS 1mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002555",205,0,{"$f":"$DA181*DB181","v":0},1,{"$f":"$DA181*DD181","v":205},0,{"$f":"$DA181*DF181","v":0},1,{"$f":"$DA181*DH181","v":205},0,{"$f":"$DA181*DJ181","v":0},1,{"$f":"$DA181*DL181","v":205},0,{"$f":"$DA181*DN181","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 1,0 Ø 450","VL-PPL 1,0",450,null,"Schiedel PRIMA PLUS 1mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"}]
[null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VL-PPL 1,0 Ø 500","VL-PPL 1,0",500,null,"Schiedel PRIMA PLUS 1mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"}]
[null,"Fertigfuß oder Montagebauweise Absolut",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U184&\" \"&\"Ø \"&V184","v":"VL-PPL 1,0 Ø 600"},"VL-PPL 1,0",600,null,"Schiedel PRIMA PLUS 1mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 600","Gesamthöhe",null,"m",{"$f":"ROUND(DC185/1000,2)","v":0.93},null,{"$f":"ROUND(DE185/1000,2)","v":1.1399999999999999},null,{"$f":"ROUND(DG185/1000,2)","v":1.39},null,{"$f":"ROUND(DI185/1000,2)","v":1.59},null,{"$f":"ROUND(DK185/1000,2)","v":1.89},null,{"$f":"ROUND(DM185/1000,2)","v":2.09},null,{"$f":"ROUND(DO185/1000,2)","v":2.34}]
[1,{"$f":"IF($V$35=30,$D$186,IF($V$35=40,$D$186,IF($V$35=\"25TL\",$D$186,IF($V$35=\"30L\",$D$186,IF($V$35=\"40L\",$D$186,$D$185)))))","v":"Fertigfuss"},{"$f":"Vokabel!$A$6","v":"Fertigfuss - Ø links"},{"$f":"Vokabel!$A$8","v":"Fertigfuss"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U185&\" \"&\"Ø \"&V185","v":"VL-PPL 1,0 Ø 700"},"VL-PPL 1,0",700,null,"Schiedel PRIMA PLUS 1mm Ø",{"$f":"Vokabel!$A$170","v":"Einwandiges Edelstahl-Sanierungssystem"},null,{"$f":"Vokabel!$A$176","v":"in Elementbauweise mit Steckmuffenverbindung"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC189+DC191+DC193+DC194+DC195+DC192","v":930},null,{"$f":"DE189+DE191+DE193+DE194+DE195+DE192","v":1135},null,{"$f":"DG189+DG191+DG193+DG194+DG195+DG192","v":1385},null,{"$f":"DI189+DI191+DI193+DI194+DI195+DI192","v":1590},null,{"$f":"DK189+DK191+DK193+DK194+DK195+DK192","v":1885},null,{"$f":"DM189+DM191+DM193+DM194+DM195+DM192","v":2090},null,{"$f":"DO189+DO191+DO193+DO194+DO195+DO192","v":2340}]
[2,{"$f":"IF(AF35=\"Ja\",Vokabel!$A$5,IF(AE35<>0,Vokabel!$A$5,IF($V$35=14,\"\",IF($AE$35=0,$C$186,\"\"))))","v":"Deckenanschlusskonus"},{"$f":"Vokabel!$A$9","v":"Deckenanschlusskonus"},{"$f":"Vokabel!$A$482","v":"Grundpaket"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408560",412]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409060",380]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404560",855,null,{"$f":"IF($C$515=\"90°\",$DA188,IF($D$515=\"85°\",$DA187,$DA189))","v":380},null,{"$f":"IF($C$515=\"90°\",$DA188,IF($D$515=\"85°\",$DA187,$DA189))","v":380},null,{"$f":"IF($C$515=\"90°\",$DA188,IF($D$515=\"85°\",$DA187,$DA189))","v":380},null,{"$f":"IF($C$515=\"90°\",$DA188,IF($D$515=\"85°\",$DA187,$DA189))","v":380},null,{"$f":"IF($C$515=\"90°\",$DA188,IF($D$515=\"85°\",$DA187,$DA189))","v":380},null,{"$f":"IF($C$515=\"90°\",$DA188,IF($D$515=\"85°\",$DA187,$DA189))","v":380},null,{"$f":"IF($C$515=\"90°\",$DA188,IF($D$515=\"85°\",$DA187,$DA189))","v":380}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund gibt es nicht 705","eckig"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",455,455,null,{"$f":"IF($B$490=2,$CZ191,$DA191)","v":455},null,{"$f":"IF($B$490=2,$CZ191,$DA191)","v":455},null,{"$f":"IF($B$490=2,$CZ191,$DA191)","v":455},null,{"$f":"IF($B$490=2,$CZ191,$DA191)","v":455},null,{"$f":"IF($B$490=2,$CZ191,$DA191)","v":455},null,{"$f":"IF($B$490=2,$CZ191,$DA191)","v":455},null,{"$f":"IF($B$490=2,$CZ191,$DA191)","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,95,null,{"$f":"$DA192","v":95},null,{"$f":"$DA192","v":95},null,{"$f":"$DA192","v":95},null,{"$f":"$DA192","v":95},null,{"$f":"$DA192","v":95},null,{"$f":"$DA192","v":95},null,{"$f":"$DA192","v":95}]
[null,2,{"$f":"INDEX(A195:A199,B193,1)","v":1},null,null,1,{"$f":"INDEX(Daten!F195:F196,F193,1)","v":"90°"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010060",955,0,{"$f":"$DA193*DB193","v":0},0,{"$f":"$DA193*DD193","v":0},0,{"$f":"$DA193*DF193","v":0},0,{"$f":"$DA193*DH193","v":0},1,{"$f":"$DA193*DJ193","v":955},1,{"$f":"$DA193*DL193","v":955},1,{"$f":"$DA193*DN193","v":955}]
[null,"1. Rauchrohranschl. Absolut,Cheminee,Keranova",null,null,null,"1. Rauchrohranschl. Grad Absolut",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005060",455,0,{"$f":"$DA194*DB194","v":0},0,{"$f":"$DA194*DD194","v":0},1,{"$f":"$DA194*DF194","v":455},1,{"$f":"$DA194*DH194","v":455},0,{"$f":"$DA194*DJ194","v":0},0,{"$f":"$DA194*DL194","v":0},1,{"$f":"$DA194*DN194","v":455}]
[0,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,{"$f":"\"90°\"","v":"90°"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002560",205,0,{"$f":"$DA195*DB195","v":0},1,{"$f":"$DA195*DD195","v":205},0,{"$f":"$DA195*DF195","v":0},1,{"$f":"$DA195*DH195","v":205},0,{"$f":"$DA195*DJ195","v":0},1,{"$f":"$DA195*DL195","v":205},0,{"$f":"$DA195*DN195","v":0}]
[1,1,null,null,null,{"$f":"\"45°\"","v":"45°"}]
[2,2]
[3,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 655","Gesamthöhe",null,"m",{"$f":"ROUND(DC199/1000,2)","v":1.51},null,{"$f":"ROUND(DE199/1000,2)","v":1.72},null,{"$f":"ROUND(DG199/1000,2)","v":1.97},null,{"$f":"ROUND(DI199/1000,2)","v":2.17},null,{"$f":"ROUND(DK199/1000,2)","v":2.4700000000000002},null,{"$f":"ROUND(DM199/1000,2)","v":2.67},null,{"$f":"ROUND(DO199/1000,2)","v":2.92}]
[4,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC203+DC205+DC207+DC208+DC209+DC206","v":1512},null,{"$f":"DE203+DE205+DE207+DE208+DE209+DE206","v":1717},null,{"$f":"DG203+DG205+DG207+DG208+DG209+DG206","v":1967},null,{"$f":"DI203+DI205+DI207+DI208+DI209+DI206","v":2172},null,{"$f":"DK203+DK205+DK207+DK208+DK209+DK206","v":2467},null,{"$f":"DM203+DM205+DM207+DM208+DM209+DM206","v":2672},null,{"$f":"DO203+DO205+DO207+DO208+DO209+DO206","v":2922}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Achsmaße"]
[null,1,{"$f":"INDEX(A204:A208,B202,1)","v":0},null,null,1,{"$f":"INDEX(Daten!F204:F205,F202,1)","v":"90°"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","DF2120655",453]
[null,"2. Rauchrohranschl. STK großer DM",null,null,null,"2. Rauchrohranschl. Grad großer DM",null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"INDEX(Daten!T204:T209,$T$203,1)","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","DF2121655",952,null,{"$f":"IF($D$17=\"90°\",$DA$202,$DA$203)","v":952},null,{"$f":"IF($D$17=\"90°\",$DA$202,$DA$203)","v":952},null,{"$f":"IF($D$17=\"90°\",$DA$202,$DA$203)","v":952},null,{"$f":"IF($D$17=\"90°\",$DA$202,$DA$203)","v":952},null,{"$f":"IF($D$17=\"90°\",$DA$202,$DA$203)","v":952},null,{"$f":"IF($D$17=\"90°\",$DA$202,$DA$203)","v":952},null,{"$f":"IF($D$17=\"90°\",$DA$202,$DA$203)","v":952}]
[0,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,"90°",null,null,null,null,null,null,null,null,null,null,null,null,null,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eckig"]
[1,1,null,null,null,"45°",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U205&\" \"&\"Ø \"&V205","v":"VL-Technostar120 Ø 80"},"VL-Technostar120",80,null,"Technostar Ø",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",null,455,null,{"$f":"IF($E$1=2,$DA205,$DA205)","v":455},null,{"$f":"IF($E$1=2,$DA205,$DA205)","v":455},null,{"$f":"IF($E$1=2,$DA205,$DA205)","v":455},null,{"$f":"IF($E$1=2,$DA205,$DA205)","v":455},null,{"$f":"IF($E$1=2,$DA205,$DA205)","v":455},null,{"$f":"IF($E$1=2,$DA205,$DA205)","v":455},null,{"$f":"IF($E$1=2,$DA205,$DA205)","v":455}]
[2,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U206&\" \"&\"Ø \"&V206","v":"VL-Technostar120 Ø 110"},"VL-Technostar120",110,null,"Technostar Ø",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,null,null,105,null,105,null,105,null,105,null,105,null,105,null,105]
[3,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U207&\" \"&\"Ø \"&V207","v":"VL-Technostar120 Ø 125"},"VL-Technostar120",125,null,"Technostar Ø",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","DF2101655",955,0,{"$f":"$DA$11*DB207","v":0},0,{"$f":"$DA$11*DD207","v":0},0,{"$f":"$DA$11*DF207","v":0},0,{"$f":"$DA$11*DH207","v":0},1,{"$f":"$DA$11*DJ207","v":955},1,{"$f":"$DA$11*DL207","v":955},1,{"$f":"$DA$11*DN207","v":955}]
[4,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U208&\" \"&\"Ø \"&V208","v":"VL-Technostar120 Ø 160"},"VL-Technostar120",160,null,"Technostar Ø",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","DF2102655",455,0,{"$f":"$DA$12*DB208","v":0},0,{"$f":"$DA$12*DD208","v":0},1,{"$f":"$DA$12*DF208","v":455},1,{"$f":"$DA$12*DH208","v":455},0,{"$f":"$DA$12*DJ208","v":0},0,{"$f":"$DA$12*DL208","v":0},1,{"$f":"$DA$12*DN208","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U209&\" \"&\"Ø \"&V209","v":"VL-Technostar LAS Ø 80"},"VL-Technostar LAS",80,null,"Technostar LAS Ø",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","DF2103655",205,0,{"$f":"$DA$13*DB209","v":0},1,{"$f":"$DA$13*DD209","v":205},0,{"$f":"$DA$13*DF209","v":0},1,{"$f":"$DA$13*DH209","v":205},0,{"$f":"$DA$13*DJ209","v":0},1,{"$f":"$DA$13*DL209","v":205},0,{"$f":"$DA$13*DN209","v":0}]
[]
[null,null,null,null,null,"nicht aktiv !"]
[null,2,{"$f":"INDEX(A214:A216,B212,1)","v":2},null,null,1,{"$f":"INDEX(Daten!F214:F220,F212,1)","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS 700","Gesamthöhe",null,"m",{"$f":"ROUND(DC213/1000,2)","v":0.98},null,{"$f":"ROUND(DE213/1000,2)","v":1.19},null,{"$f":"ROUND(DG213/1000,2)","v":1.44},null,{"$f":"ROUND(DI213/1000,2)","v":1.64},null,{"$f":"ROUND(DK213/1000,2)","v":1.94},null,{"$f":"ROUND(DM213/1000,2)","v":2.14},null,{"$f":"ROUND(DO213/1000,2)","v":2.39}]
[null,"Abdeckplatte Absolut",null,null,null,"Kaminkopf-Struktur",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhe",null,null,"mm",{"$f":"DC217+DC219+DC221+DC222+DC223+DC220","v":980},null,{"$f":"DE217+DE219+DE221+DE222+DE223+DE220","v":1185},null,{"$f":"DG217+DG219+DG221+DG222+DG223+DG220","v":1435},null,{"$f":"DI217+DI219+DI221+DI222+DI223+DI220","v":1640},null,{"$f":"DK217+DK219+DK221+DK222+DK223+DK220","v":1935},null,{"$f":"DM217+DM219+DM221+DM222+DM223+DM220","v":2140},null,{"$f":"DO217+DO219+DO221+DO222+DO223+DO220","v":2390}]
[1,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,"Nein",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(=vom 1.Rohr bis mitte Anschluss)",null,"Achsmaße"]
[{"$f":"IF($G$212=\"Nein\",2,1)","v":2},{"$f":"IF($AP$35=\"Nein\",Vokabel!$A$10,\"\")","v":"aus Faserbeton  8,5 cm Überstand"},null,null,null,"Ziegelnachbildung klassisch-rot",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 85°","231408570",467]
[{"$f":"IF($G$212=\"Nein\",3,1)","v":3},{"$f":"Vokabel!$A$11","v":"aus Edelstahl 8,5 cm Überstand"},null,null,null,"Schiefernachbildung schwarzgrau",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück 90°","231409070",430]
[{"$f":"IF($G$212=\"Nein\",4,1)","v":4},null,null,null,null,"Rauhputznachbildung weiß",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-Stück-mitte RA 45°","231404570",980,null,{"$f":"IF($C$515=\"90°\",$DA216,IF($D$515=\"85°\",$DA215,$DA217))","v":430},null,{"$f":"IF($C$515=\"90°\",$DA216,IF($D$515=\"85°\",$DA215,$DA217))","v":430},null,{"$f":"IF($C$515=\"90°\",$DA216,IF($D$515=\"85°\",$DA215,$DA217))","v":430},null,{"$f":"IF($C$515=\"90°\",$DA216,IF($D$515=\"85°\",$DA215,$DA217))","v":430},null,{"$f":"IF($C$515=\"90°\",$DA216,IF($D$515=\"85°\",$DA215,$DA217))","v":430},null,{"$f":"IF($C$515=\"90°\",$DA216,IF($D$515=\"85°\",$DA215,$DA217))","v":430},null,{"$f":"IF($C$515=\"90°\",$DA216,IF($D$515=\"85°\",$DA215,$DA217))","v":430}]
[{"$f":"IF($G$212=\"Nein\",5,1)","v":5},null,null,null,null,"glatt - betongrau",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rund gibt es nicht 705","eckig"]
[{"$f":"IF($G$212=\"Nein\",6,1)","v":6},null,null,null,null,"glatt - schwarzgrau",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inspektionselement",455,455,null,{"$f":"IF($B$490=2,$CZ219,$DA219)","v":455},null,{"$f":"IF($B$490=2,$CZ219,$DA219)","v":455},null,{"$f":"IF($B$490=2,$CZ219,$DA219)","v":455},null,{"$f":"IF($B$490=2,$CZ219,$DA219)","v":455},null,{"$f":"IF($B$490=2,$CZ219,$DA219)","v":455},null,{"$f":"IF($B$490=2,$CZ219,$DA219)","v":455},null,{"$f":"IF($B$490=2,$CZ219,$DA219)","v":455}]
[{"$f":"IF($G$212=\"Nein\",7,1)","v":7},null,null,null,null,"glatt - klassisch-rot",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sockel",null,95,null,{"$f":"$DA220","v":95},null,{"$f":"$DA220","v":95},null,{"$f":"$DA220","v":95},null,{"$f":"$DA220","v":95},null,{"$f":"$DA220","v":95},null,{"$f":"$DA220","v":95},null,{"$f":"$DA220","v":95}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 955","142010070",955,0,{"$f":"$DA221*DB221","v":0},0,{"$f":"$DA221*DD221","v":0},0,{"$f":"$DA221*DF221","v":0},0,{"$f":"$DA221*DH221","v":0},1,{"$f":"$DA221*DJ221","v":955},1,{"$f":"$DA221*DL221","v":955},1,{"$f":"$DA221*DN221","v":955}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 455","142005070",455,0,{"$f":"$DA222*DB222","v":0},0,{"$f":"$DA222*DD222","v":0},1,{"$f":"$DA222*DF222","v":455},1,{"$f":"$DA222*DH222","v":455},0,{"$f":"$DA222*DJ222","v":0},0,{"$f":"$DA222*DL222","v":0},1,{"$f":"$DA222*DN222","v":455}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrelement 205","142002570",205,0,{"$f":"$DA223*DB223","v":0},1,{"$f":"$DA223*DD223","v":205},0,{"$f":"$DA223*DF223","v":0},1,{"$f":"$DA223*DH223","v":205},0,{"$f":"$DA223*DJ223","v":0},1,{"$f":"$DA223*DL223","v":205},0,{"$f":"$DA223*DN223","v":0}]
[]
[]
[null,1,null,null,null,1]
[null,"Steckadapter Absolut großer Zug",null,null,null,"Steckadapter Absolut kleiner Zug",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Das doppelwandige Edelstahl-Abgassystem für Hochdruck-"]
[1,{"$f":"IF(C181=3,\"\",Vokabel!$A$5)","v":"Nein"},null,null,1,{"$f":"IF($AE$35=0,\"\",Vokabel!$A$5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Abgasanlagen bis 600°C (5000Pa)"]
[2,{"$f":"IF(C181=3,\"\",Vokabel!$A$12)","v":"Steckadapter"},null,null,2,{"$f":"IF($AE$35=0,\"\",Vokabel!$A$12)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ICS!$M$4","v":"ICS Matt"}]
[3,{"$f":"IF($C$181=3,\"\",IF($AO$35=14,$C$230,IF($AO$35=16,$C$230,IF($AO$35=18,$C$230,IF($AO$35=20,$C$230,\"\")))))","v":"Doppelfutter 100"},{"$f":"Vokabel!$A$13","v":"Doppelfutter 100"},null,3,{"$f":"IF($AE$35=0,\"\",IF($AN$35=14,$G$230,IF($AN$35=16,$G$230,IF($AN$35=18,$G$230,IF($AN$35=20,$G$230,\"\")))))","v":""},{"$f":"Vokabel!$A$13","v":"Doppelfutter 100"},null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"INDEX(T231:T243,T230,1)","v":"ICS5000 180"},{"$f":"INDEX(V231:V243,T230,1)","v":180},null,{"$f":"INDEX(X231:X243,T230,1)","v":"Schiedel ICS 5000"},{"$f":"INDEX(Y231:Y243,T230,1)","v":"Das doppelwandige Edelstahl-Abgassystem für"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V$230","v":"Typ ICS 5000 Matt Ø 180"}]
[4,{"$f":"IF($C$181=3,\"\",IF($AO$35=14,$C$231,IF($AO$35=16,$C$231,IF($AO$35=18,$C$231,IF($AO$35=20,$C$231,\"\")))))","v":"Doppelfutter 120"},{"$f":"Vokabel!$A$14","v":"Doppelfutter 120"},null,4,{"$f":"IF($AE$35=0,\"\",IF($AN$35=14,$G$231,IF($AN$35=16,$G$231,IF($AN$35=18,$G$231,IF($AN$35=20,$G$231,\"\")))))","v":""},{"$f":"Vokabel!$A$14","v":"Doppelfutter 120"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U231&\" \"&V231","v":"ICS5000 80"},"ICS5000",80,null,"Schiedel ICS 5000",{"$f":"Vokabel!$A$483","v":"Das doppelwandige Edelstahl-Abgassystem für"},null,{"$f":"Vokabel!$A$484","v":"Hochdruck-Abgasanlagen bis 600°C (5000Pa)"},null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V231","v":"Typ ICS 5000 Matt Ø 80"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V231","v":"Schiedel ICS 5000 Matt Ø 80"}]
[5,{"$f":"IF($C$181=3,\"\",IF($AO$35=14,$C$232,IF($AO$35=16,$C$232,IF($AO$35=18,$C$232,IF($AO$35=20,$C$232,\"\")))))","v":"Doppelfutter 130"},{"$f":"Vokabel!$A$15","v":"Doppelfutter 130"},null,5,{"$f":"IF($AE$35=0,\"\",IF($AN$35=14,$G$232,IF($AN$35=16,$G$232,IF($AN$35=18,$G$232,IF($AN$35=20,$G$232,\"\")))))","v":""},{"$f":"Vokabel!$A$15","v":"Doppelfutter 130"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U232&\" \"&V232","v":"ICS5000 100"},"ICS5000",100,null,"Schiedel ICS 5000",{"$f":"Y231","v":"Das doppelwandige Edelstahl-Abgassystem für"},null,{"$f":"AA231","v":"Hochdruck-Abgasanlagen bis 600°C (5000Pa)"},null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V232","v":"Typ ICS 5000 Matt Ø 100"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V232","v":"Schiedel ICS 5000 Matt Ø 100"}]
[6,{"$f":"IF($C$181=3,\"\",IF($AO$35=14,$C$233,IF($AO$35=16,$C$233,IF($AO$35=18,$C$233,IF($AO$35=20,$C$233,\"\")))))","v":"Doppelfutter 150"},{"$f":"Vokabel!$A$16","v":"Doppelfutter 150"},null,6,{"$f":"IF($AE$35=0,\"\",IF($AN$35=14,\"\",IF($AN$35=16,$G$233,IF($AN$35=18,$G$233,IF($AN$35=20,$G$233,\"\")))))","v":""},{"$f":"Vokabel!$A$16","v":"Doppelfutter 150"},null,null,null,null,null,null,null,null,null,null,null,null,"ICS5000 130","ICS5000",130,null,"Schiedel ICS 5000",{"$f":"Y232","v":"Das doppelwandige Edelstahl-Abgassystem für"},null,{"$f":"AA232","v":"Hochdruck-Abgasanlagen bis 600°C (5000Pa)"},null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V233","v":"Typ ICS 5000 Matt Ø 130"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V233","v":"Schiedel ICS 5000 Matt Ø 130"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anschlusshöhen mitte Anschluss"]
[7,{"$f":"IF($C$181=3,\"\",IF($AO$35=14,\"\",IF($AO$35=16,\"\",IF($AO$35=18,$C$234,IF($AO$35=20,$C$234,IF($AO$35=25,$C$234,\"\"))))))","v":"Doppelfutter 180"},{"$f":"Vokabel!$A$17","v":"Doppelfutter 180"},null,7,{"$f":"IF($AE$35=0,\"\",IF($AN$35=14,\"\",IF($AN$35=16,\"\",IF($AN$35=18,$G$234,IF($AN$35=20,$G$234,\"\")))))","v":""},{"$f":"Vokabel!$A$17","v":"Doppelfutter 180"},null,null,null,null,null,null,null,null,null,null,null,null,"ICS5000 150","ICS5000",150,null,"Schiedel ICS 5000","Das doppelwandige Edelstahl-Abgassystem für",null,"Hochdruck-Abgasanlagen bis 600°C (5000Pa)",null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V234","v":"Typ ICS 5000 Matt Ø 150"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V234","v":"Schiedel ICS 5000 Matt Ø 150"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"$CZ$234","v":""},{"$f":"INDEX(CY236:CY243,CY235,1)","v":""}]
[8,{"$f":"IF($C$181=3,\"\",IF($AO$35=14,\"\",IF($AO$35=16,\"\",IF($AO$35=18,\"\",IF($AO$35=20,$C$235,IF($AO$35=25,$C$235,\"\"))))))","v":""},{"$f":"Vokabel!$A$18","v":"Doppelfutter 200"},null,8,{"$f":"IF($AE$35=0,\"\",IF($AN$35=14,\"\",IF($AN$35=16,\"\",IF($AN$35=18,\"\",IF($AN$35=20,$G$235,\"\")))))","v":""},{"$f":"Vokabel!$A$18","v":"Doppelfutter 200"},null,null,null,null,null,null,null,null,null,null,null,null,"ICS5000 180","ICS5000",180,null,"Schiedel ICS 5000","Das doppelwandige Edelstahl-Abgassystem für",null,"Hochdruck-Abgasanlagen bis 600°C (5000Pa)",null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V235","v":"Typ ICS 5000 Matt Ø 180"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V235","v":"Schiedel ICS 5000 Matt Ø 180"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"$U$92","v":"ICS Matt 180"}]
[9,{"$f":"IF($C$181=3,\"\",IF($AO$35=14,\"\",IF($AO$35=16,\"\",IF($AO$35=18,\"\",IF($AO$35=20,\"\",IF($AO$35=25,$C$236,\"\"))))))","v":""},{"$f":"Vokabel!$A$261","v":"Doppelfutter 250"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS5000 200","ICS5000",200,null,"Schiedel ICS 5000","Das doppelwandige Edelstahl-Abgassystem für",null,"Hochdruck-Abgasanlagen bis 600°C (5000Pa)",null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V236","v":"Typ ICS 5000 Matt Ø 200"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V236","v":"Schiedel ICS 5000 Matt Ø 200"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DC",{"$f":"IF($CZ$235=\"ICS 80\",DC2,IF($CZ$235=\"ICS 100\",DC16,IF($CZ$235=\"ICS 130\",DC30,IF($CZ$235=\"ICS 150\",DC44,IF($CZ$235=\"ICS 180\",DC58,IF($CZ$235=\"ICS 200\",DC72,IF($CZ$235=\"ICS 250\",DC86,CZ236)))))))","v":""},{"$f":"IF($CZ$235=\"ICS 300\",DC100,IF($CZ$235=\"ICS 350\",DC114,IF($CZ$235=\"ICS 400\",DC128,IF($CZ$235=\"ICS 450\",DC142,IF($CZ$235=\"ICS 500\",DC156,IF($CZ$235=\"ICS 550\",DC170,DA236))))))","v":""},{"$f":"IF($CZ$235=\"ICS 600\",DC184,IF($CZ$235=\"ICS 650\",DC198,IF($CZ$235=\"ICS 700\",DC212,\"\")))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS5000 250","ICS5000",250,null,"Schiedel ICS 5000","Das doppelwandige Edelstahl-Abgassystem für",null,"Hochdruck-Abgasanlagen bis 600°C (5000Pa)",null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V237","v":"Typ ICS 5000 Matt Ø 250"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V237","v":"Schiedel ICS 5000 Matt Ø 250"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DE",{"$f":"IF($CZ$235=\"ICS 80\",DE2,IF($CZ$235=\"ICS 100\",DE16,IF($CZ$235=\"ICS 130\",DE30,IF($CZ$235=\"ICS 150\",DE44,IF($CZ$235=\"ICS 180\",DE58,IF($CZ$235=\"ICS 200\",DE72,IF($CZ$235=\"ICS 250\",DE86,CZ237)))))))","v":""},{"$f":"IF($CZ$235=\"ICS 300\",DE100,IF($CZ$235=\"ICS 350\",DE114,IF($CZ$235=\"ICS 400\",DE128,IF($CZ$235=\"ICS 450\",DE142,IF($CZ$235=\"ICS 500\",DE156,IF($CZ$235=\"ICS 550\",DE170,DA237))))))","v":""},{"$f":"IF($CZ$235=\"ICS 600\",DE184,IF($CZ$235=\"ICS 650\",DE198,IF($CZ$235=\"ICS 700\",DE212,\"\")))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS5000 300","ICS5000",300,null,"Schiedel ICS 5000","Das doppelwandige Edelstahl-Abgassystem für",null,"Hochdruck-Abgasanlagen bis 600°C (5000Pa)",null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V238","v":"Typ ICS 5000 Matt Ø 300"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V238","v":"Schiedel ICS 5000 Matt Ø 300"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DG",{"$f":"IF($CZ$235=\"ICS 80\",DG2,IF($CZ$235=\"ICS 100\",DG16,IF($CZ$235=\"ICS 130\",DG30,IF($CZ$235=\"ICS 150\",DG44,IF($CZ$235=\"ICS 180\",DG58,IF($CZ$235=\"ICS 200\",DG72,IF($CZ$235=\"ICS 250\",DG86,CZ238)))))))","v":""},{"$f":"IF($CZ$235=\"ICS 300\",DG100,IF($CZ$235=\"ICS 350\",DG114,IF($CZ$235=\"ICS 400\",DG128,IF($CZ$235=\"ICS 450\",DG142,IF($CZ$235=\"ICS 500\",DG156,IF($CZ$235=\"ICS 550\",DG170,DA238))))))","v":""},{"$f":"IF($CZ$235=\"ICS 600\",DG184,IF($CZ$235=\"ICS 650\",DG198,IF($CZ$235=\"ICS 700\",DG212,\"\")))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(T229=\"ICS Kupfer\",\"\",U239&\" \"&V239)","v":"ICS5000 350"},"ICS5000",350,null,"Schiedel ICS 5000","Das doppelwandige Edelstahl-Abgassystem für",null,"Hochdruck-Abgasanlagen bis 600°C (5000Pa)",null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V239","v":"Typ ICS 5000 Matt Ø 350"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V239","v":"Schiedel ICS 5000 Matt Ø 350"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DI",{"$f":"IF($CZ$235=\"ICS 80\",DI2,IF($CZ$235=\"ICS 100\",DI16,IF($CZ$235=\"ICS 130\",DI30,IF($CZ$235=\"ICS 150\",DI44,IF($CZ$235=\"ICS 180\",DI58,IF($CZ$235=\"ICS 200\",DI72,IF($CZ$235=\"ICS 250\",DI86,CZ239)))))))","v":""},{"$f":"IF($CZ$235=\"ICS 300\",DI100,IF($CZ$235=\"ICS 350\",DI114,IF($CZ$235=\"ICS 400\",DI128,IF($CZ$235=\"ICS 450\",DI142,IF($CZ$235=\"ICS 500\",DI156,IF($CZ$235=\"ICS 550\",DI170,DA239))))))","v":""},{"$f":"IF($CZ$235=\"ICS 600\",DI184,IF($CZ$235=\"ICS 650\",DI198,IF($CZ$235=\"ICS 700\",DI212,\"\")))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(T229=\"ICS Kupfer\",\"\",U240&\" \"&V240)","v":"ICS5000 400"},"ICS5000",400,null,"Schiedel ICS 5000","Das doppelwandige Edelstahl-Abgassystem für",null,"Hochdruck-Abgasanlagen bis 600°C (5000Pa)",null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V240","v":"Typ ICS 5000 Matt Ø 400"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V240","v":"Schiedel ICS 5000 Matt Ø 400"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DK",{"$f":"IF($CZ$235=\"ICS 80\",DK2,IF($CZ$235=\"ICS 100\",DK16,IF($CZ$235=\"ICS 130\",DK30,IF($CZ$235=\"ICS 150\",DK44,IF($CZ$235=\"ICS 180\",DK58,IF($CZ$235=\"ICS 200\",DK72,IF($CZ$235=\"ICS 250\",DK86,CZ240)))))))","v":""},{"$f":"IF($CZ$235=\"ICS 300\",DK100,IF($CZ$235=\"ICS 350\",DK114,IF($CZ$235=\"ICS 400\",DK128,IF($CZ$235=\"ICS 450\",DK142,IF($CZ$235=\"ICS 500\",DK156,IF($CZ$235=\"ICS 550\",DK170,DA240))))))","v":""},{"$f":"IF($CZ$235=\"ICS 600\",DK184,IF($CZ$235=\"ICS 650\",DK198,IF($CZ$235=\"ICS 700\",DK212,\"\")))","v":""}]
[null,1,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(T229=\"ICS Kupfer\",\"\",U241&\" \"&V241)","v":"ICS5000 450"},"ICS5000",450,null,"Schiedel ICS 5000","Das doppelwandige Edelstahl-Abgassystem für",null,"Hochdruck-Abgasanlagen bis 600°C (5000Pa)",null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V241","v":"Typ ICS 5000 Matt Ø 450"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V241","v":"Schiedel ICS 5000 Matt Ø 450"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DM",{"$f":"IF($CZ$235=\"ICS 80\",DM2,IF($CZ$235=\"ICS 100\",DM16,IF($CZ$235=\"ICS 130\",DM30,IF($CZ$235=\"ICS 150\",DM44,IF($CZ$235=\"ICS 180\",DM58,IF($CZ$235=\"ICS 200\",DM72,IF($CZ$235=\"ICS 250\",DM86,CZ241)))))))","v":""},{"$f":"IF($CZ$235=\"ICS 300\",DM100,IF($CZ$235=\"ICS 350\",DM114,IF($CZ$235=\"ICS 400\",DM128,IF($CZ$235=\"ICS 450\",DM142,IF($CZ$235=\"ICS 500\",DM156,IF($CZ$235=\"ICS 550\",DM170,DA241))))))","v":""},{"$f":"IF($CZ$235=\"ICS 600\",DM184,IF($CZ$235=\"ICS 650\",DM198,IF($CZ$235=\"ICS 700\",DM212,\"\")))","v":""}]
[null,"Zugr. m. Explkl für Absolut großer Zug",null,null,null,"Zugr. m. Explkl für Absolut kleiner Zug",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(T229=\"ICS Kupfer\",\"\",U242&\" \"&V242)","v":"ICS5000 500"},"ICS5000",500,null,"Schiedel ICS 5000","Das doppelwandige Edelstahl-Abgassystem für",null,"Hochdruck-Abgasanlagen bis 600°C (5000Pa)",null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V242","v":"Typ ICS 5000 Matt Ø 500"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V242","v":"Schiedel ICS 5000 Matt Ø 500"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DO",{"$f":"IF($CZ$235=\"ICS 80\",DO2,IF($CZ$235=\"ICS 100\",DO16,IF($CZ$235=\"ICS 130\",DO30,IF($CZ$235=\"ICS 150\",DO44,IF($CZ$235=\"ICS 180\",DO58,IF($CZ$235=\"ICS 200\",DO72,IF($CZ$235=\"ICS 250\",DO86,CZ242)))))))","v":""},{"$f":"IF($CZ$235=\"ICS 300\",DO100,IF($CZ$235=\"ICS 350\",DO114,IF($CZ$235=\"ICS 400\",DO128,IF($CZ$235=\"ICS 450\",DO142,IF($CZ$235=\"ICS 500\",DO156,IF($CZ$235=\"ICS 550\",DO170,DA242))))))","v":""},{"$f":"IF($CZ$235=\"ICS 600\",DO184,IF($CZ$235=\"ICS 650\",DO198,IF($CZ$235=\"ICS 700\",DO212,\"\")))","v":""}]
[1,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,1,{"$f":"IF($AE$35=0,\"\",Vokabel!$A$5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(T229=\"ICS Kupfer\",\"\",U243&\" \"&V243)","v":"ICS5000 600"},"ICS5000",600,null,"Schiedel ICS 5000","Das doppelwandige Edelstahl-Abgassystem für",null,"Hochdruck-Abgasanlagen bis 600°C (5000Pa)",null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$478&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V243","v":"Typ ICS 5000 Matt Ø 600"},{"$f":"\"Schiedel\"&\" ICS 5000 \"&Vokabel!$A$474&\" Ø \"&Daten!$V243","v":"Schiedel ICS 5000 Matt Ø 600"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$151","v":"noch nicht bekannt"}]
[2,{"$f":"IF($V$35=30,\"\",IF($V$35=40,\"\",IF($V$35=\"30L\",\"\",IF($V$35=\"40L\",\"\",Vokabel!$A$4))))","v":"Ja"},null,null,2,{"$f":"IF($AE$35=0,\"\",Vokabel!$A$4)","v":""}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RA-Verlängerung"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rohrbedarf bei Anschlußhöhe",null,"manuelle Nachjustierung (beim Rohr 300 oder 470)",null,null,null,null,null,null,null,null,{"$f":"ICS!$M$4","v":"ICS Matt"}]
[null,1,null,null,null,1,{"$f":"INDEX(E251:E254,F249,1)","v":0}]
[null,"LAS Zuluft-Adapter für Thermo-Luftzug Absolut",null,null,null,"Revisionstür für Thermo-Luftzug Absolut",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A-NR.",null,null,null,null,null,null,"Rohrtabelle"]
[1,{"$f":"IF($AF$35=\"Ja\",Vokabel!$A$5,\"\")","v":""},null,null,0,{"$f":"IF($AF$35=\"Ja\",Vokabel!$A$5,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Länge 205",{"$f":"$CZ$235","v":"ICS Matt 180"},{"$f":"VLOOKUP(CY251,DP252:DQ267,2,0)","v":"142002518M"},{"$f":"$CY$236","v":""},{"$f":"$DB$13","v":0},null,null,{"$f":"IF($CY$235=8,0,VLOOKUP($CZ$234,$DA$251:$DB$257,2,0))","v":0},{"$f":"IF($C$507=\"205 mm\",1,0)","v":0},{"$f":"ICS!$P$20","v":0},null,{"$f":"CZ251","v":"142002518M"},{"$f":"SUM(DE251:DG251)","v":0},null,null,null,null,null,null,"Rohr205","Rohr455","Rohr955"]
[2,{"$f":"IF(V35=\"25TL\",\"\",IF(V35=\"30L\",\"\",IF(V35=\"40L\",\"\",IF($AF$35=\"Ja\",Vokabel!$A$4,\"\"))))","v":""},null,null,1,{"$f":"IF($AF$35=\"Ja\",1,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180",{"$f":"$CZ$251","v":"142002518M"},{"$f":"$CY$237","v":""},{"$f":"$DD$13","v":1},null,"Meter",null,{"$f":"DF251*205/1000","v":0},null,null,null,null,null,null,null,null,null,{"$f":"T93","v":"ICS Matt 80"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142002508K\",IF($DP$248=\"ICS Matt\",\"142002508M\",\"142002508\"))","v":"142002508M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142005008K\",IF($DP$248=\"ICS Matt\",\"142005008M\",\"142005008\"))","v":"142005008M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142010008K\",IF($DP$248=\"ICS Matt\",\"142010008M\",\"142010008\"))","v":"142010008M"}]
[null,null,null,null,2,{"$f":"IF($AF$35=\"Ja\",2,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142002518M",{"$f":"$CY$238","v":""},{"$f":"$DF$13","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 100",{"$f":"IF($DP$248=\"ICS Kupfer\",\"142002510K\",IF($DP$248=\"ICS Matt\",\"142002510M\",\"142002510\"))","v":"142002510M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142005010K\",IF($DP$248=\"ICS Matt\",\"142005010M\",\"142005010\"))","v":"142005010M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142010010K\",IF($DP$248=\"ICS Matt\",\"142010010M\",\"142010010\"))","v":"142010010M"}]
[null,null,null,null,3,{"$f":"IF($AF$35=\"Ja\",3,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142002518M",{"$f":"$CY$239","v":""},{"$f":"$DH$13","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 130",{"$f":"IF($DP$248=\"ICS Kupfer\",\"142002513K\",IF($DP$248=\"ICS Matt\",\"142002513M\",\"142002513\"))","v":"142002513M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142005013K\",IF($DP$248=\"ICS Matt\",\"142005013M\",\"142005013\"))","v":"142005013M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142010013K\",IF($DP$248=\"ICS Matt\",\"142010013M\",\"142010013\"))","v":"142010013M"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142002518M",{"$f":"$CY$240","v":""},{"$f":"$DJ$13","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 150",{"$f":"IF($DP$248=\"ICS Kupfer\",\"142002515K\",IF($DP$248=\"ICS Matt\",\"142002515M\",\"142002515\"))","v":"142002515M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142005015K\",IF($DP$248=\"ICS Matt\",\"142005015M\",\"142005015\"))","v":"142005015M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142010015K\",IF($DP$248=\"ICS Matt\",\"142010015M\",\"142010015\"))","v":"142010015M"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142002518M",{"$f":"$CY$241","v":""},{"$f":"$DL$13","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180",{"$f":"IF($DP$248=\"ICS Kupfer\",\"142002518K\",IF($DP$248=\"ICS Matt\",\"142002518M\",\"142002518\"))","v":"142002518M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142005018K\",IF($DP$248=\"ICS Matt\",\"142005018M\",\"142005018\"))","v":"142005018M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142010018K\",IF($DP$248=\"ICS Matt\",\"142010018M\",\"142010018\"))","v":"142010018M"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142002518M",{"$f":"$CY$242","v":""},{"$f":"$DN$13","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 200",{"$f":"IF($DP$248=\"ICS Kupfer\",\"142002520K\",IF($DP$248=\"ICS Matt\",\"142002520M\",\"142002520\"))","v":"142002520M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142005020K\",IF($DP$248=\"ICS Matt\",\"142005020M\",\"142005020\"))","v":"142005020M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142010020K\",IF($DP$248=\"ICS Matt\",\"142010020M\",\"142010020\"))","v":"142010020M"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 250",{"$f":"IF($DP$248=\"ICS Kupfer\",\"142002525K\",IF($DP$248=\"ICS Matt\",\"142002525M\",\"1420025258\"))","v":"142002525M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142005025K\",IF($DP$248=\"ICS Matt\",\"142005025M\",\"1420050258\"))","v":"142005025M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142010025K\",IF($DP$248=\"ICS Matt\",\"142010025M\",\"1420100258\"))","v":"142010025M"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Länge 455",{"$f":"$CZ$235","v":"ICS Matt 180"},{"$f":"VLOOKUP(CY259,DP252:DR267,3,0)","v":"142005018M"},{"$f":"$CY$236","v":""},{"$f":"$DB$12","v":0},null,null,{"$f":"IF($CY$235=8,0,VLOOKUP($CZ$234,$DA$259:$DB$265,2,0))","v":0},{"$f":"IF($C$507=\"455 mm\",1,0)","v":0},{"$f":"ICS!$P$18","v":0},null,{"$f":"CZ259","v":"142005018M"},{"$f":"SUM(DE259:DG259)","v":0},null,null,null,null,null,"ICS Matt 300",{"$f":"IF($DP$248=\"ICS Kupfer\",\"142002530K\",IF($DP$248=\"ICS Matt\",\"142002530M\",\"142002530\"))","v":"142002530M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142005030K\",IF($DP$248=\"ICS Matt\",\"142005030M\",\"142005030\"))","v":"142005030M"},{"$f":"IF($DP$248=\"ICS Kupfer\",\"142010030K\",IF($DP$248=\"ICS Matt\",\"142010030M\",\"142010030\"))","v":"142010030M"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180",{"$f":"$CZ$259","v":"142005018M"},{"$f":"$CY$237","v":""},{"$f":"$DD$12","v":0},null,"Meter",null,{"$f":"DF259*455/1000","v":0},null,null,null,null,null,null,null,null,null,"ICS Matt 350",{"$f":"IF($DP$248=\"ICS Matt\",\"142002535M\",\"142002535\")","v":"142002535M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142005035M\",\"142005035\")","v":"142005035M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142010035M\",\"142010035\")","v":"142010035M"}]
[null,1,{"$f":"INDEX(A263:A265,B261,1)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142005018M",{"$f":"$CY$238","v":""},{"$f":"$DF$12","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 400",{"$f":"IF($DP$248=\"ICS Matt\",\"1420025404M\",\"142002540\")","v":"1420025404M"},{"$f":"IF($DP$248=\"ICS Matt\",\"1420050404M\",\"142005040\")","v":"1420050404M"},{"$f":"IF($DP$248=\"ICS Matt\",\"1420100404M\",\"142010040\")","v":"1420100404M"}]
[null,"obere Putztüre für Absolut und SIH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142005018M",{"$f":"$CY$239","v":""},{"$f":"$DH$12","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 450",{"$f":"IF($DP$248=\"ICS Matt\",\"142002545M\",\"142002545\")","v":"142002545M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142005045M\",\"142005045\")","v":"142005045M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142010045M\",\"142010045\")","v":"142010045M"}]
[0,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142005018M",{"$f":"$CY$240","v":""},{"$f":"$DJ$12","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 500",{"$f":"IF($DP$248=\"ICS Matt\",\"142002550M\",\"142002550\")","v":"142002550M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142005050M\",\"142005050\")","v":"142005050M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142010050M\",\"142010050\")","v":"142010050M"}]
[1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142005018M",{"$f":"$CY$241","v":""},{"$f":"$DL$12","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 550",{"$f":"IF($DP$248=\"ICS Matt\",\"142002555M\",\"142002555\")","v":"142002555M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142005055M\",\"142005055\")","v":"142005055M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142010055M\",\"142010055\")","v":"142010055M"}]
[2,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142005018M",{"$f":"$CY$242","v":""},{"$f":"$DN$12","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 600",{"$f":"IF($DP$248=\"ICS Matt\",\"142002560M\",\"142002560\")","v":"142002560M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142005060M\",\"142005060\")","v":"142005060M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142010060M\",\"142010060\")","v":"142010060M"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 700",{"$f":"IF($DP$248=\"ICS Matt\",\"142002570M\",\"142002570\")","v":"142002570M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142005070M\",\"142005070\")","v":"142005070M"},{"$f":"IF($DP$248=\"ICS Matt\",\"142010070M\",\"142010070\")","v":"142010070M"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Länge 955",{"$f":"$CZ$235","v":"ICS Matt 180"},{"$f":"VLOOKUP(CY267,DP252:DS267,4,0)","v":"142010018M"},{"$f":"$CY$236","v":""},{"$f":"$DB$11","v":0},null,null,{"$f":"IF($CY$235=8,0,VLOOKUP($CZ$234,$DA$267:$DB$273,2,0))","v":0},{"$f":"IF($C$507=\"955 mm\",1,0)","v":0},null,null,{"$f":"CZ267","v":"142010018M"},{"$f":"SUM(DE267:DG267)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180",{"$f":"$CZ$267","v":"142010018M"},{"$f":"$CY$237","v":""},{"$f":"$DD$11","v":0},null,"Meter",{"$f":"IF(DF267<>0,DE267*955/1000,0)","v":0},{"$f":"DF267*955/1000","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142010018M",{"$f":"$CY$238","v":""},{"$f":"$DF$11","v":0},null,"Sum.Meter",null,{"$f":"SUM(DF252,DF260,DF268)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142010018M",{"$f":"$CY$239","v":""},{"$f":"$DH$11","v":0}]
[null,1,null,null,null,1,{"$f":"INDEX(Daten!F273:F277,F271,1)","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142010018M",{"$f":"$CY$240","v":""},{"$f":"$DJ$11","v":1}]
[null,"Kragplatte",null,"Kragplatte gibt es nicht mehr",null,"Absolut Thermotrennstein für Absolut",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142010018M",{"$f":"$CY$241","v":""},{"$f":"$DL$11","v":1}]
[1,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ICS Matt 180","142010018M",{"$f":"$CY$242","v":""},{"$f":"$DN$11","v":1}]
[2,{"$f":"Vokabel!$A$4","v":"Ja"},null,null,null,{"$f":"IF($W$35=\"Nein\",\"\",1)","v":1}]
[null,null,null,null,null,{"$f":"IF($W$35=\"Nein\",\"\",2)","v":2}]
[]
[]
[]
[null,1]
[null,"Bewehrungsset",null,null,null,1,{"$f":"INDEX(Daten!F282:F284,F280,1)","v":"Nein"}]
[1,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,"Absolut Thermo-Dichtset"]
[2,"2 x 4 m",null,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[3,"4 x 4 m",null,null,null,{"$f":"IF($W$35=\"Nein\",Vokabel!$A$5,IF($E$283=\"Nein\",Vokabel!$A$5,Vokabel!$A$413))","v":"Schmalseite parallel zum First"},null,"Lüftung"]
[4,"4 x 6 m",null,null,null,{"$f":"IF($W$35=\"Nein\",Vokabel!$A$5,IF(G284=\"EZ\",Vokabel!$A$413,Vokabel!$A$414))","v":"Schmalseite parallel zum First"},{"$f":"IF($H$284=\"Ja\",Vokabel!$A$5,IF($AE$35=0,\"EZ\",Vokabel!$A$5))","v":"EZ"},{"$f":"IF($AF$35=\"Ja\",\"Ja\",\"Nein\")","v":"Nein"}]
[]
[]
[null,1]
[null,"Kaminhalter"]
[1,{"$f":"Vokabel!$A$5","v":"Nein"}]
[2,{"$f":"Vokabel!$A$19","v":"Standard"}]
[3,{"$f":"Vokabel!$A$260","v":"Verstärkt"}]
[4,{"$f":"Vokabel!$A$20","v":"Firstmittig"}]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(A299:A303,B297,1)","v":1},null,null,1,{"$f":"INDEX(E299:E303,F297,1)","v":1}]
[null,"Kaminhüte für Absolut 1.Zug",null,null,null,"Kaminhüte für Absolut  2.Zug"]
[1,{"$f":"IF($AD$35=14,\"\",Vokabel!$A$5)","v":"Nein"},null,null,1,{"$f":"IF($AE$35=\"14\",\"\",IF($AE$35=0,\"\",Vokabel!$A$5))","v":""}]
[2,{"$f":"IF($AD$35=14,\"\",Vokabel!$A$71)","v":"Basten Edelstahl"},null,null,2,{"$f":"IF($AE$35=\"14\",\"\",IF($AE$35=0,\"\",Vokabel!$A$71))","v":""}]
[3,{"$f":"IF($AD$35=14,\"\",Vokabel!$A$72)","v":"Basten Kupfer"},null,null,3,{"$f":"IF($AE$35=\"14\",\"\",IF($AE$35=0,\"\",Vokabel!$A$72))","v":""}]
[4,{"$f":"IF($AD$35=14,\"\",IF($AD$35=30,\"\",IF($AD$35=40,IF($AD$35=\"30L\",IF($AD$35=\"40L\",\"\",Vokabel!$A$73)))))","v":false},null,null,4,{"$f":"IF($AE$35=\"14\",\"\",IF($AE$35=0,\"\",IF($AE$35=0,\"\",Vokabel!$A$73)))","v":""}]
[5,{"$f":"IF($AD$35=14,\"\",IF($AD$35=30,\"\",IF($AD$35=40,IF($AD$35=\"30L\",IF($AD$35=\"40L\",\"\",Vokabel!$A$74)))))","v":false},null,null,5,{"$f":"IF($AE$35=\"14\",\"\",IF($AE$35=0,\"\",IF($AE$35=0,\"\",Vokabel!$A$74)))","v":""}]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(A310:A314,B308,1)","v":1},null,null,1,{"$f":"INDEX(E310:E314,F308,1)","v":1}]
[null,"Kaminhüte für Cheminee 1.Zug",null,null,null,"Kaminhüte für Cheminee 2.Zug"]
[1,{"$f":"IF($AE$79=14,\"\",Vokabel!$A$5)","v":"Nein"},null,null,1,{"$f":"IF($AF$79=0,\"\",Vokabel!$A$5)","v":""}]
[2,{"$f":"IF($AE$79=14,\"\",Vokabel!$A$71)","v":"Basten Edelstahl"},null,null,2,{"$f":"IF($AF$79=0,\"\",Vokabel!$A$71)","v":""}]
[3,{"$f":"IF($AE$79=14,\"\",Vokabel!$A$72)","v":"Basten Kupfer"},null,null,3,{"$f":"IF($AF$79=0,\"\",Vokabel!$A$72)","v":""}]
[4,{"$f":"IF($AE$79=14,\"\",Vokabel!$A$73)","v":"Sairlift Edelstahl"},null,null,4,{"$f":"IF($AF$79=0,\"\",Vokabel!$A$73)","v":""}]
[5,{"$f":"IF($AE$79=14,\"\",Vokabel!$A$74)","v":"Sairlift Kupfer"},null,null,5,{"$f":"IF($AF$79=0,\"\",Vokabel!$A$74)","v":""}]
[]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(A322:A323,B320,1)","v":1}]
[null,"Fertigfuß oder Montagebauweise SIH"]
[1,{"$f":"IF(AE79=30,\"\",IF(AF79=30,\"\",Vokabel!$A$69))","v":"Schnellbaufundament"}]
[2,{"$f":"IF($Z$79=\"Ja\",Vokabel!$A$70,\"\")","v":"Deckenanschlusskonus"}]
[]
[]
[]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(A333:A339,B331,1)","v":0}]
[null,"Schnellbaufundament SIH"]
[0,{"$f":"IF($AE$79=30,\"\",IF($AF$79=30,\"\",IF($B$320=2,\"\",Vokabel!$A$5)))","v":"Nein"}]
[1,{"$f":"IF($B$320=2,\"\",IF($V$79=30,\"\",IF($V$79=3030,\"\",1)))","v":1}]
[2,{"$f":"IF($B$320=2,\"\",IF($V$79=30,\"\",IF($V$79=3030,\"\",2)))","v":2}]
[3,{"$f":"IF($B$320=2,\"\",IF($V$79=30,\"\",IF($V$79=3030,\"\",3)))","v":3}]
[4,{"$f":"IF($B$320=2,\"\",IF($V$79=30,\"\",IF($V$79=3030,\"\",4)))","v":4}]
[5,{"$f":"IF($B$320=2,\"\",IF($V$79=30,\"\",IF($V$79=3030,\"\",5)))","v":5}]
[6,{"$f":"IF($B$320=2,\"\",IF($V$79=30,\"\",IF($V$79=3030,\"\",6)))","v":6}]
[]
[]
[]
[]
[null,2,{"$f":"INDEX(A346:A348,B344,1)","v":1}]
[null,"Putzanschluss Cheminee"]
[0,{"$f":"Vokabel!$A$5","v":"Nein"}]
[1,1]
[2,2]
[]
[]
[]
[]
[]
[null,2,{"$f":"INDEX(A356:A357,B354,1)","v":2}]
[null,"Abdeckplatte KWD Cheminee"]
[1,{"$f":"Vokabel!$A$5","v":"Nein"}]
[2,{"$f":"Vokabel!$A$4","v":"Ja"}]
[]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(A365:A367,B363,1)","v":0}]
[null,"Revisionstür für Thermo-Luftzug SIH"]
[0,{"$f":"IF($AG$79=\"Ja\",Vokabel!$A$5,\"\")","v":""}]
[1,{"$f":"IF($AG$79=\"Ja\",1,\"\")","v":""}]
[2,{"$f":"IF($AG$79=\"Ja\",2,\"\")","v":""}]
[null,{"$f":"IF($AG$79=\"Ja\",3,\"\")","v":""}]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(A375:A376,B373,1)","v":1}]
[null,"Schornsteinhalter für firstmittige Montage"]
[1,{"$f":"Vokabel!$A$5","v":"Nein"}]
[2,{"$f":"Vokabel!$A$4","v":"Ja"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(B392:B396,B390,1)","v":"nicht bekannt"},null,1,{"$f":"INDEX(Daten!E392:E394,E390,0)","v":"90°"}]
[null,"Brennstoffe für Kerastar",null,null,"RA Kerastar"]
[1,{"$f":"Vokabel!$A$143","v":"nicht bekannt"},null,null,"90°"]
[2,{"$f":"Vokabel!$A$144","v":"Gas"},null,null,{"$f":"IF($T$22=6,\"\",IF($T$22=7,\"\",\"45°\"))","v":"45°"}]
[3,{"$f":"Vokabel!$A$145","v":"Öl"},null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[4,{"$f":"Vokabel!$A$146","v":"Festbrennstoff"}]
[5,{"$f":"Vokabel!$A$147","v":"Holz-Pellets"}]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(B403:B405,B401,1)","v":"Bodenmontage"}]
[null,"Fußteil für Kerastar"]
[1,{"$f":"Vokabel!$A$148","v":"Bodenmontage"}]
[2,{"$f":"Vokabel!$A$149","v":"Wandmontage"}]
[3,{"$f":"IF($T$22=6,\"\",IF($T$22=7,\"\",Vokabel!$A$150))","v":"Fussteil höhenverstellbar"}]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!B412:B416,B410,1)","v":"Nein"}]
[null,"Wandhalterverlängerungen Kerastar"]
[1,{"$f":"C412","v":"Nein"},{"$f":"Vokabel!$A$5","v":"Nein"},16,18,20,25,30,40]
[2,{"$f":"IF($U$22=\"Kerastar140\",$C413,IF($U22=\"Kerastar160\",$D413,IF($U$22=\"Kerastar180\",$E413,IF($U$22=\"Kerastar200\",$F413,IF($U$22=\"Kerastar250\",$G413,IF($U$22=\"Kerastar300\",$H413,IF($U$22=\"Kerastar400\",$I413,\"\")))))))","v":"max. Abstand  220 mm"},{"$f":"Vokabel!$A$108","v":"max. Abstand  220 mm"},{"$f":"Vokabel!$A$108","v":"max. Abstand  220 mm"},{"$f":"Vokabel!$A$108","v":"max. Abstand  220 mm"},{"$f":"Vokabel!$A$108","v":"max. Abstand  220 mm"},{"$f":"Vokabel!$A$108","v":"max. Abstand  220 mm"},{"$f":"Vokabel!$A$110","v":"max. Abstand  160 mm"},{"$f":"Vokabel!$A$110","v":"max. Abstand  160 mm"}]
[3,{"$f":"IF($U$22=\"Kerastar140\",$C414,IF($U23=\"Kerastar160\",$D414,IF($U$22=\"Kerastar180\",$E414,IF($U$22=\"Kerastar200\",$F414,IF($U$22=\"Kerastar250\",$G414,IF($U$22=\"Kerastar300\",$H414,IF($U$22=\"Kerastar400\",$I414,\"\")))))))","v":"max. Abstand  370 mm"},{"$f":"Vokabel!$A$119","v":"max. Abstand  370 mm"},{"$f":"Vokabel!$A$119","v":"max. Abstand  370 mm"},{"$f":"Vokabel!$A$119","v":"max. Abstand  370 mm"},{"$f":"Vokabel!$A$119","v":"max. Abstand  370 mm"},{"$f":"Vokabel!$A$119","v":"max. Abstand  370 mm"},{"$f":"Vokabel!$A$118","v":"max. Abstand  310 mm"},{"$f":"Vokabel!$A$118","v":"max. Abstand  310 mm"}]
[4,{"$f":"IF($U$22=\"Kerastar140\",$C415,IF($U24=\"Kerastar160\",$D415,IF($U$22=\"Kerastar180\",$E415,IF($U$22=\"Kerastar200\",$F415,IF($U$22=\"Kerastar250\",$G415,IF($U$22=\"Kerastar300\",$H415,IF($U$22=\"Kerastar400\",$I415,\"\")))))))","v":"max. Abstand  470 mm"},{"$f":"Vokabel!$A$121","v":"max. Abstand  470 mm"},{"$f":"Vokabel!$A$121","v":"max. Abstand  470 mm"},{"$f":"Vokabel!$A$121","v":"max. Abstand  470 mm"},{"$f":"Vokabel!$A$121","v":"max. Abstand  470 mm"},{"$f":"Vokabel!$A$121","v":"max. Abstand  470 mm"},{"$f":"Vokabel!$A$120","v":"max. Abstand  410 mm"},{"$f":"Vokabel!$A$120","v":"max. Abstand  410 mm"}]
[5,{"$f":"IF($U$22=\"Kerastar140\",$C416,IF($U26=\"Kerastar160\",$D416,IF($U$22=\"Kerastar180\",$E416,IF($U$22=\"Kerastar200\",$F416,IF($U$22=\"Kerastar250\",$G416,IF($U$22=\"Kerastar300\",$H416,IF($U$22=\"Kerastar400\",$I416,\"\")))))))","v":"max. Abstand  670 mm"},{"$f":"Vokabel!$A$123","v":"max. Abstand  670 mm"},{"$f":"Vokabel!$A$123","v":"max. Abstand  670 mm"},{"$f":"Vokabel!$A$123","v":"max. Abstand  670 mm"},{"$f":"Vokabel!$A$123","v":"max. Abstand  670 mm"},{"$f":"Vokabel!$A$123","v":"max. Abstand  670 mm"},{"$f":"Vokabel!$A$122","v":"max. Abstand  610 mm"},{"$f":"Vokabel!$A$122","v":"max. Abstand  610 mm"}]
[]
[]
[]
[]
[]
[]
[]
[null,2,{"$f":"INDEX(A426:A428,B424,1)","v":1}]
[null,"Putzöffnungen für Kerastar"]
[0,{"$f":"Vokabel!$A$5","v":"Nein"}]
[1,1]
[2,2]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!B434:B439,B432,1)","v":"Nein"}]
[null,"Dachdurchführung"]
[1,{"$f":"Vokabel!$A$5","v":"Nein"}]
[2,"0 °"]
[3,"3 ° - 15 °"]
[4,"16 ° - 25 °"]
[5,"26 ° - 35 °"]
[6,"36 ° - 45 °"]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!$B$445:$B$446,B443,1)","v":"Nein"}]
[null,"Sparrenhalter"]
[1,{"$f":"Vokabel!$A$5","v":"Nein"}]
[2,{"$f":"Vokabel!$A$4","v":"Ja"}]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!$B$453:$B$455,B451,1)","v":"Abströmkonus"}]
[null,"Mündungslösung Kerastar"]
[1,{"$f":"Vokabel!$A$152","v":"Abströmkonus"}]
[2,{"$f":"IF($T$22=6,\"\",IF($T$22=7,\"\",Vokabel!$A$154))","v":"Basten Standard"}]
[3,{"$f":"IF($T$22=6,\"\",IF($T$22=7,\"\",Vokabel!$A$155))","v":"Basten Regulator"}]
[]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!$B$463:$B$466,B461,1)","v":"Nein"}]
[null,"RA-Verlängerung Kerastar"]
[1,{"$f":"Vokabel!$A$5","v":"Nein"}]
[2,"165 mm"]
[3,"330 mm"]
[4,"665 mm"]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!$B$473:$B$474,B471,1)","v":"Nein"}]
[null,"Regenhaube für Kerastar, Keranova"]
[1,{"$f":"Vokabel!$A$5","v":"Nein"}]
[2,{"$f":"Vokabel!$A$4","v":"Ja"}]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!$B$481:$B$482,B479,1)","v":"Nein"}]
[null,"Manschette statisch"]
[1,{"$f":"Vokabel!$A$5","v":"Nein"}]
[2,{"$f":"Vokabel!$A$4","v":"Ja"}]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,{"$f":"IF($H$490=1,\"ICS\",IF($H$490=2,\"ICS Matt\",IF($H$490=3,\"ICS Kupfer\")))","v":"ICS Matt"}]
[null,1,{"$f":"INDEX(B492:B493,B490,1)","v":"Unterdruck"},null,1,{"$f":"INDEX(E492:E496,E490,1)","v":"nicht bekannt"},null,2,{"$f":"INDEX(H493:H494,H490,1)","v":"Kupfer"}]
[null,"Ausführung Unterdruckbetrieb ICS",null,null,"Brennstoffe für ICS",null,null,"Ausführung Unterdruckbetrieb ICS"]
[null,{"$f":"Vokabel!$A$156","v":"Unterdruck"},null,1,{"$f":"IF($C$490=Vokabel!$A$157,Vokabel!$A$144,Vokabel!$A$143)","v":"nicht bekannt"},null,null,null,{"$f":"Vokabel!$A$473","v":"Glänzend"}]
[null,{"$f":"IF($V$92=405,Vokabel!$A$156,IF($V$92=455,Vokabel!$A$156,IF($V$92=505,Vokabel!$A$156,IF($V$92=555,Vokabel!$A$156,IF($V$92=605,Vokabel!$A$156,IF($V$92=655,Vokabel!$A$156,IF($V$92=705,Vokabel!$A$156,Vokabel!$A$157)))))))","v":"Überdruck"},null,2,{"$f":"Vokabel!$A$144","v":"Gas"},null,null,{"$f":"Vokabel!$A$474","v":"Matt"}]
[null,null,null,3,{"$f":"Vokabel!$A$145","v":"Öl"},null,null,{"$f":"Vokabel!$A$475","v":"Kupfer"}]
[null,null,null,4,{"$f":"IF($C$490=Vokabel!$A$157,Vokabel!$A$145,Vokabel!$A$146)","v":"Festbrennstoff"}]
[null,null,null,5,{"$f":"IF($C$490=Vokabel!$A$157,Vokabel!$A$145,Vokabel!$A$147)","v":"Holz-Pellets"}]
[]
[]
[null,1,{"$f":"INDEX(B501:B504,B499,1)","v":"Wandmontage"},1,1,{"$f":"INDEX(E501:E502,E499,1)","v":1},null,null,null,null,null,1,{"$f":"INDEX(L501:L504,L499,1)","v":"Wandmontage"},null,1,{"$f":"INDEX(O501:O502,O499,1)","v":1}]
[null,"Fußteil für ICS und ICS5000",null,null,"Putzöffnungen für ICS",null,null,{"$f":"IF($H$501=1,\"ICS5000\",IF($H$501=2,\"ICS5000\",IF($H$501=3,\"ICS5000\")))","v":"ICS5000"},null,null,null,"Fußteil für ICS5000",null,null,"Putzöffnungen für ICS5000"]
[null,{"$f":"Vokabel!$A$106","v":"Wandmontage"},null,null,1,null,null,2,{"$f":"INDEX(H503:H505,H501,1)","v":"Matt"},null,null,{"$f":"Vokabel!$A$106","v":"Wandmontage"},null,null,1]
[null,{"$f":"Vokabel!$A$105","v":"Bodenmontage"},null,null,2,null,null,"Ausführung ICS 5000",null,null,null,{"$f":"Vokabel!$A$105","v":"Bodenmontage"},null,null,2]
[null,{"$f":"Vokabel!$A$389","v":"BM mit Teleskopstütze"},null,null,null,null,null,null,{"$f":"Vokabel!$A$473","v":"Glänzend"}]
[null,{"$f":"IF(V92=80,\"\",IF(V92=100,\"\",IF(V92>250,\"\",Vokabel!$A$338)))","v":"BM mit Fussteil"},null,null,null,null,null,{"$f":"Vokabel!$A$474","v":"Matt"}]
[null,null,null,null,null,null,null,{"$f":"Vokabel!$A$475","v":"Kupfer"}]
[]
[null,1,{"$f":"INDEX(Daten!B509:B512,B507,1)","v":"Nein"},{"$f":"INDEX(Daten!C509:C512,B507,1)","v":"Nein"},1,{"$f":"INDEX(E509:E510,E507,1)","v":"Nein"},null,null,null,null,null,1,{"$f":"INDEX(Daten!L509:L512,L507,1)","v":"Nein"},null,2,{"$f":"INDEX(O509:O511,O507,1)","v":"Dichtmanschette"}]
[null,"RA-Verlängerungen ICS+25","ICSFU50",null,"Wanhalter verstellbar",null,null,null,null,null,null,"RA-Verlängerungen ICS5000",null,null,"Dichtrin/Dichtmanschette"]
[null,{"$f":"Vokabel!$A$5","v":"Nein"},{"$f":"Vokabel!$A$5","v":"Nein"},null,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,null,null,null,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,{"$f":"Vokabel!$A$485","v":"Dichtring Silikon"}]
[null,"205 mm","205 mm",null,{"$f":"Vokabel!$A$4","v":"Ja"},null,null,null,null,null,null,"205 mm",null,null,{"$f":"Vokabel!$A$486","v":"Dichtmanschette"}]
[null,"455 mm","455 mm",null,null,null,null,null,null,null,null,"455 mm",null,null,{"$f":"Vokabel!$A$485&\"+\"&Vokabel!$A$486","v":"Dichtring Silikon+Dichtmanschette"}]
[null,"955 mm","955 mm",null,null,null,null,null,null,null,null,"955 mm"]
[]
[]
[null,2,{"$f":"INDEX(Daten!B517:B519,B515,0)","v":"90°"},null,1,{"$f":"INDEX(E517:E520,E515,1)","v":"Nein"},null,null,null,null,null,2,{"$f":"INDEX(Daten!L517:L519,L515,0)","v":"90°"},null,1,{"$f":"INDEX(O517:O520,O515,1)","v":"Nein"}]
[null,"RA bei ICS ",null,null,"Abdeckblende ICS",null,null,null,null,null,null,"RA bei ICS 5000",null,null,"Abdeckblende ICS"]
[null,"45°",null,1,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,null,null,null,"45°",null,1,{"$f":"Vokabel!$A$5","v":"Nein"}]
[null,"90°",null,2,{"$f":"IF(V92>300,\"\",\"0° - 30°\")","v":"0° - 30°"},null,null,null,null,null,null,"90°",null,2,{"$f":"IF($V$230>300,\"\",\"0° - 30°\")","v":"0° - 30°"}]
[null,"85°",null,3,{"$f":"IF(V92>300,\"\",\"30° - 45°\")","v":"30° - 45°"},null,null,null,null,null,null,null,null,3,{"$f":"IF($V$230>300,\"\",\"30° - 45°\")","v":"30° - 45°"}]
[null,null,null,4,{"$f":"IF(V92>300,\"\",Vokabel!$A$332)","v":"Anschlussrosette DW"},null,null,null,null,null,null,null,null,4,{"$f":"IF($V$230>300,\"\",Vokabel!$A$332)","v":"Anschlussrosette DW"}]
[]
[null,1,{"$f":"INDEX(Daten!B524:B529,B522,1)","v":"Nein"},null,1,{"$f":"INDEX(E524:E526,E522,1)","v":"Mündungskonus"},null,null,null,null,null,1,{"$f":"INDEX(Daten!L524:L529,L522,1)","v":"Nein"},null,1,{"$f":"INDEX(O524:O526,O522,1)","v":"Mündungskonus"}]
[null,"Dachdurchführung ICS mit Wetterkragen",null,null,"Regenhaube für ICS",null,null,null,null,null,null,"Dachdurchführung ICS mit Wetterkragen",null,null,"Regenhaube für ICS"]
[null,{"$f":"Vokabel!$A$5","v":"Nein"},null,1,{"$f":"Vokabel!$A$386","v":"Mündungskonus"},null,null,null,null,null,null,{"$f":"Vokabel!$A$5","v":"Nein"},null,1,{"$f":"Vokabel!$A$386","v":"Mündungskonus"}]
[null,"0 °",null,2,{"$f":"Vokabel!$A$387","v":"Regenhaube"},null,null,null,null,null,null,"0 °",null,2,{"$f":"IF($V$230>300,\"\",Vokabel!A487)","v":"Abluftregenhut"}]
[null,{"$f":"IF($V$92>=400,\"\",\"16° - 25°\")","v":"16° - 25°"},null,3,{"$f":"IF(V92=80,\"\",IF(V92=350,\"\",IF(V92=400,\"\",IF(V92=450,\"\",IF(V92=500,\"\",IF(V92=550,\"\",IF(V92=600,\"\",IF(V92=700,\"\",Vokabel!$A$388))))))))","v":"Basten Standard"},null,null,null,null,null,null,{"$f":"IF($V$230>=400,\"\",\"16° - 25°\")","v":"16° - 25°"},null,3,{"$f":"Vokabel!A488","v":"Mündungsabschluss horizontal"}]
[null,{"$f":"IF($V$92>=400,\"\",\"26° - 35°\")","v":"26° - 35°"},null,null,null,null,null,null,null,null,null,{"$f":"IF($V$230>=400,\"\",\"26° - 35°\")","v":"26° - 35°"}]
[null,{"$f":"IF($V$92>=400,\"\",\"36° - 45°\")","v":"36° - 45°"},null,null,null,null,null,null,null,null,null,{"$f":"IF($V$230>=400,\"\",\"36° - 45°\")","v":"36° - 45°"}]
[null,null,null,null,1,{"$f":"INDEX(E531:E532,E529,1)","v":"Nein"}]
[null,null,null,null,"Manschette statisch ICS"]
[null,null,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[null,null,null,null,{"$f":"Vokabel!$A$4","v":"Ja"},null,null,null,null,null,null,null,null,null,1,{"$f":"INDEX(O534:O538,O532,1)","v":"Nein"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Winkel 15°"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($V$230>300,\"\",1)","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($V$230>300,\"\",1)","v":1}]
[null,null,"wird angepasst auf Glänzend und Matt",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($V$230>300,\"\",1)","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($V$230>300,\"\",1)","v":1}]
[null,1,{"$f":"INDEX(B541:B546,B539,1)","v":"Nein"}]
[null,"Wandkonsolen ICS Kupfer",null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"INDEX(O542:O546,O540,1)","v":"Nein"}]
[null,{"$f":"Vokabel!$A$5","v":"Nein"},"80-200",null,"250-300",null,"350 - 700",null,null,null,null,null,null,null,"Winkel 30°"]
["K1",{"$f":"IF(D542=\"W1\",C542,IF(F542=\"W2\",E542,G542))","v":"max. Abstand  100 mm"},{"$f":"IF($B$499=1,Vokabel!$A$394,\"\")","v":"max. Abstand  100 mm"},{"$f":"IF($V$92=80,\"W1\",IF($V$92<250,\"W1\",0))","v":"W1"},{"$f":"IF($B$499=1,Vokabel!$A$340,\"\")","v":"max. Abstand  114 mm"},{"$f":"IF($V$92<350,\"W2\",0)","v":"W2"},{"$f":"IF($B$499=1,Vokabel!$A$341,\"\")","v":"max. Abstand  122 mm"},"L1",null,null,null,null,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
["K2",{"$f":"IF(D543=\"L1\",C543,IF(F543=\"L1\",E543,G543))","v":"max. Abstand  250 mm"},{"$f":"IF($B$499=1,Vokabel!$A$344,\"\")","v":"max. Abstand  250 mm"},{"$f":"IF($V$92=80,\"L1\",IF($V$92<250,\"L1\",0))","v":"L1"},{"$f":"IF($B$499=1,Vokabel!$A$343,\"\")","v":"max. Abstand  220 mm"},{"$f":"IF($V$92<350,\"L1\",0)","v":"L1"},{"$f":"IF($B$499=1,Vokabel!$A$339,\"\")","v":"max. Abstand  75 - 300 mm"},"75-300",null,null,null,null,null,null,1]
["K3",{"$f":"IF(D544=\"L2\",C544,IF(F544=\"L2\",E544,\"\"))","v":"max. Abstand  440 mm"},{"$f":"IF($B$499=1,Vokabel!$A$355,\"\")","v":"max. Abstand  440 mm"},{"$f":"IF($V$92=80,\"L2\",IF($V$92<250,\"L2\",0))","v":"L2"},{"$f":"IF($B$499=1,Vokabel!$A$351,\"\")","v":"max. Abstand  370 mm"},{"$f":"IF($V$92<350,\"L2\",0)","v":"L2"},null,null,null,null,null,null,null,null,2]
["K4",{"$f":"IF(D545=\"L3\",C545,IF(F545=\"L3\",E545,\"\"))","v":"max. Abstand  500 mm"},{"$f":"IF($B$499=1,Vokabel!$A$357,\"\")","v":"max. Abstand  500 mm"},{"$f":"IF($V$92=80,\"L3\",IF($V$92<250,\"L3\",0))","v":"L3"},{"$f":"IF($B$499=1,Vokabel!$A$356,\"\")","v":"max. Abstand  470 mm"},{"$f":"IF($V$92<350,\"L3\",0)","v":"L3"},null,null,null,null,null,null,null,null,3]
["K5",{"$f":"IF(D546=\"L4\",C546,IF(F546=\"L4\",E546,\"\"))","v":"max. Abstand  700 mm"},{"$f":"IF($B$499=1,Vokabel!$A$363,\"\")","v":"max. Abstand  700 mm"},{"$f":"IF($V$92=80,\"L4\",IF($V$92<250,\"L4\",0))","v":"L4"},{"$f":"IF($B$499=1,Vokabel!$A$361,\"\")","v":"max. Abstand  670 mm"},{"$f":"IF($V$92<350,\"L4\",0)","v":"L4"},null,null,null,null,null,null,null,null,4]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"INDEX(O550:O554,O548,1)","v":"Nein"}]
[null,1,{"$f":"INDEX(Daten!B551:B555,B549,1)","v":"Nein"},null,null,null,null,null,null,null,null,1,{"$f":"INDEX(Daten!L551:L555,L549,1)","v":"Nein"},null,"Winkel 45°"]
[null,"Wandhalterverlängerungen ICS",null,null,null,null,null,null,null,null,null,"Wandhalterverlängerungen ICS",null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[null,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,1]
[null,{"$f":"IF(V92>300,\"\",Vokabel!$A$394)","v":"max. Abstand  100 mm"},null,null,null,null,null,null,null,null,null,{"$f":"IF(AF92>300,\"\",Vokabel!$A$394)","v":"max. Abstand  100 mm"},null,null,2]
[null,{"$f":"IF(V92>300,\"\",Vokabel!$A$395)","v":"max. Abstand  250 mm"},null,null,null,null,null,null,null,null,null,{"$f":"IF(AF92>300,\"\",Vokabel!$A$395)","v":"max. Abstand  250 mm"},null,null,3]
[null,{"$f":"IF(V92>300,\"\",Vokabel!$A$396)","v":"max. Abstand  400 mm"},null,null,null,null,null,null,null,null,null,{"$f":"IF(AF92>300,\"\",Vokabel!$A$396)","v":"max. Abstand  400 mm"},null,null,4]
[null,{"$f":"IF(V92>300,\"\",IF($V$92=700,Vokabel!$A$397,Vokabel!$A$398))","v":"max. Abstand  600 mm"},null,null,null,null,null,null,null,null,null,{"$f":"IF(AF92>300,\"\",IF($V$92=700,Vokabel!$A$397,Vokabel!$A$398))","v":"max. Abstand  600 mm"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"INDEX(O558:O562,O556,1)","v":"Nein"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Winkel 90°"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,4]
[]
[null,1,{"$f":"INDEX(Daten!B566:B568,B564,1)","v":"Unterdruck"}]
[null,"Ausführung Unterdruckbetrieb für Keranova:"]
[1,{"$f":"Vokabel!$A$156","v":"Unterdruck"}]
[2,{"$f":"Vokabel!$A$157","v":"Überdruck"}]
[]
[]
[]
[]
[]
[null,3,{"$f":"INDEX(Daten!B575:B577,B573,1)","v":2}]
[null,"Putzöffnungen für Keranova"]
[0,{"$f":"Vokabel!$A$5","v":"Nein"}]
[1,1]
[2,2]
[]
[]
[]
[]
[null,3,{"$f":"INDEX(Daten!B584:B587,B582,1)","v":"Festbrennstoff"}]
[null,"Brennstoffe für Keranova:"]
[1,{"$f":"Vokabel!$A$144","v":"Gas"}]
[2,{"$f":"Vokabel!$A$145","v":"Öl"}]
[3,{"$f":"Vokabel!$A$146","v":"Festbrennstoff"}]
[4,{"$f":"Vokabel!$A$147","v":"Holz-Pellets"}]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!B593:B594,B591,1)","v":"90°"}]
[null,"1. Rauchrohranschl. Grad Keranova"]
[1,"90°"]
[2,"45°"]
[]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(B602:B604,B600,1)","v":"Nein"}]
[null,"Doppelwandfutter bei Keranova"]
[1,{"$f":"Vokabel!$A$5","v":"Nein"}]
[2,{"$f":"IF($U$117=\"Keranova120\",$C$603,IF($U$117=\"Keranova140\",$D$603,IF($U$117=\"Keranova160\",$E$603,IF($U$117=\"Keranova180\",$F$603,IF($U$117=\"Keranova200\",$G$603,IF($U$117=\"Keranova250\",$H$603,\"\"))))))","v":"Doppelwandfutter Ø 150"},{"$f":"Vokabel!$A$158","v":"Doppelwandfutter Ø 120"},{"$f":"Vokabel!$A$159","v":"Doppelwandfutter Ø 130"},{"$f":"Vokabel!$A$160","v":"Doppelwandfutter Ø 150"},{"$f":"Vokabel!$A$161","v":"Doppelwandfutter Ø 180"},{"$f":"Vokabel!$A$162","v":"Doppelwandfutter Ø 200"},{"$f":"Vokabel!$A$163","v":"Doppelwandfutter Ø 250"}]
[3,{"$f":"IF($U$117=\"Keranova120\",$C$604,IF($U$117=\"Keranova140\",$D$604,IF($U$117=\"Keranova160\",$E$604,IF($U$117=\"Keranova180\",$D$604,IF($U$117=\"Keranova200\",$E$604,\"\")))))","v":"Doppelwandfutter Ø 180"},{"$f":"Vokabel!$A$159","v":"Doppelwandfutter Ø 130"},{"$f":"Vokabel!$A$160","v":"Doppelwandfutter Ø 150"},{"$f":"Vokabel!$A$161","v":"Doppelwandfutter Ø 180"}]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!$B$611:$B$613,B609,1)","v":"Nein"}]
[null,"Putztüren für Keranova"]
[0,{"$f":"Vokabel!$A$5","v":"Nein"}]
[1,1]
[2,2]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!B620:B624,B618,1)","v":"Nein"}]
[null,"Kaminhüte Keranova"]
[1,{"$f":"IF($U$117=\"Keranova120\",\"\",IF($U$117=\"Keranova140\",\"\",Vokabel!$A$5))","v":"Nein"}]
[2,{"$f":"IF($U$117=\"Keranova120\",\"\",IF($U$117=\"Keranova140\",\"\",Vokabel!$A$71))","v":"Basten Edelstahl"}]
[3,{"$f":"IF($U$117=\"Keranova120\",\"\",IF($U$117=\"Keranova140\",\"\",Vokabel!$A$72))","v":"Basten Kupfer"}]
[4,{"$f":"IF($U$117=\"Keranova120\",\"\",IF($U$117=\"Keranova140\",\"\",Vokabel!$A$73))","v":"Sairlift Edelstahl"}]
[5,{"$f":"IF($U$117=\"Keranova120\",\"\",IF($U$117=\"Keranova140\",\"\",Vokabel!$A$74))","v":"Sairlift Kupfer"}]
[]
[]
[]
[]
[null,2,{"$f":"INDEX(Daten!B631:B632,B629,1)","v":""}]
[null,"Abschlussplatte für Basten",null,"gelöscht tel. Benjamin 19.1.09"]
[1,{"$f":"IF($U$117=\"Keranova120\",\"\",IF($U$117=\"Keranova140\",\"\",IF($B$618=1,\"\",Vokabel!$A$5)))","v":""}]
[2,{"$f":"IF($U$117=\"Keranova120\",\"\",IF($U$117=\"Keranova140\",\"\",IF($B$618=1,\"\",Vokabel!$A$4)))","v":""}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!B646:B648,B644,1)","v":"Unterdruck"},null,4,{"$f":"INDEX(E646:E650,E644,1)","v":"Festbrennstoff"}]
[null,"Ausführung Unterdruckbetrieb für Prima u. Technost.",null,null,"Brennstoffe:"]
[null,{"$f":"Vokabel!$A$156","v":"Unterdruck"},null,1,{"$f":"IF($B$644=2,Vokabel!$A$144,Vokabel!$A$143)","v":"nicht bekannt"}]
[null,{"$f":"Vokabel!$A$157","v":"Überdruck"},null,2,{"$f":"Vokabel!$A$144","v":"Gas"}]
[null,null,null,3,{"$f":"F648","v":"Öl"},{"$f":"IF($V$139=405,Vokabel!$A$144,IF($V$139=455,Vokabel!$A$144,IF($V$139=505,Vokabel!$A$144,IF($V$139=555,Vokabel!$A$144,IF($V$139=605,Vokabel!$A$144,IF($V$139=655,Vokabel!$A$144,IF($V$139=705,Vokabel!$A$144,Vokabel!$A$145)))))))","v":"Öl"}]
[null,null,null,4,{"$f":"IF($B$644=2,$F$649,Vokabel!$A$146)","v":"Festbrennstoff"},{"$f":"IF($V$139=405,Vokabel!$A$144,IF($V$139=455,Vokabel!$A$144,IF($V$139=505,Vokabel!$A$144,IF($V$139=555,Vokabel!$A$144,IF($V$139=605,Vokabel!$A$144,IF($V$139=655,Vokabel!$A$144,IF($V$139=705,Vokabel!$A$144,Vokabel!$A$145)))))))","v":"Öl"}]
[null,null,null,5,{"$f":"IF($B$644=2,$F$650,Vokabel!$A$147)","v":"Holz-Pellets"},{"$f":"IF($V$139=405,Vokabel!$A$144,IF($V$139=455,Vokabel!$A$144,IF($V$139=505,Vokabel!$A$144,IF($V$139=555,Vokabel!$A$144,IF($V$139=605,Vokabel!$A$144,IF($V$139=655,Vokabel!$A$144,IF($V$139=705,Vokabel!$A$144,Vokabel!$A$145)))))))","v":"Öl"}]
[]
[]
[]
[null,1,{"$f":"INDEX(Daten!$B$656:$B$657,B654,1)","v":1}]
[null,"Putzöffnungen für Prima Plus"]
[null,1]
[null,2]
[]
[]
[]
[]
[null,2,{"$f":"INDEX(Daten!B664:B668,B662,1)","v":"T-Stück 90°"}]
[null,"Prima Plus"]
[null,{"$f":"IF($V$139=80,\"\",IF($V$139=100,\"\",IF($V$139>=355,\"\",Vokabel!$A$367)))","v":"Basiselement für RA"}]
[null,{"$f":"Vokabel!$A$369","v":"T-Stück 90°"}]
[null,{"$f":"Vokabel!$A$368","v":"T-Stück 45°"}]
[null,{"$f":"IF(V139>300,\"\",Vokabel!$A$373)","v":"Bogen 45° mit Stützfuss"}]
[]
[]
[null,1,{"$f":"INDEX(B672:B674,B670,1)","v":"Nein"}]
[null,"Putztüren "]
[null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[null,1]
[null,2]
[]
[]
[null,1,{"$f":"INDEX(Daten!B679:B680,B677,1)","v":"Nein"},null,1,{"$f":"INDEX(Daten!E679:E680,E677,1)","v":"Mündungskonus"}]
[null,"Regenhaube für PrimaPlus",null,null,"Regenhaube für PrimaPlus"]
[null,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,{"$f":"Vokabel!$A$386","v":"Mündungskonus"}]
[null,{"$f":"Vokabel!$A$4","v":"Ja"},null,null,{"$f":"Vokabel!$A$390","v":"Dehnfugenmanschette"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,3,{"$f":"INDEX(B699:B701,B697,1)","v":"Nein"}]
[null,"Putztür bei Technostar",null,null,null,2,{"$f":"INDEX(F700:F701,F698,1)","v":"Nein"}]
[null,{"$f":"Vokabel!$A$415","v":"Schachttüre grundiert"},null,null,null,"Kondensatablauf für Technostar"]
[null,{"$f":"Vokabel!$A$416","v":"Schachttüre gasdicht"},null,null,null,{"$f":"Vokabel!$A$4","v":"Ja"}]
[null,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[]
[]
[null,2,{"$f":"INDEX(B706:B707,B704,1)","v":"Nein"}]
[null,"Kaminabstützung",null,null,null,3,{"$f":"INDEX(Daten!F707:F709,F705,1)","v":"Öl"}]
[null,{"$f":"Vokabel!$A$4","v":"Ja"},null,null,null,"Brennstoffe für Technostar"]
[null,{"$f":"Vokabel!$A$5","v":"Nein"},null,null,null,{"$f":"Vokabel!$A$143","v":"nicht bekannt"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$144","v":"Gas"}]
[null,null,null,null,null,{"$f":"Vokabel!$A$145","v":"Öl"}]
[]
[]
[null,1,{"$f":"INDEX(B714:B717,B712,1)","v":"Endmuffe"}]
[null,"Mündungslösung Technostar",null,null,null,1,{"$f":"INDEX(Daten!$F$715:$F$716,F713,1)","v":"Mündungskonus"}]
[null,{"$f":"Vokabel!$A$417","v":"Endmuffe"},null,null,null,"Mündungslösung Edelstahl"]
[null,{"$f":"Vokabel!$A$418","v":"Schachtabdeckung PE"},null,null,null,{"$f":"Vokabel!$A$386","v":"Mündungskonus"}]
[null,{"$f":"Vokabel!$A$419","v":"Schachtabdeckung CNS"},null,null,null,{"$f":"Vokabel!$A$390","v":"Dehnfugenmanschette"}]
[null,{"$f":"Vokabel!$A$420","v":"Schachtabdeckung CNS Flex"}]
[]
[]
[]
[null,2,{"$f":"INDEX(Daten!B723:B725,B721,1)","v":"Überdruck"}]
[null,"Ausführung Unterdruckbetrieb für Technostar"]
[null,{"$f":"Vokabel!$A$156","v":"Unterdruck"}]
[null,{"$f":"Vokabel!$A$157","v":"Überdruck"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[20,{"$f":"INDEX(A743:A807,A741,1)","v":8.75},null,2,{"$f":"INDEX(D743:D744,D741,1)","v":"Ja"}]
["Anlagenhöhe",null,null,"Cheminee-Anfänger"]
[4,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[4.25,null,null,{"$f":"Vokabel!$A$4","v":"Ja"}]
[4.5]
[4.75]
[5]
[5.25,null,null,2,{"$f":"INDEX(D750:D752,D748,1)","v":1}]
[5.5,null,null,"Gasdichte Russtüre"]
[5.75,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[6,null,null,1]
[6.25,null,null,2]
[6.5]
[6.75]
[7]
[7.25,null,null,2,{"$f":"INDEX(D758:D760,D756,1)","v":1}]
[7.5,null,null,"Rauchrohranschlusselement"]
[7.75,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[8,null,null,1]
[8.25,null,null,2]
[8.5]
[8.75]
[9]
[9.25,null,null,2,{"$f":"INDEX(D766:D767,D764,1)","v":"Ja"}]
[9.5,null,null,2]
[9.75,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[10,null,null,{"$f":"Vokabel!$A$4","v":"Ja"}]
[10.25]
[10.5]
[10.75]
[11]
[11.25,null,null,1,{"$f":"INDEX(D774:D776,D772,1)","v":"Nein"}]
[11.5,null,null,"Kaminschleifung"]
[11.75,null,null,{"$f":"Vokabel!$A$5","v":"Nein"}]
[12,null,null,1]
[12.25,null,null,2]
[12.5]
[12.75]
[13]
[13.25]
[13.5,null,null,1,{"$f":"INDEX(C783:C787,D781,1)","v":1}]
[13.75,null,null,"Kaminhüte für Cheminee 1.Zug"]
[14,null,1,{"$f":"IF($AE$79=14,\"\",Vokabel!$A$5)","v":"Nein"}]
[14.25,null,2,{"$f":"IF($AE$79=14,\"\",Vokabel!$A$71)","v":"Basten Edelstahl"}]
[14.5,null,3,{"$f":"IF($AE$79=14,\"\",Vokabel!$A$72)","v":"Basten Kupfer"}]
[14.75,null,4,{"$f":"IF($AE$79=14,\"\",Vokabel!$A$73)","v":"Sairlift Edelstahl"}]
[15,null,5,{"$f":"IF($AE$79=14,\"\",Vokabel!$A$74)","v":"Sairlift Kupfer"}]
[15.25]
[15.5]
[15.75]
[16]
[16.25]
[16.5]
[16.75]
[17]
[17.25]
[17.5]
[17.75]
[18]
[18.25]
[18.5]
[18.75]
[19]
[19.25]
[19.5]
[19.75]
[20]

{"sheet":"Sortimente","index":29,"n_rows":7383,"n_cols":20,"rows_kept":4500,"cut":true,"hidden":true,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[null,null,null,{"$f":"A1&C1&B1","v":""},null,{"$f":"VLOOKUP(G1,sanschie!A:E,5,0)","v":{"$error":"#N/A"}},null,{"$f":"IF(VLOOKUP(G1,sanschie!B:J,9,)=0,\"0\",VLOOKUP(G1,sanschie!B:J,9,0))","v":{"$error":"#N/A"}},null,{"$f":"VLOOKUP(G1,sanschie!B:D,3,0)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(G1,sanschie!A:G,7,0)","v":{"$error":"#N/A"}}]
[]
["System","Pos.","DM","Verkn.","NR.","Artikelbezeichnung","Artikelnummer","Baulänge in mm","Anlagenhöhe","EH","Einzelpreis","Menge für ca 10m","Ber-Feld",null,"ger.Höhe","Höhen "]
["Kerastar",0,140,{"$f":"A4&C4&B4","v":"Kerastar1400"},"P","Kerastar Anlage Ø 140","Kerastar 140","0",{"$f":"Kerastar!$J$8","v":10},"Anlage",0,1,{"$f":"I4*1000","v":10000},null,{"$f":"ROUNDUP(P4,2)","v":10.18},{"$f":"SUM(P5:P47)/1000","v":10.178000000000001}]
["Kerastar",{"$f":"B4+1","v":1},{"$f":"C4","v":140},"Kerastar1401","1a","KRS 140 Fussteil Bodenmontage mit Ablauf L350mm","103245",330,null,"STK",240,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L5=\"\",0,L5*H5)","v":330},null,null,{"$f":"IF(L5=\"\",0,H5*L5)","v":330}]
["Kerastar",2,140,"Kerastar1402","1a","KRS Fusssteher-Set 4Stk. verstellbar L325-540mm","103252","0",null,"STK",422,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L6=\"\",0,L6*H6)","v":0}]
["Kerastar",3,140,"Kerastar1403","1c","KRS 140 Fussteil für Wohnraum verstelb. L186-286mm","103253",186,null,"STK",162,{"$f":"IF(Daten!$B$401=3,1,\"\")","v":""},{"$f":"IF(L7=\"\",0,L7*H7)","v":0},null,null,{"$f":"IF(L7=\"\",0,H7*L7)","v":0}]
["Kerastar",4,140,"Kerastar1404","2a","KRS 140 Grundplatte verstärkt mit Ablauf","103258",44,null,"STK",149,{"$f":"N8","v":""},null,{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""},{"$f":"IF(Daten!$B$410=1,\"\",1)","v":""}]
["Kerastar",5,140,"Kerastar1405","2b","KRS 140 Grundplatte mit Russtopf","103265",44,null,"STK",223]
["Kerastar",6,140,{"$f":"A10&C10&B10","v":"Kerastar1406"},"2b","KRS 140 Deckenanschluss-Element","140849",376,null,"STK",383]
["Kerastar",7,140,"Kerastar1407","2b","KRS 140 Ofenaufsatz-Element","140854",340,null,"STK",141]
["Kerastar",8,140,"Kerastar1408","2c","KRS Wand-Konsole Typ 475mm (Paar)","103379","0",null,"STK",138,{"$f":"N12","v":""},null,{"$f":"IF(Daten!$B$410=1,O12,\"\")","v":""},{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""}]
["Kerastar",9,140,"Kerastar1409","2c","KRS Wand-Konsole Typ 570mm (Paar)","103380","0",null,"STK",144,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$BC$401=3,\"\",IF(Daten!$B$410=2,1,\"\")))","v":""},null,278]
["Kerastar",10,140,"Kerastar14010","2c","KRS Wand-Konsole Typ 720mm (Paar)","103381","0",null,"STK",151,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=3,1,\"\")))","v":""},null,428]
["Kerastar",11,140,"Kerastar14011","2c","KRS Wand-Konsole Typ 820mm (Paar)","103382","0",null,"STK",164,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=4,1,\"\")))","v":""},null,528]
["Kerastar",{"$f":"B15+1","v":12},{"$f":"C15","v":140},{"$f":"A16&C16&B16","v":"Kerastar14012"},"2c","KRS Wand-Konsole Typ 1004mm (Paar)","103383","0",null,"STK",222,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=5,1,\"\")))","v":""},null,712]
["Kerastar",13,140,"Kerastar14013","2d","KRS 140 Konsolenbleche (Paar)","103387","0",null,"STK",54]
["Kerastar",14,140,"Kerastar14014",3,"KRS 140  Revisionselement trocken- Betrieb L665mm","103270",665,null,"STK",333,{"$f":"IF(N18=0,\"\",N18)","v":1},{"$f":"IF(N18=\"\",0,N18*H18)","v":665},{"$f":"Daten!$C$424","v":1},null,{"$f":"H18*N18","v":665}]
["Kerastar",15,140,"Kerastar14015","4a","KRS 140  T-Stück 90 ° L665mm ","103284",665,null,"STK",264,{"$f":"IF(N19=0,\"\",IF(Daten!$F$390=\"90°\",N19,\"\"))","v":1},{"$f":"IF(L19=\"\",0,L19*H19)","v":665},{"$f":"Daten!$C$193","v":1},null,{"$f":"IF(L19=\"\",0,H19*L19)","v":665}]
["Kerastar",16,140,"Kerastar14016","4b","KRS 140  Anschlussrosette zu T-Stk. Øi 145mm ","103291","0",null,"STK",44,{"$f":"IF(N19=0,\"\",N19)","v":1}]
["Kerastar",17,140,"Kerastar14017","4c","KRS 140  T-Stück 45 ° L665mm ","103298",665,null,"STK",339,{"$f":"IF(N19=0,\"\",IF(Daten!$F$390=\"45°\",N19,\"\"))","v":""},{"$f":"IF(L21=\"\",0,L21*H21)","v":0},null,null,{"$f":"IF(L21=\"\",0,H21*L21)","v":0}]
["Kerastar",18,140,"Kerastar14018","4d","KRS 140  Winkel 15 ° ","103331","0",null,"STK",159]
["Kerastar",{"$f":"B22+1","v":19},{"$f":"C22","v":140},{"$f":"A23&C23&B23","v":"Kerastar14019"},"4e","KRS 140  Winkel 30 ° ","103338","0",null,"STK",173]
["Kerastar",20,140,"Kerastar14020","4f","KRS 140  Winkel 45 ° ","103345","0",null,"STK",173,null,null,"Stk RA-VL","RA-Verl."]
["Kerastar",21,140,"Kerastar14021","5a","KRS 140  Längenelement L665mm ","103303",665,null,"STK",131,{"$f":"ROUNDUP(M25,0)+N25","v":12},{"$f":"((M4-M5-M7-M18-M19-M21-M26-M27-M37+O26+O27)/H25)","v":11.732330827067669},{"$f":"O25/H25","v":0},{"$f":"Daten!$BY$161*1000","v":0},{"$f":"(IF(L25=\"\",0,H25*L25))-O25","v":7980}]
["Kerastar",22,140,"Kerastar14022","5b","KRS 140  Längenelement L330mm ","103310",331,null,"STK",95,{"$f":"IF(Daten!$CC$151=0,\"\",Daten!$CC$151)","v":1},{"$f":"IF(L26=\"\",0,L26*H26)","v":331},{"$f":"O26/H26","v":0},{"$f":"Daten!$BY$152*1000","v":0},{"$f":"(IF(L26=\"\",0,H26*L26))-O26","v":331}]
["Kerastar",23,140,"Kerastar14023","5c","KRS 140  Längenelement L165mm ","103317",165,null,"STK",63,{"$f":"IF(Daten!$CC$142=0,\"\",Daten!$CC$142)","v":""},{"$f":"IF(L27=\"\",0,L27*H27)","v":0},{"$f":"O27/H27","v":0},{"$f":"Daten!$BY$143*1000","v":0},{"$f":"(IF(L27=\"\",0,H27*L27))-O27","v":0}]
["Kerastar",24,140,"Kerastar14024","5d","ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",12,{"$f":"ROUNDUP(M28,0)","v":2},{"$f":"((M4/1000)*44)/310","v":1.4193548387096775}]
["Kerastar",25,140,"Kerastar14025","6a","KRS 140  Wandhalter 50 Light ","103421","0",null,"STK",41]
["Kerastar",26,140,"Kerastar14026","6b","KRS 140  Wandhalterung 50mm ","103426","0",null,"STK",28,{"$f":"ROUNDUP(M30,0)-N31","v":3},{"$f":"((M4/1000)/4.3)","v":2.3255813953488373}]
["Kerastar",27,140,"Kerastar14027","6d","KRS 140 Wandhalt.statisch 50mm","103403","0",null,"STK",69,{"$f":"IF(N31=0,\"\",N31)","v":""},null,{"$f":"IF(Daten!$A$479=2,1,0)","v":0}]
["Kerastar",28,140,"Kerastar14028","6c","ICS L1 Verlängerung zu Wandhalter 50mm L300mm","101254","0",null,"STK",66,{"$f":"IF(Daten!$B$410=2,L30+N31,\"\")","v":""},null,220]
["Kerastar",29,140,"Kerastar14029","6c","ICS L2 Verlängerung zu Wandhalter 50mm L450mm","101255","0",null,"STK",83,{"$f":"IF(Daten!$B$410=3,L30+N31,\"\")","v":""},null,370]
["Kerastar",30,140,"Kerastar14030","6c","ICS L3 Verlängerung zu Wandhalter 50mm L550mm","101256","0",null,"STK",95,{"$f":"IF(Daten!$B$410=4,L30+N31,\"\")","v":""},null,470]
["Kerastar",31,140,"Kerastar14031","6c","ICS L4 Verlängerung zu Wandhalter 50mm L750mm","101257","0",null,"STK",101,{"$f":"IF(Daten!$B$410=5,L30+N31,\"\")","v":""},null,670]
["Kerastar",32,140,"Kerastar14032",7,"KRS 140 Sparrenhalter ","103414","0",null,"STK",69,{"$f":"IF(Daten!$B$443=1,\"\",\"1\")","v":""}]
["Kerastar",33,140,"Kerastar14033","8a","KRS 140  Mündungsabschluss L207mm","103324",207,null,"STK",79,{"$f":"IF(Daten!$B$451=1,1,\"\")","v":1},{"$f":"IF(L37=\"\",0,L37*H37)","v":207},null,null,{"$f":"IF(L37=\"\",0,H37*L37)","v":207}]
["Kerastar",34,140,"Kerastar14034",null,"KRS 140 Basten Standard mit Stulpring Inox","103432","0",null,"STK",328,{"$f":"IF(Daten!$B$451=2,1,\"\")","v":""}]
["Kerastar",35,140,"Kerastar14035",null,"KRS 140 Basten Regulator mit Stulpring Inox","103438","0",null,"STK",428,{"$f":"IF(Daten!$B$451=3,1,\"\")","v":""}]
["Kerastar",36,140,"Kerastar14036","9a",{"$f":"VLOOKUP(G40,sanschie!A:E,5,0)","v":"ICM 250-300 Dachdurführung 0° DN370 L500mm"},"102327","0",null,"STK",147,{"$f":"IF(Daten!$C$432=\"0 °\",1,\"\")","v":""}]
["Kerastar",37,140,"Kerastar14037","9c",{"$f":"VLOOKUP(G41,sanschie!A:E,5,0)","v":"ICM 200 Dachdurführung 16-25° DN320 mit Bleilappen"},"102338","0",null,"STK",284,{"$f":"IF(Daten!$C$432=\"16 ° - 25 °\",1,\"\")","v":""}]
["Kerastar",38,140,"Kerastar14038","9d",{"$f":"VLOOKUP(G42,sanschie!A:E,5,0)","v":"ICM 200 Dachdurführung 26-35° DN320 mit Bleilappen"},"102350","0",null,"STK",284,{"$f":"IF(Daten!$C$432=\"26 ° - 35 °\",1,\"\")","v":""}]
["Kerastar",39,140,"Kerastar14039","9e",{"$f":"VLOOKUP(G43,sanschie!A:E,5,0)","v":"ICM 200 Dachdurführung 36-45° DN320 mit Bleilappen"},"102362","0",null,"STK",358,{"$f":"IF(Daten!$C$432=\"36 ° - 45 °\",1,\"\")","v":""}]
["Kerastar",40,140,"Kerastar14040",10,"KRS Regenkragen        14","104661","0",null,"STK",48,{"$f":"IF(SUM(L40:L43)=1,1,\"\")","v":""}]
["Kerastar",41,140,{"$f":"A45&C45&B45","v":"Kerastar14041"},"11a","KRS 140 Anschlussrosette Øi 272mm ØA 442mm","103352","0",null,"STK",24]
["Kerastar",42,140,"Kerastar14042",12,"KRS 140 Abdeckros.16-21° Dachneigung ","103359","0",null,"STK",24]
["Kerastar",43,140,"Kerastar14043",13,"KRS 140 Seilabspannring","103391","0",null,"STK",19]
["Kerastar",44,140,"Kerastar14044","14a","KRS 140 Statisches Klemmband","103396","0",null,"STK",19,{"$f":"IF(Daten!$B$479=2,2,\"\")","v":""}]
["Kerastar",0,160,"Kerastar1600","P","Kerastar Anlage Ø 160","Kerastar 160","0",{"$f":"Kerastar!$J$8","v":10},"Anlage",0,1,{"$f":"I49*1000","v":10000},null,{"$f":"ROUNDUP(P49,2)","v":10.18},{"$f":"SUM(P50:P92)/1000","v":10.178000000000001}]
["Kerastar",{"$f":"B49+1","v":1},{"$f":"C49","v":160},"Kerastar1601","1a","KRS 160 Fussteil Bodenmontage mit Ablauf L350mm","103246",330,null,"STK",212,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L50=\"\",0,L50*H50)","v":330},null,null,{"$f":"IF(L50=\"\",0,H50*L50)","v":330}]
["Kerastar",{"$f":"B50+1","v":2},{"$f":"C50","v":160},"Kerastar1602","1a","KRS Fusssteher-Set 4Stk. verstellbar L325-540mm","103252","0",null,"STK",422,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L51=\"\",0,L51*H51)","v":0}]
["Kerastar",{"$f":"B51+1","v":3},{"$f":"C51","v":160},"Kerastar1603","1c","KRS 160 Fussteil für Wohnraum verstelb. L186-286mm","103254",186,null,"STK",181,{"$f":"IF(Daten!$B$401=3,1,\"\")","v":""},{"$f":"IF(L52=\"\",0,L52*H52)","v":0},null,null,{"$f":"IF(L52=\"\",0,H52*L52)","v":0}]
["Kerastar",4,160,"Kerastar1604","2a","KRS 160 Grundplatte verstärkt mit Ablauf","103259",44,null,"STK",159,{"$f":"N53","v":""},null,{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""},{"$f":"IF(Daten!$B$410=1,\"\",1)","v":""}]
["Kerastar",5,160,"Kerastar1605","2b","KRS 160 Grundplatte mit Russtopf","103266",44,null,"STK",226]
["Kerastar",6,160,{"$f":"A55&C55&B55","v":"Kerastar1606"},"2b","KRS 160 Deckenanschluss-Element","140850",376,null,"STK",405]
["Kerastar",7,160,"Kerastar1607","2b","KRS 160 Ofenaufsatz-Element","140855",340,null,"STK",147]
["Kerastar",8,160,"Kerastar1608","2c","KRS Wand-Konsole Typ 475mm (Paar)","103379","0",null,"STK",138,{"$f":"N57","v":""},null,{"$f":"IF(Daten!$B$410=1,O57,\"\")","v":""},{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""}]
["Kerastar",9,160,"Kerastar1609","2c","KRS Wand-Konsole Typ 570mm (Paar)","103380","0",null,"STK",144,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$BC$401=3,\"\",IF(Daten!$B$410=2,1,\"\")))","v":""},null,278]
["Kerastar",10,160,"Kerastar16010","2c","KRS Wand-Konsole Typ 720mm (Paar)","103381","0",null,"STK",151,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=3,1,\"\")))","v":""},null,428]
["Kerastar",11,160,"Kerastar16011","2c","KRS Wand-Konsole Typ 820mm (Paar)","103382","0",null,"STK",164,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=4,1,\"\")))","v":""},null,528]
["Kerastar",12,160,"Kerastar16012","2c","KRS Wand-Konsole Typ 1004mm (Paar)","103383","0",null,"STK",222,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=5,1,\"\")))","v":""},null,712]
["Kerastar",13,160,"Kerastar16013","2d","KRS 160 Konsolenbleche (Paar)","103388","0",null,"STK",60]
["Kerastar",14,160,"Kerastar16014",3,"KRS 160  Revisionselement trocken- Betrieb L665mm","103271",665,null,"STK",349,{"$f":"IF(N63=0,\"\",N63)","v":1},{"$f":"IF(N63=\"\",0,N63*H63)","v":665},{"$f":"Daten!$C$424","v":1},null,{"$f":"H63*N63","v":665}]
["Kerastar",15,160,"Kerastar16015","4a","KRS 160  T-Stück 90 ° L665mm ","103285",665,null,"STK",263,{"$f":"IF(N64=0,\"\",IF(Daten!$F$390=\"90°\",N64,\"\"))","v":1},{"$f":"IF(L64=\"\",0,L64*H64)","v":665},{"$f":"Daten!$C$193","v":1},null,{"$f":"IF(L64=\"\",0,H64*L64)","v":665}]
["Kerastar",16,160,"Kerastar16016","4b","KRS 160  Anschlussrosette zu T-Stk. Øi 165mm","103292","0",null,"STK",45,{"$f":"IF(N64=0,\"\",N64)","v":1}]
["Kerastar",17,160,"Kerastar16017","4c","KRS 160  T-Stück 45 ° L665mm ","103299",665,null,"STK",380,{"$f":"IF(N64=0,\"\",IF(Daten!$F$390=\"45°\",N64,\"\"))","v":""},{"$f":"IF(L66=\"\",0,L66*H66)","v":0},null,null,{"$f":"IF(L66=\"\",0,H66*L66)","v":0}]
["Kerastar",18,160,"Kerastar16018","4d","KRS 160  Winkel 15 ° ","103332","0",null,"STK",167]
["Kerastar",19,160,{"$f":"A68&C68&B68","v":"Kerastar16019"},"4e","KRS 160  Winkel 30 ° ","103339","0",null,"STK",183]
["Kerastar",20,160,"Kerastar16020","4f","KRS 160  Winkel 45 ° ","103346","0",null,"STK",183,null,null,"Stk RA-VL","RA-Verl."]
["Kerastar",21,160,"Kerastar16021","5a","KRS 160  Längenelement L665mm ","103304",665,null,"STK",138,{"$f":"ROUNDUP(M70,0)+N70","v":12},{"$f":"((M49-M50-M52-M63-M64-M66-M71-M72-M82+O71+O72)/H70)","v":11.732330827067669},{"$f":"O70/H70","v":0},{"$f":"Daten!$BY$161*1000","v":0},{"$f":"(IF(L70=\"\",0,H70*L70))-O70","v":7980}]
["Kerastar",22,160,"Kerastar16022","5b","KRS 160  Längenelement L330mm ","103311",331,null,"STK",100,{"$f":"IF(Daten!$CC$151=0,\"\",Daten!$CC$151)","v":1},{"$f":"IF(L71=\"\",0,L71*H71)","v":331},{"$f":"O71/H71","v":0},{"$f":"Daten!$BY$152*1000","v":0},{"$f":"(IF(L71=\"\",0,H71*L71))-O71","v":331}]
["Kerastar",23,160,"Kerastar16023","5c","KRS 160  Längenelement L165mm ","103318",165,null,"STK",66,{"$f":"IF(Daten!$CC$142=0,\"\",Daten!$CC$142)","v":""},{"$f":"IF(L72=\"\",0,L72*H72)","v":0},{"$f":"O72/H72","v":0},{"$f":"Daten!$BY$143*1000","v":0},{"$f":"(IF(L72=\"\",0,H72*L72))-O72","v":0}]
["Kerastar",24,160,"Kerastar16024","5d","ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",12,{"$f":"ROUNDUP(M73,0)","v":2},{"$f":"((M49/1000)*44)/310","v":1.4193548387096775}]
["Kerastar",25,160,"Kerastar16025","6a","KRS 160  Wandhalter 50 Light ","103422","0",null,"STK",42]
["Kerastar",26,160,"Kerastar16026","6b","KRS 160  Wandhalterung 50mm ","103427","0",null,"STK",29,{"$f":"ROUNDUP(M75,0)-N76","v":3},{"$f":"((M49/1000)/4.3)","v":2.3255813953488373}]
["Kerastar",27,160,"Kerastar16027","6d","KRS 160 Wandhalt.statisch 50mm","103404","0",null,"STK",72,{"$f":"IF(N76=0,\"\",N76)","v":""},null,{"$f":"IF(Daten!$A$479=2,1,0)","v":0}]
["Kerastar",28,160,{"$f":"A77&C77&B77","v":"Kerastar16028"},"6c","ICS L1 Verlängerung zu Wandhalter 50mm L300mm","101254","0",null,"STK",66,{"$f":"IF(Daten!$B$410=2,L75+N76,\"\")","v":""},null,220]
["Kerastar",29,160,"Kerastar16029","6c","ICS L2 Verlängerung zu Wandhalter 50mm L450mm","101255","0",null,"STK",83,{"$f":"IF(Daten!$B$410=3,L75+N76,\"\")","v":""},null,370]
["Kerastar",30,160,"Kerastar16030","6c","ICS L3 Verlängerung zu Wandhalter 50mm L550mm","101256","0",null,"STK",95,{"$f":"IF(Daten!$B$410=4,L75+N76,\"\")","v":""},null,470]
["Kerastar",31,160,"Kerastar16031","6c","ICS L4 Verlängerung zu Wandhalter 50mm L750mm","101257","0",null,"STK",101,{"$f":"IF(Daten!$B$410=5,L75+N76,\"\")","v":""},null,670]
["Kerastar",32,160,"Kerastar16032",7,"KRS 160 Sparrenhalter ","103415","0",null,"STK",69,{"$f":"IF(Daten!$B$443=1,\"\",\"1\")","v":""}]
["Kerastar",33,160,"Kerastar16033","8a","KRS 160  Mündungsabschluss L207mm","103325",207,null,"STK",83,{"$f":"IF(Daten!$B$451=1,1,\"\")","v":1},{"$f":"IF(L82=\"\",0,L82*H82)","v":207},null,null,{"$f":"IF(L82=\"\",0,H82*L82)","v":207}]
["Kerastar",34,160,"Kerastar16034",null,"KRS 160 Basten Standard mit Stulpring Inox","103433","0",null,"STK",340,{"$f":"IF(Daten!$B$451=2,1,\"\")","v":""}]
["Kerastar",35,160,{"$f":"A84&C84&B84","v":"Kerastar16035"},null,"KRS 160 Basten Regulator mit Stulpring Inox","103439","0",null,"STK",440,{"$f":"IF(Daten!$B$451=3,1,\"\")","v":""}]
["Kerastar",36,160,{"$f":"A85&C85&B85","v":"Kerastar16036"},"9a",{"$f":"VLOOKUP(G85,sanschie!A:E,5,0)","v":"ICM 250-300 Dachdurführung 0° DN370 L500mm"},"102327","0",null,"STK",147,{"$f":"IF(Daten!$C$432=\"0 °\",1,\"\")","v":""}]
["Kerastar",37,160,"Kerastar16037","9c",{"$f":"VLOOKUP(G86,sanschie!A:E,5,0)","v":"ICM 200 Dachdurführung 16-25° DN320 mit Bleilappen"},"102338","0",null,"STK",284,{"$f":"IF(Daten!$C$432=\"16 ° - 25 °\",1,\"\")","v":""}]
["Kerastar",38,160,"Kerastar16038","9d",{"$f":"VLOOKUP(G87,sanschie!A:E,5,0)","v":"ICM 200 Dachdurführung 26-35° DN320 mit Bleilappen"},"102350","0",null,"STK",284,{"$f":"IF(Daten!$C$432=\"26 ° - 35 °\",1,\"\")","v":""}]
["Kerastar",39,160,"Kerastar16039","9e",{"$f":"VLOOKUP(G88,sanschie!A:E,5,0)","v":"ICM 200 Dachdurführung 36-45° DN320 mit Bleilappen"},"102362","0",null,"STK",358,{"$f":"IF(Daten!$C$432=\"36 ° - 45 °\",1,\"\")","v":""}]
["Kerastar",40,160,"Kerastar16040",10,"KRS Regenkragen        16","104662","0",null,"STK",48,{"$f":"IF(SUM(L85:L88)=1,1,\"\")","v":""}]
["Kerastar",41,160,"Kerastar16041","11a","KRS 160 Anschlussrosette Øi 294mm ØA 464mm","103353","0",null,"STK",27]
["Kerastar",42,160,"Kerastar16042",12,"KRS 160 Abdeckros.16-21° Dachneigung  ","103360","0",null,"STK",27]
["Kerastar",43,160,"Kerastar16043",13,"KRS 160 Seilabspannring","103392","0",null,"STK",20]
["Kerastar",44,160,"Kerastar16044","14a","KRS 160 Statisches Klemmband","103397","0",null,"STK",20,{"$f":"IF(Daten!$B$479=2,2,\"\")","v":""}]
["Kerastar",0,180,"Kerastar1800","P","Kerastar Anlage Ø 180","Kerastar 180","0",{"$f":"Kerastar!$J$8","v":10},"Anlage",0,1,{"$f":"I94*1000","v":10000},null,{"$f":"ROUNDUP(P94,2)","v":10.18},{"$f":"SUM(P95:P137)/1000","v":10.178000000000001}]
["Kerastar",{"$f":"B94+1","v":1},{"$f":"C94","v":180},"Kerastar1801","1a","KRS 180 Fussteil Bodenmontage mit Ablauf L350mm","103247",330,null,"STK",217,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L95=\"\",0,L95*H95)","v":330},null,null,{"$f":"IF(L95=\"\",0,H95*L95)","v":330}]
["Kerastar",{"$f":"B95+1","v":2},{"$f":"C95","v":180},"Kerastar1802","1a","KRS Fusssteher-Set 4Stk. verstellbar L325-540mm","103252","0",null,"STK",422,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L96=\"\",0,L96*H96)","v":0}]
["Kerastar",{"$f":"B96+1","v":3},{"$f":"C96","v":180},"Kerastar1803","1c","KRS 180 Fussteil für Wohnraum verstelb. L186-286mm","103255",186,null,"STK",189,{"$f":"IF(Daten!$B$401=3,1,\"\")","v":""},{"$f":"IF(L97=\"\",0,L97*H97)","v":0},null,null,{"$f":"IF(L97=\"\",0,H97*L97)","v":0}]
["Kerastar",4,180,"Kerastar1804","2a","KRS 180 Grundplatte verstärkt mit Ablauf","103260",44,null,"STK",170,{"$f":"N98","v":""},null,{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""},{"$f":"IF(Daten!$B$410=1,\"\",1)","v":""}]
["Kerastar",5,180,"Kerastar1805","2b","KRS 180 Grundplatte mit Russtopf","103267",44,null,"STK",242]
["Kerastar",6,180,{"$f":"A100&C100&B100","v":"Kerastar1806"},"2b","KRS 180 Deckenanschluss-Element","140851",376,null,"STK",428]
["Kerastar",7,180,"Kerastar1807","2b","KRS 180 Ofenaufsatz-Element","140856",340,null,"STK",154]
["Kerastar",8,180,"Kerastar1808","2c","KRS Wand-Konsole Typ 475mm (Paar)","103379","0",null,"STK",138,{"$f":"N102","v":""},null,{"$f":"IF(Daten!$B$410=1,O102,\"\")","v":""},{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""}]
["Kerastar",9,180,"Kerastar1809","2c","KRS Wand-Konsole Typ 570mm (Paar)","103380","0",null,"STK",144,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$BC$401=3,\"\",IF(Daten!$B$410=2,1,\"\")))","v":""},null,278]
["Kerastar",10,180,"Kerastar18010","2c","KRS Wand-Konsole Typ 720mm (Paar)","103381","0",null,"STK",151,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=3,1,\"\")))","v":""},null,428]
["Kerastar",11,180,"Kerastar18011","2c","KRS Wand-Konsole Typ 820mm (Paar)","103382","0",null,"STK",164,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=4,1,\"\")))","v":""},null,528]
["Kerastar",12,180,"Kerastar18012","2c","KRS Wand-Konsole Typ 1004mm (Paar)","103383","0",null,"STK",222,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=5,1,\"\")))","v":""},null,712]
["Kerastar",13,180,"Kerastar18013","2d","KRS 180 Konsolenbleche (Paar)","103389","0",null,"STK",65]
["Kerastar",14,180,"Kerastar18014",3,"KRS 180  Revisionselement trocken- Betrieb L665mm","103272",665,null,"STK",375,{"$f":"IF(N108=0,\"\",N108)","v":1},{"$f":"IF(N108=\"\",0,N108*H108)","v":665},{"$f":"Daten!$C$424","v":1},null,{"$f":"H108*N108","v":665}]
["Kerastar",15,180,"Kerastar18015","4a","KRS 180  T-Stück 90 ° L665mm ","103286",665,null,"STK",277,{"$f":"IF(N109=0,\"\",IF(Daten!$F$390=\"90°\",N109,\"\"))","v":1},{"$f":"IF(L109=\"\",0,L109*H109)","v":665},{"$f":"Daten!$C$193","v":1},null,{"$f":"IF(L109=\"\",0,H109*L109)","v":665}]
["Kerastar",16,180,"Kerastar18016","4b","KRS 180  Anschlussrosette zu T-Stk. Øi 185mm","103293","0",null,"STK",46,{"$f":"IF(N109=0,\"\",N109)","v":1}]
["Kerastar",17,180,"Kerastar18017","4c","KRS 180  T-Stück 45 ° L665mm ","103300",665,null,"STK",388,{"$f":"IF(N109=0,\"\",IF(Daten!$F$390=\"45°\",N109,\"\"))","v":""},{"$f":"IF(L111=\"\",0,L111*H111)","v":0},null,null,{"$f":"IF(L111=\"\",0,H111*L111)","v":0}]
["Kerastar",18,180,"Kerastar18018","4d","KRS 180  Winkel 15 ° ","103333","0",null,"STK",180]
["Kerastar",19,180,{"$f":"A113&C113&B113","v":"Kerastar18019"},"4e","KRS 180  Winkel 30 ° ","103340","0",null,"STK",197]
["Kerastar",20,180,"Kerastar18020","4f","KRS 180  Winkel 45 ° ","103347","0",null,"STK",197,null,null,"Stk RA-VL","RA-Verl."]
["Kerastar",21,180,"Kerastar18021","5a","KRS 180  Längenelement L665mm ","103305",665,null,"STK",147,{"$f":"ROUNDUP(M115,0)+N115","v":12},{"$f":"((M94-M95-M97-M108-M109-M111-M116-M117-M127+O116+O117)/H115)","v":11.732330827067669},{"$f":"O115/H115","v":0},{"$f":"Daten!$BY$161*1000","v":0},{"$f":"(IF(L115=\"\",0,H115*L115))-O115","v":7980}]
["Kerastar",22,180,"Kerastar18022","5b","KRS 180  Längenelement L330mm ","103312",331,null,"STK",105,{"$f":"IF(Daten!$CC$151=0,\"\",Daten!$CC$151)","v":1},{"$f":"IF(L116=\"\",0,L116*H116)","v":331},{"$f":"O116/H116","v":0},{"$f":"Daten!$BY$152*1000","v":0},{"$f":"(IF(L116=\"\",0,H116*L116))-O116","v":331}]
["Kerastar",23,180,"Kerastar18023","5c","KRS 180  Längenelement L165mm ","103319",165,null,"STK",68,{"$f":"IF(Daten!$CC$142=0,\"\",Daten!$CC$142)","v":""},{"$f":"IF(L117=\"\",0,L117*H117)","v":0},{"$f":"O117/H117","v":0},{"$f":"Daten!$BY$143*1000","v":0},{"$f":"(IF(L117=\"\",0,H117*L117))-O117","v":0}]
["Kerastar",24,180,"Kerastar18024","5d","ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",12,{"$f":"ROUNDUP(M118,0)","v":2},{"$f":"((M94/1000)*44)/310","v":1.4193548387096775}]
["Kerastar",25,180,"Kerastar18025","6a","KRS 180  Wandhalter 50 Light ","103423","0",null,"STK",43]
["Kerastar",26,180,"Kerastar18026","6b","KRS 180  Wandhalterung 50mm ","103428","0",null,"STK",30,{"$f":"ROUNDUP(M120,0)-N121","v":3},{"$f":"((M94/1000)/4.3)","v":2.3255813953488373}]
["Kerastar",27,180,"Kerastar18027","6d","KRS 180 Wandhalt.statisch 50mm","103405","0",null,"STK",73,{"$f":"IF(N121=0,\"\",N121)","v":""},null,{"$f":"IF(Daten!$A$479=2,1,0)","v":0}]
["Kerastar",28,180,{"$f":"A122&C122&B122","v":"Kerastar18028"},"6c","ICS L1 Verlängerung zu Wandhalter 50mm L300mm","101254","0",null,"STK",66,{"$f":"IF(Daten!$B$410=2,L120+N121,\"\")","v":""},null,220]
["Kerastar",29,180,"Kerastar18029","6c","ICS L2 Verlängerung zu Wandhalter 50mm L450mm","101255","0",null,"STK",83,{"$f":"IF(Daten!$B$410=3,L120+N121,\"\")","v":""},null,370]
["Kerastar",30,180,"Kerastar18030","6c","ICS L3 Verlängerung zu Wandhalter 50mm L550mm","101256","0",null,"STK",95,{"$f":"IF(Daten!$B$410=4,L120+N121,\"\")","v":""},null,470]
["Kerastar",31,180,"Kerastar18031","6c","ICS L4 Verlängerung zu Wandhalter 50mm L750mm","101257","0",null,"STK",101,{"$f":"IF(Daten!$B$410=5,L120+N121,\"\")","v":""},null,670]
["Kerastar",32,180,"Kerastar18032",7,"KRS 180 Sparrenhalter ","103416","0",null,"STK",70,{"$f":"IF(Daten!$B$443=1,\"\",\"1\")","v":""}]
["Kerastar",33,180,"Kerastar18033","8a","KRS 180  Mündungsabschluss L207mm","103326",207,null,"STK",87,{"$f":"IF(Daten!$B$451=1,1,\"\")","v":1},{"$f":"IF(L127=\"\",0,L127*H127)","v":207},null,null,{"$f":"IF(L127=\"\",0,H127*L127)","v":207}]
["Kerastar",34,180,"Kerastar18034",null,"KRS 180 Basten Standard mit Stulpring Inox","103434","0",null,"STK",361,{"$f":"IF(Daten!$B$451=2,1,\"\")","v":""}]
["Kerastar",35,180,{"$f":"A129&C129&B129","v":"Kerastar18035"},null,"KRS 180 Basten Regulator mit Stulpring Inox","103440","0",null,"STK",461,{"$f":"IF(Daten!$B$451=3,1,\"\")","v":""}]
["Kerastar",36,180,{"$f":"A130&C130&B130","v":"Kerastar18036"},"9a",{"$f":"VLOOKUP(G130,sanschie!A:E,5,0)","v":"ICM 300 Dachdurführung 0° DN400 L500mm"},"102328","0",null,"STK",275,{"$f":"IF(Daten!$C$432=\"0 °\",1,\"\")","v":""}]
["Kerastar",37,180,"Kerastar18037","9c",{"$f":"VLOOKUP(G131,sanschie!A:E,5,0)","v":"ICM 250-300 Dachdurführung 16-25° DN370 "},"102339","0",null,"STK",284,{"$f":"IF(Daten!$C$432=\"16 ° - 25 °\",1,\"\")","v":""}]
["Kerastar",38,180,"Kerastar18038","9d",{"$f":"VLOOKUP(G132,sanschie!A:E,5,0)","v":"ICM 250-300 Dachdurführung 26-35° DN370 "},"102351","0",null,"STK",284,{"$f":"IF(Daten!$C$432=\"26 ° - 35 °\",1,\"\")","v":""}]
["Kerastar",39,180,"Kerastar18039","9e",{"$f":"VLOOKUP(G133,sanschie!A:E,5,0)","v":"ICM 250-300 Dachdurführung 36-45° DN370 "},"102363","0",null,"STK",358,{"$f":"IF(Daten!$C$432=\"36 ° - 45 °\",1,\"\")","v":""}]
["Kerastar",40,180,"Kerastar18040",10,"KRS Regenkragen        18","104663","0",null,"STK",48,{"$f":"IF(SUM(L130:L133)=1,1,\"\")","v":""}]
["Kerastar",41,180,"Kerastar18041","11a","KRS 180 Anschlussrosette Øi 314mm ØA 484mm","103354","0",null,"STK",26]
["Kerastar",42,180,"Kerastar18042",12,"KRS 180 Abdeckros.16-21° Dachneigung  ","103361","0",null,"STK",26]
["Kerastar",43,180,"Kerastar18043",13,"KRS 180 Seilabspannring","103393","0",null,"STK",21]
["Kerastar",44,180,"Kerastar18044","14a","KRS 180 Statisches Klemmband","103398","0",null,"STK",21,{"$f":"IF(Daten!$B$479=2,2,\"\")","v":""}]
["Kerastar",0,200,"Kerastar2000","P","Kerastar Anlage Ø 200","Kerastar 200","0",{"$f":"Kerastar!$J$8","v":10},"Anlage",0,1,{"$f":"I139*1000","v":10000},null,{"$f":"ROUNDUP(P139,2)","v":10.18},{"$f":"SUM(P140:P182)/1000","v":10.178000000000001}]
["Kerastar",{"$f":"B139+1","v":1},{"$f":"C139","v":200},"Kerastar2001","1a","KRS 200 Fussteil Bodenmontage mit Ablauf L350mm","103248",330,null,"STK",226,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L140=\"\",0,L140*H140)","v":330},null,null,{"$f":"IF(L140=\"\",0,H140*L140)","v":330}]
["Kerastar",{"$f":"B140+1","v":2},{"$f":"C140","v":200},"Kerastar2002","1a","KRS Fusssteher-Set 4Stk. verstellbar L325-540mm","103252","0",null,"STK",422,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L141=\"\",0,L141*H141)","v":0}]
["Kerastar",{"$f":"B141+1","v":3},{"$f":"C141","v":200},"Kerastar2003","1c","KRS 200 Fussteil für Wohnraum verstelb. L186-286mm","103256",186,null,"STK",196,{"$f":"IF(Daten!$B$401=3,1,\"\")","v":""},{"$f":"IF(L142=\"\",0,L142*H142)","v":0},null,null,{"$f":"IF(L142=\"\",0,H142*L142)","v":0}]
["Kerastar",4,200,"Kerastar2004","2a","KRS 200 Grundplatte verstärkt mit Ablauf","103261",44,null,"STK",194,{"$f":"N143","v":""},null,{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""},{"$f":"IF(Daten!$B$410=1,\"\",1)","v":""}]
["Kerastar",5,200,"Kerastar2005","2b","KRS 200 Grundplatte mit Russtopf.","103268",44,null,"STK",271]
["Kerastar",6,200,{"$f":"A145&C145&B145","v":"Kerastar2006"},"2b","KRS 200 Deckenanschluss-Element","140852",376,null,"STK",454]
["Kerastar",7,200,"Kerastar2007","2b","KRS 200 Ofenaufsatz-Element","140857",340,null,"STK",164]
["Kerastar",8,200,"Kerastar2008","2c","KRS Wand-Konsole Typ 475mm (Paar)","103379","0",null,"STK",138,{"$f":"N147","v":""},null,{"$f":"IF(Daten!$B$410=1,O147,\"\")","v":""},{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""}]
["Kerastar",9,200,"Kerastar2009","2c","KRS Wand-Konsole Typ 570mm (Paar)","103380","0",null,"STK",144,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$BC$401=3,\"\",IF(Daten!$B$410=2,1,\"\")))","v":""},null,278]
["Kerastar",10,200,"Kerastar20010","2c","KRS Wand-Konsole Typ 720mm (Paar)","103381","0",null,"STK",151,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=3,1,\"\")))","v":""},null,428]
["Kerastar",11,200,"Kerastar20011","2c","KRS Wand-Konsole Typ 820mm (Paar)","103382","0",null,"STK",164,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=4,1,\"\")))","v":""},null,528]
["Kerastar",12,200,"Kerastar20012","2c","KRS Wand-Konsole Typ 1004mm (Paar)","103383","0",null,"STK",222,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=5,1,\"\")))","v":""},null,712]
["Kerastar",13,200,"Kerastar20013","2d","KRS 200 Konsolenbleche (Paar)","103390","0",null,"STK",71]
["Kerastar",14,200,"Kerastar20014",3,"KRS 200  Revisionselement trocken- Betrieb L665mm","103273",665,null,"STK",439,{"$f":"IF(N153=0,\"\",N153)","v":1},{"$f":"IF(N153=\"\",0,N153*H153)","v":665},{"$f":"Daten!$C$424","v":1},null,{"$f":"H153*N153","v":665}]
["Kerastar",15,200,"Kerastar20015","4a","KRS 200  T-Stück 90 ° L665mm ","103287",665,null,"STK",306,{"$f":"IF(N154=0,\"\",IF(Daten!$F$390=\"90°\",N154,\"\"))","v":1},{"$f":"IF(L154=\"\",0,L154*H154)","v":665},{"$f":"Daten!$C$193","v":1},null,{"$f":"IF(L154=\"\",0,H154*L154)","v":665}]
["Kerastar",16,200,"Kerastar20016","4b","KRS 200  Anschlussrosette zu T-Stk. Øi 205mm","103294","0",null,"STK",48,{"$f":"IF(N154=0,\"\",N154)","v":1}]
["Kerastar",17,200,"Kerastar20017","4c","KRS 200  T-Stück 45 ° L665mm ","103301",665,null,"STK",455,{"$f":"IF(N154=0,\"\",IF(Daten!$F$390=\"45°\",N154,\"\"))","v":""},{"$f":"IF(L156=\"\",0,L156*H156)","v":0},null,null,{"$f":"IF(L156=\"\",0,H156*L156)","v":0}]
["Kerastar",18,200,"Kerastar20018","4d","KRS 200  Winkel 15 ° ","103334","0",null,"STK",198]
["Kerastar",19,200,{"$f":"A158&C158&B158","v":"Kerastar20019"},"4e","KRS 200  Winkel 30 ° ","103341","0",null,"STK",216]
["Kerastar",20,200,"Kerastar20020","4f","KRS 200  Winkel 45 ° ","103348","0",null,"STK",216,null,null,"Stk RA-VL","RA-Verl."]
["Kerastar",21,200,"Kerastar20021","5a","KRS 200  Längenelement L665mm ","103306",665,null,"STK",158,{"$f":"ROUNDUP(M160,0)+N160","v":12},{"$f":"((M139-M140-M142-M153-M154-M156-M161-M162-M172+O161+O162)/H160)","v":11.732330827067669},{"$f":"O160/H160","v":0},{"$f":"Daten!$BY$161*1000","v":0},{"$f":"(IF(L160=\"\",0,H160*L160))-O160","v":7980}]
["Kerastar",22,200,"Kerastar20022","5b","KRS 200  Längenelement L330mm ","103313",331,null,"STK",110,{"$f":"IF(Daten!$CC$151=0,\"\",Daten!$CC$151)","v":1},{"$f":"IF(L161=\"\",0,L161*H161)","v":331},{"$f":"O161/H161","v":0},{"$f":"Daten!$BY$152*1000","v":0},{"$f":"(IF(L161=\"\",0,H161*L161))-O161","v":331}]
["Kerastar",23,200,"Kerastar20023","5c","KRS 200  Längenelement L165mm ","103320",165,null,"STK",72,{"$f":"IF(Daten!$CC$142=0,\"\",Daten!$CC$142)","v":""},{"$f":"IF(L162=\"\",0,L162*H162)","v":0},{"$f":"O162/H162","v":0},{"$f":"Daten!$BY$143*1000","v":0},{"$f":"(IF(L162=\"\",0,H162*L162))-O162","v":0}]
["Kerastar",24,200,"Kerastar20024","5d","ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",12,{"$f":"ROUNDUP(M163,0)","v":2},{"$f":"((M139/1000)*44)/310","v":1.4193548387096775}]
["Kerastar",25,200,"Kerastar20025","6a","KRS 200  Wandhalter 50 Light ","103424","0",null,"STK",43]
["Kerastar",26,200,"Kerastar20026","6b","KRS 200  Wandhalterung 50mm ","103429","0",null,"STK",31,{"$f":"ROUNDUP(M165,0)-N166","v":3},{"$f":"((M139/1000)/4.3)","v":2.3255813953488373}]
["Kerastar",27,200,"Kerastar20027","6d","KRS 200 Wandhalt.statisch 50mm","103406","0",null,"STK",76,{"$f":"IF(N166=0,\"\",N166)","v":""},null,{"$f":"IF(Daten!$A$479=2,1,0)","v":0}]
["Kerastar",28,200,{"$f":"A167&C167&B167","v":"Kerastar20028"},"6c","ICS L1 Verlängerung zu Wandhalter 50mm L300mm","101254","0",null,"STK",66,{"$f":"IF(Daten!$B$410=2,L165+N166,\"\")","v":""},null,220]
["Kerastar",29,200,"Kerastar20029","6c","ICS L2 Verlängerung zu Wandhalter 50mm L450mm","101255","0",null,"STK",83,{"$f":"IF(Daten!$B$410=3,L165+N166,\"\")","v":""},null,370]
["Kerastar",30,200,"Kerastar20030","6c","ICS L3 Verlängerung zu Wandhalter 50mm L550mm","101256","0",null,"STK",95,{"$f":"IF(Daten!$B$410=4,L165+N166,\"\")","v":""},null,470]
["Kerastar",31,200,"Kerastar20031","6c","ICS L4 Verlängerung zu Wandhalter 50mm L750mm","101257","0",null,"STK",101,{"$f":"IF(Daten!$B$410=5,L165+N166,\"\")","v":""},null,670]
["Kerastar",32,200,"Kerastar20032",7,"KRS 200 Sparrenhalter ","103417","0",null,"STK",70,{"$f":"IF(Daten!$B$443=1,\"\",\"1\")","v":""}]
["Kerastar",33,200,"Kerastar20033","8a","KRS 200  Mündungsabschluss L207mm","103327",207,null,"STK",97,{"$f":"IF(Daten!$B$451=1,1,\"\")","v":1},{"$f":"IF(L172=\"\",0,L172*H172)","v":207},null,null,{"$f":"IF(L172=\"\",0,H172*L172)","v":207}]
["Kerastar",34,200,"Kerastar20034",null,"KRS 200 Basten Standard mit Stulpring Inox","103435","0",null,"STK",372,{"$f":"IF(Daten!$B$451=2,1,\"\")","v":""}]
["Kerastar",35,200,{"$f":"A174&C174&B174","v":"Kerastar20035"},null,"KRS 200 Basten Regulator mit Stulpring Inox","103441","0",null,"STK",472,{"$f":"IF(Daten!$B$451=3,1,\"\")","v":""}]
["Kerastar",36,200,{"$f":"A175&C175&B175","v":"Kerastar20036"},"9a",{"$f":"VLOOKUP(G175,sanschie!A:E,5,0)","v":"ICM 300 Dachdurführung 0° DN400 L500mm"},"102328","0",null,"STK",275,{"$f":"IF(Daten!$C$432=\"0 °\",1,\"\")","v":""}]
["Kerastar",37,200,"Kerastar20037","9c",{"$f":"VLOOKUP(G176,sanschie!A:E,5,0)","v":"ICM 250-300 Dachdurführung 16-25° DN370 "},"102339","0",null,"STK",284,{"$f":"IF(Daten!$C$432=\"16 ° - 25 °\",1,\"\")","v":""}]
["Kerastar",38,200,"Kerastar20038","9d",{"$f":"VLOOKUP(G177,sanschie!A:E,5,0)","v":"ICM 250-300 Dachdurführung 26-35° DN370 "},"102351","0",null,"STK",284,{"$f":"IF(Daten!$C$432=\"26 ° - 35 °\",1,\"\")","v":""}]
["Kerastar",39,200,"Kerastar20039","9e",{"$f":"VLOOKUP(G178,sanschie!A:E,5,0)","v":"ICM 250-300 Dachdurführung 36-45° DN370 "},"102363","0",null,"STK",358,{"$f":"IF(Daten!$C$432=\"36 ° - 45 °\",1,\"\")","v":""}]
["Kerastar",40,200,"Kerastar20040",10,"KRS Regenkragen        20","104547","0",null,"STK",49,{"$f":"IF(SUM(L175:L178)=1,1,\"\")","v":""}]
["Kerastar",41,200,"Kerastar20041","11a","KRS 200 Anschlussrosette Øi 338mm ØA 508mm","103355","0",null,"STK",44]
["Kerastar",42,200,"Kerastar20042",12,"KRS 200 Abdeckros.16-21° Dachneigung  ","103362","0",null,"STK",44]
["Kerastar",43,200,"Kerastar20043",13,"KRS 200 Seilabspannring","103394","0",null,"STK",23]
["Kerastar",44,200,"Kerastar20044","14a","KRS 200 Statisches Klemmband","103399","0",null,"STK",23,{"$f":"IF(Daten!$B$479=2,2,\"\")","v":""}]
["Kerastar",0,250,"Kerastar2500","P","Kerastar Anlage Ø 250","Kerastar 250","0",{"$f":"Kerastar!$J$8","v":10},"Anlage",0,1,{"$f":"I184*1000","v":10000},null,{"$f":"ROUNDUP(P184,2)","v":10.18},{"$f":"SUM(P185:P226)/1000","v":10.178000000000001}]
["Kerastar",{"$f":"B184+1","v":1},{"$f":"C184","v":250},"Kerastar2501","1a","KRS 250 Fussteil Bodenmontage mit Ablauf L350mm","103249",330,null,"STK",258,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L185=\"\",0,L185*H185)","v":330},null,null,{"$f":"IF(L185=\"\",0,H185*L185)","v":330}]
["Kerastar",{"$f":"B185+1","v":2},{"$f":"C185","v":250},"Kerastar2502","1a","KRS Fusssteher-Set 4Stk. verstellbar L325-540mm","103252","0",null,"STK",422,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L186=\"\",0,L186*H186)","v":0}]
["Kerastar",{"$f":"B186+1","v":3},{"$f":"C186","v":250},"Kerastar2503","1c","KRS 250 Fussteil für Wohnraum verstelb. L186-286mm","103257",186,null,"STK",216,{"$f":"IF(Daten!$B$401=3,1,\"\")","v":""},{"$f":"IF(L187=\"\",0,L187*H187)","v":0},null,null,{"$f":"IF(L187=\"\",0,H187*L187)","v":0}]
["Kerastar",4,250,"Kerastar2504","2a","KRS 250 Grundplatte verstärkt mit Ablauf","103262",44,null,"STK",200,{"$f":"N188","v":""},null,{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""},{"$f":"IF(Daten!$B$410=1,\"\",1)","v":""}]
["Kerastar",5,250,"Kerastar2505","2b","KRS 200 Grundplatte mit Russtopf.","103268",44,null,"STK",271]
["Kerastar",6,250,{"$f":"A190&C190&B190","v":"Kerastar2506"},"2b","KRS 250 Deckenanschluss-Element","140853",376,null,"STK",526]
["Kerastar",7,250,"Kerastar2507","2b","KRS 250 Ofenaufsatz-Element","140858",340,null,"STK",186]
["Kerastar",8,250,"Kerastar2508","2c","KRS Wand-Konsole Typ 475mm (Paar)","103379","0",null,"STK",138,{"$f":"N192","v":""},null,{"$f":"IF(Daten!$B$410=1,O192,\"\")","v":""},{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""}]
["Kerastar",9,250,"Kerastar2509","2c","KRS Wand-Konsole Typ 570mm (Paar)","103380","0",null,"STK",144,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$BC$401=3,\"\",IF(Daten!$B$410=2,1,\"\")))","v":""},null,278]
["Kerastar",10,250,"Kerastar25010","2c","KRS Wand-Konsole Typ 720mm (Paar)","103381","0",null,"STK",151,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=3,1,\"\")))","v":""},null,428]
["Kerastar",11,250,"Kerastar25011","2c","KRS Wand-Konsole Typ 820mm (Paar)","103382","0",null,"STK",164,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=4,1,\"\")))","v":""},null,528]
["Kerastar",12,250,"Kerastar25012","2c","KRS Wand-Konsole Typ 1004mm (Paar)","103383","0",null,"STK",222,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=5,1,\"\")))","v":""},null,712]
["Kerastar",{"$f":"B196+1","v":13},{"$f":"C196","v":250},{"$f":"A197&C197&B197","v":"Kerastar25013"},3,"KRS 250  Revisionselement trocken- Betrieb L665mm","103274",665,null,"STK",485,{"$f":"IF(N197=0,\"\",N197)","v":1},{"$f":"IF(N197=\"\",0,N197*H197)","v":665},{"$f":"Daten!$C$424","v":1},null,{"$f":"H197*N197","v":665}]
["Kerastar",{"$f":"B197+1","v":14},{"$f":"C197","v":250},"Kerastar25014","4a","KRS 250  T-Stück 90 ° L665mm ","103288",665,null,"STK",396,{"$f":"IF(N198=0,\"\",IF(Daten!$F$390=\"90°\",N198,\"\"))","v":1},{"$f":"IF(L198=\"\",0,L198*H198)","v":665},{"$f":"Daten!$C$193","v":1},null,{"$f":"IF(L198=\"\",0,H198*L198)","v":665}]
["Kerastar",{"$f":"B198+1","v":15},{"$f":"C198","v":250},"Kerastar25015","4b","KRS 250  Anschlussrosette zu T-Stk. Øi 255mm","103295","0",null,"STK",56,{"$f":"IF(N198=0,\"\",N198)","v":1}]
["Kerastar",{"$f":"B199+1","v":16},{"$f":"C199","v":250},"Kerastar25016","4c","KRS 250  T-Stück 45 ° L665mm ","103302",665,null,"STK",658,{"$f":"IF(N198=0,\"\",IF(Daten!$F$390=\"45°\",N198,\"\"))","v":""},{"$f":"IF(L200=\"\",0,L200*H200)","v":0},null,null,{"$f":"IF(L200=\"\",0,H200*L200)","v":0}]
["Kerastar",{"$f":"B200+1","v":17},{"$f":"C200","v":250},"Kerastar25017","4d","KRS 250  Winkel 15 ° ","103335","0",null,"STK",260]
["Kerastar",18,250,"Kerastar25018","4e","KRS 250  Winkel 30 ° ","103342","0",null,"STK",281]
["Kerastar",19,250,"Kerastar25019","4f","KRS 250  Winkel 45 ° ","103349","0",null,"STK",281,null,null,"Stk RA-VL","RA-Verl."]
["Kerastar",20,250,"Kerastar25020","5a","KRS 250  Längenelement L665mm ","103307",665,null,"STK",181,{"$f":"ROUNDUP(M204,0)+N204","v":12},{"$f":"((M184-M185-M187-M197-M198-M200-M205-M206-M216+O205+O206)/H204)","v":11.732330827067669},{"$f":"O204/H204","v":0},{"$f":"Daten!$BY$161*1000","v":0},{"$f":"(IF(L204=\"\",0,H204*L204))-O204","v":7980}]
["Kerastar",21,250,"Kerastar25021","5b","KRS 250  Längenelement L330mm ","103314",331,null,"STK",125,{"$f":"IF(Daten!$CC$151=0,\"\",Daten!$CC$151)","v":1},{"$f":"IF(L205=\"\",0,L205*H205)","v":331},{"$f":"O205/H205","v":0},{"$f":"Daten!$BY$152*1000","v":0},{"$f":"(IF(L205=\"\",0,H205*L205))-O205","v":331}]
["Kerastar",22,250,"Kerastar25022","5c","KRS 250  Längenelement L165mm ","103321",165,null,"STK",84,{"$f":"IF(Daten!$CC$142=0,\"\",Daten!$CC$142)","v":""},{"$f":"IF(L206=\"\",0,L206*H206)","v":0},{"$f":"O206/H206","v":0},{"$f":"Daten!$BY$143*1000","v":0},{"$f":"(IF(L206=\"\",0,H206*L206))-O206","v":0}]
["Kerastar",23,250,"Kerastar25023","5d","ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",12,{"$f":"ROUNDUP(M207,0)","v":2},{"$f":"((M184/1000)*44)/310","v":1.4193548387096775}]
["Kerastar",24,250,"Kerastar25024","6a","KRS 250  Wandhalter 50 Light ","103425","0",null,"STK",44]
["Kerastar",25,250,"Kerastar25025","6b","KRS 250  Wandhalterung 50mm ","103430","0",null,"STK",44,{"$f":"ROUNDUP(M209,0)-N210","v":3},{"$f":"((M184/1000)/4.3)","v":2.3255813953488373}]
["Kerastar",26,250,"Kerastar25026","6d","KRS 250 Wandhalt.statisch 50mm","103407","0",null,"STK",85,{"$f":"IF(N210=0,\"\",N210)","v":""},null,{"$f":"IF(Daten!$A$479=2,1,0)","v":0}]
["Kerastar",27,250,{"$f":"A211&C211&B211","v":"Kerastar25027"},"6c","ICS L1 Verlängerung zu Wandhalter 50mm L300mm","101254","0",null,"STK",66,{"$f":"IF(Daten!$B$410=2,L209+N210,\"\")","v":""},null,220]
["Kerastar",28,250,"Kerastar25028","6c","ICS L2 Verlängerung zu Wandhalter 50mm L450mm","101255","0",null,"STK",83,{"$f":"IF(Daten!$B$410=3,L209+N210,\"\")","v":""},null,370]
["Kerastar",29,250,"Kerastar25029","6c","ICS L3 Verlängerung zu Wandhalter 50mm L550mm","101256","0",null,"STK",95,{"$f":"IF(Daten!$B$410=4,L209+N210,\"\")","v":""},null,470]
["Kerastar",30,250,"Kerastar25030","6c","ICS L4 Verlängerung zu Wandhalter 50mm L750mm","101257","0",null,"STK",101,{"$f":"IF(Daten!$B$410=5,L209+N210,\"\")","v":""},null,670]
["Kerastar",31,250,"Kerastar25031",7,"KRS 250 Sparrenhalter ","103418","0",null,"STK",71,{"$f":"IF(Daten!$B$443=1,\"\",\"1\")","v":""}]
["Kerastar",32,250,"Kerastar25032","8a","KRS 250  Mündungsabschluss L207mm","103328",207,null,"STK",111,{"$f":"IF(Daten!$B$451=1,1,\"\")","v":1},{"$f":"IF(L216=\"\",0,L216*H216)","v":207},null,null,{"$f":"IF(L216=\"\",0,H216*L216)","v":207}]
["Kerastar",33,250,"Kerastar25033",null,"KRS 250 Basten Standard mit Stulpring Inox","103436","0",null,"STK",427,{"$f":"IF(Daten!$B$451=2,1,\"\")","v":""}]
["Kerastar",34,250,{"$f":"A218&C218&B218","v":"Kerastar25034"},null,"KRS 250 Basten Regulator mit Stulpring Inox","103442","0",null,"STK",527,{"$f":"IF(Daten!$B$451=3,1,\"\")","v":""}]
["Kerastar",35,250,{"$f":"A219&C219&B219","v":"Kerastar25035"},"9a",{"$f":"VLOOKUP(G219,sanschie!A:E,5,0)","v":"ICM 350 Dachdurführung 0° DN450 L500mm"},"102329","0",null,"STK",315,{"$f":"IF(Daten!$C$432=\"0 °\",1,\"\")","v":""}]
["Kerastar",36,250,"Kerastar25036","9c",{"$f":"VLOOKUP(G220,sanschie!A:E,5,0)","v":"ICM 350 Dachdurführung 16-25° DN450 mit Bleilappen"},"102341","0",null,"STK",553,{"$f":"IF(Daten!$C$432=\"16 ° - 25 °\",1,\"\")","v":""}]
["Kerastar",37,250,"Kerastar25037","9d",{"$f":"VLOOKUP(G221,sanschie!A:E,5,0)","v":"ICM 350 Dachdurführung 26-35° DN450 mit Bleilappen"},"102353","0",null,"STK",602,{"$f":"IF(Daten!$C$432=\"26 ° - 35 °\",1,\"\")","v":""}]
["Kerastar",38,250,"Kerastar25038","9e",{"$f":"VLOOKUP(G222,sanschie!A:E,5,0)","v":"ICM 350 Dachdurführung 36-45° DN450 mit Bleilappen"},"102365","0",null,"STK",678,{"$f":"IF(Daten!$C$432=\"36 ° - 45 °\",1,\"\")","v":""}]
["Kerastar",39,250,"Kerastar25039",10,"KRS Regenkragen        25","104664","0",null,"STK",53,{"$f":"IF(SUM(L219:L222)=1,1,\"\")","v":""}]
["Kerastar",40,250,"Kerastar25040","11a","KRS 250 Anschlussrosette Øi 391mm ØA 561mm","103356","0",null,"STK",39]
["Kerastar",41,250,"Kerastar25041",12,"KRS 250 Abdeckros.16-21° Dachneigung  ","103363","0",null,"STK",39]
["Kerastar",42,250,"Kerastar25042",13,"KRS 250 Seilabspannring","103395","0",null,"STK",27]
["Kerastar",43,250,"Kerastar25043","14a","KRS 250 Statisches Klemmband","103400","0",null,"STK",27,{"$f":"IF(Daten!$B$479=2,2,\"\")","v":""}]
["Kerastar",0,300,"Kerastar3000","P","Kerastar Anlage Ø 300","Kerastar 300","0",{"$f":"Kerastar!$J$8","v":10},"Anlage",0,1,{"$f":"I228*1000","v":10000},null,{"$f":"ROUNDUP(P228,2)","v":10.18},{"$f":"SUM(P229:P263)/1000","v":10.178000000000001}]
["Kerastar",{"$f":"B228+1","v":1},{"$f":"C228","v":300},"Kerastar3001","1a","KRS 300 Fussteil Bodenmontage mit Ablauf L350mm","103250",330,null,"STK",549,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L229=\"\",0,L229*H229)","v":330},null,null,{"$f":"IF(L229=\"\",0,H229*L229)","v":330}]
["Kerastar",{"$f":"B229+1","v":2},{"$f":"C229","v":300},"Kerastar3002","1a","KRS Fusssteher-Set 4Stk. verstellbar L325-540mm","103252","0",null,"STK",422,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L230=\"\",0,L230*H230)","v":0}]
["Kerastar",{"$f":"B230+1","v":3},{"$f":"C230","v":300},{"$f":"A231&C231&B231","v":"Kerastar3003"},"2a","KRS 300 Grundplatte verstärkt mit Ablauf","103263",44,null,"STK",448,{"$f":"N231","v":""},null,{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""},{"$f":"IF(Daten!$B$410=1,\"\",1)","v":""}]
["Kerastar",4,300,"Kerastar3004","2c","KRS Wand-Konsole Typ 475mm (Paar)","103379","0",null,"STK",138,{"$f":"N232","v":""},null,{"$f":"IF(Daten!$B$410=1,O232,\"\")","v":""},{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""}]
["Kerastar",5,300,"Kerastar3005","2c","KRS Wand-Konsole Typ 570mm (Paar)","103380","0",null,"STK",144,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$BC$401=3,\"\",IF(Daten!$B$410=2,1,\"\")))","v":""},null,278]
["Kerastar",6,300,"Kerastar3006","2c","KRS Wand-Konsole Typ 720mm (Paar)","103381","0",null,"STK",151,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=3,1,IF(Daten!$B$410=4,1,\"\"))))","v":""},null,428]
["Kerastar",7,300,"Kerastar3007","2c","KRS Wand-Konsole Typ 820mm (Paar)","103382","0",null,"STK",164,null,null,528]
["Kerastar",8,300,"Kerastar3008","2c","KRS Wand-Konsole Typ 1004mm (Paar)","103383","0",null,"STK",222,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=5,1,\"\")))","v":""},null,712]
["Kerastar",9,300,"Kerastar3009",3,"KRS 300  Revisionselement trocken- Betrieb L665mm","103275",665,null,"STK",889,{"$f":"IF(N237=0,\"\",N237)","v":1},{"$f":"IF(N237=\"\",0,N237*H237)","v":665},{"$f":"Daten!$C$424","v":1},null,{"$f":"H237*N237","v":665}]
["Kerastar",10,300,"Kerastar30010","4a","KRS 300  T-Stück 90 ° L665mm ","103289",665,null,"STK",659,{"$f":"IF(N238=0,\"\",IF(Daten!$F$390=\"90°\",N238,\"\"))","v":1},{"$f":"IF(L238=\"\",0,L238*H238)","v":665},{"$f":"Daten!$C$193","v":1},null,{"$f":"IF(L238=\"\",0,H238*L238)","v":665}]
["Kerastar",{"$f":"B238+1","v":11},{"$f":"C238","v":300},"Kerastar30011","4b","KRS 300  Anschlussrosette zu T-Stk. Øi 305mm","103296","0",null,"STK",170,{"$f":"IF(N238=0,\"\",N238)","v":1}]
["Kerastar",{"$f":"B239+1","v":12},{"$f":"C239","v":300},{"$f":"A240&C240&B240","v":"Kerastar30012"},"4d","KRS 300  Winkel 15 ° ","103336","0",null,"STK",508]
["Kerastar",{"$f":"B240+1","v":13},{"$f":"C240","v":300},"Kerastar30013","4e","KRS 300  Winkel 30 ° ","103343","0",null,"STK",534]
["Kerastar",{"$f":"B241+1","v":14},{"$f":"C241","v":300},"Kerastar30014","4f","KRS 300  Winkel 45 ° ","103350","0",null,"STK",534,null,null,"Stk RA-VL","RA-Verl."]
["Kerastar",{"$f":"B242+1","v":15},{"$f":"C242","v":300},"Kerastar30015","5a","KRS 300  Längenelement L665mm ","103308",665,null,"STK",339,{"$f":"ROUNDUP(M243,0)+N243","v":12},{"$f":"((M228-M229-M237-M238-M244-M245-M254+O244+O245)/H243)","v":11.732330827067669},{"$f":"O243/H243","v":0},{"$f":"Daten!$BY$161*1000","v":0},{"$f":"(IF(L243=\"\",0,H243*L243))-O243","v":7980}]
["Kerastar",16,300,"Kerastar30016","5b","KRS 300  Längenelement L330mm ","103315",331,null,"STK",271,{"$f":"IF(Daten!$CC$151=0,\"\",Daten!$CC$151)","v":1},{"$f":"IF(L244=\"\",0,L244*H244)","v":331},{"$f":"O244/H244","v":0},{"$f":"Daten!$BY$152*1000","v":0},{"$f":"(IF(L244=\"\",0,H244*L244))-O244","v":331}]
["Kerastar",17,300,"Kerastar30017","5c","KRS 300  Längenelement L165mm ","103322",165,null,"STK",231,{"$f":"IF(Daten!$CC$142=0,\"\",Daten!$CC$142)","v":""},{"$f":"IF(L245=\"\",0,L245*H245)","v":0},{"$f":"O245/H245","v":0},{"$f":"Daten!$BY$143*1000","v":0},{"$f":"(IF(L245=\"\",0,H245*L245))-O245","v":0}]
["Kerastar",18,300,"Kerastar30018","5d","ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",12,{"$f":"ROUNDUP(M246,0)","v":2},{"$f":"((M228/1000)*44)/310","v":1.4193548387096775}]
["Kerastar",{"$f":"B246+1","v":19},{"$f":"C246","v":300},"Kerastar30019","6b","KRS 300  Wandhalterung 50mm ","104659","0",null,"STK",61,{"$f":"ROUNDUP(M247,0)-N248","v":3},{"$f":"((M228/1000)/4.3)","v":2.3255813953488373}]
["Kerastar",{"$f":"B247+1","v":20},{"$f":"C247","v":300},"Kerastar30020","6d","KRS 300 Wandhalt.statisch 50mm","104657","0",null,"STK",112,{"$f":"IF(N248=0,\"\",N248)","v":""},null,{"$f":"IF(Daten!$A$479=2,1,0)","v":0}]
["Kerastar",{"$f":"B248+1","v":21},{"$f":"C248","v":300},"Kerastar30021","6c","ICS L1 Verlängerung zu Wandhalter 50mm L300mm","101254","0",null,"STK",66,{"$f":"IF(Daten!$B$410=2,L247+N248,\"\")","v":""},null,160]
["Kerastar",{"$f":"B249+1","v":22},{"$f":"C249","v":300},"Kerastar30022","6c","ICS L2 Verlängerung zu Wandhalter 50mm L450mm","101255","0",null,"STK",83,{"$f":"IF(Daten!$B$410=3,L247+N248,\"\")","v":""},null,310]
["Kerastar",23,300,"Kerastar30023","6c","ICS L3 Verlängerung zu Wandhalter 50mm L550mm","101256","0",null,"STK",95,{"$f":"IF(Daten!$B$410=4,L247+N248,\"\")","v":""},null,410]
["Kerastar",24,300,"Kerastar30024","6c","ICS L4 Verlängerung zu Wandhalter 50mm L750mm","101257","0",null,"STK",101,{"$f":"IF(Daten!$B$410=5,L247+N248,\"\")","v":""},null,610]
["Kerastar",25,300,"Kerastar30025",7,"KRS 450 Sparrenhalter ","103419","0",null,"STK",78,{"$f":"IF(Daten!$B$443=1,\"\",\"1\")","v":""}]
["Kerastar",26,300,"Kerastar30026","8a","KRS 300  Mündungsabschluss L207mm","103329",207,null,"STK",320,{"$f":"IF(Daten!$B$451=1,1,\"\")","v":1},{"$f":"IF(L254=\"\",0,L254*H254)","v":207},null,null,{"$f":"IF(L254=\"\",0,H254*L254)","v":207}]
["Kerastar",27,300,"Kerastar30027",null,"KRS 300 Basten Standard mit Stulpring Inox","103437","0",null,"STK",453,{"$f":"IF(Daten!$B$451=2,1,\"\")","v":""}]
["Kerastar",28,300,"Kerastar30028",null,"KRS 300 Basten Regulator mit Stulpring Inox","103443","0",null,"STK",553,{"$f":"IF(Daten!$B$451=3,1,\"\")","v":""}]
["Kerastar",29,300,{"$f":"A257&C257&B257","v":"Kerastar30029"},"9a",{"$f":"VLOOKUP(G257,sanschie!A:E,5,0)","v":"ICM 400 Dachdurführung 0° DN500 L500mm"},"102330","0",null,"STK",385,{"$f":"IF(Daten!$C$432=\"0 °\",1,\"\")","v":""}]
["Kerastar",30,300,"Kerastar30030","9c",{"$f":"VLOOKUP(G258,sanschie!A:E,5,0)","v":"ICM 400 Dachdurführung 16-25° DN500 mit Bleilappen"},"102342","0",null,"STK",581,{"$f":"IF(Daten!$C$432=\"16 ° - 25 °\",1,\"\")","v":""}]
["Kerastar",31,300,"Kerastar30031","9d",{"$f":"VLOOKUP(G259,sanschie!A:E,5,0)","v":"ICM 400 Dachdurführung 26-35° DN500 mit Bleilappen"},"102354","0",null,"STK",687,{"$f":"IF(Daten!$C$432=\"26 ° - 35 °\",1,\"\")","v":""}]
["Kerastar",32,300,"Kerastar30032","9e",{"$f":"VLOOKUP(G260,sanschie!A:E,5,0)","v":"ICM 400 Dachdurführung 36-45° DN500 mit Bleilappen"},"102366","0",null,"STK",729,{"$f":"IF(Daten!$C$432=\"36 ° - 45 °\",1,\"\")","v":""}]
["Kerastar",33,300,"Kerastar30033",10,"KRS Regenkragen        30","104665","0",null,"STK",87,{"$f":"IF(SUM(L257:L260)=1,1,\"\")","v":""}]
["Kerastar",34,300,"Kerastar30034","11a","KRS 300 Anschlussrosette Øi 450mm ØA 620mm","103357","0",null,"STK",49]
["Kerastar",{"$f":"B262+1","v":35},{"$f":"C262","v":300},{"$f":"A263&C263&B263","v":"Kerastar30035"},13,"KRS 300 Seilabspannring","104667","0",null,"STK",72]
["Kerastar",{"$f":"B263+1","v":36},{"$f":"C263","v":300},"Kerastar30036","14a","KRS 300 Statisches Klemmband","103401","0",null,"STK",72,{"$f":"IF(Daten!$B$479=2,2,\"\")","v":""}]
["Kerastar",0,400,"Kerastar4000","P","Kerastar Anlage Ø 400","Kerastar 400","0",{"$f":"Kerastar!$J$8","v":10},"Anlage",0,1,{"$f":"I265*1000","v":10000},null,{"$f":"ROUNDUP(P265,2)","v":10.18},{"$f":"SUM(P266:P298)/1000","v":10.178000000000001}]
["Kerastar",{"$f":"B265+1","v":1},{"$f":"C265","v":400},"Kerastar4001","1a","KRS 400 Fussteil Bodenmontage mit Ablauf L350mm","103251",330,null,"STK",641,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L266=\"\",0,L266*H266)","v":330},null,null,{"$f":"IF(L266=\"\",0,H266*L266)","v":330}]
["Kerastar",{"$f":"B266+1","v":2},{"$f":"C266","v":400},"Kerastar4002","1a","KRS Fusssteher-Set 4Stk. verstellbar L325-540mm","103252","0",null,"STK",422,{"$f":"IF(Daten!$B$401=1,1,\"\")","v":1},{"$f":"IF(L267=\"\",0,L267*H267)","v":0}]
["Kerastar",{"$f":"B267+1","v":3},{"$f":"C267","v":400},"Kerastar4003","2a","KRS 400 Grundplatte verstärkt mit Ablauf","103264",44,null,"STK",508,{"$f":"N268","v":""},null,{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""},{"$f":"IF(Daten!$B$410=1,\"\",1)","v":""}]
["Kerastar",4,400,"Kerastar4004","2c","KRS Wand-Konsole Typ 475mm (Paar)","103379","0",null,"STK",138,{"$f":"N269","v":""},null,{"$f":"IF(Daten!$B$410=1,O269,\"\")","v":""},{"$f":"IF(Daten!$B$401=2,1,\"\")","v":""}]
["Kerastar",5,400,"Kerastar4005","2c","KRS Wand-Konsole Typ 570mm (Paar)","103380","0",null,"STK",144,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$BC$401=3,\"\",IF(Daten!$B$410=2,1,\"\")))","v":""},null,278]
["Kerastar",6,400,"Kerastar4006","2c","KRS Wand-Konsole Typ 720mm (Paar)","103381","0",null,"STK",151,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=3,1,IF(Daten!$B$410=4,1,\"\"))))","v":""},null,428]
["Kerastar",7,400,"Kerastar4007","2c","KRS Wand-Konsole Typ 820mm (Paar)","103382","0",null,"STK",164,null,null,528]
["Kerastar",8,400,"Kerastar4008","2c","KRS Wand-Konsole Typ 1004mm (Paar)","103383","0",null,"STK",222,{"$f":"IF(Daten!$B$401=1,\"\",IF(Daten!$B$401=3,\"\",IF(Daten!$B$410=5,1,\"\")))","v":""},null,712]
["Kerastar",9,400,"Kerastar4009",3,"KRS 400  Revisionselement trocken- Betrieb L665mm","103276",665,null,"STK",1135,{"$f":"IF(N274=0,\"\",N274)","v":1},{"$f":"IF(N274=\"\",0,N274*H274)","v":665},{"$f":"Daten!$C$424","v":1},null,{"$f":"H274*N274","v":665}]
["Kerastar",10,400,"Kerastar40010","4a","KRS 400  T-Stück 90 ° L665mm ","103290",665,null,"STK",1186,{"$f":"IF(N275=0,\"\",IF(Daten!$F$390=\"90°\",N275,\"\"))","v":1},{"$f":"IF(L275=\"\",0,L275*H275)","v":665},{"$f":"Daten!$C$193","v":1},null,{"$f":"IF(L275=\"\",0,H275*L275)","v":665}]
["Kerastar",11,400,"Kerastar40011","4b","KRS 400  Anschlussrosette zu T-Stk. Øi 405mm","103297","0",null,"STK",189,{"$f":"IF(N275=0,\"\",N275)","v":1}]
["Kerastar",12,400,"Kerastar40012","4d","KRS 400  Winkel 15 ° ","103337","0",null,"STK",697]
["Kerastar",13,400,"Kerastar40013","4e","KRS 400  Winkel 30 ° ","103344","0",null,"STK",727]
["Kerastar",14,400,"Kerastar40014","4f","KRS 400  Winkel 45 ° ","103351","0",null,"STK",727,null,null,"Stk RA-VL","RA-Verl."]
["Kerastar",15,400,"Kerastar40015","5a","KRS 400  Längenelement L665mm ","103309",665,null,"STK",516,{"$f":"ROUNDUP(M280,0)+N280","v":12},{"$f":"((M265-M266-M274-M275-M281-M282-M291+O281+O282)/H280)","v":11.732330827067669},{"$f":"O280/H280","v":0},{"$f":"Daten!$BY$161*1000","v":0},{"$f":"(IF(L280=\"\",0,H280*L280))-O280","v":7980}]
["Kerastar",16,400,"Kerastar40016","5b","KRS 400  Längenelement L330mm ","103316",331,null,"STK",436,{"$f":"IF(Daten!$CC$151=0,\"\",Daten!$CC$151)","v":1},{"$f":"IF(L281=\"\",0,L281*H281)","v":331},{"$f":"O281/H281","v":0},{"$f":"Daten!$BY$152*1000","v":0},{"$f":"(IF(L281=\"\",0,H281*L281))-O281","v":331}]
["Kerastar",17,400,"Kerastar40017","5c","KRS 400  Längenelement L165mm ","103323",165,null,"STK",385,{"$f":"IF(Daten!$CC$142=0,\"\",Daten!$CC$142)","v":""},{"$f":"IF(L282=\"\",0,L282*H282)","v":0},{"$f":"O282/H282","v":0},{"$f":"Daten!$BY$143*1000","v":0},{"$f":"(IF(L282=\"\",0,H282*L282))-O282","v":0}]
["Kerastar",18,400,{"$f":"A283&C283&B283","v":"Kerastar40018"},"5d","ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",12,{"$f":"ROUNDUP(M283,0)","v":2},{"$f":"((M265/1000)*44)/310","v":1.4193548387096775}]
["Kerastar",19,400,{"$f":"A284&C284&B284","v":"Kerastar40019"},"6b","KRS 400  Wandhalterung 50mm ","104660","0",null,"STK",76,{"$f":"ROUNDUP(M284,0)-N285","v":3},{"$f":"((M265/1000)/4.3)","v":2.3255813953488373}]
["Kerastar",20,400,"Kerastar40020","6d","KRS 400 Wandhalt.statisch 50mm","104658","0",null,"STK",132,{"$f":"IF(N285=0,\"\",N285)","v":""},null,{"$f":"IF(Daten!$A$479=2,1,0)","v":0}]
["Kerastar",21,400,"Kerastar40021","6c","ICS L1 Verlängerung zu Wandhalter 50mm L300mm","101254","0",null,"STK",66,{"$f":"IF(Daten!$B$410=2,L284+N285,\"\")","v":""},null,160]
["Kerastar",22,400,"Kerastar40022","6c","ICS L2 Verlängerung zu Wandhalter 50mm L450mm","101255","0",null,"STK",83,{"$f":"IF(Daten!$B$410=3,L284+N285,\"\")","v":""},null,310]
["Kerastar",23,400,"Kerastar40023","6c","ICS L3 Verlängerung zu Wandhalter 50mm L550mm","101256","0",null,"STK",95,{"$f":"IF(Daten!$B$410=4,L284+N285,\"\")","v":""},null,410]
["Kerastar",24,400,"Kerastar40024","6c","ICS L4 Verlängerung zu Wandhalter 50mm L750mm","101257","0",null,"STK",101,{"$f":"IF(Daten!$B$410=5,L284+N285,\"\")","v":""},null,610]
["Kerastar",25,400,"Kerastar40025",7,"KRS 550 Sparrenhalter ","103420","0",null,"STK",114,{"$f":"IF(Daten!$B$443=1,\"\",\"1\")","v":""}]
["Kerastar",26,400,"Kerastar40026","8a","KRS 400  Mündungsabschluss L207mm","103330",207,null,"STK",388,{"$f":"IF(Daten!$B$451=1,1,\"\")","v":1},{"$f":"IF(L291=\"\",0,L291*H291)","v":207},null,null,{"$f":"IF(L291=\"\",0,H291*L291)","v":207}]
["Kerastar",{"$f":"B291+1","v":27},{"$f":"C291","v":400},{"$f":"A292&C292&B292","v":"Kerastar40027"},"9a",{"$f":"VLOOKUP(G292,sanschie!A:E,5,0)","v":"ICM 500 Dachdurführung 0° DN600 L500mm"},"102332","0",null,"STK",512,{"$f":"IF(Daten!$C$432=\"0 °\",1,\"\")","v":""}]
["Kerastar",{"$f":"B292+1","v":28},{"$f":"C292","v":400},"Kerastar40028","9c",{"$f":"VLOOKUP(G293,sanschie!A:E,5,0)","v":"ICM 500 Dachdurführung 16-25° DN600 mit Bleilappen"},"102344","0",null,"STK",722,{"$f":"IF(Daten!$C$432=\"16 ° - 25 °\",1,\"\")","v":""}]
["Kerastar",{"$f":"B293+1","v":29},{"$f":"C293","v":400},"Kerastar40029","9d",{"$f":"VLOOKUP(G294,sanschie!A:E,5,0)","v":"ICM 500 Dachdurführung 26-35° DN600 mit Bleilappen"},"102356","0",null,"STK",798,{"$f":"IF(Daten!$C$432=\"26 ° - 35 °\",1,\"\")","v":""}]
["Kerastar",{"$f":"B294+1","v":30},{"$f":"C294","v":400},"Kerastar40030","9e",{"$f":"VLOOKUP(G295,sanschie!A:E,5,0)","v":"ICM 500 Dachdurführung 36-45° DN600 mit Bleilappen"},"102368","0",null,"STK",848,{"$f":"IF(Daten!$C$432=\"36 ° - 45 °\",1,\"\")","v":""}]
["Kerastar",31,400,"Kerastar40031",10,"KRS Regenkragen        40","104666","0",null,"STK",95,{"$f":"IF(SUM(L292:L295)=1,1,\"\")","v":""}]
["Kerastar",32,400,"Kerastar40032","11a","KRS 400 Anschlussrosette Øi 550mm ØA 720mm","103358","0",null,"STK",59]
["Kerastar",33,400,"Kerastar40033",13,"KRS 400 Seilabspannring","104668","0",null,"STK",80]
["Kerastar",34,400,"Kerastar40034","14a","KRS 400 Statisches Klemmband","103402","0",null,"STK",80,{"$f":"IF(Daten!$B$479=2,2,\"\")","v":""}]
["Keranova",0,120,{"$f":"A300&C300&B300","v":"Keranova1200"},null,"Keranova Anlage Ø 120","Keranova 120","0",{"$f":"Keranova!$J$12","v":11},"Anlage",0,1,{"$f":"I300*1000","v":11000},null,{"$f":"ROUNDUP(P300,2)","v":11.31},{"$f":"SUM(P301:P340)/1000","v":11.305999999999999}]
["Keranova",{"$f":"B300+1","v":1},{"$f":"C300","v":120},"Keranova1201",null,"KER 120 Keranova-Rohr komplett L1330mm ","103454",1330,null,"STK",116,{"$f":"ROUNDUP(M301,0)","v":8},{"$f":"(M300-M303-M302-M311-M326)/H301","v":7.7706766917293235},null,null,{"$f":"H301*L301","v":10640}]
["Keranova",2,120,"Keranova1202",null,"KER 120 Keranova-Rohr komplett L660mm ","103459",665,null,"STK",80,{"$f":"1+Keranova!$P$20","v":1},{"$f":"IF(H302=0,\"\",L302*H302)","v":665},null,null,{"$f":"H302*L302","v":665}]
["Keranova",3,120,"Keranova1203",null,"KER 120 Kondensattopf komplett L132mm","103445","0",null,"STK",75,1,{"$f":"IF(H303=0,\"\",L303*H303)","v":0},null,null,{"$f":"H303*L303","v":0}]
["Keranova",4,120,"Keranova1204",null,"KER 120 T-Stück 90° L330mm Stutzen L90mm","103482",330,null,"STK",184,null,{"$f":"IF(H304=0,\"\",L304*H304)","v":0},null,null,{"$f":"H304*L304","v":0}]
["Keranova",{"$f":"B304+1","v":5},{"$f":"C304","v":120},{"$f":"A305&C305&B305","v":"Keranova1205"},null,"KER 120 Universalstutzen 0°","103492","0",null,"STK",68,{"$f":"IF(N305=0,\"\",N305)","v":3},null,{"$f":"SUM(O305:P305)","v":3},{"$f":"IF(Daten!$B$573=1,0,Daten!$C$573)","v":2},{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$B$591=2,0,Daten!$C$193))","v":1}]
["Keranova",6,120,"Keranova1206",null,"KER 120 Revisionsdeckel für Festbrennstoff","103511","0",null,"STK",46,{"$f":"IF(Daten!$B$573=0,\"\",IF(Daten!$B$582=3,Daten!$C$573,IF(Daten!$B$582=4,Daten!$C$573,\"\")))","v":2}]
["Keranova",7,120,"Keranova1207",null,"KER 120 Revisionsdeckel für Oel/Gas","103506","0",null,"STK",80,{"$f":"IF(Daten!$B$573=1,\"\",IF(Daten!$B$582=3,\"\",IF(Daten!$B$582=4,\"\",Daten!$C$573)))","v":""}]
["Keranova",8,120,"Keranova1208",null,"KER 120 Universalstutzen 45°","103499","0",null,"STK",96,{"$f":"IF(N308=0,\"\",N308)","v":""},null,{"$f":"SUM(O308:P308)","v":0},null,{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$C$591=\"90°\",0,Daten!$C$193))","v":0}]
["Keranova",9,120,"Keranova1209",null,"KER 120 Anreisschablone Universal","103517","0",null,"STK",89]
["Keranova",10,120,"Keranova12010",null,"PPL Schachtabdeckung Typ1 350 x 350mm","101272","0",null,"STK",86,1]
["Keranova",11,120,"Keranova12011",null,"KER 120 Mündungskonus","103608","0",null,"STK",69,1]
["Keranova",12,120,"Keranova12012",null,"ABS 120 Steckadapter Ø140","104266","0",null,"STK",129]
["Keranova",13,120,"Keranova12013",null,"KER 80-120 Anschlussblende mit Gummi-Einlage","103577","0",null,"STK",82]
["Keranova",14,120,"Keranova12014",null,"KER 130 Zugbegrenzer mit Explosionsklappe","103546","0",null,"STK",217]
["Keranova",15,120,"Keranova12015",null,"KER 130 Adapter für Zugbegrenzer für DN120mm","103548","0",null,"STK",41]
["Keranova",16,120,"Keranova12016",null,"KER 130 Mauerschelle","103601","0",null,"STK",15,{"$f":"IF(Daten!$C$573=2,1,\"\")","v":1}]
["Keranova",17,120,"Keranova12017",null,"KER 120 Statische-Manchette für Muffenverbindungen","103529","0",null,"STK",33]
["Keranova",18,120,"Keranova12018",null,"KER 120 Bogen verstellbar 0-30° L660mm","103523",660,null,"STK",298]
["Keranova",19,120,"Keranova12019",null,"KER 120 Statische-Abstützung für Bogen-Verstellbar","103535","0",null,"STK",66]
["Keranova",20,120,"Keranova12020",null,"KER 120 Abdeckblende 250 x 250mm","103573","0",null,"STK",20]
["Keranova",21,120,"Keranova12021",null,"KER 120  Keranova-Fugenglätter","103471","0",null,"STK",45]
["Keranova",22,120,"Keranova12022",null,"KER 120 Verbindungsmanchette inkl. Abstandhalter","103465","0",null,"STK",35]
["Keranova",23,120,"Keranova12023",null,"KER 120 Adapter für Doppelfutter 120mm","103555","0",null,"STK",46,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",24,120,"Keranova12024",null,"KER 120 Doppelfutter 120mm","103566","0",null,"STK",48,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",25,120,"Keranova12025",null,"KER 120 Adapter für Doppelfutter 120mm","103555","0",null,"STK",46,{"$f":"IF(Daten!$B$600=3,1,\"\")","v":""}]
["Keranova",26,120,"Keranova12026",null,"KER 130 Doppelfutter 120mm","103567","0",null,"STK",53,{"$f":"IF(Daten!$B$600=3,1,\"\")","v":""}]
["Keranova",27,120,"Keranova12027",null,"KER Putztür PTS1 145 x 275mm Alu bis  Ø120","103594","0",null,"STK",92,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",28,120,"Keranova12028",null,"KER Schieberahmen zu PTS1 145 x 275 mm L90mm","103595","0",null,"STK",20,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",29,120,"Keranova12029",null,"CHZ 120-180 Zuluftgitter für Hinterlüftung ","103817","0",null,"STK",24]
["Keranova",30,120,"Keranova12030",null,"KER 40 Siphon kompl.  für Schlauchanschluss DN32mm","103453","0",null,"STK",48,1]
["Keranova",31,120,"Keranova12031",null,"KER 32 PP Kondensatrohr-Erweiterung auf DN40 L50mm","103451","0",null,"STK",12,1]
["Keranova",32,120,"Keranova12032",null,"KER 40 PP Winkel 90° für Schlauchanschluss DN32mm","103452","0",null,"STK",56]
["Keranova",33,120,"Keranova12033",null,"KER 80-250 Ablasswinde schwer","103617","0",null,"STK",1552]
["Keranova",34,120,"Keranova12034",null,"KER 80-200 Ablasswinde leicht ","103618","0",null,"STK",1458]
["Keranova",35,120,"Keranova12035",null,"KER 80-160 Rollenbock ","103619","0",null,"STK",204]
["Keranova",36,120,"Keranova12036",null,"KER 160-250 Rollenbock","103620","0",null,"STK",204]
["Keranova",37,120,"Keranova12037",null,"KER 120-250 Versetzzange ","103622","0",null,"STK",1463]
["Keranova",38,120,"Keranova12038",null,"KER Rotempo Fugendichtmasse Kartusche a 310ml","103614","0",null,"STK",34,{"$f":"IF(Daten!$B$564=2,ROUNDUP(M338,0)+N305+N308,\"\")","v":""},{"$f":"((O300)*40)/310","v":1.4593548387096775}]
["Keranova",39,120,"Keranova12039",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",12]
["Keranova",40,120,"Keranova12040",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",14,{"$f":"IF(M340=0,\"\",(ROUNDUP(M340,0)+N305+N308))","v":5},{"$f":"IF(Daten!$B$564=1,((O300)*44)/310,0)","v":1.6052903225806452}]
["Keranova",41,120,{"$f":"A341&C341&B341","v":"Keranova12041"},null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",6.2]
["Keranova",42,120,{"$f":"A342&C342&B342","v":"Keranova12042"},null,"Neutralisationsbox komplett","100265","0",null,"STK",225]
["Keranova",43,120,{"$f":"A343&C343&B343","v":"Keranova12043"},null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",39]
["Keranova",0,140,"Keranova1400",null,"Keranova Anlage Ø 140","Keranova 140","0",{"$f":"Keranova!$J$12","v":11},"Anlage",0,1,{"$f":"I344*1000","v":11000},null,{"$f":"ROUNDUP(P344,2)","v":11.31},{"$f":"SUM(P345:P387)/1000","v":11.305999999999999}]
["Keranova",{"$f":"B344+1","v":1},{"$f":"C344","v":140},"Keranova1401",null,"KER 140 Keranova-Rohr komplett L1330mm ","103455",1330,null,"STK",123,{"$f":"ROUNDUP(M345,0)","v":8},{"$f":"(M344-M348-M346-M357-M373)/H345","v":7.7706766917293235},null,null,{"$f":"H345*L345","v":10640}]
["Keranova",2,140,"Keranova1402",null,"KER 140 Keranova-Rohr komplett L660mm ","103460",665,null,"STK",83,{"$f":"1+Keranova!$P$20","v":1},{"$f":"IF(H346=0,\"\",L346*H346)","v":665},null,null,{"$f":"H346*L346","v":665}]
["Keranova",3,140,"Keranova1403",null,"KER 140 Dämmrohr Klappmatte L660mm","103477","0",null,"STK",52]
["Keranova",4,140,"Keranova1404",null,"KER 140 Kondensattopf komplett L132mm","103446","0",null,"STK",83,1,{"$f":"IF(H348=0,\"\",L348*H348)","v":0},null,null,{"$f":"H348*L348","v":0}]
["Keranova",{"$f":"B348+1","v":5},{"$f":"C348","v":140},{"$f":"A349&C349&B349","v":"Keranova1405"},null,"KER 140 T-Stück 90° L330mm Stutzen L90mm","103483",330,null,"STK",194,null,{"$f":"IF(H349=0,\"\",L349*H349)","v":0},null,null,{"$f":"H349*L349","v":0}]
["Keranova",6,140,"Keranova1406",null,"KER 140 Revisionsdeckel zu T-Stück Festbrennstoffe","103488","0",null,"STK",47]
["Keranova",7,140,"Keranova1407",null,"KER 140 Universalstutzen 0°","103493","0",null,"STK",70,{"$f":"IF(N351=0,\"\",N351)","v":3},null,{"$f":"SUM(O351:P351)","v":3},{"$f":"IF(Daten!$B$573=1,0,Daten!$C$573)","v":2},{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$B$591=2,0,Daten!$C$193))","v":1}]
["Keranova",8,140,"Keranova1408",null,"KER 140 Revisionsdeckel für Festbrennstoff","103512","0",null,"STK",47,{"$f":"IF(Daten!$B$573=0,\"\",IF(Daten!$B$582=3,Daten!$C$573,IF(Daten!$B$582=4,Daten!$C$573,\"\")))","v":2}]
["Keranova",9,140,"Keranova1409",null,"KER 140 Revisionsdeckel für Oel/Gas","103507","0",null,"STK",81,{"$f":"IF(Daten!$B$573=1,\"\",IF(Daten!$B$582=3,\"\",IF(Daten!$B$582=4,\"\",Daten!$C$573)))","v":""}]
["Keranova",10,140,"Keranova14010",null,"KER 140 Universalstutzen 45°","103500","0",null,"STK",97,{"$f":"IF(N354=0,\"\",N354)","v":""},null,{"$f":"SUM(O354:P354)","v":0},null,{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$C$591=\"90°\",0,Daten!$C$193))","v":0}]
["Keranova",11,140,"Keranova14011",null,"KER 140 Anreisschablone Universal","103518","0",null,"STK",93]
["Keranova",12,140,"Keranova14012",null,"PPL Schachtabdeckung Typ2 400 x 400mm","101273","0",null,"STK",97,1]
["Keranova",13,140,"Keranova14013",null,"KER 140 Mündungskonus","103609","0",null,"STK",69,1]
["Keranova",14,140,"Keranova14014",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",139,{"$f":"IF(Daten!C600=\"Steckadapter\",1,\"\")","v":""}]
["Keranova",15,140,"Keranova14015",null,"KER 140-160 Anschlussblende mit Gummi-Einlage","103578","0",null,"STK",94]
["Keranova",{"$f":"B359+1","v":16},{"$f":"C359","v":140},"Keranova14016",null,"KER 130 Zugbegrenzer mit Explosionsklappe","103546","0",null,"STK",217]
["Keranova",{"$f":"B360+1","v":17},{"$f":"C360","v":140},"Keranova14017",null,"KER 130 Adapter für Zugbegrenzer für DN140mm","103549","0",null,"STK",41]
["Keranova",18,140,"Keranova14018",null,"KER 140 Universal-Kachelofenzargenset 120 x 120mm","103541","0",null,"STK",183]
["Keranova",19,140,"Keranova14019",null,"KER 140 Mauerschelle","103602","0",null,"STK",21,{"$f":"IF(Daten!$C$573=2,1,\"\")","v":1}]
["Keranova",20,140,"Keranova14020",null,"KER 140 Statische-Manchette für Muffenverbindungen","103530","0",null,"STK",35]
["Keranova",21,140,"Keranova14021",null,"KER 140 Bogen verstellbar 0-30° L660mm","103524",660,null,"STK",317]
["Keranova",22,140,{"$f":"A366&C366&B366","v":"Keranova14022"},null,"KER 140 Statische-Abstützung für Bogen-Verstellbar","103536","0",null,"STK",67]
["Keranova",23,140,"Keranova14023",null,"KER 140 Abdeckblende 340 x 340mm","103574","0",null,"STK",26]
["Keranova",24,140,"Keranova14024",null,"KER 140  Keranova-Fugenglätter","103472","0",null,"STK",49]
["Keranova",25,140,"Keranova14025",null,"KER 140 Verbindungsmanchette inkl. Abstandhalter","103466","0",null,"STK",36]
["Keranova",26,140,"Keranova14026",null,"KER 140 Adapter für Doppelfutter 130mm","103557","0",null,"STK",56,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",27,140,"Keranova14027",null,"KER 130 Doppelfutter 130mm","103568","0",null,"STK",62,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",28,140,"Keranova14028",null,"KER 140 Adapter für Doppelfutter 150mm","103558","0",null,"STK",56,{"$f":"IF(Daten!$B$600=3,1,\"\")","v":""}]
["Keranova",29,140,"Keranova14029",null,"KER 150 Doppelfutter 150mm","103569","0",null,"STK",65,{"$f":"IF(Daten!$B$600=3,1,\"\")","v":""}]
["Keranova",30,140,"Keranova14030",null,"KER Putztür PTS2 200 x 275mm Alu für  Ø140- 250mm","103596","0",null,"STK",112,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",31,140,"Keranova14031",null,"KER Schieberahmen zu PTS2 200 x 275mm L90mm","103597","0",null,"STK",21,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",32,140,"Keranova14032",null,"CHZ 200-300 Zuluftgitter für Hinterlüftung","103818","0",null,"STK",38]
["Keranova",33,140,"Keranova14033",null,"KER 40 Siphon kompl.  für Schlauchanschluss DN32mm","103453","0",null,"STK",48,1]
["Keranova",34,140,"Keranova14034",null,"KER 32 PP Kondensatrohr-Erweiterung auf DN40 L50mm","103451","0",null,"STK",12,1]
["Keranova",35,140,"Keranova14035",null,"KER 40 PP Winkel 90° für Schlauchanschluss DN32mm","103452","0",null,"STK",56]
["Keranova",36,140,"Keranova14036",null,"KER 80-250 Ablasswinde schwer","103617","0",null,"STK",1552]
["Keranova",37,140,"Keranova14037",null,"KER 80-200 Ablasswinde leicht ","103618","0",null,"STK",1458]
["Keranova",38,140,"Keranova14038",null,"KER 80-160 Rollenbock ","103619","0",null,"STK",204]
["Keranova",39,140,"Keranova14039",null,"KER 160-250 Rollenbock","103620","0",null,"STK",204]
["Keranova",40,140,"Keranova14040",null,"KER 120-250 Versetzzange ","103622","0",null,"STK",1463]
["Keranova",41,140,"Keranova14041",null,"KER Rotempo Fugendichtmasse Kartusche a 310ml","103614","0",null,"STK",34,{"$f":"IF(Daten!$B$564=2,ROUNDUP(M385,0)+N354+N355,\"\")","v":""},{"$f":"((O344)*55)/310","v":2.0066129032258067}]
["Keranova",42,140,"Keranova14042",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",12]
["Keranova",43,140,"Keranova14043",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",14,{"$f":"IF(M387=0,\"\",(ROUNDUP(M387,0)+N351+N354))","v":6},{"$f":"IF(Daten!$B$564=1,((O344)*60)/310,0)","v":2.1890322580645161}]
["Keranova",44,140,"Keranova14044",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",6.2]
["Keranova",45,140,"Keranova14045",null,"Neutralisationsbox komplett","100265","0",null,"STK",225]
["Keranova",46,140,"Keranova14046",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",39]
["Keranova",0,160,"Keranova1600",null,"Keranova Anlage Ø 160","Keranova 160","0",{"$f":"Keranova!$J$12","v":11},"Anlage",0,1,{"$f":"I391*1000","v":11000},null,{"$f":"ROUNDUP(P391,2)","v":11.31},{"$f":"SUM(P392:P434)/1000","v":11.305999999999999}]
["Keranova",{"$f":"B391+1","v":1},{"$f":"C391","v":160},"Keranova1601",null,"KER 160 Keranova-Rohr komplett L1330mm ","103456",1330,null,"STK",131,{"$f":"ROUNDUP(M392,0)","v":8},{"$f":"(M391-M395-M393-M404-M420)/H392","v":7.7706766917293235},null,null,{"$f":"H392*L392","v":10640}]
["Keranova",2,160,"Keranova1602",null,"KER 160 Keranova-Rohr komplett L660mm ","103461",665,null,"STK",87,{"$f":"1+Keranova!$P$20","v":1},{"$f":"IF(H393=0,\"\",L393*H393)","v":665},null,null,{"$f":"H393*L393","v":665}]
["Keranova",3,160,"Keranova1603",null,"KER 160 Dämmrohr Klappmatte L660mm","103478","0",null,"STK",56]
["Keranova",4,160,"Keranova1604",null,"KER 160 Kondensattopf komplett L132mm","103447","0",null,"STK",98,1,{"$f":"IF(H395=0,\"\",L395*H395)","v":0},null,null,{"$f":"H395*L395","v":0}]
["Keranova",{"$f":"B395+1","v":5},{"$f":"C395","v":160},"Keranova1605",null,"KER 160 T-Stück 90° L330mm Stutzen L90mm","103484",330,null,"STK",207,null,{"$f":"IF(H396=0,\"\",L396*H396)","v":0},null,null,{"$f":"H396*L396","v":0}]
["Keranova",{"$f":"B396+1","v":6},{"$f":"C396","v":160},{"$f":"A397&C397&B397","v":"Keranova1606"},null,"KER 160 Revisionsdeckel zu T-Stück Festbrennstoffe","103489","0",null,"STK",50]
["Keranova",7,160,{"$f":"A398&C398&B398","v":"Keranova1607"},null,"KER 160 Universalstutzen 0°","103494","0",null,"STK",78,{"$f":"IF(N398=0,\"\",N398)","v":3},null,{"$f":"SUM(O398:P398)","v":3},{"$f":"IF(Daten!$B$573=1,0,Daten!$C$573)","v":2},{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$B$591=2,0,Daten!$C$193))","v":1}]
["Keranova",8,160,"Keranova1608",null,"KER 160 Revisionsdeckel für Festbrennstoff","103513","0",null,"STK",50,{"$f":"IF(Daten!$B$573=0,\"\",IF(Daten!$B$582=3,Daten!$C$573,IF(Daten!$B$582=4,Daten!$C$573,\"\")))","v":2}]
["Keranova",9,160,"Keranova1609",null,"KER 160 Revisionsdeckel für Oel/Gas","103508","0",null,"STK",88,{"$f":"IF(Daten!$B$573=1,\"\",IF(Daten!$B$582=3,\"\",IF(Daten!$B$582=4,\"\",Daten!$C$573)))","v":""}]
["Keranova",10,160,"Keranova16010",null,"KER 160 Universalstutzen 45°","103501","0",null,"STK",108,{"$f":"IF(N401=0,\"\",N401)","v":""},null,{"$f":"SUM(O401:P401)","v":0},null,{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$C$591=\"90°\",0,Daten!$C$193))","v":0}]
["Keranova",11,160,"Keranova16011",null,"KER 160 Anreisschablone Universal","103519","0",null,"STK",98]
["Keranova",12,160,"Keranova16012",null,"PPL Schachtabdeckung Typ2 400 x 400mm","101273","0",null,"STK",97,{"$f":"IF(N403=0,1,\"\")","v":1},null,{"$f":"SUM(L435:L438)","v":0}]
["Keranova",13,160,"Keranova16013",null,"KER 160 Mündungskonus","103610","0",null,"STK",73,{"$f":"IF(N404=0,1,\"\")","v":1},null,{"$f":"SUM(L435:L438)","v":0}]
["Keranova",14,160,"Keranova16014",null,"ABS 180 Steckadapter ","104268","0",null,"STK",150]
["Keranova",15,160,"Keranova16015",null,"KER 140-160 Anschlussblende mit Gummi-Einlage","103578","0",null,"STK",94]
["Keranova",16,160,"Keranova16016",null,"KER 130 Zugbegrenzer mit Explosionsklappe","103546","0",null,"STK",217]
["Keranova",17,160,"Keranova16017",null,"KER 130 Adapter für Zugbegrenzer für DN160mm","103550","0",null,"STK",41]
["Keranova",18,160,"Keranova16018",null,"KER 160 Universal-Kachelofenzargenset 150 x 150mm","103542","0",null,"STK",183]
["Keranova",19,160,"Keranova16019",null,"KER 160 Mauerschelle","103603","0",null,"STK",21,{"$f":"IF(Daten!$C$573=2,1,\"\")","v":1}]
["Keranova",20,160,"Keranova16020",null,"KER 160 Statische-Manchette für Muffenverbindungen","103531","0",null,"STK",38]
["Keranova",21,160,"Keranova16021",null,"KER 160 Bogen verstellbar 0-30° L660mm","103525",660,null,"STK",343]
["Keranova",22,160,"Keranova16022",null,"KER 160 Statische-Abstützung für Bogen-Verstellbar","103537","0",null,"STK",69]
["Keranova",23,160,"Keranova16023",null,"KER 160-180 Abdeckblende 340 x 340mm","103575","0",null,"STK",26]
["Keranova",24,160,"Keranova16024",null,"KER 160  Keranova-Fugenglätter","103473","0",null,"STK",50]
["Keranova",25,160,"Keranova16025",null,"KER 160 Verbindungsmanchette inkl. Abstandhalter","103467","0",null,"STK",37]
["Keranova",26,160,"Keranova16026",null,"KER 160 Adapter für Doppelfutter 150mm","103559","0",null,"STK",59,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",27,160,"Keranova16027",null,"KER 150 Doppelfutter 150mm","103569","0",null,"STK",65,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",28,160,"Keranova16028",null,"KER 160 Adapter für Doppelfutter 180mm","103560","0",null,"STK",67,{"$f":"IF(Daten!$B$600=3,1,\"\")","v":""}]
["Keranova",29,160,"Keranova16029",null,"KER 180 Doppelfutter 180mm","103570","0",null,"STK",69,{"$f":"IF(Daten!$B$600=3,1,\"\")","v":""}]
["Keranova",30,160,"Keranova16030",null,"KER Putztür PTS2 200 x 275mm Alu für  Ø140- 250mm","103596","0",null,"STK",112,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",31,160,"Keranova16031",null,"KER Schieberahmen zu PTS2 200 x 275mm L90mm","103597","0",null,"STK",21,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",32,160,"Keranova16032",null,"CHZ 120-180 Zuluftgitter für Hinterlüftung ","103817","0",null,"STK",24]
["Keranova",33,160,"Keranova16033",null,"KER 40 Siphon kompl.  für Schlauchanschluss DN32mm","103453","0",null,"STK",48,1]
["Keranova",34,160,"Keranova16034",null,"KER 32 PP Kondensatrohr-Erweiterung auf DN40 L50mm","103451","0",null,"STK",12,1]
["Keranova",35,160,"Keranova16035",null,"KER 40 PP Winkel 90° für Schlauchanschluss DN32mm","103452","0",null,"STK",56]
["Keranova",36,160,"Keranova16036",null,"KER 80-250 Ablasswinde schwer","103617","0",null,"STK",1552]
["Keranova",37,160,"Keranova16037",null,"KER 80-200 Ablasswinde leicht ","103618","0",null,"STK",1458]
["Keranova",38,160,"Keranova16038",null,"KER 80-160 Rollenbock ","103619","0",null,"STK",204]
["Keranova",39,160,{"$f":"A430&C430&B430","v":"Keranova16039"},null,"KER 160-250 Rollenbock","103620","0",null,"STK",204]
["Keranova",40,160,"Keranova16040",null,"KER 120-250 Versetzzange ","103622","0",null,"STK",1463]
["Keranova",41,160,"Keranova16041",null,"KER Rotempo Fugendichtmasse Kartusche a 310ml","103614","0",null,"STK",34,{"$f":"IF(Daten!$B$564=2,ROUNDUP(M432,0)+N398+N401,\"\")","v":""},{"$f":"((O391)*70)/310","v":2.5538709677419358}]
["Keranova",42,160,"Keranova16042",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",12]
["Keranova",43,160,"Keranova16043",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",14,{"$f":"IF(M434=0,\"\",(ROUNDUP(M434,0)+N398+N401))","v":6},{"$f":"IF(Daten!$B$564=1,((O391)*75)/310,0)","v":2.7362903225806452}]
["Keranova",44,160,{"$f":"A435&C435&B435","v":"Keranova16044"},null,"ABS 160 Basten Standard Inox","104211","0",null,"STK",302,{"$f":"IF(N435=0,\"\",N435)","v":""},null,{"$f":"IF(Daten!$B$618=2,1,0)","v":0}]
["Keranova",45,160,"Keranova16045",null,"ABS 160 Basten Standard Kupfer","104217","0",null,"STK",323,{"$f":"IF(N436=0,\"\",N436)","v":""},null,{"$f":"IF(Daten!$B$618=3,1,0)","v":0}]
["Keranova",46,160,"Keranova16046",null,"ABS 160 Sairlift Inox","104223","0",null,"STK",325,{"$f":"IF(N437=0,\"\",N437)","v":""},null,{"$f":"IF(Daten!$B$618=4,1,0)","v":0}]
["Keranova",47,160,"Keranova16047",null,"ABS 160 Sairlift Kupfer","104228","0",null,"STK",345,{"$f":"IF(N438=0,\"\",N438)","v":""},null,{"$f":"IF(Daten!$B$618=5,1,0)","v":0}]
["Keranova",48,160,"Keranova16048",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",6.2]
["Keranova",49,160,"Keranova16049",null,"Neutralisationsbox komplett","100265","0",null,"STK",225]
["Keranova",50,160,"Keranova16050",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",39]
["Keranova",0,180,"Keranova1800","P","Keranova Anlage Ø 180","Keranova 180","0",{"$f":"Keranova!$J$12","v":11},"Anlage",0,1,{"$f":"I442*1000","v":11000},null,{"$f":"ROUNDUP(P442,2)","v":11.31},{"$f":"SUM(P443:P485)/1000","v":11.305999999999999}]
["Keranova",{"$f":"B442+1","v":1},{"$f":"C442","v":180},"Keranova1801"," ","KER 180 Keranova-Rohr komplett L1330mm ","103457",1330,null,"STK",143,{"$f":"ROUNDUP(M443,0)","v":8},{"$f":"(M442-M446-M444-M455-M471)/H443","v":7.7706766917293235},null,null,{"$f":"H443*L443","v":10640}]
["Keranova",2,180,"Keranova1802"," ","KER 180 Keranova-Rohr komplett L660mm ","103462",665,null,"STK",97,{"$f":"1+Keranova!$P$20","v":1},{"$f":"IF(H444=0,\"\",L444*H444)","v":665},null,null,{"$f":"H444*L444","v":665}]
["Keranova",3,180,"Keranova1803"," ","KER 180 Dämmrohr Klappmatte L660mm","103479","0",null,"STK",57]
["Keranova",{"$f":"B445+1","v":4},{"$f":"C445","v":180},"Keranova1804"," ","KER 180 Kondensattopf komplett L145mm","103448","0",null,"STK",105,1,{"$f":"IF(H446=0,\"\",L446*H446)","v":0},null,null,{"$f":"H446*L446","v":0}]
["Keranova",5,180,"Keranova1805"," ","KER 180 T-Stück 90° L330mm Stutzen L90mm","103485",330,null,"STK",224,null,{"$f":"IF(H447=0,\"\",L447*H447)","v":0},null,null,{"$f":"H447*L447","v":0}]
["Keranova",6,180,{"$f":"A448&C448&B448","v":"Keranova1806"},null,"KER 180 Revisionsdeckel zu T-Stück Festbrennstoffe","103490","0",null,"STK",53]
["Keranova",7,180,{"$f":"A449&C449&B449","v":"Keranova1807"}," ","KER 180 Universalstutzen 0°","103495","0",null,"STK",83,{"$f":"IF(N449=0,\"\",N449)","v":3},null,{"$f":"SUM(O449:P449)","v":3},{"$f":"IF(Daten!$B$573=1,0,Daten!$C$573)","v":2},{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$B$591=2,0,Daten!$C$193))","v":1}]
["Keranova",8,180,"Keranova1808"," ","KER 180 Revisionsdeckel für Festbrennstoff","103514","0",null,"STK",53,{"$f":"IF(Daten!$B$573=0,\"\",IF(Daten!$B$582=3,Daten!$C$573,IF(Daten!$B$582=4,Daten!$C$573,\"\")))","v":2}]
["Keranova",9,180,"Keranova1809"," ","KER 180 Revisionsdeckel für Oel/Gas","103509","0",null,"STK",94,{"$f":"IF(Daten!$B$573=1,\"\",IF(Daten!$B$582=3,\"\",IF(Daten!$B$582=4,\"\",Daten!$C$573)))","v":""}]
["Keranova",10,180,"Keranova18010"," ","KER 180 Universalstutzen 45°","103502","0",null,"STK",112,{"$f":"IF(N452=0,\"\",N452)","v":""},null,{"$f":"SUM(O452:P452)","v":0},null,{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$C$591=\"90°\",0,Daten!$C$193))","v":0}]
["Keranova",11,180,"Keranova18011"," ","KER 180 Anreisschablone Universal","103520","0",null,"STK",104]
["Keranova",12,180,"Keranova18012"," ","PPL Schachtabdeckung Typ3 450 x 450mm","101274","0",null,"STK",119,{"$f":"IF(N454=0,1,\"\")","v":1},null,{"$f":"SUM(L486:L489)","v":0}]
["Keranova",13,180,{"$f":"A455&C455&B455","v":"Keranova18013"}," ","KER 180 Mündungskonus","103611","0",null,"STK",74,{"$f":"IF(N455=0,1,\"\")","v":1},null,{"$f":"SUM(L486:L489)","v":0}]
["Keranova",14,180,"Keranova18014"," ","ABS 200 Steckadapter ","104269","0",null,"STK",160]
["Keranova",15,180,"Keranova18015"," ","KER 180-200 Anschlussblende mit Gummi-Einlage","103579","0",null,"STK",117]
["Keranova",16,180,"Keranova18016"," ","KER 180 Zugbegrenzer mit Explosionsklappe","103547","0",null,"STK",310]
["Keranova",17,180,"Keranova18017"," ","KER 180 Adapter für Zugbegrenzer für DN180mm","103551","0",null,"STK",54]
["Keranova",18,180,"Keranova18018"," ","KER 180 Universal-Kachelofenzargenset 180 x 180mm","103543","0",null,"STK",184]
["Keranova",19,180,"Keranova18019"," ","KER 180 Mauerschelle","103604","0",null,"STK",24,{"$f":"IF(Daten!$C$573=2,1,\"\")","v":1}]
["Keranova",20,180,"Keranova18020"," ","KER 180 Statische-Manchette für Muffenverbindungen","103532","0",null,"STK",40]
["Keranova",21,180,"Keranova18021"," ","KER 180 Bogen verstellbar 0-30° L660mm","103526",660,null,"STK",373]
["Keranova",22,180,"Keranova18022"," ","KER 180 Statische-Abstützung für Bogen-Verstellbar","103538","0",null,"STK",72]
["Keranova",23,180,"Keranova18023"," ","KER 160-180 Abdeckblende 340 x 340mm","103575","0",null,"STK",26]
["Keranova",24,180,"Keranova18024"," ","KER 180  Keranova-Fugenglätter","103474","0",null,"STK",53]
["Keranova",25,180,"Keranova18025"," ","KER 180 Verbindungsmanchette inkl. Abstandhalter","103468","0",null,"STK",41]
["Keranova",26,180,"Keranova18026"," ","KER 180 Adapter für Doppelfutter 180mm","103562","0",null,"STK",67,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",27,180,"Keranova18027"," ","KER 180 Doppelfutter 180mm","103570","0",null,"STK",69,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",28,180,"Keranova18028"," ","KER 180 Adapter für Doppelfutter 150mm","103561","0",null,"STK",67,{"$f":"IF(Daten!$B$600=3,1,\"\")","v":""}]
["Keranova",29,180,"Keranova18029"," ","KER 150 Doppelfutter 150mm","103569","0",null,"STK",65,{"$f":"IF(Daten!$B$600=3,1,\"\")","v":""}]
["Keranova",30,180,"Keranova18030"," ","KER Putztür PTS2 200 x 275mm Alu für  Ø140- 250mm","103596","0",null,"STK",112,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",31,180,"Keranova18031"," ","KER Schieberahmen zu PTS2 200 x 275mm L90mm","103597","0",null,"STK",21,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",32,180,"Keranova18032"," ","CHZ 120-180 Zuluftgitter für Hinterlüftung ","103817","0",null,"STK",24]
["Keranova",33,180,"Keranova18033"," ","KER 40 Siphon kompl.  für Schlauchanschluss DN32mm","103453","0",null,"STK",48,1]
["Keranova",34,180,"Keranova18034"," ","KER 32 PP Kondensatrohr-Erweiterung auf DN40 L50mm","103451","0",null,"STK",12,1]
["Keranova",35,180,"Keranova18035"," ","KER 40 PP Winkel 90° für Schlauchanschluss DN32mm","103452","0",null,"STK",56]
["Keranova",36,180,"Keranova18036"," ","KER 80-250 Ablasswinde schwer","103617","0",null,"STK",1552]
["Keranova",37,180,"Keranova18037"," ","KER 80-200 Ablasswinde leicht ","103618","0",null,"STK",1458]
["Keranova",38,180,"Keranova18038"," ","KER 80-160 Rollenbock ","103619","0",null,"STK",204]
["Keranova",39,180,"Keranova18039"," ","KER 160-250 Rollenbock","103620","0",null,"STK",204]
["Keranova",40,180,"Keranova18040"," ","KER 120-250 Versetzzange ","103622","0",null,"STK",1463]
["Keranova",41,180,"Keranova18041"," ","KER Rotempo Fugendichtmasse Kartusche a 310ml","103614","0",null,"STK",34,{"$f":"IF(Daten!$B$564=2,ROUNDUP(M483,0)+N449+N452,\"\")","v":""},{"$f":"((O442)*85)/310","v":3.1011290322580645}]
["Keranova",42,180,"Keranova18042"," ","ZBH Kittpistole für Kartuschen","103848","0",null,"STK",12]
["Keranova",43,180,"Keranova18043"," ","ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",14,{"$f":"IF(M485=0,\"\",(ROUNDUP(M485,0)+N449+N452))","v":7},{"$f":"IF(Daten!$B$564=1,((O442)*93)/310,0)","v":3.3930000000000007}]
["Keranova",44,180,"Keranova18044",null,"ABS 180 Basten Standard Inox","104212","0",null,"STK",323,{"$f":"IF(N486=0,\"\",N486)","v":""},null,{"$f":"IF(Daten!$B$618=2,1,0)","v":0}]
["Keranova",45,180,"Keranova18045",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",339,{"$f":"IF(N487=0,\"\",N487)","v":""},null,{"$f":"IF(Daten!$B$618=3,1,0)","v":0}]
["Keranova",46,180,"Keranova18046",null,"ABS 180 Sairlift Inox","104224","0",null,"STK",347,{"$f":"IF(N488=0,\"\",N488)","v":""},null,{"$f":"IF(Daten!$B$618=4,1,0)","v":0}]
["Keranova",47,180,"Keranova18047",null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",364,{"$f":"IF(N489=0,\"\",N489)","v":""},null,{"$f":"IF(Daten!$B$618=5,1,0)","v":0}]
["Keranova",48,180,{"$f":"A490&C490&B490","v":"Keranova18048"}," ","Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",6.2]
["Keranova",49,180,{"$f":"A491&C491&B491","v":"Keranova18049"}," ","Neutralisationsbox komplett","100265","0",null,"STK",225]
["Keranova",50,180,{"$f":"A492&C492&B492","v":"Keranova18050"}," ","ZBH Kondensatkanister 20Liter","103841","0",null,"STK",39]
["Keranova",0,200,"Keranova2000","P","Keranova Anlage Ø 200","Keranova 200","0",{"$f":"Keranova!$J$12","v":11},"Anlage",0,1,{"$f":"I493*1000","v":11000},null,{"$f":"ROUNDUP(P493,2)","v":11.31},{"$f":"SUM(P494:P536)/1000","v":11.305999999999999}]
["Keranova",{"$f":"B493+1","v":1},{"$f":"C493","v":200},"Keranova2001"," ","KER 200 Keranova-Rohr komplett L1330mm ","103458",1330,null,"STK",163,{"$f":"ROUNDUP(M494,0)","v":8},{"$f":"(M493-M497-M495-M506-M522)/H494","v":7.7706766917293235},null,null,{"$f":"H494*L494","v":10640}]
["Keranova",2,200,"Keranova2002"," ","KER 200 Keranova-Rohr komplett L660mm ","103463",665,null,"STK",110,{"$f":"1+Keranova!$P$20","v":1},{"$f":"IF(H495=0,\"\",L495*H495)","v":665},null,null,{"$f":"H495*L495","v":665}]
["Keranova",3,200,"Keranova2003"," ","KER 200 Dämmrohr Klappmatte L660mm","103480","0",null,"STK",60]
["Keranova",4,200,"Keranova2004"," ","KER 200 Kondensattopf komplett L145mm","103449","0",null,"STK",119,1,{"$f":"IF(H497=0,\"\",L497*H497)","v":0},null,null,{"$f":"H497*L497","v":0}]
["Keranova",{"$f":"B497+1","v":5},{"$f":"C497","v":200},{"$f":"A498&C498&B498","v":"Keranova2005"}," ","KER 200 T-Stück 90° L330mm Stutzen L90mm","103486",330,null,"STK",244,null,{"$f":"IF(H498=0,\"\",L498*H498)","v":0},null,null,{"$f":"H498*L498","v":0}]
["Keranova",{"$f":"B498+1","v":6},{"$f":"C498","v":200},"Keranova2006",null,"KER 200 Revisionsdeckel zu T-Stück Festbrennstoffe","103491","0",null,"STK",60]
["Keranova",7,200,{"$f":"A500&C500&B500","v":"Keranova2007"}," ","KER 200 Universalstutzen 0°","103496","0",null,"STK",0,{"$f":"IF(N500=0,\"\",N500)","v":3},null,{"$f":"SUM(O500:P500)","v":3},{"$f":"IF(Daten!$B$573=1,0,Daten!$C$573)","v":2},{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$B$591=2,0,Daten!$C$193))","v":1}]
["Keranova",8,200,"Keranova2008"," ","KER 200 Revisionsdeckel für Festbrennstoff","103515","0",null,"STK",60,{"$f":"IF(Daten!$B$573=0,\"\",IF(Daten!$B$582=3,Daten!$C$573,IF(Daten!$B$582=4,Daten!$C$573,\"\")))","v":2}]
["Keranova",9,200,"Keranova2009"," ","KER 200 Revisionsdeckel für Oel/Gas","103510","0",null,"STK",99,{"$f":"IF(Daten!$B$573=1,\"\",IF(Daten!$B$582=3,\"\",IF(Daten!$B$582=4,\"\",Daten!$C$573)))","v":""}]
["Keranova",10,200,"Keranova20010"," ","KER 200 Universalstutzen 45°","103503","0",null,"STK",119,{"$f":"IF(N503=0,\"\",N503)","v":""},null,{"$f":"SUM(O503:P503)","v":0},null,{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$C$591=\"90°\",0,Daten!$C$193))","v":0}]
["Keranova",11,200,"Keranova20011"," ","KER 200 Anreisschablone Universal","103521","0",null,"STK",110]
["Keranova",12,200,"Keranova20012"," ","PPL Schachtabdeckung Typ3 450 x 450mm","101274","0",null,"STK",119,{"$f":"IF(N505=0,1,\"\")","v":1},null,{"$f":"SUM(L537:L540)","v":0}]
["Keranova",13,200,"Keranova20013"," ","KER 200 Mündungskonus","103612","0",null,"STK",88,{"$f":"IF(N506=0,1,\"\")","v":1},null,{"$f":"SUM(L537:L540)","v":0}]
["Keranova",14,200,"Keranova20014"," ","ABS 220 Steckadapter ","104270","0",null,"STK",172]
["Keranova",15,200,{"$f":"A508&C508&B508","v":"Keranova20015"}," ","KER 180-200 Anschlussblende mit Gummi-Einlage","103579","0",null,"STK",117]
["Keranova",16,200,"Keranova20016"," ","KER 180 Zugbegrenzer mit Explosionsklappe","103547","0",null,"STK",310]
["Keranova",17,200,"Keranova20017"," ","KER 200 Adapter für Zugbegrenzer für DN200mm","103552","0",null,"STK",54]
["Keranova",18,200,"Keranova20018"," ","KER 200 Universal-Kachelofenzargenset 200 x 200mm","103544","0",null,"STK",184]
["Keranova",19,200,"Keranova20019"," ","KER 200 Mauerschelle","103605","0",null,"STK",24,{"$f":"IF(Daten!$C$573=2,1,\"\")","v":1}]
["Keranova",20,200,"Keranova20020"," ","KER 200 Statische-Manchette für Muffenverbindungen","103533","0",null,"STK",42]
["Keranova",21,200,"Keranova20021"," ","KER 200 Bogen verstellbar 0-30° L660mm","103527",660,null,"STK",410]
["Keranova",22,200,"Keranova20022"," ","KER 200 Statische-Abstützung für Bogen-Verstellbar","103539","0",null,"STK",80]
["Keranova",23,200,"Keranova20023"," ","KER 200 Abdeckblende 340 x 340mm","103576","0",null,"STK",26]
["Keranova",24,200,"Keranova20024"," ","KER 200  Keranova-Fugenglätter","103475","0",null,"STK",62]
["Keranova",25,200,"Keranova20025"," ","KER 200 Verbindungsmanchette inkl. Abstandhalter","103469","0",null,"STK",42]
["Keranova",26,200,"Keranova20026"," ","KER 200 Adapter für Doppelfutter 200mm","103564","0",null,"STK",71,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",27,200,"Keranova20027"," ","KER 200 Doppelfutter 200mm","103571","0",null,"STK",70,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",28,200,"Keranova20028"," ","KER 200 Adapter für Doppelfutter 180mm","103563","0",null,"STK",71,{"$f":"IF(Daten!$B$600=3,1,\"\")","v":""}]
["Keranova",29,200,"Keranova20029"," ","KER 180 Doppelfutter 180mm","103570","0",null,"STK",69,{"$f":"IF(Daten!$B$600=3,1,\"\")","v":""}]
["Keranova",30,200,"Keranova20030"," ","KER Putztür PTS2 200 x 275mm Alu für  Ø140- 250mm","103596","0",null,"STK",112,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",31,200,"Keranova20031"," ","KER Schieberahmen zu PTS2 200 x 275mm L90mm","103597","0",null,"STK",21,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",32,200,"Keranova20032"," ","CHZ 200-300 Zuluftgitter für Hinterlüftung","103818","0",null,"STK",38]
["Keranova",33,200,"Keranova20033"," ","KER 40 Siphon kompl.  für Schlauchanschluss DN32mm","103453","0",null,"STK",48,1]
["Keranova",34,200,"Keranova20034"," ","KER 32 PP Kondensatrohr-Erweiterung auf DN40 L50mm","103451","0",null,"STK",12,1]
["Keranova",35,200,"Keranova20035"," ","KER 40 PP Winkel 90° für Schlauchanschluss DN32mm","103452","0",null,"STK",56]
["Keranova",36,200,"Keranova20036"," ","KER 80-250 Ablasswinde schwer","103617","0",null,"STK",1552]
["Keranova",37,200,"Keranova20037"," ","KER 80-200 Ablasswinde leicht ","103618","0",null,"STK",1458]
["Keranova",38,200,"Keranova20038"," ","KER 80-160 Rollenbock ","103619","0",null,"STK",204]
["Keranova",39,200,"Keranova20039"," ","KER 160-250 Rollenbock","103620","0",null,"STK",204]
["Keranova",40,200,"Keranova20040"," ","KER 120-250 Versetzzange ","103622","0",null,"STK",1463]
["Keranova",41,200,"Keranova20041"," ","KER Rotempo Fugendichtmasse Kartusche a 310ml","103614","0",null,"STK",34,{"$f":"IF(Daten!$B$564=2,ROUNDUP(M534,0)+N500+N503,\"\")","v":""},{"$f":"((O493)*100)/310","v":3.6483870967741936}]
["Keranova",42,200,"Keranova20042"," ","ZBH Kittpistole für Kartuschen","103848","0",null,"STK",12]
["Keranova",43,200,"Keranova20043"," ","ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",14,{"$f":"IF(M536=0,\"\",(ROUNDUP(M536,0)+N500+N503))","v":8},{"$f":"IF(Daten!$B$564=1,((O493)*110)/310,0)","v":4.0132258064516133}]
["Keranova",44,200,"Keranova20044",null,"ABS 200 Basten Standard Inox","104213","0",null,"STK",338,{"$f":"IF(N537=0,\"\",N537)","v":""},null,{"$f":"IF(Daten!$B$618=2,1,0)","v":0}]
["Keranova",45,200,"Keranova20045",null,"ABS 200 Basten Standard Kupfer","104219","0",null,"STK",351,{"$f":"IF(N538=0,\"\",N538)","v":""},null,{"$f":"IF(Daten!$B$618=3,1,0)","v":0}]
["Keranova",46,200,"Keranova20046",null,"ABS 200 Sairlift Inox","104225","0",null,"STK",364,{"$f":"IF(N539=0,\"\",N539)","v":""},null,{"$f":"IF(Daten!$B$618=4,1,0)","v":0}]
["Keranova",47,200,"Keranova20047",null,"ABS 200 Sairlift Kupfer","104230","0",null,"STK",377,{"$f":"IF(N540=0,\"\",N540)","v":""},null,{"$f":"IF(Daten!$B$618=5,1,0)","v":0}]
["Keranova",48,200,{"$f":"A541&C541&B541","v":"Keranova20048"}," ","Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",6.2]
["Keranova",49,200,{"$f":"A542&C542&B542","v":"Keranova20049"}," ","Neutralisationsbox komplett","100265","0",null,"STK",225]
["Keranova",50,200,{"$f":"A543&C543&B543","v":"Keranova20050"}," ","ZBH Kondensatkanister 20Liter","103841","0",null,"STK",39]
["Keranova",0,250,{"$f":"A544&C544&B544","v":"Keranova2500"},"P","Keranova Anlage Ø 250","Keranova 250","0",{"$f":"Keranova!$J$12","v":11},"Anlage",0,1,{"$f":"I544*1000","v":11000},null,{"$f":"ROUNDUP(P544,2)","v":11.31},{"$f":"SUM(P545:P578)/1000","v":11.305999999999999}]
["Keranova",{"$f":"B544+1","v":1},{"$f":"C544","v":250},"Keranova2501"," ","KER 250 Keranova-Rohr komplett L660mm ","103464",665,null,"STK",126,{"$f":"ROUNDUP(M545,0)","v":17},{"$f":"(M544-M547)/H545","v":16.541353383458645},null,null,{"$f":"H545*L545","v":11305}]
["Keranova",2,250,"Keranova2502"," ","KER 250 Dämmrohr Klappmatte L660mm","103481","0",null,"STK",65]
["Keranova",3,250,"Keranova2503"," ","KER 250 Kondensattopf komplett L135mm","103450","0",null,"STK",124,1,{"$f":"IF(H547=0,\"\",L547*H547)","v":0},null,null,{"$f":"H547*L547","v":0}]
["Keranova",{"$f":"B547+1","v":4},{"$f":"C547","v":250},{"$f":"A548&C548&B548","v":"Keranova2504"}," ","KER 250 Universalstutzen 0°","103497","0",null,"STK",101,{"$f":"IF(N548=0,\"\",N548)","v":3},null,{"$f":"SUM(O548:P548)","v":3},{"$f":"IF(Daten!$B$573=1,0,Daten!$C$573)","v":2},{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$B$591=2,0,Daten!$C$193))","v":1}]
["Keranova",5,250,"Keranova2505"," ","KER 250 Revisionsdeckel Festbrennstoff mit Bügel","103516","0",null,"STK",96,{"$f":"IF(Daten!$B$573=0,\"\",IF(Daten!$B$582=3,Daten!$C$573,IF(Daten!$B$582=4,Daten!$C$573,\"\")))","v":2}]
["Keranova",6,250,"Keranova2506"," ","KER 200 Revisionsdeckel für Oel/Gas","103510","0",null,"STK",99,{"$f":"IF(Daten!$B$573=1,\"\",IF(Daten!$B$582=3,\"\",IF(Daten!$B$582=4,\"\",Daten!$C$573)))","v":""}]
["Keranova",7,250,"Keranova2507"," ","KER 250 Universalstutzen 45°","103504","0",null,"STK",126,{"$f":"IF(N551=0,\"\",N551)","v":""},null,{"$f":"SUM(O551:P551)","v":0},null,{"$f":"IF(Daten!$B$193=1,0,IF(Daten!$C$591=\"90°\",0,Daten!$C$193))","v":0}]
["Keranova",8,250,"Keranova2508"," ","KER 250 Anreisschablone Universal","103522","0",null,"STK",107]
["Keranova",9,250,"Keranova2509"," ","PPL Schachtabdeckung Typ4 500 x 500mm","101275","0",null,"STK",151,{"$f":"IF(N553=0,1,\"\")","v":1},null,{"$f":"SUM(N579:N582)","v":0}]
["Keranova",10,250,"Keranova25010"," ","KER 250 Mündungskonus","103613","0",null,"STK",99,{"$f":"IF(N554=0,1,\"\")","v":1},null,{"$f":"SUM(N579:N582)","v":0}]
["Keranova",11,250,"Keranova25011"," ","ABS 250 Steckadapter ","104271","0",null,"STK",203]
["Keranova",12,250,"Keranova25012"," ","KER 180 Zugbegrenzer mit Explosionsklappe","103547","0",null,"STK",310]
["Keranova",13,250,"Keranova25013"," ","KER 250 Adapter für Zugbegrenzer für DN250mm","103553","0",null,"STK",54]
["Keranova",14,250,"Keranova25014"," ","KER 250 Mauerschelle","103606","0",null,"STK",28,{"$f":"IF(Daten!$C$573=2,1,\"\")","v":1}]
["Keranova",15,250,"Keranova25015"," ","KER 250 Bogen verstellbar 0-30° L660mm","103528",660,null,"STK",435]
["Keranova",16,250,"Keranova25016"," ","KER 250 Statische-Abstützung für Bogen-Verstellbar","103540","0",null,"STK",80]
["Keranova",17,250,"Keranova25017"," ","KER 250 Keranova-Fugenglätter","103476","0",null,"STK",68]
["Keranova",18,250,"Keranova25018"," ","KER 250 Verbindungsmanchette inkl. Abstandhalter","103470","0",null,"STK",46]
["Keranova",19,250,"Keranova25019"," ","KER 250 Adapter für Doppelfutter 250mm","103565","0",null,"STK",79,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",20,250,"Keranova25020"," ","KER 250 Doppelfutter 250mm","103572","0",null,"STK",72,{"$f":"IF(Daten!$B$600=2,1,\"\")","v":""}]
["Keranova",21,250,"Keranova25021"," ","KER Putztür PTS2 200 x 275mm Alu für  Ø140- 250mm","103596","0",null,"STK",112,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",22,250,"Keranova25022"," ","KER Schieberahmen zu PTS2 200 x 275mm L90mm","103597","0",null,"STK",21,{"$f":"IF(Daten!$B$609=1,\"\",Daten!$C$609)","v":""}]
["Keranova",23,250,"Keranova25023"," ","CHZ 200-300 Zuluftgitter für Hinterlüftung","103818","0",null,"STK",38]
["Keranova",24,250,"Keranova25024"," ","KER 40 Siphon kompl.  für Schlauchanschluss DN32mm","103453","0",null,"STK",48,1]
["Keranova",25,250,"Keranova25025"," ","KER 32 PP Kondensatrohr-Erweiterung auf DN40 L50mm","103451","0",null,"STK",12,1]
["Keranova",26,250,"Keranova25026"," ","KER 40 PP Winkel 90° für Schlauchanschluss DN32mm","103452","0",null,"STK",56]
["Keranova",27,250,"Keranova25027"," ","KER 80-250 Ablasswinde schwer","103617","0",null,"STK",1552]
["Keranova",28,250,"Keranova25028"," ","KER 80-200 Ablasswinde leicht ","103618","0",null,"STK",1458]
["Keranova",29,250,"Keranova25029"," ","KER 80-160 Rollenbock ","103619","0",null,"STK",204]
["Keranova",30,250,"Keranova25030"," ","KER 160-250 Rollenbock","103620","0",null,"STK",204]
["Keranova",31,250,"Keranova25031"," ","KER 120-250 Versetzzange ","103622","0",null,"STK",1463]
["Keranova",32,250,"Keranova25032"," ","KER Rotempo Fugendichtmasse Kartusche a 310ml","103614","0",null,"STK",34,{"$f":"IF(Daten!$B$564=2,ROUNDUP(M576,0)+N548+N551,\"\")","v":""},{"$f":"((O544)*144)/310","v":5.2536774193548395}]
["Keranova",33,250,"Keranova25033"," ","ZBH Kittpistole für Kartuschen","103848","0",null,"STK",12]
["Keranova",34,250,"Keranova25034"," ","ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",14,{"$f":"IF(M578=0,\"\",(ROUNDUP(M578,0)+N548+N551))","v":9},{"$f":"IF(Daten!$B$564=1,((O544)*155)/310,0)","v":5.6550000000000002}]
["Keranova",35,250,"Keranova25035",null,"ABS 250 Basten Standard Inox","104214","0",null,"STK",375,{"$f":"IF(N579=0,\"\",N579)","v":""},null,{"$f":"IF(Daten!$B$618=2,1,0)","v":0}]
["Keranova",36,250,"Keranova25036",null,"ABS 250 Basten Standard Kupfer","104221","0",null,"STK",512,{"$f":"IF(N580=0,\"\",N580)","v":""},null,{"$f":"IF(Daten!$B$618=3,1,0)","v":0}]
["Keranova",37,250,"Keranova25037",null,"ABS 250 Sairlift Inox","104226","0",null,"STK",404,{"$f":"IF(N581=0,\"\",N581)","v":""},null,{"$f":"IF(Daten!$B$618=4,1,0)","v":0}]
["Keranova",38,250,"Keranova25038",null,"ABS 250 Sairlift Kupfer","104231","0",null,"STK",417,{"$f":"IF(N582=0,\"\",N582)","v":""},null,{"$f":"IF(Daten!$B$618=5,1,0)","v":0}]
["Keranova",39,250,{"$f":"A583&C583&B583","v":"Keranova25039"}," ","Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",6.2]
["Keranova",40,250,{"$f":"A584&C584&B584","v":"Keranova25040"}," ","Neutralisationsbox komplett","100265","0",null,"STK",225]
["Keranova",41,250,{"$f":"A585&C585&B585","v":"Keranova25041"}," ","ZBH Kondensatkanister 20Liter","103841","0",null,"STK",39]
["Absolut",0,14,{"$f":"A586&C586&B586","v":"Absolut140"},"P","Absolut-Kaminanlage Ø 14","Absolut 14","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G586,sanschie!A:G,7,0)","v":0},null,{"$f":"I586*1000","v":9000}]
["Absolut",{"$f":"B586+1","v":1},{"$f":"C586","v":14},{"$f":"A587&C587&B587","v":"Absolut141"},null,"ABS Mantelstein EZ 360 x 360mm L330mm","103912","0",null,"STK",{"$f":"VLOOKUP(G587,sanschie!A:G,7,0)","v":30},{"$f":"ROUND(M587,0)-N612-M588","v":23},{"$f":"((M586-M592)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N587*330","v":0}]
["Absolut",{"$f":"B587+1","v":2},{"$f":"C587","v":14},{"$f":"A588&C588&B588","v":"Absolut142"},null,"ABS Thermo-Trennstein EZ 360 x 360mm L330mm","103931","0",null,"STK",{"$f":"VLOOKUP(G588,sanschie!A:G,7,0)","v":210},{"$f":"IF(M588=0,\"\",M588)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,14,"Absolut143",null,"ABS Thermo-Fussplatte EZ 360 x 360mm","103849","0",null,"STK",{"$f":"VLOOKUP(G589,sanschie!A:G,7,0)","v":124}]
["Absolut",4,14,"Absolut144",null,"ABS 140 Profilkeramik-Rohr mit Muffe L1330mm","103946",1330,null,"STK",{"$f":"VLOOKUP(G590,sanschie!A:G,7,0)","v":106},{"$f":"ROUNDUP(M590,0)","v":5},{"$f":"(M586-O587-M592-M596-M597-M601)/1000/1.33","v":4.962406015037593}]
["Absolut",5,14,"Absolut145",null,"ABS 140 Profilkeramik-Rohr mit Muffe L660mm","103951",660,null,"STK",{"$f":"VLOOKUP(G591,sanschie!A:G,7,0)","v":59},null,{"$f":"IF(L591=0,0,IF(L591=\"\",0,L591*H591))","v":0}]
["Absolut",6,14,"Absolut146",null,"ABS 180 Fertigfuss EZ Ø140- 180 mm  L1070mm","103859",1070,null,"STK",{"$f":"VLOOKUP(G592,sanschie!A:G,7,0)","v":611},{"$f":"IF(Daten!$B$183=2,\"\",1)","v":1},{"$f":"IF(L592=\"\",0,$H592*$L592)","v":1070}]
["Absolut",7,14,"Absolut147",null,"ABS 140 Fertigfusspaket ","103889","0",null,"STK",{"$f":"VLOOKUP(G593,sanschie!A:G,7,0)","v":311},{"$f":"IF(Daten!$B$183=2,\"\",1)","v":1}]
["Absolut",8,14,"Absolut148",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G594,sanschie!A:G,7,0)","v":18}]
["Absolut",9,14,"Absolut149",null,"ABS Sockelplatte aus Beton EZ 360 x 360mm","103871","0",null,"STK",{"$f":"VLOOKUP(G595,sanschie!A:G,7,0)","v":155}]
["Absolut",10,{"$f":"C594","v":14},"Absolut1410",null,"ABS 140 Rauchrohr-Anschlusspaket 90° RA  ","103981",1330,null,"STK",{"$f":"VLOOKUP(G596,sanschie!A:G,7,0)","v":355},{"$f":"IF(N596=0,\"\",N596)","v":1},{"$f":"IF(L596=0,0,IF(L596=\"\",0,L596*H596))","v":1330},{"$f":"SUM(O596:P596)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",11,14,"Absolut1411",null,"ABS 140 Rauchrohr-Anschlusspaket 45° RA  ","103993",1330,null,"STK",{"$f":"VLOOKUP(G597,sanschie!A:G,7,0)","v":355},{"$f":"IF(N597=0,\"\",N597)","v":""},{"$f":"IF(L597=0,0,IF(L597=\"\",0,L597*H597))","v":0},{"$f":"SUM(O597:P597)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",12,14,"Absolut1412",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø140mm","103999","0",null,"STK",{"$f":"VLOOKUP(G598,sanschie!A:G,7,0)","v":191}]
["Absolut",13,14,"Absolut1413",null,"ABS 140 Rauchrohranschluss Stutzen-Set 45°","104005","0",null,"STK",{"$f":"VLOOKUP(G599,sanschie!A:G,7,0)","v":191}]
["Absolut",14,14,"Absolut1414",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G600,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=2,1,\"\")","v":""}]
["Absolut",15,14,{"$f":"A601&C601&B601","v":"Absolut1415"},null,"ABS 140 Putztür-Anschlusspaket ","103964",1330,null,"STK",{"$f":"VLOOKUP(G601,sanschie!A:G,7,0)","v":410},{"$f":"IF(N601=0,\"\",N601)","v":""},{"$f":"IF(L601=0,0,IF(L601=\"\",0,L601*H601))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",16,14,{"$f":"A602&C602&B602","v":"Absolut1416"},null,"ABS 140 Putztüranschluss Stutzen Set","104272","0",null,"STK",{"$f":"VLOOKUP(G602,sanschie!A:G,7,0)","v":311}]
["Absolut",17,14,{"$f":"A603&C603&B603","v":"Absolut1417"},null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G603,sanschie!A:G,7,0)","v":27}]
["Absolut",18,14,{"$f":"A604&C604&B604","v":"Absolut1418"},null,"ABS Thermodichtset EZ 360x360mm und 380x380mm","104190","0",null,"STK",{"$f":"VLOOKUP(G604,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$G$280=Vokabel!$A$413,1,\"\")","v":""}]
["Absolut",19,14,"Absolut1419",null,"ABS Handyplatte EZ Faserzement 360 x 360mm","104144","0",null,"STK",{"$f":"VLOOKUP(G605,sanschie!A:G,7,0)","v":106},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",20,14,"Absolut1420",null,"ABS Handyplatte EZ Inox 360 x 360mm  ","104170","0",null,"STK",{"$f":"VLOOKUP(G606,sanschie!A:G,7,0)","v":155},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",21,14,"Absolut1421",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G607,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",22,14,"Absolut1422",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G608,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",23,14,"Absolut1423",null,"ABS Handyplatte EZ Kupfer 360 x 360mm  ","140787","0",null,"STK",{"$f":"VLOOKUP(G609,sanschie!A:G,7,0)","v":229}]
["Absolut",24,14,"Absolut1424",null,"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben","140932","0",null,"STK",{"$f":"VLOOKUP(G610,sanschie!A:G,7,0)","v":75}]
["Absolut",25,14,"Absolut1425",null,"ABS 140 Abströmkonus verkupfert","104204","0",null,"STK",{"$f":"VLOOKUP(G611,sanschie!A:G,7,0)","v":161}]
["Absolut",26,14,"Absolut1426",null,"ABS Anschlussmantelstein EZ 360 x 360mm L330","103917","0",null,"STK",{"$f":"VLOOKUP(G612,sanschie!A:G,7,0)","v":80},{"$f":"IF(N612=0,\"\",N612)","v":1},null,{"$f":"IF(Daten!$B$193=0,0,N601+N596+N597)","v":1}]
["Absolut",27,14,"Absolut1427",null,"ABS 140 Schleifung EZ 15° auf Bestellung","104047","0",null,"STK",{"$f":"VLOOKUP(G613,sanschie!A:G,7,0)","v":1010}]
["Absolut",28,14,"Absolut1428",null,"ABS 140 Abstandhalter offen zu Schleifung","104081","0",null,"STK",{"$f":"VLOOKUP(G614,sanschie!A:G,7,0)","v":27}]
["Absolut",29,14,"Absolut1429",null,"ABS 160 Anschlusskonus EZ mit Doppelfutter DN150mm","103898","0",null,"STK",{"$f":"VLOOKUP(G615,sanschie!A:G,7,0)","v":241},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",30,14,"Absolut1430",null,"ABS 180 Adapterring von 180mm auf 140mm L90mm","103905","0",null,"STK",{"$f":"VLOOKUP(G616,sanschie!A:G,7,0)","v":35},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",31,14,"Absolut1431",null,"KER 140  Keranova-Fugenglätter","103472","0",null,"STK",{"$f":"VLOOKUP(G617,sanschie!A:G,7,0)","v":57}]
["Absolut",32,14,"Absolut1432",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G618,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",33,14,"Absolut1433",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G619,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",34,14,"Absolut1434",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G620,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",35,14,"Absolut1435",null,"CHZ 150 Doppelfutter lose L150mm","103803","0",null,"STK",{"$f":"VLOOKUP(G621,sanschie!A:G,7,0)","v":103},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",36,14,"Absolut1436",null,"ABS 140 Kondensatfalle zu RA 45° Ø130mm ","104028","0",null,"STK",{"$f":"VLOOKUP(G622,sanschie!A:G,7,0)","v":297}]
["Absolut",37,14,"Absolut1437",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G623,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",38,14,"Absolut1438",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G624,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",39,14,"Absolut1439",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G625,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",40,14,"Absolut1440",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G626,sanschie!A:G,7,0)","v":23},{"$f":"IF(L593=1,1,\"\")","v":1}]
["Absolut",41,14,"Absolut1441",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G627,sanschie!A:G,7,0)","v":489},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""}]
["Absolut",42,14,"Absolut1442",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G628,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",43,14,"Absolut1443",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G629,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",44,14,"Absolut1444",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G630,sanschie!A:G,7,0)","v":14},{"$f":"IF(Daten!$B$183=2,N630,Sortimente!P630)","v":""},null,{"$f":"ROUNDUP(O630,0)","v":3},{"$f":"L590/2","v":2.5},{"$f":"IF(L590<=8,\"\",IF(L590<=10,1,IF(L590<=12,2,IF(L590<=14,3,4))))","v":""}]
["Absolut",45,14,"Absolut1445",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G631,sanschie!A:G,7,0)","v":303},{"$f":"IF(N631=0,\"\",N631)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",46,14,"Absolut1446",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G632,sanschie!A:G,7,0)","v":94},{"$f":"IF(N632=0,\"\",N632)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",47,14,"Absolut1447",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G633,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",48,14,"Absolut1448",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G634,sanschie!A:G,7,0)","v":35},{"$f":"IF(N634<=12.7,1,2)","v":1},null,{"$f":"IF(L592=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",49,14,"Absolut1449",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G635,sanschie!A:G,7,0)","v":258.8}]
["Absolut",50,14,"Absolut1450",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G636,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",51,14,"Absolut1451",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G637,sanschie!A:G,7,0)","v":44.9}]
["Absolut",52,14,"Absolut1452",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G638,sanschie!A:G,7,0)","v":7.5}]
["Absolut",53,14,"Absolut1453",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G639,sanschie!A:G,7,0)","v":452}]
["Absolut",54,14,"Absolut1454",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G640,sanschie!A:G,7,0)","v":538}]
["Absolut",55,14,"Absolut1455",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G641,sanschie!A:G,7,0)","v":634}]
["Absolut",56,14,"Absolut1456",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G642,sanschie!A:G,7,0)","v":695}]
["Absolut",57,14,"Absolut1457",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G643,sanschie!A:G,7,0)","v":797}]
["Absolut",58,14,"Absolut1458",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G644,sanschie!A:G,7,0)","v":873}]
["Absolut",59,14,"Absolut1459",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G645,sanschie!A:G,7,0)","v":13.8}]
["Absolut",60,14,"Absolut1460",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G646,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",61,14,"Absolut1461",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G647,sanschie!A:G,7,0)","v":322}]
["Absolut",62,14,"Absolut1462",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G648,sanschie!A:G,7,0)","v":26}]
["Absolut",63,14,"Absolut1463",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G649,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,16,{"$f":"A650&C650&B650","v":"Absolut160"},"P","Absolut-Kaminanlage Ø 16","Absolut 16","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G650,sanschie!A:G,7,0)","v":0},null,{"$f":"I650*1000","v":9000}]
["Absolut",{"$f":"B650+1","v":1},{"$f":"C650","v":16},{"$f":"A651&C651&B651","v":"Absolut161"},null,"ABS Mantelstein EZ 360 x 360mm L330mm","103912","0",null,"STK",{"$f":"VLOOKUP(G651,sanschie!A:G,7,0)","v":30},{"$f":"ROUND(M651,0)-N677-M652","v":23},{"$f":"((M650-M656)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N651*330","v":0}]
["Absolut",{"$f":"B651+1","v":2},{"$f":"C651","v":16},{"$f":"A652&C652&B652","v":"Absolut162"},null,"ABS Thermo-Trennstein EZ 360 x 360mm L330mm","103931","0",null,"STK",{"$f":"VLOOKUP(G652,sanschie!A:G,7,0)","v":210},{"$f":"IF(M652=0,\"\",M652)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,16,"Absolut163",null,"ABS Thermo-Fussplatte EZ 360 x 360mm","103849","0",null,"STK",{"$f":"VLOOKUP(G653,sanschie!A:G,7,0)","v":124}]
["Absolut",4,16,"Absolut164",null,"ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","103947",1330,null,"STK",{"$f":"VLOOKUP(G654,sanschie!A:G,7,0)","v":113},{"$f":"ROUNDUP(M654,0)","v":5},{"$f":"(M650-O651-M656-M661-M662-M666)/1000/1.33","v":4.962406015037593}]
["Absolut",5,16,"Absolut165",null,"ABS 160 Profilkeramik-Rohr mit Muffe L660mm","103952",660,null,"STK",{"$f":"VLOOKUP(G655,sanschie!A:G,7,0)","v":61},null,{"$f":"IF(L655=0,0,IF(L655=\"\",0,L655*H655))","v":0}]
["Absolut",6,16,"Absolut166",null,"ABS 180 Fertigfuss EZ Ø140- 180 mm  L1070mm","103859",1070,null,"STK",{"$f":"VLOOKUP(G656,sanschie!A:G,7,0)","v":611},{"$f":"IF(Daten!$B$183=2,\"\",1)","v":1},{"$f":"IF(L656=\"\",0,$H656*$L656)","v":1070}]
["Absolut",7,16,"Absolut167",null,"ABS 160 Fertigfusspaket ","103890","0",null,"STK",{"$f":"VLOOKUP(G657,sanschie!A:G,7,0)","v":311},{"$f":"IF(Daten!$B$183=2,\"\",1)","v":1}]
["Absolut",8,16,"Absolut168",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G658,sanschie!A:G,7,0)","v":18}]
["Absolut",9,16,"Absolut169",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G659,sanschie!A:G,7,0)","v":32}]
["Absolut",10,16,"Absolut1610",null,"ABS Sockelplatte aus Beton EZ 360 x 360mm","103871","0",null,"STK",{"$f":"VLOOKUP(G660,sanschie!A:G,7,0)","v":155}]
["Absolut",11,16,"Absolut1611",null,"ABS 160 Rauchrohr-Anschlusspaket 90° RA  ","103982",1330,null,"STK",{"$f":"VLOOKUP(G661,sanschie!A:G,7,0)","v":367},{"$f":"IF(N661=0,\"\",N661)","v":1},{"$f":"IF(L661=0,0,IF(L661=\"\",0,L661*H661))","v":1330},{"$f":"SUM(O661:P661)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",12,16,"Absolut1612",null,"ABS 160 Rauchrohr-Anschlusspaket 45° RA  ","103994",1330,null,"STK",{"$f":"VLOOKUP(G662,sanschie!A:G,7,0)","v":367},{"$f":"IF(N662=0,\"\",N662)","v":""},{"$f":"IF(L662=0,0,IF(L662=\"\",0,L662*H662))","v":0},{"$f":"SUM(O662:P662)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",13,16,"Absolut1613",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø160mm","104000","0",null,"STK",{"$f":"VLOOKUP(G663,sanschie!A:G,7,0)","v":199}]
["Absolut",14,16,"Absolut1614",null,"ABS 160 Rauchrohranschluss Stutzen-Set 45°","104006","0",null,"STK",{"$f":"VLOOKUP(G664,sanschie!A:G,7,0)","v":199}]
["Absolut",15,16,"Absolut1615",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G665,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=2,1,\"\")","v":""}]
["Absolut",16,16,"Absolut1616",null,"ABS 160 Putztür-Anschlusspaket ","103965",1330,null,"STK",{"$f":"VLOOKUP(G666,sanschie!A:G,7,0)","v":428},{"$f":"IF(N666=0,\"\",N666)","v":""},{"$f":"IF(L666=0,0,IF(L666=\"\",0,L666*H666))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",17,16,"Absolut1617",null,"ABS 160 Putztüranschluss Stutzen Set","104273","0",null,"STK",{"$f":"VLOOKUP(G667,sanschie!A:G,7,0)","v":325}]
["Absolut",18,16,"Absolut1618",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G668,sanschie!A:G,7,0)","v":27}]
["Absolut",19,16,"Absolut1619",null,"ABS Thermodichtset EZ 360x360mm und 380x380mm","104190","0",null,"STK",{"$f":"VLOOKUP(G669,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$G$280=Vokabel!$A$413,1,\"\")","v":""}]
["Absolut",20,16,"Absolut1620",null,"ABS Handyplatte EZ Faserzement 360 x 360mm","104144","0",null,"STK",{"$f":"VLOOKUP(G670,sanschie!A:G,7,0)","v":106},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",21,16,"Absolut1621",null,"ABS Handyplatte EZ Inox 360 x 360mm  ","104170","0",null,"STK",{"$f":"VLOOKUP(G671,sanschie!A:G,7,0)","v":155},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",22,16,"Absolut1622",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G672,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",23,16,"Absolut1623",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G673,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",24,16,"Absolut1624",null,"ABS Handyplatte EZ Kupfer 360 x 360mm  ","140787","0",null,"STK",{"$f":"VLOOKUP(G674,sanschie!A:G,7,0)","v":229}]
["Absolut",25,16,"Absolut1625",null,"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben","140932","0",null,"STK",{"$f":"VLOOKUP(G675,sanschie!A:G,7,0)","v":75}]
["Absolut",26,16,"Absolut1626",null,"ABS 160 Abströmkonus verkupfert","104205","0",null,"STK",{"$f":"VLOOKUP(G676,sanschie!A:G,7,0)","v":166}]
["Absolut",27,16,"Absolut1627",null,"ABS Anschlussmantelstein EZ 360 x 360mm L330","103917","0",null,"STK",{"$f":"VLOOKUP(G677,sanschie!A:G,7,0)","v":80},{"$f":"IF(N677=0,\"\",N677)","v":1},null,{"$f":"IF(Daten!$B$193=0,0,N666+N661+N662)","v":1}]
["Absolut",28,16,"Absolut1628",null,"ABS 160 Schleifung EZ 5° auf Bestellung","104052","0",null,"STK",{"$f":"VLOOKUP(G678,sanschie!A:G,7,0)","v":1010}]
["Absolut",29,16,"Absolut1629",null,"ABS 160 Abstandhalter offen zu Schleifung","104082","0",null,"STK",{"$f":"VLOOKUP(G679,sanschie!A:G,7,0)","v":27}]
["Absolut",30,16,"Absolut1630",null,"ABS 160 Anschlusskonus EZ mit Doppelfutter DN150mm","103898","0",null,"STK",{"$f":"VLOOKUP(G680,sanschie!A:G,7,0)","v":241},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",31,16,"Absolut1631",null,"ABS 180 Adapterring von 180mm auf 160mm L90mm","103906","0",null,"STK",{"$f":"VLOOKUP(G681,sanschie!A:G,7,0)","v":41},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",32,16,"Absolut1632",null,"KER 160  Keranova-Fugenglätter","103473","0",null,"STK",{"$f":"VLOOKUP(G682,sanschie!A:G,7,0)","v":58}]
["Absolut",33,16,"Absolut1633",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G683,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",34,16,"Absolut1634",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G684,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",35,16,"Absolut1635",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G685,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",36,16,"Absolut1636",null,"CHZ 150 Doppelfutter lose L150mm","103803","0",null,"STK",{"$f":"VLOOKUP(G686,sanschie!A:G,7,0)","v":103},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",37,16,"Absolut1637",null,"ABS 160 Kondensatfalle zu RA 45° Ø130mm ","104029","0",null,"STK",{"$f":"VLOOKUP(G687,sanschie!A:G,7,0)","v":322}]
["Absolut",38,16,"Absolut1638",null,"ABS 160 Kondensatfalle zu RA 45° Ø150mm ","104030","0",null,"STK",{"$f":"VLOOKUP(G688,sanschie!A:G,7,0)","v":322}]
["Absolut",39,16,"Absolut1639",null,"ABS 160 Kondensatfalle zu RA 45° Ø160mm ","104031","0",null,"STK",{"$f":"VLOOKUP(G689,sanschie!A:G,7,0)","v":322}]
["Absolut",40,16,"Absolut1640",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G690,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",41,16,"Absolut1641",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G691,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",42,16,"Absolut1642",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G692,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",43,16,"Absolut1643",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G693,sanschie!A:G,7,0)","v":23},{"$f":"IF(L657=1,1,\"\")","v":1}]
["Absolut",44,16,"Absolut1644",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G694,sanschie!A:G,7,0)","v":489},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""}]
["Absolut",45,16,"Absolut1645",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G695,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",46,16,"Absolut1646",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G696,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",47,16,"Absolut1647",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G697,sanschie!A:G,7,0)","v":14},{"$f":"IF(Daten!$B$183=2,N697,Sortimente!P697)","v":""},null,{"$f":"ROUNDUP(O697,0)","v":3},{"$f":"L654/2","v":2.5},{"$f":"IF(L654<=8,\"\",IF(L654<=10,1,IF(L654<=12,2,IF(L654<=14,3,4))))","v":""}]
["Absolut",48,16,"Absolut1648",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G698,sanschie!A:G,7,0)","v":303},{"$f":"IF(N698=0,\"\",N698)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",49,16,"Absolut1649",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G699,sanschie!A:G,7,0)","v":94},{"$f":"IF(N699=0,\"\",N699)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",50,16,"Absolut1650",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G700,sanschie!A:G,7,0)","v":19},{"$f":"IF(L680=1,N700,IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0))))","v":""},null,{"$f":"ROUNDUP(O700,0)","v":2},{"$f":"L654*0.4","v":2}]
["Absolut",51,16,"Absolut1651",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G701,sanschie!A:G,7,0)","v":35},{"$f":"IF(N701<=12.7,1,2)","v":1},null,{"$f":"IF(L656=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",52,16,"Absolut1652",null,"ABS 160 Basten Standard Inox","104211","0",null,"STK",{"$f":"VLOOKUP(G702,sanschie!A:G,7,0)","v":323},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",53,16,"Absolut1653",null,"ABS 160 Basten Standard Kupfer","104217","0",null,"STK",{"$f":"VLOOKUP(G703,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",54,16,"Absolut1654",null,"ABS 160 Sairlift Inox","104223","0",null,"STK",{"$f":"VLOOKUP(G704,sanschie!A:G,7,0)","v":374},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",55,16,"Absolut1655",null,"ABS 160 Sairlift Kupfer","104228","0",null,"STK",{"$f":"VLOOKUP(G705,sanschie!A:G,7,0)","v":397},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",56,16,"Absolut1656",null,"ZBH 160 Verschlussbüchse weiss ØA 275mm","103837","0",null,"STK",{"$f":"VLOOKUP(G706,sanschie!A:G,7,0)","v":115}]
["Absolut",57,16,"Absolut1657",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G707,sanschie!A:G,7,0)","v":258.8}]
["Absolut",58,16,"Absolut1658",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G708,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",59,16,"Absolut1659",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G709,sanschie!A:G,7,0)","v":44.9}]
["Absolut",60,16,"Absolut1660",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G710,sanschie!A:G,7,0)","v":7.5}]
["Absolut",61,16,"Absolut1661",null,"ZBH 170 Verschlusszapfen 2Stk. aus Schaumstoff","103832","0",null,"STK",{"$f":"VLOOKUP(G711,sanschie!A:G,7,0)","v":24.2}]
["Absolut",62,16,"Absolut1662",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G712,sanschie!A:G,7,0)","v":452}]
["Absolut",63,16,"Absolut1663",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G713,sanschie!A:G,7,0)","v":538}]
["Absolut",64,16,"Absolut1664",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G714,sanschie!A:G,7,0)","v":634}]
["Absolut",65,16,"Absolut1665",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G715,sanschie!A:G,7,0)","v":695}]
["Absolut",{"$f":"B715+1","v":66},{"$f":"C715","v":16},"Absolut1666",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G716,sanschie!A:G,7,0)","v":797}]
["Absolut",67,16,"Absolut1667",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G717,sanschie!A:G,7,0)","v":873}]
["Absolut",68,16,"Absolut1668",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G718,sanschie!A:G,7,0)","v":13.8}]
["Absolut",69,16,"Absolut1669",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G719,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",70,16,"Absolut1670",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G720,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B720+1","v":71},{"$f":"C720","v":16},{"$f":"A721&C721&B721","v":"Absolut1671"},null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G721,sanschie!A:G,7,0)","v":26}]
["Absolut",{"$f":"B721+1","v":72},{"$f":"C721","v":16},{"$f":"A722&C722&B722","v":"Absolut1672"},null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G722,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,18,{"$f":"A723&C723&B723","v":"Absolut180"},"P","Absolut-Kaminanlage Ø 18","Absolut 18","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G723,sanschie!A:G,7,0)","v":0},null,{"$f":"I723*1000","v":9000}]
["Absolut",{"$f":"B723+1","v":1},{"$f":"C723","v":18},{"$f":"A724&C724&B724","v":"Absolut181"},null,"ABS Mantelstein EZ 360 x 360mm L330mm","103912","0",null,"STK",{"$f":"VLOOKUP(G724,sanschie!A:G,7,0)","v":30},{"$f":"ROUND(M724,0)-N750-M725","v":23},{"$f":"((M723-M728)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N724*330","v":0}]
["Absolut",{"$f":"B724+1","v":2},{"$f":"C724","v":18},{"$f":"A725&C725&B725","v":"Absolut182"},null,"ABS Thermo-Trennstein EZ 360 x 360mm L330mm","103931","0",null,"STK",{"$f":"VLOOKUP(G725,sanschie!A:G,7,0)","v":210},{"$f":"IF(M725=0,\"\",M725)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,18,"Absolut183",null,"ABS Thermo-Fussplatte EZ 360 x 360mm","103849","0",null,"STK",{"$f":"VLOOKUP(G726,sanschie!A:G,7,0)","v":124}]
["Absolut",4,18,"Absolut184",null,"ABS 180 Profilkeramik-Rohr mit Muffe L1330mm","103948",1330,null,"STK",{"$f":"VLOOKUP(G727,sanschie!A:G,7,0)","v":122},{"$f":"ROUNDUP(M727,0)","v":5},{"$f":"(M723-O724-M728-M734-M735-M739)/H727","v":4.9624060150375939}]
["Absolut",5,18,"Absolut185",null,"ABS 180 Fertigfuss EZ Ø140- 180 mm  L1070mm","103859",1070,null,"STK",{"$f":"VLOOKUP(G728,sanschie!A:G,7,0)","v":611},{"$f":"IF(Daten!$B$183=2,\"\",1)","v":1},{"$f":"IF(L728=\"\",0,$H728*$L728)","v":1070}]
["Absolut",6,18,"Absolut186",null,"ABS 180 Profilkeramik-Rohr mit Muffe L660mm","103953",660,null,"STK",{"$f":"VLOOKUP(G729,sanschie!A:G,7,0)","v":69},null,{"$f":"IF(L729=0,0,IF(L729=\"\",0,L729*H729))","v":0}]
["Absolut",7,18,"Absolut187",null,"ABS 180 Fertigfusspaket ","103891","0",null,"STK",{"$f":"VLOOKUP(G730,sanschie!A:G,7,0)","v":311},{"$f":"IF(Daten!$B$183=2,\"\",1)","v":1}]
["Absolut",8,18,"Absolut188",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G731,sanschie!A:G,7,0)","v":18}]
["Absolut",9,18,"Absolut189",null,"CHZ 180 Keramik Fuss-Scheibe geschlossen","103700","0",null,"STK",{"$f":"VLOOKUP(G732,sanschie!A:G,7,0)","v":35}]
["Absolut",10,18,"Absolut1810",null,"ABS Sockelplatte aus Beton EZ 360 x 360mm","103871","0",null,"STK",{"$f":"VLOOKUP(G733,sanschie!A:G,7,0)","v":155}]
["Absolut",11,18,"Absolut1811",null,"ABS 180 Rauchrohr-Anschlusspaket 90° RA  ","103983",1330,null,"STK",{"$f":"VLOOKUP(G734,sanschie!A:G,7,0)","v":386},{"$f":"IF(N734=0,\"\",N734)","v":1},{"$f":"IF(L734=0,0,IF(L734=\"\",0,L734*H734))","v":1330},{"$f":"SUM(O734:P734)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",12,18,"Absolut1812",null,"ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","103995",1330,null,"STK",{"$f":"VLOOKUP(G735,sanschie!A:G,7,0)","v":404},{"$f":"IF(N735=0,\"\",N735)","v":""},{"$f":"IF(L735=0,0,IF(L735=\"\",0,L735*H735))","v":0},{"$f":"SUM(O735:P735)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",13,18,"Absolut1813",null,"ABS 180  Rauchrohranschluss Stutzen-Set 90° Ø180mm","104001","0",null,"STK",{"$f":"VLOOKUP(G736,sanschie!A:G,7,0)","v":204}]
["Absolut",14,18,"Absolut1814",null,"ABS 180 Rauchrohranschluss Stutzen-Set 45°","104007","0",null,"STK",{"$f":"VLOOKUP(G737,sanschie!A:G,7,0)","v":204}]
["Absolut",15,18,"Absolut1815",null,"ABS 180 Steckadapter ","104268","0",null,"STK",{"$f":"VLOOKUP(G738,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=2,1,\"\")","v":""}]
["Absolut",16,18,"Absolut1816",null,"ABS 180 Putztür-Anschlusspaket ","103966",1330,null,"STK",{"$f":"VLOOKUP(G739,sanschie!A:G,7,0)","v":448},{"$f":"IF(N739=0,\"\",N739)","v":""},{"$f":"IF(L739=0,0,IF(L739=\"\",0,L739*H739))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",17,18,"Absolut1817",null,"ABS 180 Putztüranschluss Stutzen Set","104274","0",null,"STK",{"$f":"VLOOKUP(G740,sanschie!A:G,7,0)","v":336}]
["Absolut",18,18,"Absolut1818",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G741,sanschie!A:G,7,0)","v":27}]
["Absolut",19,18,"Absolut1819",null,"ABS Thermodichtset EZ 360x360mm und 380x380mm","104190","0",null,"STK",{"$f":"VLOOKUP(G742,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$G$280=Vokabel!$A$413,1,\"\")","v":""}]
["Absolut",20,18,"Absolut1820",null,"ABS Handyplatte EZ Faserzement 360 x 360mm","104144","0",null,"STK",{"$f":"VLOOKUP(G743,sanschie!A:G,7,0)","v":106},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",21,18,"Absolut1821",null,"ABS Handyplatte EZ Inox 360 x 360mm  ","104170","0",null,"STK",{"$f":"VLOOKUP(G744,sanschie!A:G,7,0)","v":155},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",22,18,"Absolut1822",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G745,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",23,18,"Absolut1823",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G746,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",24,18,"Absolut1824",null,"ABS Handyplatte EZ Kupfer 360 x 360mm  ","140787","0",null,"STK",{"$f":"VLOOKUP(G747,sanschie!A:G,7,0)","v":229}]
["Absolut",25,18,"Absolut1825",null,"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben","140932","0",null,"STK",{"$f":"VLOOKUP(G748,sanschie!A:G,7,0)","v":75}]
["Absolut",26,18,"Absolut1826",null,"ABS 180 Abströmkonus verkupfert","104206","0",null,"STK",{"$f":"VLOOKUP(G749,sanschie!A:G,7,0)","v":174}]
["Absolut",27,18,"Absolut1827",null,"ABS Anschlussmantelstein EZ 360 x 360mm L330","103917","0",null,"STK",{"$f":"VLOOKUP(G750,sanschie!A:G,7,0)","v":80},{"$f":"IF(N750=0,\"\",N750)","v":1},null,{"$f":"IF(Daten!$B$193=0,0,N739+N734+N735)","v":1}]
["Absolut",28,18,"Absolut1828",null,"ABS 180 Schleifung EZ 5° auf Bestellung","104059","0",null,"STK",{"$f":"VLOOKUP(G751,sanschie!A:G,7,0)","v":1010}]
["Absolut",29,18,"Absolut1829",null,"ABS 180 Abstandhalter offen zu Schleifung","104083","0",null,"STK",{"$f":"VLOOKUP(G752,sanschie!A:G,7,0)","v":27}]
["Absolut",30,18,"Absolut1830",null,"ABS 180 Anschlusskonus EZ mit Doppelfutter DN180mm","103899","0",null,"STK",{"$f":"VLOOKUP(G753,sanschie!A:G,7,0)","v":266},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",31,18,"Absolut1831",null,"ABS 180 Adapterring von 180mm auf 180mm L90mm","103907","0",null,"STK",{"$f":"VLOOKUP(G754,sanschie!A:G,7,0)","v":46},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",32,18,"Absolut1832",null,"KER 180  Keranova-Fugenglätter","103474","0",null,"STK",{"$f":"VLOOKUP(G755,sanschie!A:G,7,0)","v":61}]
["Absolut",33,18,"Absolut1833",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø100mm","104014","0",null,"STK",{"$f":"VLOOKUP(G756,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",34,18,"Absolut1834",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm","104015","0",null,"STK",{"$f":"VLOOKUP(G757,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",35,18,"Absolut1835",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø130mm","104016","0",null,"STK",{"$f":"VLOOKUP(G758,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",36,18,"Absolut1836",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø150mm","104017","0",null,"STK",{"$f":"VLOOKUP(G759,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",37,18,"Absolut1837",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø180mm","104018","0",null,"STK",{"$f":"VLOOKUP(G760,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",38,18,"Absolut1838",null,"ABS 180 Kondensatfalle zu RA 45° Ø130mm","104032","0",null,"STK",{"$f":"VLOOKUP(G761,sanschie!A:G,7,0)","v":347}]
["Absolut",39,18,"Absolut1839",null,"ABS 180 Kondensatfalle zu RA 45° Ø150mm","104033","0",null,"STK",{"$f":"VLOOKUP(G762,sanschie!A:G,7,0)","v":347}]
["Absolut",40,18,"Absolut1840",null,"ABS 180 Kondensatfalle zu RA 45° Ø160mm","104034","0",null,"STK",{"$f":"VLOOKUP(G763,sanschie!A:G,7,0)","v":347}]
["Absolut",41,18,"Absolut1841",null,"ABS 180 Kondensatfalle zu RA 45° Ø180mm ","104035","0",null,"STK",{"$f":"VLOOKUP(G764,sanschie!A:G,7,0)","v":347}]
["Absolut",42,18,"Absolut1842",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G765,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",43,18,"Absolut1843",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G766,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",44,18,"Absolut1844",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G767,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",45,18,"Absolut1845",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G768,sanschie!A:G,7,0)","v":23},{"$f":"IF(L730=1,1,\"\")","v":1}]
["Absolut",46,18,"Absolut1846",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G769,sanschie!A:G,7,0)","v":489},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""}]
["Absolut",47,18,"Absolut1847",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G770,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",48,18,"Absolut1848",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G771,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",49,18,"Absolut1849",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G772,sanschie!A:G,7,0)","v":14},{"$f":"IF(Daten!$B$183=2,N772,Sortimente!P772)","v":""},null,{"$f":"ROUNDUP(O772,0)","v":3},{"$f":"L727/2","v":2.5},{"$f":"IF(L727<=8,\"\",IF(L727<=10,1,IF(L727<=12,2,IF(L727<=14,3,4))))","v":""}]
["Absolut",50,18,"Absolut1850",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G773,sanschie!A:G,7,0)","v":303},{"$f":"IF(N773=0,\"\",N773)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",51,18,"Absolut1851",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G774,sanschie!A:G,7,0)","v":94},{"$f":"IF(N774=0,\"\",N774)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",52,18,"Absolut1852",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G775,sanschie!A:G,7,0)","v":19},{"$f":"IF(L753=1,N775,IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0))))","v":""},null,{"$f":"ROUNDUP(O775,0)","v":2},{"$f":"L727*0.4","v":2}]
["Absolut",53,18,"Absolut1853",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G776,sanschie!A:G,7,0)","v":35},{"$f":"IF(N776<=12.7,1,2)","v":1},null,{"$f":"IF(L728=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",54,18,"Absolut1854",null,"ABS 180 Basten Standard Inox","104212","0",null,"STK",{"$f":"VLOOKUP(G777,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",55,18,"Absolut1855",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",{"$f":"VLOOKUP(G778,sanschie!A:G,7,0)","v":362},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",56,18,"Absolut1856",null,"ABS 180 Sairlift Inox","104224","0",null,"STK",{"$f":"VLOOKUP(G779,sanschie!A:G,7,0)","v":400},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",57,18,"Absolut1857",null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",{"$f":"VLOOKUP(G780,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",58,18,"Absolut1858",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G781,sanschie!A:G,7,0)","v":123.1}]
["Absolut",59,18,"Absolut1859",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G782,sanschie!A:G,7,0)","v":258.8}]
["Absolut",60,18,"Absolut1860",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G783,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",61,18,"Absolut1861",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G784,sanschie!A:G,7,0)","v":44.9}]
["Absolut",62,18,"Absolut1862",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G785,sanschie!A:G,7,0)","v":7.5}]
["Absolut",63,18,"Absolut1863",null,"ZBH 190 Verschlusszapfen 2Stk. aus Schaumstoff","103833","0",null,"STK",{"$f":"VLOOKUP(G786,sanschie!A:G,7,0)","v":26.5}]
["Absolut",64,18,"Absolut1864",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G787,sanschie!A:G,7,0)","v":452}]
["Absolut",65,18,"Absolut1865",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G788,sanschie!A:G,7,0)","v":538}]
["Absolut",{"$f":"B788+1","v":66},{"$f":"C788","v":18},"Absolut1866",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G789,sanschie!A:G,7,0)","v":634}]
["Absolut",67,18,"Absolut1867",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G790,sanschie!A:G,7,0)","v":695}]
["Absolut",68,18,"Absolut1868",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G791,sanschie!A:G,7,0)","v":797}]
["Absolut",69,18,"Absolut1869",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G792,sanschie!A:G,7,0)","v":873}]
["Absolut",70,18,"Absolut1870",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G793,sanschie!A:G,7,0)","v":13.8}]
["Absolut",{"$f":"B793+1","v":71},{"$f":"C793","v":18},{"$f":"A794&C794&B794","v":"Absolut1871"},null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G794,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",{"$f":"B794+1","v":72},{"$f":"C794","v":18},"Absolut1872",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G795,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B795+1","v":73},{"$f":"C795","v":18},"Absolut1873",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G796,sanschie!A:G,7,0)","v":26}]
["Absolut",{"$f":"B796+1","v":74},{"$f":"C796","v":18},"Absolut1874",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G797,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,20,"Absolut200","P","Absolut-Kaminanlage Ø 20","Absolut 20","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G798,sanschie!A:G,7,0)","v":0},null,{"$f":"I798*1000","v":9000}]
["Absolut",{"$f":"B798+1","v":1},{"$f":"C798","v":20},"Absolut201",null,"ABS Mantelstein EZ 380 x 380mm L330mm","103913","0",null,"STK",{"$f":"VLOOKUP(G799,sanschie!A:G,7,0)","v":33},{"$f":"ROUND(M799,0)-N826-M800","v":23},{"$f":"((M798-M804)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N799*330","v":0}]
["Absolut",{"$f":"B799+1","v":2},{"$f":"C799","v":20},"Absolut202",null,"ABS Thermo-Trennstein EZ 380 x 380mm L330mm","103932","0",null,"STK",{"$f":"VLOOKUP(G800,sanschie!A:G,7,0)","v":222},{"$f":"IF(M800=0,\"\",M800)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,20,"Absolut203",null,"ABS Thermo-Fussplatte EZ 380 x 380mm","103850","0",null,"STK",{"$f":"VLOOKUP(G801,sanschie!A:G,7,0)","v":136}]
["Absolut",4,20,"Absolut204",null,"ABS 200 Profilkeramik-Rohr mit Muffe L1330mm","103949",1330,null,"STK",{"$f":"VLOOKUP(G802,sanschie!A:G,7,0)","v":145},{"$f":"ROUNDUP(M802,0)","v":5},{"$f":"(M798-O799-M804-M809-M810-M814)/H802","v":4.9624060150375939}]
["Absolut",5,20,"Absolut205",null,"ABS 200 Profilkeramik-Rohr mit Muffe L660mm","103954",660,null,"STK",{"$f":"VLOOKUP(G803,sanschie!A:G,7,0)","v":83},null,{"$f":"IF(L803=0,0,IF(L803=\"\",0,L803*H803))","v":0}]
["Absolut",6,20,"Absolut206",null,"ABS 200 Fertigfuss EZ  L1070mm ","103860",1070,null,"STK",{"$f":"VLOOKUP(G804,sanschie!A:G,7,0)","v":734},{"$f":"IF(Daten!$B$183=2,\"\",1)","v":1},{"$f":"IF(L804=\"\",0,$H804*$L804)","v":1070}]
["Absolut",7,20,"Absolut207",null,"ABS 200 Fertigfusspaket ","103892","0",null,"STK",{"$f":"VLOOKUP(G805,sanschie!A:G,7,0)","v":311},{"$f":"IF(Daten!$B$183=2,\"\",1)","v":1}]
["Absolut",8,20,"Absolut208",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G806,sanschie!A:G,7,0)","v":18}]
["Absolut",9,20,"Absolut209",null,"CHZ 200 Keramik Fuss-Scheibe geschlossen","103701","0",null,"STK",{"$f":"VLOOKUP(G807,sanschie!A:G,7,0)","v":45}]
["Absolut",10,20,"Absolut2010",null,"ABS Sockelplatte aus Beton EZ 380 x 380mm","103872","0",null,"STK",{"$f":"VLOOKUP(G808,sanschie!A:G,7,0)","v":160}]
["Absolut",11,20,"Absolut2011",null,"ABS 200 Rauchrohr-Anschlusspaket 90° RA  ","103984",1330,null,"STK",{"$f":"VLOOKUP(G809,sanschie!A:G,7,0)","v":434},{"$f":"IF(N809=0,\"\",N809)","v":1},{"$f":"IF(L809=0,0,IF(L809=\"\",0,L809*H809))","v":1330},{"$f":"SUM(O809:P809)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",12,20,"Absolut2012",null,"ABS 200 Rauchrohr-Anschlusspaket 45° RA  ","103996",1330,null,"STK",{"$f":"VLOOKUP(G810,sanschie!A:G,7,0)","v":466},{"$f":"IF(N810=0,\"\",N810)","v":""},{"$f":"IF(L810=0,0,IF(L810=\"\",0,L810*H810))","v":0},{"$f":"SUM(O810:P810)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",13,20,"Absolut2013",null,"ABS 200 Rauchrohranschluss Stutzen-Set 90° Ø200mm","104002","0",null,"STK",{"$f":"VLOOKUP(G811,sanschie!A:G,7,0)","v":212}]
["Absolut",14,20,"Absolut2014",null,"ABS 200 Rauchrohranschluss Stutzen-Set 45°","104008","0",null,"STK",{"$f":"VLOOKUP(G812,sanschie!A:G,7,0)","v":212}]
["Absolut",15,20,"Absolut2015",null,"ABS 200 Steckadapter ","104269","0",null,"STK",{"$f":"VLOOKUP(G813,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=2,1,\"\")","v":""}]
["Absolut",16,20,"Absolut2016",null,"ABS 200 Putztür-Anschlusspaket ","103967",1330,null,"STK",{"$f":"VLOOKUP(G814,sanschie!A:G,7,0)","v":483},{"$f":"IF(N814=0,\"\",N814)","v":""},{"$f":"IF(L814=0,0,IF(L814=\"\",0,L814*H814))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",17,20,"Absolut2017",null,"ABS 200 Putztüranschluss Stutzen Set","104275","0",null,"STK",{"$f":"VLOOKUP(G815,sanschie!A:G,7,0)","v":349}]
["Absolut",18,20,"Absolut2018",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G816,sanschie!A:G,7,0)","v":27}]
["Absolut",19,20,"Absolut2019",null,"ABS 200 Rauchzugklappe  L330mm","104239","0",null,"STK",{"$f":"VLOOKUP(G817,sanschie!A:G,7,0)","v":367}]
["Absolut",20,20,"Absolut2020",null,"ABS Thermodichtset EZ 360x360mm und 380x380mm","104190","0",null,"STK",{"$f":"VLOOKUP(G818,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$G$280=Vokabel!$A$413,1,\"\")","v":""}]
["Absolut",21,20,"Absolut2021",null,"ABS Handyplatte EZ Faserzement 380 x 380mm ","104145","0",null,"STK",{"$f":"VLOOKUP(G819,sanschie!A:G,7,0)","v":118},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",22,20,"Absolut2022",null,"ABS Handyplatte EZ Inox 380 x 380mm  ","104171","0",null,"STK",{"$f":"VLOOKUP(G820,sanschie!A:G,7,0)","v":180},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",23,20,"Absolut2023",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G821,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",24,20,"Absolut2024",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G822,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",25,20,"Absolut2025",null,"ABS Handyplatte EZ Kupfer 380 x 380mm ","140788","0",null,"STK",{"$f":"VLOOKUP(G823,sanschie!A:G,7,0)","v":241}]
["Absolut",26,20,"Absolut2026",null,"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben","140932","0",null,"STK",{"$f":"VLOOKUP(G824,sanschie!A:G,7,0)","v":75}]
["Absolut",{"$f":"B822+1","v":25},{"$f":"C822","v":20},"Absolut2025",null,"ABS 200 Abströmkonus verkupfert","104207","0",null,"STK",{"$f":"VLOOKUP(G825,sanschie!A:G,7,0)","v":197}]
["Absolut",26,20,"Absolut2026",null,"ABS Anschlussmantelstein EZ 380 x 380mm L330","103918","0",null,"STK",{"$f":"VLOOKUP(G826,sanschie!A:G,7,0)","v":82},{"$f":"IF(N826=0,\"\",N826)","v":1},null,{"$f":"IF(Daten!$B$193=0,0,N814+N809+N810)","v":1}]
["Absolut",27,20,"Absolut2027",null,"ABS 200 Schleifung EZ 5° auf Bestellung","104066","0",null,"STK",{"$f":"VLOOKUP(G827,sanschie!A:G,7,0)","v":1134}]
["Absolut",28,20,"Absolut2028",null,"ABS 200 Abstandhalter offen zu Schleifung","104084","0",null,"STK",{"$f":"VLOOKUP(G828,sanschie!A:G,7,0)","v":38}]
["Absolut",29,20,"Absolut2029",null,"ABS 200 Anschlusskonus EZ mit Doppelfutter DN200mm","103900","0",null,"STK",{"$f":"VLOOKUP(G829,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",30,20,"Absolut2030",null,"ABS 200 Adapterring von 200mm auf 200mm L90mm","103909","0",null,"STK",{"$f":"VLOOKUP(G830,sanschie!A:G,7,0)","v":65},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",31,20,"Absolut2031",null,"KER 200  Keranova-Fugenglätter","103475","0",null,"STK",{"$f":"VLOOKUP(G831,sanschie!A:G,7,0)","v":72}]
["Absolut",32,20,"Absolut2032",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø100mm","104019","0",null,"STK",{"$f":"VLOOKUP(G832,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",33,20,"Absolut2033",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø120mm","104020","0",null,"STK",{"$f":"VLOOKUP(G833,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",34,20,"Absolut2034",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø130mm","104021","0",null,"STK",{"$f":"VLOOKUP(G834,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",35,20,"Absolut2035",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø150mm","104022","0",null,"STK",{"$f":"VLOOKUP(G835,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",36,20,"Absolut2036",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø180mm","104023","0",null,"STK",{"$f":"VLOOKUP(G836,sanschie!A:G,7,0)","v":210},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",37,20,"Absolut2037",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø200mm","104024","0",null,"STK",{"$f":"VLOOKUP(G837,sanschie!A:G,7,0)","v":222},{"$f":"IF(Daten!$B$226=8,1,\"\")","v":""}]
["Absolut",38,20,"Absolut2038",null,"ABS 200 Kondensatfalle zu RA 45° Ø130mm ","104036","0",null,"STK",{"$f":"VLOOKUP(G838,sanschie!A:G,7,0)","v":365}]
["Absolut",39,20,"Absolut2039",null,"ABS 200 Kondensatfalle zu RA 45° Ø150mm ","104037","0",null,"STK",{"$f":"VLOOKUP(G839,sanschie!A:G,7,0)","v":365}]
["Absolut",40,20,"Absolut2040",null,"ABS 200 Kondensatfalle zu RA 45° Ø160mm","104038","0",null,"STK",{"$f":"VLOOKUP(G840,sanschie!A:G,7,0)","v":365}]
["Absolut",41,20,"Absolut2041",null,"ABS 200 Kondensatfalle zu RA 45° Ø180mm ","104039","0",null,"STK",{"$f":"VLOOKUP(G841,sanschie!A:G,7,0)","v":365}]
["Absolut",42,20,"Absolut2042",null,"ABS 200 Kondensatfalle zu RA 45° Ø200mm ","104040","0",null,"STK",{"$f":"VLOOKUP(G842,sanschie!A:G,7,0)","v":365}]
["Absolut",43,20,"Absolut2043",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G843,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",44,20,"Absolut2044",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G844,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",45,20,"Absolut2045",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G845,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",46,20,"Absolut2046",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G846,sanschie!A:G,7,0)","v":23},{"$f":"IF(L805=1,1,\"\")","v":1}]
["Absolut",47,20,"Absolut2047",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G847,sanschie!A:G,7,0)","v":489},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""}]
["Absolut",48,20,"Absolut2048",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G848,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",49,20,"Absolut2049",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G849,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",50,20,"Absolut2050",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G850,sanschie!A:G,7,0)","v":14},{"$f":"IF(Daten!$B$183=2,N850,Sortimente!P850)","v":""},null,{"$f":"ROUNDUP(O850,0)","v":3},{"$f":"L802/2","v":2.5},{"$f":"IF(L802<=8,\"\",IF(L802<=10,1,IF(L802<=12,2,IF(L802<=14,3,4))))","v":""}]
["Absolut",51,20,"Absolut2051",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G851,sanschie!A:G,7,0)","v":303},{"$f":"IF(N851=0,\"\",N851)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",52,20,"Absolut2052",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G852,sanschie!A:G,7,0)","v":94},{"$f":"IF(N852=0,\"\",N852)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",53,20,"Absolut2053",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G853,sanschie!A:G,7,0)","v":19},{"$f":"IF(L829=1,N853,IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0))))","v":""},null,{"$f":"ROUNDUP(O853,0)","v":2},{"$f":"L802*0.4","v":2}]
["Absolut",54,20,"Absolut2054",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G854,sanschie!A:G,7,0)","v":35},{"$f":"IF(N854<=12.7,1,2)","v":1},null,{"$f":"IF(L804=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",55,20,"Absolut2055",null,"ABS 200 Basten Standard Inox","104213","0",null,"STK",{"$f":"VLOOKUP(G855,sanschie!A:G,7,0)","v":361},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",56,20,"Absolut2056",null,"ABS 200 Basten Standard Kupfer","104219","0",null,"STK",{"$f":"VLOOKUP(G856,sanschie!A:G,7,0)","v":375},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",57,20,"Absolut2057",null,"ABS 200 Sairlift Inox","104225","0",null,"STK",{"$f":"VLOOKUP(G857,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",58,20,{"$f":"A858&C858&B858","v":"Absolut2058"},null,"ABS 200 Sairlift Kupfer","104230","0",null,"STK",{"$f":"VLOOKUP(G858,sanschie!A:G,7,0)","v":434},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",59,20,"Absolut2059",null,"ZBH 200 Verschlussbüchse weiss ØA 300mm","103839","0",null,"STK",{"$f":"VLOOKUP(G859,sanschie!A:G,7,0)","v":123.1}]
["Absolut",60,20,"Absolut2060",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G860,sanschie!A:G,7,0)","v":258.8}]
["Absolut",61,20,"Absolut2061",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G861,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",62,20,"Absolut2062",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G862,sanschie!A:G,7,0)","v":44.9}]
["Absolut",63,20,"Absolut2063",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G863,sanschie!A:G,7,0)","v":7.5}]
["Absolut",{"$f":"B863+1","v":64},{"$f":"C863","v":20},"Absolut2064",null,"ZBH 210 Verschlusszapfen 2Stk. aus Schaumstoff","103834","0",null,"STK",{"$f":"VLOOKUP(G864,sanschie!A:G,7,0)","v":26.5}]
["Absolut",65,20,"Absolut2065",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G865,sanschie!A:G,7,0)","v":13.8}]
["Absolut",66,20,"Absolut2066",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G866,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",67,20,"Absolut2067",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G867,sanschie!A:G,7,0)","v":322}]
["Absolut",68,20,"Absolut2068",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G868,sanschie!A:G,7,0)","v":26}]
["Absolut",{"$f":"B868+1","v":69},{"$f":"C868","v":20},{"$f":"A869&C869&B869","v":"Absolut2069"},null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G869,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,25,{"$f":"A870&C870&B870","v":"Absolut250"},"P","Absolut-Kaminanlage Ø 25","Absolut 25","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G870,sanschie!A:G,7,0)","v":0},null,{"$f":"I870*1000","v":9000}]
["Absolut",{"$f":"B870+1","v":1},{"$f":"C870","v":25},{"$f":"A871&C871&B871","v":"Absolut251"},null,"ABS Mantelstein EZ 480 x 480mm L330mm","103914","0",null,"STK",{"$f":"VLOOKUP(G871,sanschie!A:G,7,0)","v":55},{"$f":"ROUND(M871,0)-N893-M872","v":27},{"$f":"((M870)*3)/1000","v":27},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N871*330","v":0}]
["Absolut",{"$f":"B871+1","v":2},{"$f":"C871","v":25},{"$f":"A872&C872&B872","v":"Absolut252"},null,"ABS Thermo-Trennstein EZ 480 x 480mm L330mm","103933","0",null,"STK",{"$f":"VLOOKUP(G872,sanschie!A:G,7,0)","v":333},{"$f":"IF(M872=0,\"\",M872)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,25,"Absolut253",null,"ABS Thermo-Fussplatte EZ 480 x 480mm","103851","0",null,"STK",{"$f":"VLOOKUP(G873,sanschie!A:G,7,0)","v":149}]
["Absolut",4,25,"Absolut254",null,"ABS 250 Profilkeramik-Rohr mit Muffe L660mm","103955",665,null,"STK",{"$f":"VLOOKUP(G874,sanschie!A:G,7,0)","v":98},{"$f":"ROUNDUP(M874,0)","v":12},{"$f":"(M870-O871-M875-M879-M880-M884)/1000/0.66","v":11.113636363636363}]
["Absolut",5,25,"Absolut255",null,"ABS 250 Grundpaket","103861",1000,null,"STK",{"$f":"VLOOKUP(G875,sanschie!A:G,7,0)","v":736},{"$f":"IF(Daten!$B$183=2,\"\",1)","v":1},{"$f":"IF(L875=0,0,IF(L875=\"\",0,L875*1000))","v":1000}]
["Absolut",6,25,"Absolut256",null,"ABS Sockelplatte aus Beton EZ 480 x 480mm","103873","0",null,"STK",{"$f":"VLOOKUP(G876,sanschie!A:G,7,0)","v":179},1]
["Absolut",7,25,"Absolut257",null,"CHZ 180-200 Füllstein zu Schnellbaufund. L330mm","103710","0",null,"STK",{"$f":"VLOOKUP(G877,sanschie!A:G,7,0)","v":21}]
["Absolut",8,25,"Absolut258",null,"CHZ 250 Keramik Fuss-Scheibe geschlossen","103702","0",null,"STK",{"$f":"VLOOKUP(G878,sanschie!A:G,7,0)","v":92}]
["Absolut",9,25,"Absolut259",null,"ABS 250 Rauchrohr-Anschlusspaket 90° RA  ","103985",665,null,"STK",{"$f":"VLOOKUP(G879,sanschie!A:G,7,0)","v":490},{"$f":"IF(N879=0,\"\",N879)","v":1},{"$f":"IF(L879=0,0,IF(L879=\"\",0,L879*H879))","v":665},{"$f":"SUM(O879:P879)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",10,25,"Absolut2510",null,"ABS 250 Rauchrohr-Anschlusspaket 45° RA  ","103997",665,null,"STK",{"$f":"VLOOKUP(G880,sanschie!A:G,7,0)","v":521},{"$f":"IF(N880=0,\"\",N880)","v":""},{"$f":"IF(L880=0,0,IF(L880=\"\",0,L880*H880))","v":0},{"$f":"SUM(O880:P880)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",11,25,"Absolut2511",null,"ABS 250 Rauchrohranschluss Stutzen-Set 90° Ø250mm","104003","0",null,"STK",{"$f":"VLOOKUP(G881,sanschie!A:G,7,0)","v":249}]
["Absolut",12,25,"Absolut2512",null,"ABS 250 Rauchrohranschluss Stutzen-Set 45°","104009","0",null,"STK",{"$f":"VLOOKUP(G882,sanschie!A:G,7,0)","v":249}]
["Absolut",13,25,"Absolut2513",null,"ABS 250 Steckadapter ","104271","0",null,"STK",{"$f":"VLOOKUP(G883,sanschie!A:G,7,0)","v":234},{"$f":"IF(Daten!$B$226=2,1,\"\")","v":""}]
["Absolut",14,25,"Absolut2514",null,"ABS 250 Putztür-Anschlusspaket ","103968",665,null,"STK",{"$f":"VLOOKUP(G884,sanschie!A:G,7,0)","v":546},{"$f":"IF(N884=0,\"\",N884)","v":""},{"$f":"IF(L884=0,0,IF(L884=\"\",0,L884*H884))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",15,25,"Absolut2515",null,"ABS 250 Putztüranschluss Stutzen Set","104276","0",null,"STK",{"$f":"VLOOKUP(G885,sanschie!A:G,7,0)","v":472}]
["Absolut",16,25,"Absolut2516",null,"ABS Handyplatte EZ Faserzement 480 x 480mm ","104146","0",null,"STK",{"$f":"VLOOKUP(G886,sanschie!A:G,7,0)","v":137},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",17,25,"Absolut2517",null,"ABS Handyplatte EZ Inox 480 x 480mm","104172","0",null,"STK",{"$f":"VLOOKUP(G887,sanschie!A:G,7,0)","v":180},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",18,25,"Absolut2518",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G888,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",19,25,"Absolut2519",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G889,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",20,25,"Absolut2520",null,"ABS Handyplatte EZ Kupfer 480 x 480mm","140789","0",null,"STK",{"$f":"VLOOKUP(G890,sanschie!A:G,7,0)","v":260}]
["Absolut",21,25,"Absolut2521",null,"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben","140932","0",null,"STK",{"$f":"VLOOKUP(G891,sanschie!A:G,7,0)","v":75}]
["Absolut",22,25,"Absolut2522",null,"ABS 250 Abströmkonus verkupfert","104208","0",null,"STK",{"$f":"VLOOKUP(G892,sanschie!A:G,7,0)","v":258}]
["Absolut",23,25,"Absolut2523",null,"ABS Anschlussmantelstein EZ 480 x 480mm L330","103919","0",null,"STK",{"$f":"VLOOKUP(G893,sanschie!A:G,7,0)","v":104},{"$f":"IF(N893=0,\"\",N893)","v":""},null,0,"lt. Benjamin ist dieser Stein nicht lagernd"]
["Absolut",24,25,"Absolut2524",null,"ABS 200 Schleifung EZ 5° auf Bestellung","104066","0",null,"STK",{"$f":"VLOOKUP(G894,sanschie!A:G,7,0)","v":1134}]
["Absolut",25,25,"Absolut2525",null,"ABS 250 Abstandhalter offen zu Schleifung","104085","0",null,"STK",{"$f":"VLOOKUP(G895,sanschie!A:G,7,0)","v":44}]
["Absolut",26,25,"Absolut2526",null,"ABS 250 Anschlusskonus EZ mit Doppelfutter DN250mm","103901","0",null,"STK",{"$f":"VLOOKUP(G896,sanschie!A:G,7,0)","v":365},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",27,25,"Absolut2527",null,"ABS 250 Adapterring von 250mm auf 250mm L90mm","103910","0",null,"STK",{"$f":"VLOOKUP(G897,sanschie!A:G,7,0)","v":79},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",28,25,"Absolut2528",null,"KER 250 Keranova-Fugenglätter","103476","0",null,"STK",{"$f":"VLOOKUP(G898,sanschie!A:G,7,0)","v":79}]
["Absolut",29,25,"Absolut2529",null,"ABS 250 Doppelfutter zu Rauchrohranschluss Ø180mm","104025","0",null,"STK",{"$f":"VLOOKUP(G899,sanschie!A:G,7,0)","v":210},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",30,25,"Absolut2530",null,"ABS 250 Doppelfutter zu Rauchrohranschluss Ø200mm","104026","0",null,"STK",{"$f":"VLOOKUP(G900,sanschie!A:G,7,0)","v":222},{"$f":"IF(Daten!$B$226=8,1,\"\")","v":""}]
["Absolut",31,25,"Absolut2531",null,"ABS 250 Doppelfutter zu Rauchrohranschluss Ø250mm","104027","0",null,"STK",{"$f":"VLOOKUP(G901,sanschie!A:G,7,0)","v":234},{"$f":"IF(Daten!$B$226=9,1,\"\")","v":""}]
["Absolut",32,25,"Absolut2532",null,"ABS 250 Kondensatfalle zu RA 45° Ø180mm","104041","0",null,"STK",{"$f":"VLOOKUP(G902,sanschie!A:G,7,0)","v":426}]
["Absolut",33,25,"Absolut2533",null,"ABS 250 Kondensatfalle zu RA 45° Ø200mm","104042","0",null,"STK",{"$f":"VLOOKUP(G903,sanschie!A:G,7,0)","v":426}]
["Absolut",34,25,"Absolut2534",null,"ABS 250 Kondensatfalle zu RA 45° Ø250mm","104043","0",null,"STK",{"$f":"VLOOKUP(G904,sanschie!A:G,7,0)","v":426}]
["Absolut",35,25,"Absolut2535",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G905,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",36,25,"Absolut2536",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G906,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",37,25,"Absolut2537",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G907,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",38,25,"Absolut2538",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G908,sanschie!A:G,7,0)","v":489},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""}]
["Absolut",39,25,"Absolut2539",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G909,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",40,25,"Absolut2540",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G910,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",41,25,"Absolut2541",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G911,sanschie!A:G,7,0)","v":14},{"$f":"IF(Daten!$B$183=2,N911,Sortimente!P911)","v":2},null,{"$f":"ROUNDUP(O911,0)","v":6},{"$f":"L874/2","v":6},{"$f":"IF(L874<=8,\"\",IF(L874<=10,1,IF(L874<=12,2,IF(L874<=14,3,4))))","v":2}]
["Absolut",42,25,"Absolut2542",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G912,sanschie!A:G,7,0)","v":303},{"$f":"IF(N912=0,\"\",N912)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",43,25,"Absolut2543",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G913,sanschie!A:G,7,0)","v":94},{"$f":"IF(N913=0,\"\",N913)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",44,25,"Absolut2544",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G914,sanschie!A:G,7,0)","v":19},{"$f":"IF(L896=1,N914,IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0))))","v":""},null,{"$f":"ROUNDUP(O914,0)","v":5},{"$f":"L874*0.4","v":4.8000000000000007}]
["Absolut",45,25,"Absolut2545",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G915,sanschie!A:G,7,0)","v":35},{"$f":"IF(N915<=12.7,1,2)","v":1},null,{"$f":"Daten!$B$61","v":9}]
["Absolut",46,25,"Absolut2546",null,"ABS 250 Basten Standard Inox","104214","0",null,"STK",{"$f":"VLOOKUP(G916,sanschie!A:G,7,0)","v":400},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",47,25,"Absolut2547",null,"ABS 250 Basten Standard Kupfer","104221","0",null,"STK",{"$f":"VLOOKUP(G917,sanschie!A:G,7,0)","v":545},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",48,25,"Absolut2548",null,"ABS 250 Sairlift Inox","104226","0",null,"STK",{"$f":"VLOOKUP(G918,sanschie!A:G,7,0)","v":465},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",49,25,"Absolut2549",null,"ABS 250 Sairlift Kupfer","104231","0",null,"STK",{"$f":"VLOOKUP(G919,sanschie!A:G,7,0)","v":480},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",50,25,"Absolut2550",null,"ZBH 250 Verschlussbüchse weiss ØA 300mm","103840","0",null,"STK",{"$f":"VLOOKUP(G920,sanschie!A:G,7,0)","v":138}]
["Absolut",51,25,{"$f":"A921&C921&B921","v":"Absolut2551"},null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G921,sanschie!A:G,7,0)","v":258.8}]
["Absolut",52,25,{"$f":"A922&C922&B922","v":"Absolut2552"},null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G922,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",53,25,{"$f":"A923&C923&B923","v":"Absolut2553"},null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G923,sanschie!A:G,7,0)","v":44.9}]
["Absolut",54,25,"Absolut2554",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G924,sanschie!A:G,7,0)","v":7.5}]
["Absolut",55,25,"Absolut2555",null,"ZBH 260 Verschlusszapfen 2Stk. aus Schaumstoff","103835","0",null,"STK",{"$f":"VLOOKUP(G925,sanschie!A:G,7,0)","v":31.1}]
["Absolut",56,25,"Absolut2556",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G926,sanschie!A:G,7,0)","v":13.8}]
["Absolut",57,25,"Absolut2557",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G927,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",58,25,"Absolut2558",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G928,sanschie!A:G,7,0)","v":322}]
["Absolut",59,25,"Absolut2559",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G929,sanschie!A:G,7,0)","v":26}]
["Absolut",60,25,"Absolut2560",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G930,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,30,"Absolut300","P","Absolut-Kaminanlage Ø 30","Absolut 30","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G931,sanschie!A:G,7,0)","v":0},null,{"$f":"I931*1000","v":9000}]
["Absolut",{"$f":"B931+1","v":1},{"$f":"C931","v":30},"Absolut301",null,"ABS Mantelstein EZ 550 x 550mm L330mm","103915","0",null,"STK",{"$f":"VLOOKUP(G932,sanschie!A:G,7,0)","v":101},{"$f":"ROUND(M932,0)","v":27},{"$f":"((M931)*3)/1000","v":27},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N932*330","v":0}]
["Absolut",{"$f":"B932+1","v":2},{"$f":"C932","v":30},"Absolut302",null,"ABS 300 Profilkeramik-Rohr mit Muffe L660mm","103956",665,null,"STK",{"$f":"VLOOKUP(G933,sanschie!A:G,7,0)","v":105},{"$f":"ROUNDUP(M933,0)","v":12},{"$f":"(M931-O932-M934-M936-M937)/H933","v":11.030075187969924}]
["Absolut",{"$f":"B933+1","v":3},{"$f":"C933","v":30},"Absolut303",null,"ABS 300 Grundpaket","103862",1000,null,"STK",{"$f":"VLOOKUP(G934,sanschie!A:G,7,0)","v":983},1,{"$f":"IF(L934=0,0,IF(L934=\"\",0,L934*1000))","v":1000}]
["Absolut",{"$f":"B934+1","v":4},{"$f":"C934","v":30},"Absolut304",null,"ABS Sockelplatte aus Beton EZ 550 x 550mm","103874","0",null,"STK",{"$f":"VLOOKUP(G935,sanschie!A:G,7,0)","v":197},1]
["Absolut",{"$f":"B935+1","v":5},{"$f":"C935","v":30},{"$f":"A936&C936&B936","v":"Absolut305"},null,"ABS 300 Rauchrohr-Anschlusspaket 90° RA  ","103986",665,null,"STK",{"$f":"VLOOKUP(G936,sanschie!A:G,7,0)","v":613},1,{"$f":"IF(L936=0,0,IF(L936=\"\",0,L936*H936))","v":665},{"$f":"SUM(O936:P936)","v":1},1,""]
["Absolut",{"$f":"B936+1","v":6},{"$f":"C936","v":30},"Absolut306",null,"ABS 300 Putztür-Anschlusspaket ","103969",665,null,"STK",{"$f":"VLOOKUP(G937,sanschie!A:G,7,0)","v":607},{"$f":"IF(N937=0,\"\",N937)","v":""},{"$f":"IF(N937=0,0,IF(N937=\"\",0,N937*H937))","v":0},{"$f":"IF(Daten!$B$261=1,0,Daten!$C$261)","v":0}]
["Absolut",7,30,"Absolut307",null,"ABS Handyplatte EZ Faserzement 550 x 550mm","104147","0",null,"STK",{"$f":"VLOOKUP(G938,sanschie!A:G,7,0)","v":156},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",8,30,"Absolut308",null,"ABS Handyplatte EZ Inox 550 x 550mm  ","104173","0",null,"STK",{"$f":"VLOOKUP(G939,sanschie!A:G,7,0)","v":217},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",9,30,"Absolut309",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G940,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",10,30,"Absolut3010",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G941,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",11,30,"Absolut3011",null,"ABS Handyplatte EZ Kupfer 550 x 550mm  ","140790","0",null,"STK",{"$f":"VLOOKUP(G942,sanschie!A:G,7,0)","v":279}]
["Absolut",12,30,"Absolut3012",null,"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben","140932","0",null,"STK",{"$f":"VLOOKUP(G943,sanschie!A:G,7,0)","v":75}]
["Absolut",13,30,"Absolut3013",null,"ABS 300 Abströmkonus verkupfert","104209","0",null,"STK",{"$f":"VLOOKUP(G944,sanschie!A:G,7,0)","v":358}]
["Absolut",14,30,"Absolut3014",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G945,sanschie!A:G,7,0)","v":303},{"$f":"IF(Daten!$B$287=2,1,\"\")","v":""}]
["Absolut",15,30,"Absolut3015",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G946,sanschie!A:G,7,0)","v":94},{"$f":"IF(Daten!$B$287=2,1,\"\")","v":""}]
["Absolut",16,30,"Absolut3016",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G947,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",17,30,"Absolut3017",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G948,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",18,30,"Absolut3018",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G949,sanschie!A:G,7,0)","v":35},{"$f":"ROUNDUP(M949,0)","v":1},{"$f":"N949/10","v":0.9},{"$f":"Daten!$B$61","v":9}]
["Absolut",19,30,"Absolut3019",null,"ABS 300 Basten Standard Inox","104215","0",null,"STK",{"$f":"VLOOKUP(G950,sanschie!A:G,7,0)","v":535},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",20,30,"Absolut3020",null,"ABS 300 Basten Standard Kupfer","104220","0",null,"STK",{"$f":"VLOOKUP(G951,sanschie!A:G,7,0)","v":414},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",21,30,"Absolut3021",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G952,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",22,30,"Absolut3022",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G953,sanschie!A:G,7,0)","v":14},{"$f":"IF(M953<0,\"\",M953)","v":""},{"$f":"ROUNDUP(((K931-11.66)-SUM(N936,N937))/1.33,0)","v":-10}]
["Absolut",23,30,"Absolut3023",null,"ABS 300 Anschlusskonus EZ mit Doppelfutter DN300mm","103697","0",null,"STK",{"$f":"VLOOKUP(G954,sanschie!A:G,7,0)","v":414},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",24,30,"Absolut3024",null,"ABS 300 Adapterring von 300mm auf 300mm L90mm","103911","0",null,"STK",{"$f":"VLOOKUP(G955,sanschie!A:G,7,0)","v":90},{"$f":"IF(Daten!$B$183=2,1,\"\")","v":""}]
["Absolut",25,30,"Absolut3025",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G956,sanschie!A:G,7,0)","v":258.8}]
["Absolut",26,30,"Absolut3026",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G957,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",27,30,"Absolut3027",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G958,sanschie!A:G,7,0)","v":44.9}]
["Absolut",28,30,"Absolut3028",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G959,sanschie!A:G,7,0)","v":7.5}]
["Absolut",29,30,"Absolut3029",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G960,sanschie!A:G,7,0)","v":13.8}]
["Absolut",30,30,"Absolut3030",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G961,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",31,30,"Absolut3031",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G962,sanschie!A:G,7,0)","v":322}]
["Absolut",32,30,"Absolut3032",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G963,sanschie!A:G,7,0)","v":26}]
["Absolut",33,30,"Absolut3033",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G964,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,40,"Absolut400","P","Absolut-Kaminanlage Ø 40","Absolut 40","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G965,sanschie!A:G,7,0)","v":0},null,{"$f":"I965*1000","v":9000}]
["Absolut",{"$f":"B965+1","v":1},{"$f":"C965","v":40},"Absolut401",null,"ABS Mantelstein EZ 670 x 670mm L330mm","103916","0",null,"STK",{"$f":"VLOOKUP(G966,sanschie!A:G,7,0)","v":186},{"$f":"ROUND(M966,0)","v":27},{"$f":"((M965)*3)/1000","v":27},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N966*330","v":0}]
["Absolut",{"$f":"B966+1","v":2},{"$f":"C966","v":40},"Absolut402",null,"ABS 400 Profilkeramik-Rohr mit Muffe L660mm","103957",665,null,"STK",{"$f":"VLOOKUP(G967,sanschie!A:G,7,0)","v":158},{"$f":"ROUNDUP(M967,0)","v":12},{"$f":"(M965-O966-M968-M970-M971)/H967","v":11.030075187969924}]
["Absolut",3,40,"Absolut403",null,"ABS 400 Grundpaket","103863",1000,null,"STK",{"$f":"VLOOKUP(G968,sanschie!A:G,7,0)","v":1226},1,{"$f":"IF(L968=0,0,IF(L968=\"\",0,L968*1000))","v":1000}]
["Absolut",4,40,"Absolut404",null,"ABS Sockelplatte aus Beton EZ 670 x 670mm","103875","0",null,"STK",{"$f":"VLOOKUP(G969,sanschie!A:G,7,0)","v":217},1]
["Absolut",5,40,"Absolut405",null,"ABS 400 Rauchrohr-Anschlusspaket 90° RA  ","103987",665,null,"STK",{"$f":"VLOOKUP(G970,sanschie!A:G,7,0)","v":736},1,{"$f":"IF(L970=0,0,IF(L970=\"\",0,L970*H970))","v":665},{"$f":"SUM(O970:P970)","v":1},1,""]
["Absolut",6,40,"Absolut406",null,"ABS 400 Putztür-Anschlusspaket ","103970",665,null,"STK",{"$f":"VLOOKUP(G971,sanschie!A:G,7,0)","v":731},{"$f":"IF(N971=0,\"\",N971)","v":""},{"$f":"IF(N971=0,0,IF(N971=\"\",0,N971*H971))","v":0},{"$f":"IF(Daten!$B$261=1,0,Daten!$C$261)","v":0}]
["Absolut",7,40,"Absolut407",null,"ABS Handyplatte EZ Inox 670 x 670mm ","104174","0",null,"STK",{"$f":"VLOOKUP(G972,sanschie!A:G,7,0)","v":241},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",8,40,"Absolut408",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G973,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",9,40,"Absolut409",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G974,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",10,40,"Absolut4010",null,"ABS Handyplatte EZ Kupfer 670 x 670mm ","140791","0",null,"STK",{"$f":"VLOOKUP(G975,sanschie!A:G,7,0)","v":303}]
["Absolut",11,40,"Absolut4011",null,"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben","140932","0",null,"STK",{"$f":"VLOOKUP(G976,sanschie!A:G,7,0)","v":75}]
["Absolut",12,40,"Absolut4012",null,"ABS 400 Abströmkonus verkupfert","104210","0",null,"STK",{"$f":"VLOOKUP(G977,sanschie!A:G,7,0)","v":481}]
["Absolut",13,40,"Absolut4013",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G978,sanschie!A:G,7,0)","v":303},{"$f":"IF(Daten!$B$287=2,1,\"\")","v":""}]
["Absolut",14,40,"Absolut4014",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G979,sanschie!A:G,7,0)","v":94},{"$f":"IF(Daten!$B$287=2,1,\"\")","v":""}]
["Absolut",15,40,"Absolut4015",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G980,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",16,40,"Absolut4016",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G981,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",17,40,"Absolut4017",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G982,sanschie!A:G,7,0)","v":35},{"$f":"ROUNDUP(M982,0)","v":2},{"$f":"N982/7","v":1.2857142857142858},{"$f":"Daten!$B$61","v":9}]
["Absolut",18,40,"Absolut4018",null,"ABS 400 Basten Standard Inox","104216","0",null,"STK",{"$f":"VLOOKUP(G983,sanschie!A:G,7,0)","v":596},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",19,40,"Absolut4019",null,"ABS 400 Basten Standard Kupfer","104222","0",null,"STK",{"$f":"VLOOKUP(G984,sanschie!A:G,7,0)","v":596},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",20,40,"Absolut4020",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G985,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",21,40,"Absolut4021",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G986,sanschie!A:G,7,0)","v":14},{"$f":"IF(M986<0,\"\",M986)","v":""},{"$f":"ROUNDUP(((K965-11.66)-SUM(N970,N971))/1.33,0)","v":-10}]
["Absolut",22,40,"Absolut4022",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G987,sanschie!A:G,7,0)","v":258.8}]
["Absolut",23,40,"Absolut4023",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G988,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",24,40,"Absolut4024",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G989,sanschie!A:G,7,0)","v":44.9}]
["Absolut",25,40,"Absolut4025",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G990,sanschie!A:G,7,0)","v":7.5}]
["Absolut",26,40,"Absolut4026",null,"ZBH 260 Verschlusszapfen 2Stk. aus Schaumstoff","103835","0",null,"STK",{"$f":"VLOOKUP(G991,sanschie!A:G,7,0)","v":31.1}]
["Absolut",27,40,"Absolut4027",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G992,sanschie!A:G,7,0)","v":13.8}]
["Absolut",28,40,"Absolut4028",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G993,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",29,40,"Absolut4029",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G994,sanschie!A:G,7,0)","v":322}]
["Absolut",30,40,"Absolut4030",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G995,sanschie!A:G,7,0)","v":26}]
["Absolut",31,40,"Absolut4031",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G996,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,"14TL",{"$f":"A997&C997&B997","v":"Absolut14TL0"},"P","Absolut-Kaminanlage Ø 14TL","Absolut 14TL","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G997,sanschie!A:G,7,0)","v":0},null,{"$f":"I997*1000","v":9000}]
["Absolut",{"$f":"B997+1","v":1},{"$f":"C997","v":"14TL"},{"$f":"A998&C998&B998","v":"Absolut14TL1"},null,"ABS Mantelstein EZTL 360 x 500mm L330mm","103920","0",null,"STK",{"$f":"VLOOKUP(G998,sanschie!A:G,7,0)","v":42},{"$f":"ROUND(M998,0)-M999","v":24},{"$f":"((M997-M1003)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N998*330","v":0}]
["Absolut",{"$f":"B998+1","v":2},{"$f":"C998","v":"14TL"},{"$f":"A999&C999&B999","v":"Absolut14TL2"},null,"ABS Thermo-Trennstein EZ TL 360 x 500mm L330mm","103934","0",null,"STK",{"$f":"VLOOKUP(G999,sanschie!A:G,7,0)","v":222},{"$f":"IF(M999=0,\"\",M999)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,"14TL","Absolut14TL3",null,"ABS Thermo-Fussplatte EZTL 360 x 500mm","103852","0",null,"STK",{"$f":"VLOOKUP(G1000,sanschie!A:G,7,0)","v":160}]
["Absolut",4,"14TL","Absolut14TL4",null,"ABS Sockelplatte aus Beton EZTL 360 x 500mm","103876","0",null,"STK",{"$f":"VLOOKUP(G1001,sanschie!A:G,7,0)","v":101}]
["Absolut",5,"14TL","Absolut14TL5",null,"ABS 140 Profilkeramik-Rohr mit Muffe L1330mm","103946",1330,null,"STK",{"$f":"VLOOKUP(G1002,sanschie!A:G,7,0)","v":106},{"$f":"ROUNDUP(M1002,0)","v":5},{"$f":"(M997-O998-M1003-M1007-M1008-M1013)/1000/1.33","v":4.962406015037593}]
["Absolut",6,"14TL","Absolut14TL6",null,"ABS 180 Fertigfuss EZTL 120-180mm  L1070mm ","103864",1070,null,"STK",{"$f":"VLOOKUP(G1003,sanschie!A:G,7,0)","v":734},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1003=\"\",0,$H1003*$L1003)","v":1070}]
["Absolut",7,"14TL","Absolut14TL7",null,"ABS 140 Fertigfusspaket ","103889","0",null,"STK",{"$f":"VLOOKUP(G1004,sanschie!A:G,7,0)","v":311},{"$f":"L1003","v":1}]
["Absolut",8,"14TL","Absolut14TL8",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G1005,sanschie!A:G,7,0)","v":18}]
["Absolut",9,"14TL","Absolut14TL9",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G1006,sanschie!A:G,7,0)","v":32},{"$f":"IF(L1003=\"\",1,\"\")","v":""}]
["Absolut",10,"14TL","Absolut14TL10",null,"ABS 140 Rauchrohr-Anschlusspaket 90° RA  ","103981",1330,null,"STK",{"$f":"VLOOKUP(G1007,sanschie!A:G,7,0)","v":355},{"$f":"IF(N1007=0,\"\",N1007)","v":1},{"$f":"IF(L1007=0,0,IF(L1007=\"\",0,L1007*H1007))","v":1330},{"$f":"SUM(O1007:P1007)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",11,"14TL","Absolut14TL11",null,"ABS 140 Rauchrohr-Anschlusspaket 45° RA  ","103993",1330,null,"STK",{"$f":"VLOOKUP(G1008,sanschie!A:G,7,0)","v":355},{"$f":"IF(N1008=0,\"\",N1008)","v":""},{"$f":"IF(L1008=0,0,IF(L1008=\"\",0,L1008*H1008))","v":0},{"$f":"SUM(O1008:P1008)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",12,"14TL","Absolut14TL12",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø140mm","103999","0",null,"STK",{"$f":"VLOOKUP(G1009,sanschie!A:G,7,0)","v":191}]
["Absolut",13,"14TL","Absolut14TL13",null,"ABS 140 Rauchrohranschluss Stutzen-Set 45°","104005","0",null,"STK",{"$f":"VLOOKUP(G1010,sanschie!A:G,7,0)","v":191}]
["Absolut",14,"14TL","Absolut14TL14",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G1011,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=2,1,\"\")","v":""}]
["Absolut",15,"14TL","Absolut14TL15",null,"ABS 200 Steckadapter ","104269","0",null,"STK",{"$f":"VLOOKUP(G1012,sanschie!A:G,7,0)","v":184}]
["Absolut",16,"14TL","Absolut14TL16",null,"ABS 140 Putztür-Anschlusspaket ","103964",1330,null,"STK",{"$f":"VLOOKUP(G1013,sanschie!A:G,7,0)","v":410},{"$f":"IF(N1013=0,\"\",N1013)","v":""},{"$f":"IF(L1013=0,0,IF(L1013=\"\",0,L1013*H1013))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",17,"14TL","Absolut14TL17",null,"ABS 140 Putztüranschluss Stutzen Set","104272","0",null,"STK",{"$f":"VLOOKUP(G1014,sanschie!A:G,7,0)","v":311}]
["Absolut",18,"14TL","Absolut14TL18",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1015,sanschie!A:G,7,0)","v":27}]
["Absolut",19,"14TL","Absolut14TL19",null,"ABS Thermodichtset EZTL 360x500mm und 380x540mm","104191","0",null,"STK",{"$f":"VLOOKUP(G1016,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",20,"14TL","Absolut14TL20",null,"ABS Thermodichtset EZTL 360x500mm und 380x540mm","104194","0",null,"STK",{"$f":"VLOOKUP(G1017,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",21,"14TL","Absolut14TL21",null,"ABS Handyplatte EZTL Faserzement 360 x 500mm","104148","0",null,"STK",{"$f":"VLOOKUP(G1018,sanschie!A:G,7,0)","v":143},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",22,"14TL","Absolut14TL22",null,"ABS Handyplatte EZTL Inox 360 x 500mm ","104176","0",null,"STK",{"$f":"VLOOKUP(G1019,sanschie!A:G,7,0)","v":205},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",23,"14TL","Absolut14TL23",null,"ABS Handyplatte EZTL Kupfer 360 x 500mm ","104186","0",null,"STK",{"$f":"VLOOKUP(G1020,sanschie!A:G,7,0)","v":328}]
["Absolut",24,"14TL","Absolut14TL24",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1021,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",25,"14TL","Absolut14TL25",null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G1022,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",26,"14TL","Absolut14TL26",null,"ABS HEB-Set Handyplatte Kupfer mit Langschrauben","104189","0",null,"STK",{"$f":"VLOOKUP(G1023,sanschie!A:G,7,0)","v":101}]
["Absolut",27,"14TL","Absolut14TL27",null,"ABS Abdeckung zu Handyplatte EZTL 100 x 260mm","104163","0",null,"STK",{"$f":"VLOOKUP(G1024,sanschie!A:G,7,0)","v":51}]
["Absolut",28,"14TL","Absolut14TL28",null,"ABS Zulufthaube zu Faserzementpl. EZTL 140- 200mm","104167","0",null,"STK",{"$f":"VLOOKUP(G1025,sanschie!A:G,7,0)","v":73},{"$f":"IF(Daten!$B$212=1,\"\",IF(L1019=1,\"\",1))","v":1}]
["Absolut",29,"14TL","Absolut14TL29",null,"ABS 140 Abströmkonus verkupfert","104204","0",null,"STK",{"$f":"VLOOKUP(G1026,sanschie!A:G,7,0)","v":161}]
["Absolut",30,"14TL","Absolut14TL30",null,"KER 140  Keranova-Fugenglätter","103472","0",null,"STK",{"$f":"VLOOKUP(G1027,sanschie!A:G,7,0)","v":57}]
["Absolut",31,"14TL","Absolut14TL31",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G1028,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",32,"14TL","Absolut14TL32",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G1029,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",33,"14TL","Absolut14TL33",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G1030,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",34,"14TL","Absolut14TL34",null,"CHZ 150 Doppelfutter lose L150mm","103803","0",null,"STK",{"$f":"VLOOKUP(G1031,sanschie!A:G,7,0)","v":103},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",35,"14TL","Absolut14TL35",null,"ABS 140 Kondensatfalle zu RA 45° Ø130mm ","104028","0",null,"STK",{"$f":"VLOOKUP(G1032,sanschie!A:G,7,0)","v":297}]
["Absolut",36,"14TL","Absolut14TL36",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1033,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",37,"14TL","Absolut14TL37",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1034,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",38,"14TL","Absolut14TL38",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1035,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",39,"14TL","Absolut14TL39",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1036,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1004=1,1,\"\")","v":1}]
["Absolut",40,"14TL","Absolut14TL40",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1037,sanschie!A:G,7,0)","v":489},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""}]
["Absolut",41,"14TL","Absolut14TL41",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1038,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",42,"14TL","Absolut14TL42",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1039,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",43,"14TL","Absolut14TL43",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G1040,sanschie!A:G,7,0)","v":14},{"$f":"IF(Daten!$B$183=3,N1040,Sortimente!P1040)","v":""},null,{"$f":"ROUNDUP(O1040,0)","v":3},{"$f":"L1002/2","v":2.5},{"$f":"IF(L1002<=8,\"\",IF(L1002<=10,1,IF(L1002<=12,2,IF(L1002<=14,3,4))))","v":""}]
["Absolut",44,"14TL","Absolut14TL44",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1041,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1041=0,\"\",N1041)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",45,"14TL","Absolut14TL45",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1042,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1042=0,\"\",N1042)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",46,"14TL","Absolut14TL46",null,"ZBH Revisionstüre 100 x 275 mm Alu eloxiert","103842","0",null,"STK",{"$f":"VLOOKUP(G1043,sanschie!A:G,7,0)","v":87.4},{"$f":"IF(Daten!$G$249=0,\"\",Daten!$G$249)","v":""}]
["Absolut",47,"14TL","Absolut14TL47",null,"ABS LAS Zuluftadapter für Längsseite","104234","0",null,"STK",{"$f":"VLOOKUP(G1044,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$249=1,\"\",1)","v":""}]
["Absolut",48,"14TL","Absolut14TL48",null,"ABS LAS Zuluftadapter für Stirnseite","104235","0",null,"STK",{"$f":"VLOOKUP(G1045,sanschie!A:G,7,0)","v":317}]
["Absolut",49,"14TL","Absolut14TL49",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G1046,sanschie!A:G,7,0)","v":53}]
["Absolut",50,"14TL","Absolut14TL50",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1047,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",51,"14TL","Absolut14TL51",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1048,sanschie!A:G,7,0)","v":35},{"$f":"IF(N1048<=12.7,1,2)","v":1},null,{"$f":"IF(L1003=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",52,"14TL","Absolut14TL52",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1049,sanschie!A:G,7,0)","v":258.8}]
["Absolut",53,"14TL","Absolut14TL53",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1050,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",54,"14TL","Absolut14TL54",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1051,sanschie!A:G,7,0)","v":44.9}]
["Absolut",55,"14TL","Absolut14TL55",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1052,sanschie!A:G,7,0)","v":7.5}]
["Absolut",56,"14TL","Absolut14TL56",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G1053,sanschie!A:G,7,0)","v":452}]
["Absolut",57,"14TL","Absolut14TL57",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G1054,sanschie!A:G,7,0)","v":538}]
["Absolut",58,"14TL","Absolut14TL58",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G1055,sanschie!A:G,7,0)","v":634}]
["Absolut",59,"14TL","Absolut14TL59",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G1056,sanschie!A:G,7,0)","v":695}]
["Absolut",60,"14TL","Absolut14TL60",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G1057,sanschie!A:G,7,0)","v":797}]
["Absolut",61,"14TL","Absolut14TL61",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G1058,sanschie!A:G,7,0)","v":873}]
["Absolut",62,"14TL","Absolut14TL62",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1059,sanschie!A:G,7,0)","v":13.8}]
["Absolut",63,"14TL","Absolut14TL63",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1060,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",64,"14TL","Absolut14TL64",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1061,sanschie!A:G,7,0)","v":322}]
["Absolut",65,"14TL","Absolut14TL65",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1062,sanschie!A:G,7,0)","v":26}]
["Absolut",{"$f":"B1062+1","v":66},{"$f":"C1062","v":"14TL"},"Absolut14TL66",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1063,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,"16TL",{"$f":"A1064&C1064&B1064","v":"Absolut16TL0"},"P","Absolut-Kaminanlage Ø 16TL","Absolut 16TL","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1064,sanschie!A:G,7,0)","v":0},null,{"$f":"I1064*1000","v":9000}]
["Absolut",{"$f":"B1064+1","v":1},{"$f":"C1064","v":"16TL"},{"$f":"A1065&C1065&B1065","v":"Absolut16TL1"},null,"ABS Mantelstein EZTL 360 x 500mm L330mm","103920","0",null,"STK",{"$f":"VLOOKUP(G1065,sanschie!A:G,7,0)","v":42},{"$f":"ROUND(M1065,0)-M1066","v":24},{"$f":"((M1064-M1070)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1065*330","v":0}]
["Absolut",{"$f":"B1065+1","v":2},{"$f":"C1065","v":"16TL"},{"$f":"A1066&C1066&B1066","v":"Absolut16TL2"},null,"ABS Thermo-Trennstein EZ TL 360 x 500mm L330mm","103934","0",null,"STK",{"$f":"VLOOKUP(G1066,sanschie!A:G,7,0)","v":222},{"$f":"IF(M1066=0,\"\",M1066)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,"16TL","Absolut16TL3",null,"ABS Thermo-Fussplatte EZTL 360 x 500mm","103852","0",null,"STK",{"$f":"VLOOKUP(G1067,sanschie!A:G,7,0)","v":160}]
["Absolut",4,"16TL","Absolut16TL4",null,"ABS Sockelplatte aus Beton EZTL 360 x 500mm","103876","0",null,"STK",{"$f":"VLOOKUP(G1068,sanschie!A:G,7,0)","v":101}]
["Absolut",5,"16TL","Absolut16TL5",null,"ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","103947",1330,null,"STK",{"$f":"VLOOKUP(G1069,sanschie!A:G,7,0)","v":113},{"$f":"ROUNDUP(M1069,0)","v":5},{"$f":"(M1064-O1065-M1070-M1074-M1075-M1079)/1000/1.33","v":4.962406015037593}]
["Absolut",6,"16TL","Absolut16TL6",null,"ABS 180 Fertigfuss EZTL 120-180mm  L1070mm ","103864",1070,null,"STK",{"$f":"VLOOKUP(G1070,sanschie!A:G,7,0)","v":734},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1070=\"\",0,$H1070*$L1070)","v":1070}]
["Absolut",7,"16TL","Absolut16TL7",null,"ABS 160 Fertigfusspaket ","103890","0",null,"STK",{"$f":"VLOOKUP(G1071,sanschie!A:G,7,0)","v":311},{"$f":"L1070","v":1}]
["Absolut",8,"16TL","Absolut16TL8",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G1072,sanschie!A:G,7,0)","v":18}]
["Absolut",9,"16TL","Absolut16TL9",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G1073,sanschie!A:G,7,0)","v":32},{"$f":"IF(L1070=\"\",1,\"\")","v":""}]
["Absolut",10,"16TL","Absolut16TL10",null,"ABS 160 Rauchrohr-Anschlusspaket 90° RA  ","103982",1330,null,"STK",{"$f":"VLOOKUP(G1074,sanschie!A:G,7,0)","v":367},{"$f":"IF(N1074=0,\"\",N1074)","v":1},{"$f":"IF(L1074=0,0,IF(L1074=\"\",0,L1074*H1074))","v":1330},{"$f":"SUM(O1074:P1074)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",11,"16TL","Absolut16TL11",null,"ABS 160 Rauchrohr-Anschlusspaket 45° RA  ","103994",1330,null,"STK",{"$f":"VLOOKUP(G1075,sanschie!A:G,7,0)","v":367},{"$f":"IF(N1075=0,\"\",N1075)","v":""},{"$f":"IF(L1075=0,0,IF(L1075=\"\",0,L1075*H1075))","v":0},{"$f":"SUM(O1075:P1075)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",12,"16TL","Absolut16TL12",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø160mm","104000","0",null,"STK",{"$f":"VLOOKUP(G1076,sanschie!A:G,7,0)","v":199}]
["Absolut",13,"16TL","Absolut16TL13",null,"ABS 160 Rauchrohranschluss Stutzen-Set 45°","104006","0",null,"STK",{"$f":"VLOOKUP(G1077,sanschie!A:G,7,0)","v":199}]
["Absolut",14,"16TL","Absolut16TL14",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G1078,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=2,1,\"\")","v":""}]
["Absolut",15,"16TL","Absolut16TL15",null,"ABS 160 Putztür-Anschlusspaket ","103965",1330,null,"STK",{"$f":"VLOOKUP(G1079,sanschie!A:G,7,0)","v":428},{"$f":"IF(N1079=0,\"\",N1079)","v":""},{"$f":"IF(L1079=0,0,IF(L1079=\"\",0,L1079*H1079))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",16,"16TL","Absolut16TL16",null,"ABS 160 Putztüranschluss Stutzen Set","104273","0",null,"STK",{"$f":"VLOOKUP(G1080,sanschie!A:G,7,0)","v":325}]
["Absolut",17,"16TL","Absolut16TL17",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1081,sanschie!A:G,7,0)","v":27}]
["Absolut",18,"16TL","Absolut16TL18",null,"ABS Thermodichtset EZTL 360x500mm und 380x540mm","104191","0",null,"STK",{"$f":"VLOOKUP(G1082,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",19,"16TL","Absolut16TL19",null,"ABS Thermodichtset EZTL 360x500mm und 380x540mm","104194","0",null,"STK",{"$f":"VLOOKUP(G1083,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",20,"16TL","Absolut16TL20",null,"ABS Handyplatte EZTL Faserzement 360 x 500mm","104148","0",null,"STK",{"$f":"VLOOKUP(G1084,sanschie!A:G,7,0)","v":143},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",21,"16TL","Absolut16TL21",null,"ABS Handyplatte EZTL Inox 360 x 500mm ","104176","0",null,"STK",{"$f":"VLOOKUP(G1085,sanschie!A:G,7,0)","v":205},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",22,"16TL","Absolut16TL22",null,"ABS Handyplatte EZTL Kupfer 360 x 500mm ","104186","0",null,"STK",{"$f":"VLOOKUP(G1086,sanschie!A:G,7,0)","v":328}]
["Absolut",23,"16TL","Absolut16TL23",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1087,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",24,"16TL","Absolut16TL24",null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G1088,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",25,"16TL","Absolut16TL25",null,"ABS HEB-Set Handyplatte Kupfer mit Langschrauben","104189","0",null,"STK",{"$f":"VLOOKUP(G1089,sanschie!A:G,7,0)","v":101}]
["Absolut",26,"16TL","Absolut16TL26",null,"ABS Abdeckung zu Handyplatte EZTL 100 x 260mm","104163","0",null,"STK",{"$f":"VLOOKUP(G1090,sanschie!A:G,7,0)","v":51}]
["Absolut",27,"16TL","Absolut16TL27",null,"ABS Zulufthaube zu Faserzementpl. EZTL 140- 200mm","104167","0",null,"STK",{"$f":"VLOOKUP(G1091,sanschie!A:G,7,0)","v":73},{"$f":"IF(Daten!$B$212=1,\"\",IF(L1085=1,\"\",1))","v":1}]
["Absolut",28,"16TL","Absolut16TL28",null,"ABS 160 Abströmkonus verkupfert","104205","0",null,"STK",{"$f":"VLOOKUP(G1092,sanschie!A:G,7,0)","v":166}]
["Absolut",29,"16TL","Absolut16TL29",null,"KER 160  Keranova-Fugenglätter","103473","0",null,"STK",{"$f":"VLOOKUP(G1093,sanschie!A:G,7,0)","v":58}]
["Absolut",30,"16TL","Absolut16TL30",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G1094,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",31,"16TL","Absolut16TL31",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G1095,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",32,"16TL","Absolut16TL32",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G1096,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",33,"16TL","Absolut16TL33",null,"CHZ 150 Doppelfutter lose L150mm","103803","0",null,"STK",{"$f":"VLOOKUP(G1097,sanschie!A:G,7,0)","v":103},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",34,"16TL","Absolut16TL34",null,"ABS 160 Kondensatfalle zu RA 45° Ø130mm ","104029","0",null,"STK",{"$f":"VLOOKUP(G1098,sanschie!A:G,7,0)","v":322}]
["Absolut",35,"16TL","Absolut16TL35",null,"ABS 160 Kondensatfalle zu RA 45° Ø150mm ","104030","0",null,"STK",{"$f":"VLOOKUP(G1099,sanschie!A:G,7,0)","v":322}]
["Absolut",36,"16TL","Absolut16TL36",null,"ABS 160 Kondensatfalle zu RA 45° Ø160mm ","104031","0",null,"STK",{"$f":"VLOOKUP(G1100,sanschie!A:G,7,0)","v":322}]
["Absolut",37,"16TL","Absolut16TL37",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1101,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",38,"16TL","Absolut16TL38",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1102,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",39,"16TL","Absolut16TL39",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1103,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",40,"16TL","Absolut16TL40",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1104,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1071=1,1,\"\")","v":1}]
["Absolut",41,"16TL","Absolut16TL41",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1105,sanschie!A:G,7,0)","v":489},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""}]
["Absolut",42,"16TL","Absolut16TL42",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1106,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",43,"16TL","Absolut16TL43",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1107,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",44,"16TL","Absolut16TL44",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G1108,sanschie!A:G,7,0)","v":14},{"$f":"IF(Daten!$B$183=3,N1108,Sortimente!P1108)","v":""},null,{"$f":"ROUNDUP(O1108,0)","v":3},{"$f":"L1069/2","v":2.5},{"$f":"IF(L1069<=8,\"\",IF(L1069<=10,1,IF(L1069<=12,2,IF(L1069<=14,3,4))))","v":""}]
["Absolut",45,"16TL","Absolut16TL45",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1109,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1109=0,\"\",N1109)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",46,"16TL","Absolut16TL46",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1110,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1110=0,\"\",N1110)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",47,"16TL","Absolut16TL47",null,"ZBH Revisionstüre 100 x 275 mm Alu eloxiert","103842","0",null,"STK",{"$f":"VLOOKUP(G1111,sanschie!A:G,7,0)","v":87.4},{"$f":"IF(Daten!$G$249=0,\"\",Daten!$G$249)","v":""}]
["Absolut",48,"16TL","Absolut16TL48",null,"ABS LAS Zuluftadapter für Längsseite","104234","0",null,"STK",{"$f":"VLOOKUP(G1112,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$249=1,\"\",1)","v":""}]
["Absolut",49,"16TL","Absolut16TL49",null,"ABS LAS Zuluftadapter für Stirnseite","104235","0",null,"STK",{"$f":"VLOOKUP(G1113,sanschie!A:G,7,0)","v":317}]
["Absolut",50,"16TL","Absolut16TL50",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G1114,sanschie!A:G,7,0)","v":53}]
["Absolut",51,"16TL","Absolut16TL51",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1115,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",52,"16TL","Absolut16TL52",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1116,sanschie!A:G,7,0)","v":35},{"$f":"IF(N1116<=12.7,1,2)","v":1},null,{"$f":"IF(L1070=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",53,"16TL","Absolut16TL53",null,"ABS 160 Basten Standard Inox","104211","0",null,"STK",{"$f":"VLOOKUP(G1117,sanschie!A:G,7,0)","v":323},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",54,"16TL","Absolut16TL54",null,"ABS 160 Basten Standard Kupfer","104217","0",null,"STK",{"$f":"VLOOKUP(G1118,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",55,"16TL","Absolut16TL55",null,"ABS 160 Sairlift Inox","104223","0",null,"STK",{"$f":"VLOOKUP(G1119,sanschie!A:G,7,0)","v":374},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",56,"16TL","Absolut16TL56",null,"ABS 160 Sairlift Kupfer","104228","0",null,"STK",{"$f":"VLOOKUP(G1120,sanschie!A:G,7,0)","v":397},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",57,"16TL","Absolut16TL57",null,"ZBH 150 Verschlussbüchse weiss ØA 275mm","103836","0",null,"STK",{"$f":"VLOOKUP(G1121,sanschie!A:G,7,0)","v":115}]
["Absolut",58,"16TL","Absolut16TL58",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1122,sanschie!A:G,7,0)","v":258.8}]
["Absolut",59,"16TL","Absolut16TL59",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1123,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",60,"16TL","Absolut16TL60",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1124,sanschie!A:G,7,0)","v":44.9}]
["Absolut",61,"16TL","Absolut16TL61",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1125,sanschie!A:G,7,0)","v":7.5}]
["Absolut",62,"16TL","Absolut16TL62",null,"ZBH 170 Verschlusszapfen 2Stk. aus Schaumstoff","103832","0",null,"STK",{"$f":"VLOOKUP(G1126,sanschie!A:G,7,0)","v":24.2}]
["Absolut",63,"16TL","Absolut16TL63",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G1127,sanschie!A:G,7,0)","v":452}]
["Absolut",64,"16TL","Absolut16TL64",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G1128,sanschie!A:G,7,0)","v":538}]
["Absolut",65,"16TL","Absolut16TL65",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G1129,sanschie!A:G,7,0)","v":634}]
["Absolut",{"$f":"B1129+1","v":66},{"$f":"C1129","v":"16TL"},"Absolut16TL66",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G1130,sanschie!A:G,7,0)","v":695}]
["Absolut",67,"16TL","Absolut16TL67",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G1131,sanschie!A:G,7,0)","v":797}]
["Absolut",68,"16TL","Absolut16TL68",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G1132,sanschie!A:G,7,0)","v":873}]
["Absolut",69,"16TL","Absolut16TL69",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1133,sanschie!A:G,7,0)","v":13.8}]
["Absolut",{"$f":"B1133+1","v":70},{"$f":"C1133","v":"16TL"},{"$f":"A1134&C1134&B1134","v":"Absolut16TL70"},null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1134,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",{"$f":"B1134+1","v":71},{"$f":"C1134","v":"16TL"},{"$f":"A1135&C1135&B1135","v":"Absolut16TL71"},null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1135,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B1135+1","v":72},{"$f":"C1135","v":"16TL"},{"$f":"A1136&C1136&B1136","v":"Absolut16TL72"},null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1136,sanschie!A:G,7,0)","v":26}]
["Absolut",{"$f":"B1136+1","v":73},{"$f":"C1136","v":"16TL"},{"$f":"A1137&C1137&B1137","v":"Absolut16TL73"},null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1137,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,"18TL",{"$f":"A1138&C1138&B1138","v":"Absolut18TL0"},"P","Absolut-Kaminanlage Ø 18TL","Absolut 18TL","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1138,sanschie!A:G,7,0)","v":0},null,{"$f":"I1138*1000","v":9000}]
["Absolut",{"$f":"B1138+1","v":1},{"$f":"C1138","v":"18TL"},"Absolut18TL1",null,"ABS Mantelstein EZTL 360 x 500mm L330mm","103920","0",null,"STK",{"$f":"VLOOKUP(G1139,sanschie!A:G,7,0)","v":42},{"$f":"ROUND(M1139,0)-M1140","v":24},{"$f":"((M1138-M1144)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1139*330","v":0}]
["Absolut",2,"18TL","Absolut18TL2",null,"ABS Thermo-Trennstein EZ TL 360 x 500mm L330mm","103934","0",null,"STK",{"$f":"VLOOKUP(G1140,sanschie!A:G,7,0)","v":222},{"$f":"IF(M1140=0,\"\",M1140)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,"18TL","Absolut18TL3",null,"ABS Thermo-Fussplatte EZTL 360 x 500mm","103852","0",null,"STK",{"$f":"VLOOKUP(G1141,sanschie!A:G,7,0)","v":160}]
["Absolut",4,"18TL","Absolut18TL4",null,"ABS Sockelplatte aus Beton EZTL 360 x 500mm","103876","0",null,"STK",{"$f":"VLOOKUP(G1142,sanschie!A:G,7,0)","v":101}]
["Absolut",5,"18TL","Absolut18TL5",null,"ABS 180 Profilkeramik-Rohr mit Muffe L1330mm","103948",1330,null,"STK",{"$f":"VLOOKUP(G1143,sanschie!A:G,7,0)","v":122},{"$f":"ROUNDUP(M1143,0)","v":5},{"$f":"(M1138-O1139-M1144-M1148-M1149-M1153)/1000/1.33","v":4.962406015037593}]
["Absolut",6,"18TL","Absolut18TL6",null,"ABS 180 Fertigfuss EZTL 120-180mm  L1070mm ","103864",1070,null,"STK",{"$f":"VLOOKUP(G1144,sanschie!A:G,7,0)","v":734},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1144=\"\",0,$H1144*$L1144)","v":1070}]
["Absolut",7,"18TL","Absolut18TL7",null,"ABS 180 Fertigfusspaket ","103891","0",null,"STK",{"$f":"VLOOKUP(G1145,sanschie!A:G,7,0)","v":311},{"$f":"L1144","v":1}]
["Absolut",8,"18TL","Absolut18TL8",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G1146,sanschie!A:G,7,0)","v":18}]
["Absolut",9,"18TL","Absolut18TL9",null,"CHZ 180 Keramik Fuss-Scheibe geschlossen","103700","0",null,"STK",{"$f":"VLOOKUP(G1147,sanschie!A:G,7,0)","v":35},{"$f":"IF(L1144=\"\",1,\"\")","v":""}]
["Absolut",10,"18TL","Absolut18TL10",null,"ABS 180 Rauchrohr-Anschlusspaket 90° RA  ","103983",1330,null,"STK",{"$f":"VLOOKUP(G1148,sanschie!A:G,7,0)","v":386},{"$f":"IF(N1148=0,\"\",N1148)","v":1},{"$f":"IF(L1148=0,0,IF(L1148=\"\",0,L1148*H1148))","v":1330},{"$f":"SUM(O1148:P1148)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",11,"18TL","Absolut18TL11",null,"ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","103995",1330,null,"STK",{"$f":"VLOOKUP(G1149,sanschie!A:G,7,0)","v":404},{"$f":"IF(N1149=0,\"\",N1149)","v":""},{"$f":"IF(L1149=0,0,IF(L1149=\"\",0,L1149*H1149))","v":0},{"$f":"SUM(O1149:P1149)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",12,"18TL","Absolut18TL12",null,"ABS 180  Rauchrohranschluss Stutzen-Set 90° Ø180mm","104001","0",null,"STK",{"$f":"VLOOKUP(G1150,sanschie!A:G,7,0)","v":204}]
["Absolut",13,"18TL","Absolut18TL13",null,"ABS 180 Rauchrohranschluss Stutzen-Set 45°","104007","0",null,"STK",{"$f":"VLOOKUP(G1151,sanschie!A:G,7,0)","v":204}]
["Absolut",14,"18TL","Absolut18TL14",null,"ABS 180 Steckadapter ","104268","0",null,"STK",{"$f":"VLOOKUP(G1152,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=2,1,\"\")","v":""}]
["Absolut",15,"18TL","Absolut18TL15",null,"ABS 180 Putztür-Anschlusspaket ","103966",1330,null,"STK",{"$f":"VLOOKUP(G1153,sanschie!A:G,7,0)","v":448},{"$f":"IF(N1153=0,\"\",N1153)","v":""},{"$f":"IF(L1153=0,0,IF(L1153=\"\",0,L1153*H1153))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",16,"18TL","Absolut18TL16",null,"ABS 180 Putztüranschluss Stutzen Set","104274","0",null,"STK",{"$f":"VLOOKUP(G1154,sanschie!A:G,7,0)","v":336}]
["Absolut",17,"18TL","Absolut18TL17",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1155,sanschie!A:G,7,0)","v":27}]
["Absolut",18,"18TL","Absolut18TL18",null,"ABS Thermodichtset EZTL 360x500mm und 380x540mm","104191","0",null,"STK",{"$f":"VLOOKUP(G1156,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",19,"18TL","Absolut18TL19",null,"ABS Thermodichtset EZTL 360x500mm und 380x540mm","104194","0",null,"STK",{"$f":"VLOOKUP(G1157,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",20,"18TL","Absolut18TL20",null,"ABS Handyplatte EZTL Faserzement 360 x 500mm","104148","0",null,"STK",{"$f":"VLOOKUP(G1158,sanschie!A:G,7,0)","v":143},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",21,"18TL","Absolut18TL21",null,"ABS Handyplatte EZTL Inox 360 x 500mm ","104176","0",null,"STK",{"$f":"VLOOKUP(G1159,sanschie!A:G,7,0)","v":205},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",22,"18TL","Absolut18TL22",null,"ABS Handyplatte EZTL Kupfer 360 x 500mm ","104186","0",null,"STK",{"$f":"VLOOKUP(G1160,sanschie!A:G,7,0)","v":328}]
["Absolut",23,"18TL","Absolut18TL23",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1161,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",24,"18TL","Absolut18TL24",null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G1162,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",25,"18TL","Absolut18TL25",null,"ABS HEB-Set Handyplatte Kupfer mit Langschrauben","104189","0",null,"STK",{"$f":"VLOOKUP(G1163,sanschie!A:G,7,0)","v":101}]
["Absolut",26,"18TL","Absolut18TL26",null,"ABS Abdeckung zu Handyplatte EZTL 100 x 260mm","104163","0",null,"STK",{"$f":"VLOOKUP(G1164,sanschie!A:G,7,0)","v":51}]
["Absolut",27,"18TL","Absolut18TL27",null,"ABS Zulufthaube zu Faserzementpl. EZTL 140- 200mm","104167","0",null,"STK",{"$f":"VLOOKUP(G1165,sanschie!A:G,7,0)","v":73},{"$f":"IF(Daten!$B$212=1,\"\",IF(L1159=1,\"\",1))","v":1}]
["Absolut",28,"18TL","Absolut18TL28",null,"ABS 180 Abströmkonus verkupfert","104206","0",null,"STK",{"$f":"VLOOKUP(G1166,sanschie!A:G,7,0)","v":174}]
["Absolut",29,"18TL","Absolut18TL29",null,"KER 180  Keranova-Fugenglätter","103474","0",null,"STK",{"$f":"VLOOKUP(G1167,sanschie!A:G,7,0)","v":61}]
["Absolut",30,"18TL","Absolut18TL30",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø100mm","104014","0",null,"STK",{"$f":"VLOOKUP(G1168,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",31,"18TL","Absolut18TL31",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm","104015","0",null,"STK",{"$f":"VLOOKUP(G1169,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",32,"18TL","Absolut18TL32",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø130mm","104016","0",null,"STK",{"$f":"VLOOKUP(G1170,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",33,"18TL","Absolut18TL33",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø150mm","104017","0",null,"STK",{"$f":"VLOOKUP(G1171,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",34,"18TL","Absolut18TL34",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø180mm","104018","0",null,"STK",{"$f":"VLOOKUP(G1172,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",35,"18TL","Absolut18TL35",null,"ABS 180 Kondensatfalle zu RA 45° Ø130mm","104032","0",null,"STK",{"$f":"VLOOKUP(G1173,sanschie!A:G,7,0)","v":347}]
["Absolut",36,"18TL","Absolut18TL36",null,"ABS 180 Kondensatfalle zu RA 45° Ø150mm","104033","0",null,"STK",{"$f":"VLOOKUP(G1174,sanschie!A:G,7,0)","v":347}]
["Absolut",37,"18TL","Absolut18TL37",null,"ABS 180 Kondensatfalle zu RA 45° Ø160mm","104034","0",null,"STK",{"$f":"VLOOKUP(G1175,sanschie!A:G,7,0)","v":347}]
["Absolut",38,"18TL","Absolut18TL38",null,"ABS 180 Kondensatfalle zu RA 45° Ø180mm ","104035","0",null,"STK",{"$f":"VLOOKUP(G1176,sanschie!A:G,7,0)","v":347}]
["Absolut",39,"18TL","Absolut18TL39",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1177,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",40,"18TL","Absolut18TL40",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1178,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",41,"18TL","Absolut18TL41",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1179,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",42,"18TL","Absolut18TL42",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1180,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1145=1,1,\"\")","v":1}]
["Absolut",43,"18TL","Absolut18TL43",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1181,sanschie!A:G,7,0)","v":489},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""}]
["Absolut",44,"18TL","Absolut18TL44",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1182,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",45,"18TL","Absolut18TL45",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1183,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",46,"18TL","Absolut18TL46",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G1184,sanschie!A:G,7,0)","v":14},{"$f":"IF(Daten!$B$183=3,N1184,Sortimente!P1184)","v":""},null,{"$f":"ROUNDUP(O1184,0)","v":3},{"$f":"L1143/2","v":2.5},{"$f":"IF(L1143<=8,\"\",IF(L1143<=10,1,IF(L1143<=12,2,IF(L1143<=14,3,4))))","v":""}]
["Absolut",47,"18TL","Absolut18TL47",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1185,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1185=0,\"\",N1185)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",48,"18TL","Absolut18TL48",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1186,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1186=0,\"\",N1186)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",49,"18TL","Absolut18TL49",null,"ZBH Revisionstüre 100 x 275 mm Alu eloxiert","103842","0",null,"STK",{"$f":"VLOOKUP(G1187,sanschie!A:G,7,0)","v":87.4},{"$f":"IF(Daten!$G$249=0,\"\",Daten!$G$249)","v":""}]
["Absolut",50,"18TL","Absolut18TL50",null,"ABS LAS Zuluftadapter für Längsseite","104234","0",null,"STK",{"$f":"VLOOKUP(G1188,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$249=1,\"\",1)","v":""}]
["Absolut",51,"18TL","Absolut18TL51",null,"ABS LAS Zuluftadapter für Stirnseite","104235","0",null,"STK",{"$f":"VLOOKUP(G1189,sanschie!A:G,7,0)","v":317}]
["Absolut",52,"18TL","Absolut18TL52",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G1190,sanschie!A:G,7,0)","v":53}]
["Absolut",53,"18TL","Absolut18TL53",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1191,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",54,"18TL","Absolut18TL54",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1192,sanschie!A:G,7,0)","v":35},{"$f":"IF(N1192<=12.7,1,2)","v":1},null,{"$f":"IF(L1144=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",55,"18TL","Absolut18TL55",null,"ABS 180 Basten Standard Inox","104212","0",null,"STK",{"$f":"VLOOKUP(G1193,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",56,"18TL","Absolut18TL56",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",{"$f":"VLOOKUP(G1194,sanschie!A:G,7,0)","v":362},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",57,"18TL","Absolut18TL57",null,"ABS 180 Sairlift Inox","104224","0",null,"STK",{"$f":"VLOOKUP(G1195,sanschie!A:G,7,0)","v":400},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",58,"18TL","Absolut18TL58",null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",{"$f":"VLOOKUP(G1196,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",59,"18TL","Absolut18TL59",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G1197,sanschie!A:G,7,0)","v":123.1}]
["Absolut",60,"18TL","Absolut18TL60",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1198,sanschie!A:G,7,0)","v":258.8}]
["Absolut",61,"18TL","Absolut18TL61",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1199,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",62,"18TL","Absolut18TL62",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1200,sanschie!A:G,7,0)","v":44.9}]
["Absolut",63,"18TL","Absolut18TL63",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1201,sanschie!A:G,7,0)","v":7.5}]
["Absolut",64,"18TL",{"$f":"A1202&C1202&B1202","v":"Absolut18TL64"},null,"ZBH 190 Verschlusszapfen 2Stk. aus Schaumstoff","103833","0",null,"STK",{"$f":"VLOOKUP(G1202,sanschie!A:G,7,0)","v":26.5}]
["Absolut",{"$f":"B1202+1","v":65},{"$f":"C1202","v":"18TL"},"Absolut18TL65",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G1203,sanschie!A:G,7,0)","v":452}]
["Absolut",66,"18TL","Absolut18TL66",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G1204,sanschie!A:G,7,0)","v":538}]
["Absolut",67,"18TL","Absolut18TL67",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G1205,sanschie!A:G,7,0)","v":634}]
["Absolut",68,"18TL","Absolut18TL68",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G1206,sanschie!A:G,7,0)","v":695}]
["Absolut",69,"18TL","Absolut18TL69",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G1207,sanschie!A:G,7,0)","v":797}]
["Absolut",70,"18TL","Absolut18TL70",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G1208,sanschie!A:G,7,0)","v":873}]
["Absolut",71,"18TL",{"$f":"A1209&C1209&B1209","v":"Absolut18TL71"},null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1209,sanschie!A:G,7,0)","v":13.8}]
["Absolut",72,"18TL",{"$f":"A1210&C1210&B1210","v":"Absolut18TL72"},null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1210,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",73,"18TL",{"$f":"A1211&C1211&B1211","v":"Absolut18TL73"},null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1211,sanschie!A:G,7,0)","v":322}]
["Absolut",74,"18TL",{"$f":"A1212&C1212&B1212","v":"Absolut18TL74"},null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1212,sanschie!A:G,7,0)","v":26}]
["Absolut",75,"18TL",{"$f":"A1213&C1213&B1213","v":"Absolut18TL75"},null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1213,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,"20TL",{"$f":"A1214&C1214&B1214","v":"Absolut20TL0"},"P","Absolut-Kaminanlage Ø 20TL","Absolut 20TL","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1214,sanschie!A:G,7,0)","v":0},null,{"$f":"I1214*1000","v":9000}]
["Absolut",{"$f":"B1214+1","v":1},{"$f":"C1214","v":"20TL"},"Absolut20TL1",null,"ABS Mantelstein EZTL 380 x 540mm L330mm","103921","0",null,"STK",{"$f":"VLOOKUP(G1215,sanschie!A:G,7,0)","v":44},{"$f":"ROUND(M1215,0)-M1216","v":24},{"$f":"((M1214-M1220)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1215*330","v":0}]
["Absolut",2,"20TL","Absolut20TL2",null,"ABS Thermo-Trennstein EZ TL 380 x 540mm L330mm","103935","0",null,"STK",{"$f":"VLOOKUP(G1216,sanschie!A:G,7,0)","v":234},{"$f":"IF(M1216=0,\"\",M1216)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,"20TL","Absolut20TL3",null,"ABS Thermo-Fussplatte EZTL 380 x 540mm","103853","0",null,"STK",{"$f":"VLOOKUP(G1217,sanschie!A:G,7,0)","v":173}]
["Absolut",4,"20TL","Absolut20TL4",null,"ABS Sockelplatte aus Beton EZTL 380 x 540mm","103877","0",null,"STK",{"$f":"VLOOKUP(G1218,sanschie!A:G,7,0)","v":109}]
["Absolut",5,"20TL","Absolut20TL5",null,"ABS 200 Profilkeramik-Rohr mit Muffe L1330mm","103949",1330,null,"STK",{"$f":"VLOOKUP(G1219,sanschie!A:G,7,0)","v":145},{"$f":"ROUNDUP(M1219,0)","v":5},{"$f":"(M1214-O1215-M1220-M1224-M1225-M1229)/1000/1.33","v":4.962406015037593}]
["Absolut",6,"20TL","Absolut20TL6",null,"ABS 200 Fertigfuss EZTL  L1070mm","103865",1070,null,"STK",{"$f":"VLOOKUP(G1220,sanschie!A:G,7,0)","v":980},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1220=\"\",0,$H1220*$L1220)","v":1070}]
["Absolut",7,"20TL","Absolut20TL7",null,"ABS 200 Fertigfusspaket ","103892","0",null,"STK",{"$f":"VLOOKUP(G1221,sanschie!A:G,7,0)","v":311},{"$f":"L1220","v":1}]
["Absolut",8,"20TL","Absolut20TL8",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G1222,sanschie!A:G,7,0)","v":18}]
["Absolut",9,"20TL","Absolut20TL9",null,"CHZ 200 Keramik Fuss-Scheibe geschlossen","103701","0",null,"STK",{"$f":"VLOOKUP(G1223,sanschie!A:G,7,0)","v":45},{"$f":"IF(L1220=\"\",1,\"\")","v":""}]
["Absolut",10,"20TL","Absolut20TL10",null,"ABS 200 Rauchrohr-Anschlusspaket 90° RA  ","103984",1330,null,"STK",{"$f":"VLOOKUP(G1224,sanschie!A:G,7,0)","v":434},{"$f":"IF(N1224=0,\"\",N1224)","v":1},{"$f":"IF(L1224=0,0,IF(L1224=\"\",0,L1224*H1224))","v":1330},{"$f":"SUM(O1224:P1224)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",11,"20TL","Absolut20TL11",null,"ABS 200 Rauchrohr-Anschlusspaket 45° RA  ","103996",1330,null,"STK",{"$f":"VLOOKUP(G1225,sanschie!A:G,7,0)","v":466},{"$f":"IF(N1225=0,\"\",N1225)","v":""},{"$f":"IF(L1225=0,0,IF(L1225=\"\",0,L1225*H1225))","v":0},{"$f":"SUM(O1225:P1225)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",12,"20TL","Absolut20TL12",null,"ABS 200 Rauchrohranschluss Stutzen-Set 90° Ø200mm","104002","0",null,"STK",{"$f":"VLOOKUP(G1226,sanschie!A:G,7,0)","v":212}]
["Absolut",13,"20TL","Absolut20TL13",null,"ABS 200 Rauchrohranschluss Stutzen-Set 45°","104008","0",null,"STK",{"$f":"VLOOKUP(G1227,sanschie!A:G,7,0)","v":212}]
["Absolut",14,"20TL","Absolut20TL14",null,"ABS 200 Steckadapter ","104269","0",null,"STK",{"$f":"VLOOKUP(G1228,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=2,1,\"\")","v":""}]
["Absolut",15,"20TL","Absolut20TL15",null,"ABS 200 Putztür-Anschlusspaket ","103967",1330,null,"STK",{"$f":"VLOOKUP(G1229,sanschie!A:G,7,0)","v":483},{"$f":"IF(N1229=0,\"\",N1229)","v":""},{"$f":"IF(L1229=0,0,IF(L1229=\"\",0,L1229*H1229))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",16,"20TL","Absolut20TL16",null,"ABS 200 Putztüranschluss Stutzen Set","104275","0",null,"STK",{"$f":"VLOOKUP(G1230,sanschie!A:G,7,0)","v":349}]
["Absolut",17,"20TL","Absolut20TL17",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1231,sanschie!A:G,7,0)","v":27}]
["Absolut",18,"20TL","Absolut20TL18",null,"ABS 200 Rauchzugklappe  L330mm","104239","0",null,"STK",{"$f":"VLOOKUP(G1232,sanschie!A:G,7,0)","v":367}]
["Absolut",19,"20TL","Absolut20TL19",null,"ABS Thermodichtset EZTL 360x500mm und 380x540mm","104191","0",null,"STK",{"$f":"VLOOKUP(G1233,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",20,"20TL","Absolut20TL20",null,"ABS Thermodichtset EZTL 360x500mm und 380x540mm","104194","0",null,"STK",{"$f":"VLOOKUP(G1234,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",21,"20TL","Absolut20TL21",null,"ABS Handyplatte EZTL Faserzement 380 x 540mm","104151","0",null,"STK",{"$f":"VLOOKUP(G1235,sanschie!A:G,7,0)","v":143},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",22,"20TL","Absolut20TL22",null,"ABS Handyplatte EZTL Inox 380 x 540mm  ","104177","0",null,"STK",{"$f":"VLOOKUP(G1236,sanschie!A:G,7,0)","v":217},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",23,"20TL","Absolut20TL23",null,"ABS Handyplatte EZTL Kupfer 380 x 540mm","104187","0",null,"STK",{"$f":"VLOOKUP(G1237,sanschie!A:G,7,0)","v":341}]
["Absolut",24,"20TL","Absolut20TL24",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1238,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",25,"20TL","Absolut20TL25",null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G1239,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",26,"20TL","Absolut20TL26",null,"ABS HEB-Set Handyplatte Kupfer mit Langschrauben","104189","0",null,"STK",{"$f":"VLOOKUP(G1240,sanschie!A:G,7,0)","v":101}]
["Absolut",27,"20TL","Absolut20TL27",null,"ABS Abdeckung zu Handyplatte EZTL 120 x 280mm","104164","0",null,"STK",{"$f":"VLOOKUP(G1241,sanschie!A:G,7,0)","v":51}]
["Absolut",28,"20TL","Absolut20TL28",null,"ABS Zulufthaube zu Faserzementpl. EZTL 140- 200mm","104167","0",null,"STK",{"$f":"VLOOKUP(G1242,sanschie!A:G,7,0)","v":73},{"$f":"IF(Daten!$B$212=1,\"\",IF(L1236=1,\"\",1))","v":1}]
["Absolut",29,"20TL","Absolut20TL29",null,"ABS 200 Abströmkonus verkupfert","104207","0",null,"STK",{"$f":"VLOOKUP(G1243,sanschie!A:G,7,0)","v":197}]
["Absolut",30,"20TL","Absolut20TL30",null,"KER 200  Keranova-Fugenglätter","103475","0",null,"STK",{"$f":"VLOOKUP(G1244,sanschie!A:G,7,0)","v":72}]
["Absolut",31,"20TL","Absolut20TL31",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø100mm","104019","0",null,"STK",{"$f":"VLOOKUP(G1245,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",32,"20TL","Absolut20TL32",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø120mm","104020","0",null,"STK",{"$f":"VLOOKUP(G1246,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",33,"20TL","Absolut20TL33",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø130mm","104021","0",null,"STK",{"$f":"VLOOKUP(G1247,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",34,"20TL","Absolut20TL34",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø150mm","104022","0",null,"STK",{"$f":"VLOOKUP(G1248,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",35,"20TL","Absolut20TL35",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø180mm","104023","0",null,"STK",{"$f":"VLOOKUP(G1249,sanschie!A:G,7,0)","v":210},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",36,"20TL","Absolut20TL36",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø200mm","104024","0",null,"STK",{"$f":"VLOOKUP(G1250,sanschie!A:G,7,0)","v":222},{"$f":"IF(Daten!$B$226=8,1,\"\")","v":""}]
["Absolut",37,"20TL","Absolut20TL37",null,"ABS 200 Kondensatfalle zu RA 45° Ø130mm ","104036","0",null,"STK",{"$f":"VLOOKUP(G1251,sanschie!A:G,7,0)","v":365}]
["Absolut",38,"20TL","Absolut20TL38",null,"ABS 200 Kondensatfalle zu RA 45° Ø150mm ","104037","0",null,"STK",{"$f":"VLOOKUP(G1252,sanschie!A:G,7,0)","v":365}]
["Absolut",39,"20TL","Absolut20TL39",null,"ABS 200 Kondensatfalle zu RA 45° Ø160mm","104038","0",null,"STK",{"$f":"VLOOKUP(G1253,sanschie!A:G,7,0)","v":365}]
["Absolut",40,"20TL","Absolut20TL40",null,"ABS 200 Kondensatfalle zu RA 45° Ø180mm ","104039","0",null,"STK",{"$f":"VLOOKUP(G1254,sanschie!A:G,7,0)","v":365}]
["Absolut",41,"20TL","Absolut20TL41",null,"ABS 200 Kondensatfalle zu RA 45° Ø200mm ","104040","0",null,"STK",{"$f":"VLOOKUP(G1255,sanschie!A:G,7,0)","v":365}]
["Absolut",42,"20TL","Absolut20TL42",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1256,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",43,"20TL","Absolut20TL43",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1257,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",44,"20TL","Absolut20TL44",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1258,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",45,"20TL","Absolut20TL45",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1259,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1221=1,1,\"\")","v":1}]
["Absolut",46,"20TL","Absolut20TL46",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1260,sanschie!A:G,7,0)","v":489},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""}]
["Absolut",47,"20TL","Absolut20TL47",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1261,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",48,"20TL","Absolut20TL48",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1262,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",49,"20TL","Absolut20TL49",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G1263,sanschie!A:G,7,0)","v":14},{"$f":"IF(Daten!$B$183=3,N1263,Sortimente!P1263)","v":""},null,{"$f":"ROUNDUP(O1263,0)","v":3},{"$f":"L1219/2","v":2.5},{"$f":"IF(L1219<=8,\"\",IF(L1219<=10,1,IF(L1219<=12,2,IF(L1219<=14,3,4))))","v":""}]
["Absolut",50,"20TL","Absolut20TL50",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1264,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1264=0,\"\",N1264)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",51,"20TL","Absolut20TL51",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1265,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1265=0,\"\",N1265)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",52,"20TL","Absolut20TL52",null,"ZBH Revisionstüre 100 x 275 mm Alu eloxiert","103842","0",null,"STK",{"$f":"VLOOKUP(G1266,sanschie!A:G,7,0)","v":87.4},{"$f":"IF(Daten!$G$249=0,\"\",Daten!$G$249)","v":""}]
["Absolut",53,"20TL","Absolut20TL53",null,"ABS LAS Zuluftadapter für Längsseite","104234","0",null,"STK",{"$f":"VLOOKUP(G1267,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$249=1,\"\",1)","v":""}]
["Absolut",54,"20TL","Absolut20TL54",null,"ABS LAS Zuluftadapter für Stirnseite","104235","0",null,"STK",{"$f":"VLOOKUP(G1268,sanschie!A:G,7,0)","v":317}]
["Absolut",55,"20TL","Absolut20TL55",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G1269,sanschie!A:G,7,0)","v":53}]
["Absolut",56,"20TL","Absolut20TL56",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1270,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",57,"20TL","Absolut20TL57",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1271,sanschie!A:G,7,0)","v":35},{"$f":"IF(N1271<=12.7,1,2)","v":1},null,{"$f":"IF(L1220=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",58,"20TL","Absolut20TL58",null,"ABS 200 Basten Standard Inox","104213","0",null,"STK",{"$f":"VLOOKUP(G1272,sanschie!A:G,7,0)","v":361},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",59,"20TL","Absolut20TL59",null,"ABS 200 Basten Standard Kupfer","104219","0",null,"STK",{"$f":"VLOOKUP(G1273,sanschie!A:G,7,0)","v":375},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",60,"20TL","Absolut20TL60",null,"ABS 200 Sairlift Inox","104225","0",null,"STK",{"$f":"VLOOKUP(G1274,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",61,"20TL","Absolut20TL61",null,"ABS 200 Sairlift Kupfer","104230","0",null,"STK",{"$f":"VLOOKUP(G1275,sanschie!A:G,7,0)","v":434},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",62,"20TL","Absolut20TL62",null,"ZBH 200 Verschlussbüchse weiss ØA 300mm","103839","0",null,"STK",{"$f":"VLOOKUP(G1276,sanschie!A:G,7,0)","v":123.1}]
["Absolut",63,"20TL","Absolut20TL63",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1277,sanschie!A:G,7,0)","v":258.8}]
["Absolut",64,"20TL",{"$f":"A1278&C1278&B1278","v":"Absolut20TL64"},null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1278,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",{"$f":"B1278+1","v":65},{"$f":"C1278","v":"20TL"},"Absolut20TL65",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1279,sanschie!A:G,7,0)","v":44.9}]
["Absolut",66,"20TL","Absolut20TL66",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1280,sanschie!A:G,7,0)","v":7.5}]
["Absolut",67,"20TL","Absolut20TL67",null,"ZBH 210 Verschlusszapfen 2Stk. aus Schaumstoff","103834","0",null,"STK",{"$f":"VLOOKUP(G1281,sanschie!A:G,7,0)","v":26.5}]
["Absolut",68,"20TL","Absolut20TL68",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1282,sanschie!A:G,7,0)","v":13.8}]
["Absolut",{"$f":"B1282+1","v":69},{"$f":"C1282","v":"20TL"},{"$f":"A1283&C1283&B1283","v":"Absolut20TL69"},null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1283,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",{"$f":"B1283+1","v":70},{"$f":"C1283","v":"20TL"},{"$f":"A1284&C1284&B1284","v":"Absolut20TL70"},null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1284,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B1284+1","v":71},{"$f":"C1284","v":"20TL"},{"$f":"A1285&C1285&B1285","v":"Absolut20TL71"},null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1285,sanschie!A:G,7,0)","v":26}]
["Absolut",{"$f":"B1285+1","v":72},{"$f":"C1285","v":"20TL"},{"$f":"A1286&C1286&B1286","v":"Absolut20TL72"},null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1286,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,"25TL",{"$f":"A1287&C1287&B1287","v":"Absolut25TL0"},"P","Absolut-Kaminanlage Ø 25TL","Absolut 25TL","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1287,sanschie!A:G,7,0)","v":0},null,{"$f":"I1287*1000","v":9000}]
["Absolut",{"$f":"B1287+1","v":1},{"$f":"C1287","v":"25TL"},"Absolut25TL1",null,"ABS Mantelstein EZTL 480 x 620mm L330mm","103922","0",null,"STK",{"$f":"VLOOKUP(G1288,sanschie!A:G,7,0)","v":63},{"$f":"ROUND(M1288,0)","v":27},{"$f":"((M1287)*3)/1000","v":27},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1288*330","v":0}]
["Absolut",2,"25TL","Absolut25TL2",null,"ABS 250 Profilkeramik-Rohr mit Muffe L660mm","103955",665,null,"STK",{"$f":"VLOOKUP(G1289,sanschie!A:G,7,0)","v":98},{"$f":"ROUNDUP(M1289,0)","v":12},{"$f":"(M1287-O1288-M1290-M1293-M1294-M1298)/1000/0.66","v":11.113636363636363}]
["Absolut",3,"25TL","Absolut25TL3",null,"ABS 250 Grundpaket","103861",1000,null,"STK",{"$f":"VLOOKUP(G1290,sanschie!A:G,7,0)","v":736},{"$f":"IF(Daten!$B$183=2,\"\",1)","v":1},{"$f":"IF(L1290=\"\",0,$H1290*$L1290)","v":1000}]
["Absolut",4,"25TL","Absolut25TL4",null,"ABS Sockelplatte aus Beton EZTL 480 x 620mm","103878","0",null,"STK",{"$f":"VLOOKUP(G1291,sanschie!A:G,7,0)","v":130}]
["Absolut",5,"25TL","Absolut25TL5",null,"CHZ 250 Keramik Fuss-Scheibe geschlossen","103702","0",null,"STK",{"$f":"VLOOKUP(G1292,sanschie!A:G,7,0)","v":92}]
["Absolut",6,"25TL","Absolut25TL6",null,"ABS 250 Rauchrohr-Anschlusspaket 90° RA  ","103985",665,null,"STK",{"$f":"VLOOKUP(G1293,sanschie!A:G,7,0)","v":490},{"$f":"IF(N1293=0,\"\",N1293)","v":1},{"$f":"IF(L1293=0,0,IF(L1293=\"\",0,L1293*H1293))","v":665},{"$f":"SUM(O1293:P1293)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",7,"25TL","Absolut25TL7",null,"ABS 250 Rauchrohr-Anschlusspaket 45° RA  ","103997",665,null,"STK",{"$f":"VLOOKUP(G1294,sanschie!A:G,7,0)","v":521},{"$f":"IF(N1294=0,\"\",N1294)","v":""},{"$f":"IF(L1294=0,0,IF(L1294=\"\",0,L1294*H1294))","v":0},{"$f":"SUM(O1294:P1294)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",8,"25TL","Absolut25TL8",null,"ABS 250 Rauchrohranschluss Stutzen-Set 90° Ø250mm","104003","0",null,"STK",{"$f":"VLOOKUP(G1295,sanschie!A:G,7,0)","v":249}]
["Absolut",9,"25TL","Absolut25TL9",null,"ABS 250 Rauchrohranschluss Stutzen-Set 45°","104009","0",null,"STK",{"$f":"VLOOKUP(G1296,sanschie!A:G,7,0)","v":249}]
["Absolut",10,"25TL","Absolut25TL10",null,"ABS 250 Steckadapter ","104271","0",null,"STK",{"$f":"VLOOKUP(G1297,sanschie!A:G,7,0)","v":234},{"$f":"IF(Daten!$B$226=2,1,\"\")","v":""}]
["Absolut",{"$f":"B1297+1","v":11},{"$f":"C1297","v":"25TL"},{"$f":"A1298&C1298&B1298","v":"Absolut25TL11"},null,"ABS 250 Putztür-Anschlusspaket ","103968",665,null,"STK",{"$f":"VLOOKUP(G1298,sanschie!A:G,7,0)","v":546},{"$f":"IF(N1298=0,\"\",N1298)","v":""},{"$f":"IF(L1298=0,0,IF(L1298=\"\",0,L1298*H1298))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",{"$f":"B1298+1","v":12},{"$f":"C1298","v":"25TL"},{"$f":"A1299&C1299&B1299","v":"Absolut25TL12"},null,"ABS 250 Putztüranschluss Stutzen Set","104276","0",null,"STK",{"$f":"VLOOKUP(G1299,sanschie!A:G,7,0)","v":472}]
["Absolut",{"$f":"B1299+1","v":13},{"$f":"C1299","v":"25TL"},{"$f":"A1300&C1300&B1300","v":"Absolut25TL13"},null,"ABS Handyplatte EZTL Inox 480 x 620mm","104178","0",null,"STK",{"$f":"VLOOKUP(G1300,sanschie!A:G,7,0)","v":235},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",{"$f":"B1300+1","v":14},{"$f":"C1300","v":"25TL"},{"$f":"A1301&C1301&B1301","v":"Absolut25TL14"},null,"ABS Handyplatte EZTL Kupfer 480 x 620mm","104188","0",null,"STK",{"$f":"VLOOKUP(G1301,sanschie!A:G,7,0)","v":358}]
["Absolut",{"$f":"B1301+1","v":15},{"$f":"C1301","v":"25TL"},{"$f":"A1302&C1302&B1302","v":"Absolut25TL15"},null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G1302,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",{"$f":"B1302+1","v":16},{"$f":"C1302","v":"25TL"},{"$f":"A1303&C1303&B1303","v":"Absolut25TL16"},null,"ABS HEB-Set Handyplatte Kupfer mit Langschrauben","104189","0",null,"STK",{"$f":"VLOOKUP(G1303,sanschie!A:G,7,0)","v":101}]
["Absolut",17,"25TL","Absolut25TL17",null,"KER 250 Keranova-Fugenglätter","103476","0",null,"STK",{"$f":"VLOOKUP(G1304,sanschie!A:G,7,0)","v":79}]
["Absolut",18,"25TL","Absolut25TL18",null,"ABS 250 Abströmkonus verkupfert","104208","0",null,"STK",{"$f":"VLOOKUP(G1305,sanschie!A:G,7,0)","v":258}]
["Absolut",19,"25TL","Absolut25TL19",null,"ABS 250 Doppelfutter zu Rauchrohranschluss Ø180mm","104025","0",null,"STK",{"$f":"VLOOKUP(G1306,sanschie!A:G,7,0)","v":210},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",20,"25TL","Absolut25TL20",null,"ABS 250 Doppelfutter zu Rauchrohranschluss Ø200mm","104026","0",null,"STK",{"$f":"VLOOKUP(G1307,sanschie!A:G,7,0)","v":222},{"$f":"IF(Daten!$B$226=8,1,\"\")","v":""}]
["Absolut",21,"25TL","Absolut25TL21",null,"ABS 250 Doppelfutter zu Rauchrohranschluss Ø250mm","104027","0",null,"STK",{"$f":"VLOOKUP(G1308,sanschie!A:G,7,0)","v":234},{"$f":"IF(Daten!$B$226=9,1,\"\")","v":""}]
["Absolut",22,"25TL","Absolut25TL22",null,"ABS 250 Kondensatfalle zu RA 45° Ø180mm","104041","0",null,"STK",{"$f":"VLOOKUP(G1309,sanschie!A:G,7,0)","v":426}]
["Absolut",23,"25TL","Absolut25TL23",null,"ABS 250 Kondensatfalle zu RA 45° Ø200mm","104042","0",null,"STK",{"$f":"VLOOKUP(G1310,sanschie!A:G,7,0)","v":426}]
["Absolut",24,"25TL","Absolut25TL24",null,"ABS 250 Kondensatfalle zu RA 45° Ø250mm","104043","0",null,"STK",{"$f":"VLOOKUP(G1311,sanschie!A:G,7,0)","v":426}]
["Absolut",25,"25TL","Absolut25TL25",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1312,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",26,"25TL","Absolut25TL26",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1313,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",27,"25TL","Absolut25TL27",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1314,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",28,"25TL","Absolut25TL28",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1315,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1290=1,1,\"\")","v":1}]
["Absolut",29,"25TL","Absolut25TL29",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1316,sanschie!A:G,7,0)","v":489},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""}]
["Absolut",30,"25TL","Absolut25TL30",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1317,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",31,"25TL","Absolut25TL31",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1318,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",32,"25TL","Absolut25TL32",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G1319,sanschie!A:G,7,0)","v":14},{"$f":"IF(Daten!$B$183=2,N1319,Sortimente!P1319)","v":2},null,{"$f":"ROUNDUP(O1319,0)","v":6},{"$f":"L1289/2","v":6},{"$f":"IF(L1289<=8,\"\",IF(L1289<=10,1,IF(L1289<=12,2,IF(L1289<=14,3,4))))","v":2}]
["Absolut",33,"25TL","Absolut25TL33",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1320,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1320=0,\"\",N1320)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",34,"25TL","Absolut25TL34",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1321,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1321=0,\"\",N1321)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",35,"25TL","Absolut25TL35",null,"ZBH Revisionstüre 100 x 275 mm Alu eloxiert","103842","0",null,"STK",{"$f":"VLOOKUP(G1322,sanschie!A:G,7,0)","v":87.4},{"$f":"IF(Daten!$G$249=0,\"\",Daten!$G$249)","v":""}]
["Absolut",36,"25TL","Absolut25TL36",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1323,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",37,"25TL","Absolut25TL37",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1324,sanschie!A:G,7,0)","v":35},{"$f":"ROUNDUP(M1324,0)","v":1},{"$f":"N1324/10","v":0.9},{"$f":"Daten!$B$61","v":9}]
["Absolut",38,"25TL","Absolut25TL38",null,"ABS 250 Basten Standard Inox","104214","0",null,"STK",{"$f":"VLOOKUP(G1325,sanschie!A:G,7,0)","v":400},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",39,"25TL","Absolut25TL39",null,"ABS 250 Basten Standard Kupfer","104221","0",null,"STK",{"$f":"VLOOKUP(G1326,sanschie!A:G,7,0)","v":545},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",40,"25TL","Absolut25TL40",null,"ABS 250 Sairlift Inox","104226","0",null,"STK",{"$f":"VLOOKUP(G1327,sanschie!A:G,7,0)","v":465},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",41,"25TL","Absolut25TL41",null,"ABS 250 Sairlift Kupfer","104231","0",null,"STK",{"$f":"VLOOKUP(G1328,sanschie!A:G,7,0)","v":480},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",42,"25TL","Absolut25TL42",null,"ZBH 250 Verschlussbüchse weiss ØA 300mm","103840","0",null,"STK",{"$f":"VLOOKUP(G1329,sanschie!A:G,7,0)","v":138}]
["Absolut",43,"25TL","Absolut25TL43",null,"ZBH 250 Verschlussbüchse weiss ØA 300mm","103840","0",null,"STK",{"$f":"VLOOKUP(G1330,sanschie!A:G,7,0)","v":138}]
["Absolut",44,"25TL","Absolut25TL44",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1331,sanschie!A:G,7,0)","v":258.8}]
["Absolut",45,"25TL","Absolut25TL45",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1332,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",46,"25TL","Absolut25TL46",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1333,sanschie!A:G,7,0)","v":44.9}]
["Absolut",47,"25TL","Absolut25TL47",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1334,sanschie!A:G,7,0)","v":7.5}]
["Absolut",48,"25TL","Absolut25TL48",null,"ZBH 260 Verschlusszapfen 2Stk. aus Schaumstoff","103835","0",null,"STK",{"$f":"VLOOKUP(G1335,sanschie!A:G,7,0)","v":31.1}]
["Absolut",49,"25TL","Absolut25TL49",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1336,sanschie!A:G,7,0)","v":13.8}]
["Absolut",50,"25TL","Absolut25TL50",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1337,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",{"$f":"B1337+1","v":51},{"$f":"C1337","v":"25TL"},"Absolut25TL51",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1338,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B1338+1","v":52},{"$f":"C1338","v":"25TL"},"Absolut25TL52",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1339,sanschie!A:G,7,0)","v":26}]
["Absolut",{"$f":"B1339+1","v":53},{"$f":"C1339","v":"25TL"},"Absolut25TL53",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1340,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,"30L",{"$f":"A1341&C1341&B1341","v":"Absolut30L0"},"P","Absolut-Kaminanlage Ø 30L","Absolut 30L","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1341,sanschie!A:G,7,0)","v":0},null,{"$f":"I1341*1000","v":9000}]
["Absolut",{"$f":"B1341+1","v":1},{"$f":"C1341","v":"30L"},{"$f":"A1342&C1342&B1342","v":"Absolut30L1"},null,"ABS Mantelstein EZTL 550 x 710mm L330mm","103923","0",null,"STK",{"$f":"VLOOKUP(G1342,sanschie!A:G,7,0)","v":118},{"$f":"ROUND(M1342,0)","v":27},{"$f":"((M1341)*3)/1000","v":27},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1342*330","v":0}]
["Absolut",{"$f":"B1342+1","v":2},{"$f":"C1342","v":"30L"},{"$f":"A1343&C1343&B1343","v":"Absolut30L2"},null,"ABS 300 Profilkeramik-Rohr mit Muffe L660mm","103956",665,null,"STK",{"$f":"VLOOKUP(G1343,sanschie!A:G,7,0)","v":105},{"$f":"ROUNDUP(M1343,0)","v":12},{"$f":"(M1341-O1342-M1344-M1346-M1347)/H1343","v":11.030075187969924}]
["Absolut",3,"30L","Absolut30L3",null,"ABS 300 Grundpaket","103862",1000,null,"STK",{"$f":"VLOOKUP(G1344,sanschie!A:G,7,0)","v":983},1,{"$f":"IF(L1344=0,0,IF(L1344=\"\",0,L1344*1000))","v":1000}]
["Absolut",4,"30L","Absolut30L4",null,"ABS Sockelplatte aus Beton EZTL 550 x 710mm","103879","0",null,"STK",{"$f":"VLOOKUP(G1345,sanschie!A:G,7,0)","v":151},1]
["Absolut",5,"30L","Absolut30L5",null,"ABS 300 Rauchrohr-Anschlusspaket 90° RA  ","103986",665,null,"STK",{"$f":"VLOOKUP(G1346,sanschie!A:G,7,0)","v":613},1,{"$f":"IF(L1346=0,0,IF(L1346=\"\",0,L1346*H1346))","v":665},{"$f":"SUM(O1346:P1346)","v":1},1,""]
["Absolut",6,"30L","Absolut30L6",null,"ABS 300 Putztür-Anschlusspaket ","103969",665,null,"STK",{"$f":"VLOOKUP(G1347,sanschie!A:G,7,0)","v":607},{"$f":"IF(N1347=0,\"\",N1347)","v":""},{"$f":"IF(N1347=0,0,IF(N1347=\"\",0,N1347*H1347))","v":0},{"$f":"IF(Daten!$B$261=1,0,Daten!$C$261)","v":0}]
["Absolut",7,"30L","Absolut30L7",null,"ABS Handyplatte EZTL Inox 550 x 710mm ","104179","0",null,"STK",{"$f":"VLOOKUP(G1348,sanschie!A:G,7,0)","v":255},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",8,"30L","Absolut30L8",null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G1349,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",9,"30L","Absolut30L9",null,"ABS 300 Abströmkonus verkupfert","104209","0",null,"STK",{"$f":"VLOOKUP(G1350,sanschie!A:G,7,0)","v":358}]
["Absolut",10,"30L","Absolut30L10",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1351,sanschie!A:G,7,0)","v":303},{"$f":"IF(Daten!$B$287=2,1,\"\")","v":""}]
["Absolut",11,"30L","Absolut30L11",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1352,sanschie!A:G,7,0)","v":94},{"$f":"IF(Daten!$B$287=2,1,\"\")","v":""}]
["Absolut",12,"30L","Absolut30L12",null,"ZBH Revisionstüre 100 x 275 mm Alu eloxiert","103842","0",null,"STK",{"$f":"VLOOKUP(G1353,sanschie!A:G,7,0)","v":87.4},{"$f":"IF(Daten!$G$249=0,\"\",Daten!$G$249)","v":""}]
["Absolut",13,"30L","Absolut30L13",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1354,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",14,"30L","Absolut30L14",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1355,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",15,"30L","Absolut30L15",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1356,sanschie!A:G,7,0)","v":35},{"$f":"ROUNDUP(M1356,0)","v":1},{"$f":"N1356/10","v":0.9},{"$f":"Daten!$B$61","v":9}]
["Absolut",16,"30L","Absolut30L16",null,"ABS 300 Basten Standard Inox","104215","0",null,"STK",{"$f":"VLOOKUP(G1357,sanschie!A:G,7,0)","v":535},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",17,"30L","Absolut30L17",null,"ABS 300 Basten Standard Kupfer","104220","0",null,"STK",{"$f":"VLOOKUP(G1358,sanschie!A:G,7,0)","v":414},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",18,"30L","Absolut30L18",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1359,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",19,"30L","Absolut30L19",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G1360,sanschie!A:G,7,0)","v":14},{"$f":"IF(M1360<0,\"\",M1360)","v":""},{"$f":"ROUNDUP(((K1341-11.66)-SUM(N1346,N1347))/1.33,0)","v":-10}]
["Absolut",20,"30L","Absolut30L20",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1361,sanschie!A:G,7,0)","v":258.8}]
["Absolut",21,"30L","Absolut30L21",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1362,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",22,"30L","Absolut30L22",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1363,sanschie!A:G,7,0)","v":44.9}]
["Absolut",23,"30L","Absolut30L23",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1364,sanschie!A:G,7,0)","v":7.5}]
["Absolut",24,"30L","Absolut30L24",null,"ZBH 260 Verschlusszapfen 2Stk. aus Schaumstoff","103835","0",null,"STK",{"$f":"VLOOKUP(G1365,sanschie!A:G,7,0)","v":31.1}]
["Absolut",25,"30L","Absolut30L25",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1366,sanschie!A:G,7,0)","v":13.8}]
["Absolut",26,"30L","Absolut30L26",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1367,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",27,"30L","Absolut30L27",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1368,sanschie!A:G,7,0)","v":322}]
["Absolut",28,"30L","Absolut30L28",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1369,sanschie!A:G,7,0)","v":26}]
["Absolut",29,"30L","Absolut30L29",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1370,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,"40L","Absolut40L0","P","Absolut-Kaminanlage Ø 40L","Absolut 40L","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1371,sanschie!A:G,7,0)","v":0},null,{"$f":"I1371*1000","v":9000}]
["Absolut",{"$f":"B1371+1","v":1},{"$f":"C1371","v":"40L"},"Absolut40L1",null,"ABS Mantelstein EZTL 670 x 860mm L330mm","103924","0",null,"STK",{"$f":"VLOOKUP(G1372,sanschie!A:G,7,0)","v":199},{"$f":"ROUND(M1372,0)","v":27},{"$f":"((M1371)*3)/1000","v":27},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1372*330","v":0}]
["Absolut",2,"40L","Absolut40L2",null,"ABS 400 Profilkeramik-Rohr mit Muffe L660mm","103957",665,null,"STK",{"$f":"VLOOKUP(G1373,sanschie!A:G,7,0)","v":158},{"$f":"ROUNDUP(M1373,0)","v":12},{"$f":"(M1371-O1372-M1374-M1376-M1377)/H1373","v":11.030075187969924}]
["Absolut",3,"40L","Absolut40L3",null,"ABS 400 Grundpaket","103863",1000,null,"STK",{"$f":"VLOOKUP(G1374,sanschie!A:G,7,0)","v":1226},1,{"$f":"IF(L1374=0,0,IF(L1374=\"\",0,L1374*1000))","v":1000}]
["Absolut",4,"40L","Absolut40L4",null,"ABS Sockelplatte aus Beton EZTL 670 x 860mm","103880","0",null,"STK",{"$f":"VLOOKUP(G1375,sanschie!A:G,7,0)","v":176},1]
["Absolut",5,"40L","Absolut40L5",null,"ABS 400 Rauchrohr-Anschlusspaket 90° RA  ","103987",665,null,"STK",{"$f":"VLOOKUP(G1376,sanschie!A:G,7,0)","v":736},1,{"$f":"IF(L1376=0,0,IF(L1376=\"\",0,L1376*H1376))","v":665},{"$f":"SUM(O1376:P1376)","v":1},1,""]
["Absolut",6,"40L","Absolut40L6",null,"ABS 400 Putztür-Anschlusspaket ","103970",665,null,"STK",{"$f":"VLOOKUP(G1377,sanschie!A:G,7,0)","v":731},{"$f":"IF(N1377=0,\"\",N1377)","v":""},{"$f":"IF(N1377=0,0,IF(N1377=\"\",0,N1377*H1377))","v":0},{"$f":"IF(Daten!$B$261=1,0,Daten!$C$261)","v":0}]
["Absolut",7,"40L","Absolut40L7",null,"ABS Handyplatte EZTL Inox 670 x 860mm  ","104180","0",null,"STK",{"$f":"VLOOKUP(G1378,sanschie!A:G,7,0)","v":279},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",8,"40L","Absolut40L8",null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G1379,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",9,"40L","Absolut40L9",null,"ABS 400 Abströmkonus verkupfert","104210","0",null,"STK",{"$f":"VLOOKUP(G1380,sanschie!A:G,7,0)","v":481}]
["Absolut",10,"40L","Absolut40L10",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1381,sanschie!A:G,7,0)","v":303},{"$f":"IF(Daten!$B$287=2,1,\"\")","v":""}]
["Absolut",11,"40L","Absolut40L11",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1382,sanschie!A:G,7,0)","v":94},{"$f":"IF(Daten!$B$287=2,1,\"\")","v":""}]
["Absolut",12,"40L","Absolut40L12",null,"ZBH Revisionstüre 100 x 275 mm Alu eloxiert","103842","0",null,"STK",{"$f":"VLOOKUP(G1383,sanschie!A:G,7,0)","v":87.4},{"$f":"IF(Daten!$G$249=0,\"\",Daten!$G$249)","v":""}]
["Absolut",13,"40L","Absolut40L13",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1384,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",14,"40L","Absolut40L14",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1385,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",15,"40L","Absolut40L15",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1386,sanschie!A:G,7,0)","v":35},{"$f":"ROUNDUP(M1386,0)","v":2},{"$f":"N1386/7","v":1.2857142857142858},{"$f":"Daten!$B$61","v":9}]
["Absolut",16,"40L","Absolut40L16",null,"ABS 400 Basten Standard Inox","104216","0",null,"STK",{"$f":"VLOOKUP(G1387,sanschie!A:G,7,0)","v":596},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",17,"40L","Absolut40L17",null,"ABS 400 Basten Standard Kupfer","104222","0",null,"STK",{"$f":"VLOOKUP(G1388,sanschie!A:G,7,0)","v":596},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",18,"40L","Absolut40L18",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1389,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",19,"40L","Absolut40L19",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G1390,sanschie!A:G,7,0)","v":14},{"$f":"IF(M1390<0,\"\",M1390)","v":""},{"$f":"ROUNDUP(((K1371-11.66)-SUM(N1376,N1377))/1.33,0)","v":-10}]
["Absolut",20,"40L","Absolut40L20",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1391,sanschie!A:G,7,0)","v":258.8}]
["Absolut",21,"40L","Absolut40L21",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1392,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",22,"40L","Absolut40L22",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1393,sanschie!A:G,7,0)","v":44.9}]
["Absolut",23,"40L","Absolut40L23",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1394,sanschie!A:G,7,0)","v":7.5}]
["Absolut",24,"40L","Absolut40L24",null,"ZBH 260 Verschlusszapfen 2Stk. aus Schaumstoff","103835","0",null,"STK",{"$f":"VLOOKUP(G1395,sanschie!A:G,7,0)","v":31.1}]
["Absolut",25,"40L","Absolut40L25",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1396,sanschie!A:G,7,0)","v":13.8}]
["Absolut",26,"40L","Absolut40L26",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1397,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",27,"40L","Absolut40L27",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1398,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B1398+1","v":28},{"$f":"C1398","v":"40L"},{"$f":"A1399&C1399&B1399","v":"Absolut40L28"},null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1399,sanschie!A:G,7,0)","v":26}]
["Absolut",{"$f":"B1399+1","v":29},{"$f":"C1399","v":"40L"},{"$f":"A1400&C1400&B1400","v":"Absolut40L29"},null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1400,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,1614,{"$f":"A1401&C1401&B1401","v":"Absolut16140"},"P","Absolut-Kaminanlage Ø 1614","Absolut 1614","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1401,sanschie!A:G,7,0)","v":0},null,{"$f":"I1401*1000","v":9000}]
["Absolut",{"$f":"B1401+1","v":1},{"$f":"C1401","v":1614},{"$f":"A1402&C1402&B1402","v":"Absolut16141"},null,"ABS Mantelstein DZ 360 x 650mm L330mm","103925","0",null,"STK",{"$f":"VLOOKUP(G1402,sanschie!A:G,7,0)","v":51},{"$f":"ROUND(M1402,0)-M1403","v":24},{"$f":"((M1401-M1407)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1402*330","v":0}]
["Absolut",{"$f":"B1402+1","v":2},{"$f":"C1402","v":1614},{"$f":"A1403&C1403&B1403","v":"Absolut16142"},null,"ABS Thermo-Trennstein DZ 360 x 650mm L330mm","103937","0",null,"STK",{"$f":"VLOOKUP(G1403,sanschie!A:G,7,0)","v":259},{"$f":"IF(M1403=0,\"\",M1403)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,1614,"Absolut16143",null,"ABS Thermo-Fussplatte DZ 360 x 650mm","103855","0",null,"STK",{"$f":"VLOOKUP(G1404,sanschie!A:G,7,0)","v":198}]
["Absolut",4,1614,"Absolut16144",null,"ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","103947",1330,null,"STK",{"$f":"VLOOKUP(G1405,sanschie!A:G,7,0)","v":113},{"$f":"ROUNDUP(M1405,0)","v":6},{"$f":"(M1401-O1402-M1407-M1412-M1413-M1422)/1000/1.33","v":5.962406015037593}]
["Absolut",5,1614,"Absolut16145",null,"ABS 140 Profilkeramik-Rohr mit Muffe L1330mm","103946",1330,null,"STK",{"$f":"VLOOKUP(G1406,sanschie!A:G,7,0)","v":106},{"$f":"ROUNDUP(M1406,0)","v":5},{"$f":"(M1401-O1402-M1407-M1416-M1417-M1423)/1000/1.33","v":4.962406015037593}]
["Absolut",6,1614,"Absolut16146",null,"ABS 180 Fertigfuss DZ 2 x Ø120-180mm L1070mm","103866",1070,null,"STK",{"$f":"VLOOKUP(G1407,sanschie!A:G,7,0)","v":1472},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1407=\"\",0,$H1407*$L1407)","v":1070}]
["Absolut",7,1614,"Absolut16147",null,"ABS 160 Fertigfusspaket ","103890","0",null,"STK",{"$f":"VLOOKUP(G1408,sanschie!A:G,7,0)","v":311},{"$f":"L1407","v":1}]
["Absolut",8,1614,"Absolut16148",null,"ABS 140 Fertigfusspaket ","103889","0",null,"STK",{"$f":"VLOOKUP(G1409,sanschie!A:G,7,0)","v":311},{"$f":"L1407","v":1}]
["Absolut",9,1614,"Absolut16149",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G1410,sanschie!A:G,7,0)","v":18}]
["Absolut",10,1614,"Absolut161410",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G1411,sanschie!A:G,7,0)","v":32},{"$f":"IF(L1407=\"\",2,\"\")","v":""}]
["Absolut",11,1614,"Absolut161411",null,"ABS 160 Rauchrohr-Anschlusspaket 90° RA  ","103982",1330,null,"STK",{"$f":"VLOOKUP(G1412,sanschie!A:G,7,0)","v":367},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""},{"$f":"IF(L1412=0,0,IF(L1412=\"\",0,L1412*H1412))","v":0}]
["Absolut",12,1614,"Absolut161412",null,"ABS 160 Rauchrohr-Anschlusspaket 45° RA  ","103994",1330,null,"STK",{"$f":"VLOOKUP(G1413,sanschie!A:G,7,0)","v":367},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""},{"$f":"IF(L1413=0,0,IF(L1413=\"\",0,L1413*H1413))","v":0}]
["Absolut",13,1614,"Absolut161413",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø160mm","104000","0",null,"STK",{"$f":"VLOOKUP(G1414,sanschie!A:G,7,0)","v":199}]
["Absolut",14,1614,"Absolut161414",null,"ABS 160 Rauchrohranschluss Stutzen-Set 45°","104006","0",null,"STK",{"$f":"VLOOKUP(G1415,sanschie!A:G,7,0)","v":199}]
["Absolut",15,1614,"Absolut161415",null,"ABS 140 Rauchrohr-Anschlusspaket 90° RA  ","103981",1330,null,"STK",{"$f":"VLOOKUP(G1416,sanschie!A:G,7,0)","v":355},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(L1416=0,0,IF(L1416=\"\",0,L1416*H1416))","v":1330}]
["Absolut",16,1614,"Absolut161416",null,"ABS 140 Rauchrohr-Anschlusspaket 45° RA  ","103993",1330,null,"STK",{"$f":"VLOOKUP(G1417,sanschie!A:G,7,0)","v":355},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(L1417=0,0,IF(L1417=\"\",0,L1417*H1417))","v":0}]
["Absolut",17,1614,"Absolut161417",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø140mm","103999","0",null,"STK",{"$f":"VLOOKUP(G1418,sanschie!A:G,7,0)","v":191}]
["Absolut",18,1614,"Absolut161418",null,"ABS 140 Rauchrohranschluss Stutzen-Set 45°","104005","0",null,"STK",{"$f":"VLOOKUP(G1419,sanschie!A:G,7,0)","v":191},null,null,null,"großer Zug","kleine Zug"]
["Absolut",19,1614,"Absolut161419",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G1420,sanschie!A:G,7,0)","v":160},{"$f":"IF(N1420=0,\"\",N1420)","v":""},null,{"$f":"SUM(O1420:P1420)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",20,1614,"Absolut161420",null,"ABS 200 Steckadapter ","104269","0",null,"STK",{"$f":"VLOOKUP(G1421,sanschie!A:G,7,0)","v":184}]
["Absolut",21,1614,"Absolut161421",null,"ABS 160 Putztür-Anschlusspaket ","103965",1330,null,"STK",{"$f":"VLOOKUP(G1422,sanschie!A:G,7,0)","v":428},{"$f":"IF(N1422=0,\"\",N1422)","v":""},{"$f":"IF(L1422=0,0,IF(L1422=\"\",0,L1422*H1422))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",22,1614,"Absolut161422",null,"ABS 140 Putztür-Anschlusspaket ","103964",1330,null,"STK",{"$f":"VLOOKUP(G1423,sanschie!A:G,7,0)","v":410},{"$f":"IF(N1423=0,\"\",N1423)","v":""},{"$f":"IF(L1423=0,0,IF(L1423=\"\",0,L1423*H1423))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",23,1614,"Absolut161423",null,"ABS 160 Putztüranschluss Stutzen Set","104273","0",null,"STK",{"$f":"VLOOKUP(G1424,sanschie!A:G,7,0)","v":325}]
["Absolut",24,1614,"Absolut161424",null,"ABS 140 Putztüranschluss Stutzen Set","104272","0",null,"STK",{"$f":"VLOOKUP(G1425,sanschie!A:G,7,0)","v":311}]
["Absolut",25,1614,"Absolut161425",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1426,sanschie!A:G,7,0)","v":27}]
["Absolut",26,1614,"Absolut161426",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104192","0",null,"STK",{"$f":"VLOOKUP(G1427,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",27,1614,"Absolut161427",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104195","0",null,"STK",{"$f":"VLOOKUP(G1428,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",28,1614,"Absolut161428",null,"ABS Handyplatte DZ Faserzement 360 x 650mm ","104149","0",null,"STK",{"$f":"VLOOKUP(G1429,sanschie!A:G,7,0)","v":167},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",29,1614,"Absolut161429",null,"ABS Handyplatte DZ Inox 360 x 650mm","104181","0",null,"STK",{"$f":"VLOOKUP(G1430,sanschie!A:G,7,0)","v":229},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",30,1614,"Absolut161430",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1431,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",31,1614,"Absolut161431",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G1432,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",32,1614,"Absolut161432",null,"ABS 160 Abströmkonus verkupfert","104205","0",null,"STK",{"$f":"VLOOKUP(G1433,sanschie!A:G,7,0)","v":166}]
["Absolut",33,1614,"Absolut161433",null,"ABS 140 Abströmkonus verkupfert","104204","0",null,"STK",{"$f":"VLOOKUP(G1434,sanschie!A:G,7,0)","v":161}]
["Absolut",{"$f":"B1434+1","v":34},{"$f":"C1434","v":1614},"Absolut161434",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G1435,sanschie!A:G,7,0)","v":1900}]
["Absolut",35,1614,"Absolut161435",null,"ABS 160 Anschlusskonus DZ mit Doppelfutter DN150mm","103902","0",null,"STK",{"$f":"VLOOKUP(G1436,sanschie!A:G,7,0)","v":256.8}]
["Absolut",36,1614,"Absolut161436",null,"ABS 180 Adapterring von 180mm auf 160mm L90mm","103906","0",null,"STK",{"$f":"VLOOKUP(G1437,sanschie!A:G,7,0)","v":41}]
["Absolut",37,1614,"Absolut161437",null,"ABS 180 Adapterring von 180mm auf 140mm L90mm","103905","0",null,"STK",{"$f":"VLOOKUP(G1438,sanschie!A:G,7,0)","v":35}]
["Absolut",38,1614,"Absolut161438",null,"KER 160  Keranova-Fugenglätter","103473","0",null,"STK",{"$f":"VLOOKUP(G1439,sanschie!A:G,7,0)","v":58}]
["Absolut",39,1614,"Absolut161439",null,"KER 140  Keranova-Fugenglätter","103472","0",null,"STK",{"$f":"VLOOKUP(G1440,sanschie!A:G,7,0)","v":57}]
["Absolut",40,1614,"Absolut161440",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø80mm","104010","0",null,"STK",{"$f":"VLOOKUP(G1441,sanschie!A:G,7,0)","v":124}]
["Absolut",41,1614,"Absolut161441",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G1442,sanschie!A:G,7,0)","v":136},{"$f":"IF(N1442=0,\"\",N1442)","v":""},null,{"$f":"SUM(O1442:P1442)","v":0},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",42,1614,"Absolut161442",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G1443,sanschie!A:G,7,0)","v":149},{"$f":"IF(N1443=0,\"\",N1443)","v":""},null,{"$f":"SUM(O1443:P1443)","v":0},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",43,1614,"Absolut161443",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G1444,sanschie!A:G,7,0)","v":160},{"$f":"IF(N1444=0,\"\",N1444)","v":""},null,{"$f":"SUM(O1444:P1444)","v":0},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",44,1614,"Absolut161444",null,"CHZ 150 Doppelfutter lose L150mm","103803","0",null,"STK",{"$f":"VLOOKUP(G1445,sanschie!A:G,7,0)","v":103},{"$f":"IF(N1445=0,\"\",N1445)","v":""},null,{"$f":"SUM(O1445:P1445)","v":0},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=6,1,\"\")","v":""}]
["Absolut",45,1614,"Absolut161445",null,"ABS 140 Kondensatfalle zu RA 45° Ø130mm ","104028","0",null,"STK",{"$f":"VLOOKUP(G1446,sanschie!A:G,7,0)","v":297}]
["Absolut",46,1614,"Absolut161446",null,"ABS 160 Kondensatfalle zu RA 45° Ø130mm ","104029","0",null,"STK",{"$f":"VLOOKUP(G1447,sanschie!A:G,7,0)","v":322}]
["Absolut",47,1614,"Absolut161447",null,"ABS 160 Kondensatfalle zu RA 45° Ø150mm ","104030","0",null,"STK",{"$f":"VLOOKUP(G1448,sanschie!A:G,7,0)","v":322}]
["Absolut",48,1614,"Absolut161448",null,"ABS 160 Kondensatfalle zu RA 45° Ø160mm ","104031","0",null,"STK",{"$f":"VLOOKUP(G1449,sanschie!A:G,7,0)","v":322}]
["Absolut",49,1614,"Absolut161449",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1450,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",50,1614,"Absolut161450",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1451,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",51,1614,"Absolut161451",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1452,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",52,1614,"Absolut161452",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1453,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1408=2,1,\"\")","v":""}]
["Absolut",53,1614,"Absolut161453",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1454,sanschie!A:G,7,0)","v":489},{"$f":"IF(N1454=0,\"\",N1454)","v":""},null,{"$f":"SUM(O1454:P1454)","v":0},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""},{"$f":"IF(Daten!$F$241=1,\"\",1)","v":""}]
["Absolut",54,1614,"Absolut161454",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1455,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",55,1614,"Absolut161455",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1456,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",56,1614,"Absolut161456",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G1457,sanschie!A:G,7,0)","v":14},{"$f":"IF(N1457=0,\"\",ROUNDUP(N1457,0))","v":""},null,{"$f":"SUM(O1457:P1457)","v":0},{"$f":"IF(L1405<=8,0,(L1405-8)/2)","v":0},{"$f":"IF(L1406<=8,0,(L1406-8)/2)","v":0}]
["Absolut",57,1614,"Absolut161457",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1458,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1458=0,\"\",N1458)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",58,1614,"Absolut161458",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1459,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1459=0,\"\",N1459)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",59,1614,"Absolut161459",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1460,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",60,1614,"Absolut161460",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1461,sanschie!A:G,7,0)","v":35},{"$f":"IF(N1461<=11.5,1,2)","v":1},null,{"$f":"IF(L1407=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",61,1614,"Absolut161461",null,"ABS 160 Basten Standard Inox","104211","0",null,"STK",{"$f":"VLOOKUP(G1462,sanschie!A:G,7,0)","v":323},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",62,1614,"Absolut161462",null,"ABS 160 Basten Standard Kupfer","104217","0",null,"STK",{"$f":"VLOOKUP(G1463,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",63,1614,"Absolut161463",null,"ABS 160 Sairlift Inox","104223","0",null,"STK",{"$f":"VLOOKUP(G1464,sanschie!A:G,7,0)","v":374},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",64,1614,"Absolut161464",null,"ABS 160 Sairlift Kupfer","104228","0",null,"STK",{"$f":"VLOOKUP(G1465,sanschie!A:G,7,0)","v":397},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",65,1614,"Absolut161465",null,"ZBH 150 Verschlussbüchse weiss ØA 275mm","103836","0",null,"STK",{"$f":"VLOOKUP(G1466,sanschie!A:G,7,0)","v":115}]
["Absolut",{"$f":"B1466+1","v":66},{"$f":"C1466","v":1614},"Absolut161466",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1467,sanschie!A:G,7,0)","v":258.8}]
["Absolut",67,1614,"Absolut161467",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1468,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",68,1614,{"$f":"A1469&C1469&B1469","v":"Absolut161468"},null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1469,sanschie!A:G,7,0)","v":44.9}]
["Absolut",69,1614,"Absolut161469",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1470,sanschie!A:G,7,0)","v":7.5}]
["Absolut",70,1614,"Absolut161470",null,"ZBH 170 Verschlusszapfen 2Stk. aus Schaumstoff","103832","0",null,"STK",{"$f":"VLOOKUP(G1471,sanschie!A:G,7,0)","v":24.2}]
["Absolut",71,1614,"Absolut161471",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G1472,sanschie!A:G,7,0)","v":452}]
["Absolut",72,1614,"Absolut161472",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G1473,sanschie!A:G,7,0)","v":538}]
["Absolut",73,1614,"Absolut161473",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G1474,sanschie!A:G,7,0)","v":634}]
["Absolut",74,1614,"Absolut161474",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G1475,sanschie!A:G,7,0)","v":695}]
["Absolut",75,1614,"Absolut161475",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G1476,sanschie!A:G,7,0)","v":797}]
["Absolut",76,1614,"Absolut161476",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G1477,sanschie!A:G,7,0)","v":873}]
["Absolut",77,1614,"Absolut161477",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1478,sanschie!A:G,7,0)","v":13.8}]
["Absolut",78,1614,"Absolut161478",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1479,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",79,1614,"Absolut161479",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1480,sanschie!A:G,7,0)","v":322}]
["Absolut",80,1614,"Absolut161480",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1481,sanschie!A:G,7,0)","v":26}]
["Absolut",81,1614,"Absolut161481",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1482,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,1814,{"$f":"A1483&C1483&B1483","v":"Absolut18140"},"P","Absolut-Kaminanlage Ø 1814","Absolut 1814","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1483,sanschie!A:G,7,0)","v":0},null,{"$f":"I1483*1000","v":9000}]
["Absolut",{"$f":"B1483+1","v":1},{"$f":"C1483","v":1814},{"$f":"A1484&C1484&B1484","v":"Absolut18141"},null,"ABS Mantelstein DZ 360 x 650mm L330mm","103925","0",null,"STK",{"$f":"VLOOKUP(G1484,sanschie!A:G,7,0)","v":51},{"$f":"ROUND(M1484,0)-M1485","v":24},{"$f":"((M1483-M1489)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1484*330","v":0}]
["Absolut",{"$f":"B1484+1","v":2},{"$f":"C1484","v":1814},{"$f":"A1485&C1485&B1485","v":"Absolut18142"},null,"ABS Thermo-Trennstein DZ 360 x 650mm L330mm","103937","0",null,"STK",{"$f":"VLOOKUP(G1485,sanschie!A:G,7,0)","v":259},{"$f":"IF(M1485=0,\"\",M1485)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,1814,"Absolut18143",null,"ABS Thermo-Fussplatte DZ 360 x 650mm","103855","0",null,"STK",{"$f":"VLOOKUP(G1486,sanschie!A:G,7,0)","v":198}]
["Absolut",4,1814,"Absolut18144",null,"ABS 180 Profilkeramik-Rohr mit Muffe L1330mm","103948",1330,null,"STK",{"$f":"VLOOKUP(G1487,sanschie!A:G,7,0)","v":122},{"$f":"ROUNDUP(M1487,0)","v":6},{"$f":"(M1483-O1484-M1489-M1495-M1496-M1505)/1000/1.33","v":5.962406015037593}]
["Absolut",5,1814,"Absolut18145",null,"ABS 140 Profilkeramik-Rohr mit Muffe L1330mm","103946",1330,null,"STK",{"$f":"VLOOKUP(G1488,sanschie!A:G,7,0)","v":106},{"$f":"ROUNDUP(M1488,0)","v":5},{"$f":"(M1483-O1484-M1489-M1499-M1500-M1506)/1000/1.33","v":4.962406015037593}]
["Absolut",6,1814,"Absolut18146",null,"ABS 180 Fertigfuss DZ 2 x Ø120-180mm L1070mm","103866",1070,null,"STK",{"$f":"VLOOKUP(G1489,sanschie!A:G,7,0)","v":1472},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1489=\"\",0,$H1489*$L1489)","v":1070}]
["Absolut",7,1814,"Absolut18147",null,"ABS 180 Fertigfusspaket ","103891","0",null,"STK",{"$f":"VLOOKUP(G1490,sanschie!A:G,7,0)","v":311},{"$f":"L1489","v":1}]
["Absolut",8,1814,"Absolut18148",null,"ABS 140 Fertigfusspaket ","103889","0",null,"STK",{"$f":"VLOOKUP(G1491,sanschie!A:G,7,0)","v":311},{"$f":"L1489","v":1}]
["Absolut",9,1814,"Absolut18149",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G1492,sanschie!A:G,7,0)","v":18}]
["Absolut",10,1814,"Absolut181410",null,"CHZ 180 Keramik Fuss-Scheibe geschlossen","103700","0",null,"STK",{"$f":"VLOOKUP(G1493,sanschie!A:G,7,0)","v":35},{"$f":"IF(L1489=\"\",1,\"\")","v":""}]
["Absolut",11,1814,"Absolut181411",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G1494,sanschie!A:G,7,0)","v":32},{"$f":"IF(L1489=\"\",1,\"\")","v":""}]
["Absolut",12,1814,"Absolut181412",null,"ABS 180 Rauchrohr-Anschlusspaket 90° RA  ","103983",1330,null,"STK",{"$f":"VLOOKUP(G1495,sanschie!A:G,7,0)","v":386},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""},{"$f":"IF(L1495=0,0,IF(L1495=\"\",0,L1495*H1495))","v":0}]
["Absolut",13,1814,"Absolut181413",null,"ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","103995",1330,null,"STK",{"$f":"VLOOKUP(G1496,sanschie!A:G,7,0)","v":404},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""},{"$f":"IF(L1496=0,0,IF(L1496=\"\",0,L1496*H1496))","v":0}]
["Absolut",14,1814,"Absolut181414",null,"ABS 180  Rauchrohranschluss Stutzen-Set 90° Ø180mm","104001","0",null,"STK",{"$f":"VLOOKUP(G1497,sanschie!A:G,7,0)","v":204}]
["Absolut",15,1814,"Absolut181415",null,"ABS 180 Rauchrohranschluss Stutzen-Set 45°","104007","0",null,"STK",{"$f":"VLOOKUP(G1498,sanschie!A:G,7,0)","v":204}]
["Absolut",16,1814,"Absolut181416",null,"ABS 140 Rauchrohr-Anschlusspaket 90° RA  ","103981",1330,null,"STK",{"$f":"VLOOKUP(G1499,sanschie!A:G,7,0)","v":355},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(L1499=0,0,IF(L1499=\"\",0,L1499*H1499))","v":1330}]
["Absolut",17,1814,"Absolut181417",null,"ABS 140 Rauchrohr-Anschlusspaket 45° RA  ","103993",1330,null,"STK",{"$f":"VLOOKUP(G1500,sanschie!A:G,7,0)","v":355},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(L1500=0,0,IF(L1500=\"\",0,L1500*H1500))","v":0}]
["Absolut",18,1814,"Absolut181418",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø140mm","103999","0",null,"STK",{"$f":"VLOOKUP(G1501,sanschie!A:G,7,0)","v":191}]
["Absolut",19,1814,"Absolut181419",null,"ABS 140 Rauchrohranschluss Stutzen-Set 45°","104005","0",null,"STK",{"$f":"VLOOKUP(G1502,sanschie!A:G,7,0)","v":191},null,null,null,"großer Zug","kleine Zug"]
["Absolut",20,1814,"Absolut181420",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G1503,sanschie!A:G,7,0)","v":160},{"$f":"IF(N1503=0,\"\",N1503)","v":""},null,{"$f":"SUM(O1503:P1503)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",21,1814,"Absolut181421",null,"ABS 200 Steckadapter ","104269","0",null,"STK",{"$f":"VLOOKUP(G1504,sanschie!A:G,7,0)","v":184}]
["Absolut",22,1814,"Absolut181422",null,"ABS 180 Putztür-Anschlusspaket ","103966",1330,null,"STK",{"$f":"VLOOKUP(G1505,sanschie!A:G,7,0)","v":448},{"$f":"IF(N1505=0,\"\",N1505)","v":""},{"$f":"IF(L1505=0,0,IF(L1505=\"\",0,L1505*H1505))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",23,1814,"Absolut181423",null,"ABS 140 Putztür-Anschlusspaket ","103964",1330,null,"STK",{"$f":"VLOOKUP(G1506,sanschie!A:G,7,0)","v":410},{"$f":"IF(N1506=0,\"\",N1506)","v":""},{"$f":"IF(L1506=0,0,IF(L1506=\"\",0,L1506*H1506))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",24,1814,"Absolut181424",null,"ABS 180 Putztüranschluss Stutzen Set","104274","0",null,"STK",{"$f":"VLOOKUP(G1507,sanschie!A:G,7,0)","v":336}]
["Absolut",25,1814,"Absolut181425",null,"ABS 140 Putztüranschluss Stutzen Set","104272","0",null,"STK",{"$f":"VLOOKUP(G1508,sanschie!A:G,7,0)","v":311}]
["Absolut",26,1814,"Absolut181426",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1509,sanschie!A:G,7,0)","v":27}]
["Absolut",27,1814,"Absolut181427",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104192","0",null,"STK",{"$f":"VLOOKUP(G1510,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",28,1814,"Absolut181428",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104195","0",null,"STK",{"$f":"VLOOKUP(G1511,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",29,1814,"Absolut181429",null,"ABS Handyplatte DZ Faserzement 360 x 650mm ","104149","0",null,"STK",{"$f":"VLOOKUP(G1512,sanschie!A:G,7,0)","v":167},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",30,1814,"Absolut181430",null,"ABS Handyplatte DZ Inox 360 x 650mm","104181","0",null,"STK",{"$f":"VLOOKUP(G1513,sanschie!A:G,7,0)","v":229},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",31,1814,"Absolut181431",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1514,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",32,1814,"Absolut181432",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G1515,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",33,1814,"Absolut181433",null,"ABS 180 Abströmkonus verkupfert","104206","0",null,"STK",{"$f":"VLOOKUP(G1516,sanschie!A:G,7,0)","v":174}]
["Absolut",34,1814,"Absolut181434",null,"ABS 140 Abströmkonus verkupfert","104204","0",null,"STK",{"$f":"VLOOKUP(G1517,sanschie!A:G,7,0)","v":161}]
["Absolut",{"$f":"B1517+1","v":35},{"$f":"C1517","v":1814},"Absolut181435",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G1518,sanschie!A:G,7,0)","v":1900}]
["Absolut",36,1814,"Absolut181436",null,"ABS 180 Anschlusskonus DZ mit Doppelfutter DN180mm","103903","0",null,"STK",{"$f":"VLOOKUP(G1519,sanschie!A:G,7,0)","v":260.2}]
["Absolut",37,1814,"Absolut181437",null,"ABS 180 Adapterring von 180mm auf 180mm L90mm","103907","0",null,"STK",{"$f":"VLOOKUP(G1520,sanschie!A:G,7,0)","v":46}]
["Absolut",38,1814,"Absolut181438",null,"ABS 180 Adapterring von 180mm auf 140mm L90mm","103905","0",null,"STK",{"$f":"VLOOKUP(G1521,sanschie!A:G,7,0)","v":35}]
["Absolut",39,1814,"Absolut181439",null,"KER 180  Keranova-Fugenglätter","103474","0",null,"STK",{"$f":"VLOOKUP(G1522,sanschie!A:G,7,0)","v":61}]
["Absolut",40,1814,"Absolut181440",null,"KER 140  Keranova-Fugenglätter","103472","0",null,"STK",{"$f":"VLOOKUP(G1523,sanschie!A:G,7,0)","v":57}]
["Absolut",41,1814,"Absolut181441",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø100mm","104014","0",null,"STK",{"$f":"VLOOKUP(G1524,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",42,1814,"Absolut181442",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm","104015","0",null,"STK",{"$f":"VLOOKUP(G1525,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",43,1814,"Absolut181443",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø130mm","104016","0",null,"STK",{"$f":"VLOOKUP(G1526,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",44,1814,"Absolut181444",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø150mm","104017","0",null,"STK",{"$f":"VLOOKUP(G1527,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",45,1814,"Absolut181445",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø180mm","104018","0",null,"STK",{"$f":"VLOOKUP(G1528,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",46,1814,"Absolut181446",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G1529,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",47,1814,"Absolut181447",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G1530,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",48,1814,"Absolut181448",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G1531,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",49,1814,"Absolut181449",null,"ABS 140 Kondensatfalle zu RA 45° Ø130mm ","104028","0",null,"STK",{"$f":"VLOOKUP(G1532,sanschie!A:G,7,0)","v":297}]
["Absolut",50,1814,"Absolut181450",null,"ABS 180 Kondensatfalle zu RA 45° Ø130mm","104032","0",null,"STK",{"$f":"VLOOKUP(G1533,sanschie!A:G,7,0)","v":347}]
["Absolut",51,1814,"Absolut181451",null,"ABS 180 Kondensatfalle zu RA 45° Ø150mm","104033","0",null,"STK",{"$f":"VLOOKUP(G1534,sanschie!A:G,7,0)","v":347}]
["Absolut",52,1814,"Absolut181452",null,"ABS 180 Kondensatfalle zu RA 45° Ø160mm","104034","0",null,"STK",{"$f":"VLOOKUP(G1535,sanschie!A:G,7,0)","v":347}]
["Absolut",53,1814,"Absolut181453",null,"ABS 180 Kondensatfalle zu RA 45° Ø180mm ","104035","0",null,"STK",{"$f":"VLOOKUP(G1536,sanschie!A:G,7,0)","v":347}]
["Absolut",54,1814,"Absolut181454",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1537,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",55,1814,"Absolut181455",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1538,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",56,1814,"Absolut181456",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1539,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",57,1814,"Absolut181457",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1540,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1490=1,2,\"\")","v":2}]
["Absolut",58,1814,"Absolut181458",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1541,sanschie!A:G,7,0)","v":489},{"$f":"IF(N1541=0,\"\",N1541)","v":""},null,{"$f":"SUM(O1541:P1541)","v":0},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""},{"$f":"IF(Daten!$F$241=1,\"\",1)","v":""}]
["Absolut",59,1814,"Absolut181459",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1542,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",60,1814,"Absolut181460",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1543,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",61,1814,"Absolut181461",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G1544,sanschie!A:G,7,0)","v":14},{"$f":"IF(N1544=0,\"\",ROUNDUP(N1544,0))","v":""},null,{"$f":"SUM(O1544:P1544)","v":0},{"$f":"IF(L1487<=8,0,(L1487-8)/2)","v":0}]
["Absolut",62,1814,"Absolut181462",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G1545,sanschie!A:G,7,0)","v":14},{"$f":"IF(N1545=0,\"\",ROUNDUP(N1545,0))","v":""},null,{"$f":"SUM(O1545:P1545)","v":0},{"$f":"IF(L1488<=8,0,(L1488-8)/2)","v":0}]
["Absolut",63,1814,"Absolut181463",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1546,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1546=0,\"\",N1546)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",64,1814,"Absolut181464",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1547,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1547=0,\"\",N1547)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",65,1814,"Absolut181465",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1548,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",{"$f":"B1548+1","v":66},{"$f":"C1548","v":1814},"Absolut181466",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1549,sanschie!A:G,7,0)","v":35},{"$f":"IF(N1549<=11.5,1,2)","v":1},null,{"$f":"IF(L1489=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",67,1814,{"$f":"A1550&C1550&B1550","v":"Absolut181467"},null,"ABS 180 Basten Standard Inox","104212","0",null,"STK",{"$f":"VLOOKUP(G1550,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",68,1814,"Absolut181468",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",{"$f":"VLOOKUP(G1551,sanschie!A:G,7,0)","v":362},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",69,1814,"Absolut181469",null,"ABS 180 Sairlift Inox","104224","0",null,"STK",{"$f":"VLOOKUP(G1552,sanschie!A:G,7,0)","v":400},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",70,1814,"Absolut181470",null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",{"$f":"VLOOKUP(G1553,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",71,1814,"Absolut181471",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G1554,sanschie!A:G,7,0)","v":123.1}]
["Absolut",72,1814,"Absolut181472",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1555,sanschie!A:G,7,0)","v":258.8}]
["Absolut",73,1814,"Absolut181473",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1556,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",74,1814,"Absolut181474",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1557,sanschie!A:G,7,0)","v":44.9}]
["Absolut",75,1814,"Absolut181475",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1558,sanschie!A:G,7,0)","v":7.5}]
["Absolut",76,1814,"Absolut181476",null,"ZBH 190 Verschlusszapfen 2Stk. aus Schaumstoff","103833","0",null,"STK",{"$f":"VLOOKUP(G1559,sanschie!A:G,7,0)","v":26.5}]
["Absolut",77,1814,"Absolut181477",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G1560,sanschie!A:G,7,0)","v":452}]
["Absolut",78,1814,"Absolut181478",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G1561,sanschie!A:G,7,0)","v":538}]
["Absolut",79,1814,"Absolut181479",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G1562,sanschie!A:G,7,0)","v":634}]
["Absolut",80,1814,"Absolut181480",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G1563,sanschie!A:G,7,0)","v":695}]
["Absolut",81,1814,"Absolut181481",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G1564,sanschie!A:G,7,0)","v":797}]
["Absolut",82,1814,"Absolut181482",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G1565,sanschie!A:G,7,0)","v":873}]
["Absolut",83,1814,"Absolut181483",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1566,sanschie!A:G,7,0)","v":13.8}]
["Absolut",84,1814,"Absolut181484",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1567,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",85,1814,"Absolut181485",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1568,sanschie!A:G,7,0)","v":322}]
["Absolut",86,1814,"Absolut181486",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1569,sanschie!A:G,7,0)","v":26}]
["Absolut",87,1814,"Absolut181487",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1570,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,1816,{"$f":"A1571&C1571&B1571","v":"Absolut18160"},"P","Absolut-Kaminanlage Ø 1816","Absolut 1816","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1571,sanschie!A:G,7,0)","v":0},null,{"$f":"I1571*1000","v":9000}]
["Absolut",{"$f":"B1571+1","v":1},{"$f":"C1571","v":1816},{"$f":"A1572&C1572&B1572","v":"Absolut18161"},null,"ABS Mantelstein DZ 360 x 650mm L330mm","103925","0",null,"STK",{"$f":"VLOOKUP(G1572,sanschie!A:G,7,0)","v":51},{"$f":"ROUND(M1572,0)-M1573","v":24},{"$f":"((M1571-M1577)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1572*330","v":0}]
["Absolut",{"$f":"B1572+1","v":2},{"$f":"C1572","v":1816},{"$f":"A1573&C1573&B1573","v":"Absolut18162"},null,"ABS Thermo-Trennstein DZ 360 x 650mm L330mm","103937","0",null,"STK",{"$f":"VLOOKUP(G1573,sanschie!A:G,7,0)","v":259},{"$f":"IF(M1573=0,\"\",M1573)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,1816,"Absolut18163",null,"ABS Thermo-Fussplatte DZ 360 x 650mm","103855","0",null,"STK",{"$f":"VLOOKUP(G1574,sanschie!A:G,7,0)","v":198}]
["Absolut",4,1816,"Absolut18164",null,"ABS 180 Profilkeramik-Rohr mit Muffe L1330mm","103948",1330,null,"STK",{"$f":"VLOOKUP(G1575,sanschie!A:G,7,0)","v":122},{"$f":"ROUNDUP(M1575,0)","v":6},{"$f":"(M1571-O1572-M1577-M1583-M1584-M1592)/1000/1.33","v":5.962406015037593}]
["Absolut",5,1816,"Absolut18165",null,"ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","103947",1330,null,"STK",{"$f":"VLOOKUP(G1576,sanschie!A:G,7,0)","v":113},{"$f":"ROUNDUP(M1576,0)","v":5},{"$f":"(M1571-O1572-M1577-M1587-M1588-M1593)/1000/1.33","v":4.962406015037593}]
["Absolut",6,1816,"Absolut18166",null,"ABS 180 Fertigfuss DZ 2 x Ø120-180mm L1070mm","103866",1070,null,"STK",{"$f":"VLOOKUP(G1577,sanschie!A:G,7,0)","v":1472},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1577=\"\",0,$H1577*$L1577)","v":1070}]
["Absolut",7,1816,"Absolut18167",null,"ABS 180 Fertigfusspaket ","103891","0",null,"STK",{"$f":"VLOOKUP(G1578,sanschie!A:G,7,0)","v":311},{"$f":"L1577","v":1}]
["Absolut",8,1816,"Absolut18168",null,"ABS 160 Fertigfusspaket ","103890","0",null,"STK",{"$f":"VLOOKUP(G1579,sanschie!A:G,7,0)","v":311},{"$f":"L1577","v":1}]
["Absolut",9,1816,"Absolut18169",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G1580,sanschie!A:G,7,0)","v":18}]
["Absolut",10,1816,"Absolut181610",null,"CHZ 180 Keramik Fuss-Scheibe geschlossen","103700","0",null,"STK",{"$f":"VLOOKUP(G1581,sanschie!A:G,7,0)","v":35},{"$f":"IF(L1577=\"\",1,\"\")","v":""}]
["Absolut",11,1816,"Absolut181611",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G1582,sanschie!A:G,7,0)","v":32},{"$f":"IF(L1577=\"\",1,\"\")","v":""}]
["Absolut",12,1816,"Absolut181612",null,"ABS 180 Rauchrohr-Anschlusspaket 90° RA  ","103983",1330,null,"STK",{"$f":"VLOOKUP(G1583,sanschie!A:G,7,0)","v":386},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""},{"$f":"IF(L1583=0,0,IF(L1583=\"\",0,L1583*H1583))","v":0}]
["Absolut",13,1816,"Absolut181613",null,"ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","103995",1330,null,"STK",{"$f":"VLOOKUP(G1584,sanschie!A:G,7,0)","v":404},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""},{"$f":"IF(L1584=0,0,IF(L1584=\"\",0,L1584*H1584))","v":0}]
["Absolut",14,1816,"Absolut181614",null,"ABS 180  Rauchrohranschluss Stutzen-Set 90° Ø180mm","104001","0",null,"STK",{"$f":"VLOOKUP(G1585,sanschie!A:G,7,0)","v":204}]
["Absolut",15,1816,"Absolut181615",null,"ABS 180 Rauchrohranschluss Stutzen-Set 45°","104007","0",null,"STK",{"$f":"VLOOKUP(G1586,sanschie!A:G,7,0)","v":204}]
["Absolut",16,1816,"Absolut181616",null,"ABS 160 Rauchrohr-Anschlusspaket 90° RA  ","103982",1330,null,"STK",{"$f":"VLOOKUP(G1587,sanschie!A:G,7,0)","v":367},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(L1587=0,0,IF(L1587=\"\",0,L1587*H1587))","v":1330}]
["Absolut",17,1816,"Absolut181617",null,"ABS 160 Rauchrohr-Anschlusspaket 45° RA  ","103994",1330,null,"STK",{"$f":"VLOOKUP(G1588,sanschie!A:G,7,0)","v":367},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(L1588=0,0,IF(L1588=\"\",0,L1588*H1588))","v":0}]
["Absolut",18,1816,"Absolut181618",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø160mm","104000","0",null,"STK",{"$f":"VLOOKUP(G1589,sanschie!A:G,7,0)","v":199}]
["Absolut",19,1816,"Absolut181619",null,"ABS 160 Rauchrohranschluss Stutzen-Set 45°","104006","0",null,"STK",{"$f":"VLOOKUP(G1590,sanschie!A:G,7,0)","v":199},null,null,null,"großer Zug","kleiner Zug"]
["Absolut",20,1816,"Absolut181620",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G1591,sanschie!A:G,7,0)","v":160},{"$f":"IF(N1591=0,\"\",N1591)","v":""},null,{"$f":"SUM(O1591:P1591)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",21,1816,"Absolut181621",null,"ABS 180 Putztür-Anschlusspaket ","103966",1330,null,"STK",{"$f":"VLOOKUP(G1592,sanschie!A:G,7,0)","v":448},{"$f":"IF(N1592=0,\"\",N1592)","v":""},{"$f":"IF(L1592=0,0,IF(L1592=\"\",0,L1592*H1592))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",22,1816,"Absolut181622",null,"ABS 160 Putztür-Anschlusspaket ","103965",1330,null,"STK",{"$f":"VLOOKUP(G1593,sanschie!A:G,7,0)","v":428},{"$f":"IF(N1593=0,\"\",N1593)","v":""},{"$f":"IF(L1593=0,0,IF(L1593=\"\",0,L1593*H1593))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",23,1816,"Absolut181623",null,"ABS 180 Putztüranschluss Stutzen Set","104274","0",null,"STK",{"$f":"VLOOKUP(G1594,sanschie!A:G,7,0)","v":336}]
["Absolut",24,1816,"Absolut181624",null,"ABS 160 Putztüranschluss Stutzen Set","104273","0",null,"STK",{"$f":"VLOOKUP(G1595,sanschie!A:G,7,0)","v":325}]
["Absolut",25,1816,"Absolut181625",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1596,sanschie!A:G,7,0)","v":27}]
["Absolut",26,1816,"Absolut181626",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104192","0",null,"STK",{"$f":"VLOOKUP(G1597,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",27,1816,"Absolut181627",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104195","0",null,"STK",{"$f":"VLOOKUP(G1598,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",28,1816,"Absolut181628",null,"ABS Handyplatte DZ Faserzement 360 x 650mm ","104149","0",null,"STK",{"$f":"VLOOKUP(G1599,sanschie!A:G,7,0)","v":167},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",29,1816,"Absolut181629",null,"ABS Handyplatte DZ Inox 360 x 650mm","104181","0",null,"STK",{"$f":"VLOOKUP(G1600,sanschie!A:G,7,0)","v":229},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",30,1816,"Absolut181630",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1601,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",31,1816,"Absolut181631",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G1602,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",32,1816,"Absolut181632",null,"ABS 180 Abströmkonus verkupfert","104206","0",null,"STK",{"$f":"VLOOKUP(G1603,sanschie!A:G,7,0)","v":174}]
["Absolut",33,1816,"Absolut181633",null,"ABS 160 Abströmkonus verkupfert","104205","0",null,"STK",{"$f":"VLOOKUP(G1604,sanschie!A:G,7,0)","v":166}]
["Absolut",{"$f":"B1604+1","v":34},{"$f":"C1604","v":1816},"Absolut181634",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G1605,sanschie!A:G,7,0)","v":1900}]
["Absolut",35,1816,"Absolut181635",null,"ABS 180 Anschlusskonus DZ mit Doppelfutter DN180mm","103903","0",null,"STK",{"$f":"VLOOKUP(G1606,sanschie!A:G,7,0)","v":260.2}]
["Absolut",36,1816,"Absolut181636",null,"ABS 180 Adapterring von 180mm auf 180mm L90mm","103907","0",null,"STK",{"$f":"VLOOKUP(G1607,sanschie!A:G,7,0)","v":46}]
["Absolut",37,1816,"Absolut181637",null,"ABS 180 Adapterring von 180mm auf 160mm L90mm","103906","0",null,"STK",{"$f":"VLOOKUP(G1608,sanschie!A:G,7,0)","v":41}]
["Absolut",38,1816,"Absolut181638",null,"KER 180  Keranova-Fugenglätter","103474","0",null,"STK",{"$f":"VLOOKUP(G1609,sanschie!A:G,7,0)","v":61}]
["Absolut",39,1816,"Absolut181639",null,"KER 160  Keranova-Fugenglätter","103473","0",null,"STK",{"$f":"VLOOKUP(G1610,sanschie!A:G,7,0)","v":58}]
["Absolut",40,1816,"Absolut181640",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø100mm","104014","0",null,"STK",{"$f":"VLOOKUP(G1611,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",41,1816,"Absolut181641",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm","104015","0",null,"STK",{"$f":"VLOOKUP(G1612,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",42,1816,"Absolut181642",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø130mm","104016","0",null,"STK",{"$f":"VLOOKUP(G1613,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",43,1816,"Absolut181643",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø150mm","104017","0",null,"STK",{"$f":"VLOOKUP(G1614,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",44,1816,"Absolut181644",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø180mm","104018","0",null,"STK",{"$f":"VLOOKUP(G1615,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",45,1816,"Absolut181645",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G1616,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",46,1816,"Absolut181646",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G1617,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",47,1816,"Absolut181647",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G1618,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",48,1816,"Absolut181648",null,"CHZ 150 Doppelfutter lose L150mm","103803","0",null,"STK",{"$f":"VLOOKUP(G1619,sanschie!A:G,7,0)","v":103},{"$f":"IF(Daten!$F$226=6,1,\"\")","v":""}]
["Absolut",49,1816,"Absolut181649",null,"ABS 180 Kondensatfalle zu RA 45° Ø130mm","104032","0",null,"STK",{"$f":"VLOOKUP(G1620,sanschie!A:G,7,0)","v":347}]
["Absolut",50,1816,"Absolut181650",null,"ABS 180 Kondensatfalle zu RA 45° Ø150mm","104033","0",null,"STK",{"$f":"VLOOKUP(G1621,sanschie!A:G,7,0)","v":347}]
["Absolut",51,1816,"Absolut181651",null,"ABS 180 Kondensatfalle zu RA 45° Ø160mm","104034","0",null,"STK",{"$f":"VLOOKUP(G1622,sanschie!A:G,7,0)","v":347}]
["Absolut",52,1816,"Absolut181652",null,"ABS 180 Kondensatfalle zu RA 45° Ø180mm ","104035","0",null,"STK",{"$f":"VLOOKUP(G1623,sanschie!A:G,7,0)","v":347}]
["Absolut",53,1816,"Absolut181653",null,"ABS 160 Kondensatfalle zu RA 45° Ø130mm ","104029","0",null,"STK",{"$f":"VLOOKUP(G1624,sanschie!A:G,7,0)","v":322}]
["Absolut",54,1816,"Absolut181654",null,"ABS 160 Kondensatfalle zu RA 45° Ø150mm ","104030","0",null,"STK",{"$f":"VLOOKUP(G1625,sanschie!A:G,7,0)","v":322}]
["Absolut",55,1816,"Absolut181655",null,"ABS 160 Kondensatfalle zu RA 45° Ø160mm ","104031","0",null,"STK",{"$f":"VLOOKUP(G1626,sanschie!A:G,7,0)","v":322}]
["Absolut",56,1816,"Absolut181656",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1627,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",57,1816,"Absolut181657",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1628,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",58,1816,"Absolut181658",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1629,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",59,1816,"Absolut181659",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1630,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1578=1,2,\"\")","v":2}]
["Absolut",60,1816,"Absolut181660",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1631,sanschie!A:G,7,0)","v":489},{"$f":"IF(N1631=0,\"\",N1631)","v":""},null,{"$f":"SUM(O1631:P1631)","v":0},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""},{"$f":"IF(Daten!$F$241=1,\"\",1)","v":""}]
["Absolut",61,1816,"Absolut181661",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1632,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",62,1816,"Absolut181662",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1633,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",63,1816,"Absolut181663",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G1634,sanschie!A:G,7,0)","v":14},{"$f":"IF(N1634=0,\"\",ROUNDUP(N1634,0))","v":""},null,{"$f":"SUM(O1634:P1634)","v":0},{"$f":"IF(L1575<=8,0,(L1575-8)/2)","v":0}]
["Absolut",64,1816,"Absolut181664",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G1635,sanschie!A:G,7,0)","v":14},{"$f":"IF(N1635=0,\"\",ROUNDUP(N1635,0))","v":""},null,{"$f":"SUM(O1635:P1635)","v":0},{"$f":"IF(L1576<=8,0,(L1576-8)/2)","v":0}]
["Absolut",65,1816,"Absolut181665",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1636,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1636=0,\"\",N1636)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",{"$f":"B1636+1","v":66},{"$f":"C1636","v":1816},"Absolut181666",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1637,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1637=0,\"\",N1637)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",67,1816,{"$f":"A1638&C1638&B1638","v":"Absolut181667"},null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1638,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",68,1816,"Absolut181668",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1639,sanschie!A:G,7,0)","v":35},{"$f":"IF(N1639<=11.5,1,2)","v":1},null,{"$f":"IF(L1577=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",69,1816,"Absolut181669",null,"ABS 180 Basten Standard Inox","104212","0",null,"STK",{"$f":"VLOOKUP(G1640,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",70,1816,"Absolut181670",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",{"$f":"VLOOKUP(G1641,sanschie!A:G,7,0)","v":362},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",71,1816,"Absolut181671",null,"ABS 180 Sairlift Inox","104224","0",null,"STK",{"$f":"VLOOKUP(G1642,sanschie!A:G,7,0)","v":400},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",72,1816,"Absolut181672",null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",{"$f":"VLOOKUP(G1643,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",73,1816,"Absolut181673",null,"ABS 160 Basten Standard Inox","104211","0",null,"STK",{"$f":"VLOOKUP(G1644,sanschie!A:G,7,0)","v":323},{"$f":"IF(Daten!$F$297=2,1,\"\")","v":""}]
["Absolut",74,1816,"Absolut181674",null,"ABS 160 Basten Standard Kupfer","104217","0",null,"STK",{"$f":"VLOOKUP(G1645,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$F$297=3,1,\"\")","v":""}]
["Absolut",75,1816,"Absolut181675",null,"ABS 160 Sairlift Inox","104223","0",null,"STK",{"$f":"VLOOKUP(G1646,sanschie!A:G,7,0)","v":374},{"$f":"IF(Daten!$F$297=4,1,\"\")","v":""}]
["Absolut",76,1816,"Absolut181676",null,"ABS 160 Sairlift Kupfer","104228","0",null,"STK",{"$f":"VLOOKUP(G1647,sanschie!A:G,7,0)","v":397},{"$f":"IF(Daten!$F$297=5,1,\"\")","v":""}]
["Absolut",77,1816,"Absolut181677",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G1648,sanschie!A:G,7,0)","v":123.1}]
["Absolut",78,1816,"Absolut181678",null,"ZBH 150 Verschlussbüchse weiss ØA 275mm","103836","0",null,"STK",{"$f":"VLOOKUP(G1649,sanschie!A:G,7,0)","v":115}]
["Absolut",79,1816,"Absolut181679",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1650,sanschie!A:G,7,0)","v":258.8}]
["Absolut",80,1816,"Absolut181680",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1651,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",81,1816,"Absolut181681",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1652,sanschie!A:G,7,0)","v":44.9}]
["Absolut",82,1816,"Absolut181682",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1653,sanschie!A:G,7,0)","v":7.5}]
["Absolut",83,1816,"Absolut181683",null,"ZBH 190 Verschlusszapfen 2Stk. aus Schaumstoff","103833","0",null,"STK",{"$f":"VLOOKUP(G1654,sanschie!A:G,7,0)","v":26.5}]
["Absolut",84,1816,"Absolut181684",null,"ZBH 170 Verschlusszapfen 2Stk. aus Schaumstoff","103832","0",null,"STK",{"$f":"VLOOKUP(G1655,sanschie!A:G,7,0)","v":24.2}]
["Absolut",85,1816,"Absolut181685",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G1656,sanschie!A:G,7,0)","v":452}]
["Absolut",86,1816,"Absolut181686",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G1657,sanschie!A:G,7,0)","v":538}]
["Absolut",87,1816,"Absolut181687",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G1658,sanschie!A:G,7,0)","v":634}]
["Absolut",88,1816,"Absolut181688",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G1659,sanschie!A:G,7,0)","v":695}]
["Absolut",89,1816,"Absolut181689",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G1660,sanschie!A:G,7,0)","v":797}]
["Absolut",90,1816,"Absolut181690",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G1661,sanschie!A:G,7,0)","v":873}]
["Absolut",91,1816,"Absolut181691",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1662,sanschie!A:G,7,0)","v":13.8}]
["Absolut",92,1816,"Absolut181692",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1663,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",93,1816,"Absolut181693",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1664,sanschie!A:G,7,0)","v":322}]
["Absolut",94,1816,"Absolut181694",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1665,sanschie!A:G,7,0)","v":26}]
["Absolut",95,1816,"Absolut181695",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1666,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,2014,{"$f":"A1667&C1667&B1667","v":"Absolut20140"},"P","Absolut-Kaminanlage Ø 2014","Absolut 2014","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1667,sanschie!A:G,7,0)","v":0},null,{"$f":"I1667*1000","v":9000}]
["Absolut",{"$f":"B1667+1","v":1},{"$f":"C1667","v":2014},{"$f":"A1668&C1668&B1668","v":"Absolut20141"},null,"ABS Mantelstein DZ 380 x 710mm L330mm","103926","0",null,"STK",{"$f":"VLOOKUP(G1668,sanschie!A:G,7,0)","v":56},{"$f":"ROUND(M1668,0)-M1669","v":24},{"$f":"((M1667-M1673)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1668*330","v":0}]
["Absolut",{"$f":"B1668+1","v":2},{"$f":"C1668","v":2014},{"$f":"A1669&C1669&B1669","v":"Absolut20142"},null,"ABS Thermo-Trennstein DZ 380 x 710mm L330mm","103938","0",null,"STK",{"$f":"VLOOKUP(G1669,sanschie!A:G,7,0)","v":283},{"$f":"IF(M1669=0,\"\",M1669)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,2014,"Absolut20143",null,"ABS Thermo-Fussplatte DZ 380 x 710mm","103857","0",null,"STK",{"$f":"VLOOKUP(G1670,sanschie!A:G,7,0)","v":210}]
["Absolut",4,2014,"Absolut20144",null,"ABS 200 Profilkeramik-Rohr mit Muffe L1330mm","103949",1330,null,"STK",{"$f":"VLOOKUP(G1671,sanschie!A:G,7,0)","v":145},{"$f":"ROUNDUP(M1671,0)","v":6},{"$f":"(M1667-O1668-M1673-M1679-M1680-M1689)/1000/1.33","v":5.962406015037593}]
["Absolut",5,2014,"Absolut20145",null,"ABS 140 Profilkeramik-Rohr mit Muffe L1330mm","103946",1330,null,"STK",{"$f":"VLOOKUP(G1672,sanschie!A:G,7,0)","v":106},{"$f":"ROUNDUP(M1672,0)","v":5},{"$f":"(M1667-O1668-M1673-M1683-M1684-M1690)/1000/1.33","v":4.962406015037593}]
["Absolut",6,2014,"Absolut20146",null,"ABS 200 Fertigfuss DZ 2 x Ø200mm L1070mm","103867",1070,null,"STK",{"$f":"VLOOKUP(G1673,sanschie!A:G,7,0)","v":1476},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1673=\"\",0,$H1673*$L1673)","v":1070}]
["Absolut",7,2014,"Absolut20147",null,"ABS 200 Fertigfusspaket ","103892","0",null,"STK",{"$f":"VLOOKUP(G1674,sanschie!A:G,7,0)","v":311},{"$f":"L1673","v":1}]
["Absolut",8,2014,"Absolut20148",null,"ABS 140 Fertigfusspaket ","103889","0",null,"STK",{"$f":"VLOOKUP(G1675,sanschie!A:G,7,0)","v":311},{"$f":"L1673","v":1}]
["Absolut",9,2014,"Absolut20149",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G1676,sanschie!A:G,7,0)","v":18}]
["Absolut",10,2014,"Absolut201410",null,"CHZ 200 Keramik Fuss-Scheibe geschlossen","103701","0",null,"STK",{"$f":"VLOOKUP(G1677,sanschie!A:G,7,0)","v":45},{"$f":"IF(L1673=\"\",1,\"\")","v":""}]
["Absolut",11,2014,"Absolut201411",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G1678,sanschie!A:G,7,0)","v":32},{"$f":"IF(L1673=\"\",1,\"\")","v":""}]
["Absolut",12,2014,"Absolut201412",null,"ABS 200 Rauchrohr-Anschlusspaket 90° RA  ","103984",1330,null,"STK",{"$f":"VLOOKUP(G1679,sanschie!A:G,7,0)","v":434},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""},{"$f":"IF(L1679=0,0,IF(L1679=\"\",0,L1679*H1679))","v":0}]
["Absolut",13,2014,"Absolut201413",null,"ABS 200 Rauchrohr-Anschlusspaket 45° RA  ","103996",1330,null,"STK",{"$f":"VLOOKUP(G1680,sanschie!A:G,7,0)","v":466},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""},{"$f":"IF(L1680=0,0,IF(L1680=\"\",0,L1680*H1680))","v":0}]
["Absolut",14,2014,"Absolut201414",null,"ABS 200 Rauchrohranschluss Stutzen-Set 90° Ø200mm","104002","0",null,"STK",{"$f":"VLOOKUP(G1681,sanschie!A:G,7,0)","v":212}]
["Absolut",15,2014,"Absolut201415",null,"ABS 200 Rauchrohranschluss Stutzen-Set 45°","104008","0",null,"STK",{"$f":"VLOOKUP(G1682,sanschie!A:G,7,0)","v":212}]
["Absolut",16,2014,"Absolut201416",null,"ABS 140 Rauchrohr-Anschlusspaket 90° RA  ","103981",1330,null,"STK",{"$f":"VLOOKUP(G1683,sanschie!A:G,7,0)","v":355},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(L1683=0,0,IF(L1683=\"\",0,L1683*H1683))","v":1330}]
["Absolut",17,2014,"Absolut201417",null,"ABS 140 Rauchrohr-Anschlusspaket 45° RA  ","103993",1330,null,"STK",{"$f":"VLOOKUP(G1684,sanschie!A:G,7,0)","v":355},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(L1684=0,0,IF(L1684=\"\",0,L1684*H1684))","v":0}]
["Absolut",18,2014,"Absolut201418",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø140mm","103999","0",null,"STK",{"$f":"VLOOKUP(G1685,sanschie!A:G,7,0)","v":191}]
["Absolut",19,2014,"Absolut201419",null,"ABS 140 Rauchrohranschluss Stutzen-Set 45°","104005","0",null,"STK",{"$f":"VLOOKUP(G1686,sanschie!A:G,7,0)","v":191},null,null,null,"großer Zug","kleine Zug"]
["Absolut",20,2014,"Absolut201420",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G1687,sanschie!A:G,7,0)","v":160},{"$f":"IF(N1687=0,\"\",N1687)","v":""},null,{"$f":"SUM(O1687:P1687)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",21,2014,"Absolut201421",null,"ABS 200 Steckadapter ","104269","0",null,"STK",{"$f":"VLOOKUP(G1688,sanschie!A:G,7,0)","v":184}]
["Absolut",22,2014,"Absolut201422",null,"ABS 200 Putztür-Anschlusspaket ","103967",1330,null,"STK",{"$f":"VLOOKUP(G1689,sanschie!A:G,7,0)","v":483},{"$f":"IF(N1689=0,\"\",N1689)","v":""},{"$f":"IF(L1689=0,0,IF(L1689=\"\",0,L1689*H1689))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",23,2014,"Absolut201423",null,"ABS 140 Putztür-Anschlusspaket ","103964",1330,null,"STK",{"$f":"VLOOKUP(G1690,sanschie!A:G,7,0)","v":410},{"$f":"IF(N1690=0,\"\",N1690)","v":""},{"$f":"IF(L1690=0,0,IF(L1690=\"\",0,L1690*H1690))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",24,2014,"Absolut201424",null,"ABS 200 Putztüranschluss Stutzen Set","104275","0",null,"STK",{"$f":"VLOOKUP(G1691,sanschie!A:G,7,0)","v":349}]
["Absolut",25,2014,"Absolut201425",null,"ABS 140 Putztüranschluss Stutzen Set","104272","0",null,"STK",{"$f":"VLOOKUP(G1692,sanschie!A:G,7,0)","v":311}]
["Absolut",26,2014,"Absolut201426",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1693,sanschie!A:G,7,0)","v":27}]
["Absolut",27,2014,"Absolut201427",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104192","0",null,"STK",{"$f":"VLOOKUP(G1694,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",28,2014,"Absolut201428",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104195","0",null,"STK",{"$f":"VLOOKUP(G1695,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",29,2014,"Absolut201429",null,"ABS Handyplatte DZ Faserzement 380 x 710mm  ","104152","0",null,"STK",{"$f":"VLOOKUP(G1696,sanschie!A:G,7,0)","v":180},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",30,2014,"Absolut201430",null,"ABS Handyplatte DZ Inox 380 x 710mm","104182","0",null,"STK",{"$f":"VLOOKUP(G1697,sanschie!A:G,7,0)","v":241},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",31,2014,"Absolut201431",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1698,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",32,2014,"Absolut201432",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G1699,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",33,2014,"Absolut201433",null,"ABS 200 Abströmkonus verkupfert","104207","0",null,"STK",{"$f":"VLOOKUP(G1700,sanschie!A:G,7,0)","v":197}]
["Absolut",34,2014,"Absolut201434",null,"ABS 140 Abströmkonus verkupfert","104204","0",null,"STK",{"$f":"VLOOKUP(G1701,sanschie!A:G,7,0)","v":161}]
["Absolut",{"$f":"B1701+1","v":35},{"$f":"C1701","v":2014},"Absolut201435",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G1702,sanschie!A:G,7,0)","v":1900}]
["Absolut",36,2014,"Absolut201436",null,"ABS 200 Anschlusskonus DZ mit Doppelfutter DN200mm","103904","0",null,"STK",{"$f":"VLOOKUP(G1703,sanschie!A:G,7,0)","v":272.89999999999998}]
["Absolut",37,2014,"Absolut201437",null,"ABS 200 Adapterring von 200mm auf 200mm L90mm","103909","0",null,"STK",{"$f":"VLOOKUP(G1704,sanschie!A:G,7,0)","v":65}]
["Absolut",38,2014,"Absolut201438",null,"ABS 180 Adapterring von 180mm auf 140mm L90mm","103905","0",null,"STK",{"$f":"VLOOKUP(G1705,sanschie!A:G,7,0)","v":35}]
["Absolut",39,2014,"Absolut201439",null,"KER 200  Keranova-Fugenglätter","103475","0",null,"STK",{"$f":"VLOOKUP(G1706,sanschie!A:G,7,0)","v":72}]
["Absolut",40,2014,"Absolut201440",null,"KER 140  Keranova-Fugenglätter","103472","0",null,"STK",{"$f":"VLOOKUP(G1707,sanschie!A:G,7,0)","v":57}]
["Absolut",41,2014,"Absolut201441",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø100mm","104019","0",null,"STK",{"$f":"VLOOKUP(G1708,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",42,2014,"Absolut201442",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø120mm","104020","0",null,"STK",{"$f":"VLOOKUP(G1709,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",43,2014,"Absolut201443",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø130mm","104021","0",null,"STK",{"$f":"VLOOKUP(G1710,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",44,2014,"Absolut201444",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø150mm","104022","0",null,"STK",{"$f":"VLOOKUP(G1711,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",45,2014,"Absolut201445",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø180mm","104023","0",null,"STK",{"$f":"VLOOKUP(G1712,sanschie!A:G,7,0)","v":210},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",46,2014,"Absolut201446",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø200mm","104024","0",null,"STK",{"$f":"VLOOKUP(G1713,sanschie!A:G,7,0)","v":222},{"$f":"IF(Daten!$B$226=8,1,\"\")","v":""}]
["Absolut",47,2014,"Absolut201447",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G1714,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",48,2014,"Absolut201448",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G1715,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",49,2014,"Absolut201449",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G1716,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",50,2014,"Absolut201450",null,"ABS 200 Kondensatfalle zu RA 45° Ø130mm ","104036","0",null,"STK",{"$f":"VLOOKUP(G1717,sanschie!A:G,7,0)","v":365}]
["Absolut",51,2014,"Absolut201451",null,"ABS 200 Kondensatfalle zu RA 45° Ø150mm ","104037","0",null,"STK",{"$f":"VLOOKUP(G1718,sanschie!A:G,7,0)","v":365}]
["Absolut",52,2014,"Absolut201452",null,"ABS 200 Kondensatfalle zu RA 45° Ø160mm","104038","0",null,"STK",{"$f":"VLOOKUP(G1719,sanschie!A:G,7,0)","v":365}]
["Absolut",53,2014,"Absolut201453",null,"ABS 200 Kondensatfalle zu RA 45° Ø180mm ","104039","0",null,"STK",{"$f":"VLOOKUP(G1720,sanschie!A:G,7,0)","v":365}]
["Absolut",54,2014,"Absolut201454",null,"ABS 200 Kondensatfalle zu RA 45° Ø200mm ","104040","0",null,"STK",{"$f":"VLOOKUP(G1721,sanschie!A:G,7,0)","v":365}]
["Absolut",55,2014,"Absolut201455",null,"ABS 140 Kondensatfalle zu RA 45° Ø130mm ","104028","0",null,"STK",{"$f":"VLOOKUP(G1722,sanschie!A:G,7,0)","v":297}]
["Absolut",56,2014,"Absolut201456",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1723,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",57,2014,"Absolut201457",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1724,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",58,2014,"Absolut201458",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1725,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",59,2014,"Absolut201459",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1726,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1674=1,2,\"\")","v":2}]
["Absolut",60,2014,"Absolut201460",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1727,sanschie!A:G,7,0)","v":489},{"$f":"IF(N1727=0,\"\",N1727)","v":""},null,{"$f":"SUM(O1727:P1727)","v":0},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""},{"$f":"IF(Daten!$F$241=1,\"\",1)","v":""}]
["Absolut",61,2014,"Absolut201461",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1728,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",62,2014,"Absolut201462",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1729,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",63,2014,"Absolut201463",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G1730,sanschie!A:G,7,0)","v":14},{"$f":"IF(N1730=0,\"\",ROUNDUP(N1730,0))","v":""},null,{"$f":"SUM(O1730:P1730)","v":0},{"$f":"IF(L1671<=8,0,(L1671-8)/2)","v":0}]
["Absolut",64,2014,"Absolut201464",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G1731,sanschie!A:G,7,0)","v":14},{"$f":"IF(N1731=0,\"\",ROUNDUP(N1731,0))","v":""},null,{"$f":"SUM(O1731:P1731)","v":0},{"$f":"IF(L1672<=8,0,(L1672-8)/2)","v":0}]
["Absolut",65,2014,"Absolut201465",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1732,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1732=0,\"\",N1732)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",{"$f":"B1732+1","v":66},{"$f":"C1732","v":2014},"Absolut201466",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1733,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1733=0,\"\",N1733)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",67,2014,{"$f":"A1734&C1734&B1734","v":"Absolut201467"},null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1734,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",68,2014,"Absolut201468",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1735,sanschie!A:G,7,0)","v":35},{"$f":"IF(N1735<=11.5,1,2)","v":1},null,{"$f":"IF(L1673=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",69,2014,"Absolut201469",null,"ABS 200 Basten Standard Inox","104213","0",null,"STK",{"$f":"VLOOKUP(G1736,sanschie!A:G,7,0)","v":361},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",70,2014,"Absolut201470",null,"ABS 200 Basten Standard Kupfer","104219","0",null,"STK",{"$f":"VLOOKUP(G1737,sanschie!A:G,7,0)","v":375},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",71,2014,"Absolut201471",null,"ABS 200 Sairlift Inox","104225","0",null,"STK",{"$f":"VLOOKUP(G1738,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",72,2014,"Absolut201472",null,"ABS 200 Sairlift Kupfer","104230","0",null,"STK",{"$f":"VLOOKUP(G1739,sanschie!A:G,7,0)","v":434},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",73,2014,"Absolut201473",null,"ABS 180 Basten Standard Inox","104212","0",null,"STK",{"$f":"VLOOKUP(G1740,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$F$297=2,1,\"\")","v":""}]
["Absolut",74,2014,"Absolut201474",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",{"$f":"VLOOKUP(G1741,sanschie!A:G,7,0)","v":362},{"$f":"IF(Daten!$F$297=3,1,\"\")","v":""}]
["Absolut",75,2014,"Absolut201475",null,"ABS 180 Sairlift Inox","104224","0",null,"STK",{"$f":"VLOOKUP(G1742,sanschie!A:G,7,0)","v":400},{"$f":"IF(Daten!$F$297=4,1,\"\")","v":""}]
["Absolut",76,2014,"Absolut201476",null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",{"$f":"VLOOKUP(G1743,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$F$297=5,1,\"\")","v":""}]
["Absolut",77,2014,"Absolut201477",null,"ZBH 200 Verschlussbüchse weiss ØA 300mm","103839","0",null,"STK",{"$f":"VLOOKUP(G1744,sanschie!A:G,7,0)","v":123.1}]
["Absolut",78,2014,"Absolut201478",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G1745,sanschie!A:G,7,0)","v":123.1}]
["Absolut",79,2014,"Absolut201479",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1746,sanschie!A:G,7,0)","v":258.8}]
["Absolut",80,2014,"Absolut201480",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1747,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",81,2014,"Absolut201481",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1748,sanschie!A:G,7,0)","v":44.9}]
["Absolut",82,2014,"Absolut201482",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1749,sanschie!A:G,7,0)","v":7.5}]
["Absolut",83,2014,"Absolut201483",null,"ZBH 210 Verschlusszapfen 2Stk. aus Schaumstoff","103834","0",null,"STK",{"$f":"VLOOKUP(G1750,sanschie!A:G,7,0)","v":26.5}]
["Absolut",84,2014,"Absolut201484",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G1751,sanschie!A:G,7,0)","v":452}]
["Absolut",85,2014,"Absolut201485",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G1752,sanschie!A:G,7,0)","v":538}]
["Absolut",86,2014,"Absolut201486",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G1753,sanschie!A:G,7,0)","v":634}]
["Absolut",87,2014,"Absolut201487",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G1754,sanschie!A:G,7,0)","v":695}]
["Absolut",88,2014,"Absolut201488",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G1755,sanschie!A:G,7,0)","v":797}]
["Absolut",89,2014,"Absolut201489",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G1756,sanschie!A:G,7,0)","v":873}]
["Absolut",90,2014,"Absolut201490",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1757,sanschie!A:G,7,0)","v":13.8}]
["Absolut",91,2014,"Absolut201491",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1758,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",92,2014,"Absolut201492",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1759,sanschie!A:G,7,0)","v":322}]
["Absolut",93,2014,"Absolut201493",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1760,sanschie!A:G,7,0)","v":26}]
["Absolut",94,2014,"Absolut201494",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1761,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,2016,{"$f":"A1762&C1762&B1762","v":"Absolut20160"},"P","Absolut-Kaminanlage Ø 2016","Absolut 2016","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1762,sanschie!A:G,7,0)","v":0},null,{"$f":"I1762*1000","v":9000}]
["Absolut",{"$f":"B1762+1","v":1},{"$f":"C1762","v":2016},{"$f":"A1763&C1763&B1763","v":"Absolut20161"},null,"ABS Mantelstein DZ 380 x 710mm L330mm","103926","0",null,"STK",{"$f":"VLOOKUP(G1763,sanschie!A:G,7,0)","v":56},{"$f":"ROUND(M1763,0)-M1764","v":24},{"$f":"((M1762-M1768)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1763*330","v":0}]
["Absolut",{"$f":"B1763+1","v":2},{"$f":"C1763","v":2016},{"$f":"A1764&C1764&B1764","v":"Absolut20162"},null,"ABS Thermo-Trennstein DZ 380 x 710mm L330mm","103938","0",null,"STK",{"$f":"VLOOKUP(G1764,sanschie!A:G,7,0)","v":283},{"$f":"IF(M1764=0,\"\",M1764)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,2016,"Absolut20163",null,"ABS Thermo-Fussplatte DZ 380 x 710mm","103857","0",null,"STK",{"$f":"VLOOKUP(G1765,sanschie!A:G,7,0)","v":210}]
["Absolut",4,2016,"Absolut20164",null,"ABS 200 Profilkeramik-Rohr mit Muffe L1330mm","103949",1330,null,"STK",{"$f":"VLOOKUP(G1766,sanschie!A:G,7,0)","v":145},{"$f":"ROUNDUP(M1766,0)","v":6},{"$f":"(M1762-O1763-M1768-M1774-M1775-M1783)/1000/1.33","v":5.962406015037593}]
["Absolut",5,2016,"Absolut20165",null,"ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","103947",1330,null,"STK",{"$f":"VLOOKUP(G1767,sanschie!A:G,7,0)","v":113},{"$f":"ROUNDUP(M1767,0)","v":5},{"$f":"(M1762-O1763-M1768-M1778-M1779-M1784)/1000/1.33","v":4.962406015037593}]
["Absolut",6,2016,"Absolut20166",null,"ABS 200 Fertigfuss DZ 2 x Ø200mm L1070mm","103867",1070,null,"STK",{"$f":"VLOOKUP(G1768,sanschie!A:G,7,0)","v":1476},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1768=\"\",0,$H1768*$L1768)","v":1070}]
["Absolut",7,2016,"Absolut20167",null,"ABS 200 Fertigfusspaket ","103892","0",null,"STK",{"$f":"VLOOKUP(G1769,sanschie!A:G,7,0)","v":311},{"$f":"L1768","v":1}]
["Absolut",8,2016,"Absolut20168",null,"ABS 160 Fertigfusspaket ","103890","0",null,"STK",{"$f":"VLOOKUP(G1770,sanschie!A:G,7,0)","v":311},{"$f":"L1768","v":1}]
["Absolut",9,2016,"Absolut20169",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G1771,sanschie!A:G,7,0)","v":18}]
["Absolut",10,2016,"Absolut201610",null,"CHZ 200 Keramik Fuss-Scheibe geschlossen","103701","0",null,"STK",{"$f":"VLOOKUP(G1772,sanschie!A:G,7,0)","v":45},{"$f":"IF(L1768=\"\",1,\"\")","v":""}]
["Absolut",11,2016,"Absolut201611",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G1773,sanschie!A:G,7,0)","v":32},{"$f":"IF(L1768=\"\",1,\"\")","v":""}]
["Absolut",12,2016,"Absolut201612",null,"ABS 200 Rauchrohr-Anschlusspaket 90° RA  ","103984",1330,null,"STK",{"$f":"VLOOKUP(G1774,sanschie!A:G,7,0)","v":434},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""},{"$f":"IF(L1774=0,0,IF(L1774=\"\",0,L1774*H1774))","v":0}]
["Absolut",13,2016,"Absolut201613",null,"ABS 200 Rauchrohr-Anschlusspaket 45° RA  ","103996",1330,null,"STK",{"$f":"VLOOKUP(G1775,sanschie!A:G,7,0)","v":466},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""},{"$f":"IF(L1775=0,0,IF(L1775=\"\",0,L1775*H1775))","v":0}]
["Absolut",14,2016,"Absolut201614",null,"ABS 200 Rauchrohranschluss Stutzen-Set 90° Ø200mm","104002","0",null,"STK",{"$f":"VLOOKUP(G1776,sanschie!A:G,7,0)","v":212}]
["Absolut",15,2016,"Absolut201615",null,"ABS 200 Rauchrohranschluss Stutzen-Set 45°","104008","0",null,"STK",{"$f":"VLOOKUP(G1777,sanschie!A:G,7,0)","v":212}]
["Absolut",16,2016,"Absolut201616",null,"ABS 160 Rauchrohr-Anschlusspaket 90° RA  ","103982",1330,null,"STK",{"$f":"VLOOKUP(G1778,sanschie!A:G,7,0)","v":367},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(L1778=0,0,IF(L1778=\"\",0,L1778*H1778))","v":1330}]
["Absolut",17,2016,"Absolut201617",null,"ABS 160 Rauchrohr-Anschlusspaket 45° RA  ","103994",1330,null,"STK",{"$f":"VLOOKUP(G1779,sanschie!A:G,7,0)","v":367},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(L1779=0,0,IF(L1779=\"\",0,L1779*H1779))","v":0}]
["Absolut",18,2016,"Absolut201618",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø160mm","104000","0",null,"STK",{"$f":"VLOOKUP(G1780,sanschie!A:G,7,0)","v":199}]
["Absolut",19,2016,"Absolut201619",null,"ABS 160 Rauchrohranschluss Stutzen-Set 45°","104006","0",null,"STK",{"$f":"VLOOKUP(G1781,sanschie!A:G,7,0)","v":199},null,null,null,"großer Zug","kleine Zug"]
["Absolut",20,2016,"Absolut201620",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G1782,sanschie!A:G,7,0)","v":160},{"$f":"IF(N1782=0,\"\",N1782)","v":""},null,{"$f":"SUM(O1782:P1782)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",21,2016,"Absolut201621",null,"ABS 200 Putztür-Anschlusspaket ","103967",1330,null,"STK",{"$f":"VLOOKUP(G1783,sanschie!A:G,7,0)","v":483},{"$f":"IF(N1783=0,\"\",N1783)","v":""},{"$f":"IF(L1783=0,0,IF(L1783=\"\",0,L1783*H1783))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",22,2016,"Absolut201622",null,"ABS 160 Putztür-Anschlusspaket ","103965",1330,null,"STK",{"$f":"VLOOKUP(G1784,sanschie!A:G,7,0)","v":428},{"$f":"IF(N1784=0,\"\",N1784)","v":""},{"$f":"IF(L1784=0,0,IF(L1784=\"\",0,L1784*H1784))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",23,2016,"Absolut201623",null,"ABS 200 Putztüranschluss Stutzen Set","104275","0",null,"STK",{"$f":"VLOOKUP(G1785,sanschie!A:G,7,0)","v":349}]
["Absolut",24,2016,"Absolut201624",null,"ABS 160 Putztüranschluss Stutzen Set","104273","0",null,"STK",{"$f":"VLOOKUP(G1786,sanschie!A:G,7,0)","v":325}]
["Absolut",25,2016,"Absolut201625",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1787,sanschie!A:G,7,0)","v":27}]
["Absolut",26,2016,"Absolut201626",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104192","0",null,"STK",{"$f":"VLOOKUP(G1788,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",27,2016,"Absolut201627",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104195","0",null,"STK",{"$f":"VLOOKUP(G1789,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",28,2016,"Absolut201628",null,"ABS Handyplatte DZ Faserzement 380 x 710mm  ","104152","0",null,"STK",{"$f":"VLOOKUP(G1790,sanschie!A:G,7,0)","v":180},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",29,2016,"Absolut201629",null,"ABS Handyplatte DZ Inox 380 x 710mm","104182","0",null,"STK",{"$f":"VLOOKUP(G1791,sanschie!A:G,7,0)","v":241},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",30,2016,"Absolut201630",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1792,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",31,2016,"Absolut201631",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G1793,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",32,2016,"Absolut201632",null,"ABS 200 Abströmkonus verkupfert","104207","0",null,"STK",{"$f":"VLOOKUP(G1794,sanschie!A:G,7,0)","v":197}]
["Absolut",33,2016,"Absolut201633",null,"ABS 160 Abströmkonus verkupfert","104205","0",null,"STK",{"$f":"VLOOKUP(G1795,sanschie!A:G,7,0)","v":166}]
["Absolut",{"$f":"B1795+1","v":34},{"$f":"C1795","v":2016},"Absolut201634",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G1796,sanschie!A:G,7,0)","v":1900}]
["Absolut",35,2016,"Absolut201635",null,"ABS 200 Anschlusskonus DZ mit Doppelfutter DN200mm","103904","0",null,"STK",{"$f":"VLOOKUP(G1797,sanschie!A:G,7,0)","v":272.89999999999998}]
["Absolut",36,2016,"Absolut201636",null,"ABS 200 Adapterring von 200mm auf 200mm L90mm","103909","0",null,"STK",{"$f":"VLOOKUP(G1798,sanschie!A:G,7,0)","v":65}]
["Absolut",37,2016,"Absolut201637",null,"ABS 180 Adapterring von 180mm auf 160mm L90mm","103906","0",null,"STK",{"$f":"VLOOKUP(G1799,sanschie!A:G,7,0)","v":41}]
["Absolut",38,2016,"Absolut201638",null,"KER 200  Keranova-Fugenglätter","103475","0",null,"STK",{"$f":"VLOOKUP(G1800,sanschie!A:G,7,0)","v":72}]
["Absolut",39,2016,"Absolut201639",null,"KER 160  Keranova-Fugenglätter","103473","0",null,"STK",{"$f":"VLOOKUP(G1801,sanschie!A:G,7,0)","v":58}]
["Absolut",40,2016,"Absolut201640",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø100mm","104019","0",null,"STK",{"$f":"VLOOKUP(G1802,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",41,2016,"Absolut201641",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø120mm","104020","0",null,"STK",{"$f":"VLOOKUP(G1803,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",42,2016,"Absolut201642",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø130mm","104021","0",null,"STK",{"$f":"VLOOKUP(G1804,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",43,2016,"Absolut201643",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø150mm","104022","0",null,"STK",{"$f":"VLOOKUP(G1805,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",44,2016,"Absolut201644",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø180mm","104023","0",null,"STK",{"$f":"VLOOKUP(G1806,sanschie!A:G,7,0)","v":210},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",45,2016,"Absolut201645",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø200mm","104024","0",null,"STK",{"$f":"VLOOKUP(G1807,sanschie!A:G,7,0)","v":222},{"$f":"IF(Daten!$B$226=8,1,\"\")","v":""}]
["Absolut",46,2016,"Absolut201646",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G1808,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",47,2016,"Absolut201647",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G1809,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",48,2016,"Absolut201648",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G1810,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",49,2016,"Absolut201649",null,"CHZ 150 Doppelfutter lose L150mm","103803","0",null,"STK",{"$f":"VLOOKUP(G1811,sanschie!A:G,7,0)","v":103},{"$f":"IF(Daten!$F$226=6,1,\"\")","v":""}]
["Absolut",50,2016,"Absolut201650",null,"ABS 200 Kondensatfalle zu RA 45° Ø130mm ","104036","0",null,"STK",{"$f":"VLOOKUP(G1812,sanschie!A:G,7,0)","v":365}]
["Absolut",51,2016,"Absolut201651",null,"ABS 200 Kondensatfalle zu RA 45° Ø150mm ","104037","0",null,"STK",{"$f":"VLOOKUP(G1813,sanschie!A:G,7,0)","v":365}]
["Absolut",52,2016,"Absolut201652",null,"ABS 200 Kondensatfalle zu RA 45° Ø160mm","104038","0",null,"STK",{"$f":"VLOOKUP(G1814,sanschie!A:G,7,0)","v":365}]
["Absolut",53,2016,"Absolut201653",null,"ABS 200 Kondensatfalle zu RA 45° Ø180mm ","104039","0",null,"STK",{"$f":"VLOOKUP(G1815,sanschie!A:G,7,0)","v":365}]
["Absolut",54,2016,"Absolut201654",null,"ABS 200 Kondensatfalle zu RA 45° Ø200mm ","104040","0",null,"STK",{"$f":"VLOOKUP(G1816,sanschie!A:G,7,0)","v":365}]
["Absolut",55,2016,"Absolut201655",null,"ABS 160 Kondensatfalle zu RA 45° Ø130mm ","104029","0",null,"STK",{"$f":"VLOOKUP(G1817,sanschie!A:G,7,0)","v":322}]
["Absolut",56,2016,"Absolut201656",null,"ABS 160 Kondensatfalle zu RA 45° Ø150mm ","104030","0",null,"STK",{"$f":"VLOOKUP(G1818,sanschie!A:G,7,0)","v":322}]
["Absolut",57,2016,"Absolut201657",null,"ABS 160 Kondensatfalle zu RA 45° Ø160mm ","104031","0",null,"STK",{"$f":"VLOOKUP(G1819,sanschie!A:G,7,0)","v":322}]
["Absolut",58,2016,"Absolut201658",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1820,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",59,2016,"Absolut201659",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1821,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",60,2016,"Absolut201660",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1822,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",61,2016,"Absolut201661",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1823,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1769=1,2,\"\")","v":2}]
["Absolut",62,2016,"Absolut201662",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1824,sanschie!A:G,7,0)","v":489},{"$f":"IF(N1824=0,\"\",N1824)","v":""},null,{"$f":"SUM(O1824:P1824)","v":0},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""},{"$f":"IF(Daten!$F$241=1,\"\",1)","v":""}]
["Absolut",63,2016,"Absolut201663",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1825,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",64,2016,"Absolut201664",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1826,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",65,2016,"Absolut201665",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G1827,sanschie!A:G,7,0)","v":14},{"$f":"IF(N1827=0,\"\",ROUNDUP(N1827,0))","v":""},null,{"$f":"SUM(O1827:P1827)","v":0},{"$f":"IF(L1766<=8,0,(L1766-8)/2)","v":0}]
["Absolut",{"$f":"B1827+1","v":66},{"$f":"C1827","v":2016},"Absolut201666",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G1828,sanschie!A:G,7,0)","v":14},{"$f":"IF(N1828=0,\"\",ROUNDUP(N1828,0))","v":""},null,{"$f":"SUM(O1828:P1828)","v":0},{"$f":"IF(L1767<=8,0,(L1767-8)/2)","v":0}]
["Absolut",67,2016,{"$f":"A1829&C1829&B1829","v":"Absolut201667"},null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1829,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1829=0,\"\",N1829)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",68,2016,"Absolut201668",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1830,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1830=0,\"\",N1830)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",69,2016,"Absolut201669",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1831,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",70,2016,"Absolut201670",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1832,sanschie!A:G,7,0)","v":35},{"$f":"IF(N1832<=11.5,1,2)","v":1},null,{"$f":"IF(L1768=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",71,2016,"Absolut201671",null,"ABS 200 Basten Standard Inox","104213","0",null,"STK",{"$f":"VLOOKUP(G1833,sanschie!A:G,7,0)","v":361},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",72,2016,"Absolut201672",null,"ABS 200 Basten Standard Kupfer","104219","0",null,"STK",{"$f":"VLOOKUP(G1834,sanschie!A:G,7,0)","v":375},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",73,2016,"Absolut201673",null,"ABS 200 Sairlift Inox","104225","0",null,"STK",{"$f":"VLOOKUP(G1835,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",74,2016,"Absolut201674",null,"ABS 200 Sairlift Kupfer","104230","0",null,"STK",{"$f":"VLOOKUP(G1836,sanschie!A:G,7,0)","v":434},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",75,2016,"Absolut201675",null,"ABS 160 Basten Standard Inox","104211","0",null,"STK",{"$f":"VLOOKUP(G1837,sanschie!A:G,7,0)","v":323},{"$f":"IF(Daten!$F$297=2,1,\"\")","v":""}]
["Absolut",76,2016,"Absolut201676",null,"ABS 160 Basten Standard Kupfer","104217","0",null,"STK",{"$f":"VLOOKUP(G1838,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$F$297=3,1,\"\")","v":""}]
["Absolut",77,2016,"Absolut201677",null,"ABS 160 Sairlift Inox","104223","0",null,"STK",{"$f":"VLOOKUP(G1839,sanschie!A:G,7,0)","v":374},{"$f":"IF(Daten!$F$297=4,1,\"\")","v":""}]
["Absolut",78,2016,"Absolut201678",null,"ABS 160 Sairlift Kupfer","104228","0",null,"STK",{"$f":"VLOOKUP(G1840,sanschie!A:G,7,0)","v":397},{"$f":"IF(Daten!$F$297=5,1,\"\")","v":""}]
["Absolut",79,2016,"Absolut201679",null,"ZBH 200 Verschlussbüchse weiss ØA 300mm","103839","0",null,"STK",{"$f":"VLOOKUP(G1841,sanschie!A:G,7,0)","v":123.1}]
["Absolut",80,2016,"Absolut201680",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G1842,sanschie!A:G,7,0)","v":123.1}]
["Absolut",81,2016,"Absolut201681",null,"ZBH 150 Verschlussbüchse weiss ØA 275mm","103836","0",null,"STK",{"$f":"VLOOKUP(G1843,sanschie!A:G,7,0)","v":115}]
["Absolut",82,2016,"Absolut201682",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1844,sanschie!A:G,7,0)","v":258.8}]
["Absolut",83,2016,"Absolut201683",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1845,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",84,2016,"Absolut201684",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1846,sanschie!A:G,7,0)","v":44.9}]
["Absolut",85,2016,"Absolut201685",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1847,sanschie!A:G,7,0)","v":7.5}]
["Absolut",86,2016,"Absolut201686",null,"ZBH 210 Verschlusszapfen 2Stk. aus Schaumstoff","103834","0",null,"STK",{"$f":"VLOOKUP(G1848,sanschie!A:G,7,0)","v":26.5}]
["Absolut",87,2016,"Absolut201687",null,"ZBH 170 Verschlusszapfen 2Stk. aus Schaumstoff","103832","0",null,"STK",{"$f":"VLOOKUP(G1849,sanschie!A:G,7,0)","v":24.2}]
["Absolut",88,2016,"Absolut201688",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G1850,sanschie!A:G,7,0)","v":452}]
["Absolut",89,2016,"Absolut201689",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G1851,sanschie!A:G,7,0)","v":538}]
["Absolut",90,2016,"Absolut201690",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G1852,sanschie!A:G,7,0)","v":634}]
["Absolut",91,2016,"Absolut201691",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G1853,sanschie!A:G,7,0)","v":695}]
["Absolut",92,2016,"Absolut201692",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G1854,sanschie!A:G,7,0)","v":797}]
["Absolut",93,2016,"Absolut201693",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G1855,sanschie!A:G,7,0)","v":873}]
["Absolut",94,2016,"Absolut201694",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1856,sanschie!A:G,7,0)","v":13.8}]
["Absolut",95,2016,"Absolut201695",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1857,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",96,2016,"Absolut201696",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1858,sanschie!A:G,7,0)","v":322}]
["Absolut",97,2016,"Absolut201697",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1859,sanschie!A:G,7,0)","v":26}]
["Absolut",98,2016,"Absolut201698",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1860,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,2018,{"$f":"A1861&C1861&B1861","v":"Absolut20180"},"P","Absolut-Kaminanlage Ø 2018","Absolut 2018","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1861,sanschie!A:G,7,0)","v":0},null,{"$f":"I1861*1000","v":9000}]
["Absolut",{"$f":"B1861+1","v":1},{"$f":"C1861","v":2018},{"$f":"A1862&C1862&B1862","v":"Absolut20181"},null,"ABS Mantelstein DZ 380 x 710mm L330mm","103926","0",null,"STK",{"$f":"VLOOKUP(G1862,sanschie!A:G,7,0)","v":56},{"$f":"ROUND(M1862,0)-M1863","v":24},{"$f":"((M1861-M1867)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1862*330","v":0}]
["Absolut",{"$f":"B1862+1","v":2},{"$f":"C1862","v":2018},{"$f":"A1863&C1863&B1863","v":"Absolut20182"},null,"ABS Thermo-Trennstein DZ 380 x 710mm L330mm","103938","0",null,"STK",{"$f":"VLOOKUP(G1863,sanschie!A:G,7,0)","v":283},{"$f":"IF(M1863=0,\"\",M1863)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,2018,"Absolut20183",null,"ABS Thermo-Fussplatte DZ 380 x 710mm","103857","0",null,"STK",{"$f":"VLOOKUP(G1864,sanschie!A:G,7,0)","v":210}]
["Absolut",4,2018,"Absolut20184",null,"ABS 200 Profilkeramik-Rohr mit Muffe L1330mm","103949",1330,null,"STK",{"$f":"VLOOKUP(G1865,sanschie!A:G,7,0)","v":145},{"$f":"ROUNDUP(M1865,0)","v":6},{"$f":"(M1861-O1862-M1867-M1873-M1874-M1882)/1000/1.33","v":5.962406015037593}]
["Absolut",5,2018,"Absolut20185",null,"ABS 180 Profilkeramik-Rohr mit Muffe L1330mm","103948",1330,null,"STK",{"$f":"VLOOKUP(G1866,sanschie!A:G,7,0)","v":122},{"$f":"ROUNDUP(M1866,0)","v":5},{"$f":"(M1861-O1862-M1867-M1877-M1878-M1883)/1000/1.33","v":4.962406015037593}]
["Absolut",6,2018,"Absolut20186",null,"ABS 200 Fertigfuss DZ 2 x Ø200mm L1070mm","103867",1070,null,"STK",{"$f":"VLOOKUP(G1867,sanschie!A:G,7,0)","v":1476},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1867=\"\",0,$H1867*$L1867)","v":1070}]
["Absolut",7,2018,"Absolut20187",null,"ABS 200 Fertigfusspaket ","103892","0",null,"STK",{"$f":"VLOOKUP(G1868,sanschie!A:G,7,0)","v":311},{"$f":"L1867","v":1}]
["Absolut",8,2018,"Absolut20188",null,"ABS 180 Fertigfusspaket ","103891","0",null,"STK",{"$f":"VLOOKUP(G1869,sanschie!A:G,7,0)","v":311},{"$f":"L1867","v":1}]
["Absolut",9,2018,"Absolut20189",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G1870,sanschie!A:G,7,0)","v":18}]
["Absolut",10,2018,"Absolut201810",null,"CHZ 200 Keramik Fuss-Scheibe geschlossen","103701","0",null,"STK",{"$f":"VLOOKUP(G1871,sanschie!A:G,7,0)","v":45},{"$f":"IF(L1867=\"\",1,\"\")","v":""}]
["Absolut",11,2018,"Absolut201811",null,"CHZ 180 Keramik Fuss-Scheibe geschlossen","103700","0",null,"STK",{"$f":"VLOOKUP(G1872,sanschie!A:G,7,0)","v":35},{"$f":"IF(L1867=\"\",1,\"\")","v":""}]
["Absolut",12,2018,"Absolut201812",null,"ABS 200 Rauchrohr-Anschlusspaket 90° RA  ","103984",1330,null,"STK",{"$f":"VLOOKUP(G1873,sanschie!A:G,7,0)","v":434},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""},{"$f":"IF(L1873=0,0,IF(L1873=\"\",0,L1873*H1873))","v":0}]
["Absolut",13,2018,"Absolut201813",null,"ABS 200 Rauchrohr-Anschlusspaket 45° RA  ","103996",1330,null,"STK",{"$f":"VLOOKUP(G1874,sanschie!A:G,7,0)","v":466},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""},{"$f":"IF(L1874=0,0,IF(L1874=\"\",0,L1874*H1874))","v":0}]
["Absolut",14,2018,"Absolut201814",null,"ABS 200 Rauchrohranschluss Stutzen-Set 90° Ø200mm","104002","0",null,"STK",{"$f":"VLOOKUP(G1875,sanschie!A:G,7,0)","v":212}]
["Absolut",15,2018,"Absolut201815",null,"ABS 200 Rauchrohranschluss Stutzen-Set 45°","104008","0",null,"STK",{"$f":"VLOOKUP(G1876,sanschie!A:G,7,0)","v":212}]
["Absolut",16,2018,"Absolut201816",null,"ABS 180 Rauchrohr-Anschlusspaket 90° RA  ","103983",1330,null,"STK",{"$f":"VLOOKUP(G1877,sanschie!A:G,7,0)","v":386},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(L1877=0,0,IF(L1877=\"\",0,L1877*H1877))","v":1330}]
["Absolut",17,2018,"Absolut201817",null,"ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","103995",1330,null,"STK",{"$f":"VLOOKUP(G1878,sanschie!A:G,7,0)","v":404},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(L1878=0,0,IF(L1878=\"\",0,L1878*H1878))","v":0}]
["Absolut",18,2018,"Absolut201818",null,"ABS 180  Rauchrohranschluss Stutzen-Set 90° Ø180mm","104001","0",null,"STK",{"$f":"VLOOKUP(G1879,sanschie!A:G,7,0)","v":204}]
["Absolut",19,2018,"Absolut201819",null,"ABS 180 Rauchrohranschluss Stutzen-Set 45°","104007","0",null,"STK",{"$f":"VLOOKUP(G1880,sanschie!A:G,7,0)","v":204},null,null,null,"großer Zug","kleine Zug"]
["Absolut",20,2018,"Absolut201820",null,"ABS 180 Steckadapter ","104268","0",null,"STK",{"$f":"VLOOKUP(G1881,sanschie!A:G,7,0)","v":173},{"$f":"IF(N1881=0,\"\",N1881)","v":""},null,{"$f":"SUM(O1881:P1881)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",21,2018,"Absolut201821",null,"ABS 200 Putztür-Anschlusspaket ","103967",1330,null,"STK",{"$f":"VLOOKUP(G1882,sanschie!A:G,7,0)","v":483},{"$f":"IF(N1882=0,\"\",N1882)","v":""},{"$f":"IF(L1882=0,0,IF(L1882=\"\",0,L1882*H1882))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",22,2018,"Absolut201822",null,"ABS 180 Putztür-Anschlusspaket ","103966",1330,null,"STK",{"$f":"VLOOKUP(G1883,sanschie!A:G,7,0)","v":448},{"$f":"IF(N1883=0,\"\",N1883)","v":""},{"$f":"IF(L1883=0,0,IF(L1883=\"\",0,L1883*H1883))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",23,2018,"Absolut201823",null,"ABS 200 Putztüranschluss Stutzen Set","104275","0",null,"STK",{"$f":"VLOOKUP(G1884,sanschie!A:G,7,0)","v":349}]
["Absolut",24,2018,"Absolut201824",null,"ABS 180 Putztüranschluss Stutzen Set","104274","0",null,"STK",{"$f":"VLOOKUP(G1885,sanschie!A:G,7,0)","v":336}]
["Absolut",25,2018,"Absolut201825",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1886,sanschie!A:G,7,0)","v":27}]
["Absolut",26,2018,"Absolut201826",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104192","0",null,"STK",{"$f":"VLOOKUP(G1887,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",27,2018,"Absolut201827",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104195","0",null,"STK",{"$f":"VLOOKUP(G1888,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",28,2018,"Absolut201828",null,"ABS Handyplatte DZ Faserzement 380 x 710mm  ","104152","0",null,"STK",{"$f":"VLOOKUP(G1889,sanschie!A:G,7,0)","v":180},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",29,2018,"Absolut201829",null,"ABS Handyplatte DZ Inox 380 x 710mm","104182","0",null,"STK",{"$f":"VLOOKUP(G1890,sanschie!A:G,7,0)","v":241},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",30,2018,"Absolut201830",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1891,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",31,2018,"Absolut201831",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G1892,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",32,2018,"Absolut201832",null,"ABS 200 Abströmkonus verkupfert","104207","0",null,"STK",{"$f":"VLOOKUP(G1893,sanschie!A:G,7,0)","v":197}]
["Absolut",33,2018,"Absolut201833",null,"ABS 180 Abströmkonus verkupfert","104206","0",null,"STK",{"$f":"VLOOKUP(G1894,sanschie!A:G,7,0)","v":174}]
["Absolut",{"$f":"B1894+1","v":34},{"$f":"C1894","v":2018},"Absolut201834",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G1895,sanschie!A:G,7,0)","v":1900}]
["Absolut",35,2018,"Absolut201835",null,"ABS 200 Anschlusskonus DZ mit Doppelfutter DN200mm","103904","0",null,"STK",{"$f":"VLOOKUP(G1896,sanschie!A:G,7,0)","v":272.89999999999998}]
["Absolut",36,2018,"Absolut201836",null,"ABS 200 Adapterring von 200mm auf 200mm L90mm","103909","0",null,"STK",{"$f":"VLOOKUP(G1897,sanschie!A:G,7,0)","v":65}]
["Absolut",37,2018,"Absolut201837",null,"ABS 180 Adapterring von 180mm auf 160mm L90mm","103906","0",null,"STK",{"$f":"VLOOKUP(G1898,sanschie!A:G,7,0)","v":41}]
["Absolut",38,2018,"Absolut201838",null,"KER 200  Keranova-Fugenglätter","103475","0",null,"STK",{"$f":"VLOOKUP(G1899,sanschie!A:G,7,0)","v":72}]
["Absolut",39,2018,"Absolut201839",null,"KER 180  Keranova-Fugenglätter","103474","0",null,"STK",{"$f":"VLOOKUP(G1900,sanschie!A:G,7,0)","v":61}]
["Absolut",40,2018,"Absolut201840",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø100mm","104019","0",null,"STK",{"$f":"VLOOKUP(G1901,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",41,2018,"Absolut201841",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø120mm","104020","0",null,"STK",{"$f":"VLOOKUP(G1902,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",42,2018,"Absolut201842",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø130mm","104021","0",null,"STK",{"$f":"VLOOKUP(G1903,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",43,2018,"Absolut201843",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø150mm","104022","0",null,"STK",{"$f":"VLOOKUP(G1904,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",44,2018,"Absolut201844",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø180mm","104023","0",null,"STK",{"$f":"VLOOKUP(G1905,sanschie!A:G,7,0)","v":210},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",45,2018,"Absolut201845",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø200mm","104024","0",null,"STK",{"$f":"VLOOKUP(G1906,sanschie!A:G,7,0)","v":222},{"$f":"IF(Daten!$B$226=8,1,\"\")","v":""}]
["Absolut",46,2018,"Absolut201846",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø100mm","104014","0",null,"STK",{"$f":"VLOOKUP(G1907,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",47,2018,"Absolut201847",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm","104015","0",null,"STK",{"$f":"VLOOKUP(G1908,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",48,2018,"Absolut201848",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø130mm","104016","0",null,"STK",{"$f":"VLOOKUP(G1909,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",49,2018,"Absolut201849",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø150mm","104017","0",null,"STK",{"$f":"VLOOKUP(G1910,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$F$226=6,1,\"\")","v":""}]
["Absolut",50,2018,"Absolut201850",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø180mm","104018","0",null,"STK",{"$f":"VLOOKUP(G1911,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$F$226=7,1,\"\")","v":""}]
["Absolut",51,2018,"Absolut201851",null,"ABS 200 Kondensatfalle zu RA 45° Ø130mm ","104036","0",null,"STK",{"$f":"VLOOKUP(G1912,sanschie!A:G,7,0)","v":365}]
["Absolut",52,2018,"Absolut201852",null,"ABS 200 Kondensatfalle zu RA 45° Ø150mm ","104037","0",null,"STK",{"$f":"VLOOKUP(G1913,sanschie!A:G,7,0)","v":365}]
["Absolut",53,2018,"Absolut201853",null,"ABS 200 Kondensatfalle zu RA 45° Ø160mm","104038","0",null,"STK",{"$f":"VLOOKUP(G1914,sanschie!A:G,7,0)","v":365}]
["Absolut",54,2018,"Absolut201854",null,"ABS 200 Kondensatfalle zu RA 45° Ø180mm ","104039","0",null,"STK",{"$f":"VLOOKUP(G1915,sanschie!A:G,7,0)","v":365}]
["Absolut",55,2018,"Absolut201855",null,"ABS 200 Kondensatfalle zu RA 45° Ø200mm ","104040","0",null,"STK",{"$f":"VLOOKUP(G1916,sanschie!A:G,7,0)","v":365}]
["Absolut",56,2018,"Absolut201856",null,"ABS 180 Kondensatfalle zu RA 45° Ø130mm","104032","0",null,"STK",{"$f":"VLOOKUP(G1917,sanschie!A:G,7,0)","v":347}]
["Absolut",57,2018,"Absolut201857",null,"ABS 180 Kondensatfalle zu RA 45° Ø150mm","104033","0",null,"STK",{"$f":"VLOOKUP(G1918,sanschie!A:G,7,0)","v":347}]
["Absolut",58,2018,"Absolut201858",null,"ABS 180 Kondensatfalle zu RA 45° Ø160mm","104034","0",null,"STK",{"$f":"VLOOKUP(G1919,sanschie!A:G,7,0)","v":347}]
["Absolut",59,2018,"Absolut201859",null,"ABS 180 Kondensatfalle zu RA 45° Ø180mm ","104035","0",null,"STK",{"$f":"VLOOKUP(G1920,sanschie!A:G,7,0)","v":347}]
["Absolut",60,2018,"Absolut201860",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G1921,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",61,2018,"Absolut201861",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G1922,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",62,2018,"Absolut201862",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G1923,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",63,2018,"Absolut201863",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G1924,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1868=1,2,\"\")","v":2},null,null,"großer Zug","kleine Zug"]
["Absolut",64,2018,"Absolut201864",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G1925,sanschie!A:G,7,0)","v":489},{"$f":"IF(N1925=0,\"\",N1925)","v":""},null,{"$f":"SUM(O1925:P1925)","v":0},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""},{"$f":"IF(Daten!$F$241=1,\"\",1)","v":""}]
["Absolut",65,2018,"Absolut201865",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G1926,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",{"$f":"B1926+1","v":66},{"$f":"C1926","v":2018},"Absolut201866",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G1927,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",67,2018,"Absolut201867",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G1928,sanschie!A:G,7,0)","v":14},{"$f":"IF(N1928=0,\"\",ROUNDUP(N1928,0))","v":""},null,{"$f":"SUM(O1928:P1928)","v":0},{"$f":"IF(L1865<=8,0,(L1865-8)/2)","v":0},{"$f":"IF(L1866<=8,0,(L1866-8)/2)","v":0}]
["Absolut",68,2018,{"$f":"A1929&C1929&B1929","v":"Absolut201868"},null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G1929,sanschie!A:G,7,0)","v":303},{"$f":"IF(N1929=0,\"\",N1929)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",69,2018,"Absolut201869",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G1930,sanschie!A:G,7,0)","v":94},{"$f":"IF(N1930=0,\"\",N1930)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",70,2018,"Absolut201870",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G1931,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",71,2018,"Absolut201871",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G1932,sanschie!A:G,7,0)","v":35},{"$f":"IF(N1932<=11.5,1,2)","v":1},null,{"$f":"IF(L1867=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",72,2018,"Absolut201872",null,"ABS 200 Basten Standard Inox","104213","0",null,"STK",{"$f":"VLOOKUP(G1933,sanschie!A:G,7,0)","v":361},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",73,2018,"Absolut201873",null,"ABS 200 Basten Standard Kupfer","104219","0",null,"STK",{"$f":"VLOOKUP(G1934,sanschie!A:G,7,0)","v":375},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",74,2018,"Absolut201874",null,"ABS 200 Sairlift Inox","104225","0",null,"STK",{"$f":"VLOOKUP(G1935,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",75,2018,"Absolut201875",null,"ABS 200 Sairlift Kupfer","104230","0",null,"STK",{"$f":"VLOOKUP(G1936,sanschie!A:G,7,0)","v":434},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",76,2018,"Absolut201876",null,"ABS 180 Basten Standard Inox","104212","0",null,"STK",{"$f":"VLOOKUP(G1937,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$F$297=2,1,\"\")","v":""}]
["Absolut",77,2018,"Absolut201877",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",{"$f":"VLOOKUP(G1938,sanschie!A:G,7,0)","v":362},{"$f":"IF(Daten!$F$297=3,1,\"\")","v":""}]
["Absolut",78,2018,"Absolut201878",null,"ABS 180 Sairlift Inox","104224","0",null,"STK",{"$f":"VLOOKUP(G1939,sanschie!A:G,7,0)","v":400},{"$f":"IF(Daten!$F$297=4,1,\"\")","v":""}]
["Absolut",79,2018,"Absolut201879",null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",{"$f":"VLOOKUP(G1940,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$F$297=5,1,\"\")","v":""}]
["Absolut",80,2018,"Absolut201880",null,"ZBH 200 Verschlussbüchse weiss ØA 300mm","103839","0",null,"STK",{"$f":"VLOOKUP(G1941,sanschie!A:G,7,0)","v":123.1}]
["Absolut",81,2018,"Absolut201881",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G1942,sanschie!A:G,7,0)","v":123.1}]
["Absolut",82,2018,"Absolut201882",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G1943,sanschie!A:G,7,0)","v":258.8}]
["Absolut",83,2018,"Absolut201883",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G1944,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",84,2018,"Absolut201884",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G1945,sanschie!A:G,7,0)","v":44.9}]
["Absolut",85,2018,"Absolut201885",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G1946,sanschie!A:G,7,0)","v":7.5}]
["Absolut",86,2018,"Absolut201886",null,"ZBH 210 Verschlusszapfen 2Stk. aus Schaumstoff","103834","0",null,"STK",{"$f":"VLOOKUP(G1947,sanschie!A:G,7,0)","v":26.5}]
["Absolut",87,2018,"Absolut201887",null,"ZBH 190 Verschlusszapfen 2Stk. aus Schaumstoff","103833","0",null,"STK",{"$f":"VLOOKUP(G1948,sanschie!A:G,7,0)","v":26.5}]
["Absolut",88,2018,"Absolut201888",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G1949,sanschie!A:G,7,0)","v":452}]
["Absolut",89,2018,"Absolut201889",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G1950,sanschie!A:G,7,0)","v":538}]
["Absolut",90,2018,"Absolut201890",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G1951,sanschie!A:G,7,0)","v":634}]
["Absolut",91,2018,"Absolut201891",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G1952,sanschie!A:G,7,0)","v":695}]
["Absolut",92,2018,"Absolut201892",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G1953,sanschie!A:G,7,0)","v":797}]
["Absolut",93,2018,"Absolut201893",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G1954,sanschie!A:G,7,0)","v":873}]
["Absolut",94,2018,"Absolut201894",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G1955,sanschie!A:G,7,0)","v":13.8}]
["Absolut",95,2018,"Absolut201895",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G1956,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",96,2018,"Absolut201896",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G1957,sanschie!A:G,7,0)","v":322}]
["Absolut",97,2018,"Absolut201897",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G1958,sanschie!A:G,7,0)","v":26}]
["Absolut",98,2018,"Absolut201898",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G1959,sanschie!A:G,7,0)","v":0},2]
["Absolut",0,"16TL14",{"$f":"A1960&C1960&B1960","v":"Absolut16TL140"},"P","Absolut-Kaminanlage Ø 16TL14","Absolut 16TL14","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G1960,sanschie!A:G,7,0)","v":0},null,{"$f":"I1960*1000","v":9000}]
["Absolut",{"$f":"B1960+1","v":1},{"$f":"C1960","v":"16TL14"},{"$f":"A1961&C1961&B1961","v":"Absolut16TL141"},null,"ABS Mantelstein DZTL 360 x 830mm L330mm","103928","0",null,"STK",{"$f":"VLOOKUP(G1961,sanschie!A:G,7,0)","v":58},{"$f":"ROUND(M1961,0)-M1962","v":24},{"$f":"((M1960-M1966)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N1961*330","v":0}]
["Absolut",{"$f":"B1961+1","v":2},{"$f":"C1961","v":"16TL14"},{"$f":"A1962&C1962&B1962","v":"Absolut16TL142"},null,"ABS Thermo-Trennstein DZTL 360 x 830mm L330mm","103939","0",null,"STK",{"$f":"VLOOKUP(G1962,sanschie!A:G,7,0)","v":345},{"$f":"IF(M1962=0,\"\",M1962)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,"16TL14","Absolut16TL143",null,"ABS Thermo-Fussplatte DZTL 360 x 850mm","103856","0",null,"STK",{"$f":"VLOOKUP(G1963,sanschie!A:G,7,0)","v":234}]
["Absolut",4,"16TL14","Absolut16TL144",null,"ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","103947",1330,null,"STK",{"$f":"VLOOKUP(G1964,sanschie!A:G,7,0)","v":113},{"$f":"ROUNDUP(M1964,0)","v":6},{"$f":"(M1960-O1961-M1966-M1970-M1971-M1980)/1000/1.33","v":5.962406015037593}]
["Absolut",5,"16TL14","Absolut16TL145",null,"ABS 140 Profilkeramik-Rohr mit Muffe L1330mm","103946",1330,null,"STK",{"$f":"VLOOKUP(G1965,sanschie!A:G,7,0)","v":106},{"$f":"ROUNDUP(M1965,0)","v":5},{"$f":"(M1960-O1961-M1966-M1974-M1975-M1981)/1000/1.33","v":4.962406015037593}]
["Absolut",6,"16TL14","Absolut16TL146",null,"ABS 180 Fertigfuss DZTL 2 x Ø120-180mm L1070mm","103868",1070,null,"STK",{"$f":"VLOOKUP(G1966,sanschie!A:G,7,0)","v":1472},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L1966=\"\",0,$H1966*$L1966)","v":1070}]
["Absolut",7,"16TL14","Absolut16TL147",null,"ABS 160 Fertigfusspaket ","103890","0",null,"STK",{"$f":"VLOOKUP(G1967,sanschie!A:G,7,0)","v":311},{"$f":"L1966","v":1}]
["Absolut",8,"16TL14","Absolut16TL148",null,"ABS 140 Fertigfusspaket ","103889","0",null,"STK",{"$f":"VLOOKUP(G1968,sanschie!A:G,7,0)","v":311},{"$f":"L1966","v":1}]
["Absolut",9,"16TL14","Absolut16TL149",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G1969,sanschie!A:G,7,0)","v":32},{"$f":"IF(L1966=\"\",2,\"\")","v":""}]
["Absolut",10,"16TL14","Absolut16TL1410",null,"ABS 160 Rauchrohr-Anschlusspaket 90° RA  ","103982",1330,null,"STK",{"$f":"VLOOKUP(G1970,sanschie!A:G,7,0)","v":367},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""},{"$f":"IF(L1970=0,0,IF(L1970=\"\",0,L1970*H1970))","v":0}]
["Absolut",11,"16TL14","Absolut16TL1411",null,"ABS 160 Rauchrohr-Anschlusspaket 45° RA  ","103994",1330,null,"STK",{"$f":"VLOOKUP(G1971,sanschie!A:G,7,0)","v":367},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""},{"$f":"IF(L1971=0,0,IF(L1971=\"\",0,L1971*H1971))","v":0}]
["Absolut",12,"16TL14","Absolut16TL1412",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø160mm","104000","0",null,"STK",{"$f":"VLOOKUP(G1972,sanschie!A:G,7,0)","v":199}]
["Absolut",13,"16TL14","Absolut16TL1413",null,"ABS 160 Rauchrohranschluss Stutzen-Set 45°","104006","0",null,"STK",{"$f":"VLOOKUP(G1973,sanschie!A:G,7,0)","v":199}]
["Absolut",14,"16TL14","Absolut16TL1414",null,"ABS 140 Rauchrohr-Anschlusspaket 90° RA  ","103981",1330,null,"STK",{"$f":"VLOOKUP(G1974,sanschie!A:G,7,0)","v":355},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(L1974=0,0,IF(L1974=\"\",0,L1974*H1974))","v":1330}]
["Absolut",15,"16TL14","Absolut16TL1415",null,"ABS 140 Rauchrohr-Anschlusspaket 45° RA  ","103993",1330,null,"STK",{"$f":"VLOOKUP(G1975,sanschie!A:G,7,0)","v":355},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(L1975=0,0,IF(L1975=\"\",0,L1975*H1975))","v":0}]
["Absolut",16,"16TL14","Absolut16TL1416",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø140mm","103999","0",null,"STK",{"$f":"VLOOKUP(G1976,sanschie!A:G,7,0)","v":191}]
["Absolut",17,"16TL14","Absolut16TL1417",null,"ABS 140 Rauchrohranschluss Stutzen-Set 45°","104005","0",null,"STK",{"$f":"VLOOKUP(G1977,sanschie!A:G,7,0)","v":191},null,null,null,"großer Zug","kleine Zug"]
["Absolut",18,"16TL14","Absolut16TL1418",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G1978,sanschie!A:G,7,0)","v":160},{"$f":"IF(N1978=0,\"\",N1978)","v":""},null,{"$f":"SUM(O1978:P1978)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",19,"16TL14","Absolut16TL1419",null,"ABS 200 Steckadapter ","104269","0",null,"STK",{"$f":"VLOOKUP(G1979,sanschie!A:G,7,0)","v":184}]
["Absolut",20,"16TL14","Absolut16TL1420",null,"ABS 160 Putztür-Anschlusspaket ","103965",1330,null,"STK",{"$f":"VLOOKUP(G1980,sanschie!A:G,7,0)","v":428},{"$f":"IF(N1980=0,\"\",N1980)","v":""},{"$f":"IF(L1980=0,0,IF(L1980=\"\",0,L1980*H1980))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",21,"16TL14","Absolut16TL1421",null,"ABS 140 Putztür-Anschlusspaket ","103964",1330,null,"STK",{"$f":"VLOOKUP(G1981,sanschie!A:G,7,0)","v":410},{"$f":"IF(N1981=0,\"\",N1981)","v":""},{"$f":"IF(L1981=0,0,IF(L1981=\"\",0,L1981*H1981))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",22,"16TL14","Absolut16TL1422",null,"ABS 160 Putztüranschluss Stutzen Set","104273","0",null,"STK",{"$f":"VLOOKUP(G1982,sanschie!A:G,7,0)","v":325}]
["Absolut",23,"16TL14","Absolut16TL1423",null,"ABS 140 Putztüranschluss Stutzen Set","104272","0",null,"STK",{"$f":"VLOOKUP(G1983,sanschie!A:G,7,0)","v":311}]
["Absolut",24,"16TL14","Absolut16TL1424",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G1984,sanschie!A:G,7,0)","v":27}]
["Absolut",25,"16TL14","Absolut16TL1425",null,"ABS Thermodichtset DZTL 360x830mm und 380x880mm","104193","0",null,"STK",{"$f":"VLOOKUP(G1985,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",26,"16TL14","Absolut16TL1426",null,"ABS Thermodichtset DZTL 360x830mm und 380x880mm","104196","0",null,"STK",{"$f":"VLOOKUP(G1986,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",27,"16TL14","Absolut16TL1427",null,"ABS Handyplatte DZTL Faserzement 360 x 830mm","104150","0",null,"STK",{"$f":"VLOOKUP(G1987,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",28,"16TL14","Absolut16TL1428",null,"ABS Handyplatte DZTL Inox 360 x 830mm","104183","0",null,"STK",{"$f":"VLOOKUP(G1988,sanschie!A:G,7,0)","v":260},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",29,"16TL14","Absolut16TL1429",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G1989,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",30,"16TL14","Absolut16TL1430",null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G1990,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",31,"16TL14","Absolut16TL1431",null,"ABS Abdeckung zu Handyplatte DZTL 130 x 260mm","104165","0",null,"STK",{"$f":"VLOOKUP(G1991,sanschie!A:G,7,0)","v":51}]
["Absolut",32,"16TL14","Absolut16TL1432",null,"ABS Zulufthaube zu Faserzementpl. DZTL 140- 200mm","104169","0",null,"STK",{"$f":"VLOOKUP(G1992,sanschie!A:G,7,0)","v":106},{"$f":"IF(Daten!$B$212=1,\"\",1)","v":1}]
["Absolut",33,"16TL14","Absolut16TL1433",null,"ABS 160 Abströmkonus verkupfert","104205","0",null,"STK",{"$f":"VLOOKUP(G1993,sanschie!A:G,7,0)","v":166}]
["Absolut",34,"16TL14","Absolut16TL1434",null,"ABS 140 Abströmkonus verkupfert","104204","0",null,"STK",{"$f":"VLOOKUP(G1994,sanschie!A:G,7,0)","v":161}]
["Absolut",{"$f":"B1994+1","v":35},{"$f":"C1994","v":"16TL14"},"Absolut16TL1435",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G1995,sanschie!A:G,7,0)","v":1900}]
["Absolut",36,"16TL14","Absolut16TL1436",null,"ABS 160 Anschlusskonus DZ mit Doppelfutter DN150mm","103902","0",null,"STK",{"$f":"VLOOKUP(G1996,sanschie!A:G,7,0)","v":256.8}]
["Absolut",37,"16TL14","Absolut16TL1437",null,"ABS 180 Adapterring von 180mm auf 160mm L90mm","103906","0",null,"STK",{"$f":"VLOOKUP(G1997,sanschie!A:G,7,0)","v":41}]
["Absolut",38,"16TL14","Absolut16TL1438",null,"ABS 180 Adapterring von 180mm auf 140mm L90mm","103905","0",null,"STK",{"$f":"VLOOKUP(G1998,sanschie!A:G,7,0)","v":35}]
["Absolut",39,"16TL14","Absolut16TL1439",null,"KER 160  Keranova-Fugenglätter","103473","0",null,"STK",{"$f":"VLOOKUP(G1999,sanschie!A:G,7,0)","v":58}]
["Absolut",40,"16TL14","Absolut16TL1440",null,"KER 140  Keranova-Fugenglätter","103472","0",null,"STK",{"$f":"VLOOKUP(G2000,sanschie!A:G,7,0)","v":57}]
["Absolut",42,"16TL14","Absolut16TL1442",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G2002,sanschie!A:G,7,0)","v":149},{"$f":"IF(M2002=0,\"\",M2002)","v":""},{"$f":"SUM(N2002:O2002)","v":0},{"$f":"IF(Daten!$B$226=4,1,0)","v":0},{"$f":"IF(Daten!$F$226=4,1,0)","v":0}]
["Absolut",43,"16TL14","Absolut16TL1443",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G2003,sanschie!A:G,7,0)","v":160},{"$f":"IF(M2003=0,\"\",M2003)","v":""},{"$f":"SUM(N2003:O2003)","v":0},{"$f":"IF(Daten!$B$226=5,1,0)","v":0},{"$f":"IF(Daten!$F$226=5,1,0)","v":0}]
["Absolut",46,"16TL14","Absolut16TL1446",null,"ABS 160 Kondensatfalle zu RA 45° Ø130mm ","104029","0",null,"STK",{"$f":"VLOOKUP(G2006,sanschie!A:G,7,0)","v":322}]
["Absolut",48,"16TL14","Absolut16TL1448",null,"ABS 160 Kondensatfalle zu RA 45° Ø160mm ","104031","0",null,"STK",{"$f":"VLOOKUP(G2008,sanschie!A:G,7,0)","v":322}]
["Absolut",52,"16TL14","Absolut16TL1452",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G2012,sanschie!A:G,7,0)","v":23},{"$f":"IF(L1967=1,2,\"\")","v":2}]
["Absolut",53,"16TL14","Absolut16TL1453",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G2013,sanschie!A:G,7,0)","v":489},{"$f":"IF(N2013=0,\"\",N2013)","v":""},null,{"$f":"SUM(O2013:P2013)","v":0},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""},{"$f":"IF(Daten!$F$241=1,\"\",1)","v":""}]
["Absolut",55,"16TL14","Absolut16TL1455",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G2015,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",58,"16TL14","Absolut16TL1458",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G2018,sanschie!A:G,7,0)","v":94},{"$f":"IF(N2018=0,\"\",N2018)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",61,"16TL14","Absolut16TL1461",null,"ABS LAS Zuluftadapter für Stirnseite","104235","0",null,"STK",{"$f":"VLOOKUP(G2021,sanschie!A:G,7,0)","v":317}]
["Absolut",63,"16TL14","Absolut16TL1463",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G2023,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",{"$f":"B2025+1","v":66},{"$f":"C2025","v":"16TL14"},"Absolut16TL1466",null,"ABS 160 Basten Standard Kupfer","104217","0",null,"STK",{"$f":"VLOOKUP(G2026,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",69,"16TL14","Absolut16TL1469",null,"ZBH 150 Verschlussbüchse weiss ØA 275mm","103836","0",null,"STK",{"$f":"VLOOKUP(G2029,sanschie!A:G,7,0)","v":115}]
["Absolut",71,"16TL14","Absolut16TL1471",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G2031,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",74,"16TL14","Absolut16TL1474",null,"ZBH 170 Verschlusszapfen 2Stk. aus Schaumstoff","103832","0",null,"STK",{"$f":"VLOOKUP(G2034,sanschie!A:G,7,0)","v":24.2}]
["Absolut",76,"16TL14","Absolut16TL1476",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G2036,sanschie!A:G,7,0)","v":538}]
["Absolut",77,"16TL14","Absolut16TL1477",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G2037,sanschie!A:G,7,0)","v":634}]
["Absolut",81,"16TL14","Absolut16TL1481",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G2041,sanschie!A:G,7,0)","v":13.8}]
["Absolut",82,"16TL14","Absolut16TL1482",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G2042,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",85,"16TL14","Absolut16TL1485",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G2045,sanschie!A:G,7,0)","v":0},2]
["Absolut",{"$f":"B2046+1","v":1},{"$f":"C2046","v":"18TL14"},{"$f":"A2047&C2047&B2047","v":"Absolut18TL141"},null,"ABS Mantelstein DZTL 360 x 830mm L330mm","103928","0",null,"STK",{"$f":"VLOOKUP(G2047,sanschie!A:G,7,0)","v":58},{"$f":"ROUND(M2047,0)-M2048","v":24},{"$f":"((M2046-M2052)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N2047*330","v":0}]
["Absolut",5,"18TL14","Absolut18TL145",null,"ABS 140 Profilkeramik-Rohr mit Muffe L1330mm","103946",1330,null,"STK",{"$f":"VLOOKUP(G2051,sanschie!A:G,7,0)","v":106},{"$f":"ROUNDUP(M2051,0)","v":5},{"$f":"(M2046-O2047-M2052-M2062-M2063-M2069)/1000/1.33","v":4.962406015037593}]
["Absolut",6,"18TL14","Absolut18TL146",null,"ABS 180 Fertigfuss DZTL 2 x Ø120-180mm L1070mm","103868",1070,null,"STK",{"$f":"VLOOKUP(G2052,sanschie!A:G,7,0)","v":1472},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L2052=\"\",0,$H2052*$L2052)","v":1070}]
["Absolut",8,"18TL14","Absolut18TL148",null,"ABS 140 Fertigfusspaket ","103889","0",null,"STK",{"$f":"VLOOKUP(G2054,sanschie!A:G,7,0)","v":311},{"$f":"L2052","v":1}]
["Absolut",11,"18TL14","Absolut18TL1411",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G2057,sanschie!A:G,7,0)","v":32},{"$f":"IF(L2052=\"\",1,\"\")","v":""}]
["Absolut",14,"18TL14","Absolut18TL1414",null,"ABS 180  Rauchrohranschluss Stutzen-Set 90° Ø180mm","104001","0",null,"STK",{"$f":"VLOOKUP(G2060,sanschie!A:G,7,0)","v":204}]
["Absolut",16,"18TL14","Absolut18TL1416",null,"ABS 140 Rauchrohr-Anschlusspaket 90° RA  ","103981",1330,null,"STK",{"$f":"VLOOKUP(G2062,sanschie!A:G,7,0)","v":355},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(L2062=0,0,IF(L2062=\"\",0,L2062*H2062))","v":1330}]
["Absolut",19,"18TL14","Absolut18TL1419",null,"ABS 140 Rauchrohranschluss Stutzen-Set 45°","104005","0",null,"STK",{"$f":"VLOOKUP(G2065,sanschie!A:G,7,0)","v":191},null,null,null,"großer Zug","kleine Zug"]
["Absolut",22,"18TL14","Absolut18TL1422",null,"ABS 180 Putztür-Anschlusspaket ","103966",1330,null,"STK",{"$f":"VLOOKUP(G2068,sanschie!A:G,7,0)","v":448},{"$f":"IF(N2068=0,\"\",N2068)","v":""},{"$f":"IF(L2068=0,0,IF(L2068=\"\",0,L2068*H2068))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",24,"18TL14","Absolut18TL1424",null,"ABS 180 Putztüranschluss Stutzen Set","104274","0",null,"STK",{"$f":"VLOOKUP(G2070,sanschie!A:G,7,0)","v":336}]
["Absolut",25,"18TL14","Absolut18TL1425",null,"ABS 140 Putztüranschluss Stutzen Set","104272","0",null,"STK",{"$f":"VLOOKUP(G2071,sanschie!A:G,7,0)","v":311}]
["Absolut",29,"18TL14","Absolut18TL1429",null,"ABS Handyplatte DZTL Faserzement 360 x 830mm","104150","0",null,"STK",{"$f":"VLOOKUP(G2075,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",30,"18TL14","Absolut18TL1430",null,"ABS Handyplatte DZTL Inox 360 x 830mm","104183","0",null,"STK",{"$f":"VLOOKUP(G2076,sanschie!A:G,7,0)","v":260},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",34,"18TL14","Absolut18TL1434",null,"ABS Zulufthaube zu Faserzementpl. DZTL 140- 200mm","104169","0",null,"STK",{"$f":"VLOOKUP(G2080,sanschie!A:G,7,0)","v":106},{"$f":"IF(Daten!$B$212=1,\"\",1)","v":1}]
["Absolut",36,"18TL14","Absolut18TL1436",null,"ABS 140 Abströmkonus verkupfert","104204","0",null,"STK",{"$f":"VLOOKUP(G2082,sanschie!A:G,7,0)","v":161}]
["Absolut",39,"18TL14","Absolut18TL1439",null,"ABS 180 Adapterring von 180mm auf 180mm L90mm","103907","0",null,"STK",{"$f":"VLOOKUP(G2085,sanschie!A:G,7,0)","v":46}]
["Absolut",40,"18TL14","Absolut18TL1440",null,"ABS 180 Adapterring von 180mm auf 140mm L90mm","103905","0",null,"STK",{"$f":"VLOOKUP(G2086,sanschie!A:G,7,0)","v":35}]
["Absolut",44,"18TL14","Absolut18TL1444",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm","104015","0",null,"STK",{"$f":"VLOOKUP(G2090,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",45,"18TL14","Absolut18TL1445",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø130mm","104016","0",null,"STK",{"$f":"VLOOKUP(G2091,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",47,"18TL14","Absolut18TL1447",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø180mm","104018","0",null,"STK",{"$f":"VLOOKUP(G2093,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",50,"18TL14","Absolut18TL1450",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G2096,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",53,"18TL14","Absolut18TL1453",null,"ABS 180 Kondensatfalle zu RA 45° Ø150mm","104033","0",null,"STK",{"$f":"VLOOKUP(G2099,sanschie!A:G,7,0)","v":347}]
["Absolut",55,"18TL14","Absolut18TL1455",null,"ABS 180 Kondensatfalle zu RA 45° Ø180mm ","104035","0",null,"STK",{"$f":"VLOOKUP(G2101,sanschie!A:G,7,0)","v":347}]
["Absolut",58,"18TL14","Absolut18TL1458",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G2104,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",61,"18TL14","Absolut18TL1461",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G2107,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",63,"18TL14","Absolut18TL1463",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G2109,sanschie!A:G,7,0)","v":14},{"$f":"IF(N2109=0,\"\",ROUNDUP(N2109,0))","v":""},null,{"$f":"SUM(O2109:P2109)","v":0},{"$f":"IF(L2050<=8,0,(L2050-8)/2)","v":0}]
["Absolut",64,"18TL14","Absolut18TL1464",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G2110,sanschie!A:G,7,0)","v":14},{"$f":"IF(N2110=0,\"\",ROUNDUP(N2110,0))","v":""},null,{"$f":"SUM(O2110:P2110)","v":0},{"$f":"IF(L2051<=8,0,(L2051-8)/2)","v":0}]
["Absolut",68,"18TL14","Absolut18TL1468",null,"ABS LAS Zuluftadapter für Längsseite","104234","0",null,"STK",{"$f":"VLOOKUP(G2114,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$249=1,\"\",1)","v":""}]
["Absolut",69,"18TL14","Absolut18TL1469",null,"ABS LAS Zuluftadapter für Stirnseite","104235","0",null,"STK",{"$f":"VLOOKUP(G2115,sanschie!A:G,7,0)","v":317}]
["Absolut",73,"18TL14","Absolut18TL1473",null,"ABS 180 Basten Standard Inox","104212","0",null,"STK",{"$f":"VLOOKUP(G2119,sanschie!A:G,7,0)","v":345},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",75,"18TL14","Absolut18TL1475",null,"ABS 180 Sairlift Inox","104224","0",null,"STK",{"$f":"VLOOKUP(G2121,sanschie!A:G,7,0)","v":400},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",78,"18TL14","Absolut18TL1478",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G2124,sanschie!A:G,7,0)","v":258.8}]
["Absolut",79,"18TL14","Absolut18TL1479",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G2125,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",83,"18TL14","Absolut18TL1483",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G2129,sanschie!A:G,7,0)","v":452}]
["Absolut",84,"18TL14","Absolut18TL1484",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G2130,sanschie!A:G,7,0)","v":538}]
["Absolut",86,"18TL14","Absolut18TL1486",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G2132,sanschie!A:G,7,0)","v":695}]
["Absolut",89,"18TL14","Absolut18TL1489",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G2135,sanschie!A:G,7,0)","v":13.8}]
["Absolut",92,"18TL14","Absolut18TL1492",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G2138,sanschie!A:G,7,0)","v":26}]
["Absolut",0,"18TL16","Absolut18TL160","P","Absolut-Kaminanlage Ø 18TL16","Absolut 18TL16","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G2140,sanschie!A:G,7,0)","v":0},null,{"$f":"I2140*1000","v":9000}]
["Absolut",4,"18TL16","Absolut18TL164",null,"ABS 180 Profilkeramik-Rohr mit Muffe L1330mm","103948",1330,null,"STK",{"$f":"VLOOKUP(G2144,sanschie!A:G,7,0)","v":122},{"$f":"ROUNDUP(M2144,0)","v":6},{"$f":"(M2140-O2141-M2146-M2152-M2153-M2161)/1000/1.33","v":5.962406015037593}]
["Absolut",5,"18TL16","Absolut18TL165",null,"ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","103947",1330,null,"STK",{"$f":"VLOOKUP(G2145,sanschie!A:G,7,0)","v":113},{"$f":"ROUNDUP(M2145,0)","v":5},{"$f":"(M2140-O2141-M2146-M2156-M2157-M2162)/1000/1.33","v":4.962406015037593}]
["Absolut",8,"18TL16","Absolut18TL168",null,"ABS 160 Fertigfusspaket ","103890","0",null,"STK",{"$f":"VLOOKUP(G2148,sanschie!A:G,7,0)","v":311},{"$f":"L2146","v":1}]
["Absolut",9,"18TL16","Absolut18TL169",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G2149,sanschie!A:G,7,0)","v":18}]
["Absolut",13,"18TL16","Absolut18TL1613",null,"ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","103995",1330,null,"STK",{"$f":"VLOOKUP(G2153,sanschie!A:G,7,0)","v":404},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""},{"$f":"IF(L2153=0,0,IF(L2153=\"\",0,L2153*H2153))","v":0}]
["Absolut",15,"18TL16","Absolut18TL1615",null,"ABS 180 Rauchrohranschluss Stutzen-Set 45°","104007","0",null,"STK",{"$f":"VLOOKUP(G2155,sanschie!A:G,7,0)","v":204}]
["Absolut",18,"18TL16","Absolut18TL1618",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø160mm","104000","0",null,"STK",{"$f":"VLOOKUP(G2158,sanschie!A:G,7,0)","v":199}]
["Absolut",20,"18TL16","Absolut18TL1620",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G2160,sanschie!A:G,7,0)","v":160},{"$f":"IF(N2160=0,\"\",N2160)","v":""},null,{"$f":"SUM(O2160:P2160)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",23,"18TL16","Absolut18TL1623",null,"ABS 180 Putztüranschluss Stutzen Set","104274","0",null,"STK",{"$f":"VLOOKUP(G2163,sanschie!A:G,7,0)","v":336}]
["Absolut",26,"18TL16","Absolut18TL1626",null,"ABS Thermodichtset DZTL 360x830mm und 380x880mm","104193","0",null,"STK",{"$f":"VLOOKUP(G2166,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",28,"18TL16","Absolut18TL1628",null,"ABS Handyplatte DZTL Faserzement 360 x 830mm","104150","0",null,"STK",{"$f":"VLOOKUP(G2168,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",29,"18TL16","Absolut18TL1629",null,"ABS Handyplatte DZTL Inox 360 x 830mm","104183","0",null,"STK",{"$f":"VLOOKUP(G2169,sanschie!A:G,7,0)","v":260},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",31,"18TL16","Absolut18TL1631",null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G2171,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",34,"18TL16","Absolut18TL1634",null,"ABS 180 Abströmkonus verkupfert","104206","0",null,"STK",{"$f":"VLOOKUP(G2174,sanschie!A:G,7,0)","v":174}]
["Absolut",37,"18TL16",{"$f":"A2177&C2177&B2177","v":"Absolut18TL1637"},null,"ABS 180 Anschlusskonus DZ mit Doppelfutter DN180mm","103903","0",null,"STK",{"$f":"VLOOKUP(G2177,sanschie!A:G,7,0)","v":260.2}]
["Absolut",39,"18TL16","Absolut18TL1639",null,"ABS 180 Adapterring von 180mm auf 160mm L90mm","103906","0",null,"STK",{"$f":"VLOOKUP(G2179,sanschie!A:G,7,0)","v":41}]
["Absolut",43,"18TL16","Absolut18TL1643",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm","104015","0",null,"STK",{"$f":"VLOOKUP(G2183,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",44,"18TL16","Absolut18TL1644",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø130mm","104016","0",null,"STK",{"$f":"VLOOKUP(G2184,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",47,"18TL16","Absolut18TL1647",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G2187,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",48,"18TL16","Absolut18TL1648",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G2188,sanschie!A:G,7,0)","v":149},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",52,"18TL16","Absolut18TL1652",null,"ABS 180 Kondensatfalle zu RA 45° Ø150mm","104033","0",null,"STK",{"$f":"VLOOKUP(G2192,sanschie!A:G,7,0)","v":347}]
["Absolut",54,"18TL16","Absolut18TL1654",null,"ABS 180 Kondensatfalle zu RA 45° Ø180mm ","104035","0",null,"STK",{"$f":"VLOOKUP(G2194,sanschie!A:G,7,0)","v":347}]
["Absolut",57,"18TL16","Absolut18TL1657",null,"ABS 160 Kondensatfalle zu RA 45° Ø160mm ","104031","0",null,"STK",{"$f":"VLOOKUP(G2197,sanschie!A:G,7,0)","v":322}]
["Absolut",59,"18TL16","Absolut18TL1659",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G2199,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",62,"18TL16","Absolut18TL1662",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G2202,sanschie!A:G,7,0)","v":489},{"$f":"IF(N2202=0,\"\",N2202)","v":""},null,{"$f":"SUM(O2202:P2202)","v":0},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""},{"$f":"IF(Daten!$F$241=1,\"\",1)","v":""}]
["Absolut",{"$f":"B2204+1","v":65},{"$f":"C2204","v":"18TL16"},"Absolut18TL1665",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G2205,sanschie!A:G,7,0)","v":14},{"$f":"IF(N2205=0,\"\",ROUNDUP(N2205,0))","v":""},null,{"$f":"SUM(O2205:P2205)","v":0},{"$f":"IF(L2144<=8,0,(L2144-8)/2)","v":0}]
["Absolut",67,"18TL16","Absolut18TL1667",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G2207,sanschie!A:G,7,0)","v":303},{"$f":"IF(N2207=0,\"\",N2207)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",68,"18TL16","Absolut18TL1668",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G2208,sanschie!A:G,7,0)","v":94},{"$f":"IF(N2208=0,\"\",N2208)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",70,"18TL16","Absolut18TL1670",null,"ABS LAS Zuluftadapter für Längsseite","104234","0",null,"STK",{"$f":"VLOOKUP(G2210,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$249=1,\"\",1)","v":""}]
["Absolut",73,"18TL16","Absolut18TL1673",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G2213,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",76,"18TL16","Absolut18TL1676",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",{"$f":"VLOOKUP(G2216,sanschie!A:G,7,0)","v":362},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",78,"18TL16","Absolut18TL1678",null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",{"$f":"VLOOKUP(G2218,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",82,"18TL16","Absolut18TL1682",null,"ABS 160 Sairlift Kupfer","104228","0",null,"STK",{"$f":"VLOOKUP(G2222,sanschie!A:G,7,0)","v":397},{"$f":"IF(Daten!$F$297=5,1,\"\")","v":""}]
["Absolut",83,"18TL16","Absolut18TL1683",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G2223,sanschie!A:G,7,0)","v":123.1}]
["Absolut",85,"18TL16","Absolut18TL1685",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G2225,sanschie!A:G,7,0)","v":258.8}]
["Absolut",88,"18TL16","Absolut18TL1688",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G2228,sanschie!A:G,7,0)","v":7.5}]
["Absolut",91,"18TL16","Absolut18TL1691",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G2231,sanschie!A:G,7,0)","v":452}]
["Absolut",93,"18TL16","Absolut18TL1693",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G2233,sanschie!A:G,7,0)","v":634}]
["Absolut",96,"18TL16","Absolut18TL1696",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G2236,sanschie!A:G,7,0)","v":873}]
["Absolut",{"$f":"B2238+1","v":99},{"$f":"C2238","v":"18TL16"},"Absolut18TL1699",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G2239,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B2240+1","v":101},{"$f":"C2240","v":"18TL16"},{"$f":"A2241&C2241&B2241","v":"Absolut18TL16101"},null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G2241,sanschie!A:G,7,0)","v":0},2]
["Absolut",{"$f":"B2243+1","v":2},{"$f":"C2243","v":"20TL14"},"Absolut20TL142",null,"ABS Thermo-Trennstein DZTL 380 x 880mm L330mm","103940","0",null,"STK",{"$f":"VLOOKUP(G2244,sanschie!A:G,7,0)","v":370},{"$f":"IF(M2244=0,\"\",M2244)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",4,"20TL14","Absolut20TL144",null,"ABS 200 Profilkeramik-Rohr mit Muffe L1330mm","103949",1330,null,"STK",{"$f":"VLOOKUP(G2246,sanschie!A:G,7,0)","v":145},{"$f":"ROUNDUP(M2246,0)","v":6},{"$f":"(M2242-O2243-M2248-M2254-M2255-M2264)/1000/1.33","v":5.962406015037593}]
["Absolut",5,"20TL14","Absolut20TL145",null,"ABS 140 Profilkeramik-Rohr mit Muffe L1330mm","103946",1330,null,"STK",{"$f":"VLOOKUP(G2247,sanschie!A:G,7,0)","v":106},{"$f":"ROUNDUP(M2247,0)","v":5},{"$f":"(M2242-O2243-M2248-M2258-M2259-M2265)/1000/1.33","v":4.962406015037593}]
["Absolut",9,"20TL14","Absolut20TL149",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G2251,sanschie!A:G,7,0)","v":18}]
["Absolut",10,"20TL14","Absolut20TL1410",null,"CHZ 200 Keramik Fuss-Scheibe geschlossen","103701","0",null,"STK",{"$f":"VLOOKUP(G2252,sanschie!A:G,7,0)","v":45},{"$f":"IF(L2248=\"\",1,\"\")","v":""}]
["Absolut",13,"20TL14","Absolut20TL1413",null,"ABS 200 Rauchrohr-Anschlusspaket 45° RA  ","103996",1330,null,"STK",{"$f":"VLOOKUP(G2255,sanschie!A:G,7,0)","v":466},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""},{"$f":"IF(L2255=0,0,IF(L2255=\"\",0,L2255*H2255))","v":0}]
["Absolut",15,"20TL14","Absolut20TL1415",null,"ABS 200 Rauchrohranschluss Stutzen-Set 45°","104008","0",null,"STK",{"$f":"VLOOKUP(G2257,sanschie!A:G,7,0)","v":212}]
["Absolut",19,"20TL14","Absolut20TL1419",null,"ABS 140 Rauchrohranschluss Stutzen-Set 45°","104005","0",null,"STK",{"$f":"VLOOKUP(G2261,sanschie!A:G,7,0)","v":191},null,null,null,"großer Zug","kleine Zug"]
["Absolut",20,"20TL14","Absolut20TL1420",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G2262,sanschie!A:G,7,0)","v":160},{"$f":"IF(N2262=0,\"\",N2262)","v":""},null,{"$f":"SUM(O2262:P2262)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",22,"20TL14","Absolut20TL1422",null,"ABS 200 Putztür-Anschlusspaket ","103967",1330,null,"STK",{"$f":"VLOOKUP(G2264,sanschie!A:G,7,0)","v":483},{"$f":"IF(N2264=0,\"\",N2264)","v":""},{"$f":"IF(L2264=0,0,IF(L2264=\"\",0,L2264*H2264))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",25,"20TL14","Absolut20TL1425",null,"ABS 140 Putztüranschluss Stutzen Set","104272","0",null,"STK",{"$f":"VLOOKUP(G2267,sanschie!A:G,7,0)","v":311}]
["Absolut",28,"20TL14","Absolut20TL1428",null,"ABS Thermodichtset DZTL 360x830mm und 380x880mm","104196","0",null,"STK",{"$f":"VLOOKUP(G2270,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",30,"20TL14","Absolut20TL1430",null,"ABS Handyplatte DZTL Inox 380 x 880mm  ","104184","0",null,"STK",{"$f":"VLOOKUP(G2272,sanschie!A:G,7,0)","v":273},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",{"$f":"B2274+1","v":33},{"$f":"C2274","v":"20TL14"},{"$f":"A2275&C2275&B2275","v":"Absolut20TL1433"},null,"ABS Abdeckung zu Handyplatte DZTL 140 x 280mm","104166","0",null,"STK",{"$f":"VLOOKUP(G2275,sanschie!A:G,7,0)","v":51}]
["Absolut",36,"20TL14","Absolut20TL1436",null,"ABS 140 Abströmkonus verkupfert","104204","0",null,"STK",{"$f":"VLOOKUP(G2278,sanschie!A:G,7,0)","v":161}]
["Absolut",38,"20TL14","Absolut20TL1438",null,"ABS 200 Anschlusskonus DZ mit Doppelfutter DN200mm","103904","0",null,"STK",{"$f":"VLOOKUP(G2280,sanschie!A:G,7,0)","v":272.89999999999998}]
["Absolut",{"$f":"B2282+1","v":41},{"$f":"C2282","v":"20TL14"},{"$f":"A2283&C2283&B2283","v":"Absolut20TL1441"},null,"KER 200  Keranova-Fugenglätter","103475","0",null,"STK",{"$f":"VLOOKUP(G2283,sanschie!A:G,7,0)","v":72}]
["Absolut",43,"20TL14","Absolut20TL1443",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø100mm","104019","0",null,"STK",{"$f":"VLOOKUP(G2285,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",44,"20TL14","Absolut20TL1444",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø120mm","104020","0",null,"STK",{"$f":"VLOOKUP(G2286,sanschie!A:G,7,0)","v":173},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""}]
["Absolut",48,"20TL14","Absolut20TL1448",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø200mm","104024","0",null,"STK",{"$f":"VLOOKUP(G2290,sanschie!A:G,7,0)","v":222},{"$f":"IF(Daten!$B$226=8,1,\"\")","v":""}]
["Absolut",49,"20TL14","Absolut20TL1449",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G2291,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",52,"20TL14","Absolut20TL1452",null,"ABS 200 Kondensatfalle zu RA 45° Ø130mm ","104036","0",null,"STK",{"$f":"VLOOKUP(G2294,sanschie!A:G,7,0)","v":365}]
["Absolut",54,"20TL14","Absolut20TL1454",null,"ABS 200 Kondensatfalle zu RA 45° Ø160mm","104038","0",null,"STK",{"$f":"VLOOKUP(G2296,sanschie!A:G,7,0)","v":365}]
["Absolut",58,"20TL14","Absolut20TL1458",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G2300,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",59,"20TL14","Absolut20TL1459",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G2301,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",61,"20TL14","Absolut20TL1461",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G2303,sanschie!A:G,7,0)","v":23},{"$f":"IF(L2249=1,2,\"\")","v":2}]
["Absolut",64,"20TL14","Absolut20TL1464",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G2306,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",67,"20TL14","Absolut20TL1467",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G2309,sanschie!A:G,7,0)","v":303},{"$f":"IF(N2309=0,\"\",N2309)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",69,"20TL14","Absolut20TL1469",null,"ZBH Revisionstüre 100 x 275 mm Alu eloxiert","103842","0",null,"STK",{"$f":"VLOOKUP(G2311,sanschie!A:G,7,0)","v":87.4},{"$f":"IF(Daten!$G$249=0,\"\",Daten!$G$249)","v":""}]
["Absolut",72,"20TL14","Absolut20TL1472",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G2314,sanschie!A:G,7,0)","v":53}]
["Absolut",75,"20TL14","Absolut20TL1475",null,"ABS 200 Basten Standard Inox","104213","0",null,"STK",{"$f":"VLOOKUP(G2317,sanschie!A:G,7,0)","v":361},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""}]
["Absolut",77,"20TL14","Absolut20TL1477",null,"ABS 200 Sairlift Inox","104225","0",null,"STK",{"$f":"VLOOKUP(G2319,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",78,"20TL14","Absolut20TL1478",null,"ABS 200 Sairlift Kupfer","104230","0",null,"STK",{"$f":"VLOOKUP(G2320,sanschie!A:G,7,0)","v":434},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""}]
["Absolut",82,"20TL14","Absolut20TL1482",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G2324,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",83,"20TL14","Absolut20TL1483",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G2325,sanschie!A:G,7,0)","v":44.9}]
["Absolut",87,"20TL14","Absolut20TL1487",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G2329,sanschie!A:G,7,0)","v":538}]
["Absolut",89,"20TL14","Absolut20TL1489",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G2331,sanschie!A:G,7,0)","v":695}]
["Absolut",92,"20TL14","Absolut20TL1492",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G2334,sanschie!A:G,7,0)","v":13.8}]
["Absolut",93,"20TL14","Absolut20TL1493",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G2335,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",0,"20TL16","Absolut20TL160","P","Absolut-Kaminanlage Ø 20TL16","Absolut 20TL16","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G2339,sanschie!A:G,7,0)","v":0},null,{"$f":"I2339*1000","v":9000}]
["Absolut",{"$f":"B2339+1","v":1},{"$f":"C2339","v":"20TL16"},"Absolut20TL161",null,"ABS Mantelstein DZTL 380 x 880mm L330mm","103929","0",null,"STK",{"$f":"VLOOKUP(G2340,sanschie!A:G,7,0)","v":60},{"$f":"ROUND(M2340,0)-M2341","v":24},{"$f":"((M2339-M2345)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N2340*330","v":0}]
["Absolut",3,"20TL16","Absolut20TL163",null,"ABS Thermo-Fussplatte DZTL 380 x 880mm","103858","0",null,"STK",{"$f":"VLOOKUP(G2342,sanschie!A:G,7,0)","v":247}]
["Absolut",6,"20TL16","Absolut20TL166",null,"ABS 180 Fertigfuss DZTL 2 x Ø200mm L1070mm","103869",1070,null,"STK",{"$f":"VLOOKUP(G2345,sanschie!A:G,7,0)","v":1472},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L2345=\"\",0,$H2345*$L2345)","v":1070}]
["Absolut",9,"20TL16","Absolut20TL169",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G2348,sanschie!A:G,7,0)","v":18}]
["Absolut",11,"20TL16","Absolut20TL1611",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G2350,sanschie!A:G,7,0)","v":32},{"$f":"IF(L2345=\"\",1,\"\")","v":""}]
["Absolut",15,"20TL16","Absolut20TL1615",null,"ABS 200 Rauchrohranschluss Stutzen-Set 45°","104008","0",null,"STK",{"$f":"VLOOKUP(G2354,sanschie!A:G,7,0)","v":212}]
["Absolut",16,"20TL16","Absolut20TL1616",null,"ABS 160 Rauchrohr-Anschlusspaket 90° RA  ","103982",1330,null,"STK",{"$f":"VLOOKUP(G2355,sanschie!A:G,7,0)","v":367},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(L2355=0,0,IF(L2355=\"\",0,L2355*H2355))","v":1330}]
["Absolut",19,"20TL16","Absolut20TL1619",null,"ABS 160 Rauchrohranschluss Stutzen-Set 45°","104006","0",null,"STK",{"$f":"VLOOKUP(G2358,sanschie!A:G,7,0)","v":199},null,null,null,"großer Zug","kleine Zug"]
["Absolut",20,"20TL16","Absolut20TL1620",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G2359,sanschie!A:G,7,0)","v":160},{"$f":"IF(N2359=0,\"\",N2359)","v":""},null,{"$f":"SUM(O2359:P2359)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",24,"20TL16","Absolut20TL1624",null,"ABS 160 Putztüranschluss Stutzen Set","104273","0",null,"STK",{"$f":"VLOOKUP(G2363,sanschie!A:G,7,0)","v":325}]
["Absolut",25,"20TL16","Absolut20TL1625",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G2364,sanschie!A:G,7,0)","v":27}]
["Absolut",29,"20TL16","Absolut20TL1629",null,"ABS Handyplatte DZTL Inox 380 x 880mm  ","104184","0",null,"STK",{"$f":"VLOOKUP(G2368,sanschie!A:G,7,0)","v":273},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",31,"20TL16",{"$f":"A2370&C2370&B2370","v":"Absolut20TL1631"},null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G2370,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",34,"20TL16","Absolut20TL1634",null,"ABS 200 Abströmkonus verkupfert","104207","0",null,"STK",{"$f":"VLOOKUP(G2373,sanschie!A:G,7,0)","v":197}]
["Absolut",35,"20TL16","Absolut20TL1635",null,"ABS 160 Abströmkonus verkupfert","104205","0",null,"STK",{"$f":"VLOOKUP(G2374,sanschie!A:G,7,0)","v":166}]
["Absolut",39,"20TL16","Absolut20TL1639",null,"ABS 180 Adapterring von 180mm auf 160mm L90mm","103906","0",null,"STK",{"$f":"VLOOKUP(G2378,sanschie!A:G,7,0)","v":41}]
["Absolut",40,"20TL16","Absolut20TL1640",null,"KER 200  Keranova-Fugenglätter","103475","0",null,"STK",{"$f":"VLOOKUP(G2379,sanschie!A:G,7,0)","v":72}]
["Absolut",{"$f":"B2380+1","v":42},{"$f":"C2380","v":"20TL16"},{"$f":"A2381&C2381&B2381","v":"Absolut20TL1642"},null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø100mm","104019","0",null,"STK",{"$f":"VLOOKUP(G2381,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""}]
["Absolut",45,"20TL16","Absolut20TL1645",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø150mm","104022","0",null,"STK",{"$f":"VLOOKUP(G2384,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""}]
["Absolut",48,"20TL16","Absolut20TL1648",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G2387,sanschie!A:G,7,0)","v":136},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",50,"20TL16","Absolut20TL1650",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G2389,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",54,"20TL16","Absolut20TL1654",null,"ABS 200 Kondensatfalle zu RA 45° Ø160mm","104038","0",null,"STK",{"$f":"VLOOKUP(G2393,sanschie!A:G,7,0)","v":365}]
["Absolut",55,"20TL16","Absolut20TL1655",null,"ABS 200 Kondensatfalle zu RA 45° Ø180mm ","104039","0",null,"STK",{"$f":"VLOOKUP(G2394,sanschie!A:G,7,0)","v":365}]
["Absolut",58,"20TL16","Absolut20TL1658",null,"ABS 160 Kondensatfalle zu RA 45° Ø150mm ","104030","0",null,"STK",{"$f":"VLOOKUP(G2397,sanschie!A:G,7,0)","v":322}]
["Absolut",59,"20TL16","Absolut20TL1659",null,"ABS 160 Kondensatfalle zu RA 45° Ø160mm ","104031","0",null,"STK",{"$f":"VLOOKUP(G2398,sanschie!A:G,7,0)","v":322}]
["Absolut",63,"20TL16","Absolut20TL1663",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G2402,sanschie!A:G,7,0)","v":23},{"$f":"IF(L2346=1,2,\"\")","v":2}]
["Absolut",{"$f":"B2403+1","v":65},{"$f":"C2403","v":"20TL16"},"Absolut20TL1665",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G2404,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",68,"20TL16","Absolut20TL1668",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G2407,sanschie!A:G,7,0)","v":14},{"$f":"IF(N2407=0,\"\",ROUNDUP(N2407,0))","v":""},null,{"$f":"SUM(O2407:P2407)","v":0},{"$f":"IF(L2344<=8,0,(L2344-8)/2)","v":0}]
["Absolut",70,"20TL16","Absolut20TL1670",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G2409,sanschie!A:G,7,0)","v":94},{"$f":"IF(N2409=0,\"\",N2409)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",73,"20TL16","Absolut20TL1673",null,"ABS LAS Zuluftadapter für Stirnseite","104235","0",null,"STK",{"$f":"VLOOKUP(G2412,sanschie!A:G,7,0)","v":317}]
["Absolut",76,"20TL16","Absolut20TL1676",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G2415,sanschie!A:G,7,0)","v":35},{"$f":"IF(N2415<=11.5,1,2)","v":1},null,{"$f":"IF(L2345=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",78,"20TL16","Absolut20TL1678",null,"ABS 200 Basten Standard Kupfer","104219","0",null,"STK",{"$f":"VLOOKUP(G2417,sanschie!A:G,7,0)","v":375},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""}]
["Absolut",79,"20TL16","Absolut20TL1679",null,"ABS 200 Sairlift Inox","104225","0",null,"STK",{"$f":"VLOOKUP(G2418,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",81,"20TL16","Absolut20TL1681",null,"ABS 160 Basten Standard Inox","104211","0",null,"STK",{"$f":"VLOOKUP(G2420,sanschie!A:G,7,0)","v":323},{"$f":"IF(Daten!$F$297=2,1,\"\")","v":""}]
["Absolut",84,"20TL16","Absolut20TL1684",null,"ABS 160 Sairlift Kupfer","104228","0",null,"STK",{"$f":"VLOOKUP(G2423,sanschie!A:G,7,0)","v":397},{"$f":"IF(Daten!$F$297=5,1,\"\")","v":""}]
["Absolut",87,"20TL16","Absolut20TL1687",null,"ZBH 150 Verschlussbüchse weiss ØA 275mm","103836","0",null,"STK",{"$f":"VLOOKUP(G2426,sanschie!A:G,7,0)","v":115}]
["Absolut",89,"20TL16","Absolut20TL1689",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G2428,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",93,"20TL16","Absolut20TL1693",null,"ZBH 170 Verschlusszapfen 2Stk. aus Schaumstoff","103832","0",null,"STK",{"$f":"VLOOKUP(G2432,sanschie!A:G,7,0)","v":24.2}]
["Absolut",94,"20TL16","Absolut20TL1694",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G2433,sanschie!A:G,7,0)","v":452}]
["Absolut",98,"20TL16","Absolut20TL1698",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G2437,sanschie!A:G,7,0)","v":797}]
["Absolut",99,"20TL16","Absolut20TL1699",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G2438,sanschie!A:G,7,0)","v":873}]
["Absolut",102,"20TL16","Absolut20TL16102",null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G2441,sanschie!A:G,7,0)","v":322}]
["Absolut",104,"20TL16","Absolut20TL16104",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G2443,sanschie!A:G,7,0)","v":0},2]
["Absolut",2,"20TL18","Absolut20TL182",null,"ABS Thermo-Trennstein DZTL 380 x 880mm L330mm","103940","0",null,"STK",{"$f":"VLOOKUP(G2446,sanschie!A:G,7,0)","v":370},{"$f":"IF(M2446=0,\"\",M2446)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",4,"20TL18","Absolut20TL184",null,"ABS 200 Profilkeramik-Rohr mit Muffe L1330mm","103949",1330,null,"STK",{"$f":"VLOOKUP(G2448,sanschie!A:G,7,0)","v":145},{"$f":"ROUNDUP(M2448,0)","v":6},{"$f":"(M2444-O2445-M2450-M2456-M2457-M2465)/1000/1.33","v":5.962406015037593}]
["Absolut",7,"20TL18","Absolut20TL187",null,"ABS 200 Fertigfusspaket ","103892","0",null,"STK",{"$f":"VLOOKUP(G2451,sanschie!A:G,7,0)","v":311},{"$f":"L2450","v":1}]
["Absolut",10,"20TL18","Absolut20TL1810",null,"CHZ 200 Keramik Fuss-Scheibe geschlossen","103701","0",null,"STK",{"$f":"VLOOKUP(G2454,sanschie!A:G,7,0)","v":45},{"$f":"IF(L2450=\"\",1,\"\")","v":""}]
["Absolut",12,"20TL18","Absolut20TL1812",null,"ABS 200 Rauchrohr-Anschlusspaket 90° RA  ","103984",1330,null,"STK",{"$f":"VLOOKUP(G2456,sanschie!A:G,7,0)","v":434},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""},{"$f":"IF(L2456=0,0,IF(L2456=\"\",0,L2456*H2456))","v":0}]
["Absolut",13,"20TL18","Absolut20TL1813",null,"ABS 200 Rauchrohr-Anschlusspaket 45° RA  ","103996",1330,null,"STK",{"$f":"VLOOKUP(G2457,sanschie!A:G,7,0)","v":466},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""},{"$f":"IF(L2457=0,0,IF(L2457=\"\",0,L2457*H2457))","v":0}]
["Absolut",17,"20TL18","Absolut20TL1817",null,"ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","103995",1330,null,"STK",{"$f":"VLOOKUP(G2461,sanschie!A:G,7,0)","v":404},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(L2461=0,0,IF(L2461=\"\",0,L2461*H2461))","v":0}]
["Absolut",18,"20TL18","Absolut20TL1818",null,"ABS 180  Rauchrohranschluss Stutzen-Set 90° Ø180mm","104001","0",null,"STK",{"$f":"VLOOKUP(G2462,sanschie!A:G,7,0)","v":204}]
["Absolut",21,"20TL18","Absolut20TL1821",null,"ABS 200 Putztür-Anschlusspaket ","103967",1330,null,"STK",{"$f":"VLOOKUP(G2465,sanschie!A:G,7,0)","v":483},{"$f":"IF(N2465=0,\"\",N2465)","v":""},{"$f":"IF(L2465=0,0,IF(L2465=\"\",0,L2465*H2465))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261)","v":0}]
["Absolut",23,"20TL18","Absolut20TL1823",null,"ABS 200 Putztüranschluss Stutzen Set","104275","0",null,"STK",{"$f":"VLOOKUP(G2467,sanschie!A:G,7,0)","v":349}]
["Absolut",27,"20TL18","Absolut20TL1827",null,"ABS Thermodichtset DZTL 360x830mm und 380x880mm","104196","0",null,"STK",{"$f":"VLOOKUP(G2471,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",28,"20TL18","Absolut20TL1828",null,"ABS Handyplatte DZTL Faserzement 380 x 880mm","104153","0",null,"STK",{"$f":"VLOOKUP(G2472,sanschie!A:G,7,0)","v":211},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",30,"20TL18","Absolut20TL1830",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G2474,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",{"$f":"B2476+1","v":33},{"$f":"C2476","v":"20TL18"},{"$f":"A2477&C2477&B2477","v":"Absolut20TL1833"},null,"ABS Zulufthaube zu Faserzementpl. DZTL 140- 200mm","104169","0",null,"STK",{"$f":"VLOOKUP(G2477,sanschie!A:G,7,0)","v":106},{"$f":"IF(Daten!$B$212=1,\"\",1)","v":1}]
["Absolut",36,"20TL18","Absolut20TL1836",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G2480,sanschie!A:G,7,0)","v":1900}]
["Absolut",38,"20TL18","Absolut20TL1838",null,"ABS 200 Adapterring von 200mm auf 200mm L90mm","103909","0",null,"STK",{"$f":"VLOOKUP(G2482,sanschie!A:G,7,0)","v":65}]
["Absolut",{"$f":"B2484+1","v":41},{"$f":"C2484","v":"20TL18"},{"$f":"A2485&C2485&B2485","v":"Absolut20TL1841"},null,"KER 180  Keranova-Fugenglätter","103474","0",null,"STK",{"$f":"VLOOKUP(G2485,sanschie!A:G,7,0)","v":61}]
["Absolut",44,"20TL18","Absolut20TL1844",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø130mm","104021","0",null,"STK",{"$f":"VLOOKUP(G2488,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""}]
["Absolut",46,"20TL18","Absolut20TL1846",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø180mm","104023","0",null,"STK",{"$f":"VLOOKUP(G2490,sanschie!A:G,7,0)","v":210},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""}]
["Absolut",49,"20TL18","Absolut20TL1849",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø120mm","104015","0",null,"STK",{"$f":"VLOOKUP(G2493,sanschie!A:G,7,0)","v":160},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",51,"20TL18","Absolut20TL1851",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø150mm","104017","0",null,"STK",{"$f":"VLOOKUP(G2495,sanschie!A:G,7,0)","v":184},{"$f":"IF(Daten!$F$226=6,1,\"\")","v":""}]
["Absolut",52,"20TL18","Absolut20TL1852",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø180mm","104018","0",null,"STK",{"$f":"VLOOKUP(G2496,sanschie!A:G,7,0)","v":198},{"$f":"IF(Daten!$F$226=7,1,\"\")","v":""}]
["Absolut",56,"20TL18","Absolut20TL1856",null,"ABS 200 Kondensatfalle zu RA 45° Ø180mm ","104039","0",null,"STK",{"$f":"VLOOKUP(G2500,sanschie!A:G,7,0)","v":365}]
["Absolut",57,"20TL18","Absolut20TL1857",null,"ABS 200 Kondensatfalle zu RA 45° Ø200mm ","104040","0",null,"STK",{"$f":"VLOOKUP(G2501,sanschie!A:G,7,0)","v":365}]
["Absolut",60,"20TL18","Absolut20TL1860",null,"ABS 180 Kondensatfalle zu RA 45° Ø160mm","104034","0",null,"STK",{"$f":"VLOOKUP(G2504,sanschie!A:G,7,0)","v":347}]
["Absolut",62,"20TL18","Absolut20TL1862",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G2506,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",66,"20TL18","Absolut20TL1866",null,"ABS Zugregler 13ZUK180/CH zu Fertigfuss","104246","0",null,"STK",{"$f":"VLOOKUP(G2510,sanschie!A:G,7,0)","v":489},{"$f":"IF(N2510=0,\"\",N2510)","v":""},null,{"$f":"SUM(O2510:P2510)","v":0},{"$f":"IF(Daten!$B$241=1,\"\",1)","v":""},{"$f":"IF(Daten!$F$241=1,\"\",1)","v":""}]
["Absolut",67,"20TL18","Absolut20TL1867",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G2511,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",69,"20TL18","Absolut20TL1869",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø180,","103944","0",null,"STK",{"$f":"VLOOKUP(G2513,sanschie!A:G,7,0)","v":14},{"$f":"IF(N2513=0,\"\",ROUNDUP(N2513,0))","v":""},null,{"$f":"SUM(O2513:P2513)","v":0},{"$f":"IF(L2448<=8,0,(L2448-8)/2)","v":0},{"$f":"IF(L2449<=8,0,(L2449-8)/2)","v":0}]
["Absolut",72,"20TL18","Absolut20TL1872",null,"ZBH Revisionstüre 100 x 275 mm Alu eloxiert","103842","0",null,"STK",{"$f":"VLOOKUP(G2516,sanschie!A:G,7,0)","v":87.4},{"$f":"IF(Daten!$G$249=0,\"\",Daten!$G$249)","v":""}]
["Absolut",74,"20TL18","Absolut20TL1874",null,"ABS LAS Zuluftadapter für Stirnseite","104235","0",null,"STK",{"$f":"VLOOKUP(G2518,sanschie!A:G,7,0)","v":317}]
["Absolut",77,"20TL18","Absolut20TL1877",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G2521,sanschie!A:G,7,0)","v":35},{"$f":"IF(N2521<=11.5,1,2)","v":1},null,{"$f":"IF(L2450=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",80,"20TL18","Absolut20TL1880",null,"ABS 200 Sairlift Inox","104225","0",null,"STK",{"$f":"VLOOKUP(G2524,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$297=4,1,\"\")","v":""}]
["Absolut",83,"20TL18","Absolut20TL1883",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",{"$f":"VLOOKUP(G2527,sanschie!A:G,7,0)","v":362},{"$f":"IF(Daten!$F$297=3,1,\"\")","v":""}]
["Absolut",85,"20TL18","Absolut20TL1885",null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",{"$f":"VLOOKUP(G2529,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$F$297=5,1,\"\")","v":""}]
["Absolut",88,"20TL18","Absolut20TL1888",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G2532,sanschie!A:G,7,0)","v":258.8}]
["Absolut",90,"20TL18","Absolut20TL1890",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G2534,sanschie!A:G,7,0)","v":44.9}]
["Absolut",91,"20TL18","Absolut20TL1891",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G2535,sanschie!A:G,7,0)","v":7.5}]
["Absolut",95,"20TL18","Absolut20TL1895",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G2539,sanschie!A:G,7,0)","v":538}]
["Absolut",97,"20TL18","Absolut20TL1897",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G2541,sanschie!A:G,7,0)","v":695}]
["Absolut",100,"20TL18","Absolut20TL18100",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G2544,sanschie!A:G,7,0)","v":13.8}]
["Absolut",{"$f":"B2544+1","v":101},{"$f":"C2544","v":"20TL18"},{"$f":"A2545&C2545&B2545","v":"Absolut20TL18101"},null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G2545,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",0,1414,{"$f":"A2549&C2549&B2549","v":"Absolut14140"},"P","Absolut-Kaminanlage Ø 1414","Absolut 1414","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G2549,sanschie!A:G,7,0)","v":0},null,{"$f":"I2549*1000","v":9000}]
["Absolut",{"$f":"B2549+1","v":1},{"$f":"C2549","v":1414},"Absolut14141",null,"ABS Mantelstein DZ 360 x 650mm L330mm","103925","0",null,"STK",{"$f":"VLOOKUP(G2550,sanschie!A:G,7,0)","v":51},{"$f":"ROUND(M2550,0)-M2551","v":24},{"$f":"((M2549-M2553)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N2550*330","v":0}]
["Absolut",3,1414,"Absolut14143",null,"ABS 140 Profilkeramik-Rohr mit Muffe L1330mm","103946",1330,null,"STK",{"$f":"VLOOKUP(G2552,sanschie!A:G,7,0)","v":106},{"$f":"ROUNDUP(M2552,0)+Q2552","v":11},{"$f":"((M2549-O2550-M2553))/1000/1.33","v":5.962406015037593},null,{"$f":"ROUNDUP(P2552,0)","v":5},{"$f":"((M2549-O2550-M2553-M2557-M2559-M2558-M2563))/1000/1.33","v":4.962406015037593},{"$f":"IF(P2552<0,ROUNDDOWN(P2552,0),ROUNDUP(P2552,0))","v":5}]
["Absolut",6,1414,"Absolut14146",null,"CHZ 120-160 Füllstein zu Schnellbaufund. L330mm","103709","0",null,"STK",{"$f":"VLOOKUP(G2555,sanschie!A:G,7,0)","v":18}]
["Absolut",9,1414,"Absolut14149",null,"ABS 140 Rauchrohr-Anschlusspaket 45° RA  ","103993",1330,null,"STK",{"$f":"VLOOKUP(G2558,sanschie!A:G,7,0)","v":355},{"$f":"IF(N2558=0,\"\",N2558)","v":""},{"$f":"IF(L2558=0,0,IF(L2558=\"\",0,L2558*H2558))","v":0},{"$f":"SUM(O2558:P2558)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",11,1414,"Absolut141411",null,"ABS 140 Rauchrohranschluss Stutzen-Set 45°","104005","0",null,"STK",{"$f":"VLOOKUP(G2560,sanschie!A:G,7,0)","v":191},null,null,null,"großer Zug","kleine Zug"]
["Absolut",14,1414,"Absolut141414",null,"ABS 140 Putztür-Anschlusspaket ","103964",1330,null,"STK",{"$f":"VLOOKUP(G2563,sanschie!A:G,7,0)","v":410},{"$f":"IF(N2563=0,\"\",N2563)","v":""},{"$f":"IF(L2563=0,0,IF(L2563=\"\",0,L2563*H2563))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261*2)","v":0}]
["Absolut",17,1414,"Absolut141417",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104192","0",null,"STK",{"$f":"VLOOKUP(G2566,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",19,1414,"Absolut141419",null,"ABS Handyplatte DZ Faserzement 360 x 650mm ","104149","0",null,"STK",{"$f":"VLOOKUP(G2568,sanschie!A:G,7,0)","v":167},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",22,1414,"Absolut141422",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G2571,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",24,1414,"Absolut141424",null,"ABS 140 Abströmkonus verkupfert","104204","0",null,"STK",{"$f":"VLOOKUP(G2573,sanschie!A:G,7,0)","v":161}]
["Absolut",25,1414,"Absolut141425",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G2574,sanschie!A:G,7,0)","v":1900}]
["Absolut",29,1414,"Absolut141429",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G2578,sanschie!A:G,7,0)","v":136},{"$f":"IF(N2578=0,\"\",N2578)","v":""},null,{"$f":"SUM(O2578:P2578)","v":0},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",31,1414,"Absolut141431",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G2580,sanschie!A:G,7,0)","v":160},{"$f":"IF(N2580=0,\"\",N2580)","v":""},null,{"$f":"SUM(O2580:P2580)","v":0},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",34,1414,"Absolut141434",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G2583,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",35,1414,"Absolut141435",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G2584,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",39,1414,"Absolut141439",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G2588,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",40,1414,"Absolut141440",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G2589,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",42,1414,"Absolut141442",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G2591,sanschie!A:G,7,0)","v":303},{"$f":"IF(N2591=0,\"\",N2591)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",45,1414,"Absolut141445",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G2594,sanschie!A:G,7,0)","v":35},{"$f":"IF(N2594<=11.5,1,2)","v":1},null,{"$f":"IF(L2553=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",48,1414,"Absolut141448",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G2597,sanschie!A:G,7,0)","v":44.9}]
["Absolut",50,1414,"Absolut141450",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G2599,sanschie!A:G,7,0)","v":452}]
["Absolut",53,1414,"Absolut141453",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G2602,sanschie!A:G,7,0)","v":695}]
["Absolut",55,1414,"Absolut141455",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G2604,sanschie!A:G,7,0)","v":873}]
["Absolut",{"$f":"B2606+1","v":58},{"$f":"C2606","v":1414},{"$f":"A2607&C2607&B2607","v":"Absolut141458"},null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G2607,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B2607+1","v":59},{"$f":"C2607","v":1414},{"$f":"A2608&C2608&B2608","v":"Absolut141459"},null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G2608,sanschie!A:G,7,0)","v":26}]
["Absolut",2,1616,"Absolut16162",null,"ABS Thermo-Trennstein DZ 360 x 650mm L330mm","103937","0",null,"STK",{"$f":"VLOOKUP(G2612,sanschie!A:G,7,0)","v":259},{"$f":"IF(M2612=0,\"\",M2612)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",3,1616,"Absolut16163",null,"ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","103947",1330,null,"STK",{"$f":"VLOOKUP(G2613,sanschie!A:G,7,0)","v":113},{"$f":"ROUNDUP(M2613,0)+Q2613","v":11},{"$f":"((M2610-O2611-M2614))/1000/1.33","v":5.962406015037593},null,{"$f":"ROUNDUP(P2613,0)","v":5},{"$f":"((M2610-O2611-M2614-M2618-M2620-M2619-M2623))/1000/1.33","v":4.962406015037593},{"$f":"IF(P2613<0,ROUNDDOWN(P2613,0),ROUNDUP(P2613,0))","v":5}]
["Absolut",7,1616,"Absolut16167",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G2617,sanschie!A:G,7,0)","v":32},{"$f":"IF(L2614=\"\",2,\"\")","v":""}]
["Absolut",9,1616,"Absolut16169",null,"ABS 160 Rauchrohr-Anschlusspaket 45° RA  ","103994",1330,null,"STK",{"$f":"VLOOKUP(G2619,sanschie!A:G,7,0)","v":367},{"$f":"IF(N2619=0,\"\",N2619)","v":""},{"$f":"IF(L2619=0,0,IF(L2619=\"\",0,L2619*H2619))","v":0},{"$f":"SUM(O2619:P2619)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",12,1616,"Absolut161612",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G2622,sanschie!A:G,7,0)","v":160},{"$f":"IF(N2622=0,\"\",N2622)","v":""},null,{"$f":"SUM(O2622:P2622)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",15,1616,"Absolut161615",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G2625,sanschie!A:G,7,0)","v":27}]
["Absolut",17,1616,"Absolut161617",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104195","0",null,"STK",{"$f":"VLOOKUP(G2627,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",{"$f":"B2627+1","v":18},{"$f":"C2627","v":1616},{"$f":"A2628&C2628&B2628","v":"Absolut161618"},null,"ABS Handyplatte DZ Faserzement 360 x 650mm ","104149","0",null,"STK",{"$f":"VLOOKUP(G2628,sanschie!A:G,7,0)","v":167},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",{"$f":"B2629+1","v":20},{"$f":"C2629","v":1616},{"$f":"A2630&C2630&B2630","v":"Absolut161620"},null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G2630,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",23,1616,"Absolut161623",null,"ABS 160 Abströmkonus verkupfert","104205","0",null,"STK",{"$f":"VLOOKUP(G2633,sanschie!A:G,7,0)","v":166}]
["Absolut",26,1616,"Absolut161626",null,"ABS 180 Adapterring von 180mm auf 160mm L90mm","103906","0",null,"STK",{"$f":"VLOOKUP(G2636,sanschie!A:G,7,0)","v":41}]
["Absolut",{"$f":"B2637+1","v":28},{"$f":"C2637","v":1616},{"$f":"A2638&C2638&B2638","v":"Absolut161628"},null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G2638,sanschie!A:G,7,0)","v":136},{"$f":"IF(N2638=0,\"\",N2638)","v":""},null,{"$f":"SUM(O2638:P2638)","v":0},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",32,1616,"Absolut161632",null,"ABS 160 Kondensatfalle zu RA 45° Ø130mm ","104029","0",null,"STK",{"$f":"VLOOKUP(G2642,sanschie!A:G,7,0)","v":322}]
["Absolut",33,1616,"Absolut161633",null,"ABS 160 Kondensatfalle zu RA 45° Ø150mm ","104030","0",null,"STK",{"$f":"VLOOKUP(G2643,sanschie!A:G,7,0)","v":322}]
["Absolut",36,1616,"Absolut161636",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G2646,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",37,1616,"Absolut161637",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G2647,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",41,1616,"Absolut161641",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G2651,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",42,1616,"Absolut161642",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G2652,sanschie!A:G,7,0)","v":14},{"$f":"IF(L2613<=16,\"\",IF(L2613<=18,1,IF(L2613<=20,2,IF(L2613<=22,3,IF(L2613<=24,4,IF(L2613<=26,5,IF(L2613<=28,5,6)))))))","v":""}]
["Absolut",46,1616,"Absolut161646",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G2656,sanschie!A:G,7,0)","v":35},{"$f":"IF(N2656<=11.5,1,2)","v":1},null,{"$f":"IF(L2614=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",48,1616,"Absolut161648",null,"ABS 160 Basten Standard Kupfer","104217","0",null,"STK",{"$f":"VLOOKUP(G2658,sanschie!A:G,7,0)","v":345},{"$f":"IF(N2658=0,\"\",N2658)","v":""},null,{"$f":"SUM(O2658:P2658)","v":0},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""},{"$f":"IF(Daten!$F$297=3,1,\"\")","v":""}]
["Absolut",51,1616,"Absolut161651",null,"ZBH 150 Verschlussbüchse weiss ØA 275mm","103836","0",null,"STK",{"$f":"VLOOKUP(G2661,sanschie!A:G,7,0)","v":115}]
["Absolut",54,1616,"Absolut161654",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G2664,sanschie!A:G,7,0)","v":44.9}]
["Absolut",56,1616,"Absolut161656",null,"ZBH 170 Verschlusszapfen 2Stk. aus Schaumstoff","103832","0",null,"STK",{"$f":"VLOOKUP(G2666,sanschie!A:G,7,0)","v":24.2}]
["Absolut",57,1616,"Absolut161657",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G2667,sanschie!A:G,7,0)","v":452}]
["Absolut",59,1616,"Absolut161659",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G2669,sanschie!A:G,7,0)","v":634}]
["Absolut",62,1616,"Absolut161662",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G2672,sanschie!A:G,7,0)","v":873}]
["Absolut",{"$f":"B2674+1","v":65},{"$f":"C2674","v":1616},{"$f":"A2675&C2675&B2675","v":"Absolut161665"},null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G2675,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B2676+1","v":67},{"$f":"C2676","v":1616},{"$f":"A2677&C2677&B2677","v":"Absolut161667"},null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G2677,sanschie!A:G,7,0)","v":0},2]
["Absolut",3,1818,"Absolut18183",null,"ABS 180 Profilkeramik-Rohr mit Muffe L1330mm","103948",1330,null,"STK",{"$f":"VLOOKUP(G2681,sanschie!A:G,7,0)","v":122},{"$f":"ROUNDUP(M2681,0)+Q2681","v":11},{"$f":"((M2678-O2679-M2682))/1000/1.33","v":5.962406015037593},null,{"$f":"ROUNDUP(P2681,0)","v":5},{"$f":"((M2678-O2679-M2682-M2686-M2688-M2687-M2691))/1000/1.33","v":4.962406015037593},{"$f":"IF(P2681<0,ROUNDDOWN(P2681,0),ROUNDUP(P2681,0))","v":5}]
["Absolut",4,1818,"Absolut18184",null,"ABS 180 Fertigfuss DZ 2 x Ø120-180mm L1070mm","103866",1070,null,"STK",{"$f":"VLOOKUP(G2682,sanschie!A:G,7,0)","v":1472},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L2682=\"\",0,$H2682*$L2682)","v":1070}]
["Absolut",8,1818,"Absolut18188",null,"ABS 180 Rauchrohr-Anschlusspaket 90° RA  ","103983",1330,null,"STK",{"$f":"VLOOKUP(G2686,sanschie!A:G,7,0)","v":386},{"$f":"IF(N2686=0,\"\",N2686)","v":1},{"$f":"IF(L2686=0,0,IF(L2686=\"\",0,L2686*H2686))","v":1330},{"$f":"SUM(O2686:P2686)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",9,1818,"Absolut18189",null,"ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","103995",1330,null,"STK",{"$f":"VLOOKUP(G2687,sanschie!A:G,7,0)","v":404},{"$f":"IF(N2687=0,\"\",N2687)","v":""},{"$f":"IF(L2687=0,0,IF(L2687=\"\",0,L2687*H2687))","v":0},{"$f":"SUM(O2687:P2687)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",12,1818,"Absolut181812",null,"ABS 180 Steckadapter ","104268","0",null,"STK",{"$f":"VLOOKUP(G2690,sanschie!A:G,7,0)","v":173},{"$f":"IF(N2690=0,\"\",N2690)","v":""},null,{"$f":"SUM(O2690:P2690)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",14,1818,"Absolut181814",null,"ABS 180 Putztüranschluss Stutzen Set","104274","0",null,"STK",{"$f":"VLOOKUP(G2692,sanschie!A:G,7,0)","v":336}]
["Absolut",17,1818,"Absolut181817",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104195","0",null,"STK",{"$f":"VLOOKUP(G2695,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",19,1818,"Absolut181819",null,"ABS Handyplatte DZ Inox 360 x 650mm","104181","0",null,"STK",{"$f":"VLOOKUP(G2697,sanschie!A:G,7,0)","v":229},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",22,1818,"Absolut181822",null,"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben","140932","0",null,"STK",{"$f":"VLOOKUP(G2700,sanschie!A:G,7,0)","v":75}]
["Absolut",25,1818,"Absolut181825",null,"ABS 180 Anschlusskonus EZ mit Doppelfutter DN180mm","103899","0",null,"STK",{"$f":"VLOOKUP(G2703,sanschie!A:G,7,0)","v":266}]
["Absolut",27,1818,"Absolut181827",null,"KER 180  Keranova-Fugenglätter","103474","0",null,"STK",{"$f":"VLOOKUP(G2705,sanschie!A:G,7,0)","v":61}]
["Absolut",28,1818,"Absolut181828",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø100mm","104014","0",null,"STK",{"$f":"VLOOKUP(G2706,sanschie!A:G,7,0)","v":149},{"$f":"IF(N2706=0,\"\",N2706)","v":""},null,{"$f":"SUM(O2706:P2706)","v":0},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",32,1818,"Absolut181832",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø180mm","104018","0",null,"STK",{"$f":"VLOOKUP(G2710,sanschie!A:G,7,0)","v":198},{"$f":"IF(N2710=0,\"\",N2710)","v":""},null,{"$f":"SUM(O2710:P2710)","v":0},{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=7,1,\"\")","v":""}]
["Absolut",33,1818,"Absolut181833",null,"ABS 180 Kondensatfalle zu RA 45° Ø130mm","104032","0",null,"STK",{"$f":"VLOOKUP(G2711,sanschie!A:G,7,0)","v":347}]
["Absolut",36,1818,"Absolut181836",null,"ABS 180 Kondensatfalle zu RA 45° Ø180mm ","104035","0",null,"STK",{"$f":"VLOOKUP(G2714,sanschie!A:G,7,0)","v":347}]
["Absolut",38,1818,"Absolut181838",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G2716,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",42,1818,"Absolut181842",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G2720,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",43,1818,"Absolut181843",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G2721,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",45,1818,"Absolut181845",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G2723,sanschie!A:G,7,0)","v":303},{"$f":"IF(N2723=0,\"\",N2723)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",48,1818,"Absolut181848",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G2726,sanschie!A:G,7,0)","v":35},{"$f":"IF(N2726<=11.5,1,2)","v":1},null,{"$f":"IF(L2682=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",50,1818,"Absolut181850",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",{"$f":"VLOOKUP(G2728,sanschie!A:G,7,0)","v":362},{"$f":"IF(N2728=0,\"\",N2728)","v":""},null,{"$f":"SUM(O2728:P2728)","v":0},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""},{"$f":"IF(Daten!$F$297=3,1,\"\")","v":""}]
["Absolut",53,1818,"Absolut181853",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G2731,sanschie!A:G,7,0)","v":123.1}]
["Absolut",56,1818,"Absolut181856",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G2734,sanschie!A:G,7,0)","v":44.9}]
["Absolut",58,1818,"Absolut181858",null,"ZBH 190 Verschlusszapfen 2Stk. aus Schaumstoff","103833","0",null,"STK",{"$f":"VLOOKUP(G2736,sanschie!A:G,7,0)","v":26.5}]
["Absolut",61,1818,"Absolut181861",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G2739,sanschie!A:G,7,0)","v":634}]
["Absolut",64,1818,"Absolut181864",null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G2742,sanschie!A:G,7,0)","v":873}]
["Absolut",{"$f":"B2743+1","v":66},{"$f":"C2743","v":1818},{"$f":"A2744&C2744&B2744","v":"Absolut181866"},null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G2744,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",{"$f":"B2744+1","v":67},{"$f":"C2744","v":1818},{"$f":"A2745&C2745&B2745","v":"Absolut181867"},null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G2745,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B2748+1","v":1},{"$f":"C2748","v":2020},"Absolut20201",null,"ABS Mantelstein DZ 380 x 710mm 2 x 200mm  L330mm ","103927","0",null,"STK",{"$f":"VLOOKUP(G2749,sanschie!A:G,7,0)","v":56},{"$f":"ROUND(M2749,0)-M2750","v":24},{"$f":"((M2748-M2752)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N2749*330","v":0}]
["Absolut",2,2020,"Absolut20202",null,"ABS Thermo-Trennstein DZ 380 x 710mm L330mm","103938","0",null,"STK",{"$f":"VLOOKUP(G2750,sanschie!A:G,7,0)","v":283},{"$f":"IF(M2750=0,\"\",M2750)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",5,2020,"Absolut20205",null,"ABS 200 Fertigfusspaket ","103892","0",null,"STK",{"$f":"VLOOKUP(G2753,sanschie!A:G,7,0)","v":311},{"$f":"IF(L2752=\"\",\"\",2)","v":2}]
["Absolut",7,2020,"Absolut20207",null,"CHZ 200 Keramik Fuss-Scheibe geschlossen","103701","0",null,"STK",{"$f":"VLOOKUP(G2755,sanschie!A:G,7,0)","v":45},{"$f":"IF(L2752=\"\",2,\"\")","v":""}]
["Absolut",11,2020,"Absolut202011",null,"ABS 200 Rauchrohranschluss Stutzen-Set 45°","104008","0",null,"STK",{"$f":"VLOOKUP(G2759,sanschie!A:G,7,0)","v":212},null,null,null,"großer Zug","kleine Zug"]
["Absolut",12,2020,"Absolut202012",null,"ABS 200 Steckadapter ","104269","0",null,"STK",{"$f":"VLOOKUP(G2760,sanschie!A:G,7,0)","v":184},{"$f":"IF(N2760=0,\"\",N2760)","v":""},null,{"$f":"SUM(O2760:P2760)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",14,2020,"Absolut202014",null,"ABS 200 Putztüranschluss Stutzen Set","104275","0",null,"STK",{"$f":"VLOOKUP(G2762,sanschie!A:G,7,0)","v":349}]
["Absolut",17,2020,"Absolut202017",null,"ABS Thermodichtset DZ 360x650mm und 380x710mm","104195","0",null,"STK",{"$f":"VLOOKUP(G2765,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",19,2020,"Absolut202019",null,"ABS Handyplatte DZ Inox 380 x 710mm","104182","0",null,"STK",{"$f":"VLOOKUP(G2767,sanschie!A:G,7,0)","v":241},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",22,2020,"Absolut202022",null,"ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",{"$f":"VLOOKUP(G2770,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",25,2020,"Absolut202025",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G2773,sanschie!A:G,7,0)","v":1900}]
["Absolut",28,2020,"Absolut202028",null,"KER 200  Keranova-Fugenglätter","103475","0",null,"STK",{"$f":"VLOOKUP(G2776,sanschie!A:G,7,0)","v":72}]
["Absolut",30,2020,"Absolut202030",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø120mm","104020","0",null,"STK",{"$f":"VLOOKUP(G2778,sanschie!A:G,7,0)","v":173},"",null,0,{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",33,2020,"Absolut202033",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø180mm","104023","0",null,"STK",{"$f":"VLOOKUP(G2781,sanschie!A:G,7,0)","v":210},"",null,0,{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=7,1,\"\")","v":""}]
["Absolut",35,2020,"Absolut202035",null,"ABS 200 Kondensatfalle zu RA 45° Ø130mm ","104036","0",null,"STK",{"$f":"VLOOKUP(G2783,sanschie!A:G,7,0)","v":365}]
["Absolut",36,2020,"Absolut202036",null,"ABS 200 Kondensatfalle zu RA 45° Ø150mm ","104037","0",null,"STK",{"$f":"VLOOKUP(G2784,sanschie!A:G,7,0)","v":365}]
["Absolut",40,2020,"Absolut202040",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G2788,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",42,2020,"Absolut202042",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G2790,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",45,2020,"Absolut202045",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G2793,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",46,2020,"Absolut202046",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G2794,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",50,2020,"Absolut202050",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G2798,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",51,2020,"Absolut202051",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G2799,sanschie!A:G,7,0)","v":35},{"$f":"IF(N2799<=11.5,1,2)","v":1},null,{"$f":"IF(L2752=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",53,2020,"Absolut202053",null,"ABS 200 Basten Standard Kupfer","104219","0",null,"STK",{"$f":"VLOOKUP(G2801,sanschie!A:G,7,0)","v":375},{"$f":"IF(N2801=0,\"\",N2801)","v":""},null,{"$f":"SUM(O2801:P2801)","v":0},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""},{"$f":"IF(Daten!$F$297=3,1,\"\")","v":""}]
["Absolut",56,2020,"Absolut202056",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G2804,sanschie!A:G,7,0)","v":123.1}]
["Absolut",59,2020,"Absolut202059",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G2807,sanschie!A:G,7,0)","v":44.9}]
["Absolut",61,2020,"Absolut202061",null,"ZBH 210 Verschlusszapfen 2Stk. aus Schaumstoff","103834","0",null,"STK",{"$f":"VLOOKUP(G2809,sanschie!A:G,7,0)","v":26.5}]
["Absolut",{"$f":"B2811+1","v":64},{"$f":"C2811","v":2020},{"$f":"A2812&C2812&B2812","v":"Absolut202064"},null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G2812,sanschie!A:G,7,0)","v":322}]
["Absolut",{"$f":"B2813+1","v":66},{"$f":"C2813","v":2020},"Absolut202066",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G2814,sanschie!A:G,7,0)","v":0},2]
["Absolut",2,"14TL14","Absolut14TL142",null,"ABS Thermo-Trennstein DZTL 360 x 830mm L330mm","103939","0",null,"STK",{"$f":"VLOOKUP(G2817,sanschie!A:G,7,0)","v":345},{"$f":"IF(M2817=0,\"\",M2817)","v":""},{"$f":"IF(Daten!$F$271=1,0,Daten!$G$271)","v":0}]
["Absolut",5,"14TL14","Absolut14TL145",null,"ABS 140 Fertigfusspaket ","103889","0",null,"STK",{"$f":"VLOOKUP(G2820,sanschie!A:G,7,0)","v":311},{"$f":"IF(L2819=\"\",\"\",2)","v":2}]
["Absolut",7,"14TL14","Absolut14TL147",null,"CHZ 160 Keramik Fuss-Scheibe geschlossen ","103699","0",null,"STK",{"$f":"VLOOKUP(G2822,sanschie!A:G,7,0)","v":32},{"$f":"IF(L2819=\"\",2,\"\")","v":""}]
["Absolut",8,"14TL14","Absolut14TL148",null,"ABS 140 Rauchrohr-Anschlusspaket 90° RA  ","103981",1330,null,"STK",{"$f":"VLOOKUP(G2823,sanschie!A:G,7,0)","v":355},{"$f":"IF(N2823=0,\"\",N2823)","v":1},{"$f":"IF(L2823=0,0,IF(L2823=\"\",0,L2823*H2823))","v":1330},{"$f":"SUM(O2823:P2823)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Absolut",12,"14TL14","Absolut14TL1412",null,"ABS 140-160 Steckadapter ","104267","0",null,"STK",{"$f":"VLOOKUP(G2827,sanschie!A:G,7,0)","v":160},{"$f":"IF(N2827=0,\"\",N2827)","v":""},null,{"$f":"SUM(O2827:P2827)","v":0},{"$f":"IF(Daten!$B$226=2,1,0)","v":0},{"$f":"IF(Daten!$F$226=2,1,\"\")","v":""}]
["Absolut",14,"14TL14","Absolut14TL1414",null,"ABS 140 Putztür-Anschlusspaket ","103964",1330,null,"STK",{"$f":"VLOOKUP(G2829,sanschie!A:G,7,0)","v":410},{"$f":"IF(N2829=0,\"\",N2829)","v":""},{"$f":"IF(L2829=0,0,IF(L2829=\"\",0,L2829*H2829))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261*2)","v":0}]
["Absolut",17,"14TL14","Absolut14TL1417",null,"ABS Thermodichtset DZTL 360x830mm und 380x880mm","104193","0",null,"STK",{"$f":"VLOOKUP(G2832,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",18,"14TL14","Absolut14TL1418",null,"ABS Thermodichtset DZTL 360x830mm und 380x880mm","104196","0",null,"STK",{"$f":"VLOOKUP(G2833,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=3,1,\"\")","v":""}]
["Absolut",22,"14TL14","Absolut14TL1422",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G2837,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",23,"14TL14","Absolut14TL1423",null,"ABS HEB-Set zu Handyplatte  Inox mit Langschrauben","104185","0",null,"STK",{"$f":"VLOOKUP(G2838,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",25,"14TL14","Absolut14TL1425",null,"ABS Zulufthaube zu Faserzementpl. DZTL 140- 200mm","104169","0",null,"STK",{"$f":"VLOOKUP(G2840,sanschie!A:G,7,0)","v":106},{"$f":"IF(Daten!$B$212=1,\"\",1)","v":1}]
["Absolut",28,"14TL14","Absolut14TL1428",null,"ABS 160 Anschlusskonus EZ mit Doppelfutter DN150mm","103898","0",null,"STK",{"$f":"VLOOKUP(G2843,sanschie!A:G,7,0)","v":241}]
["Absolut",31,"14TL14","Absolut14TL1431",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø100mm","104011","0",null,"STK",{"$f":"VLOOKUP(G2846,sanschie!A:G,7,0)","v":136},{"$f":"IF(N2846=0,\"\",N2846)","v":""},null,{"$f":"SUM(O2846:P2846)","v":0},{"$f":"IF(Daten!$B$226=3,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=3,1,\"\")","v":""}]
["Absolut",33,"14TL14","Absolut14TL1433",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø130mm","104013","0",null,"STK",{"$f":"VLOOKUP(G2848,sanschie!A:G,7,0)","v":160},{"$f":"IF(N2848=0,\"\",N2848)","v":""},null,{"$f":"SUM(O2848:P2848)","v":0},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",36,"14TL14","Absolut14TL1436",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G2851,sanschie!A:G,7,0)","v":209},{"$f":"IF(Daten!$B$279=2,1,\"\")","v":""}]
["Absolut",38,"14TL14","Absolut14TL1438",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G2853,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",41,"14TL14","Absolut14TL1441",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G2856,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",42,"14TL14","Absolut14TL1442",null,"ABS Türblatt zu Putztüre Typ 3","104244","0",null,"STK",{"$f":"VLOOKUP(G2857,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",-1))","v":""}]
["Absolut",46,"14TL14","Absolut14TL1446",null,"ZBH Revisionstüre 100 x 275 mm Alu eloxiert","103842","0",null,"STK",{"$f":"VLOOKUP(G2861,sanschie!A:G,7,0)","v":87.4},{"$f":"IF(Daten!$G$249=0,\"\",Daten!$G$249)","v":""}]
["Absolut",47,"14TL14","Absolut14TL1447",null,"ABS LAS Zuluftadapter für Längsseite","104234","0",null,"STK",{"$f":"VLOOKUP(G2862,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$249=1,\"\",1)","v":""}]
["Absolut",51,"14TL14","Absolut14TL1451",null,"ABS Dünnbettmörtel zum kleben der Steine Geb.10kg","103941","0",null,"STK",{"$f":"VLOOKUP(G2866,sanschie!A:G,7,0)","v":35},{"$f":"IF(N2866<=11.5,1,2)","v":1},null,{"$f":"IF(L2819=\"\",Daten!$B$61+1.33,Daten!$B$61)","v":9}]
["Absolut",53,"14TL14","Absolut14TL1453",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G2868,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",56,"14TL14","Absolut14TL1456",null,"LBS 150 Ignis Protect 565 x 700 mm","103820","0",null,"STK",{"$f":"VLOOKUP(G2871,sanschie!A:G,7,0)","v":452}]
["Absolut",59,"14TL14","Absolut14TL1459",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G2874,sanschie!A:G,7,0)","v":695}]
["Absolut",61,"14TL14",{"$f":"A2876&C2876&B2876","v":"Absolut14TL1461"},null,"LBS 400 Ignis Protect 565 x 700 mm","103825","0",null,"STK",{"$f":"VLOOKUP(G2876,sanschie!A:G,7,0)","v":873}]
["Absolut",62,"14TL14","Absolut14TL1462",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G2877,sanschie!A:G,7,0)","v":13.8}]
["Absolut",{"$f":"B2878+1","v":64},{"$f":"C2878","v":"14TL14"},{"$f":"A2879&C2879&B2879","v":"Absolut14TL1464"},null,"ZBH Diamantblatt für Trennscheibe  Ø230mm","103847","0",null,"STK",{"$f":"VLOOKUP(G2879,sanschie!A:G,7,0)","v":322}]
["Absolut",0,"16TL16",{"$f":"A2882&C2882&B2882","v":"Absolut16TL160"},"P","Absolut-Kaminanlage Ø 16TL16","Absolut 16TL16","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G2882,sanschie!A:G,7,0)","v":0},null,{"$f":"I2882*1000","v":9000}]
["Absolut",3,"16TL16","Absolut16TL163",null,"ABS 160 Profilkeramik-Rohr mit Muffe L1330mm","103947",1330,null,"STK",{"$f":"VLOOKUP(G2885,sanschie!A:G,7,0)","v":113},{"$f":"ROUNDUP(M2885,0)+Q2885","v":11},{"$f":"((M2882-O2883-M2886))/1000/1.33","v":5.962406015037593},null,{"$f":"ROUNDUP(P2885,0)","v":5},{"$f":"((M2882-O2883-M2886-M2890-M2892-M2891-M2895))/1000/1.33","v":4.962406015037593},{"$f":"IF(P2885<0,ROUNDDOWN(P2885,0),ROUNDUP(P2885,0))","v":5}]
["Absolut",5,"16TL16","Absolut16TL165",null,"ABS 160 Fertigfusspaket ","103890","0",null,"STK",{"$f":"VLOOKUP(G2887,sanschie!A:G,7,0)","v":311},{"$f":"IF(L2886=\"\",\"\",2)","v":2}]
["Absolut",9,"16TL16","Absolut16TL169",null,"ABS 160 Rauchrohr-Anschlusspaket 45° RA  ","103994",1330,null,"STK",{"$f":"VLOOKUP(G2891,sanschie!A:G,7,0)","v":367},{"$f":"IF(N2891=0,\"\",N2891)","v":""},{"$f":"IF(L2891=0,0,IF(L2891=\"\",0,L2891*H2891))","v":0},{"$f":"SUM(O2891:P2891)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",10,"16TL16","Absolut16TL1610",null,"ABS 160 Rauchrohranschluss Stutzen-Set 90° Ø160mm","104000","0",null,"STK",{"$f":"VLOOKUP(G2892,sanschie!A:G,7,0)","v":199}]
["Absolut",14,"16TL16","Absolut16TL1614",null,"ABS 160 Putztüranschluss Stutzen Set","104273","0",null,"STK",{"$f":"VLOOKUP(G2896,sanschie!A:G,7,0)","v":325}]
["Absolut",15,"16TL16","Absolut16TL1615",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G2897,sanschie!A:G,7,0)","v":27}]
["Absolut",18,"16TL16","Absolut16TL1618",null,"ABS Handyplatte DZTL Faserzement 360 x 830mm","104150","0",null,"STK",{"$f":"VLOOKUP(G2900,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",19,"16TL16","Absolut16TL1619",null,"ABS Handyplatte DZTL Inox 360 x 830mm","104183","0",null,"STK",{"$f":"VLOOKUP(G2901,sanschie!A:G,7,0)","v":260},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",23,"16TL16","Absolut16TL1623",null,"ABS Abdeckung zu Handyplatte DZTL 140 x 280mm","104166","0",null,"STK",{"$f":"VLOOKUP(G2905,sanschie!A:G,7,0)","v":51}]
["Absolut",25,"16TL16","Absolut16TL1625",null,"ABS 160 Abströmkonus verkupfert","104205","0",null,"STK",{"$f":"VLOOKUP(G2907,sanschie!A:G,7,0)","v":166}]
["Absolut",28,"16TL16","Absolut16TL1628",null,"ABS 180 Adapterring von 180mm auf 160mm L90mm","103906","0",null,"STK",{"$f":"VLOOKUP(G2910,sanschie!A:G,7,0)","v":41}]
["Absolut",31,"16TL16","Absolut16TL1631",null,"ABS 160 Doppelfutter zu Rauchrohranschluss Ø120mm","104012","0",null,"STK",{"$f":"VLOOKUP(G2913,sanschie!A:G,7,0)","v":149},{"$f":"IF(N2913=0,\"\",N2913)","v":""},null,{"$f":"SUM(O2913:P2913)","v":0},{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",33,"16TL16","Absolut16TL1633",null,"CHZ 150 Doppelfutter lose L150mm","103803","0",null,"STK",{"$f":"VLOOKUP(G2915,sanschie!A:G,7,0)","v":103},{"$f":"IF(N2915=0,\"\",N2915)","v":""},null,{"$f":"SUM(O2915:P2915)","v":0},{"$f":"IF(Daten!$B$226=6,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=6,1,\"\")","v":""}]
["Absolut",34,"16TL16","Absolut16TL1634",null,"ABS 160 Kondensatfalle zu RA 45° Ø130mm ","104029","0",null,"STK",{"$f":"VLOOKUP(G2916,sanschie!A:G,7,0)","v":322}]
["Absolut",38,"16TL16","Absolut16TL1638",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G2920,sanschie!A:G,7,0)","v":387},{"$f":"IF(Daten!$B$279=3,1,\"\")","v":""}]
["Absolut",39,"16TL16","Absolut16TL1639",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G2921,sanschie!A:G,7,0)","v":566},{"$f":"IF(Daten!$B$279=4,1,\"\")","v":""}]
["Absolut",42,"16TL16","Absolut16TL1642",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G2924,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",44,"16TL16","Absolut16TL1644",null,"ABS Abstandhalter - Set für 2 Keramik-Rohre Ø140,","103943","0",null,"STK",{"$f":"VLOOKUP(G2926,sanschie!A:G,7,0)","v":14},{"$f":"IF(L2885<=16,\"\",IF(L2885<=18,1,IF(L2885<=20,2,IF(L2885<=22,3,IF(L2885<=24,4,IF(L2885<=26,5,IF(L2885<=28,5,6)))))))","v":""}]
["Absolut",48,"16TL16","Absolut16TL1648",null,"ABS LAS Zuluftadapter für Längsseite","104234","0",null,"STK",{"$f":"VLOOKUP(G2930,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$249=1,\"\",1)","v":""}]
["Absolut",49,"16TL16","Absolut16TL1649",null,"ABS LAS Zuluftadapter für Stirnseite","104235","0",null,"STK",{"$f":"VLOOKUP(G2931,sanschie!A:G,7,0)","v":317}]
["Absolut",53,"16TL16","Absolut16TL1653",null,"ABS 160 Basten Standard Inox","104211","0",null,"STK",{"$f":"VLOOKUP(G2935,sanschie!A:G,7,0)","v":323},{"$f":"IF(N2935=0,\"\",N2935)","v":""},null,{"$f":"SUM(O2935:P2935)","v":0},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""},{"$f":"IF(Daten!$F$297=2,1,\"\")","v":""}]
["Absolut",54,"16TL16","Absolut16TL1654",null,"ABS 160 Basten Standard Kupfer","104217","0",null,"STK",{"$f":"VLOOKUP(G2936,sanschie!A:G,7,0)","v":345},{"$f":"IF(N2936=0,\"\",N2936)","v":""},null,{"$f":"SUM(O2936:P2936)","v":0},{"$f":"IF(Daten!$B$297=3,1,\"\")","v":""},{"$f":"IF(Daten!$F$297=3,1,\"\")","v":""}]
["Absolut",57,"16TL16","Absolut16TL1657",null,"ZBH 150 Verschlussbüchse weiss ØA 275mm","103836","0",null,"STK",{"$f":"VLOOKUP(G2939,sanschie!A:G,7,0)","v":115}]
["Absolut",59,"16TL16","Absolut16TL1659",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G2941,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",62,"16TL16","Absolut16TL1662",null,"ZBH 170 Verschlusszapfen 2Stk. aus Schaumstoff","103832","0",null,"STK",{"$f":"VLOOKUP(G2944,sanschie!A:G,7,0)","v":24.2}]
["Absolut",64,"16TL16","Absolut16TL1664",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G2946,sanschie!A:G,7,0)","v":538}]
["Absolut",{"$f":"B2948+1","v":67},{"$f":"C2948","v":"16TL16"},{"$f":"A2949&C2949&B2949","v":"Absolut16TL1667"},null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G2949,sanschie!A:G,7,0)","v":797}]
["Absolut",70,"16TL16","Absolut16TL1670",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G2952,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",72,"16TL16","Absolut16TL1672",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G2954,sanschie!A:G,7,0)","v":26}]
["Absolut",73,"16TL16","Absolut16TL1673",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G2955,sanschie!A:G,7,0)","v":0},2]
["Absolut",3,"18TL18","Absolut18TL183",null,"ABS 180 Profilkeramik-Rohr mit Muffe L1330mm","103948",1330,null,"STK",{"$f":"VLOOKUP(G2959,sanschie!A:G,7,0)","v":122},{"$f":"ROUNDUP(M2959,0)+Q2959","v":11},{"$f":"((M2956-O2957-M2960))/1000/1.33","v":5.962406015037593},null,{"$f":"ROUNDUP(P2959,0)","v":5},{"$f":"((M2956-O2957-M2960-M2964-M2966-M2965-M2969))/1000/1.33","v":4.962406015037593},{"$f":"IF(P2959<0,ROUNDDOWN(P2959,0),ROUNDUP(P2959,0))","v":5}]
["Absolut",4,"18TL18","Absolut18TL184",null,"ABS 180 Fertigfuss DZTL 2 x Ø120-180mm L1070mm","103868",1070,null,"STK",{"$f":"VLOOKUP(G2960,sanschie!A:G,7,0)","v":1472},{"$f":"IF(Daten!$B$183=1,1,\"\")","v":1},{"$f":"IF(L2960=\"\",0,$H2960*$L2960)","v":1070}]
["Absolut",7,"18TL18","Absolut18TL187",null,"CHZ 180 Keramik Fuss-Scheibe geschlossen","103700","0",null,"STK",{"$f":"VLOOKUP(G2963,sanschie!A:G,7,0)","v":35},{"$f":"IF(L2960=\"\",2,\"\")","v":""}]
["Absolut",9,"18TL18","Absolut18TL189",null,"ABS 180 Rauchrohr-Anschlusspaket 45° RA  ","103995",1330,null,"STK",{"$f":"VLOOKUP(G2965,sanschie!A:G,7,0)","v":404},{"$f":"IF(N2965=0,\"\",N2965)","v":""},{"$f":"IF(L2965=0,0,IF(L2965=\"\",0,L2965*H2965))","v":0},{"$f":"SUM(O2965:P2965)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$G$193=\"45°\",Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Absolut",13,"18TL18","Absolut18TL1813",null,"ABS 180 Putztür-Anschlusspaket ","103966",1330,null,"STK",{"$f":"VLOOKUP(G2969,sanschie!A:G,7,0)","v":448},{"$f":"IF(N2969=0,\"\",N2969)","v":""},{"$f":"IF(L2969=0,0,IF(L2969=\"\",0,L2969*H2969))","v":0},{"$f":"IF(Daten!$C$261=0,0,Daten!$C$261*2)","v":0}]
["Absolut",14,"18TL18","Absolut18TL1814",null,"ABS 180 Putztüranschluss Stutzen Set","104274","0",null,"STK",{"$f":"VLOOKUP(G2970,sanschie!A:G,7,0)","v":336}]
["Absolut",16,"18TL18","Absolut18TL1816",null,"ABS Thermodichtset DZTL 360x830mm und 380x880mm","104193","0",null,"STK",{"$f":"VLOOKUP(G2972,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",19,"18TL18","Absolut18TL1819",null,"ABS Handyplatte DZTL Inox 360 x 830mm","104183","0",null,"STK",{"$f":"VLOOKUP(G2975,sanschie!A:G,7,0)","v":260},{"$f":"IF(Daten!$B$212=3,1,\"\")","v":""}]
["Absolut",21,"18TL18","Absolut18TL1821",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G2977,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",24,"18TL18","Absolut18TL1824",null,"ABS Zulufthaube zu Faserzementpl. DZTL 140- 200mm","104169","0",null,"STK",{"$f":"VLOOKUP(G2980,sanschie!A:G,7,0)","v":106},{"$f":"IF(Daten!$B$212=1,\"\",1)","v":1}]
["Absolut",27,"18TL18","Absolut18TL1827",null,"ABS 180 Anschlusskonus EZ mit Doppelfutter DN180mm","103899","0",null,"STK",{"$f":"VLOOKUP(G2983,sanschie!A:G,7,0)","v":266}]
["Absolut",29,"18TL18","Absolut18TL1829",null,"KER 180  Keranova-Fugenglätter","103474","0",null,"STK",{"$f":"VLOOKUP(G2985,sanschie!A:G,7,0)","v":61}]
["Absolut",32,"18TL18","Absolut18TL1832",null,"ABS 180 Doppelfutter zu Rauchrohranschluss Ø130mm","104016","0",null,"STK",{"$f":"VLOOKUP(G2988,sanschie!A:G,7,0)","v":173},{"$f":"IF(N2988=0,\"\",N2988)","v":""},null,{"$f":"SUM(O2988:P2988)","v":0},{"$f":"IF(Daten!$B$226=5,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=5,1,\"\")","v":""}]
["Absolut",35,"18TL18","Absolut18TL1835",null,"ABS 180 Kondensatfalle zu RA 45° Ø130mm","104032","0",null,"STK",{"$f":"VLOOKUP(G2991,sanschie!A:G,7,0)","v":347}]
["Absolut",37,"18TL18","Absolut18TL1837",null,"ABS 180 Kondensatfalle zu RA 45° Ø160mm","104034","0",null,"STK",{"$f":"VLOOKUP(G2993,sanschie!A:G,7,0)","v":347}]
["Absolut",38,"18TL18","Absolut18TL1838",null,"ABS 180 Kondensatfalle zu RA 45° Ø180mm ","104035","0",null,"STK",{"$f":"VLOOKUP(G2994,sanschie!A:G,7,0)","v":347}]
["Absolut",42,"18TL18","Absolut18TL1842",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G2998,sanschie!A:G,7,0)","v":23},{"$f":"IF(L2961=2,2,\"\")","v":2}]
["Absolut",44,"18TL18","Absolut18TL1844",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G3000,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",47,"18TL18","Absolut18TL1847",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G3003,sanschie!A:G,7,0)","v":303},{"$f":"IF(N3003=0,\"\",N3003)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",48,"18TL18","Absolut18TL1848",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G3004,sanschie!A:G,7,0)","v":94},{"$f":"IF(N3004=0,\"\",N3004)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Absolut",52,"18TL18","Absolut18TL1852",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G3008,sanschie!A:G,7,0)","v":53}]
["Absolut",53,"18TL18","Absolut18TL1853",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G3009,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",55,"18TL18","Absolut18TL1855",null,"ABS 180 Basten Standard Inox","104212","0",null,"STK",{"$f":"VLOOKUP(G3011,sanschie!A:G,7,0)","v":345},{"$f":"IF(N3011=0,\"\",N3011)","v":""},null,{"$f":"SUM(O3011:P3011)","v":0},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""},{"$f":"IF(Daten!$F$297=2,1,\"\")","v":""}]
["Absolut",58,"18TL18",{"$f":"A3014&C3014&B3014","v":"Absolut18TL1858"},null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",{"$f":"VLOOKUP(G3014,sanschie!A:G,7,0)","v":419},{"$f":"IF(N3014=0,\"\",N3014)","v":""},null,{"$f":"SUM(O3014:P3014)","v":0},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""},{"$f":"IF(Daten!$F$297=5,1,\"\")","v":""}]
["Absolut",60,"18TL18","Absolut18TL1860",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G3016,sanschie!A:G,7,0)","v":258.8}]
["Absolut",63,"18TL18","Absolut18TL1863",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G3019,sanschie!A:G,7,0)","v":7.5}]
["Absolut",66,"18TL18","Absolut18TL1866",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G3022,sanschie!A:G,7,0)","v":538}]
["Absolut",69,"18TL18","Absolut18TL1869",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G3025,sanschie!A:G,7,0)","v":797}]
["Absolut",71,"18TL18","Absolut18TL1871",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G3027,sanschie!A:G,7,0)","v":13.8}]
["Absolut",74,"18TL18",{"$f":"A3030&C3030&B3030","v":"Absolut18TL1874"},null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G3030,sanschie!A:G,7,0)","v":26}]
["Absolut",0,"20TL20",{"$f":"A3032&C3032&B3032","v":"Absolut20TL200"},"P","Absolut-Kaminanlage Ø 20TL20","Absolut 20TL20","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G3032,sanschie!A:G,7,0)","v":0},null,{"$f":"I3032*1000","v":9000}]
["Absolut",{"$f":"B3032+1","v":1},{"$f":"C3032","v":"20TL20"},"Absolut20TL201",null,"ABS Mantelstein DZTL 380 x 880mm 2 x 200mm L330mm ","103930","0",null,"STK",{"$f":"VLOOKUP(G3033,sanschie!A:G,7,0)","v":60},{"$f":"ROUND(M3033,0)-M3034","v":24},{"$f":"((M3032-M3036)*3)/1000","v":23.79},{"$f":"IF(Daten!$B$174=2,1,0)","v":0},{"$f":"N3033*330","v":0}]
["Absolut",5,"20TL20","Absolut20TL205",null,"ABS 200 Fertigfusspaket ","103892","0",null,"STK",{"$f":"VLOOKUP(G3037,sanschie!A:G,7,0)","v":311},{"$f":"IF(L3036=\"\",\"\",2)","v":2}]
["Absolut",7,"20TL20","Absolut20TL207",null,"CHZ 200 Keramik Fuss-Scheibe geschlossen","103701","0",null,"STK",{"$f":"VLOOKUP(G3039,sanschie!A:G,7,0)","v":45},{"$f":"IF(L3036=\"\",2,\"\")","v":""}]
["Absolut",10,"20TL20","Absolut20TL2010",null,"ABS 200 Rauchrohranschluss Stutzen-Set 90° Ø200mm","104002","0",null,"STK",{"$f":"VLOOKUP(G3042,sanschie!A:G,7,0)","v":212}]
["Absolut",11,"20TL20","Absolut20TL2011",null,"ABS 200 Rauchrohranschluss Stutzen-Set 45°","104008","0",null,"STK",{"$f":"VLOOKUP(G3043,sanschie!A:G,7,0)","v":212},null,null,null,"großer Zug","kleine Zug"]
["Absolut",15,"20TL20","Absolut20TL2015",null,"ABS Dichtset zu Putztüre Typ 3","104243","0",null,"STK",{"$f":"VLOOKUP(G3047,sanschie!A:G,7,0)","v":27}]
["Absolut",16,"20TL20","Absolut20TL2016",null,"ABS Thermodichtset DZTL 360x830mm und 380x880mm","104193","0",null,"STK",{"$f":"VLOOKUP(G3048,sanschie!A:G,7,0)","v":309},{"$f":"IF(Daten!$F$280=2,1,\"\")","v":""}]
["Absolut",18,"20TL20","Absolut20TL2018",null,"ABS Handyplatte DZTL Faserzement 380 x 880mm","104153","0",null,"STK",{"$f":"VLOOKUP(G3050,sanschie!A:G,7,0)","v":211},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",21,"20TL20","Absolut20TL2021",null,"ABS HEB-Set zu Handyplatte aus Faserzement","104162","0",null,"STK",{"$f":"VLOOKUP(G3053,sanschie!A:G,7,0)","v":34},{"$f":"IF(Daten!$B$212=2,1,\"\")","v":1}]
["Absolut",24,"20TL20","Absolut20TL2024",null,"ABS Zulufthaube zu Faserzementpl. DZTL 140- 200mm","104169","0",null,"STK",{"$f":"VLOOKUP(G3056,sanschie!A:G,7,0)","v":106},{"$f":"IF(Daten!$B$212=1,\"\",1)","v":1}]
["Absolut",26,"20TL20","Absolut20TL2026",null,"ABS Schleifung DZ  0 - 35° 120 bis 200 ","104080","0",null,"STK",{"$f":"VLOOKUP(G3058,sanschie!A:G,7,0)","v":1900}]
["Absolut",29,"20TL20","Absolut20TL2029",null,"KER 200  Keranova-Fugenglätter","103475","0",null,"STK",{"$f":"VLOOKUP(G3061,sanschie!A:G,7,0)","v":72}]
["Absolut",31,"20TL20","Absolut20TL2031",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø120mm","104020","0",null,"STK",{"$f":"VLOOKUP(G3063,sanschie!A:G,7,0)","v":173},"",null,0,{"$f":"IF(Daten!$B$226=4,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=4,1,\"\")","v":""}]
["Absolut",34,"20TL20","Absolut20TL2034",null,"ABS 200 Doppelfutter zu Rauchrohranschluss Ø180mm","104023","0",null,"STK",{"$f":"VLOOKUP(G3066,sanschie!A:G,7,0)","v":210},"",null,0,{"$f":"IF(Daten!$B$226=7,1,\"\")","v":""},{"$f":"IF(Daten!$F$226=7,1,\"\")","v":""}]
["Absolut",37,"20TL20","Absolut20TL2037",null,"ABS 200 Kondensatfalle zu RA 45° Ø150mm ","104037","0",null,"STK",{"$f":"VLOOKUP(G3069,sanschie!A:G,7,0)","v":365}]
["Absolut",39,"20TL20","Absolut20TL2039",null,"ABS 200 Kondensatfalle zu RA 45° Ø180mm ","104039","0",null,"STK",{"$f":"VLOOKUP(G3071,sanschie!A:G,7,0)","v":365}]
["Absolut",40,"20TL20","Absolut20TL2040",null,"ABS 200 Kondensatfalle zu RA 45° Ø200mm ","104040","0",null,"STK",{"$f":"VLOOKUP(G3072,sanschie!A:G,7,0)","v":365}]
["Absolut",44,"20TL20","Absolut20TL2044",null,"ABS Kondensatablauf DN40 zu Fertigfuss","103870","0",null,"STK",{"$f":"VLOOKUP(G3076,sanschie!A:G,7,0)","v":23},{"$f":"IF(L3037=2,2,\"\")","v":2}]
["Absolut",46,"20TL20","Absolut20TL2046",null,"ABS Türblatt gelocht Putztüre Typ3 für Zugregler","104245","0",null,"STK",{"$f":"VLOOKUP(G3078,sanschie!A:G,7,0)","v":82},{"$f":"IF(Daten!$B$241=1,\"\",IF(Daten!$B$183=3,\"\",1))","v":""}]
["Absolut",49,"20TL20","Absolut20TL2049",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G3081,sanschie!A:G,7,0)","v":303},{"$f":"IF(N3081=0,\"\",N3081)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Absolut",52,"20TL20","Absolut20TL2052",null,"ABS LAS Zuluftadapter für Längsseite","104234","0",null,"STK",{"$f":"VLOOKUP(G3084,sanschie!A:G,7,0)","v":199},{"$f":"IF(Daten!$B$249=1,\"\",1)","v":""}]
["Absolut",54,"20TL20","Absolut20TL2054",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G3086,sanschie!A:G,7,0)","v":53}]
["Absolut",55,"20TL20","Absolut20TL2055",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G3087,sanschie!A:G,7,0)","v":19},{"$f":"IF(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)=0,\"\",(VLOOKUP(Daten!$U$35,Daten!$T:$AK,18,0)))","v":""}]
["Absolut",57,"20TL20","Absolut20TL2057",null,"ABS 200 Basten Standard Inox","104213","0",null,"STK",{"$f":"VLOOKUP(G3089,sanschie!A:G,7,0)","v":361},{"$f":"IF(N3089=0,\"\",N3089)","v":""},null,{"$f":"SUM(O3089:P3089)","v":0},{"$f":"IF(Daten!$B$297=2,1,\"\")","v":""},{"$f":"IF(Daten!$F$297=2,1,\"\")","v":""}]
["Absolut",60,"20TL20","Absolut20TL2060",null,"ABS 200 Sairlift Kupfer","104230","0",null,"STK",{"$f":"VLOOKUP(G3092,sanschie!A:G,7,0)","v":434},{"$f":"IF(N3092=0,\"\",N3092)","v":""},null,{"$f":"SUM(O3092:P3092)","v":0},{"$f":"IF(Daten!$B$297=5,1,\"\")","v":""},{"$f":"IF(Daten!$F$297=5,1,\"\")","v":""}]
["Absolut",63,"20TL20","Absolut20TL2063",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G3095,sanschie!A:G,7,0)","v":67.900000000000006}]
["Absolut",{"$f":"B3096+1","v":65},{"$f":"C3096","v":"20TL20"},"Absolut20TL2065",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G3097,sanschie!A:G,7,0)","v":7.5}]
["Absolut",{"$f":"B3099+1","v":68},{"$f":"C3099","v":"20TL20"},"Absolut20TL2068",null,"ZBH Diamantblatt für Trennscheibe  Ø115mm","103846","0",null,"STK",{"$f":"VLOOKUP(G3100,sanschie!A:G,7,0)","v":162.19999999999999}]
["Absolut",{"$f":"B3101+1","v":70},{"$f":"C3101","v":"20TL20"},"Absolut20TL2070",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G3102,sanschie!A:G,7,0)","v":26}]
[{"$f":"A3104","v":"Cheminee"},{"$f":"B3104+1","v":1},{"$f":"C3104","v":16},"Cheminee161",null,"CHZ Mantelstein EZ  320 x 320mm L330mm Ø160mm","103719","0",null,"STK",{"$f":"VLOOKUP(G3105,sanschie!A:G,7,0)","v":22},{"$f":"ROUND(M3105,0)","v":27},{"$f":"((M3104)*3)/1000","v":27}]
[{"$f":"A3105","v":"Cheminee"},{"$f":"B3105+1","v":2},{"$f":"C3105","v":16},"Cheminee162",null,"CHZ 160 Keramikrohr ØA 190mm  L330mm","103734",330,null,"STK",{"$f":"VLOOKUP(G3106,sanschie!A:G,7,0)","v":22},{"$f":"ROUND(M3106,0)","v":24},{"$f":"((M3104+N3106-M3113-M3112-M3110-N3109))/1000*3","v":24},330]
["Cheminee",6,16,"Cheminee166",null,"CHZ 160 Keramik-Putztüranschluss PA L660mm","103764",665,null,"STK",{"$f":"VLOOKUP(G3110,sanschie!A:G,7,0)","v":112},{"$f":"IF(O3110=0,\"\",O3110)","v":1},{"$f":"IF(O3110=0,0,IF(O3110=\"\",0,O3110*H3110))","v":665},null,{"$f":"(IF(Daten!$C$261=0,P3110,Daten!$C$261+P3110))","v":1},{"$f":"IF(Daten!$C$344=0,0,Daten!$C$344)","v":1}]
["Cheminee",7,16,"Cheminee167",null,"CHZ Putztüre Typ 3 mit Innendeckel","104634","0",null,"STK",{"$f":"VLOOKUP(G3111,sanschie!A:G,7,0)","v":153},{"$f":"IF(O3111=0,\"\",O3111)","v":1},null,null,{"$f":"(IF(Daten!$C$261=0,P3111,Daten!$C$261+P3111))","v":1},{"$f":"IF(Daten!$C$344=0,0,Daten!$C$344)","v":1}]
["Cheminee",11,16,"Cheminee1611",null,"CHZ 160 Keramik Rauchrohrstutzen 45° für RA  lose","140796","0",null,"STK",{"$f":"VLOOKUP(G3115,sanschie!A:G,7,0)","v":75}]
["Cheminee",13,16,"Cheminee1613",null,"CHZ 160 Anschlusskonus mit Doppelfutter DN150mm","103693","0",null,"STK",{"$f":"VLOOKUP(G3117,sanschie!A:G,7,0)","v":265},{"$f":"IF(Daten!$B$320=2,1,\"\")","v":""}]
["Cheminee",16,16,"Cheminee1616",null,"Kombi-Mündungs-Manchette 16/58","104472","0",null,"STK",{"$f":"VLOOKUP(G3120,sanschie!A:G,7,0)","v":145},{"$f":"IF(Daten!$B$308=1,1,\"\")","v":1}]
["Cheminee",19,16,"Cheminee1619",null,"CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",{"$f":"VLOOKUP(G3123,sanschie!A:G,7,0)","v":61},1]
["Cheminee",21,16,"Cheminee1621",null,"CHZ 130 Doppelfutter lose L150mm","103802","0",null,"STK",{"$f":"VLOOKUP(G3125,sanschie!A:G,7,0)","v":99}]
["Cheminee",22,16,"Cheminee1622",null,"Doppelfutterrohr Einbau Werks.","104536","0",null,"STK",{"$f":"VLOOKUP(G3126,sanschie!A:G,7,0)","v":106}]
["Cheminee",24,16,"Cheminee1624",null,"Rahmentüre 30/40 gelocht","104542","0",null,"STK",{"$f":"VLOOKUP(G3128,sanschie!A:G,7,0)","v":205}]
["Cheminee",27,16,"Cheminee1627",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G3131,sanschie!A:G,7,0)","v":566}]
["Cheminee",30,16,"Cheminee1630",null,"CHZ 160 Kaminschleifung 0-35° EZ komplett ","103769","0",null,"STK",{"$f":"VLOOKUP(G3134,sanschie!A:G,7,0)","v":1010}]
["Cheminee",32,16,"Cheminee1632",null,"Zugreglerpaket PT12/18 EXE","104577","0",null,"STK",{"$f":"VLOOKUP(G3136,sanschie!A:G,7,0)","v":390}]
["Cheminee",35,16,"Cheminee1635",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G3139,sanschie!A:G,7,0)","v":44.9}]
["Cheminee",37,16,"Cheminee1637",null,"ZBH 170 Verschlusszapfen 2Stk. aus Schaumstoff","103832","0",null,"STK",{"$f":"VLOOKUP(G3141,sanschie!A:G,7,0)","v":24.2}]
["Cheminee",41,16,"Cheminee1641",null,"ABS 160 Sairlift Kupfer","104228","0",null,"STK",{"$f":"VLOOKUP(G3145,sanschie!A:G,7,0)","v":397},{"$f":"IF(Daten!$B$308=5,1,\"\")","v":""}]
["Cheminee",42,16,"Cheminee1642",null,"ZBH 160 Verschlussbüchse weiss ØA 275mm","103837","0",null,"STK",{"$f":"VLOOKUP(G3146,sanschie!A:G,7,0)","v":115}]
["Cheminee",45,16,"Cheminee1645",null,"LBS 250 Ignis Protect 565 x 700 mm","103822","0",null,"STK",{"$f":"VLOOKUP(G3149,sanschie!A:G,7,0)","v":634}]
["Cheminee",46,16,"Cheminee1646",null,"LBS 300 Ignis Protect 565 x 700 mm","103823","0",null,"STK",{"$f":"VLOOKUP(G3150,sanschie!A:G,7,0)","v":695}]
["Cheminee",50,16,"Cheminee1650",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G3154,sanschie!A:G,7,0)","v":0},2]
[{"$f":"A3155","v":"Cheminee"},{"$f":"B3155+1","v":1},{"$f":"C3155","v":18},"Cheminee181",null,"CHZ Mantelstein EZ 360 x 360mm L330mm Ø180-200mm","103720","0",null,"STK",{"$f":"VLOOKUP(G3156,sanschie!A:G,7,0)","v":23},{"$f":"ROUND(M3156,0)","v":27},{"$f":"((M3155)*3)/1000","v":27}]
["Cheminee",4,18,"Cheminee184",null,"CHZ 180 Schnellbau-Fundament Set ","103706","0",null,"STK",{"$f":"VLOOKUP(G3159,sanschie!A:G,7,0)","v":58},{"$f":"IF(Daten!$B$320=2,\"\",1)","v":1}]
["Cheminee",7,18,{"$f":"A3162&C3162&B3162","v":"Cheminee187"},null,"CHZ Putztüre Typ 3 mit Innendeckel","104634","0",null,"STK",{"$f":"VLOOKUP(G3162,sanschie!A:G,7,0)","v":153},{"$f":"IF(O3162=0,\"\",O3162)","v":1},null,null,{"$f":"(IF(Daten!$C$261=0,P3162,Daten!$C$261+P3162))","v":1},{"$f":"IF(Daten!$C$344=0,0,Daten!$C$344)","v":1}]
["Cheminee",9,18,"Cheminee189",null,"CHZ 180 Keramik T-Stück 45° für RA L660mm","103760",665,null,"STK",{"$f":"VLOOKUP(G3164,sanschie!A:G,7,0)","v":194},{"$f":"IF(N3164=0,\"\",N3164)","v":""},{"$f":"IF(L3164=0,0,IF(L3164=\"\",0,L3164*H3164))","v":0},{"$f":"SUM(O3164:P3164)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$F$193=2,Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Cheminee",10,18,"Cheminee1810",null,"CHZ 180 Keramik Rauchrohrstutzen 90° für RA  lose","140794","0",null,"STK",{"$f":"VLOOKUP(G3165,sanschie!A:G,7,0)","v":82}]
["Cheminee",14,18,"Cheminee1814",null,"CHZ 160 Abdeckplatte Beton 580 x 580mm Loch ?200mm","103780","0",null,"STK",{"$f":"VLOOKUP(G3169,sanschie!A:G,7,0)","v":172},{"$f":"IF(Daten!$B$354=1,\"\",IF(Daten!$B$354=2,1,\"\"))","v":1}]
["Cheminee",15,18,"Cheminee1815",null,"CHZ 180 Mündungsmanchette mit Tablett 350 x 350mm","103809","0",null,"STK",{"$f":"VLOOKUP(G3170,sanschie!A:G,7,0)","v":171}]
["Cheminee",18,18,"Cheminee1818",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G3173,sanschie!A:G,7,0)","v":13.8}]
["Cheminee",20,18,"Cheminee1820",null,"CHZ 130 Doppelfutter lose L150mm","103802","0",null,"STK",{"$f":"VLOOKUP(G3175,sanschie!A:G,7,0)","v":99}]
["Cheminee",24,18,"Cheminee1824",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G3179,sanschie!A:G,7,0)","v":387}]
["Cheminee",25,18,"Cheminee1825",null,"ABS Armierungs-Set 4 x 6000mm für Mantelsteine","104253","0",null,"STK",{"$f":"VLOOKUP(G3180,sanschie!A:G,7,0)","v":566}]
["Cheminee",29,18,"Cheminee1829",null,"CHZ 180 Kaminschleifung 0-35° EZ komplett ","103770","0",null,"STK",{"$f":"VLOOKUP(G3184,sanschie!A:G,7,0)","v":1010}]
["Cheminee",30,18,"Cheminee1830",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G3185,sanschie!A:G,7,0)","v":53}]
["Cheminee",32,18,"Cheminee1832",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G3187,sanschie!A:G,7,0)","v":258.8}]
["Cheminee",35,18,"Cheminee1835",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G3190,sanschie!A:G,7,0)","v":7.5}]
["Cheminee",38,18,"Cheminee1838",null,"ABS 180 Basten Standard Kupfer","104218","0",null,"STK",{"$f":"VLOOKUP(G3193,sanschie!A:G,7,0)","v":362},{"$f":"IF(Daten!$B$308=3,1,\"\")","v":""}]
["Cheminee",40,18,"Cheminee1840",null,"ABS 180 Sairlift Kupfer","104229","0",null,"STK",{"$f":"VLOOKUP(G3195,sanschie!A:G,7,0)","v":419},{"$f":"IF(Daten!$B$308=5,1,\"\")","v":""}]
["Cheminee",43,18,"Cheminee1843",null,"LBS 200 Ignis Protect 565 x 700 mm","103821","0",null,"STK",{"$f":"VLOOKUP(G3198,sanschie!A:G,7,0)","v":538}]
["Cheminee",46,18,"Cheminee1846",null,"LBS 350 Ignis Protect 565 x 700 mm","103824","0",null,"STK",{"$f":"VLOOKUP(G3201,sanschie!A:G,7,0)","v":797}]
["Cheminee",48,18,"Cheminee1848",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G3203,sanschie!A:G,7,0)","v":26}]
["Cheminee",49,18,"Cheminee1849",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G3204,sanschie!A:G,7,0)","v":0},2]
["Cheminee",3,20,"Cheminee203",null,"CHZ 200 Isoliermatte 2Stk. pro Rohr L330mm","103746","0",null,"STK",{"$f":"VLOOKUP(G3208,sanschie!A:G,7,0)","v":13},{"$f":"(L3206-M3210+N3208)*2","v":56},{"$f":"I3205","v":9},1]
["Cheminee",4,20,"Cheminee204",null,"CHZ 200 Schnellbau-Fundament Set ","103707","0",null,"STK",{"$f":"VLOOKUP(G3209,sanschie!A:G,7,0)","v":68},{"$f":"IF(Daten!$B$320=2,\"\",1)","v":1}]
["Cheminee",7,20,"Cheminee207",null,"CHZ Putztüre Typ 3 mit Innendeckel","104634","0",null,"STK",{"$f":"VLOOKUP(G3212,sanschie!A:G,7,0)","v":153},{"$f":"IF(O3212=0,\"\",O3212)","v":1},null,null,{"$f":"(IF(Daten!$C$261=0,P3212,Daten!$C$261+P3212))","v":1},{"$f":"IF(Daten!$C$344=0,0,Daten!$C$344)","v":1}]
["Cheminee",9,20,"Cheminee209",null,"CHZ 200 Keramik T-Stück 45° für RA L660mm","103761",665,null,"STK",{"$f":"VLOOKUP(G3214,sanschie!A:G,7,0)","v":209},{"$f":"IF(N3214=0,\"\",N3214)","v":""},{"$f":"IF(L3214=0,0,IF(L3214=\"\",0,L3214*H3214))","v":0},{"$f":"SUM(O3214:P3214)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$F$193=2,Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Cheminee",13,20,"Cheminee2013",null,"CHZ 200 Anschlusskonus mit Doppelfutter DN200mm","103695","0",null,"STK",{"$f":"VLOOKUP(G3218,sanschie!A:G,7,0)","v":281},{"$f":"IF(Daten!$B$320=2,1,\"\")","v":""}]
["Cheminee",14,20,"Cheminee2014",null,"CHZ 160 Abdeckplatte Beton 580 x 580mm Loch ?200mm","103780","0",null,"STK",{"$f":"VLOOKUP(G3219,sanschie!A:G,7,0)","v":172},{"$f":"IF(Daten!$B$354=1,\"\",IF(Daten!$B$354=2,1,\"\"))","v":1}]
["Cheminee",18,20,"Cheminee2018",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G3223,sanschie!A:G,7,0)","v":13.8}]
["Cheminee",19,20,"Cheminee2019",null,"CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",{"$f":"VLOOKUP(G3224,sanschie!A:G,7,0)","v":61},1]
["Cheminee",21,20,{"$f":"A3226&C3226&B3226","v":"Cheminee2021"},null,"Doppelfutterrohr Einbau Werks.","104536","0",null,"STK",{"$f":"VLOOKUP(G3226,sanschie!A:G,7,0)","v":106}]
["Cheminee",24,20,"Cheminee2024",null,"ABS Armierungs-Set 4 x 4000mm für Mantelsteine","104252","0",null,"STK",{"$f":"VLOOKUP(G3229,sanschie!A:G,7,0)","v":387}]
["Cheminee",27,20,"Cheminee2027",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G3232,sanschie!A:G,7,0)","v":303},{"$f":"IF(N3232=0,\"\",N3232)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Cheminee",29,20,"Cheminee2029",null,"CHZ 200 Kaminschleifung 0-35° EZ komplett ","103771","0",null,"STK",{"$f":"VLOOKUP(G3234,sanschie!A:G,7,0)","v":1134}]
["Cheminee",32,20,"Cheminee2032",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G3237,sanschie!A:G,7,0)","v":258.8}]
["Cheminee",35,20,"Cheminee2035",null,"Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",{"$f":"VLOOKUP(G3240,sanschie!A:G,7,0)","v":7.5}]
["Cheminee",37,20,"Cheminee2037",null,"ABS 200 Basten Standard Inox","104213","0",null,"STK",{"$f":"VLOOKUP(G3242,sanschie!A:G,7,0)","v":361},{"$f":"IF(Daten!$B$308=2,1,\"\")","v":""}]
["Cheminee",38,20,"Cheminee2038",null,"ABS 200 Basten Standard Kupfer","104219","0",null,"STK",{"$f":"VLOOKUP(G3243,sanschie!A:G,7,0)","v":375},{"$f":"IF(Daten!$B$308=3,1,\"\")","v":""}]
["Cheminee",42,20,"Cheminee2042",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G3247,sanschie!A:G,7,0)","v":26}]
["Cheminee",0,25,"Cheminee250","P","CHEMINEE-Kaminanlage Ø 25","CHEMINEE 25","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G3249,sanschie!A:G,7,0)","v":0},null,{"$f":"I3249*1000","v":9000}]
["Cheminee",3,25,"Cheminee253",null,"CHZ 250 Isoliermatte 2Stk. pro Rohr L330mm","103747","0",null,"STK",{"$f":"VLOOKUP(G3252,sanschie!A:G,7,0)","v":15},{"$f":"(L3250-M3254+N3252)*2","v":56},{"$f":"I3249","v":9},1]
["Cheminee",4,25,"Cheminee254",null,"CHZ 250 Schnellbau-Fundament Set ","103708","0",null,"STK",{"$f":"VLOOKUP(G3253,sanschie!A:G,7,0)","v":121},{"$f":"IF(Daten!$B$320=2,\"\",1)","v":1}]
["Cheminee",8,25,"Cheminee258",null,"CHZ 250 Keramik T-Stück 90° für RA L660mm","103753",665,null,"STK",{"$f":"VLOOKUP(G3257,sanschie!A:G,7,0)","v":285},{"$f":"IF(N3257=0,\"\",N3257)","v":1},{"$f":"IF(L3257=0,0,IF(L3257=\"\",0,L3257*H3257))","v":665},{"$f":"SUM(O3257:P3257)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$F$193=2,\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Cheminee",9,25,"Cheminee259",null,"CHZ 250 Keramik T-Stück 45° für RA L660mm","103762",665,null,"STK",{"$f":"VLOOKUP(G3258,sanschie!A:G,7,0)","v":285},{"$f":"IF(N3258=0,\"\",N3258)","v":""},{"$f":"IF(L3258=0,0,IF(L3258=\"\",0,L3258*H3258))","v":0},{"$f":"SUM(O3258:P3258)","v":0},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$F$193=2,Daten!$C$193,\"\"))","v":""},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",Daten!$C$202,\"\"))","v":""}]
["Cheminee",11,25,"Cheminee2511",null,"ABS 250 Anschlusskonus EZ mit Doppelfutter DN250mm","103901","0",null,"STK",{"$f":"VLOOKUP(G3260,sanschie!A:G,7,0)","v":365},{"$f":"IF(Daten!$B$320=2,1,\"\")","v":""}]
["Cheminee",14,25,"Cheminee2514",null,"CHZ 250 Mündungsmanchette mit Tablett 420 x 420mm","103811","0",null,"STK",{"$f":"VLOOKUP(G3263,sanschie!A:G,7,0)","v":213}]
["Cheminee",16,25,"Cheminee2516",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G3265,sanschie!A:G,7,0)","v":19},{"$f":"ROUNDUP(N3265,0)","v":6},null,{"$f":"I3249/1.5","v":6},"Verbrauch 1Kartusche 2 m"]
["Cheminee",19,25,"Cheminee2519",null,"CHZ 250 Grundpaket inhalt: Sockel, Frontplatte,","103715","0",null,"STK",{"$f":"VLOOKUP(G3268,sanschie!A:G,7,0)","v":341}]
["Cheminee",22,25,"Cheminee2522",null,"CHZ Rahmentüre 300 x 400mm ","103816","0",null,"STK",{"$f":"VLOOKUP(G3271,sanschie!A:G,7,0)","v":198}]
["Cheminee",24,25,"Cheminee2524",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G3273,sanschie!A:G,7,0)","v":209}]
["Cheminee",27,25,"Cheminee2527",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G3276,sanschie!A:G,7,0)","v":303},{"$f":"IF(N3276=0,\"\",N3276)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Cheminee",30,25,"Cheminee2530",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G3279,sanschie!A:G,7,0)","v":53}]
["Cheminee",32,25,"Cheminee2532",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G3281,sanschie!A:G,7,0)","v":258.8}]
["Cheminee",33,25,"Cheminee2533",null,"Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",{"$f":"VLOOKUP(G3282,sanschie!A:G,7,0)","v":67.900000000000006}]
["Cheminee",37,25,"Cheminee2537",null,"ABS 250 Basten Standard Inox","104214","0",null,"STK",{"$f":"VLOOKUP(G3286,sanschie!A:G,7,0)","v":400},{"$f":"IF(Daten!$B$308=2,1,\"\")","v":""}]
["Cheminee",39,25,"Cheminee2539",null,"ABS 250 Sairlift Inox","104226","0",null,"STK",{"$f":"VLOOKUP(G3288,sanschie!A:G,7,0)","v":465},{"$f":"IF(Daten!$B$308=4,1,\"\")","v":""}]
["Cheminee",42,25,"Cheminee2542",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G3291,sanschie!A:G,7,0)","v":26}]
["Cheminee",43,25,"Cheminee2543",null,"Euro Paletten im Austausch","104261","0",null,"STK",{"$f":"VLOOKUP(G3292,sanschie!A:G,7,0)","v":0},2]
["Cheminee",3,30,"Cheminee303",null,"CHZ 300 Isoliermatte 2Stk. pro Rohr L330mm","103748","0",null,"STK",{"$f":"VLOOKUP(G3296,sanschie!A:G,7,0)","v":18},{"$f":"(L3294+N3296)*2","v":56},{"$f":"I3293","v":9},1]
["Cheminee",4,30,"Cheminee304",null,"CHZ 300 Keramik-Putztüranschluss PA L660mm","103768",665,null,"STK",{"$f":"VLOOKUP(G3297,sanschie!A:G,7,0)","v":167},{"$f":"IF(O3297=0,\"\",O3297)","v":1},{"$f":"IF(O3297=0,0,IF(O3297=\"\",0,O3297*H3297))","v":665},null,{"$f":"(IF(Daten!$C$261=0,P3297,Daten!$C$261+P3297))","v":1},{"$f":"IF(Daten!$C$344=0,0,Daten!$C$344)","v":1}]
["Cheminee",6,30,"Cheminee306",null,"CHZ 300 Keramik T-Stück 90° für RA L660mm","103754",665,null,"STK",{"$f":"VLOOKUP(G3299,sanschie!A:G,7,0)","v":348},{"$f":"IF(N3299=0,\"\",N3299)","v":1},{"$f":"IF(L3299=0,0,IF(L3299=\"\",0,L3299*H3299))","v":665},{"$f":"SUM(O3299:P3299)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$F$193=2,\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Cheminee",9,30,"Cheminee309",null,"ABS 300 Anschlusskonus EZ mit Doppelfutter DN300mm","103697","0",null,"STK",{"$f":"VLOOKUP(G3302,sanschie!A:G,7,0)","v":414},{"$f":"IF(Daten!$B$320=2,1,\"\")","v":""}]
["Cheminee",11,30,"Cheminee3011",null,"ABS Handyplatte EZ Faserzement 550 x 550mm","104147","0",null,"STK",{"$f":"VLOOKUP(G3304,sanschie!A:G,7,0)","v":156}]
["Cheminee",14,30,"Cheminee3014",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G3307,sanschie!A:G,7,0)","v":19},{"$f":"ROUNDUP(N3307,0)","v":9},null,{"$f":"I3293/1","v":9},"Verbrauch 1Kartusche 2 m"]
["Cheminee",17,30,"Cheminee3017",null,"CHZ 300 Grundpaket inhalt: Sockel, Frontplatte,","103716","0",null,"STK",{"$f":"VLOOKUP(G3310,sanschie!A:G,7,0)","v":413},1]
["Cheminee",19,30,"Cheminee3019",null,"Doppelfutterrohr Einbau Werks.","104536","0",null,"STK",{"$f":"VLOOKUP(G3312,sanschie!A:G,7,0)","v":106}]
["Cheminee",22,30,"Cheminee3022",null,"ABS Armierungs-Set 2 x 4000mm für Mantelsteine","104251","0",null,"STK",{"$f":"VLOOKUP(G3315,sanschie!A:G,7,0)","v":209}]
["Cheminee",25,30,"Cheminee3025",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G3318,sanschie!A:G,7,0)","v":303},{"$f":"IF(N3318=0,\"\",N3318)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Cheminee",27,30,"Cheminee3027",null,"CHZ 300 Kaminschleifung 0-35° EZ komplett ","103773","0",null,"STK",{"$f":"VLOOKUP(G3320,sanschie!A:G,7,0)","v":1973}]
["Cheminee",28,30,"Cheminee3028",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G3321,sanschie!A:G,7,0)","v":53}]
["Cheminee",32,30,"Cheminee3032",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G3325,sanschie!A:G,7,0)","v":44.9}]
["Cheminee",34,30,"Cheminee3034",null,"ABS 300 Basten Standard Inox","104215","0",null,"STK",{"$f":"VLOOKUP(G3327,sanschie!A:G,7,0)","v":535},{"$f":"IF(Daten!$B$308=2,1,\"\")","v":""}]
["Cheminee",37,30,"Cheminee3037",null,"ABS 300 Sairlift Kupfer","104232","0",null,"STK",{"$f":"VLOOKUP(G3330,sanschie!A:G,7,0)","v":633},{"$f":"IF(Daten!$B$308=52,1,\"\")","v":""}]
["Cheminee",0,2020,"Cheminee20200","P","CHEMINEE-Kaminanlage Ø 2020","CHEMINEE 2020","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G3333,sanschie!A:G,7,0)","v":0},null,{"$f":"I3333*1000","v":9000}]
["Cheminee",2,2020,"Cheminee20202",null,"CHZ 200 Keramikrohr ØA 230mm  L330mm","103736",330,null,"STK",{"$f":"VLOOKUP(G3335,sanschie!A:G,7,0)","v":27},{"$f":"ROUND(M3335,0)","v":52},{"$f":"((M3333+M3333+N3335-M3342-M3341-M3339-N3338))/1000*3","v":51.989999999999995},660]
["Cheminee",3,2020,"Cheminee20203",null,"CHZ 200 Isoliermatte 2Stk. pro Rohr L330mm","103746","0",null,"STK",{"$f":"VLOOKUP(G3336,sanschie!A:G,7,0)","v":13},{"$f":"(L3334-(M3338/2)+N3336)*4","v":112},{"$f":"I3333*2","v":18},1]
["Cheminee",5,2020,"Cheminee20205",null,"CHZ 180-200 Füllstein zu Schnellbaufund. L330mm","103710","0",null,"STK",{"$f":"VLOOKUP(G3338,sanschie!A:G,7,0)","v":21}]
["Cheminee",8,2020,"Cheminee20208",null,"CHZ 200 Keramik T-Stück 90° für RA L660mm","103752",665,null,"STK",{"$f":"VLOOKUP(G3341,sanschie!A:G,7,0)","v":209},{"$f":"IF(N3341=0,\"\",N3341)","v":1},{"$f":"IF(L3341=0,0,IF(L3341=\"\",0,L3341*H3341))","v":665},{"$f":"SUM(O3341:P3341)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$F$193=2,\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Cheminee",11,2020,"Cheminee202011",null,"CHZ 200 Anschlusskonus mit Doppelfutter DN200mm","103695","0",null,"STK",{"$f":"VLOOKUP(G3344,sanschie!A:G,7,0)","v":281},{"$f":"IF(Daten!$B$320=2,2,\"\")","v":""}]
["Cheminee",13,2020,"Cheminee202013",null,"CHZ 200 Mündungsmanchette mit Tablett 370 x 370mm","103810","0",null,"STK",{"$f":"VLOOKUP(G3346,sanschie!A:G,7,0)","v":210.7}]
["Cheminee",16,2020,"Cheminee202016",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G3349,sanschie!A:G,7,0)","v":13.8}]
["Cheminee",18,2020,"Cheminee202018",null,"CHZ 150 Doppelfutter lose L150mm","103803","0",null,"STK",{"$f":"VLOOKUP(G3351,sanschie!A:G,7,0)","v":103}]
["Cheminee",22,2020,"Cheminee202022",null,"ABS Kaminhalterung Standard","104256","0",null,"STK",{"$f":"VLOOKUP(G3355,sanschie!A:G,7,0)","v":303},{"$f":"IF(N3355=0,\"\",N3355)","v":""},null,{"$f":"IF(Daten!$B$287=2,1,IF(Daten!$B$287=3,1,0))","v":0}]
["Cheminee",23,2020,"Cheminee202023",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G3356,sanschie!A:G,7,0)","v":94},{"$f":"IF(N3356=0,\"\",N3356)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Cheminee",26,2020,"Cheminee202026",null,"Zugreglerpaket PT12/18 EXE","104577","0",null,"STK",{"$f":"VLOOKUP(G3359,sanschie!A:G,7,0)","v":390}]
["Cheminee",27,2020,"Cheminee202027",null,"Neutralisationsbox komplett","100265","0",null,"STK",{"$f":"VLOOKUP(G3360,sanschie!A:G,7,0)","v":258.8}]
["Cheminee",31,2020,"Cheminee202031",null,"ZBH 210 Verschlusszapfen 2Stk. aus Schaumstoff","103834","0",null,"STK",{"$f":"VLOOKUP(G3364,sanschie!A:G,7,0)","v":26.5}]
["Cheminee",33,2020,"Cheminee202033",null,"ABS 200 Basten Standard Kupfer","104219","0",null,"STK",{"$f":"VLOOKUP(G3366,sanschie!A:G,7,0)","v":375},{"$f":"IF(N3366=0,\"\",N3366)","v":""},null,{"$f":"SUM(O3366:P3366)","v":0},{"$f":"IF(Daten!$B$308=3,1,\"\")","v":""},{"$f":"IF(Daten!$F$308=3,1,\"\")","v":""}]
["Cheminee",36,2020,"Cheminee202036",null,"ZBH 180 Verschlussbüchse weiss ØA 275mm","103838","0",null,"STK",{"$f":"VLOOKUP(G3369,sanschie!A:G,7,0)","v":123.1}]
["Cheminee",0,2525,"Cheminee25250","P","CHEMINEE-Kaminanlage Ø 2525","CHEMINEE 2525","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G3372,sanschie!A:G,7,0)","v":0},null,{"$f":"I3372*1000","v":9000}]
["Cheminee",2,2525,"Cheminee25252",null,"CHZ 250 Keramikrohr ØA 300mm  L330mm","103738",330,null,"STK",{"$f":"VLOOKUP(G3374,sanschie!A:G,7,0)","v":41},{"$f":"ROUND(M3374,0)","v":52},{"$f":"((M3372+M3372+N3374-M3381-M3380-M3378-N3377))/1000*3","v":51.989999999999995},660]
["Cheminee",3,2525,"Cheminee25253",null,"CHZ 250 Isoliermatte 2Stk. pro Rohr L330mm","103747","0",null,"STK",{"$f":"VLOOKUP(G3375,sanschie!A:G,7,0)","v":15},{"$f":"(L3373-(M3377/2)+N3375)*4","v":112},{"$f":"I3372*2","v":18},1]
["Cheminee",7,2525,"Cheminee25257",null,"CHZ Putztüre Typ 3 mit Innendeckel","104634","0",null,"STK",{"$f":"VLOOKUP(G3379,sanschie!A:G,7,0)","v":153},{"$f":"IF(O3379=0,\"\",O3379)","v":1},null,null,{"$f":"(IF(Daten!$C$261=0,P3379,Daten!$C$261+P3379))","v":1},{"$f":"IF(Daten!$C$344=0,0,Daten!$C$344)","v":1}]
["Cheminee",8,2525,"Cheminee25258",null,"CHZ 250 Keramik T-Stück 90° für RA L660mm","103753",665,null,"STK",{"$f":"VLOOKUP(G3380,sanschie!A:G,7,0)","v":285},{"$f":"IF(N3380=0,\"\",N3380)","v":1},{"$f":"IF(L3380=0,0,IF(L3380=\"\",0,L3380*H3380))","v":665},{"$f":"SUM(O3380:P3380)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$F$193=2,\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Cheminee",11,2525,"Cheminee252511",null,"ABS 250 Anschlusskonus EZ mit Doppelfutter DN250mm","103901","0",null,"STK",{"$f":"VLOOKUP(G3383,sanschie!A:G,7,0)","v":365},{"$f":"IF(Daten!$B$320=2,2,\"\")","v":""}]
["Cheminee",13,2525,"Cheminee252513",null,"CHZ Handypl.48x48 11,5 überst.","104590","0",null,"STK",{"$f":"VLOOKUP(G3385,sanschie!A:G,7,0)","v":154.9}]
["Cheminee",16,2525,"Cheminee252516",null,"ABS Rapid-Kartusche zum Kleben der Keramikrohre ","103963","0",null,"STK",{"$f":"VLOOKUP(G3388,sanschie!A:G,7,0)","v":19},{"$f":"ROUNDUP(N3388,0)","v":12},null,{"$f":"I3372*2/1.5","v":12},"Verbrauch 1Kartusche 2 m"]
["Cheminee",18,2525,"Cheminee252518",null,"CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",{"$f":"VLOOKUP(G3390,sanschie!A:G,7,0)","v":61},2]
["Cheminee",22,2525,"Cheminee252522",null,"CHZ Rahmentüre 300 x 400mm ","103816","0",null,"STK",{"$f":"VLOOKUP(G3394,sanschie!A:G,7,0)","v":198}]
["Cheminee",23,2525,"Cheminee252523",null,"Rahmentüre 30/40 gelocht","104542","0",null,"STK",{"$f":"VLOOKUP(G3395,sanschie!A:G,7,0)","v":205}]
["Cheminee",26,2525,"Cheminee252526",null,"CHZ 250 Kaminschleifung 0-35° DZ komplett ","103777","0",null,"STK",{"$f":"VLOOKUP(G3398,sanschie!A:G,7,0)","v":2208}]
["Cheminee",27,2525,"Cheminee252527",null,"ABS Zuluftgitter weiss 90 x 280mm  ","104249","0",null,"STK",{"$f":"VLOOKUP(G3399,sanschie!A:G,7,0)","v":53}]
["Cheminee",31,2525,"Cheminee252531",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G3403,sanschie!A:G,7,0)","v":44.9}]
["Cheminee",33,2525,"Cheminee252533",null,"ZBH 260 Verschlusszapfen 2Stk. aus Schaumstoff","103835","0",null,"STK",{"$f":"VLOOKUP(G3405,sanschie!A:G,7,0)","v":31.1}]
["Cheminee",36,2525,"Cheminee252536",null,"ABS 250 Sairlift Inox","104226","0",null,"STK",{"$f":"VLOOKUP(G3408,sanschie!A:G,7,0)","v":465},{"$f":"IF(N3408=0,\"\",N3408)","v":""},null,{"$f":"SUM(O3408:P3408)","v":0},{"$f":"IF(Daten!$B$308=4,1,\"\")","v":""},{"$f":"IF(Daten!$F$308=4,1,\"\")","v":""}]
["Cheminee",39,2525,"Cheminee252539",null,"Euro Paletten","104259","0",null,"STK",{"$f":"VLOOKUP(G3411,sanschie!A:G,7,0)","v":26}]
["Cheminee",0,3030,"Cheminee30300","P","CHEMINEE-Kaminanlage Ø 3030","CHEMINEE 3030","0",{"$f":"Daten!$B$61","v":9},"Anlage",{"$f":"VLOOKUP(G3413,sanschie!A:G,7,0)","v":0},null,{"$f":"I3413*1000","v":9000}]
[{"$f":"A3413","v":"Cheminee"},{"$f":"B3413+1","v":1},{"$f":"C3413","v":3030},"Cheminee30301",null,"CHZ Mantelstein DZ 550 x 1040mm L330mm 2xØ300mm","103730","0",null,"STK",{"$f":"VLOOKUP(G3414,sanschie!A:G,7,0)","v":120},{"$f":"ROUND(M3414,0)","v":27},{"$f":"((M3413)*3)/1000","v":27}]
["Cheminee",5,3030,{"$f":"A3418&C3418&B3418","v":"Cheminee30305"},null,"CHZ Putztüre Typ 3 mit Innendeckel","104634","0",null,"STK",{"$f":"VLOOKUP(G3418,sanschie!A:G,7,0)","v":153},{"$f":"IF(O3418=0,\"\",O3418)","v":1},null,null,{"$f":"(IF(Daten!$C$261=0,P3418,Daten!$C$261+P3418))","v":1},{"$f":"IF(Daten!$C$344=0,0,Daten!$C$344)","v":1}]
["Cheminee",6,3030,"Cheminee30306",null,"CHZ 300 Keramik T-Stück 90° für RA L660mm","103754",665,null,"STK",{"$f":"VLOOKUP(G3419,sanschie!A:G,7,0)","v":348},{"$f":"IF(N3419=0,\"\",N3419)","v":1},{"$f":"IF(L3419=0,0,IF(L3419=\"\",0,L3419*H3419))","v":665},{"$f":"SUM(O3419:P3419)","v":1},{"$f":"IF(Daten!$C$193=0,\"\",IF(Daten!$F$193=2,\"\",Daten!$C$193))","v":1},{"$f":"IF(Daten!$C$202=0,\"\",IF(Daten!$G$202=\"45°\",\"\",Daten!$C$202))","v":""}]
["Cheminee",9,3030,"Cheminee30309",null,"ABS 300 Anschlusskonus EZ mit Doppelfutter DN300mm","103697","0",null,"STK",{"$f":"VLOOKUP(G3422,sanschie!A:G,7,0)","v":414},{"$f":"IF(Daten!$B$320=2,2,\"\")","v":""}]
["Cheminee",11,3030,"Cheminee303011",null,"ABS Handyplatte EZ Faserzement 550 x 550mm","104147","0",null,"STK",{"$f":"VLOOKUP(G3424,sanschie!A:G,7,0)","v":156}]
["Cheminee",15,3030,"Cheminee303015",null,"ZBH Kittpistole für Kartuschen","103848","0",null,"STK",{"$f":"VLOOKUP(G3428,sanschie!A:G,7,0)","v":13.8}]
["Cheminee",16,3030,"Cheminee303016",null,"CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",{"$f":"VLOOKUP(G3429,sanschie!A:G,7,0)","v":61},2]
["Cheminee",20,3030,"Cheminee303020",null,"CHZ Rahmentüre 300 x 400mm ","103816","0",null,"STK",{"$f":"VLOOKUP(G3433,sanschie!A:G,7,0)","v":198}]
["Cheminee",21,3030,"Cheminee303021",null,"Rahmentüre 30/40 gelocht","104542","0",null,"STK",{"$f":"VLOOKUP(G3434,sanschie!A:G,7,0)","v":205}]
["Cheminee",23,3030,"Cheminee303023",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",{"$f":"VLOOKUP(G3436,sanschie!A:G,7,0)","v":94},{"$f":"IF(N3436=0,\"\",N3436)","v":""},null,{"$f":"IF(Daten!$B$287=3,1,0)","v":0}]
["Cheminee",26,3030,"Cheminee303026",null,"Zugreglerpaket PT12/18 EXE","104577","0",null,"STK",{"$f":"VLOOKUP(G3439,sanschie!A:G,7,0)","v":390}]
["Cheminee",29,3030,"Cheminee303029",null,"ZBH Kondensatkanister 20Liter","103841","0",null,"STK",{"$f":"VLOOKUP(G3442,sanschie!A:G,7,0)","v":44.9}]
["Cheminee",31,3030,"Cheminee303031",null,"ABS 300 Basten Standard Inox","104215","0",null,"STK",{"$f":"VLOOKUP(G3444,sanschie!A:G,7,0)","v":535},{"$f":"IF(N3444=0,\"\",N3444)","v":""},null,{"$f":"SUM(O3444:P3444)","v":0},{"$f":"IF(Daten!$B$308=2,1,\"\")","v":""},{"$f":"IF(Daten!$F$308=2,1,\"\")","v":""}]
["Cheminee",34,3030,"Cheminee303034",null,"ABS 300 Sairlift Kupfer","104232","0",null,"STK",{"$f":"VLOOKUP(G3447,sanschie!A:G,7,0)","v":633},{"$f":"IF(N3447=0,\"\",N3447)","v":""},null,{"$f":"SUM(O3447:P3447)","v":0},{"$f":"IF(Daten!$B$308=5,1,\"\")","v":""},{"$f":"IF(Daten!$F$308=5,1,\"\")","v":""}]
["ICS Matt",0,80,{"$f":"A3450&\" \"&C3450&B3450","v":"ICS Matt 800"}," ","Schiedel ICS MATT 25mm 80","ICS Matt 80","0",{"$f":"ICS!$J$10","v":10},"Anlage",0,1,{"$f":"I3450*1000","v":10000},null,{"$f":"ROUNDUP(P3450,2)","v":10.52},{"$f":"SUM(P3452:P3506)/1000","v":10.516}]
[{"$f":"A3451","v":"ICS Matt"},{"$f":"B3451+1","v":2},{"$f":"C3451","v":80},{"$f":"A3452&\" \"&C3452&B3452","v":"ICS Matt 802"},null,"ICM 475 Wandkonsolen  (Paar) L475mm","101974","0",null,"STK",158,{"$f":"IF(M3452=0,\"\",M3452)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3451=1,0,IF(Daten!$B$549=2,1)+O3452))))","v":0},"69-312",{"$f":"IF(Daten!$B$549=2,N3458,0)","v":0},null,100]
[{"$f":"A3452","v":"ICS Matt"},{"$f":"B3452+1","v":3},{"$f":"C3452","v":80},{"$f":"A3453&\" \"&C3453&B3453","v":"ICS Matt 803"},null,"ICM 570 Wandkonsolen  (Paar) L570mm","101975","0",null,"STK",217,{"$f":"IF(M3453=0,\"\",M3453)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3451=1,\"\",IF(Daten!$B$549=3,1)+O3453))))","v":""},"69-312",{"$f":"IF(Daten!$B$549=3,N3458,0)","v":0},null,250]
["ICS Matt",7,80,{"$f":"A3457&\" \"&C3457&B3457","v":"ICS Matt 807"},null,"ICM 80 Verankerungsplatte mit Ablauf senkr.","101983",95,null,"STK",130,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L3457=\"\",\"0\",L3457*H3457)","v":95},null,null,{"$f":"IF(L3457=\"\",\"0\",H3457*L3457)","v":95}]
["ICS Matt",9,80,{"$f":"A3459&\" \"&C3459&B3459","v":"ICS Matt 809"},null,"ICM 80 Verankerungsplatte EW auf DW","102011",97,null,"STK",109,null,{"$f":"IF(L3459=\"\",\"0\",L3459*H3459)","v":"0"},null,null,{"$f":"IF(L3459=\"\",\"0\",H3459*L3459)","v":"0"}]
["ICS Matt",12,80,"ICS Matt 8012",null,"ICM 80 Putztüranschluss rund Überdruck L288mm","102070",288,null,"STK",233,{"$f":"Daten!$F$499","v":1},288,null,null,288]
["ICS Matt",13,80,"ICS Matt 8013",null,"ICM 80 T-Stück 45° L 330mm","102084",330,null,"STK",206,{"$f":"IF(Daten!$B$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",17,80,"ICS Matt 8017",null,"ICM 80 Anschluss von EW auf DW in Rauchgasr.","102146","0",null,"STK",87,1,{"$f":"IF(L3467=\"\",\"0\",L3467*H3467)","v":0},null,null,{"$f":"IF(L3467=\"\",\"0\",H3468*L3467)","v":0}]
["ICS Matt",18,80,"ICS Matt 8018",null,"ICM 80 Anschluss von DW auf EW in Rauchgasr.","102170","0",null,"STK",87,null,{"$f":"IF(H3468=\"\",\"\",L3468*H3468)","v":0}]
["ICS Matt",22,80,"ICS Matt 8022",null,"ICM 80 Längenelement L1000mm","102226",955,null,"STK",120,{"$f":"ROUNDUP(M3472,0)+N3472","v":10},{"$f":"((M3450-SUM(M3457:M3471)-M3497)/H3472)","v":9.4596858638743448},{"$f":"O3472/H3472","v":0},{"$f":"Daten!$DF$268*1000","v":0},{"$f":"(IF(L3472=\"\",0,H3472*L3472))-O3472","v":9550}]
[{"$f":"A3472","v":"ICS Matt"},{"$f":"B3472+1","v":23},{"$f":"C3472","v":80},{"$f":"A3473&\" \"&C3473&B3473","v":"ICS Matt 8023"},null,"ICM 80 Schiebe-Element L270-375mm","102247","0",null,"STK",163,null,null,null,null,{"$f":"IF(L3473=\"\",\"0\",H3473*L3473)","v":"0"}]
["ICS Matt",25,80,"ICS Matt 8025",null,"ICM 80 Klemmband DN130","102261","0",null,"STK",15,null,null,null,null,{"$f":"IF(L3475=\"\",\"0\",H3475*L3475)","v":"0"}]
["ICS Matt",28,80,"ICS Matt 8028",null,"ICM 80 Wandhalter 50mm verlängerbar DN 130mm ","102303","0",null,"STK",33,{"$f":"ROUNDUP(M3478,0)","v":3},{"$f":"((M3450/1000)/4.3)","v":2.3255813953488373},null,null,0]
["ICS Matt",31,80,"ICS Matt 8031",null,"ICM L2 Verlängerung zu Wandhalter 50mm L450mm","102320","0",null,"STK",142,{"$f":"IF(Daten!$B$549=4,$L3478,\"\")","v":""},null,440,null,"0"]
["ICS Matt",33,80,"ICS Matt 8033",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,{"$f":"IF(Daten!$B$549=5,$L3478,\"\")","v":""},null,700,null,"0"]
["ICS Matt",36,80,"ICS Matt 8036",null,"PPL Muffe 1/2\" zu Grundplatte 1/2\" Wandabst. 50mm","101205","0",null,"STK",20,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",39,80,"ICS Matt 8039",null,"ICM 80-100 Dachdurführung 16-25° DN165  ","102335","0",null,"STK",271,{"$f":"IF(Daten!$B$522=3,1,\"\")","v":""},null,null,null,{"$f":"IF(L3489=\"\",\"0\",H3489*L3489)","v":"0"}]
["ICS Matt",41,80,"ICS Matt 8041",null,"ICM 80-100 Dachdurführung 36-45° DN165  ","102359","0",null,"STK",401,{"$f":"IF(Daten!$B$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",42,80,"ICS Matt 8042",null,"ICM 80 Regenkragen DN130 ","102371","0",null,"STK",33,{"$f":"IF(SUM(L3488:L3491)=0,\"\",SUM(L3488:L3491))","v":""},null,null,null,"0"]
["ICS Matt",46,80,"ICS Matt 8046",null,"ICM 80 Anschlussrosette Øi 130mm ØA 400mm","102415","0",null,"STK",55,{"$f":"IF(Daten!$E$515=4,1,\"\")","v":""},null,null,null,{"$f":"IF(L3496=\"\",\"0\",H3496*L3496)","v":"0"}]
["ICS Matt",48,80,"ICS Matt 8048",null,"ICM 80 Element mit Messöffnung1/2\" L205mm","102452","0",null,"STK",152,null,{"$f":"IF(L3498=\"\",0,L3498*H3498)","v":0},null,null,"0"]
["ICS Matt",51,80,"ICS Matt 8051",null,"ICM 80 Winkel 30°","102488","0",null,"STK",130,null,0,null,null,"0"]
["ICS Matt",52,80,"ICS Matt 8052",null,"ICM 80 Winkel 45°","102502","0",null,"STK",130,null,0,null,null,"0"]
["ICS Matt",56,80,"ICS Matt 8056",null,"ICM 80 Inspektions-Winkel 90°","102558","0",null,"STK",315,null,0,null,null,"0"]
["ICS Matt",0,100,"ICS Matt 1000"," ","Schiedel ICS MATT 25mm 100","ICS Matt 100","0",{"$f":"ICS!$J$10","v":10},"Anlage",0,1,{"$f":"I3507*1000","v":10000},null,{"$f":"ROUNDUP(P3507,2)","v":10.52},{"$f":"SUM(P3509:P3567)/1000","v":10.516}]
[{"$f":"A3508","v":"ICS Matt"},{"$f":"B3508+1","v":2},{"$f":"C3508","v":100},{"$f":"A3509&\" \"&C3509&B3509","v":"ICS Matt 1002"},null,"ICM 475 Wandkonsolen  (Paar) L475mm","101974","0",null,"STK",158,{"$f":"IF(M3509=0,\"\",M3509)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3508=1,0,IF(Daten!$B$549=2,1)+O3509))))","v":0},"69-292",{"$f":"IF(Daten!$B$549=2,N3515,0)","v":0},null,100]
["ICS Matt",5,100,"ICS Matt 1005",null,"ICM 720 Wandkonsolen  (Paar) L720mm","101977","0",null,"STK",228,{"$f":"IF(M3512=0,\"\",M3512)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3508=1,\"\",IF(Daten!$B$549=5,1)+O3512))))","v":0},"392-692",{"$f":"IF(Daten!$B$549=5,N3515,0)","v":0},null,600]
["ICS Matt",7,100,{"$f":"A3514&\" \"&C3514&B3514","v":"ICS Matt 1007"},null,"ICM 100 Verankerungsplatte mit Ablauf senkr.","101984",95,null,"STK",163,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L3514=\"\",\"0\",L3514*H3514)","v":95},null,null,{"$f":"IF(L3514=\"\",\"0\",H3514*L3514)","v":95}]
["ICS Matt",10,100,{"$f":"A3517&\" \"&C3517&B3517","v":"ICS Matt 10010"},null,"ICM 100 Kondensatschale mit Ablauf 1/2\"","102026",55,null,"STK",93,null,"0",null,null,"0"]
["ICS Matt",13,100,{"$f":"A3520&\" \"&C3520&B3520","v":"ICS Matt 10013"},null,"PPL 100 EW-DW Deckenanfängerset 45° kompl. L270mm","100655","0",null,"STK",432,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",15,100,{"$f":"A3522&\" \"&C3522&B3522","v":"ICS Matt 10015"},null,"ICM 100 T-Stück 45° L 355mm","102085",355,null,"STK",238,{"$f":"IF(Daten!$B$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",18,100,"ICS Matt 10018",null,"ICM 100 Verschlussdeckel","102133","0",null,"STK",103,null,"0",null,null,"0"]
["ICS Matt",21,100,"ICS Matt 10021",null,"ICM 100 Anschluss von DW auf EW in Rauchgasr.","102171","0",null,"STK",98,null,{"$f":"IF(H3528=\"\",\"\",L3528*H3528)","v":0},null,null,"0"]
["ICS Matt",23,100,"ICS Matt 10023",null,"ICM 100 Längenelement L250mm","102199",205,null,"STK",77,{"$f":"IF(Daten!$DJ$251=0,\"\",Daten!$DJ$251)","v":""},{"$f":"IF(L3530=\"\",0,L3530*H3530)","v":0},{"$f":"O3530/H3530","v":0},{"$f":"Daten!$DF$252*1000","v":0},{"$f":"(IF(L3530=\"\",0,H3530*L3530))-O3530","v":0}]
["ICS Matt",24,100,"ICS Matt 10024",null,"ICM 100 Längenelement L500mm","102213",455,null,"STK",87,{"$f":"IF(Daten!$DJ$259=0,\"\",Daten!$DJ$259)","v":""},{"$f":"IF(L3531=\"\",0,L3531*H3531)","v":0},{"$f":"O3531/H3531","v":0},{"$f":"Daten!$DF$260*1000","v":0},{"$f":"(IF(L3531=\"\",0,H3531*L3531))-O3531","v":0}]
[{"$f":"A3534","v":"ICS Matt"},{"$f":"B3534+1","v":28},{"$f":"C3534","v":100},{"$f":"A3535&\" \"&C3535&B3535","v":"ICS Matt 10028"},null,"ICM 100 Klemmband DN150","102262","0",null,"STK",16,null,null,null,null,{"$f":"IF(L3535=\"\",\"0\",H3535*L3535)","v":"0"}]
[{"$f":"A3536","v":"ICS Matt"},{"$f":"B3536+1","v":30},{"$f":"C3536","v":100},{"$f":"A3537&\" \"&C3537&B3537","v":"ICS Matt 10030"},null,"ICM 100 Wandhalter verstellbar 75 - 300mm DN 150mm","102290","0",null,"STK",60,null,null,null,null,{"$f":"IF(L3537=\"\",\"0\",H3537*L3537)","v":"0"}]
["ICS Matt",33,100,"ICS Matt 10033",null,"ICM L1 Verlängerung zu Wandhalter 50mm L300mm","102319","0",null,"STK",109,{"$f":"IF(Daten!$B$549=3,#REF!,\"\")","v":""},null,250,null,"0"]
["ICS Matt",36,100,"ICS Matt 10036",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,{"$f":"IF(Daten!$B$549=5,#REF!,\"\")","v":""},null,700,null,"0"]
["ICS Matt",38,100,"ICS Matt 10038",null,"PPL Innengewinderohr zu Rohrschelle 1/2\" 1000mm","101204","0",null,"STK",147,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",39,100,"ICS Matt 10039",null,"PPL Muffe 1/2\" zu Grundplatte 1/2\" Wandabst. 50mm","101205","0",null,"STK",20,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",41,100,"ICS Matt 10041",null,"ICM 80-100 Dachdurführung 0° DN165  L500mm","102323","0",null,"STK",142,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,{"$f":"IF(L3548=\"\",\"0\",H3548*L3548)","v":"0"}]
["ICS Matt",44,100,"ICS Matt 10044",null,"ICM 80-100 Dachdurführung 36-45° DN165  ","102359","0",null,"STK",401,{"$f":"IF(Daten!$B$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",46,100,"ICS Matt 10046",null,"ICM 100 Seilabspannring DN150","102386","0",null,"STK",60,null,null,null,null,"0"]
["ICS Matt",49,100,"ICS Matt 10049",null,"ICM 100 Anschlussrosette Øi 150mm ØA 420mm","102416","0",null,"STK",57,{"$f":"IF(Daten!$E$515=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",52,100,"ICS Matt 10052",null,"ICM 100 Element mit Messöffnung1/2\" L205mm ","102453","0",null,"STK",163,null,{"$f":"IF(L3559=\"\",0,L3559*H3559)","v":0},null,null,"0"]
["ICS Matt",54,100,"ICS Matt 10054",null,"ICM 100 Winkel 15° ","102481","0",null,"STK",136,null,0,null,null,"0"]
["ICS Matt",58,100,"ICS Matt 10058",null,"ICM 100 Inspektions-Winkel 85°","102531","0",null,"STK",347,null,0,null,null,"0"]
["ICS Matt",59,100,"ICS Matt 10059",null,"ICM 100 Winkel 90°","102545","0",null,"STK",158,null,0,null,null,"0"]
[{"$f":"A3568","v":"ICS Matt"},{"$f":"B3568+1","v":1},{"$f":"C3568","v":130},{"$f":"A3569&\" \"&C3569&B3569","v":"ICS Matt 1301"},null,"ICM 130 Konsolenbleche (Paar)","101956","0",null,"STK",136,{"$f":"N3569","v":1},null,{"$f":"IF(Daten!$B$499=1,O3569,\"\")","v":1},{"$f":"IF(Daten!$B$549=1,1,\"\")","v":1},{"$f":"IF(L3569=\"\",\"0\",H3569*L3569)","v":0}]
[{"$f":"A3569","v":"ICS Matt"},{"$f":"B3569+1","v":2},{"$f":"C3569","v":130},{"$f":"A3570&\" \"&C3570&B3570","v":"ICS Matt 1302"},null,"ICM 475 Wandkonsolen  (Paar) L475mm","101974","0",null,"STK",158,{"$f":"IF(M3570=0,\"\",M3570)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3569=1,0,IF(Daten!$B$549=2,1)+O3570))))","v":0},"69-292",{"$f":"IF(Daten!$B$549=2,N3576,0)","v":0},null,100]
["ICS Matt",6,130,{"$f":"A3574&\" \"&C3574&B3574","v":"ICS Matt 1306"},null,{"$f":"VLOOKUP(G3574,sanschie!A:E,5,0)","v":"KRS Abdeckung zu C-schienen 1m"},"103431","0",null,"STK",22,null,null,null,null,{"$f":"IF(L3574=\"\",\"0\",H3574*L3574)","v":"0"}]
["ICS Matt",8,130,{"$f":"A3576&\" \"&C3576&B3576","v":"ICS Matt 1308"},null,"ICM 130 Zwischenstütze","101999",95,null,"STK",195,{"$f":"IF(N3576=0,\"\",N3576)","v":""},{"$f":"IF(L3576=\"\",0,L3576*H3576)","v":0},{"$f":"IF(M3568>=15000,1,0)","v":0},null,{"$f":"IF(L3576=\"\",\"0\",H3576*L3576)","v":"0"}]
["ICS Matt",11,130,"ICS Matt 13011",null,"ICM 130 Teleskopstütze verstellbar L300 - 500mm","102041",300,null,"STK",293,{"$f":"IF(Daten!$B$499=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",14,130,"ICS Matt 13014",null,"PPL 130 EW-DW Deckenanfängerset 45° kompl. L270mm","100656","0",null,"STK",487,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,{"$f":"IF(L3582=\"\",\"0\",H3582*L3582)","v":"0"}]
["ICS Matt",16,130,"ICS Matt 13016",null,"ICM 130 Putztüranschluss rund Überdruck L455mm","102072",455,null,"STK",298,{"$f":"Daten!$F$499","v":1},455,null,null,455]
["ICS Matt",17,130,"ICS Matt 13017",null,"ICM 130 T-Stück 45° L455mm","102086",455,null,"STK",271,{"$f":"IF(Daten!$B$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",19,130,{"$f":"A3587&\" \"&C3587&B3587","v":"ICS Matt 13019"},null,"ICM 130 Verschlussdeckel mit Zugbegrenzer ","140840","0",null,"STK",238,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",22,130,{"$f":"A3590&\" \"&C3590&B3590","v":"ICS Matt 13022"},null,"ICM 130 Verschlussdeckel","102134","0",null,"STK",115,null,"0",null,null,"0"]
["ICS Matt",25,130,"ICS Matt 13025",null,"ICM 130 Anschluss von DW auf EW in Rauchgasr.","102172","0",null,"STK",109,null,{"$f":"IF(H3593=\"\",\"\",L3593*H3593)","v":0},null,null,{"$f":"IF(L3593=\"\",\"0\",H3593*L3593)","v":"0"}]
["ICS Matt",27,130,"ICS Matt 13027",null,"ICM 130 Längenelement L195mm","102186",150,null,"STK",77,null,{"$f":"IF(H3595=\"\",\"\",L3595*H3595)","v":0},null,null,{"$f":"IF(L3595=\"\",\"0\",H3595*L3595)","v":"0"}]
["ICS Matt",30,130,"ICS Matt 13030",null,"ICM 130 Längenelement L1000mm","102228",955,null,"STK",163,{"$f":"ROUNDUP(M3598,0)+N3598","v":9},{"$f":"((M3568-SUM(M3575:M3597)-M3624)/H3598)","v":8.6795811518324602},{"$f":"O3598/H3598","v":0},{"$f":"Daten!$DF$268*1000","v":0},{"$f":"(IF(L3598=\"\",0,H3598*L3598))-O3598","v":8595}]
["ICS Matt",32,130,"ICS Matt 13032",null,"PPL 130 Dichtung Viton","100991","0",null,"STK",15,{"$f":"IF(Daten!$B$490=1,\"\",SUM(L3575:L3578,L3580:L3591,L3595:L3598,L3628:L3634,L3624))","v":""},{"$f":"IF(L3600=\"\",\"\",L3600*H3600)","v":""},null,null,{"$f":"IF(L3600=\"\",\"0\",H3600*L3600)","v":"0"}]
["ICS Matt",36,130,"ICS Matt 13036",null,"ICM 130 Wandhalter 50mm verlängerbar DN 180mm ","102305","0",null,"STK",44,{"$f":"ROUNDUP(M3604,0)","v":3},{"$f":"((M3568/1000)/4.3)","v":2.3255813953488373},null,null,{"$f":"IF(L3604=\"\",\"0\",H3604*L3604)","v":0}]
["ICS Matt",37,130,"ICS Matt 13037",null,"ICM W1 Verlängerung zu Wandhalter 50mm L 130mm","102317","0",null,"STK",44,{"$f":"IF(Daten!$B$549=2,#REF!,\"\")","v":""},null,100,null,"0"]
["ICS Matt",40,130,"ICS Matt 13040",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,500,null,"0"]
["ICS Matt",41,130,"ICS Matt 13041",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,{"$f":"IF(Daten!$B$549=5,#REF!,\"\")","v":""},null,700,null,"0"]
["ICS Matt",45,130,"ICS Matt 13045",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",47,130,"ICS Matt 13047",null,"ICM 130 Dachdurführung 16-25° DN200 mit Bleilappen","102336","0",null,"STK",303,{"$f":"IF(Daten!$B$522=3,1,\"\")","v":""},null,null,null,{"$f":"IF(L3615=\"\",\"0\",H3615*L3615)","v":"0"}]
["ICS Matt",50,130,"ICS Matt 13050",null,"ICM 130 Regenkragen DN180 ","102373","0",null,"STK",44,{"$f":"IF(SUM(L3614:L3617)=0,\"\",SUM(L3614:L3617))","v":""},null,null,null,"0"]
["ICS Matt",53,130,"ICS Matt 13053",null,"ICM 130 Blende 32-45° DN180 ","102409","0",null,"STK",77,{"$f":"IF(Daten!$E$515=3,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",55,130,"ICS Matt 13055",null,"ICM 130 Anschlussrosette EW Øi 180mm ØA 350mm","102425","0",null,"STK",38,null,null,null,null,{"$f":"IF(L3623=\"\",\"0\",H3623*L3623)","v":"0"}]
["ICS Matt",56,130,"ICS Matt 13056",null,"ICM 130 Mündungsabschluss","102433",295,null,"STK",120,{"$f":"IF(Daten!$E$522=1,1,IF(Daten!$E$522=2,1,\"\"))","v":1},{"$f":"IF(L3624=\"\",\"0\",L3624*H3624)","v":295},null,null,295]
["ICS Matt",60,130,"ICS Matt 13060",null,"ICM 130 Winkel 15° ","102482","0",null,"STK",147,null,0,null,null,"0"]
["ICS Matt",61,130,"ICS Matt 13061",null,"ICM 130 Winkel 30°","102490","0",null,"STK",152,null,0,null,null,"0"]
["ICS Matt",64,130,"ICS Matt 13064",null,"ICM 130 Inspektions-Winkel 85°","102532","0",null,"STK",380,null,0,null,null,"0"]
["ICS Matt",66,130,"ICS Matt 13066",null,"ICM 130 Inspektions-Winkel 90°","102560","0",null,"STK",380,null,0,null,null,"0"]
[{"$f":"A3636","v":"ICS Matt"},{"$f":"B3636+1","v":2},{"$f":"C3636","v":150},{"$f":"A3637&\" \"&C3637&B3637","v":"ICS Matt 1502"},null,"ICM 475 Wandkonsolen  (Paar) L475mm","101974","0",null,"STK",158,{"$f":"IF(M3637=0,\"\",M3637)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3636=1,0,IF(Daten!$B$549=2,1)+O3637))))","v":0},"69-292",{"$f":"IF(Daten!$B$549=2,N3643,0)","v":0},null,100]
["ICS Matt",4,150,"ICS Matt 1504",null,"ICM 620 Wandkonsolen  (Paar) L620mm","101976","0",null,"STK",223,{"$f":"IF(M3639=0,\"\",M3639)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3636=1,\"\",IF(Daten!$B$549=4,1)+O3639))))","v":0},"292-392",{"$f":"IF(Daten!$B$549=4,N3643,0)","v":0},null,400]
["ICS Matt",8,150,{"$f":"A3643&\" \"&C3643&B3643","v":"ICS Matt 1508"},null,"ICM 150 Zwischenstütze","102000",95,null,"STK",206,{"$f":"IF(N3643=0,\"\",N3643)","v":""},{"$f":"IF(L3643=\"\",0,L3643*H3643)","v":0},{"$f":"IF(M3635>=15000,1,0)","v":0},null,"0"]
["ICS Matt",9,150,"ICS Matt 1509",null,"ICM 150 Verankerungsplatte EW auf DW","102014",97,null,"STK",142,null,{"$f":"IF(L3644=\"\",\"0\",L3644*H3644)","v":"0"},null,null,"0"]
["ICS Matt",11,150,"ICS Matt 15011",null,"ICM 150 Teleskopstütze verstellbar L300 - 500mm","102042",300,null,"STK",303,{"$f":"IF(Daten!$B$499=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",14,150,{"$f":"A3649&\" \"&C3649&B3649","v":"ICS Matt 15014"},null,"PPL 150 EW-DW Deckenanfängerset 45° kompl. L270mm","100657","0",null,"STK",540,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",17,150,{"$f":"A3652&\" \"&C3652&B3652","v":"ICS Matt 15017"},null,"ICM 150 T-Stück 45° L455mm","102087",455,null,"STK",315,{"$f":"IF(Daten!$B$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",19,150,{"$f":"A3654&\" \"&C3654&B3654","v":"ICS Matt 15019"},null,"ICM 150 Verschlussdeckel mit Zugbegrenzer ","140841","0",null,"STK",271,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",22,150,{"$f":"A3657&\" \"&C3657&B3657","v":"ICS Matt 15022"},null,"ICM 150 Verschlussdeckel","102135","0",null,"STK",125,null,"0",null,null,"0"]
["ICS Matt",25,150,"ICS Matt 15025",null,"ICM 150 Anschluss DW/EW mit Klemmfutter DN150","102163","0",null,"STK",142,null,{"$f":"IF(H3660=\"\",\"\",L3660*H3660)","v":0},null,null,"0"]
["ICS Matt",27,150,"ICS Matt 15027",null,"ICM 150 Schiebe-Element mit Doppelfutter DN150 ","102241","0",null,"STK",260,null,{"$f":"IF(H3662=\"\",\"\",L3662*H3662)","v":0},null,null,"0"]
["ICS Matt",28,150,"ICS Matt 15028",null,"ICM 150 Längenelement L195mm","102187",150,null,"STK",82,null,{"$f":"IF(H3663=\"\",\"\",L3663*H3663)","v":0},null,null,"0"]
[{"$f":"A3666","v":"ICS Matt"},{"$f":"B3666+1","v":32},{"$f":"C3666","v":150},{"$f":"A3667&\" \"&C3667&B3667","v":"ICS Matt 15032"},null,"ICM 150 Schiebe-Element L270-375mm","102250","0",null,"STK",195,null,null,null,null,{"$f":"IF(L3667=\"\",\"0\",H3667*L3667)","v":"0"}]
["ICS Matt",33,150,"ICS Matt 15033",null,"PPL 150 Dichtung Viton","100992","0",null,"STK",16,{"$f":"IF(Daten!$B$490=1,\"\",SUM(L3642:L3645,L3647:L3658,L3663:L3666,L3696:L3702,L3692))","v":""},{"$f":"IF(L3668=\"\",\"\",L3668*H3668)","v":""},null,null,{"$f":"IF(L3668=\"\",\"0\",H3668*L3668)","v":"0"}]
["ICS Matt",36,150,"ICS Matt 15036",null,"ICM 150 Wandhalter verstellbar 75 - 300mm DN 200mm","102292","0",null,"STK",72,null,null,null,null,{"$f":"IF(L3671=\"\",\"0\",H3671*L3671)","v":"0"}]
["ICS Matt",38,150,"ICS Matt 15038",null,"ICM W1 Verlängerung zu Wandhalter 50mm L 130mm","102317","0",null,"STK",44,{"$f":"IF(Daten!$B$549=2,#REF!,\"\")","v":""},null,100,null,"0"]
["ICS Matt",42,150,"ICS Matt 15042",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,{"$f":"IF(Daten!$B$549=5,#REF!,\"\")","v":""},null,700,null,"0"]
["ICS Matt",43,150,{"$f":"A3678&\" \"&C3678&B3678","v":"ICS Matt 15043"},null,"PPL 200 Rohrschelle Anschluss 1/2\" Aussengewinde","101200","0",null,"STK",38,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",47,150,"ICS Matt 15047",null,"ICM 150-180 Dachdurführung 0° DN250 L500mm","102325","0",null,"STK",163,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,{"$f":"IF(L3682=\"\",\"0\",H3682*L3682)","v":"0"}]
["ICS Matt",48,150,"ICS Matt 15048",null,"ICM 150-180 Dachdurführung 16-25° DN250 ","102337","0",null,"STK",347,{"$f":"IF(Daten!$B$522=3,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",50,150,"ICS Matt 15050",null,"ICM 150-180 Dachdurführung 36-45° DN250 ","102361","0",null,"STK",466,{"$f":"IF(Daten!$B$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",53,150,"ICS Matt 15053",null,"ICM 150 Blende 0-30° DN200","102402","0",null,"STK",70,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",56,150,"ICS Matt 15056",null,"ICM 150 Anschlussrosette EW Øi 200mm ØA 370mm","102426","0",null,"STK",40,null,null,null,null,"0"]
["ICS Matt",58,150,"ICS Matt 15058",null,"ICM 150 Basten Standart mit Stulpring Inox matt","102447","0",null,"STK",373,{"$f":"IF(Daten!$E$522=3,1,\"\")","v":""},{"$f":"IF(L3693=\"\",\"0\",L3693*H3693)","v":"0"},null,null,"0"]
["ICS Matt",61,150,"ICS Matt 15061",null,"ICM 150 Winkel 15° ","102483","0",null,"STK",158,null,0,null,null,"0"]
["ICS Matt",64,150,"ICS Matt 15064",null,"ICM 150 Winkel 85°","102519","0",null,"STK",190,null,0,null,null,"0"]
["ICS Matt",66,150,"ICS Matt 15066",null,"ICM 150 Winkel 90°","102547","0",null,"STK",190,null,0,null,null,"0"]
["ICS Matt",67,150,"ICS Matt 15067",null,"ICM 150 Inspektions-Winkel 90°","102561","0",null,"STK",411,null,0,null,null,"0"]
["ICS Matt",3,180,"ICS Matt 1803",null,"ICM 570 Wandkonsolen  (Paar) L570mm","101975","0",null,"STK",217,{"$f":"IF(M3706=0,\"\",M3706)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3704=1,\"\",IF(Daten!$B$549=3,1)+O3706))))","v":0},"69-292",{"$f":"IF(Daten!$B$549=3,N3711,0)","v":0},null,250]
["ICS Matt",4,180,"ICS Matt 1804",null,"ICM 620 Wandkonsolen  (Paar) L620mm","101976","0",null,"STK",223,{"$f":"IF(M3707=0,\"\",M3707)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3704=1,\"\",IF(Daten!$B$549=4,1)+O3707))))","v":0},"292-392",{"$f":"IF(Daten!$B$549=4,N3711,0)","v":0},null,400]
["ICS Matt",8,180,{"$f":"A3711&\" \"&C3711&B3711","v":"ICS Matt 1808"},null,"ICM 180 Zwischenstütze","102001",95,null,"STK",217,{"$f":"IF(N3711=0,\"\",N3711)","v":""},{"$f":"IF(L3711=\"\",0,L3711*H3711)","v":0},{"$f":"IF(M3703>=15000,1,0)","v":0},null,"0"]
["ICS Matt",9,180,{"$f":"A3712&\" \"&C3712&B3712","v":"ICS Matt 1809"},null,"ICM 180 Verankerungsplatte EW auf DW","102015",97,null,"STK",163,null,{"$f":"IF(L3712=\"\",\"0\",L3712*H3712)","v":"0"},null,null,"0"]
["ICS Matt",13,180,{"$f":"A3716&\" \"&C3716&B3716","v":"ICS Matt 18013"},null,"PPL 180 EW-DW Deckenanfängerset komplett L270mm","100651","0",null,"STK",432,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",14,180,{"$f":"A3717&\" \"&C3717&B3717","v":"ICS Matt 18014"},null,"PPL 180 EW-DW Deckenanfängerset 45° kompl. L270mm","100658","0",null,"STK",595,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",18,180,"ICS Matt 18018",null,"ICM 180 T-Stück 90° L455mm","102102",455,null,"STK",298,{"$f":"IF(Daten!$B$515=2,1,\"\")","v":1},455,null,null,455]
["ICS Matt",19,180,{"$f":"A3722&\" \"&C3722&B3722","v":"ICS Matt 18019"},null,"ICM 180 Verschlussdeckel mit Zugbegrenzer ","140842","0",null,"STK",303,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,{"$f":"IF(L3722=\"\",\"0\",H3722*L3722)","v":"0"}]
["ICS Matt",21,180,{"$f":"A3724&\" \"&C3724&B3724","v":"ICS Matt 18021"},null,"ICM 180 Inspektions-T-Stück 90° L455mm","102128",455,null,"STK",433,null,"0",null,null,"0"]
["ICS Matt",24,180,"ICS Matt 18024",null,"ICM 180 Anschluss DW/EW mit Klemmfutter DN150","102164","0",null,"STK",152,null,{"$f":"IF(H3727=\"\",\"\",L3727*H3727)","v":0},null,null,{"$f":"IF(L3727=\"\",\"0\",H3727*L3727)","v":"0"}]
["ICS Matt",27,180,"ICS Matt 18027",null,"ICM 180 Schiebe-Element mit Doppelfutter DN150 ","102242","0",null,"STK",282,null,0,null,null,"0"]
["ICS Matt",29,180,"ICS Matt 18029",null,"ICM 180 Längenelement L195mm","102188",150,null,"STK",87,null,0,null,null,"0"]
["ICS Matt",32,180,"ICS Matt 18032",null,"ICM 180 Längenelement L1000mm","102230",955,null,"STK",217,{"$f":"ROUNDUP(M3735,0)+N3735","v":9},{"$f":"((M3703-SUM(M3710:M3734)-M3761)/H3735)","v":8.6795811518324602},{"$f":"O3735/H3735","v":0},{"$f":"Daten!$DF$268*1000","v":0},{"$f":"(IF(L3735=\"\",0,H3735*L3735))-O3735","v":8595}]
["ICS Matt",35,180,"ICS Matt 18035",null,"ICM 180 Klemmband DN230","102265","0",null,"STK",19,null,null,null,null,{"$f":"IF(L3738=\"\",\"0\",H3738*L3738)","v":"0"}]
["ICS Matt",37,180,"ICS Matt 18037",null,"ICM 180 Wandhalter verstellbar 75 - 300mm DN 230mm","102293","0",null,"STK",77,null,null,null,null,{"$f":"IF(L3740=\"\",\"0\",H3740*L3740)","v":"0"}]
["ICS Matt",38,180,"ICS Matt 18038",null,"ICM 180 Wandhalter 50mm verlängerbar DN 230mm ","102307","0",null,"STK",55,{"$f":"ROUNDUP(M3741,0)","v":3},{"$f":"((M3703/1000)/4.3)","v":2.3255813953488373},null,null,{"$f":"IF(L3741=\"\",\"0\",H3741*L3741)","v":0}]
["ICS Matt",42,180,"ICS Matt 18042",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,500,null,"0"]
["ICS Matt",44,180,{"$f":"A3747&\" \"&C3747&B3747","v":"ICS Matt 18044"},null,"Rohrschelle Inox 1/2\" D230","104595","0",null,"STK",40,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",47,180,{"$f":"A3750&\" \"&C3750&B3750","v":"ICS Matt 18047"},null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,{"$f":"IF(L3750=\"\",\"0\",H3750*L3750)","v":"0"}]
["ICS Matt",48,180,{"$f":"A3751&\" \"&C3751&B3751","v":"ICS Matt 18048"},null,"ICM 150-180 Dachdurführung 0° DN250 L500mm","102325","0",null,"STK",163,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,{"$f":"IF(L3751=\"\",\"0\",H3751*L3751)","v":"0"}]
["ICS Matt",52,180,{"$f":"A3755&\" \"&C3755&B3755","v":"ICS Matt 18052"},null,"ICM 180 Regenkragen DN230","102375","0",null,"STK",55,{"$f":"IF(SUM(L3751:L3754)=0,\"\",SUM(L3751:L3754))","v":""},null,null,null,"0"]
["ICS Matt",53,180,"ICS Matt 18053",null,"ICM 180 Seilabspannring DN230","102389","0",null,"STK",77,null,null,null,null,"0"]
["ICS Matt",55,180,"ICS Matt 18055",null,"ICM 180 Blende 32-45° DN230","102411","0",null,"STK",83,{"$f":"IF(Daten!$E$515=3,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",58,180,"ICS Matt 18058",null,"ICM 180 Mündungsabschluss","102435",295,null,"STK",142,{"$f":"IF(Daten!$E$522=1,1,IF(Daten!$E$522=2,1,\"\"))","v":1},{"$f":"IF(L3761=\"\",\"0\",L3761*H3761)","v":295},null,null,{"$f":"IF(L3761=\"\",\"0\",H3761*L3761)","v":295}]
["ICS Matt",60,180,"ICS Matt 18060",null,"ICM 180 Element mit Messöffnung1/2\" L205mm","102456","0",null,"STK",195,null,{"$f":"IF(L3763=\"\",0,L3763*H3763)","v":0},null,null,"0"]
["ICS Matt",63,180,{"$f":"A3766&\" \"&C3766&B3766","v":"ICS Matt 18063"},null,"ICM 180 Winkel 15° ","102484","0",null,"STK",168,null,0,null,null,"0"]
["ICS Matt",66,180,"ICS Matt 18066",null,"ICM 180 Winkel 85°","102520","0",null,"STK",206,null,0,null,null,"0"]
["ICS Matt",68,180,"ICS Matt 18068",null,"ICM 180 Winkel 90°","102548","0",null,"STK",206,null,0,null,null,"0"]
[{"$f":"A3773","v":"ICS Matt"},{"$f":"B3773+1","v":1},{"$f":"C3773","v":200},{"$f":"A3774&\" \"&C3774&B3774","v":"ICS Matt 2001"},null,"ICM 200 Konsolenbleche (Paar)","101959","0",null,"STK",168,{"$f":"N3774","v":1},null,{"$f":"IF(Daten!$B$499=1,O3774,\"\")","v":1},{"$f":"IF(Daten!$B$549=1,1,\"\")","v":1},{"$f":"IF(L3774=\"\",\"0\",H3774*L3774)","v":0}]
["ICS Matt",4,200,"ICS Matt 2004",null,"ICM 720 Wandkonsolen  (Paar) L720mm","101977","0",null,"STK",228,{"$f":"IF(M3777=0,\"\",M3777)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3774=1,\"\",IF(Daten!$B$549=5,1,IF(Daten!$B$549=4,1))+O3777))))","v":0},"315-615",{"$f":"IF(Daten!$B$549=4,N3780,IF(Daten!$B$549=5,N3780,0))","v":0},null,"400/600"]
["ICS Matt",6,200,"ICS Matt 2006",null,"ICM 200 Verankerungsplatte mit Ablauf senkr.","101988",95,null,"STK",201,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L3779=\"\",\"0\",L3779*H3779)","v":95},null,null,{"$f":"IF(L3779=\"\",\"0\",H3779*L3779)","v":95}]
["ICS Matt",7,200,"ICS Matt 2007",null,"ICM 200 Zwischenstütze","102002",95,null,"STK",238,{"$f":"IF(N3780=0,\"\",N3780)","v":""},{"$f":"IF(L3780=\"\",0,L3780*H3780)","v":0},{"$f":"IF(M3773>=15000,1,0)","v":0},null,"0"]
["ICS Matt",11,200,"ICS Matt 20011",null,"ICM 200 Fussteil mit Kondensatablauf L1000mm","102056",1000,null,"STK",390,{"$f":"IF(Daten!$B$499=4,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",13,200,{"$f":"A3786&\" \"&C3786&B3786","v":"ICS Matt 20013"},null,"PPL 200 EW-DW Deckenanfängerset 45° kompl. L270mm","100659","0",null,"STK",648,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",16,200,{"$f":"A3789&\" \"&C3789&B3789","v":"ICS Matt 20016"},null,"ICM 200 T-Stück 45° L 530mm","102089",530,null,"STK",476,{"$f":"IF(Daten!$B$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",18,200,{"$f":"A3791&\" \"&C3791&B3791","v":"ICS Matt 20018"},null,"ICM 200 Verschlussdeckel mit Zugbegrenzer ","140843","0",null,"STK",380,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",21,200,"ICS Matt 20021",null,"ICM 200 Verschlussdeckel","102137","0",null,"STK",147,null,"0",null,null,"0"]
["ICS Matt",22,200,"ICS Matt 20022",null,"ICM 200 Anschluss von EW auf DW in Rauchgasr.","102151","0",null,"STK",142,1,0,null,null,0]
["ICS Matt",24,200,"ICS Matt 20024",null,"ICM 200 Anschluss DW/EW mit Klemmfutter DN200","102167","0",null,"STK",185,null,0,null,null,"0"]
["ICS Matt",27,200,"ICS Matt 20027",null,"ICM 200 Schiebe-Element mit Doppelfutter DN180 ","102245","0",null,"STK",347,null,0,null,null,"0"]
["ICS Matt",29,200,"ICS Matt 20029",null,"ICM 200 Längenelement L195mm","102189",150,null,"STK",93,null,0,null,null,"0"]
["ICS Matt",32,200,"ICS Matt 20032",null,"ICM 200 Längenelement L1000mm","102231",955,null,"STK",228,{"$f":"ROUNDUP(M3805,0)+N3805","v":9},{"$f":"((M3773-SUM(M3779:M3804)-M3831)/H3805)","v":8.6795811518324602},{"$f":"O3805/H3805","v":0},{"$f":"Daten!$DF$268*1000","v":0},{"$f":"(IF(L3805=\"\",0,H3805*L3805))-O3805","v":8595}]
[{"$f":"A3806","v":"ICS Matt"},{"$f":"B3806+1","v":34},{"$f":"C3806","v":200},"ICS Matt 20034",null,"ICM 200 Klemmband DN250","102266","0",null,"STK",20,null,null,null,null,{"$f":"IF(L3808=\"\",\"0\",H3808*L3808)","v":"0"}]
["ICS Matt",36,200,"ICS Matt 20036",null,"ICM 200 Wandhalter verstellbar 75 - 300mm DN 250mm","102294","0",null,"STK",82,null,null,null,null,{"$f":"IF(L3810=\"\",\"0\",H3810*L3810)","v":"0"}]
["ICS Matt",40,200,"ICS Matt 20040",null,"ICM L2 Verlängerung zu Wandhalter 50mm L450mm","102320","0",null,"STK",142,{"$f":"IF(Daten!$B$549=4,#REF!,\"\")","v":""},null,440,null,"0"]
["ICS Matt",41,200,"ICS Matt 20041",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,500,null,"0"]
["ICS Matt",44,200,"ICS Matt 20044",null,"PPL Innengewinderohr zu Rohrschelle 1/2\" 1000mm","101204","0",null,"STK",147,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",45,200,"ICS Matt 20045",null,"PPL Muffe 1/2\" zu Grundplatte 1/2\" Wandabst. 50mm","101205","0",null,"STK",20,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",49,200,"ICS Matt 20049",null,"ICM 200 Dachdurführung 26-35° DN320 mit Bleilappen","102350","0",null,"STK",476,{"$f":"IF(Daten!$B$522=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",51,200,"ICS Matt 20051",null,"ICM 200 Regenkragen DN250","102376","0",null,"STK",60,{"$f":"IF(SUM(L3821:L3824)=0,\"\",SUM(L3821:L3824))","v":""},null,null,null,"0"]
["ICS Matt",54,200,"ICS Matt 20054",null,"ICM 200 Blende 32-45° DN250","102412","0",null,"STK",87,{"$f":"IF(Daten!$E$515=3,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",57,200,"ICS Matt 20057",null,"ICM 200 Mündungsabschluss","102436",295,null,"STK",152,{"$f":"IF(Daten!$E$522=1,1,IF(Daten!$E$522=2,1,\"\"))","v":1},{"$f":"IF(L3831=\"\",\"0\",L3831*H3831)","v":295},null,null,{"$f":"IF(L3831=\"\",\"0\",H3831*L3831)","v":295}]
["ICS Matt",59,200,"ICS Matt 20059",null,"ICM 200 Element mit Messöffnung1/2\" L205mm","102457","0",null,"STK",206,null,{"$f":"IF(L3833=\"\",0,L3833*H3833)","v":0},null,null,"0"]
["ICS Matt",62,200,{"$f":"A3836&\" \"&C3836&B3836","v":"ICS Matt 20062"},null,"ICM 200 Winkel 15° ","102485","0",null,"STK",180,null,0,null,null,"0"]
["ICS Matt",64,200,"ICS Matt 20064",null,"ICM 200 Winkel 45°","102507","0",null,"STK",185,null,0,null,null,"0"]
["ICS Matt",65,200,"ICS Matt 20065",null,"ICM 200 Winkel 85°","102521","0",null,"STK",238,null,0,null,null,"0"]
["ICS Matt",68,200,"ICS Matt 20068",null,"ICM 200 Inspektions-Winkel 90°","102563","0",null,"STK",476,null,0,null,null,"0"]
[{"$f":"A3843","v":"ICS Matt"},{"$f":"B3843+1","v":1},{"$f":"C3843","v":250},"ICS Matt 2501",null,"ICM 250 Konsolenbleche (Paar)","101960","0",null,"STK",201,{"$f":"N3844","v":1},null,{"$f":"IF(Daten!$B$499=1,O3844,\"\")","v":1},{"$f":"IF(Daten!$B$549=1,1,\"\")","v":1},{"$f":"IF(L3844=\"\",\"0\",H3844*L3844)","v":0}]
["ICS Matt",4,250,"ICS Matt 2504",null,"ICM 720 Wandkonsolen  (Paar) L720mm","101977","0",null,"STK",228,{"$f":"IF(M3847=0,\"\",M3847)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3844=1,\"\",IF(Daten!$B$549=5,1,IF(Daten!$B$549=4,1))+O3847))))","v":0},"265-565",{"$f":"IF(Daten!$B$549=4,N3850,IF(Daten!$B$549=5,N3850,0))","v":0},null,"400/600"]
["ICS Matt",6,250,"ICS Matt 2506",null,"ICM 250 Verankerungsplatte mit Ablauf senkr.","101989",95,null,"STK",238,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L3849=\"\",\"0\",L3849*H3849)","v":95},null,null,{"$f":"IF(L3849=\"\",\"0\",H3849*L3849)","v":95}]
["ICS Matt",10,250,"ICS Matt 25010",null,"ICM 250 Teleskopstütze verstellbar L300 - 500mm","102045",300,null,"STK",380,{"$f":"IF(Daten!$B$499=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",11,250,"ICS Matt 25011",null,"ICM 250 Fussteil mit Kondensatablauf L1000mm","102057",1000,null,"STK",563,{"$f":"IF(Daten!$B$499=4,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",14,250,{"$f":"A3857&\" \"&C3857&B3857","v":"ICS Matt 25014"},null,"ICM 250 Putztüranschluss eckig Unterdruck L455mm","102062",411,null,"STK",390,{"$f":"IF(Daten!$B$490=2,\"\",Daten!$F$499)","v":1},411,null,null,411]
["ICS Matt",15,250,{"$f":"A3858&\" \"&C3858&B3858","v":"ICS Matt 25015"},null,"ICM 250 Putztüranschluss rund Überdruck L455mm","102076",455,null,"STK",504,{"$f":"IF(Daten!$B$490=1,\"\",Daten!$F$499)","v":""},"0",null,null,"0"]
["ICS Matt",19,250,{"$f":"A3862&\" \"&C3862&B3862","v":"ICS Matt 25019"},null,"ICM 250 T-Stück 85° L455mm","102118",455,null,"STK",428,{"$f":"IF(Daten!$B$515=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",21,250,{"$f":"A3864&\" \"&C3864&B3864","v":"ICS Matt 25021"},null,"ICM 250 Verschlussdeckel","102138","0",null,"STK",163,null,"0",null,null,"0"]
["ICS Matt",24,250,"ICS Matt 25024",null,"ICM 250 Anschluss von DW auf EW in Rauchgasr.","102176","0",null,"STK",152,null,{"$f":"IF(H3867=\"\",\"\",L3867*H3867)","v":0},null,null,"0"]
["ICS Matt",27,250,"ICS Matt 25027",null,"ICM 250 Längenelement L500mm","102218",455,null,"STK",152,{"$f":"IF(Daten!$DJ$259=0,\"\",Daten!$DJ$259)","v":""},{"$f":"IF(L3870=\"\",0,L3870*H3870)","v":0},{"$f":"O3870/H3870","v":0},{"$f":"Daten!$DF$260*1000","v":0},{"$f":"(IF(L3870=\"\",0,H3870*L3870))-O3870","v":0}]
[{"$f":"A3871","v":"ICS Matt"},{"$f":"B3871+1","v":29},{"$f":"C3871","v":250},{"$f":"A3872&\" \"&C3872&B3872","v":"ICS Matt 25029"},null,"ICM 250 Schiebe-Element L270-375mm","102253","0",null,"STK",260,null,null,null,null,{"$f":"IF(L3872=\"\",\"0\",H3872*L3872)","v":"0"}]
["ICS Matt",32,250,"ICS Matt 25032",null,"ICM 250 Statisches Klemmband DN300","102281","0",null,"STK",38,{"$f":"IF(N3875=0,\"\",N3875)","v":""},null,{"$f":"IF(Daten!$E$529=1,0,2)","v":0},null,{"$f":"IF(N3875=\"\",\"0\",H3875*N3875)","v":0}]
["ICS Matt",34,250,"ICS Matt 25034",null,"ICM 250 Wandhalter 50mm verlängerbar DN 300mm ","102309","0",null,"STK",65,{"$f":"ROUNDUP(M3877,0)","v":3},{"$f":"((M3843/1000)/4.3)","v":2.3255813953488373},null,null,{"$f":"IF(L3877=\"\",\"0\",H3877*L3877)","v":0}]
["ICS Matt",35,250,"ICS Matt 25035",null,"ICM W2 Verlängerung zu Wandhalter 50mm L 176mm","102318","0",null,"STK",65,{"$f":"IF(Daten!$B$549=2,#REF!,\"\")","v":""},null,114,null,"0"]
["ICS Matt",38,250,"ICS Matt 25038",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,470,null,"0"]
["ICS Matt",40,250,{"$f":"A3883&\" \"&C3883&B3883","v":"ICS Matt 25040"},null,"PPL 300 Rohrschelle Anschluss 1/2\" Aussengewinde","101202","0",null,"STK",44,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",43,250,"ICS Matt 25043",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",45,250,"ICS Matt 25045",null,"ICM 250-300 Dachdurführung 16-25° DN370 ","102339","0",null,"STK",444,{"$f":"IF(Daten!$B$522=3,1,\"\")","v":""},null,null,null,{"$f":"IF(L3888=\"\",\"0\",H3888*L3888)","v":"0"}]
["ICS Matt",49,250,"ICS Matt 25049",null,"ICM 250 Seilabspannring DN300","102391","0",null,"STK",87,null,null,null,null,"0"]
["ICS Matt",50,250,"ICS Matt 25050",null,"ICM 250 Blende 0-30° DN300","102405","0",null,"STK",87,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",52,250,"ICS Matt 25052",null,"ICM 250 Anschlussrosette Øi 300mm ØA 570mm","102421","0",null,"STK",68,{"$f":"IF(Daten!$E$515=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",55,250,"ICS Matt 25055",null,"ICM 250 Basten Standart mit Stulpring Inox matt","102450","0",null,"STK",418,{"$f":"IF(Daten!$E$522=3,1,\"\")","v":""},{"$f":"IF(L3898=\"\",\"0\",L3898*H3898)","v":"0"},null,null,"0"]
["ICS Matt",58,250,{"$f":"A3901&\" \"&C3901&B3901","v":"ICS Matt 25058"},null,"ICM 250 Element mit Kondensatablauf 1/2\" L205mm","102472","0",null,"STK",217,null,0,null,null,"0"]
["ICS Matt",60,250,"ICS Matt 25060",null,"ICM 250 Winkel 30°","102494","0",null,"STK",206,null,0,null,null,"0"]
["ICS Matt",63,250,"ICS Matt 25063",null,"ICM 250 Inspektions-Winkel 85°","102536","0",null,"STK",509,null,0,null,null,"0"]
["ICS Matt",0,300,"ICS Matt 3000"," ","Schiedel ICS MATT 25mm 300","ICS Matt 300","0",{"$f":"ICS!$J$10","v":10},"Anlage",0,1,{"$f":"I3909*1000","v":10000},null,{"$f":"ROUNDUP(P3909,2)","v":10.84},{"$f":"SUM(P3919:P3978)/1000","v":10.831}]
[{"$f":"A3910","v":"ICS Matt"},{"$f":"B3910+1","v":2},{"$f":"C3910","v":300},{"$f":"A3911&\" \"&C3911&B3911","v":"ICS Matt 3002"},null,"ICM 620 Wandkonsolen  (Paar) L620mm","101976","0",null,"STK",223,{"$f":"IF(M3911=0,\"\",M3911)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3910=1,0,IF(Daten!$B$549=2,1)+O3911))))","v":0},"79-215",{"$f":"IF(Daten!$B$549=2,N3920,0)","v":0},null,100]
["ICS Matt",3,300,"ICS Matt 3003",null,"ICM 720 Wandkonsolen  (Paar) L720mm","101977","0",null,"STK",228,{"$f":"IF(M3912=0,\"\",M3912)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M3911=1,0,IF(Daten!$B$549=3,1,IF(Daten!$B$549=4,1))+O3912))))","v":0},"215-515",{"$f":"IF(Daten!$B$549=3,N3920,IF(Daten!$B$549=4,N3920,0))","v":0},null,"250/400"]
["ICS Matt",7,300,{"$f":"A3916&\" \"&C3916&B3916","v":"ICS Matt 3007"},null,"ICM 1304 Wandkonsolen  (Paar) L1304mm","101981","0",null,"STK",315,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,{"$f":"IF(L3916=\"\",\"0\",H3916*L3916)","v":"0"}]
["ICS Matt",8,300,{"$f":"A3917&\" \"&C3917&B3917","v":"ICS Matt 3008"},null,"ICM 1504 Wandkonsolen  (Paar) L1504mm","101982","0",null,"STK",358,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,{"$f":"IF(L3917=\"\",\"0\",H3917*L3917)","v":"0"}]
["ICS Matt",12,300,"ICS Matt 30012",null,"ICM 300 Verankerungsplatte EW auf DW","102018",97,null,"STK",238,null,{"$f":"IF(L3921=\"\",\"0\",L3921*H3921)","v":"0"},null,null,"0"]
["ICS Matt",13,300,"ICS Matt 30013",null,"ICM 300 Kondensatschale mit Ablauf 1/2\"","102032",55,null,"STK",212,null,"0",null,null,"0"]
["ICS Matt",16,300,"ICS Matt 30016",null,"PPL 300 EW-DW Deckenanfängerset komplett L270mm","100654","0",null,"STK",595,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",18,300,"ICS Matt 30018",null,"ICM 300 Putztüranschluss eckig Unterdruck L455mm","102063",411,null,"STK",411,{"$f":"IF(Daten!$B$490=2,\"\",Daten!$F$499)","v":1},411,null,null,411]
[{"$f":"A3930","v":"ICS Matt"},{"$f":"B3930+1","v":22},{"$f":"C3930","v":300},{"$f":"A3931&\" \"&C3931&B3931","v":"ICS Matt 30022"},null,"ICM 300 Verschlussdeckel mit Zugbegrenzer ","140845","0",null,"STK",596,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
[{"$f":"A3931","v":"ICS Matt"},{"$f":"B3931+1","v":23},{"$f":"C3931","v":300},{"$f":"A3932&\" \"&C3932&B3932","v":"ICS Matt 30023"},null,"ICM 300 T-Stück 85° L485mm","102119",490,null,"STK",536,{"$f":"IF(Daten!$B$515=3,1,\"\")","v":""},"0",null,null,"0"]
[{"$f":"A3933","v":"ICS Matt"},{"$f":"B3933+1","v":25},{"$f":"C3933","v":300},{"$f":"A3934&\" \"&C3934&B3934","v":"ICS Matt 30025"},null,"ICM 300 Verschlussdeckel","102139","0",null,"STK",195,null,"0",null,null,"0"]
["ICS Matt",28,300,"ICS Matt 30028",null,"ICM 250 Anschluss von DW auf EW in Rauchgasr.","102176","0",null,"STK",152,null,{"$f":"IF(H3937=\"\",\"\",L3937*H3937)","v":0},null,null,"0"]
["ICS Matt",31,300,"ICS Matt 30031",null,"ICM 300 Längenelement L500mm","102219",455,null,"STK",195,{"$f":"IF(Daten!$DJ$259=0,\"\",Daten!$DJ$259)","v":""},{"$f":"IF(L3940=\"\",0,L3940*H3940)","v":0},{"$f":"O3940/H3940","v":0},{"$f":"Daten!$DF$260*1000","v":0},{"$f":"(IF(L3940=\"\",0,H3940*L3940))-O3940","v":0}]
["ICS Matt",33,300,"ICS Matt 30033",null,"ICM 300 Schiebe-Element L270-375mm","102254","0",null,"STK",293,null,null,null,null,{"$f":"IF(L3942=\"\",\"0\",H3942*L3942)","v":"0"}]
["ICS Matt",36,300,"ICS Matt 30036",null,"ICM 300 Statisches Klemmband DN350","102282","0",null,"STK",40,{"$f":"IF(N3945=0,\"\",N3945)","v":""},null,{"$f":"IF(Daten!$E$529=1,0,2)","v":0},null,{"$f":"IF(N3945=\"\",\"0\",H3945*N3945)","v":0}]
["ICS Matt",39,300,"ICS Matt 30039",null,"ICM W2 Verlängerung zu Wandhalter 50mm L 176mm","102318","0",null,"STK",65,{"$f":"IF(Daten!$B$549=2,#REF!,\"\")","v":""},null,114,null,"0"]
["ICS Matt",41,300,"ICS Matt 30041",null,"ICM L2 Verlängerung zu Wandhalter 50mm L450mm","102320","0",null,"STK",142,{"$f":"IF(Daten!$B$549=4,#REF!,\"\")","v":""},null,370,null,"0"]
["ICS Matt",42,300,"ICS Matt 30042",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,470,null,"0"]
["ICS Matt",46,300,"ICS Matt 30046",null,"PPL Muffe 1/2\" zu Grundplatte 1/2\" Wandabst. 50mm","101205","0",null,"STK",20,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",47,300,"ICS Matt 30047",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",51,300,"ICS Matt 30051",null,"ICM 250-300 Dachdurführung 36-45° DN370 ","102363","0",null,"STK",541,{"$f":"IF(Daten!$B$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",52,300,"ICS Matt 30052",null,"ICM 300 Regenkragen DN350","102378","0",null,"STK",77,{"$f":"IF(SUM(L3957:L3960)=0,\"\",SUM(L3957:L3960))","v":""},null,null,null,"0"]
["ICS Matt",56,300,"ICS Matt 30056",null,"ICM 300 Anschlussrosette Øi 350mm ØA 620mm","102422","0",null,"STK",71,{"$f":"IF(Daten!$E$515=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",57,300,"ICS Matt 30057",null,"ICM 250 Anschlussrosette EW Øi 300mm ØA 470mm","102429","0",null,"STK",49,null,null,null,null,{"$f":"IF(L3966=\"\",\"0\",H3966*L3966)","v":"0"}]
["ICS Matt",61,300,{"$f":"A3970&\" \"&C3970&B3970","v":"ICS Matt 30061"},null,"ICM 300 Element mit Empa Messstutzen","104669","0",null,"STK",736,null,null,null,null,"0"]
["ICS Matt",62,300,{"$f":"A3971&\" \"&C3971&B3971","v":"ICS Matt 30062"},null,"ICM 300 Element mit Kondensatablauf 1/2\" L205mm","102473","0",null,"STK",238,null,0,null,null,"0"]
["ICS Matt",64,300,"ICS Matt 30064",null,"ICM 300 Winkel 30°","102495","0",null,"STK",238,null,0,null,null,"0"]
["ICS Matt",67,300,"ICS Matt 30067",null,"ICM 300 Inspektions-Winkel 85°","102537","0",null,"STK",541,null,0,null,null,"0"]
["ICS Matt",0,350,"ICS Matt 3500"," ","Schiedel ICS MATT 25mm 350","ICS Matt 350","0",{"$f":"ICS!$J$10","v":10},"Anlage",0,1,{"$f":"I3979*1000","v":10000},null,{"$f":"ROUNDUP(P3979,2)","v":10.89},{"$f":"SUM(P3981:P4020)/1000","v":10.881}]
[{"$f":"A3980","v":"ICS Matt"},{"$f":"B3980+1","v":2},{"$f":"C3980","v":350},{"$f":"A3981&\" \"&C3981&B3981","v":"ICS Matt 3502"},null,"ICM 350 Verankerungsplatte mit Ablauf senkr.","101991",95,null,"STK",347,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L3981=\"\",\"0\",L3981*H3981)","v":95},null,null,{"$f":"IF(L3981=\"\",\"0\",H3981*L3981)","v":95}]
["ICS Matt",5,350,"ICS Matt 3505",null,"ICM 350 Kondensatschale mit Ablauf 1/2\"","102033",55,null,"STK",320,null,"0",null,null,"0"]
["ICS Matt",8,350,"ICS Matt 3508",null,"ICM 350 Putztüranschluss rund Überdruck L535mm","102078",535,null,"STK",720,{"$f":"IF(Daten!$B$490=1,\"\",Daten!$F$499)","v":""},"0",null,null,"0"]
["ICS Matt",10,350,"ICS Matt 35010",null,"ICM 350 T-Stück 90° L535mm","102106",530,null,"STK",752,{"$f":"IF(Daten!$B$515=2,1,\"\")","v":1},530,null,null,530]
["ICS Matt",11,350,{"$f":"A3990&\" \"&C3990&B3990","v":"ICS Matt 35011"},null,"ICM 350 Verschlussdeckel mit Zugbegrenzer ","140846","0",null,"STK",704,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",15,350,"ICS Matt 35015",null,"ICM 350 Anschluss von DW auf EW in Rauchgasr.","102178","0",null,"STK",195,null,{"$f":"IF(H3994=\"\",\"\",L3994*H3994)","v":0},null,null,"0"]
["ICS Matt",17,350,"ICS Matt 35017",null,"ICM 350 Längenelement L250mm","102206",205,null,"STK",217,{"$f":"IF(Daten!$DJ$251=0,\"\",Daten!$DJ$251)","v":""},{"$f":"IF(L3996=\"\",0,L3996*H3996)","v":0},{"$f":"O3996/H3996","v":0},{"$f":"Daten!$DF$252*1000","v":0},{"$f":"(IF(L3996=\"\",0,H3996*L3996))-O3996","v":0}]
[{"$f":"A3998","v":"ICS Matt"},{"$f":"B3998+1","v":20},{"$f":"C3998","v":350},{"$f":"A3999&\" \"&C3999&B3999","v":"ICS Matt 35020"},null,"ICM 350 Schiebe-Element L270-375mm","102255","0",null,"STK",325,null,{"$f":"IF(L3999=\"\",0,L3999*H3999)","v":0},null,null,{"$f":"IF(L3999=\"\",\"0\",H3999*L3999)","v":"0"}]
["ICS Matt",22,350,"ICS Matt 35022",null,"ICM 350 Klemmband DN400","102269","0",null,"STK",25,null,null,null,null,{"$f":"IF(L4001=\"\",\"0\",H4001*L4001)","v":"0"}]
["ICS Matt",25,350,"ICS Matt 35025",null,"ICM 350 Wandhalter 50mm verlängerbar DN 400mm ","102311","0",null,"STK",109,{"$f":"ROUNDUP(M4004,0)","v":3},{"$f":"((M3979/1000)/4.3)","v":2.3255813953488373},null,null,{"$f":"IF(L4004=\"\",\"0\",H4004*L4004)","v":0}]
["ICS Matt",26,350,"ICS Matt 35026",null,"ICM 350 Dachdurführung 0° DN450 L500mm","102329","0",null,"STK",341,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",30,350,"ICS Matt 35030",null,"ICM 350 Regenkragen DN400","102379","0",null,"STK",87,{"$f":"IF(SUM(L4005:L4008)=0,\"\",SUM(L4005:L4008))","v":""},null,null,null,"0"]
["ICS Matt",31,350,"ICS Matt 35031",null,"ICM 350 Seilabspannring DN400","102393","0",null,"STK",98,null,null,null,null,"0"]
["ICS Matt",33,350,"ICS Matt 35033",null,"ICM 350 Element mit Messöffnung1/2\" L205mm","102460","0",null,"STK",260,null,{"$f":"IF(L4012=\"\",0,L4012*H4012)","v":0},null,null,"0"]
["ICS Matt",36,350,{"$f":"A4015&\" \"&C4015&B4015","v":"ICS Matt 35036"},null,"ICM 350 Winkel 30°","102496","0",null,"STK",325,null,0,null,null,"0"]
["ICS Matt",39,350,"ICS Matt 35039",null,"ICM 350 Inspektions-Winkel 85°","102538","0",null,"STK",639,null,0,null,null,"0"]
["ICS Matt",41,350,"ICS Matt 35041",null,"ICM 350 Inspektions-Winkel 90°","102566","0",null,"STK",639,null,0,null,null,"0"]
["ICS Matt",3,400,"ICS Matt 4003",null,"ICM 400 Zwischenstütze","102006",95,null,"STK",411,{"$f":"IF(N4024=0,\"\",N4024)","v":""},{"$f":"IF(L4024=\"\",0,L4024*H4024)","v":0},{"$f":"IF(M4021>=15000,1,0)","v":0},null,{"$f":"IF(L4024=\"\",\"0\",H4024*L4024)","v":"0"}]
["ICS Matt",4,400,"ICS Matt 4004",null,"ICM 400 Verankerungsplatte EW auf DW","102020",97,null,"STK",325,null,{"$f":"IF(L4025=\"\",\"0\",L4025*H4025)","v":"0"},null,null,{"$f":"IF(L4025=\"\",\"0\",H4025*L4025)","v":"0"}]
["ICS Matt",7,400,"ICS Matt 4007",null,"ICM 400 Putztüranschluss eckig Unterdruck L455mm","102065",411,null,"STK",520,{"$f":"IF(Daten!$B$490=2,\"\",Daten!$F$499)","v":1},411,null,null,411]
["ICS Matt",8,400,"ICS Matt 4008",null,"ICM 400 Putztüranschluss rund Überdruck L705mm","102079",705,null,"STK",1028,{"$f":"IF(Daten!$B$490=1,\"\",Daten!$F$499)","v":""},"0",null,null,"0"]
["ICS Matt",12,400,"ICS Matt 40012",null,"ICM 400 Verschlussdeckel","102141","0",null,"STK",260,null,"0",null,null,"0"]
["ICS Matt",14,400,"ICS Matt 40014",null,"ICM 400 Anschluss von DW auf EW in Rauchgasr.","102179","0",null,"STK",315,null,{"$f":"IF(H4035=\"\",\"\",L4035*H4035)","v":0},null,null,"0"]
["ICS Matt",17,400,"ICS Matt 40017",null,"ICM 400 Längenelement L500mm","102221",455,null,"STK",320,{"$f":"IF(Daten!$DJ$259=0,\"\",Daten!$DJ$259)","v":""},{"$f":"IF(L4038=\"\",0,L4038*H4038)","v":0},{"$f":"O4038/H4038","v":0},{"$f":"Daten!$DF$260*1000","v":0},{"$f":"(IF(L4038=\"\",0,H4038*L4038))-O4038","v":0}]
[{"$f":"A4039","v":"ICS Matt"},{"$f":"B4039+1","v":19},{"$f":"C4039","v":400},{"$f":"A4040&\" \"&C4040&B4040","v":"ICS Matt 40019"},null,"ICM 400 Schiebe-Element L270-375mm","102256","0",null,"STK",536,null,{"$f":"IF(L4040=\"\",0,L4040*H4040)","v":0},null,null,{"$f":"IF(L4040=\"\",\"0\",H4040*L4040)","v":"0"}]
["ICS Matt",22,400,"ICS Matt 40022",null,"ICM 400 Statisches Klemmband DN450","102284","0",null,"STK",49,{"$f":"IF(N4043=0,\"\",N4043)","v":""},null,{"$f":"IF(Daten!$E$529=1,0,2)","v":0},null,{"$f":"IF(N4043=\"\",\"0\",H4043*N4043)","v":0}]
["ICS Matt",23,400,"ICS Matt 40023",null,"ICM 400 Wandhalter verstellbar 75 - 300mm DN 450mm","102298","0",null,"STK",109,null,null,null,null,{"$f":"IF(L4044=\"\",\"0\",H4044*L4044)","v":"0"}]
["ICS Matt",25,400,"ICS Matt 40025",null,"ICM 400 Dachdurführung 0° DN500 L500mm","102330","0",null,"STK",488,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",28,400,"ICS Matt 40028",null,"ICM 400 Dachdurführung 36-45° DN500 mit Bleilappen","102366","0",null,"STK",920,{"$f":"IF(Daten!$B$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",30,400,"ICS Matt 40030",null,"ICM 400 Seilabspannring DN450","102394","0",null,"STK",109,null,null,null,null,"0"]
["ICS Matt",33,400,"ICS Matt 40033",null,"ICM 400 Element mit Kondensatablauf 1/2\" L205mm","102475","0",null,"STK",325,null,0,null,null,"0"]
["ICS Matt",36,400,"ICS Matt 40036",null,"ICM 400 Winkel 85°","102525","0",null,"STK",596,null,0,null,null,"0"]
["ICS Matt",38,400,"ICS Matt 40038",null,"ICM 400 Winkel 90°","102553","0",null,"STK",596,null,0,null,null,"0"]
[{"$f":"A4062","v":"ICS Matt"},{"$f":"B4062+1","v":2},{"$f":"C4062","v":450},{"$f":"A4063&\" \"&C4063&B4063","v":"ICS Matt 4502"},null,"ICM 450 Verankerungsplatte mit Ablauf senkr.","101993",95,null,"STK",628,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L4063=\"\",\"0\",L4063*H4063)","v":95},null,null,{"$f":"IF(L4063=\"\",\"0\",H4063*L4063)","v":95}]
["ICS Matt",3,450,"ICS Matt 4503",null,"ICM 450 Zwischenstütze","102007",95,null,"STK",541,{"$f":"IF(N4064=0,\"\",N4064)","v":""},{"$f":"IF(L4064=\"\",0,L4064*H4064)","v":0},{"$f":"IF(M4061>=15000,1,0)","v":0},null,{"$f":"IF(L4064=\"\",\"0\",H4064*L4064)","v":"0"}]
["ICS Matt",6,450,"ICS Matt 4506",null,"ICM 450 Teleskopstütze verstellbar L300 - 500mm","102049",300,null,"STK",736,{"$f":"IF(Daten!$B$499=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",7,450,"ICS Matt 4507",null,"ICM 450 Putztüranschluss eckig Unterdruck L455mm","102066",411,null,"STK",649,{"$f":"IF(Daten!$B$490=2,\"\",Daten!$F$499)","v":1},411,null,null,411]
["ICS Matt",11,450,"ICS Matt 45011",null,"ICM 450 T-Stück 85° L705mm","102122",655,null,"STK",1726,{"$f":"IF(Daten!$B$515=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",13,450,"ICS Matt 45013",null,"ICM 450 Anschluss von EW auf DW in Rauchgasr.","102156","0",null,"STK",368,1,0,null,null,0]
["ICS Matt",16,450,"ICS Matt 45016",null,"ICM 450 Längenelement L250mm","102208",205,null,"STK",374,{"$f":"IF(Daten!$DJ$251=0,\"\",Daten!$DJ$251)","v":""},{"$f":"IF(L4077=\"\",0,L4077*H4077)","v":0},{"$f":"O4077/H4077","v":0},{"$f":"Daten!$DF$252*1000","v":0},{"$f":"(IF(L4077=\"\",0,H4077*L4077))-O4077","v":0}]
["ICS Matt",19,450,"ICS Matt 45019",null,"ICM 450 Schiebe-Element L270-375mm","102257","0",null,"STK",644,null,{"$f":"IF(L4080=\"\",0,L4080*H4080)","v":0},null,null,{"$f":"IF(L4080=\"\",\"0\",H4080*L4080)","v":"0"}]
[{"$f":"A4081","v":"ICS Matt"},{"$f":"B4081+1","v":21},{"$f":"C4081","v":450},"ICS Matt 45021",null,"ICM 450 Klemmband DN500","102271","0",null,"STK",29,null,null,null,null,{"$f":"IF(L4082=\"\",\"0\",H4082*L4082)","v":"0"}]
[{"$f":"A4084","v":"ICS Matt"},{"$f":"B4084+1","v":24},{"$f":"C4084","v":450},"ICS Matt 45024",null,"ICM 450 Wandhalter 50mm verlängerbar DN 500mm ","102313","0",null,"STK",152,{"$f":"ROUNDUP(M4085,0)","v":3},{"$f":"((M4061/1000)/4.3)","v":2.3255813953488373},null,null,{"$f":"IF(L4085=\"\",\"0\",H4085*L4085)","v":0}]
["ICS Matt",26,450,"ICS Matt 45026",null,"ICM 450 Dachdurführung 16-25° DN550 mit Bleilappen","102343","0",null,"STK",812,{"$f":"IF(Daten!$B$522=3,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",27,450,"ICS Matt 45027",null,"ICM 450 Dachdurführung 26-35° DN550 mit Bleilappen","102355","0",null,"STK",822,{"$f":"IF(Daten!$B$522=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",29,450,"ICS Matt 45029",null,"ICM 450 Regenkragen DN500","102381","0",null,"STK",109,{"$f":"IF(SUM(L4086:L4089)=0,\"\",SUM(L4086:L4089))","v":""},null,null,null,"0"]
["ICS Matt",32,450,"ICS Matt 45032",null,"ICM 450 Element mit Messöffnung1/2\" L205mm","102462","0",null,"STK",488,null,{"$f":"IF(L4093=\"\",0,L4093*H4093)","v":0},null,null,"0"]
["ICS Matt",35,450,"ICS Matt 45035",null,"ICM 450 Winkel 45°","102512","0",null,"STK",541,null,0,null,null,"0"]
["ICS Matt",37,450,"ICS Matt 45037",null,"ICM 450 Inspektions-Winkel 85°","102540","0",null,"STK",1072,null,0,null,null,"0"]
[{"$f":"A4101","v":"ICS Matt"},{"$f":"B4101+1","v":1},{"$f":"C4101","v":500},"ICS Matt 5001",null,"ICM 500 Konsolenbleche (Paar) ","101965","0",null,"STK",536,{"$f":"IF(N4102=0,\"\",N4102)","v":1},{"$f":"N4102","v":1},{"$f":"IF(Daten!$B$499=1,1,0)+N4104","v":1},null,{"$f":"IF(M4102=\"\",\"0\",H4102*M4102)","v":0}]
[{"$f":"A4102","v":"ICS Matt"},{"$f":"B4102+1","v":2},{"$f":"C4102","v":500},{"$f":"A4103&\" \"&C4103&B4103","v":"ICS Matt 5002"},null,"ICM 500 Verankerungsplatte mit Ablauf senkr.","101994",95,null,"STK",844,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L4103=\"\",\"0\",L4103*H4103)","v":95},null,null,{"$f":"IF(L4103=\"\",\"0\",H4103*L4103)","v":95}]
["ICS Matt",4,500,"ICS Matt 5004",null,"ICM 500 Verankerungsplatte EW auf DW","102022",97,null,"STK",488,null,{"$f":"IF(L4105=\"\",\"0\",L4105*H4105)","v":"0"},null,null,{"$f":"IF(L4105=\"\",\"0\",H4105*L4105)","v":"0"}]
["ICS Matt",7,500,"ICS Matt 5007",null,"ICM 500 Putztüranschluss eckig Unterdruck L455mm","102067",411,null,"STK",812,{"$f":"IF(Daten!$B$490=2,\"\",Daten!$F$499)","v":1},411,null,null,411]
["ICS Matt",10,500,"ICS Matt 50010",null,"ICM 500 T-Stück 90° L705mm","102109",705,null,"STK",2050,{"$f":"IF(Daten!$B$515=2,1,\"\")","v":1},705,null,null,705]
["ICS Matt",12,500,"ICS Matt 50012",null,"ICM 500 Verschlussdeckel","102143","0",null,"STK",428,null,"0",null,null,"0"]
["ICS Matt",15,500,"ICS Matt 50015",null,"ICM 500 Längenelement L195mm","102195",150,null,"STK",423,null,{"$f":"IF(H4116=\"\",\"\",L4116*H4116)","v":0},null,null,"0"]
["ICS Matt",18,500,"ICS Matt 50018",null,"ICM 500 Längenelement L1000mm","102237",955,null,"STK",644,{"$f":"ROUNDUP(M4119,0)+N4119","v":9},{"$f":"((M4101-SUM(M4103:M4118)-M4132)/H4119)","v":8.8942408376963353},{"$f":"O4119/H4119","v":0},{"$f":"Daten!$DF$268*1000","v":0},{"$f":"(IF(L4119=\"\",0,H4119*L4119))-O4119","v":8595}]
["ICS Matt",20,500,"ICS Matt 50020",null,"PPL 500 Dichtung Silikon","101000","0",null,"STK",33,{"$f":"IF(Daten!$B$490=1,\"\",SUM(L4103:L4106,L4108:L4114,L4116:L4119,L4135:L4140,L4132))","v":""},{"$f":"IF(L4121=\"\",\"\",L4121*H4121)","v":""},null,null,{"$f":"IF(L4121=\"\",\"0\",H4121*L4121)","v":"0"}]
["ICS Matt",23,500,"ICS Matt 50023",null,"ICM 500 Wandhalter verstellbar 75 - 300mm DN 550mm","102300","0",null,"STK",163,null,null,null,null,{"$f":"IF(L4124=\"\",\"0\",H4124*L4124)","v":"0"}]
["ICS Matt",25,500,"ICS Matt 50025",null,"ICM 500 Dachdurführung 0° DN600 L500mm","102332","0",null,"STK",812,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",26,500,"ICS Matt 50026",null,"ICM 500 Dachdurführung 16-25° DN600 mit Bleilappen","102344","0",null,"STK",920,{"$f":"IF(Daten!$B$522=3,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",29,500,"ICS Matt 50029",null,"ICM 500 Regenkragen DN550","102382","0",null,"STK",130,{"$f":"IF(SUM(L4126:L4129)=0,\"\",SUM(L4126:L4129))","v":""},null,null,null,"0"]
["ICS Matt",31,500,"ICS Matt 50031",null,"ICM 500 Mündungsabschluss","102442",295,null,"STK",509,{"$f":"IF(Daten!$E$522=1,1,IF(Daten!$E$522=2,1,\"\"))","v":1},{"$f":"IF(L4132=\"\",\"0\",L4132*H4132)","v":295},null,null,295]
["ICS Matt",34,500,"ICS Matt 50034",null,"ICM 500 Winkel 30°","102499","0",null,"STK",671,null,0,null,null,"0"]
["ICS Matt",36,500,"ICS Matt 50036",null,"ICM 500 Winkel 85°","102527","0",null,"STK",974,null,0,null,null,"0"]
["ICS Matt",0,600,"ICS Matt 6000"," ","Schiedel ICS MATT 25mm 600","ICS Matt 600","0",{"$f":"ICS!$J$10","v":10},"Anlage",0,1,{"$f":"I4141*1000","v":10000},null,{"$f":"ROUNDUP(P4141,2)","v":10.209999999999999},{"$f":"SUM(P4143:P4180)/1000","v":10.201000000000001}]
[{"$f":"A4141","v":"ICS Matt"},{"$f":"B4141+1","v":1},{"$f":"C4141","v":600},"ICS Matt 6001",null,"ICM 600 Konsolenbleche (Paar)","101966","0",null,"STK",623,{"$f":"IF(N4142=0,\"\",N4142)","v":1},{"$f":"N4142","v":1},{"$f":"IF(Daten!$B$499=1,1,0)+N4144","v":1},null,{"$f":"IF(M4142=\"\",\"0\",H4142*M4142)","v":0}]
["ICS Matt",3,600,"ICS Matt 6003",null,"ICM 600 Zwischenstütze","102009",95,null,"STK",920,{"$f":"IF(N4144=0,\"\",N4144)","v":""},{"$f":"IF(L4144=\"\",0,L4144*H4144)","v":0},{"$f":"IF(M4141>=15000,1,0)","v":0},null,{"$f":"IF(L4144=\"\",\"0\",H4144*L4144)","v":"0"}]
["ICS Matt",6,600,"ICS Matt 6006",null,"ICM 600 Teleskopstütze verstellbar L300 - 500mm","102051",300,null,"STK",1137,{"$f":"IF(Daten!$B$499=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",9,600,"ICS Matt 6009",null,"ICM 600 T-Stück 45° L 1100mm","102096",1100,null,"STK",3559,{"$f":"IF(Daten!$B$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",11,600,"ICS Matt 60011",null,"ICM 600 T-Stück 85° L705mm","102124",805,null,"STK",2375,{"$f":"IF(Daten!$B$515=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Matt",14,600,"ICS Matt 60014",null,"ICM 600 Anschluss von DW auf EW in Rauchgasr.","102182","0",null,"STK",531,null,{"$f":"IF(H4155=\"\",\"\",L4155*H4155)","v":0},null,null,"0"]
["ICS Matt",17,600,"ICS Matt 60017",null,"ICM 600 Längenelement L500mm","102224",455,null,"STK",644,{"$f":"IF(Daten!$DJ$259=0,\"\",Daten!$DJ$259)","v":""},{"$f":"IF(L4158=\"\",0,L4158*H4158)","v":0},{"$f":"O4158/H4158","v":0},{"$f":"Daten!$DF$260*1000","v":0},{"$f":"(IF(L4158=\"\",0,H4158*L4158))-O4158","v":0}]
["ICS Matt",19,600,"ICS Matt 60019",null,"ICM 600 Schiebe-Element L270-375mm","102259","0",null,"STK",915,null,{"$f":"IF(L4160=\"\",0,L4160*H4160)","v":0},null,null,{"$f":"IF(L4160=\"\",\"0\",H4160*L4160)","v":"0"}]
["ICS Matt",20,600,"ICS Matt 60020",null,"PPL 600 Dichtung Silikon","101001","0",null,"STK",39,{"$f":"IF(Daten!$B$490=1,\"\",SUM(L4143:L4146,L4148:L4154,L4156:L4159,L4175:L4180,L4172))","v":""},{"$f":"IF(L4161=\"\",\"\",L4161*H4161)","v":""},null,null,{"$f":"IF(L4161=\"\",\"0\",H4161*L4161)","v":"0"}]
["ICS Matt",24,600,"ICS Matt 60024",null,"ICM 600 Wandhalter 50mm verlängerbar DN 650mm  ","102315","0",null,"STK",228,{"$f":"ROUNDUP(M4165,0)","v":3},{"$f":"((M4141/1000)/4.3)","v":2.3255813953488373},null,null,{"$f":"IF(L4165=\"\",\"0\",H4165*L4165)","v":0}]
["ICS Matt",25,600,"ICS Matt 60025",null,"ICM 600 Dachdurführung 0° DN700 L500mm","102333","0",null,"STK",974,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",29,600,"ICS Matt 60029",null,"ICM 600 Regenkragen DN650","102383","0",null,"STK",152,{"$f":"IF(SUM(L4166:L4169)=0,\"\",SUM(L4166:L4169))","v":""},null,null,null,"0"]
["ICS Matt",30,600,"ICS Matt 60030",null,"ICM 600 Seilabspannring DN650","102397","0",null,"STK",174,null,null,null,null,"0"]
["ICS Matt",33,600,"ICS Matt 60033",null,"ICM 600 Element mit Kondensatablauf 1/2\" L205mm","102478","0",null,"STK",920,null,0,null,null,"0"]
["ICS Matt",35,600,"ICS Matt 60035",null,"ICM 600 Winkel 45°","102514","0",null,"STK",812,null,0,null,null,"0"]
["ICS Matt",39,600,"ICS Matt 60039",null,"ICM 600 Inspektions-Winkel 90°","102570","0",null,"STK",1721,null,0,null,null,"0"]
["ICS Matt",0,700,"ICS Matt 7000"," ","Schiedel ICS MATT 25mm 700","ICS Matt 700","0",{"$f":"ICS!$J$10","v":10},"Anlage",0,1,{"$f":"I4181*1000","v":10000},null,{"$f":"ROUNDUP(P4181,2)","v":10.31},{"$f":"SUM(P4183:P4220)/1000","v":10.301}]
[{"$f":"A4182","v":"ICS Matt"},{"$f":"B4182+1","v":2},{"$f":"C4182","v":700},{"$f":"A4183&\" \"&C4183&B4183","v":"ICS Matt 7002"},null,"ICM 700 Verankerungsplatte mit Ablauf senkr.","101996",95,null,"STK",1277,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L4183=\"\",\"0\",L4183*H4183)","v":95},null,null,{"$f":"IF(L4183=\"\",\"0\",H4183*L4183)","v":95}]
["ICS Matt",5,700,"ICS Matt 7005",null,"ICS 700 Kondensatschale mit Ablauf 1/2\"","102038",55,null,"STK",716,null,"0",null,null,"0"]
["ICS Matt",8,700,"ICS Matt 7008",null,"ICM 700 Putztüranschluss rund Überdruck L705mm","102083",705,null,"STK",2272,{"$f":"IF(Daten!$B$490=1,\"\",Daten!$F$499)","v":""},"0",null,null,"0"]
["ICS Matt",10,700,"ICS Matt 70010",null,"ICM 700 T-Stück 90° L705mm","102111",905,null,"STK",2807,{"$f":"IF(Daten!$B$515=2,1,\"\")","v":1},905,null,null,905]
["ICS Matt",13,700,"ICS Matt 70013",null,"ICM 700 Anschluss von EW auf DW in Rauchgasr.","102159","0",null,"STK",747,1,0,null,null,0]
["ICS Matt",16,700,"ICS Matt 70016",null,"ICM 700 Längenelement L250mm","102211",205,null,"STK",644,{"$f":"IF(Daten!$DJ$251=0,\"\",Daten!$DJ$251)","v":""},{"$f":"IF(L4197=\"\",0,L4197*H4197)","v":0},{"$f":"O4197/H4197","v":0},{"$f":"Daten!$DF$252*1000","v":0},{"$f":"(IF(L4197=\"\",0,H4197*L4197))-O4197","v":0}]
["ICS Matt",18,700,"ICS Matt 70018",null,"ICM 700 Längenelement L1000mm","102239",955,null,"STK",969,{"$f":"ROUNDUP(M4199,0)+N4199","v":9},{"$f":"((M4181-SUM(M4183:M4198)-M4212)/H4199)","v":8.684816753926702},{"$f":"O4199/H4199","v":0},{"$f":"Daten!$DF$268*1000","v":0},{"$f":"(IF(L4199=\"\",0,H4199*L4199))-O4199","v":8595}]
[{"$f":"A4199","v":"ICS Matt"},{"$f":"B4199+1","v":19},{"$f":"C4199","v":700},{"$f":"A4200&\" \"&C4200&B4200","v":"ICS Matt 70019"},null,"ICM 700 Schiebe-Element L270-375mm","102260","0",null,"STK",1077,null,{"$f":"IF(L4200=\"\",0,L4200*H4200)","v":0},null,null,{"$f":"IF(L4200=\"\",\"0\",H4200*L4200)","v":"0"}]
["ICS Matt",23,700,"ICS Matt 70023",null,"ICM 700 Wandhalter verstellbar 75 - 300mm DN 750mm","102302","0",null,"STK",271,null,null,null,null,{"$f":"IF(L4204=\"\",\"0\",H4204*L4204)","v":"0"}]
["ICS Matt",24,700,"ICS Matt 70024",null,"ICM 700 Wandhalter 50mm verlängerbar DN 750mm ","102316","0",null,"STK",282,{"$f":"ROUNDUP(M4205,0)","v":3},{"$f":"((M4181/1000)/4.3)","v":2.3255813953488373},null,null,{"$f":"IF(L4205=\"\",\"0\",H4205*L4205)","v":0}]
["ICS Matt",28,700,"ICS Matt 70028",null,"ICM 700 Dachdurführung 36-45° DN800 mit Bleilappen","102370","0",null,"STK",1785,{"$f":"IF(Daten!$B$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS Matt",29,700,"ICS Matt 70029",null,"ICM 700 Regenkragen DN750","102384","0",null,"STK",174,{"$f":"IF(SUM(L4206:L4209)=0,\"\",SUM(L4206:L4209))","v":""},null,null,null,"0"]
["ICS Matt",33,700,"ICS Matt 70033",null,"ICM 700 Element mit Kondensatablauf 1/2\" L205mm","102479","0",null,"STK",1190,null,0,null,null,"0"]
["ICS Matt",34,700,"ICS Matt 70034",null,"ICM 700 Winkel 30°","102501","0",null,"STK",974,null,0,null,null,"0"]
["ICS Matt",38,700,"ICS Matt 70038",null,"ICM 700 Winkel 90°","102557","0",null,"STK",1406,null,0,null,null,"0"]
["ICS Matt",39,700,"ICS Matt 70039",null,"ICM 700 Inspektions-Winkel 90°","102571","0",null,"STK",2153,null,0,null,null,"0"]
[{"$f":"A4221","v":"ICS Kupfer"},{"$f":"B4221+1","v":1},{"$f":"C4221","v":80},{"$f":"A4222&\" \"&C4222&B4222","v":"ICS Kupfer 801"},null,"ICK 80 Konsolenbleche (Paar)","102574","0",null,"STK",135,{"$f":"N4222","v":1},{"$f":"IF(Daten!$B$549=1,1,\"\")","v":1},{"$f":"IF(Daten!$B$499=1,M4222,\"\")","v":1},null,{"$f":"IF(L4222=\"\",\"0\",H4222*L4222)","v":0}]
["ICS Kupfer",4,80,"ICS Kupfer 804",null,"ICK 800 Wandkonsolen (Paar) L600mm","102584","0",null,"STK",324,{"$f":"IF(M4225=0,\"\",M4225)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4222=1,\"\",IF(Daten!$B$549=4,1)+O4225))))","v":""},"312-412",{"$f":"IF(Daten!$B$549=4,N4228,0)","v":0},null,400]
["ICS Kupfer",7,80,"ICS Kupfer 807",null,"ICK 80 Zwischenstütze","102595",95,null,"STK",240,{"$f":"IF(N4228=0,\"\",N4228)","v":""},{"$f":"IF(L4228=\"\",0,L4228*H4228)","v":0},{"$f":"IF(M4221>=15000,1,0)","v":0},null,{"$f":"IF(L4228=\"\",\"0\",H4228*L4228)","v":"0"}]
["ICS Kupfer",9,80,"ICS Kupfer 809",null,"ICK 80 Kondensatschale mit Ablauf 1/2\"","102611",55,null,"STK",107,null,"0",null,null,"0"]
["ICS Kupfer",12,80,"ICS Kupfer 8012",null,"ICK 80 T-Stück 45° L 330mm","102646",330,null,"STK",268,{"$f":"IF(Daten!$B$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS Kupfer",15,80,"ICS Kupfer 8015",null,"ICK 80 Anschluss von EW auf DW in Rauchgasr.","102670","0",null,"STK",114,1,{"$f":"IF(L4236=\"\",\"0\",L4236*H4236)","v":0},null,null,{"$f":"IF(L4236=\"\",\"0\",H4237*L4236)","v":0}]
[{"$f":"A4237","v":"ICS Kupfer"},{"$f":"B4237+1","v":17},{"$f":"C4237","v":80},{"$f":"A4238&\" \"&C4238&B4238","v":"ICS Kupfer 8017"},null,"ICK 80 Anschluss von DW auf EW in Rauchgasr.","102688","0",null,"STK",114,null,{"$f":"IF(H4238=\"\",\"\",L4238*H4238)","v":0}]
[{"$f":"A4237","v":"ICS Kupfer"},{"$f":"B4237+1","v":17},{"$f":"C4237","v":80},"ICS Kupfer 8017",null,"ICK 80 Längenelement L195mm","102696",150,null,"STK",85,null,{"$f":"IF(H4239=\"\",\"\",L4239*H4239)","v":0},null,null,{"$f":"IF(L4239=\"\",\"0\",H4239*L4239)","v":"0"}]
[{"$f":"A4242","v":"ICS Kupfer"},{"$f":"B4242+1","v":21},{"$f":"C4242","v":80},{"$f":"A4243&\" \"&C4243&B4243","v":"ICS Kupfer 8021"},null,"ICK 80 Schiebe-Element L270-375mm","102728","0",null,"STK",212,null,null,null,null,{"$f":"IF(L4243=\"\",\"0\",H4243*L4243)","v":"0"}]
["ICS Kupfer",23,80,"ICS Kupfer 8023",null,"ICK 80 Klemmband DN130","102736","0",null,"STK",19,null,null,null,null,{"$f":"IF(L4245=\"\",\"0\",H4245*L4245)","v":"0"}]
["ICS Kupfer",26,80,"ICS Kupfer 8026",null,"ICK 80 Wandhalter verstellbar 75 - 300mm DN 130mm","102760","0",null,"STK",72,null,null,"75-300",null,"0"]
["ICS Kupfer",28,80,"ICS Kupfer 8028",null,"ICK W1 Verlängerung zu Wandhalter 50mm L 130mm","102776","0",null,"STK",57,{"$f":"IF(Daten!$B$549=2,$L4249,\"\")","v":""},null,100,null,"0"]
["ICS Kupfer",31,80,"ICS Kupfer 8031",null,"ICK L3 Verlängerung zu Wandhalter 50mm L 550mm","102780","0",null,"STK",212,null,null,500,null,"0"]
["ICS Kupfer",32,80,"ICS Kupfer 8032",null,"ICK L4 Verlängerung zu Wandhalter 50mm L 750mm","102781","0",null,"STK",254,{"$f":"IF(Daten!$B$549=5,$L4249,\"\")","v":""},null,700,null,"0"]
["ICS Kupfer",36,80,"ICS Kupfer 8036",null,"ICK 80-100 Dachdurführung 36-45° DN165  ","102797","0",null,"STK",522,{"$f":"IF(Daten!$B$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",37,80,"ICS Kupfer 8037",null,"ICK 80 Regenkragen DN130 ","102802","0",null,"STK",43,{"$f":"IF(SUM(L4255:L4258)=0,\"\",SUM(L4255:L4258))","v":""},null,null,null,"0"]
["ICS Kupfer",39,80,"ICS Kupfer 8039",null,"ICK 80 Blende 0-30° DN130 ","102818","0",null,"STK",79,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",42,80,"ICS Kupfer 8042",null,"ICK 80 Mündungsabschluss","102842",295,null,"STK",142,{"$f":"IF(Daten!$E$522=1,1,IF(Daten!$E$522=2,1,\"\"))","v":1},{"$f":"IF(L4264=\"\",\"0\",L4264*H4264)","v":295},null,null,{"$f":"IF(L4264=\"\",\"0\",H4264*L4264)","v":295}]
["ICS Kupfer",45,80,"ICS Kupfer 8045",null,"ICK 80 Winkel 15°","102873","0",null,"STK",169,null,0,null,null,"0"]
["ICS Kupfer",47,80,"ICS Kupfer 8047",null,"ICK 80 Winkel 45°","102889","0",null,"STK",169,null,0,null,null,"0"]
[{"$f":"A4272","v":"ICS Kupfer"},{"$f":"B4272+1","v":1},{"$f":"C4272","v":100},{"$f":"A4273&\" \"&C4273&B4273","v":"ICS Kupfer 1001"},null,"ICK 100 Konsolenbleche (Paar)","102575","0",null,"STK",163,{"$f":"N4273","v":1},{"$f":"IF(Daten!$B$549=1,1,\"\")","v":1},{"$f":"IF(Daten!$B$499=1,M4273,\"\")","v":1},null,{"$f":"IF(L4273=\"\",\"0\",H4273*L4273)","v":0}]
[{"$f":"A4273","v":"ICS Kupfer"},{"$f":"B4273+1","v":2},{"$f":"C4273","v":100},{"$f":"A4274&\" \"&C4274&B4274","v":"ICS Kupfer 1002"},null,"ICK 700 Wandkonsolen (Paar) L500mm","102582","0",null,"STK",233,{"$f":"IF(M4274=0,\"\",M4274)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4273=1,0,IF(Daten!$B$549=2,1)+O4274))))","v":0},"69-312",{"$f":"IF(Daten!$B$549=2,N4279,0)","v":0},null,100]
["ICS Kupfer",5,100,"ICS Kupfer 1005",null,"ICK 900 Wandkonsolen (Paar) L900mm","102585","0",null,"STK",381,{"$f":"IF(M4277=0,\"\",M4277)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4273=1,\"\",IF(Daten!$B$549=5,1)+O4277))))","v":""},"412-712",{"$f":"IF(Daten!$B$549=5,N4279,0)","v":0},null,600]
["ICS Kupfer",6,100,"ICS Kupfer 1006",null,"ICK 100 Verankerungsplatte mit Ablauf senkr.","102588",95,null,"STK",212,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L4278=\"\",\"0\",L4278*H4278)","v":95},null,null,{"$f":"IF(L4278=\"\",\"0\",H4278*L4278)","v":95}]
["ICS Kupfer",10,100,"ICS Kupfer 10010",null,"ICK 100 Teleskopstütze verstellbar L300 - 500mm","102620",300,null,"STK",360,{"$f":"IF(Daten!$B$499=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Kupfer",12,100,"ICS Kupfer 10012",null,"ICK 100 T-Stück 45° L 355mm","102647",355,null,"STK",311,{"$f":"IF(Daten!$B$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS Kupfer",15,100,"ICS Kupfer 10015",null,"ICK 100 Anschluss von EW auf DW in Rauchgasr.","102671","0",null,"STK",127,1,{"$f":"IF(L4287=\"\",\"0\",L4287*H4287)","v":0},null,null,{"$f":"IF(L4287=\"\",\"0\",H4288*L4287)","v":0}]
["ICS Kupfer",17,100,"ICS Kupfer 10017",null,"ICK 100 Anschluss von DW auf EW in Rauchgasr.","102689","0",null,"STK",127,null,{"$f":"IF(H4289=\"\",\"\",L4289*H4289)","v":0}]
["ICS Kupfer",20,100,"ICS Kupfer 10020",null,"ICK 100 Längenelement L500mm","102713",455,null,"STK",114,{"$f":"IF(Daten!$DJ$259=0,\"\",Daten!$DJ$259)","v":""},{"$f":"IF(L4292=\"\",0,L4292*H4292)","v":0},{"$f":"O4292/H4292","v":0},{"$f":"Daten!$DF$260*1000","v":0},{"$f":"(IF(L4292=\"\",0,H4292*L4292))-O4292","v":0}]
["ICS Kupfer",23,100,"ICS Kupfer 10023",null,"PPL 100 Dichtung Viton","100990","0",null,"STK",13,{"$f":"IF(Daten!$B$490=1,\"\",SUM(L4278:L4281,L4283:L4287,L4290:L4293,L4317:L4323,L4315))","v":""},{"$f":"IF(L4295=\"\",\"\",L4295*H4295)","v":""},null,null,{"$f":"IF(L4295=\"\",\"0\",H4295*L4295)","v":"0"}]
["ICS Kupfer",25,100,"ICS Kupfer 10025",null,"ICK 100 Statisches Klemmband DN 150","102745","0",null,"STK",36,{"$f":"IF(N4297=0,\"\",N4297)","v":""},null,{"$f":"IF(Daten!$E$529=1,0,2)","v":0},null,{"$f":"IF(N4297=\"\",\"0\",H4297*N4297)","v":0}]
["ICS Kupfer",26,100,"ICS Kupfer 10026",null,"ICK 100 Wandhalter 50mm fix DN 150mm ","102753","0",null,"STK",51,null,null,null,null,{"$f":"IF(L4298=\"\",\"0\",H4298*L4298)","v":"0"}]
["ICS Kupfer",28,100,"ICS Kupfer 10028",null,"ICK 100 Wandhalter 50mm verlängerbar DN 150mm ","102769","0",null,"STK",51,{"$f":"ROUNDUP(M4300,0)","v":3},{"$f":"((M4272/1000)/4.3)","v":2.3255813953488373},null,null,0]
["ICS Kupfer",31,100,"ICS Kupfer 10031",null,"ICK L2 Verlängerung zu Wandhalter 50mm L450mm","102779","0",null,"STK",184,{"$f":"IF(Daten!$B$549=4,$L4300,\"\")","v":""},null,440,null,"0"]
["ICS Kupfer",34,100,"ICS Kupfer 10034",null,"ICK 80-100 Dachdurführung 0° DN165  L500mm","102782","0",null,"STK",184,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",36,100,"ICS Kupfer 10036",null,"ICK 80-100 Dachdurführung 26-35° DN165  ","102792","0",null,"STK",451,{"$f":"IF(Daten!$B$522=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",40,100,"ICS Kupfer 10040",null,"ICK 100 Blende 0-30° DN150","102819","0",null,"STK",82,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",41,100,"ICS Kupfer 10041",null,"ICK 100 Blende 32-45° DN150","102827","0",null,"STK",96,{"$f":"IF(Daten!$E$515=3,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",44,100,"ICS Kupfer 10044",null,"ICK 100 Basten Standart mit Stulpring Kupfer","102850","0",null,"STK",387,{"$f":"IF(Daten!$E$522=3,1,\"\")","v":""},{"$f":"IF(L4316=\"\",\"0\",L4316*H4316)","v":"0"},null,null,"0"]
["ICS Kupfer",45,100,"ICS Kupfer 10045",null,"ICK 100 Element mit Messöffnung L205mm","102858","0",null,"STK",212,null,{"$f":"IF(L4317=\"\",0,L4317*H4317)","v":0},null,null,"0"]
["ICS Kupfer",49,100,"ICS Kupfer 10049",null,"ICK 100 Winkel 45°","102890","0",null,"STK",184,null,0,null,null,"0"]
["ICS Kupfer",51,100,"ICS Kupfer 10051",null,"ICK 100 Inspektionswinkel 90°","102906","0",null,"STK",451,null,0,null,null,"0"]
[{"$f":"A4325","v":"ICS Kupfer"},{"$f":"B4325+1","v":2},{"$f":"C4325","v":130},{"$f":"A4326&\" \"&C4326&B4326","v":"ICS Kupfer 1302"},null,"ICK 700 Wandkonsolen (Paar) L500mm","102582","0",null,"STK",233,{"$f":"IF(M4326=0,\"\",M4326)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4325=1,0,IF(Daten!$B$549=2,1)+O4326))))","v":0},"69-312",{"$f":"IF(Daten!$B$549=2,N4331,0)","v":0},null,100]
["ICS Kupfer",5,130,"ICS Kupfer 1305",null,"ICK 900 Wandkonsolen (Paar) L900mm","102585","0",null,"STK",381,{"$f":"IF(M4329=0,\"\",M4329)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4325=1,\"\",IF(Daten!$B$549=5,1)+O4329))))","v":""},"412-712",{"$f":"IF(Daten!$B$549=5,N4331,0)","v":0},null,600]
["ICS Kupfer",7,130,"ICS Kupfer 1307",null,"ICK 130 Zwischenstütze","102597",95,null,"STK",254,{"$f":"IF(N4331=0,\"\",N4331)","v":""},{"$f":"IF(L4331=\"\",0,L4331*H4331)","v":0},{"$f":"IF(M4324>=15000,1,0)","v":0},null,{"$f":"IF(L4331=\"\",\"0\",H4331*L4331)","v":"0"}]
["ICS Kupfer",10,130,"ICS Kupfer 13010",null,"ICK 130 Teleskopstütze verstellbar L300 - 500mm","102621",300,null,"STK",381,{"$f":"IF(Daten!$B$499=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Kupfer",12,130,"ICS Kupfer 13012",null,"ICK 130 Putztüranschluss eckig Unterdruck L455mm","102632",411,null,"STK",451,{"$f":"IF(Daten!$B$490=2,\"\",Daten!$F$499)","v":1},{"$f":"IF(L4336=\"\",\"0\",L4336*H4336)","v":411},null,null,{"$f":"IF(L4336=\"\",\"0\",H4336*L4336)","v":411}]
["ICS Kupfer",13,130,"ICS Kupfer 13013",null,"ICK 130 Putztüranschluss rund Überdruck L455mm","102640",455,null,"STK",388,{"$f":"Daten!$F$499","v":1},455,null,null,455]
["ICS Kupfer",15,130,"ICS Kupfer 13015",null,"ICK 130 T-Stück 90° L455mm","102656",455,null,"STK",318,{"$f":"IF(Daten!$B$515=2,1,\"\")","v":1},455,null,null,455]
["ICS Kupfer",18,130,"ICS Kupfer 13018",null,"ICK 150 Anschluss DW/EW mit Klemmfutter DN130","102680","0",null,"STK",169,null,{"$f":"IF(H4342=\"\",\"\",L4342*H4342)","v":0}]
["ICS Kupfer",21,130,"ICS Kupfer 13021",null,"ICK 130 Längenelement L250mm","102706",205,null,"STK",114,{"$f":"IF(Daten!$DJ$251=0,\"\",Daten!$DJ$251)","v":""},{"$f":"IF(L4345=\"\",0,L4345*H4345)","v":0},{"$f":"O4345/H4345","v":0},{"$f":"Daten!$DF$252*1000","v":0},{"$f":"(IF(L4345=\"\",0,H4345*L4345))-O4345","v":0}]
["ICS Kupfer",23,130,"ICS Kupfer 13023",null,"ICK 130 Längenelement L1000mm","102722",955,null,"STK",212,{"$f":"ROUNDUP(M4347,0)+N4347","v":9},{"$f":"((M4324-SUM(M4330:M4346)-M4369)/H4347)","v":8.6795811518324602},{"$f":"O4347/H4347","v":0},{"$f":"Daten!$DF$268*1000","v":0},{"$f":"(IF(L4347=\"\",0,H4347*L4347))-O4347","v":8595}]
["ICS Kupfer",27,130,"ICS Kupfer 13027",null,"ICK 130 Statisches Klemmband DN 180","102746","0",null,"STK",38,{"$f":"IF(N4351=0,\"\",N4351)","v":""},null,{"$f":"IF(Daten!$E$529=1,0,2)","v":0},null,{"$f":"IF(N4351=\"\",\"0\",H4351*N4351)","v":0}]
["ICS Kupfer",28,130,"ICS Kupfer 13028",null,"ICK 130 Wandhalter 50mm fix DN 180mm ","102754","0",null,"STK",57,null,null,null,null,{"$f":"IF(L4352=\"\",\"0\",H4352*L4352)","v":"0"}]
["ICS Kupfer",30,130,"ICS Kupfer 13030",null,"ICK 130 Wandhalter 50mm verlängerbar DN 180mm ","102770","0",null,"STK",57,{"$f":"ROUNDUP(M4354,0)","v":3},{"$f":"((M4324/1000)/4.3)","v":2.3255813953488373},null,null,0]
["ICS Kupfer",33,130,"ICS Kupfer 13033",null,"ICK L2 Verlängerung zu Wandhalter 50mm L450mm","102779","0",null,"STK",184,{"$f":"IF(Daten!$B$549=4,$L4354,\"\")","v":""},null,440,null,"0"]
["ICS Kupfer",36,130,"ICS Kupfer 13036",null,"ICK 130 Dachdurführung 0° DN200 L500mm","102783","0",null,"STK",198,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",38,130,"ICS Kupfer 13038",null,"ICK 130 Dachdurführung 26-35° DN200 mit Bleilappen","102793","0",null,"STK",507,{"$f":"IF(Daten!$B$522=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",41,130,"ICS Kupfer 13041",null,"ICK 130 Seilabspannring DN180 ","102812","0",null,"STK",85,null,null,null,null,"0"]
["ICS Kupfer",44,130,"ICS Kupfer 13044",null,"ICK 130 Anschlussrosette Øi 180mm ØA 450mm","102836","0",null,"STK",78,{"$f":"IF(Daten!$E$515=4,1,\"\")","v":""},null,null,null,{"$f":"IF(L4368=\"\",\"0\",H4368*L4368)","v":"0"}]
["ICS Kupfer",46,130,"ICS Kupfer 13046",null,"ICK 130 Basten Standart mit Stulpring Kupfer","102851","0",null,"STK",406,{"$f":"IF(Daten!$E$522=3,1,\"\")","v":""},{"$f":"IF(L4370=\"\",\"0\",L4370*H4370)","v":"0"},null,null,"0"]
["ICS Kupfer",49,130,"ICS Kupfer 13049",null,"ICK 130 Winkel 15°","102875","0",null,"STK",191,null,0,null,null,"0"]
["ICS Kupfer",51,130,"ICS Kupfer 13051",null,"ICK 130 Winkel 45°","102891","0",null,"STK",198,null,0,null,null,"0"]
["ICS Kupfer",52,130,"ICS Kupfer 13052",null,"ICK 130 Winkel 90°","102899","0",null,"STK",226,null,0,null,null,"0"]
[{"$f":"A4379","v":"ICS Kupfer"},{"$f":"B4379+1","v":2},{"$f":"C4379","v":150},{"$f":"A4380&\" \"&C4380&B4380","v":"ICS Kupfer 1502"},null,"ICK 700 Wandkonsolen (Paar) L500mm","102582","0",null,"STK",233,{"$f":"IF(M4380=0,\"\",M4380)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4379=1,0,IF(Daten!$B$549=2,1)+O4380))))","v":0},"69-312",{"$f":"IF(Daten!$B$549=2,N4385,0)","v":0},null,100]
["ICS Kupfer",3,150,"ICS Kupfer 1503",null,"ICK 750 Wandkonsolen (Paar) L500mm verstärkt","102583","0",null,"STK",318,{"$f":"IF(M4381=0,\"\",M4381)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4379=1,\"\",IF(Daten!$B$549=3,1)+O4381))))","v":""},"69-312",{"$f":"IF(Daten!$B$549=3,N4385,0)","v":0},null,250]
["ICS Kupfer",6,150,"ICS Kupfer 1506",null,"ICK 150 Verankerungsplatte mit Ablauf senkr.","102590",95,null,"STK",248,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L4384=\"\",\"0\",L4384*H4384)","v":95},null,null,{"$f":"IF(L4384=\"\",\"0\",H4384*L4384)","v":95}]
["ICS Kupfer",8,150,"ICS Kupfer 1508",null,"ICK 150 Verankerungsplatte EW auf DW","102606",97,null,"STK",184,null,{"$f":"IF(L4386=\"\",\"0\",L4386*H4386)","v":"0"},null,null,"0"]
["ICS Kupfer",12,150,"ICS Kupfer 15012",null,"ICK 150 Putztüranschluss eckig Unterdruck L455mm","102633",411,null,"STK",465,{"$f":"IF(Daten!$B$490=2,\"\",Daten!$F$499)","v":1},411,null,null,411]
["ICS Kupfer",13,150,"ICS Kupfer 15013",null,"ICK 150 Putztüranschluss rund Überdruck L455mm","102641",455,null,"STK",430,{"$f":"Daten!$F$499","v":1},455,null,null,{"$f":"IF(L4391=\"\",\"0\",H4391*L4391)","v":455}]
["ICS Kupfer",15,150,"ICS Kupfer 15015",null,"ICK 150 T-Stück 90° L455mm","102657",455,null,"STK",353,{"$f":"IF(Daten!$B$515=2,1,\"\")","v":1},455,null,null,{"$f":"IF(L4393=\"\",\"0\",H4393*L4393)","v":455}]
["ICS Kupfer",18,150,"ICS Kupfer 15018",null,"ICK 150 Anschluss DW/EW mit Klemmfutter DN150","102681","0",null,"STK",184,null,{"$f":"IF(H4396=\"\",\"\",L4396*H4396)","v":0}]
["ICS Kupfer",21,150,"ICS Kupfer 15021",null,"ICK 150 Längenelement L250mm","102707",205,null,"STK",121,{"$f":"IF(Daten!$DJ$251=0,\"\",Daten!$DJ$251)","v":""},{"$f":"IF(L4399=\"\",0,L4399*H4399)","v":0},{"$f":"O4399/H4399","v":0},{"$f":"Daten!$DF$252*1000","v":0},{"$f":"(IF(L4399=\"\",0,H4399*L4399))-O4399","v":0}]
[{"$f":"A4400","v":"ICS Kupfer"},{"$f":"B4400+1","v":23},{"$f":"C4400","v":150},{"$f":"A4401&\" \"&C4401&B4401","v":"ICS Kupfer 15023"},null,"ICK 150 Längenelement L1000mm","102723",955,null,"STK",240,{"$f":"ROUNDUP(M4401,0)+N4401","v":9},{"$f":"((M4378-SUM(M4384:M4400)-M4423)/H4401)","v":8.6795811518324602},{"$f":"O4401/H4401","v":0},{"$f":"Daten!$DF$268*1000","v":0},{"$f":"(IF(L4401=\"\",0,H4401*L4401))-O4401","v":8595}]
["ICS Kupfer",26,150,"ICS Kupfer 15026",null,"ICK 150 Klemmband DN200","102739","0",null,"STK",24,null,null,null,null,{"$f":"IF(L4404=\"\",\"0\",H4404*L4404)","v":"0"}]
["ICS Kupfer",29,150,"ICS Kupfer 15029",null,"ICK 150 Wandhalter verstellbar 75 - 300mm DN 200mm","102763","0",null,"STK",93,null,null,"75-300",null,"0"]
["ICS Kupfer",31,150,"ICS Kupfer 15031",null,"ICK W1 Verlängerung zu Wandhalter 50mm L 130mm","102776","0",null,"STK",57,{"$f":"IF(Daten!$B$549=2,$L4408,\"\")","v":""},null,100,null,"0"]
["ICS Kupfer",32,150,"ICS Kupfer 15032",null,"ICK L1 Verlängerung zu Wandhalter 50mm L300mm","102778","0",null,"STK",142,{"$f":"IF(Daten!$B$549=3,$L4408,\"\")","v":""},null,250,null,"0"]
["ICS Kupfer",36,150,"ICS Kupfer 15036",null,"ICK 150-180 Dachdurführung 0° DN250 L500mm","102784","0",null,"STK",212,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",37,150,"ICS Kupfer 15037",null,"ICK 150-180 Dachdurführung 16-25° DN250 ","102789","0",null,"STK",451,{"$f":"IF(Daten!$B$522=3,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",41,150,"ICS Kupfer 15041",null,"ICK 150 Seilabspannring DN200","102813","0",null,"STK",93,null,null,null,null,"0"]
["ICS Kupfer",42,150,"ICS Kupfer 15042",null,"ICK 150 Blende 0-30° DN200","102821","0",null,"STK",90,{"$f":"IF(Daten!$E$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",45,150,"ICS Kupfer 15045",null,"ICK 150 Mündungsabschluss","102845",295,null,"STK",169,{"$f":"IF(Daten!$E$522=1,1,IF(Daten!$E$522=2,1,\"\"))","v":1},{"$f":"IF(L4423=\"\",\"0\",L4423*H4423)","v":295},null,null,{"$f":"IF(L4423=\"\",\"0\",H4423*L4423)","v":295}]
["ICS Kupfer",47,150,"ICS Kupfer 15047",null,"ICK 150 Element mit Messöffnung L205mm","102860","0",null,"STK",240,null,{"$f":"IF(L4425=\"\",0,L4425*H4425)","v":0},null,null,"0"]
["ICS Kupfer",51,150,"ICS Kupfer 15051",null,"ICK 150 Winkel 45°","102892","0",null,"STK",212,null,0,null,null,"0"]
["ICS Kupfer",52,150,"ICS Kupfer 15052",null,"ICK 150 Winkel 90°","102900","0",null,"STK",248,null,0,null,null,"0"]
["ICS Kupfer",0,180,"ICS Kupfer 1800"," ","Schiedel ICS Kupfer 180","ICS Kupfer 180","0",{"$f":"ICS!$J$10","v":10},"Anlage",0,1,{"$f":"I4432*1000","v":10000},null,{"$f":"ROUNDUP(P4432,2)","v":10.31},{"$f":"SUM(P4434:P4486)/1000","v":10.305999999999999}]
["ICS Kupfer",3,180,"ICS Kupfer 1803",null,"ICK 750 Wandkonsolen (Paar) L500mm verstärkt","102583","0",null,"STK",318,{"$f":"IF(M4435=0,\"\",M4435)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4433=1,\"\",IF(Daten!$B$549=3,1)+O4435))))","v":""},"69-312",{"$f":"IF(Daten!$B$549=3,N4439,0)","v":0},null,250]
["ICS Kupfer",6,180,"ICS Kupfer 1806",null,"ICK 180 Verankerungsplatte mit Ablauf senkr.","102591",95,null,"STK",254,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L4438=\"\",\"0\",L4438*H4438)","v":95},null,null,{"$f":"IF(L4438=\"\",\"0\",H4438*L4438)","v":95}]
["ICS Kupfer",8,180,"ICS Kupfer 1808",null,"ICK 180 Verankerungsplatte EW auf DW","102607",97,null,"STK",212,null,{"$f":"IF(L4440=\"\",\"0\",L4440*H4440)","v":"0"},null,null,"0"]
["ICS Kupfer",11,180,"ICS Kupfer 18011",null,"ICK 180 Fussteil mit Kondensatablauf L1000mm","102629",1000,null,"STK",472,{"$f":"IF(Daten!$B$499=4,1,\"\")","v":""},"0",null,null,"0"]
["ICS Kupfer",14,180,"ICS Kupfer 18014",null,"ICK 180 T-Stück 45° L455mm","102650",455,null,"STK",493,{"$f":"IF(Daten!$B$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS Kupfer",16,180,"ICS Kupfer 18016",null,"ICK 180 Verschlussdeckel","102666","0",null,"STK",178,null,"0",null,null,"0"]
["ICS Kupfer",17,180,"ICS Kupfer 18017",null,"ICK 180 Anschluss von EW auf DW in Rauchgasr.","102674","0",null,"STK",169,1,0,null,null,{"$f":"IF(L4449=\"\",\"0\",H4450*L4449)","v":0}]
["ICS Kupfer",21,180,"ICS Kupfer 18021",null,"ICK 180 Längenelement L195mm","102700",150,null,"STK",114,null,{"$f":"IF(H4453=\"\",\"\",L4453*H4453)","v":0},null,null,{"$f":"IF(L4453=\"\",\"0\",H4453*L4453)","v":"0"}]
["ICS Kupfer",22,180,"ICS Kupfer 18022",null,"ICK 180 Längenelement L250mm","102708",205,null,"STK",127,{"$f":"IF(Daten!$DJ$251=0,\"\",Daten!$DJ$251)","v":""},{"$f":"IF(L4454=\"\",0,L4454*H4454)","v":0},{"$f":"O4454/H4454","v":0},{"$f":"Daten!$DF$252*1000","v":0},{"$f":"(IF(L4454=\"\",0,H4454*L4454))-O4454","v":0}]
[{"$f":"A4457","v":"ICS Kupfer"},{"$f":"B4457+1","v":26},{"$f":"C4457","v":180},{"$f":"A4458&\" \"&C4458&B4458","v":"ICS Kupfer 18026"},null,"ICK 180 Klemmband DN230","102740","0",null,"STK",26,null,null,null,null,{"$f":"IF(L4458=\"\",\"0\",H4458*L4458)","v":"0"}]
["ICS Kupfer",28,180,"ICS Kupfer 18028",null,"ICK 180 Statisches Klemmband DN 230","102748","0",null,"STK",43,{"$f":"IF(N4460=0,\"\",N4460)","v":""},null,{"$f":"IF(Daten!$E$529=1,0,2)","v":0},null,{"$f":"IF(N4460=\"\",\"0\",H4460*N4460)","v":0}]
["ICS Kupfer",31,180,"ICS Kupfer 18031",null,"ICK 180 Wandhalter 50mm verlängerbar DN 230mm ","102772","0",null,"STK",72,{"$f":"ROUNDUP(M4463,0)","v":3},{"$f":"((M4432/1000)/4.3)","v":2.3255813953488373},null,null,0]
["ICS Kupfer",32,180,"ICS Kupfer 18032",null,"ICK W1 Verlängerung zu Wandhalter 50mm L 130mm","102776","0",null,"STK",57,{"$f":"IF(Daten!$B$549=2,$L4463,\"\")","v":""},null,100,null,"0"]
["ICS Kupfer",36,180,"ICS Kupfer 18036",null,"ICK L4 Verlängerung zu Wandhalter 50mm L 750mm","102781","0",null,"STK",254,{"$f":"IF(Daten!$B$549=5,$L4463,\"\")","v":""},null,700,null,"0"]
["ICS Kupfer",37,180,"ICS Kupfer 18037",null,"ICK 150-180 Dachdurführung 0° DN250 L500mm","102784","0",null,"STK",212,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",39,180,"ICS Kupfer 18039",null,"ICK 150-180 Dachdurführung 26-35° DN250 ","102794","0",null,"STK",563,{"$f":"IF(Daten!$B$522=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",42,180,"ICS Kupfer 18042",null,"ICK 180 Seilabspannring DN230","102814","0",null,"STK",99,null,null,null,null,"0"]
["ICS Kupfer",45,180,"ICS Kupfer 18045",null,"ICK 180 Anschlussrosette Øi 230mm ØA 500mm","102838","0",null,"STK",83,{"$f":"IF(Daten!$E$515=4,1,\"\")","v":""},null,null,null,{"$f":"IF(L4477=\"\",\"0\",H4477*L4477)","v":"0"}]
["ICS Kupfer",47,180,"ICS Kupfer 18047",null,"ICK 180 Basten Standart mit Stulpring Kupfer","102853","0",null,"STK",441,{"$f":"IF(Daten!$E$522=3,1,\"\")","v":""},{"$f":"IF(L4479=\"\",\"0\",L4479*H4479)","v":"0"},null,null,"0"]
["ICS Kupfer",51,180,"ICS Kupfer 18051",null,"ICK 180 Winkel 30°","102885","0",null,"STK",240,null,0,null,null,"0"]
["ICS Kupfer",52,180,"ICS Kupfer 18052",null,"ICK 180 Winkel 45°","102893","0",null,"STK",226,null,0,null,null,"0"]
["ICS Kupfer",0,200,"ICS Kupfer 2000"," ","Schiedel ICS Kupfer 200","ICS Kupfer 200","0",{"$f":"ICS!$J$10","v":10},"Anlage",0,1,{"$f":"I4487*1000","v":10000},null,{"$f":"ROUNDUP(P4487,2)","v":10.31},{"$f":"SUM(P4493:P4541)/1000","v":10.305999999999999}]
[{"$f":"A4487","v":"ICS Kupfer"},{"$f":"B4487+1","v":1},{"$f":"C4487","v":200},{"$f":"A4488&\" \"&C4488&B4488","v":"ICS Kupfer 2001"},null,"ICK 200 Konsolenbleche (Paar)","102579","0",null,"STK",220,{"$f":"N4488","v":1},{"$f":"IF(Daten!$B$549=1,1,\"\")","v":1},{"$f":"IF(Daten!$B$499=1,M4488,\"\")","v":1},null,{"$f":"IF(L4488=\"\",\"0\",H4488*L4488)","v":0}]
["ICS Kupfer",5,200,"ICS Kupfer 2005",null,"ICK 999 Wandkonsolen (Paar) L1304mm","102586","0",null,"STK",549,{"$f":"IF(M4492=0,\"\",M4492)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4488=1,\"\",IF(Daten!$B$549=5,1,IF(Daten!$B$549=4,1))+O4492))))","v":""},"315-615",{"$f":"IF(Daten!$B$549=4,#REF!,IF(Daten!$B$549=5,#REF!,0))","v":0},null,"400/600"]
["ICS Kupfer",6,200,"ICS Kupfer 2006",null,"ICK 200 Verankerungsplatte mit Ablauf senkr.","102592",95,null,"STK",262,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L4493=\"\",\"0\",L4493*H4493)","v":95},null,null,{"$f":"IF(L4493=\"\",\"0\",H4493*L4493)","v":95}]
["ICS Kupfer",10,200,"ICS Kupfer 20010",null,"ICK 200 Teleskopstütze verstellbar L300 - 500mm","102624",300,null,"STK",437,{"$f":"IF(Daten!$B$499=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Kupfer",12,200,"ICS Kupfer 20012",null,"ICK 200 Putztüranschluss eckig Unterdruck L455mm","102635",411,null,"STK",493,{"$f":"IF(Daten!$B$490=2,\"\",Daten!$F$499)","v":1},411,null,null,411]
["ICS Kupfer",15,200,"ICS Kupfer 20015",null,"ICK 200 T-Stück 90° L455mm","102659",455,null,"STK",423,{"$f":"IF(Daten!$B$515=2,1,\"\")","v":1},455,null,null,455]
["ICS Kupfer",16,200,"ICS Kupfer 20016",null,"ICK 200 Verschlussdeckel","102667","0",null,"STK",191,null,"0",null,null,"0"]
["ICS Kupfer",20,200,"ICS Kupfer 20020",null,"ICK 200 Anschluss von DW auf EW in Rauchgasr.","102693","0",null,"STK",184,null,{"$f":"IF(H4507=\"\",\"\",L4507*H4507)","v":0}]
["ICS Kupfer",21,200,"ICS Kupfer 20021",null,"ICK 200 Längenelement L195mm","102701",150,null,"STK",121,null,{"$f":"IF(H4508=\"\",\"\",L4508*H4508)","v":0},null,null,{"$f":"IF(L4508=\"\",\"0\",H4508*L4508)","v":"0"}]
["ICS Kupfer",23,200,"ICS Kupfer 20023",null,"ICK 200 Längenelement L500mm","102717",455,null,"STK",169,{"$f":"IF(Daten!$DJ$259=0,\"\",Daten!$DJ$259)","v":""},{"$f":"IF(L4510=\"\",0,L4510*H4510)","v":0},{"$f":"O4510/H4510","v":0},{"$f":"Daten!$DF$260*1000","v":0},{"$f":"(IF(L4510=\"\",0,H4510*L4510))-O4510","v":0}]
["ICS Kupfer",26,200,"ICS Kupfer 20026",null,"PPL 200 Dichtung Viton","100994","0",null,"STK",19,{"$f":"IF(Daten!$B$490=1,\"\",SUM(L4493:L4496,L4498:L4504,L4508:L4511,L4535:L4541,L4533))","v":""},{"$f":"IF(L4513=\"\",\"\",L4513*H4513)","v":""},null,null,{"$f":"IF(L4513=\"\",\"0\",H4513*L4513)","v":"0"}]
["ICS Kupfer",29,200,"ICS Kupfer 20029",null,"ICK 200 Wandhalter 50mm fix DN 250mm","102757","0",null,"STK",79,null,null,null,null,{"$f":"IF(L4516=\"\",\"0\",H4516*L4516)","v":"0"}]
["ICS Kupfer",31,200,"ICS Kupfer 20031",null,"ICK 200 Wandhalter 50mm verlängerbar DN 250mm","102773","0",null,"STK",79,{"$f":"ROUNDUP(M4518,0)","v":3},{"$f":"((M4487/1000)/4.3)","v":2.3255813953488373},null,null,0]
["ICS Kupfer",35,200,"ICS Kupfer 20035",null,"ICK L3 Verlängerung zu Wandhalter 50mm L 550mm","102780","0",null,"STK",212,null,null,500,null,"0"]
["ICS Kupfer",36,200,"ICS Kupfer 20036",null,"ICK L4 Verlängerung zu Wandhalter 50mm L 750mm","102781","0",null,"STK",254,{"$f":"IF(Daten!$B$549=5,$L4518,\"\")","v":""},null,700,null,"0"]
["ICS Kupfer",39,200,"ICS Kupfer 20039",null,"ICK 200 Dachdurführung 26-35° DN320 mit Bleilappen","102795","0",null,"STK",620,{"$f":"IF(Daten!$B$522=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",40,200,"ICS Kupfer 20040",null,"ICK 200 Dachdurführung 36-45° DN320 mit Bleilappen","102800","0",null,"STK",647,{"$f":"IF(Daten!$B$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",44,200,"ICS Kupfer 20044",null,"ICK 200 Blende 32-45° DN250","102831","0",null,"STK",114,{"$f":"IF(Daten!$E$515=3,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",46,200,"ICS Kupfer 20046",null,"ICK 200 Mündungsabschluss","102847",295,null,"STK",198,{"$f":"IF(Daten!$E$522=1,1,IF(Daten!$E$522=2,1,\"\"))","v":1},{"$f":"IF(L4533=\"\",\"0\",L4533*H4533)","v":295},null,null,{"$f":"IF(L4533=\"\",\"0\",H4533*L4533)","v":295}]
["ICS Kupfer",49,200,"ICS Kupfer 20049",null,"ICK 200 Element mit Kondensatablauf L205mm","102870","0",null,"STK",268,null,0,null,null,"0"]
["ICS Kupfer",51,200,"ICS Kupfer 20051",null,"ICK 200 Winkel 30°","102886","0",null,"STK",268,null,0,null,null,"0"]
["ICS Kupfer",54,200,"ICS Kupfer 20054",null,"ICK 200 Inspektionswinkel 90°","102910","0",null,"STK",620,null,0,null,null,"0"]
[{"$f":"A4543","v":"ICS Kupfer"},{"$f":"B4543+1","v":2},{"$f":"C4543","v":250},{"$f":"A4544&\" \"&C4544&B4544","v":"ICS Kupfer 2502"},null,"ICK 750 Wandkonsolen (Paar) L500mm verstärkt","102583","0",null,"STK",318,{"$f":"IF(M4544=0,\"\",M4544)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4543=1,0,IF(Daten!$B$549=2,1)+O4544))))","v":0},"69-165",{"$f":"IF(Daten!$B$549=2,N4549,0)","v":0},null,100]
["ICS Kupfer",4,250,"ICS Kupfer 2504",null,"ICK 900 Wandkonsolen (Paar) L900mm","102585","0",null,"STK",381,{"$f":"IF(M4546=0,\"\",M4546)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4543=1,\"\",IF(Daten!$B$549=3,1)+O4546))))","v":0},"165-265",{"$f":"IF(Daten!$B$549=3,N4549,0)","v":0},null,250]
["ICS Kupfer",5,250,"ICS Kupfer 2505",null,"ICK 999 Wandkonsolen (Paar) L1304mm","102586","0",null,"STK",549,{"$f":"IF(M4547=0,\"\",M4547)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4543=1,\"\",IF(Daten!$B$549=5,1,IF(Daten!$B$549=4,1))+O4547))))","v":0},"265-565",{"$f":"IF(Daten!$B$549=4,N4549,IF(Daten!$B$549=5,N4549,0))","v":0},null,"400/600"]
["ICS Kupfer",7,250,"ICS Kupfer 2507",null,"ICK 250 Zwischenstütze","102601",95,null,"STK",353,{"$f":"IF(N4549=0,\"\",N4549)","v":""},{"$f":"IF(L4549=\"\",0,L4549*H4549)","v":0},{"$f":"IF(M4542>=15000,1,0)","v":0},null,"0"]
["ICS Kupfer",10,250,"ICS Kupfer 25010",null,"ICK 250 Teleskopstütze verstellbar L300 - 500mm","102625",300,null,"STK",493,{"$f":"IF(Daten!$B$499=3,1,\"\")","v":""},"0",null,null,"0"]
["ICS Kupfer",13,250,"ICS Kupfer 25013",null,"ICK 250 Putztüranschluss rund Überdruck L455mm","102644",455,null,"STK",656,{"$f":"IF(Daten!$B$490=1,\"\",Daten!$F$499)","v":""},"0",null,null,"0"]
["ICS Kupfer",15,250,"ICS Kupfer 25015",null,"ICK 250 T-Stück 90° L455mm","102660",455,null,"STK",557,{"$f":"IF(Daten!$B$515=2,1,\"\")","v":1},455,null,null,455]
["ICS Kupfer",19,250,"ICS Kupfer 25019",null,"ICK 250 Anschluss von DW auf EW in Rauchgasr.","102694","0",null,"STK",198,null,{"$f":"IF(H4561=\"\",\"\",L4561*H4561)","v":0},null,null,"0"]
["ICS Kupfer",20,250,"ICS Kupfer 25020",null,"ICK 250 Längenelement L195mm","102702",150,null,"STK",142,null,{"$f":"IF(H4562=\"\",\"\",L4562*H4562)","v":0},null,null,"0"]
["ICS Kupfer",22,250,"ICS Kupfer 25022",null,"ICK 250 Längenelement L500mm","102718",455,null,"STK",198,{"$f":"IF(Daten!$DJ$259=0,\"\",Daten!$DJ$259)","v":""},{"$f":"IF(L4564=\"\",0,L4564*H4564)","v":0},{"$f":"O4564/H4564","v":0},{"$f":"Daten!$DF$260*1000","v":0},{"$f":"(IF(L4564=\"\",0,H4564*L4564))-O4564","v":0}]
["ICS Kupfer",25,250,"ICS Kupfer 25025",null,"PPL 250 Dichtung Viton","100995","0",null,"STK",22,{"$f":"IF(Daten!$B$490=1,\"\",SUM(L4548:L4551,L4553:L4559,L4562:L4565,L4589:L4595,L4587))","v":""},{"$f":"IF(L4567=\"\",\"\",L4567*H4567)","v":""},null,null,{"$f":"IF(L4567=\"\",\"0\",H4567*L4567)","v":"0"}]
["ICS Kupfer",28,250,"ICS Kupfer 25028",null,"ICK 250 Wandhalter 50mm fix DN 300mm ","102758","0",null,"STK",85,null,null,null,null,{"$f":"IF(L4570=\"\",\"0\",H4570*L4570)","v":"0"}]
["ICS Kupfer",30,250,"ICS Kupfer 25030",null,"ICK 250 Wandhalter 50mm verlängerbar DN 300mm ","102774","0",null,"STK",85,{"$f":"ROUNDUP(M4572,0)","v":3},{"$f":"((M4542/1000)/4.3)","v":2.3255813953488373},null,null,{"$f":"IF(L4572=\"\",\"0\",H4572*L4572)","v":0}]
["ICS Kupfer",33,250,"ICS Kupfer 25033",null,"ICK L2 Verlängerung zu Wandhalter 50mm L450mm","102779","0",null,"STK",184,{"$f":"IF(Daten!$B$549=4,#REF!,\"\")","v":""},null,370,null,"0"]
["ICS Kupfer",35,250,"ICS Kupfer 25035",null,"ICK L4 Verlängerung zu Wandhalter 50mm L 750mm","102781","0",null,"STK",254,{"$f":"IF(Daten!$B$549=5,$L4572,\"\")","v":""},null,670,null,"0"]
["ICS Kupfer",38,250,"ICS Kupfer 25038",null,"ICK 250-300 Dachdurführung 26-35° DN370 ","102796","0",null,"STK",676,{"$f":"IF(Daten!$B$522=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",41,250,"ICS Kupfer 25041",null,"ICK 250 Seilabspannring DN300","102816","0",null,"STK",114,null,null,null,null,"0"]
["ICS Kupfer",43,250,"ICS Kupfer 25043",null,"ICK 250 Blende 32-45° DN300","102832","0",null,"STK",127,{"$f":"IF(Daten!$E$515=3,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",44,250,"ICS Kupfer 25044",null,"ICK 250 Anschlussrosette Øi 300mm ØA 570mm","102840","0",null,"STK",89,{"$f":"IF(Daten!$E$515=4,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",46,250,"ICS Kupfer 25046",null,"ICK 250 Basten Standart mit Stulpring Kupfer","102855","0",null,"STK",463,{"$f":"IF(Daten!$E$522=3,1,\"\")","v":""},{"$f":"IF(L4588=\"\",\"0\",L4588*H4588)","v":"0"},null,null,"0"]
["ICS Kupfer",49,250,"ICS Kupfer 25049",null,"ICK 250 Winkel 15°","102879","0",null,"STK",248,null,0,null,null,"0"]
["ICS Kupfer",52,250,"ICS Kupfer 25052",null,"ICK 250 Winkel 90°","102903","0",null,"STK",338,null,0,null,null,"0"]
["ICS Kupfer",0,300,"ICS Kupfer 3000"," ","Schiedel ICS Kupfer 300","ICS Kupfer 300","0",{"$f":"ICS!$J$10","v":10},"Anlage",0,1,{"$f":"I4596*1000","v":10000},null,{"$f":"ROUNDUP(P4596,2)","v":10.84},{"$f":"SUM(P4601:P4647)/1000","v":10.831}]
["ICS Kupfer",4,300,"ICS Kupfer 3004",null,"ICK 999 Wandkonsolen (Paar) L1304mm","102586","0",null,"STK",549,{"$f":"IF(M4600=0,\"\",M4600)","v":""},{"$f":"IF(Daten!$B$499=2,\"\",IF(Daten!$B$499=3,\"\",IF(Daten!$B$499=4,\"\",IF(M4599=1,0,IF(Daten!$B$549=5,1)+O4600))))","v":0},"515-919",{"$f":"IF(Daten!$B$549=5,#REF!,0)","v":0},null,600]
["ICS Kupfer",5,300,"ICS Kupfer 3005",null,"ICK 300 Verankerungsplatte mit Ablauf senkr.","102594",95,null,"STK",381,{"$f":"IF(Daten!$B$499=4,\"\",1)","v":1},{"$f":"IF(L4601=\"\",\"0\",L4601*H4601)","v":95},null,null,{"$f":"IF(L4601=\"\",\"0\",H4601*L4601)","v":95}]
["ICS Kupfer",7,300,"ICS Kupfer 3007",null,"ICK 300 Verankerungsplatte EW auf DW","102610",97,null,"STK",311,null,{"$f":"IF(L4603=\"\",\"0\",L4603*H4603)","v":"0"},null,null,"0"]
["ICS Kupfer",10,300,"ICS Kupfer 30010",null,"ICK 300 Putztüranschluss eckig Unterdruck L455mm","102637",411,null,"STK",535,{"$f":"IF(Daten!$B$490=2,\"\",Daten!$F$499)","v":1},411,null,null,411]
["ICS Kupfer",13,300,"ICS Kupfer 30013",null,"ICK 300 T-Stück 90° L485mm","102661",480,null,"STK",698,{"$f":"IF(Daten!$B$515=2,1,\"\")","v":1},480,null,null,480]
["ICS Kupfer",15,300,"ICS Kupfer 30015",null,"ICK 300 Anschluss von EW auf DW in Rauchgasr.","102677","0",null,"STK",226,1,0,null,null,0]
["ICS Kupfer",18,300,"ICS Kupfer 30018",null,"ICK 300 Längenelement L195mm","102703",150,null,"STK",178,null,{"$f":"IF(H4614=\"\",\"\",L4614*H4614)","v":0},null,null,"0"]
[{"$f":"A4616","v":"ICS Kupfer"},{"$f":"B4616+1","v":21},{"$f":"C4616","v":300},{"$f":"A4617&\" \"&C4617&B4617","v":"ICS Kupfer 30021"},null,"ICK 300 Längenelement L1000mm","102727",955,null,"STK",408,{"$f":"ROUNDUP(M4617,0)+N4617","v":10},{"$f":"((M4596-SUM(M4601:M4616)-M4639)/H4617)","v":9.1298429319371728},{"$f":"O4617/H4617","v":0},{"$f":"Daten!$DF$268*1000","v":0},{"$f":"(IF(L4617=\"\",0,H4617*L4617))-O4617","v":9550}]
["ICS Kupfer",23,300,"ICS Kupfer 30023",null,"PPL 300 Dichtung Viton","100996","0",null,"STK",25,{"$f":"IF(Daten!$B$490=1,\"\",SUM(L4601:L4604,L4606:L4611,L4614:L4617,L4641:L4647,L4639))","v":""},{"$f":"IF(L4619=\"\",\"\",L4619*H4619)","v":""},null,null,{"$f":"IF(L4619=\"\",\"0\",H4619*L4619)","v":"0"}]
["ICS Kupfer",26,300,"ICS Kupfer 30026",null,"ICK 300 Wandhalter 50mm fix DN 350mm ","102759","0",null,"STK",114,null,null,null,null,{"$f":"IF(L4622=\"\",\"0\",H4622*L4622)","v":"0"}]
["ICS Kupfer",28,300,"ICS Kupfer 30028",null,"ICK 300 Wandhalter 50mm verlängerbar DN 350mm ","102775","0",null,"STK",114,{"$f":"ROUNDUP(M4624,0)","v":3},{"$f":"((M4596/1000)/4.3)","v":2.3255813953488373},null,null,{"$f":"IF(L4624=\"\",\"0\",H4624*L4624)","v":0}]
["ICS Kupfer",29,300,"ICS Kupfer 30029",null,"ICK W2 Verlängerung zu Wandhalter 50mm L 176mm","102777","0",null,"STK",85,{"$f":"IF(Daten!$B$549=2,#REF!,\"\")","v":""},null,114,null,"0"]
["ICS Kupfer",33,300,"ICS Kupfer 30033",null,"ICK L4 Verlängerung zu Wandhalter 50mm L 750mm","102781","0",null,"STK",254,{"$f":"IF(Daten!$B$549=5,$L4624,\"\")","v":""},null,670,null,"0"]
["ICS Kupfer",34,300,"ICS Kupfer 30034",null,"ICK 250-300 Dachdurführung 0° DN370 L500mm","102786","0",null,"STK",296,{"$f":"IF(Daten!$B$522=2,1,\"\")","v":""},null,null,null,{"$f":"IF(L4630=\"\",\"0\",H4630*L4630)","v":"0"}]
["ICS Kupfer",37,300,"ICS Kupfer 30037",null,"ICK 250-300 Dachdurführung 36-45° DN370 ","102801","0",null,"STK",704,{"$f":"IF(Daten!$B$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS Kupfer",39,300,"ICS Kupfer 30039",null,"ICK 300 Seilabspannring DN350","102817","0",null,"STK",121,null,null,null,null,"0"]
["ICS Kupfer",43,300,"ICS Kupfer 30043",null,"ICK 300 Mündungsabschluss","102849",295,null,"STK",282,{"$f":"IF(Daten!$E$522=1,1,IF(Daten!$E$522=2,1,\"\"))","v":1},{"$f":"IF(L4639=\"\",\"0\",L4639*H4639)","v":295},null,null,295]
["ICS Kupfer",44,300,"ICS Kupfer 30044",null,"ICK 300 Basten Standart mit Stulpring Kupfer","102856","0",null,"STK",503,{"$f":"IF(Daten!$E$522=3,1,\"\")","v":""},{"$f":"IF(L4640=\"\",\"0\",L4640*H4640)","v":"0"},null,null,"0"]
["ICS Kupfer",46,300,"ICS Kupfer 30046",null,"ICK 300 Element mit Kondensatablauf L205mm","102872","0",null,"STK",311,null,0,null,null,"0"]
["ICS Kupfer",49,300,"ICS Kupfer 30049",null,"ICK 300 Winkel 45°","102896","0",null,"STK",311,null,0,null,null,"0"]
["ICS5000",0,80,{"$f":"A4648&\" \"&C4648&B4648","v":"ICS5000 800"}," ","Schiedel ICS5000 25mm 80","ICS5000 80","0",{"$f":"'ICS5000'!$J$10","v":10},"Anlage",0,1,{"$f":"I4648*1000","v":10000},null,{"$f":"ROUNDUP(P4648,2)","v":10.52},{"$f":"SUM(P4650:P4703)/1000","v":10.516}]
[{"$f":"A4649","v":"ICS5000"},{"$f":"B4649+1","v":2},{"$f":"C4649","v":80},{"$f":"A4650&\" \"&C4650&B4650","v":"ICS5000 802"},null,"ICM 325 Wandkonsolen  (Paar) L325mm","101973","0",null,"STK",142,{"$f":"IF(M4650=0,\"\",M4650)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M4649=1,0,IF(Daten!$L$549=2,1)+O4650))))","v":0},157,{"$f":"IF(Daten!$L$549=2,N4662,0)","v":0},null,100]
["ICS5000",5,80,"ICS5000 805",null,"ICM 620 Wandkonsolen  (Paar) L620mm","101976","0",null,"STK",223,null,null,452]
["ICS5000",8,80,"ICS5000 808",null,"ICM 1004 Wandkonsolen  (Paar) L1004mm","101979","0",null,"STK",260,null,null,836]
["ICS5000",10,80,"ICS5000 8010",null,"ICM 1304 Wandkonsolen  (Paar) L1304mm","101981","0",null,"STK",315,null,null,1136]
["ICS5000",13,80,{"$f":"A4661&\" \"&C4661&B4661","v":"ICS5000 8013"},null,"ICM5000 80  Verankerungsplatte mit Ablauf waagr.","102926",97,null,"STK",103,{"$f":"IF(Daten!$L$499=2,1,\"\")","v":""},{"$f":"IF(L4661=\"\",\"0\",L4661*H4661)","v":"0"},null,null,{"$f":"IF(L4661=\"\",\"0\",H4661*L4661)","v":"0"}]
["ICS5000",15,80,"ICS5000 8015",null,"ICM5000 80 Kondensattopf","102952","0",null,"STK",67,null,{"$f":"IF(L4663=\"\",\"0\",L4663*H4663)","v":"0"},null,null,"0"]
["ICS5000",16,80,"ICS5000 8016",null,"ICM5000 80 Putztüranschluss rund Überdruck","102965",288,null,"STK",234,{"$f":"Daten!$P$499","v":1},288,null,null,288]
["ICS5000",20,80,"ICS5000 8020",null,"ICM5000 80 Anschluss von EW auf DW in Rauchgasr.","103017","0",null,"STK",163,1,0,null,null,{"$f":"IF(L4668=\"\",\"0\",H4669*L4668)","v":0}]
["ICS5000",22,80,"ICS5000 8022",null,"ICM5000 80 Flansch zum Anschweissen im Auftrag","103041","0",null,"STK",77,null,{"$f":"IF(H4670=\"\",\"\",L4670*H4670)","v":0}]
["ICS5000",25,80,"ICS5000 8025",null,"ICM5000 80 Längenelement L250mm","103067",205,null,"STK",70,{"$f":"IF(N4673+O4673=0,\"\",N4673+O4673)","v":""},{"$f":"IF(L4673=\"\",0,L4673*H4673)","v":0},{"$f":"'ICS5000'!$P$20","v":0},{"$f":"IF(Daten!$L$507=2,1,0)","v":0},{"$f":"(IF(L4673=\"\",0,H4673*L4673))-O4673","v":0}]
["ICS5000",26,80,"ICS5000 8026",null,"ICM5000 80 Längenelement L500mm","103080",455,null,"STK",84,{"$f":"IF(N4674+O4674=0,\"\",N4674+O4674)","v":""},{"$f":"IF(L4674=\"\",0,L4674*H4674)","v":0},{"$f":"'ICS5000'!$P$18","v":0},{"$f":"IF(Daten!$L$507=3,1,0)","v":0},{"$f":"(IF(L4674=\"\",0,H4674*L4674))-O4674","v":0}]
["ICS5000",30,80,"ICS5000 8030",null,"ICM5000 80 Dichtmanchette für Aussenmantel","103132","0",null,"STK",30,null,"im Bauteil enthalten",null,null,{"$f":"IF(L4678=\"\",\"0\",H4678*L4678)","v":"0"}]
["ICS5000",31,80,"ICS5000 8031",null,"ICM5000 80 Klemmband bei jedem Bauteil inkl. ","103145","0",null,"STK",11,null,"im Bauteil enthalten",null,null,{"$f":"IF(L4679=\"\",\"0\",H4679*L4679)","v":"0"}]
["ICS5000",33,80,"ICS5000 8033",null,"ICM 80 Wandhalter 50mm verlängerbar DN 130mm ","102303","0",null,"STK",33,{"$f":"ROUNDUP(M4681,0)","v":3},{"$f":"((M4648/1000)/4.3)","v":2.3255813953488373},null,null,0]
["ICS5000",36,80,"ICS5000 8036",null,"ICM L2 Verlängerung zu Wandhalter 50mm L450mm","102320","0",null,"STK",142,{"$f":"IF(Daten!$L$549=4,$L4681,\"\")","v":""},null,440,null,"0"]
["ICS5000",39,80,"ICS5000 8039",null,"ICM 80-100 Dachdurführung 0° DN165  L500mm","102323","0",null,"STK",142,{"$f":"IF(Daten!$L$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",41,80,"ICS5000 8041",null,"ICM 80-100 Dachdurführung 26-35° DN165  ","102347","0",null,"STK",347,{"$f":"IF(Daten!$L$522=4,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",44,80,"ICS5000 8044",null,"ICM 80 Seilabspannring DN130 ","102385","0",null,"STK",55,null,null,null,null,"0"]
["ICS5000",47,80,"ICS5000 8047",null,"ICM 80 Anschlussrosette Øi 130mm ØA 400mm","102415","0",null,"STK",55,{"$f":"IF(Daten!$O$515=4,1,\"\")","v":""},null,null,null,{"$f":"IF(L4695=\"\",\"0\",H4695*L4695)","v":"0"}]
["ICS5000",49,80,"ICS5000 8049",null,"ICM5000 80 Abluftregenhut Typ AT Inox ","140755","0",null,"STK",361,{"$f":"IF(Daten!$O$522=2,1,\"\")","v":""},{"$f":"IF(L4697=\"\",\"0\",L4697*H4697)","v":"0"},null,null,{"$f":"IF(L4697=\"\",\"0\",H4697*L4697)","v":"0"}]
["ICS5000",50,80,"ICS5000 8050",null,"ICM5000 80 Mündungsabschluss horizontal","103171","0",null,"STK",156,{"$f":"IF(Daten!$O$522=3,1,\"\")","v":""},{"$f":"IF(L4698=\"\",\"0\",L4698*H4698)","v":"0"},null,null,{"$f":"IF(L4698=\"\",\"0\",H4698*L4698)","v":"0"}]
["ICS5000",54,80,"ICS5000 8054",null,"ICM5000 80 Winkel 45°","103218","0",null,"STK",93,{"$f":"IF(N4702=1,\"\",O4702)","v":""},{"$f":"IF(L4702=\"\",0,L4702*H4702)","v":0},{"$f":"Daten!$O$548","v":1},{"$f":"Daten!$P$548","v":"Nein"},"0"]
["ICS5000",55,80,"ICS5000 8055",null,"ICM5000 80 Winkel 90°","103231","0",null,"STK",103,{"$f":"IF(N4703=1,\"\",O4703)","v":""},{"$f":"IF(L4703=\"\",0,L4703*H4703)","v":0},{"$f":"Daten!$O$556","v":1},{"$f":"Daten!$P$556","v":"Nein"},"0"]
[{"$f":"A4706","v":"ICS5000"},{"$f":"B4706+1","v":3},{"$f":"C4706","v":100},{"$f":"A4707&\" \"&C4707&B4707","v":"ICS5000 1003"},null,"ICM 475 Wandkonsolen  (Paar) L475mm","101974","0",null,"STK",158,{"$f":"IF(M4707=0,\"\",M4707)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M4705=1,0,IF(Daten!$L$549=3,1)+O4707))))","v":0},287,{"$f":"IF(Daten!$L$549=3,N4718,0)","v":0},null,250]
["ICS5000",5,100,"ICS5000 1005",null,"ICM 620 Wandkonsolen  (Paar) L620mm","101976","0",null,"STK",223,{"$f":"IF(M4709=0,\"\",M4709)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M4705=1,0,IF(Daten!$L$549=4,1)+O4709))))","v":0},432,{"$f":"IF(Daten!$L$549=4,N4719,0)","v":0},null,400]
["ICS5000",8,100,"ICS5000 1008",null,"ICM 1004 Wandkonsolen  (Paar) L1004mm","101979","0",null,"STK",260,null,null,816]
["ICS5000",9,100,"ICS5000 1009",null,"ICM 1120 Wandkonsolen  (Paar) L1120mm","101980","0",null,"STK",288,null,null,932]
["ICS5000",13,100,{"$f":"A4717&\" \"&C4717&B4717","v":"ICS5000 10013"},null,"ICM5000 100  Verankerungsplatte mit Ablauf waagr.","102927",97,null,"STK",117,{"$f":"IF(Daten!$L$499=2,1,\"\")","v":""},{"$f":"IF(L4717=\"\",\"0\",L4717*H4717)","v":"0"},null,null,{"$f":"IF(L4717=\"\",\"0\",H4717*L4717)","v":"0"}]
["ICS5000",14,100,"ICS5000 10014",null,"ICM5000 100 Zwischenstütze","102940",208,null,"STK",127,{"$f":"IF(N4718=0,\"\",N4718)","v":""},{"$f":"IF(L4718=\"\",0,L4718*H4718)","v":0},{"$f":"IF(M4704>=15000,1,0)","v":0},null,"0"]
["ICS5000",16,100,"ICS5000 10016",null,"ICM5000 100 Putztüranschluss rund Überdruck","102966",288,null,"STK",217,{"$f":"Daten!$P$499","v":1},288,null,null,288]
["ICS5000",19,100,"ICS5000 10019",null,"ICM5000 100 Verschlussdeckel","103005","0",null,"STK",78,null,"0",null,null,"0"]
["ICS5000",22,100,"ICS5000 10022",null,"ICM5000 100 Flansch zum Anschweissen im Auftrag","103042","0",null,"STK",79,null,{"$f":"IF(H4726=\"\",\"\",L4726*H4726)","v":0}]
["ICS5000",24,100,"ICS5000 10024",null,"ICM5000 100 Längenelement L195mm","103055",155,null,"STK",58,null,{"$f":"IF(H4728=\"\",\"\",L4728*H4728)","v":0},null,null,{"$f":"IF(L4728=\"\",\"0\",H4728*L4728)","v":"0"}]
["ICS5000",28,100,"ICS5000 10028",null,"ICM5000 100 Schiebeelement L375 - 585mm","103107","0",null,"STK",158,null,null,null,null,{"$f":"IF(L4732=\"\",\"0\",H4732*L4732)","v":"0"}]
["ICS5000",29,100,"ICS5000 10029",null,"ICM5000 100 Dichtring Silikon inkl. Gleitmittel","103120","0",null,"STK",12,null,"im Bauteil enthalten",null,null,{"$f":"IF(L4733=\"\",\"0\",H4733*L4733)","v":"0"}]
["ICS5000",32,100,"ICS5000 10032",null,"ICM 100 Wandhalter verstellbar 75 - 300mm DN 150mm","102290","0",null,"STK",60,null,null,"75-300",null,{"$f":"IF(L4736=\"\",\"0\",H4736*L4736)","v":"0"}]
["ICS5000",33,100,"ICS5000 10033",null,"ICM 100 Wandhalter 50mm verlängerbar DN 150mm ","102304","0",null,"STK",39,{"$f":"ROUNDUP(M4737,0)","v":3},{"$f":"((M4704/1000)/4.3)","v":2.3255813953488373},null,null,0]
["ICS5000",37,100,"ICS5000 10037",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,500,null,"0"]
["ICS5000",38,100,"ICS5000 10038",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,{"$f":"IF(Daten!$L$549=5,$L4737,\"\")","v":""},null,700,null,"0"]
["ICS5000",42,100,"ICS5000 10042",null,"ICM 80-100 Dachdurführung 36-45° DN165  ","102359","0",null,"STK",401,{"$f":"IF(Daten!$L$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",44,100,"ICS5000 10044",null,"ICM 100 Seilabspannring DN150","102386","0",null,"STK",60,null,null,null,null,"0"]
["ICS5000",47,100,"ICS5000 10047",null,"ICM 100 Anschlussrosette Øi 150mm ØA 420mm","102416","0",null,"STK",57,{"$f":"IF(Daten!$O$515=4,1,\"\")","v":""},null,null,null,{"$f":"IF(L4751=\"\",\"0\",H4751*L4751)","v":"0"}]
["ICS5000",50,100,"ICS5000 10050",null,"ICM5000 100 Mündungsabschluss horizontal","103172","0",null,"STK",146,{"$f":"IF(Daten!$O$522=3,1,\"\")","v":""},{"$f":"IF(L4754=\"\",\"0\",L4754*H4754)","v":"0"},null,null,"0"]
["ICS5000",52,100,"ICS5000 10052",null,"ICM5000 100 Winkel 15°","103198","0",null,"STK",97,{"$f":"IF(N4756=1,\"\",O4756)","v":""},{"$f":"IF(L4756=\"\",0,L4756*H4756)","v":0},{"$f":"Daten!$O$532","v":1},{"$f":"Daten!$P$532","v":"Nein"},"0"]
["ICS5000",53,100,"ICS5000 10053",null,"ICM5000 100 Winkel 30°","103206","0",null,"STK",95,{"$f":"IF(N4757=1,\"\",O4757)","v":""},{"$f":"IF(L4757=\"\",0,L4757*H4757)","v":0},{"$f":"Daten!$O$540","v":1},{"$f":"Daten!$P$540","v":"Nein"},"0"]
["ICS5000",55,100,"ICS5000 10055",null,"ICM5000 100 Winkel 90°","103232","0",null,"STK",107,{"$f":"IF(N4759=1,\"\",O4759)","v":""},{"$f":"IF(L4759=\"\",0,L4759*H4759)","v":0},{"$f":"Daten!$O$556","v":1},{"$f":"Daten!$P$556","v":"Nein"},"0"]
[{"$f":"A4761","v":"ICS5000"},{"$f":"B4761+1","v":2},{"$f":"C4761","v":130},{"$f":"A4762&\" \"&C4762&B4762","v":"ICS5000 1302"},null,"ICM 325 Wandkonsolen  (Paar) L325mm","101973","0",null,"STK",142,{"$f":"IF(M4762=0,\"\",M4762)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M4761=1,0,IF(Daten!$L$549=2,1)+O4762))))","v":0},107,{"$f":"IF(Daten!$L$549=2,N4774,0)","v":0},null,100]
["ICS5000",5,130,"ICS5000 1305",null,"ICM 620 Wandkonsolen  (Paar) L620mm","101976","0",null,"STK",223,{"$f":"IF(M4765=0,\"\",M4765)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M4761=1,0,IF(Daten!$L$549=4,1)+O4765))))","v":0},402,{"$f":"IF(Daten!$L$549=4,N4775,0)","v":0},null,400]
["ICS5000",7,130,"ICS5000 1307",null,"ICM 820 Wandkonsolen  (Paar) L820mm","101978","0",null,"STK",238,{"$f":"IF(M4767=0,\"\",M4767)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M4761=1,0,IF(Daten!$L$549=5,1)+O4767))))","v":0},602,{"$f":"IF(Daten!$L$549=5,N4776,0)","v":0},null,600]
[{"$f":"A4770","v":"ICS5000"},{"$f":"B4770+1","v":11},{"$f":"C4770","v":130},"ICS5000 13011",null,"ICM 1504 Wandkonsolen  (Paar) L1504mm","101982","0",null,"STK",358,null,null,1100]
["ICS5000",12,130,"ICS5000 13012",null,"ICM5000 130  Verankerungsplatte mit Ablauf senkr.","102915",95,null,"STK",102,{"$f":"IF(Daten!$L$499=1,1,\"\")","v":1},{"$f":"IF(L4772=\"\",\"0\",L4772*H4772)","v":95},null,null,{"$f":"IF(L4772=\"\",\"0\",H4772*L4772)","v":95}]
["ICS5000",15,130,{"$f":"A4775&\" \"&C4775&B4775","v":"ICS5000 13015"},null,"ICM5000 130 Kondensattopf","102954","0",null,"STK",73,null,{"$f":"IF(L4775=\"\",\"0\",L4775*H4775)","v":"0"},null,null,"0"]
["ICS5000",16,130,"ICS5000 13016",null,"ICM5000 130 Element mit Empa Messstutzen","140742","0",null,"STK",423,null,{"$f":"IF(L4776=\"\",\"0\",L4776*H4776)","v":"0"},null,null,{"$f":"IF(L4776=\"\",\"0\",H4776*L4776)","v":"0"}]
["ICS5000",20,130,"ICS5000 13020",null,"ICM5000 130 Verschlussdeckel","103006","0",null,"STK",83,null,"0",null,null,"0"]
["ICS5000",22,130,"ICS5000 13022",null,"ICM5000 130 Anschluss von DW auf EW in Rauchgasr.","140758","0",null,"STK",133,null,{"$f":"IF(H4782=\"\",\"\",L4782*H4782)","v":0}]
["ICS5000",25,130,"ICS5000 13025",null,"ICM5000 130 Längenelement L195mm","103056",155,null,"STK",64,null,{"$f":"IF(H4785=\"\",\"\",L4785*H4785)","v":0},null,null,{"$f":"IF(L4785=\"\",\"0\",H4785*L4785)","v":"0"}]
["ICS5000",27,130,"ICS5000 13027",null,"ICM5000 130 Längenelement L500mm","103082",455,null,"STK",92,{"$f":"IF(N4787+O4787=0,\"\",N4787+O4787)","v":""},{"$f":"IF(L4787=\"\",0,L4787*H4787)","v":0},{"$f":"'ICS5000'!$P$18","v":0},{"$f":"IF(Daten!$L$507=3,1,0)","v":0},{"$f":"(IF(L4787=\"\",0,H4787*L4787))-O4787","v":0}]
["ICS5000",30,130,"ICS5000 13030",null,"ICM5000 130 Dichtring Silikon inkl. Gleitmittel","103121","0",null,"STK",13,null,"im Bauteil enthalten",null,null,{"$f":"IF(L4790=\"\",\"0\",H4790*L4790)","v":"0"}]
["ICS5000",33,130,"ICS5000 13033",null,"ICM 130 Wandhalter verstellbar 75 - 300mm DN 180mm","102291","0",null,"STK",65,null,null,"75-300",null,{"$f":"IF(L4793=\"\",\"0\",H4793*L4793)","v":"0"}]
["ICS5000",35,130,"ICS5000 13035",null,"ICM W1 Verlängerung zu Wandhalter 50mm L 130mm","102317","0",null,"STK",44,{"$f":"IF(Daten!$L$549=2,$L4794,\"\")","v":""},null,100,null,"0"]
["ICS5000",36,130,"ICS5000 13036",null,"ICM L1 Verlängerung zu Wandhalter 50mm L300mm","102319","0",null,"STK",109,{"$f":"IF(Daten!$L$549=3,$L4794,\"\")","v":""},null,250,null,"0"]
["ICS5000",38,130,"ICS5000 13038",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,500,null,"0"]
["ICS5000",41,130,"ICS5000 13041",null,"ICM 130 Dachdurführung 16-25° DN200 mit Bleilappen","102336","0",null,"STK",303,{"$f":"IF(Daten!$L$522=3,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",44,130,"ICS5000 13044",null,"ICM 130 Regenkragen DN180 ","102373","0",null,"STK",44,{"$f":"IF(SUM(L4800:L4803)=0,\"\",SUM(L4800:L4803))","v":""},null,null,null,"0"]
["ICS5000",46,130,"ICS5000 13046",null,"ICM 130 Blende 0-30° DN180 ","102401","0",null,"STK",65,{"$f":"IF(Daten!$O$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",50,130,"ICS5000 13050",null,"ICM5000 130 Abluftregenhut Typ AT Inox ","140719","0",null,"STK",382,{"$f":"IF(Daten!$O$522=2,1,\"\")","v":""},{"$f":"IF(L4810=\"\",\"0\",L4810*H4810)","v":"0"},null,null,"0"]
["ICS5000",51,130,"ICS5000 13051",null,"ICM5000 130 Mündungsabschluss horizontal","103173","0",null,"STK",159,{"$f":"IF(Daten!$O$522=3,1,\"\")","v":""},{"$f":"IF(L4811=\"\",\"0\",L4811*H4811)","v":"0"},null,null,"0"]
["ICS5000",53,130,"ICS5000 13053",null,"ICM5000 130 Winkel 15°","103199","0",null,"STK",107,{"$f":"IF(N4813=1,\"\",O4813)","v":""},{"$f":"IF(L4813=\"\",0,L4813*H4813)","v":0},{"$f":"Daten!$O$532","v":1},{"$f":"Daten!$P$532","v":"Nein"},"0"]
["ICS5000",56,130,"ICS5000 13056",null,"ICM5000 130 Winkel 90°","103233","0",null,"STK",122,{"$f":"IF(N4816=1,\"\",O4816)","v":""},{"$f":"IF(L4816=\"\",0,L4816*H4816)","v":0},{"$f":"Daten!$O$556","v":1},{"$f":"Daten!$P$556","v":"Nein"},"0"]
[{"$f":"A4818","v":"ICS5000"},{"$f":"B4818+1","v":2},{"$f":"C4818","v":150},{"$f":"A4819&\" \"&C4819&B4819","v":"ICS5000 1502"},null,"ICM 325 Wandkonsolen  (Paar) L325mm","101973","0",null,"STK",142,null,null,87]
["ICS5000",4,150,"ICS5000 1504",null,"ICM 570 Wandkonsolen  (Paar) L570mm","101975","0",null,"STK",217,{"$f":"IF(M4821=0,\"\",M4821)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M4818=1,0,IF(Daten!$L$549=3,1)+O4821))))","v":0},332,{"$f":"IF(Daten!$L$549=3,N4832,0)","v":0},null,250]
["ICS5000",7,150,"ICS5000 1507",null,"ICM 820 Wandkonsolen  (Paar) L820mm","101978","0",null,"STK",238,null,null,582]
["ICS5000",9,150,"ICS5000 1509",null,"ICM 1120 Wandkonsolen  (Paar) L1120mm","101980","0",null,"STK",288,null,null,882]
[{"$f":"A4828","v":"ICS5000"},{"$f":"B4828+1","v":12},{"$f":"C4828","v":150},"ICS5000 15012",null,"ICM5000 150  Verankerungsplatte mit Ablauf senkr.","102916",95,null,"STK",146,{"$f":"IF(Daten!$L$499=1,1,\"\")","v":1},{"$f":"IF(L4829=\"\",\"0\",L4829*H4829)","v":95},null,null,{"$f":"IF(L4829=\"\",\"0\",H4829*L4829)","v":95}]
["ICS5000",15,150,"ICS5000 15015",null,"ICM5000 150 Kondensattopf","102955","0",null,"STK",87,null,{"$f":"IF(L4832=\"\",\"0\",L4832*H4832)","v":"0"},null,null,"0"]
["ICS5000",17,150,"ICS5000 15017",null,"ICM5000 150 Putztüranschluss rund Überdruck","102968",455,null,"STK",280,{"$f":"Daten!$P$499","v":1},455,null,null,455]
["ICS5000",18,150,"ICS5000 15018",null,"ICM5000 150 T-Stück 45°","102981",455,null,"STK",525,{"$f":"IF(Daten!$L$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS5000",22,150,"ICS5000 15022",null,"ICM5000 150 Anschluss von DW auf EW in Rauchgasr.","140759","0",null,"STK",146,null,{"$f":"IF(H4839=\"\",\"\",L4839*H4839)","v":0}]
["ICS5000",23,150,"ICS5000 15023",null,"ICM5000 150 Flansch zum Anschweissen im Auftrag","103044","0",null,"STK",84,null,{"$f":"IF(H4840=\"\",\"\",L4840*H4840)","v":0}]
["ICS5000",26,150,"ICS5000 15026",null,"ICM5000 150 Längenelement L250mm","103070",205,null,"STK",75,{"$f":"IF(N4843+O4843=0,\"\",N4843+O4843)","v":""},{"$f":"IF(L4843=\"\",0,L4843*H4843)","v":0},{"$f":"'ICS5000'!$P$20","v":0},{"$f":"IF(Daten!$L$507=2,1,0)","v":0},{"$f":"(IF(L4843=\"\",0,H4843*L4843))-O4843","v":0}]
["ICS5000",28,150,"ICS5000 15028",null,"ICM5000 150 Längenelement L1000mm","103096",955,null,"STK",141,{"$f":"ROUNDUP(M4845,0)+O4845","v":10},{"$f":"((M4817-SUM(M4829:M4844)-M4866)/H4845)","v":9.1099476439790568},null,{"$f":"IF(Daten!$L$507=4,1,0)","v":0},{"$f":"(IF(L4845=\"\",0,H4845*L4845))-O4845","v":9550}]
["ICS5000",32,150,"ICS5000 15032",null,"ICM5000 150 Klemmband bei jedem Bauteil inkl. ","103148","0",null,"STK",13,null,"im Bauteil enthalten",null,null,{"$f":"IF(L4849=\"\",\"0\",H4849*L4849)","v":"0"}]
["ICS5000",33,150,"ICS5000 15033",null,"ICM 150 Wandhalter verstellbar 75 - 300mm DN 200mm","102292","0",null,"STK",72,null,null,"75-300",null,{"$f":"IF(L4850=\"\",\"0\",H4850*L4850)","v":"0"}]
["ICS5000",35,150,"ICS5000 15035",null,"ICM W1 Verlängerung zu Wandhalter 50mm L 130mm","102317","0",null,"STK",44,{"$f":"IF(Daten!$L$549=2,$L4851,\"\")","v":""},null,100,null,"0"]
["ICS5000",38,150,"ICS5000 15038",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,500,null,"0"]
["ICS5000",41,150,"ICS5000 15041",null,"ICM 150-180 Dachdurführung 16-25° DN250 ","102337","0",null,"STK",347,{"$f":"IF(Daten!$L$522=3,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",43,150,"ICS5000 15043",null,"ICM 150-180 Dachdurführung 36-45° DN250 ","102361","0",null,"STK",466,{"$f":"IF(Daten!$L$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",46,150,"ICS5000 15046",null,"ICM 150 Blende 0-30° DN200","102402","0",null,"STK",70,{"$f":"IF(Daten!$O$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",49,150,"ICS5000 15049",null,"ICM 150 Mündungsabschluss","102434",295,null,"STK",130,{"$f":"IF(Daten!$O$522=1,1,\"\")","v":1},{"$f":"IF(L4866=\"\",\"0\",L4866*H4866)","v":295},null,null,295]
["ICS5000",51,150,"ICS5000 15051",null,"ICM5000 150 Mündungsabschluss horizontal","103174","0",null,"STK",174,{"$f":"IF(Daten!$O$522=3,1,\"\")","v":""},{"$f":"IF(L4868=\"\",\"0\",L4868*H4868)","v":"0"},null,null,"0"]
["ICS5000",54,150,"ICS5000 15054",null,"ICM5000 150 Winkel 30°","103208","0",null,"STK",115,{"$f":"IF(N4871=1,\"\",O4871)","v":""},{"$f":"IF(L4871=\"\",0,L4871*H4871)","v":0},{"$f":"Daten!$O$540","v":1},{"$f":"Daten!$P$540","v":"Nein"},"0"]
["ICS5000",56,150,"ICS5000 15056",null,"ICM5000 150 Winkel 90°","103234","0",null,"STK",132,{"$f":"IF(N4873=1,\"\",O4873)","v":""},{"$f":"IF(L4873=\"\",0,L4873*H4873)","v":0},{"$f":"Daten!$O$556","v":1},{"$f":"Daten!$P$556","v":"Nein"},"0"]
["ICS5000",0,180,{"$f":"A4874&\" \"&C4874&B4874","v":"ICS5000 1800"}," ","Schiedel ICS5000 25mm 180","ICS5000 180","0",{"$f":"'ICS5000'!$J$10","v":10},"Anlage",0,1,{"$f":"I4874*1000","v":10000},null,{"$f":"ROUNDUP(P4874,2)","v":10.85},{"$f":"SUM(P4876:P4929)/1000","v":10.85}]
["ICS5000",4,180,"ICS5000 1804",null,"ICM 620 Wandkonsolen  (Paar) L620mm","101976","0",null,"STK",223,null,null,382]
["ICS5000",5,180,"ICS5000 1805",null,"ICM 720 Wandkonsolen  (Paar) L720mm","101977","0",null,"STK",228,{"$f":"IF(M4879=0,\"\",M4879)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M4875=1,0,IF(Daten!$L$549=4,1)+O4879))))","v":0},482,{"$f":"IF(Daten!$L$549=4,N4889,0)","v":0},null,400]
["ICS5000",8,180,"ICS5000 1808",null,"ICM 1120 Wandkonsolen  (Paar) L1120mm","101980","0",null,"STK",288,null,null,882]
[{"$f":"A4883","v":"ICS5000"},{"$f":"B4883+1","v":10},{"$f":"C4883","v":180},"ICS5000 18010",null,"ICM 1504 Wandkonsolen  (Paar) L1504mm","101982","0",null,"STK",358,null,null,1100]
["ICS5000",14,180,"ICS5000 18014",null,"ICM5000 180 Kondensattopf","102956","0",null,"STK",96,null,{"$f":"IF(L4888=\"\",\"0\",L4888*H4888)","v":"0"},null,null,"0"]
["ICS5000",15,180,"ICS5000 18015",null,"ICM5000 180 Element mit Empa Messstutzen","140769","0",null,"STK",596,null,"0",null,null,"0"]
["ICS5000",17,180,"ICS5000 18017",null,"ICM5000 180 T-Stück 45°","102982",455,null,"STK",571,{"$f":"IF(Daten!$L$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS5000",20,180,"ICS5000 18020",null,"ICM5000 180 Anschluss von EW auf DW in Rauchgasr.","103021","0",null,"STK",250,1,0,null,null,{"$f":"IF(L4894=\"\",\"0\",H4895*L4894)","v":0}]
["ICS5000",23,180,"ICS5000 18023",null,"ICM5000 180 Erweiterung um 1Ø in Rauchgasrichtung","103034","0",null,"STK",99,null,{"$f":"IF(H4897=\"\",\"\",L4897*H4897)","v":0}]
["ICS5000",25,180,"ICS5000 18025",null,"ICM5000 180 Längenelement L250mm","103071",205,null,"STK",82,{"$f":"IF(N4899+O4899=0,\"\",N4899+O4899)","v":""},{"$f":"IF(L4899=\"\",0,L4899*H4899)","v":0},{"$f":"'ICS5000'!$P$20","v":0},{"$f":"IF(Daten!$L$507=2,1,0)","v":0},{"$f":"(IF(L4899=\"\",0,H4899*L4899))-O4899","v":0}]
["ICS5000",28,180,"ICS5000 18028",null,"ICM5000 180 Schiebeelement L375 - 585mm","103110","0",null,"STK",201,null,null,null,null,{"$f":"IF(L4902=\"\",\"0\",H4902*L4902)","v":"0"}]
["ICS5000",31,180,"ICS5000 18031",null,"ICM5000 180 Klemmband bei jedem Bauteil inkl. ","103149","0",null,"STK",14,null,"im Bauteil enthalten",null,null,{"$f":"IF(L4905=\"\",\"0\",H4905*L4905)","v":"0"}]
["ICS5000",33,180,"ICS5000 18033",null,"ICM 180 Wandhalter 50mm verlängerbar DN 230mm ","102307","0",null,"STK",55,{"$f":"ROUNDUP(M4907,0)","v":3},{"$f":"((M4874/1000)/4.3)","v":2.3255813953488373},null,null,0]
["ICS5000",36,180,"ICS5000 18036",null,"ICM L2 Verlängerung zu Wandhalter 50mm L450mm","102320","0",null,"STK",142,{"$f":"IF(Daten!$L$549=4,$L4907,\"\")","v":""},null,440,null,"0"]
["ICS5000",38,180,"ICS5000 18038",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,{"$f":"IF(Daten!$L$549=5,$L4907,\"\")","v":""},null,700,null,"0"]
["ICS5000",39,180,"ICS5000 18039",null,"ICM 150-180 Dachdurführung 0° DN250 L500mm","102325","0",null,"STK",163,{"$f":"IF(Daten!$L$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",43,180,"ICS5000 18043",null,"ICM 180 Regenkragen DN230","102375","0",null,"STK",55,{"$f":"IF(SUM(L4913:L4916)=0,\"\",SUM(L4913:L4916))","v":""},null,null,null,"0"]
["ICS5000",45,180,"ICS5000 18045",null,"ICM 180 Blende 0-30° DN230","102403","0",null,"STK",73,{"$f":"IF(Daten!$O$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",48,180,"ICS5000 18048",null,"ICM 180 Mündungsabschluss","102435",295,null,"STK",142,{"$f":"IF(Daten!$O$522=1,1,\"\")","v":1},{"$f":"IF(L4922=\"\",\"0\",L4922*H4922)","v":295},null,null,295]
["ICS5000",49,180,"ICS5000 18049",null,"ICM5000 180 Abluftregenhut Typ AT Inox ","140751","0",null,"STK",450,{"$f":"IF(Daten!$O$522=2,1,\"\")","v":""},{"$f":"IF(L4923=\"\",\"0\",L4923*H4923)","v":"0"},null,null,"0"]
["ICS5000",53,180,"ICS5000 18053",null,"ICM5000 180 Winkel 30°","103209","0",null,"STK",125,{"$f":"IF(N4927=1,\"\",O4927)","v":""},{"$f":"IF(L4927=\"\",0,L4927*H4927)","v":0},{"$f":"Daten!$O$540","v":1},{"$f":"Daten!$P$540","v":"Nein"},"0"]
["ICS5000",54,180,"ICS5000 18054",null,"ICM5000 180 Winkel 45°","103222","0",null,"STK",124,{"$f":"IF(N4928=1,\"\",O4928)","v":""},{"$f":"IF(L4928=\"\",0,L4928*H4928)","v":0},{"$f":"Daten!$O$548","v":1},{"$f":"Daten!$P$548","v":"Nein"},"0"]
["ICS5000",0,200,{"$f":"A4930&\" \"&C4930&B4930","v":"ICS5000 2000"}," ","Schiedel ICS5000 25mm 200","ICS5000 200","0",{"$f":"'ICS5000'!$J$10","v":10},"Anlage",0,1,{"$f":"I4930*1000","v":10000},null,{"$f":"ROUNDUP(P4930,2)","v":10.85},{"$f":"SUM(P4932:P4985)/1000","v":10.85}]
["ICS5000",3,200,"ICS5000 2003",null,"ICM 570 Wandkonsolen  (Paar) L570mm","101975","0",null,"STK",217,{"$f":"IF(M4933=0,\"\",M4933)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M4931=1,0,IF(Daten!$L$549=3,1)+O4933))))","v":0},302,{"$f":"IF(Daten!$L$549=3,N4944,0)","v":0},null,250]
["ICS5000",6,200,"ICS5000 2006",null,"ICM 820 Wandkonsolen  (Paar) L820mm","101978","0",null,"STK",238,null,null,552]
["ICS5000",8,200,"ICS5000 2008",null,"ICM 1120 Wandkonsolen  (Paar) L1120mm","101980","0",null,"STK",288,null,null,852]
["ICS5000",11,200,"ICS5000 20011",null,"ICM5000 200  Verankerungsplatte mit Ablauf senkr.","102918",95,null,"STK",181,{"$f":"IF(Daten!$L$499=1,1,\"\")","v":1},{"$f":"IF(L4941=\"\",\"0\",L4941*H4941)","v":95},null,null,{"$f":"IF(L4941=\"\",\"0\",H4941*L4941)","v":95}]
["ICS5000",13,200,"ICS5000 20013",null,"ICM5000 200 Zwischenstütze","102944",285,null,"STK",181,{"$f":"IF(N4943=0,\"\",N4943)","v":""},{"$f":"IF(L4943=\"\",0,L4943*H4943)","v":0},{"$f":"IF(M4930>=15000,1,0)","v":0},null,"0"]
["ICS5000",16,200,"ICS5000 20016",null,"ICM5000 200 Putztüranschluss rund Überdruck","102970",455,null,"STK",320,{"$f":"Daten!$P$499","v":1},455,null,null,455]
["ICS5000",17,200,"ICS5000 20017",null,"ICM5000 200 T-Stück 45°","102983",530,null,"STK",592,{"$f":"IF(Daten!$L$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS5000",21,200,"ICS5000 20021",null,"ICM5000 200 Anschluss von DW auf EW in Rauchgasr.","140761","0",null,"STK",160,null,{"$f":"IF(H4951=\"\",\"\",L4951*H4951)","v":0}]
["ICS5000",22,200,"ICS5000 20022",null,"ICM5000 200 Flansch zum Anschweissen im Auftrag","103046","0",null,"STK",100,null,{"$f":"IF(H4952=\"\",\"\",L4952*H4952)","v":0}]
["ICS5000",26,200,"ICS5000 20026",null,"ICM5000 200 Längenelement L500mm","103085",455,null,"STK",116,{"$f":"IF(N4956+O4956=0,\"\",N4956+O4956)","v":""},{"$f":"IF(L4956=\"\",0,L4956*H4956)","v":0},{"$f":"'ICS5000'!$P$18","v":0},{"$f":"IF(Daten!$L$507=3,1,0)","v":0},{"$f":"(IF(L4956=\"\",0,H4956*L4956))-O4956","v":0}]
["ICS5000",28,200,"ICS5000 20028",null,"ICM5000 200 Schiebeelement L375 - 585mm","103111","0",null,"STK",209,null,null,null,null,{"$f":"IF(L4958=\"\",\"0\",H4958*L4958)","v":"0"}]
["ICS5000",31,200,"ICS5000 20031",null,"ICM5000 200 Klemmband bei jedem Bauteil inkl. ","103150","0",null,"STK",14,null,"im Bauteil enthalten",null,null,{"$f":"IF(L4961=\"\",\"0\",H4961*L4961)","v":"0"}]
["ICS5000",32,200,"ICS5000 20032",null,"ICM 200 Wandhalter verstellbar 75 - 300mm DN 250mm","102294","0",null,"STK",82,null,null,"75-300",null,{"$f":"IF(L4962=\"\",\"0\",H4962*L4962)","v":"0"}]
["ICS5000",36,200,"ICS5000 20036",null,"ICM L2 Verlängerung zu Wandhalter 50mm L450mm","102320","0",null,"STK",142,{"$f":"IF(Daten!$L$549=4,$L4963,\"\")","v":""},null,440,null,"0"]
["ICS5000",37,200,"ICS5000 20037",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,500,null,"0"]
["ICS5000",39,200,"ICS5000 20039",null,"ICM 200 Dachdurführung 0° DN300 L500mm","102326","0",null,"STK",185,{"$f":"IF(Daten!$L$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",42,200,"ICS5000 20042",null,"ICM 200 Dachdurführung 36-45° DN320 mit Bleilappen","102362","0",null,"STK",498,{"$f":"IF(Daten!$L$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",45,200,"ICS5000 20045",null,"ICM 200 Blende 0-30° DN250","102404","0",null,"STK",77,{"$f":"IF(Daten!$O$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",47,200,"ICS5000 20047",null,"ICM 200 Anschlussrosette Øi 250mm ØA 520mm","102420","0",null,"STK",65,{"$f":"IF(Daten!$O$515=4,1,\"\")","v":""},null,null,null,{"$f":"IF(L4977=\"\",\"0\",H4977*L4977)","v":"0"}]
["ICS5000",50,200,"ICS5000 20050",null,"ICM5000 200 Mündungsabschluss horizontal","103176","0",null,"STK",198,{"$f":"IF(Daten!$O$522=3,1,\"\")","v":""},{"$f":"IF(L4980=\"\",\"0\",L4980*H4980)","v":"0"},null,null,"0"]
["ICS5000",52,200,"ICS5000 20052",null,"ICM5000 200 Winkel 15°","103202","0",null,"STK",143,{"$f":"IF(N4982=1,\"\",O4982)","v":""},{"$f":"IF(L4982=\"\",0,L4982*H4982)","v":0},{"$f":"Daten!$O$532","v":1},{"$f":"Daten!$P$532","v":"Nein"},"0"]
["ICS5000",55,200,"ICS5000 20055",null,"ICM5000 200 Winkel 90°","103236","0",null,"STK",156,{"$f":"IF(N4985=1,\"\",O4985)","v":""},{"$f":"IF(L4985=\"\",0,L4985*H4985)","v":0},{"$f":"Daten!$O$556","v":1},{"$f":"Daten!$P$556","v":"Nein"},"0"]
["ICS5000",0,250,{"$f":"A4986&\" \"&C4986&B4986","v":"ICS5000 2500"}," ","Schiedel ICS5000 25mm 250","ICS5000 250","0",{"$f":"'ICS5000'!$J$10","v":10},"Anlage",0,1,{"$f":"I4986*1000","v":10000},null,{"$f":"ROUNDUP(P4986,2)","v":10.85},{"$f":"SUM(P4988:P5041)/1000","v":10.85}]
["ICS5000",4,250,"ICS5000 2504",null,"ICM 620 Wandkonsolen  (Paar) L620mm","101976","0",null,"STK",223,null,null,252]
["ICS5000",5,250,"ICS5000 2505",null,"ICM 720 Wandkonsolen  (Paar) L720mm","101977","0",null,"STK",228,{"$f":"IF(M4991=0,\"\",M4991)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF($M$4987=1,0,IF(Daten!$L$549=4,1)+O4991))))","v":0},402,{"$f":"IF(Daten!$L$549=4,N5001,0)","v":0},null,400]
["ICS5000",9,250,"ICS5000 2509",null,"ICM 1304 Wandkonsolen  (Paar) L1304mm","101981","0",null,"STK",315,null,null,986]
[{"$f":"A4996","v":"ICS5000"},{"$f":"B4996+1","v":11},{"$f":"C4996","v":250},"ICS5000 25011",null,"ICM5000 250  Verankerungsplatte mit Ablauf senkr.","102919",95,null,"STK",226,{"$f":"IF(Daten!$L$499=1,1,\"\")","v":1},{"$f":"IF(L4997=\"\",\"0\",L4997*H4997)","v":95},null,null,{"$f":"IF(L4997=\"\",\"0\",H4997*L4997)","v":95}]
["ICS5000",14,250,"ICS5000 25014",null,"ICM5000 250 Kondensattopf","102958","0",null,"STK",121,null,{"$f":"IF(L5000=\"\",\"0\",L5000*H5000)","v":"0"},null,null,"0"]
["ICS5000",17,250,"ICS5000 25017",null,"ICM5000 250 T-Stück 45°","102984",560,null,"STK",708,{"$f":"IF(Daten!$L$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS5000",19,250,"ICS5000 25019",null,"ICM5000 250 Verschlussdeckel","103010","0",null,"STK",123,null,"0",null,null,"0"]
["ICS5000",20,250,"ICS5000 25020",null,"ICM5000 250 Anschluss von EW auf DW in Rauchgasr.","103023","0",null,"STK",286,1,0,null,null,{"$f":"IF(L5006=\"\",\"0\",H5007*L5006)","v":0}]
["ICS5000",22,250,"ICS5000 25022",null,"ICM5000 250 Flansch zum Anschweissen im Auftrag","103047","0",null,"STK",103,null,{"$f":"IF(H5008=\"\",\"\",L5008*H5008)","v":0}]
["ICS5000",25,250,"ICS5000 25025",null,"ICM5000 250 Längenelement L250mm","103073",205,null,"STK",99,{"$f":"IF(N5011+O5011=0,\"\",N5011+O5011)","v":""},{"$f":"IF(L5011=\"\",0,L5011*H5011)","v":0},{"$f":"'ICS5000'!$P$20","v":0},{"$f":"IF(Daten!$L$507=2,1,0)","v":0},{"$f":"(IF(L5011=\"\",0,H5011*L5011))-O5011","v":0}]
["ICS5000",28,250,"ICS5000 25028",null,"ICM5000 250 Schiebeelement L375 - 585mm","103112","0",null,"STK",231,null,null,null,null,{"$f":"IF(L5014=\"\",\"0\",H5014*L5014)","v":"0"}]
["ICS5000",30,250,"ICS5000 25030",null,"ICM5000 250 Dichtmanchette für Aussenmantel","103138","0",null,"STK",60,null,"im Bauteil enthalten",null,null,{"$f":"IF(L5016=\"\",\"0\",H5016*L5016)","v":"0"}]
["ICS5000",34,250,"ICS5000 25034",null,"ICM W1 Verlängerung zu Wandhalter 50mm L 130mm","102317","0",null,"STK",44,{"$f":"IF(Daten!$L$549=2,$L5019,\"\")","v":""},null,100,100,"0"]
["ICS5000",35,250,"ICS5000 25035",null,"ICM L1 Verlängerung zu Wandhalter 50mm L300mm","102319","0",null,"STK",109,null,null,220,null,"0"]
["ICS5000",39,250,"ICS5000 25039",null,"ICM 250-300 Dachdurführung 0° DN370 L500mm","102327","0",null,"STK",228,{"$f":"IF(Daten!$L$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",40,250,"ICS5000 25040",null,"ICM 250-300 Dachdurführung 16-25° DN370 ","102339","0",null,"STK",444,{"$f":"IF(Daten!$L$522=3,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",43,250,"ICS5000 25043",null,"ICM 250 Regenkragen DN300","102377","0",null,"STK",65,{"$f":"IF(SUM(L5025:L5028)=0,\"\",SUM(L5025:L5028))","v":""},null,null,null,"0"]
["ICS5000",45,250,"ICS5000 25045",null,"ICM 250 Blende 0-30° DN300","102405","0",null,"STK",87,{"$f":"IF(Daten!$O$515=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",48,250,"ICS5000 25048",null,"ICM 250 Mündungsabschluss","102437",295,null,"STK",174,{"$f":"IF(Daten!$O$522=1,1,\"\")","v":1},{"$f":"IF(L5034=\"\",\"0\",L5034*H5034)","v":295},null,null,295]
["ICS5000",50,250,"ICS5000 25050",null,"ICM5000 250 Mündungsabschluss horizontal","103177","0",null,"STK",230,{"$f":"IF(Daten!$O$522=3,1,\"\")","v":""},{"$f":"IF(L5036=\"\",\"0\",L5036*H5036)","v":"0"},null,null,"0"]
["ICS5000",53,250,"ICS5000 25053",null,"ICM5000 250 Winkel 30°","103211","0",null,"STK",167,{"$f":"IF(N5039=1,\"\",O5039)","v":""},{"$f":"IF(L5039=\"\",0,L5039*H5039)","v":0},{"$f":"Daten!$O$540","v":1},{"$f":"Daten!$P$540","v":"Nein"},"0"]
["ICS5000",0,300,{"$f":"A5042&\" \"&C5042&B5042","v":"ICS5000 3000"}," ","Schiedel ICS5000 25mm 300","ICS5000 300","0",{"$f":"'ICS5000'!$J$10","v":10},"Anlage",0,1,{"$f":"I5042*1000","v":10000},null,{"$f":"ROUNDUP(P5042,2)","v":10.9},{"$f":"SUM(P5044:P5097)/1000","v":10.9}]
[{"$f":"A5043","v":"ICS5000"},{"$f":"B5043+1","v":2},{"$f":"C5043","v":300},{"$f":"A5044&\" \"&C5044&B5044","v":"ICS5000 3002"},null,"ICM 475 Wandkonsolen  (Paar) L475mm","101974","0",null,"STK",158,{"$f":"IF(M5044=0,\"\",M5044)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M5043=1,0,IF(Daten!$L$549=2,1)+O5044))))","v":0},107,{"$f":"IF(Daten!$L$549=2,N5056,0)","v":0},null,100]
["ICS5000",3,300,"ICS5000 3003",null,"ICM 570 Wandkonsolen  (Paar) L570mm","101975","0",null,"STK",217,null,null,202,null,null,250]
["ICS5000",5,300,"ICS5000 3005",null,"ICM 720 Wandkonsolen  (Paar) L720mm","101977","0",null,"STK",228,{"$f":"IF(M5047=0,\"\",M5047)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF($M$5043=1,0,IF(Daten!$L$549=3,1)+O5047))))","v":0},352,{"$f":"IF(Daten!$L$549=3,N5054,0)","v":0},null,250]
["ICS5000",8,300,"ICS5000 3008",null,"ICM 1120 Wandkonsolen  (Paar) L1120mm","101980","0",null,"STK",288,null,null,752]
[{"$f":"A5052","v":"ICS5000"},{"$f":"B5052+1","v":11},{"$f":"C5052","v":300},"ICS5000 30011",null,"ICM5000 300  Verankerungsplatte mit Ablauf senkr.","102920",95,null,"STK",251,{"$f":"IF(Daten!$L$499=1,1,\"\")","v":1},{"$f":"IF(L5053=\"\",\"0\",L5053*H5053)","v":95},null,null,{"$f":"IF(L5053=\"\",\"0\",H5053*L5053)","v":95}]
["ICS5000",13,300,"ICS5000 30013",null,"ICM5000 300 Zwischenstütze","102946",385,null,"STK",251,{"$f":"IF(N5055=0,\"\",N5055)","v":""},{"$f":"IF(L5055=\"\",0,L5055*H5055)","v":0},{"$f":"IF(M5042>=15000,1,0)","v":0},null,"0"]
["ICS5000",17,300,"ICS5000 30017",null,"ICM5000 300 T-Stück 45°","102985",623,null,"STK",851,{"$f":"IF(Daten!$L$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS5000",18,300,"ICS5000 30018",null,"ICM5000 300 T-Stück 90°","102998",480,null,"STK",437,{"$f":"IF(Daten!$L$515=2,1,\"\")","v":1},480,null,null,480]
["ICS5000",22,300,"ICS5000 30022",null,"ICM5000 300 Flansch zum Anschweissen im Auftrag","103048","0",null,"STK",112,null,{"$f":"IF(H5064=\"\",\"\",L5064*H5064)","v":0}]
["ICS5000",23,300,"ICS5000 30023",null,"ICM5000 300 Erweiterung um 1Ø in Rauchgasrichtung","103037","0",null,"STK",112,null,{"$f":"IF(H5065=\"\",\"\",L5065*H5065)","v":0}]
["ICS5000",26,300,"ICS5000 30026",null,"ICM5000 300 Längenelement L500mm","103087",455,null,"STK",154,{"$f":"IF(N5068+O5068=0,\"\",N5068+O5068)","v":""},{"$f":"IF(L5068=\"\",0,L5068*H5068)","v":0},{"$f":"'ICS5000'!$P$18","v":0},{"$f":"IF(Daten!$L$507=3,1,0)","v":0},{"$f":"(IF(L5068=\"\",0,H5068*L5068))-O5068","v":0}]
["ICS5000",28,300,"ICS5000 30028",null,"ICM5000 300 Schiebeelement L375 - 585mm","103113","0",null,"STK",248,null,null,null,null,{"$f":"IF(L5070=\"\",\"0\",H5070*L5070)","v":"0"}]
["ICS5000",31,300,"ICS5000 30031",null,"ICM5000 300 Klemmband bei jedem Bauteil inkl. ","103152","0",null,"STK",15,null,"im Bauteil enthalten",null,null,{"$f":"IF(L5073=\"\",\"0\",H5073*L5073)","v":"0"}]
["ICS5000",33,300,"ICS5000 30033",null,"ICM 300 Wandhalter 50mm verlängerbar DN 350mm ","102310","0",null,"STK",87,{"$f":"ROUNDUP(M5075,0)","v":3},{"$f":"((M5042/1000)/4.3)","v":2.3255813953488373},null,null,0]
["ICS5000",36,300,"ICS5000 30036",null,"ICM L2 Verlängerung zu Wandhalter 50mm L450mm","102320","0",null,"STK",142,{"$f":"IF(Daten!$L$549=3,$L5076,\"\")","v":""},null,370,250,"0"]
["ICS5000",39,300,"ICS5000 30039",null,"ICM 300 Dachdurführung 0° DN400 L500mm","102328","0",null,"STK",271,{"$f":"IF(Daten!$L$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",41,300,"ICS5000 30041",null,"ICM 300 Dachdurführung 26-35° DN400 mit Bleilappen","102352","0",null,"STK",585,{"$f":"IF(Daten!$L$522=4,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",42,300,"ICS5000 30042",null,"ICM 300 Dachdurführung 36-45° DN400 mit Bleilappen","102364","0",null,"STK",596,{"$f":"IF(Daten!$L$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",46,300,"ICS5000 30046",null,"ICM 300 Blende 32-45° DN350","102414","0",null,"STK",109,{"$f":"IF(Daten!$O$515=3,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",47,300,"ICS5000 30047",null,"ICM 300 Anschlussrosette Øi 350mm ØA 620mm","102422","0",null,"STK",71,{"$f":"IF(Daten!$O$515=4,1,\"\")","v":""},null,null,null,{"$f":"IF(L5089=\"\",\"0\",H5089*L5089)","v":"0"}]
["ICS5000",50,300,"ICS5000 30050",null,"ICM5000 300 Mündungsabschluss horizontal","103178","0",null,"STK",300,{"$f":"IF(Daten!$O$522=3,1,\"\")","v":""},{"$f":"IF(L5092=\"\",\"0\",L5092*H5092)","v":"0"},null,null,"0"]
["ICS5000",52,300,"ICS5000 30052",null,"ICM5000 300 Winkel 15°","103204","0",null,"STK",179,{"$f":"IF(N5094=1,\"\",O5094)","v":""},{"$f":"IF(L5094=\"\",0,L5094*H5094)","v":0},{"$f":"Daten!$O$532","v":1},{"$f":"Daten!$P$532","v":"Nein"},"0"]
["ICS5000",0,350,{"$f":"A5098&\" \"&C5098&B5098","v":"ICS5000 3500"}," ","Schiedel ICS5000 25mm 350","ICS5000 350","0",{"$f":"'ICS5000'!$J$10","v":10},"Anlage",0,1,{"$f":"I5098*1000","v":10000},null,{"$f":"ROUNDUP(P5098,2)","v":10.049999999999999},{"$f":"SUM(P5100:P5147)/1000","v":10.045}]
[{"$f":"A5098","v":"ICS5000"},{"$f":"B5098+1","v":1},{"$f":"C5098","v":350},{"$f":"A5099&\" \"&C5099&B5099","v":"ICS5000 3501"},null,"ICM 350 Konsolenbleche (Paar)","101962","0",null,"STK",309,{"$f":"N5099","v":1},{"$f":"IF(Daten!$L$549=1,1,\"\")","v":1},{"$f":"IF(Daten!$L$499=1,M5099,\"\")","v":1},null,{"$f":"IF(L5099=\"\",\"0\",H5099*L5099)","v":0}]
["ICS5000",3,350,"ICS5000 3503",null,"ICM 570 Wandkonsolen  (Paar) L570mm","101975","0",null,"STK",217,{"$f":"IF(M5101=0,\"\",M5101)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF($M$5099=1,0,IF(Daten!$L$549=2,1)+O5101))))","v":0},152,{"$f":"IF(Daten!$L$549=2,#REF!,0)","v":0},null,100]
["ICS5000",6,350,"ICS5000 3506",null,"ICM 820 Wandkonsolen  (Paar) L820mm","101978","0",null,"STK",238,{"$f":"IF(M5104=0,\"\",M5104)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF($M$5099=1,0,IF(Daten!$L$549=4,1)+O5104))))","v":0},402,{"$f":"IF(Daten!$L$549=4,N5110,0)","v":0},null,400]
["ICS5000",8,350,"ICS5000 3508",null,"ICM 1120 Wandkonsolen  (Paar) L1120mm","101980","0",null,"STK",288,{"$f":"IF(M5106=0,\"\",M5106)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF($M$5099=1,0,IF(Daten!$L$549=5,1)+O5106))))","v":0},702,{"$f":"IF(Daten!$L$549=5,N5113,0)","v":0},null,600]
[{"$f":"A5108","v":"ICS5000"},{"$f":"B5108+1","v":11},{"$f":"C5108","v":350},"ICS5000 35011",null,"ICM5000 350  Verankerungsplatte mit Ablauf senkr.","102921",95,null,"STK",281,{"$f":"IF(Daten!$L$499=1,1,\"\")","v":1},{"$f":"IF(L5109=\"\",\"0\",L5109*H5109)","v":95},null,null,{"$f":"IF(L5109=\"\",\"0\",H5109*L5109)","v":95}]
["ICS5000",14,350,"ICS5000 35014",null,"ICM5000 350 Kondensattopf","102960","0",null,"STK",228,null,{"$f":"IF(L5112=\"\",\"0\",L5112*H5112)","v":"0"},null,null,"0"]
["ICS5000",17,350,"ICS5000 35017",null,"ICM5000 350 T-Stück 90°","102999",530,null,"STK",548,{"$f":"IF(Daten!$L$515=2,1,\"\")","v":1},530,null,null,530]
["ICS5000",19,350,"ICS5000 35019",null,"ICM5000 350 Anschluss von EW auf DW in Rauchgasr.","103025","0",null,"STK",327,1,0,null,null,{"$f":"IF(L5117=\"\",\"0\",H5118*L5117)","v":0}]
["ICS5000",22,350,"ICS5000 35022",null,"ICM5000 350 Erweiterung um 1Ø in Rauchgasrichtung","103038","0",null,"STK",118,null,{"$f":"IF(H5120=\"\",\"\",L5120*H5120)","v":0}]
["ICS5000",24,350,"ICS5000 35024",null,"ICM5000 350 Längenelement L250mm","103075",205,null,"STK",132,{"$f":"IF(N5122+O5122=0,\"\",N5122+O5122)","v":""},{"$f":"IF(L5122=\"\",0,L5122*H5122)","v":0},{"$f":"'ICS5000'!$P$20","v":0},{"$f":"IF(Daten!$L$507=2,1,0)","v":0},{"$f":"(IF(L5122=\"\",0,H5122*L5122))-O5122","v":0}]
["ICS5000",25,350,"ICS5000 35025",null,"ICM5000 350 Längenelement L500mm","103088",455,null,"STK",237,{"$f":"IF(N5123+O5123=0,\"\",N5123+O5123)","v":""},{"$f":"IF(L5123=\"\",0,L5123*H5123)","v":0},{"$f":"'ICS5000'!$P$18","v":0},{"$f":"IF(Daten!$L$507=3,1,0)","v":0},{"$f":"(IF(L5123=\"\",0,H5123*L5123))-O5123","v":0}]
["ICS5000",29,350,"ICS5000 35029",null,"ICM5000 350 Dichtmanchette für Aussenmantel","103140","0",null,"STK",74,null,"im Bauteil enthalten",null,null,{"$f":"IF(L5127=\"\",\"0\",H5127*L5127)","v":"0"}]
["ICS5000",31,350,"ICS5000 35031",null,"ICM 350 Wandhalter verstellbar 75 - 300mm DN 400mm","102297","0",null,"STK",98,null,null,"75-300",null,{"$f":"IF(L5129=\"\",\"0\",H5129*L5129)","v":"0"}]
["ICS5000",34,350,"ICS5000 35034",null,"ICM L1 Verlängerung zu Wandhalter 50mm L300mm","102319","0",null,"STK",109,null,null,160,null,"0"]
["ICS5000",35,350,"ICS5000 35035",null,"ICM L2 Verlängerung zu Wandhalter 50mm L450mm","102320","0",null,"STK",142,{"$f":"IF(Daten!$L$549=3,$L5131,\"\")","v":""},null,310,250,"0"]
["ICS5000",39,350,"ICS5000 35039",null,"ICM 350 Dachdurführung 16-25° DN450 mit Bleilappen","102341","0",null,"STK",596,{"$f":"IF(Daten!$L$522=3,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",40,350,"ICS5000 35040",null,"ICM 350 Dachdurführung 26-35° DN450 mit Bleilappen","102353","0",null,"STK",649,{"$f":"IF(Daten!$L$522=4,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",42,350,"ICS5000 35042",null,"ICM 350 Regenkragen DN400","102379","0",null,"STK",87,{"$f":"IF(SUM(L5136:L5139)=0,\"\",SUM(L5136:L5139))","v":""},null,null,null,"0"]
["ICS5000",45,350,"ICS5000 35045",null,"ICM5000 350 Mündungsabschluss horizontal","103179","0",null,"STK",309,{"$f":"IF(Daten!$O$522=3,1,\"\")","v":""},{"$f":"IF(L5143=\"\",\"0\",L5143*H5143)","v":"0"},null,null,"0"]
["ICS5000",47,350,"ICS5000 35047",null,"ICM5000 350 Winkel 30°","103213","0",null,"STK",299,{"$f":"IF(N5145=1,\"\",O5145)","v":""},{"$f":"IF(L5145=\"\",0,L5145*H5145)","v":0},{"$f":"Daten!$O$540","v":1},{"$f":"Daten!$P$540","v":"Nein"},"0"]
["ICS5000",0,400,"ICS5000 4000"," ","Schiedel ICS5000 25mm 400","ICS5000 400","0",{"$f":"'ICS5000'!$J$10","v":10},"Anlage",0,1,{"$f":"I5148*1000","v":10000},null,{"$f":"ROUNDUP(P5148,2)","v":10.199999999999999},{"$f":"SUM(P5150:P5197)/1000","v":10.195}]
["ICS5000",3,400,"ICS5000 4003",null,"ICM 570 Wandkonsolen  (Paar) L570mm","101975","0",null,"STK",217,{"$f":"IF(M5151=0,\"\",M5151)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF($M$5099=1,0,IF(Daten!$L$549=2,1)+O5151))))","v":0},102,{"$f":"IF(Daten!$L$549=2,#REF!,0)","v":0},null,100]
["ICS5000",6,400,"ICS5000 4006",null,"ICM 820 Wandkonsolen  (Paar) L820mm","101978","0",null,"STK",238,null,null,352]
["ICS5000",8,400,"ICS5000 4008",null,"ICM 1120 Wandkonsolen  (Paar) L1120mm","101980","0",null,"STK",288,{"$f":"IF(M5156=0,\"\",M5156)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF($M$5099=1,0,IF(Daten!$L$549=5,1)+O5156))))","v":0},652,{"$f":"IF(Daten!$L$549=5,N5163,0)","v":0},null,600]
["ICS5000",11,400,"ICS5000 40011",null,"ICM5000 400  Verankerungsplatte mit Ablauf senkr.","102922",95,null,"STK",359,{"$f":"IF(Daten!$L$499=1,1,\"\")","v":1},{"$f":"IF(L5159=\"\",\"0\",L5159*H5159)","v":95},null,null,{"$f":"IF(L5159=\"\",\"0\",H5159*L5159)","v":95}]
["ICS5000",13,400,{"$f":"A5161&\" \"&C5161&B5161","v":"ICS5000 40013"},null,"ICM5000 400 Zwischenstütze","102948",485,null,"STK",329,{"$f":"IF(N5161=0,\"\",N5161)","v":""},{"$f":"IF(L5161=\"\",0,L5161*H5161)","v":0},{"$f":"IF(M5148>=15000,1,0)","v":0},null,{"$f":"IF(L5161=\"\",\"0\",H5161*L5161)","v":"0"}]
["ICS5000",14,400,"ICS5000 40014",null,"ICM5000 400 Kondensattopf","102961","0",null,"STK",320,null,{"$f":"IF(L5162=\"\",\"0\",L5162*H5162)","v":"0"},null,null,"0"]
["ICS5000",18,400,"ICS5000 40018",null,"ICM5000 400 Verschlussdeckel","103013","0",null,"STK",197,null,"0",null,null,"0"]
["ICS5000",20,400,"ICS5000 40020",null,"ICM5000 400 Anschluss von DW auf EW in Rauchgasr.","140765","0",null,"STK",228,null,{"$f":"IF(H5168=\"\",\"\",L5168*H5168)","v":0}]
["ICS5000",23,400,"ICS5000 40023",null,"ICM5000 400 Längenelement L195mm","103063",155,null,"STK",229,null,{"$f":"IF(H5171=\"\",\"\",L5171*H5171)","v":0},null,null,{"$f":"IF(L5171=\"\",\"0\",H5171*L5171)","v":"0"}]
["ICS5000",24,400,"ICS5000 40024",null,"ICM5000 400 Längenelement L250mm","103076",205,null,"STK",216,{"$f":"IF(N5172+O5172=0,\"\",N5172+O5172)","v":""},{"$f":"IF(L5172=\"\",0,L5172*H5172)","v":0},{"$f":"'ICS5000'!$P$20","v":0},{"$f":"IF(Daten!$L$507=2,1,0)","v":0},{"$f":"(IF(L5172=\"\",0,H5172*L5172))-O5172","v":0}]
["ICS5000",28,400,"ICS5000 40028",null,"ICM5000 400 Dichtring Silikon inkl. Gleitmittel","103128","0",null,"STK",16,null,"im Bauteil enthalten",null,null,{"$f":"IF(L5176=\"\",\"0\",H5176*L5176)","v":"0"}]
["ICS5000",29,400,"ICS5000 40029",null,"ICM5000 400 Dichtmanchette für Aussenmantel","103141","0",null,"STK",82,null,"im Bauteil enthalten",null,null,{"$f":"IF(L5177=\"\",\"0\",H5177*L5177)","v":"0"}]
["ICS5000",31,400,"ICS5000 40031",null,"ICM 400 Wandhalter verstellbar 75 - 300mm DN 450mm","102298","0",null,"STK",109,null,null,"75-300",null,{"$f":"IF(L5179=\"\",\"0\",H5179*L5179)","v":"0"}]
["ICS5000",34,400,"ICS5000 40034",null,"ICM L1 Verlängerung zu Wandhalter 50mm L300mm","102319","0",null,"STK",109,null,null,160,null,"0"]
["ICS5000",37,400,"ICS5000 40037",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,{"$f":"IF(Daten!$L$549=5,$L5180,\"\")","v":""},null,610,600,"0"]
["ICS5000",39,400,"ICS5000 40039",null,"ICM 400 Dachdurführung 16-25° DN500 mit Bleilappen","102342","0",null,"STK",704,{"$f":"IF(Daten!$L$522=3,1,\"\")","v":""},null,null,null,"0"]
[{"$f":"A5189","v":"ICS5000"},{"$f":"B5189+1","v":42},{"$f":"C5189","v":400},"ICS5000 40042",null,"ICM 400 Regenkragen DN450","102380","0",null,"STK",98,{"$f":"IF(SUM(L5186:L5189)=0,\"\",SUM(L5186:L5189))","v":""},null,null,null,"0"]
["ICS5000",44,400,"ICS5000 40044",null,"ICM 400 Mündungsabschluss","102440",295,null,"STK",325,{"$f":"IF(Daten!$O$522=1,1,\"\")","v":1},{"$f":"IF(L5192=\"\",\"0\",L5192*H5192)","v":295},null,null,295]
["ICS5000",47,400,"ICS5000 40047",null,"ICM5000 400 Winkel 30°","103214","0",null,"STK",399,{"$f":"IF(N5195=1,\"\",O5195)","v":""},{"$f":"IF(L5195=\"\",0,L5195*H5195)","v":0},{"$f":"Daten!$O$540","v":1},{"$f":"Daten!$P$540","v":"Nein"},{"$f":"IF(L5195=\"\",\"0\",H5195*L5195)","v":"0"}]
["ICS5000",0,450,{"$f":"A5198&\" \"&C5198&B5198","v":"ICS5000 4500"}," ","Schiedel ICS5000 25mm 450","ICS5000 450","0",{"$f":"'ICS5000'!$J$10","v":10},"Anlage",0,1,{"$f":"I5198*1000","v":10000},null,{"$f":"ROUNDUP(P5198,2)","v":10.299999999999999},{"$f":"SUM(P5200:P5247)/1000","v":10.295}]
[{"$f":"A5199","v":"ICS5000"},{"$f":"B5199+1","v":2},{"$f":"C5199","v":450},{"$f":"A5200&\" \"&C5200&B5200","v":"ICS5000 4502"},null,"ICM 475 Wandkonsolen  (Paar) L475mm","101974","0",null,"STK",158]
["ICS5000",3,450,"ICS5000 4503",null,"ICM 570 Wandkonsolen  (Paar) L570mm","101975","0",null,"STK",217]
["ICS5000",7,450,"ICS5000 4507",null,"ICM 1004 Wandkonsolen  (Paar) L1004mm","101979","0",null,"STK",260,{"$f":"IF(M5205=0,\"\",M5205)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M5199=1,0,IF(Daten!$L$549=4,1)+O5205))))","v":0},486,{"$f":"IF(Daten!$L$549=4,N5211,0)","v":0},null,400]
["ICS5000",9,450,"ICS5000 4509",null,"ICM 1304 Wandkonsolen  (Paar) L1304mm","101981","0",null,"STK",315,null,null,786]
["ICS5000",12,450,{"$f":"A5210&\" \"&C5210&B5210","v":"ICS5000 45012"},null,"ICM5000 450  Verankerungsplatte mit Ablauf waagr.","102936",97,null,"STK",448,{"$f":"IF(Daten!$L$499=2,1,\"\")","v":""},{"$f":"IF(L5210=\"\",\"0\",L5210*H5210)","v":"0"},null,null,{"$f":"IF(L5210=\"\",\"0\",H5210*L5210)","v":"0"}]
["ICS5000",15,450,"ICS5000 45015",null,"ICM5000 450 Putztüranschluss rund Überdruck","102975",655,null,"STK",1426,{"$f":"Daten!$P$499","v":1},655,null,null,655]
["ICS5000",17,450,"ICS5000 45017",null,"ICM5000 450 T-Stück 90°","103001",655,null,"STK",1186,{"$f":"IF(Daten!$L$515=2,1,\"\")","v":1},655,null,null,655]
["ICS5000",18,450,"ICS5000 45018",null,"ICM5000 450 Verschlussdeckel","103014","0",null,"STK",301,null,"0",null,null,"0"]
["ICS5000",20,450,"ICS5000 45020",null,"ICM5000 450 Anschluss von DW auf EW in Rauchgasr.","140766","0",null,"STK",255,null,{"$f":"IF(H5218=\"\",\"\",L5218*H5218)","v":0}]
["ICS5000",23,450,"ICS5000 45023",null,"ICM5000 450 Längenelement L195mm","103064",155,null,"STK",233,null,{"$f":"IF(H5221=\"\",\"\",L5221*H5221)","v":0},null,null,{"$f":"IF(L5221=\"\",\"0\",H5221*L5221)","v":"0"}]
["ICS5000",26,450,"ICS5000 45026",null,"ICM5000 450 Längenelement L1000mm","103103",955,null,"STK",427,{"$f":"ROUNDUP(M5224,0)+O5224","v":9},{"$f":"((M5198-SUM(M5209:M5223)-M5242)/H5224)","v":8.6910994764397902},null,{"$f":"IF(Daten!$L$507=4,1,0)","v":0},{"$f":"(IF(L5224=\"\",0,H5224*L5224))-O5224","v":8595}]
["ICS5000",28,450,"ICS5000 45028",null,"ICM5000 450 Dichtring Silikon inkl. Gleitmittel","103129","0",null,"STK",16,null,"im Bauteil enthalten",null,null,{"$f":"IF(L5226=\"\",\"0\",H5226*L5226)","v":"0"}]
["ICS5000",31,450,"ICS5000 45031",null,"ICM 450 Wandhalter verstellbar 75 - 300mm DN 500mm","102299","0",null,"STK",130,null,null,"75-300",null,{"$f":"IF(L5229=\"\",\"0\",H5229*L5229)","v":"0"}]
["ICS5000",33,450,"ICS5000 45033",null,"ICM W1 Verlängerung zu Wandhalter 50mm L 130mm","102317","0",null,"STK",44,{"$f":"IF(Daten!$L$549=2,$L5230,\"\")","v":""},null,100,100,"0"]
["ICS5000",36,450,"ICS5000 45036",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,{"$f":"IF(Daten!$L$549=4,$L5231,\"\")","v":""},null,410,400,"0"]
["ICS5000",37,450,"ICS5000 45037",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,{"$f":"IF(Daten!$L$549=5,$L5230,\"\")","v":""},null,610,600,"0"]
["ICS5000",41,450,"ICS5000 45041",null,"ICM 450 Dachdurführung 36-45° DN550 mit Bleilappen","102367","0",null,"STK",1082,{"$f":"IF(Daten!$L$522=5,1,\"\")","v":""},null,null,null,"0"]
[{"$f":"A5239","v":"ICS5000"},{"$f":"B5239+1","v":42},{"$f":"C5239","v":450},"ICS5000 45042",null,"ICM 450 Regenkragen DN500","102381","0",null,"STK",109,{"$f":"IF(SUM(L5236:L5239)=0,\"\",SUM(L5236:L5239))","v":""},null,null,null,"0"]
["ICS5000",46,450,"ICS5000 45046",null,"ICM5000 450 Element mit Kondensatablauf 1/2\"","103194","0",null,"STK",432,null,{"$f":"IF(L5244=\"\",0,L5244*H5244)","v":0},null,null,{"$f":"IF(L5244=\"\",\"0\",H5244*L5244)","v":"0"}]
["ICS5000",48,450,"ICS5000 45048",null,"ICM5000 450 Winkel 45°","103228","0",null,"STK",437,{"$f":"IF(N5246=1,\"\",O5246)","v":""},{"$f":"IF(L5246=\"\",0,L5246*H5246)","v":0},{"$f":"Daten!$O$548","v":1},{"$f":"Daten!$P$548","v":"Nein"},{"$f":"IF(L5246=\"\",\"0\",H5246*L5246)","v":"0"}]
[{"$f":"A5248","v":"ICS5000"},{"$f":"B5248+1","v":1},{"$f":"C5248","v":500},{"$f":"A5249&\" \"&C5249&B5249","v":"ICS5000 5001"},null,"ICM 500 Konsolenbleche (Paar) ","101965","0",null,"STK",536,{"$f":"N5249","v":1},{"$f":"IF(Daten!$L$549=1,1,\"\")","v":1},{"$f":"IF(Daten!$L$499=1,M5249,\"\")","v":1},null,{"$f":"IF(L5249=\"\",\"0\",H5249*L5249)","v":0}]
["ICS5000",4,500,"ICS5000 5004",null,"ICM 620 Wandkonsolen  (Paar) L620mm","101976","0",null,"STK",223]
["ICS5000",6,500,"ICS5000 5006",null,"ICM 820 Wandkonsolen  (Paar) L820mm","101978","0",null,"STK",238,{"$f":"IF(M5254=0,\"\",M5254)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF($M$5043=1,0,IF(Daten!$L$549=3,1)+O5254))))","v":0},252,{"$f":"IF(Daten!$L$549=3,N5261,0)","v":0},null,250]
["ICS5000",7,500,"ICS5000 5007",null,"ICM 1004 Wandkonsolen  (Paar) L1004mm","101979","0",null,"STK",260,{"$f":"IF(M5255=0,\"\",M5255)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF(M5249=1,0,IF(Daten!$L$549=4,1)+O5255))))","v":0},436,{"$f":"IF(Daten!$L$549=4,N5261,0)","v":0},null,400]
["ICS5000",9,500,"ICS5000 5009",null,"ICM 1304 Wandkonsolen  (Paar) L1304mm","101981","0",null,"STK",315,{"$f":"IF(M5257=0,\"\",M5257)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF($M$5099=1,0,IF(Daten!$L$549=5,1)+O5257))))","v":0},736,{"$f":"IF(Daten!$L$549=5,N5264,0)","v":0},null,600]
["ICS5000",12,500,{"$f":"A5260&\" \"&C5260&B5260","v":"ICS5000 50012"},null,"ICM5000 500  Verankerungsplatte mit Ablauf waagr.","102937",97,null,"STK",557,{"$f":"IF(Daten!$L$499=2,1,\"\")","v":""},{"$f":"IF(L5260=\"\",\"0\",L5260*H5260)","v":"0"},null,null,{"$f":"IF(L5260=\"\",\"0\",H5260*L5260)","v":"0"}]
["ICS5000",15,500,"ICS5000 50015",null,"ICM5000 500 Putztüranschluss rund Überdruck","102976",705,null,"STK",1648,{"$f":"Daten!$P$499","v":1},705,null,null,705]
["ICS5000",17,500,"ICS5000 50017",null,"ICM5000 500 T-Stück 90°","103002",705,null,"STK",1367,{"$f":"IF(Daten!$L$515=2,1,\"\")","v":1},705,null,null,705]
[{"$f":"A5268","v":"ICS5000"},{"$f":"B5268+1","v":21},{"$f":"C5268","v":500},{"$f":"A5269&\" \"&C5269&B5269","v":"ICS5000 50021"},null,"ICM5000 500 Flansch zum Anschweissen im Auftrag","103052","0",null,"STK",214,null,{"$f":"IF(H5269=\"\",\"\",L5269*H5269)","v":0}]
["ICS5000",22,500,"ICS5000 50022",null,"ICM5000 500 Längenelement L195mm","103065",155,null,"STK",245,null,{"$f":"IF(H5270=\"\",\"\",L5270*H5270)","v":0},null,null,{"$f":"IF(L5270=\"\",\"0\",H5270*L5270)","v":"0"}]
["ICS5000",26,500,"ICS5000 50026",null,"ICM5000 500 Schiebeelement L375 - 585mm","103117","0",null,"STK",527,null,null,null,null,{"$f":"IF(L5274=\"\",\"0\",H5274*L5274)","v":"0"}]
["ICS5000",27,500,"ICS5000 50027",null,"ICM5000 500 Dichtring Silikon inkl. Gleitmittel","103130","0",null,"STK",17,null,"im Bauteil enthalten",null,null,{"$f":"IF(L5275=\"\",\"0\",H5275*L5275)","v":"0"}]
["ICS5000",30,500,"ICS5000 50030",null,"ICM 500 Wandhalter verstellbar 75 - 300mm DN 550mm","102300","0",null,"STK",163,null,null,"75-300",null,{"$f":"IF(L5278=\"\",\"0\",H5278*L5278)","v":"0"}]
["ICS5000",31,500,"ICS5000 50031",null,"ICM 500 Wandhalter 50mm verlängerbar DN 550mm ","102314","0",null,"STK",174,{"$f":"ROUNDUP(M5279,0)","v":3},{"$f":"((M5248/1000)/4.3)","v":2.3255813953488373},null,null,0]
["ICS5000",35,500,"ICS5000 50035",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,{"$f":"IF(Daten!$L$549=4,$L5280,\"\")","v":""},null,410,400,"0"]
["ICS5000",37,500,"ICS5000 50037",null,"ICM 500 Dachdurführung 0° DN600 L500mm","102332","0",null,"STK",812,{"$f":"IF(Daten!$L$522=2,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",40,500,"ICS5000 50040",null,"ICM 500 Dachdurführung 36-45° DN600 mit Bleilappen","102368","0",null,"STK",1245,{"$f":"IF(Daten!$L$522=5,1,\"\")","v":""},null,null,null,"0"]
["ICS5000",43,500,"ICS5000 50043",null,"ICM 500 Mündungsabschluss","102442",295,null,"STK",509,{"$f":"IF(Daten!$O$522=1,1,\"\")","v":1},{"$f":"IF(L5291=\"\",\"0\",L5291*H5291)","v":295},null,null,295]
["ICS5000",45,500,"ICS5000 50045",null,"ICM5000 500 Element mit Kondensatablauf 1/2\"","103195","0",null,"STK",469,null,{"$f":"IF(L5293=\"\",0,L5293*H5293)","v":0},null,null,{"$f":"IF(L5293=\"\",\"0\",H5293*L5293)","v":"0"}]
["ICS5000",46,500,"ICS5000 50046",null,"ICM5000 500 Winkel 30°","103216","0",null,"STK",479,{"$f":"IF(N5294=1,\"\",O5294)","v":""},{"$f":"IF(L5294=\"\",0,L5294*H5294)","v":0},{"$f":"Daten!$O$540","v":1},{"$f":"Daten!$P$540","v":"Nein"},{"$f":"IF(L5294=\"\",\"0\",H5294*L5294)","v":"0"}]
[{"$f":"A5297","v":"ICS5000"},{"$f":"B5297+1","v":1},{"$f":"C5297","v":600},{"$f":"A5298&\" \"&C5298&B5298","v":"ICS5000 6001"},null,"ICM 600 Konsolenbleche (Paar)","101966","0",null,"STK",623,{"$f":"N5298","v":1},{"$f":"IF(Daten!$L$549=1,1,\"\")","v":1},{"$f":"IF(Daten!$L$499=1,M5298,\"\")","v":1},null,{"$f":"IF(L5298=\"\",\"0\",H5298*L5298)","v":0}]
[{"$f":"A5298","v":"ICS5000"},{"$f":"B5298+1","v":2},{"$f":"C5298","v":600},{"$f":"A5299&\" \"&C5299&B5299","v":"ICS5000 6002"},null,"ICM 475 Wandkonsolen  (Paar) L475mm","101974","0",null,"STK",158]
["ICS5000",5,600,"ICS5000 6005",null,"ICM 720 Wandkonsolen  (Paar) L720mm","101977","0",null,"STK",228]
["ICS5000",7,600,"ICS5000 6007",null,"ICM 1004 Wandkonsolen  (Paar) L1004mm","101979","0",null,"STK",260,{"$f":"IF(M5304=0,\"\",M5304)","v":""},{"$f":"IF(Daten!$L$499=2,\"\",IF(Daten!$L$499=3,\"\",IF(Daten!$L$499=4,\"\",IF($M$5043=1,0,IF(Daten!$L$549=3,1)+O5304))))","v":0},336,{"$f":"IF(Daten!$L$549=3,N5311,0)","v":0},null,250]
["ICS5000",11,600,"ICS5000 60011",null,"ICM5000 600  Verankerungsplatte mit Ablauf senkr.","102925",95,null,"STK",551,{"$f":"IF(Daten!$L$499=1,1,\"\")","v":1},{"$f":"IF(L5308=\"\",\"0\",L5308*H5308)","v":95},null,null,{"$f":"IF(L5308=\"\",\"0\",H5308*L5308)","v":95}]
["ICS5000",12,600,{"$f":"A5309&\" \"&C5309&B5309","v":"ICS5000 60012"},null,"ICM5000 600  Verankerungsplatte mit Ablauf waagr.","102938",97,null,"STK",692,{"$f":"IF(Daten!$L$499=2,1,\"\")","v":""},{"$f":"IF(L5309=\"\",\"0\",L5309*H5309)","v":"0"},null,null,{"$f":"IF(L5309=\"\",\"0\",H5309*L5309)","v":"0"}]
["ICS5000",16,600,"ICS5000 60016",null,"ICM5000 600 T-Stück 45°","102990",1100,null,"STK",2253,{"$f":"IF(Daten!$L$515=1,1,\"\")","v":""},"0",null,null,"0"]
["ICS5000",17,600,"ICS5000 60017",null,"ICM5000 600 T-Stück 90°","103003",805,null,"STK",1906,{"$f":"IF(Daten!$L$515=2,1,\"\")","v":1},805,null,null,805]
["ICS5000",20,600,"ICS5000 60020",null,"ICM5000 600 Anschluss von DW auf EW in Rauchgasr.","140768","0",null,"STK",299,null,{"$f":"IF(H5317=\"\",\"\",L5317*H5317)","v":0}]
["ICS5000",22,600,"ICS5000 60022",null,"ICM5000 600 Längenelement L195mm","103066",155,null,"STK",265,null,{"$f":"IF(H5319=\"\",\"\",L5319*H5319)","v":0},null,null,{"$f":"IF(L5319=\"\",\"0\",H5319*L5319)","v":"0"}]
["ICS5000",25,600,"ICS5000 60025",null,"ICM5000 600 Längenelement L1000mm","103105",955,null,"STK",518,{"$f":"ROUNDUP(M5322,0)+O5322","v":9},{"$f":"((M5297-SUM(M5308:M5321)-M5340)/H5322)","v":8.3769633507853403},null,{"$f":"IF(Daten!$L$507=4,1,0)","v":0},{"$f":"(IF(L5322=\"\",0,H5322*L5322))-O5322","v":8595}]
["ICS5000",27,600,"ICS5000 60027",null,"ICM5000 600 Dichtring Silikon inkl. Gleitmittel","103131","0",null,"STK",18,null,"im Bauteil enthalten",null,null,{"$f":"IF(L5324=\"\",\"0\",H5324*L5324)","v":"0"}]
["ICS5000",30,600,"ICS5000 60030",null,"ICM 600 Wandhalter verstellbar 75 - 300mm DN 650mm","102301","0",null,"STK",217,null,null,"75-300",null,{"$f":"IF(L5327=\"\",\"0\",H5327*L5327)","v":"0"}]
["ICS5000",33,600,"ICS5000 60033",null,"ICM L1 Verlängerung zu Wandhalter 50mm L300mm","102319","0",null,"STK",109,null,null,160,null,"0"]
["ICS5000",35,600,"ICS5000 60035",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,{"$f":"IF(Daten!$L$549=4,$L5329,\"\")","v":""},null,410,400,"0"]
["ICS5000",36,600,"ICS5000 60036",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,{"$f":"IF(Daten!$L$549=5,$L5328,\"\")","v":""},null,610,600,"0"]
["ICS5000",40,600,"ICS5000 60040",null,"ICM 600 Dachdurführung 36-45° DN700 mit Bleilappen","102369","0",null,"STK",1461,{"$f":"IF(Daten!$L$522=5,1,\"\")","v":""},null,null,null,"0"]
[{"$f":"A5337","v":"ICS5000"},{"$f":"B5337+1","v":41},{"$f":"C5337","v":600},"ICS5000 60041",null,"ICM 600 Regenkragen DN650","102383","0",null,"STK",152,{"$f":"IF(SUM(L5334:L5337)=0,\"\",SUM(L5334:L5337))","v":""},null,null,null,"0"]
["ICS5000",44,600,"ICS5000 60044",null,"ICM5000 600 Mündungsabschluss horizontal","103183","0",null,"STK",351,{"$f":"IF(Daten!$O$522=3,1,\"\")","v":""},{"$f":"IF(L5341=\"\",\"0\",L5341*H5341)","v":"0"},null,null,{"$f":"IF(L5341=\"\",\"0\",H5341*L5341)","v":"0"}]
["ICS5000",46,600,"ICS5000 60046",null,"ICM5000 600 Winkel 30°","103217","0",null,"STK",545,{"$f":"IF(N5343=1,\"\",O5343)","v":""},{"$f":"IF(L5343=\"\",0,L5343*H5343)","v":0},{"$f":"Daten!$O$540","v":1},{"$f":"Daten!$P$540","v":"Nein"},{"$f":"IF(L5343=\"\",\"0\",H5343*L5343)","v":"0"}]
[{"$f":"A5346","v":"Prima Plus"},{"$f":"B5346+1","v":1},{"$f":"C5346","v":80},{"$f":"A5347&\" \"&C5347&B5347","v":"Prima Plus 801"},null,"PPL 80 Kaminfuss 45° m.Stütze L195mm","100578","0",null,"STK",129,{"$f":"IF(Daten!$B$662=4,1,\"\")","v":""},{"$f":"IF(L5347=\"\",0,L5347*H5347)","v":0},null,null,{"$f":"IF(L5347=\"\",0,H5347*L5347)","v":0}]
["Prima Plus",2,80,{"$f":"A5348&\" \"&C5348&B5348","v":"Prima Plus 802"},null,"PPL 80 Lang-Bogen 45° L205mm","100586","0",null,"STK",76,null,0,null,null,{"$f":"IF(L5348=\"\",0,H5348*L5348)","v":0}]
["Prima Plus",4,80,"Prima Plus 804",null,"PPL 80-130 Konsolenbleche für Zwischenstütze(Paar)","100608","0",null,"STK",108,null,0]
["Prima Plus",7,80,"Prima Plus 807",null,"PPL 80 Revisions.-und Anschluss-Basiselement DN80 ","100698",283,null,"STK",76,{"$f":"Daten!$C$654","v":1},283,null,null,{"$f":"IF(L5353=\"\",0,H5353*L5353)","v":283}]
["Prima Plus",9,80,"Prima Plus 809",null,"PPL 80 Revisionsdeckel für Festbrennstoffe","100737","0",null,"STK",54,{"$f":"IF(Daten!$B$644=1,Daten!$C$654,\"\")","v":1},0]
["Prima Plus",12,80,"Prima Plus 8012",null,"PPL 80-130 Montagerahmen L150mm","100786","0",null,"STK",64,{"$f":"IF(L5357=\"\",\"\",L5357)","v":""},0,null,null,{"$f":"IF(L5358=\"\",0,H5358*L5358)","v":0}]
["Prima Plus",15,80,"Prima Plus 8015",null,"PPL 80 T-Stück 85° L 283mm","100794",283,null,"STK",76,null,{"$f":"IF(L5361=\"\",0,L5361*H5361)","v":0},null,null,{"$f":"IF(L5361=\"\",0,H5361*L5361)","v":0}]
["Prima Plus",17,80,"Prima Plus 8017",null,"PPL 80 T-Stück 90° mit Putztüre Festbrennstoff","100816",283,null,"STK",119,null,0,null,null,0]
["Prima Plus",20,80,"Prima Plus 8020",null,"PPL 80 Längenelement L250mm","100846",200,null,"STK",22,{"$f":"IF(N5366=0,\"\",N5366)","v":""},0,{"$f":"IF('PRIMA PLUS'!$P$18=\"\",0,IF('PRIMA PLUS'!$P$18=0,0,'PRIMA PLUS'!$P$18))","v":0},null,0]
["Prima Plus",23,80,{"$f":"A5369&\" \"&C5369&B5369","v":"Prima Plus 8023"},null,"PPL 80 Element mit 3 Messöffnungen 3/4\" L150mm","100902","0",null,"STK",86,null,{"$f":"IF(L5369=\"\",0,L5369*H5369)","v":0},null,null,0]
["Prima Plus",25,80,"Prima Plus 8025",null,"PPL 80 Ablass-Element L200mm","100888",200,null,"STK",54,1,{"$f":"IF(L5371=\"\",0,L5371*H5371)","v":200},null,null,200]
["Prima Plus",26,80,"Prima Plus 8026",null,"PPL 80 Abstandhalter","100916","0",null,"STK",0,{"$f":"IF(N5372=0,\"\",ROUNDUP(N5372,0))","v":3},null,{"$f":"P5346/5","v":2.1572}]
["Prima Plus",30,80,"Prima Plus 8030",null,"PPL 80 Kondensatabscheider L150mm","100960","0",null,"STK",108,null,null,null,null,{"$f":"IF(L5376=\"\",0,H5376*L5376)","v":0}]
["Prima Plus",32,80,"Prima Plus 8032",null,"PPL 80 Dichtung Viton","100989","0",null,"STK",12,{"$f":"IF(N5378=\"\",\"\",N5378)","v":""},null,{"$f":"IF(Daten!$B$644=1,\"\",O5378)","v":""},{"$f":"SUM(L5347,L5349,L5353,L5362,L5364,L5366,L5367,L5368,L5371)","v":15}]
["Prima Plus",35,80,"Prima Plus 8035",null,"PPL 80 Winkel 45°","101031","0",null,"STK",44]
["Prima Plus",36,80,"Prima Plus 8036",null,"PPL 80 Winkel 85°","101045","0",null,"STK",55]
["Prima Plus",40,80,"Prima Plus 8040",null,"PPL 80 Kesselanschluss DN + 6mm L150mm","101107","0",null,"STK",43]
["Prima Plus",41,80,"Prima Plus 8041",null,"PPL 80 Erweiterung auf DN100mm L150mm","101116","0",null,"STK",86]
["Prima Plus",43,80,"Prima Plus 8043",null,"PPL 80 Abgasschalldämpfer Schallred. 15DB L580mm","101156","0",null,"STK",799]
["Prima Plus",46,80,{"$f":"A5392&\" \"&C5392&B5392","v":"Prima Plus 8046"},null,"ICM 80 Anschluss von EW auf DW in Rauchgasr.","102146","0",null,"STK",87]
["Prima Plus",48,80,"Prima Plus 8048",null,"PPL 80 Anschlussrosette ØA 250mm","101183","0",null,"STK",27]
["Prima Plus",51,80,"Prima Plus 8051",null,"ICM L1 Verlängerung zu Wandhalter 50mm L300mm","102319","0",null,"STK",109]
["Prima Plus",54,80,"Prima Plus 8054",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195]
["Prima Plus",56,80,"Prima Plus 8056",null,"PPL 80 Rohrschelle  Anschluss 1/2\" Aussengewinde","101193","0",null,"STK",20]
["Prima Plus",59,80,"Prima Plus 8059",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25]
["Prima Plus",62,80,"Prima Plus 8062",null,"PPL 80 Mündungskonus zu Schachtabdeckung","101276","0",null,"STK",54,{"$f":"IF(Daten!$E$677=1,1,\"\")","v":1}]
["Prima Plus",64,80,"Prima Plus 8064",null,"PPL 80 Mündungsmanchette L130mm 350 x 350mm","101284","0",null,"STK",86,{"$f":"IF(Daten!$E$677=2,1,\"\")","v":""}]
["Prima Plus",65,80,"Prima Plus 8065",null,"PPL 80 Dämmrohr 20mm Steinwolle L1000mm","101315","0",null,"STK",13]
["Prima Plus",69,80,{"$f":"A5415&\" \"&C5415&B5415","v":"Prima Plus 8069"},null,"CHI 80 Adapter Flex zu Flex","101365","0",null,"STK",52,null,null,null,null,{"$f":"IF(L5415=\"\",0,H5415*L5415)","v":0}]
["Prima Plus",71,80,"Prima Plus 8071",null,"CHI 80 CHI Flexrohr 2 lagig Rolle a 50000mm","101378",50000,null,"STK",2310]
["Prima Plus",74,80,"Prima Plus 8074",null,"CHZ Mantelstein EZ  280 x 280mm L330mm","103718","0",null,"STK",24]
["Prima Plus",75,80,"Prima Plus 8075",null,"CHZ Mantelstein EZ  320 x 320mm L330mm Ø160mm","103719","0",null,"STK",19]
[{"$f":"A5424","v":"Prima Plus"},{"$f":"B5424+1","v":79},{"$f":"C5424","v":80},{"$f":"A5425&\" \"&C5425&B5425","v":"Prima Plus 8079"},null,"LBS 150 Leichtbauschacht NWi150mm NWA240mm L1000mm","140813","0",null,"STK",{"$f":"VLOOKUP(G5425,sanschie!A:G,7,0)","v":113}]
["Prima Plus",80,80,{"$f":"A5426&\" \"&C5426&B5426","v":"Prima Plus 8080"},null,"LBS Kleber zu Leichtbauschacht 1kg","103829","0",null,"STK",9]
[{"$f":"A5427","v":"Prima Plus"},{"$f":"B5427+1","v":82},{"$f":"C5427","v":80},{"$f":"A5428&\" \"&C5428&B5428","v":"Prima Plus 8082"},null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",81]
["Prima Plus",2,100,"Prima Plus 1002",null,"PPL 100 Lang-Bogen 45° L201mm","100587","0",null,"STK",86,null,0,null,null,{"$f":"IF(L5431=\"\",0,H5431*L5431)","v":0}]
["Prima Plus",5,100,"Prima Plus 1005",null,"PPL 80-130 Konsolenbleche für Zwischenstütze(Paar)","100608","0",null,"STK",108,null,0]
["Prima Plus",7,100,"Prima Plus 1007",null,"PPL 100 Kondensattopf mit Ablauf senkrecht","100635",48,null,"STK",43,null,0,null,null,{"$f":"IF(L5436=\"\",0,H5436*L5436)","v":0}]
["Prima Plus",10,100,"Prima Plus 10010",null,"PPL 100 Revisions-und Anschluss-Basiselement DN100","100699",283,null,"STK",86,{"$f":"Daten!$C$654","v":1},283,null,null,{"$f":"IF(L5439=\"\",0,H5439*L5439)","v":283}]
["Prima Plus",12,100,"Prima Plus 10012",null,"PPL 100 Revisionsdeckel für Festbrennstoffe","100738","0",null,"STK",59,{"$f":"IF(Daten!$B$644=1,Daten!$C$654,\"\")","v":1},0]
["Prima Plus",15,100,"Prima Plus 10015",null,"PPL 80-130 Montagerahmen L150mm","100786","0",null,"STK",64,{"$f":"IF(L5443=\"\",\"\",L5443)","v":""},0,null,null,{"$f":"IF(L5444=\"\",0,H5444*L5444)","v":0}]
["Prima Plus",18,100,"Prima Plus 10018",null,"PPL 100 T-Stück 85° L 283mm","100795",283,null,"STK",86,null,{"$f":"IF(L5447=\"\",0,L5447*H5447)","v":0},null,null,{"$f":"IF(L5447=\"\",0,H5447*L5447)","v":0}]
["Prima Plus",20,100,"Prima Plus 10020",null,"PPL 100 T-Stück 90° mit Putztüre Festbrennstoff","100817",283,null,"STK",129,null,0,null,null,0]
["Prima Plus",21,100,"Prima Plus 10021",null,"PPL 100 T-Stück 45° L283mm","100825",283,null,"STK",151,{"$f":"IF(Daten!$B$662=3,1,\"\")","v":""},0,null,null,0]
["Prima Plus",25,100,"Prima Plus 10025",null,"PPL 100 Längenelement L1000mm","100875",950,null,"STK",60,{"$f":"ROUNDUP(M5454,0)","v":10},{"$f":"(M5429-(SUM(M5430:M5453))-(SUM(M5455:M5461)))/H5454","v":9.1726315789473691},null,null,9500]
["Prima Plus",27,100,{"$f":"A5456&\" \"&C5456&B5456","v":"Prima Plus 10027"},null,"PPL 100 Element mit 3 Messöffnungen 3/4\" L150mm","100903","0",null,"STK",97,null,{"$f":"IF(L5456=\"\",0,L5456*H5456)","v":0},null,null,0]
["Prima Plus",30,100,"Prima Plus 10030",null,"PPL 100 Schiebe-Element 270-415mm","100925","0",null,"STK",64,null,{"$f":"IF(L5459=\"\",0,L5459*H5459)","v":0}]
["Prima Plus",33,100,"Prima Plus 10033",null,"PPL 100 Kondensatabscheider L150mm","100961","0",null,"STK",114,null,null,null,null,{"$f":"IF(L5462=\"\",0,H5462*L5462)","v":0}]
["Prima Plus",35,100,{"$f":"A5464&\" \"&C5464&B5464","v":"Prima Plus 10035"},null,"PPL 100 Dichtung Viton","100990","0",null,"STK",13,{"$f":"IF(N5464=\"\",\"\",N5464)","v":""},null,{"$f":"IF(Daten!$B$644=1,\"\",O5464)","v":""},{"$f":"SUM(L5430,L5433,L5439,L5448,L5450,L5452,L5453,L5454,L5455)","v":15}]
["Prima Plus",36,100,{"$f":"A5465&\" \"&C5465&B5465","v":"Prima Plus 10036"},null,"PPL 100 Winkel 15°","101004","0",null,"STK",44]
["Prima Plus",38,100,"Prima Plus 10038",null,"PPL 100 Winkel 45°","101032","0",null,"STK",50]
["Prima Plus",41,100,"Prima Plus 10041",null,"PPL 100 Winkel 85° mit Revisionsöffnung","101074","0",null,"STK",129]
["Prima Plus",44,100,"Prima Plus 10044",null,"PPL 100 Erweiterung DN130 L150mm","101119","0",null,"STK",97]
["Prima Plus",46,100,"Prima Plus 10046",null,"PPL 150 Reduktion  DN100 L150mm","101141","0",null,"STK",97]
["Prima Plus",49,100,"Prima Plus 10049",null,"PPL 100 Schallabsorber Oel-Gas","101169","0",null,"STK",129]
["Prima Plus",51,100,{"$f":"A5480&\" \"&C5480&B5480","v":"Prima Plus 10051"},null,"ICM 100 Anschluss von EW auf DW in Rauchgasr.","102147","0",null,"STK",98]
["Prima Plus",55,100,"Prima Plus 10055",null,"ICM W1 Verlängerung zu Wandhalter 50mm L 130mm","102317","0",null,"STK",44]
["Prima Plus",56,100,"Prima Plus 10056",null,"ICM L1 Verlängerung zu Wandhalter 50mm L300mm","102319","0",null,"STK",109]
["Prima Plus",59,100,"Prima Plus 10059",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195]
["Prima Plus",60,100,"Prima Plus 10060",null,"ICS 100 Wandhalter verstellbar 75 - 300mm DN150mm","101219","0",null,"STK",58.71]
["Prima Plus",64,100,"Prima Plus 10064",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25]
["Prima Plus",66,100,"Prima Plus 10066",null,"PPL Schachtabdeckung Typ1 350 x 350mm","101272","0",null,"STK",86,{"$f":"IF(L5496=1,1,\"\")","v":1}]
["Prima Plus",69,100,"Prima Plus 10069",null,"PPL 100 Basten Standard passend zu Münd. Manchette","101293","0",null,"STK",220]
["Prima Plus",72,100,"Prima Plus 10072",null,"PPL 100 Dämmrohr 20mm Steinwolle L1000mm","101316","0",null,"STK",14]
["Prima Plus",74,100,"Prima Plus 10074",null,"PPL Stopf-Steinwolle  Sack 10kg","101349","0",null,"STK",50]
["Prima Plus",75,100,"Prima Plus 10075",null,"CHI 100 Adapter PPL zu Flex","101352","0",null,"STK",52,null,null,null,null,{"$f":"IF(L5504=\"\",0,H5504*L5504)","v":0}]
["Prima Plus",77,100,"Prima Plus 10077",null,"CHI 100 Adapter Flex zu Flex","101366","0",null,"STK",56,null,null,null,null,{"$f":"IF(L5506=\"\",0,H5506*L5506)","v":0}]
["Prima Plus",80,100,"Prima Plus 10080",null,"CHI 100 Aufhängeschelle zu Flex","101387","0",null,"STK",27]
["Prima Plus",83,100,"Prima Plus 10083",null,"CHZ Mantelstein EZ  320 x 320mm L330mm Ø160mm","103719","0",null,"STK",19]
["Prima Plus",85,100,"Prima Plus 10085",null,"CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",53]
["Prima Plus",89,100,"Prima Plus 10089",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",81]
["Prima Plus",0,130,"Prima Plus 1300"," ","Schiedel Prima Plus 0,6mm Ø 130","PRIMA PLUS 130","0",{"$f":"'PRIMA PLUS'!$J$11","v":10},"Anlage",0,1,{"$f":"I5519*1000","v":10000},null,{"$f":"ROUNDUP(P5519,2)","v":10.79},{"$f":"SUM(P5520:P5611)/1000","v":10.786}]
["Prima Plus",4,130,"Prima Plus 1304",null,"PPL 130 Kondensattopf mit Ablauf seitlich","100596",70,null,"STK",{"$f":"VLOOKUP(G5523,sanschie!A:G,7,0)","v":81},{"$f":"IF(L5520=1,\"\",IF(L5520=1,\"\",1))","v":1},70,null,null,{"$f":"IF(L5523=\"\",0,H5523*L5523)","v":70},null,null,null,"100596"]
["Prima Plus",5,130,"Prima Plus 1305",null,"PPL 80-130 Konsolenbleche für Zwischenstütze(Paar)","100608","0",null,"STK",108,null,0,null,null,null,null,null,null,"100608"]
["Prima Plus",8,130,"Prima Plus 1308",null,"PPL 130 EW-DW Deckenanfängerset komplett L270mm","100649","0",null,"STK",379,null,0,null,null,0,null,null,null,"100649"]
["Prima Plus",9,130,"Prima Plus 1309",null,"PPL 130 EW-DW Deckenanfängerset 45° kompl. L270mm","100656","0",null,"STK",487,null,0,null,null,0,null,null,null,"100656"]
["Prima Plus",13,130,"Prima Plus 13013",null,"PPL 130 Revisionsdeckel für Oel/Gas ","100731","0",null,"STK",43,{"$f":"IF(Daten!$B$644=2,Daten!$C$654,\"\")","v":""},0,null,null,null,null,null,null,"100731"]
["Prima Plus",15,130,"Prima Plus 13015",null,"PPL 130 Verschlussdeckel mit Griff","100747","0",null,"STK",54,null,0,null,null,null,null,null,null,"100747"]
["Prima Plus",18,130,"Prima Plus 13018",null,"PPL 130 Basiselement-Adapter für Zugbegrenzer","100766","0",null,"STK",73,null,0,null,null,0,null,null,null,"100766"]
["Prima Plus",21,130,"Prima Plus 13021",null,"PPL 80-130 Montagerahmen L150mm","100786","0",null,"STK",64,{"$f":"IF(L5539=\"\",\"\",L5539)","v":""},0,null,null,0,null,null,null,"100786"]
["Prima Plus",23,130,"Prima Plus 13023",null,"PPL 80-130 Zuluft-Türe 140 x 200mm","100791","0",null,"STK",97,null,0,null,null,null,null,null,null,"100791"]
["Prima Plus",24,130,"Prima Plus 13024",null,"PPL 130 T-Stück 85° L 283mm","100796",283,null,"STK",97,null,{"$f":"IF(L5543=\"\",0,L5543*H5543)","v":0},null,null,{"$f":"IF(L5543=\"\",0,H5543*L5543)","v":0},null,null,null,"100796"]
["Prima Plus",28,130,"Prima Plus 13028",null,"PPL 130 Doppelfutterrohr zu T-Stück L120mm","100840","0",null,"STK",59,null,0,null,null,0,null,null,null,"100840"]
["Prima Plus",29,130,"Prima Plus 13029",null,"PPL 130 Längenelement L250mm","100848",200,null,"STK",28,{"$f":"IF(N5548=0,\"\",N5548)","v":""},0,{"$f":"IF('PRIMA PLUS'!$P$18=\"\",0,IF('PRIMA PLUS'!$P$18=0,0,'PRIMA PLUS'!$P$18))","v":0},null,0,null,null,null,"100848"]
["Prima Plus",32,130,"Prima Plus 13032",null,"PPL 130 Ablass-Element L200mm","100890",200,null,"STK",59,1,{"$f":"IF(L5551=\"\",0,L5551*H5551)","v":200},null,null,200,null,null,null,"100890"]
["Prima Plus",34,130,{"$f":"A5553&\" \"&C5553&B5553","v":"Prima Plus 13034"},null,"PPL 130 Empa Messtutzen L450mm","140744","0",null,"STK",250,null,{"$f":"IF(L5553=\"\",0,L5553*H5553)","v":0},null,null,0,null,null,null,"140744"]
["Prima Plus",38,130,"Prima Plus 13038",null,"PPL 130 Endrohr mit beidseitiger Muffe L1000mm","100940",950,null,"STK",76,null,{"$f":"IF(L5557=\"\",0,L5557*H5557)","v":0},null,null,{"$f":"IF(L5557=\"\",0,H5557*L5557)","v":0},null,null,null,"100940"]
["Prima Plus",39,130,"Prima Plus 13039",null,"PPL 130 Revisions-Basiselement mit Kondensatfalle ","100954",283,null,"STK",129,null,{"$f":"IF(L5558=\"\",0,L5558*H5558)","v":0},null,null,{"$f":"IF(L5558=\"\",0,H5558*L5558)","v":0},null,null,null,"100954"]
["Prima Plus",43,130,"Prima Plus 13043",null,"PPL 130 Dichtung Viton","100991","0",null,"STK",15,{"$f":"IF(N5562=\"\",\"\",N5562)","v":""},null,{"$f":"IF(Daten!$B$644=1,\"\",O5562)","v":""},{"$f":"SUM(L5520,L5523,L5529,L5544,L5546,L5548,L5549,L5550,L5551)","v":15},null,null,null,null,"100991"]
["Prima Plus",44,130,"Prima Plus 13044",null,"PPL 130 Winkel 15°","101005","0",null,"STK",50,null,null,null,null,null,null,null,null,"101005"]
["Prima Plus",46,130,"Prima Plus 13046",null,"PPL 130 Winkel 45°","101033","0",null,"STK",55,null,null,null,null,null,null,null,null,"101033"]
["Prima Plus",49,130,"Prima Plus 13049",null,"PPL 130 Winkel 85° mit Revisionsöffnung","101075","0",null,"STK",151,null,null,null,null,null,null,null,null,"101075"]
["Prima Plus",52,130,"Prima Plus 13052",null,"PPL 130 Winkel 0-90° verstellbar  Trockenbetrieb  ","101095","0",null,"STK",54,null,null,null,null,null,null,null,null,"101095"]
["Prima Plus",54,130,"Prima Plus 13054",null,"PPL 130 Kesselanschluss DN + 6mm L150mm","101109","0",null,"STK",54,null,null,null,null,null,null,null,null,"101109"]
["Prima Plus",57,130,"Prima Plus 13057",null,"PPL 120 Erweiterung DN130 L150mm","101121","0",null,"STK",97,null,null,null,null,null,null,null,null,"101121"]
["Prima Plus",60,130,"Prima Plus 13060",null,"PPL 130 Abgasschalldämpfer Schallred. 15DB L580mm","101158","0",null,"STK",999,null,null,null,null,null,null,null,null,"101158"]
["Prima Plus",62,130,"Prima Plus 13062",null,"PPL 130 Schallabsorber Oel-Gas","101170","0",null,"STK",141,null,null,null,null,null,null,null,null,"101170"]
["Prima Plus",63,130,"Prima Plus 13063",null,"PPL 130 Schallabsorber Festbrennstoffe","101177","0",null,"STK",108,null,null,null,null,null,null,null,null,"101177"]
["Prima Plus",67,130,"Prima Plus 13067",null,"ICM 80 Wandhalter 50mm verlängerbar DN 130mm ","102303","0",null,"STK",33,null,null,null,null,null,null,null,null,"102303"]
["Prima Plus",69,130,"Prima Plus 13069",null,"ICM L1 Verlängerung zu Wandhalter 50mm L300mm","102319","0",null,"STK",109,null,null,null,null,null,null,null,null,"102319"]
["Prima Plus",72,130,"Prima Plus 13072",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,null,null,null,null,null,null,null,null,"102322"]
["Prima Plus",73,130,"Prima Plus 13073",null,"ICM 80 Wandhalter verstellbar 75 - 300mm DN 130mm","102289","0",null,"STK",55,null,null,null,null,null,null,null,null,"102289"]
["Prima Plus",77,130,"Prima Plus 13077",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25,null,null,null,null,null,null,null,null,"101206"]
["Prima Plus",78,130,"Prima Plus 13078",null,"PPL 130 Regenkragen ","101260","0",null,"STK",43,null,null,null,null,null,null,null,null,"101260"]
[{"$f":"A5598","v":"Prima Plus"},{"$f":"B5598+1","v":80},{"$f":"C5598","v":130},"Prima Plus 13080",null,"PPL 130 Mündungskonus zu Schachtabdeckung","101278","0",null,"STK",64,{"$f":"IF(Daten!$E$677=1,1,\"\")","v":1},null,null,null,null,null,null,null,"101278"]
["Prima Plus",83,130,"Prima Plus 13083",null,"PPL 130 Basten Standard mit Dila zu Dämmrohr 30mm","101301","0",null,"STK",356,null,null,null,null,null,null,null,null,"101301"]
["Prima Plus",85,130,{"$f":"A5604&\" \"&C5604&B5604","v":"Prima Plus 13085"},null,"PPL 130 Dämmschale 30mm Alu-Kaschiert L1000mm","101324","0",null,"STK",36,{"$f":"IF(Daten!$B$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"101324"]
["Prima Plus",88,130,"Prima Plus 13088",null,"CHI 130 Adapter Flex zu PPL","101360","0",null,"STK",57,null,null,null,null,{"$f":"IF(L5607=\"\",0,H5607*L5607)","v":0},null,null,null,"101360"]
["Prima Plus",91,130,"Prima Plus 13091",null,"CHI 130 CHI Flexrohr 2 lagig Rolle a 35000mm","101380",35000,null,"STK",2521,null,null,null,null,null,null,null,null,"101380"]
["Prima Plus",93,130,"Prima Plus 13093",null,"CHZ Mantelstein EZ  280 x 280mm L330mm","103718","0",null,"STK",24,null,null,null,null,null,null,null,null,"103718"]
["Prima Plus",96,130,"Prima Plus 13096",null,{"$f":"VLOOKUP(G5615,sanschie!A:E,5,0)","v":"CHZ Kaminmörtel Sack 25kg "},"103790","0",null,"STK",{"$f":"VLOOKUP(G5615,sanschie!A:G,7,0)","v":61},null,null,null,null,null,null,null,null,"103790"]
["Prima Plus",99,130,"Prima Plus 13099",null,{"$f":"VLOOKUP(G5618,sanschie!A:E,5,0)","v":"ABS HEB-Set zu Handyplatte EZ Inox "},"104175","0",null,"STK",{"$f":"VLOOKUP(G5618,sanschie!A:G,7,0)","v":34},null,null,null,null,null,null,null,null,"104175"]
["Prima Plus",101,130,"Prima Plus 130101",null,{"$f":"VLOOKUP(G5620,sanschie!A:E,5,0)","v":"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben"},"140932","0",null,"STK",{"$f":"VLOOKUP(G5620,sanschie!A:G,7,0)","v":75},null,null,null,null,null,null,null,null,"140932"]
["Prima Plus",102,130,{"$f":"A5621&\" \"&C5621&B5621","v":"Prima Plus 130102"},null,{"$f":"VLOOKUP(G5621,sanschie!A:E,5,0)","v":"LBS 230 Leichtbauschacht i 230mm A 320mm L1000mm"},"103826","0",null,"STK",{"$f":"VLOOKUP(G5621,sanschie!A:G,7,0)","v":135},null,null,null,null,null,null,null,null,"103826"]
["Prima Plus",0,150,"Prima Plus 1500"," ","Schiedel Prima Plus 0,6mm Ø 150","PRIMA PLUS 150","0",{"$f":"'PRIMA PLUS'!$J$11","v":10},"Anlage",0,1,{"$f":"I5625*1000","v":10000},null,{"$f":"ROUNDUP(P5625,2)","v":10.87},{"$f":"SUM(P5626:P5720)/1000","v":10.87}]
["Prima Plus",2,150,{"$f":"A5627&\" \"&C5627&B5627","v":"Prima Plus 1502"},null,"PPL 150 Lang-Bogen 45° L220mm","100589","0",null,"STK",108,null,0,null,null,{"$f":"IF(L5627=\"\",0,H5627*L5627)","v":0},null,null,null,"100589"]
["Prima Plus",5,150,"Prima Plus 1505",null,"PPL 150 Konsolenbleche für Zwischenstütze (Paar)","100609","0",null,"STK",119,null,0,null,null,null,null,null,null,"100609"]
["Prima Plus",6,150,{"$f":"A5631&\" \"&C5631&B5631","v":"Prima Plus 1506"},null,"PPL 150 Zwischenstütze","100623",100,null,"STK",114,null,0,null,null,{"$f":"IF(L5631=\"\",0,H5631*L5631)","v":0},null,null,null,"100623"]
["Prima Plus",10,150,"Prima Plus 15010",null,"PPL 150 Revisions-und Anschluss-Basiselement DN150","100701",325,null,"STK",108,{"$f":"IF(Daten!$B$662=1,1+Daten!$C$654,Daten!$C$654)","v":1},325,null,null,325,null,null,null,"100701"]
["Prima Plus",11,150,"Prima Plus 15011",null,"PPL 150 Anschluss glatt zu Basiselement L120mm","100717","0",null,"STK",64,{"$f":"IF(Daten!$B$662=1,1,\"\")","v":""},{"$f":"IF(L5636=\"\",0,L5636*H5636)","v":0},null,null,0,null,null,null,"100717"]
["Prima Plus",13,150,"Prima Plus 15013",null,"PPL 150 Revisionsdeckel für Oel/Gas ","100732","0",null,"STK",54,{"$f":"IF(Daten!$B$644=2,Daten!$C$654,\"\")","v":""},0,null,null,null,null,null,null,"100732"]
["Prima Plus",16,150,"Prima Plus 15016",null,"PPL 150 Zugbergrenzerset zu Basiselement","100760","0",null,"STK",324,null,0,null,null,{"$f":"IF(L5641=\"\",0,H5641*L5641)","v":0},null,null,null,"100760"]
["Prima Plus",18,150,"Prima Plus 15018",null,"PPL 150 Basiselement-Adapter für Zugbegrenzer","100767","0",null,"STK",83,null,0,null,null,0,null,null,null,"100767"]
["Prima Plus",21,150,"Prima Plus 15021",null,"PPL Verlängerung zu Putztüre eckig  155 x 215mm ","100784","0",null,"STK",108,{"$f":"IF(L5645=\"\",\"\",L5645)","v":""},0,null,null,0,null,null,null,"100784"]
["Prima Plus",24,150,"Prima Plus 15024",null,"PPL 150-700 Montagerahmen L250mm","100790","0",null,"STK",97,null,0,null,null,{"$f":"IF(L5649=\"\",0,H5649*L5649)","v":0},null,null,null,"100790"]
["Prima Plus",26,150,"Prima Plus 15026",null,"PPL 150 T-Stück 90° L325mm","100805",325,null,"STK",108,{"$f":"IF(Daten!$B$662=2,1,\"\")","v":1},325,null,null,325,null,null,null,"100805"]
["Prima Plus",29,150,"Prima Plus 15029",null,"PPL 150 Doppelfutterrohr zu T-Stück L120mm","100841","0",null,"STK",64,null,0,null,null,0,null,null,null,"100841"]
["Prima Plus",32,150,"Prima Plus 15032",null,"PPL 150 Längenelement L1000mm","100877",950,null,"STK",82,{"$f":"ROUNDUP(M5657,0)","v":10},{"$f":"(M5625-(SUM(M5626:M5656))-(SUM(M5658:M5665)))/H5657","v":9.0842105263157897},null,null,9500,null,null,null,"100877"]
["Prima Plus",34,150,{"$f":"A5659&\" \"&C5659&B5659","v":"Prima Plus 15034"},null,"PPL 150 Element mit 3 Messöffnungen 3/4\" L150mm","100905","0",null,"STK",119,null,{"$f":"IF(L5659=\"\",0,L5659*H5659)","v":0},null,null,0,null,null,null,"100905"]
["Prima Plus",35,150,"Prima Plus 15035",null,"PPL 150 Empa Messtutzen L450mm","140745","0",null,"STK",260,null,{"$f":"IF(L5660=\"\",0,L5660*H5660)","v":0},null,null,0,null,null,null,"140745"]
["Prima Plus",39,150,"Prima Plus 15039",null,"PPL 150 Endrohr mit beidseitiger Muffe L1000mm","100941",950,null,"STK",86,null,{"$f":"IF(L5664=\"\",0,L5664*H5664)","v":0},null,null,{"$f":"IF(L5664=\"\",0,H5664*L5664)","v":0},null,null,null,"100941"]
["Prima Plus",41,150,"Prima Plus 15041",null,"PPL 150 Kondensatabscheider L150mm","100963","0",null,"STK",124,null,null,null,null,{"$f":"IF(L5666=\"\",0,H5666*L5666)","v":0},null,null,null,"100963"]
["Prima Plus",44,150,{"$f":"A5669&\" \"&C5669&B5669","v":"Prima Plus 15044"},null,"PPL 150 Dichtung Viton","100992","0",null,"STK",16,{"$f":"IF(N5669=\"\",\"\",N5669)","v":""},null,{"$f":"IF(Daten!$B$644=1,\"\",O5669)","v":""},{"$f":"SUM(L5626,L5629,L5635,L5651,L5653,L5655,L5656,L5657,L5658)","v":15},null,null,null,null,"100992"]
["Prima Plus",47,150,"Prima Plus 15047",null,"PPL 150 Winkel 45°","101034","0",null,"STK",60,null,null,null,null,null,null,null,null,"101034"]
["Prima Plus",49,150,"Prima Plus 15049",null,"PPL 150 Winkel 90°","101062","0",null,"STK",72,null,null,null,null,null,null,null,null,"101062"]
["Prima Plus",50,150,"Prima Plus 15050",null,"PPL 150 Winkel 85° mit Revisionsöffnung","101076","0",null,"STK",173,null,null,null,null,null,null,null,null,"101076"]
["Prima Plus",52,150,"Prima Plus 15052",null,"PPL 150 Winkel 0-45° verstellbar  Trockenbetrieb ","101090","0",null,"STK",54,null,null,null,null,null,null,null,null,"101090"]
["Prima Plus",55,150,"Prima Plus 15055",null,"PPL 150 Kesselanschluss DN + 6mm L150mm","101110","0",null,"STK",64,null,null,null,null,null,null,null,null,"101110"]
["Prima Plus",58,150,"Prima Plus 15058",null,"PPL 150 Erweiterung DN200 L150mm","101126","0",null,"STK",108,null,null,null,null,null,null,null,null,"101126"]
["Prima Plus",60,150,"Prima Plus 15060",null,"PPL 180 Reduktion  DN150 L150mm","101145","0",null,"STK",108,null,null,null,null,null,null,null,null,"101145"]
["Prima Plus",63,150,"Prima Plus 15063",null,"PPL 150 Verlängerung zu Schalldämpfer -10DB ","101165","0",null,"STK",449,null,null,null,null,null,null,null,null,"101165"]
["Prima Plus",65,150,{"$f":"A5690&\" \"&C5690&B5690","v":"Prima Plus 15065"},null,"PPL 150 Schallabsorber Festbrennstoffe","101178","0",null,"STK",119,null,null,null,null,null,null,null,null,"101178"]
["Prima Plus",68,150,"Prima Plus 15068",null,"PPL 150 Anschlussrosette ØA 320mm","101186","0",null,"STK",43,null,null,null,null,null,null,null,null,"101186"]
["Prima Plus",71,150,"Prima Plus 15071",null,"ICM L1 Verlängerung zu Wandhalter 50mm L300mm","102319","0",null,"STK",109,null,null,null,null,null,null,null,null,"102319"]
["Prima Plus",73,150,"Prima Plus 15073",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,null,null,null,null,null,null,"102321"]
["Prima Plus",74,150,"Prima Plus 15074",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,null,null,null,null,null,null,null,null,"102322"]
["Prima Plus",78,150,"Prima Plus 15078",null,"PPL Muffe 1/2\" zu Grundplatte 1/2\" Wandabst. 50mm","101205","0",null,"STK",20,null,null,null,null,null,null,null,null,"101205"]
["Prima Plus",80,150,"Prima Plus 15080",null,"PPL 150 Regenkragen ","101261","0",null,"STK",49,null,null,null,null,null,null,null,null,"101261"]
["Prima Plus",83,150,"Prima Plus 15083",null,"PPL 150 Regenhaube ","101310","0",null,"STK",81,{"$f":"IF(Daten!$B$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"101310"]
["Prima Plus",86,150,{"$f":"A5711&\" \"&C5711&B5711","v":"Prima Plus 15086"},null,"Basten Stand.Dila 220mm.150CU","104622","0",null,"STK",418,null,null,null,null,null,null,null,null,"104622"]
["Prima Plus",88,150,{"$f":"A5713&\" \"&C5713&B5713","v":"Prima Plus 15088"},null,"PPL 150 Dämmschale 30mm Alu-Kaschiert L1000mm","101325","0",null,"STK",39,{"$f":"IF(Daten!$B$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"101325"]
["Prima Plus",89,150,"Prima Plus 15089",null,"PPL Stopf-Steinwolle  Sack 10kg","101349","0",null,"STK",50,null,null,null,null,null,null,null,null,"101349"]
["Prima Plus",91,150,"Prima Plus 15091",null,"CHI 150 Adapter Flex zu PPL","101361","0",null,"STK",60,null,null,null,null,{"$f":"IF(L5716=\"\",0,H5716*L5716)","v":0},null,null,null,"101361"]
["Prima Plus",94,150,"Prima Plus 15094",null,"CHI 150 CHI Flexrohr 2 lagig Rolle a 30000mm","101381",30000,null,"STK",2516,null,null,null,null,null,null,null,null,"101381"]
["Prima Plus",97,150,"Prima Plus 15097",null,"CHZ Mantelstein EZ  320 x 320mm L330mm Ø160mm","103719","0",null,"STK",19,null,null,null,null,null,null,null,null,"103719"]
["Prima Plus",99,150,{"$f":"A5724&\" \"&C5724&B5724","v":"Prima Plus 15099"},null,"CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",{"$f":"VLOOKUP(G5724,sanschie!A:G,7,0)","v":61},null,null,null,null,null,null,null,null,"103790"]
["Prima Plus",102,150,"Prima Plus 150102",null,{"$f":"VLOOKUP(G5727,sanschie!A:E,5,0)","v":"ABS HEB-Set zu Handyplatte EZ Inox "},"104175","0",null,"STK",{"$f":"VLOOKUP(G5727,sanschie!A:G,7,0)","v":34},null,null,null,null,null,null,null,null,"104175"]
["Prima Plus",104,150,"Prima Plus 150104",null,{"$f":"VLOOKUP(G5729,sanschie!A:E,5,0)","v":"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben"},"140932","0",null,"STK",{"$f":"VLOOKUP(G5729,sanschie!A:G,7,0)","v":75},null,null,null,null,null,null,null,null,"140932"]
["Prima Plus",108,150,"Prima Plus 150108",null,"ABS Verstärkung zu Kaminhalterung","104256","0",null,"STK",{"$f":"VLOOKUP(G5733,sanschie!A:G,7,0)","v":303},null,null,null,null,null,null,null,null,"104256"]
["Prima Plus",0,180,"Prima Plus 1800"," ","Schiedel Prima Plus 0,6mm Ø 180","PRIMA PLUS 180","0",{"$f":"'PRIMA PLUS'!$J$11","v":10},"Anlage",0,1,{"$f":"I5734*1000","v":10000},null,{"$f":"ROUNDUP(P5734,2)","v":10.17},{"$f":"SUM(P5735:P5833)/1000","v":10.17}]
["Prima Plus",3,180,{"$f":"A5737&\" \"&C5737&B5737","v":"Prima Plus 1803"},null,{"$f":"VLOOKUP(G5737,sanschie!A:E,5,0)","v":"PPL 180 Kaminfuss 85° "},"140868","0",null,"STK",{"$f":"VLOOKUP(G5737,sanschie!A:G,7,0)","v":151},null,{"$f":"IF(L5737=\"\",0,L5737*H5737)","v":0},null,null,{"$f":"IF(L5737=\"\",0,H5737*L5737)","v":0},null,null,null,"140868"]
["Prima Plus",4,180,"Prima Plus 1804",null,"PPL 180 Kondensattopf mit Ablauf seitlich","100598",70,null,"STK",76,{"$f":"IF(L5735=1,\"\",IF(L5735=1,\"\",1))","v":1},70,null,null,{"$f":"IF(L5738=\"\",0,H5738*L5738)","v":70},null,null,null,"100598"]
[{"$f":"A5741","v":"Prima Plus"},{"$f":"B5741+1","v":8},{"$f":"C5741","v":180},{"$f":"A5742&\" \"&C5742&B5742","v":"Prima Plus 1808"},null,"PPL 180 EW-DW Deckenanfängerset komplett L270mm","100651","0",null,"STK",432,null,0,null,null,{"$f":"IF(L5742=\"\",0,H5742*L5742)","v":0},null,null,null,"100651"]
["Prima Plus",10,180,{"$f":"A5744&\" \"&C5744&B5744","v":"Prima Plus 18010"},null,"PPL 180 Revisions-Basiselement für Deckel DN150 ","100706",450,null,"STK",119,{"$f":"Daten!$C$654","v":1},450,null,null,{"$f":"IF(L5744=\"\",0,H5744*L5744)","v":450},null,null,null,"100706"]
["Prima Plus",13,180,"Prima Plus 18013",null,"PPL 180 Anschluss-Doppelfutter zu Basiselement ","100725","0",null,"STK",119,null,0,null,null,{"$f":"IF(L5747=\"\",0,H5747*L5747)","v":0},null,null,null,"100725"]
["Prima Plus",16,180,"Prima Plus 18016",null,"PPL 180 Revisionsdeckel für Festbrennstoffe","100741","0",null,"STK",86,null,{"$f":"IF(L5750=\"\",0,L5750*H5750)","v":0},null,null,null,null,null,null,"100741"]
["Prima Plus",18,180,"Prima Plus 18018",null,"PPL 180 Zugbergrenzerset zu Basiselement","100761","0",null,"STK",335,null,0,null,null,{"$f":"IF(L5752=\"\",0,H5752*L5752)","v":0},null,null,null,"100761"]
["Prima Plus",19,180,"Prima Plus 18019",null,"PPL 130 Zugbergrenzer","100764","0",null,"STK",241,null,0,null,null,0,null,null,null,"100764"]
["Prima Plus",23,180,{"$f":"A5757&\" \"&C5757&B5757","v":"Prima Plus 18023"},null,"PPL Putztüre 150 x 200mm zu Putztüranschluss eckig","100783","0",null,"STK",108,{"$f":"IF(Daten!$B$670=1,\"\",IF(L5744=\"\",\"\",Daten!$C$670))","v":""},0,null,null,0,null,null,null,"100783"]
["Prima Plus",24,180,{"$f":"A5758&\" \"&C5758&B5758","v":"Prima Plus 18024"},null,"PPL Verlängerung zu Putztüre eckig  155 x 215mm ","100784","0",null,"STK",108,null,0,null,null,0,null,null,null,"100784"]
["Prima Plus",27,180,"Prima Plus 18027",null,"PPL 150-700 Montagerahmen L250mm","100790","0",null,"STK",97,null,0,null,null,0,null,null,null,"100790"]
["Prima Plus",29,180,"Prima Plus 18029",null,"PPL 180 T-Stück 90° L450mm","100806",450,null,"STK",119,{"$f":"IF(Daten!$B$662=2,1,\"\")","v":1},450,null,null,450,null,null,null,"100806"]
["Prima Plus",32,180,"Prima Plus 18032",null,"PPL 180 Doppelfutterrohr zu T-Stück L120mm","100842","0",null,"STK",64,null,0,null,null,0,null,null,null,"100842"]
["Prima Plus",34,180,"Prima Plus 18034",null,"PPL 180 Längenelement L500mm","100864",450,null,"STK",55,{"$f":"1+N5768","v":1},450,{"$f":"IF('PRIMA PLUS'!$P$17=\"\",0,IF('PRIMA PLUS'!$P$17=0,0,'PRIMA PLUS'!$P$17))","v":0},null,450,null,null,null,"100864"]
["Prima Plus",38,180,"Prima Plus 18038",null,"PPL 180 Empa Messtutzen L450mm","140746","0",null,"STK",271,null,{"$f":"IF(L5772=\"\",0,L5772*H5772)","v":0},null,null,{"$f":"IF(L5772=\"\",0,H5772*L5772)","v":0},null,null,null,"140746"]
["Prima Plus",39,180,"Prima Plus 18039",null,"PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7,null,{"$f":"IF(L5773=\"\",0,L5773*H5773)","v":0},null,null,{"$f":"IF(L5773=\"\",0,H5773*L5773)","v":0},null,null,null,"100974"]
["Prima Plus",41,180,"Prima Plus 18041",null,"PPL 180 Schiebe-Element 270-415mm","100928","0",null,"STK",97,null,{"$f":"IF(L5775=\"\",0,L5775*H5775)","v":0},null,null,null,null,null,null,"100928"]
["Prima Plus",44,180,"Prima Plus 18044",null,"PPL 180 Kondensatabscheider L150mm","100964","0",null,"STK",129,null,null,null,null,{"$f":"IF(L5778=\"\",0,H5778*L5778)","v":0},null,null,null,"100964"]
["Prima Plus",47,180,"Prima Plus 18047",null,"PPL 180 Dichtung Viton","100993","0",null,"STK",18,{"$f":"IF(N5781=\"\",\"\",N5781)","v":""},null,{"$f":"IF(Daten!$B$644=1,\"\",O5781)","v":""},{"$f":"SUM(L5735,L5738,L5744:L5746,L5763,L5765,L5767,L5768,L5769,L5770)","v":14},null,null,null,null,"100993"]
["Prima Plus",49,180,"Prima Plus 18049",null,"PPL 180 Winkel 30°","101021","0",null,"STK",60,null,null,null,null,null,null,null,null,"101021"]
["Prima Plus",52,180,"Prima Plus 18052",null,"PPL 180 Winkel 90°","101063","0",null,"STK",77,null,null,null,null,null,null,null,null,"101063"]
["Prima Plus",55,180,"Prima Plus 18055",null,"PPL 180 Winkel 0-45° verstellbar  Trockenbetrieb ","101091","0",null,"STK",64,null,null,null,null,null,null,null,null,"101091"]
["Prima Plus",57,180,"Prima Plus 18057",null,"PPL 180 Revisions-Winkel 0-90° verstellbar   ","101103","0",null,"STK",162,null,null,null,null,null,null,null,null,"101103"]
["Prima Plus",58,180,"Prima Plus 18058",null,"PPL 180 Kesselanschluss DN + 6mm L150mm","101112","0",null,"STK",76,null,null,null,null,null,null,null,null,"101112"]
["Prima Plus",62,180,"Prima Plus 18062",null,"PPL 180 Erweiterung DN200 L150mm","101128","0",null,"STK",119,null,null,null,null,null,null,null,null,"101128"]
["Prima Plus",63,180,"Prima Plus 18063",null,"PPL 180 Reduktion  DN130 L150mm","101144","0",null,"STK",108,null,null,null,null,null,null,null,null,"101144"]
["Prima Plus",66,180,"Prima Plus 18066",null,"PPL 180-200 Verlängerung zu Schalldämpfer -10DB ","101166","0",null,"STK",999,null,null,null,null,null,null,null,null,"101166"]
["Prima Plus",68,180,"Prima Plus 18068",null,"PPL 180 Schallabsorber Festbrennstoffe","101179","0",null,"STK",141,null,null,null,null,null,null,null,null,"101179"]
["Prima Plus",72,180,"Prima Plus 18072",null,"ICM 130 Wandhalter 50mm verlängerbar DN 180mm ","102305","0",null,"STK",44,null,null,null,null,null,null,null,null,"102305"]
["Prima Plus",73,180,"Prima Plus 18073",null,"ICM W1 Verlängerung zu Wandhalter 50mm L 130mm","102317","0",null,"STK",44,null,null,null,null,null,null,null,null,"102317"]
["Prima Plus",77,180,"Prima Plus 18077",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,null,null,null,null,null,null,null,null,"102322"]
["Prima Plus",78,180,"Prima Plus 18078",null,"ICM 130 Wandhalter verstellbar 75 - 300mm DN 180mm","102291","0",null,"STK",65,null,null,null,null,null,null,null,null,"102291"]
["Prima Plus",80,180,"Prima Plus 18080",null,"PPL Innengewinderohr zu Rohrschelle 1/2\" 1000mm","101204","0",null,"STK",147,null,null,null,null,null,null,null,null,"101204"]
["Prima Plus",83,180,"Prima Plus 18083",null,"PPL 180 Regenkragen ","101262","0",null,"STK",54,null,null,null,null,null,null,null,null,"101262"]
["Prima Plus",86,180,"Prima Plus 18086",null,"PPL 180 Mündungsmanchette L130mm 450 x 450mm","101288","0",null,"STK",141,{"$f":"IF(Daten!$E$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"101288"]
["Prima Plus",88,180,"Prima Plus 18088",null,"PPL 180 Basten Standard Kupfer zu Münd. Manchette","140823","0",null,"STK",320,null,null,null,null,null,null,null,null,"140823"]
["Prima Plus",91,180,"Prima Plus 18091",null,"PPL 180 Regenhaube ","101311","0",null,"STK",97,{"$f":"IF(Daten!$B$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"101311"]
["Prima Plus",94,180,"Prima Plus 18094",null,"CHI 180 Adapter PPL zu Flex","101355","0",null,"STK",65,null,null,null,null,{"$f":"IF(L5828=\"\",0,H5828*L5828)","v":0},null,null,null,"101355"]
["Prima Plus",96,180,"Prima Plus 18096",null,"CHI 180 Adapter Flex zu Flex","101369","0",null,"STK",74,null,null,null,null,{"$f":"IF(L5830=\"\",0,H5830*L5830)","v":0},null,null,null,"101369"]
["Prima Plus",97,180,"Prima Plus 18097",null,"CHI 180 CHI Flexrohr 2 lagig Rolle a 12000mm","101376",12000,null,"STK",1255,null,null,null,null,null,null,null,null,"101376"]
["Prima Plus",101,180,"Prima Plus 180101",null,"CHZ Mantelstein EZ 360 x 360mm L330mm Ø180-200mm","103720","0",null,"STK",20,null,null,null,null,null,null,null,null,"103720"]
["Prima Plus",103,180,"Prima Plus 180103",null,{"$f":"VLOOKUP(G5837,sanschie!A:E,5,0)","v":"CHZ Kaminmörtel Sack 25kg "},"103790","0",null,"STK",{"$f":"VLOOKUP(G5837,sanschie!A:G,7,0)","v":61},null,null,null,null,null,null,null,null,"103790"]
["Prima Plus",106,180,"Prima Plus 180106",null,{"$f":"VLOOKUP(G5840,sanschie!A:E,5,0)","v":"ABS HEB-Set zu Handyplatte EZ Inox "},"104175","0",null,"STK",{"$f":"VLOOKUP(G5840,sanschie!A:G,7,0)","v":34},null,null,null,null,null,null,null,null,"104175"]
["Prima Plus",107,180,"Prima Plus 180107",null,{"$f":"VLOOKUP(G5841,sanschie!A:E,5,0)","v":"ABS Handyplatte EZ Kupfer 360 x 360mm  "},"140787","0",null,"STK",{"$f":"VLOOKUP(G5841,sanschie!A:G,7,0)","v":229},null,null,null,null,null,null,null,null,"140787"]
["Prima Plus",111,180,"Prima Plus 180111",null,{"$f":"VLOOKUP(G5845,sanschie!A:E,5,0)","v":"LBS Kleber zu Leichtbauschacht 1kg"},"103829","0",null,"STK",{"$f":"VLOOKUP(G5845,sanschie!A:G,7,0)","v":14},null,null,null,null,null,null,null,null,"103829"]
["Prima Plus",112,180,"Prima Plus 180112",null,{"$f":"VLOOKUP(G5846,sanschie!A:E,5,0)","v":"ABS Kaminhalterung Standard"},"104256","0",null,"STK",{"$f":"VLOOKUP(G5846,sanschie!A:G,7,0)","v":303},null,null,null,null,null,null,null,null,"104256"]
["Prima Plus",3,200,"Prima Plus 2003",null,{"$f":"VLOOKUP(G5850,sanschie!A:E,5,0)","v":"PPL 200 Kaminfuss 85° "},"140869","0",null,"STK",{"$f":"VLOOKUP(G5850,sanschie!A:G,7,0)","v":179},null,0,null,null,{"$f":"IF(L5850=\"\",0,H5850*L5850)","v":0},null,null,null,"140869"]
["Prima Plus",4,200,"Prima Plus 2004",null,"PPL 200 Kondensattopf mit Ablauf seitlich","100599",70,null,"STK",86,{"$f":"IF(L5848=1,\"\",IF(L5848=1,\"\",1))","v":1},70,null,null,{"$f":"IF(L5851=\"\",0,H5851*L5851)","v":70},null,null,null,"100599"]
["Prima Plus",6,200,"Prima Plus 2006",null,"PPL 200 Zwischenstütze","100625",100,null,"STK",129,null,0,null,null,{"$f":"IF(L5853=\"\",0,H5853*L5853)","v":0},null,null,null,"100625"]
[{"$f":"A5855","v":"Prima Plus"},{"$f":"B5855+1","v":9},{"$f":"C5855","v":200},{"$f":"A5856&\" \"&C5856&B5856","v":"Prima Plus 2009"},null,"PPL 200 EW-DW Deckenanfängerset 45° kompl. L270mm","100659","0",null,"STK",648,null,0,null,null,{"$f":"IF(L5856=\"\",0,H5856*L5856)","v":0},null,null,null,"100659"]
["Prima Plus",12,200,"Prima Plus 20012",null,"PPL 150 Anschluss glatt zu Basiselement L120mm","100717","0",null,"STK",64,null,0,null,null,{"$f":"IF(L5859=\"\",0,H5859*L5859)","v":0},null,null,null,"100717"]
["Prima Plus",14,200,"Prima Plus 20014",null,"PPL 200 Anschluss-Doppelfutter zu Basiselement ","100726","0",null,"STK",129,null,0,null,null,{"$f":"IF(L5861=\"\",0,H5861*L5861)","v":0},null,null,null,"100726"]
["Prima Plus",17,200,"Prima Plus 20017",null,"PPL 150 Revisionsdeckel für Festbrennstoffe","100740","0",null,"STK",76,{"$f":"IF(Daten!$B$644=1,Daten!$C$654,\"\")","v":1},0,null,null,null,null,null,null,"100740"]
["Prima Plus",20,200,"Prima Plus 20020",null,"PPL 200 Zugbergrenzerset zu Basiselement","100762","0",null,"STK",482,null,0,null,null,{"$f":"IF(L5867=\"\",0,H5867*L5867)","v":0},null,null,null,"100762"]
["Prima Plus",22,200,"Prima Plus 20022",null,"PPL 200 Basiselement-Adapter für Zugbegrenzer","100769","0",null,"STK",115,null,0,null,null,0,null,null,null,"100769"]
["Prima Plus",23,200,"Prima Plus 20023",null,"PPL 200 Putztüranschluss eckig mit Innentüre ","100774",325,null,"STK",184,null,0,null,null,0,null,null,null,"100774"]
["Prima Plus",27,200,"Prima Plus 20027",null,"PPL 150-700 Montagerahmen L150mm","100789","0",null,"STK",86,null,0,null,null,0,null,null,null,"100789"]
["Prima Plus",29,200,"Prima Plus 20029",null,"PPL 200 T-Stück 85° L450mm","100799",450,null,"STK",141,null,{"$f":"IF(L5876=\"\",0,L5876*H5876)","v":0},null,null,0,null,null,null,"100799"]
["Prima Plus",32,200,"Prima Plus 20032",null,"PPL 200 T-Stück 45° L450mm","100829",450,null,"STK",237,{"$f":"IF(Daten!$B$662=3,1,\"\")","v":""},0,null,null,0,null,null,null,"100829"]
["Prima Plus",33,200,"Prima Plus 20033",null,"PPL 200 Doppelfutterrohr zu T-Stück L120mm","100843","0",null,"STK",71,null,0,null,null,0,null,null,null,"100843"]
["Prima Plus",37,200,"Prima Plus 20037",null,"PPL 200 Ablass-Element L200mm","100893",200,null,"STK",86,1,{"$f":"IF(L5884=\"\",0,L5884*H5884)","v":200},null,null,200,null,null,null,"100893"]
["Prima Plus",38,200,{"$f":"A5885&\" \"&C5885&B5885","v":"Prima Plus 20038"},null,"PPL 200 Element mit 3 Messöffnungen 3/4\" L150mm","100907","0",null,"STK",141,null,{"$f":"IF(L5885=\"\",0,L5885*H5885)","v":0},null,null,0,null,null,null,"100907"]
["Prima Plus",40,200,{"$f":"A5887&\" \"&C5887&B5887","v":"Prima Plus 20040"},null,"PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7,null,{"$f":"IF(L5887=\"\",0,L5887*H5887)","v":0},null,null,0,null,null,null,"100974"]
["Prima Plus",43,200,"Prima Plus 20043",null,"PPL 200 Endrohr mit beidseitiger Muffe L1000mm","100943",950,null,"STK",108,null,{"$f":"IF(L5890=\"\",0,L5890*H5890)","v":0},null,null,{"$f":"IF(L5890=\"\",0,H5890*L5890)","v":0},null,null,null,"100943"]
["Prima Plus",45,200,"Prima Plus 20045",null,"PPL 200 Kondensatabscheider L150mm","100965","0",null,"STK",135,null,null,null,null,{"$f":"IF(L5892=\"\",0,H5892*L5892)","v":0},null,null,null,"100965"]
["Prima Plus",48,200,{"$f":"A5895&\" \"&C5895&B5895","v":"Prima Plus 20048"},null,"PPL 200 Dichtung Viton","100994","0",null,"STK",19,{"$f":"IF(N5895=\"\",\"\",N5895)","v":""},null,{"$f":"IF(Daten!$B$644=1,\"\",O5895)","v":""},{"$f":"SUM(L5848,L5851,L5857:L5860,L5877,L5879,L5881,L5882,L5883,L5884)","v":14},null,null,null,null,"100994"]
["Prima Plus",51,200,{"$f":"A5898&\" \"&C5898&B5898","v":"Prima Plus 20051"},null,"PPL 200 Winkel 45°","101036","0",null,"STK",72,null,null,null,null,null,null,null,null,"101036"]
["Prima Plus",53,200,"Prima Plus 20053",null,"PPL 200 Winkel 90°","101064","0",null,"STK",93,null,null,null,null,null,null,null,null,"101064"]
["Prima Plus",56,200,"Prima Plus 20056",null,"PPL 200 Winkel 0-45° verstellbar  Trockenbetrieb ","101092","0",null,"STK",76,null,null,null,null,null,null,null,null,"101092"]
["Prima Plus",59,200,"Prima Plus 20059",null,"PPL 200 Kesselanschluss DN + 6mm L150mm","101113","0",null,"STK",86,null,null,null,null,null,null,null,null,"101113"]
["Prima Plus",61,200,"Prima Plus 20061",null,"PPL 150 Erweiterung DN200 L150mm","101126","0",null,"STK",108,null,null,null,null,null,null,null,null,"101126"]
["Prima Plus",62,200,"Prima Plus 20062",null,"PPL 200 Reduktion  DN150 L150mm","101146","0",null,"STK",108,null,null,null,null,null,null,null,null,"101146"]
["Prima Plus",66,200,{"$f":"A5913&\" \"&C5913&B5913","v":"Prima Plus 20066"},null,"PPL 200 Schallabsorber Oel-Gas","101173","0",null,"STK",194,null,null,null,null,null,null,null,null,"101173"]
["Prima Plus",68,200,"Prima Plus 20068",null,"ICM 200 Anschluss von EW auf DW in Rauchgasr.","102151","0",null,"STK",142,null,null,null,null,null,null,null,null,"102151"]
["Prima Plus",71,200,"Prima Plus 20071",null,"ICM 150 Wandhalter 50mm verlängerbar DN 200mm ","102306","0",null,"STK",50,null,null,null,null,null,null,null,null,"102306"]
["Prima Plus",74,200,"Prima Plus 20074",null,"ICM L2 Verlängerung zu Wandhalter 50mm L450mm","102320","0",null,"STK",142,null,null,null,null,null,null,null,null,"102320"]
["Prima Plus",76,200,"Prima Plus 20076",null,"ICM L4 Verlängerung zu Wandhalter 50mm L 750mm","102322","0",null,"STK",195,null,null,null,null,null,null,null,null,"102322"]
["Prima Plus",77,200,"Prima Plus 20077",null,"ICM 150 Wandhalter verstellbar 75 - 300mm DN 200mm","102292","0",null,"STK",72,null,null,null,null,null,null,null,null,"102292"]
[{"$f":"A5925","v":"Prima Plus"},{"$f":"B5925+1","v":79},{"$f":"C5925","v":200},"Prima Plus 20079",null,"PPL Innengewinderohr zu Rohrschelle 1/2\" 1000mm","101204","0",null,"STK",147,null,null,null,null,null,null,null,null,"101204"]
["Prima Plus",82,200,"Prima Plus 20082",null,"PPL 200 Regenkragen ","101263","0",null,"STK",59,null,null,null,null,null,null,null,null,"101263"]
["Prima Plus",84,200,"Prima Plus 20084",null,"PPL 200 Mündungskonus zu Schachtabdeckung","101281","0",null,"STK",81,{"$f":"IF(Daten!$E$677=1,1,\"\")","v":1},null,null,null,null,null,null,null,"101281"]
["Prima Plus",87,200,"Prima Plus 20087",null,"PPL 200 Basten Standard mit Dila zu Dämmrohr 30mm","101304","0",null,"STK",403,null,null,null,null,null,null,null,null,"101304"]
["Prima Plus",90,200,{"$f":"A5937&\" \"&C5937&B5937","v":"Prima Plus 20090"},null,"PPL Stopf-Steinwolle  Sack 10kg","101349","0",null,"STK",50,null,null,null,null,null,null,null,null,"101349"]
["Prima Plus",92,200,"Prima Plus 20092",null,"CHI 200 Adapter PPL zu Flex","101356","0",null,"STK",70,null,null,null,null,{"$f":"IF(L5939=\"\",0,H5939*L5939)","v":0},null,null,null,"101356"]
["Prima Plus",96,200,"Prima Plus 20096",null,"CHI Flexrohr Rolle 15m D200","104559","0",null,"STK",1889,null,null,null,null,null,null,null,null,"104559"]
["Prima Plus",97,200,"Prima Plus 20097",null,"CHI 200 Aufhängeschelle zu Flex","101391","0",null,"STK",30,null,null,null,null,null,null,null,null,"101391"]
["Prima Plus",100,200,"Prima Plus 200100",null,"CHZ Mantelstein EZ  480 x 480mm L330mm Ø250mm","103722","0",null,"STK",24,null,null,null,null,null,null,null,null,"103722"]
["Prima Plus",101,200,{"$f":"A5948&\" \"&C5948&B5948","v":"Prima Plus 200101"},null,"CHZ Mantelstein rund ØA 400mm Øi 280mm L330mm","103725","0",null,"STK",23,null,null,null,null,null,null,null,null,"103725"]
["Prima Plus",105,200,"Prima Plus 200105",null,"LBS Kleber zu Leichtbauschacht 1kg","103829","0",null,"STK",9,null,null,null,null,null,null,null,null,"103829"]
["Prima Plus",107,200,"Prima Plus 200107",null,{"$f":"VLOOKUP(G5954,sanschie!A:E,5,0)","v":"ABS Handyplatte EZ Inox 360 x 360mm  "},"104170","0",null,"STK",{"$f":"VLOOKUP(G5954,sanschie!A:G,7,0)","v":155},null,null,null,null,null,null,null,null,"104170"]
["Prima Plus",110,200,"Prima Plus 200110",null,{"$f":"VLOOKUP(G5957,sanschie!A:E,5,0)","v":"ABS HEB-Set zu Handyplatte EZ CU kurze Schrauben"},"140932","0",null,"STK",{"$f":"VLOOKUP(G5957,sanschie!A:G,7,0)","v":75},null,null,null,null,null,null,null,null,"140932"]
["Prima Plus",0,250,"Prima Plus 2500"," ","Schiedel Prima Plus 0,6mm Ø 250","PRIMA PLUS 250","0",{"$f":"'PRIMA PLUS'!$J$11","v":10},"Anlage",0,1,{"$f":"I5960*1000","v":10000},null,{"$f":"ROUNDUP(P5960,2)","v":10.17},{"$f":"SUM(P5961:P6066)/1000","v":10.17}]
["Prima Plus",2,250,{"$f":"A5962&\" \"&C5962&B5962","v":"Prima Plus 2502"},null,"PPL 250 Lang-Bogen 45° L240mm","100592","0",null,"STK",151,null,0,null,null,{"$f":"IF(L5962=\"\",0,H5962*L5962)","v":0},null,null,null,"100592"]
["Prima Plus",3,250,"Prima Plus 2503",null,{"$f":"VLOOKUP(G5963,sanschie!A:E,5,0)","v":"PPL 250 Kaminfuss 85° "},"140870","0",null,"STK",{"$f":"VLOOKUP(G5963,sanschie!A:G,7,0)","v":205},null,{"$f":"IF(L5963=\"\",0,L5963*H5963)","v":0},null,null,{"$f":"IF(L5963=\"\",0,H5963*L5963)","v":0},null,null,null,"140870"]
["Prima Plus",5,250,"Prima Plus 2505",null,"PPL 250 Konsolenbleche für Zwischenstütze (Paar)","100612","0",null,"STK",151,null,0,null,null,null,null,null,null,"100612"]
["Prima Plus",8,250,"Prima Plus 2508",null,"PPL 250 EW-DW Deckenanfängerset komplett L270mm","100653","0",null,"STK",540,null,0,null,null,{"$f":"IF(L5968=\"\",0,H5968*L5968)","v":0},null,null,null,"100653"]
["Prima Plus",11,250,"Prima Plus 25011",null,"PPL 250 Anschluss-Basiselement DN250 L450mm","100704",450,null,"STK",173,{"$f":"IF(Daten!$B$662=1,1,\"\")","v":""},0,null,null,null,null,null,null,"100704"]
["Prima Plus",13,250,"Prima Plus 25013",null,"PPL 250 Anschluss glatt zu Basiselement L120mm","100720","0",null,"STK",129,{"$f":"IF(Daten!$B$662=1,1,\"\")","v":""},0,null,null,{"$f":"IF(L5973=\"\",0,H5973*L5973)","v":0},null,null,null,"100720"]
["Prima Plus",16,250,"Prima Plus 25016",null,"PPL 250 Revisionsdeckel für Oel/Gas ","100735","0",null,"STK",108,null,0,null,null,null,null,null,null,"100735"]
["Prima Plus",18,250,"Prima Plus 25018",null,"PPL 250 Revisionsdeckel für Festbrennstoffe","100743","0",null,"STK",129,null,0,null,null,null,null,null,null,"100743"]
["Prima Plus",22,250,"Prima Plus 25022",null,"PPL 250 Basiselement-Adapter für Zugbegrenzer","100770","0",null,"STK",136,null,0,null,null,0,null,null,null,"100770"]
["Prima Plus",23,250,"Prima Plus 25023",null,"PPL 250 Putztüranschluss eckig mit Innentüre ","100775",325,null,"STK",194,null,0,null,null,0,null,null,null,"100775"]
["Prima Plus",26,250,"Prima Plus 25026",null,"PPL 150-700 Putztüre 200 x 300mm gasdicht","100788","0",null,"STK",141,null,0,null,null,0,null,null,null,"100788"]
["Prima Plus",27,250,{"$f":"A5987&\" \"&C5987&B5987","v":"Prima Plus 25027"},null,"PPL 150-700 Montagerahmen L150mm","100789","0",null,"STK",86,null,0,null,null,0,null,null,null,"100789"]
["Prima Plus",31,250,"Prima Plus 25031",null,"PPL 250 T-Stück 90° mit Putztüre Festbrennstoff","100822",450,null,"STK",194,null,0,null,null,0,null,null,null,"100822"]
["Prima Plus",33,250,"Prima Plus 25033",null,"PPL 250 Doppelfutterrohr zu T-Stück L120mm","100844","0",null,"STK",76,null,0,null,null,0,null,null,null,"100844"]
["Prima Plus",36,250,"Prima Plus 25036",null,"PPL 250 Längenelement L1000mm","100880",950,null,"STK",120,{"$f":"ROUNDUP(M5996,0)","v":9},{"$f":"(M5960-(SUM(M5961:M5995))-(SUM(M5997:M6004)))/H5996","v":8.8210526315789473},null,null,8550,null,null,null,"100880"]
["Prima Plus",39,250,"Prima Plus 25039",null,"PPL 250 Empa Messtutzen L450mm","140748","0",null,"STK",303,null,{"$f":"IF(L5999=\"\",0,L5999*H5999)","v":0},null,null,0,null,null,null,"140748"]
["Prima Plus",41,250,"Prima Plus 25041",null,"PPL 250 Abstandhalter","100921","0",null,"STK",31,{"$f":"IF(N6001=0,\"\",ROUNDUP(N6001,0))","v":3},null,{"$f":"P5960/5","v":2.0339999999999998},null,null,null,null,null,"100921"]
["Prima Plus",42,250,"Prima Plus 25042",null,"PPL 250 Schiebe-Element 270-415mm","100930","0",null,"STK",119,null,{"$f":"IF(L6002=\"\",0,L6002*H6002)","v":0},null,null,null,null,null,null,"100930"]
["Prima Plus",46,250,"Prima Plus 25046",null,"PPL 250 Klemmband","100981","0",null,"STK",14,{"$f":"L6008","v":""},null,null,null,null,null,null,null,"100981"]
["Prima Plus",47,250,{"$f":"A6007&\" \"&C6007&B6007","v":"Prima Plus 25047"},null,"ICM 180 Klemmband DN230","102265","0",null,"STK",19,null,null,null,null,null,null,null,null,"102265"]
["Prima Plus",50,250,{"$f":"A6010&\" \"&C6010&B6010","v":"Prima Plus 25050"},null,"PPL 250 Winkel 30°","101023","0",null,"STK",82,null,null,null,null,null,null,null,null,"101023"]
["Prima Plus",52,250,{"$f":"A6012&\" \"&C6012&B6012","v":"Prima Plus 25052"},null,"PPL 250 Winkel 85°","101051","0",null,"STK",120,null,null,null,null,null,null,null,null,"101051"]
["Prima Plus",55,250,"Prima Plus 25055",null,"PPL 250 Winkel 90° mit Revisionsöffnung","101087","0",null,"STK",270,null,null,null,null,null,null,null,null,"101087"]
["Prima Plus",57,250,"Prima Plus 25057",null,"PPL 250 Winkel 0-90° verstellbar  Trockenbetrieb  ","101099","0",null,"STK",97,null,null,null,null,null,null,null,null,"101099"]
["Prima Plus",61,250,"Prima Plus 25061",null,"PPL 180 Erweiterung DN250 L150mm","101129","0",null,"STK",119,null,null,null,null,null,null,null,null,"101129"]
["Prima Plus",62,250,"Prima Plus 25062",null,"PPL 250 Reduktion  DN200 L150mm","101148","0",null,"STK",129,null,null,null,null,null,null,null,null,"101148"]
["Prima Plus",64,250,"Prima Plus 25064",null,"PPL 250 Abgasschalldämpfer Schallred. 15DB L760mm","101162","0",null,"STK",1799,null,null,null,null,null,null,null,null,"101162"]
["Prima Plus",67,250,"Prima Plus 25067",null,"PPL 250 Schallabsorber Festbrennstoffe","101181","0",null,"STK",162,null,null,null,null,null,null,null,null,"101181"]
["Prima Plus",70,250,"Prima Plus 25070",null,"PPL 250 Anschlussrosette ØA 420mm","101190","0",null,"STK",64,null,null,null,null,null,null,null,null,"101190"]
["Prima Plus",72,250,"Prima Plus 25072",null,"ICM W1 Verlängerung zu Wandhalter 50mm L 130mm","102317","0",null,"STK",44,null,null,null,null,null,null,null,null,"102317"]
["Prima Plus",75,250,"Prima Plus 25075",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163,null,null,null,null,null,null,null,null,"102321"]
[{"$f":"A6037","v":"Prima Plus"},{"$f":"B6037+1","v":78},{"$f":"C6037","v":250},"Prima Plus 25078",null,"PPL 250 Rohrschelle Anschluss 1/2\" Aussengewinde","101201","0",null,"STK",41,null,null,null,null,null,null,null,null,"101201"]
["Prima Plus",80,250,"Prima Plus 25080",null,"PPL Muffe 1/2\" zu Grundplatte 1/2\" Wandabst. 50mm","101205","0",null,"STK",20,null,null,null,null,null,null,null,null,"101205"]
["Prima Plus",81,250,"Prima Plus 25081",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25,null,null,null,null,null,null,null,null,"101206"]
["Prima Plus",85,250,"Prima Plus 25085",null,"PPL 250 Regenhaube ","101313","0",null,"STK",129,{"$f":"IF(Daten!$B$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"101313"]
[{"$f":"A6045","v":"Prima Plus"},{"$f":"B6045+1","v":86},{"$f":"C6045","v":250},{"$f":"A6046&\" \"&C6046&B6046","v":"Prima Plus 25086"},null,"PPL 250 Basten Standard passend zu Münd. Manchette","101298","0",null,"STK",305,null,null,null,null,null,null,null,null,"101298"]
["Prima Plus",90,250,{"$f":"A6050&\" \"&C6050&B6050","v":"Prima Plus 25090"},null,{"$f":"VLOOKUP(G6050,sanschie!A:E,5,0)","v":"PPL 250 Dämmschale 30mm Alu-Kaschiert L1000mm"},"101328","0",null,"STK",{"$f":"VLOOKUP(G6050,sanschie!A:G,7,0)","v":62.7},{"$f":"IF(Daten!$E$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"101328"]
["Prima Plus",91,250,"Prima Plus 25091",null,{"$f":"VLOOKUP(G6051,sanschie!A:E,5,0)","v":"PPL Stopf-Steinwolle  Sack 10kg"},"101349","0",null,"STK",{"$f":"VLOOKUP(G6051,sanschie!A:G,7,0)","v":59.8},{"$f":"IF(Daten!$E$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"101349"]
["Prima Plus",95,250,"Prima Plus 25095",null,{"$f":"VLOOKUP(G6055,sanschie!A:E,5,0)","v":"CHI 250 CHI Flexrohr 2 lagig Rolle a 5000mm"},"101384","0",null,"STK",{"$f":"VLOOKUP(G6055,sanschie!A:G,7,0)","v":1049},{"$f":"IF(Daten!$E$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"101384"]
["Prima Plus",96,250,"Prima Plus 25096",null,{"$f":"VLOOKUP(G6056,sanschie!A:E,5,0)","v":"CHI 250 Aufhängeschelle zu Flex"},"101392","0",null,"STK",{"$f":"VLOOKUP(G6056,sanschie!A:G,7,0)","v":51},{"$f":"IF(Daten!$E$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"101392"]
["Prima Plus",100,250,"Prima Plus 250100",null,{"$f":"VLOOKUP(G6060,sanschie!A:E,5,0)","v":"CHZ Mantelstein rund ØA 550mm Øi 390mm L330mm"},"103726","0",null,"STK",{"$f":"VLOOKUP(G6060,sanschie!A:G,7,0)","v":33},{"$f":"IF(Daten!$B$677=2,1,\"\")","v":""},null,null,null,null,null,null,null,"103726"]
["Prima Plus",101,250,"Prima Plus 250101",null,{"$f":"VLOOKUP(G6061,sanschie!A:E,5,0)","v":"CHZ Kaminmörtel Sack 25kg "},"103790","0",null,"STK",{"$f":"VLOOKUP(G6061,sanschie!A:G,7,0)","v":61},null,null,null,null,null,null,null,null,"103790"]
["Prima Plus",103,250,"Prima Plus 250103",null,{"$f":"VLOOKUP(G6063,sanschie!A:E,5,0)","v":"LBS 320 Leichtbauschacht i 320mm A 410mm L1000mm"},"103828","0",null,"STK",{"$f":"VLOOKUP(G6063,sanschie!A:G,7,0)","v":189},null,null,null,null,null,null,null,null,"103828"]
["Prima Plus",106,250,"Prima Plus 250106",null,{"$f":"VLOOKUP(G6066,sanschie!A:E,5,0)","v":"ABS Kaminhalterung Standard"},"104256","0",null,"STK",{"$f":"VLOOKUP(G6066,sanschie!A:G,7,0)","v":303},null,null,null,null,null,null,null,null,"104256"]
["Prima Plus",{"$f":"B6068+1","v":1},{"$f":"C6068","v":300},"Prima Plus 3001",null,"PPL 300 Kaminfuss 45° m.Stütze L240mm","100585","0",null,"STK",227,{"$f":"IF(Daten!$B$662=4,1,\"\")","v":""},{"$f":"IF(L6069=\"\",0,L6069*H6069)","v":0},null,null,{"$f":"IF(L6069=\"\",0,H6069*L6069)","v":0}]
["Prima Plus",3,300,"Prima Plus 3003",null,"PPL 300 Kondensattopf mit Ablauf seitlich","100601",70,null,"STK",141,{"$f":"IF(L6069=1,\"\",IF(L6069=1,\"\",1))","v":1},70,null,null,{"$f":"IF(L6071=\"\",0,H6071*L6071)","v":70}]
["Prima Plus",6,300,"Prima Plus 3006",null,"PPL 300 EW-DW Deckenanfängerset komplett L270mm","100654","0",null,"STK",595,null,0,null,null,{"$f":"IF(L6074=\"\",0,H6074*L6074)","v":0}]
["Prima Plus",9,300,"Prima Plus 3009",null,"PPL 300 Anschluss-Basiselement DN300 L450mm","100705",450,null,"STK",216,{"$f":"IF(Daten!$B$662=1,1,\"\")","v":""},0]
["Prima Plus",11,300,"Prima Plus 30011",null,"PPL 300 Anschluss glatt zu Basiselement L120mm","100721","0",null,"STK",151,{"$f":"IF(Daten!$B$662=1,1,\"\")","v":""},0,null,null,{"$f":"IF(L6079=\"\",0,H6079*L6079)","v":0}]
["Prima Plus",12,300,"Prima Plus 30012",null,"PPL 300 Anschluss-Doppelfutter zu Basiselement ","100728","0",null,"STK",205,null,0,null,null,{"$f":"IF(L6080=\"\",0,H6080*L6080)","v":0}]
["Prima Plus",16,300,"Prima Plus 30016",null,"PPL 300 Revisionsdeckel für Festbrennstoffe","100744","0",null,"STK",184,null,0]
["Prima Plus",18,300,"Prima Plus 30018",null,"PPL 180 Zugbergrenzer","100765","0",null,"STK",367,null,0,null,null,{"$f":"IF(L6086=\"\",0,H6086*L6086)","v":0}]
["Prima Plus",21,300,"Prima Plus 30021",null,"PPL Putztüre 150 x 200mm zu Putztüranschluss eckig","100783","0",null,"STK",108,{"$f":"IF(Daten!$B$670=1,\"\",IF(#REF!=\"\",\"\",Daten!$C$670))","v":""},0,null,null,0]
["Prima Plus",22,300,"Prima Plus 30022",null,"PPL Verlängerung zu Putztüre eckig  155 x 215mm ","100784","0",null,"STK",108,null,0,null,null,0]
["Prima Plus",26,300,"Prima Plus 30026",null,"PPL 150-700 Zuluft-Türe 200 x 300mm","100792","0",null,"STK",108,null,0,null,null,0]
["Prima Plus",27,300,"Prima Plus 30027",null,"PPL 300 T-Stück 85° L450mm","100801",450,null,"STK",237,null,{"$f":"IF(L6095=\"\",0,L6095*H6095)","v":0},null,null,0]
["Prima Plus",31,300,"Prima Plus 30031",null,"PPL 300 Doppelfutterrohr zu T-Stück L120mm","100845","0",null,"STK",86,null,0,null,null,0]
["Prima Plus",32,300,"Prima Plus 30032",null,"PPL 300 Längenelement L250mm","100853",200,null,"STK",55,{"$f":"IF(N6100=0,\"\",N6100)","v":""},0,{"$f":"IF('PRIMA PLUS'!$P$18=\"\",0,IF('PRIMA PLUS'!$P$18=0,0,'PRIMA PLUS'!$P$18))","v":0},null,0]
["Prima Plus",34,300,"Prima Plus 30034",null,"PPL 300 Längenelement L1000mm","100881",950,null,"STK",142,{"$f":"ROUNDUP(M6102,0)","v":9},{"$f":"(M6068-(SUM(M6069:M6101))-(SUM(M6103:M6110)))/H6102","v":8.8210526315789473},null,null,8550]
["Prima Plus",37,300,"Prima Plus 30037",null,"PPL 300 Empa Messtutzen L450mm","140749","0",null,"STK",325,null,{"$f":"IF(L6105=\"\",0,L6105*H6105)","v":0},null,null,0]
["Prima Plus",40,300,"Prima Plus 30040",null,"PPL 300 Schiebe-Element 270-415mm","100931","0",null,"STK",129,null,{"$f":"IF(L6108=\"\",0,L6108*H6108)","v":0}]
["Prima Plus",42,300,"Prima Plus 30042",null,"PPL 300 Revisions-Basiselement mit Kondensatfalle ","100959",450,null,"STK",227,null,{"$f":"IF(L6110=\"\",0,L6110*H6110)","v":0},null,null,{"$f":"IF(L6110=\"\",0,H6110*L6110)","v":0}]
["Prima Plus",45,300,{"$f":"A6113&\" \"&C6113&B6113","v":"Prima Plus 30045"},null,"ICM 250 Klemmband DN300","102267","0",null,"STK",21]
["Prima Plus",48,300,{"$f":"A6116&\" \"&C6116&B6116","v":"Prima Plus 30048"},null,"PPL 300 Winkel 30°","101024","0",null,"STK",98]
["Prima Plus",50,300,"Prima Plus 30050",null,"PPL 300 Winkel 85°","101052","0",null,"STK",152]
["Prima Plus",51,300,"Prima Plus 30051",null,"PPL 300 Winkel 90°","101066","0",null,"STK",152]
["Prima Plus",55,300,"Prima Plus 30055",null,"PPL 300 Winkel 0-90° verstellbar  Trockenbetrieb  ","101100","0",null,"STK",108]
["Prima Plus",57,300,"Prima Plus 30057",null,"PPL 300 Kesselanschluss DN + 6mm L150mm","101115","0",null,"STK",108]
["Prima Plus",60,300,"Prima Plus 30060",null,"PPL 300 Abgasschalldämpfer Schallred. 15DB L760mm","101163","0",null,"STK",1999]
["Prima Plus",62,300,"Prima Plus 30062",null,"PPL 300 Schallabsorber Oel-Gas","101175","0",null,"STK",237]
["Prima Plus",65,300,"Prima Plus 30065",null,"ICM 300 Anschluss von DW auf EW in Rauchgasr.","102177","0",null,"STK",174]
["Prima Plus",66,300,"Prima Plus 30066",null,"PPL 300 Anschlussrosette ØA 470mm","101191","0",null,"STK",71]
["Prima Plus",68,300,"Prima Plus 30068",null,"ICM W1 Verlängerung zu Wandhalter 50mm L 130mm","102317","0",null,"STK",44]
["Prima Plus",71,300,"Prima Plus 30071",null,"ICM L3 Verlängerung zu Wandhalter 50mm L 550mm","102321","0",null,"STK",163]
["Prima Plus",73,300,"Prima Plus 30073",null,"ICM 250 Wandhalter verstellbar 75 - 300mm DN 300mm","102295","0",null,"STK",87]
["Prima Plus",{"$f":"B6143+1","v":76},{"$f":"C6143","v":300},"Prima Plus 30076",null,"PPL Muffe 1/2\" zu Grundplatte 1/2\" Wandabst. 50mm","101205","0",null,"STK",20]
["Prima Plus",{"$f":"B6146+1","v":79},{"$f":"C6146","v":300},{"$f":"A6147&\" \"&C6147&B6147","v":"Prima Plus 30079"},null,"PPL Schachtabdeckung Typ4 500 x 500mm","101275","0",null,"STK",151,{"$f":"IF(L6148=1,1,\"\")","v":1}]
["Prima Plus",81,300,"Prima Plus 30081",null,"PPL 300 Regenhaube ","101314","0",null,"STK",141,{"$f":"IF(Daten!$B$677=2,1,\"\")","v":""}]
["Prima Plus",84,300,"Prima Plus 30084",null,"PPL 300 Basten Stand. Kupfer mit Dila Isol 30mm","140892","0",null,"STK",503]
["Prima Plus",87,300,"Prima Plus 30087",null,"PPL 300 Dämmschale 30mm Alu-Kaschiert L1000mm","101329","0",null,"STK",62,{"$f":"IF(Daten!$B$677=2,1,\"\")","v":""}]
["Prima Plus",89,300,"Prima Plus 30089",null,"CHZ Mantelstein EZ  480 x 480mm L330mm Ø250mm","103722","0",null,"STK",24]
["Prima Plus",90,300,"Prima Plus 30090",null,"CHZ Mantelstein EZ  550 x 550mm L330mm Ø300mm","103723","0",null,"STK",30]
[{"$f":"A6161","v":"Prima Plus"},94,300,"Prima Plus 30094",null,"LBS Kleber zu Leichtbauschacht 1kg","103829","0",null,"STK",9]
[{"$f":"A6163","v":"Prima Plus"},96,300,"Prima Plus 30096",null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",81]
["Prima Plus",2,350,"Prima Plus 3502",null,"PPL 350 Konsolenbleche für Zwischenstütze (Paar)","100614","0",null,"STK",194,null,{"$f":"IF(L6167=\"\",0,L6167*H6167)","v":0}]
["Prima Plus",{"$f":"B6169+1","v":5},{"$f":"C6169","v":350},"Prima Plus 3505",null,"PPL 350 Revisions-Basiselement für Deckel DN300 ","100710",450,null,"STK",324,{"$f":"Daten!C654","v":1},{"$f":"IF(L6170=\"\",0,L6170*H6170)","v":450},null,null,{"$f":"IF(L6170=\"\",0,L6170*H6170)","v":450}]
["Prima Plus",7,350,"Prima Plus 3507",null,"PPL 300 Revisionsdeckel für Festbrennstoffe","100744","0",null,"STK",184,{"$f":"IF(Daten!$B$644=1,Daten!$C$654,\"\")","v":1},0]
["Prima Plus",8,350,"Prima Plus 3508",null,"PPL 350 Verschlussdeckel mit Griff","100753","0",null,"STK",129,null,0]
["Prima Plus",10,350,"Prima Plus 35010",null,"PPL Putztüre 150 x 200mm zu Putztüranschluss eckig","100783","0",null,"STK",108,{"$f":"IF(Daten!$B$670=1,\"\",Daten!$C$670)","v":""},0,null,null,0]
["Prima Plus",13,350,"Prima Plus 35013",null,"PPL 150-700 Montagerahmen L250mm","100790","0",null,"STK",97,null,0,null,null,0]
["Prima Plus",15,350,"Prima Plus 35015",null,"PPL 350 T-Stück 90° L450mm","100810",450,null,"STK",324,{"$f":"IF(N6180=\"\",\"\",N6180)","v":1},{"$f":"IF(N6180=\"\",0,N6180*H6180)","v":450},{"$f":"IF(Daten!$B$662=1,1,IF(Daten!$B$662=2,1,\"\"))","v":1},null,{"$f":"IF(N6180=\"\",0,H6180*N6180)","v":450}]
["Prima Plus",18,350,"Prima Plus 35018",null,"PPL 350 Längenelement L500mm","100868",450,null,"STK",120,{"$f":"1+N6183","v":1},{"$f":"IF(L6183=\"\",0,L6183*H6183)","v":450},{"$f":"IF('PRIMA PLUS'!$P$17=\"\",0,IF('PRIMA PLUS'!$P$17=0,0,'PRIMA PLUS'!$P$17))","v":0},null,450]
["Prima Plus",21,350,"Prima Plus 35021",null,"PPL 350 Element mit 3 Messöffnungen 3/4\" L150mm","100910","0",null,"STK",184,null,{"$f":"IF(L6186=\"\",0,L6186*H6186)","v":0},null,null,{"$f":"IF(L6186=\"\",0,H6186*L6186)","v":0}]
["Prima Plus",23,350,"Prima Plus 35023",null,"PPL 350 Schiebe-Element 270-415mm","100932","0",null,"STK",162,null,{"$f":"IF(L6188=\"\",0,L6188*H6188)","v":0}]
["Prima Plus",27,350,"Prima Plus 35027",null,"PPL 350 Klemmband","100983","0",null,"STK",16,{"$f":"L6193","v":""}]
["Prima Plus",28,350,"Prima Plus 35028",null,"PPL 350 Dichtung Viton","100997","0",null,"STK",27,{"$f":"IF(N6193=\"\",\"\",N6193)","v":""},null,{"$f":"IF(Daten!$B$644=1,\"\",O6193)","v":""},{"$f":"SUM(L6166,L6170,N6180,L6181,L6182,L6183,L6184,L6185)","v":14}]
["Prima Plus",31,350,"Prima Plus 35031",null,"PPL 350 Winkel 45°","101039","0",null,"STK",163]
["Prima Plus",32,350,"Prima Plus 35032",null,"PPL 350 Winkel 85°","101053","0",null,"STK",195]
["Prima Plus",36,350,"Prima Plus 35036",null,"ICM 300 Wandhalter 50mm verlängerbar DN 350mm ","102310","0",null,"STK",87]
["Prima Plus",38,350,"Prima Plus 35038",null,"PPL Innengewinderohr zu Rohrschelle 1/2\" 1000mm","101204","0",null,"STK",147]
["Prima Plus",41,350,"Prima Plus 35041",null,"PPL 350 Regenkragen ","101266","0",null,"STK",76]
["Prima Plus",2,400,"Prima Plus 4002",null,"PPL 400 Konsolenbleche für Zwischenstütze (Paar)","100615","0",null,"STK",216,null,{"$f":"IF(L6209=\"\",0,L6209*H6209)","v":0}]
["Prima Plus",4,400,"Prima Plus 4004",null,"PPL 400 Kondensattopf mit Ablauf senkrecht","100643",48,null,"STK",162,null,{"$f":"IF(L6211=\"\",0,L6211*H6211)","v":0},null,null,{"$f":"IF(L6211=\"\",0,H6211*L6211)","v":0}]
["Prima Plus",7,400,"Prima Plus 4007",null,"PPL 300 Revisionsdeckel für Festbrennstoffe","100744","0",null,"STK",184,{"$f":"IF(Daten!$B$644=1,Daten!$C$654,\"\")","v":1},0]
["Prima Plus",9,400,"Prima Plus 4009",null,"PPL 400 Putztüranschluss eckig mit Innentüre ","100778",325,null,"STK",379,null,0,null,null,{"$f":"IF(L6216=\"\",0,H6216*L6216)","v":0}]
["Prima Plus",10,400,"Prima Plus 40010",null,"PPL Putztüre 150 x 200mm zu Putztüranschluss eckig","100783","0",null,"STK",108,{"$f":"IF(Daten!$B$670=1,\"\",Daten!$C$670)","v":""},0,null,null,0]
["Prima Plus",13,400,"Prima Plus 40013",null,"PPL 150-700 Montagerahmen L250mm","100790","0",null,"STK",97,null,0,null,null,0]
["Prima Plus",15,400,"Prima Plus 40015",null,"PPL 400 T-Stück 90° L530mm","100811",530,null,"STK",487,{"$f":"IF(N6222=\"\",\"\",N6222)","v":1},{"$f":"IF(N6222=\"\",0,N6222*H6222)","v":530},{"$f":"IF(Daten!$B$662=1,1,IF(Daten!$B$662=2,1,\"\"))","v":1},null,{"$f":"IF(N6222=\"\",0,H6222*N6222)","v":530}]
["Prima Plus",18,400,"Prima Plus 40018",null,"PPL 400 Längenelement L500mm","100869",450,null,"STK",142,{"$f":"1+N6225","v":1},{"$f":"IF(L6225=\"\",0,L6225*H6225)","v":450},{"$f":"IF('PRIMA PLUS'!$P$17=\"\",0,IF('PRIMA PLUS'!$P$17=0,0,'PRIMA PLUS'!$P$17))","v":0},null,450]
["Prima Plus",{"$f":"B6226+1","v":20},{"$f":"C6226","v":400},{"$f":"A6227&\" \"&C6227&B6227","v":"Prima Plus 40020"},null,"PPL 400 Ablass-Element L200mm","100897",200,null,"STK",162,1,{"$f":"IF(L6227=\"\",0,L6227*H6227)","v":200},null,null,200]
["Prima Plus",24,400,"Prima Plus 40024",null,"PPL 400 Kondensatabscheider L150mm","100969","0",null,"STK",249,null,null,null,null,{"$f":"IF(L6231=\"\",0,H6231*L6231)","v":0}]
["Prima Plus",25,400,"Prima Plus 40025",null,"PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7]
["Prima Plus",27,400,"Prima Plus 40027",null,"PPL 400 Dichtung Silikon","100998","0",null,"STK",29,{"$f":"IF(N6234=\"\",\"\",N6234)","v":""},null,{"$f":"IF(Daten!$B$644=1,\"\",O6234)","v":""},{"$f":"SUM(L6208,L6212,N6222,L6223,L6224,L6225,L6226,L6227)","v":14}]
["Prima Plus",30,400,"Prima Plus 40030",null,"PPL 400 Winkel 45°","101040","0",null,"STK",271]
["Prima Plus",33,400,{"$f":"A6240&\" \"&C6240&B6240","v":"Prima Plus 40033"},null,"ICM 400 Anschluss von EW auf DW in Rauchgasr.","102155","0",null,"STK",315]
["Prima Plus",35,400,{"$f":"A6242&\" \"&C6242&B6242","v":"Prima Plus 40035"},null,"PPL 400 Regenkragen ","101267","0",null,"STK",108]
["Prima Plus",2,450,"Prima Plus 4502",null,"PPL 450 Konsolenbleche für Zwischenstütze (Paar)","100616","0",null,"STK",270,null,{"$f":"IF(L6245=\"\",0,L6245*H6245)","v":0}]
["Prima Plus",5,450,"Prima Plus 4505",null,"PPL 450 Revisions-Basiselement für Deckel DN300 ","100712",450,null,"STK",540,{"$f":"Daten!C728","v":0},{"$f":"IF(L6248=\"\",0,L6248*H6248)","v":0},null,null,{"$f":"IF(L6248=\"\",0,L6248*H6248)","v":0}]
["Prima Plus",7,450,"Prima Plus 4507",null,"PPL 300 Revisionsdeckel für Festbrennstoffe","100744","0",null,"STK",184,{"$f":"IF(Daten!$B$644=1,Daten!$C$654,\"\")","v":1},0]
["Prima Plus",8,450,"Prima Plus 4508",null,"PPL 450 Verschlussdeckel mit Griff","100755","0",null,"STK",216,null,0]
["Prima Plus",12,450,"Prima Plus 45012",null,"PPL 150-700 Putztüre 200 x 300mm gasdicht","100788","0",null,"STK",141,null,0,null,null,0]
["Prima Plus",13,450,"Prima Plus 45013",null,"PPL 150-700 Montagerahmen L250mm","100790","0",null,"STK",97,null,0,null,null,0]
["Prima Plus",16,450,"Prima Plus 45016",null,"PPL 450 T-Stück 45° L780mm","100834",780,null,"STK",1027,{"$f":"IF(Daten!$B$662=3,1,\"\")","v":""},{"$f":"IF(L6259=\"\",0,L6259*H6259)","v":0},null,null,{"$f":"IF(L6259=\"\",0,H6259*L6259)","v":0}]
["Prima Plus",18,450,"Prima Plus 45018",null,"PPL 450 Längenelement L500mm","100870",450,null,"STK",174,{"$f":"1+N6261","v":1},{"$f":"IF(L6261=\"\",0,L6261*H6261)","v":450},{"$f":"IF('PRIMA PLUS'!$P$17=\"\",0,IF('PRIMA PLUS'!$P$17=0,0,'PRIMA PLUS'!$P$17))","v":0},null,450]
["Prima Plus",21,450,"Prima Plus 45021",null,"PPL 450 Element mit 3 Messöffnungen 3/4\" L150mm","100912","0",null,"STK",249,null,{"$f":"IF(L6264=\"\",0,L6264*H6264)","v":0},null,null,0]
["Prima Plus",23,450,"Prima Plus 45023",null,"PPL 450 Endrohr mit beidseitiger Muffe L1000mm","100948",950,null,"STK",292,null,{"$f":"IF(L6266=\"\",0,L6266*H6266)","v":0},null,null,{"$f":"IF(L6266=\"\",0,H6266*L6266)","v":0}]
["Prima Plus",27,450,"Prima Plus 45027",null,"PPL 450 Dichtung Silikon","100999","0",null,"STK",31,{"$f":"IF(N6270=\"\",\"\",N6270)","v":""},null,{"$f":"IF(Daten!$B$644=1,\"\",O6270)","v":""},{"$f":"SUM(L6244,L6248,N6258,L6259,L6260,L6261,L6262,L6263)","v":14}]
["Prima Plus",28,450,"Prima Plus 45028",null,"PPL 450 Winkel 15°","101013","0",null,"STK",325]
["Prima Plus",30,450,"Prima Plus 45030",null,"PPL 450 Winkel 45°","101041","0",null,"STK",380]
["Prima Plus",33,450,"Prima Plus 45033",null,"ICM 450 Anschluss von EW auf DW in Rauchgasr.","102156","0",null,"STK",368]
["Prima Plus",0,500,"Prima Plus 5000"," ","Schiedel Prima Plus 0,6mm Ø 500","PRIMA PLUS 500","0",{"$f":"'PRIMA PLUS'!$J$11","v":10},"Anlage",0,1,{"$f":"I6279*1000","v":10000},null,{"$f":"ROUNDUP(P6279,2)","v":10.85},{"$f":"SUM(P6280:P6314)/1000","v":10.85}]
["Prima Plus",2,500,"Prima Plus 5002",null,"PPL 500 Konsolenbleche für Zwischenstütze (Paar)","100617","0",null,"STK",346,null,{"$f":"IF(L6281=\"\",0,L6281*H6281)","v":0}]
["Prima Plus",5,500,"Prima Plus 5005",null,"PPL 500 Revisions-Basiselement für Deckel DN300 ","100713",450,null,"STK",648,{"$f":"Daten!C765","v":0},{"$f":"IF(L6284=\"\",0,L6284*H6284)","v":0},null,null,{"$f":"IF(L6284=\"\",0,L6284*H6284)","v":0}]
["Prima Plus",8,500,"Prima Plus 5008",null,"PPL 500 Verschlussdeckel mit Griff","100756","0",null,"STK",270,null,0]
["Prima Plus",10,500,"Prima Plus 50010",null,"PPL Putztüre 150 x 200mm zu Putztüranschluss eckig","100783","0",null,"STK",108,{"$f":"IF(Daten!$B$670=1,\"\",Daten!$C$670)","v":""},0,null,null,0]
["Prima Plus",11,500,"Prima Plus 50011",null,"PPL Verlängerung zu Putztüre eckig  155 x 215mm ","100784","0",null,"STK",108,null,0,null,null,0]
["Prima Plus",15,500,"Prima Plus 50015",null,"PPL 500 T-Stück 90° L630mm","100813",630,null,"STK",757,{"$f":"IF(N6294=\"\",\"\",N6294)","v":1},{"$f":"IF(N6294=\"\",0,N6294*H6294)","v":630},{"$f":"IF(Daten!$B$662=1,1,IF(Daten!$B$662=2,1,\"\"))","v":1},null,{"$f":"IF(N6294=\"\",0,H6294*N6294)","v":630}]
["Prima Plus",16,500,"Prima Plus 50016",null,"PPL 500 T-Stück 45° L850mm","100835",850,null,"STK",1244,{"$f":"IF(Daten!$B$662=3,1,\"\")","v":""},{"$f":"IF(L6295=\"\",0,L6295*H6295)","v":0},null,null,{"$f":"IF(L6295=\"\",0,H6295*L6295)","v":0}]
["Prima Plus",20,500,"Prima Plus 50020",null,"PPL 500 Ablass-Element L200mm","100899",200,null,"STK",237,1,{"$f":"IF(L6299=\"\",0,L6299*H6299)","v":200},null,null,200]
["Prima Plus",21,500,"Prima Plus 50021",null,"PPL 500 Element mit 3 Messöffnungen 3/4\" L150mm","100913","0",null,"STK",292,null,{"$f":"IF(L6300=\"\",0,L6300*H6300)","v":0},null,null,0]
["Prima Plus",25,500,"Prima Plus 50025",null,"PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7]
["Prima Plus",26,500,"Prima Plus 50026",null,"PPL 500 Klemmband","100986","0",null,"STK",39,{"$f":"L6306","v":""}]
["Prima Plus",30,500,"Prima Plus 50030",null,"PPL 500 Winkel 45°","101042","0",null,"STK",433]
["Prima Plus",31,500,"Prima Plus 50031",null,"PPL 500 Winkel 85°","101056","0",null,"STK",704]
["Prima Plus",33,500,{"$f":"A6312&\" \"&C6312&B6312","v":"Prima Plus 50033"},null,"ICM 500 Anschluss von EW auf DW in Rauchgasr.","102157","0",null,"STK",423]
["Prima Plus",0,600,"Prima Plus 6000"," ","Schiedel Prima Plus 0,6mm Ø 600","PRIMA PLUS 600","0",{"$f":"'PRIMA PLUS'!$J$11","v":10},"Anlage",0,1,{"$f":"I6315*1000","v":10000},null,{"$f":"ROUNDUP(P6315,2)","v":10},{"$f":"SUM(P6316:P6351)/1000","v":10}]
["Prima Plus",3,600,"Prima Plus 6003",null,"PPL 600 Zwischenstütze","100632",100,null,"STK",379,null,{"$f":"IF(L6318=\"\",0,L6318*H6318)","v":0},null,null,{"$f":"IF(L6318=\"\",0,H6318*L6318)","v":0}]
["Prima Plus",5,600,"Prima Plus 6005",null,"PPL 600 Revisions-Basiselement für Deckel DN300 ","100714",450,null,"STK",811,{"$f":"Daten!C802","v":0},{"$f":"IF(L6320=\"\",0,L6320*H6320)","v":0},null,null,{"$f":"IF(L6320=\"\",0,L6320*H6320)","v":0}]
["Prima Plus",8,600,"Prima Plus 6008",null,"PPL 600 Verschlussdeckel mit Griff","100757","0",null,"STK",324,null,0]
["Prima Plus",11,600,"Prima Plus 60011",null,"PPL Verlängerung zu Putztüre eckig  155 x 215mm ","100784","0",null,"STK",108,null,0,null,null,0]
["Prima Plus",13,600,"Prima Plus 60013",null,"PPL 150-700 Montagerahmen L250mm","100790","0",null,"STK",97,null,0,null,null,0]
["Prima Plus",14,600,"Prima Plus 60014",null,"PPL 150-700 Zuluft-Türe 200 x 300mm","100792","0",null,"STK",108,null,0,null,null,0]
["Prima Plus",18,600,"Prima Plus 60018",null,"PPL 600 Längenelement L500mm","100872",450,null,"STK",282,{"$f":"1+N6333","v":1},{"$f":"IF(L6333=\"\",0,L6333*H6333)","v":450},{"$f":"IF('PRIMA PLUS'!$P$17=\"\",0,IF('PRIMA PLUS'!$P$17=0,0,'PRIMA PLUS'!$P$17))","v":0},null,450]
["Prima Plus",19,600,"Prima Plus 60019",null,"PPL 600 Längenelement L1000mm","100886",950,null,"STK",433,{"$f":"ROUNDUP(M6334,0)","v":9},{"$f":"(M6315-(SUM(M6316:M6333))-(SUM(M6335:M6339)))/H6334","v":9},null,null,8550]
["Prima Plus",23,600,"Prima Plus 60023",null,"PPL 600 Endrohr mit beidseitiger Muffe L1000mm","100950",950,null,"STK",432,null,{"$f":"IF(L6338=\"\",0,L6338*H6338)","v":0},null,null,{"$f":"IF(L6338=\"\",0,H6338*L6338)","v":0}]
["Prima Plus",24,600,"Prima Plus 60024",null,"PPL 600 Kondensatabscheider L150mm","100972","0",null,"STK",379,null,null,null,null,{"$f":"IF(L6339=\"\",0,H6339*L6339)","v":0}]
["Prima Plus",28,600,"Prima Plus 60028",null,"PPL 600 Winkel 15°","101015","0",null,"STK",488]
["Prima Plus",29,600,"Prima Plus 60029",null,"PPL 600 Winkel 30°","101029","0",null,"STK",509]
["Prima Plus",33,600,"Prima Plus 60033",null,"ICM 600 Anschluss von EW auf DW in Rauchgasr.","102158","0",null,"STK",531]
["Prima Plus",34,600,"Prima Plus 60034",null,"ICM 600 Anschluss von DW auf EW in Rauchgasr.","102182","0",null,"STK",531]
["Prima Plus",36,600,"Prima Plus 60036",null,"PPL 600 Regenkragen ","101270","0",null,"STK",173]
["Prima Plus",2,700,"Prima Plus 7002",null,"PPL 700 Konsolenbleche für Zwischenstütze (Paar)","100619","0",null,"STK",540,null,{"$f":"IF(L6354=\"\",0,L6354*H6354)","v":0}]
["Prima Plus",5,700,"Prima Plus 7005",null,"PPL 700 Revisions-Basiselement für Deckel DN300 ","100715",450,null,"STK",1027,{"$f":"Daten!C839","v":0},{"$f":"IF(L6357=\"\",0,L6357*H6357)","v":0},null,null,{"$f":"IF(L6357=\"\",0,L6357*H6357)","v":0}]
["Prima Plus",7,700,"Prima Plus 7007",null,"PPL 300 Revisionsdeckel für Festbrennstoffe","100744","0",null,"STK",184,{"$f":"IF(Daten!$B$644=1,Daten!$C$654,\"\")","v":1},0]
["Prima Plus",10,700,"Prima Plus 70010",null,"PPL Putztüre 150 x 200mm zu Putztüranschluss eckig","100783","0",null,"STK",108,{"$f":"IF(Daten!$B$670=1,\"\",Daten!$C$670)","v":""},0,null,null,0]
["Prima Plus",13,700,"Prima Plus 70013",null,"PPL 150-700 Montagerahmen L250mm","100790","0",null,"STK",97,null,0,null,null,0]
["Prima Plus",15,700,"Prima Plus 70015",null,"PPL 700 T-Stück 90° L830mm","100815",830,null,"STK",1189,{"$f":"IF(N6367=\"\",\"\",N6367)","v":1},{"$f":"IF(N6367=\"\",0,N6367*H6367)","v":830},{"$f":"IF(Daten!$B$662=1,1,IF(Daten!$B$662=2,1,\"\"))","v":1},null,{"$f":"IF(N6367=\"\",0,H6367*N6367)","v":830}]
["Prima Plus",16,700,"Prima Plus 70016",null,"PPL 700 T-Stück 45° L1200mm","100837",1200,null,"STK",1893,{"$f":"IF(Daten!$B$662=3,1,\"\")","v":""},{"$f":"IF(L6368=\"\",0,L6368*H6368)","v":0},null,null,{"$f":"IF(L6368=\"\",0,H6368*L6368)","v":0}]
["Prima Plus",20,700,"Prima Plus 70020",null,"PPL 700 Ablass-Element L200mm","100901",200,null,"STK",324,1,{"$f":"IF(L6372=\"\",0,L6372*H6372)","v":200},null,null,200]
["Prima Plus",22,700,"Prima Plus 70022",null,"PPL 700 Schiebe-Element 100-400mm","100937","0",null,"STK",379,null,{"$f":"IF(L6374=\"\",0,L6374*H6374)","v":0}]
["Prima Plus",25,700,"Prima Plus 70025",null,"PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7]
["Prima Plus",27,700,"Prima Plus 70027",null,"PPL 700 Dichtung Silikon","101002","0",null,"STK",44,{"$f":"IF(N6379=\"\",\"\",N6379)","v":""},null,{"$f":"IF(Daten!$B$644=1,\"\",O6379)","v":""},{"$f":"SUM(L6353,L6357,N6367,L6368,L6369,L6370,L6371,L6372)","v":13}]
["Prima Plus",30,700,"Prima Plus 70030",null,"PPL 700 Winkel 45°","101044","0",null,"STK",596]
["Prima Plus",31,700,"Prima Plus 70031",null,"PPL 700 Winkel 85°","101058","0",null,"STK",1082]
["Prima Plus",33,700,{"$f":"A6385&\" \"&C6385&B6385","v":"Prima Plus 70033"},null,"ICM 700 Anschluss von EW auf DW in Rauchgasr.","102159","0",null,"STK",747]
["Prima Plus",36,700,{"$f":"A6388&\" \"&C6388&B6388","v":"Prima Plus 70036"},null,"PPL 700 Regenkragen ","101271","0",null,"STK",216]
[{"$f":"A6389","v":"VL-PPL 0,6 Ø 80"},{"$f":"B6389+1","v":1},{"$f":"C6389","v":80},{"$f":"A6390&B6390","v":"VL-PPL 0,6 Ø 801"}," ","PPL 80 Revisions.-und Anschluss-Basiselement DN80 ","100698","0",null,"STK",76]
["VL-PPL 0,6 Ø 80",4,80,"VL-PPL 0,6 Ø 804"," ","PPL 80 Verschlussdeckel mit Griff","100745","0",null,"STK",43]
["VL-PPL 0,6 Ø 80",7,80,"VL-PPL 0,6 Ø 807"," ","PPL 80 Längenelement L1000mm","100874","0",null,"STK",50]
["VL-PPL 0,6 Ø 80",9,80,"VL-PPL 0,6 Ø 809"," ","PPL 80 Endrohr mit beidseitiger Muffe L1000mm","100938","0",null,"STK",54]
["VL-PPL 0,6 Ø 80",13,80,"VL-PPL 0,6 Ø 8013"," ","PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7]
["VL-PPL 0,6 Ø 80",14,80,"VL-PPL 0,6 Ø 8014"," ","PPL 80 Klemmband","100975","0",null,"STK",10]
["VL-PPL 0,6 Ø 80",17,80,"VL-PPL 0,6 Ø 8017"," ","PPL 80 Winkel 15°","101003","0",{"$f":"IF(VLOOKUP(G6406,sanschie!B:J,9,)=0,\"0\",VLOOKUP(G6406,sanschie!B:J,9,0))","v":{"$error":"#N/A"}},"STK",39]
["VL-PPL 0,6 Ø 80",18,80,"VL-PPL 0,6 Ø 8018"," ","PPL 80 Winkel 30°","101017","0",null,"STK",39]
["VL-PPL 0,6 Ø 80",22,80,"VL-PPL 0,6 Ø 8022"," ","PPL 80 Winkel 85° mit Revisionsöffnung","101073","0",null,"STK",108]
["VL-PPL 0,6 Ø 80",24,80,"VL-PPL 0,6 Ø 8024"," ","PPL 80 Kesselanschluss DN + 6mm L150mm","101107","0",null,"STK",43]
["VL-PPL 0,6 Ø 80",27,80,"VL-PPL 0,6 Ø 8027"," ","PPL 80 Wandhalter 50mm fix DN 80mm","101207","0",null,"STK",38]
["VL-PPL 0,6 Ø 80",29,80,"VL-PPL 0,6 Ø 8029",null,"PPL 80 Rohrschelle  Anschluss 1/2\" Aussengewinde","101193","0",null,"STK",20]
["VL-PPL 0,6 Ø 80",32,80,"VL-PPL 0,6 Ø 8032",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25]
["VL-PPL 0,6 Ø 100",0,100,{"$f":"A6422&B6422","v":"VL-PPL 0,6 Ø 1000"}," ","Schiedel VL-Prima 0,6 mm Ø 100","VL-PPL 0,6 Ø 100","0",null,"Anlage",0]
["VL-PPL 0,6 Ø 100",2,100,"VL-PPL 0,6 Ø 1002"," ","PPL 100 Revisionsdeckel für Oel/Gas ","100730","0",null,"STK",38]
["VL-PPL 0,6 Ø 100",5,100,"VL-PPL 0,6 Ø 1005"," ","PPL 100 Längenelement L250mm","100847","0",null,"STK",22]
["VL-PPL 0,6 Ø 100",7,100,"VL-PPL 0,6 Ø 1007"," ","PPL 100 Längenelement L1000mm","100875","0",null,"STK",60]
["VL-PPL 0,6 Ø 100",10,100,"VL-PPL 0,6 Ø 10010"," ","PPL 100 Revisions-Basiselement mit Kondensatfalle ","100953","0",null,"STK",119]
["VL-PPL 0,6 Ø 100",13,100,"VL-PPL 0,6 Ø 10013"," ","PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7]
["VL-PPL 0,6 Ø 100",15,100,"VL-PPL 0,6 Ø 10015"," ","PPL 100 Dichtung Viton","100990","0",null,"STK",13]
["VL-PPL 0,6 Ø 100",19,100,"VL-PPL 0,6 Ø 10019"," ","PPL 100 Winkel 45°","101032","0",null,"STK",50]
["VL-PPL 0,6 Ø 100",20,100,"VL-PPL 0,6 Ø 10020"," ","PPL 100 Winkel 85°","101046","0",null,"STK",60]
["VL-PPL 0,6 Ø 100",23,100,"VL-PPL 0,6 Ø 10023"," ","PPL 100 Winkel 90° mit Revisionsöffnung","101082","0",null,"STK",129]
["VL-PPL 0,6 Ø 100",24,100,"VL-PPL 0,6 Ø 10024"," ","PPL 100 Kesselanschluss DN + 6mm L150mm","101108","0",null,"STK",54]
["VL-PPL 0,6 Ø 100",28,100,"VL-PPL 0,6 Ø 10028"," ","PPL 100 Schallabsorber Festbrennstoffe","101176","0",null,"STK",97]
["VL-PPL 0,6 Ø 100",30,100,"VL-PPL 0,6 Ø 10030"," ","CHI 100 Aufhängeschelle zu Flex","101387","0",null,"STK",27]
["VL-PPL 0,6 Ø 100",33,100,"VL-PPL 0,6 Ø 10033",null,"PPL Muffe 1/2\" zu Grundplatte 1/2\" Wandabst. 50mm","101205","0",null,"STK",20]
[{"$f":"A6457","v":"VL-PPL 0,6 Ø 130"},{"$f":"B6457+1","v":1},{"$f":"C6457","v":130},"VL-PPL 0,6 Ø 1301"," ","PPL 130 Revisions-und Anschluss-Basiselement DN130","100700","0",null,"STK",97]
["VL-PPL 0,6 Ø 130",3,130,"VL-PPL 0,6 Ø 1303"," ","PPL 130 Revisionsdeckel für Festbrennstoffe","100739","0",null,"STK",64]
["VL-PPL 0,6 Ø 130",6,130,"VL-PPL 0,6 Ø 1306"," ","PPL 130 Längenelement L250mm","100848","0",null,"STK",28]
["VL-PPL 0,6 Ø 130",8,130,"VL-PPL 0,6 Ø 1308"," ","PPL 130 Längenelement L1000mm","100876","0",null,"STK",72]
["VL-PPL 0,6 Ø 130",9,130,"VL-PPL 0,6 Ø 1309"," ","PPL 130 Schiebe-Element 270-415mm","100926","0",null,"STK",76]
["VL-PPL 0,6 Ø 130",11,130,"VL-PPL 0,6 Ø 13011"," ","PPL 130 Revisions-Basiselement mit Kondensatfalle ","100954","0",null,"STK",129]
["VL-PPL 0,6 Ø 130",14,130,"VL-PPL 0,6 Ø 13014"," ","PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7]
["VL-PPL 0,6 Ø 130",17,130,"VL-PPL 0,6 Ø 13017"," ","TS120 Gleitmittel 250ml","100275","0",null,"STK",15.6]
["VL-PPL 0,6 Ø 130",19,130,"VL-PPL 0,6 Ø 13019"," ","PPL 130 Winkel 30°","101019","0",null,"STK",50]
["VL-PPL 0,6 Ø 130",23,130,"VL-PPL 0,6 Ø 13023"," ","PPL 130 Winkel 85° mit Revisionsöffnung","101075","0",null,"STK",151]
["VL-PPL 0,6 Ø 130",24,130,"VL-PPL 0,6 Ø 13024"," ","PPL 130 Winkel 90° mit Revisionsöffnung","101083","0",null,"STK",151]
["VL-PPL 0,6 Ø 130",26,130,"VL-PPL 0,6 Ø 13026"," ","PPL 130 Winkel 0-90° verstellbar  Trockenbetrieb  ","101095","0",null,"STK",54]
["VL-PPL 0,6 Ø 130",29,130,"VL-PPL 0,6 Ø 13029",null,"PPL 130 Erweiterung DN180 L150mm","101123","0",null,"STK",108]
["VL-PPL 0,6 Ø 130",32,130,"VL-PPL 0,6 Ø 13032"," ","PPL 130 Schallabsorber Oel-Gas","101170","0",null,"STK",141]
["VL-PPL 0,6 Ø 130",34,130,"VL-PPL 0,6 Ø 13034"," ","ICS 80 Wandhalter verstellbar 75 - 300mm DN130mm","102289","0",null,"STK",55]
["VL-PPL 0,6 Ø 130",37,130,"VL-PPL 0,6 Ø 13037",null,"PPL Innengewinderohr zu Rohrschelle 1/2\" 1000mm","101204","0",null,"STK",147]
["VL-PPL 0,6 Ø 150",0,150,{"$f":"A6497&B6497","v":"VL-PPL 0,6 Ø 1500"}," ","Schiedel VL-Prima 0,6 mm Ø 150","VL-PPL 0,6 Ø 150","0",null,"Anlage",0]
["VL-PPL 0,6 Ø 150",2,150,"VL-PPL 0,6 Ø 1502"," ","PPL 150 Revisionsdeckel für Oel/Gas ","100732","0",null,"STK",54]
["VL-PPL 0,6 Ø 150",5,150,"VL-PPL 0,6 Ø 1505"," ","PPL 150 Zugbergrenzerset zu Basiselement","100760","0",null,"STK",324]
["VL-PPL 0,6 Ø 150",7,150,"VL-PPL 0,6 Ø 1507"," ","PPL 150 Längenelement L500mm","100863","0",null,"STK",50]
["VL-PPL 0,6 Ø 150",8,150,"VL-PPL 0,6 Ø 1508"," ","PPL 150 Längenelement L1000mm","100877","0",null,"STK",82]
["VL-PPL 0,6 Ø 150",12,150,"VL-PPL 0,6 Ø 15012"," ","PPL 150 Kondensatabscheider L150mm","100963","0",null,"STK",124]
["VL-PPL 0,6 Ø 150",13,150,"VL-PPL 0,6 Ø 15013",null,"PPL 150 Anschlussrosette ØA 320mm","101186","0",null,"STK",43]
["VL-PPL 0,6 Ø 150",16,150,"VL-PPL 0,6 Ø 15016"," ","PPL 150 Dichtung Viton","100992","0",null,"STK",16]
["VL-PPL 0,6 Ø 150",18,150,"VL-PPL 0,6 Ø 15018"," ","PPL 150 Winkel 15°","101006","0",{"$f":"IF(VLOOKUP(G6515,sanschie!B:J,9,)=0,\"0\",VLOOKUP(G6515,sanschie!B:J,9,0))","v":{"$error":"#N/A"}},"STK",55]
["VL-PPL 0,6 Ø 150",22,150,"VL-PPL 0,6 Ø 15022"," ","PPL 150 Winkel 90°","101062","0",null,"STK",72]
["VL-PPL 0,6 Ø 150",23,150,"VL-PPL 0,6 Ø 15023"," ","PPL 150 Winkel 85° mit Revisionsöffnung","101076","0",null,"STK",173]
["VL-PPL 0,6 Ø 150",25,150,"VL-PPL 0,6 Ø 15025"," ","PPL 150 Winkel 0-45° verstellbar  Trockenbetrieb ","101090","0",null,"STK",54]
["VL-PPL 0,6 Ø 150",28,150,"VL-PPL 0,6 Ø 15028"," ","PPL 150 Kesselanschluss DN + 6mm L150mm","101110","0",null,"STK",64]
["VL-PPL 0,6 Ø 150",31,150,"VL-PPL 0,6 Ø 15031"," ","PPL 150 Verlängerung zu Schalldämpfer -10DB ","101165","0",null,"STK",449]
["VL-PPL 0,6 Ø 150",33,150,"VL-PPL 0,6 Ø 15033"," ","PPL 150 Schallabsorber Festbrennstoffe","101178","0",null,"STK",119]
["VL-PPL 0,6 Ø 150",36,150,"VL-PPL 0,6 Ø 15036",null,"PPL 150 Rohrschelle Anschluss 1/2\" Aussengewinde","101197","0",null,"STK",31]
["VL-PPL 0,6 Ø 150",39,150,"VL-PPL 0,6 Ø 15039",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25]
[{"$f":"A6537","v":"VL-PPL 0,6 Ø 180"},{"$f":"B6537+1","v":1},{"$f":"C6537","v":180},"VL-PPL 0,6 Ø 1801"," ","PPL 180 Anschluss-Basiselement DN180 L450mm","100702","0",null,"STK",119]
["VL-PPL 0,6 Ø 180",2,180,"VL-PPL 0,6 Ø 1802"," ","PPL 180 Revisionsdeckel für Oel/Gas ","100733","0",null,"STK",64]
["VL-PPL 0,6 Ø 180",6,180,"VL-PPL 0,6 Ø 1806"," ","PPL 180 Längenelement L250mm","100850","0",null,"STK",39]
["VL-PPL 0,6 Ø 180",7,180,"VL-PPL 0,6 Ø 1807"," ","PPL 180 Längenelement L500mm","100864","0",null,"STK",55]
["VL-PPL 0,6 Ø 180",11,180,"VL-PPL 0,6 Ø 18011"," ","PPL 180 Revisions-Basiselement mit Kondensatfalle ","100956","0",null,"STK",162]
["VL-PPL 0,6 Ø 180",12,180,"VL-PPL 0,6 Ø 18012"," ","PPL 180 Kondensatabscheider L150mm","100964","0",null,"STK",129]
["VL-PPL 0,6 Ø 180",15,180,"VL-PPL 0,6 Ø 18015"," ","PPL 180 Klemmband","100979","0",null,"STK",12]
["VL-PPL 0,6 Ø 180",17,180,"VL-PPL 0,6 Ø 18017"," ","TS120 Gleitmittel 250ml","100275","0",null,"STK",15.6]
["VL-PPL 0,6 Ø 180",21,180,"VL-PPL 0,6 Ø 18021"," ","PPL 180 Winkel 85°","101049","0",null,"STK",77]
["VL-PPL 0,6 Ø 180",22,180,"VL-PPL 0,6 Ø 18022"," ","PPL 180 Winkel 90°","101063","0",null,"STK",77]
["VL-PPL 0,6 Ø 180",24,180,"VL-PPL 0,6 Ø 18024"," ","PPL 180 Winkel 90° mit Revisionsöffnung","101085","0",null,"STK",194]
["VL-PPL 0,6 Ø 180",27,180,"VL-PPL 0,6 Ø 18027"," ","PPL 180 Revisions-Winkel 0-90° verstellbar   ","101103","0",null,"STK",162]
["VL-PPL 0,6 Ø 180",30,180,"VL-PPL 0,6 Ø 18030",null,"PPL 180 Reduktion  DN130 L150mm","101144","0",null,"STK",108]
["VL-PPL 0,6 Ø 180",32,180,"VL-PPL 0,6 Ø 18032"," ","PPL 180-200 Verlängerung zu Schalldämpfer -10DB ","101166","0",null,"STK",999]
["VL-PPL 0,6 Ø 180",35,180,"VL-PPL 0,6 Ø 18035"," ","ICS 130 Wandhalter verstellbar 75 - 300mm DN180mm","102291","0",null,"STK",65]
["VL-PPL 0,6 Ø 180",38,180,"VL-PPL 0,6 Ø 18038",null,"PPL Innengewinderohr zu Rohrschelle 1/2\" 1000mm","101204","0",null,"STK",147]
["VL-PPL 0,6 Ø 180",40,180,"VL-PPL 0,6 Ø 18040",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25]
["VL-PPL 0,6 Ø 200",0,200,{"$f":"A6578&B6578","v":"VL-PPL 0,6 Ø 2000"}," ","Schiedel VL-Prima 0,6 mm Ø 200","VL-PPL 0,6 Ø 200","0",null,"Anlage",0]
["VL-PPL 0,6 Ø 200",4,200,"VL-PPL 0,6 Ø 2004"," ","PPL 200 Verschlussdeckel mit Griff","100750","0",null,"STK",86]
["VL-PPL 0,6 Ø 200",5,200,"VL-PPL 0,6 Ø 2005"," ","PPL 200 Zugbergrenzerset zu Basiselement","100762","0",null,"STK",482]
["VL-PPL 0,6 Ø 200",9,200,"VL-PPL 0,6 Ø 2009"," ","PPL 200 Schiebe-Element 270-415mm","100929","0",null,"STK",108]
["VL-PPL 0,6 Ø 200",11,200,"VL-PPL 0,6 Ø 20011"," ","PPL 200 Revisions-Basiselement mit Kondensatfalle ","100957","0",null,"STK",184]
["VL-PPL 0,6 Ø 200",14,200,"VL-PPL 0,6 Ø 20014"," ","PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7]
["VL-PPL 0,6 Ø 200",15,200,"VL-PPL 0,6 Ø 20015"," ","PPL 200 Klemmband","100980","0",null,"STK",13]
["VL-PPL 0,6 Ø 200",19,200,"VL-PPL 0,6 Ø 20019"," ","PPL 200 Winkel 30°","101022","0",null,"STK",65]
["VL-PPL 0,6 Ø 200",20,200,"VL-PPL 0,6 Ø 20020"," ","PPL 200 Winkel 45°","101036","0",null,"STK",72]
["VL-PPL 0,6 Ø 200",22,200,"VL-PPL 0,6 Ø 20022"," ","PPL 200 Winkel 90°","101064","0",null,"STK",93]
["VL-PPL 0,6 Ø 200",25,200,"VL-PPL 0,6 Ø 20025"," ","PPL 200 Winkel 0-45° verstellbar  Trockenbetrieb ","101092","0",null,"STK",76]
["VL-PPL 0,6 Ø 200",28,200,"VL-PPL 0,6 Ø 20028"," ","PPL 200 Kesselanschluss DN + 6mm L150mm","101113","0",null,"STK",86]
["VL-PPL 0,6 Ø 200",30,200,"VL-PPL 0,6 Ø 20030"," ","PPL 200 Abgasschalldämpfer Schallred. 15DB L760mm","101161","0",null,"STK",1599]
["VL-PPL 0,6 Ø 200",33,200,"VL-PPL 0,6 Ø 20033"," ","PPL 200 Schallabsorber Festbrennstoffe","101180","0",null,"STK",151]
["VL-PPL 0,6 Ø 200",36,200,"VL-PPL 0,6 Ø 20036",null,"PPL 200 Rohrschelle Anschluss 1/2\" Aussengewinde","101200","0",null,"STK",38]
["VL-PPL 0,6 Ø 200",38,200,"VL-PPL 0,6 Ø 20038",null,"PPL Muffe 1/2\" zu Grundplatte 1/2\" Wandabst. 50mm","101205","0",null,"STK",20]
["VL-PPL 0,6 Ø 200",39,200,"VL-PPL 0,6 Ø 20039",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25]
["VL-PPL 0,6 Ø 250",3,250,"VL-PPL 0,6 Ø 2503"," ","PPL 250 Revisionsdeckel für Festbrennstoffe","100743","0",null,"STK",129]
["VL-PPL 0,6 Ø 250",5,250,"VL-PPL 0,6 Ø 2505"," ","PPL 250 Zugbergrenzerset zu Basiselement","100763","0",null,"STK",503]
["VL-PPL 0,6 Ø 250",8,250,"VL-PPL 0,6 Ø 2508"," ","PPL 250 Längenelement L1000mm","100880","0",null,"STK",120]
["VL-PPL 0,6 Ø 250",10,250,"VL-PPL 0,6 Ø 25010"," ","PPL 250 Endrohr mit beidseitiger Muffe L1000mm","100944","0",null,"STK",129]
["VL-PPL 0,6 Ø 250",13,250,"VL-PPL 0,6 Ø 25013",null,"PPL 250 Anschlussrosette ØA 420mm","101190","0",null,"STK",64]
["VL-PPL 0,6 Ø 250",14,250,"VL-PPL 0,6 Ø 25014"," ","PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7]
["VL-PPL 0,6 Ø 250",18,250,"VL-PPL 0,6 Ø 25018"," ","PPL 250 Winkel 15°","101009","0",null,"STK",77]
["VL-PPL 0,6 Ø 250",19,250,"VL-PPL 0,6 Ø 25019"," ","PPL 250 Winkel 30°","101023","0",null,"STK",82]
["VL-PPL 0,6 Ø 250",21,250,"VL-PPL 0,6 Ø 25021"," ","PPL 250 Winkel 85°","101051","0",null,"STK",120]
["VL-PPL 0,6 Ø 250",24,250,"VL-PPL 0,6 Ø 25024"," ","PPL 250 Winkel 90° mit Revisionsöffnung","101087","0",null,"STK",270]
["VL-PPL 0,6 Ø 250",27,250,"VL-PPL 0,6 Ø 25027"," ","PPL 250 Revisions-Winkel 0-90° verstellbar   ","101105","0",null,"STK",216]
["VL-PPL 0,6 Ø 250",29,250,"VL-PPL 0,6 Ø 25029"," ","PPL 250 Abgasschalldämpfer Schallred. 15DB L760mm","101162","0",null,"STK",1799]
["VL-PPL 0,6 Ø 250",33,250,"VL-PPL 0,6 Ø 25033"," ","ICS 200 Wandhalter verstellbar 75 - 300mm DN250mm","102294","0",null,"STK",82]
["VL-PPL 0,6 Ø 250",34,250,"VL-PPL 0,6 Ø 25034",null,"PPL 250 Rohrschelle Anschluss 1/2\" Aussengewinde","101201","0",null,"STK",41]
["VL-PPL 0,6 Ø 250",37,250,"VL-PPL 0,6 Ø 25037",null,"PPL Grundplatte 1/2\" zu Rohrschelle ","101206","0",null,"STK",25]
["VL-PPL 0,6 Ø 300",0,300,{"$f":"A6656&B6656","v":"VL-PPL 0,6 Ø 3000"}," ","Schiedel VL-Prima 0,6 mm Ø 300","VL-PPL 0,6 Ø 300","0",null,"Anlage",0]
["VL-PPL 0,6 Ø 300",4,300,"VL-PPL 0,6 Ø 3004"," ","PPL 300 Verschlussdeckel mit Griff","100752","0",null,"STK",108]
["VL-PPL 0,6 Ø 300",6,300,"VL-PPL 0,6 Ø 3006"," ","PPL 300 Längenelement L500mm","100867","0",null,"STK",77]
["VL-PPL 0,6 Ø 300",9,300,"VL-PPL 0,6 Ø 3009"," ","PPL 300 Endrohr mit beidseitiger Muffe L1000mm","100945","0",null,"STK",162]
["VL-PPL 0,6 Ø 300",11,300,"VL-PPL 0,6 Ø 30011"," ","PPL 300 Kondensatabscheider L150mm","100967","0",null,"STK",162]
["VL-PPL 0,6 Ø 300",14,300,"VL-PPL 0,6 Ø 30014"," ","PPL 300 Klemmband","100982","0",null,"STK",15]
["VL-PPL 0,6 Ø 300",17,300,"VL-PPL 0,6 Ø 30017"," ","PPL 300 Winkel 15°","101010","0",{"$f":"IF(VLOOKUP(G6673,sanschie!B:J,9,)=0,\"0\",VLOOKUP(G6673,sanschie!B:J,9,0))","v":{"$error":"#N/A"}},"STK",87]
["VL-PPL 0,6 Ø 300",19,300,"VL-PPL 0,6 Ø 30019"," ","PPL 300 Winkel 45°","101038","0",null,"STK",109]
["VL-PPL 0,6 Ø 300",20,300,"VL-PPL 0,6 Ø 30020"," ","PPL 300 Winkel 85°","101052","0",null,"STK",152]
["VL-PPL 0,6 Ø 300",22,300,"VL-PPL 0,6 Ø 30022"," ","PPL 300 Winkel 85° mit Revisionsöffnung","101080","0",null,"STK",324]
["VL-PPL 0,6 Ø 300",25,300,"VL-PPL 0,6 Ø 30025"," ","PPL 300 Winkel 0-90° verstellbar  Trockenbetrieb  ","101100","0",null,"STK",108]
["VL-PPL 0,6 Ø 300",28,300,"VL-PPL 0,6 Ø 30028"," ","PPL 300 Abgasschalldämpfer Schallred. 15DB L760mm","101163","0",null,"STK",1999]
["VL-PPL 0,6 Ø 300",30,300,"VL-PPL 0,6 Ø 30030"," ","PPL 300 Schallabsorber Oel-Gas","101175","0",null,"STK",237]
["VL-PPL 0,6 Ø 300",34,300,"VL-PPL 0,6 Ø 30034",null,"PPL Innengewinderohr zu Rohrschelle 1/2\" 1000mm","101204","0",null,"STK",147]
["VL-PPL 0,6 Ø 300",35,300,"VL-PPL 0,6 Ø 30035",null,"PPL Muffe 1/2\" zu Grundplatte 1/2\" Wandabst. 50mm","101205","0",null,"STK",20]
["VL-PPL 1,0 Ø 350",0,350,{"$f":"A6693&B6693","v":"VL-PPL 1,0 Ø 3500"}," ","Schiedel VL-Prima 1,0 mm Ø 350","VL-PPL 1,0 Ø 350","0","0","Anlage",0]
["VL-PPL 1,0 Ø 350",3,350,"VL-PPL 1,0 Ø 3503",null,"PPL 300 Revisionsdeckel für Festbrennstoffe","100744","0",null,"STK",184]
["VL-PPL 1,0 Ø 350",6,350,"VL-PPL 1,0 Ø 3506",null,"PPL 350 Längenelement L250mm","100854","0",null,"STK",77]
["VL-PPL 1,0 Ø 350",8,350,"VL-PPL 1,0 Ø 3508",null,"PPL 350 Längenelement L1000mm","100882","0",null,"STK",217]
["VL-PPL 1,0 Ø 350",11,350,"VL-PPL 1,0 Ø 35011",null,"PPL 350 Endrohr mit beidseitiger Muffe L1000mm","100946","0",null,"STK",194]
["VL-PPL 1,0 Ø 350",14,350,"VL-PPL 1,0 Ø 35014",null,"PPL 350 Klemmband","100983","0",null,"STK",16]
["VL-PPL 1,0 Ø 350",16,350,"VL-PPL 1,0 Ø 35016",null,"PPL 350 Winkel 15°","101011","0",null,"STK",109]
["VL-PPL 1,0 Ø 350",19,350,"VL-PPL 1,0 Ø 35019",null,"PPL 350 Winkel 85°","101053","0",null,"STK",195]
["VL-PPL 1,0 Ø 400",0,400,{"$f":"A6714&B6714","v":"VL-PPL 1,0 Ø 4000"}," ","Schiedel VL-Prima 1,0 mm Ø 400","VL-PPL 1,0 Ø 400","0","0","Anlage",0]
["VL-PPL 1,0 Ø 400",{"$f":"B6714+1","v":1},{"$f":"C6714","v":400},{"$f":"A6715&\" \"&C6715&B6715","v":"VL-PPL 1,0 Ø 400 4001"},null,"PPL 400 Revisions-Basiselement für Deckel DN300 ","100711","0",null,"STK",432]
["VL-PPL 1,0 Ø 400",3,400,"VL-PPL 1,0 Ø 400 4003",null,"PPL 300 Revisionsdeckel für Festbrennstoffe","100744","0",null,"STK",184]
["VL-PPL 1,0 Ø 400",6,400,"VL-PPL 1,0 Ø 400 4006",null,"PPL 400 Längenelement L250mm","100855","0",null,"STK",109]
["VL-PPL 1,0 Ø 400",9,400,"VL-PPL 1,0 Ø 400 4009",null,"PPL 400 Element mit 3 Messöffnungen 3/4\" L150mm","100911","0",null,"STK",216]
["VL-PPL 1,0 Ø 400",11,400,"VL-PPL 1,0 Ø 400 40011",null,"PPL 400 Endrohr mit beidseitiger Muffe L1000mm","100947","0",null,"STK",237]
["VL-PPL 1,0 Ø 400",15,400,"VL-PPL 1,0 Ø 400 40015",null,"PPL 400 Dichtung Silikon","100998","0",null,"STK",29]
["VL-PPL 1,0 Ø 400",16,400,"VL-PPL 1,0 Ø 400 40016",null,"PPL 400 Winkel 15°","101012","0",null,"STK",217]
["VL-PPL 1,0 Ø 400",18,400,"VL-PPL 1,0 Ø 400 40018",null,"PPL 400 Winkel 45°","101040","0",null,"STK",271]
["VL-PPL 1,0 Ø 450",0,450,{"$f":"A6735&B6735","v":"VL-PPL 1,0 Ø 4500"}," ","Schiedel VL-Prima 0,6 mm Ø 450","VL-PPL 1,0 Ø 450","0","0","Anlage",0]
["VL-PPL 1,0 Ø 450",3,450,"VL-PPL 1,0 Ø 450 4503",null,"PPL 300 Revisionsdeckel für Festbrennstoffe","100744","0",null,"STK",184]
["VL-PPL 1,0 Ø 450",5,450,"VL-PPL 1,0 Ø 450 4505",null,"PPL 450 T-Stück 90° L580mm","100812","0",null,"STK",595]
["VL-PPL 1,0 Ø 450",8,450,"VL-PPL 1,0 Ø 450 4508",null,"PPL 450 Längenelement L1000mm","100884","0",null,"STK",325]
["VL-PPL 1,0 Ø 450",11,450,"VL-PPL 1,0 Ø 450 45011",null,"PPL 450 Endrohr mit beidseitiger Muffe L1000mm","100948","0",null,"STK",292]
["VL-PPL 1,0 Ø 450",13,450,"VL-PPL 1,0 Ø 450 45013",null,"PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7]
["VL-PPL 1,0 Ø 450",16,450,"VL-PPL 1,0 Ø 450 45016",null,"PPL 450 Winkel 15°","101013","0",null,"STK",325]
["VL-PPL 1,0 Ø 450",18,450,"VL-PPL 1,0 Ø 450 45018",null,"PPL 450 Winkel 45°","101041","0",null,"STK",380]
["VL-PPL 1,0 Ø 450",19,450,"VL-PPL 1,0 Ø 450 45019",null,"PPL 450 Winkel 85°","101055","0",null,"STK",596]
[{"$f":"A6757","v":"VL-PPL 1,0 Ø 500"},{"$f":"B6757+1","v":1},{"$f":"C6757","v":500},{"$f":"A6758&\" \"&C6758&B6758","v":"VL-PPL 1,0 Ø 500 5001"},null,"PPL 500 Revisions-Basiselement für Deckel DN300 ","100713","0",null,"STK",648]
["VL-PPL 1,0 Ø 500",2,500,"VL-PPL 1,0 Ø 500 5002",null,"PPL 300 Revisionsdeckel für Oel/Gas ","100736","0",null,"STK",141]
["VL-PPL 1,0 Ø 500",5,500,"VL-PPL 1,0 Ø 500 5005",null,"PPL 500 T-Stück 90° L630mm","100813","0",null,"STK",757]
["VL-PPL 1,0 Ø 500",7,500,"VL-PPL 1,0 Ø 500 5007",null,"PPL 500 Längenelement L500mm","100871","0",null,"STK",217]
["VL-PPL 1,0 Ø 500",11,500,"VL-PPL 1,0 Ø 500 50011",null,"PPL 500 Endrohr mit beidseitiger Muffe L1000mm","100949","0",null,"STK",357]
["VL-PPL 1,0 Ø 500",12,500,"VL-PPL 1,0 Ø 500 50012",null,"PPL 500 Kondensatabscheider L150mm","100971","0",null,"STK",335]
["VL-PPL 1,0 Ø 500",14,500,"VL-PPL 1,0 Ø 500 50014",null,"PPL 500 Klemmband","100986","0",null,"STK",39]
["VL-PPL 1,0 Ø 500",17,500,"VL-PPL 1,0 Ø 500 50017",null,"PPL 500 Winkel 30°","101028","0",null,"STK",401]
["VL-PPL 1,0 Ø 500",20,500,"VL-PPL 1,0 Ø 500 50020",null,"PPL 500 Winkel 90°","101070","0",null,"STK",704]
[{"$f":"A6778","v":"VL-PPL 1,0 Ø 600"},{"$f":"B6778+1","v":1},{"$f":"C6778","v":600},{"$f":"A6779&\" \"&C6779&B6779","v":"VL-PPL 1,0 Ø 600 6001"},null,"PPL 600 Revisions-Basiselement für Deckel DN300 ","100714","0",null,"STK",811]
["VL-PPL 1,0 Ø 600",4,600,"VL-PPL 1,0 Ø 600 6004",null,"PPL 600 Verschlussdeckel mit Griff","100757","0",null,"STK",324]
["VL-PPL 1,0 Ø 600",7,600,"VL-PPL 1,0 Ø 600 6007",null,"PPL 600 Längenelement L250mm","100858","0",null,"STK",217]
["VL-PPL 1,0 Ø 600",9,600,"VL-PPL 1,0 Ø 600 6009",null,"PPL 600 Längenelement L1000mm","100886","0",null,"STK",433]
["VL-PPL 1,0 Ø 600",10,600,"VL-PPL 1,0 Ø 600 60010",null,"PPL 600 Element mit 3 Messöffnungen 3/4\" L150mm","100914","0",null,"STK",324]
["VL-PPL 1,0 Ø 600",14,600,"VL-PPL 1,0 Ø 600 60014",null,"PPL EPDM Stopfen für Messöffnung","100974","0",null,"STK",7]
["VL-PPL 1,0 Ø 600",15,600,"VL-PPL 1,0 Ø 600 60015",null,"PPL 600 Klemmband","100987","0",null,"STK",50]
["VL-PPL 1,0 Ø 600",19,600,"VL-PPL 1,0 Ø 600 60019",null,"PPL 600 Winkel 45°","101043","0",null,"STK",541]
["VL-PPL 1,0 Ø 600",20,600,"VL-PPL 1,0 Ø 600 60020",null,"PPL 600 Winkel 85°","101057","0",null,"STK",920]
["VL-PPL 1,0 Ø 700",0,700,{"$f":"A6801&B6801","v":"VL-PPL 1,0 Ø 7000"}," ","Schiedel VL-Prima 0,6 mm Ø 700","VL-PPL 1,0 Ø 700","0","0","Anlage",0]
["VL-PPL 1,0 Ø 700",2,700,"VL-PPL 1,0 Ø 700 7002",null,"PPL 300 Revisionsdeckel für Oel/Gas ","100736","0",null,"STK",141]
["VL-PPL 1,0 Ø 700",6,700,"VL-PPL 1,0 Ø 700 7006",null,"PPL 700 T-Stück 45° L1200mm","100837","0",null,"STK",1893]
["VL-PPL 1,0 Ø 700",7,700,"VL-PPL 1,0 Ø 700 7007",null,"PPL 700 Längenelement L250mm","100859","0",null,"STK",293]
["VL-PPL 1,0 Ø 700",9,700,"VL-PPL 1,0 Ø 700 7009",null,"PPL 700 Längenelement L1000mm","100887","0",null,"STK",541]
["VL-PPL 1,0 Ø 700",12,700,"VL-PPL 1,0 Ø 700 70012",null,"PPL 700 Endrohr mit beidseitiger Muffe L1000mm","100951","0",null,"STK",508]
["VL-PPL 1,0 Ø 700",15,700,"VL-PPL 1,0 Ø 700 70015",null,"PPL 700 Klemmband","100988","0",null,"STK",60]
["VL-PPL 1,0 Ø 700",17,700,"VL-PPL 1,0 Ø 700 70017",null,"PPL 700 Winkel 15°","101016","0",null,"STK",541]
["VL-PPL 1,0 Ø 700",20,700,"VL-PPL 1,0 Ø 700 70020",null,"PPL 700 Winkel 85°","101058","0",null,"STK",1082]
["Technostar120",0,60,{"$f":"A6824&C6824&B6824","v":"Technostar120600"}," ","Technostar Anlage Ø 60","Technostar12060","0",{"$f":"Technostar120!$J$11","v":9.99},"Anlage",0,1,{"$f":"I6824*1000","v":9990},null,{"$f":"ROUNDUP(P6824,2)","v":0},{"$f":"SUM(P6825:P6884)/1000","v":0}]
[{"$f":"A6825","v":"Technostar120"},{"$f":"B6825+1","v":2},{"$f":"C6825","v":60},{"$f":"A6826&C6826&B6826","v":"Technostar120602"}," ","TS120 60 Rohr mit Muffe L500mm ","100001",500,null,"STK",14.8,null,null,null,null,0]
["Technostar120",3,60,"Technostar120603"," ","TS120 60 Rohr mit Muffe L1000mm ","100002",1000,null,"STK",20.3,null,null,null,null,0]
["Technostar120",7,60,"Technostar120607"," ","TS120 60 Bogen 15°","100088",150,null,"STK",12.3,null,null,null,null,0]
["Technostar120",8,60,"Technostar120608"," ","TS120 60 Bogen 30°","100089",170,null,"STK",12.3,null,null,null,null,0]
["Technostar120",12,60,"Technostar1206012"," ","TS120 60 Revisionsrohr mit Schraubdeckel","100058",160,null,"STK",42.3,null,null,null,null,0]
["Technostar120",14,60,"Technostar1206014"," ","TS120 60 160 Endmuffe schwarz mit Mündungsrohr","100201",117,null,"STK",69.900000000000006,null,null,null,null,0]
["Technostar120",17,60,"Technostar1206017"," ","TS120 60 Verbindungskupplung zu Flex mit Muffe","100040","0",null,"STK",74.7,null,null,null,null,0]
["Technostar120",18,60,"Technostar1206018"," ","TS120 60 Verbindungskupplung zu Flex Steckteil","100043","0",null,"STK",74.7,null,null,null,null,0]
["Technostar120",22,60,"Technostar1206022"," ","TS120 1/2\" Gewinderohr L2000mm","100308","0",null,"STK",23,null,null,null,null,{"$f":"IF(H6846=\"\",\"0\",H6846*L6846)","v":0}]
["Technostar120",23,60,"Technostar1206023"," ","TS120 60 Rohrhalter gleitend ohne Gewinderohr","100288","0",null,"STK",31.5,null,null,null,null,{"$f":"IF(H6847=\"\",\"0\",H6847*L6847)","v":0}]
["Technostar120",25,60,"Technostar1206025"," ","TS120 Verschlussnippel für Messöffnung","100258","0",null,"STK",9.5,null,null,null,null,0]
["Technostar120",28,60,"Technostar1206028"," ","Neutralisationsbox komplett","100265","0",null,"STK",225,null,null,null,null,0]
["Technostar120",31,60,"Technostar1206031"," ","KER Putztür PTS2 200 x 275mm Alu für  Ø140- 250mm","103596","0",null,"STK",112,null,null,null,null,0]
["Technostar120",33,60,"Technostar1206033"," ","KER Schieberahmen zu PTS2 200 x 275mm L90mm","103597","0",null,"STK",21,null,null,null,null,0]
["Technostar120",37,60,"Technostar1206037"," ","ZBH Schachttüre grundiert gasdicht 200 x 300mm","103844","0",null,"STK",206,null,null,null,null,0]
["Technostar120",38,60,"Technostar1206038"," ","TS120 Gleitmittel 250ml","100275","0",null,"STK",15.6,null,null,null,null,0]
["Technostar120",41,60,"Technostar1206041"," ","TS120 Montagebriede zu Kondensatschlauch","100263","0",null,"STK",4.8,null,null,null,null,0]
["Technostar120",42,60,"Technostar1206042"," ","CHZ Mantelstein EZ  220 x 220mm L330mm","103717","0",null,"STK",19,null,null,null,null,0]
["Technostar120",46,60,"Technostar1206046"," ","TS120 Schachtabdeckung 320x320mm Inox","100246","0",null,"STK",247.2,null,null,null,null,0]
["Technostar120",48,60,"Technostar1206048"," ","ABS HEB-Set zu Handyplatte EZ Inox ","104175","0",null,"STK",29,null,null,null,null,{"$f":"IF(H6872=\"\",\"0\",H6872*L6872)","v":0}]
["Technostar120",51,60,"Technostar1206051"," ","TS120LAS 60/100 Rohr L 500 weiss ","100310",500,null,"STK",69.5,null,null,null,null,0]
["Technostar120",53,60,"Technostar1206053"," ","TS120LAS 60/100 Rohr L 2000 weiss ","100312",2000,null,"STK",135.19999999999999,null,null,null,null,0]
["Technostar120",56,60,"Technostar1206056"," ","TS120LAS 60/100 Revisions Bogen 87° weiss ","100323",115,null,"STK",101.5,null,null,null,null,0]
["Technostar120",59,60,"Technostar1206059"," ","TS120LAS 60/100 Kondensatablauf waagrecht weiss","100360","0",null,"STK",126.7,null,null,null,null,0]
["Technostar120",60,60,"Technostar1206060"," ","TS120LAS 60/100 Revisionsrohr gerade weiss","100342",220,null,"STK",137,null,null,null,null,0]
["Technostar120",61,60,"Technostar1206061"," ","TS120LAS 60/100  Wandurchführung L500mm","100466","0",null,"STK",76.3,null,null,null,null,{"$f":"IF(H6885=\"\",\"0\",H6885*L6885)","v":0}]
["Technostar120",62,60,"Technostar1206062"," ","TS120LAS 60/100  Dachdurchführ. L400mm ü Dach sw","100476","0",null,"STK",184,null,null,null,null,{"$f":"IF(H6886=\"\",\"0\",H6886*L6886)","v":0}]
["Technostar120",63,60,{"$f":"A6887&\" \"&C6887&B6887","v":"Technostar120 6063"},null,"LBS 200 Leichtbauschacht i 200mm A 290mm L1000mm","140753","0",null,"STK",101]
["Technostar120",64,60,{"$f":"A6888&\" \"&C6888&B6888","v":"Technostar120 6064"},null,"LBS Kleber zu Leichtbauschacht 1kg","103829","0",null,"STK",9]
[{"$f":"A6888","v":"Technostar120"},{"$f":"B6888+1","v":65},{"$f":"C6888","v":60},{"$f":"A6889&\" \"&C6889&B6889","v":"Technostar120 6065"},null,"ABS Kaminhalterung Standard","104256","0",null,"STK",263]
[{"$f":"A6889","v":"Technostar120"},{"$f":"B6889+1","v":66},{"$f":"C6889","v":60},{"$f":"A6890&\" \"&C6890&B6890","v":"Technostar120 6066"},null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",81]
["Technostar120",0,80,{"$f":"A6891&C6891&B6891","v":"Technostar120800"}," ","Technostar Anlage Ø 80","Technostar12080","0",{"$f":"Technostar120!$J$11","v":9.99},"Anlage",0,1,{"$f":"I6891*1000","v":9990},null,{"$f":"ROUNDUP(P6891,2)","v":0},{"$f":"SUM(P6892:P7016)/1000","v":0}]
[{"$f":"A6891","v":"Technostar120"},{"$f":"B6891+1","v":1},{"$f":"C6891","v":80},"Technostar120801"," ","TS120 80 Rohr mit Muffe L250mm ","100004",250,null,"STK",15.5,null,null,null,null,{"$f":"IF(H6892=\"\",\"0\",H6892*L6892)","v":0},null,null,null,"100004"]
["Technostar120",2,80,"Technostar120802"," ","TS120 80 Rohr mit Muffe L500mm ","100005",500,null,"STK",17.100000000000001,null,null,null,null,0,null,null,null,"100005"]
["Technostar120",3,80,"Technostar120803"," ","TS120 80 Rohr mit Muffe L1000mm ","100006",1000,null,"STK",23.3,null,null,null,null,0,null,null,null,"100006"]
["Technostar120",4,80,"Technostar120804"," ","TS120 80 Rohr mit Muffe L2000mm ","100007",2000,null,"STK",44.2,null,null,null,null,0,null,null,null,"100007"]
["Technostar120",5,80,"Technostar120805"," ","TS120 80 Rohr mit Muffe mit Messöffnung L100mm","100008",0,null,"STK",20,null,null,null,null,0,null,null,null,"100008"]
["Technostar120",6,80,"Technostar120806"," ","TS120 80 Kesselanschluss Reduktion zentr. 60","100157",0,null,"STK",42.8,null,null,null,null,0,null,null,null,"100157"]
["Technostar120",7,80,"Technostar120807"," ","TS120 80 Kesselanschluss Reduktion zentr. 70","100158",0,null,"STK",98.6,null,null,null,null,0,null,null,null,"100158"]
["Technostar120",8,80,"Technostar120808"," ","TS120 80 Kesselanschluss Reduktion zentr. 75","100159",0,null,"STK",74.3,null,null,null,null,0,null,null,null,"100159"]
["Technostar120",9,80,"Technostar120809"," ","TS120 80 Kesselanschluss Erweiterung zentr. 100","100174",0,null,"STK",67.400000000000006,null,null,null,null,0,null,null,null,100174]
["Technostar120",10,80,"Technostar1208010"," ","TS120 80 Kesselanschluss Erweiterung zentr. 110","100175",0,null,"STK",50.3,null,null,null,null,0,null,null,null,"100175"]
["Technostar120",11,80,"Technostar1208011"," ","TS120 80 Abgasabsperrung 80 für Kaskade","100182",0,null,"STK",204,null,null,null,null,{"$f":"IF(H6902=\"\",\"0\",H6902*L6902)","v":0},null,null,null,"100182"]
["Technostar120",12,80,"Technostar1208012"," ","TS120 80 Lippendichtung Peroxyd für Muffe","100249",0,null,"STK",9.1,null,null,null,null,{"$f":"IF(H6903=\"\",\"0\",H6903*L6903)","v":0},null,null,null,"100249"]
["Technostar120",13,80,"Technostar1208013"," ","TS120 80 Revisionsrohr Eckform ","100067",0,null,"STK",60,null,null,null,null,0,null,null,null,"100067"]
["Technostar120",14,80,"Technostar1208014"," ","TS120 80 Revisionsbogen 87° ","100121",0,null,"STK",36.6,null,null,null,null,0,null,null,null,"100121"]
["Technostar120",15,80,"Technostar1208015"," ","TS120LAS 125/80/80 Kesselanschl. Luft Abgas getr.","100347",0,null,"STK",124.1,null,null,null,null,0,null,null,null,"100347"]
["Technostar120",16,80,"Technostar1208016"," ","TS120 80 Kondensatablauf waagrecht ","100195",0,null,"STK",60,null,null,null,null,0,null,null,null,"100195"]
["Technostar120",17,80,"Technostar1208017"," ","TS120 80 Kondensatanblauf senkrecht ","100188",215,null,"STK",60,null,null,null,null,0,null,null,null,"100188"]
["Technostar120",18,80,"Technostar1208018"," ","TS120 80 Bogen 15°","100092",85,null,"STK",13.1,null,null,null,null,0,null,null,null,"100092"]
["Technostar120",19,80,"Technostar1208019"," ","TS120 80 Bogen 30°","100093",124,null,"STK",13.1,null,null,null,null,0,null,null,null,"100093"]
["Technostar120",20,80,"Technostar1208020"," ","TS120 80 Bogen 45°","100094",149,null,"STK",13.1,null,null,null,null,0,null,null,null,"100094"]
["Technostar120",21,80,"Technostar1208021"," ","TS120 80 Langbogen 45° ","100117",260,null,"STK",13.7,null,null,null,null,0,null,null,null,"100117"]
["Technostar120",22,80,"Technostar1208022"," ","TS120 80 Bogen 87°","100095",186,null,"STK",13.7,null,null,null,null,0,null,null,null,"100095"]
["Technostar120",23,80,"Technostar1208023"," ","TS120 80 Langbogen 87° ","100118",260,null,"STK",19.600000000000001,null,null,null,null,0,null,null,null,"100118"]
["Technostar120",24,80,"Technostar1208024"," ","TS120 80 Lang-Revisionsbogen 87° Putz hinten","100129",130,null,"STK",47.3,null,null,null,null,0,null,null,null,"100129"]
["Technostar120",25,80,"Technostar1208025"," ","TS120 80 Lang-Revisionsbogen 87° Putz rechts","100131",130,null,"STK",47.3,null,null,null,null,0,null,null,null,"100131"]
["Technostar120",26,80,"Technostar1208026"," ","TS120 80 Lang-Revisionsbogen 87° Putz links","100130",130,null,"STK",47.3,null,null,null,null,0,null,null,null,"100130"]
["Technostar120",27,80,"Technostar1208027"," ","TS120 80  Revisionsrohr  flach  Typ 3","100060",225,null,"STK",60,null,null,null,null,{"$f":"IF(H6918=\"\",\"0\",H6918*L6918)","v":0},null,null,null,"100060"]
["Technostar120",28,80,"Technostar1208028"," ","TS120 80 Revisionsrohr mit Schraubdeckel","100059",225,null,"STK",60,null,null,null,null,{"$f":"IF(H6919=\"\",\"0\",H6919*L6919)","v":0},null,null,null,"100059"]
["Technostar120",29,80,"Technostar1208029"," ","TS120 80 T-Stück 90°","100074",225,null,"STK",60,null,null,null,null,{"$f":"IF(H6920=\"\",\"0\",H6920*L6920)","v":0},null,null,null,"100074"]
["Technostar120",30,80,"Technostar1208030"," ","TS120 80  Abzweiger 45°","100080",250,null,"STK",118.8,null,null,null,null,0,null,null,null,"100080"]
["Technostar120",31,80,"Technostar1208031"," ","TS120 80 Kaminabstützung komplett mit Bogen 87°","100140",0,null,"STK",61.2,null,null,null,null,0,null,null,null,"100140"]
["Technostar120",32,80,"Technostar1208032"," ","TS120 80 Wandfutter hinterlüftet","100132",100,null,"STK",12.5,null,null,null,null,0,null,null,null,"100132"]
["Technostar120",33,80,"Technostar1208033"," ","TS120 80 160 Endmuffe schwarz mit Mündungsrohr","100202",117,null,"STK",69.900000000000006,null,null,null,null,0,null,null,null,"100202"]
["Technostar120",34,80,"Technostar1208034"," ","TS120 80 200 Endmuffe schwarz mit Mündungsrohr","100203",117,null,"STK",107.2,null,null,null,null,{"$f":"IF(H6925=\"\",\"0\",H6925*L6925)","v":0},null,null,null,"100203"]
["Technostar120",35,80,"Technostar1208035"," ","TS120 80 250 Endmuffe schwarz mit Mündungsrohr","100204",117,null,"STK",108.2,null,null,null,null,{"$f":"IF(H6926=\"\",\"0\",H6926*L6926)","v":0},null,null,null,"100204"]
["Technostar120",36,80,"Technostar1208036"," ","TS120 80 300 Endmuffe schwarz mit Mündungsrohr","104636",0,null,"STK",166.9,null,null,null,null,0,null,null,null,"104636"]
["Technostar120",37,80,"Technostar1208037"," ","TS120 80 350 Endmuffe schwarz mit Mündungsrohr","104639",0,null,"STK",194.7,null,null,null,null,0,null,null,null,"104639"]
["Technostar120",38,80,"Technostar1208038"," ","TS120 80 Flex 75/83 Rolle L12500mm","100034",12500,null,"STK",546.70000000000005,null,null,null,null,0,null,null,null,"100034"]
["Technostar120",39,80,"Technostar1208039"," ","TS120 80 Flex 75/83 Rolle L25000mm","100035",25000,null,"STK",1063,null,null,null,null,0,null,null,null,"100035"]
["Technostar120",40,80,"Technostar1208040"," ","TS120 80 Flex 75/83 Rolle L50000mm","100036",50000,null,"STK",1625.4,null,null,null,null,0,null,null,null,"100036"]
["Technostar120",41,80,"Technostar1208041"," ","TS120 80 Verbindungskupplung zu Flex mit Muffe","100041",0,null,"STK",101.1,null,null,null,null,0,null,null,null,"100041"]
["Technostar120",42,80,"Technostar1208042"," ","TS120 80 Verbindungskupplung zu Flex Steckteil","100044",0,null,"STK",101.1,null,null,null,null,0,null,null,null,"100044"]
["Technostar120",43,80,"Technostar1208043"," ","TS120 80 Schraubkupplung Flex/Flex","100047",0,null,"STK",102,null,null,null,null,0,null,null,null,"100047"]
["Technostar120",44,80,"Technostar1208044"," ","TS120 80 Revisionsrohr für Flex","100049",259,null,"STK",146.1,null,null,null,null,0,null,null,null,"100049"]
["Technostar120",45,80,"Technostar1208045"," ","TS120 80 Einzugshilfe mit Seil 20Meter","100055",147,null,"STK",166.9,null,null,null,null,0,null,null,null,"100055"]
["Technostar120",46,80,"Technostar1208046"," ","TS120 80 Abstandhalter für flex und starr","100148",0,null,"STK",7.7,null,null,null,null,0,null,null,null,"100148"]
["Technostar120",47,80,"Technostar1208047"," ","TS120 80 Rohrhalter fest ohne Gewinderohr","100281",0,null,"STK",14.6,null,null,null,null,0,null,null,null,"100281"]
["Technostar120",48,80,"Technostar1208048"," ","TS120 1/2\" Gewinderohr L2000mm","100308",0,null,"STK",23,null,null,null,null,0,null,null,null,"100308"]
["Technostar120",49,80,"Technostar1208049"," ","TS120 Verschlussnippel für Messöffnung","100258",0,null,"STK",9.5,null,null,null,null,0,null,null,null,"100258"]
["Technostar120",50,80,"Technostar1208050"," ","TS120 Syphon Typ A","100256",0,null,"STK",39.5,null,null,null,null,0,null,null,null,"100256"]
["Technostar120",51,80,"Technostar1208051"," ","TS120 Gleitmittel 250ml","100275",0,null,"STK",15.6,null,null,null,null,0,null,null,null,"100275"]
["Technostar120",52,80,"Technostar1208052"," ","Kondesatschlauch 36mm L1000mm","100264",0,null,"STK",6.2,null,null,null,null,0,null,null,null,"100264"]
["Technostar120",53,80,"Technostar1208053"," ","Neutralisationsbox komplett","100265",0,null,"STK",225,null,null,null,null,0,null,null,null,"100265"]
["Technostar120",54,80,"Technostar1208054"," ","ZBH Schachttüre grundiert gasdicht 200 x 300mm","103844",0,null,"STK",206,null,null,null,null,0,null,null,null,"103844"]
["Technostar120",55,80,"Technostar1208055"," ","CHZ Mantelstein EZ  220 x 220mm L330mm","103717",0,null,"STK",19,null,null,null,null,0,null,null,null,"103717"]
["Technostar120",56,80,"Technostar1208056"," ","CHZ Mantelstein EZ  280 x 280mm L330mm","103718",0,null,"STK",24,null,null,null,null,0,null,null,null,"103718"]
["Technostar120",57,80,"Technostar1208057"," ","CHZ Kaminmörtel Sack 25kg ","103790",0,null,"STK",53,null,null,null,null,0,null,null,null,"103790"]
["Technostar120",58,80,"Technostar1208058"," ","LBS 150 Leichtbauschacht NWi150mm NWA240mm L1000mm","140813","1000",null,"STK",88,null,null,null,null,0,null,null,null,140813]
["Technostar120",59,80,"Technostar1208059"," ","LBS 200 Leichtbauschacht i 200mm A 290mm L1000mm","140753",0,null,"STK",101,null,null,null,null,0,null,null,null,"140753"]
["Technostar120",60,80,"Technostar1208060"," ","LBS Kleber zu Leichtbauschacht 1kg","103829",0,null,"STK",9,null,null,null,null,0,null,null,null,"103829"]
["Technostar120",61,80,"Technostar1208061"," ","ABS Kaminhalterung Standard","104256",0,null,"STK",263,null,null,null,null,0,null,null,null,"104256"]
["Technostar120",62,80,"Technostar1208062"," ","TS120 80/125 Flachdachkragen Alu D125","100230",0,null,"STK",164.4,null,null,null,null,0,null,null,null,"100230"]
["Technostar120",63,80,"Technostar1208063"," ","TS120 Schachtabdeckung 320x320mm Inox","100246",0,null,"STK",247.2,null,null,null,null,0,null,null,null,"100246"]
["Technostar120",64,80,"Technostar1208064"," ","TS120 Schachtabdeckung 400x400mm Inox","100247",0,null,"STK",247.2,null,null,null,null,0,null,null,null,"100247"]
[{"$f":"A6955","v":"Technostar120"},{"$f":"B6955+1","v":65},{"$f":"C6955","v":80},"Technostar1208065"," ","TS120 80 Schachtabdeckung für starres Rohr Inox","100222",0,null,"STK",226.6,null,null,null,null,0,null,null,null,"100222"]
["Technostar120",66,80,"Technostar1208066"," ","TS120 80 Kaminkopfabedeckung schwarz","100216",0,null,"STK",161,null,null,null,null,0,null,null,null,"100216"]
["Technostar120",67,80,"Technostar1208067"," ","TS120LAS 80/125 Rohr L 250 weiss ","100313",250,null,"STK",63,null,null,null,null,0,null,null,null,"100313"]
["Technostar120",68,80,"Technostar1208068"," ","TS120LAS 80/125 Rohr L 500 weiss ","100314",500,null,"STK",83.8,null,null,null,null,0,null,null,null,"100314"]
["Technostar120",69,80,"Technostar1208069"," ","TS120LAS 80/125 Rohr L 1000 weiss ","100315",1000,null,"STK",119.6,null,null,null,null,0,null,null,null,"100315"]
["Technostar120",70,80,{"$f":"A6961&C6961&B6961","v":"Technostar1208070"}," ","TS120LAS 80/125 Rohr L 2000 weiss ","100316",2000,null,"STK",245.5,null,null,null,null,0,null,null,null,"100316"]
["Technostar120",71,80,"Technostar1208071"," ","TS120LAS 80/125 Bogen 15° weiss ","100324",150,null,"STK",82.7,null,null,null,null,0,null,null,null,"100324"]
["Technostar120",72,80,"Technostar1208072"," ","TS120LAS 80/125 Bogen 30° weiss ","100325",133,null,"STK",83.8,null,null,null,null,0,null,null,null,"100325"]
["Technostar120",73,80,"Technostar1208073"," ","TS120LAS 80/125 Bogen 45° weiss ","100327",110,null,"STK",84.9,null,null,null,null,0,null,null,null,"100327"]
["Technostar120",74,80,"Technostar1208074"," ","TS120LAS 80/125 Bogen 87° weiss ","100328",136,null,"STK",118.4,null,null,null,null,0,null,null,null,"100328"]
["Technostar120",75,80,"Technostar1208075"," ","TS120LAS 80/125 Revisionsrohr ecke weiss","100344",0,null,"STK",196.7,null,null,null,null,0,null,null,null,"100344"]
["Technostar120",76,80,"Technostar1208076"," ","TS120LAS 80/125 Revisions Bogen 87° weiss ","100329",0,null,"STK",196.7,null,null,null,null,0,null,null,null,"100329"]
["Technostar120",77,80,"Technostar1208077"," ","TS120LAS 80/125 Revisions Bogen flach 87° weiss ","100330",0,null,"STK",196.7,null,null,null,null,0,null,null,null,100330]
["Technostar120",78,80,"Technostar1208078"," ","TS120LAS 80/125 Kesselanschluss mit Messöffnung","100337",150,null,"STK",98.4,null,null,null,null,0,null,null,null,"100337"]
["Technostar120",79,80,"Technostar1208079"," ","TS120LAS 80/125 Reduktion auf 100/60 weiss","100339",70,null,"STK",123.6,null,null,null,null,0,null,null,null,"100339"]
["Technostar120",80,80,"Technostar1208080"," ","TS120LAS 125 Klemmband weiss","100349",0,null,"STK",137.6,null,null,null,null,0,null,null,null,"100349"]
["Technostar120",81,80,"Technostar1208081"," ","TS120LAS 80/125/50 Kesselanschl. Luft Abgas getr. ","100350",0,null,"STK",128.80000000000001,null,null,null,null,0,null,null,null,100350]
["Technostar120",82,80,"Technostar1208082"," ","TS120LAS 80/125/80 Kesselanschl. Luft Abgas getr. ","140909","0",null,"STK",128.80000000000001,null,null,null,null,0,null,null,null,140909]
["Technostar120",83,80,"Technostar1208083"," ","TS120LAS 80/125 Kaminabstützung für Schacht","100370",0,null,"STK",175.1,null,null,null,null,0,null,null,null,"100370"]
["Technostar120",84,80,"Technostar1208084"," ","TS120LAS 80/125 Kondensatablauf waagrecht weiss","100361",0,null,"STK",196.7,null,null,null,null,0,null,null,null,"100361"]
["Technostar120",85,80,"Technostar1208085"," ","TS120LAS 80/125 T-Stück mit Kondensatanblauf senk.","100365",220,null,"STK",196.7,null,null,null,null,0,null,null,null,"100365"]
["Technostar120",86,80,"Technostar1208086"," ","TS120LAS 80/125 Kondensat. senkr. mit rev.öffnung","100363",220,null,"STK",270.8,null,null,null,null,0,null,null,null,"100363"]
["Technostar120",87,80,"Technostar1208087"," ","TS120LAS 80/125 Revisionsrohr gerade weiss","100343",220,null,"STK",196.7,null,null,null,null,0,null,null,null,"100343"]
["Technostar120",88,80,"Technostar1208088"," ","TS120LAS 80/125 Revisionsrohr gerade flach weiss","100345",220,null,"STK",196.7,null,null,null,null,0,null,null,null,"100345"]
["Technostar120",89,80,"Technostar1208089"," ","TS120LAS 80/125 Rohr L250mm geschlitzt weiss","100487",0,null,"STK",76.3,null,null,null,null,0,null,null,null,"100487"]
["Technostar120",90,80,"Technostar1208090"," ","TS120LAS 80/125 T-Stück weiss","100368",220,null,"STK",196.7,null,null,null,null,0,null,null,null,"100368"]
["Technostar120",91,80,"Technostar1208091"," ","TS120LAS 80/125 Schiebestück 305mm weiss","100366",240,null,"STK",131.30000000000001,null,null,null,null,0,null,null,null,"100366"]
["Technostar120",92,80,"Technostar1208092"," ","TS120LAS 80/125 Verbindungselement 2 Teilig","100372",0,null,"STK",105.1,null,null,null,null,0,null,null,null,"100372"]
["Technostar120",93,80,"Technostar1208093"," ","TS120LAS 80/125 Klemmband Kesselanschluss weiss","100357",0,null,"STK",51.5,null,null,null,null,0,null,null,null,"100357"]
["Technostar120",94,80,"Technostar1208094"," ","TS120 125 Abdeckblende DN125 für schrägdach weiss ","100355",0,null,"STK",49.3,null,null,null,null,0,null,null,null,"100355"]
["Technostar120",95,80,"Technostar1208095"," ","TS120LAS 80/125 Kesselanschlussgitter weiss","100358",0,null,"STK",74.2,null,null,null,null,0,null,null,null,"100358"]
["Technostar120",96,80,"Technostar1208096"," ","TS120  Zuluftgitter 200mm x 200mm weiss","100373",0,null,"STK",105.1,null,null,null,null,{"$f":"IF(H6987=\"\",\"0\",H6987*L6987)","v":0},null,null,null,"100373"]
["Technostar120",97,80,"Technostar1208097"," ","TS120 125 Abdeckblende weiss ","100353",0,null,"STK",52.8,null,null,null,null,0,null,null,null,"100353"]
["Technostar120",98,80,"Technostar1208098"," ","TS120LAS 125 LAS Anfängerplatte 400x400 Inox","100380",0,null,"STK",92.6,null,null,null,null,0,null,null,null,"100380"]
["Technostar120",99,80,"Technostar1208099"," ","TS120LAS 80/125 Rohr L 250 Inox ","100382",250,null,"STK",72.099999999999994,null,null,null,null,0,null,null,null,"100382"]
["Technostar120",100,80,"Technostar12080100"," ","TS120LAS 80/125 Rohr L 500 Inox ","100383",500,null,"STK",97.2,null,null,null,null,0,null,null,null,"100383"]
["Technostar120",101,80,"Technostar12080101"," ","TS120LAS 80/125 Rohr L 1000 Inox ","100384",1000,null,"STK",163.1,null,null,null,null,0,null,null,null,"100384"]
["Technostar120",102,80,"Technostar12080102"," ","TS120LAS 80/125 Rohr L 2000 Inox ","100385",2000,null,"STK",273.60000000000002,null,null,null,null,0,null,null,null,"100385"]
["Technostar120",103,80,"Technostar12080103"," ","TS120LAS 80/125 Bogen 15° Inox","100427",129,null,"STK",100.2,null,null,null,null,0,null,null,null,"100427"]
["Technostar120",104,80,"Technostar12080104"," ","TS120LAS 80/125 Bogen 30° Inox","100428",133,null,"STK",100.2,null,null,null,null,0,null,null,null,"100428"]
["Technostar120",105,80,"Technostar12080105"," ","TS120LAS 80/125 Bogen 45° Inox","100429",147,null,"STK",100.2,null,null,null,null,{"$f":"IF(H6996=\"\",\"0\",H6996*L6996)","v":0},null,null,null,"100429"]
["Technostar120",106,80,"Technostar12080106"," ","TS120LAS 80/125 Bogen 87° Inox","100430",126,null,"STK",126.2,null,null,null,null,0,null,null,null,"100430"]
["Technostar120",107,80,"Technostar12080107"," ","TS120LAS 80/125 Aussenwandanschluss komplett Inox","100399",0,null,"STK",355.6,null,null,null,null,0,null,null,null,"100399"]
["Technostar120",108,80,"Technostar12080108"," ","TS120LAS 125 Abdeckblende  Inox","100418",0,null,"STK",38,null,null,null,null,0,null,null,null,"100418"]
["Technostar120",109,80,"Technostar12080109"," ","TS120LAS 125 Verl. Typ 1 zu Aussenwandanschluss","100405",0,null,"STK",154.69999999999999,null,null,null,null,0,null,null,null,"100405"]
["Technostar120",110,80,"Technostar12080110"," ","TS120LAS 125 Verl. Typ 2 zu Aussenwandanschluss","100406",0,null,"STK",193.3,null,null,null,null,0,null,null,null,"100406"]
["Technostar120",111,80,"Technostar12080111"," ","TS120LAS 125 Verl. Typ 3 zu Aussenwandanschluss","100407",0,null,"STK",231.9,null,null,null,null,0,null,null,null,"100407"]
["Technostar120",112,80,"Technostar12080112"," ","TS120LAS 80/125  Wandurchführung L500mm","100467",0,null,"STK",46.5,null,null,null,null,0,null,null,null,"100467"]
["Technostar120",113,80,"Technostar12080113"," ","TS120LAS 80/125 Revisionsrohr Inox ","100414",0,null,"STK",209.9,null,null,null,null,0,null,null,null,"100414"]
["Technostar120",114,80,"Technostar12080114"," ","TS120LAS 80/125 Dachdurchführung Inox","100421",0,null,"STK",297.39999999999998,null,null,null,null,0,null,null,null,"100421"]
["Technostar120",115,80,"Technostar12080115"," ","TS120LAS 80 Mündungsrohr Inox","100451",250,null,"STK",49.1,null,null,null,null,0,null,null,null,"100451"]
["Technostar120",116,80,"Technostar12080116"," ","TS120LAS 125 Klemmband Inox","100442",0,null,"STK",51.4,null,null,null,null,0,null,null,null,"100442"]
["Technostar120",117,80,"Technostar12080117"," ","TS120LAS 80/125 Zuluftstutzen Inox","100439",0,null,"STK",211.6,null,null,null,null,0,null,null,null,"100439"]
["Technostar120",118,80,"Technostar12080118"," ","TS120LAS 80/125 Mündungsabschluss mit Klemmband","100445",145,null,"STK",111.3,null,null,null,null,0,null,null,null,"100445"]
["Technostar120",119,80,"Technostar12080119"," ","TS120LAS 80/125 Dachdurchführ. L400mm ü Dach sw","100477",0,null,"STK",196.1,null,null,null,null,0,null,null,null,"100477"]
["Technostar120",120,80,"Technostar12080120"," ","TS120LAS 80/125 Dachdurchführ. L1000mm ü Dach sw","100479",0,null,"STK",213.5,null,null,null,null,0,null,null,null,"100479"]
["Technostar120",121,80,"Technostar12080121"," ","TS120 80/125 Dachpfanne 5-25° schwarz","100233",0,null,"STK",101.7,null,null,null,null,0,null,null,null,"100233"]
["Technostar120",122,80,"Technostar12080122"," ","TS120 80/125 Dachpfanne 25-45°  schwarz","100235",0,null,"STK",101.7,null,null,null,null,0,null,null,null,"100235"]
["Technostar120",123,80,"Technostar12080123"," ","TS120LAS 125 Wandhalterung Inox","100454",0,null,"STK",70.8,null,null,null,null,0,null,null,null,"100454"]
["Technostar120",124,80,"Technostar12080124"," ","TS120LAS 125 Verlängerung Typ 1 zu Wandhalterung ","100455",0,null,"STK",77.400000000000006,null,null,null,null,0,null,null,null,"100455"]
["Technostar120",125,80,"Technostar12080125"," ","TS120LAS 125 Verlängerung Typ 2 zu Wandhalterung ","100456",0,null,"STK",116,null,null,null,null,0,null,null,null,"100456"]
["Technostar120",126,80,"Technostar12080126"," ","TS120LAS 125 Verlängerung Typ 3 zu Wandhalterung ","100457",0,null,"STK",154.69999999999999,null,null,null,null,0,null,null,null,"100457"]
["Technostar120",127,80,"Technostar12080127"," ","TS120 80 Schachtabdeckung für flex. Rohr Inox","100223",0,null,"STK",247.2,null,null,null,null,0,null,null,null,"100223"]
["Technostar120",128,80,"Technostar12080128"," ","TS120 80 Sprengring Flex zu Mündungasabschluss","100218",0,null,"STK",30.9,null,null,null,null,0,null,null,null,"100218"]
["Technostar120",0,110,{"$f":"A7020&C7020&B7020","v":"Technostar1201100"}," ","Technostar Anlage Ø 110","Technostar120110","0",{"$f":"Technostar120!$J$11","v":9.99},"Anlage",0,1,{"$f":"I7020*1000","v":9990},null,{"$f":"ROUNDUP(P7020,2)","v":0},{"$f":"SUM(P7021:P7129)/1000","v":0}]
[{"$f":"A7020","v":"Technostar120"},{"$f":"B7020+1","v":1},{"$f":"C7020","v":110},"Technostar1201101"," ","TS120 110 Rohr mit Muffe L250mm","100010",250,null,"STK",17.399999999999999,null,null,null,null,{"$f":"IF(H7021=\"\",\"0\",H7021*L7021)","v":0},null,null,null,"100010"]
["Technostar120",2,110,"Technostar1201102"," ","TS120 110 Rohr mit Muffe L500mm ","100011",500,null,"STK",26.2,null,null,null,null,0,null,null,null,"100011"]
["Technostar120",3,110,{"$f":"A7023&C7023&B7023","v":"Technostar1201103"}," ","TS120 110 Rohr mit Muffe L1000mm ","100012",1000,null,"STK",43.7,null,null,null,null,0,null,null,null,"100012"]
["Technostar120",4,110,"Technostar1201104"," ","TS120 110 Rohr mit Muffe L2000mm ","100013",2000,null,"STK",73.400000000000006,null,null,null,null,0,null,null,null,"100013"]
["Technostar120",5,110,"Technostar1201105"," ","TS120 110 Rohr mit Muffe mit Messöffnung L100mm","100009",100,null,"STK",22,null,null,null,null,null,null,null,null,"100009"]
["Technostar120",6,110,"Technostar1201106"," ","TS120 110 Kesselanschluss Reduktion zentr. 80","100160",0,null,"STK",50.3,null,null,null,null,0,null,null,null,"100160"]
["Technostar120",7,110,"Technostar1201107"," ","TS120 110 Kesselanschluss Reduktion zentr. 100","100161",0,null,"STK",90.6,null,null,null,null,0,null,null,null,"100161"]
["Technostar120",8,110,"Technostar1201108"," ","TS120 110 Kesselanschluss Reduktion exzentr. 80","100171",0,null,"STK",31.7,null,null,null,null,0,null,null,null,"100171"]
["Technostar120",9,110,"Technostar1201109"," ","TS120 110 Kesselanschluss Erweiterung exzentr. 125","100177",0,null,"STK",98.3,null,null,null,null,0,null,null,null,"100177"]
["Technostar120",10,110,"Technostar12011010"," ","TS120 110 Kesselanschluss auf 153mm","140680","100",null,"STK",195.3,null,null,null,null,0,null,null,null,"140680"]
["Technostar120",11,110,"Technostar12011011"," ","TS120 110 Kesselanschluss auf 183mm","140684","100",null,"STK",232,null,null,null,null,0,null,null,null,"140684"]
["Technostar120",12,110,"Technostar12011012"," ","TS120 110 Abgasabsperrung 80 für Kaskade","100184",0,null,"STK",300.8,null,null,null,null,0,null,null,null,"100184"]
["Technostar120",13,110,"Technostar12011013"," ","TS120 110 Abgasabsperrung 100 für Kaskade","100183",0,null,"STK",300.8,null,null,null,null,0,null,null,null,"100183"]
["Technostar120",14,110,"Technostar12011014"," ","TS120 110 Lippenndichtung Peroxyd für Muffe","100250",0,null,"STK",10.7,null,null,null,null,0,null,null,null,"100250"]
["Technostar120",15,110,"Technostar12011015"," ","TS120 110 Kondensatablauf waagrecht","100196",0,null,"STK",104.4,null,null,null,null,0,null,null,null,"100196"]
["Technostar120",16,110,"Technostar12011016"," ","TS120 110 Kondensatanblauf senkrecht ","100189",130,null,"STK",178.4,null,null,null,null,0,null,null,null,"100189"]
["Technostar120",17,110,"Technostar12011017"," ","TS120 110 Bogen 15°","100096",99,null,"STK",16.600000000000001,null,null,null,null,0,null,null,null,"100096"]
["Technostar120",18,110,"Technostar12011018"," ","TS120 110 Bogen 30°","100097",184,null,"STK",16.600000000000001,null,null,null,null,0,null,null,null,"100097"]
["Technostar120",19,110,"Technostar12011019"," ","TS120 110 Bogen 45°","100098",201,null,"STK",17.3,null,null,null,null,0,null,null,null,"100098"]
["Technostar120",20,110,"Technostar12011020"," ","TS120 110 Langbogen 45° ","100119",270,null,"STK",17.3,null,null,null,null,0,null,null,null,"100119"]
["Technostar120",21,110,"Technostar12011021"," ","TS120 110 Bogen 87°","100099",266,null,"STK",18.5,null,null,null,null,0,null,null,null,"100099"]
["Technostar120",22,110,"Technostar12011022"," ","TS120 110 Langbogen 87° ","100120",270,null,"STK",18.5,null,null,null,null,0,null,null,null,"100120"]
["Technostar120",23,110,"Technostar12011023"," ","TS120 110 Revisionsbogen 87° ","100122",210,null,"STK",41.6,null,null,null,null,{"$f":"IF(H7043=\"\",\"0\",H7043*L7043)","v":0},null,null,null,"100122"]
["Technostar120",24,110,"Technostar12011024"," ","TS120 110 Revisionsrohr mit Schraubdeckel","100061",185,null,"STK",33.700000000000003,null,null,null,null,{"$f":"IF(H7044=\"\",\"0\",H7044*L7044)","v":0},null,null,null,"100061"]
["Technostar120",25,110,"Technostar12011025"," ","TS120 110 T-Stück 90°","100075",250,null,"STK",125.8,null,null,null,null,{"$f":"IF(H7045=\"\",\"0\",H7045*L7045)","v":0},null,null,null,"100075"]
["Technostar120",26,110,"Technostar12011026"," ","TS120 110 Abzweiger 45°","100081",300,null,"STK",148.6,null,null,null,null,0,null,null,null,"100081"]
["Technostar120",27,110,"Technostar12011027"," ","TS120 110 Kaminabstützung komplett mit Bogen 87°","100141",0,null,"STK",70.8,null,null,null,null,0,null,null,null,"100141"]
["Technostar120",28,110,"Technostar12011028"," ","TS120LAS 110/160 Kaminabstützung für Schacht","100371",0,null,"STK",231.8,null,null,null,null,0,null,null,null,"100371"]
["Technostar120",29,110,"Technostar12011029"," ","TS120 110 Wandfutter hinterlüftet","100133",137,null,"STK",18.3,null,null,null,null,0,null,null,null,"100133"]
["Technostar120",30,110,"Technostar12011030"," ","TS120 110 200 Endmuffe schwarz mit Mündungsrohr","100205",100,null,"STK",111.8,null,null,null,null,{"$f":"IF(H7050=\"\",\"0\",H7050*L7050)","v":0},null,null,null,"100205"]
["Technostar120",31,110,"Technostar12011031"," ","TS120 110 250 Endmuffe schwarz mit Mündungsrohr","100206",100,null,"STK",142.1,null,null,null,null,0,null,null,null,"100206"]
["Technostar120",32,110,"Technostar12011032"," ","TS120 110 300 Endmuffe schwarz mit Mündungsrohr","104642",0,null,"STK",166.9,null,null,null,null,0,null,null,null,"104642"]
["Technostar120",33,110,"Technostar12011033"," ","TS120 110 350 Endmuffe schwarz mit Mündungsrohr","104643",0,null,"STK",194.7,null,null,null,null,0,null,null,null,"104643"]
["Technostar120",34,110,"Technostar12011034"," ","TS120 110 Flex 105/113 Rolle L15000mm","100037",15000,null,"STK",853.9,null,null,null,null,0,null,null,null,"100037"]
["Technostar120",35,110,"Technostar12011035"," ","TS120 110 Flex 105/113 Rolle L25000mm","100038",25000,null,"STK",1423,null,null,null,null,0,null,null,null,"100038"]
["Technostar120",36,110,"Technostar12011036"," ","TS120 110 Verbindungskupplung zu Flex mit Muffe","100042",0,null,"STK",185.4,null,null,null,null,0,null,null,null,"100042"]
["Technostar120",37,110,"Technostar12011037"," ","TS120 110 Verbindungskupplung zu Flex Steckteil","100045",0,null,"STK",185.4,null,null,null,null,0,null,null,null,"100045"]
["Technostar120",38,110,"Technostar12011038"," ","TS120 110 Schraubkupplung Flex/Flex","100048",0,null,"STK",206,null,null,null,null,0,null,null,null,"100048"]
["Technostar120",39,110,"Technostar12011039"," ","TS120 110 Revisionsrohr für Flex","100050",269,null,"STK",278.10000000000002,null,null,null,null,0,null,null,null,"100050"]
["Technostar120",40,110,"Technostar12011040"," ","TS120 110 Einzugshilfe mit Seil 20Meter","100054",165,null,"STK",221.5,null,null,null,null,0,null,null,null,"100054"]
["Technostar120",41,110,"Technostar12011041"," ","PPL 130 Abstandhalter","100918",0,null,"STK",25,null,null,null,null,0,null,null,null,"100918"]
["Technostar120",42,110,"Technostar12011042"," ","TS120 110 Abstandhalter für flex und starr","100149",0,null,"STK",8.3000000000000007,null,null,null,null,0,null,null,null,"100149"]
["Technostar120",43,110,"Technostar12011043"," ","TS120 110 Rohrhalter fest ohne Gewinderohr","100283",0,null,"STK",15,null,null,null,null,0,null,null,null,"100283"]
["Technostar120",44,110,"Technostar12011044"," ","TS120 Syphon Typ A","100256",0,null,"STK",39.5,null,null,null,null,0,null,null,null,"100256"]
["Technostar120",45,110,"Technostar12011045"," ","TS120 Gleitmittel 250ml","100275",0,null,"STK",15.6,null,null,null,null,0,null,null,null,"100275"]
["Technostar120",46,110,"Technostar12011046"," ","Kondesatschlauch 36mm L1000mm","100264",0,null,"STK",6.2,null,null,null,null,0,null,null,null,"100264"]
["Technostar120",47,110,"Technostar12011047"," ","TS120 Schlauchbriede zu Kondensatschlauch","100262",0,null,"STK",4.8,null,null,null,null,0,null,null,null,"100262"]
["Technostar120",48,110,"Technostar12011048"," ","TS120 Montagebriede zu Kondensatschlauch","100263",0,null,"STK",4.8,null,null,null,null,0,null,null,null,"100263"]
["Technostar120",49,110,"Technostar12011049"," ","Neutralisationsbox komplett","100265",0,null,"STK",225,null,null,null,null,0,null,null,null,"100265"]
["Technostar120",50,110,"Technostar12011050"," ","ZBH Schachttüre grundiert gasdicht 200 x 300mm","103844",0,null,"STK",206,null,null,null,null,0,null,null,null,"103844"]
["Technostar120",51,110,"Technostar12011051"," ","CHZ Mantelstein EZ  280 x 280mm L330mm","103718",0,null,"STK",24,null,null,null,null,0,null,null,null,"103718"]
["Technostar120",52,110,"Technostar12011052"," ","CHZ Mantelstein EZ  320 x 320mm L330mm Ø160mm","103719",0,null,"STK",19,null,null,null,null,0,null,null,null,"103719"]
["Technostar120",53,110,"Technostar12011053"," ","CHZ Kaminmörtel Sack 25kg ","103790",0,null,"STK",53,null,null,null,null,0,null,null,null,"103790"]
["Technostar120",54,110,"Technostar12011054"," ","LBS 200 Leichtbauschacht i 200mm A 290mm L1000mm","140753",0,null,"STK",101,null,null,null,null,0,null,null,null,"140753"]
["Technostar120",55,110,"Technostar12011055"," ","LBS 230 Leichtbauschacht i 230mm A 320mm L1000mm","103826",0,null,"STK",106,null,null,null,null,0,null,null,null,"103826"]
["Technostar120",56,110,"Technostar12011056"," ","LBS Kleber zu Leichtbauschacht 1kg","103829",0,null,"STK",9,null,null,null,null,0,null,null,null,"103829"]
["Technostar120",57,110,"Technostar12011057"," ","ABS Kaminhalterung Standard","104256",0,null,"STK",263,null,null,null,null,0,null,null,null,"104256"]
["Technostar120",58,110,"Technostar12011058"," ","TS120 110/160 Flachdachkragen Alu D160","100231",0,null,"STK",181.7,null,null,null,null,0,null,null,null,"100231"]
["Technostar120",59,110,"Technostar12011059"," ","TS120 Schachtabdeckung 400x400mm Inox","100247",0,null,"STK",247.2,null,null,null,null,0,null,null,null,"100247"]
["Technostar120",60,110,"Technostar12011060"," ","PPL 150 Mündungsmanchette L130mm 400 x 400mm","101287",0,null,"STK",129,null,null,null,null,0,null,null,null,"101287"]
["Technostar120",61,110,"Technostar12011061"," ","TS120 110 Schachtabdeckung für starres Rohr Inox","100224",0,null,"STK",247.2,null,null,null,null,0,null,null,null,"100224"]
["Technostar120",62,110,"Technostar12011062"," ","TS120 110 Schachtabdeckung für flex. Rohr Inox","100225",0,null,"STK",267.8,null,null,null,null,0,null,null,null,"100225"]
["Technostar120",63,110,"Technostar12011063"," ","TS120 110 Kaminkopfabdeckung schwarz","100217",0,null,"STK",214.8,null,null,null,null,0,null,null,null,"100217"]
["Technostar120",64,110,"Technostar12011064"," ","TS120LAS 110/160 Rohr L 250 weiss ","100317",250,null,"STK",87.8,null,null,null,null,0,null,null,null,"100317"]
[{"$f":"A7084","v":"Technostar120"},{"$f":"B7084+1","v":65},{"$f":"C7084","v":110},"Technostar12011065"," ","TS120LAS 110/160 Rohr L 500 weiss","100318",500,null,"STK",106,null,null,null,null,0,null,null,null,"100318"]
["Technostar120",66,110,"Technostar12011066"," ","TS120LAS 110/160 Rohr L 1000 weiss ","100319",1000,null,"STK",156.9,null,null,null,null,0,null,null,null,"100319"]
["Technostar120",67,110,{"$f":"A7087&C7087&B7087","v":"Technostar12011067"}," ","TS120LAS 110/160 Rohr L 2000 weiss ","100320",2000,null,"STK",308.39999999999998,null,null,null,null,0,null,null,null,"100320"]
["Technostar120",68,110,"Technostar12011068"," ","TS120LAS 110/160 Bogen 15° weiss","100331",145,null,"STK",121.9,null,null,null,null,0,null,null,null,"100331"]
["Technostar120",69,110,"Technostar12011069"," ","TS120LAS 110/160 Bogen 30° weiss","100332",150,null,"STK",121.9,null,null,null,null,0,null,null,null,"100332"]
["Technostar120",70,110,"Technostar12011070"," ","TS120LAS 110/160 Bogen 45° weiss","100333",150,null,"STK",121.9,null,null,null,null,0,null,null,null,"100333"]
["Technostar120",71,110,"Technostar12011071"," ","TS120LAS 110/160 Bogen 87° weiss","100334",150,null,"STK",140.30000000000001,null,null,null,null,0,null,null,null,"100334"]
["Technostar120",72,110,"Technostar12011072"," ","TS120LAS 110/160 Revisions Bogen 87° weiss ","100335",150,null,"STK",226.8,null,null,null,null,0,null,null,null,"100335"]
["Technostar120",73,110,"Technostar12011073"," ","TS120LAS 110/160 Kesselanschluss mit Messöffnung","100338",150,null,"STK",137.6,null,null,null,null,0,null,null,null,"100338"]
["Technostar120",74,110,"Technostar12011074"," ","TS120LAS 110/160 Reduktion auf 80/125 weiss","100340",150,null,"STK",153.4,null,null,null,null,0,null,null,null,"100340"]
["Technostar120",75,110,"Technostar12011075"," ","TS120LAS 110/160 Reduktion auf 150/100 weiss","100341",150,null,"STK",176.3,null,null,null,null,{"$f":"IF(H7095=\"\",\"0\",H7095*L7095)","v":0},null,null,null,"100341"]
["Technostar120",76,110,"Technostar12011076"," ","TS120LAS 110/160/80 Kesselanschl. Luft Abgas getr ","140910","0",null,"STK",184.4,null,null,null,null,0,null,null,null,"140910"]
["Technostar120",77,110,"Technostar12011077"," ","TS120LAS 110/160 Kondensatablauf waagrecht weiss","100362",0,null,"STK",293.89999999999998,null,null,null,null,0,null,null,null,"100362"]
["Technostar120",78,110,"Technostar12011078"," ","TS120LAS 110/160 Kondensat. senkr. mit rev.öffnung","100364",250,null,"STK",222.4,null,null,null,null,0,null,null,null,"100364"]
["Technostar120",79,110,"Technostar12011079"," ","TS120LAS 110/160 Revisionsrohr gerade weiss","100346",250,null,"STK",199.3,null,null,null,null,0,null,null,null,"100346"]
["Technostar120",80,110,"Technostar12011080"," ","TS120LAS 110/160 T-Stück weiss","100369",250,null,"STK",199.3,null,null,null,null,0,null,null,null,"100369"]
["Technostar120",81,110,"Technostar12011081"," ","TS120LAS 80/125  Wandurchführung L500mm","100467",0,null,"STK",46.5,null,null,null,null,0,null,null,null,"100467"]
["Technostar120",82,110,"Technostar12011082"," ","TS120LAS 110/160 Kesselanschlussgitter weiss","100359",0,null,"STK",81.400000000000006,null,null,null,null,0,null,null,null,"100359"]
["Technostar120",83,110,"Technostar12011083"," ","TS120 160 Abdeckblende weiss","100354",0,null,"STK",74.2,null,null,null,null,0,null,null,null,"100354"]
["Technostar120",84,110,"Technostar12011084"," ","TS120 125 Abdeckblende DN160 für schrägdach weiss ","100356",0,null,"STK",58.8,null,null,null,null,0,null,null,null,"100356"]
["Technostar120",85,110,"Technostar12011085"," ","TS120LAS 110/160 Rohr L 250 Inox ","100386",250,null,"STK",89.7,null,null,null,null,0,null,null,null,"100386"]
["Technostar120",86,110,"Technostar12011086"," ","TS120LAS 110/160 Rohr L 500 Inox ","100387",500,null,"STK",130.19999999999999,null,null,null,null,0,null,null,null,"100387"]
["Technostar120",87,110,"Technostar12011087"," ","TS120LAS 110/160 Rohr L 1000 Inox ","100388",1000,null,"STK",227.1,null,null,null,null,{"$f":"IF(H7107=\"\",\"0\",H7107*L7107)","v":0},null,null,null,"100388"]
["Technostar120",88,110,"Technostar12011088"," ","TS120LAS 110/160 Rohr L 2000 Inox ","100389",2000,null,"STK",319.3,null,null,null,null,0,null,null,null,"100389"]
["Technostar120",89,110,"Technostar12011089"," ","TS120LAS 110/160 Bogen 15° Inox","100431",142,null,"STK",145.4,null,null,null,null,0,null,null,null,"100431"]
["Technostar120",90,110,"Technostar12011090"," ","TS120LAS 110/160 Bogen 30° Inox","100432",148,null,"STK",145.4,null,null,null,null,0,null,null,null,"100432"]
["Technostar120",91,110,"Technostar12011091"," ","TS120LAS 110/160 Bogen 45° Inox","100433",148,null,"STK",156.80000000000001,null,null,null,null,0,null,null,null,"100433"]
["Technostar120",92,110,"Technostar12011092"," ","TS120LAS 110/160 Bogen 87° Inox","100434",170,null,"STK",187.3,null,null,null,null,0,null,null,null,"100434"]
["Technostar120",93,110,"Technostar12011093"," ","TS120LAS 110/160 Aussenwandanschluss komplett Inox","100400",0,null,"STK",491.5,null,null,null,null,0,null,null,null,"100400"]
["Technostar120",94,110,"Technostar12011094"," ","TS120LAS 160 Verl. Typ 1 zu Aussenwandanschluss","100408",0,null,"STK",154.69999999999999,null,null,null,null,0,null,null,null,"100408"]
["Technostar120",95,110,"Technostar12011095"," ","TS120LAS 160 Verl. Typ 2 zu Aussenwandanschluss","100409",0,null,"STK",193.3,null,null,null,null,0,null,null,null,"100409"]
["Technostar120",96,110,"Technostar12011096"," ","TS120LAS 160 Verl. Typ 3 zu Aussenwandanschluss","100410",0,null,"STK",231.9,null,null,null,null,0,null,null,null,"100410"]
["Technostar120",97,110,"Technostar12011097"," ","TS120LAS 160 Abdeckblende  Inox","100419",0,null,"STK",52.3,null,null,null,null,0,null,null,null,"100419"]
["Technostar120",98,110,"Technostar12011098"," ","TS120LAS 110/160 Wandurchführung L500mm","100468",0,null,"STK",75.8,null,null,null,null,0,null,null,null,"100468"]
["Technostar120",99,110,"Technostar12011099"," ","TS120LAS 110/160 Revisionsrohr Inox ","100415",0,null,"STK",250.9,null,null,null,null,0,null,null,null,"100415"]
["Technostar120",100,110,"Technostar120110100"," ","TS120LAS 110/160 Dachdurchführung Inox","100422",0,null,"STK",386.5,null,null,null,null,0,null,null,null,"100422"]
["Technostar120",101,110,"Technostar120110101"," ","TS120LAS 110 Mündungsrohr Inox","100452",250,null,"STK",55.7,null,null,null,null,0,null,null,null,"100452"]
["Technostar120",102,110,"Technostar120110102"," ","TS120LAS 160 Klemmband Inox","100443",0,null,"STK",67.3,null,null,null,null,0,null,null,null,"100443"]
["Technostar120",103,110,"Technostar120110103"," ","TS120LAS 110/160 Zuluftstutzen Inox","100440",0,null,"STK",223.3,null,null,null,null,0,null,null,null,"100440"]
["Technostar120",104,110,"Technostar120110104"," ","TS120LAS 110/160 Mündungsabschluss mit Klemmband","100446",145,null,"STK",123.1,null,null,null,null,0,null,null,null,"100446"]
["Technostar120",105,110,"Technostar120110105"," ","TS120LAS 110/160 Dachdurchführ. L1000mm ü Dach sw","100481",0,null,"STK",387.3,null,null,null,null,0,null,null,null,"100481"]
["Technostar120",106,110,"Technostar120110106"," ","TS120LAS 110/160 Dachdurchführ. L1000mm ü Dach rot","100482",0,null,"STK",387.3,null,null,null,null,0,null,null,null,"100482"]
["Technostar120",107,110,"Technostar120110107"," ","TS120 110/160 Dachpfanne 25-45°  schwarz","100239",0,null,"STK",180.6,null,null,null,null,0,null,null,null,"100239"]
["Technostar120",108,110,"Technostar120110108"," ","TS120 110/160 Dachpfanne 25-45°  rot","100238",0,null,"STK",180.6,null,null,null,null,0,null,null,null,"100238"]
["Technostar120",109,110,"Technostar120110109"," ","TS120LAS 160 Wandhalterung Inox","100458",0,null,"STK",78.400000000000006,null,null,null,null,0,null,null,null,"100458"]
["Technostar120",110,110,"Technostar120110110"," ","TS120LAS 160 Verlängerung Typ 1 zu Wandhalterung ","100459",0,null,"STK",92.9,null,null,null,null,0,null,null,null,"100459"]
["Technostar120",111,110,"Technostar120110111"," ","TS120LAS 160 Verlängerung Typ 2 zu Wandhalterung ","100460",0,null,"STK",131.5,null,null,null,null,{"$f":"IF(H7131=\"\",\"0\",H7131*L7131)","v":0},null,null,null,"100460"]
["Technostar120",112,110,"Technostar120110112"," ","TS120LAS 160 Verlängerung Typ 3 zu Wandhalterung ","100461",0,null,"STK",170.1,null,null,null,null,{"$f":"IF(H7132=\"\",\"0\",H7132*L7132)","v":0},null,null,null,"100461"]
["Technostar120",0,125,{"$f":"A7133&C7133&B7133","v":"Technostar1201250"}," ","Technostar Anlage Ø 125","Technostar120125","0",{"$f":"Technostar120!$J$11","v":9.99},"Anlage",0,1,{"$f":"I7133*1000","v":9990},null,{"$f":"ROUNDUP(P7133,2)","v":0},{"$f":"SUM(P7134:P7187)/1000","v":0}]
[{"$f":"A7133","v":"Technostar120"},{"$f":"B7133+1","v":1},{"$f":"C7133","v":125},"Technostar1201251"," ","TS120 125 Rohr mit Muffe L250mm","100014",250,null,"STK",23.5,null,null,null,null,{"$f":"IF(H7134=\"\",\"0\",H7134*L7134)","v":0}]
["Technostar120",2,125,"Technostar1201252"," ","TS120 125 Rohr mit Muffe L500mm ","100015",500,null,"STK",34.799999999999997,null,null,null,null,0]
["Technostar120",3,125,"Technostar1201253"," ","TS120 125 Rohr mit Muffe L1000mm ","100016",1000,null,"STK",57.3,null,null,null,null,0]
["Technostar120",4,125,"Technostar1201254"," ","TS120 125 Rohr mit Muffe L2000mm ","100017",2000,null,"STK",88.1,null,null,null,null,0]
["Technostar120",5,125,"Technostar1201255"," ","TS120 125 Kesselanschluss Reduktion zentr. 80","100162","0",null,"STK",154.1,null,null,null,null,0]
["Technostar120",6,125,"Technostar1201256"," ","TS120 125 Kesselanschluss Reduktion zentr. 110","100164","0",null,"STK",105.5,null,null,null,null,0]
["Technostar120",7,125,"Technostar1201257"," ","TS120 125 Kesselanschluss Erweiterung zentr. 130","100176","0",null,"STK",77.099999999999994,null,null,null,null,0]
["Technostar120",8,125,"Technostar1201258"," ","TS120 125 Lippendichtung Peroxyd für Muffe","100251","0",null,"STK",11.7,null,null,null,null,0]
["Technostar120",9,125,"Technostar1201259"," ","TS120 125 Kesselanschluss Reduktion exzentr. 80","100172","0",null,"STK",132.4,null,null,null,null,0]
["Technostar120",10,125,"Technostar12012510"," ","TS120 125 Kesselanschluss Reduktion exzentr. 110","100173","0",null,"STK",129.30000000000001,null,null,null,null,0]
["Technostar120",11,125,"Technostar12012511"," ","TS120 125 Kesselanschluss Erweiterung exzentr. 160","100178","0",null,"STK",143,null,null,null,null,0]
["Technostar120",12,125,"Technostar12012512"," ","TS120 125 Flanschverbindung komplett","100518","0",null,"STK",172.4,null,null,null,null,0]
["Technostar120",13,125,"Technostar12012513"," ","TS120 125 Kondensatablauf waagrecht","100197","0",null,"STK",209.1,null,null,null,null,0]
["Technostar120",14,125,"Technostar12012514"," ","TS120 125 Kondensatanblauf senkrecht ","100190",130,null,"STK",192.4,null,null,null,null,0]
["Technostar120",15,125,"Technostar12012515"," ","TS120 125 Bogen 15°","100100",106,null,"STK",26.1,null,null,null,null,0]
["Technostar120",16,125,"Technostar12012516"," ","TS120 125 Bogen 30°","100101",197,null,"STK",26.1,null,null,null,null,0]
["Technostar120",17,125,"Technostar12012517"," ","TS120 125 Bogen 45°","100102",217,null,"STK",26.1,null,null,null,null,0]
["Technostar120",18,125,"Technostar12012518"," ","TS120 125 Bogen 87°","100103",291,null,"STK",30.1,null,null,null,null,0]
["Technostar120",19,125,"Technostar12012519"," ","TS120 125 Revisionsbogen 87° ","100123",222,null,"STK",103.9,null,null,null,null,0]
["Technostar120",20,125,"Technostar12012520"," ","TS120 125 Revisionsrohr mit Schraubdeckel","100062",214,null,"STK",57.8,null,null,null,null,0]
["Technostar120",21,125,"Technostar12012521"," ","TS120 125 T-Stück 90°","100076",250,null,"STK",162.4,null,null,null,null,0]
["Technostar120",22,125,"Technostar12012522"," ","TS120 125 Abzweiger 45°","100082",350,null,"STK",173.3,null,null,null,null,0]
["Technostar120",23,125,"Technostar12012523"," ","TS120 125 Kaminabstützung komplett mit Bogen 87° ","100142","0",null,"STK",158.5,null,null,null,null,{"$f":"IF(H7156=\"\",\"0\",H7156*L7156)","v":0}]
["Technostar120",24,125,"Technostar12012524"," ","TS120 125 Wandfutter hinterlüftet inox","100134",149,null,"STK",124.9,null,null,null,null,{"$f":"IF(H7157=\"\",\"0\",H7157*L7157)","v":0}]
["Technostar120",25,125,"Technostar12012525"," ","TS120 125 200 Endmuffe schwarz mit Mündungsrohr","100207",100,null,"STK",111.8,null,null,null,null,{"$f":"IF(H7158=\"\",\"0\",H7158*L7158)","v":0}]
["Technostar120",26,125,"Technostar12012526"," ","TS120 125 Abstandhalter für starr","100150","0",null,"STK",12.6,null,null,null,null,0]
["Technostar120",27,125,"Technostar12012527"," ","TS120 125 Zentrierhalter Typ 65","100493","0",null,"STK",49.6,null,null,null,null,{"$f":"IF(H7160=\"\",\"0\",H7160*L7160)","v":0}]
["Technostar120",28,125,"Technostar12012528"," ","TS120 125 Zentrierhalter Typ 100","100492","0",null,"STK",51,null,null,null,null,0]
["Technostar120",29,125,"Technostar12012529"," ","TS120 125 Rohrhalter fest ohne Gewinderohr","100284","0",null,"STK",15.5,null,null,null,null,0]
["Technostar120",30,125,"Technostar12012530"," ","TS120 1/2\" Gewinderohr L2000mm","100308","0",null,"STK",23,null,null,null,null,0]
["Technostar120",31,125,"Technostar12012531"," ","TS120 125 Rohrhalter gleitend ohne Gewinderohr","100292","0",null,"STK",34.9,null,null,null,null,0]
["Technostar120",32,125,"Technostar12012532"," ","TS120 Temperarturbegrenzer 120° mit montage Nippel","100187","0",null,"STK",184.9,null,null,null,null,0]
["Technostar120",33,125,"Technostar12012533"," ","TS120 Verschlussnippel für Messöffnung","100258","0",null,"STK",9.5,null,null,null,null,0]
["Technostar120",34,125,"Technostar12012534"," ","TS120 Syphon Typ A","100256","0",null,"STK",39.5,null,null,null,null,0]
["Technostar120",35,125,"Technostar12012535"," ","TS120 Syphon Typ B","100257","0",null,"STK",35.6,null,null,null,null,0]
["Technostar120",36,125,"Technostar12012536"," ","Neutralisationsbox komplett","100265","0",null,"STK",225,null,null,null,null,0]
["Technostar120",37,125,"Technostar12012537"," ","Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",59,null,null,null,null,0]
["Technostar120",38,125,"Technostar12012538"," ","KER Putztür PTS1 145 x 275mm Alu bis  Ø120","103594","0",null,"STK",92,null,null,null,null,0]
["Technostar120",39,125,"Technostar12012539"," ","KER Putztür PTS2 200 x 275mm Alu für  Ø140- 250mm","103596","0",null,"STK",112,null,null,null,null,0]
["Technostar120",40,125,"Technostar12012540"," ","KER Schieberahmen zu PTS1 145 x 275 mm L90mm","103595","0",null,"STK",20,null,null,null,null,0]
["Technostar120",41,125,"Technostar12012541"," ","KER Schieberahmen zu PTS2 200 x 275mm L90mm","103597","0",null,"STK",21,null,null,null,null,0]
["Technostar120",42,125,"Technostar12012542"," ","CHZ 120-180 Zuluftgitter für Hinterlüftung ","103817","0",null,"STK",24,null,null,null,null,0]
["Technostar120",43,125,"Technostar12012543"," ","CHZ 200-300 Zuluftgitter für Hinterlüftung","103818","0",null,"STK",38,null,null,null,null,0]
["Technostar120",44,125,"Technostar12012544"," ","ZBH Schachttüre grundiert  200 x 300mm","103843","0",null,"STK",123,null,null,null,null,0]
["Technostar120",45,125,"Technostar12012545"," ","ZBH Schachttüre grundiert gasdicht 200 x 300mm","103844","0",null,"STK",206,null,null,null,null,0]
["Technostar120",46,125,"Technostar12012546"," ","TS120 Gleitmittel 250ml","100275","0",null,"STK",15.6,null,null,null,null,0]
["Technostar120",47,125,"Technostar12012547"," ","Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",6.2,null,null,null,null,0]
["Technostar120",48,125,"Technostar12012548"," ","TS120 Schlauchbriede zu Kondensatschlauch","100262","0",null,"STK",4.8,null,null,null,null,0]
["Technostar120",49,125,"Technostar12012549"," ","TS120 Montagebriede zu Kondensatschlauch","100263","0",null,"STK",4.8,null,null,null,null,0]
["Technostar120",50,125,"Technostar12012550"," ","CHZ Mantelstein EZ  280 x 280mm L330mm","103718","0",null,"STK",24,null,null,null,null,0]
["Technostar120",51,125,"Technostar12012551"," ","CHZ Mantelstein EZ  320 x 320mm L330mm Ø160mm","103719","0",null,"STK",19,null,null,null,null,0]
["Technostar120",52,125,"Technostar12012552"," ","CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",53,null,null,null,null,0]
["Technostar120",53,125,"Technostar12012553"," ","TS120 Schachtabdeckung 400x400mm Inox","100247","0",null,"STK",247.2,null,null,null,null,0]
["Technostar120",54,125,"Technostar12012554"," ","TS120 125 Schachtabdeckung für starres Rohr Inox","100226","0",null,"STK",329.6,null,null,null,null,0]
["Technostar120",55,125,"Technostar12012555"," ","TS120LAS 125/185 Rohr L 250 Inox ","100390",250,null,"STK",102,null,null,null,null,{"$f":"IF(H7188=\"\",\"0\",H7188*L7188)","v":0}]
["Technostar120",56,125,"Technostar12012556"," ","TS120LAS 125/185 Rohr L 500 Inox ","100391",500,null,"STK",132.9,null,null,null,null,0]
["Technostar120",57,125,"Technostar12012557"," ","TS120LAS 125/185 Rohr L 1000 Inox ","100392",1000,null,"STK",253.4,null,null,null,null,0]
["Technostar120",58,125,"Technostar12012558"," ","TS120LAS 125/185 Bogen 15° Inox","100435",155,null,"STK",195.7,null,null,null,null,0]
["Technostar120",59,125,"Technostar12012559"," ","TS120LAS 125/185 Bogen 30° Inox","100436",186,null,"STK",195.7,null,null,null,null,0]
["Technostar120",60,125,"Technostar12012560"," ","TS120LAS 125/185 Bogen 45° Inox","100437",188,null,"STK",216.3,null,null,null,null,0]
["Technostar120",61,125,"Technostar12012561"," ","TS120LAS 125/185 Bogen 87° Inox","100438",189,null,"STK",236.9,null,null,null,null,0]
["Technostar120",62,125,"Technostar12012562"," ","TS120LAS 125/185 Aussenwandanschluss komplett Inox","100401","0",null,"STK",803.4,null,null,null,null,0]
["Technostar120",63,125,"Technostar12012563"," ","TS120LAS 185 Abdeckblende  Inox","100420","0",null,"STK",52.3,null,null,null,null,0]
["Technostar120",64,125,{"$f":"A7197&C7197&B7197","v":"Technostar12012564"}," ","TS120LAS 125/185 Wandurchführung L500mm","100469","0",null,"STK",133.4,null,null,null,null,0]
[{"$f":"A7197","v":"Technostar120"},{"$f":"B7197+1","v":65},{"$f":"C7197","v":125},{"$f":"A7198&C7198&B7198","v":"Technostar12012565"}," ","TS120LAS 125/185 Revisionsrohr Inox ","100416","0",null,"STK",303.89999999999998,null,null,null,null,0]
[{"$f":"A7198","v":"Technostar120"},{"$f":"B7198+1","v":66},{"$f":"C7198","v":125},{"$f":"A7199&C7199&B7199","v":"Technostar12012566"}," ","TS120LAS 125/185 Dachdurchführung Inox","100423","0",null,"STK",432.6,null,null,null,null,0]
[{"$f":"A7199","v":"Technostar120"},{"$f":"B7199+1","v":67},{"$f":"C7199","v":125},{"$f":"A7200&C7200&B7200","v":"Technostar12012567"}," ","TS120LAS 125 Mündungsrohr Inox","100453",250,null,"STK",61.7,null,null,null,null,0]
[{"$f":"A7197","v":"Technostar120"},{"$f":"B7197+1","v":65},{"$f":"C7197","v":125},{"$f":"A7201&C7201&B7201","v":"Technostar12012565"}," ","TS120LAS 125 Klemmband Inox","100442","0",null,"STK",51.4,null,null,null,null,{"$f":"IF(H7201=\"\",\"0\",H7201*L7201)","v":0}]
["Technostar120",66,125,{"$f":"A7202&C7202&B7202","v":"Technostar12012566"}," ","TS120LAS 125/185 Zuluftstutzen Inox","100441","0",null,"STK",324.5,null,null,null,null,0]
["Technostar120",67,125,"Technostar12012567"," ","TS120LAS 125/185 Mündungsabschluss mit Klemmband","100447",145,null,"STK",213.3,null,null,null,null,0]
["Technostar120",68,125,"Technostar12012568"," ","TS120LAS 160/185 Dachdurchführ. L1000mm schwarz","100484","0",null,"STK",566.5,null,null,null,null,0]
["Technostar120",66,125,"Technostar12012566"," ","TS120 125/185 Dachpfanne 25-45°  schwarz","100240","0",null,"STK",267.8,null,null,null,null,0]
["Technostar120",67,125,"Technostar12012567"," ","TS120LAS 160 Verl. Typ 3 zu Aussenwandanschluss","100410","0",null,"STK",231.9,null,null,null,null,{"$f":"IF(H7206=\"\",\"0\",H7206*L7206)","v":0}]
["Technostar120",68,125,"Technostar12012568"," ","TS120LAS 185 Verl. Typ 1 zu Aussenwandanschluss","100411","0",null,"STK",185.4,null,null,null,null,{"$f":"IF(H7207=\"\",\"0\",H7207*L7207)","v":0}]
["Technostar120",69,125,"Technostar12012569"," ","TS120LAS 185 Verl. Typ 2 zu Aussenwandanschluss","100412","0",null,"STK",257,null,null,null,null,{"$f":"IF(H7208=\"\",\"0\",H7208*L7208)","v":0}]
["Technostar120",67,125,"Technostar12012567"," ","TS120LAS 185 Verl. Typ 3 zu Aussenwandanschluss","100413","0",null,"STK",308.8,null,null,null,null,{"$f":"IF(H7209=\"\",\"0\",H7209*L7209)","v":0}]
[{"$f":"A7209","v":"Technostar120"},{"$f":"B7209+1","v":68},{"$f":"C7209","v":125},{"$f":"A7210&\" \"&C7210&B7210","v":"Technostar120 12568"},null,"LBS 200 Leichtbauschacht i 200mm A 290mm L1000mm","140753","0",null,"STK",101]
[{"$f":"A7210","v":"Technostar120"},{"$f":"B7210+1","v":69},{"$f":"C7210","v":125},{"$f":"A7211&\" \"&C7211&B7211","v":"Technostar120 12569"},null,"LBS Kleber zu Leichtbauschacht 1kg","103829","0",null,"STK",9]
[{"$f":"A7211","v":"Technostar120"},{"$f":"B7211+1","v":70},{"$f":"C7211","v":125},{"$f":"A7212&\" \"&C7212&B7212","v":"Technostar120 12570"},null,"ABS Kaminhalterung Standard","104256","0",null,"STK",263]
[{"$f":"A7212","v":"Technostar120"},{"$f":"B7212+1","v":71},{"$f":"C7212","v":125},{"$f":"A7213&\" \"&C7213&B7213","v":"Technostar120 12571"},null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",81]
["Technostar120",0,160,{"$f":"A7214&C7214&B7214","v":"Technostar1201600"}," ","Technostar Anlage Ø 160","Technostar120160","0",{"$f":"Technostar120!$J$11","v":9.99},"Anlage",0,1,{"$f":"I7214*1000","v":9990},null,{"$f":"ROUNDUP(P7214,2)","v":0},{"$f":"SUM(P7215:P7268)/1000","v":0}]
[{"$f":"A7214","v":"Technostar120"},{"$f":"B7214+1","v":1},{"$f":"C7214","v":160},"Technostar1201601"," ","TS120 160 Rohr mit Muffe L250mm","100018",250,null,"STK",36.299999999999997,null,null,null,null,{"$f":"IF(H7215=\"\",\"0\",H7215*L7215)","v":0}]
["Technostar120",2,160,"Technostar1201602"," ","TS120 160 Rohr mit Muffe L500mm ","100019",500,null,"STK",54.2,null,null,null,null,0]
["Technostar120",3,160,"Technostar1201603"," ","TS120 160 Rohr mit Muffe L1000mm ","100020",1000,null,"STK",90.1,null,null,null,null,0]
["Technostar120",4,160,"Technostar1201604"," ","TS120 160 Rohr mit Muffe L2000mm ","100021",2000,null,"STK",140.6,null,null,null,null,0]
["Technostar120",5,160,"Technostar1201605"," ","TS120 160 Kesselanschluss Reduktion zentr. 130","100167","0",null,"STK",222.4,null,null,null,null,0]
["Technostar120",6,160,"Technostar1201606"," ","TS120 160 Kesselanschluss Reduktion zentr. 150","100168","0",null,"STK",245.2,null,null,null,null,0]
["Technostar120",7,160,"Technostar1201607"," ","TS120 160 Lippendichtung Peroxyd für Muffe","100252","0",null,"STK",16.3,null,null,null,null,0]
["Technostar120",8,160,"Technostar1201608"," ","TS120 160 Kesselanschluss Erweiterung exzentr. 200","100179","0",null,"STK",212.5,null,null,null,null,0]
["Technostar120",9,160,"Technostar1201609"," ","TS120 160 Flanschverbindung komplett","100519","0",null,"STK",205.4,null,null,null,null,0]
["Technostar120",10,160,"Technostar12016010"," ","TS120 160 Kondensatablauf waagrecht","100198","0",null,"STK",287.3,null,null,null,null,0]
["Technostar120",11,160,"Technostar12016011"," ","TS120 160 Kondensatanblauf senkrecht ","100191",140,null,"STK",218.9,null,null,null,null,0]
["Technostar120",12,160,"Technostar12016012"," ","TS120 160 Bogen 15°","100104",121,null,"STK",36.799999999999997,null,null,null,null,0]
["Technostar120",13,160,"Technostar12016013"," ","TS120 160 Bogen 30°","100105",235,null,"STK",36.799999999999997,null,null,null,null,0]
["Technostar120",14,160,"Technostar12016014"," ","TS120 160 Bogen 45°","100106",261,null,"STK",36.799999999999997,null,null,null,null,0]
["Technostar120",15,160,"Technostar12016015"," ","TS120 160 Bogen 87°","100107",355,null,"STK",42.4,null,null,null,null,0]
["Technostar120",16,160,"Technostar12016016"," ","TS120 160 Revisionsbogen 87° ","100124",295,null,"STK",223.1,null,null,null,null,0]
["Technostar120",17,160,"Technostar12016017"," ","TS120 160 Revisionsrohr mit Schraubdeckel","100063",280,null,"STK",117.8,null,null,null,null,0]
["Technostar120",18,160,"Technostar12016018"," ","TS120 160 T-Stück 90°","100077",280,null,"STK",231.7,null,null,null,null,0]
["Technostar120",19,160,"Technostar12016019"," ","TS120 160 Abzweiger 45°","100083",400,null,"STK",263.39999999999998,null,null,null,null,0]
["Technostar120",20,160,"Technostar12016020"," ","TS120 160 Kaminabstützung komplett mit Bogen 87°","100143","0",null,"STK",201.8,null,null,null,null,0]
["Technostar120",21,160,"Technostar12016021"," ","TS120 160 Wandfutter hinterlüftet inox","100135",149,null,"STK",139.4,null,null,null,null,0]
["Technostar120",22,160,"Technostar12016022"," ","TS120 160 250 Endmuffe schwarz mit Mündungsrohr","100208",100,null,"STK",142.1,null,null,null,null,0]
["Technostar120",23,160,"Technostar12016023"," ","TS120 160 Flexrohr verschraubbar L1000mm","100039",1000,null,"STK",175.7,null,null,null,null,{"$f":"IF(H7237=\"\",\"0\",H7237*L7237)","v":0}]
["Technostar120",24,160,"Technostar12016024"," ","TS120 160 Revisionsrohr 1000mm für Flex","100052","0",null,"STK",401.7,null,null,null,null,{"$f":"IF(H7238=\"\",\"0\",H7238*L7238)","v":0}]
["Technostar120",25,160,"Technostar12016025"," ","TS120 160  Revisionsrohr für Flex kurz","100051",700,null,"STK",355.4,null,null,null,null,{"$f":"IF(H7239=\"\",\"0\",H7239*L7239)","v":0}]
["Technostar120",26,160,"Technostar12016026"," ","TS120 160 Aufhängeschelle zu Flex ","100053","0",null,"STK",30.9,null,null,null,null,0]
["Technostar120",27,160,"Technostar12016027"," ","TS120 160 Abstandhalter für starr","100152","0",null,"STK",13.5,null,null,null,null,0]
["Technostar120",28,160,"Technostar12016028"," ","TS120 160 Abstandhalter für flex ","100151","0",null,"STK",13.9,null,null,null,null,0]
["Technostar120",29,160,"Technostar12016029"," ","TS120 160 Zentrierhalter Typ 65","100495","0",null,"STK",52,null,null,null,null,0]
["Technostar120",30,160,"Technostar12016030"," ","TS120 160 Zentrierhalter Typ 100","100494","0",null,"STK",53.4,null,null,null,null,0]
["Technostar120",31,160,"Technostar12016031"," ","TS120 160 Rohrhalter fest ohne Gewinderohr","100285","0",null,"STK",17.2,null,null,null,null,0]
["Technostar120",32,160,"Technostar12016032"," ","TS120 1/2\" Gewinderohr L2000mm","100308","0",null,"STK",23,null,null,null,null,0]
["Technostar120",33,160,"Technostar12016033"," ","TS120 160 Rohrhalter gleitend ohne Gewinderohr","100293","0",null,"STK",36,null,null,null,null,0]
["Technostar120",34,160,"Technostar12016034"," ","TS120 Temperarturbegrenzer 120° mit montage Nippel","100187","0",null,"STK",184.9,null,null,null,null,0]
["Technostar120",35,160,"Technostar12016035"," ","TS120 Verschlussnippel für Messöffnung","100258","0",null,"STK",9.5,null,null,null,null,0]
["Technostar120",36,160,"Technostar12016036"," ","TS120 Syphon Typ A","100256","0",null,"STK",39.5,null,null,null,null,0]
["Technostar120",37,160,"Technostar12016037"," ","TS120 Syphon Typ B","100257","0",null,"STK",35.6,null,null,null,null,0]
["Technostar120",38,160,"Technostar12016038"," ","Neutralisationsbox komplett","100265","0",null,"STK",225,null,null,null,null,0]
["Technostar120",39,160,"Technostar12016039"," ","Nachfüllset zu Neutralisationsbox","100266","0",null,"STK",59,null,null,null,null,0]
["Technostar120",40,160,"Technostar12016040"," ","KER Putztür PTS1 145 x 275mm Alu bis  Ø120","103594","0",null,"STK",92,null,null,null,null,0]
["Technostar120",41,160,"Technostar12016041"," ","KER Putztür PTS2 200 x 275mm Alu für  Ø140- 250mm","103596","0",null,"STK",112,null,null,null,null,0]
["Technostar120",42,160,"Technostar12016042"," ","KER Schieberahmen zu PTS1 145 x 275 mm L90mm","103595","0",null,"STK",20,null,null,null,null,0]
["Technostar120",43,160,"Technostar12016043"," ","KER Schieberahmen zu PTS2 200 x 275mm L90mm","103597","0",null,"STK",21,null,null,null,null,0]
["Technostar120",44,160,"Technostar12016044"," ","CHZ 120-180 Zuluftgitter für Hinterlüftung ","103817","0",null,"STK",24,null,null,null,null,0]
["Technostar120",45,160,"Technostar12016045"," ","CHZ 200-300 Zuluftgitter für Hinterlüftung","103818","0",null,"STK",38,null,null,null,null,0]
["Technostar120",46,160,"Technostar12016046"," ","ZBH Schachttüre grundiert  200 x 300mm","103843","0",null,"STK",123,null,null,null,null,0]
["Technostar120",47,160,{"$f":"A7261&C7261&B7261","v":"Technostar12016047"}," ","ZBH Schachttüre grundiert gasdicht 200 x 300mm","103844","0",null,"STK",206,null,null,null,null,0]
["Technostar120",48,160,"Technostar12016048"," ","TS120 Gleitmittel 250ml","100275","0",null,"STK",15.6,null,null,null,null,0]
["Technostar120",49,160,"Technostar12016049"," ","Kondesatschlauch 36mm L1000mm","100264","0",null,"STK",6.2,null,null,null,null,0]
["Technostar120",50,160,"Technostar12016050"," ","TS120 Schlauchbriede zu Kondensatschlauch","100262","0",null,"STK",4.8,null,null,null,null,0]
["Technostar120",51,160,"Technostar12016051"," ","TS120 Montagebriede zu Kondensatschlauch","100263","0",null,"STK",4.8,null,null,null,null,0]
["Technostar120",52,160,"Technostar12016052"," ","CHZ Mantelstein EZ  320 x 320mm L330mm Ø160mm","103719","0",null,"STK",19,null,null,null,null,{"$f":"IF(H7266=\"\",\"0\",H7266*L7266)","v":0}]
["Technostar120",53,160,"Technostar12016053"," ","CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",53,null,null,null,null,0]
["Technostar120",54,160,"Technostar12016054"," ","TS120 160 Schachtabdeckung für starres Rohr Inox","100228","0",null,"STK",365.7,null,null,null,null,0]
["Technostar120",55,160,{"$f":"A7269&\" \"&C7269&B7269","v":"Technostar120 16055"},null,"LBS 200 Leichtbauschacht i 200mm A 290mm L1000mm","140753","0",null,"STK",101]
["Technostar120",56,160,{"$f":"A7270&\" \"&C7270&B7270","v":"Technostar120 16056"},null,"LBS Kleber zu Leichtbauschacht 1kg","103829","0",null,"STK",9]
["Technostar120",57,160,{"$f":"A7271&\" \"&C7271&B7271","v":"Technostar120 16057"},null,"ABS Kaminhalterung Standard","104256","0",null,"STK",263]
["Technostar120",58,160,{"$f":"A7272&\" \"&C7272&B7272","v":"Technostar120 16058"},null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",81]
["Technostar120",0,200,"Technostar1202000"," ","Technostar Anlage Ø 200","Technostar120200","0",{"$f":"Technostar120!$J$11","v":9.99},"Anlage",0,1,{"$f":"I7273*1000","v":9990},null,{"$f":"ROUNDUP(P7273,2)","v":0},{"$f":"SUM(P7274:P7354)/1000","v":0}]
[{"$f":"A7273","v":"Technostar120"},{"$f":"B7273+1","v":1},{"$f":"C7273","v":200},"Technostar1202001"," ","TS120 200 Rohr mit Muffe L500mm ","100023",500,null,"STK",134.9,null,null,null,null,{"$f":"IF(H7274=\"\",\"0\",H7274*L7274)","v":0}]
["Technostar120",2,200,"Technostar1202002"," ","TS120 200 Rohr mit Muffe L1000mm ","100024",1000,null,"STK",184.2,null,null,null,null,0]
["Technostar120",3,200,"Technostar1202003"," ","TS120 200 Rohr mit Muffe L2000mm ","100025",2000,null,"STK",275.10000000000002,null,null,null,null,0]
["Technostar120",4,200,"Technostar1202004"," ","TS120 200 Kesselanschluss Reduktion zentr. 180","100169","0",null,"STK",226.6,null,null,null,null,0]
["Technostar120",5,200,"Technostar1202005"," ","TS120 200 Kesselanschluss Erweiterung exzentr. 250","100180",165,null,"STK",257.5,null,null,null,null,0]
["Technostar120",6,200,"Technostar1202006"," ","TS120 200 Kondensatablauf waagrecht ","100199","0",null,"STK",252.4,null,null,null,null,0]
["Technostar120",7,200,"Technostar1202007"," ","TS120 200 Kondensatanblauf senkrecht ","100192",170,null,"STK",252.4,null,null,null,null,0]
["Technostar120",8,200,"Technostar1202008"," ","TS120 200 Bogen 30°","100108",390,null,"STK",206,null,null,null,null,0]
["Technostar120",9,200,"Technostar1202009"," ","TS120 200 Bogen 45°","100109",480,null,"STK",216.3,null,null,null,null,0]
["Technostar120",10,200,"Technostar12020010"," ","TS120 200 Bogen 87°","100110",400,null,"STK",257.5,null,null,null,null,0]
["Technostar120",11,200,"Technostar12020011"," ","TS120 200 Revisionsbogen 87° ","100125",310,null,"STK",288.39999999999998,null,null,null,null,0]
["Technostar120",12,200,"Technostar12020012"," ","TS120 200 Revisionsrohr mit Schraubdeckel","100064",340,null,"STK",257.5,null,null,null,null,0]
["Technostar120",13,200,"Technostar12020013"," ","TS120 200 T-Stück 90°","100078",350,null,"STK",257.5,null,null,null,null,0]
["Technostar120",14,200,"Technostar12020014"," ","TS120 200 Abzweiger 45°","100084",470,null,"STK",309,null,null,null,null,0]
[{"$f":"A7287","v":"Technostar120"},{"$f":"B7287+1","v":15},{"$f":"C7287","v":200},{"$f":"A7288&C7288&B7288","v":"Technostar12020015"}," ","TS120 200 Rohrhalter fest ohne Gewinderohr","100286","0",null,"STK",21.5,null,null,null,null,{"$f":"IF(H7288=\"\",\"0\",H7288*L7288)","v":0}]
["Technostar120",16,200,{"$f":"A7289&C7289&B7289","v":"Technostar12020016"}," ","TS120 200 Rohrhalter gleitend ohne Gewinderohr","100294","0",null,"STK",44.2,null,null,null,null,{"$f":"IF(H7289=\"\",\"0\",H7289*L7289)","v":0}]
["Technostar120",17,200,{"$f":"A7290&C7290&B7290","v":"Technostar12020017"}," ","TS120 Temperarturbegrenzer 120° mit montage Nippel","100187","0",null,"STK",184.9,null,null,null,null,{"$f":"IF(H7290=\"\",\"0\",H7290*L7290)","v":0}]
["Technostar120",18,200,{"$f":"A7291&C7291&B7291","v":"Technostar12020018"}," ","TS120 Verschlussnippel für Messöffnung","100258","0",null,"STK",9.5,null,null,null,null,{"$f":"IF(H7291=\"\",\"0\",H7291*L7291)","v":0}]
["Technostar120",19,200,{"$f":"A7292&\" \"&C7292&B7292","v":"Technostar120 20019"},null,"LBS 270 Leichtbauschacht i 270mm A 360mm L1000mm","103827","0",null,"STK",130]
["Technostar120",20,200,{"$f":"A7293&\" \"&C7293&B7293","v":"Technostar120 20020"},null,"LBS Kleber zu Leichtbauschacht 1kg","103829","0",null,"STK",9]
["Technostar120",21,200,{"$f":"A7294&\" \"&C7294&B7294","v":"Technostar120 20021"},null,"ABS Kaminhalterung Standard","104256","0",null,"STK",263]
["Technostar120",22,200,{"$f":"A7295&\" \"&C7295&B7295","v":"Technostar120 20022"},null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",81]
["Technostar120",23,200,{"$f":"A7296&\" \"&C7296&B7296","v":"Technostar120 20023"},null,"TS120 200 Wandfutter hinterlüftet inox","100136","0",null,"STK",87.2]
["Technostar120",24,200,"Technostar120 20024",null,"TS120 200 Kaminabstützung komplett mit Bogen 87°","100144","0",null,"STK",279]
["Technostar120",25,200,"Technostar120 20025",null,"TS120 200 Abstandhalter Inox","100153","0",null,"STK",49]
["Technostar120",26,200,"Technostar120 20026",null,"TS120 200 Schachtabdeckung für starres Rohr Inox","140734","0",null,"STK",391.4]
["Technostar120",0,250,{"$f":"A7300&C7300&B7300","v":"Technostar1202500"}," ","Technostar Anlage Ø 250","Technostar120250","0",{"$f":"Technostar120!$J$11","v":9.99},"Anlage",0,1,{"$f":"I7300*1000","v":9990},null,{"$f":"ROUNDUP(P7300,2)","v":0},{"$f":"SUM(P7301:P7369)/1000","v":0}]
[{"$f":"A7300","v":"Technostar120"},{"$f":"B7300+1","v":1},{"$f":"C7300","v":250},"Technostar1202501"," ","TS120 250 Rohr mit Muffe L500mm ","100026",500,null,"STK",166.9,null,null,null,null,{"$f":"IF(H7301=\"\",\"0\",H7301*L7301)","v":0}]
["Technostar120",2,250,"Technostar1202502"," ","TS120 250 Rohr mit Muffe L1000mm ","100027",1000,null,"STK",231.4,null,null,null,null,0]
["Technostar120",3,250,"Technostar1202503"," ","TS120 250 Rohr mit Muffe L2000mm ","100028",2000,null,"STK",357,null,null,null,null,0]
["Technostar120",4,250,"Technostar1202504"," ","TS120 250 Kesselanschluss Reduktion zentr. 200","100170","0",null,"STK",226.6,null,null,null,null,0]
["Technostar120",5,250,"Technostar1202505"," ","TS120 250 Kesselanschluss Erweiterung exzentr. 315","100181",230,null,"STK",278.10000000000002,null,null,null,null,0]
["Technostar120",6,250,"Technostar1202506"," ","TS120 250 Kondensatablauf waagrecht ","100200","0",null,"STK",324.5,null,null,null,null,0]
["Technostar120",7,250,"Technostar1202507"," ","TS120 250 Kondensatanblauf senkrecht ","100193",170,null,"STK",324.5,null,null,null,null,0]
["Technostar120",8,250,"Technostar1202508"," ","TS120 250 Bogen 30°","100111",430,null,"STK",226.6,null,null,null,null,0]
["Technostar120",9,250,"Technostar1202509"," ","TS120 250 Bogen 45°","100112",510,null,"STK",247.2,null,null,null,null,0]
["Technostar120",10,250,"Technostar12025010"," ","TS120 250 Bogen 87°","100113",475,null,"STK",298.7,null,null,null,null,0]
["Technostar120",11,250,"Technostar12025011"," ","TS120 250 Revisionsbogen 87° ","100126",310,null,"STK",309,null,null,null,null,0]
["Technostar120",12,250,"Technostar12025012"," ","TS120 250 Revisionsrohr mit Schraubdeckel","100065",340,null,"STK",288.39999999999998,null,null,null,null,0]
["Technostar120",13,250,"Technostar12025013"," ","TS120 250 T-Stück 90°","100079",400,null,"STK",288.39999999999998,null,null,null,null,0]
["Technostar120",14,250,"Technostar12025014"," ","TS120 250 Abzweiger 45°","100085",535,null,"STK",360.5,null,null,null,null,0]
["Technostar120",15,250,{"$f":"A7315&\" \"&C7315&B7315","v":"Technostar120 25015"},null,"LBS 320 Leichtbauschacht i 320mm A 410mm L1000mm","103828","0",null,"STK",149]
["Technostar120",16,250,{"$f":"A7316&\" \"&C7316&B7316","v":"Technostar120 25016"},null,"LBS Kleber zu Leichtbauschacht 1kg","103829","0",null,"STK",9]
["Technostar120",17,250,{"$f":"A7317&\" \"&C7317&B7317","v":"Technostar120 25017"},null,"ABS Kaminhalterung Standard","104256","0",null,"STK",263]
["Technostar120",18,250,{"$f":"A7318&\" \"&C7318&B7318","v":"Technostar120 25018"},null,"ABS Verstärkung zu Kaminhalterung","104257","0",null,"STK",81]
["Technostar120",19,250,{"$f":"A7319&\" \"&C7319&B7319","v":"Technostar120 25019"},null,"TS120 250 Wandfutter hinterlüftet inox","100137","0",null,"STK",90.3]
["Technostar120",20,250,"Technostar120 25020",null,"TS120 250 Kaminabstützung verstellbar ohne Bogen","100145","0",null,"STK",343.5]
["Technostar120",21,250,"Technostar120 25021",null,"TS120 250 Rohrhalter fest ohne Gewinderohr","100287","0",null,"STK",32]
["Technostar120",22,250,{"$f":"A7322&\" \"&C7322&B7322","v":"Technostar120 25022"},null,"TS120 250 Rohrhalter gleitend ohne Gewinderohr","100295","0",null,"STK",45]
["Technostar120",23,250,"Technostar120 25023",null,"TS120 250 Schachtabdeckung für starres Rohr Inox","140735","0",null,"STK",518.1]
["ISOLIT",0,16,{"$f":"A7324&C7324&B7324","v":"ISOLIT160"},"P","Schiedel ISOLIT 16/16","ISOLIT16","0",{"$f":"Daten!$B$741","v":8.75},"Anlage",0,null,{"$f":"I7324*1000","v":8750}]
[{"$f":"A7324","v":"ISOLIT"},{"$f":"B7324+1","v":1},{"$f":"C7324","v":16},"ISOLIT161",null,"ISOLIT 160 Einzügerelement 16","103625",250,null,"STK",38,{"$f":"ROUND(M7325,0)-M7326-M7327-M7328-M7328","v":31},{"$f":"((M7324)*4)/1000","v":35}]
["ISOLIT",2,16,"ISOLIT162",null,"ISOLIT 160 Anfängerelement 16","103637",250,null,"STK",125,{"$f":"IF(M7326=0,\"\",M7326)","v":1},{"$f":"IF(Daten!$D$741=2,1,0)","v":1}]
["ISOLIT",3,16,"ISOLIT163",null,"ISOLIT 160 Russtürelement gasdicht RE 16","103647",250,null,"STK",527,{"$f":"IF(M7327=0,\"\",M7327)","v":1},{"$f":"IF(Daten!$D$748=1,0,Daten!$E$748)","v":1}]
["ISOLIT",4,16,"ISOLIT164",null,"ISOLIT 160 Rauchrohranschlusselement RA 16/16/90°","103641",500,null,"STK",282,{"$f":"IF(M7328=0,\"\",M7328)","v":1},{"$f":"IF(Daten!$D$756=1,0,Daten!$E$756)","v":1}]
["ISOLIT",5,16,"ISOLIT165",null,"CHZ 160 Abdeckplatte Beton 580 x 580mm Loch ?200mm","103780","0",null,"STK",149,{"$f":"IF(Daten!$D$764=1,\"\",1)","v":1}]
["ISOLIT",6,16,"ISOLIT166",null,"ISOLIT 160 Kombi-Mündungs-Manchette Inox 16","103669","0",null,"STK",208,{"$f":"IF(N7335=0,1,\"\")","v":1}]
["ISOLIT",7,16,"ISOLIT167",null,"CHZ Abdeckplatte Beton 600 x 600mm ohne Loch","103786","0",null,"STK",137]
["ISOLIT",8,16,"ISOLIT168",null,"CHZ Postament 80 x 80mm  L250mm","103789","0",null,"STK",28]
["ISOLIT",9,16,"ISOLIT169",null,"ISOLIT 160 Schleifung einzügig 16","103658","0",null,"STK",423,{"$f":"IF(Daten!$D$772=1,\"\",Daten!$E$772)","v":""}]
["ISOLIT",10,16,"ISOLIT1610",null,"CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",53,{"$f":"ROUNDUP(M7334,0)","v":3},{"$f":"I7324/3.1","v":2.82258064516129}]
["ISOLIT",11,16,"ISOLIT1611",null,"ISOLIT 160 Basten Standard Inox eckig  160mm","103673","0",null,"STK",302,{"$f":"IF(Daten!$D$781=2,1,\"\")","v":""},null,{"$f":"SUM(L7335:L7338)","v":0}]
["ISOLIT",12,16,"ISOLIT1612",null,"ISOLIT 160 Basten Standard Kupfer eckig  160mm","103677","0",null,"STK",323,{"$f":"IF(Daten!$D$781=3,1,\"\")","v":""}]
["ISOLIT",13,16,"ISOLIT1613",null,"ISOLIT 160 Sairlift Inox eckig  160mm","103681","0",null,"STK",359,{"$f":"IF(Daten!$D$781=4,1,\"\")","v":""}]
["ISOLIT",14,16,"ISOLIT1614",null,"ISOLIT 160 Sairlift Kupfer eckig 160mm","103688","0",null,"STK",374,{"$f":"IF(Daten!$D$781=5,1,\"\")","v":""}]
["ISOLIT",0,20,{"$f":"A7339&C7339&B7339","v":"ISOLIT200"},"P","Schiedel ISOLIT 20/20","ISOLIT20","0",{"$f":"Daten!$B$741","v":8.75},"Anlage",0,null,{"$f":"I7339*1000","v":8750}]
[{"$f":"A7339","v":"ISOLIT"},{"$f":"B7339+1","v":1},{"$f":"C7339","v":20},"ISOLIT201",null,"ISOLIT 200 Einzügerelement 20","103626",250,null,"STK",47,{"$f":"ROUND(M7340,0)-M7341-M7342-M7343-M7343","v":31},{"$f":"((M7339)*4)/1000","v":35}]
["ISOLIT",2,20,"ISOLIT202",null,"ISOLIT 200 Anfängerelement 20","103638",250,null,"STK",129,{"$f":"IF(M7341=0,\"\",M7341)","v":1},{"$f":"IF(Daten!$D$741=2,1,0)","v":1}]
["ISOLIT",3,20,"ISOLIT203",null,"ISOLIT 200 Russtürelement gasdicht RE 20","103648",250,null,"STK",529,{"$f":"IF(M7342=0,\"\",M7342)","v":1},{"$f":"IF(Daten!$D$748=1,0,Daten!$E$748)","v":1}]
["ISOLIT",4,20,"ISOLIT204",null,"ISOLIT 200 Rauchrohranschlusselement RA 20/20/90°","103642",500,null,"STK",291,{"$f":"IF(M7343=0,\"\",M7343)","v":1},{"$f":"IF(Daten!$D$756=1,0,Daten!$E$756)","v":1}]
["ISOLIT",5,20,"ISOLIT205",null,"CHZ 160 Abdeckplatte Beton 580 x 580mm Loch ?200mm","103780","0",null,"STK",149,{"$f":"IF(Daten!$D$764=1,\"\",1)","v":1}]
["ISOLIT",6,20,"ISOLIT206",null,"ISOLIT 200 Kombi-Mündungs-Manchette Inox 20","103670","0",null,"STK",263,{"$f":"IF(N7350=0,1,\"\")","v":1}]
["ISOLIT",7,20,"ISOLIT207",null,"CHZ Abdeckplatte Beton 600 x 600mm ohne Loch","103786","0",null,"STK",137]
["ISOLIT",8,20,"ISOLIT208",null,"CHZ Postament 80 x 80mm  L250mm","103789","0",null,"STK",28]
["ISOLIT",9,20,"ISOLIT209",null,"ISOLIT 200 Schleifung einzügig 20","103663","0",null,"STK",513,{"$f":"IF(Daten!$D$772=1,\"\",Daten!$E$772)","v":""}]
["ISOLIT",10,20,"ISOLIT2010",null,"CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",53,{"$f":"ROUNDUP(M7349,0)","v":4},{"$f":"I7339/2.7","v":3.2407407407407405}]
["ISOLIT",11,20,"ISOLIT2011",null,"ISOLIT 200 Basten Standard Inox eckig  200mm","103674","0",null,"STK",338,{"$f":"IF(Daten!$D$781=2,1,\"\")","v":""},null,{"$f":"SUM(L7350:L7353)","v":0}]
["ISOLIT",12,20,"ISOLIT2012",null,"ISOLIT 200 Basten Standard Kupfer eckig  200mm","103678","0",null,"STK",351,{"$f":"IF(Daten!$D$781=3,1,\"\")","v":""}]
["ISOLIT",13,20,"ISOLIT2013",null,"ISOLIT 200 Sairlift Inox eckig  200mm","103682","0",null,"STK",375,{"$f":"IF(Daten!$D$781=4,1,\"\")","v":""}]
["ISOLIT",14,20,"ISOLIT2014",null,"ISOLIT 200 Sairlift Kupfer eckig  200mm","103687","0",null,"STK",389,{"$f":"IF(Daten!$D$781=5,1,\"\")","v":""}]
["ISOLIT",0,25,{"$f":"A7354&C7354&B7354","v":"ISOLIT250"},"P","Schiedel ISOLIT 25/25","ISOLIT25","0",{"$f":"Daten!$B$741","v":8.75},"Anlage",0,null,{"$f":"I7354*1000","v":8750}]
[{"$f":"A7354","v":"ISOLIT"},{"$f":"B7354+1","v":1},{"$f":"C7354","v":25},"ISOLIT251",null,"ISOLIT 250 Einzügerelement 25","103627",250,null,"STK",52,{"$f":"ROUND(M7355,0)-M7356-M7357-M7358-M7358","v":31},{"$f":"((M7354)*4)/1000","v":35}]
["ISOLIT",2,25,"ISOLIT252",null,"ISOLIT 250 Anfängerelement 25","103639",250,null,"STK",136,{"$f":"IF(M7356=0,\"\",M7356)","v":1},{"$f":"IF(Daten!$D$741=2,1,0)","v":1}]
["ISOLIT",3,25,"ISOLIT253",null,"ISOLIT 250 Russtürelement gasdicht RE 25","103649",250,null,"STK",535,{"$f":"IF(M7357=0,\"\",M7357)","v":1},{"$f":"IF(Daten!$D$748=1,0,Daten!$E$748)","v":1}]
["ISOLIT",4,25,"ISOLIT254",null,"ISOLIT 250 Rauchrohranschlusselement RA 25/25/90°","103644",500,null,"STK",300,{"$f":"IF(M7358=0,\"\",M7358)","v":1},{"$f":"IF(Daten!$D$756=1,0,Daten!$E$756)","v":1}]
["ISOLIT",5,25,"ISOLIT255",null,{"$f":"VLOOKUP(G7359,sanschie!A:E,5,0)","v":"CHZ 200 Abdeckplatte Beton 680 x 680mm Loch ?250mm"},"103781","0",null,"STK",177,{"$f":"IF(Daten!$D$764=1,\"\",1)","v":1}]
["ISOLIT",6,25,"ISOLIT256",null,"ISOLIT 250 Kombi-Mündungs-Manchette Inox 25","103671","0",null,"STK",278,{"$f":"IF(N7365=0,1,\"\")","v":1}]
["ISOLIT",7,25,"ISOLIT257",null,"CHZ Abdeckplatte Beton 680 x 680mm ohne Loch","103787","0",null,"STK",160]
["ISOLIT",8,25,"ISOLIT258",null,"CHZ Postament 80 x 80mm  L250mm","103789","0",null,"STK",28]
["ISOLIT",9,25,"ISOLIT259",null,"ISOLIT 250 Schleifung einzügig 25","103664","0",null,"STK",586,{"$f":"IF(Daten!$D$772=1,\"\",Daten!$E$772)","v":""}]
["ISOLIT",10,25,"ISOLIT2510",null,"CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",53,{"$f":"ROUNDUP(M7364,0)","v":4},{"$f":"I7354/2.3","v":3.804347826086957}]
["ISOLIT",11,25,"ISOLIT2511",null,"ISOLIT 250 Basten Standard Inox eckig  250mm","103675","0",null,"STK",375,{"$f":"IF(Daten!$D$781=2,1,\"\")","v":""},null,{"$f":"SUM(L7365:L7368)","v":0}]
["ISOLIT",12,25,"ISOLIT2512",null,"ISOLIT 250 Basten Standard Kupfer eckig  250mm","103679","0",null,"STK",388,{"$f":"IF(Daten!$D$781=3,1,\"\")","v":""}]
["ISOLIT",13,25,"ISOLIT2513",null,"ISOLIT 250 Sairlift Inox eckig  250mm","103683","0",null,"STK",415,{"$f":"IF(Daten!$D$781=4,1,\"\")","v":""}]
["ISOLIT",14,25,"ISOLIT2514",null,"ISOLIT 250 Sairlift Kupfer eckig 250mm","103686","0",null,"STK",430,{"$f":"IF(Daten!$D$781=5,1,\"\")","v":""}]
["ISOLIT",0,30,{"$f":"A7369&C7369&B7369","v":"ISOLIT300"},"P","Schiedel ISOLIT 30/30","ISOLIT30","0",{"$f":"Daten!$B$741","v":8.75},"Anlage",0,null,{"$f":"I7369*1000","v":8750}]
[{"$f":"A7369","v":"ISOLIT"},{"$f":"B7369+1","v":1},{"$f":"C7369","v":30},"ISOLIT301",null,"ISOLIT 300 Einzügerelement 30","103628",250,null,"STK",61,{"$f":"ROUND(M7370,0)-M7371-M7372-M7372-M7373-M7373","v":30},{"$f":"((M7369)*4)/1000","v":35}]
["ISOLIT",2,30,"ISOLIT302",null,"ISOLIT 300 Anfängerelement 30","103640",250,null,"STK",170,{"$f":"IF(M7371=0,\"\",M7371)","v":1},{"$f":"IF(Daten!$D$741=2,1,0)","v":1}]
["ISOLIT",3,30,"ISOLIT303",null,"ISOLIT 300 Russtürelement gasdicht RE 30","103650",250,null,"STK",710,{"$f":"IF(M7372=0,\"\",M7372)","v":1},{"$f":"IF(Daten!$D$748=1,0,Daten!$E$748)","v":1}]
["ISOLIT",4,30,"ISOLIT304",null,"ISOLIT 300 Rauchrohranschlusselement RA 30/25/90°","103646",500,null,"STK",326,{"$f":"IF(M7373=0,\"\",M7373)","v":1},{"$f":"IF(Daten!$D$756=1,0,Daten!$E$756)","v":1}]
["ISOLIT",5,30,"ISOLIT305",null,"CHZ 300 Abdeckplatte Beton 780 x 780mm Loch ?350mm","103782","0",null,"STK",213,{"$f":"IF(Daten!$D$764=1,\"\",1)","v":1}]
["ISOLIT",6,30,"ISOLIT306",null,"ISOLIT 300 Kombi-Mündungs-Manchette Inox 30","103672","0",null,"STK",303,{"$f":"IF(N7380=0,1,\"\")","v":1}]
["ISOLIT",7,30,"ISOLIT307",null,"CHZ Abdeckplatte Beton 780 x 780mm ohne Loch","103788","0",null,"STK",198]
["ISOLIT",8,30,"ISOLIT308",null,"CHZ Postament 80 x 80mm  L250mm","103789","0",null,"STK",28]
["ISOLIT",9,30,"ISOLIT309",null,"ISOLIT 300 Schleifung einzügig  30","103659","0",null,"STK",654,{"$f":"IF(Daten!$D$772=1,\"\",Daten!$E$772)","v":""}]
["ISOLIT",10,30,"ISOLIT3010",null,"CHZ Kaminmörtel Sack 25kg ","103790","0",null,"STK",53,{"$f":"ROUNDUP(M7379,0)","v":5},{"$f":"I7369/2","v":4.375}]
["ISOLIT",11,30,"ISOLIT3011",null,"ISOLIT 300 Basten Standard Inox eckig  300mm","103676","0",null,"STK",492,{"$f":"IF(Daten!$D$781=2,1,\"\")","v":""},null,{"$f":"SUM(L7380:L7383)","v":0}]
["ISOLIT",12,30,"ISOLIT3012",null,"ISOLIT 300 Basten Standard Kupfer eckig  300mm","103680","0",null,"STK",512,{"$f":"IF(Daten!$D$781=3,1,\"\")","v":""}]
["ISOLIT",13,30,"ISOLIT3013",null,"ISOLIT 300 Sairlift Inox eckig  300mm","103684","0",null,"STK",546,{"$f":"IF(Daten!$D$781=4,1,\"\")","v":""}]
["ISOLIT",14,30,"ISOLIT3014",null,"ISOLIT 300 Sairlift Kupfer eckig 300mm","103685","0",null,"STK",565,{"$f":"IF(Daten!$D$781=5,1,\"\")","v":""}]

{"sheet":"Vokabel","index":30,"n_rows":495,"n_cols":5,"rows_kept":495,"cut":false,"hidden":true,"merged":[]}
[{"$f":"Daten!$B$161","v":1}]
[]
["Auswahl","Deutsch","Französisch","Italienisch"]
[{"$f":"IF($A$1=1,B4,IF($A$1=2,C4,IF($A$1=3,D4,E4)))","v":"Ja"},"Ja","Oui","Si"]
[{"$f":"IF($A$1=1,B5,IF($A$1=2,C5,IF($A$1=3,D5,E5)))","v":"Nein"},"Nein","Non","No"]
["Fertigfuss - Ø links","Fertigfuss - Ø links","Pied préfabriqué - Ø gauche","Basamento prefabbricato Ø sinistra"]
["Fertigfuss - Ø rechts","Fertigfuss - Ø rechts","Pied préfabriqué - Ø droit","Basamento prefabbricato Ø destra"]
["Fertigfuss","Fertigfuss","Pied préfabriqué ","Basamento prefabbricato"]
["Deckenanschlusskonus","Deckenanschlusskonus","Cône de raccordement","Coni d raccordo con fodera"]
["aus Faserbeton  8,5 cm Überstand","aus Faserbeton  8,5 cm Überstand","en béton de fibre, saillie 8,5 cm  ","di fibrocemento, sporgenza 8.5 cm"]
["aus Edelstahl 8,5 cm Überstand","aus Edelstahl 8,5 cm Überstand","en béton de fibre, saillie 19 cm","di fibrocemento, sporgenza 19 cm"]
["Steckadapter","Steckadapter","Adaptateur emboitable","Adattore a innesto"]
["Doppelfutter 100","Doppelfutter 100","Manchon double Ø100","Tubo fodera Ø100"]
["Doppelfutter 120","Doppelfutter 120","Manchon double Ø120","Tubo fodera Ø120"]
["Doppelfutter 130","Doppelfutter 130","Manchon double Ø130","Tubo fodera Ø130"]
["Doppelfutter 150","Doppelfutter 150","Manchon double Ø150","Tubo fodera Ø150"]
["Doppelfutter 180","Doppelfutter 180","Manchon double Ø180","Tubo fodera Ø180"]
["Doppelfutter 200","Doppelfutter 200","Manchon double Ø200","Tubo fodera Ø200"]
["Standard","Standard","Montage au chevrons","Standard"]
["Firstmittig","Firstmittig","Montage au millieu du faît","Montaggio a metà colmo"]
["Kunden-Adressdaten","Kunden-Adressdaten","Données d'adresse de client","Dati e indirizzi clienti "]
["PLZ","PLZ","NP","Codice postale "]
["Ort","Ort","Lieu","Luogo"]
["Ansprechpartner","Ansprechpartner","Responsble","Responsabile"]
["Tel.Nr.","Tel.Nr.","N°. Téléphone","Nr. Tel."]
["Fax.Nr.","Fax.Nr.","N°. Télécopie","Fax."]
["Objekt","Objekt","Objet","Ogetto"]
["Konditionen / Lohn","Konditionen / Lohn","Conditions/salaire","Condizioni"]
["   Rabatt 1","   Rabatt 1","   Rabais 1","   Ribasso 1"]
["Stunden","Stunden","Heures","Ore"]
["Kilometer","Kilometer","Kilomètres","Chilometri"]
["Pauschale","Pauschale","Forfait","Prezzo inclusivo"]
["   Rabatt 2","   Rabatt 2","   Rabais 2","   Ribasso 2"]
[{"$f":"IF($A$1=1,B34,IF($A$1=2,C34,IF($A$1=3,D34,E34)))","v":"Rabatt 3"},"Rabatt 3","Rabais 3","Ribasso 3"]
["   CHF per Std.","   CHF per Std.","  Frs à l'heure","   CHF per ora"]
["   CHF per km","   CHF per km","  Frs par km","   CHF per chilom."]
["   CHF per P.","   CHF per P.","  Frs par P.","   CHF per P. "]
["   MwSt","   MwSt","  TVA","   IVA"]
["Lichter Ø cm","Lichter Ø cm","Dimension intérieur Ø cm","Dimensione interiore "]
["Anlagenhöhe in m","Anlagenhöhe in m","Hauteur de l'installation en m","Altezza installazione in metri "]
["Fussausführung","Fussausführung","Détail pied de cheminée","Basamento dettagliato"]
["Rauchrohranschluss","Rauchrohranschluss","Raccordement tube de fumée","Raccordo"]
["Handy-Abdeckplatte","Handy-Abdeckplatte","Plaque de recouvrement Handy","Posa copertura lastra "]
["Zubehör","Zubehör","Accessoire","Accessori"]
["Anschlussvariante","Anschlussvariante","Variante de raccordement","Variante di raccordo"]
["Zugregler ","Zugregler ","Régulateur de tirage","Regulatore di tiraggio"]
["zusätzlicher Rauchrohranschluss ","zusätzlicher Rauchrohranschluss ","Raccordement tube de fumée sup.","Raccordo canna fumaria supplementare"]
["LAS Zuluft-Adapter ","LAS Zuluft-Adapter ","Adaptateur LAS","Adattore LAS"]
["Revisionstür ","Revisionstür ","Porte de révision","Porta di revisione"]
["obere Putztür ","obere Putztür ","Porte de nettoyage supérieur","Portina d'ispezione superiore"]
["Absolut Thermo-Trennstein","Absolut Thermo-Trennstein","Élément de seperation thermo Absolut","Nuovo! Absolut elemento thermico"]
["Bewehrungs-Set","Bewehrungs-Set","Set d'armature","Completo armature"]
["Kaminhalter","Kaminhalter","Support de cheminée","Dispositivo di fissaggio"]
["Kaminaufsätze","Kaminaufsätze","Cape de cheminée","Cappa del caminetto"]
["(mit Expl. Kl.)    ","(mit Expl. Kl.)    ","(avec clapet d'explosion)","Con portina antiesplosione"]
["(bei kombiniert kleiner Ø)","(bei kombiniert kleiner Ø)","(pour combine petit Ø)","Per piccole combine"]
["(für Festbrennstoffzug)","(für Festbrennstoffzug)","(pour canal combustible solide)","Per canali con combustibile solido"]
["(für Thermo-Luftzug)","(für Thermo-Luftzug)","(pour gaine de ventilation Thermo)","Per condotto di tiraggio thermo"]
["(bei zweizügigen, für beide Züge)","(bei zweizügigen, für beide Züge)","(lors double tirage pour les deux conduits)","Doppio tiraggio per due condotti"]
["   2.kl.Zug                                           1.Zug","   2.kl.Zug                                           1.Zug","  2.p.canal                                    1.canal","2. condotto piccolo                  1. condotto"]
["(bei kombiniert grosser Ø)","(bei kombiniert grosser Ø)","(pour combine grand Ø)","Per combine con grande diametro"]
["Sockel","Sockel","Socle","Piede"]
[" (ab Ø 16)"," (ab Ø 16)"," (des ø 16)"," (Da Ø 16)"]
["Fundamentsockel","Fundamentsockel","Socle fondation","Basamento piede"]
["(zweizügig - für beide Züge) ","(zweizügig - für beide Züge) ","(double tirage pour les deux conduits)","Doppio tiraggio per i due condotti"]
["Putzanschluss","Putzanschluss","Raccordement de nettoyage","Raccordo portina pulizia"]
["für Lüftungszug","für Lüftungszug","pour gaine de ventilation","Per condotti di ventilazioni"]
["Abdeckplatte (KWD)","Abdeckplatte (KWD)","Plaque de recouvrement (KWD)","Posa copertura lastra "]
["Schnellbaufundament","Schnellbaufundament","Fondation à montage rapide","Fondazione a montaggio rapido"]
[{"$f":"IF($A$1=1,B70,IF($A$1=2,C70,IF($A$1=3,D70,E70)))","v":"Deckenanschlusskonus"},"Deckenanschlusskonus","Cône de raccordement","Cono di raccordo"]
["Basten Edelstahl","Basten Edelstahl","Basten acier inoxydable","Basten acciaio inossidabile"]
["Basten Kupfer","Basten Kupfer","Basten cuivre","Basten rame"]
["Sairlift Edelstahl","Sairlift Edelstahl","Sairlift acier inoxydable","Sairlift acciaio inossidabile"]
["Sairlift Kupfer","Sairlift Kupfer","Sairlift cuivre","Sairlift rame "]
["Brennstoff","Brennstoff","Combustible","Combustibile"]
["Wand- o. Bodenmontage","Wand- o. Bodenmontage","Montage mur ou sol","Montaggio per muro o terra "]
["Putztüranschluss","Putztüranschluss","Raccordement porte de ramonage","Portina d'ispezione "]
["Rauchrohranschluss RA","Rauchrohranschluss RA","Raccordement tube de fumée RA","Raccordo tubo fumario RA"]
["RA-Höhe in m","RA-Höhe in m","Hauteur RA en m","Altezza installazione in metri "]
["RA-Verlängerung (KRS)","RA-Verlängerung (KRS)","Prolongation RA (KRS)","Prolunga RA"]
["Sparrenhalterung","Sparrenhalterung","Fixation au chevrons","Fissaggio tetti e solette"]
["Dachdurchführung","Dachdurchführung","Passage de toiture","Passaggio tetto"]
["Regenhaube","Regenhaube","Cape parpluie","Cappa del caminetto isolazione pioggia"]
["Mündungslösung","Mündungslösung","Solution de finition de souche","Soluzione terminale"]
["Wandabstand (>=50 mm)","Wandabstand (>=50 mm)","Distance au mur (>=60mm)","Distanza parete"]
["Wandhalterung statisch","Wandhalterung statisch","Fixation mural statique","Fissaggio murale statico "]
["(inkl. 2 St. statischer Manschetten)","(inkl. 2 St. statischer Manschetten)","(y compris 2 brides statique)","Incluso 2 bride statiche"]
["Verbindungsleitung","Verbindungsleitung","Tube de raccordement","Tubo di raccordo "]
["Anpassung der Anlagenhöhe","Anpassung der Anlagenhöhe","Adaptation de la hauteur d'installation","Adattamento per altezza installazione"]
["tatsächliche Anlagenhöhe ","tatsächliche Anlagenhöhe ","Hauteur d'installation effective","Effettiva altezza installazione"]
["Differenz +/-","Differenz +/-","Différence +/-","Differenza +/-"]
["Anpassung durch Eingabe ","Anpassung durch Eingabe ","Adaptation par une entrée","Adattazione per un entrata "]
["kürzerer Rohrelemente:","kürzerer Rohrelemente:","des éléments plus courts  ","Elemti tubi accorciati"]
["Rohr 330 mm","Rohr 330 mm","Tube 165mm","Tubo 330 mm"]
["Rohr 165 mm","Rohr 165 mm","Tube 330mm","Tubo 165 mm"]
["Betriebsweise","Betriebsweise","Mode de function","Modo di funzione"]
["Differenz +/- ","Differenz +/- ","Différence +/-","Diferenza +/-"]
["(14 cm für Mündung vorsehen!)","(14 cm für Mündung vorsehen!)","(prévoir 14 cm pour l'embouchure!)","Prevenzione 14 cm per la foce"]
["Doppelwandfutter in mm","Doppelwandfutter in mm","Manchon double en mm","Manicotto doppio in mm "]
["Putztür","Putztür","porte de ramonage","Porta di pulizia"]
["Anpassung durch Eingabe kürzerer Rohrelemente:","Anpassung durch Eingabe kürzerer Rohrelemente:","Adaptation par l'entrée d'éléments plus courts:","Adattamento entrata elementi piu corti"]
["Regenhaube","Regenhaube","Cape parpluie","Cappa isolamento pioggia "]
["Abschlussplatte für Kaminaufsatz","Abschlussplatte für Kaminaufsatz","Plaque de finition pour cape de cheminée","Lastra finale per copertura camino"]
["Rohr 660 mm","Rohr 660 mm","Tube 660mm","Tubo 660 mm"]
["Bodenmontage","Bodenmontage","Montage au sol","Montaggio terra"]
["Wandmontage","Wandmontage","Montage mural","Montaggio pareti "]
["Fussteil höhenverstellbar","Fussteil höhenverstellbar","Pied réglable","Piede regolabile"]
["max. Abstand  220 mm","max. Abstand  220 mm","Distance max. 220mm","max. distanza 220 mm"]
["max. Abstand  140 mm","max. Abstand  140 mm","Distance max. 140mm","max. distanza 140 mm"]
[{"$f":"IF($A$1=1,B110,IF($A$1=2,C110,IF($A$1=3,D110,E110)))","v":"max. Abstand  160 mm"},"max. Abstand  160 mm","Distance max. 160mm","max. distanza 160 mm","x"]
["max. Abstand  120 mm","max. Abstand  120 mm","Distance max. 120mm","max. distanza 120 mm"]
["max. Abstand  100 mm","max. Abstand  100 mm","Distance max. 100mm","max. distanza 100 mm"]
["max. Abstand  215 mm","max. Abstand  215 mm","Distance max. 215mm","max. distanza 215 mm"]
["max. Abstand  195 mm","max. Abstand  195 mm","Distance max. 195mm","max. distanza 195 mm"]
["max. Abstand  175 mm","max. Abstand  175 mm","Distance max. 175mm","max. distanza 175mm"]
["max. Abstand  155 mm","max. Abstand  155 mm","Distance max. 155mm","max. distanza 155 mm"]
["max. Abstand  85 mm","max. Abstand  85 mm","Distance max. 85mm","max. distanza 85 mm"]
[{"$f":"IF($A$1=1,B118,IF($A$1=2,C118,IF($A$1=3,D118,E118)))","v":"max. Abstand  310 mm"},"max. Abstand  310 mm","Distance max. 310mm","max. distanza 310 mm","x"]
["max. Abstand  370 mm","max. Abstand  370 mm","Distance max. 370mm","max. distanza 370 mm","x"]
["max. Abstand  410 mm","max. Abstand  410 mm","Distance max. 410mm","max. distanza 410 mm","x"]
[{"$f":"IF($A$1=1,B121,IF($A$1=2,C121,IF($A$1=3,D121,E121)))","v":"max. Abstand  470 mm"},"max. Abstand  470 mm","Distance max. 470mm","max. distanza 470 mm","x"]
[{"$f":"IF($A$1=1,B122,IF($A$1=2,C122,IF($A$1=3,D122,E122)))","v":"max. Abstand  610 mm"},"max. Abstand  610 mm","Distance max. 610mm","max. distanza 610 mm","x"]
[{"$f":"IF($A$1=1,B123,IF($A$1=2,C123,IF($A$1=3,D123,E123)))","v":"max. Abstand  670 mm"},"max. Abstand  670 mm","Distance max. 670mm","max. distanza 670 mm","x"]
["max. Abstand  305 mm","max. Abstand  305 mm","Distance max. 305mm","max. distanza 305 mm"]
["max. Abstand  285 mm","max. Abstand  285 mm","Distance max. 285mm","max. distanza 285 mm"]
["max. Abstand  265 mm","max. Abstand  265 mm","Distance max. 265mm","max. distanza 265 mm"]
["max. Abstand  195 mm","max. Abstand  195 mm","Distance max. 195mm","max. distanza 195 mm"]
["max. Abstand  425 mm","max. Abstand  425 mm","Distance max. 425mm","max. distanza 425 mm"]
["max. Abstand  405 mm","max. Abstand  405 mm","Distance max. 405mm","max. distanza 405 mm"]
["max. Abstand  385 mm","max. Abstand  385 mm","Distance max. 385mm","max. distanza 385 mm"]
["max. Abstand  365 mm","max. Abstand  365 mm","Distance max. 365mm","max. distanza 365 mm"]
["max. Abstand  295 mm","max. Abstand  295 mm","Distance max. 295mm","max. distanza 295 mm"]
["max. Abstand  525 mm","max. Abstand  525 mm","Distance max. 525mm","max. distanza 525 mm"]
["max. Abstand  505 mm","max. Abstand  505 mm","Distance max. 505mm","max. distanza 505 mm"]
["max. Abstand  485 mm","max. Abstand  485 mm","Distance max. 485mm","max. distanza 485 mm"]
["max. Abstand  465 mm","max. Abstand  465 mm","Distance max. 465mm","max. distanza 465 mm"]
["max. Abstand  395 mm","max. Abstand  395 mm","Distance max. 395mm","max. distanza 395 mm"]
["max. Abstand  635 mm","max. Abstand  635 mm","Distance max. 635mm","max. distanza 635 mm"]
["max. Abstand  635 mm","max. Abstand  635 mm","Distance max. 635mm","max. distanza 635 mm"]
[{"$f":"IF($A$1=1,B140,IF($A$1=2,C140,IF($A$1=3,D140,E140)))","v":"max. Abstand  615 mm"},"max. Abstand  615 mm","Distance max. 615mm","max. distanza 615 mm"]
["max. Abstand  595 mm","max. Abstand  595 mm","Distance max. 595mm","max. distanza 595 mm"]
["max. Abstand  525 mm","max. Abstand  525 mm","Distance max. 525mm","max. distanza 525 mm"]
["nicht bekannt","nicht bekannt","non connu","Sconosciuto"]
["Gas","Gas","gaz","Gas"]
["Öl","Öl","mazout","Olio"]
["Festbrennstoff","Festbrennstoff","combustible solide","Combustibile solido "]
["Holz-Pellets","Holz-Pellets","Pastilles de bois","Pastiglie in legno (Pellets)"]
["Bodenmontage","Bodenmontage","Montage au sol","Montaggio terra"]
["Wandmontage","Wandmontage","Montage mural","Montaggio pareti "]
["Fussteil höhenverstellbar","Fussteil höhenverstellbar","Pied réglable","Piede regolabile"]
["noch nicht bekannt","noch nicht bekannt","pas encore connu","Sconosciuto"]
["Abströmkonus","Abströmkonus","Cône d'échappement","Terminale conico"]
["Mündundsabschluss","Mündundsabschluss","Cape de finition","Raccordo finale"]
["Basten Standard","Basten Standard","Basten Standard","Basten standard"]
["Basten Regulator","Basten Regulator","Basten Regulator","Basten regolatore"]
["Unterdruck","Unterdruck","Suspression","Sottopressione"]
["Überdruck",{"$f":"IF(R170>355,\"\",\"Überdruck\")","v":"Überdruck"},"Surpression","Soprapressione"]
["Doppelwandfutter Ø 120","Doppelwandfutter Ø 120","Manchon double Ø 120","Manicotto doppio  Ø120 "]
["Doppelwandfutter Ø 130","Doppelwandfutter Ø 130","Manchon double Ø 130","Manicotto doppio  Ø130"]
["Doppelwandfutter Ø 150","Doppelwandfutter Ø 150","Manchon double Ø 150","Manicotto doppio  Ø150 "]
["Doppelwandfutter Ø 180","Doppelwandfutter Ø 180","Manchon double Ø 180","Manicotto doppio  Ø180"]
["Doppelwandfutter Ø 200","Doppelwandfutter Ø 200","Manchon double Ø 200","Manicotto doppio  Ø200"]
["Doppelwandfutter Ø 250","Doppelwandfutter Ø 250","Manchon double Ø 250","Manicotto doppio Ø250"]
["Dreischaliges Edelstahl-Kaminsystem mit","Dreischaliges Edelstahl-Kaminsystem mit","Système de cheminée à triple parois, en acier inoxydabel","Sistema canna fumaria a tre pareti in acciaio inossidabile"]
["Einwandiges Kamin-Sanierungssystem","Einwandiges Kamin-Sanierungssystem","Système d'assainissement de cheminée, monoparois  ","Risanamento canna fumaria semplice"]
["Mehrschaliges feuchteunempfindliches Kaminsystem","Mehrschaliges feuchteunempfindliches Kaminsystem","Système de cheminée à multi parois, résistant à l'humidité","Sistema canna fumaria a tripla pareti resistente all umidità"]
["Dreischaliges Kaminsystem","Dreischaliges Kaminsystem","Système de cheminée à triple parois","Sistema di canna fumaria a tre pareti "]
["Doppelwandiges Edelstahl-Kaminsystem","Doppelwandiges Edelstahl-Kaminsystem","Système de cheminée à double parois, en acier inoxydable","Sistema di canna fumaria a doppia pareti in acciaio inossidabile "]
["Doppelwandiges Kupfer-Kaminsystem","Doppelwandiges Kupfer-Kaminsystem","Système de cheminée à double parois, en cuivre","Sistema di canna fumaria a doppia parete in rame"]
["Einwandiges Edelstahl-Sanierungssystem","Einwandiges Edelstahl-Sanierungssystem","Système de tubage monoparois, en acier inoxydable  ","Sistema di canna fumaria semplice in acciaio inossidabile "]
["PP-Kunststoff-Abgasleitungssystem","PP-Kunststoff-Abgasleitungssystem","Système d'évacuation monoparois, en mat. synthètique PP","Sistema d'evaquazione PP materiale sintetico"]
["keramischem Profil-Innenrohr in Elementbauweise","keramischem Profil-Innenrohr in Elementbauweise","Tube profilé en céramique, construction par éléments","Tubo in ceramica, profilato con construzione elementi"]
["aus Profilkeramik mit keramischer Steckverbindung","aus Profilkeramik mit keramischer Steckverbindung","en céramique profilée avec emboitement en céramique","Tubo in ceramica, profilato con attacco"]
["mit integrierter Wärmedämmung","mit integrierter Wärmedämmung","avec une isolation thermique intégrée","Con isolazione termica intergrata"]
["mit Hinterlüftung und Schamotte-Innenrohr","mit Hinterlüftung und Schamotte-Innenrohr","avec aération et tube intérieur en argile réfractaire","Con ventilazione del tubo interiore in argilla"]
["in Elementbauweise mit Steckmuffenverbindung","in Elementbauweise mit Steckmuffenverbindung","en construction par éléments avec emboitement ","In elementi di costruzione con presa di connessione"]
["in Elementbauweise mit Drehkupplungen","in Elementbauweise mit Drehkupplungen","en construction par éléments avec couplage rotatifs","In elementi di costruzione con rotazione della frizione"]
["und keramischer Steckverbindung","und keramischer Steckverbindung","et emboitement céramique","Con presa di connessione in ceramica"]
["und keramischem Profil-Innenrohr","und keramischem Profil-Innenrohr","et tube profilé céramique","Tubo con profilo interiore in ceramica"]
["Ansprechpartner:","Ansprechpartner:","Responsable","Responsabile"]
["Nr.","Nr.","N°. ","Nr. "]
["Kalkulation","Kalkulation","Calcul","Calcolazione"]
["Angebot","Angebot","Offre","Offerta"]
["Auftragsbestätigung","Auftragsbestätigung","Confirmation de commande","Conferma di comanda"]
["Datum :","Datum :","Date","Data "]
["Sachbearbeiter:","Sachbearbeiter:","Spécialiste","Responsabile"]
["Tel.Nr.:","Tel.Nr.:","N°. Téléphone","Nr.Tel.  "]
["Fax.Nr.:","Fax.Nr.:","N°. Télécopie","Fax. Nr. "]
["Obj :","Obj :","Objet","Oggetto"]
["Anlagenhöhe:","Anlagenhöhe:","Hauteur d'installation:","Altezza installazione "]
["Gesamtgewicht:","Gesamtgewicht:","Poids total:","Peso totale "]
["Artikel-Nr.","Artikel-Nr.","N° d'article","Nr. articolo"]
["PL NR","PL NR","N° CP","Nr codice postale "]
["Bezeichung","Bezeichung","Désignation","Designazione"]
["Gewicht                                           kg","Gewicht                                           kg","Poids                              kg","Peso                            kg"]
["Bauhöhe  mm","Bauhöhe  mm","Constr. mm","Altezza mm "]
["Menge","Menge","Quantité","Quantità"]
["Einheit","Einheit","Unité","Unità"]
["Einzelpreis CHF","Einzelpreis CHF","Prix de l'unité CHF","Prezzo unico"]
["Gesamtpreis CHF","Gesamtpreis CHF","Prix total CHF","Prezzo totale in CHF"]
["Nettobetrag","Nettobetrag","Montant net","Prezzo netto "]
["Summe Bauteile","Summe Bauteile","Total des éléments","Somma totale degli elementi"]
["% Rabatt 1 von ","% Rabatt 1 von ","% rabais 1 de","% ribasso 1 da"]
[{"$f":"IF($A$1=1,B204,IF($A$1=2,C204,IF($A$1=3,D204,E204)))","v":"Fracht (per to)"},"Fracht (per to)","Transp.(par t)","Merce (per ton.)"]
["Fracht (ab Werk)","Fracht (ab Werk)","Transp.(depart usine)","Merce (dalla fabbrica)"]
["Nettobetrag CHF","Nettobetrag CHF","Montant net CHF","Prezzo netto in CHF"]
[" % MwSt."," % MwSt."," % TVA","% iva"]
["Gesamtbetrag  CHF","Gesamtbetrag  CHF","Montant total CHF","Netto totale in CHF"]
["per Tonne","per Tonne","par tonne","Per tonne."]
["Fracht","Fracht","Transp./Fret","Merci"]
["lief.PLZ","lief.PLZ","CP livraison","Consegna","Consegna nummero di codice"]
["man. Fracht","man. Fracht","Transp.manuel","Trasporto manuale"]
["Ku.Nr.","Ku.Nr.","N° client","Nr. cliente "]
["Anschrift 1","Anschrift 1","Adresse 1","Indirizzo 1 "]
["Anschrift 2","Anschrift 2","Adresse 2","Indirizzo 2 "]
["Strasse","Strasse","Rue","Strada"]
["PLZ","PLZ","NP","Codice postale "]
["Ort","Ort","Lieu","Luogo"]
["Ansprechpartner","Ansprechpartner","Responsble","Responsabile"]
["Tel.Nr.","Tel.Nr.","N°. Téléphone","Nr. Tel."]
["Fax.Nr.","Fax.Nr.","N°. Télécopie","Fax. Nr. "]
["Handy","Handy","N°. Mobil","Cellulare"]
["E-Mail","E-Mail","Courriel","Email"]
["Info","Info","Information","Informazione "]
["Variabler Text für Montagearbeiten","Variabler Text für Montagearbeiten","Texte variable pour les travaux de montage","Tassa variabile per lavoro di montaggio"]
["1.Zeile","1.Zeile","1.Ligne","1. riga"]
["2.Zeile","2.Zeile","2.Ligne","2. riga"]
["3.Zeile","3.Zeile","3.Ligne","3. riga"]
["4.Zeile","4.Zeile","4.Ligne","4. riga"]
["5.Zeile","5.Zeile","5.Ligne","5.riga"]
["1.u.2.Zeile","1.u.2.Zeile","1.et.2.Ligne","1. e 2. riga"]
["Variabler Kopftext für Angebot","Variabler Kopftext für Angebot","Texte variable pour l'entête de l'offre","Titolo variabile per l`entità dell`offerta "]
["Sehr geehrter ","Sehr geehrter ","Madame,Monsieur","Signora, Signore"]
["wir bedanken uns für Ihre Anfrage und bieten Ihnen folgendes an:","wir bedanken uns für Ihre Anfrage und bieten Ihnen folgendes an:","nous vous remercions de votre demande et vous offrons ce qui suit :","Vi ringraziamo per la vostra ordinazione vi offriamo quanto segue:"]
["Wir bedanken uns für Ihre Anfrage und bieten Ihnen folgendes an:","Wir bedanken uns für Ihre Anfrage und bieten Ihnen folgendes an:","nous vous remercions de votre demande et vous offrons ce qui suit :","Vi ringraziamo per la vostra ordinazione e vi offriamo quanto segue:"]
["Wenn es keine Ansprechperson gibt wird der Kopftext (1.u.2.Zeile) genommen","Wenn es keine Ansprechperson gibt wird der Kopftext (1.u.2.Zeile) genommen","S'il n'y a pas de personne de contact. l'en-tête est composer de la1.et la.2.ligne  ","Se nessuna persona di contatto. l'intestazione è composta da la1.e2.riga"]
["Variabler Schlusstext für Angebot","Variabler Schlusstext für Angebot","Texte variable pour la fin de l'offre","Testo variabile per l`offerta finale "]
["Wir hoffen, dass Ihnen unser Angebot zusagt und freuen uns auf Ihren Auftrag.","Wir hoffen, dass Ihnen unser Angebot zusagt und freuen uns auf Ihren Auftrag.","En espérant que notre offre est à votre convenance et nous réjouissons de votre ordre. ","Sperando che la nostra offerta sia di vostro gradimento, aspettiamo una vostra ordinazione"]
["Freundliche Grüsse","Freundliche Grüsse","Veuillez agréer nos salutations distinguées ","Cordiali saluti "]
["In den Zeilen 5-10 tragen Sie bitte Ihre Firma, und den Zeilen 14-15 den Sachbearbeiter u. Tel.Nr., ein.","In den Zeilen 5-10 tragen Sie bitte Ihre Firma, und den Zeilen 14-15 den Sachbearbeiter u. Tel.Nr., ein.","Veuillez enregistrer dans les lignes 5-10 votre entreprise et aux lignes 14-15 la personne de contacte et le n° tél.","Per la riga 5-10 inserire la firma e per la riga 14-15 il Nr. tel. del responsabile "]
["INFO:","INFO:","INFORMATION:","Informazione "]
["Firmendaten:","Firmendaten:","Données de la société :","Dati della Società"]
["Schiedel Kaminsysteme AG","Schiedel Kaminsysteme AG","Schiedel Conduits de fumée SA","Schiedel sistema canne fumarie SA"]
["5312 Döttingen, Badstrasse 38","5312 Döttingen, Badstrasse 38","1030 Bussigny, Rue de l'Arc-en-Ciel 12","5312 Döttingen, Bastrasse 38"]
["Tel. 056 268 00 00  Fax. 056 268 00 01","Tel. 056 268 00 00  Fax. 056 268 00 01","Tel. 021 803 60 01  Fax. 021 803 60 05","Tel. 056 268 00 00 Fax. 056 268 00 01"]
["e-Mail: info@schiedel.ch   www.schiedel.ch","e-Mail: info@schiedel.ch   www.schiedel.ch","e-Mail: info@schiedel.ch   www.schiedel.ch","e-mail: info@schiedel.ch   www.schiedel.ch"]
["Sachbearbeiter:","Sachbearbeiter:","Spécialiste","Responsabile"]
["Pers.-Nr.","Pers.-Nr.","N°. pers.","Nr. personale"]
["Frachteinstellungen:","Frachteinstellungen:","Forfait transport","Merci inpostazioni"]
["Vorname/Name","Vorname/Name","Prénom/Nom","Nome/cognome"]
["Telefon","Telefon","Téléphone","Telefono"]
["Fax","Fax","Fax","Fax. "]
["Heinz Allemann","Heinz Allemann","Frédéric Widmer","Massimo Insalata"]
["079 605 42 77","079 605 42 77","076 578 60 01","079 236 88 22"]
["032 323 67 25","032 323 67 25","021 803 60 05","081 630 24 34"]
["CHF per Tonne","CHF per Tonne","CHF par tonne","CHF per tonnellate "]
["Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten.","Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten.","L'offre est valable d'ici le 31.12.2023. Modifications réserver.","L`offerta e valida dal 31.12.2023 modificazioni possibili"]
["Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten.","Das Angebot ist gültig bis 31.12.2023. Änderungen vorbehalten.","L'offre est valable d'ici le 31.12.2023. Modifications réserver.","L`offerta e valida dal 31.12.2023 modificazioni possibili"]
["RA-Verlängerung","RA-Verlängerung","Prolongation RA","Allungo raccordo tubo fumario "]
["Verstärkt","Verstärkt","renforcé","Rinforzato "]
["Doppelfutter 250","Doppelfutter 250","Manchon double Ø 250","Manicotto doppio Ø250"]
["Kunde speichern","Kunde speichern","Enregister client","Registro cliente"]
["Der Name für jeses Kaminsystem !","Der Name für jeses Kaminsystem !","Le nom pour le conduits de fumée !","Il nome per ogni canna fumaria "]
["Beenden","Beenden","Terminer","Terminare"]
["Verbindungsleitung","Verbindungsleitung","Tube de raccordement","Tubo di raccordo "]
["weiter","weiter","de plus","Procedi"]
["Achtung:","Achtung:","attention","Attenzione:"]
[{"$f":"IF($A$1=1,B268,IF($A$1=2,C268,IF($A$1=3,D268,E268)))","v":"Für die Verbindungsleitung werden"},"Für die Verbindungsleitung werden","Pour la conduite de raccord devenir","Per la condotta sono utilizabili"]
["höchstens 14 Artikel übernommen !","höchstens 14 Artikel übernommen !","les tout au plus 14 articles chargé","sono utilizzabili non più di 14 articoli "]
["Artikelnummer","Artikelnummer","N° d'article","Nr. di articolo"]
["Artikelbezeichnung","Artikelbezeichnung","désignation d'article","Designazione dell articolo"]
["Baulänge","Baulänge","longueur hors tout","Lunghezza costruzione"]
["Menge","Menge","Quantité","Quantità"]
["Kaminsysteme Neubau","Kaminsysteme Neubau","Systemes de conduits  - de fumée, pour nouvelles constructions","Sistema canne fumarie per nuove costruzioni"]
["zurück zur Eingabe","zurück zur Eingabe","retour à l'entrée","Ritornare al punto di entrata "]
["Kalkulation Anlage","Kalkulation Anlage","Calcul de installation","Calcolo di installazione"]
["Einzelteileingabe","Einzelteileingabe","Entrée d'élément","Inserire pezzo dettaigliato"]
["Hinweise","Hinweise","Indications","Indicazioni"]
["Händler","Händler","Commerçant","Commerciante"]
["Texte","Texte","Textes","Testi"]
["Programm beenden","Programm beenden","programme terminer","Terminare programme "]
["Verrechnungspartner","Verrechnungspartner","partenaire de facturation","Trasferimento partner"]
["Kundenstamm","Kundenstamm","base de clients","Base die clienti "]
["2 x 3 m = bis 1,50 m über Dach*","2 x 3 m = bis 1,50 m über Dach*","2 x 3 m = bis 1,50 m hors toiture*","2 x 3 m = 1,50 m al di sopra tetto*"]
["4 x 4 m = bis 2,00 m über Dach*","4 x 4 m = bis 2,00 m über Dach*","4 x 4 m = bis 2,00 m hors toiture*","4 x 4 m = bis 2,00 m al di sopra tetto"]
["4 x 6 m = bis 3,00 m über Dach*","4 x 6 m = bis 3,00 m über Dach*","4 x 6 m = bis 3,00 m hors toiture*","4 x 6 m = bis 3,00 m al di sopra tetto "]
["*ab Kaminhalterung","*ab Kaminhalterung","*entre et sur chevrons","* entrata dispositivo di fissaggio "]
["Bauhöhe 33 cm","Bauhöhe 33 cm","hauteur 33cm","Altezza 33 cm"]
["INFO:","INFO:","INFORMATION:","Informazione "]
["Rauchrohranschlusshöhe auf Achse","Rauchrohranschlusshöhe auf Achse","Raccordement de fumée sur axe","Altezza di raccordo per asse "]
["gerechnet  ab UK Sockel (bei Bodenmontage)","gerechnet  ab UK Sockel (bei Bodenmontage)","calcul à partir bases (pour sol assembalage)","Calcolo base a partire da sotto piede (montaggio terra)"]
["                  ab OK Wandkonsole (bei Wandmontage)","                  ab OK Wandkonsole (bei Wandmontage)","                  à partir des Console murale (montage de murale)","Calcolo base a partire da sopra consola murale per (montaggio murale)"]
["Ein Rauchrohranschluss ist in der Anlage enthalten !","Ein Rauchrohranschluss ist in der Anlage enthalten !","1 Raccordement on contient !","E incluso nel raccordo "]
["INFO:","INFO:","INFORMATION:","Informazione "]
["Dachdurchführung inkl. Regenkragen","Dachdurchführung inkl. Regenkragen","Garniture de cheminé avec collerette","Guarnizione per canna fumaria con sistema antipioggia "]
["INFO:","INFO:","INFORMATION:","INFORMAZIONE: "]
["Erfoderlich bei Höhen über oberster","Erfoderlich bei Höhen über oberster","Né essairement avec des hauteurs sur","Neccessario per altezze al di sopra "]
["Wandhalterung ab 1,5 m freistehend !","Wandhalterung ab 1,5 m freistehend !","l'appui de paroi supérieur à patir de 1,5 mètre isolément","Montaggio a  parete da 1,5 m libero"]
["- Unterdruck im Schornstein: ","- Unterdruck im Schornstein: ","- Dépression dans la cheminée: ","Sottopressione nella canna fumaria "]
["  Ausführung mit Rapid fugendicht.","  Ausführung mit Rapid fugendicht.","  mise en Masse de jointoiement rapide.","Esecuzione con tenuta Rapid "]
["- Überdruck im Schornstein: ","- Überdruck im Schornstein: ","- Surpression dans la cheminée: ","Soprapressione nella canna fumaria "]
["  Ausführung mit Rotempo Fugenmasse,","  Ausführung mit Rotempo Fugenmasse,","  mise en Masse de joitoiement Rotempo,","Esecuzione con tenuta Rotempo "]
["  Abgastemperatur bis 200° C.","  Abgastemperatur bis 200° C.","  à 200° température des gaz d'échappement.","Temperatura di scarico fino a 200° C."]
["Schliessen","Schliessen","fermer","Chiudere"]
["Facharbeiterstunden","Facharbeiterstunden","Monteu spécialisé (Heures)","Montaggio speciale ad ore "]
["Kilometer","Kilometer","Kilomètres","Chilometri"]
["Pauschale Montagearbeit","Pauschale Montagearbeit","Forfait travaux de montage","Prezzo inclusivo per montaggio "]
["STD","STD","H","Ore"]
["Pausch","Pausch","Forfait","Prezzo incluso"]
["Summe Montage","Summe Montage","Summe Montage","Somma montaggio"]
["Lichter Ø mm","Lichter Ø mm","Dimension intérieur Ø mm","Dimensione interiore Ømm"]
["Lieferantenübersicht","Lieferantenübersicht","Fournisseurs","Fornitori"]
["Adresse 1","Adresse 1","Adresse 1","Indirizzo 1 "]
["Adresse 2","Adresse 2","Adresse 2","Indirizzo 2 "]
["Um eine Bestellung an den Lieferanten mailen zu können, muss im Feld \"E-Mail\" die Adresse hinterlegt sein!","Um eine Bestellung an den Lieferanten mailen zu können, muss im Feld \"E-Mail\" die Adresse hinterlegt sein!","Pour passer une commande par \"E-Mail\" veuillez introduire l'adresse dans le champs prevu!","per voler inviare un E-Mail al fornitore utilizzare l`apposito campo con l`indirizzo  "]
["Montage:","Montage:","Montage:","Montaggio:"]
["Thermo-Fussplatte + 1 Trennstein","Thermo-Fussplatte + 1 Trennstein","Plaque de base thermo Absolut e 1 élément de seperation","Thermo pedana + 1 Elemento separazione","Löschen"]
["Thermo-Fussplatte + 2 Trennsteine","Thermo-Fussplatte + 2 Trennsteine","Plaque de base thermo Absolut e 2 élément de seperation","Thermo pedana + 2 Elemento separazione","Löschen"]
["1 Thermo-Trennstein ohne Fussplatte","1 Thermo-Trennstein ohne Fussplatte","1 Élément de seperation thermo sans plaque de base","1 Elemento di separazione thermo senza pedana di base ","Löschen"]
["2 Thermo-Trennsteine ohne Fussplatte","2 Thermo-Trennsteine ohne Fussplatte","2 Élément de seperation thermo sans plaque de base","2 Elementi di separazione thermo senza pedana di base ","Löschen"]
["% Rabatt 2 von ","% Rabatt 2 von ","% rabais 2 de","% Ribasso 2 di"]
["Edelstahlsysteme - doppelwandig","Edelstahlsysteme - doppelwandig","Système de conduits - de fumée, double parois","Sistema in accaio inossidabile doppia parete "]
["Edelstahlsysteme - einwandig","Edelstahlsysteme - einwandig","Système de conduits - de fumée et tubage, simple parois","Sistema in accaio inossidabile parete semplice"]
["Sanierungssystem - Keramisch","Sanierungssystem - Keramisch","Système de tubage - et d'assainissement en céramique","Sistema sanatura in ceramica"]
["PP-Kunststoffsystem","PP-Kunststoffsystem","Système d'évacuation en plastique PP","Sistema d`evaquazione in PP"]
["Kalkulation Anlage","Kalkulation Anlage","Calcul de installation","Calcolo di installazione"]
["Einzelteileingabe","Einzelteileingabe","Entrée d'élément","Inserire pezzo dettaigliato"]
["zurück zur Eingabe","zurück zur Eingabe","Retour à l'entrée","Ritornare al punto di entrata "]
["Rabatt 1  = Systemrabatt","Rabatt 1  = Systemrabatt","Rabais 1  = Système","Ribasso 1 = Sistema ribasso "]
["Rabatt 2  = Zubehörrabatt","Rabatt 2  = Zubehörrabatt","Rabais 2  = Accessoire","Ribasso 2 = Sistema riabsso accessori "]
["RA-Verlängerung (ICS)","RA-Verlängerung (ICS)","Prolongation RA (ICS)","Prolunga RA (ICS)"]
[{"$f":"IF($A$1=1,B332,IF($A$1=2,C332,IF($A$1=3,D332,E332)))","v":"Anschlussrosette DW"},"Anschlussrosette DW","Rosace DW","Raccordo rosette DW"]
["Statische Klemmbänder (2 Stk)","Statische Klemmbänder (2 Stk)","Bride securité large (2 Stk)","Brida statica larga (2 pezzi)"]
["Rohr 200 mm","Rohr 200 mm","Tube 200 mm","Tubo 200 mm"]
["Rohr 450 mm","Rohr 450 mm","Tube 450 mm","Tubo 450 mm"]
["Rohr 455 mm","Rohr 455 mm","Tube 455 mm","Tubo 455 mm"]
["Rohr 205 mm","Rohr 205 mm","Tube 205 mm","Tubo 205 mm"]
["BM mit Fussteil","BM mit Fussteil","Socle avec écoulement","Montaggio terra con scarico di condensa"]
["max. Abstand  75 - 300 mm","max. Abstand  75 - 300 mm","Distance max. 75 - 300 mm","max. distanza 75 - 300 mm"]
[{"$f":"IF($A$1=1,B340,IF($A$1=2,C340,IF($A$1=3,D340,E340)))","v":"max. Abstand  114 mm"},"max. Abstand  114 mm","Distance max. 114 mm","max. distanza 114 mm"]
[{"$f":"IF($A$1=1,B341,IF($A$1=2,C341,IF($A$1=3,D341,E341)))","v":"max. Abstand  122 mm"},"max. Abstand  122 mm","Distance max. 122 mm","max. distanza 122 mm"]
["max. Abstand  200 mm","max. Abstand  200 mm","Distance max. 200 mm","max. distanza 200 mm"]
["max. Abstand  220 mm","max. Abstand  220 mm","Distance max. 220 mm","max. distanza 220 mm"]
["max. Abstand  250 mm","max. Abstand  250 mm","Distance max. 250 mm","max. distanza 250 mm"]
["max. Abstand  270 mm","max. Abstand  270 mm","Distance max. 270 mm","max. distanza 270 mm"]
["max. Abstand  300 mm","max. Abstand  300 mm","Distance max. 300 mm","max. distanza 300 mm"]
["max. Abstand  315 mm","max. Abstand  315 mm","Distance max. 315 mm","max. distanza 315 mm"]
["max. Abstand  320 mm","max. Abstand  320 mm","Distance max. 320 mm","max. distanza 320 mm"]
["max. Abstand  335 mm","max. Abstand  335 mm","Distance max. 335 mm","max. distanza 335 mm"]
["max. Abstand  365 mm","max. Abstand  365 mm","Distance max. 365 mm","max. distanza 365 mm"]
["max. Abstand  370 mm","max. Abstand  370 mm","Distance max. 370 mm","max. distanza 370 mm"]
["max. Abstand  385 mm","max. Abstand  385 mm","Distance max. 385 mm","max. distanza 385 mm"]
["max. Abstand  415 mm","max. Abstand  415 mm","Distance max. 415 mm","max. distanza 415 mm"]
["max. Abstand  435 mm","max. Abstand  435 mm","Distance max. 435 mm","max. distanza 435 mm"]
[{"$f":"IF($A$1=1,B355,IF($A$1=2,C355,IF($A$1=3,D355,E355)))","v":"max. Abstand  440 mm"},"max. Abstand  440 mm","Distance max. 440 mm","max. distanza 440 mm"]
[{"$f":"IF($A$1=1,B356,IF($A$1=2,C356,IF($A$1=3,D356,E356)))","v":"max. Abstand  470 mm"},"max. Abstand  470 mm","Distance max. 470 mm","max. distanza 470 mm"]
[{"$f":"IF($A$1=1,B357,IF($A$1=2,C357,IF($A$1=3,D357,E357)))","v":"max. Abstand  500 mm"},"max. Abstand  500 mm","Distance max. 500 mm","max. distanza 500 mm"]
["max. Abstand  615 mm","max. Abstand  615 mm","Distance max. 615 mm","max. distanza 615mm"]
["max. Abstand  635 mm","max. Abstand  635 mm","Distance max. 635 mm","max. distanza 635 mm"]
["max. Abstand  665 mm","max. Abstand  665 mm","Distance max. 665 mm","max. distanza 665 mm"]
[{"$f":"IF($A$1=1,B361,IF($A$1=2,C361,IF($A$1=3,D361,E361)))","v":"max. Abstand  670 mm"},"max. Abstand  670 mm","Distance max. 670 mm","max. distanza 670 mm"]
["max. Abstand  685 mm","max. Abstand  685 mm","Distance max. 685 mm","max. distanza 685 mm"]
[{"$f":"IF($A$1=1,B363,IF($A$1=2,C363,IF($A$1=3,D363,E363)))","v":"max. Abstand  700 mm"},"max. Abstand  700 mm","Distance max. 700 mm","max. distanza 700 mm"]
["max. Abstand  715 mm","max. Abstand  715 mm","Distance max. 715 mm","max. distanza 715 mm"]
["max. Abstand  735 mm","max. Abstand  735 mm","Distance max. 735 mm","max. distanza 735 mm"]
["(10 cm für Mündung vorsehen!)","(10 cm für Mündung vorsehen!)","(prévoir 10 cm pour l'embouchure!)","(10 cm previsti per l`imboccatura!)  "]
["Basiselement für RA","Basiselement für RA","Embranchement","Elemento base per raccordo RA"]
["T-Stück 45°","T-Stück 45°","Racc. de fumée 45°","Pezzo T 45°"]
["T-Stück 90°","T-Stück 90°","Racc. de fumée 90°","Pezzo T 90°"]
["Bogen 85° mit Stützfuss","Bogen 85° mit Stützfuss","Pied de cheminée 85°","Curva 85° con rinforzo piede"]
["max. Abstand  400 mm","max. Abstand  400 mm","Distance max. 400 mm","max. distanza 400 mm"]
["max. Abstand  600 mm","max. Abstand  600 mm","Distance max. 600 mm","max. distanza 600 mm"]
["Bogen 45° mit Stützfuss","Bogen 45° mit Stützfuss","Pied de cheminée 45°","Curva 45° con rinforzo piede"]
["max. Abstand  165 mm","max. Abstand  165 mm","Distance max. 165 mm","max. distanza 165 mm"]
["max. Abstand  280 mm","max. Abstand  280 mm","Distance max. 280 mm","max. distanza 280 mm"]
["max. Abstand  225 mm","max. Abstand  225 mm","Distance max. 225 mm","max. distanza 225 mm"]
["max. Abstand  580 mm","max. Abstand  580 mm","Distance max. 580 mm","max. distanza 580 mm"]
["max. Abstand  525 mm","max. Abstand  525 mm","Distance max. 525 mm","max. distanza 525 mm"]
["max. Abstand  740 mm","max. Abstand  740 mm","Distance max. 740 mm","max. distanza 740 mm"]
["max. Abstand  690 mm","max. Abstand  690 mm","Distance max. 690 mm","max. distanza 690 mm"]
["max. Abstand  640 mm","max. Abstand  640 mm","Distance max. 640 mm","max. distanza 640 mm"]
["Wandabstand (>50 mm)","Wandabstand (>50 mm)","distance de murale (>50 mm)","distanza parete murale (<50 mm)"]
["Wandhalter verstellbar 75-300mm","Wandhalter verstellbar 75-300mm","Fixation murale réglable 75-300mm","Fissaggio murale regolabile 75-300mm"]
["Abdeckblende","Abdeckblende","Recouvrement","Copertura"]
["Mündungslösung","Mündungslösung","Solution de la souche","Soluzione terminale"]
["Mündungskonus","Mündungskonus","Cône de finition","Rifinizione cono"]
["Regenhaube","Regenhaube","Cape parapluie","Cappa isolamento pioggia"]
["Basten Standard","Basten Standard","Basten Standard","Basten standard"]
["BM mit Teleskopstütze","BM mit Teleskopstütze","Pied réglable, monté au sol","Piede regolabile, montaggio sopra"]
["Dehnfugenmanschette","Dehnfugenmanschette","Tôle de dilatation","Colletto con dilatazione"]
["Zwischensumme - Kamin","Zwischensumme - Kamin","Sous-total conduit","Somma parziale"]
["Verbindungsleitung","Verbindungsleitung","Raccordement","Raccordo inserimento"]
["Zwischensumme - Verbindungsleitung","Zwischensumme - Verbindungsleitung","Sous-total raccordement","Somma parziale raccordo inserimento"]
["max. Abstand  100 mm","max. Abstand  100 mm","Distance max. 100 mm","max. distanza 100 mm"]
["max. Abstand  250 mm","max. Abstand  250 mm","Distance max. 250 mm","max. distanza 250 mm"]
["max. Abstand  400 mm","max. Abstand  400 mm","Distance max. 400 mm","max. distanza 400 mm"]
["max. Abstand  510 mm","max. Abstand  510 mm","Distance max. 510 mm","max. distanza 510 mm"]
["max. Abstand  600 mm","max. Abstand  600 mm","Distance max. 600 mm","max. distanza 600 mm"]
["Angebot speichern","Angebot speichern","Enregistrer l'offre","Registrare l'offerta"]
["Stückliste erweitern","Stückliste erweitern","Étendre la liste des pièces","Estendere lista prezzi"]
["Stückliste schliessen","Stückliste schliessen","Fermer la liste des pièces","Chiudere lista prezzi"]
["Druckansicht","Druckansicht","Apercu avant imression","Anteprima "]
["Seitenwechsel","Seitenwechsel","Changer de page ","Pagina succesiva "]
[{"$f":"IF($A$1=1,B404,IF($A$1=2,C404,IF($A$1=3,D404,E404)))","v":"aufheben"},"aufheben","annuler","Concludere"]
["Frachtberechnungen:","Frachtberechnungen:","Barème des frais de transport","Calcolazione di trasporto:"]
["1. Frachtberechnung nach Tonne","1. Frachtberechnung nach Tonne","1. Facturation par tonne ","1. Calcolazione per tonnellate"]
["(ab Baustoffhandel)","(ab Baustoffhandel)","(Départ marchand matériaux)","(departe Materiali construtione ) "]
["2. Frachtberechnung nach","2. Frachtberechnung nach","2. Facturation selon barème Schiedel,","2. Calcolazione per"]
["Schiedel Transportpreise ab Werk Döttingen","Schiedel Transportpreise ab Werk Döttingen","   (Départ usine Döttingen)","Schiedel listino prezzi di transporto da fabbrica Döttingen"]
["Thermo-Dichtset","Thermo-Dichtset","Set d’étanchéité Thermo","Guarnizione termico"]
["für","für","pour","Per"]
["Aussenmass:","Aussenmass:","diametre extérieures ","Misura esteriore"]
["Schmalseite parallel zum First","Schmalseite parallel zum First","Parallèlement à la fine crête ","Parte sottile parallela alla cresta"]
["Längsseite parallel zum First","Längsseite parallel zum First","La longueur parallèle à la crête ","Parte lungh parallela alla cresta"]
["Schachttüre grundiert","Schachttüre grundiert","Porte pour gaine ","Portina  impermiabile "]
["Schachttüre gasdicht","Schachttüre gasdicht","Porte pour gaine ÉTANCHE AUX GAZ","Portina impermiabile a gas"]
["Endmuffe","Endmuffe","Manchon Termine","Muffa finale"]
["Schachtabdeckung PE","Schachtabdeckung PE","Recouvrement de souche en PE","Copertura del tombino PE"]
["Schachtabdeckung CNS","Schachtabdeckung CNS","Recouvrement de souche en inox","Copertura del tombino CNS"]
["Schachtabdeckung CNS Flex","Schachtabdeckung CNS Flex","Recouvrement de souche en inox CHFLX","Copertura del tombino CNS flex"]
["ISOLIT Monoblock Feststoffkaminsystem","ISOLIT Monoblock Feststoffkaminsystem","ISOLIT système canaux monoblocs pour les combustibles solides ","Isolit canna fumaria monoblocco per combustibili solidi"]
["mit eingebetteten Luftkammern in den Wandungen","mit eingebetteten Luftkammern in den Wandungen","Embedded avec des chambres à air dans les murs ","Embedded con camere d'aria nelle pareti "]
["Cheminée-Anfänger","Cheminée-Anfänger","Dépard de cheminée","Elemanto iniziale "]
["Gasdichte Russtüre","Gasdichte Russtüre","Porte de ramonage étanche","Portina fuliggine ermetica ai gas"]
["Elementhöhe 25 cm","Elementhöhe 25 cm","Hauteur de Conduit 25cm","Altezza dell'elemento 25 cm "]
["Bauhöhe 50 cm","Bauhöhe 50 cm","hauteur 50cm","Altezza 50 cm"]
["Rauchrohranschlusselement","Rauchrohranschlusselement","Raccord de conduit de fumée","Elemento con raccordo per condotto"]
["Kaminschleifung","Kaminschleifung","Déviation de canaux","Deviazione dell canna fumaria "]
["Schleifungen bis max. 30°","Schleifungen bis max. 30°","Déviation de canaux max.30°","Deviazione dell canna fumaria fino max. 30°"]
["1.Zug","1.Zug","1.canal","1. condotto"]
["2.kl.Zug","2.kl.Zug","2.p.canal","2. condotto piccolo"]
["Absolut Thermo gibt es ","Absolut Thermo gibt es ","Absolut thermique il ya  ","Thermo Absolut è disponibile "]
["nur für die Kamintypen:","nur für die Kamintypen:","seulement pour les types de foyer:","solo per il caminetto tipi: "]
["2 x 4 m = bis 1,50 m über Dach*","2 x 4 m = bis 1,50 m über Dach*","2 x 4 m  = jusque à 1.50m sur toit *","2 x 4 m = 1.50m fino al tetto * "]
["4 x 4 m = bis 2,00 m über Dach*","4 x 4 m = bis 2,00 m über Dach*","4 x 4 m  = jusque à 2.00m sur toit *","4 x 4 m = 1.50m fino al tetto * "]
["4 x 6 m = bis 3,00 m über Dach*","4 x 6 m = bis 3,00 m über Dach*","4 x 6 m  = jusque à 3.00m sur toit *","4 x 6 m = 1.50m fino al tetto * "]
["*ab Kaminhalter","*ab Kaminhalter","* depuis la dernière fixation ","* Dopo l'ultima fissazione "]
["Bauhöhe 33 cm","Bauhöhe 33 cm","Hauteur 33 cm ","Altezza 33 cm "]
["Rauchrohranschlusshöhe auf Achse","Rauchrohranschlusshöhe auf Achse","Axe tube de raccordement","Asse di collegamento tubo"]
["gerechnet  ab UK Sockel (bei Bodenmontage)","gerechnet  ab UK Sockel (bei Bodenmontage)","calculer depuis sous le Socle (Montage au sol)","dal momento che nel calcolo della base (terra montato) "]
["ab OK Wandkonsole (bei Wandmontage)","ab OK Wandkonsole (bei Wandmontage)","calculer depuis sur la plaque de base (montage murale)","calcolati a partire dalla piastra di base (il montaggio a parete)"]
["Ein Rauchrohranschluss ist in der Anlage enthalten !","Ein Rauchrohranschluss ist in der Anlage enthalten !","Un raccordement de fumée par conduit est compris !","A proposito di fumo condotta è incluso! "]
["Dachdurchführung inkl. Regenkragen","Dachdurchführung inkl. Regenkragen","Garniture de cheminée y compris collerette","Roof pioggia collo incluso l'attuazione"]
["Erfoderlich bei Höhen über oberster","Erfoderlich bei Höhen über oberster","Nécessaire à partir d’une hauteur dépassant","Obbligatorio ad altitudini al di sopra del muro "]
["Wandhalterung ab 1,5 - 3,0 m freistehend !","Wandhalterung ab 1,5 - 3,0 m freistehend !","1,5 m - 3m depuis la dernière fixation !","1.5m - 3m dopo l'ultima impostazione! "]
[{"$f":"IF($A$1=1,B446,IF($A$1=2,C446,IF($A$1=3,D446,E446)))","v":"Unterdruck im Kamin: "},"Unterdruck im Kamin: ","Dépression dans le conduit","Sotto pressione nel camino"]
["Ausführung ohne Dichtringe","Ausführung ohne Dichtringe","Montage sans joint","Montaggio senza anelli di tenuta "]
["Überdruck im Kamin","Überdruck im Kamin","Surpression dans le conduit","Su pressione nel camino"]
["Ausführung mit Dichtringen  ","Ausführung mit Dichtringen  ","Montage avec joint","Montaggio con guarnizione "]
["Wandhalter verstellbar 75 -300mm","Wandhalter verstellbar 75 -300mm","Fixation murale réglable 75 – 300mm","Collare a muro regolabile 75 - 300mm"]
["ab 350mm Sonderanfertigung !","ab 350mm Sonderanfertigung !","à partir de 350mm fabrication spéciale","Da 350 millimetri di fabbricazione speciale "]
["Erforderlich bei Höhen über oberster Wandhalterung","Erforderlich bei Höhen über oberster Wandhalterung","Nécessaire à partir d’une hauteur dépassant 1.50 – 3.00m ","Necessario da una altezza superiore a 1,50 - 3,00 m "]
["ab 1,5 - 3,0 m (bis Ø 405 mm), bzw. ab 1,5 m - 2,00 m","ab 1,5 - 3,0 m (bis Ø 405 mm), bzw. ab 1,5 m - 2,00 m","(jusqu’à ø 405mm) resp. 1.5 – 2.00 (dès ø 455mm) ","(fino a ø 405 millimetri), resp. 1,5 - 2,00 (da ø 455 millimetri) "]
["(ab Ø 455 mm) freistehend !","(ab Ø 455 mm) freistehend !","depuis la dernière fixation murale !","da l'ultima fissazione murale !"]
["ab Ø 405 ist bei Betriebsweise Überdruck","ab Ø 405 ist bei Betriebsweise Überdruck","Dès Ø 405mm le mode de fonctionnement en surpression ","Una volta Ø 405 millimetri come sovrapressione "]
["nur Brennstoff Gas möglich !","nur Brennstoff Gas möglich !","uniquement pour le combustible gaz","solo per il gas combustibile "]
["Unterdruck im Schornstein: ","Unterdruck im Schornstein: ","Dépression dans le conduit","Depressione in condotto"]
["Ausführung mit Rapid fugendicht.","Ausführung mit Rapid fugendicht.","Montage avec joint ”Rapid”","Sistemazione con allegata rapida "]
[{"$f":"IF($A$1=1,B459,IF($A$1=2,C459,IF($A$1=3,D459,E459)))","v":"Überdruck im Schornstein: "},"Überdruck im Schornstein: ","Surpression dans le conduit","Soprapressione in condotta "]
[{"$f":"IF($A$1=1,B460,IF($A$1=2,C460,IF($A$1=3,D460,E460)))","v":"Ausführung mit Rotempo Fugenmasse,"},"Ausführung mit Rotempo Fugenmasse,","Montage avec joint ”Rotempo”,","Sistemazione con allegata Rotempo "]
[{"$f":"IF($A$1=1,B461,IF($A$1=2,C461,IF($A$1=3,D461,E461)))","v":"Abgastemperatur bis 200° C."},"Abgastemperatur bis 200° C.","Température des gaz de fumée max. 200°C","Temperatura dei gas di scarico max. 200 ° C "]
[{"$f":"IF($A$1=1,B462,IF($A$1=2,C462,IF($A$1=3,D462,E462)))","v":"Hier haben Sie die Möglichkeit im abgespeicherten Angebot, bei der Materialbestellung Lieferanten vorzubelegen."},"Hier haben Sie die Möglichkeit im abgespeicherten Angebot, bei der Materialbestellung Lieferanten vorzubelegen.","Ici, vous avez la possibilité de données de l'offre, lors de la vorzubelegen fournisseurs de matériel. ","Qui avete la possibilità per l'offerta gia salvata di proporre il fornitori per l'ordinazione dei materiali"]
["Wählen Sie einen Dateinamen:","Wählen Sie einen Dateinamen:","Sélectionnez un nom de fichier: ","Scegli un file: "]
["Dieses Angebot wird in den Desktop-Ordner 'Kaminprofi_Offerte' gespeichert.","Dieses Angebot wird in den Desktop-Ordner 'Kaminprofi_Offerte' gespeichert.","Cette offre est dans le bureau le dossier 'Kaminprofi_Offerte' enregistré. ","Questa offerta è nella cartella del desktop 'Kaminprofi_Offerte salvato. "]
["Datei speichern unter:","Datei speichern unter:","Enregistrer sous: ","Salva il file come: "]
["Schiedel Ku.Nr.","Schiedel Ku.Nr.","Schiedel N° client","Schiedel Nr. cliente "]
["STK","STK","PCE","PZ"]
["PAR","PAR","2PCE","2PZ"]
["Versandart bitte wählen!","Versandart bitte wählen!","Veuillez choisir d'envoi! ","Spedizione selezionate! "]
["Lieferung an  Lager","Lieferung an  Lager","Livraison en stock","Consegna in magazzino "]
["Lieferung auf Baustelle","Lieferung auf Baustelle","Livraison sur chantier ","Consegna al sito "]
["Liefertermin","Liefertermin","Délais de livraison ","Termini di consegna "]
["Glänzend","Glänzend","Brillant","Lucido"]
["Matt","Matt","Mat","Oppaco"]
[{"$f":"IF($A$1=1,B475,IF($A$1=2,C475,IF($A$1=3,D475,E476)))","v":"Kupfer"},"Kupfer","Cuivre","Rame"]
[{"$f":"IF($A$1=1,B476,IF($A$1=2,C476,IF($A$1=3,D476,E476)))","v":"ICS Kupfer"},"ICS Kupfer","ICS Cuivre","ICS Rame"]
["Typ  ICK Kupfer Ø ","Typ  ICK Kupfer Ø ","Type ICK Cuivre Ø","Tipo ICK Rame Ø"]
["Typ","Typ","Type","Tipo"]
["Typ/Lichter Ø mm","Typ/Lichter Ø mm","Type/Dimension intérieur Ø mm","Tipo/Dimensione interiore Ømm"]
[{"$f":"IF($A$1=1,B480,IF($A$1=2,C480,IF($A$1=3,D480,E480)))","v":"ICS Matt"},"ICS Matt","ICS Mat","ICS Oppaco"]
["ICS Glänzend","ICS Glänzend","ICS Brillant","ICS Lucido"]
[{"$f":"IF($A$1=1,B482,IF($A$1=2,C482,IF($A$1=3,D482,E482)))","v":"Grundpaket"},"Grundpaket","Set de base","Set di Piedi"]
[{"$f":"IF($A$1=1,B483,IF($A$1=2,C483,IF($A$1=3,D483,E483)))","v":"Das doppelwandige Edelstahl-Abgassystem für"},"Das doppelwandige Edelstahl-Abgassystem für","ICS 5000 Système de conduit de fumée double paroi enacier inox,","ICS 5000Sistema a doppia parete di acciaio inossidabile"]
[{"$f":"IF($A$1=1,B484,IF($A$1=2,C484,IF($A$1=3,D484,E484)))","v":"Hochdruck-Abgasanlagen bis 600°C (5000Pa)"},"Hochdruck-Abgasanlagen bis 600°C (5000Pa)","pour les systèmes à haute pression (5000 Pa) à des températures de 600°C","per sistemi ad alta pressione (5000 Pa) a temperature di 600°C"]
[{"$f":"IF($A$1=1,B485,IF($A$1=2,C485,IF($A$1=3,D485,E485)))","v":"Dichtring Silikon"},"Dichtring Silikon","Joint en silicone","Guarnizione silicone"]
["Dichtmanschette","Dichtmanschette","Manchon de Joint","Manicotto di tenuta"]
["Abluftregenhut","Abluftregenhut","échappement capuchon de pluie","scarico parapioggia"]
["Mündungsabschluss horizontal","Mündungsabschluss horizontal","Cape de finition horizontal","Terminale horizontale"]
["Winkel","Winkel","Coude","Gomito"]
["% Rabatt 3 von ","% Rabatt 3 von ","% rabais 3 de","% Ribasso 3 di"]
["Preis","Preis","Prix","Prezzo"]
[0]
[0]
[0]
[0]

{"sheet":"Rabattübersicht","index":31,"n_rows":17,"n_cols":4,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["Gruppen Nr.","Bezeichnung","Gruppen Nr.","Rab-Gr"]
[15,"Zubehör",15,2]
[111,"Schiedel ABSOLUT",111,1]
[112,"Schiedel CHEMINEE ZUG",112,1]
[113,"Schiedel KERANOVA",113,1]
[114,"ISOLIT",114,1]
[121,"TECHNOSTAR 120",121,1]
[122,"TECHNOSTAR 120 LAS",122,1]
[131,"Schiedel PRIMA PLUS",131,1]
[132,"Schiedel CHIMFLEX",132,1]
[133,"Schiedel ICS glänzend",133,1]
[134,"Schiedel ICM matt",134,1]
[135,"Schiedel ICK verkupfert",135,1]
[136,"Schiedel ICM5000",136,1]
[137,"Schiedel KERASTAR",137,1]
[138,"Schiedel CLV",138,1]
[141,"ganztec-LEICHTBAUSCHACHT",141,1]

{"sheet":"Absolut Thermoset_I","index":32,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Absolut Thermoset","index":33,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Lieferanten","index":34,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":true,"merged":[]}
[]
["Lieferantenstamm"]
[]
[]
["Li.Nr.","Anschrift 1","Anschrift 2","Straße","PLZ","Ort","Tel.Nr.","Fax.Nr.","E-Mail","Matchcode"]
[1,"Ganztec AG",null,"Badstrasse 38",5312,"Döttingen","Tel. 0562680000","Fax. 0562680001","info@ganztec.ch",{"$f":"B6&\" \"&E6&\" \"&F6","v":"Ganztec AG 5312 Döttingen"}]
[2,null,null,null,null,null,null,null,null,{"$f":"B7&\" \"&E7&\" \"&F7","v":"  "}]
[3,null,null,null,null,null,null,null,null,{"$f":"B8&\" \"&E8&\" \"&F8","v":"  "}]
[4,null,null,null,null,null,null,null,null,{"$f":"B9&\" \"&E9&\" \"&F9","v":"  "}]
[5,null,null,null,null,null,null,null,null,{"$f":"B10&\" \"&E10&\" \"&F10","v":"  "}]
[6,null,null,null,null,null,null,null,null,"  "]
[7,null,null,null,null,null,null,null,null,"  "]
[8,null,null,null,null,null,null,null,null,"  "]
[9,null,null,null,null,null,null,null,null,"  "]
[10,null,null,null,null,null,null,null,null,"  "]
[11,null,null,null,null,null,null,null,null,"  "]
[12,null,null,null,null,null,null,null,null,"  "]
[13,null,null,null,null,null,null,null,null,"  "]
[14,null,null,null,null,null,null,null,null,"  "]
[15,null,null,null,null,null,null,null,null,"  "]
[16,null,null,null,null,null,null,null,null,"  "]
[17,null,null,null,null,null,null,null,null,"  "]
[18,null,null,null,null,null,null,null,null,"  "]
[19,null,null,null,null,null,null,null,null,"  "]
[20,null,null,null,null,null,null,null,null,"  "]
[21,null,null,null,null,null,null,null,null,"  "]
[22,null,null,null,null,null,null,null,null,"  "]
[23,null,null,null,null,null,null,null,null,"  "]
[24,null,null,null,null,null,null,null,null,"  "]
[25,null,null,null,null,null,null,null,null,"  "]
[26,null,null,null,null,null,null,null,null,"  "]
[27,null,null,null,null,null,null,null,null,"  "]
[28,null,null,null,null,null,null,null,null,"  "]
[29,null,null,null,null,null,null,null,null,{"$f":"B34&\" \"&E34&\" \"&F34","v":"  "}]
[30,null,null,null,null,null,null,null,null,{"$f":"B35&\" \"&E35&\" \"&F35","v":"  "}]

{"sheet":"Fornitori","index":35,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":true,"merged":[]}
[]
["Fornitori"]
[]
[]
["Nr.","Indirizzo 1 ","Indirizzo 2 ","Strada","Codice postale ","Luogo","Nr. Tel.","Fax.Nr.","E-Mail","Matchcode"]
[1,"Ganztec AG",null,"Badstrasse 38",5312,"Döttingen","Tel. 0562680000","Fax. 0562680001","info@ganztec.ch",{"$f":"B6&\" \"&E6&\" \"&F6","v":"Ganztec AG 5312 Döttingen"}]
[2,null,null,null,null,null,null,null,null,"  "]
[3,null,null,null,null,null,null,null,null,"  "]
[4,null,null,null,null,null,null,null,null,"  "]
[5,null,null,null,null,null,null,null,null,"  "]
[6,null,null,null,null,null,null,null,null,"  "]
[7,null,null,null,null,null,null,null,null,"  "]
[8,null,null,null,null,null,null,null,null,"  "]
[9,null,null,null,null,null,null,null,null,"  "]
[10,null,null,null,null,null,null,null,null,"  "]
[11,null,null,null,null,null,null,null,null,"  "]
[12,null,null,null,null,null,null,null,null,"  "]
[13,null,null,null,null,null,null,null,null,"  "]
[14,null,null,null,null,null,null,null,null,"  "]
[15,null,null,null,null,null,null,null,null,"  "]
[16,null,null,null,null,null,null,null,null,"  "]
[17,null,null,null,null,null,null,null,null,"  "]
[18,null,null,null,null,null,null,null,null,"  "]
[19,null,null,null,null,null,null,null,null,"  "]
[20,null,null,null,null,null,null,null,null,"  "]
[21,null,null,null,null,null,null,null,null,"  "]
[22,null,null,null,null,null,null,null,null,"  "]
[23,null,null,null,null,null,null,null,null,"  "]
[24,null,null,null,null,null,null,null,null,"  "]
[25,null,null,null,null,null,null,null,null,"  "]
[26,null,null,null,null,null,null,null,null,"  "]
[27,null,null,null,null,null,null,null,null,"  "]
[28,null,null,null,null,null,null,null,null,"  "]
[29,null,null,null,null,null,null,null,null,"  "]
[30,null,null,null,null,null,null,null,null,"  "]

{"sheet":"Einstellungstabelle","index":36,"n_rows":7942,"n_cols":27,"rows_kept":4500,"cut":true,"hidden":true,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["Gewicht",{"$f":"SUBTOTAL(9,Kalkulation!D25:D170)","v":749.11},"Zone",{"$f":"Kalkulation!O181+0","v":5312}]
[null,{"$f":"IF(ISNA(VLOOKUP(D1,M:P,4,0))=TRUE,\"N\",VLOOKUP(D1,M:P,4,0))","v":1},null,null,null,null,null,null,"Verkn."]
[null,null,null,null,null,null,null,null,"Transportkosten"]
[null,"Zone und kg","Ergebnis",null,null,null,null,null,"Preis 2012",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Altpreis","Preis 2011","Preis 2012"]
[{"$f":"IF(B1<A8,B7,IF(B1<A9,B8,IF(B1<A10,B9,IF(B1<A11,B10,IF(B1<A12,B11,IF(B1<A13,B12,IF(B1<A14,B13,IF(B1<A15,B14,D5))))))))","v":"N"},{"$f":"B2&A5","v":"1N"},{"$f":"IF(B2=\"N\",\"\",VLOOKUP(B5,H:I,2,0))","v":197},{"$f":"IF(B1<A16,B15,IF(B1<A17,B16,IF(B1<A18,B17,IF(B1<A19,B18,IF(B1<A20,B19,IF(B1<A21,B20,IF(B1<A22,B21,E5)))))))","v":"N"},{"$f":"IF(B1<A23,B22,IF(B1<A24,B23,IF(B1<A25,B24,IF(B1<A26,B25,IF(B1<A27,B26,IF(B1<A28,B27,IF(B1<A29,B28,F5)))))))","v":"P"},{"$f":"IF(B1<A30,B29,IF(B1<A31,B30,IF(B1<A32,B31,IF(B1<A32,B31,IF(B1<A33,B32,IF(B1<A34,B33,IF(B1<A35,B34,G5)))))))","v":"W"},{"$f":"IF(B1<A36,B35,IF(B1<A37,B36,IF(B1<A38,B37,IF(B1<A39,B38,B39))))","v":"AC"},"Ergebnis","Preis",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Preis","Preis","Preis"]
[null,null,null,null,null,null,null,{"$f":"J6&K6","v":"1A"},{"$f":"Transportkosten!$C$23","v":59},1,"A",null,null,null,null,null,null,null,null,null,null,null,null,null,39,49,50]
[null,"A",null,20,null,null,null,"1B",{"$f":"Transportkosten!$D$23","v":64},1,"B",null,"PLZ","NR.","Vertreter","Zone",null,"Nr.","Vertreter","Tel.Nr.","Fax.Nr.",null,null,null,40,53,54]
[30,"B",null,30,null,null,null,"1C",{"$f":"Transportkosten!$E$23","v":70},1,"C",null,1001,856,"Frederic Widmer",4,null,883,"Kaspar Ganz","056 268 00 00","056 268 00 01",null,null,null,42,56,57]
[50,"C",null,50,null,null,null,"1D",{"$f":"Transportkosten!$F$23","v":75},1,"D",null,1002,856,"Frederic Widmer",4,null,882,"Hansruedi Blumenthal","079 236 88 22","081 633 53 43",null,null,null,45,60,61]
[75,"D",null,75,null,null,null,"1E",{"$f":"Transportkosten!$G$23","v":82},1,"E",null,1003,856,"Frederic Widmer",4,null,822,"Walter Benz","079 605 42 76","061 403 01 21",null,null,null,48,63,64]
[100,"E",null,100,null,null,null,"1F",{"$f":"Transportkosten!$H$23","v":87},1,"F",null,1004,856,"Frederic Widmer",4,null,832,"Heinz Allemann","079 605 42 77","032 323 67 25",null,null,null,50,68,70]
[125,"F",null,125,null,null,null,"1G",{"$f":"Transportkosten!$I$23","v":98},1,"G",null,1005,856,"Frederic Widmer",4,null,856,"Frédéric Widmer","076 578 60 01","021 803 60 05",null,null,null,55,80,81]
[150,"G",null,150,null,null,null,"1H",{"$f":"Transportkosten!$J$23","v":112},1,"H",null,1006,856,"Frederic Widmer",4,null,430,"Georgio Solari","079 331 11 51","091 9 94 73 64",null,null,null,60,90,92]
[200,"H",null,200,null,null,null,"1I",{"$f":"Transportkosten!$K$23","v":125},1,"I",null,1007,856,"Frederic Widmer",4,null,880,"Walter Benz","079 605 42 76","061 403 01 21",null,null,null,68,106,108]
[250,"I",null,250,null,null,null,"1J",{"$f":"Transportkosten!$L$23","v":139},1,"J",null,1008,856,"Frederic Widmer",4,null,811,"Hans Kathriner","079 474 39 20","032 631 20 25",null,null,null,79,111,114]
[300,"J",null,300,null,null,null,"1K",{"$f":"Transportkosten!$M$23","v":153},1,"K",null,1009,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,83,119,121]
[400,"K",null,400,null,null,null,"1L",{"$f":"Transportkosten!$N$23","v":167},1,"L",null,1010,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,87,128,131]
[500,"L",null,500,null,null,null,"1M",{"$f":"Transportkosten!$O$23","v":181},1,"M",null,1011,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,93,139,141]
[600,"M",null,600,null,null,null,"1N",{"$f":"Transportkosten!$P$23","v":197},1,"N",null,1012,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,101,155,159]
[700,"N",null,700,null,null,null,"1O",{"$f":"Transportkosten!$Q$23","v":214},1,"O",null,1014,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,114,176,180]
[800,"O",null,800,null,null,null,"1P",{"$f":"Transportkosten!$R$23","v":237},1,"P",null,1015,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,129,194,198]
[900,"P",null,900,null,null,null,"1Q",{"$f":"Transportkosten!$S$23","v":260},1,"Q",null,1017,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,141,212,216]
[1000,"Q",null,1000,null,null,null,"1R",{"$f":"Transportkosten!$T$23","v":283},1,"R",null,1018,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,156,227,231]
[1250,"R",null,1250,null,null,null,"1S",{"$f":"Transportkosten!$U$23","v":306},1,"S",null,1020,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,168,246,251]
[1500,"S",null,1500,null,null,null,"1T",{"$f":"Transportkosten!$V$23","v":336},1,"T",null,1022,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,181,261,267]
[1750,"T",null,1750,null,null,null,"1U",{"$f":"Transportkosten!$W$23","v":405},1,"U",null,1023,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,194,335,342]
[2000,"U",null,2000,null,null,null,"1V",{"$f":"Transportkosten!$X$23","v":480},1,"V",null,1024,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,250,400,408]
[3000,"V",null,3000,null,null,null,"1W",{"$f":"Transportkosten!$Y$23","v":560},1,"W",null,1025,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,302,454,463]
[4000,"W",null,4000,null,null,null,"1X",{"$f":"Transportkosten!$Z$23","v":653},1,"X",null,1026,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,340,533,544]
[5000,"X",null,5000,null,null,null,"1Y",{"$f":"Transportkosten!$AA$23","v":763},1,"Y",null,1027,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,404,636,649]
[7500,"Y",null,7500,null,null,null,"1Z",{"$f":"Transportkosten!$AB$23","v":844},1,"Z",null,1028,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,487,689,703]
[10000,"Z",null,10000,null,null,null,"1AA",{"$f":"Transportkosten!$AC$23","v":901},1,"AA",null,1029,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,533,741,756]
[12500,"AA",null,12500,null,null,null,"1AB",{"$f":"Transportkosten!$AD$23","v":0},1,"AB",null,1030,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,579,776,791]
[15000,"AB",null,15000,null,null,null,"1AC",{"$f":"Transportkosten!$AE$23","v":0},1,"AC",null,1031,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,606,837,854]
[17500,"AC",null,17500,null,null,null,"1AD",{"$f":"Transportkosten!$AF$23","v":0},1,"AD",null,1032,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,661,907,925]
[20000,"AD",null,20000,null,null,null,"1AE",{"$f":"Transportkosten!$AG$23","v":0},1,"AE",null,1033,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,717,978,997]
[22500,"AE",null,22500,null,null,null,"1AF",{"$f":"Transportkosten!$AG$23","v":0},1,"AF",null,1034,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,781,978,997]
[25000,"AE",null,25000,null,null,null,"2A",{"$f":"Transportkosten!$C$14","v":65},2,"A",null,1035,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,44,54,55]
[25000,"AF",null,null,null,null,null,"2B",{"$f":"Transportkosten!$D$14","v":71},2,"B",null,1036,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,47,58,59]
[null,null,null,null,null,null,null,"2C",{"$f":"Transportkosten!$E$14","v":75},2,"C",null,1037,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,49,61,62]
[null,null,null,null,null,null,null,"2D",{"$f":"Transportkosten!$F$14","v":82},2,"D",null,1038,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,53,64,65]
[null,null,null,null,null,null,null,"2E",{"$f":"Transportkosten!$G$14","v":91},2,"E",null,1040,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,62,76,77]
[null,null,null,null,null,null,null,"2F",{"$f":"Transportkosten!$H$14","v":99},2,"F",null,1041,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,67,83,85]
[null,null,null,null,null,null,null,"2G",{"$f":"Transportkosten!$I$14","v":118},2,"G",null,1042,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,75,98,100]
[null,null,null,null,null,null,null,"2H",{"$f":"Transportkosten!$J$14","v":140},2,"H",null,1043,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,87,114,117]
[null,null,null,null,null,null,null,"2I",{"$f":"Transportkosten!$K$14","v":162},2,"I",null,1044,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,102,134,137]
[null,null,null,null,null,null,null,"2J",{"$f":"Transportkosten!$L$14","v":178},2,"J",null,1045,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,108,142,145]
[null,null,null,null,null,null,null,"2K",{"$f":"Transportkosten!$M$14","v":193},2,"K",null,1046,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,114,150,153]
[null,null,null,null,null,null,null,"2L",{"$f":"Transportkosten!$N$14","v":208},2,"L",null,1051,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,124,163,166]
[null,null,null,null,null,null,null,"2M",{"$f":"Transportkosten!$O$14","v":227},2,"M",null,1052,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,134,177,181]
[null,null,null,null,null,null,null,"2N",{"$f":"Transportkosten!$P$14","v":252},2,"N",null,1053,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,149,200,203]
[null,null,null,null,null,null,null,"2O",{"$f":"Transportkosten!$Q$14","v":278},2,"O",null,1054,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,165,223,227]
[null,null,null,null,null,null,null,"2P",{"$f":"Transportkosten!$R$14","v":301},2,"P",null,1055,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,182,247,252]
[null,null,null,null,null,null,null,"2Q",{"$f":"Transportkosten!$S$14","v":324},2,"Q",null,1058,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,197,266,271]
[null,null,null,null,null,null,null,"2R",{"$f":"Transportkosten!$T$14","v":347},2,"R",null,1059,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,211,282,288]
[null,null,null,null,null,null,null,"2S",{"$f":"Transportkosten!$U$14","v":376},2,"S",null,1061,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,232,307,313]
[null,null,null,null,null,null,null,"2T",{"$f":"Transportkosten!$V$14","v":416},2,"T",null,1062,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,250,324,331]
[null,null,null,null,null,null,null,"2U",{"$f":"Transportkosten!$W$14","v":509},2,"U",null,1063,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,392,424,433]
[null,null,null,null,null,null,null,"2V",{"$f":"Transportkosten!$X$14","v":607},2,"V",null,1064,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,494,494,503]
[null,null,null,null,null,null,null,"2W",{"$f":"Transportkosten!$Y$14","v":693},2,"W",null,1066,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,450,575,587]
[null,null,null,null,null,null,null,"2X",{"$f":"Transportkosten!$Z$14","v":809},2,"X",null,1068,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,524,670,683]
[null,null,null,null,null,null,null,"2Y",{"$f":"Transportkosten!$AA$14","v":971},2,"Y",null,1073,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,634,802,818]
[null,null,null,null,null,null,null,"2Z",{"$f":"Transportkosten!$AB$14","v":1086},2,"Z",null,1074,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,735,930,949]
[null,null,null,null,null,null,null,"2AA",{"$f":"Transportkosten!$AC$14","v":1155},2,"AA",null,1076,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,781,978,997]
[null,null,null,null,null,null,null,"2AB",{"$f":"Transportkosten!$AD$14","v":0},2,"AB",null,1077,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,836,1048,1069]
[null,null,null,null,null,null,null,"2AC",{"$f":"Transportkosten!$AE$14","v":0},2,"AC",null,1078,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,900,1128,1150]
[null,null,null,null,null,null,null,"2AD",{"$f":"Transportkosten!$AF$14","v":0},2,"AD",null,1080,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,983,1217,1241]
[null,null,null,null,null,null,null,"2AE",{"$f":"Transportkosten!$AG$14","v":0},2,"AE",null,1081,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1038,1272,1297]
[null,null,null,null,null,null,null,"3A",{"$f":"Transportkosten!$C$5","v":70},3,"A",null,1082,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,47,58,59]
[null,null,null,null,null,null,null,{"$f":"J70&K70","v":"3B"},{"$f":"Transportkosten!$D$5","v":76},3,"B",null,1083,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,53,63,64]
[null,null,null,null,null,null,null,"3C",{"$f":"Transportkosten!$E$5","v":83},3,"C",null,1084,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,55,66,67]
[null,null,null,null,null,null,null,"3D",{"$f":"Transportkosten!$F$5","v":87},3,"D",null,1085,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,59,70,72]
[null,null,null,null,null,null,null,"3E",{"$f":"Transportkosten!$G$5","v":101},3,"E",null,1086,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,67,82,84]
[null,null,null,null,null,null,null,"3F",{"$f":"Transportkosten!$H$5","v":115},3,"F",null,1088,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,75,92,94]
[null,null,null,null,null,null,null,"3G",{"$f":"Transportkosten!$I$5","v":136},3,"G",null,1092,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,85,111,114]
[null,null,null,null,null,null,null,"3H",{"$f":"Transportkosten!$J$5","v":163},3,"H",null,1093,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,102,133,136]
[null,null,null,null,null,null,null,"3I",{"$f":"Transportkosten!$K$5","v":194},3,"I",null,1094,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,120,156,160]
[null,null,null,null,null,null,null,"3J",{"$f":"Transportkosten!$L$5","v":214},3,"J",null,1095,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,130,170,174]
[null,null,null,null,null,null,null,"3K",{"$f":"Transportkosten!$M$5","v":227},3,"K",null,1096,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,140,185,188]
[null,null,null,null,null,null,null,"3L",{"$f":"Transportkosten!$N$5","v":252},3,"L",null,1097,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,157,206,210]
[null,null,null,null,null,null,null,"3M",{"$f":"Transportkosten!$O$5","v":275},3,"M",null,1098,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,175,231,236]
[null,null,null,null,null,null,null,"3N",{"$f":"Transportkosten!$P$5","v":313},3,"N",null,1110,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,197,260,266]
[null,null,null,null,null,null,null,"3O",{"$f":"Transportkosten!$Q$5","v":347},3,"O",null,1112,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,218,288,293]
[null,null,null,null,null,null,null,"3P",{"$f":"Transportkosten!$R$5","v":382},3,"P",null,1113,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,238,312,318]
[null,null,null,null,null,null,null,"3Q",{"$f":"Transportkosten!$S$5","v":405},3,"Q",null,1114,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,259,334,341]
[null,null,null,null,null,null,null,"3R",{"$f":"Transportkosten!$T$5","v":428},3,"R",null,1115,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,279,358,365]
[null,null,null,null,null,null,null,"3S",{"$f":"Transportkosten!$U$5","v":457},3,"S",null,1116,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,302,385,393]
[null,null,null,null,null,null,null,"3T",{"$f":"Transportkosten!$V$5","v":509},3,"T",null,1117,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,331,416,424]
[null,null,null,null,null,null,null,"3U",{"$f":"Transportkosten!$W$5","v":647},3,"U",null,1121,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,425,534,545]
[null,null,null,null,null,null,null,"3V",{"$f":"Transportkosten!$X$5","v":775},3,"V",null,1122,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,509,642,654]
[null,null,null,null,null,null,null,"3W",{"$f":"Transportkosten!$Y$5","v":890},3,"W",null,1123,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,570,736,751]
[null,null,null,null,null,null,null,"3X",{"$f":"Transportkosten!$Z$5","v":1029},3,"X",null,1124,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,661,855,872]
[null,null,null,null,null,null,null,"3Y",{"$f":"Transportkosten!$AA$5","v":1214},3,"Y",null,1125,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,827,1058,1080]
[null,null,null,null,null,null,null,"3Z",{"$f":"Transportkosten!$AB$5","v":1352},3,"Z",null,1126,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,928,1188,1211]
[null,null,null,null,null,null,null,"3AA",{"$f":"Transportkosten!$AC$5","v":1456},3,"AA",null,1127,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1001,1281,1307]
[null,null,null,null,null,null,null,"3AB",{"$f":"Transportkosten!$AD$5","v":0},3,"AB",null,1128,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1084,1372,1400]
[null,null,null,null,null,null,null,"3AC",{"$f":"Transportkosten!$AE$5","v":0},3,"AC",null,1131,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1148,1454,1483]
[null,null,null,null,null,null,null,"3AD",{"$f":"Transportkosten!$AF$5","v":0},3,"AD",null,1132,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1231,1558,1589]
[null,null,null,null,null,null,null,"3AE",{"$f":"Transportkosten!$AG$5","v":0},3,"AE",null,1133,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1286,1629,1661]
[null,null,null,null,null,null,null,"4A",{"$f":"Transportkosten!$C$2","v":74},4,"A",null,1134,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,50,60,61]
[null,null,null,null,null,null,null,"4B",{"$f":"Transportkosten!$D$2","v":83},4,"B",null,1135,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,59,69,71]
[null,null,null,null,null,null,null,"4C",{"$f":"Transportkosten!$E$2","v":88},4,"C",null,1136,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,61,72,74]
[null,null,null,null,null,null,null,"4D",{"$f":"Transportkosten!$F$2","v":93},4,"D",null,1137,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,63,76,77]
[null,null,null,null,null,null,null,"4E",{"$f":"Transportkosten!$G$2","v":110},4,"E",null,1138,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,76,90,92]
[null,null,null,null,null,null,null,"4F",{"$f":"Transportkosten!$H$2","v":128},4,"F",null,1141,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,86,104,106]
[null,null,null,null,null,null,null,"4G",{"$f":"Transportkosten!$I$2","v":154},4,"G",null,1142,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,99,128,131]
[null,null,null,null,null,null,null,"4H",{"$f":"Transportkosten!$J$2","v":189},4,"H",null,1143,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,122,158,161]
[null,null,null,null,null,null,null,"4I",{"$f":"Transportkosten!$K$2","v":226},4,"I",null,1144,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,145,189,193]
[null,null,null,null,null,null,null,"4J",{"$f":"Transportkosten!$L$2","v":249},4,"J",null,1145,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,159,207,211]
[null,null,null,null,null,null,null,"4K",{"$f":"Transportkosten!$M$2","v":271},4,"K",null,1146,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,173,228,232]
[null,null,null,null,null,null,null,"4L",{"$f":"Transportkosten!$N$2","v":301},4,"L",null,1147,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,191,252,257]
[null,null,null,null,null,null,null,"4M",{"$f":"Transportkosten!$O$2","v":336},4,"M",null,1148,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,211,279,285]
[null,null,null,null,null,null,null,"4N",{"$f":"Transportkosten!$P$2","v":376},4,"N",null,1149,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,238,315,321]
[null,null,null,null,null,null,null,"4O",{"$f":"Transportkosten!$Q$2","v":416},4,"O",null,1162,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,261,343,350]
[null,null,null,null,null,null,null,"4P",{"$f":"Transportkosten!$R$2","v":451},4,"P",null,1163,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,282,368,375]
[null,null,null,null,null,null,null,"4Q",{"$f":"Transportkosten!$S$2","v":475},4,"Q",null,1164,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,304,394,402]
[null,null,null,null,null,null,null,"4R",{"$f":"Transportkosten!$T$2","v":503},4,"R",null,1165,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,324,417,425]
[null,null,null,null,null,null,null,"4S",{"$f":"Transportkosten!$U$2","v":537},4,"S",null,1166,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,359,456,465]
[null,null,null,null,null,null,null,"4T",{"$f":"Transportkosten!$V$2","v":601},4,"T",null,1170,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,392,494,503]
[null,null,null,null,null,null,null,"4U",{"$f":"Transportkosten!$W$2","v":775},4,"U",null,1172,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,520,653,666]
[null,null,null,null,null,null,null,"4V",{"$f":"Transportkosten!$X$2","v":930},4,"V",null,1173,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,619,778,794]
[null,null,null,null,null,null,null,"4W",{"$f":"Transportkosten!$Y$2","v":1058},4,"W",null,1174,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,689,882,900]
[null,null,null,null,null,null,null,"4X",{"$f":"Transportkosten!$Z$2","v":1242},4,"X",null,1175,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,808,1034,1055]
[null,null,null,null,null,null,null,"4Y",{"$f":"Transportkosten!$AA$2","v":1468},4,"Y",null,1176,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,983,1244,1269]
[null,null,null,null,null,null,null,"4Z",{"$f":"Transportkosten!$AB$2","v":1617},4,"Z",null,1180,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1111,1408,1436]
[null,null,null,null,null,null,null,"4AA",{"$f":"Transportkosten!$AC$2","v":1756},4,"AA",null,1182,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1221,1547,1578]
[null,null,null,null,null,null,null,"4AB",{"$f":"Transportkosten!$AD$2","v":0},4,"AB",null,1183,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1304,1652,1685]
[null,null,null,null,null,null,null,"4AC",{"$f":"Transportkosten!$AE$2","v":0},4,"AC",null,1184,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1377,1726,1761]
[null,null,null,null,null,null,null,"4AD",{"$f":"Transportkosten!$AF$2","v":0},4,"AD",null,1185,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1469,1841,1877]
[null,null,null,null,null,null,null,"4AE",{"$f":"Transportkosten!$AG$2","v":0},4,"AE",null,1186,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1560,1956,1995]
[null,null,null,null,null,null,null,"5A",{"$f":"Transportkosten!$C$43","v":70},5,"A",null,1187,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,54,64,59]
[null,null,null,null,null,null,null,"5B",{"$f":"Transportkosten!$D$43","v":76},5,"B",null,1188,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,63,76,64]
[null,null,null,null,null,null,null,"5C",{"$f":"Transportkosten!$E$43","v":83},5,"C",null,1189,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,66,80,67]
[null,null,null,null,null,null,null,{"$f":"J134&K134","v":"5D"},{"$f":"Transportkosten!$F$43","v":87},5,"D",null,1195,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,67,82,72]
[null,null,null,null,null,null,null,"5E",{"$f":"Transportkosten!$G$43","v":101},5,"E",null,1196,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,81,98,84]
[null,null,null,null,null,null,null,"5F",{"$f":"Transportkosten!$H$43","v":115},5,"F",null,1197,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,96,118,94]
[null,null,null,null,null,null,null,"5G",{"$f":"Transportkosten!$I$43","v":136},5,"G",null,1200,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,111,143,114]
[null,null,null,null,null,null,null,"5H",{"$f":"Transportkosten!$J$43","v":163},5,"H",null,1201,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,130,170,136]
[null,null,null,null,null,null,null,"5I",{"$f":"Transportkosten!$K$43","v":194},5,"I",null,1202,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,153,201,160]
[null,null,null,null,null,null,null,"5J",{"$f":"Transportkosten!$L$43","v":214},5,"J",null,1203,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,176,231,174]
[null,null,null,null,null,null,null,"5K",{"$f":"Transportkosten!$M$43","v":227},5,"K",null,1204,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,198,261,188]
[null,null,null,null,null,null,null,"5L",{"$f":"Transportkosten!$N$43","v":252},5,"L",null,1205,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,221,292,210]
[null,null,null,null,null,null,null,"5M",{"$f":"Transportkosten!$O$43","v":275},5,"M",null,1206,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,244,323,236]
[null,null,null,null,null,null,null,"5N",{"$f":"Transportkosten!$P$43","v":313},5,"N",null,1207,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,268,354,266]
[null,null,null,null,null,null,null,"5O",{"$f":"Transportkosten!$Q$43","v":347},5,"O",null,1208,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,290,384,293]
[null,null,null,null,null,null,null,"5P",{"$f":"Transportkosten!$R$43","v":382},5,"P",null,1209,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,320,418,318]
[null,null,null,null,null,null,null,"5Q",{"$f":"Transportkosten!$S$43","v":405},5,"Q",null,1211,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,357,464,341]
[null,null,null,null,null,null,null,"5R",{"$f":"Transportkosten!$T$43","v":428},5,"R",null,1212,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,375,482,365]
[null,null,null,null,null,null,null,"5S",{"$f":"Transportkosten!$U$43","v":457},5,"S",null,1213,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,419,531,393]
[null,null,null,null,null,null,null,"5T",{"$f":"Transportkosten!$V$43","v":509},5,"T",null,1214,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,468,588,424]
[null,null,null,null,null,null,null,"5U",{"$f":"Transportkosten!$W$43","v":647},5,"U",null,1215,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,619,778,545]
[null,null,null,null,null,null,null,"5V",{"$f":"Transportkosten!$X$43","v":775},5,"V",null,1216,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,741,932,654]
[null,null,null,null,null,null,null,"5W",{"$f":"Transportkosten!$Y$43","v":890},5,"W",null,1217,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,808,1034,751]
[null,null,null,null,null,null,null,"5X",{"$f":"Transportkosten!$Z$43","v":1029},5,"X",null,1218,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,964,1235,872]
[null,null,null,null,null,null,null,"5Y",{"$f":"Transportkosten!$AA$43","v":1214},5,"Y",null,1219,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1120,1419,1080]
[null,null,null,null,null,null,null,"5Z",{"$f":"Transportkosten!$AB$43","v":1352},5,"Z",null,1220,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1277,1616,1211]
[null,null,null,null,null,null,null,"5AA",{"$f":"Transportkosten!$AC$43","v":1456},5,"AA",null,1222,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1405,1761,1307]
[null,null,null,null,null,null,null,"5AB",{"$f":"Transportkosten!$AD$43","v":0},5,"AB",null,1223,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1515,1898,1400]
[null,null,null,null,null,null,null,"5AC",{"$f":"Transportkosten!$AE$43","v":0},5,"AC",null,1224,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1597,1979,1483]
[null,null,null,null,null,null,null,"5AD",{"$f":"Transportkosten!$AF$43","v":0},5,"AD",null,1225,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1698,2105,1589]
[null,null,null,null,null,null,null,"5AE",{"$f":"Transportkosten!$AG$43","v":0},5,"AE",null,1226,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1817,2253,1661]
[null,null,null,null,null,null,null,"6A",{"$f":"Transportkosten!$C$11","v":83},6,"A",null,1227,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,59,69,71]
[null,null,null,null,null,null,null,"6B",{"$f":"Transportkosten!$D$11","v":94},6,"B",null,1228,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,67,81,82]
[null,null,null,null,null,null,null,"6C",{"$f":"Transportkosten!$E$11","v":102},6,"C",null,1231,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,70,84,86]
[null,null,null,null,null,null,null,"6D",{"$f":"Transportkosten!$F$11","v":108},6,"D",null,1232,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,72,87,89]
[null,null,null,null,null,null,null,"6E",{"$f":"Transportkosten!$G$11","v":128},6,"E",null,1233,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,84,104,106]
[null,null,null,null,null,null,null,"6F",{"$f":"Transportkosten!$H$11","v":148},6,"F",null,1234,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,101,123,125]
[null,null,null,null,null,null,null,"6G",{"$f":"Transportkosten!$I$11","v":187},6,"G",null,1236,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,114,147,150]
[null,null,null,null,null,null,null,"6H",{"$f":"Transportkosten!$J$11","v":231},6,"H",null,1237,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,148,191,195]
[null,null,null,null,null,null,null,"6I",{"$f":"Transportkosten!$K$11","v":278},6,"I",null,1239,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,175,227,231]
[null,null,null,null,null,null,null,"6J",{"$f":"Transportkosten!$L$11","v":301},6,"J",null,1241,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,192,249,254]
[null,null,null,null,null,null,null,"6K",{"$f":"Transportkosten!$M$11","v":343},6,"K",null,1242,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,216,281,287]
[null,null,null,null,null,null,null,"6L",{"$f":"Transportkosten!$N$11","v":387},6,"L",null,1243,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,245,321,328]
[null,null,null,null,null,null,null,"6M",{"$f":"Transportkosten!$O$11","v":439},6,"M",null,1244,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,273,357,364]
[null,null,null,null,null,null,null,"6N",{"$f":"Transportkosten!$P$11","v":480},6,"N",null,1245,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,301,396,404]
[null,null,null,null,null,null,null,"6O",{"$f":"Transportkosten!$Q$11","v":521},6,"O",null,1246,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,329,431,439]
[null,null,null,null,null,null,null,"6P",{"$f":"Transportkosten!$R$11","v":560},6,"P",null,1247,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,356,467,477]
[null,null,null,null,null,null,null,"6Q",{"$f":"Transportkosten!$S$11","v":613},6,"Q",null,1248,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,390,506,516]
[null,null,null,null,null,null,null,"6R",{"$f":"Transportkosten!$T$11","v":653},6,"R",null,1251,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,421,542,553]
[null,null,null,null,null,null,null,"6S",{"$f":"Transportkosten!$U$11","v":699},6,"S",null,1252,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,466,591,603]
[null,null,null,null,null,null,null,"6T",{"$f":"Transportkosten!$V$11","v":786},6,"T",null,1253,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,520,653,666]
[null,null,null,null,null,null,null,"6U",{"$f":"Transportkosten!$W$11","v":1040},6,"U",null,1254,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,684,853,870]
[null,null,null,null,null,null,null,"6V",{"$f":"Transportkosten!$X$11","v":1237},6,"V",null,1255,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,821,1023,1043]
[null,null,null,null,null,null,null,"6W",{"$f":"Transportkosten!$Y$11","v":1399},6,"W",null,1256,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,918,1163,1187]
[null,null,null,null,null,null,null,"6X",{"$f":"Transportkosten!$Z$11","v":1630},6,"X",null,1257,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1075,1361,1388]
[null,null,null,null,null,null,null,"6Y",{"$f":"Transportkosten!$AA$11","v":1941},6,"Y",null,1258,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1240,1553,1584]
[null,null,null,null,null,null,null,"6Z",{"$f":"Transportkosten!$AB$11","v":2126},6,"Z",null,1260,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1414,1771,1807]
[null,null,null,null,null,null,null,"6AA",{"$f":"Transportkosten!$AC$11","v":2334},6,"AA",null,1261,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1551,1944,1982]
[null,null,null,null,null,null,null,"6AB",{"$f":"Transportkosten!$AD$11","v":0},6,"AB",null,1262,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1661,2083,2125]
[null,null,null,null,null,null,null,"6AC",{"$f":"Transportkosten!$AE$11","v":0},6,"AC",null,1263,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1744,2162,2205]
[null,null,null,null,null,null,null,"6AD",{"$f":"Transportkosten!$AF$11","v":0},6,"AD",null,1264,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1863,2310,2356]
[null,null,null,null,null,null,null,"6AE",{"$f":"Transportkosten!$AG$11","v":0},6,"AE",null,1265,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1973,2447,2495]
[null,null,null,null,null,null,null,{"$f":"J193&K193","v":"7A"},{"$f":"Transportkosten!$C$10","v":87},7,"A",null,1266,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,62,74,75]
[null,null,null,null,null,null,null,"7B",{"$f":"Transportkosten!$D$10","v":98},7,"B",null,1267,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,71,85,87]
[null,null,null,null,null,null,null,"7C",{"$f":"Transportkosten!$E$10","v":108},7,"C",null,1268,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,73,89,91]
[null,null,null,null,null,null,null,"7D",{"$f":"Transportkosten!$F$10","v":114},7,"D",null,1269,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,76,92,94]
[null,null,null,null,null,null,null,"7E",{"$f":"Transportkosten!$G$10","v":135},7,"E",null,1270,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,89,109,111]
[null,null,null,null,null,null,null,"7F",{"$f":"Transportkosten!$H$10","v":158},7,"F",null,1271,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,107,128,131]
[null,null,null,null,null,null,null,"7G",{"$f":"Transportkosten!$I$10","v":202},7,"G",null,1272,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,123,158,161]
[null,null,null,null,null,null,null,"7H",{"$f":"Transportkosten!$J$10","v":249},7,"H",null,1273,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,158,204,208]
[null,null,null,null,null,null,null,"7I",{"$f":"Transportkosten!$K$10","v":295},7,"I",null,1274,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,188,244,248]
[null,null,null,null,null,null,null,"7J",{"$f":"Transportkosten!$L$10","v":324},7,"J",null,1275,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,211,273,278]
[null,null,null,null,null,null,null,"7K",{"$f":"Transportkosten!$M$10","v":370},7,"K",null,1276,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,236,310,316]
[null,null,null,null,null,null,null,"7L",{"$f":"Transportkosten!$N$10","v":421},7,"L",null,1277,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,268,351,358]
[null,null,null,null,null,null,null,"7M",{"$f":"Transportkosten!$O$10","v":475},7,"M",null,1278,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,297,391,398]
[null,null,null,null,null,null,null,"7N",{"$f":"Transportkosten!$P$10","v":521},7,"N",null,1279,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,330,433,441]
[null,null,null,null,null,null,null,"7O",{"$f":"Transportkosten!$Q$10","v":572},7,"O",null,1281,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,362,475,484]
[null,null,null,null,null,null,null,"7P",{"$f":"Transportkosten!$R$10","v":619},7,"P",null,1282,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,393,516,526]
[null,null,null,null,null,null,null,"7Q",{"$f":"Transportkosten!$S$10","v":670},7,"Q",null,1283,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,425,551,562]
[null,null,null,null,null,null,null,"7R",{"$f":"Transportkosten!$T$10","v":722},7,"R",null,1284,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,457,588,600]
[null,null,null,null,null,null,null,"7S",{"$f":"Transportkosten!$U$10","v":780},7,"S",null,1285,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,516,656,669]
[null,null,null,null,null,null,null,"7T",{"$f":"Transportkosten!$V$10","v":890},7,"T",null,1286,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,585,736,751]
[null,null,null,null,null,null,null,"7U",{"$f":"Transportkosten!$W$10","v":1144},7,"U",null,1287,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,769,968,987]
[null,null,null,null,null,null,null,"7V",{"$f":"Transportkosten!$X$10","v":1381},7,"V",null,1288,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,925,1164,1188]
[null,null,null,null,null,null,null,"7W",{"$f":"Transportkosten!$Y$10","v":1577},7,"W",null,1289,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1029,1317,1343]
[null,null,null,null,null,null,null,"7X",{"$f":"Transportkosten!$Z$10","v":1831},7,"X",null,1290,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1185,1516,1547]
[null,null,null,null,null,null,null,"7Y",{"$f":"Transportkosten!$AA$10","v":2149},7,"Y",null,1291,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1359,1722,1756]
[null,null,null,null,null,null,null,"7Z",{"$f":"Transportkosten!$AB$10","v":2357},7,"Z",null,1292,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1560,1977,2017]
[null,null,null,null,null,null,null,"7AA",{"$f":"Transportkosten!$AC$10","v":2577},7,"AA",null,1293,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1698,2128,2171]
[null,null,null,null,null,null,null,"7AB",{"$f":"Transportkosten!$AD$10","v":0},7,"AB",null,1294,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1799,2255,2301]
[null,null,null,null,null,null,null,"7AC",{"$f":"Transportkosten!$AE$10","v":0},7,"AC",null,1295,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1872,2322,2368]
[null,null,null,null,null,null,null,"7AD",{"$f":"Transportkosten!$AF$10","v":0},7,"AD",null,1296,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,1992,2470,2519]
[null,null,null,null,null,null,null,"7AE",{"$f":"Transportkosten!$AG$10","v":0},7,"AE",null,1297,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,2111,2618,2670]
[null,null,null,null,null,null,null,"8A",{"$f":"Transportkosten!$C$21","v":93},8,"A",null,1298,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,65,79,80]
[null,null,null,null,null,null,null,"8B",{"$f":"Transportkosten!$D$21","v":105},8,"B",null,1299,856,"Frederic Widmer",5,null,null,null,null,null,null,null,null,74,91,93]
[null,null,null,null,null,null,null,"8C",{"$f":"Transportkosten!$E$21","v":114},8,"C",null,1302,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,76,93,95]
[null,null,null,null,null,null,null,"8D",{"$f":"Transportkosten!$F$21","v":120},8,"D",null,1303,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,79,97,99]
[null,null,null,null,null,null,null,"8E",{"$f":"Transportkosten!$G$21","v":141},8,"E",null,1304,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,93,114,117]
[null,null,null,null,null,null,null,"8F",{"$f":"Transportkosten!$H$21","v":167},8,"F",null,1305,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,113,135,138]
[null,null,null,null,null,null,null,"8G",{"$f":"Transportkosten!$I$21","v":215},8,"G",null,1306,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,134,174,178]
[null,null,null,null,null,null,null,"8H",{"$f":"Transportkosten!$J$21","v":267},8,"H",null,1307,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,166,217,222]
[null,null,null,null,null,null,null,"8I",{"$f":"Transportkosten!$K$21","v":313},8,"I",null,1308,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,198,260,266]
[null,null,null,null,null,null,null,"8J",{"$f":"Transportkosten!$L$21","v":347},8,"J",null,1309,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,219,287,292]
[null,null,null,null,null,null,null,{"$f":"J234&K234","v":"8K"},{"$f":"Transportkosten!$M$21","v":393},8,"K",null,1312,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,250,332,338]
[null,null,null,null,null,null,null,"8L",{"$f":"Transportkosten!$N$21","v":451},8,"L",null,1313,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,285,378,386]
[null,null,null,null,null,null,null,"8M",{"$f":"Transportkosten!$O$21","v":506},8,"M",null,1314,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,321,423,432]
[null,null,null,null,null,null,null,"8N",{"$f":"Transportkosten!$P$21","v":555},8,"N",null,1315,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,355,470,480]
[null,null,null,null,null,null,null,"8O",{"$f":"Transportkosten!$Q$21","v":619},8,"O",null,1316,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,391,518,528]
[null,null,null,null,null,null,null,"8P",{"$f":"Transportkosten!$R$21","v":665},8,"P",null,1317,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,425,558,569]
[null,null,null,null,null,null,null,"8Q",{"$f":"Transportkosten!$S$21","v":717},8,"Q",null,1318,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,468,607,619]
[null,null,null,null,null,null,null,"8R",{"$f":"Transportkosten!$T$21","v":791},8,"R",null,1321,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,507,660,674]
[null,null,null,null,null,null,null,"8S",{"$f":"Transportkosten!$U$21","v":861},8,"S",null,1322,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,569,731,745]
[null,null,null,null,null,null,null,"8T",{"$f":"Transportkosten!$V$21","v":983},8,"T",null,1323,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,642,817,833]
[null,null,null,null,null,null,null,"8U",{"$f":"Transportkosten!$W$21","v":1248},8,"U",null,1324,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,844,1064,1085]
[null,null,null,null,null,null,null,"8V",{"$f":"Transportkosten!$X$21","v":1525},8,"V",null,1325,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1009,1271,1296]
[null,null,null,null,null,null,null,"8W",{"$f":"Transportkosten!$Y$21","v":1756},8,"W",null,1326,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1120,1449,1478]
[null,null,null,null,null,null,null,"8X",{"$f":"Transportkosten!$Z$21","v":2033},8,"X",null,1327,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1313,1699,1733]
[null,null,null,null,null,null,null,"8Y",{"$f":"Transportkosten!$AA$21","v":2357},8,"Y",null,1328,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1488,1904,1942]
[null,null,null,null,null,null,null,"8Z",{"$f":"Transportkosten!$AB$21","v":2588},8,"Z",null,1329,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1689,2202,2246]
[null,null,null,null,null,null,null,"8AA",{"$f":"Transportkosten!$AC$21","v":2819},8,"AA",null,1337,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1808,2323,2369]
[null,null,null,null,null,null,null,"8AB",{"$f":"Transportkosten!$AD$21","v":0},8,"AB",null,1338,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1918,2444,2493]
[null,null,null,null,null,null,null,"8AC",{"$f":"Transportkosten!$AE$21","v":0},8,"AC",null,1341,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,2001,2566,2618]
[null,null,null,null,null,null,null,"8AD",{"$f":"Transportkosten!$AF$21","v":0},8,"AD",null,1342,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,2120,2687,2741]
[null,null,null,null,null,null,null,"8AE",{"$f":"Transportkosten!$AG$21","v":0},8,"AE",null,1343,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,2249,2850,2907]
[null,null,null,null,null,null,null,"9A",{"$f":"Transportkosten!$C$20","v":98},9,"A",null,1344,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,66,82,84]
[null,null,null,null,null,null,null,"9B",{"$f":"Transportkosten!$D$20","v":112},9,"B",null,1345,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,77,96,97]
[null,null,null,null,null,null,null,"9C",{"$f":"Transportkosten!$E$20","v":121},9,"C",null,1346,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,79,99,101]
[null,null,null,null,null,null,null,"9D",{"$f":"Transportkosten!$F$20","v":130},9,"D",null,1347,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,86,104,106]
[null,null,null,null,null,null,null,"9E",{"$f":"Transportkosten!$G$20","v":151},9,"E",null,1348,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,100,124,126]
[null,null,null,null,null,null,null,"9F",{"$f":"Transportkosten!$H$20","v":176},9,"F",null,1350,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,121,146,149]
[null,null,null,null,null,null,null,"9G",{"$f":"Transportkosten!$I$20","v":227},9,"G",null,1352,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,144,184,187]
[null,null,null,null,null,null,null,"9H",{"$f":"Transportkosten!$J$20","v":278},9,"H",null,1353,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,175,225,229]
[null,null,null,null,null,null,null,"9I",{"$f":"Transportkosten!$K$20","v":328},9,"I",null,1354,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,211,270,275]
[null,null,null,null,null,null,null,"9J",{"$f":"Transportkosten!$L$20","v":376},9,"J",null,1355,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,237,305,311]
[null,null,null,null,null,null,null,"9K",{"$f":"Transportkosten!$M$20","v":422},9,"K",null,1356,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,266,341,348]
[null,null,null,null,null,null,null,"9L",{"$f":"Transportkosten!$N$20","v":477},9,"L",null,1357,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,298,383,391]
[null,null,null,null,null,null,null,"9M",{"$f":"Transportkosten!$O$20","v":532},9,"M",null,1358,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,334,431,439]
[null,null,null,null,null,null,null,"9N",{"$f":"Transportkosten!$P$20","v":585},9,"N",null,1359,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,372,477,486]
[null,null,null,null,null,null,null,"9O",{"$f":"Transportkosten!$Q$20","v":652},9,"O",null,1372,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,413,530,541]
[null,null,null,null,null,null,null,"9P",{"$f":"Transportkosten!$R$20","v":711},9,"P",null,1373,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,459,590,602]
[null,null,null,null,null,null,null,"9Q",{"$f":"Transportkosten!$S$20","v":786},9,"Q",null,1374,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,507,652,665]
[null,null,null,null,null,null,null,"9R",{"$f":"Transportkosten!$T$20","v":867},9,"R",null,1375,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,559,728,742]
[null,null,null,null,null,null,null,"9S",{"$f":"Transportkosten!$U$20","v":948},9,"S",null,1376,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,616,799,815]
[null,null,null,null,null,null,null,"9T",{"$f":"Transportkosten!$V$20","v":1075},9,"T",null,1400,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,684,889,907]
[null,null,null,null,null,null,null,"9U",{"$f":"Transportkosten!$W$20","v":1363},9,"U",null,1401,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,896,1164,1188]
[null,null,null,null,null,null,null,"9V",{"$f":"Transportkosten!$X$20","v":1676},9,"V",null,1404,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1076,1411,1439]
[null,null,null,null,null,null,null,"9W",{"$f":"Transportkosten!$Y$20","v":1941},9,"W",null,1405,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1212,1634,1666]
[null,null,null,null,null,null,null,"9X",{"$f":"Transportkosten!$Z$20","v":2253},9,"X",null,1406,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1423,1919,1958]
[null,null,null,null,null,null,null,"9Y",{"$f":"Transportkosten!$AA$20","v":2600},9,"Y",null,1407,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1606,2166,2209]
[null,null,null,null,null,null,null,"9Z",{"$f":"Transportkosten!$AB$20","v":2854},9,"Z",null,1408,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1826,2427,2475]
[null,null,null,null,null,null,null,"9AA",{"$f":"Transportkosten!$AC$20","v":3062},9,"AA",null,1409,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,1927,2564,2615]
[null,null,null,null,null,null,null,"9AB",{"$f":"Transportkosten!$AD$20","v":0},9,"AB",null,1410,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,2047,2703,2757]
[null,null,null,null,null,null,null,"9AC",{"$f":"Transportkosten!$AE$20","v":0},9,"AC",null,1412,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,2120,2840,2897]
[null,null,null,null,null,null,null,"9AD",{"$f":"Transportkosten!$AF$20","v":0},9,"AD",null,1413,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,2230,2979,3038]
[null,null,null,null,null,null,null,"9AE",{"$f":"Transportkosten!$AG$20","v":0},9,"AE",null,1414,856,"Frederic Widmer",4,null,null,null,null,null,null,null,null,2368,3098,3159]
[null,null,null,null,null,null,null,null,null,null,null,null,1415,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1416,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1417,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1418,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1420,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1421,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1422,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1423,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1424,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1425,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1426,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1427,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1428,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1429,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1430,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1431,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1432,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1433,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1434,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1435,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1436,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1437,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1438,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1441,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1442,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1443,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1445,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1446,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1450,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1452,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1453,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1454,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1462,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1463,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1464,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1468,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1470,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1473,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1474,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1482,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1483,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1484,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1485,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1486,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1487,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1488,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1489,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1503,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1510,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1512,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1513,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1514,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1515,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1516,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1521,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1522,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1523,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1524,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1525,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1526,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1527,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1528,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1529,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1530,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1532,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1533,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1534,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1535,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1536,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1541,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1542,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1543,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1544,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1545,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1551,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1552,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1553,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1554,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1555,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1556,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1557,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1562,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1563,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1564,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1565,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1566,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1567,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1568,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1569,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1580,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1582,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1583,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1584,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1585,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1586,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1587,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1588,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1589,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1595,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1602,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1603,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1604,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1605,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1606,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1607,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1608,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1609,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1610,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1611,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1612,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1613,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1614,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1615,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1616,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1617,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1618,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1619,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1623,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1624,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1625,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1626,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1627,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1628,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1630,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1631,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1632,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1633,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1634,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1635,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1636,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1637,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1638,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1641,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1642,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1643,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1644,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1645,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1646,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1647,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1648,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1649,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1651,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1652,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1653,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1654,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1655,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1656,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1657,832,"Heinz Allemann",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1661,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1662,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1663,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1664,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1665,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1666,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1667,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1668,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1669,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1670,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1671,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1673,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1674,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1675,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1676,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1677,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1678,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1679,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1680,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1681,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1682,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1683,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1684,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1685,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1686,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1687,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1688,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1689,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1690,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1691,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1692,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1693,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1694,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1695,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1696,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1697,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1698,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1699,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1700,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1701,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1702,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1703,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1704,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1705,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1706,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1707,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1708,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1709,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1711,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1712,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1713,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1714,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1715,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1716,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1717,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1718,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1719,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1720,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1721,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1722,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1723,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1724,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1725,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1726,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1727,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1728,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1729,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1730,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1731,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1732,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1733,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1734,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1735,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1736,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1737,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1738,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1740,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1741,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1742,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1743,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1744,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1745,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1746,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1747,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1748,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1749,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1752,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1753,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1754,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1756,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1757,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1762,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1763,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1772,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1773,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1774,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1775,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1776,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1782,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1783,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1784,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1785,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1786,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1787,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1788,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1789,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1791,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1792,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1793,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1794,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1795,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1796,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1797,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1800,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1801,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1802,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1803,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1804,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1805,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1806,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1807,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1808,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1809,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1811,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1812,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1813,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1814,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1815,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1816,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1817,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1820,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1822,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1823,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1824,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1831,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1832,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1833,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1835,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1836,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1837,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1838,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1839,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1844,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1845,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1846,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1847,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1852,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1853,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1854,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1856,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1858,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1860,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1862,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1863,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1864,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1865,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1866,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1867,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1868,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1869,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1870,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1871,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1872,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1873,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1874,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1875,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1880,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1882,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1884,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1885,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1886,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1888,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1890,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1891,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1892,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1893,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1894,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1895,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1896,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1897,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1898,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1899,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1902,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1903,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1904,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1905,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1906,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1907,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1908,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1911,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1912,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1913,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1914,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1918,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1920,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1921,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1922,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1923,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1925,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1926,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1927,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1928,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1929,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1932,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1933,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1934,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1936,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1937,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1938,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1941,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1942,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1943,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1944,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1945,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1946,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1947,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1948,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1950,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1951,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1955,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1956,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1957,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1958,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1961,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1962,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1963,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1964,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1965,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1966,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1967,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1968,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1969,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1971,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1972,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1973,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1974,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1975,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1976,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1977,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1978,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1981,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1982,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1983,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1984,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1985,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1986,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1987,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1988,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1991,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1992,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1993,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1994,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1996,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1997,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,2000,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2001,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2002,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2003,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2004,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2005,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2006,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2007,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2008,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2009,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2010,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2012,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2013,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2014,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2015,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2016,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2017,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2022,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2023,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2024,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2025,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2026,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2027,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2028,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2034,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2035,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2036,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2042,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2043,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2046,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2052,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2053,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2054,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2056,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2057,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2058,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2063,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2065,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2067,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2068,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2072,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2073,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2074,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2075,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2076,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2087,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2088,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2096,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2103,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2105,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2108,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2112,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2113,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2114,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2115,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2116,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2117,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2123,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2124,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2126,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2127,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2149,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2202,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2203,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2205,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2206,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2207,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2208,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2209,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2300,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2301,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2302,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2303,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2304,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2305,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2306,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2314,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2315,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2316,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2318,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2322,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2325,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2332,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2333,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2336,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2338,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2340,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2345,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2350,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2353,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2354,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2400,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2405,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2406,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2407,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2408,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2413,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2414,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2416,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2500,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2501,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2502,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2503,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2504,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2505,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2512,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2513,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2514,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2515,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2516,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2517,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2518,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2520,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2523,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2525,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2532,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2533,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2534,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2535,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2536,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2537,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2538,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2540,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2542,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2543,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2544,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2545,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2552,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2553,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2554,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2555,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2556,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2557,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2558,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2560,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2562,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2563,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2564,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2565,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2572,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2575,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2576,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2577,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2578,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2603,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2604,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2605,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2606,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2607,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2608,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2610,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2612,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2613,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2615,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2616,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2710,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2711,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2712,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2713,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2714,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2715,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2716,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2717,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2718,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2720,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2722,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2723,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2732,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2733,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2735,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2736,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2738,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2740,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2742,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2743,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2744,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2745,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2746,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2747,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2748,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2762,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2800,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2802,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2803,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2805,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2806,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2807,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2812,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2813,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2814,822,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2822,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2823,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2824,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2825,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2826,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2827,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2828,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2829,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2830,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2832,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2842,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2843,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2852,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2853,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2854,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2855,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2856,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2857,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2863,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2864,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2873,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2874,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2875,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2877,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2882,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2883,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2884,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2885,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2886,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2887,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2888,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2889,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2900,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2902,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2903,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2904,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2905,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2906,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2907,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2908,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2912,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2914,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2915,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2916,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2922,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2923,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2924,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2925,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2926,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2932,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2933,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2935,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2942,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2943,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2944,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2946,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2947,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2950,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2952,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2953,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2954,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3000,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3001,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3002,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3003,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3004,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3005,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3006,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3007,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3008,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3010,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3011,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3012,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3013,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3014,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3015,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3018,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3019,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3020,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3024,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3027,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3030,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3032,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3033,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3034,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3035,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3036,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3037,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3038,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3040,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3042,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3043,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3044,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3045,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3046,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3047,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3048,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3050,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3052,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3053,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3054,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3063,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3065,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3066,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3067,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3068,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3072,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3073,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3074,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3075,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3076,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3077,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3078,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3082,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3083,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3084,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3086,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3087,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3088,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3089,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3095,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3096,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3097,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3098,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3099,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3110,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3112,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3113,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3114,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3115,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3116,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3122,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3123,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3124,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3125,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3126,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3127,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3128,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3132,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3144,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3145,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3147,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3148,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3150,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3152,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3153,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3154,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3155,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3156,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3157,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3158,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3159,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3172,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3173,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3174,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3175,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3176,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3177,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3178,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3179,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3182,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3183,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3184,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3185,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3186,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3202,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3203,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3204,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3205,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3206,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3207,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3208,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3210,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3212,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3213,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3214,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3215,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3216,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3225,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3226,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3232,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3233,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3234,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3235,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3236,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3250,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3251,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3252,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3253,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3254,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3255,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3256,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3257,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3262,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3263,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3264,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3266,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3267,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3268,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3270,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3271,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3272,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3273,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3274,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3280,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3282,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3283,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3284,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3285,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3286,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3292,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3293,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3294,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3295,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3296,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3297,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3298,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3302,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3303,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3305,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3306,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3307,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3308,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3309,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3312,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3313,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3314,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3315,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3317,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3321,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3322,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3323,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3324,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3325,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3326,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3360,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3362,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3363,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3365,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3366,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3367,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3368,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3372,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3373,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3374,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3375,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3376,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3377,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3380,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3400,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3401,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3402,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3412,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3413,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3414,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3415,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3416,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3417,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3418,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3419,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3421,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3422,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3423,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3424,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3425,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3426,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3427,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3428,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3429,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3432,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3433,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3434,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3435,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3436,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3437,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3438,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3439,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3452,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3453,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3454,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3455,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3456,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3457,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3462,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3463,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3464,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3465,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3472,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3473,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3474,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3475,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3476,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3502,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3503,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3504,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3506,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3507,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3508,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3510,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3512,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3513,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3517,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3531,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3532,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3533,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3534,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3535,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3536,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3537,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3538,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3543,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3550,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3551,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3552,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3553,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3555,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3556,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3557,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3600,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3601,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3602,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3603,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3604,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3605,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3606,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3607,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3608,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3612,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3613,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3614,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3615,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3616,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3617,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3618,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3619,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3622,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3623,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3624,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3625,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3626,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3627,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3628,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3629,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3631,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3632,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3633,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3634,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3635,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3636,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3638,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3645,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3646,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3647,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3652,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3653,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3654,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3655,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3656,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3657,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3658,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3661,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3662,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3663,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3664,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3665,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3671,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3672,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3673,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3674,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3700,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3702,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3703,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3704,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3705,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3706,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3707,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3711,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3712,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3713,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3714,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3715,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3716,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3717,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3718,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3722,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3723,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3724,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3725,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3752,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3753,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3754,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3755,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3756,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3757,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3758,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3762,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3763,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3764,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3765,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3766,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3770,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3771,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3772,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3773,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3775,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3776,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3777,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3778,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3780,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3781,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3782,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3783,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3784,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3785,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3792,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3800,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3801,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3802,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3803,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3804,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3805,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3806,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3807,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3812,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3813,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3814,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3815,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3816,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3818,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3822,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3823,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3824,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3825,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3826,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3852,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3853,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3854,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3855,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3856,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3857,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3858,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3860,880,"Walter Benz",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3862,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3863,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3864,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3900,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3901,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3902,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3903,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3904,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3905,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3906,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3907,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3908,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3909,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3910,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3911,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3912,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3913,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3914,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3915,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3916,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3917,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3918,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3919,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3920,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3922,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3923,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3924,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3925,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3926,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3927,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3928,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3929,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3930,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3931,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3932,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3933,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3934,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3935,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3936,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3937,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3938,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3939,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3940,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3942,880,"Walter Benz",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3943,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3944,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3945,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3946,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3947,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3948,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3949,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3951,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3952,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3953,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3954,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3955,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3956,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3957,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3960,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3961,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3962,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3963,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3964,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3965,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3966,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3967,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3968,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3969,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3970,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3971,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3972,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3973,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3974,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3975,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3976,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3977,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3978,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3979,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3981,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3982,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3983,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3984,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3985,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3986,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3987,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3988,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3989,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3991,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3992,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3993,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3994,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3995,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3996,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3997,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3998,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3999,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,4000,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4001,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4002,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4003,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4004,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4005,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4006,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4007,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4008,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4009,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4010,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4011,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4012,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4013,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4015,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4016,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4017,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4018,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4019,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4020,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4021,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4023,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4024,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4025,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4027,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4028,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4030,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4031,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4032,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4039,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4040,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4051,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4052,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4053,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4054,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4055,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4056,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4057,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4058,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4059,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4091,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4101,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4102,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4103,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4104,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4105,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4106,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4107,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4108,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4112,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4114,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4115,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4116,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4117,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4118,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4123,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4124,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4125,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4126,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4127,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4132,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4133,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4142,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4143,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4144,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4145,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4146,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4147,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4148,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4153,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,4202,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4203,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4204,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4206,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4207,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4208,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4222,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4223,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4224,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4225,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4226,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4227,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4228,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4229,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4232,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4233,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4234,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4242,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4243,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4244,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4245,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4246,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4247,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4252,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4253,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4254,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4302,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4303,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4304,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4305,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4310,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4312,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4313,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4314,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4315,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4316,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4317,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4322,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4323,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4324,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4325,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4332,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4333,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4334,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4402,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4410,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4411,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4412,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4413,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4414,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4415,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4416,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4417,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4418,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4419,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4421,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4422,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4423,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4424,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4425,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4426,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4431,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4432,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4433,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4434,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4435,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4436,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4437,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4438,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4441,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4442,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4443,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4444,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4445,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4446,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4447,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4448,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4450,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4451,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4452,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4453,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4455,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4456,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4457,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4458,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4460,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4461,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4462,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4463,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4464,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4465,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4466,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4467,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4468,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4469,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4492,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4493,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4494,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4495,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4496,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4497,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4500,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4501,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4502,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4503,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4504,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4509,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4512,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4513,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4514,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4515,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4522,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4523,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4524,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4525,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4528,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4532,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4533,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4534,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4535,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4536,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4537,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4538,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4539,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4542,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4543,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4552,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4553,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4554,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4556,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4557,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4558,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4562,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4563,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4564,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4565,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4566,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4571,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4573,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4574,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4576,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4577,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4578,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4579,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4581,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4582,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4583,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4584,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4585,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4586,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4587,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4588,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4600,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4601,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4603,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4612,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4613,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4614,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4615,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4616,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4617,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4618,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4622,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4623,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4624,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4625,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4626,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4628,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4629,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4632,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4633,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4634,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4652,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4653,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4654,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4655,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4656,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4657,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4658,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4663,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4665,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4702,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4703,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4704,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4710,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4712,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4713,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4714,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4715,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4716,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4717,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4718,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4719,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4800,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4801,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4802,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4803,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4805,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4806,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4812,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4813,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4814,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4852,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4853,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4856,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4900,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4901,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4902,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4903,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4911,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4912,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4913,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4914,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4915,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4916,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4917,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4919,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4922,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4923,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4924,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4932,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4933,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4934,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4935,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4936,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4937,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4938,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4942,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4943,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4944,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4950,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4952,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4953,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4954,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4955,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5000,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5001,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5004,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5010,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5012,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5013,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5014,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5015,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5016,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5017,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5018,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5022,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5023,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5024,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5025,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5026,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5027,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5028,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5032,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5033,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5034,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5035,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5036,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5037,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5040,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5042,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5043,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5044,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5046,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5053,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5054,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5056,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5057,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5058,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5062,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5063,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5064,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5070,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5072,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5073,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5074,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5075,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5076,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5077,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5078,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5079,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5080,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5082,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5083,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5084,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5085,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5102,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5103,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5105,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5106,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5107,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5108,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5112,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5113,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5116,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5200,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5201,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5210,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5212,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5213,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5222,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5223,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5224,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5225,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5233,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5234,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5235,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5236,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5237,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5242,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5243,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5244,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5245,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5246,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5272,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5273,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5274,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5275,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5276,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5277,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5300,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5301,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5303,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5304,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5305,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5306,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5312,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5313,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5314,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5315,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5316,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5317,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5318,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5322,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5323,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5324,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5325,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5326,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5330,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5332,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5333,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5334,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5400,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5401,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5402,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5403,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5404,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5405,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5406,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5408,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5412,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5413,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5415,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5416,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5417,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5422,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5423,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5424,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5425,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5426,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5430,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5432,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5436,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5442,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5443,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5444,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5445,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5452,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5453,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5454,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5462,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5463,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5464,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5465,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5466,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5467,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5502,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5503,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5504,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5505,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5506,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5507,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5512,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5522,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5524,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5525,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5600,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5603,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5604,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5605,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5606,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5607,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5608,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5610,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5611,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5612,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5613,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5614,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5615,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5616,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5617,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5618,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5619,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5620,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5621,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5622,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5623,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5624,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5625,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5626,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5627,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5628,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5630,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5632,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5634,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5636,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5637,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5642,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5643,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5644,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5645,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5646,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5647,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5702,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5703,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5704,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5705,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5706,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5707,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5708,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5712,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5722,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5723,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5724,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5725,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5726,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5727,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5728,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5732,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5733,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5734,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5735,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5736,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5737,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5742,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5745,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,5746,822,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6000,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6002,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6003,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6004,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6005,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6006,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6007,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6009,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6010,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6011,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6012,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6013,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6014,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6015,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6016,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6017,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6018,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6019,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6020,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6021,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6022,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6023,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6024,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6025,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6026,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6027,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6028,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6030,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6031,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6032,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6033,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6034,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6035,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6036,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6037,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6038,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6042,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6043,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6044,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6045,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6047,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6048,880,"Walter Benz",1]
[null,null,null,null,null,null,null,null,null,null,null,null,6052,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6053,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6055,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6056,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6060,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6061,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6062,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6063,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6064,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6066,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6067,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6068,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6072,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6073,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6074,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6076,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6078,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6082,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6083,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6084,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6085,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6086,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6102,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6103,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6105,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6106,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6112,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6114,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6125,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6130,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6143,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6146,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6147,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6154,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6161,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6166,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6173,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6192,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6203,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6206,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6208,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6210,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6214,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6216,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6221,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6233,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6236,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6242,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6244,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6247,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6260,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6263,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6274,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6280,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6283,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6284,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6287,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6294,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6302,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6304,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6312,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6314,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6319,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6330,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6340,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6343,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6349,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6356,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6370,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6371,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6375,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6376,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6386,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6387,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6402,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6405,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6415,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6418,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6424,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6430,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6432,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6438,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6442,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6452,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6462,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6465,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6467,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6468,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6473,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6482,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6487,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6491,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6503,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6513,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6515,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6516,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6523,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6526,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6532,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6535,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6541,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6542,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6544,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6547,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6557,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6562,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6571,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6574,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6577,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6582,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6583,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6593,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6597,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6599,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6602,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6605,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6614,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6622,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6631,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6634,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6636,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6646,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6652,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6655,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6658,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6662,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6664,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6670,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6674,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6677,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6683,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6692,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6695,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6696,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6703,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6710,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6716,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6718,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6721,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6742,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6744,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6747,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6748,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6762,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6773,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6775,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6780,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6802,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6806,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6809,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6810,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6816,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6821,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6825,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6828,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6832,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6836,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6837,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6852,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6853,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6863,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6866,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6873,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6877,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6900,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6901,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6903,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6906,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6912,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6914,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6918,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6922,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6925,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6926,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6929,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6933,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6937,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6939,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6945,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6948,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6950,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6954,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6957,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6962,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6965,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6974,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6976,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6980,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6981,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6986,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6988,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6991,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6994,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6997,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,7000,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7003,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7004,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7012,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7014,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7017,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7019,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7028,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7032,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7057,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7058,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7063,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7076,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7082,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7084,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7108,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7112,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7114,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7115,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7126,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7130,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7134,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7137,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7143,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7144,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7146,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7149,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7153,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7156,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7159,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7165,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7167,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7173,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7174,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7180,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7185,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7187,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7199,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7202,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7206,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7212,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7213,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7220,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7223,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7231,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7235,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7241,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7245,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7249,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7252,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7260,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7276,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7302,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7306,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7312,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7315,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7317,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7323,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7326,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7405,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7411,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7414,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7418,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7421,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7424,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7425,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7428,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7433,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7435,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7438,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7444,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7446,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7447,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7451,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7454,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7457,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7460,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7464,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7473,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7492,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7493,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7503,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7504,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7514,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7517,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7524,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7527,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7533,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7534,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7542,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7543,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7551,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7553,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7558,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7562,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7603,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7604,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7606,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7710,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7744,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7746,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,8001,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8004,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8006,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8008,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8021,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8024,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8027,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8030,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8034,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8035,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8039,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8040,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8043,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8046,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8049,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8052,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8056,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8059,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8060,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8063,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8070,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8079,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8086,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8088,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8093,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8102,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8103,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8106,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8108,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8115,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8121,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8123,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8127,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8134,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8136,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8142,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8153,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8157,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8164,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8172,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8175,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8180,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8182,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8187,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8194,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8197,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8202,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8206,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8208,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8214,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8215,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8218,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8224,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8226,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8232,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8236,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8240,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8243,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8245,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8248,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8254,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8260,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8263,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8265,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8272,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8280,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8301,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8302,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8306,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8309,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8312,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8317,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8322,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8330,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8340,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8342,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8353,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8355,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8360,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8372,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8400,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8401,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8404,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8407,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8411,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8413,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8416,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8423,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8425,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8426,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8442,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8450,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8454,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8457,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8461,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8462,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8466,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8467,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8472,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8476,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8479,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8484,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8488,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8494,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8497,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8498,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8502,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8505,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8508,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8512,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8524,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8532,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8537,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8542,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8545,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8552,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8555,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8558,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8564,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8570,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8573,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8574,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8577,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8583,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8586,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8588,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8593,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8594,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8596,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8599,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8603,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8606,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8610,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8614,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8618,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8620,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8622,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8625,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8632,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8634,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8637,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8640,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8700,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8704,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8706,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8712,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8714,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8718,882,"Hansruedi Blumenthal",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8725,882,"Hansruedi Blumenthal",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8727,882,"Hansruedi Blumenthal",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8734,882,"Hansruedi Blumenthal",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8738,882,"Hansruedi Blumenthal",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8750,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8751,880,"Walter Benz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8754,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8758,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8766,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8773,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8782,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8800,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8802,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8803,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8807,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8810,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8815,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8825,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8834,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8835,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8840,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8843,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8847,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8852,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8855,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8862,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8864,882,"Hansruedi Blumenthal",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8867,882,"Hansruedi Blumenthal",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8868,882,"Hansruedi Blumenthal",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8874,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8880,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8882,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8885,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8887,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8892,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8893,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8896,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,8902,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8905,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8908,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8911,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8914,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8917,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8918,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8932,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8933,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8952,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8954,883,"Kaspar Ganz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8957,822,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,8965,880,"Walter Benz",2]
[null,null,null,null,null,null,null,null,null,null,null,null,9000,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9001,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9004,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9008,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9012,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9014,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9024,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9027,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9029,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9030,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9034,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9037,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9044,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9052,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9056,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9057,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9064,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9100,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9103,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9107,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9113,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9116,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9126,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9127,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9204,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9205,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9215,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9220,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9230,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9242,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9245,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9248,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9303,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9304,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9306,883,"Kaspar Ganz",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9314,883,"Kaspar Ganz",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9322,883,"Kaspar Ganz",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9325,883,"Kaspar Ganz",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9401,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9404,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9410,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9411,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9422,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9426,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9430,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9435,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9443,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9450,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9452,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9453,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9464,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9467,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9470,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9475,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9478,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9479,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9486,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9490,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9494,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9496,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9500,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9504,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9507,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9512,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9514,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9523,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9527,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9533,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9536,882,"Hansruedi Blumenthal",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9543,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9548,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9554,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9555,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9565,883,"Kaspar Ganz",3]
[null,null,null,null,null,null,null,null,null,null,null,null,9601,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9606,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9612,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9615,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9622,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9633,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9643,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9650,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9656,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,3065,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3066,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3067,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3068,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3068,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3072,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3074,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3084,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3096,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3098,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3144,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3145,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3145,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3172,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3174,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,2500,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2501,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2503,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2504,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2532,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2532,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2542,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2543,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3251,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3264,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3294,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3294,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3298,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3068,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3324,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3325,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3326,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3326,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3400,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3402,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3412,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3413,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3413,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3414,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3415,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3421,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3422,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3422,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3423,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3424,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3425,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3429,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3432,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3472,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3474,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3474,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2332,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2333,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2534,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2535,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2537,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2603,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2605,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2605,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2608,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2608,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2610,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2610,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2612,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2615,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2720,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2720,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2722,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2723,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2076,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2525,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2577,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2578,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3226,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3232,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3232,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3234,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3235,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3236,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3053,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3053,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3256,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3303,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3303,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3303,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3306,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3309,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3314,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3317,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3322,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3322,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3427,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3703,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3711,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3711,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3713,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3714,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3714,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3715,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3715,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3716,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3717,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3718,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3723,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3725,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3800,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3800,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3800,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3801,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3804,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3806,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3812,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3814,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3816,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3816,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3818,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3818,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3823,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3826,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3854,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3855,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3855,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3855,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3855,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3858,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3075,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3076,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3077,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3083,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3112,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3113,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3113,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3114,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3502,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3503,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3506,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3508,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3508,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3508,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3510,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3510,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3512,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3531,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3533,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3533,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3629,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3671,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3672,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3672,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3673,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3673,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1595,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3174,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3176,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3176,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3179,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3202,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3203,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3203,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3204,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3204,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3205,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3205,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3205,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3206,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3207,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3208,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3233,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,2712,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2713,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2715,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2717,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2732,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2732,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2732,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2735,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2735,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2738,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2740,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2742,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2745,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2747,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2748,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2827,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2514,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2515,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2515,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2518,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2520,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2512,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2512,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2513,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2514,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2514,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2552,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2555,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2557,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2562,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2564,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2572,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2575,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3252,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3272,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3274,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3274,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3632,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3647,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3700,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3702,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3752,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3753,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3755,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3757,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3758,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3762,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3764,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3764,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3765,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3857,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3860,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3860,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3860,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3860,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3860,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3860,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3862,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3862,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3863,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3864,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6082,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6084,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6086,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3766,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3766,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3766,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3770,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3770,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3772,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3772,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3775,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3775,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3776,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1657,832,"Heinz Allemann",4]
[null,null,null,null,null,null,null,null,null,null,null,null,3780,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3782,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3784,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3792,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1738,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1738,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3148,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3148,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3152,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3152,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3154,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3154,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3156,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3157,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3158,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3086,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3086,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3087,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3088,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3089,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3115,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3115,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3116,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3123,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3124,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3126,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3127,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3128,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3132,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3154,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3628,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3662,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3665,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3665,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3436,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3436,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3436,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3438,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3438,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3535,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3536,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3537,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3538,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3543,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3543,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3543,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3550,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3555,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3556,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3557,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,6197,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,6197,832,"Heinz Allemann",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3600,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3603,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3604,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3607,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3612,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3612,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3614,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3615,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3615,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3615,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3616,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3616,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3617,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3619,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3622,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3623,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3623,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3625,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3626,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3633,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3634,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3635,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3638,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3645,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3652,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3653,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3656,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3657,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3658,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3661,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3415,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3418,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3432,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3432,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3435,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3439,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3452,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3454,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3455,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3456,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3457,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3462,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3464,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,4942,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4952,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4954,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,3362,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3363,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3365,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3367,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3373,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3375,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3380,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3380,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3476,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3476,832,"Heinz Allemann",3]
[null,null,null,null,null,null,null,null,null,null,null,null,4537,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4539,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,4704,832,"Heinz Allemann",1]
[null,null,null,null,null,null,null,null,null,null,null,null,7077,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7078,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7082,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7082,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7083,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7431,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7431,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7451,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7452,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7454,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7455,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7456,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7457,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7458,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7460,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7462,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7463,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7464,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7477,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7482,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7482,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7482,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7492,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7493,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7494,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7741,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7741,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7742,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7742,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7743,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7744,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7745,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7746,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7748,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7748,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7032,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7104,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7112,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7114,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7115,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7116,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7122,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7126,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7126,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7128,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7130,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7132,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7132,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7133,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7134,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7135,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7136,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7136,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7138,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7142,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7144,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7145,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7147,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7149,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7149,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7149,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7151,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7153,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7155,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7156,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7158,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7158,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7159,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7104,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7107,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7108,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7404,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7408,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7412,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7415,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7415,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7417,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7419,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7421,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7423,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7424,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7425,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7425,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7427,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7428,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7430,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7432,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7433,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7433,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7433,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7434,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7438,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7440,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7442,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7444,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7446,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7447,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7012,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7013,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7013,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7014,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7017,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7018,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7019,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7402,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7403,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7527,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7530,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7543,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7545,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7546,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7550,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7550,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7552,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7553,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7554,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7556,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7557,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7558,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7560,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7562,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7500,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7500,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7503,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7504,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7505,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7512,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7514,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7515,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7516,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7516,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7522,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7522,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7524,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7526,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7602,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7605,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7606,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7610,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,6534,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6540,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6542,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6543,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6546,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6547,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6548,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6549,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6557,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6558,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6562,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6563,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7532,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7532,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7534,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7535,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7537,882,"Hansruedi Blumenthal",8]
[null,null,null,null,null,null,null,null,null,null,null,null,7224,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7232,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7240,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7241,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7244,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7245,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7246,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7246,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7249,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7250,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7250,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7265,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7270,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7270,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7276,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7278,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7000,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7002,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7005,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7007,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7027,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7028,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7028,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7050,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7057,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7058,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7063,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7074,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7075,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7023,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7202,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7206,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7208,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7213,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7214,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7214,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7215,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7222,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7228,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7304,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7304,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7307,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,7163,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7166,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7166,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7166,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7168,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7173,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7174,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7175,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7176,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7180,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7180,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7183,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7184,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7185,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7185,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7186,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7188,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7189,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,7189,882,"Hansruedi Blumenthal",6]
[null,null,null,null,null,null,null,null,null,null,null,null,2800,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2802,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2805,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2806,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2813,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2823,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2825,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2826,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2828,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2830,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2842,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2852,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2855,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2857,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2863,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2864,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2300,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2336,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2336,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2338,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2340,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2345,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2345,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2345,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2354,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2354,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2714,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2718,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2875,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2875,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2875,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2877,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2887,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2807,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2883,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2888,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2900,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2904,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2905,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2908,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2912,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2922,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2923,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2925,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2932,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2935,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2943,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2944,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2947,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2950,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2953,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2954,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2013,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2014,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2015,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2017,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2022,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2023,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2025,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2028,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2034,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2036,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2103,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2149,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2203,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2205,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2300,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2302,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2305,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2314,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2314,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2325,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2400,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2315,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2318,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2318,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2400,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2405,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2406,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2407,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2413,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2416,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2001,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2003,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2006,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2007,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2009,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2067,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2073,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2074,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2075,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2087,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2523,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2525,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2042,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2043,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2053,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2054,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2054,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2057,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2058,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2058,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2058,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2063,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2065,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2205,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2209,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2209,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2103,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2105,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2108,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2108,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2115,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2116,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2117,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2123,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2126,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,2126,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1468,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1470,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1473,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1474,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1482,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1483,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1485,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1486,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1489,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1527,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1529,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1532,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1541,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1544,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1564,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1565,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1567,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1569,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1773,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1773,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1775,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1775,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1776,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1503,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1670,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1671,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1673,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1674,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1675,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1677,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1677,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1678,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1680,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1680,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1681,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1681,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1686,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1687,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1688,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1690,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1690,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1692,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1693,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1694,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1748,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1625,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1626,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1626,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1627,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1630,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1633,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1634,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1636,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1637,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1637,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1637,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1642,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1644,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1645,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1647,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1651,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1652,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1653,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1654,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1656,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1656,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1661,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1663,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1665,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1667,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1668,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1669,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1835,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1696,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1700,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1700,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1702,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1703,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1707,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1708,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1721,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1723,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1723,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1724,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1724,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1724,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1724,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1724,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1724,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1725,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1726,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1726,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1727,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1728,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1729,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1729,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1731,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1733,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1741,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1743,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1745,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1746,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1752,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1754,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1756,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1757,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1763,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1763,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1772,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1772,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1782,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1782,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1783,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1721,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1721,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1783,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1784,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1784,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1786,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1787,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1788,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1789,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1792,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1793,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1793,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1794,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1795,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3206,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3212,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3212,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3213,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3215,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3215,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3215,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3216,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3280,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3280,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3280,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3285,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3285,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3286,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,1711,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1712,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1712,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1713,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1714,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1714,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1714,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1714,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1715,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1716,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1716,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1716,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1718,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1719,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1722,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1734,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1735,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1736,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,3175,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3178,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3178,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3178,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3178,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3178,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3182,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3184,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3184,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3184,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3185,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3185,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3185,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3186,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3186,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3186,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3186,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3186,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,3186,856,"Frederic Widmer",2]
[null,null,null,null,null,null,null,null,null,null,null,null,1609,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1609,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1611,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1616,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1617,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1618,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1619,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1624,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1624,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1698,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1699,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1845,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1852,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1854,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1858,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1860,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1862,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1862,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1863,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1864,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1865,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1866,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1867,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1867,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1880,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1880,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1880,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1880,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1882,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1882,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1884,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1886,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1892,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1892,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1143,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1145,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1170,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1172,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1174,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1176,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1188,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1188,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1261,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1580,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1584,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1585,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1586,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1586,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1588,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1588,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1589,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1787,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1034,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1041,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1124,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1141,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1147,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1148,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1304,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1304,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1306,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1308,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1312,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1315,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1316,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1318,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1328,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1040,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1041,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1041,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1041,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1042,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1042,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1053,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1055,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1376,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1416,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1417,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1418,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1421,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1422,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1422,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1423,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1424,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1425,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1427,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1428,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1429,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1450,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1450,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1453,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1453,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1454,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1004,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1006,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1008,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1008,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1008,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1010,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1011,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1015,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1018,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1032,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1051,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1052,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1066,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1068,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1073,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1093,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1095,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1096,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1096,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1602,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1602,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1603,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1604,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1606,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1813,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1024,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1025,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1026,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1029,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1112,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1114,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1121,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1126,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1128,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1131,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1133,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1135,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1137,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1162,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1041,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1041,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1041,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1041,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1062,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1064,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1086,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1510,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1512,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1513,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1515,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1516,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1526,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1557,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1682,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1683,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1197,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1260,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1261,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1261,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1263,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1266,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1268,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1270,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1273,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1274,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1275,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1276,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1277,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1279,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1291,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1295,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1298,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1322,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1323,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1323,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1326,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1337,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1338,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1352,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1355,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1355,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1356,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1359,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1373,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1445,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1059,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1078,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1082,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1084,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1084,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1088,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1607,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1607,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1608,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1610,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1613,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1488,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1523,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1525,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1525,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1536,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1543,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1551,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1552,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1554,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1556,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1556,856,"Frederic Widmer",3]
[null,null,null,null,null,null,null,null,null,null,null,null,1831,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1837,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1837,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1839,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1165,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1166,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1180,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1182,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1185,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1186,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1195,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1341,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1343,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1345,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1345,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1346,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1347,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1347,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1348,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1348,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1800,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1800,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1803,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1806,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1806,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1807,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1807,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1808,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1814,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1814,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1815,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1816,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1820,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1820,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1820,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1822,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1824,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1824,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1832,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1833,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1400,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1400,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1404,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1406,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1407,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1408,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1412,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1413,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1415,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1431,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1432,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1434,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1436,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1436,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1441,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1443,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1462,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1462,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1200,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1200,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1201,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1202,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1205,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1207,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1208,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1209,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1211,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1212,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1213,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1213,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1215,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1216,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1217,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1218,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1219,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1219,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1220,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1222,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1222,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1224,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1225,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1225,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1226,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1227,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1228,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1231,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1233,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1234,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1236,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1236,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1239,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1239,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1239,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1241,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1242,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1242,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1242,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1244,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1245,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1247,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1247,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1251,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1252,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1252,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1253,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1254,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1255,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1257,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1257,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1258,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1281,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1282,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1283,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1284,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1285,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1288,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1290,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1290,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1290,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1292,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1293,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1294,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1298,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3900,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3900,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3900,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3901,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3903,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3904,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3907,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3907,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3911,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3913,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3914,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,1933,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1955,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1956,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1963,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1975,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1975,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1976,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1976,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1993,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1994,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1994,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1996,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1996,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1996,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1997,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1997,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1997,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1933,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1934,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1934,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1934,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1934,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1936,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1936,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1937,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1937,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1937,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1937,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1941,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1941,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1942,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1944,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1945,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1945,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1945,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1946,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1947,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1947,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1947,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1948,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,3801,832,"Heinz Allemann",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3981,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3981,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3981,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3984,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3988,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3989,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3995,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3996,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3997,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3997,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3999,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3999,832,"Heinz Allemann",8]
[null,null,null,null,null,null,null,null,null,null,null,null,1966,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1966,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1966,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1966,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1969,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1969,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1973,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1973,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1981,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1982,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1983,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1985,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1985,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1987,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1987,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1988,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1988,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1992,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,3945,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3946,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3947,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3948,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3951,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3951,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3952,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3953,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3953,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3954,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3955,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3956,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3957,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3957,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3969,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1906,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1906,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1907,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1912,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1912,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1914,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1914,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1918,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1920,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1920,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1921,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1921,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1926,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1926,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1926,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1928,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1932,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1868,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1870,856,"Frederic Widmer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,1871,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1873,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1873,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1874,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1875,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1894,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1896,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1896,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1897,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1899,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1899,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,3915,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3917,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3919,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3919,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3936,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3940,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3942,880,"Walter Benz",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3942,880,"Walter Benz",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3943,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3949,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3983,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3983,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3983,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3986,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3993,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,3993,856,"Frederic Widmer",8]
[null,null,null,null,null,null,null,null,null,null,null,null,1871,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1890,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1891,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1891,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1902,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1904,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1905,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1905,856,"Frederic Widmer",5]
[null,null,null,null,null,null,null,null,null,null,null,null,1922,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1922,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1925,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1958,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3960,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3960,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3960,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3961,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3961,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3961,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3961,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3961,856,"Frederic Widmer",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3962,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3963,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3964,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3965,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3966,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3971,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3972,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3973,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3974,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3974,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3975,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3976,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3978,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3978,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3979,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3979,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1950,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1950,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1950,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1950,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1958,856,"Frederic Widmer",6]
[null,null,null,null,null,null,null,null,null,null,null,null,1962,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1965,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1965,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1965,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1965,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1967,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1971,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1974,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1991,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1991,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,1993,856,"Frederic Widmer",7]
[null,null,null,null,null,null,null,null,null,null,null,null,3906,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3908,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3909,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3909,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3920,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3920,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3920,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3922,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3924,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3924,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3925,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3926,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3928,832,"Heinz Allemann",9]
[null,null,null,null,null,null,null,null,null,null,null,null,3930,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3931,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3933,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,3937,832,"Heinz Allemann",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6500,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6500,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6500,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6506,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6512,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6515,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6517,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6523,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6524,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6528,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6582,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6583,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6583,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6584,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6592,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6809,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6809,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6713,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6713,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6714,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6716,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6717,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6718,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6718,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6718,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6719,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6720,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6720,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6722,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6723,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6723,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6724,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,7185,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6742,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6745,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6746,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6747,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6749,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6749,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6760,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6760,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6760,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6760,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6763,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6763,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6773,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6776,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6776,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6776,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6776,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6777,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6777,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6777,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6777,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6777,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6780,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6780,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6780,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6780,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6780,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6780,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6780,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6781,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6781,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6781,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6781,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6781,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6781,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6781,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6516,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6516,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6571,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6572,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6572,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6573,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6573,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6574,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6574,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6575,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6575,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6575,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6576,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6576,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6576,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6577,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6577,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6577,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6577,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6578,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6578,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6579,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6594,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6595,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6595,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6595,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6596,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6596,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6596,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6596,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6596,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6597,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6597,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6597,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6598,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6600,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6600,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6600,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6600,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6601,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6602,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6604,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6604,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6605,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6605,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6605,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6611,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6611,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6611,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6611,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6612,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6612,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6612,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6613,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6614,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6614,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6614,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6614,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6614,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6614,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6614,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6614,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6616,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6618,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6622,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6622,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6631,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6632,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6632,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6632,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6632,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6633,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6633,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6634,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6634,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6634,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6635,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6636,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6637,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6637,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6644,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6644,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6645,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6646,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6647,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6648,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6652,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6652,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6652,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6653,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6654,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6655,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6655,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6655,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6655,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6655,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6655,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6655,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6656,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6657,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6657,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6658,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6658,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6658,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6659,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6659,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6659,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6661,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6661,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6661,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6661,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6662,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6663,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6663,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6663,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6663,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6663,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6664,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6802,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6802,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6802,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6802,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6802,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6802,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6802,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6803,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6804,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6805,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6805,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6806,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6807,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6808,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6808,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6814,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6814,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6814,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6815,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6816,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6817,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6818,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6821,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6822,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6823,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6823,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6823,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6825,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6827,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6867,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6900,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6900,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6900,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6900,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6900,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6900,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6901,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6902,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6903,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6903,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6903,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6903,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6904,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6905,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6906,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6907,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6908,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6910,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6912,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6913,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6914,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6914,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6915,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6915,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6915,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6916,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6917,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6917,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6917,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6918,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6918,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6919,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6921,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6921,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6922,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6922,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6924,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6924,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6925,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6925,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6925,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6926,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6926,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6926,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6926,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6927,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6927,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6928,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6928,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6929,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6929,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6930,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6932,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6932,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6932,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6933,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6933,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6934,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6934,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6935,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6936,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6936,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6937,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6938,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6938,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6939,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6939,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6942,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6942,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6943,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6944,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6945,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6945,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6946,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6947,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6948,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6948,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6949,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6950,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6950,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6950,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6950,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6951,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6952,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6953,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6953,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6954,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6954,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6954,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6955,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6955,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6956,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6957,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6957,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6958,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6958,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6958,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6959,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6959,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6959,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6959,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6959,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6962,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6962,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6962,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6963,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6963,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6963,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6963,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6963,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6964,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6964,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6964,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6965,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6966,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6967,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6968,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6974,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6976,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6977,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6977,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6978,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6979,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6980,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6980,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6981,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6981,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6981,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6981,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6981,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6981,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6982,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6982,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6983,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6983,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6984,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6986,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6986,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6986,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6987,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6987,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6987,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6988,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6989,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6989,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6990,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6991,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6992,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6992,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6993,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6994,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6995,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6995,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6996,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6996,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6996,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6997,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6997,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6997,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6998,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6998,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6998,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6999,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6825,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6826,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6827,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6828,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6828,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6828,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6828,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6828,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6830,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6830,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6830,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6832,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6832,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6833,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6833,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6833,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6833,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6834,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6834,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6834,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6835,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6836,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6837,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6837,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6838,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6838,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6838,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6838,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6839,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6850,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6850,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6852,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6852,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6852,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6852,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6853,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6854,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6855,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6855,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6862,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6863,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6864,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6865,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6866,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6872,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6872,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6872,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6873,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6873,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6874,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6874,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6874,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6875,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6875,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6875,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6877,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6877,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6877,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6882,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6882,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6883,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6883,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6526,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6527,430,"Georgio Solari",4]
[null,null,null,null,null,null,null,null,null,null,null,null,6702,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6702,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6702,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6702,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6702,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6702,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6702,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6702,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6703,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6705,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6707,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6710,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6713,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6713,430,"Georgio Solari",5]
[null,null,null,null,null,null,null,null,null,null,null,null,6670,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6670,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6670,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6670,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6672,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6673,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6674,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6674,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6675,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6675,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6675,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6675,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6676,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6677,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6677,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6677,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6677,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6677,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6678,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6678,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6678,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6682,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6683,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6683,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6683,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6684,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6684,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6684,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6685,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6685,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6690,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6692,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6692,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6693,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6693,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6693,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6694,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6694,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6694,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6695,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6695,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6695,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6695,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,6696,430,"Georgio Solari",6]
[null,null,null,null,null,null,null,null,null,null,null,null,9485,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9486,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9487,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9487,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9488,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9490,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9490,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9491,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9492,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9492,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9492,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9493,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9494,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9495,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9496,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9496,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9497,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9497,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9497,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9497,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9497,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9497,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9497,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9497,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9497,882,"Hansruedi Blumenthal",4]
[null,null,null,null,null,null,null,null,null,null,null,null,9498,882,"Hansruedi Blumenthal",4]

{"sheet":"Transportkosten","index":37,"n_rows":46,"n_cols":68,"rows_kept":46,"cut":false,"hidden":true,"merged":[]}
["Postleitzahl","Zone","kg 1-30","kg 31-50","kg 51-75","kg 76-100","kg 101-125","kg 126-150","kg 151-200","kg 201-250","kg 251-300","kg 301-400","kg 401-500","kg 501-600","kg 601-700","kg 701-800","kg 801-900","kg 901-1'000","kg 1'001-1'250","kg 1'251-1'500","kg 1'501-1'750","kg 1'751-2'000","kg 2'001-3'000","kg 3'001-4'000","kg 4'001-5'000","kg 5'001-7'500","kg 7'501-10'000","kg 10'001-12'500","kg 12'501-15'000","kg 15'001-17'500","kg 17'501-20'000","kg 20'001-22'500","kg 22'501-25'000"]
["PLZ 1000-1199",4,74,83,88,93,110,128,154,189,226,249,271,301,336,376,416,451,475,503,537,601,775,930,1058,1242,1468,1617,1756,null,null,null,null,null,null,null,null,49,57,59,61,74,84,97,119,142,155,169,187,206,233,255,276,298,317,351,384,509,606,675,792,963,1089,1197,1278,1350,1440,1529]
["PLZ 1200-1299",5,79,88,95,99,119,139,171,211,255,278,313,349,389,434,475,509,544,578,619,693,913,1092,1237,1456,1722,1872,2056,null,null,null,null,null,null,null,null,52,61,64,65,79,94,108,127,150,172,194,216,239,262,284,313,350,367,410,458,606,726,792,945,1098,1251,1377,1485,1565,1664,1781]
["PLZ 1300-1499",4,74,83,88,93,110,128,154,189,226,249,271,301,336,376,416,451,475,503,537,601,775,930,1058,1242,1468,1617,1756,null,null,null,null,null,null,null,null,49,57,59,61,74,84,97,119,142,155,169,187,206,233,255,276,298,317,351,384,509,606,675,792,963,1089,1197,1278,1350,1440,1529]
["PLZ 1500-1599",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 1600-1699",4,74,83,88,93,110,128,154,189,226,249,271,301,336,376,416,451,475,503,537,601,775,930,1058,1242,1468,1617,1756,null,null,null,null,null,null,null,null,49,57,59,61,74,84,97,119,142,155,169,187,206,233,255,276,298,317,351,384,509,606,675,792,963,1089,1197,1278,1350,1440,1529]
["PLZ 1700-1799",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 1800-1870",4,74,83,88,93,110,128,154,189,226,249,271,301,336,376,416,451,475,503,537,601,775,930,1058,1242,1468,1617,1756,null,null,null,null,null,null,null,null,49,57,59,61,74,84,97,119,142,155,169,187,206,233,255,276,298,317,351,384,509,606,675,792,963,1089,1197,1278,1350,1440,1529]
["PLZ 1871-1920",5,79,88,95,99,119,139,171,211,255,278,313,349,389,434,475,509,544,578,619,693,913,1092,1237,1456,1722,1872,2056,null,null,null,null,null,null,null,null,52,61,64,65,79,94,108,127,150,172,194,216,239,262,284,313,350,367,410,458,606,726,792,945,1098,1251,1377,1485,1565,1664,1781]
["PLZ 1921-1949",7,87,98,108,114,135,158,202,249,295,324,370,421,475,521,572,619,670,722,780,890,1144,1381,1577,1831,2149,2357,2577,null,null,null,null,null,null,null,null,60,69,71,74,87,104,120,154,184,206,231,262,291,323,354,385,416,448,505,573,753,906,1008,1161,1332,1529,1664,1763,1835,1952,2069]
["PLZ 1950-1960",6,83,94,102,108,128,148,187,231,278,301,343,387,439,480,521,560,613,653,699,786,1040,1237,1399,1630,1941,2126,2334,null,null,null,null,null,null,null,null,57,65,68,70,82,99,111,145,171,188,211,240,267,295,322,349,382,412,456,509,670,804,900,1053,1215,1386,1520,1628,1709,1826,1934]
["PLZ 1961-1999",7,87,98,108,114,135,158,202,249,295,324,370,421,475,521,572,619,670,722,780,890,1144,1381,1577,1831,2149,2357,2577,null,null,null,null,null,null,null,null,60,69,71,74,87,104,120,154,184,206,231,262,291,323,354,385,416,448,505,573,753,906,1008,1161,1332,1529,1664,1763,1835,1952,2069]
["PLZ 2000-2999",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 3000-3299",2,65,71,75,82,91,99,118,140,162,178,193,208,227,252,278,301,324,347,376,416,509,607,693,809,971,1086,1155,null,null,null,null,null,null,null,null,43,46,48,51,60,65,73,85,100,105,111,121,131,146,161,178,193,206,227,245,324,384,441,513,621,720,765,819,882,963,1017]
["PLZ 3300-3707",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 3708-3799",5,79,88,95,99,119,139,171,211,255,278,313,349,389,434,475,509,544,578,619,693,913,1092,1237,1456,1722,1872,2056,null,null,null,null,null,null,null,null,52,61,64,65,79,94,108,127,150,172,194,216,239,262,284,313,350,367,410,458,606,726,792,945,1098,1251,1377,1485,1565,1664,1781]
["PLZ 3800",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 3801-3899",5,79,88,95,99,119,139,171,211,255,278,313,349,389,434,475,509,544,578,619,693,913,1092,1237,1456,1722,1872,2056,null,null,null,null,null,null,null,null,48,56,59,61,73,87,106,126,149,171,192,214,237,260,382,310,350,367,410,458,606,726,792,945,1098,1251,1377,1485,1565,1664,1781]
["PLZ 3900-3979 ( excl. 3901, 3961, 3905-3929 )",6,83,94,102,108,128,148,187,231,278,301,343,387,439,480,521,560,613,653,699,786,1040,1237,1399,1630,1941,2126,2334,null,null,null,null,null,null,null,null,57,65,68,70,82,99,111,145,171,188,211,240,267,295,322,349,382,412,456,509,670,804,900,1053,1215,1386,1520,1628,1709,1826,1934]
["PLZ 3901, 3961, 3905-3929 ( excl. 3920 )",9,98,112,121,130,151,176,227,278,328,376,422,477,532,585,652,711,786,867,948,1075,1363,1676,1941,2253,2600,2854,3062,null,null,null,null,null,null,null,null,64,75,77,84,98,118,141,171,206,232,260,292,327,364,404,450,497,548,603,670,878,1054,1188,1395,1574,1790,1889,2006,2078,2186,2321]
["PLZ 3980-3999",8,93,105,114,120,141,167,215,267,313,347,393,451,506,555,619,665,717,791,861,983,1248,1525,1756,2033,2357,2588,2819,null,null,null,null,null,null,null,null,63,72,74,77,91,110,131,162,194,214,245,279,314,348,383,416,458,497,557,629,827,989,1098,1287,1458,1655,1772,1880,1961,2078,2204]
["PLZ 4000-4199",2,65,71,75,82,91,99,118,140,162,178,193,208,227,252,278,301,324,347,376,416,509,607,693,809,971,1086,1155,null,null,null,null,null,null,null,null,43,46,48,51,60,65,73,85,100,105,111,121,131,146,161,178,193,206,227,245,324,384,441,513,621,720,765,819,882,963,1017]
["PLZ 4200-6050",1,59,64,70,75,82,87,98,112,125,139,153,167,181,197,214,237,260,283,306,336,405,480,560,653,763,844,901,null,null,null,null,null,null,null,null,39,41,44,47,49,53,58,66,77,81,85,91,99,111,126,138,152,164,177,190,245,296,333,396,477,522,567,594,648,702,765]
["PLZ 6051-6350",2,65,71,75,82,91,99,118,140,162,178,193,208,227,252,278,301,324,347,376,416,509,607,693,809,971,1086,1155,null,null,null,null,null,null,null,null,43,46,48,51,60,65,73,85,100,105,111,121,131,146,161,178,193,206,227,245,324,384,441,513,621,720,765,819,882,963,1017]
["PLZ 6351-6499",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 6500-6599 ( excl. 6534-6589 )",4,74,83,88,93,110,128,154,189,226,249,271,301,336,376,416,451,475,503,537,601,775,930,1058,1242,1468,1617,1756,null,null,null,null,null,null,null,null,49,57,59,61,74,84,97,119,142,155,169,187,206,233,255,276,298,317,351,384,509,606,675,792,963,1089,1197,1278,1350,1440,1529]
["PLZ 6534-6589",6,83,94,102,108,128,148,187,231,278,301,343,387,439,480,521,560,613,653,699,786,1040,1237,1399,1630,1941,2126,2334,null,null,null,null,null,null,null,null,57,65,68,70,82,99,111,145,171,188,211,240,267,295,322,349,382,412,456,509,670,804,900,1053,1215,1386,1520,1628,1709,1826,1934]
["PLZ 6600-6799 ( excl. 6611-6699 )",5,79,88,95,99,119,139,171,211,255,278,313,349,389,434,475,509,544,578,619,693,913,1092,1237,1456,1722,1872,2056,null,null,null,null,null,null,null,null,52,61,64,65,79,94,108,127,150,172,194,216,239,262,284,313,350,367,410,458,606,726,792,945,1098,1251,1377,1485,1565,1664,1781]
["PLZ 6611-6699",6,83,94,102,108,128,148,187,231,278,301,343,387,439,480,521,560,613,653,699,786,1040,1237,1399,1630,1941,2126,2334,null,null,null,null,null,null,null,null,57,65,68,70,82,99,111,145,171,188,211,240,267,295,322,349,382,412,456,509,670,804,900,1053,1215,1386,1520,1628,1709,1826,1934]
["PLZ 6800-6999",5,79,88,95,99,119,139,171,211,255,278,313,349,389,434,475,509,544,578,619,693,913,1092,1237,1456,1722,1872,2056,null,null,null,null,null,null,null,null,52,61,64,65,79,94,108,127,150,172,194,216,239,262,284,313,350,367,410,458,606,726,792,945,1098,1251,1377,1485,1565,1664,1781]
["PLZ 7000-7023",4,74,83,88,93,110,128,154,189,226,249,271,301,336,376,416,451,475,503,537,601,775,930,1058,1242,1468,1617,1756,null,null,null,null,null,null,null,null,49,57,59,61,74,84,97,119,142,155,169,187,206,233,255,276,298,317,351,384,509,606,675,792,963,1089,1197,1278,1350,1440,1529]
["PLZ 7024-7299 ( excl. 7200-7209 )",6,83,94,102,108,128,148,187,231,278,301,343,387,439,480,521,560,613,653,699,786,1040,1237,1399,1630,1941,2126,2334,null,null,null,null,null,null,null,null,57,65,68,70,82,99,111,145,171,188,211,240,267,295,322,349,382,412,456,509,670,804,900,1053,1215,1386,1520,1628,1709,1826,1934]
["PLZ 7200-7209",4,74,83,88,93,110,128,154,189,226,249,271,301,336,376,416,451,475,503,537,601,775,930,1058,1242,1468,1617,1756,null,null,null,null,null,null,null,null,49,57,59,61,74,84,97,119,142,155,169,187,206,233,255,276,298,317,351,384,509,606,675,792,963,1089,1197,1278,1350,1440,1529]
["PLZ 7300-7430",4,74,83,88,93,110,128,154,189,226,249,271,301,336,376,416,451,475,503,537,601,775,930,1058,1242,1468,1617,1756,null,null,null,null,null,null,null,null,49,57,59,61,74,84,97,119,142,155,169,187,206,233,255,276,298,317,351,384,509,606,675,792,963,1089,1197,1278,1350,1440,1529]
["PLZ 7431-7999",8,93,105,114,120,141,167,215,267,313,347,393,451,506,555,619,665,717,791,861,983,1248,1525,1756,2033,2357,2588,2819,null,null,null,null,null,null,null,null,63,72,74,77,91,110,131,162,194,214,245,279,314,348,383,416,458,497,557,629,827,989,1098,1287,1458,1655,1772,1880,1961,2078,2204]
["PLZ 8000-8199",2,65,71,75,82,91,99,118,140,162,178,193,208,227,252,278,301,324,347,376,416,509,607,693,809,971,1086,1155,null,null,null,null,null,null,null,null,43,46,48,51,60,65,73,85,100,105,111,121,131,146,161,178,193,206,227,245,324,384,441,513,621,720,765,819,882,963,1017]
["PLZ 8200-8299",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 8300-8550",2,65,71,75,82,91,99,118,140,162,178,193,208,227,252,278,301,324,347,376,416,509,607,693,809,971,1086,1155,null,null,null,null,null,null,null,null,43,46,48,51,60,65,73,85,100,105,111,121,131,146,161,178,193,206,227,245,324,384,441,513,621,720,765,819,882,963,1017]
["PLZ 8551-8599",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 8600-8899 ( excl. 8750-8799, 8873-8899 )",2,65,71,75,82,91,99,118,140,162,178,193,208,227,252,278,301,324,347,376,416,509,607,693,809,971,1086,1155,null,null,null,null,null,null,null,null,43,46,48,51,60,65,73,85,100,105,111,121,131,146,161,178,193,206,227,245,324,384,441,513,621,720,765,819,882,963,1017]
["PLZ 8750-8799, 8873-8899",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 8900-8999",2,65,71,75,82,91,99,118,140,162,178,193,208,227,252,278,301,324,347,376,416,509,607,693,809,971,1086,1155,null,null,null,null,null,null,null,null,43,46,48,51,60,65,73,85,100,105,111,121,131,146,161,178,193,206,227,245,324,384,441,513,621,720,765,819,882,963,1017]
["PLZ 9000-9299",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 9300-9499",4,74,83,88,93,110,128,154,189,226,249,271,301,336,376,416,451,475,503,537,601,775,930,1058,1242,1468,1617,1756,null,null,null,null,null,null,null,null,49,57,59,61,74,84,97,119,142,155,169,187,206,233,255,276,298,317,351,384,509,606,675,792,963,1089,1197,1278,1350,1440,1529]
["PLZ 9500-9599",3,70,76,83,87,101,115,136,163,194,214,227,252,275,313,347,382,405,428,457,509,647,775,890,1029,1214,1352,1456,null,null,null,null,null,null,null,null,46,51,53,57,65,73,83,100,117,127,137,153,171,193,213,233,253,273,296,324,416,499,558,648,810,909,981,1062,1125,1206,1260]
["PLZ 9600-9699",4,74,83,88,93,110,128,154,189,226,249,271,301,336,376,416,451,475,503,537,601,775,930,1058,1242,1468,1617,1756,null,null,null,null,null,null,null,null,49,57,59,61,74,84,97,119,142,155,169,187,206,233,255,276,298,317,351,384,509,606,675,792,963,1089,1197,1278,1350,1440,1529]